  COVER INFORMATION 
 
 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GLOBAL-18cm-2016+112
 Exp. Code:  GP030B  

 
Schedule Version:       1.00                                              
Processed by SCHED version: 16 Oct. 2001                                  
 
PI:       Richard Porcas                                                  
 
Address:  MPIfR                                                           
          Auf dem Huegel 69                                               
          D 53121 BONN                                                    
          Germany                                                         
 
Phone:    +49 228 525288                                                  
EMAIL:    porcas@mpifr-bonn.mpg.de                                        
Fax:      +49 228 525229                                                  
Phone during observation:                                                 
 
Observing mode: Continuum                                                 
 
Notes:    VLA: Put T in column 57 of antenna file to                      
          VLA: disable analog sum for outer antennas                      
          VLA: at AE9, AN9, and AW9.                                      
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
 Next scan frequencies:  1642.49  1650.49  1658.49  1666.49
 Next BBC frequencies:    757.51   749.51   741.51   733.51
 Next scan bandwidths:      8.00     8.00     8.00     8.00
  
11 36 00  2029+121     15 00 52  12.4  82.9 -5.5     -60.9     0   1  1      0  11 36 00
11 38 00  ---          15 02 53  12.8  83.1 -5.5     -61.0   120   F  1    800
  
11 38 00  2016+112     15 02 53  15.1  85.4 -5.3     -61.1    -7   1  1    800  11 38 00
11 42 30  ---          15 07 23  16.1  86.0 -5.2     -61.1   263   F  1   2600
  
11 42 30  2029+121     15 07 23  13.8  83.7 -5.4     -61.1    -7   1  1   2600  11 42 30
11 45 00  ---          15 09 54  14.3  84.0 -5.4     -61.1   143   F  1   3600
  
11 45 00  2016+112     15 09 54  16.6  86.3 -5.2     -61.2    -7   1  1   3600  11 45 00
11 49 30  ---          15 14 25  17.6  86.9 -5.1     -61.2   263   F  1   5400
  
11 49 30  2029+121     15 14 25  15.3  84.5 -5.3     -61.2    -7   1  1   5400  11 49 30
11 52 00  ---          15 16 55  15.8  84.8 -5.3     -61.3   143   F  1   6400
  
11 52 00  2016+112     15 16 55  18.1  87.2 -5.0     -61.3    -7   1  1   6400  11 52 00
11 56 30  ---          15 21 26  19.1  87.7 -5.0     -61.3   263   F  1   8200
  
11 56 30  2029+121     15 21 26  16.8  85.4 -5.2     -61.4    -7   1  1   8200  11 56 30
11 59 00  ---          15 23 56  17.3  85.7 -5.1     -61.4   143   F  1   9200
  
11 59 00  2016+112     15 23 56  19.6  88.0 -4.9     -61.3    -7   1  1   9200  11 59 00
12 03 30  ---          15 28 27  20.6  88.6 -4.8     -61.4   263   F  1  11000
  
12 03 30  2029+121     15 28 27  18.3  86.2 -5.1     -61.5    -7   1  1  11000  12 03 30
12 06 00  ---          15 30 57  18.8  86.5 -5.0     -61.5   143   F  1  12000
  
12 06 00  2016+112     15 30 57  21.1  88.9 -4.8     -61.4    -7   1  1  12000  12 06 00
12 10 30  ---          15 35 28  22.1  89.5 -4.7     -61.4   263   F  1  13800
  
12 10 30  2029+121     15 35 28  19.8  87.1 -4.9     -61.6    -7   1  1  13800  12 10 30
12 13 00  ---          15 37 58  20.3  87.4 -4.9     -61.6   143   F  1  14800
  
12 13 00  2016+112     15 37 58  22.6  89.8 -4.7     -61.4    -7   1  1  14800  12 13 00
12 17 30  ---          15 42 29  23.6  90.4 -4.6     -61.4   263   F  1  16600
  
12 17 30  2029+121     15 42 29  21.3  88.0 -4.8     -61.7    -7   1  1  16600  12 17 30
12 20 00  ---          15 45 00  21.8  88.3 -4.8     -61.7   143   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
12 24 00  2029+121     15 49 00  22.7  88.8 -4.7     -61.7   236   1  2  17600  12 24 00
12 26 30  ---          15 51 31  23.2  89.1 -4.7     -61.7   150   R  1  16600
  
12 26 30  2016+112     15 51 31  25.5  91.6 -4.5     -61.4    -7   1  2  16600  12 26 30
12 31 00  ---          15 56 01  26.5  92.1 -4.4     -61.3   263   R  1  14800
  
12 31 00  2029+121     15 56 01  24.2  89.7 -4.6     -61.7    -7   1  2  14800  12 31 00
12 33 30  ---          15 58 32  24.8  90.0 -4.6     -61.7   143   R  1  13800
  
12 33 30  2016+112     15 58 32  27.1  92.5 -4.3     -61.3    -7   1  2  13800  12 33 30
12 38 00  ---          16 03 03  28.0  93.1 -4.3     -61.2   263   R  1  12000
  
12 38 00  2029+121     16 03 03  25.7  90.6 -4.5     -61.7    -7   1  2  12000  12 38 00
12 40 30  ---          16 05 33  26.3  90.9 -4.4     -61.7   143   R  1  11000
  
12 40 30  2016+112     16 05 33  28.6  93.4 -4.2     -61.2    -7   1  2  11000  12 40 30
12 45 00  ---          16 10 04  29.5  94.0 -4.2     -61.1   263   R  1   9200
  
12 45 00  2029+121     16 10 04  27.2  91.5 -4.4     -61.7    -7   1  2   9200  12 45 00
12 47 30  ---          16 12 34  27.8  91.8 -4.3     -61.7   143   R  1   8200
  
12 47 30  2016+112     16 12 34  30.1  94.4 -4.1     -61.1    -7   1  2   8200  12 47 30
12 52 00  ---          16 17 05  31.0  95.0 -4.0     -61.0   263   R  1   6400
  
12 52 00  2029+121     16 17 05  28.7  92.4 -4.2     -61.6    -7   1  2   6400  12 52 00
12 54 30  ---          16 19 35  29.3  92.7 -4.2     -61.6   143   R  1   5400
  
12 54 30  2016+112     16 19 35  31.6  95.3 -4.0     -60.9    -7   1  2   5400  12 54 30
12 59 00  ---          16 24 06  32.5  96.0 -3.9     -60.8   263   R  1   3600
  
12 59 00  2029+121     16 24 06  30.3  93.3 -4.1     -61.6    -7   1  2   3600  12 59 00
13 08 00  ---          16 33 07  32.2  94.6 -4.0     -61.4   533   R  1      0
  
13 12 00  2029+121     16 37 08  33.1  95.1 -3.9     -61.3   236   1  3      0  13 12 00
13 14 00  ---          16 39 08  33.5  95.4 -3.9     -61.3   120   F  1    800
  
13 14 00  2016+112     16 39 08  35.7  98.2 -3.7     -60.3    -7   1  3    800  13 14 00
13 18 30  ---          16 43 39  36.7  98.8 -3.6     -60.2   263   F  1   2600
  
13 18 30  2029+121     16 43 39  34.4  96.0 -3.8     -61.1    -7   1  3   2600  13 18 30
13 21 00  ---          16 46 10  35.0  96.4 -3.8     -61.1   143   F  1   3600
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
13 21 00  2016+112     16 46 10  37.2  99.2 -3.6     -60.1    -7   1  3   3600  13 21 00
13 25 30  ---          16 50 40  38.2  99.9 -3.5     -59.9   263   F  1   5400
  
13 25 30  2029+121     16 50 40  35.9  97.1 -3.7     -60.9    -7   1  3   5400  13 25 30
13 28 00  ---          16 53 11  36.5  97.4 -3.6     -60.9   143   F  1   6400
  
13 28 00  2016+112     16 53 11  38.7 100.3 -3.4     -59.7    -6   1  3   6400  13 28 00
13 32 30  ---          16 57 42  39.7 101.0 -3.4     -59.5   264   F  1   8200
  
13 32 30  2029+121     16 57 42  37.4  98.1 -3.6     -60.7    -6   1  3   8200  13 32 30
13 35 00  ---          17 00 12  38.0  98.5 -3.5     -60.6   144   F  1   9200
  
13 35 00  2016+112     17 00 12  40.2 101.4 -3.3     -59.4    -6   1  3   9200  13 35 00
13 39 30  ---          17 04 43  41.2 102.2 -3.2     -59.1   264   F  1  11000
  
13 39 30  2029+121     17 04 43  38.9  99.2 -3.5     -60.4    -6   1  3  11000  13 39 30
13 42 00  ---          17 07 13  39.5  99.6 -3.4     -60.3   144   F  1  12000
  
13 42 00  2016+112     17 07 13  41.7 102.6 -3.2     -59.0    -6   1  3  12000  13 42 00
13 46 30  ---          17 11 44  42.6 103.4 -3.1     -58.7   264   F  1  13800
  
13 46 30  2029+121     17 11 44  40.4 100.3 -3.3     -60.1    -6   1  3  13800  13 46 30
13 49 00  ---          17 14 14  41.0 100.7 -3.3     -59.9   144   F  1  14800
  
13 49 00  2016+112     17 14 14  43.2 103.8 -3.1     -58.5    -6   1  3  14800  13 49 00
13 53 30  ---          17 18 45  44.1 104.6 -3.0     -58.2   264   F  1  16600
  
13 53 30  2029+121     17 18 45  41.9 101.4 -3.2     -59.7    -6   1  3  16600  13 53 30
13 56 00  ---          17 21 15  42.4 101.8 -3.2     -59.5   144   F  1  17600
  
13 59 00  2029+121     17 24 16  43.1 102.3 -3.1     -59.4   177   1  4  17600  13 59 00
14 01 00  ---          17 26 16  43.5 102.7 -3.1     -59.2   120   R  1  16800
  
14 01 00  2016+112     17 26 16  45.7 106.0 -2.9     -57.6    -6   1  4  16800  14 01 00
14 05 30  ---          17 30 47  46.6 106.9 -2.8     -57.2   264   R  1  15000
  
14 05 30  2029+121     17 30 47  44.4 103.5 -3.0     -58.9    -6   1  4  15000  14 05 30
14 08 00  ---          17 33 17  45.0 103.9 -3.0     -58.7   144   R  1  14000
  
14 08 00  2016+112     17 33 17  47.1 107.4 -2.8     -56.9    -6   1  4  14000  14 08 00
14 12 30  ---          17 37 48  48.0 108.3 -2.7     -56.5   264   R  1  12200
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
14 12 30  2029+121     17 37 48  45.9 104.7 -2.9     -58.4    -6   1  4  12200  14 12 30
14 15 00  ---          17 40 18  46.4 105.2 -2.9     -58.2   144   R  1  11200
  
14 15 00  2016+112     17 40 18  48.5 108.8 -2.7     -56.2    -6   1  4  11200  14 15 00
14 19 30  ---          17 44 49  49.5 109.7 -2.6     -55.7   264   R  1   9400
  
14 19 30  2029+121     17 44 49  47.4 106.1 -2.8     -57.8    -6   1  4   9400  14 19 30
14 22 00  ---          17 47 20  47.9 106.5 -2.7     -57.6   144   R  1   8400
  
14 22 00  2016+112     17 47 20  50.0 110.2 -2.5     -55.5    -6   1  4   8400  14 22 00
14 26 30  ---          17 51 50  50.9 111.2 -2.5     -54.9   264   R  1   6600
  
14 26 30  2029+121     17 51 50  48.8 107.4 -2.7     -57.2    -6   1  4   6600  14 26 30
14 29 00  ---          17 54 21  49.3 107.9 -2.6     -56.9   144   R  1   5600
  
14 29 00  2016+112     17 54 21  51.4 111.8 -2.4     -54.6    -6   1  4   5600  14 29 00
14 33 30  ---          17 58 52  52.3 112.8 -2.3     -54.0   264   R  1   3800
  
14 33 30  2029+121     17 58 52  50.2 108.9 -2.6     -56.4    -6   1  4   3800  14 33 30
14 36 00  ---          18 01 22  50.7 109.4 -2.5     -56.2   144   R  1   2800
  
14 36 00  2016+112     18 01 22  52.8 113.4 -2.3     -53.7    -6   1  4   2800  14 36 00
14 40 30  ---          18 05 53  53.7 114.5 -2.2     -53.0   264   R  1   1000
  
14 40 30  2029+121     18 05 53  51.7 110.4 -2.4     -55.6    -6   1  4   1000  14 40 30
14 43 00  ---          18 08 23  52.2 111.0 -2.4     -55.3   144   R  1      0
  
14 46 00  2029+121     18 11 24  52.8 111.7 -2.3     -54.9   177   1  5      0  14 46 00
14 48 00  ---          18 13 24  53.2 112.1 -2.3     -54.7   120   F  1    800
  
14 48 00  2016+112     18 13 24  55.1 116.5 -2.1     -51.8    -6   1  5    800  14 48 00
14 52 30  ---          18 17 55  56.0 117.7 -2.0     -51.0   264   F  1   2600
  
14 52 30  2029+121     18 17 55  54.1 113.2 -2.2     -54.0    -6   1  5   2600  14 52 30
14 55 00  ---          18 20 25  54.6 113.8 -2.2     -53.7   144   F  1   3600
  
14 55 00  2016+112     18 20 25  56.5 118.4 -2.0     -50.6    -6   1  5   3600  14 55 00
14 59 30  ---          18 24 56  57.3 119.7 -1.9     -49.7   264   F  1   5400
  
14 59 30  2029+121     18 24 56  55.4 115.0 -2.1     -53.0    -6   1  5   5400  14 59 30
15 02 00  ---          18 27 26  55.9 115.6 -2.1     -52.6   144   F  1   6400
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
15 02 00  2016+112     18 27 26  57.8 120.4 -1.9     -49.2    -6   1  5   6400  15 02 00
15 06 30  ---          18 31 57  58.6 121.8 -1.8     -48.2   264   F  1   8200
  
15 06 30  2029+121     18 31 57  56.8 116.8 -2.0     -51.8    -6   1  5   8200  15 06 30
15 09 00  ---          18 34 27  57.3 117.5 -2.0     -51.3   144   F  1   9200
  
15 09 00  2016+112     18 34 27  59.1 122.6 -1.7     -47.7    -6   1  5   9200  15 09 00
15 13 30  ---          18 38 58  59.9 124.1 -1.7     -46.6   264   F  1  11000
  
15 13 30  2029+121     18 38 58  58.1 118.8 -1.9     -50.5    -5   1  5  11000  15 13 30
15 16 00  ---          18 41 29  58.6 119.6 -1.8     -50.0   145   F  1  12000
  
15 16 00  2016+112     18 41 29  60.3 124.9 -1.6     -46.0    -6   1  5  12000  15 16 00
15 20 30  ---          18 45 59  61.1 126.5 -1.6     -44.9   264   F  1  13800
  
15 20 30  2029+121     18 45 59  59.4 121.0 -1.8     -49.0    -6   1  5  13800  15 20 30
15 30 00  ---          18 55 31  61.2 124.1 -1.6     -46.8   564   F  1  17600
  
15 33 00  2029+121     18 58 31  61.7 125.2 -1.6     -46.0   177   1  6  17600  15 33 00
15 35 00  ---          19 00 32  62.1 125.9 -1.5     -45.5   120   R  1  16800
  
15 35 00  2016+112     19 00 32  63.5 132.2 -1.3     -40.6    -6   1  6  16800  15 35 00
15 39 00  ---          19 04 32  64.2 133.9 -1.2     -39.3   234   R  1  15200
  
15 39 00  2029+121     19 04 32  62.7 127.4 -1.5     -44.4    -6   1  6  15200  15 39 00
15 49 00  ---          19 14 34  64.4 131.4 -1.3     -41.3   594   R  1  11200
  
15 49 00  2016+112     19 14 34  65.6 138.5 -1.1     -35.6    -7   1  6  11200  15 49 00
15 53 30  ---          19 19 05  66.3 140.7 -1.0     -33.8   263   R  1   9400
  
15 53 30  2029+121     19 19 05  65.1 133.4 -1.2     -39.8    -7   1  6   9400  15 53 30
15 56 00  ---          19 21 35  65.5 134.5 -1.2     -38.9   143   R  1   8400
  
15 56 00  2016+112     19 21 35  66.6 142.0 -1.0     -32.7    -7   1  6   8400  15 56 00
16 00 30  ---          19 26 06  67.2 144.4  -.9     -30.8   263   R  1   6600
  
16 00 30  2029+121     19 26 06  66.2 136.7 -1.1     -37.2    -7   1  6   6600  16 00 30
16 03 00  ---          19 28 36  66.6 137.9 -1.1     -36.2   143   R  1   5600
  
16 03 00  2016+112     19 28 36  67.5 145.8  -.8     -29.6    -7   1  6   5600  16 03 00
16 07 30  ---          19 33 07  68.0 148.3  -.8     -27.5   263   R  1   3800
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
16 07 30  2029+121     19 33 07  67.2 140.2 -1.0     -34.3    -7   1  6   3800  16 07 30
16 10 00  ---          19 35 37  67.5 141.5  -.9     -33.2   143   R  1   2800
  
16 10 00  2016+112     19 35 37  68.3 149.8  -.7     -26.2    -8   1  6   2800  16 10 00
16 14 30  ---          19 40 08  68.8 152.5  -.7     -23.9   262   R  1   1000
  
16 14 30  2029+121     19 40 08  68.1 144.0  -.9     -31.2    -8   1  6   1000  16 14 30
16 17 00  ---          19 42 39  68.4 145.4  -.8     -30.0   142   R  1      0
  
16 18 00  2029+121     19 43 39  68.6 146.0  -.8     -29.5    58   1  7      0  16 18 00
16 20 00  ---          19 45 39  68.8 147.2  -.8     -28.5   120   F  1    800
  
16 20 00  2016+112     19 45 39  69.3 156.0  -.6     -20.9    -8   1  7    800  16 20 00
16 24 30  ---          19 50 10  69.7 159.0  -.5     -18.3   262   F  1   2600
  
16 24 30  2029+121     19 50 10  69.3 149.9  -.7     -26.2    -8   1  7   2600  16 24 30
16 26 00  ---          19 51 40  69.5 150.8  -.7     -25.4    82   F  1   3200
  
16 26 00  2016+112     19 51 40  69.8 160.0  -.5     -17.5    -8   1  7   3200  16 26 00
16 30 30  ---          19 56 11  70.1 163.1  -.4     -14.8   262   F  1   5000
  
16 30 30  2029+121     19 56 11  69.9 153.7  -.6     -22.9    -8   1  7   5000  16 30 30
16 32 00  ---          19 57 41  70.1 154.7  -.6     -22.1    82   F  1   5600
  
16 32 00  2016+112     19 57 41  70.2 164.2  -.4     -13.9    -8   1  7   5600  16 32 00
16 36 30  ---          20 02 12  70.4 167.4  -.3     -11.1   262   F  1   7400
  
16 36 30  2029+121     20 02 12  70.4 157.8  -.5     -19.5    -8   1  7   7400  16 36 30
16 38 00  ---          20 03 42  70.6 158.8  -.5     -18.6    82   F  1   8000
  
16 38 00  2016+112     20 03 42  70.5 168.4  -.3     -10.1    -8   1  7   8000  16 38 00
16 42 30  ---          20 08 13  70.6 171.7  -.2      -7.3   262   F  1   9800
  
16 42 30  2029+121     20 08 13  70.9 162.0  -.4     -15.8    -8   1  7   9800  16 42 30
16 44 00  ---          20 09 43  71.0 163.1  -.4     -14.8    82   F  1  10400
  
16 44 00  2016+112     20 09 43  70.7 172.8  -.2      -6.3    -8   1  7  10400  16 44 00
16 48 30  ---          20 14 14  70.8 176.2  -.1      -3.4   262   F  1  12200
  
16 48 30  2029+121     20 14 14  71.2 166.4  -.3     -12.0    -9   1  7  12200  16 48 30
16 50 00  ---          20 15 44  71.3 167.5  -.3     -11.0    81   F  1  12800
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
16 50 00  2016+112     20 15 44  70.8 177.3  -.1      -2.4    -9   1  7  12800  16 50 00
16 54 30  ---          20 20 15  70.8 180.7   .0        .6   261   F  1  14600
  
16 54 30  2029+121     20 20 15  71.5 170.9  -.2      -8.0    -8   1  7  14600  16 54 30
16 56 00  ---          20 21 45  71.5 172.1  -.2      -7.0    82   F  1  15200
  
16 56 00  2016+112     20 21 45  70.8 181.8   .0       1.6    -8   1  7  15200  16 56 00
17 00 30  ---          20 26 16  70.8 185.1   .1       4.5   262   F  1  17000
  
17 00 30  2029+121     20 26 16  71.6 175.6  -.1      -3.9    -8   1  7  17000  17 00 30
17 02 00  ---          20 27 46  71.7 176.7  -.1      -2.9    82   F  1  17600
  
17 04 00  2029+121     20 29 46  71.7 178.3   .0      -1.5   117   1  8  17600  17 04 00
17 06 00  ---          20 31 47  71.7 179.8   .0       -.1   120   R  1  16800
  
17 06 00  2016+112     20 31 47  70.6 189.2   .2       8.1    -8   1  8  16800  17 06 00
17 10 30  ---          20 36 17  70.4 192.5   .3      10.9   262   R  1  15000
  
17 10 30  2029+121     20 36 17  71.7 183.3   .1       2.9    -8   1  8  15000  17 10 30
17 12 00  ---          20 37 48  71.6 184.5   .1       4.0    82   R  1  14400
  
17 12 00  2016+112     20 37 48  70.4 193.5   .3      11.9    -8   1  8  14400  17 12 00
17 16 30  ---          20 42 18  70.1 196.7   .4      14.6   262   R  1  12600
  
17 16 30  2029+121     20 42 18  71.5 188.0   .2       7.0    -8   1  8  12600  17 16 30
17 18 00  ---          20 43 49  71.5 189.1   .2       8.0    82   R  1  12000
  
17 18 00  2016+112     20 43 49  70.0 197.8   .4      15.5    -8   1  8  12000  17 18 00
17 22 30  ---          20 48 19  69.7 200.8   .5      18.2   262   R  1  10200
  
17 22 30  2029+121     20 48 19  71.3 192.5   .3      11.0    -8   1  8  10200  17 22 30
17 24 00  ---          20 49 50  71.2 193.7   .3      12.0    82   R  1   9600
  
17 24 00  2016+112     20 49 50  69.6 201.8   .5      19.1    -7   1  8   9600  17 24 00
17 28 30  ---          20 54 20  69.2 204.8   .6      21.6   263   R  1   7800
  
17 28 30  2029+121     20 54 20  71.0 197.0   .4      14.9    -7   1  8   7800  17 28 30
17 30 00  ---          20 55 51  70.9 198.1   .4      15.8    83   R  1   7200
  
17 30 00  2016+112     20 55 51  69.0 205.7   .6      22.4    -7   1  8   7200  17 30 00
17 34 30  ---          21 00 21  68.6 208.5   .7      24.8   263   R  1   5400
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
17 34 30  2029+121     21 00 21  70.6 201.2   .5      18.6    -7   1  8   5400  17 34 30
17 36 00  ---          21 01 52  70.4 202.3   .5      19.5    83   R  1   4800
  
17 36 00  2016+112     21 01 52  68.4 209.5   .7      25.6    -7   1  8   4800  17 36 00
17 40 30  ---          21 06 22  67.9 212.1   .8      27.8   263   R  1   3000
  
17 40 30  2029+121     21 06 22  70.0 205.3   .6      22.1    -7   1  8   3000  17 40 30
17 42 00  ---          21 07 52  69.9 206.3   .6      23.0    83   R  1   2400
  
17 42 00  2016+112     21 07 52  67.8 213.0   .8      28.5    -6   1  8   2400  17 42 00
17 46 30  ---          21 12 23  67.2 215.5   .9      30.6   264   R  1    600
  
17 46 30  2029+121     21 12 23  69.5 209.2   .7      25.5    -6   1  8    600  17 46 30
17 48 00  ---          21 13 53  69.3 210.2   .7      26.3    84   R  1      0
  
17 50 00  2029+121     21 15 54  69.1 211.4   .7      27.3   117   1  9      0  17 50 00
17 58 00  ---          21 23 55  68.1 216.1   .9      31.2   480   F  1   3200
  
17 58 00  2016+112     21 23 55  65.7 221.4  1.1      35.5    -7   1  9   3200  17 58 00
18 02 30  ---          21 28 26  65.0 223.5  1.2      37.2   263   F  1   5000
  
18 02 30  2029+121     21 28 26  67.5 218.5   .9      33.3    -7   1  9   5000  18 02 30
18 04 00  ---          21 29 56  67.3 219.3  1.0      33.9    83   F  1   5600
  
18 04 00  2016+112     21 29 56  64.8 224.2  1.2      37.8    -7   1  9   5600  18 04 00
18 08 30  ---          21 34 27  64.1 226.2  1.3      39.4   263   F  1   7400
  
18 08 30  2029+121     21 34 27  66.7 221.7  1.0      35.8    -7   1  9   7400  18 08 30
18 10 00  ---          21 35 57  66.5 222.4  1.1      36.4    83   F  1   8000
  
18 10 00  2016+112     21 35 57  63.9 226.9  1.3      39.9    -7   1  9   8000  18 10 00
18 14 30  ---          21 40 28  63.2 228.8  1.4      41.3   263   F  1   9800
  
18 14 30  2029+121     21 40 28  65.8 224.6  1.1      38.2    -7   1  9   9800  18 14 30
18 16 00  ---          21 41 58  65.6 225.3  1.2      38.7    83   F  1  10400
  
18 16 00  2016+112     21 41 58  62.9 229.4  1.4      41.8    -7   1  9  10400  18 16 00
18 20 30  ---          21 46 29  62.2 231.2  1.5      43.1   263   F  1  12200
  
18 20 30  2029+121     21 46 29  64.9 227.3  1.2      40.3    -7   1  9  12200  18 20 30
18 22 00  ---          21 47 59  64.6 227.9  1.3      40.8    83   F  1  12800
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
18 22 00  2016+112     21 47 59  61.9 231.7  1.5      43.6    -7   1  9  12800  18 22 00
18 26 30  ---          21 52 30  61.1 233.4  1.6      44.8   263   F  1  14600
  
18 26 30  2029+121     21 52 30  63.9 229.8  1.3      42.3    -8   1  9  14600  18 26 30
18 28 00  ---          21 54 00  63.7 230.5  1.4      42.8    82   F  1  15200
  
18 28 00  2016+112     21 54 00  60.9 233.9  1.6      45.2    -8   1  9  15200  18 28 00
18 32 30  ---          21 58 31  60.1 235.5  1.7      46.3   262   F  1  17000
  
18 32 30  2029+121     21 58 31  62.9 232.2  1.4      44.1    -8   1  9  17000  18 32 30
18 34 00  ---          22 00 01  62.6 232.8  1.5      44.6    82   F  1  17600
  
18 36 00  2029+121     22 02 01  62.3 233.6  1.5      45.1   117   1 10  17600  18 36 00
18 38 00  ---          22 04 02  61.9 234.3  1.5      45.7   120   R  1  16800
  
18 38 00  2016+112     22 04 02  59.1 237.3  1.7      47.6    -8   1 10  16800  18 38 00
18 42 30  ---          22 08 32  58.3 238.7  1.8      48.6   262   R  1  15000
  
18 42 30  2029+121     22 08 32  61.2 235.9  1.6      46.8    -8   1 10  15000  18 42 30
18 44 00  ---          22 10 03  60.9 236.4  1.6      47.2    82   R  1  14400
  
18 44 00  2016+112     22 10 03  58.0 239.2  1.8      48.9    -8   1 10  14400  18 44 00
18 48 30  ---          22 14 33  57.2 240.5  1.9      49.8   262   R  1  12600
  
18 48 30  2029+121     22 14 33  60.1 237.9  1.7      48.3    -8   1 10  12600  18 48 30
18 50 00  ---          22 16 04  59.8 238.4  1.7      48.6    82   R  1  12000
  
18 50 00  2016+112     22 16 04  56.9 241.0  1.9      50.1    -8   1 10  12000  18 50 00
18 54 30  ---          22 20 34  56.0 242.2  2.0      51.0   262   R  1  10200
  
18 54 30  2029+121     22 20 34  59.0 239.8  1.8      49.6    -8   1 10  10200  18 54 30
18 56 00  ---          22 22 05  58.7 240.3  1.8      49.9    82   R  1   9600
  
18 56 00  2016+112     22 22 05  55.7 242.7  2.0      51.2    -8   1 10   9600  18 56 00
19 00 30  ---          22 26 35  54.9 243.9  2.1      52.0   262   R  1   7800
  
19 00 30  2029+121     22 26 35  57.8 241.6  1.9      50.8    -8   1 10   7800  19 00 30
19 02 00  ---          22 28 06  57.5 242.1  1.9      51.1    82   R  1   7200
  
19 02 00  2016+112     22 28 06  54.6 244.2  2.1      52.3    -8   1 10   7200  19 02 00
19 06 30  ---          22 32 36  53.7 245.4  2.2      53.0   262   R  1   5400
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
19 06 30  2029+121     22 32 36  56.7 243.3  2.0      51.9    -8   1 10   5400  19 06 30
19 08 00  ---          22 34 07  56.4 243.7  2.0      52.2    82   R  1   4800
  
19 08 00  2016+112     22 34 07  53.4 245.8  2.2      53.2    -8   1 10   4800  19 08 00
19 12 30  ---          22 38 37  52.5 246.9  2.3      53.8   262   R  1   3000
  
19 12 30  2029+121     22 38 37  55.5 244.9  2.1      52.9    -8   1 10   3000  19 12 30
19 14 00  ---          22 40 08  55.2 245.3  2.1      53.2    82   R  1   2400
  
19 14 00  2016+112     22 40 08  52.2 247.2  2.3      54.0    -8   1 10   2400  19 14 00
19 18 30  ---          22 44 38  51.3 248.3  2.4      54.6   262   R  1    600
  
19 18 30  2029+121     22 44 38  54.3 246.4  2.2      53.8    -8   1 10    600  19 18 30
19 20 00  ---          22 46 09  54.0 246.8  2.2      54.1    82   R  1      0
  
19 22 00  2029+121     22 48 09  53.6 247.3  2.3      54.3   117   1 11      0  19 22 00
19 24 00  ---          22 50 09  53.2 247.8  2.3      54.6   120   F  1    800
  
19 24 00  2016+112     22 50 09  50.2 249.5  2.5      55.3    -8   1 11    800  19 24 00
19 28 30  ---          22 54 40  49.3 250.5  2.6      55.8   262   F  1   2600
  
19 28 30  2029+121     22 54 40  52.3 248.8  2.4      55.2    -8   1 11   2600  19 28 30
19 30 00  ---          22 56 10  52.0 249.2  2.4      55.4    82   F  1   3200
  
19 30 00  2016+112     22 56 10  49.0 250.8  2.6      56.0    -8   1 11   3200  19 30 00
19 34 30  ---          23 00 41  48.1 251.7  2.7      56.5   262   F  1   5000
  
19 34 30  2029+121     23 00 41  51.1 250.2  2.5      55.9    -8   1 11   5000  19 34 30
19 36 00  ---          23 02 11  50.8 250.5  2.5      56.1    82   F  1   5600
  
19 36 00  2016+112     23 02 11  47.8 252.0  2.7      56.6    -8   1 11   5600  19 36 00
19 40 30  ---          23 06 42  46.8 252.9  2.8      57.0   262   F  1   7400
  
19 40 30  2029+121     23 06 42  49.9 251.5  2.6      56.6    -8   1 11   7400  19 40 30
19 42 00  ---          23 08 12  49.6 251.8  2.6      56.8    82   F  1   8000
  
19 42 00  2016+112     23 08 12  46.5 253.2  2.8      57.2    -8   1 11   8000  19 42 00
19 46 30  ---          23 12 43  45.6 254.0  2.9      57.6   262   F  1   9800
  
19 46 30  2029+121     23 12 43  48.7 252.7  2.7      57.2    -8   1 11   9800  19 46 30
19 48 00  ---          23 14 13  48.4 253.0  2.7      57.4    82   F  1  10400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
19 48 00  2016+112     23 14 13  45.3 254.3  2.9      57.7    -8   1 11  10400  19 48 00
19 52 30  ---          23 18 44  44.4 255.2  3.0      58.1   262   F  1  12200
  
19 52 30  2029+121     23 18 44  47.4 253.9  2.8      57.8    -8   1 11  12200  19 52 30
19 54 00  ---          23 20 14  47.1 254.2  2.8      57.9    82   F  1  12800
  
19 54 00  2016+112     23 20 14  44.0 255.4  3.0      58.2    -8   1 11  12800  19 54 00
19 58 30  ---          23 24 45  43.1 256.2  3.1      58.5   262   F  1  14600
  
19 58 30  2029+121     23 24 45  46.2 255.0  2.9      58.3    -8   1 11  14600  19 58 30
20 00 00  ---          23 26 15  45.9 255.3  2.9      58.4    82   F  1  15200
  
20 00 00  2016+112     23 26 15  42.8 256.5  3.1      58.6    -8   1 11  15200  20 00 00
20 04 30  ---          23 30 46  41.8 257.3  3.2      58.9   262   F  1  17000
  
20 04 30  2029+121     23 30 46  44.9 256.1  3.0      58.8    -8   1 11  17000  20 04 30
20 06 00  ---          23 32 16  44.6 256.4  3.0      58.9    82   F  1  17600
  
20 08 00  2029+121     23 34 16  44.2 256.7  3.0      59.0   117   1 12  17600  20 08 00
20 10 00  ---          23 36 17  43.8 257.1  3.1      59.1   120   R  1  16800
  
20 10 00  2016+112     23 36 17  40.7 258.2  3.3      59.2    -8   1 12  16800  20 10 00
20 14 30  ---          23 40 48  39.7 258.9  3.4      59.5   262   R  1  15000
  
20 14 30  2029+121     23 40 48  42.8 257.8  3.1      59.4    -8   1 12  15000  20 14 30
20 16 00  ---          23 42 18  42.5 258.1  3.2      59.5    82   R  1  14400
  
20 16 00  2016+112     23 42 18  39.4 259.2  3.4      59.6    -8   1 12  14400  20 16 00
20 20 30  ---          23 46 49  38.5 259.9  3.5      59.8   262   R  1  12600
  
20 20 30  2029+121     23 46 49  41.6 258.8  3.2      59.8    -8   1 12  12600  20 20 30
20 22 00  ---          23 48 19  41.3 259.1  3.3      59.9    82   R  1  12000
  
20 22 00  2016+112     23 48 19  38.1 260.1  3.5      59.9    -8   1 12  12000  20 22 00
20 26 30  ---          23 52 50  37.2 260.8  3.6      60.1   262   R  1  10200
  
20 26 30  2029+121     23 52 50  40.3 259.8  3.3      60.1    -8   1 12  10200  20 26 30
20 28 00  ---          23 54 20  40.0 260.1  3.4      60.2    82   R  1   9600
  
20 28 00  2016+112     23 54 20  36.9 261.0  3.6      60.1    -8   1 12   9600  20 28 00
20 32 30  ---          23 58 51  35.9 261.7  3.7      60.3   262   R  1   7800
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
20 32 30  2029+121     23 58 51  39.0 260.8  3.4      60.4    -8   1 12   7800  20 32 30
20 34 00  ---          00 00 21  38.7 261.0  3.5      60.4    82   R  1   7200
  
20 34 00  2016+112     00 00 21  35.6 262.0  3.7      60.4    -8   1 12   7200  20 34 00
20 38 30  ---          00 04 51  34.6 262.6  3.8      60.5   262   R  1   5400
  
20 38 30  2029+121     00 04 51  37.7 261.7  3.5      60.6    -8   1 12   5400  20 38 30
20 40 00  ---          00 06 22  37.4 261.9  3.6      60.7    82   R  1   4800
  
20 40 00  2016+112     00 06 22  34.3 262.8  3.8      60.6    -8   1 12   4800  20 40 00
20 44 30  ---          00 10 52  33.3 263.5  3.9      60.7   262   R  1   3000
  
20 44 30  2029+121     00 10 52  36.5 262.6  3.6      60.9    -8   1 12   3000  20 44 30
20 46 00  ---          00 12 23  36.1 262.8  3.7      60.9    82   R  1   2400
  
20 46 00  2016+112     00 12 23  33.0 263.7  3.9      60.8    -8   1 12   2400  20 46 00
20 50 30  ---          00 16 53  32.1 264.3  4.0      60.9   262   R  1    600
  
20 50 30  2029+121     00 16 53  35.2 263.5  3.7      61.0    -8   1 12    600  20 50 30
20 52 00  ---          00 18 24  34.9 263.7  3.8      61.1    82   R  1      0
  
20 54 00  2029+121     00 20 24  34.4 264.0  3.8      61.1   117   1 13      0  20 54 00
20 56 00  ---          00 22 24  34.0 264.3  3.8      61.2   120   F  1    800
  
20 56 00  2016+112     00 22 24  30.9 265.1  4.1      61.0    -8   1 13    800  20 56 00
21 00 30  ---          00 26 55  29.9 265.7  4.1      61.1   262   F  1   2600
  
21 00 30  2029+121     00 26 55  33.0 264.9  3.9      61.3    -8   1 13   2600  21 00 30
21 02 00  ---          00 28 25  32.7 265.1  3.9      61.3    82   F  1   3200
  
21 02 00  2016+112     00 28 25  29.6 265.9  4.2      61.1    -8   1 13   3200  21 02 00
21 06 30  ---          00 32 56  28.6 266.6  4.2      61.2   262   F  1   5000
  
21 06 30  2029+121     00 32 56  31.7 265.7  4.0      61.4    -8   1 13   5000  21 06 30
21 08 00  ---          00 34 26  31.4 265.9  4.0      61.5    82   F  1   5600
  
21 08 00  2016+112     00 34 26  28.3 266.8  4.3      61.2    -8   1 13   5600  21 08 00
21 12 30  ---          00 38 57  27.3 267.4  4.3      61.3   262   F  1   7400
  
21 12 30  2029+121     00 38 57  30.5 266.5  4.1      61.5    -8   1 13   7400  21 12 30
21 14 00  ---          00 40 27  30.1 266.7  4.1      61.6    82   F  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GLOBAL-18cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Mon  25 Feb 2002   Day  56 ---
  
21 14 00  2016+112     00 40 27  27.0 267.6  4.4      61.3    -8   1 13   8000  21 14 00
21 18 30  ---          00 44 58  26.0 268.1  4.4      61.3   262   F  1   9800
  
21 18 30  2029+121     00 44 58  29.2 267.4  4.2      61.6    -8   1 13   9800  21 18 30
21 20 00  ---          00 46 28  28.8 267.6  4.2      61.6    82   F  1  10400
  
21 20 00  2016+112     00 46 28  25.7 268.3  4.5      61.3    -8   1 13  10400  21 20 00
21 24 30  ---          00 50 59  24.7 268.9  4.5      61.4   262   F  1  12200
  
21 24 30  2029+121     00 50 59  27.9 268.1  4.3      61.7    -8   1 13  12200  21 24 30
21 30 00  ---          00 56 30  26.7 268.9  4.4      61.7   322   F  1  14400
 
 
SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.
 
 
 Setup file: gp030b.18cm
   Matches group v20cm_2 in /homes/p062gra/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.
 
   Setup group:    9         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00
 
   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00
 
   1st LO=   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U
   Pol.  =      LCP       LCP       LCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         L         L
   IF    =        C         C         C         C 
 
   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4
 
  The following frequency sets based on this setup were used.
 
   Frequency Set:   9  Setup file default.  Used pcal sets:   1
   LO sum=    1642.49   1650.49   1658.49   1666.49
   BBC fr=     757.51    749.51    741.51    733.51
   Bandwd=      8.000     8.000     8.000     8.000
 
  The following pulse cal sets were used with this setup:
 
   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=   510   510  6510  6510     0     0     0     0
    PCALFR2=   510   510  6510  6510     0     0     0     0
 
   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- GLOBAL-18cm-2016+112
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
  
   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 
  
 * 2016+112          20 16 55.366162   * 20 19 18.080000     20 19 22.160639   
                     11 17 44.94038    * 11 27 12.96000      11 27 23.59141    
                     From catalog imbedded in main SCHED input file.
 
 * 2029+121          20 29 32.681203   * 20 31 54.994210     20 31 59.021417   
                     12 09 28.75325    * 12 19 41.34040      12 19 53.73835    
                     From catalog imbedded in main SCHED input file.
 
 * 2134+004          21 34 05.207365   * 21 36 38.586300     21 36 42.947869   
                     00 28 25.08052    * 00 41 54.21335      00 42 15.69146    
                     From catalog imbedded in main SCHED input file.
 
 
 
  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   2016+112            39.2
   2029+121            37.1
   2134+004            17.3
 
  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

