  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: High-resolution, multi-frequency mapping of the compact sources in M82
 Exp. Code:  GF019A  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       D. Fenech

Address:  Department of Physics and Astronomy
          University College London
          Gower street, London, WC1E 6BT
          United Kingdom

Phone:    +44 (0)20 7679 7682
EMAIL:    dmf@star.ucl.ac.uk
Fax:      +44 (0)20 7679 7145
Phone during observation: +44 (0)7791 563887

Observing mode: Phase-referencing of M82 at 6cm (512 Mb/s)

Notes:    Lovell telescope missing alternate phase reference scans to keep slewing rate down.
          Phase-cal is switched off for GF019 observation.
          Use of a single WSRT antenna required instead of the full array
          Effelsberg gaps included for pointing checks

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

 Next scan frequencies:  4924.25  4924.25  4940.25  4940.25  4956.25  4956.25  4972.25  4972.25
 Next BBC frequencies:    824.25   824.25   840.25   840.25   856.25   856.25   872.25   872.25
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

00 00 00  J0958+65     02 57 46  21.6  25.5 -7.0     -63.0     0        0   00 00 00
00 02 30  ---          03 00 17  21.8  25.6 -7.0     -63.6   150       10   00 00 01

00 02 30  M82PTCEN     03 00 17  23.8  21.7 -6.9     -65.7   -12       10   00 02 42
00 07 20  ---          03 05 08  24.2  21.9 -6.9     -66.8   278       28   00 02 31

00 07 50  J0958+65     03 05 38  22.3  25.8 -6.9     -64.7    18       28   00 07 50
00 10 30  ---          03 08 18  22.6  26.0 -6.9     -65.2   160       38   00 07 51

00 10 30  M82PTCEN     03 08 18  24.5  22.0 -6.8     -67.5   -12       38   00 10 42
00 15 20  ---          03 13 09  24.9  22.2 -6.7     -68.6   278       56   00 10 31

00 15 50  J0958+65     03 13 39  23.1  26.2 -6.8     -66.4    18       56   00 15 50
00 18 30  ---          03 16 19  23.3  26.3 -6.7     -66.9   160       66   00 15 51

00 24 24  3C84         03 22 15  79.1  -1.4  0.0     178.4   237       66   00 24 24
00 30 24  ---          03 28 16  79.0  -7.2  0.1     171.7   360       89   00 24 25

00 35 24  J0958+65     03 33 16  25.0  27.0 -6.4     -70.5   185       89   00 35 24
00 37 54  ---          03 35 47  25.2  27.1 -6.4     -71.0   150       99   00 35 25

00 50 05  J0927+39     03 47 59  22.2  56.8 -5.7     -67.8   702       99   00 50 05
00 56 05  ---          03 54 00  23.3  57.3 -5.6     -68.6   360      122   00 50 06

01 00 05  J0958+65     03 58 01  27.4  27.9 -6.0     -75.8   211      122   01 00 05
01 02 35  ---          04 00 31  27.7  27.9 -6.0     -76.3   150      132   01 00 06

01 02 35  M82PTCEN     04 00 31  28.8  23.4 -5.9     -79.1   -11      132   01 02 46
01 07 10  ---          04 05 07  29.2  23.5 -5.9     -80.1   264      149   01 02 36

01 08 05  J0958+65     04 06 02  28.2  28.1 -5.9     -77.5    44      149   01 08 05
01 10 35  ---          04 08 33  28.5  28.1 -5.9     -78.0   150      158   01 08 06

01 10 35  M82PTCEN     04 08 33  29.5  23.6 -5.8     -80.9   -11      158   01 10 46
01 15 10  ---          04 13 08  29.9  23.6 -5.7     -81.9   264      175   01 10 36

01 16 05  J0958+65     04 14 04  29.0  28.3 -5.8     -79.2    44      175   01 16 05
01 18 35  ---          04 16 34  29.3  28.3 -5.7     -79.8   150      185   01 16 06

01 18 35  M82PTCEN     04 16 34  30.2  23.7 -5.7     -82.7   -11      185   01 18 46
01 23 10  ---          04 21 10  30.6  23.7 -5.6     -83.8   264      202   01 18 36
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

01 24 05  J0958+65     04 22 05  29.9  28.4 -5.6     -81.0    44      202   01 24 05
01 26 35  ---          04 24 35  30.1  28.5 -5.6     -81.5   150      212   01 24 06

01 26 35  M82PTCEN     04 24 35  30.9  23.8 -5.5     -84.5   -11      212   01 26 46
01 31 10  ---          04 29 11  31.3  23.8 -5.5     -85.6   264      229   01 26 36

01 32 05  J0958+65     04 30 06  30.7  28.6 -5.5     -82.7    44      229   01 32 05
01 34 35  ---          04 32 37  30.9  28.6 -5.5     -83.3   150      238   01 32 06

01 34 35  M82PTCEN     04 32 37  31.6  23.8 -5.4     -86.4   -11      238   01 34 46
01 39 10  ---          04 37 12  32.0  23.9 -5.3     -87.5   264      255   01 34 36

01 40 05  J0958+65     04 38 07  31.5  28.7 -5.4     -84.5    44      255   01 40 05
01 42 35  ---          04 40 38  31.8  28.7 -5.3     -85.0   150      265   01 40 06

01 42 35  M82PTCEN     04 40 38  32.3  23.9 -5.3     -88.3   -11      265   01 42 46
01 47 10  ---          04 45 14  32.7  23.9 -5.2     -89.3   264      282   01 42 36

01 48 05  J0958+65     04 46 09  32.3  28.8 -5.2     -86.3    44      282   01 48 05
01 50 35  ---          04 48 39  32.6  28.8 -5.2     -86.8   150      292   01 48 06

01 50 35  M82PTCEN     04 48 39  33.0  23.9 -5.1     -90.1   -11      292   01 50 46
01 55 10  ---          04 53 15  33.4  23.9 -5.1     -91.2   264      309   01 50 36

01 56 05  J0958+65     04 54 10  33.2  28.8 -5.1     -88.1    44      309   01 56 05
01 58 35  ---          04 56 41  33.4  28.8 -5.1     -88.6   150      318   01 56 06

01 58 35  M82PTCEN     04 56 41  33.7  23.9 -5.0     -92.0   -11      318   01 58 46
02 03 10  ---          05 01 16  34.1  23.9 -4.9     -93.1   264      335   01 58 36

02 04 05  J0958+65     05 02 11  34.0  28.8 -5.0     -89.9    44      335   02 04 05
02 06 35  ---          05 04 42  34.3  28.8 -4.9     -90.5   150      345   02 04 06

02 06 35  M82PTCEN     05 04 42  34.4  23.8 -4.9     -93.9   -11      345   02 06 46
02 11 10  ---          05 09 18  34.8  23.8 -4.8     -95.0   264      362   02 06 36

02 12 05  J0958+65     05 10 13  34.8  28.8 -4.8     -91.7    44      362   02 12 05
02 14 35  ---          05 12 43  35.1  28.8 -4.8     -92.3   150      372   02 12 06

02 14 35  M82PTCEN     05 12 43  35.1  23.8 -4.7     -95.8   -11      372   02 14 46
02 19 10  ---          05 17 19  35.5  23.7 -4.7     -96.9   264      389   02 14 36

02 20 05  J0958+65     05 18 14  35.7  28.8 -4.7     -93.6    44      389   02 20 05
02 22 35  ---          05 20 44  35.9  28.7 -4.7     -94.1   150      398   02 20 06
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

02 22 35  M82PTCEN     05 20 44  35.8  23.7 -4.6     -97.8   -11      398   02 22 46
02 27 10  ---          05 25 20  36.2  23.6 -4.5     -98.9   264      415   02 22 36

02 28 05  J0958+65     05 26 15  36.5  28.7 -4.6     -95.4    43      415   02 28 05
02 30 35  ---          05 28 46  36.8  28.7 -4.5     -96.0   150      425   02 28 06

02 30 35  M82PTCEN     05 28 46  36.5  23.5 -4.5     -99.7   -12      425   02 30 46
02 35 10  ---          05 33 22  36.9  23.4 -4.4    -100.9   263      442   02 30 36

02 36 05  J0958+65     05 34 17  37.3  28.6 -4.4     -97.3    43      442   02 36 05
02 38 35  ---          05 36 47  37.6  28.5 -4.4     -97.9   150      452   02 36 06

02 38 35  M82PTCEN     05 36 47  37.1  23.4 -4.3    -101.7   -12      452   02 38 46
02 43 10  ---          05 41 23  37.5  23.3 -4.3    -102.9   263      469   02 38 36

02 44 05  J0958+65     05 42 18  38.1  28.4 -4.3     -99.2    43      469   02 44 05
02 46 35  ---          05 44 48  38.4  28.4 -4.3     -99.9   150      478   02 44 06

02 46 35  M82PTCEN     05 44 48  37.8  23.2 -4.2    -103.7   -12      478   02 46 46
02 51 10  ---          05 49 24  38.2  23.1 -4.1    -104.9   263      495   02 46 36

02 52 05  J0958+65     05 50 19  39.0  28.2 -4.2    -101.2    43      495   02 52 05
02 54 35  ---          05 52 50  39.2  28.2 -4.1    -101.8   150      505   02 52 06

02 54 35  M82PTCEN     05 52 50  38.5  23.0 -4.1    -105.7   -12      505   02 54 46
02 59 10  ---          05 57 25  38.9  22.8 -4.0    -106.9   263      522   02 54 36

03 00 05  J0958+65     05 58 21  39.8  28.0 -4.0    -103.2    43      522   03 00 05
03 02 35  ---          06 00 51  40.0  27.9 -4.0    -103.8   150      532   03 00 06

03 02 35  M82PTCEN     06 00 51  39.2  22.7 -3.9    -107.8   -12      532   03 02 46
03 07 10  ---          06 05 27  39.6  22.5 -3.9    -109.0   263      548   03 02 36

03 08 05  J0958+65     06 06 22  40.6  27.7 -3.9    -105.2    43      548   03 08 05
03 10 35  ---          06 08 52  40.8  27.6 -3.9    -105.8   150      558   03 08 06

03 10 35  M82PTCEN     06 08 52  39.8  22.4 -3.8    -109.8   -12      558   03 10 46
03 15 10  ---          06 13 28  40.2  22.2 -3.7    -111.0   263      575   03 10 36

03 16 05  J0958+65     06 14 23  41.4  27.4 -3.8    -107.2    43      575   03 16 05
03 18 35  ---          06 16 54  41.6  27.3 -3.7    -107.8   150      585   03 16 06

03 18 35  M82PTCEN     06 16 54  40.5  22.1 -3.7    -111.9   -12      585   03 18 46
03 23 10  ---          06 21 29  40.9  21.9 -3.6    -113.1   263      602   03 18 36
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

03 24 05  J0958+65     06 22 25  42.2  27.1 -3.6    -109.2    43      602   03 24 05
03 26 35  ---          06 24 55  42.4  27.0 -3.6    -109.9   150      611   03 24 06

03 26 35  M82PTCEN     06 24 55  41.1  21.7 -3.5    -114.0   -12      611   03 26 46
03 31 10  ---          06 29 31  41.5  21.5 -3.5    -115.3   263      628   03 26 36

03 32 05  J0958+65     06 30 26  43.0  26.7 -3.5    -111.3    43      628   03 32 05
03 34 35  ---          06 32 56  43.2  26.6 -3.5    -112.0   150      638   03 32 06

03 34 35  M82PTCEN     06 32 56  41.8  21.3 -3.4    -116.2   -12      638   03 34 46
03 39 10  ---          06 37 32  42.1  21.1 -3.3    -117.4   263      655   03 34 36

03 40 05  J0958+65     06 38 27  43.7  26.3 -3.4    -113.5    43      655   03 40 05
03 42 35  ---          06 40 58  44.0  26.1 -3.3    -114.1   150      665   03 40 06

03 42 35  M82PTCEN     06 40 58  42.4  20.9 -3.3    -118.4   -12      665   03 42 46
03 47 10  ---          06 45 33  42.7  20.6 -3.2    -119.6   263      681   03 42 36

03 48 05  J0958+65     06 46 29  44.5  25.8 -3.2    -115.6    43      681   03 48 05
03 50 35  ---          06 48 59  44.7  25.6 -3.2    -116.3   150      691   03 48 06

03 50 35  M82PTCEN     06 48 59  43.0  20.4 -3.1    -120.5   -12      691   03 50 46
03 55 10  ---          06 53 35  43.3  20.1 -3.1    -121.8   263      708   03 50 36

03 56 05  J0958+65     06 54 30  45.2  25.2 -3.1    -117.8    43      708   03 56 05
03 58 35  ---          06 57 00  45.5  25.1 -3.1    -118.5   150      718   03 56 06

03 58 35  M82PTCEN     06 57 00  43.6  19.9 -3.0    -122.8   -12      718   03 58 46
04 03 10  ---          07 01 36  43.9  19.6 -2.9    -124.1   263      735   03 58 36

04 04 05  J0958+65     07 02 31  46.0  24.7 -3.0    -120.0    43      735   04 04 05
04 06 35  ---          07 05 02  46.2  24.5 -2.9    -120.8   150      744   04 04 06

04 06 35  M82PTCEN     07 05 02  44.2  19.4 -2.9    -125.0   -12      744   04 06 47
04 11 10  ---          07 09 37  44.5  19.0 -2.8    -126.3   263      761   04 06 36

04 12 05  J0958+65     07 10 32  46.7  24.0 -2.8    -122.3    43      761   04 12 05
04 14 35  ---          07 13 03  46.9  23.8 -2.8    -123.0   150      771   04 12 06

04 14 35  M82PTCEN     07 13 03  44.7  18.8 -2.7    -127.3   -12      771   04 14 47
04 19 10  ---          07 17 39  45.0  18.4 -2.7    -128.6   263      788   04 14 36

04 20 05  J0958+65     07 18 34  47.4  23.4 -2.7    -124.6    43      788   04 20 05
04 22 35  ---          07 21 04  47.6  23.2 -2.6    -125.4   150      798   04 20 06
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

04 22 35  M82PTCEN     07 21 04  45.3  18.2 -2.6    -129.6   -13      798   04 22 47
04 27 10  ---          07 25 40  45.6  17.8 -2.5    -131.0   262      814   04 22 36

04 28 05  J0958+65     07 26 35  48.0  22.7 -2.6    -127.0    42      814   04 28 05
04 30 35  ---          07 29 06  48.2  22.4 -2.5    -127.7   150      824   04 28 06

04 30 35  M82PTCEN     07 29 06  45.8  17.5 -2.5    -132.0   -13      824   04 30 48
04 35 15  ---          07 33 46  46.1  17.1 -2.4    -133.4   267      841   04 30 36

04 36 05  J0958+65     07 34 36  48.7  21.9 -2.4    -129.4    37      841   04 36 05
04 38 35  ---          07 37 07  48.9  21.6 -2.4    -130.2   150      851   04 36 06

04 38 35  M82PTCEN     07 37 07  46.3  16.8 -2.3    -134.4   -13      851   04 38 48
04 43 15  ---          07 41 48  46.6  16.4 -2.3    -135.8   267      868   04 38 36

04 44 05  J0958+65     07 42 38  49.3  21.1 -2.3    -131.8    37      868   04 44 05
04 46 35  ---          07 45 08  49.5  20.8 -2.2    -132.6   150      878   04 44 06

04 46 35  M82PTCEN     07 45 08  46.8  16.1 -2.2    -136.8   -13      878   04 46 48
04 51 15  ---          07 49 49  47.1  15.7 -2.1    -138.2   267      895   04 46 36

04 52 05  J0958+65     07 50 39  49.9  20.2 -2.2    -134.3    36      895   04 52 05
04 54 35  ---          07 53 09  50.1  19.9 -2.1    -135.1   150      905   04 52 06

04 54 35  M82PTCEN     07 53 09  47.3  15.4 -2.1    -139.2   -14      905   04 54 48
04 59 15  ---          07 57 50  47.5  14.9 -2.0    -140.6   266      922   04 54 36

05 00 05  J0958+65     07 58 40  50.5  19.2 -2.0    -136.9    36      922   05 00 05
05 02 35  ---          08 01 11  50.7  18.9 -2.0    -137.7   150      931   05 00 06

05 02 35  M82PTCEN     08 01 11  47.7  14.6 -1.9    -141.7   -14      931   05 02 49
05 07 15  ---          08 05 52  48.0  14.1 -1.9    -143.1   266      949   05 02 36

05 08 05  J0958+65     08 06 42  51.1  18.3 -1.9    -139.5    36      949   05 08 05
05 10 35  ---          08 09 12  51.2  17.9 -1.8    -140.3   150      958   05 08 06

05 10 35  M82PTCEN     08 09 12  48.1  13.7 -1.8    -144.2   -14      958   05 10 49
05 15 15  ---          08 13 53  48.4  13.2 -1.7    -145.6   266      975   05 10 36

05 16 05  J0958+65     08 14 43  51.6  17.2 -1.8    -142.1    36      975   05 16 05
05 18 35  ---          08 17 13  51.8  16.9 -1.7    -142.9   150      985   05 16 06

05 18 35  M82PTCEN     08 17 13  48.5  12.9 -1.7    -146.7   -14      985   05 18 49
05 23 15  ---          08 21 54  48.8  12.3 -1.6    -148.2   266     1002   05 18 36
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

05 24 05  J0958+65     08 22 44  52.1  16.2 -1.6    -144.8    36     1002   05 24 05
05 26 35  ---          08 25 15  52.2  15.8 -1.6    -145.6   150     1012   05 24 06

05 26 35  M82PTCEN     08 25 15  48.9  12.0 -1.5    -149.2   -15     1012   05 26 49
05 31 15  ---          08 29 55  49.1  11.4 -1.5    -150.7   265     1029   05 26 36

05 32 05  J0958+65     08 30 46  52.6  15.0 -1.5    -147.5    35     1029   05 32 05
05 34 35  ---          08 33 16  52.7  14.7 -1.4    -148.4   150     1039   05 32 06

05 34 35  M82PTCEN     08 33 16  49.3  11.0 -1.4    -151.8   -15     1039   05 34 50
05 39 15  ---          08 37 57  49.4  10.5 -1.3    -153.3   265     1056   05 34 36

05 40 05  J0958+65     08 38 47  53.0  13.8 -1.4    -150.3    35     1056   05 40 05
05 42 35  ---          08 41 17  53.1  13.5 -1.3    -151.1   150     1065   05 40 06

05 42 35  M82PTCEN     08 41 17  49.6  10.1 -1.3    -154.4   -15     1065   05 42 50
05 47 15  ---          08 45 58  49.7   9.5 -1.2    -156.0   265     1082   05 42 36

05 48 05  J0958+65     08 46 48  53.4  12.6 -1.2    -153.1    35     1082   05 48 05
05 50 35  ---          08 49 19  53.5  12.2 -1.2    -153.9   150     1092   05 48 06

05 50 35  M82PTCEN     08 49 19  49.9   9.1 -1.1    -157.1   -15     1092   05 50 50
05 55 15  ---          08 53 59  50.0   8.5 -1.1    -158.6   265     1109   05 50 36

05 56 05  J0958+65     08 54 50  53.7  11.4 -1.1    -155.9    35     1109   05 56 05
05 58 35  ---          08 57 20  53.8  11.0 -1.0    -156.8   150     1119   05 56 06

06 06 35  J0927+39     09 05 21  80.5  27.7 -0.4    -149.1   421     1119   06 06 35
06 12 35  ---          09 11 22  81.0  21.2 -0.3    -156.4   360     1142   06 06 36

06 16 35  J0958+65     09 15 23  54.5   7.9 -0.7    -163.3   180     1142   06 16 35
06 19 05  ---          09 17 53  54.6   7.5 -0.7    -164.3   150     1152   06 16 36

06 19 05  M82PTCEN     09 17 53  50.6   5.4 -0.7    -166.6   -16     1152   06 19 20
06 23 45  ---          09 22 34  50.7   4.8 -0.6    -168.2   264     1169   06 19 06

06 24 35  J0958+65     09 23 24  54.7   6.6 -0.6    -166.3    34     1169   06 24 35
06 27 05  ---          09 25 55  54.8   6.1 -0.6    -167.2   150     1178   06 24 36

06 27 05  M82PTCEN     09 25 55  50.8   4.3 -0.5    -169.3   -16     1178   06 27 21
06 31 45  ---          09 30 35  50.9   3.7 -0.4    -170.9   264     1195   06 27 06

06 32 35  J0958+65     09 31 26  54.9   5.2 -0.5    -169.3    34     1195   06 32 35
06 35 05  ---          09 33 56  54.9   4.7 -0.4    -170.2   150     1205   06 32 36
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

06 35 05  M82PTCEN     09 33 56  50.9   3.2 -0.4    -172.0   -16     1205   06 35 21
06 39 45  ---          09 38 37  50.9   2.6 -0.3    -173.6   264     1222   06 35 06

06 40 35  J0958+65     09 39 27  55.0   3.7 -0.3    -172.3    34     1222   06 40 35
06 43 05  ---          09 41 57  55.0   3.3 -0.3    -173.2   150     1232   06 40 36

06 43 05  M82PTCEN     09 41 57  51.0   2.1 -0.3    -174.8   -16     1232   06 43 21
06 47 45  ---          09 46 38  51.0   1.5 -0.2    -176.4   264     1249   06 43 06

06 48 35  J0958+65     09 47 28  55.1   2.3 -0.2    -175.3    34     1249   06 48 35
06 51 05  ---          09 49 59  55.1   1.8 -0.2    -176.2   150     1258   06 48 36

06 51 05  M82PTCEN     09 49 59  51.0   1.0 -0.1    -177.5   -16     1258   06 51 21
06 55 45  ---          09 54 39  51.0   0.4 -0.0    -179.1   264     1275   06 51 06

06 56 35  J0958+65     09 55 29  55.1   0.8 -0.1    -178.3    34     1275   06 56 35
06 59 05  ---          09 58 00  55.1   0.4 -0.0    -179.2   150     1285   06 56 36

06 59 05  M82PTCEN     09 58 00  51.0  -0.1  0.0     179.7   -16     1285   06 59 21
07 03 45  ---          10 02 41  51.0  -0.8  0.1     178.1   264     1302   06 59 06

07 04 35  J0958+65     10 03 31  55.1  -0.6  0.1     178.7    34     1302   07 04 35
07 07 05  ---          10 06 01  55.1  -1.1  0.1     177.8   150     1312   07 04 36

07 07 05  M82PTCEN     10 06 01  51.0  -1.2  0.1     177.0   -16     1312   07 07 21
07 11 45  ---          10 10 42  51.0  -1.9  0.2     175.4   264     1329   07 07 06

07 12 35  J0958+65     10 11 32  55.1  -2.1  0.2     175.7    34     1329   07 12 35
07 15 05  ---          10 14 03  55.1  -2.5  0.2     174.7   150     1338   07 12 36

07 15 05  M82PTCEN     10 14 03  51.0  -2.3  0.3     174.3   -16     1338   07 15 21
07 19 45  ---          10 18 43  50.9  -3.0  0.4     172.7   264     1355   07 15 06

07 20 35  J0958+65     10 19 33  55.0  -3.5  0.3     172.7    34     1355   07 20 35
07 23 05  ---          10 22 04  55.0  -4.0  0.4     171.7   150     1365   07 20 36

07 23 05  M82PTCEN     10 22 04  50.9  -3.4  0.4     171.5   -16     1365   07 23 21
07 27 45  ---          10 26 45  50.8  -4.1  0.5     169.9   264     1382   07 23 06

07 28 35  J0958+65     10 27 35  54.9  -5.0  0.5     169.7    34     1382   07 28 35
07 31 05  ---          10 30 05  54.8  -5.4  0.5     168.7   150     1392   07 28 36

07 31 05  M82PTCEN     10 30 05  50.8  -4.5  0.5     168.8   -16     1392   07 31 21
07 35 45  ---          10 34 46  50.7  -5.1  0.6     167.2   264     1409   07 31 06
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

07 36 35  J0958+65     10 35 36  54.7  -6.4  0.6     166.7    34     1409   07 36 35
07 39 05  ---          10 38 06  54.7  -6.8  0.6     165.8   150     1418   07 36 36

07 39 05  M82PTCEN     10 38 06  50.6  -5.6  0.7     166.1   -16     1418   07 39 21
07 43 45  ---          10 42 47  50.5  -6.2  0.8     164.5   264     1435   07 39 06

07 44 35  J0958+65     10 43 37  54.5  -7.8  0.7     163.7    34     1435   07 44 35
07 47 05  ---          10 46 08  54.4  -8.2  0.8     162.8   150     1445   07 44 36

07 47 05  M82PTCEN     10 46 08  50.4  -6.7  0.8     163.4   -16     1445   07 47 21
07 51 45  ---          10 50 49  50.3  -7.3  0.9     161.8   264     1462   07 47 06

07 52 35  J0958+65     10 51 39  54.3  -9.1  0.9     160.8    34     1462   07 52 35
07 55 05  ---          10 54 09  54.2  -9.5  0.9     159.9   150     1472   07 52 36

07 55 05  M82PTCEN     10 54 09  50.2  -7.7  0.9     160.7   -16     1472   07 55 21
07 59 45  ---          10 58 50  50.1  -8.3  1.0     159.1   264     1489   07 55 06

08 00 35  J0958+65     10 59 40  54.0 -10.5  1.0     157.9    34     1489   08 00 35
08 03 05  ---          11 02 10  53.9 -10.9  1.0     157.0   150     1498   08 00 36

08 03 05  M82PTCEN     11 02 10  50.0  -8.7  1.1     158.0   -16     1498   08 03 20
08 07 45  ---          11 06 51  49.8  -9.3  1.2     156.5   264     1515   08 03 06

08 08 35  J0958+65     11 07 41  53.6 -11.7  1.1     155.0    34     1515   08 08 35
08 11 05  ---          11 10 12  53.5 -12.1  1.2     154.1   150     1525   08 08 36

08 11 05  M82PTCEN     11 10 12  49.7  -9.7  1.2     155.4   -16     1525   08 11 20
08 15 45  ---          11 14 52  49.5 -10.3  1.3     153.9   264     1542   08 11 06

08 16 35  J0958+65     11 15 43  53.3 -13.0  1.3     152.2    35     1542   08 16 35
08 19 05  ---          11 18 13  53.1 -13.4  1.3     151.3   150     1552   08 16 36

08 19 05  M82PTCEN     11 18 13  49.4 -10.7  1.3     152.8   -15     1552   08 19 20
08 23 45  ---          11 22 54  49.2 -11.2  1.4     151.3   265     1569   08 19 06

08 24 35  J0958+65     11 23 44  52.9 -14.2  1.4     149.4    35     1569   08 24 35
08 27 05  ---          11 26 14  52.7 -14.6  1.4     148.5   150     1578   08 24 36

08 27 05  M82PTCEN     11 26 14  49.0 -11.6  1.5     150.2   -15     1578   08 27 20
08 31 45  ---          11 30 55  48.8 -12.2  1.6     148.7   265     1595   08 27 06

08 32 25  J0958+65     11 31 35  52.4 -15.3  1.5     146.7    25     1595   08 32 25
08 34 55  ---          11 34 06  52.3 -15.7  1.6     145.9   150     1605   08 32 26
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

08 34 55  M82PTCEN     11 34 06  48.7 -12.5  1.6     147.7   -15     1605   08 35 10
08 39 35  ---          11 38 46  48.5 -13.0  1.7     146.2   265     1622   08 34 56

08 40 15  J0958+65     11 39 27  52.0 -16.4  1.7     144.1    25     1622   08 40 15
08 42 45  ---          11 41 57  51.8 -16.8  1.7     143.2   150     1632   08 40 16

08 42 45  M82PTCEN     11 41 57  48.3 -13.4  1.7     145.2   -15     1632   08 43 00
08 47 35  ---          11 46 48  48.1 -13.9  1.8     143.7   275     1649   08 42 46

08 48 15  J0958+65     11 47 28  51.5 -17.5  1.8     141.4    25     1649   08 48 15
08 50 55  ---          11 50 08  51.3 -17.9  1.8     140.5   160     1660   08 48 16

08 50 55  M82PTCEN     11 50 08  47.9 -14.2  1.9     142.6   -15     1660   08 51 09
08 55 45  ---          11 54 59  47.6 -14.7  2.0     141.1   275     1677   08 50 56

08 56 25  J0958+65     11 55 39  50.9 -18.5  1.9     138.7    25     1677   08 56 25
08 59 05  ---          11 58 20  50.7 -18.9  2.0     137.9   160     1688   08 56 26

08 59 05  M82PTCEN     11 58 20  47.4 -15.1  2.0     140.1   -15     1688   08 59 19
09 03 55  ---          12 03 10  47.2 -15.5  2.1     138.6   275     1706   08 59 06

09 04 35  J0958+65     12 03 51  50.3 -19.5  2.1     136.1    26     1706   09 04 35
09 07 15  ---          12 06 31  50.1 -19.8  2.1     135.3   160     1716   09 04 36

09 07 15  M82PTCEN     12 06 31  47.0 -15.9  2.2     137.6   -14     1716   09 07 29
09 12 05  ---          12 11 22  46.7 -16.3  2.2     136.1   276     1734   09 07 16

09 12 45  J0958+65     12 12 02  49.7 -20.5  2.2     133.5    26     1734   09 12 45
09 15 25  ---          12 14 42  49.5 -20.8  2.2     132.7   160     1744   09 12 46

09 15 25  M82PTCEN     12 14 42  46.5 -16.6  2.3     135.1   -14     1744   09 15 39
09 20 15  ---          12 19 33  46.2 -17.0  2.4     133.7   276     1762   09 15 26

09 20 55  J0958+65     12 20 13  49.1 -21.3  2.3     131.0    26     1762   09 20 55
09 23 35  ---          12 22 54  48.9 -21.6  2.4     130.2   160     1772   09 20 56

09 23 35  M82PTCEN     12 22 54  46.0 -17.3  2.4     132.7   -14     1772   09 23 49
09 28 25  ---          12 27 44  45.7 -17.7  2.5     131.3   276     1790   09 23 36

09 29 05  J0958+65     12 28 25  48.5 -22.2  2.5     128.5    26     1790   09 29 05
09 31 45  ---          12 31 05  48.2 -22.4  2.5     127.7   160     1800   09 29 06

09 31 45  M82PTCEN     12 31 05  45.4 -18.0  2.6     130.3   -14     1800   09 31 58
09 36 35  ---          12 35 56  45.1 -18.4  2.6     128.9   276     1818   09 31 46
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

09 37 15  J0958+65     12 36 36  47.8 -22.9  2.6     126.1    27     1818   09 37 15
09 39 55  ---          12 39 16  47.6 -23.2  2.7     125.3   160     1828   09 37 16

09 39 55  M82PTCEN     12 39 16  44.9 -18.6  2.7     127.9   -13     1828   09 40 08
09 44 45  ---          12 44 07  44.5 -19.0  2.8     126.5   277     1846   09 39 56

09 45 25  J0958+65     12 44 47  47.1 -23.7  2.7     123.7    27     1846   09 45 25
09 48 05  ---          12 47 28  46.8 -23.9  2.8     122.9   160     1856   09 45 26

09 48 05  M82PTCEN     12 47 28  44.3 -19.2  2.8     125.6   -13     1856   09 48 18
09 52 55  ---          12 52 18  44.0 -19.6  2.9     124.2   277     1874   09 48 06

09 53 35  J0958+65     12 52 59  46.4 -24.3  2.9     121.3    27     1874   09 53 35
09 56 15  ---          12 55 39  46.1 -24.5  2.9     120.6   160     1884   09 53 36

09 56 15  M82PTCEN     12 55 39  43.7 -19.8  3.0     123.3   -13     1884   09 56 28
10 01 05  ---          13 00 30  43.4 -20.1  3.1     121.9   277     1902   09 56 16

10 01 45  J0958+65     13 01 10  45.6 -24.9  3.0     119.0    27     1902   10 01 45
10 04 25  ---          13 03 50  45.4 -25.1  3.1     118.3   160     1913   10 01 46

10 04 25  M82PTCEN     13 03 50  43.1 -20.3  3.1     121.0   -13     1913   10 04 37
10 09 15  ---          13 08 41  42.8 -20.6  3.2     119.7   277     1930   10 04 26

10 09 55  J0958+65     13 09 21  44.9 -25.5  3.2     116.8    28     1930   10 09 55
10 12 35  ---          13 12 02  44.6 -25.7  3.2     116.0   160     1941   10 09 56

10 12 35  M82PTCEN     13 12 02  42.5 -20.8  3.2     118.7   -12     1941   10 12 47
10 17 25  ---          13 16 52  42.1 -21.1  3.3     117.4   278     1959   10 12 36

10 18 05  J0958+65     13 17 33  44.1 -26.0  3.3     114.5    28     1959   10 18 05
10 20 45  ---          13 20 13  43.9 -26.2  3.3     113.8   160     1969   10 18 06

10 20 45  M82PTCEN     13 20 13  41.9 -21.3  3.4     116.5   -12     1969   10 20 57
10 25 35  ---          13 25 04  41.5 -21.5  3.5     115.2   278     1987   10 20 46

10 26 15  J0958+65     13 25 44  43.3 -26.5  3.4     112.4    28     1987   10 26 15
10 28 55  ---          13 28 24  43.1 -26.6  3.5     111.7   160     1997   10 26 16

10 28 55  M82PTCEN     13 28 24  41.2 -21.7  3.5     114.3   -12     1997   10 29 06
10 33 45  ---          13 33 15  40.8 -21.9  3.6     113.1   278     2015   10 28 56

10 34 25  J0958+65     13 33 55  42.5 -26.9  3.6     110.2    28     2015   10 34 25
10 37 05  ---          13 36 36  42.3 -27.0  3.6     109.5   160     2025   10 34 26
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

10 37 05  M82PTCEN     13 36 36  40.6 -22.0  3.7     112.2   -11     2025   10 37 16
10 41 55  ---          13 41 27  40.2 -22.2  3.7     110.9   279     2043   10 37 06

10 42 35  J0958+65     13 42 07  41.7 -27.3  3.7     108.1    29     2043   10 42 35
10 45 15  ---          13 44 47  41.5 -27.4  3.7     107.4   160     2054   10 42 36

10 45 15  M82PTCEN     13 44 47  39.9 -22.4  3.8     110.0   -11     2054   10 45 26
10 50 05  ---          13 49 38  39.5 -22.6  3.9     108.8   279     2072   10 45 16

10 50 45  J0958+65     13 50 18  40.9 -27.6  3.8     106.0    29     2072   10 50 45
10 53 25  ---          13 52 58  40.7 -27.7  3.9     105.3   160     2082   10 50 46

10 53 25  M82PTCEN     13 52 58  39.2 -22.7  3.9     107.9   -11     2082   10 53 36
10 58 15  ---          13 57 49  38.8 -22.8  4.0     106.7   279     2100   10 53 26

10 58 55  J0958+65     13 58 29  40.1 -27.9  4.0     104.0    29     2100   10 58 55
11 01 35  ---          14 01 10  39.8 -28.0  4.0     103.3   160     2110   10 58 56

11 01 35  M82PTCEN     14 01 10  38.5 -22.9  4.1     105.8   -11     2110   11 01 46
11 06 25  ---          14 06 01  38.1 -23.1  4.1     104.6   279     2128   11 01 36

11 07 05  J0958+65     14 06 41  39.3 -28.2  4.1     101.9    29     2128   11 07 05
11 09 45  ---          14 09 21  39.0 -28.2  4.2     101.3   160     2138   11 07 06

11 09 45  M82PTCEN     14 09 21  37.9 -23.2  4.2     103.8   -11     2138   11 09 56
11 14 35  ---          14 14 12  37.4 -23.3  4.3     102.6   279     2156   11 09 46

11 15 15  J0958+65     14 14 52  38.4 -28.4  4.2     100.0    29     2156   11 15 15
11 17 55  ---          14 17 32  38.2 -28.4  4.3      99.3   160     2167   11 15 16

11 17 55  M82PTCEN     14 17 32  37.2 -23.4  4.3     101.7   -11     2167   11 18 06
11 22 45  ---          14 22 23  36.7 -23.5  4.4     100.5   279     2185   11 17 56

11 23 25  J0958+65     14 23 03  37.6 -28.5  4.4      98.0    29     2185   11 23 25
11 26 05  ---          14 25 44  37.3 -28.6  4.4      97.3   160     2195   11 23 26

11 26 05  M82PTCEN     14 25 44  36.5 -23.5  4.5      99.7   -11     2195   11 26 16
11 30 55  ---          14 30 35  36.0 -23.6  4.6      98.5   279     2213   11 26 06

11 31 35  J0958+65     14 31 15  36.8 -28.7  4.5      96.0    29     2213   11 31 35
11 34 15  ---          14 33 55  36.5 -28.7  4.6      95.4   160     2223   11 31 36

11 34 15  M82PTCEN     14 33 55  35.7 -23.7  4.6      97.7   -11     2223   11 34 26
11 39 05  ---          14 38 46  35.3 -23.7  4.7      96.6   279     2241   11 34 16
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

11 39 45  J0958+65     14 39 26  35.9 -28.7  4.7      94.1    29     2241   11 39 45
11 42 25  ---          14 42 06  35.6 -28.8  4.7      93.5   160     2252   11 39 46

11 42 25  M82PTCEN     14 42 06  35.0 -23.8  4.7      95.7   -11     2252   11 42 36
11 47 15  ---          14 46 57  34.6 -23.8  4.8      94.6   279     2270   11 42 26

11 47 55  J0958+65     14 47 37  35.1 -28.8  4.8      92.2    29     2270   11 47 55
11 50 35  ---          14 50 18  34.8 -28.8  4.8      91.6   160     2280   11 47 56

11 50 35  M82PTCEN     14 50 18  34.3 -23.8  4.9      93.8   -11     2280   11 50 46
11 55 25  ---          14 55 09  33.9 -23.9  5.0      92.6   279     2298   11 50 36

11 56 05  J0958+65     14 55 49  34.2 -28.8  4.9      90.4    29     2298   11 56 05
11 58 45  ---          14 58 29  33.9 -28.8  5.0      89.7   160     2308   11 56 06

11 58 45  M82PTCEN     14 58 29  33.6 -23.9  5.0      91.8   -11     2308   11 58 56
12 03 35  ---          15 03 20  33.2 -23.9  5.1      90.7   279     2326   11 58 46

12 04 15  J0958+65     15 04 00  33.4 -28.8  5.1      88.5    29     2326   12 04 15
12 06 55  ---          15 06 40  33.1 -28.8  5.1      87.9   160     2336   12 04 16

12 06 55  M82PTCEN     15 06 40  32.9 -23.9  5.2      89.9   -11     2336   12 07 06
12 11 45  ---          15 11 31  32.5 -23.9  5.2      88.8   279     2354   12 06 56

12 12 25  J0958+65     15 12 11  32.5 -28.8  5.2      86.7    29     2354   12 12 25
12 15 05  ---          15 14 52  32.2 -28.8  5.2      86.1   160     2365   12 12 26

12 15 05  M82PTCEN     15 14 52  32.2 -23.9  5.3      88.0   -11     2365   12 15 16
12 19 55  ---          15 19 43  31.8 -23.9  5.4      86.9   279     2383   12 15 06

12 20 35  J0958+65     15 20 23  31.7 -28.7  5.3      84.8    29     2383   12 20 35
12 23 15  ---          15 23 03  31.4 -28.7  5.4      84.2   160     2393   12 20 36

12 23 15  M82PTCEN     15 23 03  31.5 -23.8  5.4      86.1   -11     2393   12 23 26
12 28 05  ---          15 27 54  31.1 -23.8  5.5      85.0   279     2411   12 23 16

12 28 45  J0958+65     15 28 34  30.8 -28.6  5.5      83.0    29     2411   12 28 45
12 31 25  ---          15 31 14  30.6 -28.6  5.5      82.4   160     2421   12 28 46

12 31 25  M82PTCEN     15 31 14  30.8 -23.8  5.6      84.2   -11     2421   12 31 36
12 36 15  ---          15 36 05  30.3 -23.7  5.6      83.1   279     2439   12 31 26

12 36 55  J0958+65     15 36 45  30.0 -28.5  5.6      81.2    29     2439   12 36 55
12 39 35  ---          15 39 26  29.7 -28.4  5.7      80.6   160     2449   12 36 56
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

12 39 35  M82PTCEN     15 39 26  30.1 -23.7  5.7      82.4   -11     2449   12 39 46
12 44 25  ---          15 44 17  29.6 -23.6  5.8      81.3   279     2467   12 39 36

12 45 05  J0958+65     15 44 57  29.2 -28.3  5.7      79.4    29     2467   12 45 05
12 47 45  ---          15 47 37  28.9 -28.2  5.8      78.9   160     2478   12 45 06

12 47 45  M82PTCEN     15 47 37  29.4 -23.6  5.8      80.5   -11     2478   12 47 56
12 52 35  ---          15 52 28  28.9 -23.5  5.9      79.4   279     2496   12 47 46

12 53 15  J0958+65     15 53 08  28.3 -28.1  5.9      77.7    29     2496   12 53 15
12 55 45  ---          15 55 38  28.1 -28.0  5.9      77.1   150     2505   12 53 16

12 55 45  M82PTCEN     15 55 38  28.7 -23.4  6.0      78.7   -11     2505   12 55 56
13 00 35  ---          16 00 29  28.3 -23.3  6.1      77.6   279     2523   12 55 46

13 01 15  J0958+65     16 01 09  27.5 -27.9  6.0      76.0    29     2523   13 01 15
13 03 45  ---          16 03 40  27.3 -27.8  6.1      75.4   150     2533   13 01 16

13 25 24  J0958+65     16 25 23  25.1 -27.1  6.4      70.8  1293     2533   13 25 24
13 27 24  ---          16 27 23  24.9 -27.0  6.5      70.4   120     2541   13 25 25

13 27 24  M82PTCEN     16 27 23  26.0 -22.6  6.5      71.6   -11     2541   13 27 35
13 32 14  ---          16 32 14  25.6 -22.5  6.6      70.5   279     2559   13 27 25

13 32 54  J0958+65     16 32 54  24.4 -26.8  6.5      69.2    29     2559   13 32 54
13 35 24  ---          16 35 25  24.1 -26.7  6.6      68.7   150     2568   13 32 55

13 35 24  M82PTCEN     16 35 25  25.3 -22.4  6.6      69.8   -11     2568   13 35 35
13 40 14  ---          16 40 15  24.9 -22.2  6.7      68.8   279     2586   13 35 25

13 40 54  J0958+65     16 40 56  23.6 -26.5  6.7      67.5    29     2586   13 40 54
13 43 24  ---          16 43 26  23.4 -26.4  6.7      67.0   150     2596   13 40 55

13 43 24  M82PTCEN     16 43 26  24.7 -22.1  6.8      68.1   -11     2596   13 43 35
13 48 14  ---          16 48 17  24.3 -21.9  6.9      67.0   279     2614   13 43 25

13 48 54  J0958+65     16 48 57  22.8 -26.1  6.8      65.8    29     2614   13 48 54
13 51 24  ---          16 51 27  22.6 -26.0  6.9      65.3   150     2624   13 48 55

13 51 24  M82PTCEN     16 51 27  24.0 -21.8  6.9      66.3   -11     2624   13 51 35
13 56 14  ---          16 56 18  23.7 -21.6  7.0      65.3   279     2642   13 51 25

13 56 54  J0958+65     16 56 58  22.1 -25.7  6.9      64.2    29     2642   13 56 54
13 59 24  ---          16 59 29  21.8 -25.6  7.0      63.6   150     2651   13 56 55
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

13 59 24  M82PTCEN     16 59 29  23.4 -21.5  7.0      64.6   -11     2651   13 59 35
14 04 14  ---          17 04 19  23.0 -21.3  7.1      63.5   279     2669   13 59 25

14 04 54  J0958+65     17 05 00  21.3 -25.3  7.1      62.5    29     2669   14 04 54
14 07 24  ---          17 07 30  21.1 -25.2  7.1      62.0   150     2679   14 04 55

14 07 24  M82PTCEN     17 07 30  22.8 -21.1  7.2      62.8   -11     2679   14 07 36
14 12 14  ---          17 12 21  22.4 -20.9  7.3      61.8   279     2697   14 07 25

14 12 54  J0958+65     17 13 01  20.6 -24.9  7.2      60.8    29     2697   14 12 54
14 15 24  ---          17 15 31  20.4 -24.8  7.3      60.3   150     2707   14 12 55

14 15 24  M82PTCEN     17 15 31  22.2 -20.8  7.3      61.1   -12     2707   14 15 36
14 20 14  ---          17 20 22  21.8 -20.5  7.4      60.0   278     2724   14 15 25

14 20 54  J0958+65     17 21 02  19.9 -24.5  7.3      59.1    28     2724   14 20 54
14 23 24  ---          17 23 33  19.7 -24.3  7.4      58.6   150     2734   14 20 55

14 23 24  M82PTCEN     17 23 33  21.5 -20.4  7.4      59.3   -12     2734   14 23 36
14 28 14  ---          17 28 23  21.2 -20.2  7.5      58.3   278     2752   14 23 25

14 28 54  J0958+65     17 29 03  19.2 -24.0  7.5      57.5    28     2752   14 28 54
14 31 24  ---          17 31 34  19.0 -23.8  7.5      56.9   150     2762   14 28 55

14 31 24  M82PTCEN     17 31 34  21.0 -20.0  7.6      57.6   -12     2762   14 31 36
14 36 14  ---          17 36 25  20.6 -19.8  7.7      56.6   278     2780   14 31 25

14 36 54  J0958+65     17 37 05  18.5 -23.5  7.6      55.8    28     2780   14 36 54
14 39 24  ---          17 39 35  18.3 -23.4  7.7      55.3   150     2789   14 36 55

14 39 24  M82PTCEN     17 39 35  20.4 -19.6  7.7      55.9   -12     2789   14 39 37
14 44 14  ---          17 44 26  20.0 -19.3  7.8      54.8   278     2807   14 39 25

14 44 54  J0958+65     17 45 06  17.8 -23.0  7.8      54.1    28     2807   14 44 54
14 47 24  ---          17 47 36  17.6 -22.8  7.8      53.6   150     2817   14 44 55

14 47 24  M82PTCEN     17 47 36  19.8 -19.2  7.8      54.1   -12     2817   14 47 37
14 52 14  ---          17 52 27  19.5 -18.9  7.9      53.1   278     2835   14 47 25

14 52 54  J0958+65     17 53 07  17.1 -22.5  7.9      52.5    27     2835   14 52 54
14 55 24  ---          17 55 38  16.9 -22.3  7.9      51.9   150     2844   14 52 55

14 55 24  M82PTCEN     17 55 38  19.2 -18.7  8.0      52.4   -13     2844   14 55 37
15 00 14  ---          18 00 29  18.9 -18.4  8.1      51.4   277     2862   14 55 25
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

15 00 54  J0958+65     18 01 09  16.5 -21.9  8.0      50.8    27     2862   15 00 54
15 03 24  ---          18 03 39  16.3 -21.8  8.1      50.3   150     2872   15 00 55

15 03 24  M82PTCEN     18 03 39  18.7 -18.3  8.1      50.7   -13     2872   15 03 37
15 08 14  ---          18 08 30  18.4 -18.0  8.2      49.6   277     2890   15 03 25

15 08 54  J0958+65     18 09 10  15.8 -21.4  8.2      49.1    27     2890   15 08 54
15 11 24  ---          18 11 40  15.6 -21.2  8.2      48.6   150     2899   15 08 55

15 11 24  M82PTCEN     18 11 40  18.2 -17.8  8.2      48.9   -13     2899   15 11 37
15 16 14  ---          18 16 31  17.8 -17.5  8.3      47.9   277     2917   15 11 25

15 16 54  J0958+65     18 17 11  15.2 -20.8  8.3      47.5    27     2917   15 16 54
15 19 24  ---          18 19 42  15.0 -20.6  8.3      46.9   150     2927   15 16 55

15 19 24  M82PTCEN     18 19 42  17.6 -17.3  8.4      47.2   -13     2927   15 19 38
15 24 14  ---          18 24 33  17.3 -17.0  8.5      46.2   277     2945   15 19 25

15 24 54  J0958+65     18 25 13  14.6 -20.2  8.4      45.8    27     2945   15 24 54
15 27 24  ---          18 27 43  14.4 -20.0  8.5      45.3   150     2954   15 24 55

15 27 24  M82PTCEN     18 27 43  17.1 -16.8  8.5      45.5   -13     2954   15 27 38
15 32 14  ---          18 32 34  16.8 -16.5  8.6      44.4   277     2972   15 27 25

15 32 54  J0958+65     18 33 14  14.0 -19.6  8.6      44.1    27     2972   15 32 54
15 35 24  ---          18 35 44  13.8 -19.4  8.6      43.6   150     2982   15 32 55

15 35 24  M82PTCEN     18 35 44  16.6 -16.3  8.6      43.8   -14     2982   15 35 38
15 40 14  ---          18 40 35  16.3 -16.0  8.7      42.7   276     3000   15 35 25

15 40 54  J0958+65     18 41 15  13.5 -19.0  8.7      42.4    26     3000   15 40 54
15 43 24  ---          18 43 46  13.3 -18.8  8.7      41.9   150     3009   15 40 55

15 43 24  M82PTCEN     18 43 46  16.2 -15.7  8.8      42.0   -14     3009   15 43 38
15 48 14  ---          18 48 36  15.9 -15.4  8.9      41.0   276     3027   15 43 25

15 48 54  J0958+65     18 49 17  12.9 -18.3  8.8      40.8    26     3027   15 48 54
15 51 24  ---          18 51 47  12.7 -18.1  8.9      40.2   150     3037   15 48 55

15 51 24  M82PTCEN     18 51 47  15.7 -15.2  8.9      40.3   -14     3037   15 51 38
15 56 14  ---          18 56 38  15.4 -14.9  9.0      39.3   276     3055   15 51 25

15 56 54  J0958+65     18 57 18  12.4 -17.7  9.0      39.1    26     3055   15 56 54
15 59 24  ---          18 59 48  12.2 -17.5  9.0      38.5   150     3064   15 56 55
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

15 59 24  M82PTCEN     18 59 48  15.3 -14.6  9.0      38.6   -14     3064   15 59 38
16 04 14  ---          19 04 39  15.0 -14.3  9.1      37.5   276     3082   15 59 25

16 04 54  J0958+65     19 05 19  11.9 -17.0  9.1      37.4    26     3082   16 04 54
16 07 24  ---          19 07 50  11.7 -16.8  9.1      36.9   150     3092   16 04 55

16 07 24  M82PTCEN     19 07 50  14.8 -14.1  9.2      36.8   -14     3092   16 07 39
16 12 14  ---          19 12 40  14.6 -13.7  9.3      35.8   276     3109   16 07 25

16 12 54  J0958+65     19 13 21  11.4 -16.3  9.2      35.7    26     3109   16 12 54
16 15 24  ---          19 15 51  11.2 -16.1  9.3      35.2   150     3119   16 12 55

16 15 24  M82PTCEN     19 15 51  14.4 -13.5  9.3      35.1   -14     3119   16 15 39
16 20 14  ---          19 20 42  14.2 -13.1  9.4      34.1   276     3137   16 15 25

16 20 54  J0958+65     19 21 22  10.9 -15.6  9.4      34.0    26     3137   16 20 54
16 23 24  ---          19 23 52  10.7 -15.4  9.4      33.5   150     3147   16 20 55

16 23 24  M82PTCEN     19 23 52  14.0 -12.9  9.4      33.4   -14     3147   16 23 39
16 28 14  ---          19 28 43  13.8 -12.5  9.5      32.3   276     3164   16 23 25

16 28 54  J0958+65     19 29 23  10.4 -14.9  9.5      32.3    25     3164   16 28 54
16 31 24  ---          19 31 54  10.3 -14.7  9.5      31.8   150     3174   16 28 55

16 31 24  M82PTCEN     19 31 54  13.7 -12.3  9.6      31.6   -15     3174   16 31 39
16 36 14  ---          19 36 44  13.4 -11.9  9.7      30.6   275     3192   16 31 25

16 36 54  J0958+65     19 37 24  10.0 -14.2  9.6      30.6    25     3192   16 36 54
16 39 24  ---          19 39 55   9.9 -14.0  9.7      30.1   150     3201   16 36 55

16 39 24  M82PTCEN     19 39 55  13.3 -11.7  9.7      29.9   -15     3201   16 39 39
16 44 14  ---          19 44 46  13.1 -11.3  9.8      28.9   275     3219   16 39 25

16 44 54  J0958+65     19 45 26   9.6 -13.5  9.8      28.9    25     3219   16 44 54
16 47 24  ---          19 47 56   9.5 -13.3  9.8      28.4   150     3229   16 44 55

16 47 24  M82PTCEN     19 47 56  13.0 -11.0  9.8      28.2   -15     3229   16 47 39
16 52 14  ---          19 52 47  12.8 -10.6  9.9      27.1   275     3246   16 47 25

16 52 54  J0958+65     19 53 27   9.2 -12.7  9.9      27.2    25     3246   16 52 54
16 55 24  ---          19 55 58   9.1 -12.5  9.9      26.7   150     3256   16 52 55

16 55 24  M82PTCEN     19 55 58  12.6 -10.4 10.0      26.4   -15     3256   16 55 39
17 00 14  ---          20 00 48  12.4 -10.0 10.1      25.4   275     3274   16 55 25
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

17 00 54  J0958+65     20 01 28   8.8 -12.0 10.0      25.5    25     3274   17 00 54
17 03 24  ---          20 03 59   8.7 -11.7 10.1      25.0   150     3283   17 00 55

17 03 24  M82PTCEN     20 03 59  12.3  -9.7 10.1      24.7   -15     3283   17 03 40
17 08 14  ---          20 08 50  12.2  -9.3 10.2      23.6   275     3301   17 03 25

17 08 54  J0958+65     20 09 30   8.5 -11.2 10.2      23.8    25     3301   17 08 54
17 11 24  ---          20 12 00   8.4 -11.0 10.2      23.3   150     3311   17 08 55

17 11 24  M82PTCEN     20 12 00  12.0  -9.1 10.2      22.9   -15     3311   17 11 40
17 16 14  ---          20 16 51  11.9  -8.7 10.3      21.9   275     3329   17 11 25

17 16 54  J0958+65     20 17 31   8.1 -10.4 10.3      22.1    25     3329   17 16 54
17 19 24  ---          20 20 01   8.1 -10.2 10.3      21.6   150     3338   17 16 55

17 19 24  M82PTCEN     20 20 01  11.8  -8.4 10.4      21.2   -15     3338   17 19 40
17 24 14  ---          20 24 52  11.6  -8.0 10.5      20.2   275     3356   17 19 25

17 24 54  J0958+65     20 25 32   7.8  -9.7 10.4      20.4    25     3356   17 24 54
17 27 24  ---          20 28 03   7.8  -9.4 10.5      19.8   150     3366   17 24 55

17 27 24  M82PTCEN     20 28 03  11.5  -7.8 10.5      19.5   -15     3366   17 27 40
17 32 14  ---          20 32 54  11.4  -7.3 10.6      18.4   275     3383   17 27 25

17 32 54  J0958+65     20 33 34   7.6  -8.9 10.6      18.7    24     3383   17 32 54
17 35 24  ---          20 36 04   7.5  -8.6 10.6      18.1   150     3393   17 32 55

17 35 24  M82PTCEN     20 36 04  11.3  -7.1 10.6      17.7   -16     3393   17 35 40
17 40 14  ---          20 40 55  11.2  -6.7 10.7      16.7   274     3411   17 35 25

17 40 54  J0958+65     20 41 35   7.3  -8.1 10.7      16.9    24     3411   17 40 54
17 43 24  ---          20 44 05   7.2  -7.8 10.7      16.4   150     3420   17 40 55

17 43 24  M82PTCEN     20 44 05  11.1  -6.4 10.8      16.0   -16     3420   17 43 40
17 48 14  ---          20 48 56  11.0  -6.0 10.9      14.9   274     3438   17 43 25

17 48 54  J0958+65     20 49 36   7.1  -7.3 10.8      15.2    24     3438   17 48 54
17 51 24  ---          20 52 07   7.0  -7.0 10.9      14.7   150     3448   17 48 55

18 06 24  J0958+65     21 07 09   6.7  -5.5 11.1      11.4   894     3448   18 06 24
18 08 24  ---          21 09 10   6.6  -5.3 11.2      11.0   120     3455   18 06 25

18 17 47  3C84         21 18 34  19.4  52.5 -6.0     -65.8   514     3455   18 17 47
18 23 47  ---          21 24 35  20.4  52.9 -5.9     -66.6   360     3479   18 17 48
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

18 31 47  J0958+65     21 32 36   6.3  -2.9 11.5       5.9   432     3479   18 31 47
18 33 47  ---          21 34 36   6.2  -2.7 11.6       5.5   120     3486   18 31 48

18 33 47  M82PTCEN     21 34 36  10.3  -2.0 11.6       4.9   -16     3486   18 34 03
18 38 27  ---          21 39 17  10.3  -1.6 11.7       3.9   264     3503   18 33 48

18 39 17  J0958+65     21 40 07   6.2  -2.1 11.7       4.3    34     3503   18 39 17
18 41 47  ---          21 42 37   6.2  -1.8 11.7       3.8   150     3513   18 39 18

18 41 47  M82PTCEN     21 42 37  10.3  -1.3 11.8       3.2   -16     3513   18 42 03
18 46 27  ---          21 47 18  10.3  -0.9 11.8       2.2   264     3530   18 41 48

18 47 17  J0958+65     21 48 08   6.1  -1.2 11.8       2.6    34     3530   18 47 17
18 49 47  ---          21 50 39   6.1  -1.0 11.8       2.0   150     3540   18 47 18

18 49 47  M82PTCEN     21 50 39  10.2  -0.6 11.9       1.4   -16     3540   18 50 03
18 54 27  ---          21 55 20  10.2  -0.2 12.0       0.4   264     3557   18 49 48

18 55 17  J0958+65     21 56 10   6.1  -0.4 11.9       0.8    34     3557   18 55 17
18 57 47  ---          21 58 40   6.1  -0.1 12.0       0.3   150     3566   18 55 18

18 57 47  M82PTCEN     21 58 40  10.2   0.1-12.0      -0.3   -16     3566   18 58 03
19 02 27  ---          22 03 21  10.2   0.5-11.9      -1.3   264     3583   18 57 48

19 03 17  J0958+65     22 04 11   6.1   0.4-11.9      -0.9    34     3583   19 03 17
19 05 47  ---          22 06 41   6.1   0.7-11.9      -1.4   150     3593   19 03 18

19 05 47  M82PTCEN     22 06 41  10.3   0.8-11.8      -2.1   -16     3593   19 06 03
19 10 27  ---          22 11 22  10.3   1.3-11.8      -3.1   264     3610   19 05 48

19 11 17  J0958+65     22 12 12   6.1   1.3-11.8      -2.6    34     3610   19 11 17
19 13 47  ---          22 14 43   6.2   1.5-11.8      -3.2   150     3620   19 11 18

19 13 47  M82PTCEN     22 14 43  10.3   1.5-11.7      -3.8   -16     3620   19 14 03
19 18 27  ---          22 19 23  10.3   2.0-11.6      -4.8   264     3637   19 13 48

19 19 17  J0958+65     22 20 14   6.2   2.1-11.7      -4.4    34     3637   19 19 17
19 21 47  ---          22 22 44   6.2   2.4-11.6      -4.9   150     3646   19 19 18

19 21 47  M82PTCEN     22 22 44  10.3   2.3-11.6      -5.6   -16     3646   19 22 03
19 26 27  ---          22 27 25  10.4   2.7-11.5      -6.6   264     3663   19 21 48

19 27 17  J0958+65     22 28 15   6.3   2.9-11.5      -6.1    34     3663   19 27 17
19 29 47  ---          22 30 45   6.3   3.2-11.5      -6.6   150     3673   19 27 18
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

19 29 47  M82PTCEN     22 30 45  10.4   3.0-11.4      -7.3   -16     3673   19 30 03
19 34 27  ---          22 35 26  10.5   3.4-11.4      -8.4   264     3690   19 29 48

19 35 17  J0958+65     22 36 16   6.4   3.8-11.4      -7.8    34     3690   19 35 17
19 37 47  ---          22 38 47   6.4   4.0-11.4      -8.4   150     3700   19 35 18

19 37 47  M82PTCEN     22 38 47  10.5   3.7-11.3      -9.1   -16     3700   19 38 03
19 42 27  ---          22 43 27  10.6   4.1-11.2     -10.1   264     3717   19 37 48

19 43 17  J0958+65     22 44 18   6.5   4.6-11.3      -9.6    34     3717   19 43 17
19 45 47  ---          22 46 48   6.5   4.9-11.2     -10.1   150     3726   19 43 18

19 45 47  M82PTCEN     22 46 48  10.6   4.4-11.2     -10.8   -16     3726   19 46 03
19 50 27  ---          22 51 29  10.7   4.8-11.1     -11.9   264     3743   19 45 48

19 51 17  J0958+65     22 52 19   6.7   5.4-11.1     -11.3    34     3743   19 51 17
19 53 47  ---          22 54 49   6.7   5.7-11.1     -11.8   150     3753   19 51 18

19 53 47  M82PTCEN     22 54 49  10.8   5.1-11.0     -12.6   -16     3753   19 54 03
19 58 27  ---          22 59 30  10.9   5.5-11.0     -13.6   264     3770   19 53 48

19 59 17  J0958+65     23 00 20   6.8   6.2-11.0     -13.0    34     3770   19 59 17
20 01 47  ---          23 02 51   6.9   6.5-11.0     -13.6   150     3780   19 59 18

20 01 47  M82PTCEN     23 02 51  10.9   5.8-10.9     -14.3   -16     3780   20 02 03
20 06 27  ---          23 07 31  11.1   6.2-10.8     -15.4   264     3797   20 01 48

20 07 17  J0958+65     23 08 22   7.0   7.1-10.9     -14.8    34     3797   20 07 17
20 09 47  ---          23 10 52   7.1   7.3-10.8     -15.3   150     3806   20 07 18

20 09 47  M82PTCEN     23 10 52  11.1   6.4-10.8     -16.1   -16     3806   20 10 03
20 14 27  ---          23 15 33  11.2   6.8-10.7     -17.1   264     3823   20 09 48

20 15 17  J0958+65     23 16 23   7.3   7.9-10.7     -16.5    34     3823   20 15 17
20 17 47  ---          23 18 53   7.3   8.1-10.7     -17.0   150     3833   20 15 18

20 17 47  M82PTCEN     23 18 53  11.3   7.1-10.6     -17.8   -16     3833   20 18 03
20 22 27  ---          23 23 34  11.5   7.5-10.6     -18.8   264     3850   20 17 48

20 23 17  J0958+65     23 24 24   7.5   8.7-10.6     -18.2    34     3850   20 23 17
20 25 47  ---          23 26 55   7.6   8.9-10.6     -18.7   150     3860   20 23 18

20 25 47  M82PTCEN     23 26 55  11.6   7.8-10.5     -19.6   -16     3860   20 26 03
20 30 27  ---          23 31 35  11.7   8.2-10.4     -20.6   264     3877   20 25 48
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

20 31 17  J0958+65     23 32 25   7.8   9.5-10.5     -19.9    34     3877   20 31 17
20 33 47  ---          23 34 56   7.9   9.7-10.4     -20.5   150     3886   20 31 18

20 33 47  M82PTCEN     23 34 56  11.8   8.5-10.4     -21.3   -16     3886   20 34 03
20 38 27  ---          23 39 37  12.0   8.9-10.3     -22.3   264     3903   20 33 48

20 39 17  J0958+65     23 40 27   8.1  10.2-10.3     -21.6    34     3903   20 39 17
20 41 47  ---          23 42 57   8.2  10.5-10.3     -22.2   150     3913   20 39 18

20 41 47  M82PTCEN     23 42 57  12.1   9.1-10.2     -23.1   -16     3913   20 42 03
20 46 27  ---          23 47 38  12.2   9.5-10.2     -24.1   264     3930   20 41 48

20 47 17  J0958+65     23 48 28   8.4  11.0-10.2     -23.3    34     3930   20 47 17
20 49 47  ---          23 50 59   8.5  11.3-10.2     -23.9   150     3940   20 47 18

20 49 47  M82PTCEN     23 50 59  12.4   9.8-10.1     -24.8   -16     3940   20 50 03
20 54 27  ---          23 55 39  12.5  10.2-10.0     -25.8   264     3957   20 49 48

20 55 17  J0958+65     23 56 29   8.7  11.8-10.1     -25.1    34     3957   20 55 17
20 57 47  ---          23 59 00   8.8  12.0-10.0     -25.6   150     3966   20 55 18

20 57 47  M82PTCEN     23 59 00  12.7  10.4-10.0     -26.5   -16     3966   20 58 02
21 02 22  ---          00 03 36  12.8  10.8 -9.9     -27.5   259     3983   20 57 48

21 03 17  J0958+65     00 04 31   9.1  12.5 -9.9     -26.8    40     3983   21 03 17
21 05 47  ---          00 07 01   9.2  12.8 -9.9     -27.3   150     3993   21 03 18

21 05 47  M82PTCEN     00 07 01  13.0  11.1 -9.8     -28.3   -15     3993   21 06 02
21 10 22  ---          00 11 37  13.2  11.4 -9.8     -29.3   260     4009   21 05 48

21 11 17  J0958+65     00 12 32   9.5  13.3 -9.8     -28.5    40     4009   21 11 17
21 13 47  ---          00 15 02   9.6  13.5 -9.8     -29.0   150     4019   21 11 18

21 13 47  M82PTCEN     00 15 02  13.3  11.7 -9.7     -30.0   -15     4019   21 14 02
21 18 22  ---          00 19 38  13.5  12.0 -9.6     -31.0   260     4036   21 13 48

21 19 17  J0958+65     00 20 33   9.9  14.0 -9.7     -30.2    40     4036   21 19 17
21 21 47  ---          00 23 04  10.0  14.3 -9.6     -30.7   150     4045   21 19 18

21 21 47  M82PTCEN     00 23 04  13.7  12.3 -9.6     -31.8   -15     4045   21 22 02
21 26 22  ---          00 27 40  13.9  12.7 -9.5     -32.7   260     4062   21 21 48

21 27 17  J0958+65     00 28 35  10.3  14.7 -9.5     -31.9    40     4062   21 27 17
21 29 47  ---          00 31 05  10.5  15.0 -9.5     -32.4   150     4072   21 27 18
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

21 29 47  M82PTCEN     00 31 05  14.1  12.9 -9.4     -33.5   -15     4072   21 30 02
21 34 22  ---          00 35 41  14.3  13.3 -9.4     -34.5   260     4089   21 29 48

21 35 17  J0958+65     00 36 36  10.8  15.5 -9.4     -33.6    40     4089   21 35 17
21 37 47  ---          00 39 06  10.9  15.7 -9.3     -34.1   150     4098   21 35 18

21 37 47  M82PTCEN     00 39 06  14.4  13.5 -9.3     -35.2   -15     4098   21 38 02
21 42 22  ---          00 43 42  14.7  13.8 -9.2     -36.2   260     4115   21 37 48

21 43 17  J0958+65     00 44 37  11.2  16.2 -9.3     -35.3    40     4115   21 43 17
21 45 47  ---          00 47 08  11.4  16.4 -9.2     -35.8   150     4125   21 43 18

21 45 47  M82PTCEN     00 47 08  14.9  14.1 -9.2     -37.0   -15     4125   21 46 02
21 50 22  ---          00 51 43  15.1  14.4 -9.1     -37.9   260     4141   21 45 48

21 51 17  J0958+65     00 52 39  11.7  16.8 -9.1     -36.9    40     4141   21 51 17
21 53 47  ---          00 55 09  11.9  17.1 -9.1     -37.5   150     4151   21 51 18

21 53 47  M82PTCEN     00 55 09  15.3  14.7 -9.0     -38.7   -15     4151   21 54 02
21 58 22  ---          00 59 45  15.5  15.0 -9.0     -39.7   260     4168   21 53 48

21 59 17  J0958+65     01 00 40  12.2  17.5 -9.0     -38.6    40     4168   21 59 17
22 01 47  ---          01 03 10  12.4  17.7 -8.9     -39.2   150     4177   21 59 18

22 01 47  M82PTCEN     01 03 10  15.7  15.2 -8.9     -40.4   -15     4177   22 02 02
22 06 22  ---          01 07 46  16.0  15.5 -8.8     -41.4   260     4194   22 01 48

22 07 17  J0958+65     01 08 41  12.8  18.2 -8.9     -40.3    41     4194   22 07 17
22 09 47  ---          01 11 12  12.9  18.4 -8.8     -40.8   150     4204   22 07 18

22 09 47  M82PTCEN     01 11 12  16.2  15.8 -8.8     -42.1   -14     4204   22 10 01
22 14 22  ---          01 15 47  16.5  16.1 -8.7     -43.1   261     4221   22 09 48

22 15 17  J0958+65     01 16 43  13.3  18.8 -8.7     -42.0    41     4221   22 15 17
22 17 47  ---          01 19 13  13.5  19.0 -8.7     -42.5   150     4230   22 15 18

22 17 47  M82PTCEN     01 19 13  16.7  16.3 -8.6     -43.9   -14     4230   22 18 01
22 22 22  ---          01 23 49  16.9  16.6 -8.6     -44.9   261     4247   22 17 48

22 23 17  J0958+65     01 24 44  13.9  19.4 -8.6     -43.7    41     4247   22 23 17
22 25 47  ---          01 27 14  14.1  19.6 -8.5     -44.2   150     4257   22 23 18

22 25 47  M82PTCEN     01 27 14  17.2  16.8 -8.5     -45.6   -14     4257   22 26 01
22 30 22  ---          01 31 50  17.4  17.1 -8.4     -46.6   261     4274   22 25 48
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

22 31 17  J0958+65     01 32 45  14.5  20.1 -8.5     -45.3    41     4274   22 31 17
22 33 47  ---          01 35 16  14.6  20.2 -8.4     -45.9   150     4283   22 31 18

22 33 47  M82PTCEN     01 35 16  17.7  17.3 -8.4     -47.3   -14     4283   22 34 01
22 38 22  ---          01 39 51  18.0  17.6 -8.3     -48.3   261     4300   22 33 48

22 39 17  J0958+65     01 40 46  15.1  20.7 -8.3     -47.0    41     4300   22 39 17
22 41 47  ---          01 43 17  15.2  20.8 -8.3     -47.5   150     4310   22 39 18

22 41 47  M82PTCEN     01 43 17  18.2  17.8 -8.2     -49.1   -14     4310   22 42 01
22 46 22  ---          01 47 53  18.5  18.1 -8.2     -50.0   261     4327   22 41 48

22 47 17  J0958+65     01 48 48  15.7  21.2 -8.2     -48.7    41     4327   22 47 17
22 49 47  ---          01 51 18  15.9  21.4 -8.1     -49.2   150     4336   22 47 18

22 49 47  M82PTCEN     01 51 18  18.7  18.3 -8.1     -50.8   -14     4336   22 50 01
22 54 22  ---          01 55 54  19.0  18.6 -8.0     -51.8   261     4353   22 49 48

22 55 17  J0958+65     01 56 49  16.3  21.8 -8.1     -50.4    41     4353   22 55 17
22 57 47  ---          01 59 20  16.5  22.0 -8.0     -50.9   150     4363   22 55 18

22 57 47  M82PTCEN     01 59 20  19.3  18.8 -8.0     -52.5   -13     4363   22 58 00
23 02 22  ---          02 03 55  19.6  19.0 -7.9     -53.5   262     4380   22 57 48

23 03 17  J0958+65     02 04 50  17.0  22.3 -7.9     -52.0    42     4380   23 03 17
23 05 47  ---          02 07 21  17.2  22.5 -7.9     -52.5   150     4389   23 03 18

23 05 47  M82PTCEN     02 07 21  19.8  19.2 -7.8     -54.2   -13     4389   23 06 00
23 10 22  ---          02 11 57  20.2  19.4 -7.8     -55.2   262     4406   23 05 48

23 11 17  J0958+65     02 12 52  17.6  22.9 -7.8     -53.7    42     4406   23 11 17
23 13 47  ---          02 15 22  17.8  23.0 -7.7     -54.2   150     4416   23 11 18

23 13 47  M82PTCEN     02 15 22  20.4  19.6 -7.7     -56.0   -13     4416   23 14 00
23 18 22  ---          02 19 58  20.7  19.9 -7.6     -57.0   262     4433   23 13 48

23 19 17  J0958+65     02 20 53  18.3  23.4 -7.7     -55.4    42     4433   23 19 17
23 21 47  ---          02 23 23  18.5  23.5 -7.6     -55.9   150     4442   23 19 18

23 21 47  M82PTCEN     02 23 23  21.0  20.0 -7.6     -57.7   -13     4442   23 22 00
23 26 22  ---          02 27 59  21.3  20.3 -7.5     -58.7   262     4459   23 21 48

23 27 17  J0958+65     02 28 54  19.0  23.9 -7.5     -57.0    42     4459   23 27 17
23 29 47  ---          02 31 25  19.2  24.0 -7.5     -57.6   150     4469   23 27 18
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  19 Feb 2016   Day  50 ---

23 29 47  M82PTCEN     02 31 25  21.6  20.4 -7.4     -59.5   -13     4469   23 30 00
23 34 22  ---          02 36 01  21.9  20.6 -7.4     -60.5   262     4486   23 29 48

23 35 17  J0958+65     02 36 56  19.7  24.3 -7.4     -58.7    42     4486   23 35 17
23 37 47  ---          02 39 26  19.9  24.5 -7.3     -59.2   150     4495   23 35 18

23 37 47  M82PTCEN     02 39 26  22.2  20.8 -7.3     -61.2   -13     4495   23 37 59
23 42 22  ---          02 44 02  22.5  21.0 -7.2     -62.2   262     4512   23 37 48

23 43 17  J0958+65     02 44 57  20.4  24.8 -7.3     -60.4    43     4512   23 43 17
23 45 47  ---          02 47 27  20.6  24.9 -7.2     -60.9   150     4522   23 43 18

23 45 47  M82PTCEN     02 47 27  22.8  21.1 -7.2     -62.9   -12     4522   23 45 59
23 50 22  ---          02 52 03  23.2  21.3 -7.1     -63.9   263     4539   23 45 48

23 51 17  J0958+65     02 52 58  21.1  25.2 -7.1     -62.0    43     4539   23 51 17
23 53 47  ---          02 55 29  21.4  25.3 -7.1     -62.6   150     4548   23 51 18

23 53 47  M82PTCEN     02 55 29  23.4  21.5 -7.0     -64.7   -12     4548   23 53 59
23 57 27  ---          02 59 09  23.7  21.6 -7.0     -65.5   208     4562   23 53 48

23 57 47  J0958+65     02 59 29  21.7  25.5 -7.0     -63.4     8     4562   23 57 47
23 59 45  ---          03 01 28  21.9  25.6 -7.0     -63.8   118     4569   23 57 48


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess116.C512glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq_RDBE.dat:
     vc_d

   Setup group:    2         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  13.6      4.1     13.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  13  Setup file default.  Used with PCAL = off
   LO sum=   4924.25  4924.25  4940.25  4940.25  4956.25  4956.25  4972.25  4972.25
   BBC fr=    824.25   824.25   840.25   840.25   856.25   856.25   872.25   872.25
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     840.25    840.25    856.25    856.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  13  14  15  16  17  18  19  20  21  22

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * M82PTCEN          09 51 42.970082   * 09 55 51.700000     09 57 13.368307       0.00
                     69 55 00.43524    * 69 40 46.70000      69 36 01.60467        0.00
                     From catalog imbedded in main SCHED input file.

 * 3C84              03 16 29.567263   * 03 19 48.160094     03 20 52.493734       1.30
   J0319+4130        41 19 51.91701    * 41 30 42.10413      41 34 09.99437        2.69
   0316+413          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
   J0319+41          GSFC 2015a astro solution, unpublished  10208 observations.

   4C39.25           09 23 55.319215   * 09 27 03.013936     09 28 04.619441       0.30
   J0927+3902        39 15 23.56645    * 39 02 20.85186      38 57 56.69607        0.16
   0923+392          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
 * J0927+39          GSFC 2015a astro solution, unpublished 245753 observations.

   0954+658          09 54 57.847923   * 09 58 47.245104     10 00 02.552138       0.02
   J0958+6533        65 48 15.53888    * 65 33 54.81807      65 29 07.09653        0.01
 * J0958+65          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished  13811 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  M82PTCEN   sess116.C512glob      1 2 3 4 5 6 7 8 9 12 13          12.781  2412.179
  3C84       sess116.C512glob      1 2 3 4 5 6 7 8 9 12 13           0.300    39.199
  J0927+39   sess116.C512glob      1 2 3 4 5 6 7 8 9 12 13           0.300    42.899
  J0958+65   sess116.C512glob      1 2 3 4 5 6 7 8 9 12 13           7.138  1455.986


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   M82PTCEN           121.7
   3C84                88.7
   J0927+39           150.9
   J0958+65           125.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

