  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Improving K-band celestial ref.frame for the next multi-waveband ICRF
 Exp. Code:  GC040B  


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       P. Charlot

Address:  Laboratoire d'Astrophysique de Bordeaux
          Universite de Bordeaux - Bat. B18N
          Allee Geoffroy Saint-Hilaire, CS 50023
          33615 Pessac Cedex - France

Phone:    +33 540003284
EMAIL:    patrick.charlot@u-bordeaux.fr
Fax:
Phone during observation:

Observing mode: vlbi

Notes:    Phase cal should be on, Tsys should be measured
          Pointing gaps of 8 min for Effelsberg every 2 hours
          FFs: 0458-020, OJ287, 1546+027, 1921-293 (two 300s scans on each)
          v2: includes preliminary (2hr) ftp fringe test portion for At,Mp

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

 Next scan frequencies:  22012.00  22076.00  22140.00  22204.00  22268.00  22332.00  22396.00  22460.00
 Next BBC frequencies:     512.00    576.00    640.00    704.00    768.00    832.00    896.00    960.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

07 00 00  0736+017     10 33 42  39.8 243.1  2.9      50.1     0        0   07 00 00
07 01 35  ---          10 35 17  39.5 243.4  2.9      50.3    95       24   07 00 01

07 02 21  0904-201     10 36 03  34.7 205.3  1.5      23.1    11       24   07 02 21
07 03 29  ---          10 37 11  34.6 205.6  1.5      23.4    68       42   07 02 22

07 03 58  0847-120     10 37 40  40.0 214.8  1.8      30.2    10       42   07 03 58
07 05 08  ---          10 38 51  39.9 215.1  1.8      30.4    70       60   07 03 59

07 05 38  0938-133     10 39 21  43.6 199.3  1.0      17.0    11       60   07 05 38
07 06 45  ---          10 40 28  43.5 199.7  1.0      17.3    67       77   07 05 39

07 07 35  1016-311     10 41 18  27.6 185.2  0.4       5.3    11       77   07 07 35
07 08 39  ---          10 42 22  27.6 185.5  0.4       5.5    64       94   07 07 36

07 09 02  1034-293     10 42 45  29.7 181.1  0.1       1.1    11       94   07 09 02
07 10 05  ---          10 43 48  29.7 181.3  0.1       1.3    63      110   07 09 03

07 10 28  1048-313     10 44 12  27.6 178.1 -0.1      -2.0    11      110   07 10 28
07 13 00  ---          10 46 44  27.6 178.7 -0.1      -1.3   152      149   07 10 29

07 14 06  1511-100     10 47 50  14.0 111.2 -4.5     -54.6    10      149   07 14 06
07 17 32  ---          10 51 17  14.7 111.7 -4.4     -54.3   206      202   07 14 07

07 18 19  1406-076     10 52 04  28.8 120.7 -3.3     -48.4    11      202   07 18 19
07 19 22  ---          10 53 07  29.0 120.9 -3.3     -48.2    63      218   07 18 20

07 21 10  0723-008     10 54 55  31.4 247.3  3.5      52.6    10      218   07 21 10
07 23 00  ---          10 56 46  31.1 247.7  3.5      52.8   110      247   07 21 11

07 23 45  0610+260     10 57 31  28.8 284.9  4.7      67.8    11      247   07 23 45
07 25 39  ---          10 59 25  28.4 285.1  4.7      67.6   114      276   07 23 46

07 26 34  0805-077     11 00 20  33.8 233.9  2.8      44.6    11      276   07 26 34
07 27 40  ---          11 01 26  33.6 234.2  2.9      44.8    66      293   07 26 35

07 28 07  0802-010     11 01 53  37.5 240.8  2.9      48.7    11      293   07 28 07
07 29 32  ---          11 03 19  37.3 241.1  2.9      48.9    85      315   07 28 08

07 30 09  0834-201     11 03 56  28.1 219.2  2.4      35.5    11      315   07 30 09
07 32 06  ---          11 05 53  27.8 219.7  2.5      35.9   117      345   07 30 10
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

07 33 27  1354-152     11 07 14  28.1 132.1 -2.9     -41.5    11      345   07 33 27
07 35 44  ---          11 09 32  28.5 132.5 -2.8     -41.2   137      381   07 33 28

07 36 34  1606+106     11 10 22  18.2  88.5 -5.0     -61.0    11      381   07 36 34
07 39 21  ---          11 13 09  18.8  88.8 -4.9     -61.0   167      424   07 36 35

07 40 02  NRAO512      11 13 50  24.8  57.0 -5.5     -69.8    10      424   07 40 02
07 41 14  ---          11 15 03  25.0  57.1 -5.4     -69.9    72      442   07 40 03

07 41 49  1746+470     11 15 38  16.8  44.9 -6.5     -62.9    11      442   07 41 49
07 43 22  ---          11 17 11  17.1  45.0 -6.5     -63.1    93      466   07 41 50

07 44 00  1751+288     11 17 49   7.2  60.7 -6.6     -58.9    10      466   07 44 00
07 45 32  ---          11 19 21   7.4  60.9 -6.6     -59.0    92      490   07 44 01

07 46 00  1717+178     11 19 49   8.8  74.6 -6.0     -60.5    10      490   07 46 00
07 47 41  ---          11 21 31   9.2  74.8 -6.0     -60.6   101      516   07 46 01

07 48 34  1514+004     11 22 24  26.5 106.9 -3.9     -55.4    11      516   07 48 34
07 49 58  ---          11 23 48  26.8 107.2 -3.9     -55.3    84      537   07 48 35

07 51 46  0728-235     11 25 36  12.0 232.8  3.9      48.5    11      537   07 51 46
07 52 47  ---          11 26 37  11.8 233.0  3.9      48.6    61      553   07 51 47

07 53 11  0723-265     11 27 02   8.8 231.6  4.0      49.0    10      553   07 53 11
07 54 35  ---          11 28 26   8.6 231.8  4.0      49.2    84      575   07 53 12

07 55 06  0835-339     11 28 57  13.6 215.3  2.8      36.9    11      575   07 55 06
07 56 22  ---          11 30 13  13.5 215.5  2.9      37.2    76      594   07 55 07

07 57 08  1143-332     11 30 59  25.6 176.1 -0.3      -4.0    10      594   07 57 08
07 59 00  ---          11 32 51  25.6 176.6 -0.2      -3.6   112      623   07 57 09

08 00 16  1614+051     11 34 08  18.9  95.6 -4.7     -59.3    10      623   08 00 16
08 01 23  ---          11 35 15  19.1  95.7 -4.7     -59.2    67      640   08 00 17

08 01 51  1546+027     11 35 43  23.7 101.8 -4.3     -57.5    11      640   08 01 51
08 04 18  ---          11 38 10  24.3 102.1 -4.2     -57.4   147      678   08 01 52

08 08 46  1555+001     11 42 39  22.0 104.0 -4.3     -56.6   254      678   08 08 46
08 09 59  ---          11 43 52  22.3 104.2 -4.3     -56.5    73      697   08 08 47

08 10 54  1514+197     11 44 47  40.9  90.0 -3.6     -65.8    10      697   08 10 54
08 12 59  ---          11 46 53  41.3  90.3 -3.5     -65.8   125      729   08 10 55
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

08 14 09  1342+663     11 48 03  50.5  18.2 -1.9    -138.7    11      729   08 14 09
08 16 00  ---          11 49 54  50.6  18.0 -1.9    -139.3   111      758   08 14 10

08 16 36  1357+769     11 50 30  41.7   9.4 -2.1    -142.5    10      758   08 16 36
08 18 20  ---          11 52 15  41.7   9.3 -2.1    -143.0   104      785   08 16 37

08 18 44  1231+811     11 52 39  39.7   2.2 -0.7    -168.4    11      785   08 18 44
08 21 07  ---          11 55 02  39.7   2.0 -0.7    -169.0   143      822   08 18 45

08 21 44  0716+714     11 55 39  36.0 -21.5  4.5     100.4    12      822   08 21 44
08 23 01  ---          11 56 56  35.9 -21.5  4.5     100.1    77      841   08 21 45

08 23 47  0917+624     11 57 43  49.9 -26.8  2.6     123.7    10      841   08 23 47
08 25 23  ---          11 59 19  49.7 -27.0  2.6     123.2    96      866   08 23 48

08 27 18  1324+224     12 01 14  68.7 108.6 -1.5     -61.6    11      866   08 27 18
08 31 51  ---          12 05 48  69.7 110.1 -1.4     -60.7   273      937   08 27 19

08 32 36  1252+119     12 06 33  67.7 146.4 -0.8     -29.1    11      937   08 32 36
08 33 38  ---          12 07 35  67.9 147.0 -0.8     -28.6    62      952   08 32 37

08 34 33  1315-058     12 08 30  49.3 152.1 -1.2     -23.9    10      952   08 34 33
08 35 35  ---          12 09 32  49.4 152.5 -1.2     -23.6    62      968   08 34 34

08 35 57  1329-049     12 09 55  48.9 147.3 -1.4     -27.8    10      968   08 35 57
08 38 11  ---          12 12 09  49.2 148.1 -1.4     -27.2   134     1003   08 35 58

08 40 15  0016+731     12 14 13  14.2  -0.5 11.9       1.5    10     1003   08 40 15
08 43 08  ---          12 17 07  14.2  -0.3 11.9       0.9   173     1048   08 40 16

08 43 48  1849+670     12 17 47  25.1  25.2 -6.5     -70.2    11     1048   08 43 48
08 45 20  ---          12 19 19  25.2  25.2 -6.5     -70.5    92     1071   08 43 49

08 45 52  2116+818     12 19 51  25.1   6.3 -8.9     -43.9    11     1071   08 45 52
08 47 55  ---          12 21 55  25.2   6.4 -8.8     -44.4   123     1103   08 45 53

08 49 42  1622-297     12 23 42   6.2 130.3 -4.1     -49.2    11     1103   08 49 42
08 51 41  ---          12 25 41   6.5 130.6 -4.0     -48.9   119     1134   08 49 43

08 52 17  1650-157     12 26 17  10.4 115.7 -4.5     -53.8    17     1134   08 52 17
08 56 04  ---          12 30 05  11.2 116.2 -4.4     -53.4   227     1192   08 52 18

08 56 32  1656-075     12 30 33  15.0 108.7 -4.5     -55.3    12     1192   08 56 32
09 01 25  ---          12 35 27  16.0 109.4 -4.4     -55.0   293     1268   08 56 33
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

09 02 33  2000+472     12 36 35   9.3  39.5 -7.4     -54.2    10     1268   09 02 33
09 05 25  ---          12 39 27   9.7  39.8 -7.4     -54.7   172     1312   09 02 34

09 05 52  1935+360     12 39 54   7.2  51.9 -7.0     -57.1    11     1312   09 05 52
09 07 23  ---          12 41 26   7.5  52.1 -6.9     -57.3    91     1335   09 05 53

09 09 23  1505+428     12 43 26  59.0  57.3 -2.4    -100.6    11     1335   09 09 23
09 11 19  ---          12 45 22  59.3  57.2 -2.4    -101.0   116     1365   09 09 24

09 12 23  OP326        12 46 27  82.3  59.7 -0.5    -115.9    11     1365   09 12 23
09 16 28  ---          12 50 32  83.0  56.7 -0.5    -119.5   245     1428   09 12 24

09 17 21  1424+240     12 51 25  67.4 102.0 -1.6     -66.8    13     1428   09 17 21
09 18 47  ---          12 52 52  67.7 102.4 -1.6     -66.6    86     1451   09 17 22

09 19 48  1346-109     12 53 53  45.9 159.9 -0.9     -17.6    10     1451   09 19 48
09 20 52  ---          12 54 57  46.0 160.2 -0.9     -17.3    64     1467   09 19 49

09 22 29  1538+477     12 56 34  54.6  49.8 -2.7    -103.5    11     1467   09 22 29
09 24 03  ---          12 58 08  54.8  49.7 -2.7    -103.8    94     1491   09 22 30

09 24 37  1504+377     12 58 43  62.7  66.9 -2.1     -94.8    11     1491   09 24 37
09 27 57  ---          13 02 03  63.3  66.8 -2.1     -95.4   200     1543   09 24 38

09 29 20  0603+882     13 03 26  30.6  -2.1  6.0      88.3    11     1543   09 29 20
09 31 37  ---          13 05 44  30.6  -2.1  6.1      87.8   137     1578   09 29 21

09 32 37  4C67.05      13 06 44   9.4  -8.0 10.6      18.2    10     1578   09 32 37
09 33 37  ---          13 07 44   9.3  -7.9 10.6      18.0    60     1593   09 32 38

09 34 34  1851+488     13 08 41  25.0  46.3 -5.7     -71.3    11     1593   09 34 34
09 37 43  ---          13 11 51  25.5  46.5 -5.7     -71.8   189     1642   09 34 35

09 39 01  0529+483     13 13 09   8.3 -37.6  7.6      52.3    10     1642   09 39 01
09 40 44  ---          13 14 52   8.1 -37.5  7.7      52.0   103     1669   09 39 02

09 41 40  0738+491     13 15 48  27.0 -47.0  5.5      73.4    11     1669   09 41 40
09 43 18  ---          13 17 27  26.7 -46.9  5.6      73.1    98     1694   09 41 41

09 45 41  1708-250     13 19 50  11.1 128.3 -3.9     -48.2    10     1694   09 45 41
09 47 04  ---          13 21 13  11.3 128.5 -3.9     -48.0    83     1715   09 45 42

09 47 31  1726-269     13 21 40   7.2 127.3 -4.2     -50.1    11     1715   09 47 31
09 49 37  ---          13 23 47   7.6 127.6 -4.1     -49.9   126     1748   09 47 32
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

09 50 12  1739-152     13 24 22  12.6 116.6 -4.3     -52.9    17     1748   09 50 12
09 53 55  ---          13 28 05  13.3 117.1 -4.3     -52.6   223     1805   09 50 13

09 56 21  0805+410     13 30 32  26.5 -56.4  5.3      71.2    15     1805   09 56 21
09 58 01  ---          13 32 12  26.2 -56.3  5.4      71.0   100     1831   09 56 22

09 59 30  2039+452     13 33 41  10.8  43.0 -7.1     -56.9    10     1831   09 59 30
10 01 56  ---          13 36 08  11.2  43.2 -7.1     -57.3   146     1869   09 59 31

10 02 34  1929+226     13 36 46  12.2  70.6 -5.9     -61.7    11     1869   10 02 34
10 04 02  ---          13 38 14  12.5  70.8 -5.9     -61.8    88     1891   10 02 35

10 04 31  1959+241     13 38 43   7.3  66.0 -6.4     -59.6    11     1891   10 04 31
10 06 59  ---          13 41 12   7.8  66.3 -6.4     -59.8   148     1929   10 04 32

10 07 47  1829-106     13 42 00   8.9 108.0 -4.9     -56.4    10     1929   10 07 47
10 12 35  ---          13 46 48   9.9 108.6 -4.8     -56.0   288     2004   10 07 48

10 14 21  1636+473     13 48 35  53.6  50.6 -2.8    -101.7    12     2004   10 14 21
10 16 04  ---          13 50 18  53.9  50.5 -2.8    -102.1   103     2030   10 14 22

10 16 32  NRAO512      13 50 46  54.3  63.3 -2.8     -91.2    11     2030   10 16 32
10 18 13  ---          13 52 27  54.7  63.3 -2.8     -91.5   101     2056   10 16 33

10 21 01  1040+244     13 55 16  47.4 -86.9  3.2      70.1    53     2056   10 21 01
10 22 01  ---          13 56 16  47.2 -86.8  3.2      70.1    60     2072   10 21 02

10 22 39  1123+264     13 56 54  56.9 -88.5  2.5      73.2    11     2072   10 22 39
10 23 52  ---          13 58 07  56.6 -88.4  2.5      73.2    73     2090   10 22 40

10 25 50  1555+001     14 00 06  48.2 131.8 -2.0     -39.9   -47     2090   10 26 37
10 27 31  ---          14 01 47  48.5 132.3 -2.0     -39.5    54     2104   10 25 51

10 28 28  1339-206     14 02 44  38.2 185.7  0.3       5.3    11     2104   10 28 28
10 29 28  ---          14 03 44  38.1 186.0  0.3       5.5    60     2120   10 28 29

10 30 03  1339-287     14 04 19  30.0 185.2  0.3       5.1    11     2120   10 30 03
10 32 49  ---          14 07 06  30.0 185.9  0.4       5.8   166     2163   10 30 04

10 33 35  1149-084     14 07 52  39.1 224.7  2.2      37.8    11     2163   10 33 35
10 34 56  ---          14 09 13  38.9 225.1  2.3      38.1    81     2183   10 33 36

10 36 09  1034-293     14 10 26  11.4 225.0  3.5      44.5    11     2183   10 36 09
10 37 11  ---          14 11 28  11.2 225.2  3.6      44.7    62     2199   10 36 10
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

10 37 38  1016-311     14 11 56   7.0 226.8  3.9      47.4    11     2199   10 37 38
10 39 14  ---          14 13 32   6.7 227.0  3.9      47.6    96     2224   10 37 39

10 40 26  1213-172     14 14 44  34.0 214.4  2.0      30.6    10     2224   10 40 26
10 41 36  ---          14 15 54  33.9 214.7  2.0      30.9    70     2242   10 40 27

10 42 03  1156-094     14 16 21  38.0 224.3  2.3      37.6    11     2242   10 42 03
10 43 05  ---          14 17 23  37.9 224.6  2.3      37.8    62     2258   10 42 04

10 43 41  1218-024     14 18 00  46.7 224.6  1.9      37.2    11     2258   10 43 41
10 46 49  ---          14 21 08  46.2 225.5  2.0      37.9   188     2307   10 43 42

10 48 49  0057+678     14 23 08  10.0 367.4-10.7     -17.5    11     2307   10 48 49
10 52 30  ---          14 26 50  10.2 367.8-10.6     -18.3   221     2364   10 48 50

10 53 48  1150+812     14 28 08  37.6 352.8  2.6     137.6    16     2364   10 53 48
10 55 01  ---          14 29 21  37.6 352.8  2.6     137.3    73     2382   10 53 49

10 57 31  1504-166     14 31 52  41.6 168.3 -0.6     -10.6    11     2382   10 57 31
11 00 03  ---          14 34 24  41.7 169.1 -0.6      -9.8   152     2422   10 57 32

11 00 53  1330+022     14 35 14  57.8 209.6  1.0      25.2    10     2422   11 00 53
11 02 14  ---          14 36 36  57.7 210.2  1.0      25.6    81     2442   11 00 54

11 03 26  1704-141     14 37 48  32.2 135.5 -2.5     -38.5    11     2442   11 03 26
11 05 28  ---          14 39 50  32.6 135.9 -2.5     -38.1   122     2474   11 03 27

11 07 05  1142+052     14 41 27  41.5 246.8  2.9      52.5    10     2474   11 07 05
11 09 23  ---          14 43 46  41.0 247.2  3.0      52.8   138     2509   11 07 06

11 10 13  0955+326     14 44 36  30.4 291.8  4.7      70.9    10     2509   11 10 13
11 12 28  ---          14 46 51  30.0 292.0  4.8      70.7   135     2544   11 10 14

11 12 55  1022+237     14 47 18  32.2 279.9  4.3      67.4    11     2544   11 12 55
11 14 00  ---          14 48 24  32.0 280.1  4.4      67.4    65     2561   11 12 56

11 16 22  1749+096     14 50 46  42.8 106.5 -3.0     -56.8    11     2561   11 16 22
11 18 25  ---          14 52 49  43.3 106.9 -3.0     -56.6   123     2593   11 16 23

11 19 51  1514+197     14 54 15  77.6 152.9 -0.4     -24.5    11     2593   11 19 51
11 20 56  ---          14 55 21  77.7 154.0 -0.4     -23.6    65     2609   11 19 52

11 22 11  1511-100     14 56 36  48.8 173.1 -0.3      -6.1    10     2609   11 22 11
11 23 15  ---          14 57 40  48.9 173.5 -0.3      -5.7    64     2626   11 22 12
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

11 23 49  1456-179     14 58 14  41.1 179.2 -0.0      -0.8    11     2626   11 23 49
11 25 07  ---          14 59 32  41.1 179.6 -0.0      -0.4    78     2646   11 23 50

11 25 42  1406-076     15 00 07  49.6 199.2  0.8      16.6    10     2646   11 25 42
11 28 21  ---          15 02 47  49.4 200.2  0.9      17.5   159     2687   11 25 43

11 30 00  OJ287        15 04 26   8.4 288.4  6.1      60.4    10     2687   11 30 00
11 35 00  ---          15 09 27   7.4 288.9  6.2      60.0   300     2764   11 30 01

11 37 59  1746+470     15 12 26  56.0 410.1 -2.6    -104.7    76     2764   11 37 59
11 39 39  ---          15 14 07  56.3 410.0 -2.6    -105.1   100     2790   11 38 00

11 42 23  1354-152     15 16 51  40.1 204.9  1.3      22.1    10     2790   11 42 23
11 43 40  ---          15 18 08  40.0 205.3  1.3      22.5    77     2810   11 42 24

11 45 14  1936+046     15 19 43  23.9  98.9 -4.3     -58.6    10     2810   11 45 14
11 48 31  ---          15 23 00  24.6  99.4 -4.3     -58.4   197     2861   11 45 15

11 54 01  1717+178     15 28 31  61.5 110.5 -1.9     -57.8   251     2861   11 54 01
11 55 20  ---          15 29 50  61.8 110.8 -1.8     -57.6    79     2881   11 54 02

11 56 33  1739-152     15 31 04  34.1 140.5 -2.2     -34.6    10     2881   11 56 33
11 57 54  ---          15 32 25  34.3 140.8 -2.2     -34.3    81     2902   11 56 34

11 59 19  1606+106     15 33 50  68.1 155.5 -0.6     -21.2    10     2902   11 59 19
12 00 22  ---          15 34 53  68.2 156.2 -0.6     -20.7    63     2918   11 59 20

12 02 02  1647-296     15 36 33  27.0 161.6 -1.3     -18.2    11     2918   12 02 02
12 03 11  ---          15 37 43  27.0 161.9 -1.2     -18.0    69     2936   12 02 03

12 03 37  1604-333     15 38 09  25.4 172.8 -0.5      -7.4    10     2936   12 03 37
12 05 33  ---          15 40 05  25.4 173.3 -0.5      -6.9   116     2966   12 03 38

12 07 38  1849+670     15 42 10  44.3  23.3 -3.1    -118.8    10     2966   12 07 38
12 09 02  ---          15 43 35  44.4  23.2 -3.1    -119.2    84     2987   12 07 39

12 11 05  1622-297     15 45 38  28.6 169.6 -0.7     -10.3    11     2987   12 11 05
12 12 10  ---          15 46 43  28.7 169.9 -0.7     -10.0    65     3004   12 11 06

12 13 58  2135+508     15 48 31  25.0  43.7 -5.8     -71.4    10     3004   12 13 58
12 15 11  ---          15 49 45  25.1  43.8 -5.8     -71.7    73     3023   12 13 59

12 15 54  1959+332     15 50 28  37.3  69.3 -4.2     -74.7    11     3023   12 15 54
12 17 26  ---          15 52 00  37.6  69.4 -4.2     -74.8    92     3047   12 15 55
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

12 18 16  2159+505     15 52 50  21.9  42.7 -6.2     -67.9    11     3047   12 18 16
12 19 59  ---          15 54 33  22.1  42.8 -6.1     -68.2   103     3073   12 18 17

12 20 40  2018+295     15 55 14  33.5  72.5 -4.4     -71.0    11     3073   12 20 40
12 22 52  ---          15 57 27  33.9  72.7 -4.4     -71.2   132     3107   12 20 41

12 24 14  0716+714     15 58 49  18.1 -15.3  8.6      45.1    11     3107   12 24 14
12 26 20  ---          16 00 55  18.0 -15.2  8.6      44.6   126     3140   12 24 15

12 26 49  0917+624     16 01 24  22.6 -29.9  6.6      66.9    11     3140   12 26 49
12 28 14  ---          16 02 50  22.5 -29.9  6.7      66.6    85     3161   12 26 50

12 31 15  1424-418     16 05 51  13.9 198.1  1.6      21.2    11     3161   12 31 15
12 32 19  ---          16 06 55  13.8 198.3  1.6      21.4    64     3178   12 31 16

12 32 44  1451-400     16 07 20  17.2 194.1  1.2      16.0    10     3178   12 32 44
12 34 18  ---          16 08 55  17.1 194.4  1.2      16.3    94     3202   12 32 45

12 36 12  1441+522     16 10 49  63.4 329.3  1.4     134.7    10     3202   12 36 12
12 37 27  ---          16 12 04  63.3 329.0  1.5     134.1    75     3222   12 36 13

12 38 29  1357+769     16 13 06  41.4 350.1  2.2     140.4    11     3222   12 38 29
12 41 45  ---          16 16 23  41.3 349.9  2.3     139.5   196     3272   12 38 30

12 42 55  1851+488     16 17 33  55.5 406.7 -2.6    -107.5    22     3272   12 42 55
12 45 10  ---          16 19 48  55.8 406.5 -2.6    -108.1   135     3307   12 42 56

12 47 28  1156-215     16 22 07   8.1 238.4  4.4      52.2    10     3307   12 47 28
12 48 29  ---          16 23 08   7.9 238.6  4.4      52.3    61     3323   12 47 29

12 49 42  1329-049     16 24 21  35.6 236.2  2.8      45.9    10     3323   12 49 42
12 54 42  ---          16 29 22  34.7 237.3  2.9      46.6   300     3400   12 49 43

12 58 07  2215+150     16 32 48  10.6  78.2 -5.8     -60.9    84     3400   12 58 07
12 59 18  ---          16 33 59  10.9  78.4 -5.8     -61.0    71     3418   12 58 08

12 59 50  2150+173     16 34 31  17.5  79.4 -5.3     -62.6    11     3418   12 59 50
13 00 57  ---          16 35 38  17.7  79.5 -5.3     -62.6    67     3435   12 59 51

13 03 37  1315-058     16 38 19  29.9 240.9  3.3      49.1    37     3435   13 03 37
13 07 26  ---          16 42 08  29.2 241.6  3.4      49.6   229     3494   13 03 38

13 08 39  0920+390     16 43 21   5.4 312.4  7.3      54.5    15     3494   13 08 39
13 09 39  ---          16 44 22   5.2 312.5  7.3      54.3    60     3510   13 08 40
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

13 13 41  1252+119     16 48 24  33.2 263.7  3.9      60.8   178     3510   13 13 41
13 15 05  ---          16 49 48  32.9 263.9  3.9      60.8    84     3531   13 13 42

13 15 45  1346-109     16 50 29  29.8 233.0  3.0      44.5    10     3531   13 15 45
13 18 59  ---          16 53 43  29.2 233.7  3.1      45.0   194     3581   13 15 46

13 20 06  1144+402     16 54 50  28.6 301.7  5.1      72.5    11     3581   13 20 06
13 22 14  ---          16 56 59  28.2 301.8  5.1      72.2   128     3614   13 20 07

13 23 01  1324+224     16 57 46  42.7 272.7  3.5      68.0    10     3614   13 23 01
13 24 14  ---          16 58 59  42.4 272.8  3.5      68.0    73     3633   13 23 02

13 24 59  1424+240     16 59 44  55.7 267.7  2.5      69.8    11     3633   13 24 59
13 26 13  ---          17 00 58  55.5 267.9  2.5      69.9    74     3652   13 25 00

13 26 58  1505+428     17 01 43  64.4 305.7  1.9     108.4    10     3652   13 26 58
13 28 43  ---          17 03 29  64.1 305.4  1.9     107.9   105     3679   13 26 59

13 30 35  1726-269     17 05 21  32.1 173.3 -0.4      -6.4    10     3679   13 30 35
13 32 03  ---          17 06 49  32.1 173.7 -0.4      -6.1    88     3702   13 30 36

13 32 56  2051-204     17 07 42  15.3 125.3 -3.8     -48.4    11     3702   13 32 56
13 34 45  ---          17 09 32  15.6 125.6 -3.8     -48.2   109     3730   13 32 57

13 35 10  2047-266     17 09 57  12.1 131.0 -3.7     -46.5    10     3730   13 35 10
13 36 57  ---          17 11 44  12.4 131.3 -3.7     -46.2   107     3758   13 35 11

13 38 17  2351+456     17 13 04  14.9  44.9 -6.7     -61.0    11     3758   13 38 17
13 39 31  ---          17 14 18  15.0  45.0 -6.7     -61.2    74     3777   13 38 18

13 40 22  2229+591     17 15 10  31.4  35.7 -5.3     -81.9    11     3777   13 40 22
13 42 53  ---          17 17 41  31.7  35.8 -5.2     -82.4   151     3816   13 40 23

13 43 45  2319+317     17 18 33  14.9  61.1 -6.1     -62.9    11     3816   13 43 45
13 45 22  ---          17 20 10  15.2  61.3 -6.0     -63.1    97     3841   13 43 46

13 48 44  1903+196     17 23 33  64.3 109.0 -1.7     -59.8    98     3841   13 48 44
13 50 24  ---          17 25 13  64.7 109.5 -1.7     -59.5   100     3866   13 48 45

13 51 20  1751+288     17 26 09  83.5 104.8 -0.5     -71.7    11     3866   13 51 20
13 53 20  ---          17 28 10  84.0 106.1 -0.4     -70.6   120     3897   13 51 21

13 54 21  1935+360     17 29 11  62.6  69.6 -2.2     -92.2    11     3897   13 54 21
13 59 03  ---          17 33 54  63.5  69.5 -2.1     -93.0   282     3970   13 54 22
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

14 01 03  2254+074     17 35 54  12.0  87.9 -5.4     -60.2    10     3970   14 01 03
14 03 02  ---          17 37 53  12.4  88.2 -5.3     -60.2   119     4001   14 01 04

14 03 55  2142+110     17 38 46  29.8  94.3 -4.1     -61.1    11     4001   14 03 55
14 05 10  ---          17 40 02  30.1  94.5 -4.1     -61.0    75     4020   14 03 56

14 07 24  OP326        17 42 16  35.3 -67.5  4.4      74.2    11     4020   14 07 24
14 08 36  ---          17 43 28  35.1 -67.4  4.4      74.0    72     4038   14 07 25

14 12 04  1622-297     17 46 57  26.6 199.2  1.3      19.0    10     4038   14 12 04
14 14 08  ---          17 49 01  26.4 199.7  1.4      19.5   124     4070   14 12 05

14 14 56  1339-206     17 49 49  11.5 236.9  4.1      50.6    11     4070   14 14 56
14 16 02  ---          17 50 55  11.3 237.1  4.1      50.7    66     4087   14 14 57

14 16 31  1339-287     17 51 24   6.1 230.8  4.1      49.8    11     4087   14 16 31
14 19 02  ---          17 53 56   5.6 231.2  4.2      50.1   151     4126   14 16 32

14 20 17  1101+384     17 55 11   9.8 308.7  6.8      58.5    12     4126   14 20 17
14 25 17  ---          18 00 12   8.9 309.2  6.9      57.8   300     4204   14 20 18

14 26 55  0003+380     18 01 50  17.5 415.2 -6.1     -64.4    15     4204   14 26 55
14 28 55  ---          18 03 51  17.9 415.3 -6.1     -64.7   120     4235   14 26 56

14 29 45  2344+798     18 04 41  30.9 371.3 -5.7     -88.5    11     4235   14 29 45
14 32 09  ---          18 07 05  31.0 371.3 -5.7     -89.1   144     4272   14 29 46

14 34 35  1749+096     18 09 31  68.6 191.4  0.3      10.0    10     4272   14 34 35
14 35 41  ---          18 10 38  68.6 192.2  0.3      10.6    66     4289   14 34 36

14 37 11  1708-250     18 12 08  32.4 195.9  1.0      15.1    11     4289   14 37 11
14 38 17  ---          18 13 14  32.3 196.2  1.0      15.4    66     4306   14 37 12

14 38 50  1650-157     18 13 47  39.8 204.9  1.3      22.2    10     4306   14 38 50
14 39 52  ---          18 14 49  39.7 205.2  1.3      22.4    62     4322   14 38 51

14 40 26  1656-075     18 15 23  47.6 208.3  1.3      24.3    10     4322   14 40 26
14 41 45  ---          18 16 43  47.5 208.8  1.3      24.7    79     4342   14 40 27

14 42 28  1829-106     18 17 26  48.6 173.9 -0.3      -5.3    10     4342   14 42 28
14 43 33  ---          18 18 31  48.6 174.3 -0.3      -5.0    65     4359   14 42 29

14 44 13  1908-201     18 19 11  37.7 164.1 -0.9     -14.6    10     4359   14 44 13
14 45 31  ---          18 20 29  37.8 164.5 -0.9     -14.2    78     4379   14 44 14
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

14 47 17  2000+472     18 22 16  64.4  41.7 -1.7    -122.1    11     4379   14 47 17
14 49 03  ---          18 24 02  64.7  41.3 -1.6    -122.8   106     4406   14 47 18

14 49 32  2039+452     18 24 31  59.5  51.0 -2.3    -107.3    11     4406   14 49 32
14 51 36  ---          18 26 35  59.9  50.8 -2.3    -107.8   124     4438   14 49 33

14 53 14  1922-224     18 28 14  35.2 163.3 -1.0     -15.5    10     4438   14 53 14
14 54 43  ---          18 29 43  35.3 163.7 -1.0     -15.2    89     4461   14 53 15

14 55 24  1739-152     18 30 24  42.7 195.4  0.8      13.7    11     4461   14 55 24
14 56 36  ---          18 31 36  42.6 195.8  0.8      14.1    72     4480   14 55 25

14 57 36  1504-166     18 32 36  21.6 233.1  3.4      46.0    11     4480   14 57 36
14 59 44  ---          18 34 45  21.3 233.5  3.4      46.3   128     4513   14 57 37

15 00 28  1514+004     18 35 29  34.2 246.5  3.3      52.1    11     4513   15 00 28
15 01 55  ---          18 36 56  33.9 246.8  3.3      52.3    87     4535   15 00 29

15 03 49  2204-007     18 38 50  31.5 111.9 -3.5     -53.0    10     4535   15 03 49
15 05 35  ---          18 40 37  31.9 112.2 -3.5     -52.8   106     4562   15 03 50

15 06 28  2005-044     18 41 30  49.3 145.0 -1.5     -29.7    11     4562   15 06 28
15 08 15  ---          18 43 17  49.5 145.6 -1.4     -29.2   107     4590   15 06 29

15 09 48  0002+541     18 44 50  29.9  41.2 -5.4     -78.2    11     4590   15 09 48
15 11 02  ---          18 46 04  30.1  41.2 -5.3     -78.4    74     4609   15 09 49

15 11 26  0012+610     18 46 29  30.1  33.2 -5.5     -80.4    10     4609   15 11 26
15 13 04  ---          18 48 07  30.3  33.3 -5.5     -80.8    98     4634   15 11 27

15 13 29  0057+678     18 48 32  27.0  24.5 -6.2     -74.6    10     4634   15 13 29
15 14 51  ---          18 49 54  27.1  24.5 -6.2     -74.9    82     4655   15 13 30

15 15 26  0203+625     18 50 29  18.8  27.0 -7.3     -58.9    11     4655   15 15 26
15 17 10  ---          18 52 13  19.0  27.1 -7.3     -59.2   104     4682   15 15 27

15 17 53  0016+731     18 52 57  31.5  19.1 -5.5     -88.0    10     4682   15 17 53
15 19 29  ---          18 54 33  31.6  19.1 -5.4     -88.4    96     4707   15 17 54

15 19 58  2116+818     18 55 02  37.0   5.5 -2.3    -142.6    10     4707   15 19 58
15 21 16  ---          18 56 20  37.0   5.5 -2.3    -142.9    78     4727   15 19 59

15 21 51  0603+882     18 56 55  28.8  -0.0 11.9       1.0    11     4727   15 21 51
15 24 20  ---          18 59 25  28.8  -0.0 12.0       0.4   149     4765   15 21 52
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

15 25 23  NGC0262      19 00 28  17.7  62.7 -5.8     -64.4    11     4765   15 25 23
15 27 30  ---          19 02 35  18.1  62.9 -5.8     -64.7   127     4798   15 25 24

15 30 00  1546+027     19 05 06  36.2 248.3  3.2      53.1    10     4798   15 30 00
15 35 00  ---          19 10 06  35.2 249.2  3.3      53.6   300     4875   15 30 01

15 37 15  1921-293     19 12 22  30.1 176.5 -0.2      -3.5    75     4875   15 37 15
15 42 15  ---          19 17 23  30.1 177.7 -0.2      -2.2   300     4953   15 37 16

15 44 45  1849+670     19 19 53  53.2 355.0  0.5     168.9    16     4953   15 44 45
15 45 47  ---          19 20 55  53.2 354.9  0.5     168.6    62     4969   15 44 46

15 48 16  1953-325     19 23 25  26.5 171.7 -0.6      -8.4    11     4969   15 48 16
15 50 04  ---          19 25 13  26.5 172.1 -0.6      -8.0   108     4996   15 48 17

15 50 58  1704-141     19 26 07  34.2 221.4  2.3      36.0    11     4996   15 50 58
15 55 05  ---          19 30 15  33.7 222.4  2.4      36.7   247     5060   15 50 59

15 55 49  1606+106     19 30 59  39.3 257.7  3.4      58.7    11     5060   15 55 49
15 57 05  ---          19 32 15  39.0 257.9  3.4      58.8    76     5080   15 55 50

15 58 34  1928+154     19 33 44  75.0 181.6  0.0       1.4    10     5080   15 58 34
15 59 35  ---          19 34 45  74.9 182.5  0.0       2.3    61     5095   15 58 35

16 00 15  1936+046     19 35 26  64.2 177.5 -0.1      -2.1    11     5095   16 00 15
16 02 28  ---          19 37 39  64.2 178.8 -0.0      -1.0   133     5130   16 00 16

16 04 39  1456-179     19 39 50   7.1 243.8  4.6      54.4    11     5130   16 04 39
16 07 29  ---          19 42 41   6.5 244.2  4.7      54.7   170     5173   16 04 40

16 08 03  1511-100     19 43 15  13.8 248.9  4.5      54.7    11     5173   16 08 03
16 10 11  ---          19 45 23  13.4 249.2  4.5      54.8   128     5206   16 08 04

16 11 08  1504+377     19 46 20  33.1 297.2  4.7      74.5    10     5206   16 11 08
16 12 17  ---          19 47 30  32.8 297.3  4.7      74.3    69     5224   16 11 09

16 12 50  1514+197     19 48 03  28.7 276.7  4.5      65.0    10     5224   16 12 50
16 14 39  ---          19 49 52  28.3 276.9  4.5      64.9   109     5252   16 12 51

16 16 30  0133+476     19 51 43  24.3 407.2 -5.8     -70.5    10     5252   16 16 30
16 18 14  ---          19 53 27  24.6 407.3 -5.8     -70.8   104     5279   16 16 31

16 20 21  1614+051     19 55 35  32.9 254.7  3.6      56.4    11     5279   16 20 21
16 21 25  ---          19 56 39  32.6 254.9  3.6      56.5    64     5295   16 20 22
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

16 21 57  1546+027     19 57 11  25.6 256.9  4.1      57.0    10     5295   16 21 57
16 23 40  ---          19 58 54  25.2 257.2  4.1      57.1   103     5322   16 21 58

16 24 24  1647-296     19 59 39  14.9 220.9  3.1      40.5    10     5322   16 24 24
16 26 03  ---          20 01 18  14.7 221.2  3.2      40.8    99     5348   16 24 25

16 26 45  1555+001     20 02 00  24.8 254.0  4.0      55.8    11     5348   16 26 45
16 28 07  ---          20 03 22  24.6 254.2  4.1      55.9    82     5369   16 26 46

16 28 54  1556+335     20 04 09  38.9 290.0  4.1      75.3    11     5369   16 28 54
16 30 30  ---          20 05 46  38.6 290.1  4.1      75.2    96     5393   16 28 55

16 31 53  1622-297     20 07 09  10.1 226.1  3.7      45.6    19     5393   16 31 53
16 34 12  ---          20 09 28   9.7 226.4  3.7      46.0   139     5429   16 31 54

16 35 41  0008-264     20 10 57   9.1 127.8 -4.0     -49.2    11     5429   16 35 41
16 37 03  ---          20 12 20   9.4 128.0 -4.0     -49.0    82     5450   16 35 42

16 37 31  0013-184     20 12 48  13.8 121.0 -4.1     -50.8    11     5450   16 37 31
16 39 46  ---          20 15 03  14.3 121.4 -4.0     -50.6   135     5485   16 37 32

16 42 05  1441+522     20 17 22  27.5 -43.7  5.6      74.6    14     5485   16 42 05
16 43 07  ---          20 18 25  27.4 -43.7  5.6      74.4    62     5501   16 42 06

16 43 41  1538+477     20 18 59  35.3 -50.9  4.6      81.3    10     5501   16 43 41
16 45 40  ---          20 20 58  35.0 -50.8  4.7      81.0   119     5532   16 43 42

16 47 58  2150+173     20 23 16  65.8 117.0 -1.5     -53.5    11     5532   16 47 58
16 49 00  ---          20 24 19  65.9 117.4 -1.5     -53.3    62     5548   16 47 59

16 50 59  0048-097     20 26 18  14.9 110.7 -4.4     -54.7    10     5548   16 50 59
16 52 02  ---          20 27 21  15.1 110.8 -4.4     -54.6    63     5564   16 51 00

16 54 10  1717+178     20 29 29  45.3 264.5  3.2      64.0    11     5564   16 54 10
16 56 11  ---          20 31 31  44.9 264.8  3.2      64.1   121     5595   16 54 11

16 58 02  2315-172     20 33 22  27.9 134.1 -2.8     -40.2    10     5595   16 58 02
17 00 23  ---          20 35 43  28.3 134.6 -2.7     -39.8   141     5631   16 58 03

17 01 48  2215+150     20 37 09  62.1 117.2 -1.7     -52.6    11     5631   17 01 48
17 03 09  ---          20 38 30  62.4 117.6 -1.7     -52.3    81     5652   17 01 49

17 03 41  2142+110     20 39 02  65.2 137.3 -1.1     -36.5    10     5652   17 03 41
17 05 41  ---          20 41 02  65.5 138.3 -1.1     -35.8   120     5683   17 03 42
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

17 07 22  2135+508     20 42 44  67.1  22.6 -0.9    -148.2    11     5683   17 07 22
17 08 49  ---          20 44 11  67.2  22.1 -0.9    -149.0    87     5706   17 07 23

17 09 13  2159+505     20 44 35  65.1  29.9 -1.3    -137.0    10     5706   17 09 13
17 11 10  ---          20 46 32  65.3  29.4 -1.3    -137.9   117     5736   17 09 14

17 12 19  1851+488     20 47 41  61.7 -41.5  1.9     119.7    11     5736   17 12 19
17 13 24  ---          20 48 47  61.5 -41.7  1.9     119.3    65     5753   17 12 20

17 14 02  1746+470     20 49 25  51.8 -51.6  3.0      98.8    11     5753   17 14 02
17 16 16  ---          20 51 39  51.4 -51.7  3.1      98.3   134     5787   17 14 03

17 18 21  0119+041     20 53 44  21.7  97.9 -4.5     -58.7    11     5787   17 18 21
17 19 40  ---          20 55 04  22.0  98.1 -4.5     -58.7    79     5807   17 18 22

17 21 46  1505+428     20 57 10  22.0 -52.5  5.8      67.9    11     5807   17 21 46
17 22 57  ---          20 58 21  21.8 -52.4  5.8      67.8    71     5826   17 21 47

17 26 54  1749+096     21 02 19  41.3 254.9  3.2      57.4    10     5826   17 26 54
17 28 20  ---          21 03 45  41.0 255.1  3.2      57.5    86     5848   17 26 55

17 29 42  1657-261     21 05 07   8.8 232.3  4.0      49.4    11     5848   17 29 42
17 34 42  ---          21 10 08   7.9 233.1  4.1      50.0   300     5925   17 29 43

17 40 39  0056-001     21 16 06  28.9 108.7 -3.7     -54.6   260     5925   17 40 39
17 43 12  ---          21 18 39  29.4 109.1 -3.7     -54.4   153     5965   17 40 40

17 43 45  2355-106     21 19 13  33.9 130.2 -2.7     -41.9    10     5965   17 43 45
17 45 36  ---          21 21 04  34.2 130.7 -2.6     -41.5   111     5993   17 43 46

17 47 15  2229+591     21 22 43  58.9  17.0 -1.2    -150.2    10     5993   17 47 15
17 50 24  ---          21 25 53  59.1  16.4 -1.1    -151.5   189     6042   17 47 16

17 51 38  0017+200     21 27 07  49.8  94.0 -2.9     -66.4    11     6042   17 51 38
17 53 34  ---          21 29 03  50.2  94.3 -2.9     -66.4   116     6072   17 51 39

17 54 13  0003+380     21 29 42  56.9  65.4 -2.6     -91.6    11     6072   17 54 13
17 55 50  ---          21 31 20  57.2  65.4 -2.6     -91.8    97     6097   17 54 14

17 56 45  2234+282     21 32 15  75.7  94.0 -1.1     -77.9    11     6097   17 56 45
17 57 49  ---          21 33 19  75.9  94.2 -1.1     -77.8    64     6113   17 56 46

18 00 02  0249+171     21 35 32  17.6  79.8 -5.3     -62.6    10     6113   18 00 02
18 03 56  ---          21 39 27  18.4  80.2 -5.2     -62.7   234     6174   18 00 03
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

18 05 15  1150+812     21 40 46  22.9  -5.5  9.8      31.0    10     6174   18 05 15
18 06 44  ---          21 42 15  22.8  -5.4  9.8      30.7    89     6196   18 05 16

18 07 04  1231+811     21 42 35  23.7  -6.8  9.1      39.8    10     6196   18 07 04
18 09 42  ---          21 45 14  23.6  -6.8  9.2      39.1   158     6237   18 07 05

18 11 31  2319+317     21 47 03  69.5  79.4 -1.6     -88.0    11     6237   18 11 31
18 13 14  ---          21 48 46  69.9  79.4 -1.6     -88.2   103     6264   18 11 32

18 15 14  0115-214     21 50 47  18.1 129.3 -3.5     -45.6    10     6264   18 15 14
18 16 57  ---          21 52 30  18.4 129.6 -3.4     -45.3   103     6290   18 15 15

18 18 13  0345+460     21 53 46  22.0  48.2 -6.0     -68.1    10     6290   18 18 13
18 19 28  ---          21 55 01  22.2  48.3 -5.9     -68.3    75     6310   18 18 14

18 20 14  4C67.05      21 55 48  36.2  26.3 -4.6     -96.6    11     6310   18 20 14
18 21 39  ---          21 57 13  36.3  26.2 -4.6     -96.9    85     6331   18 20 15

18 22 51  1851+488     21 58 25  50.8 -48.7  3.1     100.3    11     6331   18 22 51
18 25 25  ---          22 00 59  50.3 -48.8  3.1      99.8   154     6371   18 22 52

18 26 53  1342+663     22 02 28  15.5 -20.4  8.3      47.5    12     6371   18 26 53
18 29 29  ---          22 05 04  15.3 -20.2  8.3      46.9   156     6411   18 26 54

18 30 28  1751+288     22 06 03  36.1 -74.9  4.2      71.4    10     6411   18 30 28
18 32 55  ---          22 08 31  35.6 -74.7  4.2      71.2   147     6449   18 30 29

18 33 58  1357+769     22 09 34  22.8 -12.2  8.2      51.6    11     6449   18 33 58
18 36 25  ---          22 12 01  22.7 -12.1  8.2      51.1   147     6487   18 33 59

18 37 01  0716+714     22 12 37  16.1  12.9 -9.2     -36.8    10     6487   18 37 01
18 38 34  ---          22 14 11  16.2  13.0 -9.2     -37.1    93     6511   18 37 02

18 39 42  NRAO512      22 15 19  23.6 -56.5  5.6      68.9    11     6511   18 39 42
18 42 06  ---          22 17 43  23.2 -56.3  5.6      68.6   144     6548   18 39 43

18 42 30  1636+473     22 18 07  25.2 -48.4  5.7      71.3    10     6548   18 42 30
18 44 13  ---          22 19 50  24.9 -48.3  5.7      71.0   103     6575   18 42 31

18 45 00  1441+522     22 20 38  10.6 -34.9  7.6      53.0    11     6575   18 45 00
18 46 06  ---          22 21 44  10.4 -34.8  7.6      52.8    66     6592   18 45 01

18 49 32  1908-201     22 25 10  21.4 228.7  3.2      43.5    11     6592   18 49 32
18 50 45  ---          22 26 24  21.2 228.9  3.2      43.7    73     6610   18 49 33
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

18 51 14  1829-106     22 26 53  20.6 243.3  3.9      51.4    11     6610   18 51 14
18 52 50  ---          22 28 29  20.2 243.5  3.9      51.6    96     6635   18 51 15

18 54 38  0245-167     22 30 17  12.0 117.5 -4.3     -52.7    10     6635   18 54 38
18 55 43  ---          22 31 22  12.2 117.7 -4.3     -52.6    65     6652   18 54 39

18 56 35  0139-097     22 32 15  29.3 123.3 -3.2     -46.8    11     6652   18 56 35
18 58 56  ---          22 34 36  29.7 123.7 -3.1     -46.5   141     6688   18 56 36

19 01 17  2039+452     22 36 57  63.1 -48.3  1.9     113.6    11     6688   19 01 17
19 02 28  ---          22 38 08  62.9 -48.4  1.9     113.2    71     6707   19 01 18

19 03 07  1935+360     22 38 48  52.3 -69.2  3.0      85.1    10     6707   19 03 07
19 04 50  ---          22 40 31  51.9 -69.1  3.0      84.8   103     6733   19 03 08

19 06 00  2116+818     22 41 41  37.8  -3.7  1.5     155.6    16     6733   19 06 00
19 07 51  ---          22 43 32  37.8  -3.8  1.5     155.1   111     6762   19 06 01

19 08 24  0016+731     22 44 05  45.3   9.5 -1.6    -149.9    10     6762   19 08 24
19 10 13  ---          22 45 55  45.3   9.3 -1.6    -150.4   109     6790   19 08 25

19 10 52  0012+610     22 46 34  55.9  18.9 -1.5    -144.2    10     6790   19 10 52
19 12 10  ---          22 47 52  56.0  18.7 -1.5    -144.7    78     6810   19 10 53

19 12 45  0057+678     22 48 27  47.6  17.6 -2.2    -135.2    11     6810   19 12 45
19 14 48  ---          22 50 30  47.8  17.4 -2.2    -135.8   123     6842   19 12 46

19 15 50  NGC0262      22 51 33  64.7  78.9 -2.0     -85.4    10     6842   19 15 50
19 20 50  ---          22 56 33  65.8  79.1 -1.9     -85.9   300     6919   19 15 51

19 24 08  1749+096     22 59 52  16.2 -88.3  5.1      60.7    71     6919   19 24 08
19 29 08  ---          23 04 53  15.1 -87.6  5.2      60.7   300     6996   19 24 09

19 31 32  1717+178     23 07 17  11.6 -76.2  5.8      61.3   128     6996   19 31 32
19 32 46  ---          23 08 31  11.4 -76.0  5.8      61.2    74     7015   19 31 33

19 35 06  0215+015     23 10 52  37.0 113.6 -3.1     -52.1    -3     7015   19 35 09
19 39 22  ---          23 15 09  37.9 114.4 -3.1     -51.6   253     7080   19 35 07

19 41 11  2005-044     23 16 58  33.3 240.5  3.1      48.7    11     7080   19 41 11
19 42 40  ---          23 18 27  33.1 240.8  3.1      48.9    89     7103   19 41 12

19 43 23  1929+226     23 19 10  39.3 275.6  3.8      68.2    10     7103   19 43 23
19 44 43  ---          23 20 30  39.0 275.7  3.8      68.2    80     7124   19 43 24
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

19 45 16  1936+046     23 21 04  32.1 255.2  3.7      56.6    11     7124   19 45 16
19 46 54  ---          23 22 42  31.7 255.5  3.7      56.7    98     7149   19 45 17

19 47 27  1903+196     23 23 15  31.7 275.5  4.3      65.5    11     7149   19 47 27
19 50 41  ---          23 26 29  31.0 275.9  4.3      65.4   194     7199   19 47 28

19 52 37  0222-262     23 28 26  19.2 138.2 -3.0     -39.7    10     7199   19 52 37
19 54 25  ---          23 30 14  19.5 138.5 -2.9     -39.4   108     7227   19 52 38

19 55 39  0309+411     23 31 28  44.4  60.2 -3.7     -85.0    10     7227   19 55 39
19 57 30  ---          23 33 20  44.8  60.3 -3.7     -85.3   111     7256   19 55 40

20 00 54  2135+508     23 36 44  60.0 -38.4  2.0     121.6   126     7256   20 00 54
20 02 22  ---          23 38 12  59.8 -38.7  2.0     121.1    88     7278   20 00 55

20 03 15  1959+241     23 39 05  42.1 -83.7  3.6      69.8    10     7278   20 03 15
20 04 36  ---          23 40 27  41.8 -83.5  3.6      69.8    81     7299   20 03 16

20 05 38  2143-156     23 41 29  36.5 214.9  1.9  W   30.7  -159     7299   20 08 17
20 06 51  ---          23 42 42  36.4 215.2  1.9  W   30.9     0     7277   20 05 39

20 07 48  2251-419     23 43 39  17.0 189.3  0.8      10.7    11     7277   20 07 48
20 09 57  ---          23 45 49  16.9 189.7  0.8      11.2   129     7310   20 07 49

20 10 41  1953-325     23 46 33   7.1 225.5  3.8      46.6    11     7310   20 10 41
20 15 41  ---          23 51 34   6.3 226.3  3.9      47.4   300     7388   20 10 42

20 19 58  2159+505     23 55 51  60.8 322.2  1.9     123.2   141     7388   20 19 58
20 21 45  ---          23 57 38  60.6 321.9  1.9     122.6   107     7415   20 19 59

20 23 11  0459+415     23 59 05  29.4 416.4 -5.1     -73.7    11     7415   20 23 11
20 25 36  ---          00 01 30  29.8 416.5 -5.0     -74.0   145     7452   20 23 12

20 28 44  0008-264     00 04 39  33.3 177.9 -0.1      -2.0    10     7452   20 28 44
20 30 44  ---          00 06 39  33.3 178.5 -0.1      -1.4   120     7483   20 28 45

20 34 02  0218+357     00 09 58  61.9  69.9 -2.2     -91.5   113     7483   20 34 02
20 39 02  ---          00 14 58  62.9  69.9 -2.1     -92.3   300     7561   20 34 03

20 41 38  0507+179     00 17 35  23.0  82.0 -4.9     -63.6    69     7561   20 41 38
20 45 44  ---          00 21 41  23.9  82.4 -4.8     -63.8   246     7624   20 41 39

20 47 59  2018+295     00 23 57  38.2 -74.4  4.0      72.7    15     7624   20 47 59
20 49 43  ---          00 25 41  37.8 -74.3  4.1      72.6   104     7651   20 48 00
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

20 52 07  0306+102     00 28 05  47.4 109.2 -2.7     -55.8     6     7651   20 52 07
20 54 51  ---          00 30 50  47.9 109.7 -2.7     -55.5   164     7693   20 52 08

20 56 05  0133+476     00 32 04  68.5  31.5 -1.1    -137.8    10     7693   20 56 05
20 58 13  ---          00 34 12  68.7  30.7 -1.1    -138.9   128     7726   20 56 06

20 59 27  0235+164     00 35 27  58.4 108.9 -2.1     -58.2    11     7726   20 59 27
21 01 07  ---          00 37 07  58.8 109.4 -2.0     -58.0   100     7752   20 59 28

21 01 47  0312+100     00 37 47  47.9 110.2 -2.6     -55.1    11     7752   21 01 47
21 03 33  ---          00 39 33  48.3 110.6 -2.6     -54.9   106     7779   21 01 48

21 04 09  0240-060     00 40 09  43.0 135.4 -2.1     -37.4    11     7779   21 04 09
21 07 04  ---          00 43 05  43.5 136.2 -2.0     -36.8   175     7824   21 04 10

21 08 00  0406-127     00 44 01  24.3 123.0 -3.4     -47.7    10     7824   21 08 00
21 10 26  ---          00 46 27  24.7 123.4 -3.4     -47.4   146     7862   21 08 01

21 12 18  2059+034     00 48 20  30.6 254.9  3.8      56.3    11     7862   21 12 18
21 15 52  ---          00 51 54  29.9 255.4  3.8      56.6   214     7917   21 12 19

21 16 55  1746+470     00 52 58  12.0 317.9  7.1      57.7    11     7917   21 16 55
21 18 04  ---          00 54 07  11.9 318.0  7.1      57.5    69     7935   21 16 56

21 19 18  2204-007     00 55 21  39.6 240.0  2.8      48.2    11     7935   21 19 18
21 21 04  ---          00 57 07  39.3 240.4  2.8      48.4   106     7962   21 19 19

21 21 41  2150+173     00 57 44  46.4 263.7  3.1      63.9    13     7962   21 21 41
21 23 27  ---          00 59 31  46.0 264.0  3.1      63.9   106     7989   21 21 42

21 24 23  2315-172     01 00 27  36.7 210.6  1.7      27.2    10     7989   21 24 23
21 26 36  ---          01 02 40  36.4 211.2  1.7      27.7   133     8024   21 24 24

21 27 27  2254+074     01 03 31  53.0 238.6  2.1      47.8    10     8024   21 27 27
21 28 51  ---          01 04 56  52.7 239.0  2.1      48.1    84     8045   21 27 28

21 29 34  2355-106     01 05 39  46.2 203.9  1.1      20.7    10     8045   21 29 34
21 30 52  ---          01 06 57  46.1 204.3  1.1      21.1    78     8065   21 29 35

21 31 45  0119+041     01 07 50  63.6 171.3 -0.3      -7.5    10     8065   21 31 45
21 32 50  ---          01 08 55  63.7 171.9 -0.2      -7.0    65     8082   21 31 46

21 34 53  0451-282     01 10 59  10.8 132.0 -3.7     -46.4    11     8082   21 34 53
21 37 37  ---          01 13 43  11.2 132.4 -3.7     -46.0   164     8124   21 34 54
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

21 40 02  2000+472     01 16 08  29.6 310.5  5.2      75.6    10     8124   21 40 02
21 41 11  ---          01 17 18  29.4 310.5  5.2      75.4    69     8142   21 40 03

21 43 13  0220-349     01 19 20  23.0 165.6 -1.1     -15.1    11     8142   21 43 13
21 44 43  ---          01 20 50  23.1 165.9 -1.1     -14.7    90     8165   21 43 14

21 45 50  0113-118     01 21 57  47.9 181.6  0.1       1.4    10     8165   21 45 50
21 49 26  ---          01 25 34  47.8 183.0  0.1       2.6   216     8221   21 45 51

21 50 52  0640+090     01 27 00  13.6  87.6 -5.3     -60.5    10     8221   21 50 52
21 52 06  ---          01 28 14  13.8  87.7 -5.3     -60.5    74     8240   21 50 53

21 52 41  0611+131     01 28 49  22.3  87.6 -4.8     -62.0    10     8240   21 52 41
21 54 26  ---          01 30 35  22.7  87.8 -4.7     -62.0   105     8267   21 52 42

21 54 59  0558+234     01 31 08  29.8  78.9 -4.5     -66.9    11     8267   21 54 59
21 56 33  ---          01 32 42  30.2  79.1 -4.5     -67.0    94     8291   21 55 00

21 56 54  0610+260     01 33 03  28.7  75.1 -4.7     -67.7    10     8291   21 56 54
21 58 40  ---          01 34 49  29.1  75.2 -4.7     -67.9   106     8319   21 56 55

21 59 20  0738+491     01 35 30  21.3  44.8 -6.1     -67.4    10     8319   21 59 20
22 00 26  ---          01 36 36  21.5  44.9 -6.1     -67.5    66     8336   21 59 21

22 01 44  0430+289     01 37 54  51.8  80.6 -3.0     -76.4    10     8336   22 01 44
22 03 14  ---          01 39 24  52.1  80.7 -2.9     -76.5    90     8359   22 01 45

22 04 49  1849+670     01 40 59  23.2 -24.4  6.9      65.9    12     8359   22 04 49
22 07 23  ---          01 43 34  23.0 -24.2  6.9      65.3   154     8398   22 04 50

22 08 40  4C67.05      01 44 51  52.5   7.2 -0.8    -163.6    11     8398   22 08 40
22 11 36  ---          01 47 48  52.6   6.8 -0.7    -164.6   176     8444   22 08 41

22 13 21  0249+171     01 49 33  70.3 128.6 -1.1     -44.8    11     8444   22 13 21
22 16 42  ---          01 52 54  70.9 130.3 -1.0     -43.4   201     8496   22 13 22

22 18 18  0248-266     01 54 31  31.4 165.0 -1.0     -14.4    10     8496   22 18 18
22 20 07  ---          01 56 20  31.5 165.4 -0.9     -14.0   109     8524   22 18 19

22 22 21  1231+811     01 58 34  22.0   3.6-10.6     -19.5    11     8524   22 22 21
22 24 16  ---          02 00 30  22.0   3.6-10.6     -20.0   115     8553   22 22 22

22 26 23  0327-241     02 02 37  31.5 156.2 -1.5     -22.3    11     8553   22 26 23
22 30 29  ---          02 06 44  31.9 157.2 -1.4     -21.4   246     8617   22 26 24
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

22 31 27  0537-286     02 07 42  11.9 134.0 -3.6     -44.8    11     8617   22 31 27
22 34 01  ---          02 10 16  12.3 134.4 -3.5     -44.4   154     8656   22 31 28

22 34 55  0527-053     02 11 10  30.2 118.0 -3.3     -49.7    11     8656   22 34 55
22 36 01  ---          02 12 17  30.5 118.2 -3.3     -49.6    66     8673   22 34 56

22 38 22  1935+360     02 14 38  11.0 -54.3  6.6      60.0    10     8673   22 38 22
22 39 58  ---          02 16 14  10.8 -54.1  6.6      59.8    96     8698   22 38 23

22 44 06  2215+150     02 20 23  33.2 269.0  4.0      63.2    10     8698   22 44 06
22 45 23  ---          02 21 40  32.9 269.2  4.0      63.2    77     8718   22 44 07

22 45 45  CTA102       02 22 02  34.2 263.4  3.8      60.9    10     8718   22 45 45
22 48 20  ---          02 24 38  33.7 263.8  3.8      60.9   155     8758   22 45 46

22 49 31  1959+241     02 25 49   7.6 293.9  6.4      59.7    12     8758   22 49 31
22 51 23  ---          02 27 41   7.2 294.1  6.4      59.6   112     8787   22 49 32

22 52 46  2234+282     02 29 04  40.2 283.2  3.9      72.6    10     8787   22 52 46
22 54 37  ---          02 30 56  39.8 283.3  3.9      72.5   111     8815   22 52 47

22 57 03  0548+084     02 33 22  38.6 104.7 -3.3     -57.3    11     8815   22 57 03
23 00 26  ---          02 36 46  39.4 105.3 -3.3     -57.1   203     8868   22 57 04

23 01 21  0814+425     02 37 41  23.1  53.3 -5.7     -68.8    10     8868   23 01 21
23 03 17  ---          02 39 37  23.4  53.4 -5.7     -69.1   116     8898   23 01 22

23 05 22  0115-214     02 41 42  34.6 203.6  1.4      21.7    10     8898   23 05 22
23 06 25  ---          02 42 46  34.5 203.9  1.4      21.9    63     8914   23 05 23

23 07 09  0139-097     02 43 30  47.4 202.4  1.0      19.4    11     8914   23 07 09
23 10 08  ---          02 46 29  47.2 203.4  1.1      20.3   179     8960   23 07 10

23 12 14  0920+390     02 48 36  12.3  52.1 -6.6     -60.4    10     8960   23 12 14
23 14 09  ---          02 50 31  12.6  52.2 -6.6     -60.7   115     8990   23 12 15

23 15 59  0244-470     02 52 21  12.6 181.0  0.1       1.2    11     8990   23 15 59
23 18 02  ---          02 54 24  12.6 181.3  0.1       1.7   123     9021   23 16 00

23 19 20  0245-167     02 55 43  42.9 182.1  0.1       1.9    10     9021   23 19 20
23 20 50  ---          02 57 13  42.9 182.6  0.1       2.3    90     9044   23 19 21

23 22 05  0104-408     02 58 28  14.5 201.4  1.8      24.3    11     9044   23 22 05
23 27 05  ---          03 03 29  14.1 202.3  1.9      25.4   300     9122   23 22 06
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  27 Feb 2025   Day  58 ---

23 30 00  OJ287        03 06 24  12.1  73.8 -5.8     -61.5    76     9122   23 30 00
23 35 00  ---          03 11 25  13.2  74.3 -5.7     -61.9   300     9199   23 30 01

23 38 06  0458-020     03 14 32  48.5 136.8 -1.8     -36.1   109     9199   23 38 06
23 43 06  ---          03 19 33  49.2 138.4 -1.7     -34.9   300     9276   23 38 07

23 44 57  0222-262     03 21 24  31.9 194.6  0.9      14.0    63     9276   23 44 57
23 46 08  ---          03 22 35  31.8 194.9  0.9      14.3    71     9295   23 44 58

23 47 29  NGC0262      03 23 56  57.3 282.7  2.6      82.2    11     9295   23 47 29
23 48 42  ---          03 25 09  57.1 282.8  2.6      82.1    73     9313   23 47 30

23 49 20  0017+200     03 25 48  47.4 267.6  3.1      66.6    11     9313   23 49 20
23 51 22  ---          03 27 50  47.0 267.8  3.1      66.6   122     9345   23 49 21

23 53 10  0458-020     03 29 38  50.6 141.6 -1.5     -32.3    10     9345   23 53 10
23 54 32  ---          03 31 00  50.8 142.1 -1.5     -31.9    82     9366   23 53 11

23 55 51  0426-380     03 32 20  20.2 168.0 -1.0     -13.1    11     9366   23 55 51
23 57 08  ---          03 33 37  20.2 168.3 -0.9     -12.8    77     9386   23 55 52

 --- Start: Thu  27 Feb 2025   Day  58 -- Stop: Fri  28 Feb 2025   Day  59 ---

23 57 49  0632-235     03 34 18  20.4 135.8 -3.0     -40.9    10     9386   23 57 49
00 00 04  ---          03 36 33  20.8 136.3 -3.0     -40.5   135     9421   23 57 50

00 02 13  0300+470     03 38 43  72.1 -18.6  0.6     156.0    11     9421   00 02 13
00 03 39  ---          03 40 09  72.0 -19.4  0.6     155.1    86     9443   00 02 14

00 04 16  0345+460     03 40 46  74.3   6.6 -0.2    -171.8    11     9443   00 04 16
00 06 09  ---          03 42 39  74.3   5.4 -0.1    -173.3   113     9472   00 04 17

00 07 07  0203+625     03 43 38  54.4 -18.3  1.6     143.6    11     9472   00 07 07
00 08 25  ---          03 44 56  54.3 -18.5  1.6     143.2    78     9492   00 07 08

00 11 18  0220-349     03 47 49  21.9 198.5  1.4      19.4    11     9492   00 11 18
00 13 08  ---          03 49 40  21.7 198.9  1.4      19.8   110     9520   00 11 19

00 13 48  0008-264     03 50 20  13.0 228.6  3.6      46.0    11     9520   00 13 48
00 15 12  ---          03 51 44  12.8 228.9  3.7      46.2    84     9542   00 13 49

00 16 22  0511-220     03 52 54  33.8 157.0 -1.4     -21.3    11     9542   00 16 22
00 17 29  ---          03 54 01  33.9 157.3 -1.3     -21.0    67     9559   00 16 23
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

00 17 56  0451-282     03 54 28  29.6 164.8 -1.0     -14.8    10     9559   00 17 56
00 21 00  ---          03 57 33  29.7 165.6 -0.9     -14.0   184     9607   00 17 57

00 22 28  OK290        03 59 01  12.6  68.1 -6.0     -61.9    11     9607   00 22 28
00 24 24  ---          04 00 57  13.0  68.3 -6.0     -62.0   116     9636   00 22 29

00 25 04  OJ287        04 01 37  23.7  80.0 -4.9     -64.4    11     9636   00 25 04
00 26 29  ---          04 03 03  24.0  80.1 -4.9     -64.4    85     9658   00 25 05

00 27 18  0735+178     04 03 52  39.6  91.9 -3.6     -64.5    10     9658   00 27 18
00 28 48  ---          04 05 22  39.9  92.1 -3.6     -64.5    90     9682   00 27 19

00 30 14  0459+415     04 06 48  74.0  42.3 -1.0    -129.1    11     9682   00 30 14
00 33 05  ---          04 09 40  74.4  41.1 -0.9    -130.8   171     9726   00 30 15

00 34 43  0723-008     04 11 18  33.8 114.8 -3.3     -51.3    10     9726   00 34 43
00 36 13  ---          04 12 48  34.1 115.1 -3.2     -51.2    90     9749   00 34 44

00 37 59  0013-184     04 14 35  15.0 238.0  4.0      50.1    11     9749   00 37 59
00 39 21  ---          04 15 57  14.7 238.2  4.0      50.2    82     9770   00 38 00

00 39 46  2355-106     04 16 22  16.1 247.3  4.3      53.8    11     9770   00 39 46
00 42 00  ---          04 18 36  15.7 247.7  4.3      54.0   134     9804   00 39 47

00 42 54  0056-001     04 19 30  33.9 246.9  3.3      52.3    10     9804   00 42 54
00 45 49  ---          04 22 26  33.3 247.5  3.4      52.6   175     9850   00 42 55

00 46 56  0420-014     04 23 33  58.1 179.5 -0.0      -0.4    10     9850   00 46 56
00 49 16  ---          04 25 53  58.1 180.6  0.0       0.5   140     9886   00 46 57

00 50 20  0640+090     04 26 58  51.3 116.7 -2.3     -51.1    11     9886   00 50 20
00 51 41  ---          04 28 19  51.5 117.1 -2.3     -50.9    81     9906   00 50 21

00 52 26  0527-053     04 29 04  51.1 154.9 -1.0     -21.5    10     9906   00 52 26
00 53 49  ---          04 30 27  51.2 155.4 -1.0     -21.1    83     9928   00 52 27

00 55 46  2319+317     04 32 25  25.6 293.8  5.2      68.5    11     9928   00 55 46
00 58 11  ---          04 34 50  25.1 294.0  5.2      68.3   145     9965   00 55 47

00 59 22  0256-005     04 36 01  51.7 220.7  1.6      34.1    10     9965   00 59 22
01 01 21  ---          04 38 00  51.4 221.3  1.6      34.6   119     9996   00 59 23

01 02 27  0606-223     04 39 07  32.7 154.9 -1.5     -23.3    11     9996   01 02 27
01 05 04  ---          04 41 44  32.9 155.5 -1.5     -22.7   157    10036   01 02 28
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

01 08 00  0716+714     04 44 41  43.9  16.6 -2.7    -129.8    69    10036   01 08 00
01 09 31  ---          04 46 12  44.0  16.5 -2.6    -130.2    91    10060   01 08 01

01 11 18  0119+041     04 47 59  35.3 252.1  3.4      55.2   -69    10060   01 12 27
01 13 18  ---          04 49 59  34.9 252.5  3.4      55.4    51    10073   01 11 19

01 14 30  0244-470     04 51 12   7.7 200.9  2.1      26.6    11    10073   01 14 30
01 18 33  ---          04 55 15   7.4 201.5  2.1      27.4   243    10135   01 14 31

01 20 07  0406-127     04 56 50  45.4 196.3  0.8      14.3    11    10135   01 20 07
01 21 27  ---          04 58 10  45.3 196.7  0.8      14.7    80    10156   01 20 08

01 22 07  0240-060     04 58 50  41.5 227.3  2.2      39.4    10    10156   01 22 07
01 24 20  ---          05 01 03  41.1 227.8  2.3      39.9   133    10190   01 22 08

01 25 48  0012+610     05 02 31  35.3 326.2  4.8      89.6    10    10190   01 25 48
01 28 06  ---          05 04 50  35.0 326.2  4.8      89.1   138    10226   01 25 49

01 28 35  0016+731     05 05 19  34.6 341.1  4.7      98.7    11    10226   01 28 35
01 29 37  ---          05 06 21  34.5 341.1  4.8      98.4    62    10242   01 28 36

01 30 01  2344+798     05 06 45  31.9 348.7  5.3      94.3    11    10242   01 30 01
01 31 30  ---          05 08 14  31.8 348.7  5.3      93.9    89    10265   01 30 02

01 32 09  1357+769     05 08 53  21.2 370.6 -8.8     -43.0    10    10265   01 32 09
01 34 51  ---          05 11 36  21.3 370.7 -8.8     -43.6   162    10307   01 32 10

01 38 18  0610+260     05 15 03  76.0 105.3 -1.0     -67.5    10    10307   01 38 18
01 41 16  ---          05 18 02  76.6 106.4 -1.0     -66.8   178    10352   01 38 19

01 43 11  0346-279     05 19 57  27.8 202.6  1.5      21.9    11    10352   01 43 11
01 44 58  ---          05 21 45  27.6 203.0  1.5      22.3   107    10380   01 43 12

01 45 47  0215+015     05 22 34  38.0 245.5  3.1      51.6    11    10380   01 45 47
01 47 08  ---          05 23 55  37.7 245.8  3.1      51.7    81    10401   01 45 48

01 48 07  0113-118     05 24 54  17.2 244.8  4.1      52.6    11    10401   01 48 07
01 49 53  ---          05 26 40  16.9 245.1  4.2      52.8   106    10428   01 48 08

01 50 51  0003+380     05 27 39  25.6 301.2  5.3      70.1    10    10428   01 50 51
01 52 30  ---          05 29 18  25.3 301.3  5.4      69.9    99    10454   01 50 52

01 53 24  0133+476     05 30 12  43.2 308.9  3.9      89.9    11    10454   01 53 24
01 54 54  ---          05 31 42  42.9 308.9  3.9      89.6    90    10477   01 53 25
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

01 55 47  2351+456     05 32 35  25.3 310.2  5.6      71.2    10    10477   01 55 47
01 57 17  ---          05 34 06  25.0 310.3  5.6      71.0    90    10500   01 55 48

01 57 49  NGC0262      05 34 38  30.4 291.6  4.7      70.8    11    10500   01 57 49
02 00 29  ---          05 37 18  29.9 291.8  4.8      70.5   160    10541   01 57 50

02 01 39  0248-266     05 38 28  20.5 219.5  2.8      37.7    11    10541   02 01 39
02 02 50  ---          05 39 40  20.3 219.7  2.8      37.9    71    10560   02 01 40

02 03 22  0327-241     05 40 12  27.3 213.4  2.2      31.2    10    10560   02 03 22
02 04 45  ---          05 41 35  27.2 213.7  2.2      31.4    83    10581   02 03 23

02 05 27  0537-286     05 42 17  30.7 180.4  0.0       0.3    10    10581   02 05 27
02 08 54  ---          05 45 45  30.7 181.2  0.1       1.2   207    10634   02 05 28

02 10 26  0017+200     05 47 17  17.2 284.0  5.4      63.0    11    10634   02 10 26
02 12 51  ---          05 49 42  16.7 284.3  5.5      62.9   145    10672   02 10 27

02 14 11  0306+102     05 51 02  47.7 250.5  2.7      55.6    11    10672   02 14 11
02 16 14  ---          05 53 06  47.3 250.9  2.7      55.8   123    10703   02 14 12

02 17 31  0627-199     05 54 23  38.6 169.1 -0.6     -10.0    11    10703   02 17 31
02 22 00  ---          05 58 53  38.8 170.5 -0.5      -8.7   269    10773   02 17 32

02 22 43  0834-201     05 59 36  26.4 138.2 -2.6     -37.7    11    10773   02 22 43
02 27 15  ---          06 04 09  27.0 139.2 -2.6     -36.9   272    10843   02 22 44

02 30 21  0529+483     06 07 15  71.2 -16.7  0.5     158.1    68    10843   02 30 21
02 31 49  ---          06 08 43  71.1 -17.4  0.6     157.2    88    10865   02 30 22

02 34 17  0723-265     06 11 12  29.9 160.6 -1.3     -18.7    13    10865   02 34 17
02 35 19  ---          06 12 14  30.0 160.9 -1.2     -18.4    62    10881   02 34 18

02 35 42  0728-235     06 12 37  32.4 158.4 -1.3     -20.3    10    10881   02 35 42
02 36 48  ---          06 13 43  32.5 158.6 -1.3     -20.0    66    10898   02 35 43

02 37 23  0904-201     06 14 18  24.1 135.1 -2.9     -40.4    10    10898   02 37 23
02 38 26  ---          06 15 21  24.2 135.3 -2.9     -40.2    63    10915   02 37 24

02 39 21  0805-077     06 16 17  42.8 140.2 -1.9     -33.8    10    10915   02 39 21
02 41 14  ---          06 18 10  43.1 140.7 -1.9     -33.4   113    10944   02 39 22

02 43 17  2116+818     06 20 13  24.8  -5.9  9.1      40.3    11    10944   02 43 17
02 44 47  ---          06 21 43  24.8  -5.8  9.2      40.0    90    10967   02 43 18
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

02 45 50  1144+402     06 22 47  25.2  57.0 -5.4     -70.1    10    10967   02 45 50
02 46 55  ---          06 23 52  25.4  57.1 -5.4     -70.2    65    10984   02 45 51

02 49 42  0056-001     06 26 39   7.4 265.9  5.4      59.1    11    10984   02 49 42
02 52 12  ---          06 29 10   6.8 266.2  5.5      59.2   150    11022   02 49 43

02 53 34  0249+171     06 30 32  39.2 268.0  3.6      64.3    10    11022   02 53 34
02 55 11  ---          06 32 09  38.9 268.3  3.6      64.3    97    11047   02 53 35

02 55 38  0312+100     06 32 36  40.3 256.7  3.3      58.3    11    11047   02 55 38
02 57 53  ---          06 34 52  39.8 257.1  3.3      58.5   135    11082   02 55 39

02 58 59  0430+289     06 35 58  63.9 274.5  2.0      79.2    11    11082   02 58 59
03 01 06  ---          06 38 05  63.4 274.7  2.0      79.1   127    11115   02 59 00

03 03 04  0805+410     06 40 03  69.1 414.7 -1.5    -111.9    10    11115   03 03 04
03 04 31  ---          06 41 31  69.3 414.4 -1.5    -112.4    87    11137   03 03 05

03 04 54  0814+425     06 41 54  67.2 412.4 -1.6    -112.8    11    11137   03 04 54
03 06 27  ---          06 43 27  67.5 412.1 -1.6    -113.3    93    11161   03 04 55

03 07 03  0738+491     06 44 03  68.5 387.5 -1.0    -142.7    11    11161   03 07 03
03 09 53  ---          06 46 54  68.7 386.5 -1.0    -144.2   170    11205   03 07 04

03 11 34  0235+164     06 48 35  32.1 271.3  4.1      63.9    11    11205   03 11 34
03 13 05  ---          06 50 06  31.8 271.5  4.2      63.9    91    11228   03 11 35

03 13 33  0234+285     06 50 34  36.2 285.2  4.2      71.5    10    11228   03 13 33
03 14 58  ---          06 51 59  35.9 285.4  4.2      71.4    85    11250   03 13 34

03 16 16  0139-097     06 53 18   5.7 255.6  5.2      57.6    11    11250   03 16 16
03 18 59  ---          06 56 01   5.1 255.9  5.2      57.8   163    11292   03 16 17

03 21 25  0955+326     06 58 27  51.6 435.4 -3.0     -80.0    10    11292   03 21 25
03 22 28  ---          06 59 31  51.8 435.5 -3.0     -80.1    63    11309   03 21 26

03 23 26  1123+264     07 00 29  32.0 436.6 -4.4     -68.7    11    11309   03 23 26
03 25 28  ---          07 02 31  32.4 436.8 -4.4     -68.8   122    11340   03 23 27

03 26 24  0917+624     07 03 27  51.2 385.4 -2.3    -127.9    11    11340   03 26 24
03 27 39  ---          07 04 42  51.3 385.2 -2.3    -128.3    75    11359   03 26 25

03 31 15  OJ287        07 08 19  63.5 107.2 -1.8     -61.0    10    11359   03 31 15
03 34 19  ---          07 11 24  64.1 108.0 -1.7     -60.6   184    11407   03 31 16
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

03 35 39  0938-133     07 12 44  32.9 135.4 -2.5     -38.5    11    11407   03 35 39
03 36 40  ---          07 13 45  33.1 135.6 -2.5     -38.3    61    11422   03 35 40

03 37 39  1034-293     07 14 44  12.6 136.3 -3.4     -43.2    11    11422   03 37 39
03 40 00  ---          07 17 05  13.0 136.7 -3.4     -42.8   141    11459   03 37 40

03 40 46  1142+052     07 17 52  22.0  97.8 -4.5     -58.8    10    11459   03 40 46
03 41 55  ---          07 19 01  22.3  97.9 -4.5     -58.8    69    11476   03 40 47

03 43 36  0511-220     07 20 42  29.4 213.7  2.1      31.0    11    11476   03 43 36
03 44 43  ---          07 21 49  29.2 214.0  2.1      31.2    67    11494   03 43 37

03 45 38  0426-380     07 22 44  10.4 213.4  2.9      36.9    10    11494   03 45 38
03 50 06  ---          07 27 13   9.9 214.1  3.0      37.7   268    11563   03 45 39

03 50 57  0256-005     07 28 04  19.7 257.5  4.5      57.1    12    11563   03 50 57
03 52 07  ---          07 29 14  19.4 257.7  4.5      57.2    70    11581   03 50 58

03 52 51  0245-167     07 29 59   7.8 245.6  4.7      54.8    13    11581   03 52 51
03 54 27  ---          07 31 35   7.5 245.8  4.7      54.9    96    11606   03 52 52

03 55 46  0203+625     07 32 54  31.0 328.3  5.4      82.5    12    11606   03 55 46
03 56 59  ---          07 34 07  30.9 328.4  5.4      82.2    73    11624   03 55 47

03 57 31  0300+470     07 34 39  36.8 308.7  4.5      82.7    10    11624   03 57 31
04 01 23  ---          07 38 32  36.2 308.8  4.6      82.1   232    11684   03 57 32

04 02 33  0458-020     07 39 42  40.4 236.2  2.6      45.7    10    11684   04 02 33
04 03 43  ---          07 40 52  40.2 236.5  2.6      45.9    70    11702   04 02 34

04 04 43  0451-282     07 41 53  19.0 218.5  2.8      37.4    10    11702   04 04 43
04 05 58  ---          07 43 08  18.8 218.8  2.8      37.6    75    11722   04 04 44

04 06 27  0537-286     07 43 37  23.9 209.3  2.0      28.7    11    11722   04 06 27
04 08 04  ---          07 45 14  23.7 209.7  2.1      29.0    97    11747   04 06 28

04 08 54  0847-354     07 46 04  21.9 165.9 -1.1     -15.0    11    11747   04 08 54
04 09 56  ---          07 47 06  21.9 166.1 -1.1     -14.7    62    11762   04 08 55

04 10 19  0835-339     07 47 29  24.0 168.6 -0.8     -11.9    11    11762   04 10 19
04 11 23  ---          07 48 34  24.1 168.8 -0.8     -11.6    64    11779   04 10 20

04 12 48  0802-010     07 49 59  57.9 172.2 -0.3      -6.7    11    11779   04 12 48
04 14 09  ---          07 51 20  57.9 172.8 -0.3      -6.2    81    11800   04 12 49
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

04 15 13  0611+131     07 52 24  61.6 237.2  1.6      48.0    10    11800   04 15 13
04 16 15  ---          07 53 26  61.4 237.6  1.6      48.2    62    11816   04 15 14

04 16 48  0548+084     07 54 00  54.1 238.4  2.0      47.8    11    11816   04 16 48
04 18 09  ---          07 55 21  53.8 238.8  2.0      48.1    81    11837   04 16 49

04 18 59  0723-008     07 56 11  57.7 193.7  0.5      11.7    10    11837   04 18 59
04 20 16  ---          07 57 28  57.6 194.2  0.5      12.2    77    11857   04 19 00

04 22 48  1849+670     08 00 01   8.7 366.9-10.8     -15.3    21    11857   04 22 48
04 24 02  ---          08 01 15   8.7 367.0-10.8     -15.6    74    11876   04 22 49

04 26 40  0632-235     08 03 53  31.8 203.8  1.5      22.3    34    11876   04 26 40
04 30 50  ---          08 08 04  31.4 204.8  1.5      23.2   250    11940   04 26 41

04 31 56  0306+102     08 09 10  18.5 271.6  5.0      61.0    11    11940   04 31 56
04 33 53  ---          08 11 07  18.1 271.8  5.0      61.0   117    11970   04 31 57

04 34 33  0422+004     08 11 47  28.8 251.9  3.8      54.9    11    11970   04 34 33
04 36 48  ---          08 14 03  28.3 252.3  3.8      55.1   135    12005   04 34 34

04 37 43  0507+179     08 14 58  46.7 264.1  3.1      64.2    11    12005   04 37 43
04 39 08  ---          08 16 23  46.4 264.3  3.1      64.2    85    12027   04 37 44

04 40 06  0420-014     08 17 21  26.2 251.3  3.9      54.6    10    12027   04 40 06
04 43 23  ---          08 20 39  25.5 251.8  3.9      54.9   197    12078   04 40 07

04 44 28  0459+415     08 21 44  49.3 299.8  3.3      89.3    10    12078   04 44 28
04 47 00  ---          08 24 16  48.8 299.8  3.3      88.9   152    12117   04 44 29

04 49 27  1244-255     08 26 44   5.7 124.8 -4.4     -51.8    15    12117   04 49 27
04 54 27  ---          08 31 45   6.6 125.5 -4.3     -51.2   300    12194   04 49 28

04 57 40  0345+460     08 34 58  34.2 -52.2  4.7      79.6    59    12194   04 57 40
05 00 16  ---          08 37 35  33.8 -52.1  4.8      79.2   156    12234   04 57 41

05 03 14  1342+663     08 40 33  33.3  28.2 -5.1     -88.7   113    12234   05 03 14
05 04 39  ---          08 41 58  33.5  28.2 -5.0     -89.0    85    12256   05 03 15

05 05 17  1441+522     08 42 37  23.5  42.3 -6.0     -69.7    10    12256   05 05 17
05 06 29  ---          08 43 49  23.6  42.3 -6.0     -69.9    72    12275   05 05 18

05 08 00  1218-024     08 45 20  28.4 112.7 -3.6     -52.6    33    12275   05 08 00
05 10 01  ---          08 47 21  28.8 113.0 -3.6     -52.4   121    12306   05 08 01
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

05 11 50  0640+090     08 49 11  53.8 239.8  2.1      48.8    11    12306   05 11 50
05 13 27  ---          08 50 48  53.5 240.2  2.1      49.1    97    12331   05 11 51

05 14 28  0847-120     08 51 49  47.0 180.2  0.0       0.1    10    12331   05 14 28
05 15 52  ---          08 53 13  47.0 180.7  0.0       0.6    84    12352   05 14 29

05 16 34  0736+017     08 53 55  56.1 214.3  1.2      29.0    10    12352   05 16 34
05 17 43  ---          08 55 05  56.0 214.8  1.2      29.4    69    12370   05 16 35

05 18 26  0735+178     08 55 48  68.4 237.5  1.3      49.6    11    12370   05 18 26
05 23 26  ---          09 00 48  67.4 239.5  1.4      51.1   300    12448   05 18 27

05 26 23  1004+141     09 03 46  67.4 134.6 -1.1     -39.1    94    12448   05 26 23
05 28 06  ---          09 05 29  67.7 135.5 -1.1     -38.4   103    12474   05 26 24

05 30 03  0610+260     09 07 27  52.1 274.1  2.9      72.8    11    12474   05 30 03
05 31 07  ---          09 08 31  51.9 274.2  2.9      72.8    64    12491   05 30 04

05 33 28  1330+022     09 10 52  21.6 101.2 -4.4     -57.6    10    12491   05 33 28
05 38 28  ---          09 15 53  22.7 101.9 -4.3     -57.4   300    12568   05 33 29

05 44 22  0218+357     09 21 48   7.0 -52.0  7.0      56.9   236    12568   05 44 22
05 45 44  ---          09 23 10   6.8 -51.8  7.0      56.8    82    12589   05 44 23

05 46 35  2344+798     09 24 01  22.6  -6.2  9.6      33.1    11    12589   05 46 35
05 48 04  ---          09 25 31  22.6  -6.1  9.6      32.7    89    12612   05 46 36

05 50 26  1016-311     09 27 53  26.6 167.7 -0.9     -12.4    10    12612   05 50 26
05 51 56  ---          09 29 23  26.7 168.0 -0.8     -12.1    90    12635   05 50 27

05 53 20  1424+240     09 30 47  24.7  76.0 -5.0     -65.7    11    12635   05 53 20
05 55 31  ---          09 32 59  25.1  76.2 -4.9     -65.9   131    12669   05 53 21

05 57 01  1144+402     09 34 29  61.4  62.0 -2.2     -98.2    11    12669   05 57 01
05 58 40  ---          09 36 08  61.7  61.9 -2.2     -98.6    99    12694   05 57 02

05 59 16  1101+384     09 36 44  70.2  61.9 -1.5    -105.4    11    12694   05 59 16
06 00 16  ---          09 37 45  70.4  61.7 -1.5    -105.7    60    12710   05 59 17

06 02 54  0458-020     09 40 23  16.5 257.5  4.6      57.2    11    12710   06 02 54
06 04 17  ---          09 41 46  16.2 257.7  4.7      57.3    83    12731   06 02 55

06 04 54  0511-220     09 42 23   7.1 239.3  4.5      52.9    11    12731   06 04 54
06 06 02  ---          09 43 31   6.8 239.4  4.5      53.0    68    12749   06 04 55
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               Improving K-band celestial ref.frame for the next multi-waveband ICRF
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri  28 Feb 2025   Day  59 ---

06 07 15  0300+470     09 44 45  16.0 316.1  6.7      61.9    11    12749   06 07 15
06 08 16  ---          09 45 46  15.8 316.1  6.7      61.7    61    12764   06 07 16

06 08 39  0309+411     09 46 09  14.4 309.9  6.5      61.6    11    12764   06 08 39
06 10 03  ---          09 47 33  14.2 310.1  6.5      61.4    84    12786   06 08 40

06 12 23  1213-172     09 49 54  30.1 138.7 -2.5     -36.6    10    12786   06 12 23
06 14 34  ---          09 52 05  30.4 139.2 -2.4     -36.2   131    12820   06 12 24

06 16 39  OK290        09 54 10  84.4 170.4 -0.1      -9.1    11    12820   06 16 39
06 21 03  ---          09 58 35  84.5 180.7  0.0       0.7   264    12888   06 16 40

06 23 13  1329-049     10 00 45  27.8 115.7 -3.5     -51.1    10    12888   06 23 13
06 24 17  ---          10 01 49  28.0 115.9 -3.5     -51.0    64    12904   06 23 14

06 24 58  1354-152     10 02 31  16.8 120.4 -3.9     -50.4    11    12904   06 24 58
06 26 58  ---          10 04 31  17.2 120.7 -3.9     -50.2   120    12935   06 24 59

06 27 59  1504+377     10 05 32  28.8  61.3 -5.0     -71.8    11    12935   06 27 59
06 29 44  ---          10 07 17  29.1  61.4 -5.0     -72.1   105    12962   06 28 00

06 31 25  0814+425     10 08 59  65.3 -54.2  1.8     109.3    11    12962   06 31 25
06 32 40  ---          10 10 14  65.1 -54.4  1.8     108.9    75    12982   06 31 26

06 36 00  0826-373     10 13 34  17.5 201.5  1.7      23.4    10    12982   06 36 00
06 40 54  ---          10 18 29  17.1 202.4  1.8      24.4   294    13057   06 36 01

06 41 26  0723-265     10 19 01  19.4 220.3  2.9      38.6    11    13057   06 41 26
06 44 05  ---          10 21 41  19.0 220.8  2.9      39.0   159    13098   06 41 27

06 45 17  0430+289     10 22 53  16.8 294.4  5.8      63.8    12    13098   06 45 17
06 50 17  ---          10 27 54  15.8 294.9  5.9      63.3   300    13176   06 45 18

06 51 06  0459+415     10 28 43  26.0 304.8  5.4      71.1    21    13176   06 51 06
06 55 07  ---          10 32 45  25.3 305.1  5.5      70.5   241    13238   06 51 07

06 55 39  0354+559     10 33 17  20.8 323.9  6.5      65.6    11    13238   06 55 39
06 56 43  ---          10 34 21  20.7 324.0  6.6      65.5    64    13254   06 55 40

06 57 13  4C67.05      10 34 51  17.5 339.8  8.1      50.7    11    13254   06 57 13
06 58 15  ---          10 35 53  17.4 339.9  8.1      50.4    62    13270   06 57 14

06 58 50  2116+818     10 36 28  23.3 363.0-10.6     -19.6    11    13270   06 58 50
07 00 00  ---          10 37 38  23.3 363.1-10.6     -19.9    70    13288   06 58 51


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess125.K2048globgeo
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    1         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       RCP       RCP       RCP       RCP       RCP       RCP       RCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         B         B         B         B         B         B         B 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   3  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22012.00  22076.00  22140.00  22204.00  22268.00  22332.00  22396.00  22460.00
   BBC fr=     512.00    576.00    640.00    704.00    768.00    832.00    896.00    960.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   2  4  5  7
   CRD fr=     599.99    727.99    791.99    919.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   3   4   5   6   7   8   9  10  11  12

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 0002+541          00 02 29.056237   * 00 05 04.363337     00 06 20.100410       0.00
   0002+541          54 11 43.18502    * 54 28 24.92431      54 36 52.12346        0.00
                     From catalog imbedded in main SCHED input file.

 * 0003+380          00 03 22.335497   * 00 05 57.175386     00 07 13.416058       0.00
   0003+380          38 03 33.40987    * 38 20 15.14894      38 28 39.23503        0.00
                     From catalog imbedded in main SCHED input file.

 * 0008-264          00 08 28.884832   * 00 11 01.246737     00 12 16.902994       0.00
   0008-264         -26 29 14.77706    *-26 12 33.37700     -26 04 19.37428        0.00
                     From catalog imbedded in main SCHED input file.

 * 0012+610          00 12 07.893397   * 00 14 48.792099     00 16 06.868545       0.00
   0012+610          61 01 03.42419    * 61 17 43.54242      61 26 12.08805        0.00
                     From catalog imbedded in main SCHED input file.

 * 0013-184          00 13 01.930830   * 00 15 34.324529     00 16 50.023437       0.00
   0013-184         -18 24 05.90004    *-18 07 25.58581     -17 59 11.37658        0.00
                     From catalog imbedded in main SCHED input file.

 * 0016+731          00 16 54.195078   * 00 19 45.786356     00 21 07.273109       0.00
   0016+731          73 10 51.40707    * 73 27 30.01751      73 36 00.48476        0.00
                     From catalog imbedded in main SCHED input file.

 * 0017+200          00 17 02.119547   * 00 19 37.854490     00 20 54.984766       0.00
   0017+200          20 05 06.80757    * 20 21 45.64453      20 30 05.46902        0.00
                     From catalog imbedded in main SCHED input file.

   0046+316          00 46 04.857324   * 00 48 47.141481     00 50 07.495706       0.00
 * NGC0262           31 41 04.49523    * 31 57 25.08475      32 05 39.83914        0.00
                     From catalog imbedded in main SCHED input file.

 * 0048-097          00 48 09.975906   * 00 50 41.317374     00 51 56.596655       0.00
   0048-097         -09 45 24.21192    *-09 29 05.21029     -09 21 00.24767        0.00
                     From catalog imbedded in main SCHED input file.

 * 0056-001          00 56 31.756754   * 00 59 05.514933     01 00 21.998613       0.00
   0056-001         -00 09 18.82697    * 00 06 51.62070      00 14 54.29821        0.00
                     From catalog imbedded in main SCHED input file.

 * 0057+678          00 57 35.633560   * 01 00 51.663929     01 02 27.281204       0.00
   0057+678          67 52 11.98183    * 68 08 20.53125      68 16 38.24292        0.00
                     From catalog imbedded in main SCHED input file.

 * 0104-408          01 04 27.574524   * 01 06 45.107979     01 07 53.484174       0.00
   0104-408         -40 50 21.55660    *-40 34 19.96069     -40 26 27.91939        0.00
                     From catalog imbedded in main SCHED input file.

 * 0113-118          01 13 43.218974   * 01 16 12.522018     01 17 26.886146       0.00
   0113-118         -11 52 04.53068    *-11 36 15.43459     -11 28 25.64272        0.00
                     From catalog imbedded in main SCHED input file.

 * 0115-214          01 15 23.570466   * 01 17 48.780128     01 19 01.110562       0.00
   0115-214         -21 26 53.45599    *-21 11 06.63317     -21 03 19.72511        0.00
                     From catalog imbedded in main SCHED input file.

 * 0119+041          01 19 21.391387   * 01 21 56.861684     01 23 14.276827       0.00
   0119+041          04 06 44.01331    * 04 22 24.73426      04 30 13.96877        0.00
                     From catalog imbedded in main SCHED input file.

 * 0133+476          01 33 55.103062   * 01 36 58.594807     01 38 29.554310       0.00
   0133+476          47 36 12.85362    * 47 51 29.10001      47 59 18.24779        0.00
                     From catalog imbedded in main SCHED input file.

 * 0139-097          01 39 08.986366   * 01 41 37.939741     01 42 52.233394       0.00
   0139-097         -09 45 09.38648    *-09 30 01.78610     -09 22 32.14645        0.00
                     From catalog imbedded in main SCHED input file.

 * 0203+625          02 03 22.157625   * 02 07 03.016779     02 08 52.583093       0.00
   0203+625          62 31 56.07856    * 62 46 12.06762      62 53 36.00566        0.00
                     From catalog imbedded in main SCHED input file.

 * 0208-512          02 08 56.947207   * 02 10 46.200458     02 11 40.715178       0.00
   0208-512         -51 15 07.67929    *-51 01 01.89206     -50 54 09.66677        0.00
                     From catalog imbedded in main SCHED input file.

 * 0215+015          02 15 14.130222   * 02 17 48.954743     02 19 06.327150       0.00
   0215+015          01 31 00.16086    * 01 44 49.69896      01 51 43.51525        0.00
                     From catalog imbedded in main SCHED input file.

 * 0218+357          02 18 04.125914   * 02 21 05.468239     02 22 35.922737       0.00
   0218+357          35 42 31.94481    * 35 56 13.73649      36 03 14.05197        0.00
                     From catalog imbedded in main SCHED input file.

 * 0220-349          02 20 49.597016   * 02 22 56.401633     02 23 59.809233       0.00
   0220-349         -34 55 05.08040    *-34 41 28.73016     -34 34 49.72329        0.00
                     From catalog imbedded in main SCHED input file.

 * 0222-262          02 22 56.437334   * 02 25 10.889574     02 26 18.141429       0.00
   0222-262         -26 16 49.54626    *-26 03 18.79753     -25 56 41.12939        0.00
                     From catalog imbedded in main SCHED input file.

   0224+671          02 24 41.169027   * 02 28 50.051463     02 30 53.893189       0.00
 * 4C67.05           67 07 39.70867    * 67 21 03.02930      67 28 02.21649        0.00
                     From catalog imbedded in main SCHED input file.

 * 0234+285          02 34 55.589582   * 02 37 52.405669     02 39 20.774103       0.00
   0234+285          28 35 11.40764    * 28 48 08.98989      28 54 45.43181        0.00
                     From catalog imbedded in main SCHED input file.

 * 0235+164          02 35 52.630205   * 02 38 38.930097     02 40 02.103611       0.00
   0235+164          16 24 04.01613    * 16 36 59.27455      16 43 30.71843        0.00
                     From catalog imbedded in main SCHED input file.

 * 0240-060          02 40 43.239986   * 02 43 12.469466     02 44 27.187962       0.00
   0240-060         -06 03 37.48476    *-05 50 55.29535     -05 44 37.10557        0.00
                     From catalog imbedded in main SCHED input file.

 * 0244-470          02 44 13.566940   * 02 46 00.117986     02 46 53.502281       0.00
   0244-470         -47 03 50.58470    *-46 51 17.23260     -46 45 11.39975        0.00
                     From catalog imbedded in main SCHED input file.

 * 0245-167          02 45 47.266520   * 02 48 07.732228     02 49 18.101927       0.00
   0245-167         -16 44 14.26824    *-16 31 46.38570     -16 25 38.13774        0.00
                     From catalog imbedded in main SCHED input file.

 * 0248-266          02 48 24.330369   * 02 50 35.569192     02 51 41.337836       0.00
   0248-266         -26 40 03.00057    *-26 27 42.51544     -26 21 40.18874        0.00
                     From catalog imbedded in main SCHED input file.

 * 0249+171          02 49 19.937204   * 02 52 07.718696     02 53 31.711881       0.00
   0249+171          17 06 26.05860    * 17 18 42.68853      17 24 55.23081        0.00
                     From catalog imbedded in main SCHED input file.

 * 0256-005          02 56 55.117078   * 02 59 28.516158     03 00 45.395932       0.00
   0256-005         -00 31 54.17503    *-00 19 59.97557     -00 14 04.11448        0.00
                     From catalog imbedded in main SCHED input file.

 * 0300+470          03 00 10.111194   * 03 03 35.242212     03 05 17.876681       0.00
   0300+470          47 04 33.67698    * 47 16 16.27532      47 22 21.29471        0.00
                     From catalog imbedded in main SCHED input file.

 * 0306+102          03 06 20.921063   * 03 09 03.623488     03 10 25.192394       0.00
   0306+102          10 17 51.96468    * 10 29 16.34087      10 35 00.72199        0.00
                     From catalog imbedded in main SCHED input file.

 * 0309+411          03 09 44.793503   * 03 13 01.962118     03 14 40.723821       0.00
   0309+411          41 08 48.80282    * 41 20 01.18341      41 25 49.51195        0.00
                     From catalog imbedded in main SCHED input file.

 * 0312+100          03 12 38.457838   * 03 15 21.139816     03 16 42.735059       0.00
   0312+100          10 01 39.05818    * 10 12 43.08377      10 18 17.23993        0.00
                     From catalog imbedded in main SCHED input file.

 * 0327-241          03 27 43.872799   * 03 29 54.075541     03 30 59.520703       0.00
   0327-241         -24 07 23.06437    *-23 57 08.77328     -23 52 09.16689        0.00
                     From catalog imbedded in main SCHED input file.

 * 0345+460          03 45 46.869267   * 03 49 18.741575     03 51 05.187756       0.00
   0345+460          46 00 52.34669    * 46 09 59.65777      46 14 47.08212        0.00
                     From catalog imbedded in main SCHED input file.

 * 0346-279          03 46 34.026295   * 03 48 38.144559     03 49 40.640484       0.00
   0346-279         -27 58 20.96631    *-27 49 13.56577     -27 44 48.29607        0.00
                     From catalog imbedded in main SCHED input file.

 * 0354+559          03 54 31.306907   * 03 58 30.188157     04 00 30.319867       0.00
   0354+559          55 58 10.41744    * 56 06 44.46057      56 11 17.75398        0.00
                     From catalog imbedded in main SCHED input file.

 * 0406-127          04 06 45.326890   * 04 09 05.769715     04 10 16.531794       0.00
   0406-127         -12 46 38.98053    *-12 38 48.14394     -12 34 57.56253        0.00
                     From catalog imbedded in main SCHED input file.

 * 0420-014          04 20 43.539844   * 04 23 15.800721     04 24 32.555368       0.00
   0420-014         -01 27 28.70038    *-01 20 33.06567     -01 17 06.84625        0.00
                     From catalog imbedded in main SCHED input file.

 * 0422+004          04 22 12.515410   * 04 24 46.842055     04 26 04.640571       0.00
   0422+004          00 29 16.67920    * 00 36 06.32939      00 39 30.15093        0.00
                     From catalog imbedded in main SCHED input file.

 * 0426-380          04 26 54.700111   * 04 28 40.424270     04 29 33.927379       0.00
   0426-380         -38 02 52.12294    *-37 56 19.58039     -37 53 13.59436        0.00
                     From catalog imbedded in main SCHED input file.

 * 0430+289          04 30 29.680348   * 04 33 37.829854     04 35 12.681095       0.00
   0430+289          28 59 40.38990    * 29 05 55.47708      29 09 11.25649        0.00
                     From catalog imbedded in main SCHED input file.

 * 0451-282          04 51 15.126320   * 04 53 14.646801     04 54 15.155309       0.00
   0451-282         -28 12 29.38859    *-28 07 37.32707     -28 05 19.94738        0.00
                     From catalog imbedded in main SCHED input file.

 * 0454-810          04 54 17.961981   * 04 50 05.440230     04 48 02.657023       0.00
   0454-810         -81 05 54.60914    *-81 01 02.23137     -80 58 39.42162        0.00
                     From catalog imbedded in main SCHED input file.

 * 0458-020          04 58 41.344685   * 05 01 12.809881     05 02 29.360359       0.00
   0458-020         -02 03 33.86898    *-01 59 14.25643     -01 57 06.53682        0.00
                     From catalog imbedded in main SCHED input file.

 * 0459+415          04 59 06.857453   * 05 02 37.988219     05 04 24.652359       0.00
   0459+415          41 35 03.74559    * 41 39 19.34756      41 41 38.70769        0.00
                     From catalog imbedded in main SCHED input file.

 * 0507+179          05 07 07.486537   * 05 10 02.369123     05 11 30.754215       0.00
   0507+179          17 56 58.64620    * 18 00 41.58165      18 02 37.12382        0.00
                     From catalog imbedded in main SCHED input file.

 * 0511-220          05 11 41.814305   * 05 13 49.114323     05 14 53.608677       0.00
   0511-220         -22 02 41.28436    *-21 59 16.09223     -21 57 40.92256        0.00
                     From catalog imbedded in main SCHED input file.

 * 0524-485          05 24 57.685528   * 05 26 16.671327     05 26 57.110936       0.00
   0524-485         -48 33 06.67003    *-48 30 36.79168     -48 29 32.97001        0.00
                     From catalog imbedded in main SCHED input file.

 * 0527-053          05 27 25.984602   * 05 29 53.533504     05 31 08.256473       0.00
   0527-053         -05 21 58.25817    *-05 19 41.61728     -05 18 36.64879        0.00
                     From catalog imbedded in main SCHED input file.

 * 0529+483          05 29 27.565374   * 05 33 15.865783     05 35 11.478304       0.00
   0529+483          48 20 47.97041    * 48 22 52.80774      48 24 07.64434        0.00
                     From catalog imbedded in main SCHED input file.

 * 0537-286          05 37 56.930590   * 05 39 54.281469     05 40 53.914824       0.00
   0537-286         -28 41 28.03796    *-28 39 55.94809     -28 39 18.70319        0.00
                     From catalog imbedded in main SCHED input file.

 * 0548+084          05 48 27.535062   * 05 51 11.229346     05 52 34.186156       0.00
   0548+084          08 28 26.71858    * 08 29 11.22194      08 29 33.77747        0.00
                     From catalog imbedded in main SCHED input file.

 * 0558+234          05 58 44.684485   * 06 01 47.357025     06 03 19.971385       0.00
   0558+234          23 24 54.65126    * 23 24 53.48480      23 24 57.38392        0.00
                     From catalog imbedded in main SCHED input file.

 * 0603+882          06 04 00.850864   * 06 42 06.135531     07 01 08.672585       0.00
   0603+882          88 13 36.00619    * 88 11 55.01559      88 10 26.70020        0.00
                     From catalog imbedded in main SCHED input file.

 * 0606-223          06 06 53.376437   * 06 08 59.686844     06 10 03.925752       0.00
   0606-223         -22 19 46.28506    *-22 20 20.95666     -22 20 45.98547        0.00
                     From catalog imbedded in main SCHED input file.

 * 0610+260          06 10 43.739224   * 06 13 50.139159     06 15 24.711697       0.00
   0610+260          26 05 30.39476    * 26 04 36.71979      26 04 14.74079        0.00
                     From catalog imbedded in main SCHED input file.

 * 0611+131          06 11 08.402142   * 06 13 57.692746     06 15 23.589924       0.00
   0611+131          13 07 40.23484    * 13 06 45.40069      13 06 19.09526        0.00
                     From catalog imbedded in main SCHED input file.

 * 0627-199          06 27 14.114674   * 06 29 23.761865     06 30 29.754619       0.00
   0627-199         -19 57 16.26236    *-19 59 19.72374     -20 00 28.78865        0.00
                     From catalog imbedded in main SCHED input file.

 * 0632-235          06 32 54.082544   * 06 34 59.001001     06 36 02.645757       0.00
   0632-235         -23 32 44.11701    *-23 35 11.95727     -23 36 33.87606        0.00
                     From catalog imbedded in main SCHED input file.

 * 0640+090          06 40 42.315585   * 06 43 26.445027     06 44 49.865690       0.00
   0640+090          09 00 40.92098    * 08 57 38.01205      08 56 05.71412        0.00
                     From catalog imbedded in main SCHED input file.

 * 0716+714          07 16 13.029719   * 07 21 53.448454     07 24 47.439905       0.00
   0716+714          71 26 15.17408    * 71 20 36.36343      71 17 56.27096        0.00
                     From catalog imbedded in main SCHED input file.

 * 0723-008          07 23 17.838447   * 07 25 50.639950     07 27 08.494092       0.00
   0723-008         -00 48 55.11275    *-00 54 56.54382     -00 58 01.52034        0.00
                     From catalog imbedded in main SCHED input file.

 * 0723-265          07 23 21.920928   * 07 25 24.413149     07 26 27.021373       0.00
   0723-265         -26 34 31.97292    *-26 40 32.67923     -26 43 41.53451        0.00
                     From catalog imbedded in main SCHED input file.

 * 0728-235          07 28 59.946307   * 07 31 06.668015     07 32 11.412829       0.00
   0728-235         -23 35 24.15020    *-23 41 47.87076     -23 45 07.88042        0.00
                     From catalog imbedded in main SCHED input file.

 * 0735+178          07 35 14.126461   * 07 38 07.393749     07 39 35.689258       0.00
   0735+178          17 49 09.26236    * 17 42 18.99815      17 38 53.22476        0.00
                     From catalog imbedded in main SCHED input file.

 * 0736+017          07 36 42.512344   * 07 39 18.033902     07 40 37.310990       0.00
   0736+017          01 44 00.18080    * 01 37 04.61772      01 33 32.74957        0.00
                     From catalog imbedded in main SCHED input file.

 * 0738+491          07 38 19.233764   * 07 42 02.748938     07 43 56.856692       0.00
   0738+491          49 07 19.77517    * 49 00 15.60899      48 56 49.31974        0.00
                     From catalog imbedded in main SCHED input file.

 * 0802-010          08 02 40.259898   * 08 05 12.888480     08 06 30.780669       0.00
   0802-010         -01 02 37.90133    *-01 11 13.79549     -01 15 37.00760        0.00
                     From catalog imbedded in main SCHED input file.

 * 0805+410          08 05 33.646144   * 08 08 56.652046     08 10 40.368449       0.00
   0805+410          41 01 33.06357    * 40 52 44.88897      40 48 23.28781        0.00
                     From catalog imbedded in main SCHED input file.

 * 0805-077          08 05 49.552835   * 08 08 15.536036     08 09 30.074716       0.00
   0805-077         -07 42 22.40693    *-07 51 09.88651     -07 55 39.97908        0.00
                     From catalog imbedded in main SCHED input file.

 * 0814+425          08 14 51.669849   * 08 18 15.999609     08 20 00.459288       0.00
   0814+425          42 32 07.73234    * 42 22 45.41484      42 18 06.38295        0.00
                     From catalog imbedded in main SCHED input file.

 * 0826-373          08 26 12.001567   * 08 28 04.780230     08 29 02.723724       0.00
   0826-373         -37 21 06.12613    *-37 31 06.28132     -37 36 15.18858        0.00
                     From catalog imbedded in main SCHED input file.

 * 0834-201          08 34 24.601691   * 08 36 39.215251     08 37 48.095611       0.00
   0834-201         -20 06 30.40842    *-20 16 59.50411     -20 22 22.06665        0.00
                     From catalog imbedded in main SCHED input file.

 * 0835-339          08 35 01.682133   * 08 37 00.316675     08 38 01.203820       0.00
   0835-339         -33 58 44.07719    *-34 09 14.85948     -34 14 38.92391        0.00
                     From catalog imbedded in main SCHED input file.

 * 0843-547          08 43 40.337343   * 08 45 02.482705     08 45 45.263712       0.00
   0843-547         -54 47 09.78339    *-54 58 08.54021     -55 03 45.85671        0.00
                     From catalog imbedded in main SCHED input file.

 * 0847-120          08 47 46.523272   * 08 50 09.635638     08 51 22.821083       0.00
   0847-120         -12 02 21.67236    *-12 13 35.37613     -12 19 19.73270        0.00
                     From catalog imbedded in main SCHED input file.

 * 0847-354          08 47 47.306092   * 08 49 45.623487     08 50 46.385844       0.00
   0847-354         -35 29 48.13146    *-35 41 01.27843     -35 46 46.40907        0.00
                     From catalog imbedded in main SCHED input file.

   0851+202          08 51 57.250615   * 08 54 48.874927     08 56 16.615501       0.00
 * OJ287             20 17 58.41744    * 20 06 30.64089      20 00 42.90708        0.00
                     From catalog imbedded in main SCHED input file.

 * 0904-201          09 04 34.530811   * 09 06 51.305371     09 08 01.330026       0.00
   0904-201         -20 07 48.70259    *-20 19 54.80516     -20 26 05.99266        0.00
                     From catalog imbedded in main SCHED input file.

 * 0917+624          09 17 40.306879   * 09 21 36.231092     09 23 37.768319       0.00
   0917+624          62 28 38.64007    * 62 15 52.18029      62 09 28.83156        0.00
                     From catalog imbedded in main SCHED input file.

 * 0918-534          09 18 08.791728   * 09 19 44.039517     09 20 33.459659       0.00
   0918-534         -53 27 21.60342    *-53 40 06.44752     -53 46 36.04934        0.00
                     From catalog imbedded in main SCHED input file.

 * 0920+390          09 20 06.318434   * 09 23 14.452934     09 24 50.907135       0.00
   0920+390          39 02 32.11181    * 38 49 39.91008      38 43 10.73733        0.00
                     From catalog imbedded in main SCHED input file.

 * 0938-133          09 38 37.998633   * 09 41 02.549473     09 42 16.534594       0.00
   0938-133         -13 22 10.46801    *-13 35 50.98483     -13 42 49.43432        0.00
                     From catalog imbedded in main SCHED input file.

   0953+254          09 53 59.738494   * 09 56 49.875388     09 58 17.061494       0.00
 * OK290             25 29 33.58600    * 25 15 16.05010      25 08 00.49587        0.00
                     From catalog imbedded in main SCHED input file.

 * 0955+326          09 55 25.405777   * 09 58 20.949634     09 59 50.992669       0.00
   0955+326          32 38 23.03245    * 32 24 02.20949      32 16 45.51632        0.00
                     From catalog imbedded in main SCHED input file.

 * 1004+141          10 04 59.783935   * 10 07 41.498089     10 09 04.305012       0.00
   1004+141          14 11 10.91507    * 13 56 29.60084      13 49 00.85943        0.00
                     From catalog imbedded in main SCHED input file.

 * 1016-311          10 16 12.577890   * 10 18 28.753504     10 19 38.580876       0.00
   1016-311         -31 08 50.46285    *-31 23 53.84966     -31 31 33.18012        0.00
                     From catalog imbedded in main SCHED input file.

 * 1022+237          10 22 07.918330   * 10 24 53.637284     10 26 18.600069       0.00
   1022+237          23 47 48.44913    * 23 32 33.96374      23 24 48.14546        0.00
                     From catalog imbedded in main SCHED input file.

 * 1034-293          10 34 55.824630   * 10 37 16.079742     10 38 27.954774       0.00
   1034-293         -29 18 26.97249    *-29 34 02.81338     -29 41 58.30332        0.00
                     From catalog imbedded in main SCHED input file.

 * 1040+244          10 40 25.199381   * 10 43 09.035781     10 44 33.068387       0.00
   1040+244          24 24 19.59864    * 24 08 35.40950      24 00 33.67714        0.00
                     From catalog imbedded in main SCHED input file.

 * 1048-313          10 48 43.355331   * 10 51 04.777525     10 52 17.248911       0.00
   1048-313         -31 22 18.55751    *-31 38 14.30731     -31 46 19.37138        0.00
                     From catalog imbedded in main SCHED input file.

 * 1101+384          11 01 40.567853   * 11 04 27.313943     11 05 53.126657       0.00
   1101+384          38 28 42.95192    * 38 12 31.79899      38 04 15.50915        0.00
                     From catalog imbedded in main SCHED input file.

 * 1123+264          11 23 14.869299   * 11 25 53.711919     11 27 15.251906       0.00
   1123+264          26 26 49.99110    * 26 10 19.97870      26 01 52.77244        0.00
                     From catalog imbedded in main SCHED input file.

 * 1124-186          11 24 34.018132   * 11 27 04.392457     11 28 21.307972       0.00
   1124-186         -18 40 46.35956    *-18 57 17.44164     -19 05 41.44626        0.00
                     From catalog imbedded in main SCHED input file.

 * 1142+052          11 42 47.144901   * 11 45 21.315161     11 46 40.207946       0.00
   1142+052          05 12 06.34046    * 04 55 26.68782      04 46 55.19877        0.00
                     From catalog imbedded in main SCHED input file.

 * 1143-332          11 43 57.526816   * 11 46 28.451793     11 47 45.672753       0.00
   1143-332         -33 12 02.42944    *-33 28 42.63240     -33 37 08.75224        0.00
                     From catalog imbedded in main SCHED input file.

 * 1143-696          11 43 31.954236   * 11 45 53.624206     11 47 07.408936       0.00
   1143-696         -69 37 21.59645    *-69 54 01.79753     -70 02 21.48968        0.00
                     From catalog imbedded in main SCHED input file.

 * 1144+402          11 44 21.020895   * 11 46 58.297907     11 48 19.368716       0.00
   1144+402          40 15 14.23954    * 39 58 34.30446      39 50 00.47912        0.00
                     From catalog imbedded in main SCHED input file.

 * 1149-084          11 49 43.843437   * 11 52 17.209517     11 53 35.611509       0.00
   1149-084         -08 24 21.93409    *-08 41 03.31383     -08 49 34.06325        0.00
                     From catalog imbedded in main SCHED input file.

 * 1150+812          11 50 23.482380   * 11 53 12.499219     11 54 46.956694       0.00
   1150+812          81 15 10.31171    * 80 58 29.15454      80 49 56.30015        0.00
                     From catalog imbedded in main SCHED input file.

 * 1156-094          11 56 39.052547   * 11 59 12.711653     12 00 31.246526       0.00
   1156-094         -09 24 09.93238    *-09 40 52.04858     -09 49 23.09069        0.00
                     From catalog imbedded in main SCHED input file.

 * 1156-215          11 56 37.268703   * 11 59 10.785361     12 00 29.240861       0.00
   1156-215         -21 33 22.48860    *-21 50 04.67334     -21 58 33.69120        0.00
                     From catalog imbedded in main SCHED input file.

 * 1157-215          11 57 18.309698   * 11 59 51.905998     12 01 10.400362       0.00
   1157-215         -21 32 11.49814    *-21 48 53.70579     -21 57 22.73501        0.00
                     From catalog imbedded in main SCHED input file.

 * 1213-172          12 13 11.668022   * 12 15 46.751776     12 17 05.960761       0.00
   1213-172         -17 15 05.20066    *-17 31 45.40303     -17 40 14.18059        0.00
                     From catalog imbedded in main SCHED input file.

 * 1218-024          12 18 49.916799   * 12 21 23.941193     12 22 42.643376       0.00
   1218-024         -02 25 11.35058    *-02 41 49.60958     -02 50 20.20455        0.00
                     From catalog imbedded in main SCHED input file.

 * 1231+811          12 31 38.947377   * 12 33 12.893056     12 34 10.509963       0.00
   1231+811          81 11 05.74719    * 80 54 33.97236      80 46 01.80878        0.00
                     From catalog imbedded in main SCHED input file.

 * 1244-255          12 44 06.713930   * 12 46 46.802044     12 48 08.468778       0.00
   1244-255         -25 31 26.67465    *-25 47 49.28899     -25 56 07.28193        0.00
                     From catalog imbedded in main SCHED input file.

 * 1252+119          12 52 07.716977   * 12 54 38.255619     12 55 55.224554       0.00
   1252+119          11 57 20.86466    * 11 41 05.89510      11 32 43.53378        0.00
                     From catalog imbedded in main SCHED input file.

 * 1306-395          13 06 58.426945   * 13 09 48.488329     13 11 15.206160       0.00
   1306-395         -39 32 35.04982    *-39 48 33.08585     -39 56 34.79736        0.00
                     From catalog imbedded in main SCHED input file.

   1315+346          13 15 17.789366   * 13 17 36.494176     13 18 47.793801       0.00
 * OP326             34 41 02.60445    * 34 25 15.93257      34 17 03.22617        0.00
                     From catalog imbedded in main SCHED input file.

 * 1315-058          13 15 57.621584   * 13 18 33.709431     13 19 53.271993       0.00
   1315-058         -05 51 38.09009    *-06 07 23.82022     -06 15 28.20058        0.00
                     From catalog imbedded in main SCHED input file.

 * 1324+224          13 24 37.118630   * 13 27 00.861314     13 28 14.423171       0.00
   1324+224          22 26 22.70233    * 22 10 50.16277      22 02 45.93780        0.00
                     From catalog imbedded in main SCHED input file.

 * 1329-049          13 29 28.424712   * 13 32 04.464684     13 33 23.958494       0.00
   1329-049         -04 54 18.75778    *-05 09 43.30595     -05 17 37.46947        0.00
                     From catalog imbedded in main SCHED input file.

 * 1330+022          13 30 20.472740   * 13 32 53.270536     13 34 11.165204       0.00
   1330+022          02 16 08.78136    * 02 00 45.69919      01 52 50.41122        0.00
                     From catalog imbedded in main SCHED input file.

 * 1334-127          13 34 59.803875   * 13 37 39.782780     13 39 01.217566       0.00
   1334-127         -12 42 09.74298    *-12 57 24.69325     -13 05 11.94652        0.00
                     From catalog imbedded in main SCHED input file.

 * 1339-206          13 39 20.210661   * 13 42 04.739557     13 43 28.446499       0.00
   1339-206         -20 36 22.52425    *-20 51 29.54126     -20 59 10.52068        0.00
                     From catalog imbedded in main SCHED input file.

 * 1339-287          13 39 25.874232   * 13 42 15.345637     13 43 41.562495       0.00
   1339-287         -28 45 35.02197    *-29 00 41.83125     -29 08 20.27855        0.00
                     From catalog imbedded in main SCHED input file.

 * 1342+663          13 42 41.043751   * 13 44 08.679590     13 44 56.101638       0.00
   1342+663          66 21 13.16145    * 66 06 11.64383      65 58 17.62547        0.00
                     From catalog imbedded in main SCHED input file.

 * 1346-109          13 46 23.516487   * 13 49 03.193047     13 50 24.434430       0.00
   1346-109         -10 55 07.32904    *-11 10 00.81902     -11 17 37.87078        0.00
                     From catalog imbedded in main SCHED input file.

 * 1349-439          13 49 52.526242   * 13 52 56.534970     13 54 30.162289       0.00
   1349-439         -43 57 54.14032    *-44 12 40.38796     -44 20 03.74500        0.00
                     From catalog imbedded in main SCHED input file.

 * 1354-152          13 54 28.601593   * 13 57 11.244984     13 58 33.941040       0.00
   1354-152         -15 12 51.88896    *-15 27 28.78664     -15 34 56.25195        0.00
                     From catalog imbedded in main SCHED input file.

 * 1357+769          13 57 42.116997   * 13 57 55.371528     13 58 08.589478       0.00
   1357+769          76 57 53.35428    * 76 43 21.05108      76 35 40.18499        0.00
                     From catalog imbedded in main SCHED input file.

 * 1406-076          14 06 17.898824   * 14 08 56.481202     14 10 17.096519       0.00
   1406-076         -07 38 15.91679    *-07 52 26.66651     -07 59 43.38928        0.00
                     From catalog imbedded in main SCHED input file.

 * 1424+240          14 24 44.222622   * 14 27 00.391774     14 28 09.871261       0.00
   1424+240          24 01 25.78956    * 23 48 00.03768      23 40 56.80418        0.00
                     From catalog imbedded in main SCHED input file.

 * 1424-418          14 24 46.670323   * 14 27 56.297572     14 29 32.551425       0.00
   1424-418         -41 52 54.61345    *-42 06 19.43760     -42 13 01.78793        0.00
                     From catalog imbedded in main SCHED input file.

 * 1441+522          14 41 24.844167   * 14 43 02.760702     14 43 53.568217       0.00
   1441+522          52 14 18.42027    * 52 01 37.29861      51 54 50.84383        0.00
                     From catalog imbedded in main SCHED input file.

 * 1451-400          14 51 20.583540   * 14 54 32.912361     14 56 10.359179       0.00
   1451-400         -40 00 22.26293    *-40 12 32.51478     -40 18 37.60235        0.00
                     From catalog imbedded in main SCHED input file.

 * 1456-179          14 56 39.692814   * 14 59 28.763197     15 00 54.402874       0.00
   1456-179         -17 58 50.56977    *-18 10 45.18622     -18 16 50.27787        0.00
                     From catalog imbedded in main SCHED input file.

 * 1504+377          15 04 12.956687   * 15 06 09.529975     15 07 09.103649       0.00
   1504+377          37 42 23.33441    * 37 30 51.13251      37 24 40.60735        0.00
                     From catalog imbedded in main SCHED input file.

 * 1504-166          15 04 16.415562   * 15 07 04.786961     15 08 30.035873       0.00
   1504-166         -16 40 59.36698    *-16 52 30.26710     -16 58 23.92086        0.00
                     From catalog imbedded in main SCHED input file.

 * 1505+428          15 05 04.054997   * 15 06 53.041840     15 07 48.899025       0.00
   1505+428          42 50 52.72440    * 42 39 23.03562      42 33 12.78541        0.00
                     From catalog imbedded in main SCHED input file.

 * 1511-100          15 11 02.250582   * 15 13 44.893422     15 15 07.232010       0.00
   1511-100         -10 00 50.96545    *-10 12 00.26470     -10 17 45.50157        0.00
                     From catalog imbedded in main SCHED input file.

 * 1514+004          15 14 06.740345   * 15 16 40.219059     15 17 57.958561       0.00
   1514+004          00 26 01.34266    * 00 15 01.90911      00 09 17.93377        0.00
                     From catalog imbedded in main SCHED input file.

 * 1514+197          15 14 40.985840   * 15 16 56.796163     15 18 05.752356       0.00
   1514+197          19 43 10.94246    * 19 32 12.99203      19 26 23.70601        0.00
                     From catalog imbedded in main SCHED input file.

 * 1538+477          15 38 00.886009   * 15 39 34.810369     15 40 22.899796       0.00
   1538+477          47 45 10.16107    * 47 35 31.26416      47 30 14.73211        0.00
                     From catalog imbedded in main SCHED input file.

 * 1546+027          15 46 58.292169   * 15 49 29.436843     15 50 45.823792       0.00
   1546+027          02 46 06.07607    * 02 37 01.16342      02 32 13.58329        0.00
                     From catalog imbedded in main SCHED input file.

 * 1555+001          15 55 17.692624   * 15 57 51.433976     15 59 09.071083       0.00
   1555+001          00 06 43.53285    *-00 01 50.41375     -00 06 21.55984        0.00
                     From catalog imbedded in main SCHED input file.

 * 1556+335          15 56 59.438416   * 15 58 55.186274     15 59 53.869198       0.00
   1556+335          33 31 47.24644    * 33 23 18.60651      33 18 39.88116        0.00
                     From catalog imbedded in main SCHED input file.

 * 1604-333          16 04 22.187024   * 16 07 34.762327     16 09 11.855897       0.00
   1604-333         -33 23 10.54151    *-33 31 08.91306     -33 35 09.38697        0.00
                     From catalog imbedded in main SCHED input file.

 * 1606+106          16 06 23.396625   * 16 08 46.203189     16 09 58.303287       0.00
   1606+106          10 36 59.80115    * 10 29 07.77585      10 24 53.96133        0.00
                     From catalog imbedded in main SCHED input file.

 * 1606-742          16 06 29.032744   * 16 12 33.884991     16 15 38.620710       0.00
   1606-742         -74 15 55.35174    *-74 23 40.14294     -74 27 17.31098        0.00
                     From catalog imbedded in main SCHED input file.

 * 1614+051          16 14 09.076773   * 16 16 37.556825     16 17 52.447275       0.00
   1614+051          05 06 54.39661    * 04 59 32.73644      04 55 36.00442        0.00
                     From catalog imbedded in main SCHED input file.

 * 1619-680          16 19 13.497235   * 16 24 18.437068     16 26 52.271882       0.00
   1619-680         -68 02 15.80516    *-68 09 12.49572     -68 12 28.38681        0.00
                     From catalog imbedded in main SCHED input file.

 * 1622-297          16 22 57.242927   * 16 26 06.020833     16 27 41.085914       0.00
   1622-297         -29 44 41.40043    *-29 51 26.97116     -29 54 52.30461        0.00
                     From catalog imbedded in main SCHED input file.

 * 1636+473          16 36 19.144414   * 16 37 45.130557     16 38 28.591069       0.00
   1636+473          47 23 28.57998    * 47 17 33.83118      47 14 09.00144        0.00
                     From catalog imbedded in main SCHED input file.

   1638+398          16 38 48.169691   * 16 40 29.632775     16 41 20.807186       0.00
 * NRAO512           39 52 30.08662    * 39 46 46.02843      39 43 28.10911        0.00
                     From catalog imbedded in main SCHED input file.

 * 1647-296          16 47 29.477786   * 16 50 39.544108     16 52 15.103907       0.00
   1647-296         -29 38 41.69505    *-29 43 46.95445     -29 46 22.00320        0.00
                     From catalog imbedded in main SCHED input file.

 * 1650-157          16 50 42.316783   * 16 53 34.206425     16 55 00.623285       0.00
   1650-157         -15 46 37.45182    *-15 51 29.88808     -15 54 03.96915        0.00
                     From catalog imbedded in main SCHED input file.

 * 1656-075          16 56 01.672877   * 16 58 44.061964     17 00 05.678758       0.00
   1656-075         -07 34 47.28709    *-07 39 17.69435     -07 41 43.87530        0.00
                     From catalog imbedded in main SCHED input file.

 * 1657-261          16 57 47.714239   * 17 00 53.154062     17 02 26.328857       0.00
   1657-261         -26 06 29.52819    *-26 10 51.72538     -26 13 06.58501        0.00
                     From catalog imbedded in main SCHED input file.

 * 1704-141          17 04 30.138394   * 17 07 20.390555     17 08 45.905096       0.00
   1704-141         -14 11 28.84018    *-14 15 23.12673     -14 17 28.65338        0.00
                     From catalog imbedded in main SCHED input file.

 * 1708-250          17 08 18.736723   * 17 11 23.102274     17 12 55.674884       0.00
   1708-250         -25 05 23.98224    *-25 09 01.56281     -25 10 54.46340        0.00
                     From catalog imbedded in main SCHED input file.

 * 1717+178          17 17 00.324740   * 17 19 13.048489     17 20 19.620805       0.00
   1717+178          17 48 08.51611    * 17 45 06.43734      17 43 15.88152        0.00
                     From catalog imbedded in main SCHED input file.

 * 1726-269          17 26 00.807051   * 17 29 08.216370     17 30 42.208509       0.00
   1726-269         -26 55 29.40849    *-26 57 50.74421     -26 59 04.73968        0.00
                     From catalog imbedded in main SCHED input file.

 * 1739-152          17 39 19.687711   * 17 42 11.662847     17 43 37.841842       0.00
   1739-152         -15 16 05.13548    *-15 17 29.15830     -15 18 18.89726        0.00
                     From catalog imbedded in main SCHED input file.

 * 1746+470          17 46 04.346063   * 17 47 26.647281     17 48 07.466220       0.00
   1746+470          46 59 48.71224    * 46 58 50.92627      46 57 56.10443        0.00
                     From catalog imbedded in main SCHED input file.

 * 1749+096          17 49 10.387933   * 17 51 32.818576     17 52 44.077880       0.00
   1749+096          09 39 42.82591    * 09 39 00.72846      09 38 23.32830        0.00
                     From catalog imbedded in main SCHED input file.

 * 1751+288          17 51 45.401876   * 17 53 42.473649     17 54 40.887882       0.00
   1751+288          28 48 36.64969    * 28 48 04.93897      28 47 27.31655        0.00
                     From catalog imbedded in main SCHED input file.

 * 1829-106          18 29 34.652811   * 18 32 20.836430     18 33 43.837015       0.00
   1829-106         -10 37 26.19909    *-10 35 11.19938     -10 34 12.66566        0.00
                     From catalog imbedded in main SCHED input file.

 * 1849+670          18 49 16.505884   * 18 49 16.072296     18 49 13.393770       0.00
   1849+670          67 02 07.88053    * 67 05 41.68027      67 07 02.68479        0.00
                     From catalog imbedded in main SCHED input file.

 * 1851+488          18 51 09.379856   * 18 52 28.547813     18 53 07.042733       0.00
   1851+488          48 52 02.82129    * 48 55 47.48131      48 57 16.83572        0.00
                     From catalog imbedded in main SCHED input file.

 * 1903+196          19 03 25.637178   * 19 05 36.472106     19 06 41.405621       0.00
   1903+196          19 38 29.62721    * 19 43 08.04504      19 45 10.42725        0.00
                     From catalog imbedded in main SCHED input file.

 * 1908-201          19 08 12.464439   * 19 11 09.652887     19 12 37.983234       0.00
   1908-201         -20 11 55.17839    *-20 06 55.10898     -20 04 30.67539        0.00
                     From catalog imbedded in main SCHED input file.

 * 1921-293          19 21 42.234129   * 19 24 51.055956     19 26 25.123567       0.00
   1921-293         -29 20 26.35392    *-29 14 30.12101     -29 11 34.81637        0.00
                     From catalog imbedded in main SCHED input file.

 * 1922-224          19 22 40.330225   * 19 25 39.790187     19 27 09.190549       0.00
   1922-224         -22 25 34.97747    *-22 19 35.11276     -22 16 40.09946        0.00
                     From catalog imbedded in main SCHED input file.

 * 1928+154          19 28 36.092062   * 19 30 52.766986     19 32 00.545468       0.00
   1928+154          15 26 11.96593    * 15 32 34.42733      15 35 30.83943        0.00
                     From catalog imbedded in main SCHED input file.

 * 1929+226          19 29 16.894891   * 19 31 24.916785     19 32 28.261806       0.00
   1929+226          22 37 06.35050    * 22 43 31.25853      22 46 27.45549        0.00
                     From catalog imbedded in main SCHED input file.

 * 1935+360          19 35 42.047358   * 19 37 31.436618     19 38 25.135797       0.00
   1935+360          36 00 45.81335    * 36 07 35.84171      36 10 42.71661        0.00
                     From catalog imbedded in main SCHED input file.

 * 1936+046          19 36 01.936452   * 19 38 30.669552     19 39 44.555346       0.00
   1936+046          04 41 18.91434    * 04 48 11.61444      04 51 25.85359        0.00
                     From catalog imbedded in main SCHED input file.

 * 1953-325          19 53 48.389539   * 19 56 59.455276     19 58 34.490268       0.00
   1953-325         -32 33 49.62828    *-32 25 46.00691     -32 21 46.45668        0.00
                     From catalog imbedded in main SCHED input file.

 * 1959+241          19 59 45.946262   * 20 01 53.777904     20 02 56.856456       0.00
   1959+241          24 08 15.79837    * 24 16 39.98976      24 20 37.21566        0.00
                     From catalog imbedded in main SCHED input file.

 * 1959+332          19 59 46.390075   * 20 01 42.209088     20 02 39.068421       0.00
   1959+332          33 15 20.94229    * 33 23 44.76614      33 27 40.54209        0.00
                     From catalog imbedded in main SCHED input file.

 * 2000+472          20 00 39.216077   * 20 02 10.418262     20 02 54.420114       0.00
   2000+472          47 17 02.42447    * 47 25 28.77368      47 29 24.39020        0.00
                     From catalog imbedded in main SCHED input file.

 * 2005-044          20 05 46.290693   * 20 08 24.429202     20 09 42.969597       0.00
   2005-044         -04 27 17.00396    *-04 18 29.29813     -04 14 14.70294        0.00
                     From catalog imbedded in main SCHED input file.

 * 2018+295          20 18 03.980870   * 20 20 06.563624     20 21 06.821330       0.00
   2018+295          29 32 42.69989    * 29 42 14.18637      29 46 45.48461        0.00
                     From catalog imbedded in main SCHED input file.

 * 2039+452          20 39 06.383173   * 20 40 48.333115     20 41 37.605713       0.00
   2039+452          45 16 33.22992    * 45 27 17.14590      45 32 25.06723        0.00
                     From catalog imbedded in main SCHED input file.

 * 2047-266          20 47 26.172413   * 20 50 24.693835     20 51 53.325608       0.00
   2047-266         -26 39 31.71536    *-26 28 18.05750     -26 22 45.60352        0.00
                     From catalog imbedded in main SCHED input file.

 * 2051-204          20 51 30.216827   * 20 54 22.072452     20 55 47.381376       0.00
   2051-204         -20 27 43.34805    *-20 16 16.81934     -20 10 39.14103        0.00
                     From catalog imbedded in main SCHED input file.

 * 2052-474          20 52 50.091130   * 20 56 16.359822     20 57 58.565453       0.00
   2052-474         -47 26 19.35812    *-47 14 47.62756     -47 09 01.95033        0.00
                     From catalog imbedded in main SCHED input file.

 * 2059+034          20 59 08.011532   * 21 01 38.834151     21 02 53.516963       0.00
   2059+034          03 29 41.48364    * 03 41 31.32089      03 47 17.06036        0.00
                     From catalog imbedded in main SCHED input file.

 * 2116+818          21 16 39.216630   * 21 14 01.171095     21 12 24.280019       0.00
   2116+818          81 52 14.08119    * 82 04 48.34034      82 10 52.04392        0.00
                     From catalog imbedded in main SCHED input file.

 * 2135+508          21 35 15.499526   * 21 37 00.986166     21 37 51.512190       0.00
   2135+508          50 48 05.19433    * 51 01 36.12903      51 08 12.97992        0.00
                     From catalog imbedded in main SCHED input file.

 * 2142+110          21 42 52.346936   * 21 45 18.775064     21 46 31.116695       0.00
   2142+110          11 01 36.29880    * 11 15 27.31229      11 22 14.79970        0.00
                     From catalog imbedded in main SCHED input file.

 * 2143-156          21 43 38.873701   * 21 46 22.979329     21 47 44.340209       0.00
   2143-156         -15 39 37.25748    *-15 25 43.88569     -15 18 53.40953        0.00
                     From catalog imbedded in main SCHED input file.

 * 2150+173          21 50 02.232822   * 21 52 24.819389     21 53 35.140245       0.00
   2150+173          17 20 29.78521    * 17 34 37.79499      17 41 33.98895        0.00
                     From catalog imbedded in main SCHED input file.

 * 2159+505          21 59 50.311748   * 22 01 43.537256     22 02 37.940125       0.00
   2159+505          50 34 26.99217    * 50 48 56.38903      50 56 04.99907        0.00
                     From catalog imbedded in main SCHED input file.

 * 2204-007          22 04 09.145192   * 22 06 43.282605     22 07 59.590005       0.00
   2204-007         -00 45 42.03980    *-00 31 02.49515     -00 23 49.52376        0.00
                     From catalog imbedded in main SCHED input file.

 * 2215+150          22 15 45.032352   * 22 18 10.913899     22 19 22.917746       0.00
   2215+150          15 05 33.20689    * 15 20 35.71741      15 28 00.55797        0.00
                     From catalog imbedded in main SCHED input file.

 * 2229+591          22 29 26.076350   * 22 31 17.075500     22 32 09.600165       0.00
   2229+591          59 06 34.62563    * 59 22 00.84719      59 29 41.74116        0.00
                     From catalog imbedded in main SCHED input file.

   2230+114          22 30 07.803937   * 22 32 36.408895     22 33 49.834604       0.00
 * CTA102            11 28 22.81075    * 11 43 50.90403      11 51 29.14577        0.00
                     From catalog imbedded in main SCHED input file.

 * 2234+282          22 34 01.728781   * 22 36 22.470825     22 37 31.654329       0.00
   2234+282          28 13 23.21015    * 28 28 57.41288      28 36 39.88042        0.00
                     From catalog imbedded in main SCHED input file.

 * 2245-328          22 45 51.504504   * 22 48 38.685746     22 50 01.533859       0.00
   2245-328         -32 51 44.44017    *-32 35 52.18825     -32 28 01.62678        0.00
                     From catalog imbedded in main SCHED input file.

 * 2251-419          22 51 45.752580   * 22 54 36.697480     22 56 01.320424       0.00
   2251-419         -41 55 40.32383    *-41 39 40.25402     -41 31 45.47909        0.00
                     From catalog imbedded in main SCHED input file.

 * 2254+074          22 54 45.978807   * 22 57 17.303116     22 58 32.164097       0.00
   2254+074          07 27 08.97034    * 07 43 12.30253      07 51 09.01481        0.00
                     From catalog imbedded in main SCHED input file.

 * 2315-172          23 15 33.735728   * 23 18 11.361393     23 19 29.537763       0.00
   2315-172         -17 15 53.75241    *-16 59 29.18882     -16 51 22.81358        0.00
                     From catalog imbedded in main SCHED input file.

 * 2319+317          23 19 28.286856   * 23 21 54.955984     23 23 07.108171       0.00
   2319+317          31 47 40.33722    * 32 04 07.62251      32 12 20.27854        0.00
                     From catalog imbedded in main SCHED input file.

 * 2344+798          23 44 16.001516   * 23 46 25.609020     23 47 21.171660       0.00
   2344+798          79 51 15.47520    * 80 07 55.23948      80 16 24.07922        0.00
                     From catalog imbedded in main SCHED input file.

 * 2351+456          23 51 49.972521   * 23 54 21.680232     23 55 36.011872       0.00
   2351+456          45 36 22.77759    * 45 53 04.23653      46 01 28.76683        0.00
                     From catalog imbedded in main SCHED input file.

 * 2353-686          23 53 22.983609   * 23 56 00.681443     23 57 17.785995       0.00
   2353-686         -68 36 45.65546    *-68 20 03.47241     -68 11 48.64126        0.00
                     From catalog imbedded in main SCHED input file.

 * 2355-106          23 55 36.945014   * 23 58 10.882397     23 59 27.293493       0.00
   2355-106         -10 36 50.74022    *-10 20 08.61143     -10 11 52.70312        0.00
                     From catalog imbedded in main SCHED input file.

 * 0537-441          05 37 21.071425   * 05 38 50.361559     05 39 35.987116       0.01
   J0538-4405       -44 06 44.66633    *-44 05 08.93901     -44 04 31.84469        0.01
   J0538-44          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  72326 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  0002+541   sess125.K2048globgeo  3 13 14 16 17 18 19 20 21 2 +     1.106     0.791
  0003+380   sess125.K2048globgeo  1 2 3 13 14 16 17 18 19 20  +     1.142     0.317
  0008-264   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.823     0.363
  0012+610   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.684     1.603
  0013-184   sess125.K2048globgeo  1 2 3 13 15 16 17 18 19 20  +     1.232     1.006
  0016+731   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.592     1.499
  0017+200   sess125.K2048globgeo  2 3 13 14 15 16 17 18 19 20 +     1.339     0.795
  NGC0262    sess125.K2048globgeo  2 3 13 14 15 16 17 18 19 20 +     1.641     1.269
  0048-097   sess125.K2048globgeo  2 3 13 14 15 16 17 18 19 20 +     0.709     0.378
  0056-001   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.995     1.975
  0057+678   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.571     1.426
  0104-408   sess125.K2048globgeo  1 2 3                             0.139     0.833
  0113-118   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.303     0.669
  0115-214   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.853     1.765
  0119+041   sess125.K2048globgeo  1 2 3 13 14 16 17 18 19 20  +     1.027     0.682
  0133+476   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.677     1.009
  0139-097   sess125.K2048globgeo  1 3 13 14 15 16 17 18 19 20 +     1.220     0.630
  0203+625   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.319     1.069
  0208-512   sess125.K2048globgeo  1 2 3 22                          0.372     0.439
  0215+015   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.195     0.637
  0218+357   sess125.K2048globgeo  2 3 13 14 15 16 17 18 19 20 +     1.219     1.430
  0220-349   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     0.669     0.612
  0222-262   sess125.K2048globgeo  1 2 3 15 16 17 19 20 21 22  +     1.062     0.443
  4C67.05    sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.803     1.778
  0234+285   sess125.K2048globgeo  2 3 13 14 15 16 17 18 19 20 +     0.841     0.299
  0235+164   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.795     0.631
  0240-060   sess125.K2048globgeo  2 3 13 14 15 16 17 18 19 20 +     1.430     0.754
  0244-470   sess125.K2048globgeo  1 2 3 22                          0.683     0.459
  0245-167   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.304     1.020
  0248-266   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.788     0.428
  0249+171   sess125.K2048globgeo  1 2 3 14 15 17 19 20 21 25        1.678     0.573
  0256-005   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.143     0.691
  0300+470   sess125.K2048globgeo  3 13 15 16 17 19 20 21 25 2 +     1.129     0.853
  0306+102   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.589     0.639
  0309+411   sess125.K2048globgeo  2 3 13 15 16 17 18 19 20 21 +     1.251     0.780
  0312+100   sess125.K2048globgeo  1 2 3 13 14 15 16 17 19 20  +     1.379     1.445
  0327-241   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.248     0.834
  0345+460   sess125.K2048globgeo  3 13 14 16 17 18 19 20 21 2 +     1.091     0.361
  0346-279   sess125.K2048globgeo  1 2 3 13 14 15 16 18 19 20  +     0.647     0.396
  0354+559   sess125.K2048globgeo  3 13 15 16 17 19 20 21 25 2 +     1.007     1.056
  0406-127   sess125.K2048globgeo  1 3 13 14 16 17 18 19 20 21 +     0.891     0.519
  0420-014   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.641     1.185
  0422+004   sess125.K2048globgeo  1 2 3 13 15 16 17 19 20 21  +     1.039     0.821
  0426-380   sess125.K2048globgeo  1 2 3 15 16 20 21 22 25 26        0.721     0.344
  0430+289   sess125.K2048globgeo  2 3 13 15 16 17 19 20 21 22 +     1.115     6.682
  0451-282   sess125.K2048globgeo  1 2 3 15 19 20 21 22 25           0.939     0.968
  0454-810   sess125.K2048globgeo  1 2 22                            0.455     0.250
  0458-020   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.474    10.699
  0459+415   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     2.264     1.445
  0507+179   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.318     0.949
  0511-220   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.103     0.702
  0524-485   sess125.K2048globgeo  1 2 3 15 20 22                    0.419     0.132
  0527-053   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.148     0.773
  0529+483   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.275     0.743
  0537-286   sess125.K2048globgeo  1 2 3 15 16 18 19 20 21 22  +     1.070     0.755
  0548+084   sess125.K2048globgeo  3 13 14 16 17 18 19 20 21 2 +     0.986     0.787
  0558+234   sess125.K2048globgeo  3 13 15 16 17 18 19 20 21 2 +     0.867     1.013
  0603+882   sess125.K2048globgeo  3 13 16 17 18 19 20 21 25 2 +     1.201     0.614
  0606-223   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.148     0.528
  0610+260   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.990     0.644
  0611+131   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.610     0.603
  0627-199   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.236     0.799
  0632-235   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.405     0.747
  0640+090   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.404     1.593
  0716+714   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.706     1.095
  0723-008   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.524     0.756
  0723-265   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.892     0.911
  0728-235   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.131     0.893
  0735+178   sess125.K2048globgeo  1 2 3 13 15 16 17 19 20 21  +     0.859     4.040
  0736+017   sess125.K2048globgeo  1 2 3 13 14 15 16 17 19 20  +     0.798     0.285
  0738+491   sess125.K2048globgeo  3 13 15 16 17 19 20 21 25 2 +     1.283     0.444
  0802-010   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.968     0.434
  0805+410   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.315     1.093
  0805-077   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.305     0.703
  0814+425   sess125.K2048globgeo  1 2 3 13 14 15 16 17 19 20  +     1.577     0.916
  0826-373   sess125.K2048globgeo  1 2 3 15 19 20 21 22              0.377     0.945
  0834-201   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.211     1.031
  0835-339   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     0.641     0.418
  0843-547   sess125.K2048globgeo  1 2 3 22                          0.499     0.478
  0847-120   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.626     0.559
  0847-354   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     0.568     0.463
  OJ287      sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.368    19.062
  0904-201   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.071     0.727
  0917+624   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.824     0.957
  0918-534   sess125.K2048globgeo  1 2 3 22                          0.378     0.211
  0920+390   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.709     4.481
  0938-133   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.237     0.711
  OK290      sess125.K2048globgeo  1 2 3 13 14 15 16 17 19 20  +     1.114     0.821
  0955+326   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     0.686     0.872
  1004+141   sess125.K2048globgeo  3 13 15 16 17 19 20 21 22 2 +     0.881     0.438
  1016-311   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     0.703     0.834
  1022+237   sess125.K2048globgeo  1 2 3 13 15 16 17 19 20 21  +     0.736     0.334
  1034-293   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25        0.833     0.859
  1040+244   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.716     0.985
  1048-313   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     1.118     1.197
  1101+384   sess125.K2048globgeo  1 2 3 13 14 16 17 18 21 22  +     1.174     0.897
  1123+264   sess125.K2048globgeo  3 15 16 17 18 19 20 21 22 2 +     0.882     0.549
  1124-186   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.554     0.305
  1142+052   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.972     0.658
  1143-332   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 26        0.344     0.546
  1143-696   sess125.K2048globgeo  1 2 22                            0.303     0.167
  1144+402   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     2.010     1.710
  1149-084   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.714     0.587
  1150+812   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.204     1.265
  1156-094   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.983     1.031
  1156-215   sess125.K2048globgeo  3 13 16 17 18 19 20 21 22 2 +     0.661     0.471
  1157-215   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.512     0.523
  1213-172   sess125.K2048globgeo  1 2 3 13 14 16 17 18 19 20  +     0.967     0.833
  1218-024   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.970     1.326
  1231+811   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.994     0.952
  1244-255   sess125.K2048globgeo  1 2 3 13 15 16 19 20 21 22  +     0.528     0.505
  1252+119   sess125.K2048globgeo  1 2 3 14 15 16 17 19 20 21  +     0.703     0.669
  1306-395   sess125.K2048globgeo  1 2 3 15 19 20 21 22              0.327     0.573
  OP326      sess125.K2048globgeo  3 14 15 16 17 19 20 21 25 2 +     1.373     1.413
  1315-058   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.272     1.334
  1324+224   sess125.K2048globgeo  1 2 3 14 15 16 17 18 19 20  +     1.519     0.738
  1329-049   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.207     1.163
  1330+022   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.823     2.716
  1334-127   sess125.K2048globgeo  1 2 3 13 14 15 16 17 19 20  +     0.322     0.211
  1339-206   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.573     0.819
  1339-287   sess125.K2048globgeo  1 2 3 13 14 15 16 18 19 20  +     0.944     0.581
  1342+663   sess125.K2048globgeo  3 13 15 16 17 18 19 20 21 2 +     1.106     0.823
  1346-109   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 20  +     0.923     0.371
  1349-439   sess125.K2048globgeo  1 2 3 22 25                       0.151     0.068
  1354-152   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.205     0.867
  1357+769   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.548     1.771
  1406-076   sess125.K2048globgeo  1 3 13 14 16 17 18 19 20 21 +     1.096     1.121
  1424+240   sess125.K2048globgeo  3 13 14 16 17 18 19 20 21 2 +     1.150     0.769
  1424-418   sess125.K2048globgeo  1 2 3 15 20 22                    0.248     0.214
  1441+522   sess125.K2048globgeo  3 13 16 17 18 19 20 21 25 2 +     0.938     0.547
  1451-400   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     0.481     0.388
  1456-179   sess125.K2048globgeo  1 3 13 14 16 17 18 19 20 21 +     0.760     0.615
  1504+377   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.586     0.590
  1504-166   sess125.K2048globgeo  1 2 3 13 14 16 17 18 19 20  +     1.199     0.378
  1505+428   sess125.K2048globgeo  1 2 3 13 14 15 17 18 19 20  +     1.494     0.614
  1511-100   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.245     0.744
  1514+004   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.055     0.623
  1514+197   sess125.K2048globgeo  1 2 3 14 16 17 19 20 21 25  +     1.037     0.553
  1538+477   sess125.K2048globgeo  3 14 15 16 17 19 20 21 25 2 +     1.063     1.112
  1546+027   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.507    15.282
  1555+001   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.049     0.759
  1556+335   sess125.K2048globgeo  1 3 15 16 17 19 20 21 26          0.530     0.416
  1604-333   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     0.696     0.384
  1606+106   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.287     0.692
  1606-742   sess125.K2048globgeo  1 2 22                            0.329     0.261
  1614+051   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.689     0.515
  1619-680   sess125.K2048globgeo  1 2 22                            0.083     0.250
  1622-297   sess125.K2048globgeo  1 2 3 15 16 20 21 22 25 26        1.207     0.826
  1636+473   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     0.859     0.732
  NRAO512    sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.708     1.364
  1647-296   sess125.K2048globgeo  1 2 3 14 16 19 20 21 22 25  +     0.734     0.991
  1650-157   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.281     0.874
  1656-075   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.316     0.578
  1657-261   sess125.K2048globgeo  1 2 3 15 19 20 21 22              0.377     0.632
  1704-141   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.597     1.608
  1708-250   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.114     0.661
  1717+178   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.803     0.748
  1726-269   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.854     0.452
  1739-152   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.369     0.728
  1746+470   sess125.K2048globgeo  1 3 13 14 15 16 17 18 19 20 +     1.129     1.281
  1749+096   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     2.172     2.509
  1751+288   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.305     0.809
  1829-106   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.712     0.536
  1849+670   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     2.302     4.153
  1851+488   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.639     1.087
  1903+196   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.213     0.857
  1908-201   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.696     1.187
  1921-293   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     0.423     5.273
  1922-224   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22           0.797     0.425
  1928+154   sess125.K2048globgeo  3 13 15 16 17 19 20 21 22 2 +     0.520     0.354
  1929+226   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.734     0.666
  1935+360   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.883     0.617
  1936+046   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.325     0.692
  1953-325   sess125.K2048globgeo  1 2 3 15 16 19 20 21 22 25  +     1.057     0.337
  1959+241   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.211     0.467
  1959+332   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     0.937     0.978
  2000+472   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.477     1.744
  2005-044   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.053     0.710
  2018+295   sess125.K2048globgeo  1 2 3 13 15 16 17 19 20 21  +     1.110     0.457
  2039+452   sess125.K2048globgeo  3 13 15 16 17 19 20 21 25 2 +     1.001     0.645
  2047-266   sess125.K2048globgeo  1 2 3 15 19 20 21 22 25           0.524     0.491
  2051-204   sess125.K2048globgeo  1 2 3 14 15 16 18 19 20 21  +     0.967     0.900
  2052-474   sess125.K2048globgeo  1 2 15 20 22                      0.311     0.083
  2059+034   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.208     0.464
  2116+818   sess125.K2048globgeo  3 13 14 15 16 17 19 20 21 2 +     0.986     2.194
  2135+508   sess125.K2048globgeo  3 13 14 15 16 17 18 19 20 2 +     1.058     0.723
  2142+110   sess125.K2048globgeo  1 2 3 13 14 16 17 18 19 20  +     0.902     0.420
  2143-156   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     0.688     0.319
  2150+173   sess125.K2048globgeo  1 2 3 13 15 16 17 19 20 21  +     0.920     0.809
  2159+505   sess125.K2048globgeo  3 14 15 16 17 18 19 20 21 2 +     0.824     0.561
  2204-007   sess125.K2048globgeo  2 3 13 14 15 16 17 18 19 20 +     1.434     0.856
  2215+150   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.113     1.162
  2229+591   sess125.K2048globgeo  3 13 14 16 17 18 19 20 21 2 +     1.451     0.642
  CTA102     sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.066     1.048
  2234+282   sess125.K2048globgeo  1 2 3 13 15 16 17 19 20 21  +     1.294     0.621
  2245-328   sess125.K2048globgeo  2 3 15 16 19 20 21 22 25 26       0.414     0.491
  2251-419   sess125.K2048globgeo  1 2 3 15 16 20 22 25 26           0.699     0.452
  2254+074   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.210     0.564
  2315-172   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.389     1.683
  2319+317   sess125.K2048globgeo  1 2 3 13 14 15 16 17 18 19  +     1.124     0.901
  2344+798   sess125.K2048globgeo  3 13 16 17 19 20 21 26            1.194     0.729
  2351+456   sess125.K2048globgeo  3 14 15 16 17 19 20 21 25 2 +     0.590     0.425
  2353-686   sess125.K2048globgeo  1 2 22                            0.331     0.198
  2355-106   sess125.K2048globgeo  1 2 3 13 15 16 17 18 19 20  +     1.477     0.909
  0537-441   sess125.K2048globgeo  1 2                               1.267     1.267


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0002+541            65.0
   0003+380            50.4
   0008-264            27.7
   0012+610            71.8
   0013-184            24.7
   0016+731            83.1
   0017+200            37.2
   NGC0262             50.2
   0048-097            31.7
   0056-001            35.0
   0057+678            80.1
   0104-408            45.5
   0113-118            38.0
   0115-214            39.6
   0119+041            41.7
   0133+476            67.9
   0139-097            44.2
   0203+625            80.9
   0208-512            60.4
   0215+015            54.6
   0218+357            67.6
   0220-349            56.9
   0222-262            55.7
   4C67.05             85.5
   0234+285            67.6
   0235+164            63.4
   0240-060            59.7
   0244-470            64.3
   0245-167            60.3
   0248-266            61.4
   0249+171            66.7
   0256-005            64.5
   0300+470            79.8
   0306+102            68.9
   0309+411            79.1
   0312+100            70.3
   0327-241            70.1
   0345+460            86.8
   0346-279            74.3
   0354+559            90.7
   0406-127            80.1
   0420-014            85.0
   0422+004            85.7
   0426-380            82.3
   0430+289            92.0
   0451-282            88.5
   0454-810            82.2
   0458-020            94.3
   0459+415            99.2
   0507+179            99.0
   0511-220            94.1
   0524-485            91.0
   0527-053           100.9
   0529+483           104.5
   0537-286            98.4
   0548+084           108.0
   0558+234           111.4
   0603+882            99.1
   0606-223           106.4
   0610+260           114.0
   0611+131           114.0
   0627-199           111.7
   0632-235           111.7
   0640+090           120.9
   0716+714           109.7
   0723-008           130.1
   0723-265           120.9
   0728-235           123.4
   0735+178           134.2
   0736+017           133.9
   0738+491           124.4
   0802-010           139.7
   0805+410           132.8
   0805-077           138.3
   0814+425           133.4
   0826-373           124.6
   0834-201           137.9
   0835-339           128.3
   0843-547           112.3
   0847-120           145.4
   0847-354           128.7
   OJ287              151.3
   0904-201           143.0
   0917+624           123.9
   0918-534           115.7
   0920+390           144.5
   0938-133           153.4
   OK290              159.7
   0955+326           153.7
   1004+141           169.7
   1016-311           140.0
   1022+237           164.1
   1034-293           142.2
   1040+244           164.0
   1048-313           140.1
   1101+384           149.6
   1123+264           159.3
   1124-186           150.7
   1142+052           164.1
   1143-332           135.7
   1143-696           101.2
   1144+402           145.1
   1149-084           155.8
   1150+812           106.8
   1156-094           153.9
   1156-215           144.6
   1157-215           144.5
   1213-172           145.5
   1218-024           153.1
   1231+811           106.2
   1244-255           134.6
   1252+119           147.3
   1306-395           121.2
   OP326              135.8
   1315-058           138.6
   1324+224           138.1
   1329-049           135.7
   1330+022           137.2
   1334-127           131.7
   1339-206           127.2
   1339-287           123.0
   1342+663           114.3
   1346-109           129.7
   1349-439           112.3
   1354-152           126.3
   1357+769           106.7
   1406-076           126.1
   1424+240           124.2
   1424-418           108.2
   1441+522           114.6
   1451-400           104.6
   1456-179           111.4
   1504+377           114.0
   1504-166           110.0
   1505+428           113.0
   1511-100           110.1
   1514+004           111.3
   1514+197           112.8
   1538+477           106.6
   1546+027           103.5
   1555+001           101.1
   1556+335           103.6
   1604-333            92.7
   1606+106            99.7
   1606-742            84.1
   1614+051            97.1
   1619-680            84.1
   1622-297            89.5
   1636+473            96.8
   NRAO512             95.6
   1647-296            84.2
   1650-157            85.2
   1656-075            84.9
   1657-261            82.3
   1704-141            82.0
   1708-250            80.1
   1717+178            83.9
   1726-269            76.0
   1739-152            73.6
   1746+470            85.1
   1749+096            74.6
   1751+288            78.7
   1829-106            61.7
   1849+670            85.9
   1851+488            76.0
   1903+196            60.2
   1908-201            52.4
   1921-293            50.9
   1922-224            49.3
   1928+154            53.1
   1929+226            56.1
   1935+360            62.0
   1936+046            47.7
   1953-325            45.3
   1959+241            50.9
   1959+332            56.4
   2000+472            65.9
   2005-044            38.5
   2018+295            51.1
   2039+452            60.2
   2047-266            32.3
   2051-204            28.8
   2052-474            45.1
   2059+034            27.8
   2116+818            90.8
   2135+508            60.9
   2142+110            24.1
   2143-156            15.5
   2150+173            28.6
   2159+505            59.7
   2204-007            11.8
   2215+150            24.3
   2229+591            67.6
   CTA102              20.1
   2234+282            36.7
   2245-328            24.5
   2251-419            33.6
   2254+074            16.3
   2315-172            12.4
   2319+317            41.3
   2344+798            88.7
   2351+456            56.4
   2353-686            61.4
   2355-106            18.8
   0537-441            94.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

