  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
 Exp. Code:  GB049C  


Schedule Version:       1.00                                              
Processed by SCHED version: NRAO internal release of 4 October 2004       

PI:       N. Bartel, M.P. Rupen                                           

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@yorku.ca                                                 
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 256-8-2-ul 6cm                                       

Notes:    Fringe finder  : 0954+658                                       
          Pol. Calibrator: 0954+658, OQ208                                
          Amplitude check: 0954+658, OQ208                                
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

 Next scan frequencies:  4979.49  4979.49  4979.49  4979.49  4995.49  4995.49
                         4995.49  4995.49
 Next BBC frequencies:    879.49   879.49   879.49   879.49   895.49   895.49
                          895.49   895.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

17 40 00  0954+658     04 04 52  28.2  28.0 -5.9     -77.4     0   1  1      0  17 40 00
17 43 00  ---          04 07 52  28.5  28.1 -5.9     -78.1   180   F  1   2400

17 43 00  M81          04 07 52  29.5  24.2 -5.8     -80.7    -9   1  1   2400  17 43 00
17 45 20  ---          04 10 13  29.7  24.3 -5.8     -81.2   131   F  1   4267

17 45 20  SN1993J      04 10 13  29.7  24.3 -5.8     -81.2    -5   1  1   4267  17 45 20
17 47 20  ---          04 12 13  29.9  24.3 -5.7     -81.7   115   F  1   5867

17 47 20  M81          04 12 13  29.8  24.3 -5.7     -81.7    -5   1  1   5867  17 47 20
17 48 30  ---          04 13 23  29.9  24.3 -5.7     -82.0    65   F  1   6800

17 48 30  SN1993J      04 13 23  30.0  24.4 -5.7     -82.0    -5   1  1   6800  17 48 30
17 50 30  ---          04 15 23  30.1  24.4 -5.7     -82.4   115   F  1   8400

17 50 30  M81          04 15 23  30.1  24.3 -5.7     -82.4    -5   1  1   8400  17 50 30
17 51 40  ---          04 16 34  30.2  24.3 -5.7     -82.7    65   F  1   9333

17 51 40  SN1993J      04 16 34  30.2  24.4 -5.7     -82.7    -5   1  1   9333  17 51 40
17 53 40  ---          04 18 34  30.4  24.4 -5.6     -83.1   115   F  1  10933

17 53 40  M81          04 18 34  30.4  24.4 -5.6     -83.1    -5   1  1  10933  17 53 40
17 54 50  ---          04 19 44  30.5  24.4 -5.6     -83.4    65   F  1  11867

17 54 50  SN1993J      04 19 44  30.5  24.4 -5.6     -83.4    -5   1  1  11867  17 54 50
17 56 50  ---          04 21 44  30.7  24.5 -5.6     -83.9   115   F  1  13467

17 56 50  M81          04 21 44  30.7  24.4 -5.6     -83.9    -5   1  1  13467  17 56 50
17 58 00  ---          04 22 55  30.8  24.4 -5.6     -84.1    65   F  1  14400

17 58 00  SN1993J      04 22 55  30.8  24.5 -5.5     -84.1    -5   1  1  14400  17 58 00
18 00 00  ---          04 24 55  31.0  24.5 -5.5     -84.6   115   F  1  16000

18 00 00  M81          04 24 55  31.0  24.4 -5.5     -84.6    -5   1  1  16000  18 00 00
18 02 00  ---          04 26 55  31.2  24.5 -5.5     -85.0   115   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

18 02 40  M81          04 27 35  31.2  24.5 -5.5     -85.2    35   1  2  17600  18 02 40
18 04 50  ---          04 29 46  31.4  24.5 -5.4     -85.7   130   R  1  15867

18 04 50  SN1993J      04 29 46  31.4  24.5 -5.4     -85.7    -5   1  2  15867  18 04 50
18 06 50  ---          04 31 46  31.6  24.6 -5.4     -86.1   115   R  1  14267

18 06 50  M81          04 31 46  31.6  24.5 -5.4     -86.1    -5   1  2  14267  18 06 50
18 08 00  ---          04 32 56  31.7  24.5 -5.4     -86.4    65   R  1  13333

18 08 00  SN1993J      04 32 56  31.7  24.6 -5.4     -86.4    -5   1  2  13333  18 08 00
18 10 00  ---          04 34 57  31.9  24.6 -5.3     -86.9   115   R  1  11733

18 10 00  M81          04 34 57  31.9  24.5 -5.4     -86.9    -5   1  2  11733  18 10 00
18 11 10  ---          04 36 07  32.0  24.5 -5.3     -87.1    65   R  1  10800

18 11 10  SN1993J      04 36 07  32.0  24.6 -5.3     -87.1    -5   1  2  10800  18 11 10
18 13 10  ---          04 38 07  32.2  24.6 -5.3     -87.6   115   R  1   9200

18 13 10  M81          04 38 07  32.1  24.5 -5.3     -87.6    -5   1  2   9200  18 13 10
18 14 20  ---          04 39 17  32.3  24.5 -5.3     -87.9    65   R  1   8267

18 14 20  SN1993J      04 39 17  32.3  24.6 -5.3     -87.9    -5   1  2   8267  18 14 20
18 16 20  ---          04 41 18  32.4  24.6 -5.2     -88.3   115   R  1   6667

18 16 20  M81          04 41 18  32.4  24.5 -5.2     -88.3    -5   1  2   6667  18 16 20
18 17 30  ---          04 42 28  32.5  24.6 -5.2     -88.6    65   R  1   5733

18 17 30  SN1993J      04 42 28  32.5  24.6 -5.2     -88.6    -5   1  2   5733  18 17 30
18 19 30  ---          04 44 28  32.7  24.6 -5.2     -89.1   115   R  1   4133

18 19 30  M81          04 44 28  32.7  24.6 -5.2     -89.1    -5   1  2   4133  18 19 30
18 20 40  ---          04 45 38  32.8  24.6 -5.2     -89.4    65   R  1   3200

18 20 40  SN1993J      04 45 38  32.8  24.6 -5.2     -89.4    -5   1  2   3200  18 20 40
18 22 40  ---          04 47 39  33.0  24.6 -5.1     -89.8   115   R  1   1600

18 22 40  M81          04 47 39  33.0  24.6 -5.1     -89.8    -5   1  2   1600  18 22 40
18 24 40  ---          04 49 39  33.2  24.6 -5.1     -90.3   115   R  1      0

18 34 40  0954+658     04 59 41  33.8  28.8 -5.0     -89.5   591   1  3      0  18 34 40
18 37 40  ---          05 02 41  34.1  28.8 -4.9     -90.2   180   F  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

18 37 40  M81          05 02 41  34.3  24.5 -4.9     -93.4    -9   1  3   2400  18 37 40
18 40 00  ---          05 05 02  34.6  24.5 -4.8     -93.9   131   F  1   4267

18 40 00  SN1993J      05 05 02  34.6  24.6 -4.8     -93.9    -5   1  3   4267  18 40 00
18 42 00  ---          05 07 02  34.7  24.5 -4.8     -94.4   115   F  1   5867

18 42 00  M81          05 07 02  34.7  24.5 -4.8     -94.4    -5   1  3   5867  18 42 00
18 43 10  ---          05 08 12  34.8  24.5 -4.8     -94.7    65   F  1   6800

18 43 10  SN1993J      05 08 12  34.9  24.5 -4.8     -94.7    -5   1  3   6800  18 43 10
18 45 10  ---          05 10 12  35.0  24.5 -4.8     -95.1   115   F  1   8400

18 45 10  M81          05 10 12  35.0  24.5 -4.8     -95.1    -5   1  3   8400  18 45 10
18 46 20  ---          05 11 23  35.1  24.4 -4.7     -95.4    65   F  1   9333

18 46 20  SN1993J      05 11 23  35.1  24.5 -4.7     -95.4    -5   1  3   9333  18 46 20
18 48 20  ---          05 13 23  35.3  24.5 -4.7     -95.9   115   F  1  10933

18 48 20  M81          05 13 23  35.3  24.4 -4.7     -95.9    -5   1  3  10933  18 48 20
18 49 30  ---          05 14 33  35.4  24.4 -4.7     -96.2    65   F  1  11867

18 49 30  SN1993J      05 14 33  35.4  24.5 -4.7     -96.2    -5   1  3  11867  18 49 30
18 51 30  ---          05 16 33  35.6  24.4 -4.7     -96.7   115   F  1  13467

18 51 30  M81          05 16 33  35.6  24.4 -4.7     -96.7    -5   1  3  13467  18 51 30
18 52 40  ---          05 17 44  35.7  24.4 -4.6     -97.0    65   F  1  14400

18 52 40  SN1993J      05 17 44  35.7  24.4 -4.6     -97.0    -5   1  3  14400  18 52 40
18 54 40  ---          05 19 44  35.9  24.4 -4.6     -97.4   115   F  1  16000

18 54 40  M81          05 19 44  35.9  24.3 -4.6     -97.4    -5   1  3  16000  18 54 40
18 56 40  ---          05 21 44  36.0  24.3 -4.6     -97.9   115   F  1  17600

18 57 20  M81          05 22 24  36.1  24.3 -4.6     -98.1    35   1  4  17600  18 57 20
18 59 30  ---          05 24 35  36.3  24.3 -4.5     -98.6   130   R  1  15867

18 59 30  SN1993J      05 24 35  36.3  24.3 -4.5     -98.6    -5   1  4  15867  18 59 30
19 01 30  ---          05 26 35  36.5  24.3 -4.5     -99.1   115   R  1  14267

19 01 30  M81          05 26 35  36.5  24.2 -4.5     -99.1    -5   1  4  14267  19 01 30
19 02 40  ---          05 27 45  36.6  24.2 -4.5     -99.4    65   R  1  13333
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

19 02 40  SN1993J      05 27 45  36.6  24.3 -4.5     -99.4    -5   1  4  13333  19 02 40
19 04 40  ---          05 29 46  36.8  24.2 -4.4     -99.9   115   R  1  11733

19 04 40  M81          05 29 46  36.7  24.2 -4.4     -99.9    -5   1  4  11733  19 04 40
19 05 50  ---          05 30 56  36.9  24.1 -4.4    -100.2    65   R  1  10800

19 05 50  SN1993J      05 30 56  36.9  24.2 -4.4    -100.2    -5   1  4  10800  19 05 50
19 07 50  ---          05 32 56  37.0  24.2 -4.4    -100.7   115   R  1   9200

19 07 50  M81          05 32 56  37.0  24.1 -4.4    -100.7    -5   1  4   9200  19 07 50
19 09 00  ---          05 34 06  37.1  24.1 -4.4    -100.9    65   R  1   8267

19 09 00  SN1993J      05 34 06  37.2  24.1 -4.4    -100.9    -5   1  4   8267  19 09 00
19 11 00  ---          05 36 07  37.3  24.1 -4.3    -101.4   115   R  1   6667

19 11 00  M81          05 36 07  37.3  24.0 -4.3    -101.4    -5   1  4   6667  19 11 00
19 12 10  ---          05 37 17  37.4  24.0 -4.3    -101.7    65   R  1   5733

19 12 10  SN1993J      05 37 17  37.4  24.1 -4.3    -101.7    -5   1  4   5733  19 12 10
19 14 10  ---          05 39 17  37.6  24.0 -4.3    -102.2   115   R  1   4133

19 14 10  M81          05 39 17  37.6  24.0 -4.3    -102.2    -5   1  4   4133  19 14 10
19 15 20  ---          05 40 27  37.7  23.9 -4.3    -102.5    65   R  1   3200

19 15 20  SN1993J      05 40 27  37.7  24.0 -4.3    -102.5    -5   1  4   3200  19 15 20
19 17 20  ---          05 42 28  37.9  23.9 -4.2    -103.0   115   R  1   1600

19 17 20  M81          05 42 28  37.9  23.9 -4.2    -103.0    -5   1  4   1600  19 17 20
19 19 20  ---          05 44 28  38.0  23.8 -4.2    -103.5   115   R  1      0

19 20 00  M81          05 45 08  38.1  23.8 -4.2    -103.7    35   1  5      0  19 20 00
19 22 10  ---          05 47 18  38.3  23.8 -4.1    -104.2   130   F  1   1733

19 22 10  SN1993J      05 47 18  38.3  23.8 -4.1    -104.2    -5   1  5   1733  19 22 10
19 24 10  ---          05 49 19  38.5  23.8 -4.1    -104.7   115   F  1   3333

19 24 10  M81          05 49 19  38.5  23.7 -4.1    -104.7    -5   1  5   3333  19 24 10
19 25 20  ---          05 50 29  38.6  23.7 -4.1    -105.0    65   F  1   4267

19 25 20  SN1993J      05 50 29  38.6  23.7 -4.1    -105.0    -5   1  5   4267  19 25 20
19 27 20  ---          05 52 29  38.8  23.7 -4.1    -105.5   115   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

19 27 20  M81          05 52 29  38.7  23.6 -4.1    -105.5    -5   1  5   5867  19 27 20
19 28 30  ---          05 53 40  38.8  23.6 -4.0    -105.8    65   F  1   6800

19 28 30  SN1993J      05 53 40  38.9  23.6 -4.0    -105.8    -5   1  5   6800  19 28 30
19 30 30  ---          05 55 40  39.0  23.6 -4.0    -106.3   115   F  1   8400

19 30 30  M81          05 55 40  39.0  23.5 -4.0    -106.3    -5   1  5   8400  19 30 30
19 31 40  ---          05 56 50  39.1  23.5 -4.0    -106.6    65   F  1   9333

19 31 40  SN1993J      05 56 50  39.1  23.5 -4.0    -106.6    -5   1  5   9333  19 31 40
19 33 40  ---          05 58 50  39.3  23.5 -4.0    -107.1   115   F  1  10933

19 33 40  M81          05 58 50  39.3  23.4 -4.0    -107.1    -5   1  5  10933  19 33 40
19 34 50  ---          06 00 01  39.4  23.4 -3.9    -107.4    65   F  1  11867

19 34 50  SN1993J      06 00 01  39.4  23.4 -3.9    -107.4    -5   1  5  11867  19 34 50
19 36 50  ---          06 02 01  39.6  23.3 -3.9    -108.0   115   F  1  13467

19 36 50  M81          06 02 01  39.5  23.3 -3.9    -108.0    -5   1  5  13467  19 36 50
19 38 00  ---          06 03 11  39.6  23.2 -3.9    -108.3    65   F  1  14400

19 38 00  SN1993J      06 03 11  39.7  23.3 -3.9    -108.3    -5   1  5  14400  19 38 00
19 40 00  ---          06 05 11  39.8  23.2 -3.8    -108.8   115   F  1  16000

19 40 00  M81          06 05 11  39.8  23.2 -3.8    -108.8    -5   1  5  16000  19 40 00
19 42 00  ---          06 07 12  40.0  23.1 -3.8    -109.3   115   F  1  17600

19 42 40  M81          06 07 52  40.0  23.1 -3.8    -109.5    35   1  6  17600  19 42 40
19 44 50  ---          06 10 02  40.2  23.0 -3.8    -110.0   130   R  1  15867

19 44 50  SN1993J      06 10 02  40.3  23.0 -3.8    -110.0    -5   1  6  15867  19 44 50
19 46 50  ---          06 12 03  40.4  23.0 -3.7    -110.5   115   R  1  14267

19 46 50  M81          06 12 03  40.4  22.9 -3.7    -110.5    -5   1  6  14267  19 46 50
19 48 00  ---          06 13 13  40.5  22.9 -3.7    -110.8    65   R  1  13333

19 48 00  SN1993J      06 13 13  40.5  22.9 -3.7    -110.8    -5   1  6  13333  19 48 00
19 50 00  ---          06 15 13  40.7  22.8 -3.7    -111.4   115   R  1  11733

19 50 00  M81          06 15 13  40.7  22.8 -3.7    -111.4    -5   1  6  11733  19 50 00
19 51 10  ---          06 16 23  40.8  22.7 -3.7    -111.7    65   R  1  10800
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

19 51 10  SN1993J      06 16 23  40.8  22.8 -3.7    -111.7    -5   1  6  10800  19 51 10
19 53 10  ---          06 18 24  40.9  22.7 -3.6    -112.2   115   R  1   9200

19 53 10  M81          06 18 24  40.9  22.6 -3.6    -112.2    -5   1  6   9200  19 53 10
19 54 20  ---          06 19 34  41.0  22.6 -3.6    -112.5    65   R  1   8267

19 54 20  SN1993J      06 19 34  41.0  22.6 -3.6    -112.5    -5   1  6   8267  19 54 20
19 56 20  ---          06 21 34  41.2  22.5 -3.6    -113.0   115   R  1   6667

19 56 20  M81          06 21 34  41.2  22.5 -3.6    -113.0    -5   1  6   6667  19 56 20
19 57 30  ---          06 22 44  41.3  22.4 -3.6    -113.3    65   R  1   5733

19 57 30  SN1993J      06 22 44  41.3  22.5 -3.6    -113.4    -5   1  6   5733  19 57 30
19 59 30  ---          06 24 45  41.5  22.4 -3.5    -113.9   115   R  1   4133

19 59 30  M81          06 24 45  41.4  22.3 -3.5    -113.9    -5   1  6   4133  19 59 30
20 00 40  ---          06 25 55  41.5  22.3 -3.5    -114.2    65   R  1   3200

20 00 40  SN1993J      06 25 55  41.6  22.3 -3.5    -114.2    -5   1  6   3200  20 00 40
20 02 40  ---          06 27 55  41.7  22.2 -3.5    -114.7   115   R  1   1600

20 02 40  M81          06 27 55  41.7  22.2 -3.5    -114.7    -5   1  6   1600  20 02 40
20 04 40  ---          06 29 55  41.9  22.1 -3.4    -115.3   115   R  1      0

20 05 20  M81          06 30 36  41.9  22.0 -3.4    -115.4    35   1  7      0  20 05 20
20 07 30  ---          06 32 46  42.1  21.9 -3.4    -116.0   130   F  1   1733

20 07 30  SN1993J      06 32 46  42.1  22.0 -3.4    -116.0    -5   1  7   1733  20 07 30
20 09 30  ---          06 34 46  42.3  21.9 -3.4    -116.6   115   F  1   3333

20 09 30  M81          06 34 46  42.3  21.8 -3.4    -116.6    -5   1  7   3333  20 09 30
20 10 40  ---          06 35 56  42.3  21.8 -3.3    -116.9    65   F  1   4267

20 10 40  SN1993J      06 35 56  42.4  21.8 -3.3    -116.9    -5   1  7   4267  20 10 40
20 12 40  ---          06 37 57  42.5  21.7 -3.3    -117.4   115   F  1   5867

20 12 40  M81          06 37 57  42.5  21.6 -3.3    -117.4    -5   1  7   5867  20 12 40
20 13 50  ---          06 39 07  42.6  21.6 -3.3    -117.7    65   F  1   6800

20 13 50  SN1993J      06 39 07  42.6  21.6 -3.3    -117.7    -5   1  7   6800  20 13 50
20 15 50  ---          06 41 07  42.8  21.5 -3.2    -118.3   115   F  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

20 15 50  M81          06 41 07  42.8  21.5 -3.2    -118.3    -5   1  7   8400  20 15 50
20 17 00  ---          06 42 18  42.8  21.4 -3.2    -118.6    65   F  1   9333

20 17 00  SN1993J      06 42 18  42.9  21.4 -3.2    -118.6    -5   1  7   9333  20 17 00
20 19 00  ---          06 44 18  43.0  21.3 -3.2    -119.2   115   F  1  10933

20 19 00  M81          06 44 18  43.0  21.3 -3.2    -119.2    -5   1  7  10933  20 19 00
20 20 10  ---          06 45 28  43.1  21.2 -3.2    -119.5    65   F  1  11867

20 20 10  SN1993J      06 45 28  43.1  21.3 -3.2    -119.5    -5   1  7  11867  20 20 10
20 22 10  ---          06 47 28  43.3  21.1 -3.1    -120.0   115   F  1  13467

20 22 10  M81          06 47 28  43.3  21.1 -3.1    -120.0    -5   1  7  13467  20 22 10
20 23 20  ---          06 48 39  43.3  21.0 -3.1    -120.3    65   F  1  14400

20 23 20  SN1993J      06 48 39  43.4  21.1 -3.1    -120.4    -5   1  7  14400  20 23 20
20 25 20  ---          06 50 39  43.5  20.9 -3.1    -120.9   115   F  1  16000

20 25 20  M81          06 50 39  43.5  20.9 -3.1    -120.9    -5   1  7  16000  20 25 20
20 27 20  ---          06 52 39  43.7  20.8 -3.1    -121.5   115   F  1  17600

20 37 20  0954+658     07 02 41  46.0  24.5 -2.9    -120.4   589   1  8  17600  20 37 20
20 40 20  ---          07 05 41  46.3  24.3 -2.9    -121.2   180   R  1  15200

20 40 20  M81          07 05 41  44.6  19.9 -2.8    -125.1    -9   1  8  15200  20 40 20
20 42 40  ---          07 08 02  44.8  19.7 -2.8    -125.8   131   R  1  13333

20 42 40  SN1993J      07 08 02  44.8  19.7 -2.8    -125.8    -5   1  8  13333  20 42 40
20 44 40  ---          07 10 02  45.0  19.6 -2.8    -126.4   115   R  1  11733

20 44 40  M81          07 10 02  44.9  19.6 -2.8    -126.4    -5   1  8  11733  20 44 40
20 45 50  ---          07 11 12  45.0  19.5 -2.7    -126.7    65   R  1  10800

20 45 50  SN1993J      07 11 12  45.1  19.5 -2.7    -126.7    -5   1  8  10800  20 45 50
20 47 50  ---          07 13 13  45.2  19.4 -2.7    -127.3   115   R  1   9200

20 47 50  M81          07 13 13  45.2  19.3 -2.7    -127.3    -5   1  8   9200  20 47 50
20 49 00  ---          07 14 23  45.3  19.2 -2.7    -127.6    65   R  1   8267

20 49 00  SN1993J      07 14 23  45.3  19.3 -2.7    -127.6    -5   1  8   8267  20 49 00
20 51 00  ---          07 16 23  45.4  19.1 -2.7    -128.2   115   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

20 51 00  M81          07 16 23  45.4  19.1 -2.7    -128.2    -5   1  8   6667  20 51 00
20 52 10  ---          07 17 33  45.5  19.0 -2.6    -128.5    65   R  1   5733

20 52 10  SN1993J      07 17 33  45.5  19.0 -2.6    -128.5    -5   1  8   5733  20 52 10
20 54 10  ---          07 19 34  45.7  18.9 -2.6    -129.1   115   R  1   4133

20 54 10  M81          07 19 34  45.6  18.8 -2.6    -129.1    -5   1  8   4133  20 54 10
20 55 20  ---          07 20 44  45.7  18.7 -2.6    -129.5    65   R  1   3200

20 55 20  SN1993J      07 20 44  45.7  18.8 -2.6    -129.5    -5   1  8   3200  20 55 20
20 57 20  ---          07 22 44  45.9  18.6 -2.6    -130.0   115   R  1   1600

20 57 20  M81          07 22 44  45.8  18.6 -2.6    -130.0    -5   1  8   1600  20 57 20
20 59 20  ---          07 24 44  46.0  18.4 -2.5    -130.6   115   R  1      0

21 00 00  M81          07 25 25  46.0  18.3 -2.5    -130.8    35   1  9      0  21 00 00
21 02 10  ---          07 27 35  46.2  18.1 -2.5    -131.5   130   F  1   1733

21 02 10  SN1993J      07 27 35  46.2  18.2 -2.5    -131.5    -5   1  9   1733  21 02 10
21 04 10  ---          07 29 35  46.3  18.0 -2.4    -132.1   115   F  1   3333

21 04 10  M81          07 29 35  46.3  18.0 -2.4    -132.1    -5   1  9   3333  21 04 10
21 05 20  ---          07 30 45  46.4  17.9 -2.4    -132.4    65   F  1   4267

21 05 20  SN1993J      07 30 45  46.4  17.9 -2.4    -132.4    -5   1  9   4267  21 05 20
21 07 20  ---          07 32 46  46.5  17.7 -2.4    -133.0   115   F  1   5867

21 07 20  M81          07 32 46  46.5  17.7 -2.4    -133.0    -5   1  9   5867  21 07 20
21 08 30  ---          07 33 56  46.6  17.6 -2.4    -133.4    65   F  1   6800

21 08 30  SN1993J      07 33 56  46.6  17.6 -2.4    -133.4    -5   1  9   6800  21 08 30
21 10 30  ---          07 35 56  46.8  17.4 -2.3    -134.0   115   F  1   8400

21 10 30  M81          07 35 56  46.7  17.4 -2.3    -134.0    -5   1  9   8400  21 10 30
21 11 40  ---          07 37 06  46.8  17.3 -2.3    -134.3    65   F  1   9333

21 11 40  SN1993J      07 37 06  46.8  17.3 -2.3    -134.3    -5   1  9   9333  21 11 40
21 13 40  ---          07 39 07  47.0  17.2 -2.3    -134.9   115   F  1  10933

21 13 40  M81          07 39 07  46.9  17.1 -2.3    -134.9    -5   1  9  10933  21 13 40
21 14 50  ---          07 40 17  47.0  17.0 -2.3    -135.3    65   F  1  11867
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

21 14 50  SN1993J      07 40 17  47.0  17.0 -2.3    -135.3    -5   1  9  11867  21 14 50
21 16 50  ---          07 42 17  47.2  16.9 -2.2    -135.9   115   F  1  13467

21 16 50  M81          07 42 17  47.1  16.8 -2.2    -135.9    -5   1  9  13467  21 16 50
21 18 00  ---          07 43 28  47.2  16.7 -2.2    -136.2    65   F  1  14400

21 18 00  SN1993J      07 43 28  47.2  16.7 -2.2    -136.2    -5   1  9  14400  21 18 00
21 20 00  ---          07 45 28  47.3  16.6 -2.2    -136.8   115   F  1  16000

21 20 00  M81          07 45 28  47.3  16.5 -2.2    -136.8    -5   1  9  16000  21 20 00
21 22 00  ---          07 47 28  47.4  16.3 -2.1    -137.4   115   F  1  17600

21 22 40  M81          07 48 08  47.5  16.3 -2.1    -137.6    35   1 10  17600  21 22 40
21 24 50  ---          07 50 19  47.6  16.0 -2.1    -138.3   130   R  1  15867

21 24 50  SN1993J      07 50 19  47.6  16.1 -2.1    -138.3    -5   1 10  15867  21 24 50
21 26 50  ---          07 52 19  47.8  15.9 -2.1    -138.9   115   R  1  14267

21 26 50  M81          07 52 19  47.7  15.8 -2.1    -138.9    -5   1 10  14267  21 26 50
21 28 00  ---          07 53 29  47.8  15.7 -2.0    -139.3    65   R  1  13333

21 28 00  SN1993J      07 53 29  47.8  15.8 -2.0    -139.3    -5   1 10  13333  21 28 00
21 30 00  ---          07 55 29  47.9  15.6 -2.0    -139.9   115   R  1  11733

21 30 00  M81          07 55 29  47.9  15.5 -2.0    -139.9    -5   1 10  11733  21 30 00
21 31 10  ---          07 56 40  48.0  15.4 -2.0    -140.3    65   R  1  10800

21 31 10  SN1993J      07 56 40  48.0  15.4 -2.0    -140.3    -5   1 10  10800  21 31 10
21 33 10  ---          07 58 40  48.1  15.2 -2.0    -140.9   115   R  1   9200

21 33 10  M81          07 58 40  48.1  15.2 -2.0    -140.9    -5   1 10   9200  21 33 10
21 34 20  ---          07 59 50  48.2  15.1 -1.9    -141.2    65   R  1   8267

21 34 20  SN1993J      07 59 50  48.2  15.1 -1.9    -141.3    -5   1 10   8267  21 34 20
21 36 20  ---          08 01 51  48.3  14.9 -1.9    -141.9   115   R  1   6667

21 36 20  M81          08 01 51  48.3  14.9 -1.9    -141.9    -5   1 10   6667  21 36 20
21 37 30  ---          08 03 01  48.3  14.7 -1.9    -142.2    65   R  1   5733

21 37 30  SN1993J      08 03 01  48.4  14.8 -1.9    -142.3    -5   1 10   5733  21 37 30
21 39 30  ---          08 05 01  48.5  14.6 -1.8    -142.9   115   R  1   4133
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

21 39 30  M81          08 05 01  48.4  14.5 -1.8    -142.9    -5   1 10   4133  21 39 30
21 40 40  ---          08 06 11  48.5  14.4 -1.8    -143.2    65   R  1   3200

21 40 40  SN1993J      08 06 11  48.5  14.4 -1.8    -143.2    -5   1 10   3200  21 40 40
21 42 40  ---          08 08 12  48.6  14.2 -1.8    -143.9   115   R  1   1600

21 42 40  M81          08 08 12  48.6  14.2 -1.8    -143.9    -5   1 10   1600  21 42 40
21 44 40  ---          08 10 12  48.7  14.0 -1.8    -144.5   115   R  1      0

21 45 20  M81          08 10 52  48.7  13.9 -1.8    -144.7    35   1 11      0  21 45 20
21 47 30  ---          08 13 02  48.9  13.7 -1.7    -145.4   130   F  1   1733

21 47 30  SN1993J      08 13 02  48.9  13.7 -1.7    -145.4    -5   1 11   1733  21 47 30
21 49 30  ---          08 15 03  49.0  13.4 -1.7    -146.1   115   F  1   3333

21 49 30  M81          08 15 03  49.0  13.4 -1.7    -146.0    -5   1 11   3333  21 49 30
21 50 40  ---          08 16 13  49.0  13.3 -1.7    -146.4    65   F  1   4267

21 50 40  SN1993J      08 16 13  49.1  13.3 -1.7    -146.4    -5   1 11   4267  21 50 40
21 52 40  ---          08 18 13  49.2  13.1 -1.6    -147.1   115   F  1   5867

21 52 40  M81          08 18 13  49.1  13.1 -1.6    -147.1    -5   1 11   5867  21 52 40
21 53 50  ---          08 19 23  49.2  12.9 -1.6    -147.4    65   F  1   6800

21 53 50  SN1993J      08 19 23  49.2  13.0 -1.6    -147.4    -5   1 11   6800  21 53 50
21 55 50  ---          08 21 24  49.3  12.7 -1.6    -148.1   115   F  1   8400

21 55 50  M81          08 21 24  49.3  12.7 -1.6    -148.1    -5   1 11   8400  21 55 50
21 57 00  ---          08 22 34  49.3  12.6 -1.6    -148.4    65   F  1   9333

21 57 00  SN1993J      08 22 34  49.4  12.6 -1.6    -148.5    -5   1 11   9333  21 57 00
21 59 00  ---          08 24 34  49.5  12.3 -1.5    -149.1   115   F  1  10933

21 59 00  M81          08 24 34  49.4  12.3 -1.5    -149.1    -5   1 11  10933  21 59 00
22 00 10  ---          08 25 44  49.5  12.2 -1.5    -149.5    65   F  1  11867

22 00 10  SN1993J      08 25 44  49.5  12.2 -1.5    -149.5    -5   1 11  11867  22 00 10
22 02 10  ---          08 27 45  49.6  12.0 -1.5    -150.1   115   F  1  13467

22 02 10  M81          08 27 45  49.6  11.9 -1.5    -150.1    -5   1 11  13467  22 02 10
22 03 20  ---          08 28 55  49.6  11.8 -1.5    -150.5    65   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

22 03 20  SN1993J      08 28 55  49.7  11.8 -1.4    -150.5    -5   1 11  14400  22 03 20
22 05 20  ---          08 30 55  49.7  11.6 -1.4    -151.2   115   F  1  16000

22 05 20  M81          08 30 55  49.7  11.6 -1.4    -151.2    -5   1 11  16000  22 05 20
22 07 20  ---          08 32 56  49.8  11.3 -1.4    -151.8   115   F  1  17600

22 08 00  M81          08 33 36  49.8  11.2 -1.4    -152.0    35   1 12  17600  22 08 00
22 10 10  ---          08 35 46  49.9  11.0 -1.3    -152.7   130   R  1  15867

22 10 10  SN1993J      08 35 46  49.9  11.0 -1.3    -152.8    -5   1 12  15867  22 10 10
22 12 10  ---          08 37 46  50.0  10.7 -1.3    -153.4   115   R  1  14267

22 12 10  M81          08 37 46  50.0  10.7 -1.3    -153.4    -5   1 12  14267  22 12 10
22 13 20  ---          08 38 57  50.0  10.6 -1.3    -153.8    65   R  1  13333

22 13 20  SN1993J      08 38 57  50.1  10.6 -1.3    -153.8    -5   1 12  13333  22 13 20
22 15 20  ---          08 40 57  50.2  10.3 -1.2    -154.5   115   R  1  11733

22 15 20  M81          08 40 57  50.1  10.3 -1.3    -154.4    -5   1 12  11733  22 15 20
22 16 30  ---          08 42 07  50.2  10.2 -1.2    -154.8    65   R  1  10800

22 16 30  SN1993J      08 42 07  50.2  10.2 -1.2    -154.9    -5   1 12  10800  22 16 30
22 18 30  ---          08 44 07  50.3   9.9 -1.2    -155.5   115   R  1   9200

22 18 30  M81          08 44 07  50.2   9.9 -1.2    -155.5    -5   1 12   9200  22 18 30
22 19 40  ---          08 45 18  50.3   9.8 -1.2    -155.9    65   R  1   8267

22 19 40  SN1993J      08 45 18  50.3   9.8 -1.2    -155.9    -5   1 12   8267  22 19 40
22 21 40  ---          08 47 18  50.4   9.5 -1.1    -156.6   115   R  1   6667

22 21 40  M81          08 47 18  50.3   9.5 -1.1    -156.5    -5   1 12   6667  22 21 40
22 22 50  ---          08 48 28  50.4   9.4 -1.1    -156.9    65   R  1   5733

22 22 50  SN1993J      08 48 28  50.4   9.4 -1.1    -157.0    -5   1 12   5733  22 22 50
22 24 50  ---          08 50 29  50.5   9.1 -1.1    -157.6   115   R  1   4133

22 24 50  M81          08 50 29  50.5   9.1 -1.1    -157.6    -5   1 12   4133  22 24 50
22 26 00  ---          08 51 39  50.5   9.0 -1.1    -158.0    65   R  1   3200

22 26 00  SN1993J      08 51 39  50.5   9.0 -1.1    -158.0    -5   1 12   3200  22 26 00
22 28 00  ---          08 53 39  50.6   8.7 -1.0    -158.7   115   R  1   1600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

22 28 00  M81          08 53 39  50.6   8.7 -1.0    -158.7    -5   1 12   1600  22 28 00
22 30 00  ---          08 55 39  50.6   8.4 -1.0    -159.3   115   R  1      0

22 40 00  0954+658     09 05 41  54.1   9.4 -0.9    -160.1   587   1 13      0  22 40 00
22 43 00  ---          09 08 41  54.2   8.9 -0.8    -161.2   180   F  1   2400

22 43 00  M81          09 08 41  51.0   6.7 -0.8    -163.7   -12   1 13   2400  22 43 00
22 45 20  ---          09 11 02  51.0   6.4 -0.7    -164.5   128   F  1   4267

22 45 20  SN1993J      09 11 02  51.1   6.4 -0.7    -164.6    -5   1 13   4267  22 45 20
22 47 20  ---          09 13 02  51.1   6.1 -0.7    -165.2   115   F  1   5867

22 47 20  M81          09 13 02  51.1   6.1 -0.7    -165.2    -5   1 13   5867  22 47 20
22 48 30  ---          09 14 12  51.1   5.9 -0.7    -165.6    65   F  1   6800

22 48 30  SN1993J      09 14 12  51.2   5.9 -0.7    -165.6    -5   1 13   6800  22 48 30
22 50 30  ---          09 16 13  51.2   5.6 -0.7    -166.3   115   F  1   8400

22 50 30  M81          09 16 13  51.2   5.7 -0.7    -166.3    -5   1 13   8400  22 50 30
22 51 40  ---          09 17 23  51.2   5.5 -0.6    -166.7    65   F  1   9333

22 51 40  SN1993J      09 17 23  51.2   5.5 -0.6    -166.7    -5   1 13   9333  22 51 40
22 53 40  ---          09 19 23  51.3   5.2 -0.6    -167.4   115   F  1  10933

22 53 40  M81          09 19 23  51.2   5.2 -0.6    -167.4    -5   1 13  10933  22 53 40
22 54 50  ---          09 20 33  51.3   5.0 -0.6    -167.8    65   F  1  11867

22 54 50  SN1993J      09 20 33  51.3   5.0 -0.6    -167.8    -5   1 13  11867  22 54 50
22 56 50  ---          09 22 34  51.3   4.8 -0.6    -168.5   115   F  1  13467

22 56 50  M81          09 22 34  51.3   4.8 -0.6    -168.5    -5   1 13  13467  22 56 50
22 58 00  ---          09 23 44  51.3   4.6 -0.5    -168.9    65   F  1  14400

22 58 00  SN1993J      09 23 44  51.4   4.6 -0.5    -168.9    -5   1 13  14400  22 58 00
23 00 00  ---          09 25 44  51.4   4.3 -0.5    -169.6   115   F  1  16000

23 00 00  M81          09 25 44  51.3   4.3 -0.5    -169.6    -5   1 13  16000  23 00 00
23 02 00  ---          09 27 45  51.4   4.0 -0.5    -170.2   115   F  1  17600

23 02 40  M81          09 28 25  51.4   3.9 -0.5    -170.5    35   1 14  17600  23 02 40
23 04 50  ---          09 30 35  51.4   3.6 -0.4    -171.2   130   R  1  15867
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

23 04 50  SN1993J      09 30 35  51.5   3.6 -0.4    -171.3    -5   1 14  15867  23 04 50
23 06 50  ---          09 32 35  51.5   3.3 -0.4    -172.0   115   R  1  14267

23 06 50  M81          09 32 35  51.4   3.4 -0.4    -171.9    -5   1 14  14267  23 06 50
23 08 00  ---          09 33 46  51.5   3.2 -0.4    -172.3    65   R  1  13333

23 08 00  SN1993J      09 33 46  51.5   3.2 -0.4    -172.4    -5   1 14  13333  23 08 00
23 10 00  ---          09 35 46  51.5   2.9 -0.3    -173.1   115   R  1  11733

23 10 00  M81          09 35 46  51.5   2.9 -0.3    -173.0    -5   1 14  11733  23 10 00
23 11 10  ---          09 36 56  51.5   2.7 -0.3    -173.4    65   R  1  10800

23 11 10  SN1993J      09 36 56  51.5   2.7 -0.3    -173.5    -5   1 14  10800  23 11 10
23 13 10  ---          09 38 56  51.6   2.4 -0.3    -174.1   115   R  1   9200

23 13 10  M81          09 38 56  51.5   2.4 -0.3    -174.1    -5   1 14   9200  23 13 10
23 14 20  ---          09 40 07  51.5   2.3 -0.3    -174.5    65   R  1   8267

23 14 20  SN1993J      09 40 07  51.6   2.3 -0.3    -174.6    -5   1 14   8267  23 14 20
23 16 20  ---          09 42 07  51.6   2.0 -0.2    -175.2   115   R  1   6667

23 16 20  M81          09 42 07  51.5   2.0 -0.2    -175.2    -5   1 14   6667  23 16 20
23 17 30  ---          09 43 17  51.5   1.8 -0.2    -175.6    65   R  1   5733

23 17 30  SN1993J      09 43 17  51.6   1.8 -0.2    -175.7    -5   1 14   5733  23 17 30
23 19 30  ---          09 45 17  51.6   1.5 -0.2    -176.3   115   R  1   4133

23 19 30  M81          09 45 17  51.6   1.5 -0.2    -176.3    -5   1 14   4133  23 19 30
23 20 40  ---          09 46 28  51.6   1.4 -0.2    -176.7    65   R  1   3200

23 20 40  SN1993J      09 46 28  51.6   1.4 -0.2    -176.7    -5   1 14   3200  23 20 40
23 22 40  ---          09 48 28  51.6   1.1 -0.1    -177.4   115   R  1   1600

23 22 40  M81          09 48 28  51.6   1.1 -0.1    -177.4    -5   1 14   1600  23 22 40
23 24 40  ---          09 50 28  51.6   0.8 -0.1    -178.1   115   R  1      0

-----------  Tape Change ------------

23 39 40  M81          10 05 31  51.6  -1.4  0.2     176.7   893   2  1      0  23 39 40
23 41 50  ---          10 07 41  51.6  -1.7  0.2     175.9   130   F  1   1733

23 41 50  SN1993J      10 07 41  51.6  -1.7  0.2     175.9    -5   2  1   1733  23 41 50
23 43 50  ---          10 09 41  51.6  -2.0  0.2     175.2   115   F  1   3333
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  11 Jun 2005   Day 162 ---

23 43 50  M81          10 09 41  51.5  -2.0  0.2     175.3    -5   2  1   3333  23 43 50
23 45 00  ---          10 10 52  51.5  -2.1  0.2     174.9    65   F  1   4267

23 45 00  SN1993J      10 10 52  51.6  -2.2  0.3     174.8    -5   2  1   4267  23 45 00
23 47 00  ---          10 12 52  51.6  -2.5  0.3     174.1   115   F  1   5867

23 47 00  M81          10 12 52  51.5  -2.4  0.3     174.2    -5   2  1   5867  23 47 00
23 48 10  ---          10 14 02  51.5  -2.6  0.3     173.8    65   F  1   6800

23 48 10  SN1993J      10 14 02  51.5  -2.6  0.3     173.7    -5   2  1   6800  23 48 10
23 50 10  ---          10 16 03  51.5  -2.9  0.3     173.0   115   F  1   8400

23 50 10  M81          10 16 03  51.5  -2.9  0.3     173.1    -5   2  1   8400  23 50 10
23 51 20  ---          10 17 13  51.5  -3.0  0.4     172.7    65   F  1   9333

23 51 20  SN1993J      10 17 13  51.5  -3.1  0.4     172.6    -5   2  1   9333  23 51 20
23 53 20  ---          10 19 13  51.5  -3.4  0.4     171.9   115   F  1  10933

23 53 20  M81          10 19 13  51.4  -3.3  0.4     172.0    -5   2  1  10933  23 53 20
23 54 30  ---          10 20 23  51.4  -3.5  0.4     171.6    65   F  1  11867

23 54 30  SN1993J      10 20 23  51.5  -3.5  0.4     171.5    -5   2  1  11867  23 54 30
23 56 30  ---          10 22 24  51.4  -3.8  0.4     170.8   115   F  1  13467

23 56 30  M81          10 22 24  51.4  -3.8  0.4     170.9    -5   2  1  13467  23 56 30
23 57 40  ---          10 23 34  51.4  -3.9  0.5     170.5    65   F  1  14400

23 57 40  SN1993J      10 23 34  51.4  -4.0  0.5     170.4    -5   2  1  14400  23 57 40
23 59 40  ---          10 25 34  51.4  -4.3  0.5     169.7   115   F  1  16000

 --- Start: Sat  11 Jun 2005   Day 162 -- Stop: Sun  12 Jun 2005   Day 163 ---

23 59 40  M81          10 25 34  51.4  -4.2  0.5     169.8    -5   2  1  16000  23 59 40
00 01 40  ---          10 27 34  51.3  -4.5  0.5     169.1   115   F  1  17600

00 02 20  M81          10 28 15  51.3  -4.6  0.5     168.9    35   2  2  17600  00 02 20
00 04 30  ---          10 30 25  51.3  -4.9  0.6     168.1   130   R  1  15867

00 04 30  SN1993J      10 30 25  51.3  -4.9  0.6     168.1    -5   2  2  15867  00 04 30
00 06 30  ---          10 32 25  51.3  -5.2  0.6     167.4   115   R  1  14267

00 06 30  M81          10 32 25  51.2  -5.2  0.6     167.4    -5   2  2  14267  00 06 30
00 07 40  ---          10 33 35  51.2  -5.4  0.6     167.0    65   R  1  13333
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

00 07 40  SN1993J      10 33 35  51.3  -5.4  0.6     167.0    -5   2  2  13333  00 07 40
00 09 40  ---          10 35 36  51.2  -5.7  0.7     166.3   115   R  1  11733

00 09 40  M81          10 35 36  51.2  -5.6  0.7     166.3    -5   2  2  11733  00 09 40
00 10 50  ---          10 36 46  51.1  -5.8  0.7     165.9    65   R  1  10800

00 10 50  SN1993J      10 36 46  51.2  -5.8  0.7     165.9    -5   2  2  10800  00 10 50
00 12 50  ---          10 38 46  51.1  -6.1  0.7     165.2   115   R  1   9200

00 12 50  M81          10 38 46  51.1  -6.1  0.7     165.3    -5   2  2   9200  00 12 50
00 14 00  ---          10 39 56  51.1  -6.2  0.7     164.9    65   R  1   8267

00 14 00  SN1993J      10 39 56  51.1  -6.3  0.7     164.8    -5   2  2   8267  00 14 00
00 16 00  ---          10 41 57  51.1  -6.5  0.8     164.1   115   R  1   6667

00 16 00  M81          10 41 57  51.0  -6.5  0.8     164.2    -5   2  2   6667  00 16 00
00 17 10  ---          10 43 07  51.0  -6.7  0.8     163.8    65   R  1   5733

00 17 10  SN1993J      10 43 07  51.0  -6.7  0.8     163.7    -5   2  2   5733  00 17 10
00 19 10  ---          10 45 07  51.0  -7.0  0.8     163.0   115   R  1   4133

00 19 10  M81          10 45 07  50.9  -6.9  0.8     163.1    -5   2  2   4133  00 19 10
00 20 20  ---          10 46 17  50.9  -7.1  0.8     162.7    65   R  1   3200

00 20 20  SN1993J      10 46 17  51.0  -7.1  0.8     162.6    -5   2  2   3200  00 20 20
00 22 20  ---          10 48 18  50.9  -7.4  0.9     162.0   115   R  1   1600

00 22 20  M81          10 48 18  50.9  -7.4  0.9     162.0    -5   2  2   1600  00 22 20
00 24 20  ---          10 50 18  50.8  -7.6  0.9     161.4   115   R  1      0

00 25 00  M81          10 50 58  50.8  -7.7  0.9     161.1    35   2  3      0  00 25 00
00 27 10  ---          10 53 09  50.7  -8.0  1.0     160.4   130   F  1   1733

00 27 10  SN1993J      10 53 09  50.8  -8.1  1.0     160.3    -5   2  3   1733  00 27 10
00 29 10  ---          10 55 09  50.7  -8.3  1.0     159.7   115   F  1   3333

00 29 10  M81          10 55 09  50.7  -8.3  1.0     159.7    -5   2  3   3333  00 29 10
00 30 20  ---          10 56 19  50.6  -8.4  1.0     159.3    65   F  1   4267

00 30 20  SN1993J      10 56 19  50.7  -8.5  1.0     159.3    -5   2  3   4267  00 30 20
00 32 20  ---          10 58 19  50.6  -8.7  1.0     158.6   115   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

00 32 20  M81          10 58 19  50.6  -8.7  1.0     158.7    -5   2  3   5867  00 32 20
00 33 30  ---          10 59 30  50.5  -8.9  1.1     158.3    65   F  1   6800

00 33 30  SN1993J      10 59 30  50.6  -8.9  1.1     158.2    -5   2  3   6800  00 33 30
00 35 30  ---          11 01 30  50.5  -9.2  1.1     157.5   115   F  1   8400

00 35 30  M81          11 01 30  50.5  -9.1  1.1     157.6    -5   2  3   8400  00 35 30
00 36 40  ---          11 02 40  50.4  -9.3  1.1     157.2    65   F  1   9333

00 36 40  SN1993J      11 02 40  50.4  -9.3  1.1     157.1    -5   2  3   9333  00 36 40
00 38 40  ---          11 04 40  50.4  -9.6  1.1     156.5   115   F  1  10933

00 38 40  M81          11 04 40  50.3  -9.5  1.1     156.5    -5   2  3  10933  00 38 40
00 39 50  ---          11 05 51  50.3  -9.7  1.2     156.2    65   F  1  11867

00 39 50  SN1993J      11 05 51  50.3  -9.7  1.2     156.1    -5   2  3  11867  00 39 50
00 41 50  ---          11 07 51  50.3 -10.0  1.2     155.4   115   F  1  13467

00 41 50  M81          11 07 51  50.2  -9.9  1.2     155.5    -5   2  3  13467  00 41 50
00 43 00  ---          11 09 01  50.2 -10.1  1.2     155.1    65   F  1  14400

00 43 00  SN1993J      11 09 01  50.2 -10.1  1.2     155.0    -5   2  3  14400  00 43 00
00 45 00  ---          11 11 02  50.1 -10.4  1.3     154.4   115   F  1  16000

00 45 00  M81          11 11 02  50.1 -10.3  1.3     154.4    -5   2  3  16000  00 45 00
00 47 00  ---          11 13 02  50.0 -10.6  1.3     153.8   115   F  1  17600

00 52 00  OQ208        11 18 03  53.3  82.5 -2.8     -75.9   232   2  4  17600  00 52 00
00 54 10  ---          11 20 13  53.8  82.7 -2.8     -76.0   130   R  1  15867

00 54 10  M81          11 20 13  49.7 -11.5  1.4     151.4   -69   2  4  15867  00 54 10
00 57 20  ---          11 23 24  49.6 -11.9  1.5     150.4   121   R  1  13333

00 57 20  SN1993J      11 23 24  49.6 -11.9  1.5     150.3    -5   2  4  13333  00 57 20
00 59 20  ---          11 25 24  49.5 -12.1  1.5     149.7   115   R  1  11733

00 59 20  M81          11 25 24  49.5 -12.1  1.5     149.7    -5   2  4  11733  00 59 20
01 00 30  ---          11 26 34  49.5 -12.2  1.5     149.4    65   R  1  10800

01 00 30  SN1993J      11 26 34  49.5 -12.3  1.5     149.3    -5   2  4  10800  01 00 30
01 02 30  ---          11 28 34  49.4 -12.5  1.5     148.6   115   R  1   9200
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

01 02 30  M81          11 28 34  49.4 -12.5  1.5     148.7    -5   2  4   9200  01 02 30
01 03 40  ---          11 29 45  49.3 -12.6  1.6     148.3    65   R  1   8267

01 03 40  SN1993J      11 29 45  49.3 -12.7  1.6     148.3    -5   2  4   8267  01 03 40
01 05 40  ---          11 31 45  49.2 -12.9  1.6     147.6   115   R  1   6667

01 05 40  M81          11 31 45  49.2 -12.8  1.6     147.7    -5   2  4   6667  01 05 40
01 06 50  ---          11 32 55  49.2 -13.0  1.6     147.3    65   R  1   5733

01 06 50  SN1993J      11 32 55  49.2 -13.0  1.6     147.2    -5   2  4   5733  01 06 50
01 08 50  ---          11 34 55  49.1 -13.3  1.7     146.6   115   R  1   4133

01 08 50  M81          11 34 55  49.1 -13.2  1.6     146.7    -5   2  4   4133  01 08 50
01 10 00  ---          11 36 06  49.0 -13.3  1.7     146.3    65   R  1   3200

01 10 00  SN1993J      11 36 06  49.0 -13.4  1.7     146.2    -5   2  4   3200  01 10 00
01 12 00  ---          11 38 06  48.9 -13.6  1.7     145.6   115   R  1   1600

01 12 00  M81          11 38 06  48.9 -13.6  1.7     145.7    -5   2  4   1600  01 12 00
01 14 00  ---          11 40 06  48.8 -13.8  1.7     145.0   115   R  1      0

01 14 40  M81          11 40 46  48.8 -13.9  1.7     144.8    35   2  5      0  01 14 40
01 16 50  ---          11 42 57  48.6 -14.1  1.8     144.1   130   F  1   1733

01 16 50  SN1993J      11 42 57  48.7 -14.2  1.8     144.1    -5   2  5   1733  01 16 50
01 18 50  ---          11 44 57  48.6 -14.4  1.8     143.4   115   F  1   3333

01 18 50  M81          11 44 57  48.5 -14.3  1.8     143.5    -5   2  5   3333  01 18 50
01 20 00  ---          11 46 07  48.5 -14.4  1.8     143.1    65   F  1   4267

01 20 00  SN1993J      11 46 07  48.5 -14.5  1.8     143.1    -5   2  5   4267  01 20 00
01 22 00  ---          11 48 08  48.4 -14.7  1.9     142.4   115   F  1   5867

01 22 00  M81          11 48 08  48.4 -14.7  1.9     142.5    -5   2  5   5867  01 22 00
01 23 10  ---          11 49 18  48.3 -14.8  1.9     142.1    65   F  1   6800

01 23 10  SN1993J      11 49 18  48.3 -14.8  1.9     142.1    -5   2  5   6800  01 23 10
01 25 10  ---          11 51 18  48.2 -15.1  1.9     141.4   115   F  1   8400

01 25 10  M81          11 51 18  48.2 -15.0  1.9     141.5    -5   2  5   8400  01 25 10
01 26 20  ---          11 52 28  48.1 -15.1  1.9     141.1    65   F  1   9333
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

01 26 20  SN1993J      11 52 28  48.2 -15.2  1.9     141.1    -5   2  5   9333  01 26 20
01 28 20  ---          11 54 29  48.0 -15.4  2.0     140.4   115   F  1  10933

01 28 20  M81          11 54 29  48.0 -15.3  2.0     140.5    -5   2  5  10933  01 28 20
01 29 30  ---          11 55 39  48.0 -15.4  2.0     140.2    65   F  1  11867

01 29 30  SN1993J      11 55 39  48.0 -15.5  2.0     140.1    -5   2  5  11867  01 29 30
01 31 30  ---          11 57 39  47.9 -15.7  2.0     139.5   115   F  1  13467

01 31 30  M81          11 57 39  47.8 -15.6  2.0     139.5    -5   2  5  13467  01 31 30
01 32 40  ---          11 58 49  47.8 -15.8  2.0     139.2    65   F  1  14400

01 32 40  SN1993J      11 58 49  47.8 -15.8  2.0     139.1    -5   2  5  14400  01 32 40
01 34 40  ---          12 00 50  47.7 -16.0  2.1     138.5   115   F  1  16000

01 34 40  M81          12 00 50  47.6 -16.0  2.1     138.6    -5   2  5  16000  01 34 40
01 36 40  ---          12 02 50  47.5 -16.2  2.1     137.9   115   F  1  17600

01 37 20  M81          12 03 30  47.5 -16.2  2.1     137.7    35   2  6  17600  01 37 20
01 39 30  ---          12 05 40  47.4 -16.4  2.2     137.1   130   R  1  15867

01 39 30  SN1993J      12 05 40  47.4 -16.5  2.2     137.0    -5   2  6  15867  01 39 30
01 41 30  ---          12 07 41  47.3 -16.7  2.2     136.4   115   R  1  14267

01 41 30  M81          12 07 41  47.2 -16.6  2.2     136.5    -5   2  6  14267  01 41 30
01 42 40  ---          12 08 51  47.2 -16.7  2.2     136.1    65   R  1  13333

01 42 40  SN1993J      12 08 51  47.2 -16.8  2.2     136.0    -5   2  6  13333  01 42 40
01 44 40  ---          12 10 51  47.1 -17.0  2.3     135.4   115   R  1  11733

01 44 40  M81          12 10 51  47.0 -16.9  2.2     135.5    -5   2  6  11733  01 44 40
01 45 50  ---          12 12 02  47.0 -17.0  2.3     135.2    65   R  1  10800

01 45 50  SN1993J      12 12 02  47.0 -17.1  2.3     135.1    -5   2  6  10800  01 45 50
01 47 50  ---          12 14 02  46.9 -17.3  2.3     134.5   115   R  1   9200

01 47 50  M81          12 14 02  46.8 -17.2  2.3     134.5    -5   2  6   9200  01 47 50
01 49 00  ---          12 15 12  46.8 -17.3  2.3     134.2    65   R  1   8267

01 49 00  SN1993J      12 15 12  46.8 -17.4  2.3     134.1    -5   2  6   8267  01 49 00
01 51 00  ---          12 17 12  46.7 -17.6  2.4     133.5   115   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

01 51 00  M81          12 17 12  46.6 -17.5  2.4     133.6    -5   2  6   6667  01 51 00
01 52 10  ---          12 18 23  46.6 -17.6  2.4     133.2    65   R  1   5733

01 52 10  SN1993J      12 18 23  46.6 -17.7  2.4     133.2    -5   2  6   5733  01 52 10
01 54 10  ---          12 20 23  46.4 -17.9  2.4     132.6   115   R  1   4133

01 54 10  M81          12 20 23  46.4 -17.8  2.4     132.7    -5   2  6   4133  01 54 10
01 55 20  ---          12 21 33  46.3 -17.9  2.4     132.3    65   R  1   3200

01 55 20  SN1993J      12 21 33  46.4 -18.0  2.4     132.2    -5   2  6   3200  01 55 20
01 57 20  ---          12 23 33  46.2 -18.1  2.5     131.6   115   R  1   1600

01 57 20  M81          12 23 33  46.2 -18.1  2.5     131.7    -5   2  6   1600  01 57 20
01 59 20  ---          12 25 34  46.1 -18.2  2.5     131.1   115   R  1      0

02 00 00  M81          12 26 14  46.0 -18.3  2.5     130.9    35   2  7      0  02 00 00
02 02 10  ---          12 28 24  45.9 -18.5  2.5     130.3   130   F  1   1733

02 02 10  SN1993J      12 28 24  45.9 -18.5  2.5     130.2    -5   2  7   1733  02 02 10
02 04 10  ---          12 30 25  45.8 -18.7  2.6     129.6   115   F  1   3333

02 04 10  M81          12 30 25  45.8 -18.7  2.6     129.7    -5   2  7   3333  02 04 10
02 05 20  ---          12 31 35  45.7 -18.7  2.6     129.4    65   F  1   4267

02 05 20  SN1993J      12 31 35  45.7 -18.8  2.6     129.3    -5   2  7   4267  02 05 20
02 07 20  ---          12 33 35  45.6 -19.0  2.6     128.7   115   F  1   5867

02 07 20  M81          12 33 35  45.5 -18.9  2.6     128.8    -5   2  7   5867  02 07 20
02 08 30  ---          12 34 45  45.5 -19.0  2.6     128.4    65   F  1   6800

02 08 30  SN1993J      12 34 45  45.5 -19.1  2.6     128.4    -5   2  7   6800  02 08 30
02 10 30  ---          12 36 46  45.3 -19.2  2.7     127.8   115   F  1   8400

02 10 30  M81          12 36 46  45.3 -19.2  2.7     127.9    -5   2  7   8400  02 10 30
02 11 40  ---          12 37 56  45.2 -19.2  2.7     127.5    65   F  1   9333

02 11 40  SN1993J      12 37 56  45.2 -19.3  2.7     127.4    -5   2  7   9333  02 11 40
02 13 40  ---          12 39 56  45.1 -19.5  2.7     126.9   115   F  1  10933

02 13 40  M81          12 39 56  45.1 -19.4  2.7     126.9    -5   2  7  10933  02 13 40
02 14 50  ---          12 41 06  45.0 -19.5  2.8     126.6    65   F  1  11867
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

02 14 50  SN1993J      12 41 06  45.0 -19.6  2.8     126.5    -5   2  7  11867  02 14 50
02 16 50  ---          12 43 07  44.9 -19.7  2.8     126.0   115   F  1  13467

02 16 50  M81          12 43 07  44.9 -19.6  2.8     126.0    -5   2  7  13467  02 16 50
02 18 00  ---          12 44 17  44.8 -19.7  2.8     125.7    65   F  1  14400

02 18 00  SN1993J      12 44 17  44.8 -19.8  2.8     125.6    -5   2  7  14400  02 18 00
02 20 00  ---          12 46 17  44.6 -19.9  2.8     125.0   115   F  1  16000

02 20 00  M81          12 46 17  44.6 -19.9  2.8     125.1    -5   2  7  16000  02 20 00
02 22 00  ---          12 48 17  44.5 -20.0  2.9     124.6   115   F  1  17600

02 22 40  M81          12 48 58  44.4 -20.1  2.9     124.4    35   2  8  17600  02 22 40
02 24 50  ---          12 51 08  44.3 -20.2  2.9     123.8   130   R  1  15867

02 24 50  SN1993J      12 51 08  44.3 -20.3  2.9     123.7    -5   2  8  15867  02 24 50
02 26 50  ---          12 53 08  44.1 -20.4  3.0     123.1   115   R  1  14267

02 26 50  M81          12 53 08  44.1 -20.4  3.0     123.2    -5   2  8  14267  02 26 50
02 28 00  ---          12 54 18  44.0 -20.4  3.0     122.9    65   R  1  13333

02 28 00  SN1993J      12 54 18  44.0 -20.5  3.0     122.8    -5   2  8  13333  02 28 00
02 30 00  ---          12 56 19  43.9 -20.6  3.0     122.2   115   R  1  11733

02 30 00  M81          12 56 19  43.9 -20.6  3.0     122.3    -5   2  8  11733  02 30 00
02 31 10  ---          12 57 29  43.8 -20.6  3.0     122.0    65   R  1  10800

02 31 10  SN1993J      12 57 29  43.8 -20.7  3.0     121.9    -5   2  8  10800  02 31 10
02 33 10  ---          12 59 29  43.7 -20.8  3.1     121.3   115   R  1   9200

02 33 10  M81          12 59 29  43.6 -20.8  3.1     121.4    -5   2  8   9200  02 33 10
02 34 20  ---          13 00 39  43.5 -20.9  3.1     121.1    65   R  1   8267

02 34 20  SN1993J      13 00 39  43.6 -20.9  3.1     121.0    -5   2  8   8267  02 34 20
02 36 20  ---          13 02 40  43.4 -21.0  3.1     120.5   115   R  1   6667

02 36 20  M81          13 02 40  43.4 -21.0  3.1     120.5    -5   2  8   6667  02 36 20
02 37 30  ---          13 03 50  43.3 -21.1  3.1     120.2    65   R  1   5733

02 37 30  SN1993J      13 03 50  43.3 -21.1  3.1     120.1    -5   2  8   5733  02 37 30
02 39 30  ---          13 05 50  43.2 -21.2  3.2     119.6   115   R  1   4133
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

02 39 30  M81          13 05 50  43.1 -21.2  3.2     119.7    -5   2  8   4133  02 39 30
02 40 40  ---          13 07 01  43.1 -21.2  3.2     119.3    65   R  1   3200

02 40 40  SN1993J      13 07 01  43.1 -21.3  3.2     119.3    -5   2  8   3200  02 40 40
02 42 40  ---          13 09 01  42.9 -21.4  3.2     118.7   115   R  1   1600

02 42 40  M81          13 09 01  42.9 -21.4  3.2     118.8    -5   2  8   1600  02 42 40
02 44 40  ---          13 11 01  42.7 -21.5  3.3     118.2   115   R  1      0

02 54 40  0954+658     13 21 03  43.7 -26.2  3.4     113.4   591   2  9      0  02 54 40
02 57 40  ---          13 24 03  43.4 -26.4  3.4     112.6   180   F  1   2400

02 57 40  M81          13 24 03  41.7 -22.2  3.5     114.7    -9   2  9   2400  02 57 40
03 00 00  ---          13 26 24  41.5 -22.3  3.5     114.1   131   F  1   4267

03 00 00  SN1993J      13 26 24  41.5 -22.4  3.5     114.0    -5   2  9   4267  03 00 00
03 02 00  ---          13 28 24  41.4 -22.5  3.5     113.5   115   F  1   5867

03 02 00  M81          13 28 24  41.3 -22.4  3.5     113.6    -5   2  9   5867  03 02 00
03 03 10  ---          13 29 34  41.2 -22.4  3.6     113.3    65   F  1   6800

03 03 10  SN1993J      13 29 34  41.3 -22.5  3.6     113.2    -5   2  9   6800  03 03 10
03 05 10  ---          13 31 35  41.1 -22.6  3.6     112.7   115   F  1   8400

03 05 10  M81          13 31 35  41.1 -22.5  3.6     112.7    -5   2  9   8400  03 05 10
03 06 20  ---          13 32 45  41.0 -22.6  3.6     112.4    65   F  1   9333

03 06 20  SN1993J      13 32 45  41.0 -22.7  3.6     112.3    -5   2  9   9333  03 06 20
03 08 20  ---          13 34 45  40.8 -22.7  3.6     111.8   115   F  1  10933

03 08 20  M81          13 34 45  40.8 -22.7  3.6     111.9    -5   2  9  10933  03 08 20
03 09 30  ---          13 35 55  40.7 -22.7  3.7     111.6    65   F  1  11867

03 09 30  SN1993J      13 35 55  40.7 -22.8  3.7     111.5    -5   2  9  11867  03 09 30
03 11 30  ---          13 37 56  40.6 -22.9  3.7     111.0   115   F  1  13467

03 11 30  M81          13 37 56  40.6 -22.8  3.7     111.1    -5   2  9  13467  03 11 30
03 12 40  ---          13 39 06  40.5 -22.9  3.7     110.8    65   F  1  14400

03 12 40  SN1993J      13 39 06  40.5 -22.9  3.7     110.7    -5   2  9  14400  03 12 40
03 14 40  ---          13 41 06  40.3 -23.0  3.8     110.2   115   F  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

03 14 40  M81          13 41 06  40.3 -23.0  3.8     110.2    -5   2  9  16000  03 14 40
03 16 40  ---          13 43 06  40.1 -23.0  3.8     109.7   115   F  1  17600

03 17 20  M81          13 43 47  40.1 -23.1  3.8     109.5    35   2 10  17600  03 17 20
03 19 30  ---          13 45 57  39.9 -23.1  3.8     109.0   130   R  1  15867

03 19 30  SN1993J      13 45 57  39.9 -23.2  3.8     108.9    -5   2 10  15867  03 19 30
03 21 30  ---          13 47 57  39.7 -23.3  3.9     108.4   115   R  1  14267

03 21 30  M81          13 47 57  39.7 -23.2  3.9     108.5    -5   2 10  14267  03 21 30
03 22 40  ---          13 49 07  39.6 -23.3  3.9     108.2    65   R  1  13333

03 22 40  SN1993J      13 49 07  39.6 -23.3  3.9     108.1    -5   2 10  13333  03 22 40
03 24 40  ---          13 51 08  39.4 -23.4  3.9     107.6   115   R  1  11733

03 24 40  M81          13 51 08  39.4 -23.3  3.9     107.7    -5   2 10  11733  03 24 40
03 25 50  ---          13 52 18  39.3 -23.4  3.9     107.4    65   R  1  10800

03 25 50  SN1993J      13 52 18  39.3 -23.4  3.9     107.3    -5   2 10  10800  03 25 50
03 27 50  ---          13 54 18  39.2 -23.5  4.0     106.8   115   R  1   9200

03 27 50  M81          13 54 18  39.2 -23.4  4.0     106.8    -5   2 10   9200  03 27 50
03 29 00  ---          13 55 28  39.1 -23.5  4.0     106.5    65   R  1   8267

03 29 00  SN1993J      13 55 28  39.1 -23.5  4.0     106.5    -5   2 10   8267  03 29 00
03 31 00  ---          13 57 29  38.9 -23.6  4.0     106.0   115   R  1   6667

03 31 00  M81          13 57 29  38.9 -23.5  4.0     106.0    -5   2 10   6667  03 31 00
03 32 10  ---          13 58 39  38.8 -23.6  4.0     105.7    65   R  1   5733

03 32 10  SN1993J      13 58 39  38.8 -23.6  4.0     105.7    -5   2 10   5733  03 32 10
03 34 10  ---          14 00 39  38.6 -23.7  4.1     105.2   115   R  1   4133

03 34 10  M81          14 00 39  38.6 -23.6  4.1     105.2    -5   2 10   4133  03 34 10
03 35 20  ---          14 01 50  38.5 -23.7  4.1     104.9    65   R  1   3200

03 35 20  SN1993J      14 01 50  38.5 -23.7  4.1     104.9    -5   2 10   3200  03 35 20
03 37 20  ---          14 03 50  38.4 -23.8  4.1     104.4   115   R  1   1600

03 37 20  M81          14 03 50  38.4 -23.7  4.1     104.4    -5   2 10   1600  03 37 20
03 39 20  ---          14 05 50  38.2 -23.8  4.2     103.9   115   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

03 44 20  OQ208        14 10 51  87.7 199.7  0.1      19.2   145   2 11      0  03 44 20
03 46 30  ---          14 13 01  87.5 209.9  0.1      29.2   130   F  1   1733

03 46 30  M81          14 13 01  37.6 336.0  4.3     102.1  -106   2 11   1733  03 46 30
03 49 40  ---          14 16 12  37.3 336.0  4.3     101.4    84   F  1   4267

03 49 40  SN1993J      14 16 12  37.3 335.9  4.3     101.3    -5   2 11   4267  03 49 40
03 51 40  ---          14 18 12  37.1 335.9  4.4     100.8   115   F  1   5867

03 51 40  M81          14 18 12  37.1 335.9  4.4     100.9    -5   2 11   5867  03 51 40
03 52 50  ---          14 19 22  37.0 335.9  4.4     100.6    65   F  1   6800

03 52 50  SN1993J      14 19 22  37.0 335.8  4.4     100.5    -5   2 11   6800  03 52 50
03 54 50  ---          14 21 23  36.8 335.8  4.4     100.0   115   F  1   8400

03 54 50  M81          14 21 23  36.8 335.8  4.4     100.1    -5   2 11   8400  03 54 50
03 56 00  ---          14 22 33  36.7 335.8  4.4      99.8    65   F  1   9333

03 56 00  SN1993J      14 22 33  36.7 335.8  4.4      99.7    -5   2 11   9333  03 56 00
03 58 00  ---          14 24 33  36.5 335.7  4.5      99.2   115   F  1  10933

03 58 00  M81          14 24 33  36.5 335.8  4.5      99.3    -5   2 11  10933  03 58 00
03 59 10  ---          14 25 43  36.4 335.8  4.5      99.0    65   F  1  11867

03 59 10  SN1993J      14 25 43  36.4 335.7  4.5      99.0    -5   2 11  11867  03 59 10
04 01 10  ---          14 27 44  36.3 335.7  4.5      98.5   115   F  1  13467

04 01 10  M81          14 27 44  36.3 335.7  4.5      98.5    -5   2 11  13467  04 01 10
04 02 20  ---          14 28 54  36.2 335.7  4.5      98.2    65   F  1  14400

04 02 20  SN1993J      14 28 54  36.2 335.7  4.6      98.2    -5   2 11  14400  04 02 20
04 04 20  ---          14 30 54  36.0 335.6  4.6      97.7   115   F  1  16000

04 04 20  M81          14 30 54  36.0 335.7  4.6      97.8    -5   2 11  16000  04 04 20
04 06 20  ---          14 32 55  35.8 335.7  4.6      97.3   115   F  1  17600

04 07 00  M81          14 33 35  35.7 335.6  4.6      97.1    35   2 12  17600  04 07 00
04 09 10  ---          14 35 45  35.5 335.6  4.7      96.6   130   R  1  15867

04 09 10  SN1993J      14 35 45  35.5 335.6  4.7      96.5    -5   2 12  15867  04 09 10
04 11 10  ---          14 37 45  35.4 335.5  4.7      96.0   115   R  1  14267
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

04 11 10  M81          14 37 45  35.4 335.6  4.7      96.1    -5   2 12  14267  04 11 10
04 12 20  ---          14 38 56  35.3 335.6  4.7      95.8    65   R  1  13333

04 12 20  SN1993J      14 38 56  35.3 335.5  4.7      95.8    -5   2 12  13333  04 12 20
04 14 20  ---          14 40 56  35.1 335.5  4.8      95.3   115   R  1  11733

04 14 20  M81          14 40 56  35.1 335.6  4.7      95.3    -5   2 12  11733  04 14 20
04 15 30  ---          14 42 06  35.0 335.5  4.8      95.1    65   R  1  10800

04 15 30  SN1993J      14 42 06  35.0 335.5  4.8      95.0    -5   2 12  10800  04 15 30
04 17 30  ---          14 44 06  34.8 335.5  4.8      94.5   115   R  1   9200

04 17 30  M81          14 44 06  34.8 335.5  4.8      94.6    -5   2 12   9200  04 17 30
04 18 40  ---          14 45 17  34.7 335.5  4.8      94.3    65   R  1   8267

04 18 40  SN1993J      14 45 17  34.7 335.5  4.8      94.2    -5   2 12   8267  04 18 40
04 20 40  ---          14 47 17  34.5 335.4  4.9      93.8   115   R  1   6667

04 20 40  M81          14 47 17  34.5 335.5  4.9      93.8    -5   2 12   6667  04 20 40
04 21 50  ---          14 48 27  34.4 335.5  4.9      93.6    65   R  1   5733

04 21 50  SN1993J      14 48 27  34.4 335.4  4.9      93.5    -5   2 12   5733  04 21 50
04 23 50  ---          14 50 27  34.2 335.4  4.9      93.0   115   R  1   4133

04 23 50  M81          14 50 27  34.2 335.5  4.9      93.1    -5   2 12   4133  04 23 50
04 25 00  ---          14 51 38  34.1 335.5  4.9      92.8    65   R  1   3200

04 25 00  SN1993J      14 51 38  34.1 335.4  4.9      92.7    -5   2 12   3200  04 25 00
04 27 00  ---          14 53 38  33.9 335.4  5.0      92.3   115   R  1   1600

04 27 00  M81          14 53 38  34.0 335.5  5.0      92.3    -5   2 12   1600  04 27 00
04 29 00  ---          14 55 38  33.8 335.5  5.0      91.9   115   R  1      0

04 29 40  M81          14 56 18  33.7 335.5  5.0      91.7    35   2 13      0  04 29 40
04 31 50  ---          14 58 29  33.5 335.4  5.0      91.2   130   F  1   1733

04 31 50  SN1993J      14 58 29  33.5 335.4  5.0      91.1    -5   2 13   1733  04 31 50
04 33 50  ---          15 00 29  33.3 335.4  5.1      90.7   115   F  1   3333

04 33 50  M81          15 00 29  33.3 335.4  5.1      90.7    -5   2 13   3333  04 33 50
04 35 00  ---          15 01 39  33.2 335.4  5.1      90.4    65   F  1   4267
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

04 35 00  SN1993J      15 01 39  33.2 335.4  5.1      90.4    -5   2 13   4267  04 35 00
04 37 00  ---          15 03 40  33.0 335.4  5.1      89.9   115   F  1   5867

04 37 00  M81          15 03 40  33.1 335.4  5.1      90.0    -5   2 13   5867  04 37 00
04 38 10  ---          15 04 50  33.0 335.4  5.1      89.7    65   F  1   6800

04 38 10  SN1993J      15 04 50  32.9 335.4  5.1      89.6    -5   2 13   6800  04 38 10
04 40 10  ---          15 06 50  32.8 335.4  5.2      89.2   115   F  1   8400

04 40 10  M81          15 06 50  32.8 335.4  5.2      89.2    -5   2 13   8400  04 40 10
04 41 20  ---          15 08 00  32.7 335.4  5.2      89.0    65   F  1   9333

04 41 20  SN1993J      15 08 00  32.7 335.4  5.2      88.9    -5   2 13   9333  04 41 20
04 43 20  ---          15 10 01  32.5 335.4  5.2      88.4   115   F  1  10933

04 43 20  M81          15 10 01  32.5 335.4  5.2      88.5    -5   2 13  10933  04 43 20
04 44 30  ---          15 11 11  32.4 335.5  5.3      88.2    65   F  1  11867

04 44 30  SN1993J      15 11 11  32.4 335.4  5.3      88.2    -5   2 13  11867  04 44 30
04 46 30  ---          15 13 11  32.2 335.4  5.3      87.7   115   F  1  13467

04 46 30  M81          15 13 11  32.2 335.5  5.3      87.8    -5   2 13  13467  04 46 30
04 47 40  ---          15 14 21  32.1 335.5  5.3      87.5    65   F  1  14400

04 47 40  SN1993J      15 14 21  32.1 335.4  5.3      87.4    -5   2 13  14400  04 47 40
04 49 40  ---          15 16 22  31.9 335.4  5.3      87.0   115   F  1  16000

04 49 40  M81          15 16 22  31.9 335.5  5.3      87.0    -5   2 13  16000  04 49 40
04 51 40  ---          15 18 22  31.7 335.5  5.4      86.6   115   F  1  17600

04 52 20  M81          15 19 02  31.7 335.5  5.4      86.4    35   2 14  17600  04 52 20
04 54 30  ---          15 21 13  31.5 335.5  5.4      85.9   130   R  1  15867

04 54 30  SN1993J      15 21 13  31.5 335.5  5.4      85.9    -5   2 14  15867  04 54 30
04 56 30  ---          15 23 13  31.3 335.5  5.5      85.4   115   R  1  14267

04 56 30  M81          15 23 13  31.3 335.5  5.5      85.5    -5   2 14  14267  04 56 30
04 57 40  ---          15 24 23  31.2 335.5  5.5      85.2    65   R  1  13333

04 57 40  SN1993J      15 24 23  31.2 335.5  5.5      85.1    -5   2 14  13333  04 57 40
04 59 40  ---          15 26 23  31.0 335.5  5.5      84.7   115   R  1  11733
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  12 Jun 2005   Day 163 ---

04 59 40  M81          15 26 23  31.0 335.6  5.5      84.7    -5   2 14  11733  04 59 40
05 00 50  ---          15 27 34  30.9 335.6  5.5      84.5    65   R  1  10800

05 00 50  SN1993J      15 27 34  30.9 335.5  5.5      84.4    -5   2 14  10800  05 00 50
05 02 50  ---          15 29 34  30.7 335.5  5.6      83.9   115   R  1   9200

05 02 50  M81          15 29 34  30.7 335.6  5.6      84.0    -5   2 14   9200  05 02 50
05 04 00  ---          15 30 44  30.6 335.6  5.6      83.7    65   R  1   8267

05 04 00  SN1993J      15 30 44  30.6 335.5  5.6      83.7    -5   2 14   8267  05 04 00
05 06 00  ---          15 32 44  30.4 335.6  5.6      83.2   115   R  1   6667

05 06 00  M81          15 32 44  30.5 335.6  5.6      83.3    -5   2 14   6667  05 06 00
05 07 10  ---          15 33 55  30.4 335.6  5.6      83.0    65   R  1   5733

05 07 10  SN1993J      15 33 55  30.3 335.6  5.6      83.0    -5   2 14   5733  05 07 10
05 09 10  ---          15 35 55  30.2 335.6  5.7      82.5   115   R  1   4133

05 09 10  M81          15 35 55  30.2 335.7  5.7      82.6    -5   2 14   4133  05 09 10
05 10 20  ---          15 37 05  30.1 335.7  5.7      82.3    65   R  1   3200

05 10 20  SN1993J      15 37 05  30.1 335.6  5.7      82.2    -5   2 14   3200  05 10 20
05 12 20  ---          15 39 05  29.9 335.7  5.7      81.8   115   R  1   1600

05 12 20  M81          15 39 05  29.9 335.7  5.7      81.8    -5   2 14   1600  05 12 20
05 14 20  ---          15 41 06  29.7 335.7  5.8      81.4   115   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/sched.2004oct04/setups/v6cm-256-8-2-UL.set
   Matches group v6cm_2 in /usr/local/sched.2004oct04/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4979.49   4979.49   4979.49   4979.49   4995.49   4995.49   4995.49   4995.49
   BBC fr=     879.49    879.49    879.49    879.49    895.49    895.49    895.49    895.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   510   490   510  6490  6510  6490  6510
    PCALFR2=   490   510   490   510  6490  6510  6490  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- 34rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SN1993J           09 51 19.038889   * 09 55 24.774900     09 55 50.512240 
                     69 15 26.46784    * 69 01 13.70300      69 00 03.32321 
                     From catalog imbedded in main SCHED input file.
                        5.367 scan hours,    615.116 baseline hours above horizon.

 * M81               09 51 27.310854   * 09 55 33.173100     09 55 58.925621 
                     69 18 08.14534    * 69 03 55.06200      69 02 44.65485 
                     From catalog imbedded in main SCHED input file.
                        4.578 scan hours,    501.511 baseline hours above horizon.

 * 0954+658          09 54 57.847119   * 09 58 47.244300     09 59 11.346897 
                     65 48 15.53178    * 65 33 54.81100      65 32 43.12403 
                     From catalog imbedded in main SCHED input file.
                        0.250 scan hours,     31.600 baseline hours above horizon.

   J1407+2827        14 04 45.615151   * 14 07 00.394410     14 07 15.984243 
   1404+286          28 41 29.23495    * 28 27 14.68998      28 25 45.80409 
   J1407+28          /usr/local/sched.2004oct04/catalogs/sources.vlba
 * OQ208             ICRF - Ext.1 Source - 1998 IERS Annual Report
                        0.072 scan hours,      7.078 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1993J             60.9
   M81                 60.9
   0954+658            60.6
   OQ208              110.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

