  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
 Exp. Code:  GI004   


Schedule Version:       4.00                                              
Processed by SCHED version:   6.05  June 2006                             

PI:       Hiroshi Imai                                                    

Address:  Department of Physics                                           
          Kagoshima University                                            
          Japan                                                           
          1-21-35 Korimoto, Kagoshima 890-0065                            

Phone:    81-99-285-8085                                                  
EMAIL:    hiroimai@sci.kagoshima-u.ac.jp                                  
Fax:      81-99-285-8085                                                  
Phone during observation: 81-99-285-8085                                  

Observing mode: VLBA/MKIV                                                 

Notes:    P-cal signal should be off.                                     
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

 Next scan frequencies:  1611.69  1611.69  1614.21  1614.21  1618.21  1618.21
                         1622.21  1622.21
 Next BBC frequencies:    788.31   788.31   785.79   785.79   781.79   781.79
                          777.79   777.79
 Next scan bandwidths:      1.00     1.00     4.00     4.00     4.00     4.00
                            4.00     4.00

03 18 00  1830+139     13 34 39  20.2  85.3 -5.0     -62.1     0   1  1      0  03 18 00
03 22 00  ---          13 38 40  21.0  85.8 -4.9     -62.2   240   F  1      4  03 18 01

03 24 00  W43AOH       13 40 40  10.4  98.3 -5.1     -58.4    93   1  1      4  03 24 00
03 39 00  ---          13 55 42  13.6 100.3 -4.9     -57.9   900   F  1     18  03 24 01

03 41 00  1830+139     13 57 43  25.1  88.2 -4.6     -62.4    91   1  1     18  03 41 00
03 45 00  ---          14 01 43  26.0  88.7 -4.5     -62.4   240   F  1     22  03 41 01

03 47 00  W43AOH       14 03 44  15.3 101.4 -4.7     -57.5    93   1  1     22  03 47 00
04 02 00  ---          14 18 46  18.4 103.6 -4.5     -56.8   900   F  1     37  03 47 01

04 02 30  W43AOH       14 19 16  18.5 103.6 -4.5     -56.8    25   1  1     37  04 02 30
04 17 30  ---          14 34 19  21.6 105.9 -4.2     -55.9   900   F  1     51  04 02 31

04 19 30  1830+139     14 36 19  33.4  93.1 -3.9     -62.3    90   1  1     51  04 19 30
04 23 30  ---          14 40 20  34.3  93.7 -3.9     -62.2   240   F  1     55  04 19 31

04 25 30  W43AOH       14 42 20  23.3 107.1 -4.1     -55.4    92   1  1     55  04 25 30
04 40 30  ---          14 57 23  26.4 109.5 -3.8     -54.3   900   F  1     70  04 25 31

04 41 00  W43AOH       14 57 53  26.5 109.5 -3.8     -54.2    25   1  1     70  04 41 00
04 56 00  ---          15 12 55  29.5 112.1 -3.6     -52.9   900   F  1     84  04 41 01

04 57 30  1830+139     15 14 25  41.6  98.6 -3.3     -61.2    60   1  1     84  04 57 30
05 01 30  ---          15 18 26  42.4  99.3 -3.2     -61.1   240   F  1     88  04 57 31

05 03 00  W43AOH       15 19 56  30.9 113.3 -3.5     -52.2    61   1  1     88  05 03 00
05 18 00  ---          15 34 59  33.8 116.1 -3.2     -50.6   900   F  1    103  05 03 01

05 18 30  W43AOH       15 35 29  33.9 116.2 -3.2     -50.6    25   1  1    103  05 18 30
05 33 30  ---          15 50 31  36.8 119.2 -3.0     -48.7   900   F  1    117  05 18 31

05 34 00  W43AOH       15 51 01  36.9 119.3 -3.0     -48.7    25   1  1    117  05 34 00
05 49 00  ---          16 06 04  39.7 122.5 -2.7     -46.6   900   F  1    132  05 34 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

05 50 30  1830+139     16 07 34  52.7 108.3 -2.4     -57.3    58   1  1    132  05 50 30
05 54 30  ---          16 11 35  53.5 109.2 -2.4     -56.9   240   F  1    135  05 50 31

06 00 00  W43AOH       16 17 06  41.6 125.0 -2.5     -44.8   300   1  1    135  06 00 00
06 10 00  ---          16 27 07  43.4 127.5 -2.3     -43.1   600   F  1    145  06 00 01

06 10 30  W43AOH       16 27 37  43.5 127.6 -2.3     -43.0    25   1  1    145  06 10 30
06 20 30  ---          16 37 39  45.1 130.2 -2.2     -41.1   600   F  1    155  06 10 31

06 21 30  1830+139     16 38 39  58.9 116.0 -1.9     -52.8    27   1  1    155  06 21 30
06 24 30  ---          16 41 40  59.5 116.8 -1.9     -52.3   180   F  1    158  06 21 31

06 25 00  J1833+01     16 42 10  50.5 132.7 -1.9     -39.2     6   1  1    158  06 25 00
06 26 00  ---          16 43 10  50.7 133.0 -1.8     -39.0    60   F  1    159  06 25 01

06 26 00  W43AOH       16 43 10  46.0 131.7 -2.1     -40.0   -15   1  1    159  06 26 00
06 28 30  ---          16 45 40  46.4 132.4 -2.0     -39.5   135   F  1    161  06 26 01

06 28 30  J1833+01     16 45 40  51.1 133.8 -1.8     -38.4   -15   1  1    161  06 28 30
06 30 00  ---          16 47 11  51.3 134.3 -1.8     -38.0    75   F  1    163  06 28 31

06 30 00  W43AOH       16 47 11  46.7 132.8 -2.0     -39.2   -15   1  1    163  06 30 00
06 32 30  ---          16 49 41  47.1 133.5 -2.0     -38.6   135   F  1    165  06 30 01

06 32 30  J1833+01     16 49 41  51.7 135.1 -1.7     -37.4   -15   1  1    165  06 32 30
06 34 00  ---          16 51 11  51.9 135.6 -1.7     -37.0    75   F  1    166  06 32 31

06 34 00  W43AOH       16 51 11  47.3 134.0 -1.9     -38.3   -15   1  1    166  06 34 00
06 36 30  ---          16 53 42  47.7 134.7 -1.9     -37.7   135   F  1    169  06 34 01

06 36 30  J1833+01     16 53 42  52.3 136.4 -1.7     -36.4   -15   1  1    169  06 36 30
06 38 00  ---          16 55 12  52.5 136.9 -1.6     -36.0    75   F  1    170  06 36 31

06 38 00  W43AOH       16 55 12  47.9 135.1 -1.9     -37.4   -15   1  1    170  06 38 00
06 40 30  ---          16 57 42  48.3 135.9 -1.8     -36.8   135   F  1    173  06 38 01

06 40 30  J1833+01     16 57 42  52.9 137.7 -1.6     -35.4   -15   1  1    173  06 40 30
06 42 00  ---          16 59 12  53.1 138.2 -1.6     -35.0    75   F  1    174  06 40 31

06 42 00  W43AOH       16 59 12  48.5 136.3 -1.8     -36.5   -15   1  1    174  06 42 00
06 44 30  ---          17 01 43  48.9 137.1 -1.8     -35.9   135   F  1    177  06 42 01

06 44 30  J1833+01     17 01 43  53.5 139.1 -1.5     -34.3   -15   1  1    177  06 44 30
06 46 00  ---          17 03 13  53.7 139.6 -1.5     -33.9    75   F  1    178  06 44 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

06 46 00  W43AOH       17 03 13  49.1 137.6 -1.7     -35.5   -15   1  1    178  06 46 00
06 48 30  ---          17 05 44  49.5 138.4 -1.7     -34.9   135   F  1    180  06 46 01

06 48 30  J1833+01     17 05 44  54.0 140.5 -1.5     -33.2   -15   1  1    180  06 48 30
06 50 00  ---          17 07 14  54.2 141.0 -1.4     -32.8    75   F  1    182  06 48 31

06 50 00  W43AOH       17 07 14  49.7 138.8 -1.7     -34.5   -15   1  1    182  06 50 00
06 52 30  ---          17 09 44  50.0 139.6 -1.6     -33.9   135   F  1    184  06 50 01

06 52 30  J1833+01     17 09 44  54.5 142.0 -1.4     -32.0   -15   1  1    184  06 52 30
06 54 00  ---          17 11 14  54.7 142.5 -1.4     -31.6    75   F  1    186  06 52 31

06 54 00  W43AOH       17 11 14  50.2 140.1 -1.6     -33.5   -15   1  1    186  06 54 00
06 56 30  ---          17 13 45  50.6 140.9 -1.6     -32.8   135   F  1    188  06 54 01

06 56 30  J1833+01     17 13 45  55.1 143.4 -1.3     -30.8   -15   1  1    188  06 56 30
06 58 00  ---          17 15 15  55.3 144.0 -1.3     -30.4    75   F  1    190  06 56 31

06 58 00  W43AOH       17 15 15  50.8 141.4 -1.5     -32.4   -15   1  1    190  06 58 00
07 00 30  ---          17 17 46  51.1 142.3 -1.5     -31.8   135   F  1    192  06 58 01

07 00 30  J1833+01     17 17 46  55.6 145.0 -1.3     -29.6   -15   1  1    192  07 00 30
07 02 00  ---          17 19 16  55.8 145.5 -1.2     -29.1    75   F  1    194  07 00 31

07 02 00  W43AOH       17 19 16  51.3 142.8 -1.5     -31.4   -15   1  1    194  07 02 00
07 04 30  ---          17 21 46  51.6 143.7 -1.4     -30.7   135   F  1    196  07 02 01

07 04 30  J1833+01     17 21 46  56.1 146.5 -1.2     -28.3   -15   1  1    196  07 04 30
07 06 00  ---          17 23 16  56.2 147.1 -1.2     -27.9    75   F  1    197  07 04 31

07 06 30  1830+139     17 23 47  66.9 132.5 -1.2     -40.9     3   1  1    197  07 06 30
07 09 30  ---          17 26 47  67.4 133.9 -1.1     -39.7   180   F  1    200  07 06 31

07 10 00  J1833+01     17 27 17  56.7 148.7 -1.1     -26.5     3   1  1    200  07 10 00
07 11 00  ---          17 28 17  56.8 149.1 -1.1     -26.2    60   F  1    201  07 10 01

07 11 00  W43AOH       17 28 17  52.5 146.0 -1.3     -28.8   -15   1  1    201  07 11 00
07 13 30  ---          17 30 48  52.8 146.9 -1.3     -28.1   135   F  1    204  07 11 01

07 13 30  J1833+01     17 30 48  57.1 150.2 -1.0     -25.3   -15   1  1    204  07 13 30
07 15 00  ---          17 32 18  57.2 150.8 -1.0     -24.8    75   F  1    205  07 13 31

07 15 00  W43AOH       17 32 18  52.9 147.4 -1.3     -27.6   -15   1  1    205  07 15 00
07 17 30  ---          17 34 48  53.2 148.3 -1.2     -26.9   135   F  1    208  07 15 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

07 17 30  J1833+01     17 34 48  57.5 151.9 -1.0     -23.9   -15   1  1    208  07 17 30
07 19 00  ---          17 36 19  57.6 152.5 -1.0     -23.4    75   F  1    209  07 17 31

07 19 00  W43AOH       17 36 19  53.4 148.9 -1.2     -26.4   -15   1  1    209  07 19 00
07 21 30  ---          17 38 49  53.7 149.9 -1.2     -25.6   135   F  1    211  07 19 01

07 21 30  J1833+01     17 38 49  57.9 153.6 -0.9     -22.5   -14   1  1    211  07 21 30
07 23 00  ---          17 40 19  58.0 154.2 -0.9     -22.0    76   F  1    213  07 21 31

07 23 00  W43AOH       17 40 19  53.8 150.4 -1.1     -25.1   -14   1  1    213  07 23 00
07 25 30  ---          17 42 50  54.1 151.4 -1.1     -24.3   136   F  1    215  07 23 01

07 25 30  J1833+01     17 42 50  58.3 155.3 -0.8     -21.0   -14   1  1    215  07 25 30
07 27 00  ---          17 44 20  58.4 156.0 -0.8     -20.5    76   F  1    217  07 25 31

07 27 00  W43AOH       17 44 20  54.2 152.0 -1.1     -23.9   -14   1  1    217  07 27 00
07 29 30  ---          17 46 50  54.5 153.0 -1.0     -23.0   136   F  1    219  07 27 01

07 29 30  J1833+01     17 46 50  58.6 157.1 -0.8     -19.5   -14   1  1    219  07 29 30
07 31 00  ---          17 48 21  58.7 157.8 -0.8     -19.0    76   F  1    221  07 29 31

07 31 00  W43AOH       17 48 21  54.6 153.6 -1.0     -22.5   -14   1  1    221  07 31 00
07 33 30  ---          17 50 51  54.9 154.6 -1.0     -21.7   136   F  1    223  07 31 01

07 33 30  J1833+01     17 50 51  58.9 159.0 -0.7     -18.0   -14   1  1    223  07 33 30
07 35 00  ---          17 52 21  59.0 159.7 -0.7     -17.4    76   F  1    225  07 33 31

07 35 00  W43AOH       17 52 21  55.0 155.2 -0.9     -21.2   -14   1  1    225  07 35 00
07 37 30  ---          17 54 52  55.2 156.2 -0.9     -20.3   136   F  1    227  07 35 01

07 37 30  J1833+01     17 54 52  59.2 160.8 -0.6     -16.4   -14   1  1    227  07 37 30
07 39 00  ---          17 56 22  59.3 161.5 -0.6     -15.8    76   F  1    228  07 37 31

07 39 00  W43AOH       17 56 22  55.4 156.8 -0.9     -19.8   -14   1  1    228  07 39 00
07 41 30  ---          17 58 52  55.6 157.9 -0.8     -18.9   136   F  1    231  07 39 01

07 41 30  J1833+01     17 58 52  59.5 162.7 -0.6     -14.8   -14   1  1    231  07 41 30
07 43 00  ---          18 00 23  59.6 163.5 -0.6     -14.2    76   F  1    232  07 41 31

07 43 00  W43AOH       18 00 23  55.7 158.5 -0.8     -18.4   -14   1  1    232  07 43 00
07 45 30  ---          18 02 53  55.9 159.6 -0.8     -17.5   136   F  1    235  07 43 01

07 45 30  J1833+01     18 02 53  59.7 164.7 -0.5     -13.2   -14   1  1    235  07 45 30
07 47 00  ---          18 04 23  59.8 165.4 -0.5     -12.5    76   F  1    236  07 45 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

07 47 00  W43AOH       18 04 23  56.0 160.2 -0.7     -17.0   -14   1  1    236  07 47 00
07 49 30  ---          18 06 54  56.2 161.3 -0.7     -16.0   136   F  1    239  07 47 01

07 49 30  J1833+01     18 06 54  60.0 166.6 -0.4     -11.5   -14   1  1    239  07 49 30
07 51 00  ---          18 08 24  60.0 167.3 -0.4     -10.9    76   F  1    240  07 49 31

07 51 30  1830+139     18 08 54  72.4 160.2 -0.4     -17.5    -1   1  1    240  07 51 30
07 54 30  ---          18 11 54  72.6 162.5 -0.4     -15.4   179   F  1    243  07 51 31

07 55 00  J1833+01     18 12 24  60.2 169.3 -0.4      -9.2    -1   1  1    243  07 55 00
07 56 00  ---          18 13 25  60.2 169.8 -0.3      -8.7    59   F  1    244  07 55 01

07 56 00  W43AOH       18 13 25  56.6 164.1 -0.6     -13.6   -13   1  1    244  07 56 00
07 58 30  ---          18 15 55  56.7 165.2 -0.5     -12.7   137   F  1    246  07 56 01

07 58 30  J1833+01     18 15 55  60.3 171.1 -0.3      -7.7   -13   1  1    246  07 58 30
08 00 00  ---          18 17 25  60.4 171.8 -0.3      -7.0    77   F  1    248  07 58 31

08 00 00  W43AOH       18 17 25  56.8 165.9 -0.5     -12.1   -13   1  1    248  08 00 00
08 02 30  ---          18 19 56  56.9 167.0 -0.5     -11.1   137   F  1    250  08 00 01

08 02 30  J1833+01     18 19 56  60.5 173.1 -0.2      -5.9   -13   1  1    250  08 02 30
08 04 00  ---          18 21 26  60.5 173.9 -0.2      -5.3    77   F  1    252  08 02 31

08 04 00  W43AOH       18 21 26  57.0 167.7 -0.4     -10.6   -13   1  1    252  08 04 00
08 06 30  ---          18 23 56  57.1 168.8 -0.4      -9.6   137   F  1    254  08 04 01

08 06 30  J1833+01     18 23 56  60.5 175.1 -0.2      -4.2   -13   1  1    254  08 06 30
08 08 00  ---          18 25 27  60.6 175.9 -0.1      -3.5    77   F  1    255  08 06 31

08 08 00  W43AOH       18 25 27  57.2 169.5 -0.4      -9.0   -13   1  1    255  08 08 00
08 10 30  ---          18 27 57  57.3 170.7 -0.3      -8.0   137   F  1    258  08 08 01

08 10 30  J1833+01     18 27 57  60.6 177.2 -0.1      -2.4   -13   1  1    258  08 10 30
08 12 00  ---          18 29 27  60.6 177.9 -0.1      -1.8    77   F  1    259  08 10 31

08 12 00  W43AOH       18 29 27  57.3 171.3 -0.3      -7.4   -13   1  1    259  08 12 00
08 14 30  ---          18 31 58  57.4 172.5 -0.3      -6.4   137   F  1    262  08 12 01

08 14 30  J1833+01     18 31 58  60.6 179.2  0.0      -0.7   -12   1  1    262  08 14 30
08 16 00  ---          18 33 28  60.6 180.0  0.0       0.0    78   F  1    263  08 14 31

08 16 00  W43AOH       18 33 28  57.4 173.2 -0.2      -5.9   -12   1  1    263  08 16 00
08 18 30  ---          18 35 58  57.5 174.4 -0.2      -4.9   138   F  1    266  08 16 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

08 18 30  J1833+01     18 35 58  60.6 181.2  0.0       1.1   -12   1  1    266  08 18 30
08 20 00  ---          18 37 29  60.6 182.0  0.1       1.7    78   F  1    267  08 18 31

08 20 00  W43AOH       18 37 29  57.5 175.1 -0.2      -4.3   -12   1  1    267  08 20 00
08 22 30  ---          18 39 59  57.6 176.2 -0.1      -3.3   138   F  1    269  08 20 01

08 22 30  J1833+01     18 39 59  60.6 183.3  0.1       2.8   -12   1  1    269  08 22 30
08 24 00  ---          18 41 29  60.6 184.0  0.1       3.5    78   F  1    271  08 22 31

08 24 00  W43AOH       18 41 29  57.6 176.9 -0.1      -2.7   -12   1  1    271  08 24 00
08 26 30  ---          18 44 00  57.6 178.1 -0.1      -1.6   138   F  1    273  08 24 01

08 26 30  J1833+01     18 44 00  60.5 185.3  0.2       4.6   -12   1  1    273  08 26 30
08 28 00  ---          18 45 30  60.5 186.1  0.2       5.2    78   F  1    275  08 26 31

08 28 00  W43AOH       18 45 30  57.6 178.8  0.0      -1.0   -12   1  1    275  08 28 00
08 30 30  ---          18 48 00  57.6 180.0  0.0       0.0   138   F  1    277  08 28 01

08 30 30  J1833+01     18 48 00  60.4 187.3  0.2       6.3   -12   1  1    277  08 30 30
08 32 00  ---          18 49 31  60.4 188.1  0.3       7.0    78   F  1    279  08 30 31

08 32 00  W43AOH       18 49 31  57.6 180.7  0.0       0.6   -12   1  1    279  08 32 00
08 34 30  ---          18 52 01  57.6 181.8  0.1       1.6   138   F  1    281  08 32 01

08 34 30  J1833+01     18 52 01  60.3 189.4  0.3       8.0   -11   1  1    281  08 34 30
08 36 00  ---          18 53 31  60.2 190.1  0.3       8.7    79   F  1    283  08 34 31

08 36 30  1830+139     18 54 01  72.6 197.3  0.3      15.3    -1   1  1    283  08 36 30
08 39 30  ---          18 57 02  72.4 199.6  0.4      17.3   179   F  1    285  08 36 31

08 40 00  J1833+01     18 57 32  60.1 192.1  0.4      10.4    -1   1  1    285  08 40 00
08 41 00  ---          18 58 32  60.0 192.6  0.4      10.8    59   F  1    286  08 40 01

08 41 00  W43AOH       18 58 32  57.5 184.9  0.2       4.2   -11   1  1    286  08 41 00
08 43 30  ---          19 01 02  57.5 186.0  0.2       5.2   139   F  1    289  08 41 01

08 43 30  J1833+01     19 01 02  59.9 193.8  0.5      11.9   -11   1  1    289  08 43 30
08 45 00  ---          19 02 33  59.8 194.5  0.5      12.5    79   F  1    290  08 43 31

08 45 00  W43AOH       19 02 33  57.4 186.7  0.2       5.8   -11   1  1    290  08 45 00
08 47 30  ---          19 05 03  57.4 187.9  0.3       6.8   139   F  1    293  08 45 01

08 47 30  J1833+01     19 05 03  59.7 195.8  0.5      13.5   -11   1  1    293  08 47 30
08 49 00  ---          19 06 33  59.6 196.5  0.6      14.1    79   F  1    294  08 47 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

08 49 00  W43AOH       19 06 33  57.3 188.6  0.3       7.4   -11   1  1    294  08 49 00
08 51 30  ---          19 09 04  57.2 189.7  0.3       8.4   139   F  1    297  08 49 01

08 51 30  J1833+01     19 09 04  59.4 197.7  0.6      15.1   -11   1  1    297  08 51 30
08 53 00  ---          19 10 34  59.3 198.4  0.6      15.8    79   F  1    298  08 51 31

08 53 00  W43AOH       19 10 34  57.2 190.4  0.4       8.9   -11   1  1    298  08 53 00
08 55 30  ---          19 13 04  57.1 191.5  0.4       9.9   139   F  1    300  08 53 01

08 55 30  J1833+01     19 13 04  59.2 199.6  0.7      16.8   -11   1  1    300  08 55 30
08 57 00  ---          19 14 35  59.1 200.3  0.7      17.3    79   F  1    302  08 55 31

08 57 00  W43AOH       19 14 35  57.0 192.2  0.4      10.5   -11   1  1    302  08 57 00
08 59 30  ---          19 17 05  56.9 193.3  0.5      11.5   139   F  1    304  08 57 01

08 59 30  J1833+01     19 17 05  58.9 201.4  0.7      18.3   -11   1  1    304  08 59 30
09 01 00  ---          19 18 35  58.7 202.1  0.8      18.9    79   F  1    306  08 59 31

09 01 00  W43AOH       19 18 35  56.8 194.0  0.5      12.0   -11   1  1    306  09 01 00
09 03 30  ---          19 21 06  56.7 195.1  0.5      13.0   139   F  1    308  09 01 01

09 03 30  J1833+01     19 21 06  58.5 203.2  0.8      19.9   -11   1  1    308  09 03 30
09 05 00  ---          19 22 36  58.4 203.9  0.8      20.4    79   F  1    310  09 03 31

09 05 00  W43AOH       19 22 36  56.6 195.8  0.6      13.6   -11   1  1    310  09 05 00
09 07 30  ---          19 25 06  56.4 196.9  0.6      14.5   139   F  1    312  09 05 01

09 07 30  J1833+01     19 25 06  58.2 205.0  0.9      21.4   -11   1  1    312  09 07 30
09 09 00  ---          19 26 37  58.0 205.7  0.9      21.9    79   F  1    314  09 07 31

09 09 00  W43AOH       19 26 37  56.3 197.6  0.6      15.1   -11   1  1    314  09 09 00
09 11 30  ---          19 29 07  56.2 198.6  0.7      16.0   139   F  1    316  09 09 01

09 11 30  J1833+01     19 29 07  57.8 206.8  0.9      22.8   -11   1  1    316  09 11 30
09 13 00  ---          19 30 37  57.7 207.4  1.0      23.4    79   F  1    317  09 11 31

09 13 00  W43AOH       19 30 37  56.1 199.3  0.7      16.5   -11   1  1    317  09 13 00
09 15 30  ---          19 33 08  55.9 200.4  0.8      17.4   139   F  1    320  09 13 01

09 15 30  J1833+01     19 33 08  57.4 208.5  1.0      24.2   -11   1  1    320  09 15 30
09 17 00  ---          19 34 38  57.3 209.1  1.0      24.8    79   F  1    321  09 15 31

09 17 00  W43AOH       19 34 38  55.8 201.0  0.8      18.0   -11   1  1    321  09 17 00
09 19 30  ---          19 37 08  55.6 202.1  0.8      18.9   139   F  1    324  09 17 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

09 19 30  J1833+01     19 37 08  57.0 210.2  1.1      25.6   -11   1  1    324  09 19 30
09 21 00  ---          19 38 39  56.8 210.8  1.1      26.1    79   F  1    325  09 19 31

09 21 00  W43AOH       19 38 39  55.5 202.7  0.8      19.4   -11   1  1    325  09 21 00
09 23 30  ---          19 41 09  55.2 203.7  0.9      20.3   139   F  1    328  09 21 01

09 23 30  J1833+01     19 41 09  56.5 211.8  1.1      27.0   -11   1  1    328  09 23 30
09 25 00  ---          19 42 39  56.4 212.4  1.2      27.5    79   F  1    329  09 23 31

09 25 00  W43AOH       19 42 39  55.1 204.3  0.9      20.8   -11   1  1    329  09 25 00
09 27 30  ---          19 45 10  54.9 205.4  1.0      21.6   139   F  1    331  09 25 01

09 27 30  J1833+01     19 45 10  56.1 213.4  1.2      28.3   -11   1  1    331  09 27 30
09 29 00  ---          19 46 40  55.9 214.0  1.2      28.8    79   F  1    333  09 27 31

09 29 30  1830+139     19 47 10  66.2 229.7  1.2      42.6     3   1  1    333  09 29 30
09 32 30  ---          19 50 10  65.7 231.0  1.3      43.6   180   F  1    336  09 29 31

09 33 00  J1833+01     19 50 41  55.4 215.6  1.3      30.0     3   1  1    336  09 33 00
09 34 00  ---          19 51 41  55.3 215.9  1.3      30.3    60   F  1    337  09 33 01

09 34 00  W43AOH       19 51 41  54.3 207.9  1.1      23.8   -11   1  1    337  09 34 00
09 36 30  ---          19 54 11  54.0 208.9  1.1      24.6   139   F  1    339  09 34 01

09 36 30  J1833+01     19 54 11  55.0 216.9  1.3      31.1   -11   1  1    339  09 36 30
09 38 00  ---          19 55 41  54.8 217.4  1.4      31.5    79   F  1    341  09 36 31

09 38 00  W43AOH       19 55 41  53.8 209.5  1.1      25.1   -11   1  1    341  09 38 00
09 40 30  ---          19 58 12  53.6 210.5  1.2      25.9   139   F  1    343  09 38 01

09 40 30  J1833+01     19 58 12  54.4 218.4  1.4      32.3   -11   1  1    343  09 40 30
09 42 00  ---          19 59 42  54.2 218.9  1.4      32.7    79   F  1    344  09 40 31

09 42 00  W43AOH       19 59 42  53.4 211.0  1.2      26.3   -11   1  1    344  09 42 00
09 44 30  ---          20 02 12  53.1 212.0  1.2      27.1   139   F  1    347  09 42 01

09 44 30  J1833+01     20 02 12  53.9 219.8  1.5      33.4   -11   1  1    347  09 44 30
09 46 00  ---          20 03 43  53.7 220.3  1.5      33.8    79   F  1    348  09 44 31

09 46 00  W43AOH       20 03 43  53.0 212.5  1.3      27.6   -11   1  1    348  09 46 00
09 48 30  ---          20 06 13  52.7 213.4  1.3      28.3   139   F  1    351  09 46 01

09 48 30  J1833+01     20 06 13  53.3 221.2  1.5      34.5   -11   1  1    351  09 48 30
09 50 00  ---          20 07 43  53.1 221.7  1.6      34.9    79   F  1    352  09 48 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

09 50 00  W43AOH       20 07 43  52.5 214.0  1.3      28.8   -11   1  1    352  09 50 00
09 52 30  ---          20 10 14  52.2 214.9  1.4      29.5   139   F  1    355  09 50 01

09 52 30  J1833+01     20 10 14  52.8 222.6  1.6      35.6   -11   1  1    355  09 52 30
09 54 00  ---          20 11 44  52.5 223.1  1.6      36.0    79   F  1    356  09 52 31

09 54 00  W43AOH       20 11 44  52.0 215.4  1.4      29.9   -11   1  1    356  09 54 00
09 56 30  ---          20 14 14  51.7 216.3  1.4      30.6   139   F  1    359  09 54 01

09 56 30  J1833+01     20 14 14  52.2 223.9  1.7      36.6   -11   1  1    359  09 56 30
09 58 00  ---          20 15 45  51.9 224.4  1.7      37.0    79   F  1    360  09 56 31

09 58 00  W43AOH       20 15 45  51.5 216.8  1.5      31.0   -11   1  1    360  09 58 00
10 00 30  ---          20 18 15  51.2 217.6  1.5      31.7   139   F  1    362  09 58 01

10 00 30  J1833+01     20 18 15  51.6 225.2  1.7      37.6   -11   1  1    362  10 00 30
10 02 00  ---          20 19 45  51.3 225.7  1.8      38.0    79   F  1    364  10 00 31

10 02 00  W43AOH       20 19 45  51.0 218.2  1.5      32.1   -11   1  1    364  10 02 00
10 04 30  ---          20 22 16  50.6 219.0  1.6      32.8   139   F  1    366  10 02 01

10 04 30  J1833+01     20 22 16  50.9 226.4  1.8      38.6   -11   1  1    366  10 04 30
10 06 00  ---          20 23 46  50.7 226.9  1.8      38.9    79   F  1    368  10 04 31

10 06 00  W43AOH       20 23 46  50.4 219.5  1.6      33.2   -11   1  1    368  10 06 00
10 08 30  ---          20 26 16  50.1 220.3  1.6      33.8   139   F  1    370  10 06 01

10 08 30  J1833+01     20 26 16  50.3 227.7  1.9      39.5   -11   1  1    370  10 08 30
10 10 00  ---          20 27 47  50.1 228.1  1.9      39.9    79   F  1    372  10 08 31

10 10 00  W43AOH       20 27 47  49.9 220.8  1.7      34.2   -11   1  1    372  10 10 00
10 12 30  ---          20 30 17  49.5 221.6  1.7      34.8   139   F  1    374  10 10 01

10 12 30  J1833+01     20 30 17  49.7 228.9  1.9      40.4   -11   1  1    374  10 12 30
10 14 00  ---          20 31 47  49.4 229.3  2.0      40.7    79   F  1    375  10 12 31

10 14 00  W43AOH       20 31 47  49.3 222.1  1.7      35.2   -11   1  1    375  10 14 00
10 16 30  ---          20 34 18  48.9 222.8  1.8      35.8   139   F  1    378  10 14 01

10 16 30  J1833+01     20 34 18  49.0 230.0  2.0      41.3   -11   1  1    378  10 16 30
10 18 00  ---          20 35 48  48.8 230.5  2.0      41.6    79   F  1    379  10 16 31

10 18 00  W43AOH       20 35 48  48.7 223.3  1.8      36.2   -11   1  1    379  10 18 00
10 20 30  ---          20 38 18  48.3 224.1  1.8      36.8   139   F  1    382  10 18 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

10 20 30  J1833+01     20 38 18  48.3 231.2  2.1      42.1   -11   1  1    382  10 20 30
10 22 00  ---          20 39 49  48.1 231.6  2.1      42.4    79   F  1    383  10 20 31

10 22 30  1830+139     20 40 19  56.4 247.4  2.1      55.0     7   1  1    383  10 22 30
10 25 30  ---          20 43 19  55.8 248.2  2.2      55.4   180   F  1    386  10 22 31

10 26 00  J1833+01     20 43 49  47.4 232.7  2.2      43.2     7   1  1    386  10 26 00
10 27 00  ---          20 44 49  47.2 232.9  2.2      43.4    60   F  1    387  10 26 01

10 27 00  W43AOH       20 44 49  47.3 226.0  1.9      38.2   -11   1  1    387  10 27 00
10 29 30  ---          20 47 20  46.9 226.7  2.0      38.8   139   F  1    389  10 27 01

10 29 30  J1833+01     20 47 20  46.8 233.6  2.2      43.9   -11   1  1    389  10 29 30
10 31 00  ---          20 48 50  46.5 234.0  2.3      44.1    79   F  1    391  10 29 31

10 31 00  W43AOH       20 48 50  46.7 227.1  2.0      39.1   -11   1  1    391  10 31 00
10 33 30  ---          20 51 21  46.3 227.8  2.1      39.6   139   F  1    393  10 31 01

10 33 30  J1833+01     20 51 21  46.1 234.7  2.3      44.6   -11   1  1    393  10 33 30
10 35 00  ---          20 52 51  45.8 235.0  2.3      44.9    79   F  1    395  10 33 31

10 35 00  W43AOH       20 52 51  46.1 228.3  2.1      40.0   -11   1  1    395  10 35 00
10 37 30  ---          20 55 21  45.7 228.9  2.1      40.5   139   F  1    397  10 35 01

10 37 30  J1833+01     20 55 21  45.4 235.7  2.4      45.3   -10   1  1    397  10 37 30
10 39 00  ---          20 56 51  45.1 236.0  2.4      45.6    80   F  1    399  10 37 31

10 39 00  W43AOH       20 56 51  45.4 229.3  2.1      40.8   -10   1  1    399  10 39 00
10 41 30  ---          20 59 22  45.0 230.0  2.2      41.3   140   F  1    401  10 39 01

10 41 30  J1833+01     20 59 22  44.7 236.7  2.4      46.0   -10   1  1    401  10 41 30
10 43 00  ---          21 00 52  44.4 237.0  2.5      46.2    80   F  1    403  10 41 31

10 43 00  W43AOH       21 00 52  44.8 230.4  2.2      41.6   -10   1  1    403  10 43 00
10 45 30  ---          21 03 22  44.3 231.1  2.3      42.0   140   F  1    405  10 43 01

10 45 30  J1833+01     21 03 22  44.0 237.6  2.5      46.6   -10   1  1    405  10 45 30
10 47 00  ---          21 04 53  43.7 238.0  2.5      46.9    80   F  1    406  10 45 31

10 47 00  W43AOH       21 04 53  44.1 231.5  2.3      42.3   -10   1  1    406  10 47 00
10 49 30  ---          21 07 23  43.7 232.1  2.3      42.8   140   F  1    409  10 47 01

10 49 30  J1833+01     21 07 23  43.2 238.6  2.6      47.3   -10   1  1    409  10 49 30
10 51 00  ---          21 08 53  42.9 238.9  2.6      47.5    80   F  1    410  10 49 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

10 51 00  W43AOH       21 08 53  43.4 232.5  2.3      43.1   -10   1  1    410  10 51 00
10 53 30  ---          21 11 24  43.0 233.1  2.4      43.5   140   F  1    413  10 51 01

10 53 30  J1833+01     21 11 24  42.5 239.5  2.6      47.9   -10   1  1    413  10 53 30
10 55 00  ---          21 12 54  42.2 239.8  2.7      48.1    80   F  1    414  10 53 31

10 55 00  W43AOH       21 12 54  42.7 233.5  2.4      43.8   -10   1  1    414  10 55 00
10 57 30  ---          21 15 24  42.3 234.1  2.5      44.2   140   F  1    417  10 55 01

10 57 30  J1833+01     21 15 24  41.7 240.4  2.7      48.4   -10   1  1    417  10 57 30
10 59 00  ---          21 16 55  41.5 240.7  2.7      48.7    80   F  1    418  10 57 31

10 59 00  W43AOH       21 16 55  42.0 234.4  2.5      44.5   -10   1  1    418  10 59 00
11 01 30  ---          21 19 25  41.6 235.0  2.5      44.9   140   F  1    420  10 59 01

11 01 30  J1833+01     21 19 25  41.0 241.3  2.8      49.0   -10   1  1    420  11 01 30
11 03 00  ---          21 20 55  40.7 241.6  2.8      49.2    80   F  1    422  11 01 31

11 03 00  W43AOH       21 20 55  41.3 235.4  2.5      45.1   -10   1  1    422  11 03 00
11 05 30  ---          21 23 26  40.9 236.0  2.6      45.5   140   F  1    424  11 03 01

11 05 30  J1833+01     21 23 26  40.2 242.1  2.8      49.5   -10   1  1    424  11 05 30
11 07 00  ---          21 24 56  39.9 242.5  2.9      49.7    80   F  1    426  11 05 31

11 07 00  W43AOH       21 24 56  40.6 236.3  2.6      45.8   -10   1  1    426  11 07 00
11 09 30  ---          21 27 26  40.2 236.9  2.7      46.2   140   F  1    428  11 07 01

11 09 30  J1833+01     21 27 26  39.5 243.0  2.9      50.1   -10   1  1    428  11 09 30
11 11 00  ---          21 28 57  39.2 243.3  2.9      50.3    80   F  1    430  11 09 31

11 11 00  W43AOH       21 28 57  39.9 237.2  2.7      46.4   -10   1  1    430  11 11 00
11 13 30  ---          21 31 27  39.4 237.8  2.7      46.8   140   F  1    432  11 11 01

11 13 30  J1833+01     21 31 27  38.7 243.8  3.0      50.6   -10   1  1    432  11 13 30
11 15 00  ---          21 32 57  38.4 244.1  3.0      50.7    80   F  1    434  11 13 31

11 16 30  2145+067     21 34 28  66.1 171.4 -0.2      -7.5    29   1  1    434  11 16 30
11 26 30  ---          21 44 29  66.3 177.5 -0.1      -2.1   600   F  1    443  11 16 31

11 27 00  2145+067     21 44 59  66.3 177.8 -0.1      -1.9    25   1  1    443  11 27 00
11 37 00  ---          21 55 01  66.3 184.0  0.1       3.5   600   F  1    453  11 27 01

11 38 30  W43AOH       21 56 31  34.7 243.0  3.1      50.1    21   1  1    453  11 38 30
11 53 30  ---          22 11 34  31.8 245.8  3.4      51.8   900   F  1    467  11 38 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sun  10 Jun 2007   Day 161 ---

11 54 00  W43AOH       22 12 04  31.7 245.9  3.4      51.8    25   1  1    467  11 54 00
12 09 00  ---          22 27 06  28.7 248.6  3.7      53.3   900   F  1    482  11 54 01

12 09 30  1830+139     22 27 36  33.9 266.6  3.9      62.3    12   1  1    482  12 09 30
12 13 30  ---          22 31 37  33.0 267.1  4.0      62.3   240   F  1    486  12 09 31

12 14 00  W43AOH       22 32 07  27.7 249.4  3.7      53.7    12   1  1    486  12 14 00
12 29 00  ---          22 47 09  24.7 251.9  4.0      54.9   900   F  1    500  12 14 01

12 29 30  W43AOH       22 47 40  24.6 252.0  4.0      54.9    25   1  1    500  12 29 30
12 44 30  ---          23 02 42  21.5 254.3  4.2      56.0   900   F  1    515  12 29 31

12 45 30  1830+139     23 03 42  26.1 271.3  4.5      62.4    43   1  1    515  12 45 30
12 49 30  ---          23 07 43  25.3 271.8  4.6      62.4   240   F  1    519  12 45 31

12 50 00  1830+139     23 08 13  25.2 271.8  4.6      62.4    25   1  1    519  12 50 00
12 54 00  ---          23 12 14  24.3 272.3  4.7      62.4   240   F  1    523  12 50 01

12 54 30  W43AOH       23 12 44  19.4 255.8  4.4      56.5    13   1  1    523  12 54 30
13 09 30  ---          23 27 46  16.2 257.9  4.7      57.3   900   F  1    537  12 54 31

13 10 00  W43AOH       23 28 16  16.1 258.0  4.7      57.3    25   1  1    537  13 10 00
13 25 00  ---          23 43 19  13.0 260.1  4.9      58.0   900   F  1    552  13 10 01

13 25 30  1830+139     23 43 49  17.5 276.1  5.2      61.8    13   1  1    552  13 25 30
13 29 30  ---          23 47 49  16.7 276.6  5.2      61.7   240   F  1    555  13 25 31


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gw43a-oh.set
   Matches group v20cm_2 in /usr/local/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:   12         Station: VLBA_FD           Total bit rate:  128
   Format: VLBA1:2           Bits per sample: 2         Sample rate:  8.000
   Number of channels:  8                               Speedup factor:   2.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

  Frequency Set:  12  Based on FREQ, BW, and/or DOPPLER in schedule.  Used pcal sets:   1
   LO sum=    1611.69   1611.69   1614.21   1614.21   1618.21   1618.21   1622.21   1622.21
   BBC fr=     788.31    788.31    785.79    785.79    781.79    781.79    777.79    777.79
   Bandwd=      1.000     1.000     4.000     4.000     4.000     4.000     4.000     4.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = OFF 
    PCALXB1=   S1    S2    S3    S4    S5    S6    S7    S8 
    PCALXB2=   M1    M2    M3    M4    M5    M6    M7    M8 
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_off 
 SOURCE LIST -- GI04: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J1751+0939        17 49 10.387930   * 17 51 32.818573     17 51 55.621286       0.00
   1749+096          09 39 42.82582    * 09 39 00.72837      09 38 44.90433        0.00
   J1751+09          From catalog imbedded in main SCHED input file.
 * OT081             USNO - Ref Frame 1998-6, Eubanks June 1998
                     Doppler based on other sources.
                        0.492 scan hours,     13.767 baseline hours above horizon.

   J1832+1357        18 30 26.112214   * 18 32 43.471123     18 33 05.445221       0.00
 * 1830+139          13 55 26.71680    * 13 57 44.40030      13 57 54.65781        0.00
                     From catalog imbedded in main SCHED input file.
                     VLBA Calib. Survey - ICRF Frame - reduced by GSFC group
                     Doppler based on other sources.
                        1.408 scan hours,     71.697 baseline hours above horizon.

   J2148+0657        21 45 36.078481   * 21 48 05.458679     21 48 28.404738       0.00
 * 2145+067          06 43 40.90462    * 06 57 38.60422      06 59 36.95742        0.00
   J2148+06          From catalog imbedded in main SCHED input file.
                     ICRF - Ext.1 Source - 1998 IERS Annual Report
                     Doppler based on other sources.
                        0.333 scan hours,     14.972 baseline hours above horizon.

 * W43AOH            18 45 05.339856   * 18 47 41.163000     18 48 05.868908       0.00
                    -01 48 32.70202    *-01 45 11.22000     -01 44 49.36929        0.00
                     From catalog imbedded in main SCHED input file.
                     Doppler based on LSR frame and radio definition.  Velocities:
                         35.00    35.00    35.00    35.00    35.00    35.00    35.00    35.00
                       11.225 scan hours,    527.911 baseline hours above horizon.

   J1833+0115        18 30 35.405618   * 18 33 07.760875     18 33 31.971672       0.00
 * J1833+01          01 13 16.40937    * 01 15 35.30098      01 15 47.23295        0.00
   LANA              From catalog imbedded in main SCHED input file.
                     VCS4 source, 0.12 Jy at S-band in long baselines
                     Doppler based on other sources.
                        2.575 scan hours,     81.508 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   OT081              145.9
   1830+139           138.1
   2145+067           106.1
   W43AOH             148.5
   J1833+01           148.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

