  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: M82 transient (ToO)
 Exp. Code:  GB071C  


Schedule Version:       2.00
Processed by SCHED version:   9.30  Release near March 23, 2010

PI:       Andreas Brunthaler

Address:  MPIfR
          Auf dem Huegel 69
          53121 Bonn
          Germany

Phone:    +49 228 525 377
EMAIL:    brunthal@mpifr-bonn.mpg.de
Fax:      +49 228 525 229
Phone during observation: +49 228 525 377

Observing mode: VLBA+EVN at 18 cm

Notes:    VLBA 512 Mbps; EVN 1 Gbps
          CORRELATION IN SOCORRO
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

 Next scan frequencies:  1610.49  1610.49  1610.49  1610.49  1642.49  1642.49
                         1642.49  1642.49  1674.49  1674.49  1674.49  1674.49
                         1706.49  1706.49  1706.49  1706.49
 Next BBC frequencies:    789.51   789.51   789.51   789.51   757.51   757.51
                          757.51   757.51   725.51   725.51   725.51   725.51
                          693.51   693.51   693.51   693.51
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00    16.00    16.00

12 00 00  J1048+7143   22 07 20  12.6  -3.4 11.3       9.2     0   1  1      0  12 00 00
12 04 00  =1044+719    22 11 20  12.5  -3.0 11.4       8.3   240   F  1     15  12 00 00

12 04 00  M81          22 11 20   9.7   1.4-11.8      -3.3   -12   1  1     15  No stop 
12 06 00  ---          22 13 21   9.7   1.5-11.7      -3.7   108   F  1     23  12 04 00

12 06 00  M82          22 13 21  10.3   1.5-11.7      -3.6    -7   1  1     23  No stop 
12 08 00  ---          22 15 21  10.3   1.6-11.7      -4.1   113   F  1     31  12 06 00

12 08 00  M81          22 15 21   9.7   1.7-11.7      -4.1    -7   1  1     31  No stop 
12 09 30  ---          22 16 51   9.7   1.9-11.7      -4.5    83   F  1     37  12 08 00

12 09 30  M82          22 16 51  10.3   1.8-11.7      -4.4    -7   1  1     37  No stop 
12 11 30  ---          22 18 52  10.3   2.0-11.6      -4.8   113   F  1     45  12 09 30

12 12 00  M81          22 19 22   9.7   2.1-11.6      -5.0    23   1  1     45  12 12 00
12 13 00  ---          22 20 22   9.8   2.2-11.6      -5.2    60   F  1     48  12 12 00

12 13 00  M82          22 20 22  10.4   2.1-11.6      -5.2    -7   1  1     48  No stop 
12 15 00  ---          22 22 22  10.4   2.3-11.6      -5.6   113   F  1     56  12 13 00

12 15 00  M81          22 22 22   9.8   2.4-11.6      -5.7    -7   1  1     56  No stop 
12 16 30  ---          22 23 52   9.8   2.5-11.5      -6.0    83   F  1     62  12 15 00

12 16 30  M82          22 23 52  10.4   2.4-11.5      -5.9    -7   1  1     62  No stop 
12 18 30  ---          22 25 53  10.4   2.6-11.5      -6.4   113   F  1     70  12 16 30

12 18 30  M81          22 25 53   9.8   2.7-11.5      -6.4    -7   1  1     70  No stop 
12 20 00  ---          22 27 23   9.8   2.8-11.5      -6.8    83   F  1     75  12 18 30

12 20 00  M82          22 27 23  10.4   2.7-11.5      -6.7    -7   1  1     75  No stop 
12 22 00  ---          22 29 23  10.4   2.9-11.5      -7.1   113   F  1     83  12 20 00
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

12 22 30  M81          22 29 53   9.8   3.0-11.4      -7.3    23   1  1     83  12 22 30
12 23 30  ---          22 30 54   9.9   3.1-11.4      -7.5    60   F  1     87  12 22 30

12 23 30  M82          22 30 54  10.5   3.0-11.4      -7.5    -7   1  1     87  No stop 
12 25 30  ---          22 32 54  10.5   3.2-11.4      -7.9   113   F  1     95  12 23 30

12 25 30  M81          22 32 54   9.9   3.3-11.4      -8.0    -7   1  1     95  No stop 
12 27 00  ---          22 34 24   9.9   3.4-11.4      -8.3    83   F  1    101  12 25 30

12 27 00  M82          22 34 24  10.5   3.3-11.4      -8.2    -7   1  1    101  No stop 
12 29 00  ---          22 36 25  10.5   3.5-11.3      -8.7   113   F  1    108  12 27 00

12 29 30  M81          22 36 55   9.9   3.7-11.3      -8.8    23   1  1    108  12 29 30
12 30 30  ---          22 37 55   9.9   3.8-11.3      -9.1    60   F  1    112  12 29 30

12 30 30  M82          22 37 55  10.5   3.6-11.3      -9.0    -7   1  1    112  No stop 
12 32 30  ---          22 39 55  10.6   3.8-11.3      -9.4   113   F  1    120  12 30 30

12 32 30  M81          22 39 55  10.0   3.9-11.3      -9.5    -7   1  1    120  No stop 
12 34 00  ---          22 41 25  10.0   4.1-11.2      -9.8    83   F  1    126  12 32 30

12 34 00  M82          22 41 25  10.6   3.9-11.3      -9.8    -7   1  1    126  No stop 
12 36 00  ---          22 43 26  10.6   4.1-11.2     -10.2   113   F  1    134  12 34 00

12 36 00  M81          22 43 26  10.0   4.2-11.2     -10.3    -7   1  1    134  No stop 
12 37 30  ---          22 44 56  10.1   4.4-11.2     -10.6    83   F  1    139  12 36 00

12 37 30  M82          22 44 56  10.7   4.2-11.2     -10.5    -7   1  1    139  No stop 
12 39 30  ---          22 46 56  10.7   4.4-11.2     -11.0   113   F  1    147  12 37 30

12 40 00  M81          22 47 26  10.1   4.6-11.1     -11.1    23   1  1    147  12 40 00
12 41 00  ---          22 48 26  10.1   4.7-11.1     -11.3    60   F  1    151  12 40 00

12 41 00  M82          22 48 26  10.7   4.5-11.1     -11.3    -7   1  1    151  No stop 
12 43 00  ---          22 50 27  10.7   4.7-11.1     -11.7   113   F  1    159  12 41 00

12 43 00  M81          22 50 27  10.1   4.9-11.1     -11.8    -7   1  1    159  No stop 
12 44 30  ---          22 51 57  10.2   5.0-11.1     -12.1    83   F  1    165  12 43 00

12 44 30  M82          22 51 57  10.8   4.8-11.1     -12.1    -7   1  1    165  No stop 
12 46 30  ---          22 53 57  10.8   5.0-11.0     -12.5   113   F  1    172  12 44 30

12 47 00  M81          22 54 27  10.2   5.2-11.0     -12.7    23   1  1    172  12 47 00
12 48 00  ---          22 55 28  10.2   5.3-11.0     -12.9    60   F  1    176  12 47 00
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

12 48 00  M82          22 55 28  10.8   5.2-11.0     -12.8    -7   1  1    176  No stop 
12 50 00  ---          22 57 28  10.9   5.3-11.0     -13.3   113   F  1    184  12 48 00

12 50 00  M81          22 57 28  10.3   5.5-11.0     -13.3    -7   1  1    184  No stop 
12 51 30  ---          22 58 58  10.3   5.6-11.0     -13.6    83   F  1    190  12 50 00

12 51 30  M82          22 58 58  10.9   5.5-11.0     -13.6    -7   1  1    190  No stop 
12 53 30  ---          23 00 59  10.9   5.6-10.9     -14.0   113   F  1    197  12 51 30

12 53 30  M81          23 00 59  10.4   5.8-10.9     -14.1    -7   1  1    197  No stop 
12 55 00  ---          23 02 29  10.4   5.9-10.9     -14.4    83   F  1    203  12 53 30

12 55 00  M82          23 02 29  11.0   5.8-10.9     -14.4    -7   1  1    203  No stop 
12 57 00  ---          23 04 29  11.0   5.9-10.9     -14.8   113   F  1    211  12 55 00

12 57 30  M81          23 04 59  10.5   6.2-10.9     -14.9    23   1  1    211  12 57 30
12 58 30  ---          23 05 59  10.5   6.2-10.8     -15.2    60   F  1    215  12 57 30

12 59 00  J1048+7143   23 06 29  12.4   1.4-11.7      -3.8    20   1  1    215  12 59 00
13 02 00  =1044+719    23 09 30  12.4   1.6-11.7      -4.5   180   F  1    226  12 59 00

13 02 00  M81          23 09 30  10.6   6.6-10.8     -15.9   -10   1  1    226  No stop 
13 04 00  ---          23 11 30  10.6   6.7-10.7     -16.4   110   F  1    234  13 02 00

13 04 00  M82          23 11 30  11.2   6.5-10.8     -16.3    -7   1  1    234  No stop 
13 06 00  ---          23 13 31  11.2   6.7-10.7     -16.8   113   F  1    242  13 04 00

13 06 00  M81          23 13 31  10.7   6.9-10.7     -16.8    -7   1  1    242  No stop 
13 07 30  ---          23 15 01  10.7   7.0-10.7     -17.1    83   F  1    248  13 06 00

13 07 30  M82          23 15 01  11.3   6.8-10.7     -17.1    -7   1  1    248  No stop 
13 09 30  ---          23 17 01  11.3   7.0-10.7     -17.5   113   F  1    255  13 07 30

13 10 00  M81          23 17 31  10.8   7.3-10.6     -17.7    23   1  1    255  13 10 00
13 11 00  ---          23 18 31  10.8   7.3-10.6     -17.9    60   F  1    259  13 10 00

13 11 00  M82          23 18 31  11.4   7.1-10.6     -17.9    -7   1  1    259  No stop 
13 13 00  ---          23 20 32  11.4   7.3-10.6     -18.3   113   F  1    267  13 11 00

13 13 00  M81          23 20 32  10.8   7.5-10.6     -18.3    -7   1  1    267  No stop 
13 14 30  ---          23 22 02  10.9   7.6-10.6     -18.7    83   F  1    273  13 13 00

13 14 30  M82          23 22 02  11.5   7.4-10.6     -18.6    -7   1  1    273  No stop 
13 16 30  ---          23 24 02  11.5   7.6-10.5     -19.1   113   F  1    281  13 14 30
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

13 16 30  M81          23 24 02  10.9   7.8-10.5     -19.1    -7   1  1    281  No stop 
13 18 00  ---          23 25 33  11.0   7.9-10.5     -19.4    83   F  1    286  13 16 30

13 18 00  M82          23 25 33  11.6   7.7-10.5     -19.4    -7   1  1    286  No stop 
13 20 00  ---          23 27 33  11.6   7.9-10.5     -19.8   113   F  1    294  13 18 00

13 20 30  M81          23 28 03  11.1   8.2-10.5     -20.0    23   1  1    294  13 20 30
13 21 30  ---          23 29 03  11.1   8.3-10.5     -20.2    60   F  1    298  13 20 30

13 21 30  M82          23 29 03  11.7   8.0-10.5     -20.1    -7   1  1    298  No stop 
13 23 30  ---          23 31 03  11.7   8.2-10.4     -20.6   113   F  1    306  13 21 30

13 23 30  M81          23 31 03  11.2   8.4-10.4     -20.6    -7   1  1    306  No stop 
13 25 00  ---          23 32 34  11.2   8.6-10.4     -20.9    83   F  1    312  13 23 30

13 25 00  M82          23 32 34  11.8   8.3-10.4     -20.9    -7   1  1    312  No stop 
13 27 00  ---          23 34 34  11.8   8.5-10.4     -21.3   113   F  1    319  13 25 00

13 27 30  M81          23 35 04  11.3   8.8-10.4     -21.5    23   1  1    319  13 27 30
13 28 30  ---          23 36 04  11.3   8.8-10.3     -21.7    60   F  1    323  13 27 30

13 28 30  M82          23 36 04  11.9   8.6-10.3     -21.7    -7   1  1    323  No stop 
13 30 30  ---          23 38 05  12.0   8.8-10.3     -22.1   113   F  1    331  13 28 30

13 30 30  M81          23 38 05  11.4   9.0-10.3     -22.1    -7   1  1    331  No stop 
13 32 00  ---          23 39 35  11.4   9.1-10.3     -22.5    83   F  1    337  13 30 30

13 32 00  M82          23 39 35  12.0   8.9-10.3     -22.4    -7   1  1    337  No stop 
13 34 00  ---          23 41 35  12.1   9.0-10.3     -22.9   113   F  1    344  13 32 00

13 34 00  M81          23 41 35  11.5   9.3-10.2     -22.9    -7   1  1    344  No stop 
13 35 30  ---          23 43 05  11.6   9.4-10.2     -23.2    83   F  1    350  13 34 00

13 35 30  M82          23 43 05  12.1   9.2-10.2     -23.2    -7   1  1    350  No stop 
13 37 30  ---          23 45 06  12.2   9.3-10.2     -23.6   113   F  1    358  13 35 30

13 38 00  M81          23 45 36  11.7   9.7-10.2     -23.8    23   1  1    358  13 38 00
13 39 00  ---          23 46 36  11.7   9.7-10.2     -24.0    60   F  1    362  13 38 00

13 39 00  M82          23 46 36  12.2   9.5-10.2     -24.0    -7   1  1    362  No stop 
13 41 00  ---          23 48 36  12.3   9.6-10.1     -24.4   113   F  1    370  13 39 00

13 41 00  M81          23 48 36  11.8   9.9-10.1     -24.4    -7   1  1    370  No stop 
13 42 30  ---          23 50 07  11.8  10.0-10.1     -24.7    83   F  1    375  13 41 00
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

13 42 30  M82          23 50 07  12.4   9.7-10.1     -24.7    -7   1  1    375  No stop 
13 44 30  ---          23 52 07  12.4   9.9-10.1     -25.2   113   F  1    383  13 42 30

13 45 00  M81          23 52 37  11.9  10.2-10.1     -25.3    23   1  1    383  13 45 00
13 46 00  ---          23 53 37  12.0  10.3-10.0     -25.5    60   F  1    387  13 45 00

13 46 00  M82          23 53 37  12.5  10.0-10.1     -25.5    -7   1  1    387  No stop 
13 48 00  ---          23 55 37  12.6  10.2-10.0     -25.9   113   F  1    395  13 46 00

13 48 00  M81          23 55 37  12.0  10.5-10.0     -25.9    -7   1  1    395  No stop 
13 49 30  ---          23 57 08  12.1  10.6-10.0     -26.3    83   F  1    401  13 48 00

13 49 30  M82          23 57 08  12.6  10.3-10.0     -26.2    -7   1  1    401  No stop 
13 51 30  ---          23 59 08  12.7  10.5-10.0     -26.7   113   F  1    408  13 49 30

13 51 30  M81          23 59 08  12.2  10.8-10.0     -26.7    -7   1  1    408  No stop 
13 53 00  ---          00 00 38  12.2  10.9 -9.9     -27.0    83   F  1    414  13 51 30

13 53 00  M82          00 00 38  12.8  10.6 -9.9     -27.0    -7   1  1    414  No stop 
13 55 00  ---          00 02 39  12.8  10.7 -9.9     -27.4   113   F  1    422  13 53 00

13 55 30  M81          00 03 09  12.3  11.1 -9.9     -27.6    23   1  1    422  13 55 30
13 56 30  ---          00 04 09  12.4  11.2 -9.9     -27.8    60   F  1    426  13 55 30

13 57 00  J1048+7143   00 04 39  13.2   6.0-10.7     -16.6    21   1  1    426  13 57 00
14 00 00  =1044+719    00 07 39  13.2   6.2-10.7     -17.3   180   F  1    437  13 57 00

14 00 00  M81          00 07 39  12.5  11.5 -9.8     -28.5    -9   1  1    437  No stop 
14 02 00  ---          00 09 40  12.6  11.6 -9.8     -29.0   111   F  1    445  14 00 00

14 02 00  M82          00 09 40  13.1  11.3 -9.8     -29.0    -7   1  1    445  No stop 
14 04 00  ---          00 11 40  13.2  11.5 -9.8     -29.4   113   F  1    453  14 02 00

14 04 00  M81          00 11 40  12.7  11.8 -9.7     -29.4    -7   1  1    453  No stop 
14 05 30  ---          00 13 10  12.8  11.9 -9.7     -29.7    83   F  1    459  14 04 00

14 05 30  M82          00 13 10  13.3  11.6 -9.7     -29.7    -7   1  1    459  No stop 
14 07 30  ---          00 15 11  13.4  11.7 -9.7     -30.2   113   F  1    466  14 05 30

14 08 00  M81          00 15 41  12.9  12.1 -9.7     -30.3    23   1  1    466  14 08 00
14 09 00  ---          00 16 41  12.9  12.2 -9.7     -30.5    60   F  1    470  14 08 00

14 09 00  M82          00 16 41  13.4  11.8 -9.7     -30.5    -7   1  1    470  No stop 
14 11 00  ---          00 18 41  13.5  12.0 -9.6     -30.9   113   F  1    478  14 09 00
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

14 11 00  M81          00 18 41  13.0  12.3 -9.6     -30.9    -7   1  1    478  No stop 
14 12 30  ---          00 20 12  13.1  12.5 -9.6     -31.2    83   F  1    484  14 11 00

14 12 30  M82          00 20 12  13.6  12.1 -9.6     -31.2    -7   1  1    484  No stop 
14 14 30  ---          00 22 12  13.7  12.3 -9.6     -31.7   113   F  1    492  14 12 30

14 14 30  M81          00 22 12  13.2  12.6 -9.6     -31.7    -7   1  1    492  No stop 
14 16 00  ---          00 23 42  13.2  12.7 -9.5     -32.0    83   F  1    497  14 14 30

14 16 00  M82          00 23 42  13.8  12.4 -9.6     -32.0    -7   1  1    497  No stop 
14 18 00  ---          00 25 42  13.8  12.5 -9.5     -32.4   113   F  1    505  14 16 00

14 18 30  M81          00 26 12  13.4  12.9 -9.5     -32.5    23   1  1    505  14 18 30
14 19 30  ---          00 27 13  13.4  13.0 -9.5     -32.7    60   F  1    509  14 18 30

14 19 30  M82          00 27 13  13.9  12.6 -9.5     -32.8    -7   1  1    509  No stop 
14 21 30  ---          00 29 13  14.0  12.8 -9.5     -33.2   113   F  1    517  14 19 30

14 21 30  M81          00 29 13  13.5  13.2 -9.5     -33.2    -7   1  1    517  No stop 
14 23 00  ---          00 30 43  13.6  13.3 -9.4     -33.5    83   F  1    523  14 21 30

14 23 00  M82          00 30 43  14.1  12.9 -9.4     -33.5    -7   1  1    523  No stop 
14 25 00  ---          00 32 44  14.2  13.1 -9.4     -34.0   113   F  1    530  14 23 00

14 25 30  M81          00 33 14  13.7  13.5 -9.4     -34.0    23   1  1    530  14 25 30
14 26 30  ---          00 34 14  13.8  13.5 -9.4     -34.3    60   F  1    534  14 25 30

14 26 30  M82          00 34 14  14.3  13.2 -9.4     -34.3    -7   1  1    534  No stop 
14 28 30  ---          00 36 14  14.4  13.3 -9.3     -34.7   113   F  1    542  14 26 30

14 28 30  M81          00 36 14  13.9  13.7 -9.3     -34.7    -7   1  1    542  No stop 
14 30 00  ---          00 37 44  13.9  13.8 -9.3     -35.0    83   F  1    548  14 28 30

14 30 00  M82          00 37 44  14.4  13.4 -9.3     -35.0    -7   1  1    548  No stop 
14 32 00  ---          00 39 45  14.5  13.6 -9.3     -35.5   113   F  1    555  14 30 00

14 32 00  M81          00 39 45  14.0  14.0 -9.3     -35.4    -7   1  1    555  No stop 
14 33 30  ---          00 41 15  14.1  14.1 -9.3     -35.8    83   F  1    561  14 32 00

14 33 30  M82          00 41 15  14.6  13.7 -9.3     -35.8    -7   1  1    561  No stop 
14 35 30  ---          00 43 15  14.7  13.8 -9.2     -36.2   113   F  1    569  14 33 30

14 36 00  M81          00 43 45  14.3  14.3 -9.2     -36.3    23   1  1    569  14 36 00
14 37 00  ---          00 44 46  14.3  14.3 -9.2     -36.5    60   F  1    573  14 36 00
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

14 37 00  M82          00 44 46  14.8  13.9 -9.2     -36.6    -7   1  1    573  No stop 
14 39 00  ---          00 46 46  14.9  14.1 -9.2     -37.0   113   F  1    581  14 37 00

14 39 00  M81          00 46 46  14.4  14.5 -9.2     -37.0    -7   1  1    581  No stop 
14 40 30  ---          00 48 16  14.5  14.6 -9.1     -37.3    83   F  1    586  14 39 00

14 40 30  M82          00 48 16  15.0  14.2 -9.1     -37.3    -7   1  1    586  No stop 
14 42 30  ---          00 50 16  15.1  14.3 -9.1     -37.7   113   F  1    594  14 40 30

14 43 00  M81          00 50 47  14.6  14.8 -9.1     -37.8    23   1  1    594  14 43 00
14 44 00  ---          00 51 47  14.7  14.9 -9.1     -38.0    60   F  1    598  14 43 00

14 44 00  M82          00 51 47  15.2  14.4 -9.1     -38.1    -7   1  1    598  No stop 
14 46 00  ---          00 53 47  15.3  14.6 -9.0     -38.5   113   F  1    606  14 44 00

14 46 00  M81          00 53 47  14.8  15.0 -9.0     -38.5    -7   1  1    606  No stop 
14 47 30  ---          00 55 17  14.9  15.1 -9.0     -38.8    83   F  1    612  14 46 00

14 47 30  M82          00 55 17  15.3  14.7 -9.0     -38.8    -7   1  1    612  No stop 
14 49 30  ---          00 57 18  15.5  14.8 -9.0     -39.3   113   F  1    619  14 47 30

14 49 30  M81          00 57 18  15.0  15.3 -9.0     -39.2    -7   1  1    619  No stop 
14 51 00  ---          00 58 48  15.1  15.4 -9.0     -39.5    83   F  1    625  14 49 30

14 51 00  M82          00 58 48  15.5  14.9 -9.0     -39.6    -7   1  1    625  No stop 
14 53 00  ---          01 00 48  15.7  15.1 -8.9     -40.0   113   F  1    633  14 51 00

14 53 30  M81          01 01 18  15.2  15.5 -8.9     -40.1    23   1  1    633  14 53 30
14 54 30  ---          01 02 18  15.3  15.6 -8.9     -40.3    60   F  1    637  14 53 30

14 55 00  J1048+7143   01 02 48  14.9  10.3 -9.8     -29.4    20   1  1    637  14 55 00
14 58 00  =1044+719    01 05 49  15.1  10.5 -9.7     -30.0   180   F  1    648  14 55 00

14 58 30  3C84         01 06 19  61.0  58.6 -2.2    -101.2   -68   1  1    648  14 58 30
15 04 30  ---          01 12 20  62.1  58.1 -2.1    -102.6   292   F  1    672  14 58 30

15 10 08  M81          01 17 59  16.2  16.7 -8.6     -43.7   240   1  1    672  15 10 08
15 12 08  ---          01 19 59  16.3  16.8 -8.6     -44.1   120   F  1    679  15 10 08

15 12 08  M82          01 19 59  16.8  16.4 -8.6     -44.2    -7   1  1    679  No stop 
15 14 08  ---          01 22 00  16.9  16.5 -8.6     -44.6   113   F  1    687  15 12 08

15 14 08  M81          01 22 00  16.5  17.0 -8.6     -44.5    -7   1  1    687  No stop 
15 15 38  ---          01 23 30  16.6  17.1 -8.5     -44.8    83   F  1    693  15 14 08
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

15 15 38  M82          01 23 30  17.0  16.6 -8.6     -44.9    -7   1  1    693  No stop 
15 17 38  ---          01 25 30  17.1  16.7 -8.5     -45.3   113   F  1    701  15 15 38

15 18 08  M81          01 26 00  16.7  17.2 -8.5     -45.4    24   1  1    701  15 18 08
15 19 08  ---          01 27 00  16.8  17.3 -8.5     -45.6    60   F  1    704  15 18 08

15 19 08  M82          01 27 00  17.2  16.8 -8.5     -45.7    -7   1  1    704  No stop 
15 21 08  ---          01 29 01  17.3  16.9 -8.5     -46.1   113   F  1    712  15 19 08

15 21 08  M81          01 29 01  16.9  17.4 -8.5     -46.0    -7   1  1    712  No stop 
15 22 38  ---          01 30 31  17.0  17.5 -8.4     -46.4    83   F  1    718  15 21 08

15 22 38  M82          01 30 31  17.4  17.0 -8.4     -46.4    -7   1  1    718  No stop 
15 24 38  ---          01 32 31  17.5  17.2 -8.4     -46.9   113   F  1    726  15 22 38

15 24 38  M81          01 32 31  17.1  17.7 -8.4     -46.8    -7   1  1    726  No stop 
15 26 08  ---          01 34 02  17.2  17.7 -8.4     -47.1    83   F  1    732  15 24 38

15 26 08  M82          01 34 02  17.6  17.3 -8.4     -47.2    -7   1  1    732  No stop 
15 28 08  ---          01 36 02  17.8  17.4 -8.3     -47.6   113   F  1    739  15 26 08

15 28 38  M81          01 36 32  17.4  17.9 -8.3     -47.6    24   1  1    739  15 28 38
15 29 38  ---          01 37 32  17.5  18.0 -8.3     -47.9    60   F  1    743  15 28 38

15 29 38  M82          01 37 32  17.9  17.5 -8.3     -47.9    -7   1  1    743  No stop 
15 31 38  ---          01 39 33  18.0  17.6 -8.3     -48.4   113   F  1    751  15 29 38

15 31 38  M81          01 39 33  17.6  18.1 -8.3     -48.3    -6   1  1    751  No stop 
15 33 08  ---          01 41 03  17.7  18.2 -8.3     -48.6    84   F  1    757  15 31 38

15 33 08  M82          01 41 03  18.1  17.7 -8.3     -48.7    -6   1  1    757  No stop 
15 35 08  ---          01 43 03  18.2  17.8 -8.2     -49.1   114   F  1    764  15 33 08

15 35 38  M81          01 43 33  17.9  18.3 -8.2     -49.1    24   1  1    764  15 35 38
15 36 38  ---          01 44 33  17.9  18.4 -8.2     -49.4    60   F  1    768  15 35 38

15 36 38  M82          01 44 33  18.3  17.9 -8.2     -49.4    -6   1  1    768  No stop 
15 38 38  ---          01 46 34  18.5  18.0 -8.2     -49.9   114   F  1    776  15 36 38

15 38 38  M81          01 46 34  18.1  18.5 -8.2     -49.8    -6   1  1    776  No stop 
15 40 08  ---          01 48 04  18.2  18.6 -8.1     -50.1    84   F  1    782  15 38 38

15 40 08  M82          01 48 04  18.6  18.1 -8.1     -50.2    -6   1  1    782  No stop 
15 42 08  ---          01 50 04  18.7  18.2 -8.1     -50.6   114   F  1    790  15 40 08
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

15 42 08  M81          01 50 04  18.3  18.7 -8.1     -50.5    -6   1  1    790  No stop 
15 43 38  ---          01 51 34  18.4  18.8 -8.1     -50.9    84   F  1    795  15 42 08

15 43 38  M82          01 51 34  18.8  18.3 -8.1     -51.0    -6   1  1    795  No stop 
15 45 38  ---          01 53 35  18.9  18.4 -8.1     -51.4   114   F  1    803  15 43 38

15 46 08  M81          01 54 05  18.6  19.0 -8.0     -51.4    24   1  1    803  15 46 08
15 47 08  ---          01 55 05  18.7  19.0 -8.0     -51.6    60   F  1    807  15 46 08

15 47 08  M82          01 55 05  19.0  18.5 -8.0     -51.7    -6   1  1    807  No stop 
15 49 08  ---          01 57 05  19.2  18.6 -8.0     -52.2   114   F  1    815  15 47 08

15 49 08  M81          01 57 05  18.8  19.2 -8.0     -52.1    -6   1  1    815  No stop 
15 50 38  ---          01 58 36  18.9  19.2 -8.0     -52.4    84   F  1    821  15 49 08

15 50 38  M82          01 58 36  19.3  18.7 -8.0     -52.5    -6   1  1    821  No stop 
15 52 38  ---          02 00 36  19.4  18.8 -7.9     -52.9   114   F  1    828  15 50 38

15 53 08  M81          02 01 06  19.1  19.4 -7.9     -52.9    24   1  1    828  15 53 08
15 54 08  ---          02 02 06  19.2  19.4 -7.9     -53.1    60   F  1    832  15 53 08

15 54 08  M82          02 02 06  19.5  18.9 -7.9     -53.2    -6   1  1    832  No stop 
15 56 08  ---          02 04 07  19.7  19.0 -7.9     -53.7   114   F  1    840  15 54 08

15 56 08  M81          02 04 07  19.3  19.6 -7.9     -53.6    -6   1  1    840  No stop 
15 57 38  ---          02 05 37  19.4  19.6 -7.8     -53.9    84   F  1    846  15 56 08

15 57 38  M82          02 05 37  19.8  19.1 -7.9     -54.0    -6   1  1    846  No stop 
15 59 38  ---          02 07 37  19.9  19.2 -7.8     -54.4   114   F  1    853  15 57 38

15 59 38  M81          02 07 37  19.6  19.8 -7.8     -54.3    -6   1  1    853  No stop 
16 01 08  ---          02 09 07  19.7  19.8 -7.8     -54.6    84   F  1    859  15 59 38

16 01 08  M82          02 09 07  20.0  19.3 -7.8     -54.7    -6   1  1    859  No stop 
16 03 08  ---          02 11 08  20.2  19.4 -7.8     -55.2   114   F  1    867  16 01 08

16 03 38  M81          02 11 38  19.9  20.0 -7.7     -55.2    24   1  1    867  16 03 38
16 04 38  ---          02 12 38  19.9  20.0 -7.7     -55.4    60   F  1    871  16 03 38

16 05 08  J1048+7143   02 13 08  18.3  14.9 -8.6     -44.7    21   1  1    871  16 05 08
16 08 08  =1044+719    02 16 09  18.4  15.1 -8.6     -45.4   180   F  1    883  16 05 08

16 08 08  M81          02 16 09  20.2  20.2 -7.7     -56.1   -10   1  1    883  No stop 
16 10 08  ---          02 18 09  20.3  20.3 -7.6     -56.6   110   F  1    890  16 08 08
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

16 10 08  M82          02 18 09  20.7  19.8 -7.6     -56.7    -6   1  1    890  No stop 
16 12 08  ---          02 20 09  20.8  19.9 -7.6     -57.1   114   F  1    898  16 10 08

16 12 08  M81          02 20 09  20.5  20.4 -7.6     -57.0    -6   1  1    898  No stop 
16 13 38  ---          02 21 39  20.6  20.5 -7.6     -57.3    84   F  1    904  16 12 08

16 13 38  M82          02 21 39  20.9  19.9 -7.6     -57.5    -6   1  1    904  No stop 
16 15 38  ---          02 23 40  21.1  20.0 -7.6     -57.9   114   F  1    912  16 13 38

16 16 08  M81          02 24 10  20.8  20.6 -7.5     -57.9    24   1  1    912  16 16 08
16 17 08  ---          02 25 10  20.9  20.7 -7.5     -58.1    60   F  1    915  16 16 08

16 17 08  M82          02 25 10  21.2  20.1 -7.5     -58.2    -6   1  1    915  No stop 
16 19 08  ---          02 27 10  21.3  20.2 -7.5     -58.7   114   F  1    923  16 17 08

16 19 08  M81          02 27 10  21.0  20.8 -7.5     -58.5    -6   1  1    923  No stop 
16 20 38  ---          02 28 41  21.1  20.9 -7.5     -58.8    84   F  1    929  16 19 08

16 20 38  M82          02 28 41  21.4  20.3 -7.5     -59.0    -6   1  1    929  No stop 
16 22 38  ---          02 30 41  21.6  20.4 -7.4     -59.4   114   F  1    937  16 20 38

16 22 38  M81          02 30 41  21.3  21.0 -7.4     -59.3    -6   1  1    937  No stop 
16 24 08  ---          02 32 11  21.4  21.0 -7.4     -59.6    84   F  1    943  16 22 38

16 24 08  M82          02 32 11  21.7  20.4 -7.4     -59.7    -6   1  1    943  No stop 
16 26 08  ---          02 34 11  21.9  20.5 -7.4     -60.2   114   F  1    950  16 24 08

16 26 38  M81          02 34 42  21.6  21.2 -7.4     -60.1    24   1  1    950  16 26 38
16 27 38  ---          02 35 42  21.7  21.2 -7.3     -60.4    60   F  1    954  16 26 38

16 27 38  M82          02 35 42  22.0  20.6 -7.4     -60.5    -6   1  1    954  No stop 
16 29 38  ---          02 37 42  22.1  20.7 -7.3     -60.9   114   F  1    962  16 27 38

16 29 38  M81          02 37 42  21.8  21.3 -7.3     -60.8    -6   1  1    962  No stop 
16 31 08  ---          02 39 12  22.0  21.4 -7.3     -61.1    84   F  1    968  16 29 38

16 31 08  M82          02 39 12  22.2  20.8 -7.3     -61.3    -6   1  1    968  No stop 
16 33 08  ---          02 41 13  22.4  20.9 -7.3     -61.7   114   F  1    975  16 31 08

16 33 38  M81          02 41 43  22.2  21.5 -7.2     -61.7    24   1  1    975  16 33 38
16 34 38  ---          02 42 43  22.2  21.5 -7.2     -61.9    60   F  1    979  16 33 38

16 34 38  M82          02 42 43  22.5  20.9 -7.2     -62.0    -6   1  1    979  No stop 
16 36 38  ---          02 44 43  22.7  21.0 -7.2     -62.5   114   F  1    987  16 34 38
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

16 36 38  M81          02 44 43  22.4  21.6 -7.2     -62.3    -6   1  1    987  No stop 
16 38 08  ---          02 46 13  22.5  21.7 -7.2     -62.6    84   F  1    993  16 36 38

16 38 08  M82          02 46 13  22.8  21.1 -7.2     -62.8    -6   1  1    993  No stop 
16 40 08  ---          02 48 14  22.9  21.2 -7.1     -63.2   114   F  1   1001  16 38 08

16 40 08  M81          02 48 14  22.7  21.8 -7.1     -63.1    -6   1  1   1001  No stop 
16 41 38  ---          02 49 44  22.8  21.8 -7.1     -63.4    84   F  1   1006  16 40 08

16 41 38  M82          02 49 44  23.0  21.2 -7.1     -63.6    -6   1  1   1006  No stop 
16 43 38  ---          02 51 44  23.2  21.3 -7.1     -64.0   114   F  1   1014  16 41 38

16 44 08  M81          02 52 14  23.0  22.0 -7.1     -63.9    24   1  1   1014  16 44 08
16 45 08  ---          02 53 15  23.1  22.0 -7.1     -64.2    60   F  1   1018  16 44 08

16 45 08  M82          02 53 15  23.3  21.4 -7.1     -64.3    -6   1  1   1018  No stop 
16 47 08  ---          02 55 15  23.5  21.5 -7.0     -64.8   114   F  1   1026  16 45 08

16 47 08  M81          02 55 15  23.2  22.1 -7.0     -64.6    -6   1  1   1026  No stop 
16 48 38  ---          02 56 45  23.4  22.1 -7.0     -64.9    84   F  1   1032  16 47 08

16 48 38  M82          02 56 45  23.6  21.5 -7.0     -65.1    -6   1  1   1032  No stop 
16 50 38  ---          02 58 45  23.8  21.6 -7.0     -65.5   114   F  1   1039  16 48 38

16 51 08  M81          02 59 16  23.6  22.2 -7.0     -65.5    24   1  1   1039  16 51 08
16 52 08  ---          03 00 16  23.6  22.3 -6.9     -65.7    60   F  1   1043  16 51 08

16 52 08  M82          03 00 16  23.9  21.7 -6.9     -65.9    -6   1  1   1043  No stop 
16 54 08  ---          03 02 16  24.0  21.7 -6.9     -66.3   114   F  1   1051  16 52 08

16 54 08  M81          03 02 16  23.8  22.4 -6.9     -66.1    -6   1  1   1051  No stop 
16 55 38  ---          03 03 46  23.9  22.4 -6.9     -66.4    84   F  1   1057  16 54 08

16 55 38  M82          03 03 46  24.2  21.8 -6.9     -66.6    -6   1  1   1057  No stop 
16 57 38  ---          03 05 47  24.3  21.9 -6.8     -67.1   114   F  1   1064  16 55 38

16 57 38  M81          03 05 47  24.1  22.5 -6.8     -66.9    -6   1  1   1064  No stop 
16 59 08  ---          03 07 17  24.2  22.6 -6.8     -67.2    84   F  1   1070  16 57 38

16 59 08  M82          03 07 17  24.4  21.9 -6.8     -67.4    -6   1  1   1070  No stop 
17 01 08  ---          03 09 17  24.6  22.0 -6.8     -67.8   114   F  1   1078  16 59 08

17 01 38  M81          03 09 47  24.4  22.7 -6.8     -67.7    24   1  1   1078  17 01 38
17 02 38  ---          03 10 47  24.5  22.7 -6.8     -68.0    60   F  1   1082  17 01 38
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

17 03 08  J1048+7143   03 11 18  21.8  18.0 -7.6     -57.5    19   1  1   1082  17 03 08
17 06 08  =1044+719    03 14 18  22.0  18.1 -7.6     -58.2   180   F  1   1093  17 03 08

17 06 08  M81          03 14 18  24.8  22.8 -6.7     -68.7   -12   1  1   1093  No stop 
17 08 08  ---          03 16 18  25.0  22.9 -6.7     -69.2   108   F  1   1101  17 06 08

17 08 08  M82          03 16 18  25.2  22.2 -6.7     -69.4    -6   1  1   1101  No stop 
17 10 08  ---          03 18 19  25.3  22.3 -6.6     -69.8   114   F  1   1109  17 08 08

17 10 08  M81          03 18 19  25.1  23.0 -6.6     -69.6    -6   1  1   1109  No stop 
17 11 38  ---          03 19 49  25.3  23.0 -6.6     -69.9    84   F  1   1115  17 10 08

17 11 38  M82          03 19 49  25.4  22.4 -6.6     -70.1    -6   1  1   1115  No stop 
17 13 38  ---          03 21 49  25.6  22.4 -6.6     -70.6   114   F  1   1123  17 11 38

17 14 08  M81          03 22 19  25.5  23.1 -6.6     -70.5    24   1  1   1123  17 14 08
17 15 08  ---          03 23 20  25.6  23.1 -6.6     -70.7    60   F  1   1126  17 14 08

17 15 08  M82          03 23 20  25.7  22.5 -6.6     -70.9    -6   1  1   1126  No stop 
17 17 08  ---          03 25 20  25.9  22.5 -6.5     -71.4   114   F  1   1134  17 15 08

17 17 08  M81          03 25 20  25.7  23.2 -6.5     -71.1    -6   1  1   1134  No stop 
17 18 38  ---          03 26 50  25.9  23.2 -6.5     -71.5    84   F  1   1140  17 17 08

17 18 38  M82          03 26 50  26.0  22.6 -6.5     -71.7    -6   1  1   1140  No stop 
17 20 38  ---          03 28 50  26.2  22.6 -6.5     -72.1   114   F  1   1148  17 18 38

17 20 38  M81          03 28 50  26.0  23.3 -6.5     -71.9    -6   1  1   1148  No stop 
17 22 08  ---          03 30 21  26.2  23.3 -6.4     -72.3    84   F  1   1153  17 20 38

17 22 08  M82          03 30 21  26.3  22.7 -6.4     -72.5    -6   1  1   1153  No stop 
17 24 08  ---          03 32 21  26.5  22.7 -6.4     -72.9   114   F  1   1161  17 22 08

17 24 38  M81          03 32 51  26.4  23.4 -6.4     -72.8    24   1  1   1161  17 24 38
17 25 38  ---          03 33 51  26.5  23.5 -6.4     -73.0    60   F  1   1165  17 24 38

17 25 38  M82          03 33 51  26.6  22.8 -6.4     -73.2    -6   1  1   1165  No stop 
17 27 38  ---          03 35 52  26.8  22.8 -6.3     -73.7   114   F  1   1173  17 25 38

17 27 38  M81          03 35 52  26.6  23.5 -6.3     -73.5    -6   1  1   1173  No stop 
17 29 08  ---          03 37 22  26.8  23.6 -6.3     -73.8    84   F  1   1179  17 27 38

17 29 08  M82          03 37 22  26.9  22.9 -6.3     -74.0    -6   1  1   1179  No stop 
17 31 08  ---          03 39 22  27.1  22.9 -6.3     -74.5   114   F  1   1186  17 29 08
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

17 31 38  M81          03 39 52  27.0  23.6 -6.3     -74.4    24   1  1   1186  17 31 38
17 32 38  ---          03 40 52  27.1  23.6 -6.3     -74.6    60   F  1   1190  17 31 38

17 32 38  M82          03 40 52  27.2  23.0 -6.3     -74.8    -6   1  1   1190  No stop 
17 34 38  ---          03 42 53  27.4  23.0 -6.2     -75.3   114   F  1   1198  17 32 38

17 34 38  M81          03 42 53  27.2  23.7 -6.2     -75.0    -6   1  1   1198  No stop 
17 36 08  ---          03 44 23  27.4  23.7 -6.2     -75.4    84   F  1   1204  17 34 38

17 36 08  M82          03 44 23  27.5  23.1 -6.2     -75.6    -6   1  1   1204  No stop 
17 38 08  ---          03 46 23  27.7  23.1 -6.2     -76.0   114   F  1   1212  17 36 08

17 38 08  M81          03 46 23  27.5  23.8 -6.2     -75.8    -6   1  1   1212  No stop 
17 39 38  ---          03 47 54  27.7  23.8 -6.1     -76.1    84   F  1   1217  17 38 08

17 39 38  M82          03 47 54  27.8  23.1 -6.1     -76.4    -6   1  1   1217  No stop 
17 41 38  ---          03 49 54  28.0  23.2 -6.1     -76.8   114   F  1   1225  17 39 38

17 42 08  M81          03 50 24  27.9  23.9 -6.1     -76.7    24   1  1   1225  17 42 08
17 43 08  ---          03 51 24  28.0  23.9 -6.1     -76.9    60   F  1   1229  17 42 08

17 43 08  M82          03 51 24  28.1  23.2 -6.1     -77.2    -6   1  1   1229  No stop 
17 45 08  ---          03 53 24  28.3  23.3 -6.1     -77.6   114   F  1   1237  17 43 08

17 45 08  M81          03 53 24  28.1  24.0 -6.1     -77.4    -6   1  1   1237  No stop 
17 46 38  ---          03 54 55  28.3  24.0 -6.0     -77.7    84   F  1   1243  17 45 08

17 46 38  M82          03 54 55  28.4  23.3 -6.0     -77.9    -6   1  1   1243  No stop 
17 48 38  ---          03 56 55  28.6  23.3 -6.0     -78.4   114   F  1   1250  17 46 38

17 49 08  M81          03 57 25  28.5  24.0 -6.0     -78.3    24   1  1   1250  17 49 08
17 50 08  ---          03 58 25  28.6  24.1 -6.0     -78.5    60   F  1   1254  17 49 08

17 50 08  M82          03 58 25  28.7  23.4 -6.0     -78.7    -6   1  1   1254  No stop 
17 52 08  ---          04 00 26  28.9  23.4 -5.9     -79.2   114   F  1   1262  17 50 08

17 52 08  M81          04 00 26  28.8  24.1 -5.9     -78.9    -6   1  1   1262  No stop 
17 53 38  ---          04 01 56  28.9  24.1 -5.9     -79.3    84   F  1   1268  17 52 08

17 53 38  M82          04 01 56  29.0  23.4 -5.9     -79.5    -6   1  1   1268  No stop 
17 55 38  ---          04 03 56  29.2  23.5 -5.9     -80.0   114   F  1   1275  17 53 38

17 55 38  M81          04 03 56  29.1  24.2 -5.9     -79.7    -6   1  1   1275  No stop 
17 57 08  ---          04 05 26  29.2  24.2 -5.8     -80.1    84   F  1   1281  17 55 38
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

17 57 08  M82          04 05 26  29.3  23.5 -5.9     -80.3    -6   1  1   1281  No stop 
17 59 08  ---          04 07 27  29.5  23.5 -5.8     -80.8   114   F  1   1289  17 57 08

17 59 38  M81          04 07 57  29.4  24.2 -5.8     -80.6    24   1  1   1289  17 59 38
18 00 38  ---          04 08 57  29.5  24.3 -5.8     -80.8    60   F  1   1293  17 59 38

18 01 08  J1048+7143   04 09 27  25.9  20.1 -6.7     -70.4    17   1  1   1293  18 01 08
18 04 08  =1044+719    04 12 28  26.1  20.2 -6.6     -71.1   180   F  1   1304  18 01 08

18 04 08  M81          04 12 28  29.8  24.3 -5.7     -81.6   -13   1  1   1304  No stop 
18 06 08  ---          04 14 28  30.0  24.3 -5.7     -82.1   107   F  1   1312  18 04 08

18 06 08  M82          04 14 28  30.1  23.6 -5.7     -82.4    -6   1  1   1312  No stop 
18 08 08  ---          04 16 28  30.2  23.7 -5.7     -82.8   114   F  1   1320  18 06 08

18 08 08  M81          04 16 28  30.2  24.4 -5.7     -82.5    -6   1  1   1320  No stop 
18 09 38  ---          04 17 58  30.3  24.4 -5.6     -82.9    84   F  1   1326  18 08 08

18 09 38  M82          04 17 58  30.4  23.7 -5.6     -83.2    -6   1  1   1326  No stop 
18 11 38  ---          04 19 59  30.5  23.7 -5.6     -83.6   114   F  1   1333  18 09 38

18 12 08  M81          04 20 29  30.5  24.4 -5.6     -83.5    24   1  1   1333  18 12 08
18 13 08  ---          04 21 29  30.6  24.4 -5.6     -83.7    60   F  1   1337  18 12 08

18 13 08  M82          04 21 29  30.7  23.7 -5.6     -84.0    -6   1  1   1337  No stop 
18 15 08  ---          04 23 29  30.8  23.7 -5.6     -84.4   114   F  1   1345  18 13 08

18 15 08  M81          04 23 29  30.8  24.5 -5.5     -84.1    -6   1  1   1345  No stop 
18 16 38  ---          04 25 00  30.9  24.5 -5.5     -84.5    84   F  1   1351  18 15 08

18 16 38  M82          04 25 00  31.0  23.8 -5.5     -84.8    -6   1  1   1351  No stop 
18 18 38  ---          04 27 00  31.1  23.8 -5.5     -85.2   114   F  1   1359  18 16 38

18 18 38  M81          04 27 00  31.1  24.5 -5.5     -84.9    -6   1  1   1359  No stop 
18 20 08  ---          04 28 30  31.3  24.5 -5.5     -85.3    84   F  1   1364  18 18 38

18 20 08  M82          04 28 30  31.3  23.8 -5.5     -85.6    -6   1  1   1364  No stop 
18 22 08  ---          04 30 31  31.4  23.8 -5.4     -86.0   114   F  1   1372  18 20 08

18 22 38  M81          04 31 01  31.5  24.5 -5.4     -85.9    24   1  1   1372  18 22 38
18 23 38  ---          04 32 01  31.6  24.5 -5.4     -86.1    60   F  1   1376  18 22 38

18 23 38  M82          04 32 01  31.6  23.8 -5.4     -86.4    -6   1  1   1376  No stop 
18 25 38  ---          04 34 01  31.8  23.8 -5.4     -86.9   114   F  1   1384  18 23 38
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

18 25 38  M81          04 34 01  31.7  24.5 -5.4     -86.5    -6   1  1   1384  No stop 
18 27 08  ---          04 35 31  31.9  24.6 -5.3     -86.9    84   F  1   1390  18 25 38

18 27 08  M82          04 35 31  31.9  23.8 -5.4     -87.2    -6   1  1   1390  No stop 
18 29 08  ---          04 37 32  32.1  23.8 -5.3     -87.7   114   F  1   1397  18 27 08

18 29 38  M81          04 38 02  32.1  24.6 -5.3     -87.5    24   1  1   1397  18 29 38
18 30 38  ---          04 39 02  32.2  24.6 -5.3     -87.7    60   F  1   1401  18 29 38

18 30 38  M82          04 39 02  32.2  23.8 -5.3     -88.0    -6   1  1   1401  No stop 
18 32 38  ---          04 41 02  32.4  23.8 -5.3     -88.5   114   F  1   1409  18 30 38

18 32 38  M81          04 41 02  32.4  24.6 -5.3     -88.2    -6   1  1   1409  No stop 
18 34 08  ---          04 42 32  32.5  24.6 -5.2     -88.5    84   F  1   1415  18 32 38

18 34 08  M82          04 42 32  32.5  23.9 -5.2     -88.8    -6   1  1   1415  No stop 
18 36 08  ---          04 44 33  32.7  23.9 -5.2     -89.3   114   F  1   1422  18 34 08

18 36 08  M81          04 44 33  32.7  24.6 -5.2     -89.0    -6   1  1   1422  No stop 
18 37 38  ---          04 46 03  32.8  24.6 -5.2     -89.3    84   F  1   1428  18 36 08

18 37 38  M82          04 46 03  32.8  23.9 -5.2     -89.7    -6   1  1   1428  No stop 
18 39 38  ---          04 48 03  33.0  23.9 -5.1     -90.1   114   F  1   1436  18 37 38

18 40 08  M81          04 48 33  33.0  24.6 -5.1     -89.9    24   1  1   1436  18 40 08
18 41 08  ---          04 49 34  33.1  24.6 -5.1     -90.2    60   F  1   1440  18 40 08

18 41 08  M82          04 49 34  33.1  23.9 -5.1     -90.5    -6   1  1   1440  No stop 
18 43 08  ---          04 51 34  33.3  23.9 -5.1     -90.9   114   F  1   1448  18 41 08

18 43 08  M81          04 51 34  33.3  24.6 -5.1     -90.6    -6   1  1   1448  No stop 
18 44 38  ---          04 53 04  33.4  24.6 -5.1     -91.0    84   F  1   1453  18 43 08

18 44 38  M82          04 53 04  33.4  23.9 -5.1     -91.3    -6   1  1   1453  No stop 
18 46 38  ---          04 55 05  33.6  23.8 -5.0     -91.8   114   F  1   1461  18 44 38

18 47 08  M81          04 55 35  33.7  24.6 -5.0     -91.6    24   1  1   1461  18 47 08
18 48 08  ---          04 56 35  33.8  24.6 -5.0     -91.8    60   F  1   1465  18 47 08

18 48 08  M82          04 56 35  33.7  23.8 -5.0     -92.1    -6   1  1   1465  No stop 
18 50 08  ---          04 58 35  33.9  23.8 -5.0     -92.6   114   F  1   1473  18 48 08

18 50 08  M81          04 58 35  33.9  24.6 -5.0     -92.3    -6   1  1   1473  No stop 
18 51 38  ---          05 00 05  34.1  24.6 -4.9     -92.6    84   F  1   1479  18 50 08
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

18 51 38  M82          05 00 05  34.0  23.8 -4.9     -93.0    -6   1  1   1479  No stop 
18 53 38  ---          05 02 06  34.2  23.8 -4.9     -93.4   114   F  1   1486  18 51 38

18 53 38  M81          05 02 06  34.3  24.6 -4.9     -93.1    -6   1  1   1486  No stop 
18 55 08  ---          05 03 36  34.4  24.5 -4.9     -93.5    84   F  1   1492  18 53 38

18 55 08  M82          05 03 36  34.3  23.8 -4.9     -93.8    -6   1  1   1492  No stop 
18 57 08  ---          05 05 36  34.5  23.8 -4.9     -94.3   114   F  1   1500  18 55 08

18 57 38  M81          05 06 06  34.6  24.5 -4.8     -94.0    24   1  1   1500  18 57 38
18 58 38  ---          05 07 07  34.7  24.5 -4.8     -94.3    60   F  1   1504  18 57 38

18 59 08  J1048+7143   05 07 37  30.4  21.3 -5.7     -83.7    15   1  1   1504  18 59 08
19 02 08  =1044+719    05 10 37  30.6  21.3 -5.6     -84.4   180   F  1   1515  18 59 08

19 02 08  M81          05 10 37  35.0  24.5 -4.8     -95.1   -15   1  1   1515  No stop 
19 04 08  ---          05 12 37  35.2  24.5 -4.7     -95.6   105   F  1   1523  19 02 08

19 04 08  M82          05 12 37  35.1  23.7 -4.7     -96.0    -6   1  1   1523  No stop 
19 06 08  ---          05 14 38  35.3  23.7 -4.7     -96.4   114   F  1   1531  19 04 08

19 06 08  M81          05 14 38  35.4  24.4 -4.7     -96.1    -6   1  1   1531  No stop 
19 07 38  ---          05 16 08  35.5  24.4 -4.7     -96.4    84   F  1   1537  19 06 08

19 07 38  M82          05 16 08  35.4  23.7 -4.7     -96.8    -6   1  1   1537  No stop 
19 09 38  ---          05 18 08  35.6  23.7 -4.6     -97.3   114   F  1   1544  19 07 38

19 10 08  M81          05 18 38  35.7  24.4 -4.6     -97.1    24   1  1   1544  19 10 08
19 11 08  ---          05 19 39  35.8  24.4 -4.6     -97.3    60   F  1   1548  19 10 08

19 11 08  M82          05 19 39  35.7  23.6 -4.6     -97.7    -6   1  1   1548  No stop 
19 13 08  ---          05 21 39  35.9  23.6 -4.6     -98.1   114   F  1   1556  19 11 08

19 13 08  M81          05 21 39  36.0  24.3 -4.6     -97.8    -6   1  1   1556  No stop 
19 14 38  ---          05 23 09  36.1  24.3 -4.6     -98.1    84   F  1   1562  19 13 08

19 14 38  M82          05 23 09  36.0  23.6 -4.6     -98.5    -6   1  1   1562  No stop 
19 16 38  ---          05 25 09  36.2  23.5 -4.5     -99.0   114   F  1   1570  19 14 38

19 16 38  M81          05 25 09  36.3  24.3 -4.5     -98.6    -6   1  1   1570  No stop 
19 18 08  ---          05 26 40  36.4  24.3 -4.5     -99.0    84   F  1   1575  19 16 38

19 18 08  M82          05 26 40  36.3  23.5 -4.5     -99.4    -6   1  1   1575  No stop 
19 20 08  ---          05 28 40  36.5  23.5 -4.5     -99.9   114   F  1   1583  19 18 08
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

19 20 38  M81          05 29 10  36.7  24.2 -4.5     -99.6    24   1  1   1583  19 20 38
19 21 38  ---          05 30 10  36.8  24.2 -4.4     -99.9    60   F  1   1587  19 20 38

19 21 38  M82          05 30 10  36.6  23.5 -4.4    -100.2    -6   1  1   1587  No stop 
19 23 38  ---          05 32 11  36.8  23.4 -4.4    -100.7   114   F  1   1595  19 21 38

19 23 38  M81          05 32 11  36.9  24.2 -4.4    -100.3    -6   1  1   1595  No stop 
19 25 08  ---          05 33 41  37.1  24.1 -4.4    -100.7    84   F  1   1601  19 23 38

19 25 08  M82          05 33 41  36.9  23.4 -4.4    -101.1    -6   1  1   1601  No stop 
19 27 08  ---          05 35 41  37.1  23.3 -4.4    -101.6   114   F  1   1608  19 25 08

19 27 38  M81          05 36 11  37.3  24.1 -4.3    -101.3    24   1  1   1608  19 27 38
19 28 38  ---          05 37 11  37.4  24.1 -4.3    -101.6    60   F  1   1612  19 27 38

19 28 38  M82          05 37 11  37.2  23.3 -4.3    -102.0    -6   1  1   1612  No stop 
19 30 38  ---          05 39 12  37.4  23.3 -4.3    -102.5   114   F  1   1620  19 28 38

19 30 38  M81          05 39 12  37.5  24.0 -4.3    -102.1    -6   1  1   1620  No stop 
19 32 08  ---          05 40 42  37.7  24.0 -4.3    -102.5    84   F  1   1626  19 30 38

19 32 08  M82          05 40 42  37.5  23.2 -4.3    -102.8    -6   1  1   1626  No stop 
19 34 08  ---          05 42 42  37.7  23.2 -4.2    -103.3   114   F  1   1633  19 32 08

19 34 08  M81          05 42 42  37.9  23.9 -4.2    -102.9    -6   1  1   1633  No stop 
19 35 38  ---          05 44 13  38.0  23.9 -4.2    -103.3    84   F  1   1639  19 34 08

19 35 38  M82          05 44 13  37.8  23.1 -4.2    -103.7    -6   1  1   1639  No stop 
19 37 38  ---          05 46 13  38.0  23.1 -4.2    -104.2   114   F  1   1647  19 35 38

19 38 08  M81          05 46 43  38.2  23.8 -4.2    -104.0    24   1  1   1647  19 38 08
19 39 08  ---          05 47 43  38.3  23.8 -4.1    -104.2    60   F  1   1651  19 38 08

19 39 08  M82          05 47 43  38.1  23.0 -4.2    -104.6    -6   1  1   1651  No stop 
19 41 08  ---          05 49 43  38.3  23.0 -4.1    -105.1   114   F  1   1659  19 39 08

19 41 08  M81          05 49 43  38.5  23.7 -4.1    -104.7    -6   1  1   1659  No stop 
19 42 38  ---          05 51 14  38.6  23.7 -4.1    -105.1    84   F  1   1664  19 41 08

19 42 38  M82          05 51 14  38.4  22.9 -4.1    -105.5    -6   1  1   1664  No stop 
19 44 38  ---          05 53 14  38.6  22.9 -4.1    -106.0   114   F  1   1672  19 42 38

19 45 08  M81          05 53 44  38.8  23.6 -4.0    -105.7    24   1  1   1672  19 45 08
19 46 08  ---          05 54 44  38.9  23.6 -4.0    -106.0    60   F  1   1676  19 45 08
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

19 46 08  M82          05 54 44  38.7  22.8 -4.0    -106.4    -6   1  1   1676  No stop 
19 48 08  ---          05 56 45  38.9  22.8 -4.0    -106.9   114   F  1   1684  19 46 08

19 48 08  M81          05 56 45  39.1  23.5 -4.0    -106.5    -6   1  1   1684  No stop 
19 49 38  ---          05 58 15  39.2  23.5 -4.0    -106.9    84   F  1   1690  19 48 08

19 49 38  M82          05 58 15  39.0  22.7 -4.0    -107.3    -6   1  1   1690  No stop 
19 51 38  ---          06 00 15  39.2  22.7 -3.9    -107.8   114   F  1   1697  19 49 38

19 51 38  M81          06 00 15  39.4  23.4 -3.9    -107.4    -6   1  1   1697  No stop 
19 53 08  ---          06 01 45  39.5  23.3 -3.9    -107.8    84   F  1   1703  19 51 38

19 53 08  M82          06 01 45  39.3  22.6 -3.9    -108.2    -6   1  1   1703  No stop 
19 55 08  ---          06 03 46  39.4  22.5 -3.9    -108.7   114   F  1   1711  19 53 08

19 55 38  M81          06 04 16  39.7  23.3 -3.9    -108.4    24   1  1   1711  19 55 38
19 56 38  ---          06 05 16  39.8  23.2 -3.9    -108.7    60   F  1   1715  19 55 38

19 57 08  J1048+7143   06 05 46  34.9  21.2 -4.7     -97.5    14   1  1   1715  19 57 08
20 00 08  =1044+719    06 08 47  35.2  21.2 -4.7     -98.3   180   F  1   1726  19 57 08

20 00 08  M81          06 08 47  40.1  23.1 -3.8    -109.6   -16   1  1   1726  No stop 
20 02 08  ---          06 10 47  40.3  23.0 -3.8    -110.1   104   F  1   1734  20 00 08

20 02 08  M82          06 10 47  40.0  22.3 -3.8    -110.5    -6   1  1   1734  No stop 
20 04 08  ---          06 12 47  40.2  22.2 -3.7    -111.0   114   F  1   1742  20 02 08

20 04 08  M81          06 12 47  40.4  22.9 -3.7    -110.6    -6   1  1   1742  No stop 
20 05 38  ---          06 14 18  40.6  22.9 -3.7    -111.0    84   F  1   1748  20 04 08

20 05 38  M82          06 14 18  40.3  22.1 -3.7    -111.4    -6   1  1   1748  No stop 
20 07 38  ---          06 16 18  40.5  22.0 -3.7    -111.9   114   F  1   1755  20 05 38

20 08 08  M81          06 16 48  40.8  22.8 -3.7    -111.7    24   1  1   1755  20 08 08
20 09 08  ---          06 17 48  40.8  22.7 -3.6    -111.9    60   F  1   1759  20 08 08

20 09 08  M82          06 17 48  40.6  22.0 -3.6    -112.3    -6   1  1   1759  No stop 
20 11 08  ---          06 19 48  40.7  21.9 -3.6    -112.8   114   F  1   1767  20 09 08

20 11 08  M81          06 19 48  41.0  22.6 -3.6    -112.4    -6   1  1   1767  No stop 
20 12 38  ---          06 21 19  41.1  22.6 -3.6    -112.8    84   F  1   1773  20 11 08

20 12 38  M82          06 21 19  40.9  21.8 -3.6    -113.2    -6   1  1   1773  No stop 
20 14 38  ---          06 23 19  41.0  21.7 -3.6    -113.8   114   F  1   1781  20 12 38
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

20 14 38  M81          06 23 19  41.3  22.5 -3.6    -113.4    -6   1  1   1781  No stop 
20 16 08  ---          06 24 49  41.4  22.4 -3.5    -113.8    84   F  1   1786  20 14 38

20 16 08  M82          06 24 49  41.1  21.7 -3.5    -114.2    -6   1  1   1786  No stop 
20 18 08  ---          06 26 50  41.3  21.6 -3.5    -114.7   114   F  1   1794  20 16 08

20 18 38  M81          06 27 20  41.6  22.3 -3.5    -114.4    24   1  1   1794  20 18 38
20 19 38  ---          06 28 20  41.7  22.2 -3.5    -114.7    60   F  1   1798  20 18 38

20 19 38  M82          06 28 20  41.4  21.5 -3.5    -115.1    -6   1  1   1798  No stop 
20 21 38  ---          06 30 20  41.6  21.4 -3.4    -115.6   114   F  1   1806  20 19 38

20 21 38  M81          06 30 20  41.9  22.1 -3.4    -115.2    -6   1  1   1806  No stop 
20 23 08  ---          06 31 50  42.0  22.0 -3.4    -115.6    84   F  1   1811  20 21 38

20 23 08  M82          06 31 50  41.7  21.3 -3.4    -116.0    -6   1  1   1811  No stop 
20 25 08  ---          06 33 51  41.9  21.2 -3.4    -116.6   114   F  1   1819  20 23 08

20 25 38  M81          06 34 21  42.2  21.9 -3.4    -116.3    24   1  1   1819  20 25 38
20 26 38  ---          06 35 21  42.3  21.8 -3.4    -116.6    60   F  1   1823  20 25 38

20 26 38  M82          06 35 21  42.0  21.1 -3.4    -117.0    -6   1  1   1823  No stop 
20 28 38  ---          06 37 21  42.1  21.0 -3.3    -117.5   114   F  1   1831  20 26 38

20 28 38  M81          06 37 21  42.4  21.7 -3.3    -117.1    -6   1  1   1831  No stop 
20 30 08  ---          06 38 52  42.6  21.7 -3.3    -117.5    84   F  1   1837  20 28 38

20 30 08  M82          06 38 52  42.2  20.9 -3.3    -117.9    -6   1  1   1837  No stop 
20 32 08  ---          06 40 52  42.4  20.8 -3.3    -118.5   114   F  1   1844  20 30 08

20 32 08  M81          06 40 52  42.7  21.5 -3.3    -118.1    -6   1  1   1844  No stop 
20 33 38  ---          06 42 22  42.8  21.5 -3.2    -118.5    84   F  1   1850  20 32 08

20 33 38  M82          06 42 22  42.5  20.7 -3.2    -118.9    -6   1  1   1850  No stop 
20 35 38  ---          06 44 22  42.7  20.6 -3.2    -119.4   114   F  1   1858  20 33 38

20 36 08  M81          06 44 53  43.0  21.3 -3.2    -119.2    24   1  1   1858  20 36 08
20 37 08  ---          06 45 53  43.1  21.2 -3.2    -119.4    60   F  1   1862  20 36 08

20 37 08  M82          06 45 53  42.8  20.5 -3.2    -119.9    -6   1  1   1862  No stop 
20 39 08  ---          06 47 53  42.9  20.4 -3.1    -120.4   114   F  1   1870  20 37 08

20 39 08  M81          06 47 53  43.3  21.1 -3.1    -120.0    -6   1  1   1870  No stop 
20 40 38  ---          06 49 23  43.4  21.0 -3.1    -120.4    84   F  1   1875  20 39 08
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

20 40 38  M82          06 49 23  43.0  20.3 -3.1    -120.8    -6   1  1   1875  No stop 
20 42 38  ---          06 51 24  43.2  20.2 -3.1    -121.4   114   F  1   1883  20 40 38

20 43 08  M81          06 51 54  43.6  20.9 -3.1    -121.1    24   1  1   1883  20 43 08
20 44 08  ---          06 52 54  43.7  20.8 -3.1    -121.4    60   F  1   1887  20 43 08

20 44 08  M82          06 52 54  43.3  20.1 -3.1    -121.8    -6   1  1   1887  No stop 
20 46 08  ---          06 54 54  43.5  20.0 -3.0    -122.4   114   F  1   1895  20 44 08

20 46 08  M81          06 54 54  43.8  20.7 -3.0    -121.9    -6   1  1   1895  No stop 
20 47 38  ---          06 56 24  43.9  20.6 -3.0    -122.4    84   F  1   1901  20 46 08

20 47 38  M82          06 56 24  43.6  19.9 -3.0    -122.8    -6   1  1   1901  No stop 
20 49 38  ---          06 58 25  43.7  19.8 -3.0    -123.3   114   F  1   1908  20 47 38

20 49 38  M81          06 58 25  44.1  20.4 -3.0    -122.9    -6   1  1   1908  No stop 
20 51 08  ---          06 59 55  44.2  20.3 -2.9    -123.4    84   F  1   1914  20 49 38

20 51 08  M82          06 59 55  43.8  19.7 -2.9    -123.8    -6   1  1   1914  No stop 
20 53 08  ---          07 01 55  44.0  19.5 -2.9    -124.3   114   F  1   1922  20 51 08

20 53 38  M81          07 02 25  44.4  20.2 -2.9    -124.1    23   1  1   1922  20 53 38
20 54 38  ---          07 03 26  44.4  20.1 -2.9    -124.3    60   F  1   1926  20 53 38

20 55 08  J1048+7143   07 03 56  39.3  19.8 -3.8    -112.2    14   1  1   1926  20 55 08
20 58 08  =1044+719    07 06 56  39.5  19.7 -3.7    -113.0   180   F  1   1937  20 55 08

20 58 08  M81          07 06 56  44.7  19.8 -2.8    -125.3   -16   1  1   1937  No stop 
21 00 08  ---          07 08 56  44.8  19.7 -2.8    -125.9   104   F  1   1945  20 58 08

21 00 08  M82          07 08 56  44.5  19.0 -2.8    -126.3    -6   1  1   1945  No stop 
21 02 08  ---          07 10 57  44.6  18.9 -2.8    -126.9   114   F  1   1953  21 00 08

21 02 08  M81          07 10 57  45.0  19.5 -2.8    -126.5    -6   1  1   1953  No stop 
21 03 38  ---          07 12 27  45.1  19.4 -2.7    -126.9    84   F  1   1959  21 02 08

21 03 38  M82          07 12 27  44.7  18.8 -2.7    -127.3    -7   1  1   1959  No stop 
21 05 38  ---          07 14 27  44.8  18.6 -2.7    -127.9   113   F  1   1966  21 03 38

21 06 08  M81          07 14 57  45.3  19.2 -2.7    -127.6    23   1  1   1966  21 06 08
21 07 08  ---          07 15 58  45.3  19.2 -2.7    -127.9    60   F  1   1970  21 06 08

21 07 08  M82          07 15 58  44.9  18.5 -2.7    -128.3    -7   1  1   1970  No stop 
21 09 08  ---          07 17 58  45.1  18.3 -2.6    -128.9   113   F  1   1978  21 07 08
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

21 09 08  M81          07 17 58  45.5  19.0 -2.6    -128.5    -7   1  1   1978  No stop 
21 10 38  ---          07 19 28  45.6  18.9 -2.6    -128.9    83   F  1   1984  21 09 08

21 10 38  M82          07 19 28  45.2  18.2 -2.6    -129.3    -7   1  1   1984  No stop 
21 12 38  ---          07 21 29  45.3  18.1 -2.6    -129.9   113   F  1   1991  21 10 38

21 12 38  M81          07 21 29  45.7  18.7 -2.6    -129.5    -7   1  1   1991  No stop 
21 14 08  ---          07 22 59  45.8  18.6 -2.6    -130.0    83   F  1   1997  21 12 38

21 14 08  M82          07 22 59  45.4  18.0 -2.6    -130.4    -7   1  1   1997  No stop 
21 16 08  ---          07 24 59  45.6  17.8 -2.5    -130.9   113   F  1   2005  21 14 08

21 16 38  M81          07 25 29  46.0  18.4 -2.5    -130.7    23   1  1   2005  21 16 38
21 17 38  ---          07 26 29  46.1  18.3 -2.5    -131.0    60   F  1   2009  21 16 38

21 17 38  M82          07 26 29  45.7  17.7 -2.5    -131.4    -7   1  1   2009  No stop 
21 19 38  ---          07 28 30  45.8  17.5 -2.5    -132.0   113   F  1   2017  21 17 38

21 19 38  M81          07 28 30  46.2  18.1 -2.5    -131.6    -7   1  1   2017  No stop 
21 21 08  ---          07 30 00  46.3  18.0 -2.4    -132.0    83   F  1   2022  21 19 38

21 21 08  M82          07 30 00  45.9  17.4 -2.4    -132.4    -7   1  1   2022  No stop 
21 23 08  ---          07 32 00  46.0  17.2 -2.4    -133.0   113   F  1   2030  21 21 08

21 23 38  M81          07 32 30  46.5  17.8 -2.4    -132.8    23   1  1   2030  21 23 38
21 24 38  ---          07 33 30  46.5  17.7 -2.4    -133.1    60   F  1   2034  21 23 38

21 24 38  M82          07 33 30  46.1  17.1 -2.4    -133.5    -7   1  1   2034  No stop 
21 26 38  ---          07 35 31  46.2  16.9 -2.4    -134.0   113   F  1   2042  21 24 38

21 26 38  M81          07 35 31  46.7  17.5 -2.3    -133.7    -7   1  1   2042  No stop 
21 28 08  ---          07 37 01  46.8  17.4 -2.3    -134.1    83   F  1   2048  21 26 38

21 28 08  M82          07 37 01  46.3  16.8 -2.3    -134.5    -7   1  1   2048  No stop 
21 30 08  ---          07 39 01  46.4  16.6 -2.3    -135.1   113   F  1   2055  21 28 08

21 30 08  M81          07 39 01  46.9  17.2 -2.3    -134.7    -7   1  1   2055  No stop 
21 31 38  ---          07 40 32  47.0  17.1 -2.3    -135.2    83   F  1   2061  21 30 08

21 31 38  M82          07 40 32  46.5  16.5 -2.3    -135.5    -7   1  1   2061  No stop 
21 33 38  ---          07 42 32  46.7  16.3 -2.2    -136.1   113   F  1   2069  21 31 38

21 34 08  M81          07 43 02  47.2  16.8 -2.2    -135.9    23   1  1   2069  21 34 08
21 35 08  ---          07 44 02  47.2  16.7 -2.2    -136.2    60   F  1   2073  21 34 08
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2010   Day 158 ---

21 35 08  M82          07 44 02  46.7  16.1 -2.2    -136.6    -7   1  1   2073  No stop 
21 37 08  ---          07 46 03  46.9  15.9 -2.2    -137.2   113   F  1   2081  21 35 08

21 37 08  M81          07 46 03  47.3  16.5 -2.2    -136.9    -7   1  1   2081  No stop 
21 38 38  ---          07 47 33  47.4  16.4 -2.1    -137.3    83   F  1   2086  21 37 08

21 38 38  M82          07 47 33  47.0  15.8 -2.2    -137.7    -7   1  1   2086  No stop 
21 40 38  ---          07 49 33  47.1  15.6 -2.1    -138.3   113   F  1   2094  21 38 38

21 41 08  M81          07 50 03  47.6  16.1 -2.1    -138.1    23   1  1   2094  21 41 08
21 42 08  ---          07 51 03  47.6  16.0 -2.1    -138.4    60   F  1   2098  21 41 08

21 42 08  M82          07 51 03  47.2  15.5 -2.1    -138.7    -7   1  1   2098  No stop 
21 44 08  ---          07 53 04  47.3  15.3 -2.1    -139.3   113   F  1   2106  21 42 08

21 44 08  M81          07 53 04  47.8  15.8 -2.1    -139.0    -7   1  1   2106  No stop 
21 45 38  ---          07 54 34  47.8  15.7 -2.0    -139.5    83   F  1   2111  21 44 08

21 46 08  J1048+7143   07 55 04  42.8  17.2 -2.9    -126.1    14   1  1   2111  21 46 08
21 49 08  =1044+719    07 58 05  43.0  17.0 -2.9    -126.9   180   F  1   2123  21 46 08

21 51 54  4C39.25      08 00 51  70.4  58.9 -1.4    -108.6   105   1  1   2123  21 51 54
21 57 54  ---          08 06 52  71.5  57.7 -1.3    -110.7   360   F  1   2146  21 51 54


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gb071.18cm
   Matching groups in /aps3/sched9.3/catalogs/freq.dat:
     v20cm_2         FD filtered above 1760.  SC filtered above 1740.

   Setup group:   10         Station: VLBA_FD           Total bit rate:  512
   Format: VLBA1:4           Bits per sample: 1         Sample rate: 32.000
   Number of channels: 16                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
             2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
                   5         6         5         6         7         8         7         8
   BBC SB=         U         U         L         L         U         U         L         L
                   U         U         L         L         U         U         L         L
   IF    =        A         C         A         C         A         C         A         C 
                  A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   9  Setup file default.  Used pcal sets:   2
   LO sum=    1610.49   1610.49   1610.49   1610.49   1642.49   1642.49   1642.49   1642.49
              1674.49   1674.49   1674.49   1674.49   1706.49   1706.49   1706.49   1706.49
   BBC fr=     789.51    789.51    789.51    789.51    757.51    757.51    757.51    757.51
               725.51    725.51    725.51    725.51    693.51    693.51    693.51    693.51
   Bandwd=     16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000
               16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   2  PCAL = OFF 
    PCALXB1=   S1    S3    S5    S7    S9    S11   S13   S15
    PCALXB2=   S2    S4    S6    S8    S10   S12   S14   S16
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27, 66, 74, 82, 90, 67, 75, 83, 91
    barrel=roll_off 
 SOURCE LIST -- M82 transient (ToO)
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * M82               09 51 42.820698   * 09 55 51.551000     09 56 43.578732       0.00
                     69 54 59.52156    * 69 40 45.79200      69 37 59.17101        0.00
                     From catalog imbedded in main SCHED input file.
                        4.933 scan hours,    494.577 baseline hours above horizon.

   J0319+4130        03 16 29.567270   * 03 19 48.160100     03 20 29.296003       0.08
   0316+413          41 19 51.91596    * 41 30 42.10309      41 32 54.28698        0.06
 * 3C84              /aps3/sched9.3/catalogs/sources.vlba
   J0319+41          GSFC Nov. 2009 Solution 2009a     10149 Observations
                        0.100 scan hours,      5.740 baseline hours above horizon.

   J0927+3902        09 23 55.319215   * 09 27 03.013936     09 27 42.588260       0.01
   0923+392          39 15 23.56644    * 39 02 20.85184      38 59 42.50563        0.01
 * 4C39.25           /aps3/sched9.3/catalogs/sources.vlba
   J0927+39          GSFC Nov. 2009 Solution 2009a    226075 Observations
                        0.100 scan hours,     10.500 baseline hours above horizon.

   J0955+6903        09 51 27.310825   * 09 55 33.173069     09 56 24.628186       0.11
   0951+693          69 18 08.14426    * 69 03 55.06092      69 01 08.49288        0.03
 * M81               /aps3/sched9.3/catalogs/sources.vlba
                     GSFC Nov. 2009 Solution 2009a      2054 Observations
                        3.542 scan hours,    350.422 baseline hours above horizon.

 * J1048+7143        10 44 49.735104   * 10 48 27.619920     10 49 13.903814       0.02
   1044+719          71 59 26.88537    * 71 43 35.93840      71 40 29.78719        0.01
   J1048+71          /aps3/sched9.3/catalogs/sources.vlba
                     GSFC Nov. 2009 Solution 2009a    118344 Observations
                        0.567 scan hours,     59.202 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   M82                 63.0
   3C84                28.5
   4C39.25             57.8
   M81                 62.9
   J1048+7143          67.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

