  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
 Exp. Code:  gl039   


Schedule Version:       2.00
Processed by SCHED version:  11.30  Release of April 4, 2014

PI:       Andrei Lobanov

Address:  Max-Planck-Institut fuer Radioastronomie
          Auf dem Huegel 69
          53121 Bonn
          Germany

Phone:    +49 228 525 191
EMAIL:    alobanov@mpifr-bonn.mpg.de
Fax:      +49 228 525 229
Phone during observation:

Observing mode: Continuum

Notes:
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

 ---------- Block 05b: 05:15 -- 05:27. Fringe finder scan for EVN and VLBA ----------

 Next scan frequencies:  8351.25  8351.25  8383.25  8383.25  8415.25  8415.25  8447.25  8447.25
 Next BBC frequencies:    751.25   751.25   783.25   783.25   815.25   815.25   847.25   847.25
 Next scan bandwidths:     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00

05 15 00  3C345        15 04 37  67.9  58.8 -1.6    -106.8     0        0   05 15 00
05 27 00  ---          15 16 39  70.1  56.7 -1.4    -110.6   720       93   05 15 01

 ---------- Block 05c: 05:27 -- 05:54. Target/Phase reference scans for EVN & VLBA ----------

05 31 30  J2047-0236   15 21 10   5.8  96.4 -5.4     -58.9   134       93   05 31 30
05 33 00  =2044-027    15 22 40   6.1  96.6 -5.4     -58.8    90      104   05 31 31

05 33 40  AEAQR        15 23 20   8.7  96.1 -5.3     -58.8    27      104   05 33 40
05 36 30  ---          15 26 11   9.3  96.5 -5.2     -58.8   170      126   05 33 41

05 37 10  J2047-0236   15 26 51   7.0  97.2 -5.4     -58.7    27      126   05 37 10
05 38 00  =2044-027    15 27 41   7.2  97.3 -5.3     -58.7    50      133   05 37 11

05 38 40  AEAQR        15 28 21   9.8  96.8 -5.2     -58.7    27      133   05 38 40
05 41 30  ---          15 31 11  10.4  97.2 -5.2     -58.6   170      155   05 38 41

05 42 10  J2047-0236   15 31 52   8.1  97.8 -5.3     -58.6    27      155   05 42 10
05 43 00  =2044-027    15 32 42   8.3  98.0 -5.3     -58.5    50      161   05 42 11

05 43 40  AEAQR        15 33 22  10.8  97.5 -5.1     -58.6    27      161   05 43 40
05 46 30  ---          15 36 12  11.4  97.8 -5.1     -58.5   170      183   05 43 41

05 47 10  J2047-0236   15 36 52   9.2  98.5 -5.2     -58.4    27      183   05 47 10
05 48 00  =2044-027    15 37 43   9.3  98.6 -5.2     -58.4    50      189   05 47 11

05 48 40  AEAQR        15 38 23  11.9  98.1 -5.0     -58.4    27      189   05 48 40
05 51 30  ---          15 41 13  12.5  98.5 -5.0     -58.3   170      211   05 48 41

05 52 10  J2047-0236   15 41 53  10.2  99.2 -5.1     -58.2    27      211   05 52 10
05 53 00  =2044-027    15 42 43  10.4  99.3 -5.1     -58.2    50      218   05 52 11

 ---------- Block 06: 05:54 -- 06:30. Target/Phase reference scans for EVN/VLBA/JVLA ----------

05 54 30  J2050+0407   15 44 14  13.6  93.2 -5.1     -59.5    76      218   05 54 30
05 55 30  =2047+039    15 45 14  13.8  93.3 -5.1     -59.5    60      225   05 54 31

05 57 00  J2047-0236   15 46 44  11.3  99.8 -5.0     -58.1    76      225   05 57 00
05 58 00  =2044-027    15 47 44  11.5 100.0 -5.0     -58.0    60      233   05 57 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

05 58 40  AEAQR        15 48 24  14.0  99.5 -4.9     -58.1    27      233   05 58 40
06 01 30  ---          15 51 15  14.6  99.9 -4.8     -58.0   170      255   05 58 41

06 02 10  J2047-0236   15 51 55  12.4 100.5 -4.9     -57.9    27      255   06 02 10
06 03 00  =2044-027    15 52 45  12.5 100.6 -4.9     -57.8    50      262   06 02 11

06 03 40  AEAQR        15 53 25  15.1 100.2 -4.8     -57.9    27      262   06 03 40
06 06 30  ---          15 56 16  15.7 100.6 -4.7     -57.8   170      283   06 03 41

06 07 10  J2047-0236   15 56 56  13.4 101.2 -4.9     -57.7    27      283   06 07 10
06 08 00  =2044-027    15 57 46  13.6 101.3 -4.8     -57.6    50      290   06 07 11

06 08 40  AEAQR        15 58 26  16.1 100.9 -4.7     -57.7    27      290   06 08 40
06 11 30  ---          16 01 16  16.7 101.3 -4.7     -57.6   170      312   06 08 41

06 12 10  J2047-0236   16 01 56  14.5 101.9 -4.8     -57.4    27      312   06 12 10
06 13 00  =2044-027    16 02 47  14.6 102.0 -4.8     -57.4    50      318   06 12 11

06 14 30  J2050+0407   16 04 17  17.9  95.9 -4.8     -59.1    76      318   06 14 30
06 15 40  =2047+039    16 05 27  18.2  96.0 -4.8     -59.1    70      327   06 14 31

06 17 10  AEAQR        16 06 57  17.9 102.1 -4.6     -57.3    78      327   06 17 10
06 20 00  ---          16 09 48  18.5 102.5 -4.5     -57.2   170      349   06 17 11

06 20 40  J2047-0236   16 10 28  16.3 103.1 -4.6     -57.0    27      349   06 20 40
06 21 30  =2044-027    16 11 18  16.4 103.2 -4.6     -57.0    50      356   06 20 41

06 22 10  AEAQR        16 11 58  19.0 102.8 -4.5     -57.1    27      356   06 22 10
06 25 00  ---          16 14 49  19.6 103.2 -4.4     -56.9   170      377   06 22 11

06 25 40  J2047-0236   16 15 29  17.3 103.8 -4.5     -56.8    27      377   06 25 40
06 26 30  =2044-027    16 16 19  17.5 103.9 -4.5     -56.7    50      384   06 25 41

06 27 10  AEAQR        16 16 59  20.0 103.5 -4.4     -56.8    27      384   06 27 10
06 30 00  ---          16 19 49  20.6 103.9 -4.4     -56.6   170      406   06 27 11

 ---------- Block 07: 06:30 -- 08:00 ----------

06 31 30  J2050+0407   16 21 20  21.5  98.2 -4.5     -58.6    78      406   06 31 30
06 32 30  =2047+039    16 22 20  21.8  98.3 -4.5     -58.6    60      414   06 31 31

06 34 00  J2047-0236   16 23 50  19.1 105.0 -4.4     -56.3    76      414   06 34 00
06 35 00  =2044-027    16 24 50  19.3 105.2 -4.4     -56.2    60      421   06 34 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

06 35 40  AEAQR        16 25 30  21.8 104.8 -4.3     -56.3    27      421   06 35 40
06 38 30  ---          16 28 21  22.4 105.2 -4.2     -56.1   170      443   06 35 41

06 39 10  J2047-0236   16 29 01  20.1 105.8 -4.3     -56.0    27      443   06 39 10
06 40 00  =2044-027    16 29 51  20.3 105.9 -4.3     -55.9    50      450   06 39 11

06 41 30  J2050+0407   16 31 21  23.7  99.6 -4.3     -58.3    76      450   06 41 30
06 42 30  =2047+039    16 32 21  23.9  99.8 -4.3     -58.2    60      457   06 41 31

06 44 00  J2047-0236   16 33 52  21.1 106.5 -4.2     -55.7    76      457   06 44 00
06 45 00  =2044-027    16 34 52  21.3 106.7 -4.2     -55.6    60      465   06 44 01

06 45 40  AEAQR        16 35 32  23.9 106.3 -4.1     -55.7    27      465   06 45 40
06 48 30  ---          16 38 22  24.5 106.7 -4.0     -55.5   170      487   06 45 41

06 49 10  J2047-0236   16 39 03  22.2 107.3 -4.1     -55.3    27      487   06 49 10
06 50 00  =2044-027    16 39 53  22.4 107.4 -4.1     -55.3    50      493   06 49 11

06 51 30  J2050+0407   16 41 23  25.8 101.1 -4.2     -57.9    76      493   06 51 30
06 52 30  =2047+039    16 42 23  26.0 101.2 -4.1     -57.8    60      501   06 51 31

06 54 00  J2047-0236   16 43 53  23.2 108.1 -4.1     -55.0    76      501   06 54 00
06 55 00  =2044-027    16 44 54  23.4 108.2 -4.1     -54.9    60      509   06 54 01

06 55 40  AEAQR        16 45 34  26.0 107.9 -3.9     -55.0    27      509   06 55 40
06 58 30  ---          16 48 24  26.5 108.3 -3.9     -54.8   170      531   06 55 41

06 59 10  J2047-0236   16 49 04  24.2 108.9 -4.0     -54.6    27      531   06 59 10
07 00 00  =2044-027    16 49 54  24.4 109.0 -4.0     -54.5    50      537   06 59 11

07 01 30  J2050+0407   16 51 25  27.9 102.6 -4.0     -57.4    76      537   07 01 30
07 02 30  =2047+039    16 52 25  28.1 102.7 -4.0     -57.3    60      545   07 01 31

07 04 00  J2047-0236   16 53 55  25.2 109.6 -3.9     -54.2    76      545   07 04 00
07 05 00  =2044-027    16 54 55  25.4 109.8 -3.9     -54.1    60      553   07 04 01

07 05 40  AEAQR        16 55 35  28.0 109.5 -3.8     -54.2    27      553   07 05 40
07 08 30  ---          16 58 26  28.6 110.0 -3.7     -54.0   170      575   07 05 41

07 09 10  J2047-0236   16 59 06  26.3 110.5 -3.8     -53.8    27      575   07 09 10
07 10 00  =2044-027    16 59 56  26.4 110.6 -3.8     -53.7    50      581   07 09 11

07 11 30  J2050+0407   17 01 26  30.0 104.1 -3.8     -56.8    76      581   07 11 30
07 12 30  =2047+039    17 02 26  30.2 104.3 -3.8     -56.7    60      589   07 11 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

07 14 00  J2047-0236   17 03 57  27.3 111.3 -3.7     -53.4    76      589   07 14 00
07 15 00  =2044-027    17 04 57  27.5 111.5 -3.7     -53.3    60      596   07 14 01

07 15 40  AEAQR        17 05 37  30.0 111.2 -3.6     -53.4    27      596   07 15 40
07 18 30  ---          17 08 27  30.6 111.7 -3.5     -53.1   170      618   07 15 41

07 19 10  J2047-0236   17 09 07  28.3 112.2 -3.6     -52.9    27      618   07 19 10
07 20 00  =2044-027    17 09 58  28.5 112.3 -3.6     -52.8    50      625   07 19 11

07 21 30  J2050+0407   17 11 28  32.1 105.7 -3.7     -56.1    75      625   07 21 30
07 22 30  =2047+039    17 12 28  32.3 105.9 -3.6     -56.1    60      633   07 21 31

07 24 00  J2047-0236   17 13 58  29.2 113.0 -3.6     -52.4    75      633   07 24 00
07 25 00  =2044-027    17 14 58  29.4 113.2 -3.6     -52.3    60      640   07 24 01

07 25 40  AEAQR        17 15 39  32.0 113.0 -3.4     -52.4    27      640   07 25 40
07 28 30  ---          17 18 29  32.6 113.5 -3.4     -52.1   170      662   07 25 41

07 29 10  J2047-0236   17 19 09  30.3 113.9 -3.5     -51.9    27      662   07 29 10
07 30 00  =2044-027    17 19 59  30.4 114.1 -3.5     -51.8    50      669   07 29 11

07 31 30  J2050+0407   17 21 30  34.2 107.4 -3.5     -55.4    75      669   07 31 30
07 32 30  =2047+039    17 22 30  34.4 107.6 -3.5     -55.3    60      676   07 31 31

07 34 00  J2047-0236   17 24 00  31.2 114.8 -3.4     -51.4    75      676   07 34 00
07 35 00  =2044-027    17 25 00  31.4 115.0 -3.4     -51.3    60      684   07 34 01

07 35 40  AEAQR        17 25 40  34.0 114.8 -3.3     -51.4    27      684   07 35 40
07 38 30  ---          17 28 31  34.6 115.3 -3.2     -51.1   170      706   07 35 41

07 39 10  J2047-0236   17 29 11  32.2 115.7 -3.3     -50.9    27      706   07 39 10
07 40 00  =2044-027    17 30 01  32.4 115.9 -3.3     -50.8    50      712   07 39 11

07 41 30  J2050+0407   17 31 31  36.2 109.2 -3.3     -54.6    75      712   07 41 30
07 42 30  =2047+039    17 32 31  36.4 109.3 -3.3     -54.5    60      720   07 41 31

07 44 00  J2047-0236   17 34 02  33.2 116.7 -3.2     -50.3    75      720   07 44 00
07 45 00  =2044-027    17 35 02  33.4 116.9 -3.2     -50.2    60      728   07 44 01

07 45 40  AEAQR        17 35 42  35.9 116.7 -3.1     -50.2    27      728   07 45 40
07 48 30  ---          17 38 32  36.5 117.3 -3.0     -49.9   170      750   07 45 41

07 49 10  J2047-0236   17 39 12  34.2 117.7 -3.1     -49.7    27      750   07 49 10
07 50 00  =2044-027    17 40 03  34.3 117.8 -3.1     -49.6    50      756   07 49 11
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

07 51 30  J2050+0407   17 41 33  38.2 111.0 -3.2     -53.7    75      756   07 51 30
07 52 30  =2047+039    17 42 33  38.4 111.2 -3.1     -53.6    60      764   07 51 31

07 54 00  J2047-0236   17 44 03  35.1 118.6 -3.1     -49.1    75      764   07 54 00
07 55 00  =2044-027    17 45 03  35.3 118.8 -3.0     -49.0    60      772   07 54 01

07 55 40  AEAQR        17 45 43  37.9 118.8 -2.9     -49.0    27      772   07 55 40
07 58 30  ---          17 48 34  38.4 119.4 -2.9     -48.6   170      794   07 55 41

07 59 10  J2047-0236   17 49 14  36.0 119.7 -3.0     -48.5    27      794   07 59 10
08 00 00  =2044-027    17 50 04  36.2 119.8 -3.0     -48.3    50      800   07 59 11

 ---------- Block 08: 08:00 -- 09:00 ----------

08 01 30  J2050+0407   17 51 34  40.2 112.9 -3.0     -52.6    75      800   08 01 30
08 02 30  =2047+039    17 52 35  40.4 113.1 -3.0     -52.5    60      808   08 01 31

08 04 00  J2047-0236   17 54 05  36.9 120.7 -2.9     -47.8    75      808   08 04 00
08 05 00  =2044-027    17 55 05  37.1 120.9 -2.9     -47.7    60      815   08 04 01

08 05 40  AEAQR        17 55 45  39.7 120.9 -2.8     -47.6    27      815   08 05 40
08 08 20  ---          17 58 26  40.2 121.5 -2.7     -47.2   160      836   08 05 41

08 09 00  J2047-0236   17 59 06  37.9 121.7 -2.8     -47.1    27      836   08 09 00
08 09 50  =2044-027    17 59 56  38.0 121.9 -2.8     -47.0    50      842   08 09 01

08 10 20  J2050+0407   18 00 26  42.0 114.7 -2.8     -51.6    14      842   08 10 20
08 11 20  =2047+039    18 01 26  42.2 114.9 -2.8     -51.5    60      850   08 10 21

08 11 50  J2047-0236   18 01 56  38.4 122.4 -2.8     -46.7    14      850   08 11 50
08 12 50  =2044-027    18 02 56  38.6 122.6 -2.8     -46.5    60      858   08 11 51

08 13 10  AEAQR        18 03 16  41.1 122.6 -2.6     -46.5     7      858   08 13 10
08 15 50  ---          18 05 57  41.6 123.2 -2.6     -46.1   160      879   08 13 11

08 16 10  J2047-0236   18 06 17  39.2 123.3 -2.7     -46.0     7      879   08 16 10
08 17 00  =2044-027    18 07 07  39.3 123.5 -2.7     -45.9    50      885   08 16 11

08 17 30  J2050+0407   18 07 37  43.4 116.3 -2.7     -50.7    14      885   08 17 30
08 18 30  =2047+039    18 08 37  43.6 116.5 -2.7     -50.5    60      893   08 17 31

08 19 00  J2047-0236   18 09 07  39.7 124.0 -2.6     -45.6    14      893   08 19 00
08 20 00  =2044-027    18 10 07  39.9 124.2 -2.6     -45.4    60      900   08 19 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

08 20 20  AEAQR        18 10 28  42.4 124.3 -2.5     -45.3     7      900   08 20 20
08 23 00  ---          18 13 08  42.9 124.9 -2.5     -44.9   160      921   08 20 21

08 23 20  J2047-0236   18 13 28  40.5 125.0 -2.6     -44.9     7      921   08 23 20
08 24 10  =2044-027    18 14 18  40.6 125.1 -2.6     -44.8    50      927   08 23 21

08 24 40  J2050+0407   18 14 48  44.7 117.9 -2.6     -49.7    14      927   08 24 40
08 25 40  =2047+039    18 15 48  44.9 118.1 -2.6     -49.6    60      935   08 24 41

08 26 10  J2047-0236   18 16 18  41.0 125.6 -2.5     -44.4    14      935   08 26 10
08 27 10  =2044-027    18 17 19  41.1 125.9 -2.5     -44.3    60      943   08 26 11

08 27 30  AEAQR        18 17 39  43.7 126.0 -2.4     -44.1     7      943   08 27 30
08 30 10  ---          18 20 19  44.1 126.7 -2.3     -43.6   160      964   08 27 31

08 30 30  J2047-0236   18 20 39  41.7 126.7 -2.5     -43.7     7      964   08 30 30
08 31 20  =2044-027    18 21 29  41.9 126.9 -2.4     -43.6    50      970   08 30 31

08 31 50  J2050+0407   18 21 59  46.1 119.5 -2.5     -48.6    14      970   08 31 50
08 32 50  =2047+039    18 23 00  46.3 119.8 -2.5     -48.5    60      978   08 31 51

08 33 20  J2047-0236   18 23 30  42.2 127.3 -2.4     -43.2    14      978   08 33 20
08 34 20  =2044-027    18 24 30  42.4 127.6 -2.4     -43.0    60      985   08 33 21

08 34 40  AEAQR        18 24 50  44.9 127.8 -2.3     -42.8     7      985   08 34 40
08 37 20  ---          18 27 30  45.3 128.5 -2.2     -42.3   160     1006   08 34 41

08 37 40  J2047-0236   18 27 50  42.9 128.4 -2.3     -42.4     7     1006   08 37 40
08 38 30  =2044-027    18 28 41  43.1 128.6 -2.3     -42.3    50     1013   08 37 41

08 39 00  J2050+0407   18 29 11  47.4 121.3 -2.4     -47.5    14     1013   08 39 00
08 40 00  =2047+039    18 30 11  47.6 121.5 -2.3     -47.3    60     1020   08 39 01

08 40 30  J2047-0236   18 30 41  43.4 129.2 -2.3     -41.9    14     1020   08 40 30
08 41 30  =2044-027    18 31 41  43.6 129.4 -2.3     -41.7    60     1028   08 40 31

08 41 50  AEAQR        18 32 01  46.1 129.7 -2.1     -41.4     7     1028   08 41 50
08 44 30  ---          18 34 42  46.5 130.5 -2.1     -40.9   160     1049   08 41 51

08 44 50  J2047-0236   18 35 02  44.1 130.3 -2.2     -41.1     7     1049   08 44 50
08 45 40  =2044-027    18 35 52  44.3 130.5 -2.2     -40.9    50     1055   08 44 51

08 46 10  J2050+0407   18 36 22  48.7 123.1 -2.2     -46.3    13     1055   08 46 10
08 47 10  =2047+039    18 37 22  48.9 123.4 -2.2     -46.1    60     1063   08 46 11
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

08 47 40  J2047-0236   18 37 52  44.6 131.0 -2.2     -40.5    13     1063   08 47 40
08 48 40  =2044-027    18 38 52  44.8 131.3 -2.2     -40.3    60     1070   08 47 41

08 49 00  AEAQR        18 39 12  47.3 131.7 -2.0     -40.0     7     1070   08 49 00
08 51 40  ---          18 41 53  47.7 132.5 -2.0     -39.4   160     1091   08 49 01

08 52 00  J2047-0236   18 42 13  45.3 132.2 -2.1     -39.6     7     1091   08 52 00
08 52 50  =2044-027    18 43 03  45.4 132.4 -2.1     -39.5    50     1098   08 52 01

08 53 20  J2050+0407   18 43 33  50.0 125.0 -2.1     -44.9    13     1098   08 53 20
08 54 20  =2047+039    18 44 33  50.2 125.3 -2.1     -44.7    60     1105   08 53 21

08 54 50  J2047-0236   18 45 03  45.7 133.0 -2.0     -39.1    13     1105   08 54 50
08 55 50  =2044-027    18 46 03  45.9 133.3 -2.0     -38.8    60     1113   08 54 51

08 56 10  AEAQR        18 46 23  48.4 133.8 -1.9     -38.4     7     1113   08 56 10
08 58 50  ---          18 49 04  48.8 134.6 -1.9     -37.8   160     1134   08 56 11

08 59 10  J2047-0236   18 49 24  46.4 134.2 -2.0     -38.1     7     1134   08 59 10
09 00 00  =2044-027    18 50 14  46.5 134.4 -2.0     -37.9    50     1140   08 59 11

 ---------- Block 09: 09:00 -- 14:00 ----------

09 00 30  J2050+0407   18 50 44  51.3 127.1 -2.0     -43.5    13     1140   09 00 30
09 01 30  =2047+039    18 51 44  51.4 127.4 -2.0     -43.3    60     1148   09 00 31

09 02 00  J2047-0236   18 52 14  46.9 135.0 -1.9     -37.5    13     1148   09 02 00
09 03 00  =2044-027    18 53 15  47.0 135.3 -1.9     -37.3    60     1156   09 02 01

09 03 20  AEAQR        18 53 35  49.5 136.0 -1.8     -36.7     7     1156   09 03 20
09 06 10  ---          18 56 25  49.9 136.8 -1.7     -36.1   170     1177   09 03 21

09 06 30  J2047-0236   18 56 45  47.5 136.3 -1.9     -36.5     7     1177   09 06 30
09 07 20  =2044-027    18 57 35  47.7 136.6 -1.8     -36.3    50     1184   09 06 31

09 07 50  J2050+0407   18 58 05  52.5 129.2 -1.9     -41.9    13     1184   09 07 50
09 08 50  =2047+039    18 59 06  52.7 129.6 -1.9     -41.7    60     1192   09 07 51

09 09 20  J2047-0236   18 59 36  48.0 137.2 -1.8     -35.8    13     1192   09 09 20
09 10 20  =2044-027    19 00 36  48.1 137.5 -1.8     -35.6    60     1199   09 09 21

09 10 40  AEAQR        19 00 56  50.6 138.3 -1.7     -34.9     7     1199   09 10 40
09 13 30  ---          19 03 46  51.0 139.2 -1.6     -34.2   170     1221   09 10 41
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

09 13 50  J2047-0236   19 04 06  48.6 138.6 -1.7     -34.7     7     1221   09 13 50
09 14 40  =2044-027    19 04 56  48.7 138.8 -1.7     -34.5    50     1228   09 13 51

09 15 10  J2050+0407   19 05 27  53.7 131.6 -1.8     -40.2    12     1228   09 15 10
09 16 10  =2047+039    19 06 27  53.9 131.9 -1.7     -40.0    60     1235   09 15 11

09 16 40  J2047-0236   19 06 57  49.0 139.5 -1.7     -34.0    12     1235   09 16 40
09 17 40  =2044-027    19 07 57  49.1 139.8 -1.7     -33.8    60     1243   09 16 41

09 18 00  AEAQR        19 08 17  51.6 140.7 -1.5     -33.0     7     1243   09 18 00
09 20 50  ---          19 11 07  52.0 141.7 -1.5     -32.3   170     1265   09 18 01

09 21 10  J2047-0236   19 11 28  49.6 140.9 -1.6     -32.9     7     1265   09 21 10
09 22 00  =2044-027    19 12 18  49.7 141.2 -1.6     -32.7    50     1271   09 21 11

09 22 30  J2050+0407   19 12 48  54.9 134.0 -1.6     -38.4    12     1271   09 22 30
09 23 30  =2047+039    19 13 48  55.0 134.3 -1.6     -38.1    60     1279   09 22 31

09 24 00  J2047-0236   19 14 18  50.0 141.8 -1.6     -32.2    12     1279   09 24 00
09 25 00  =2044-027    19 15 18  50.1 142.2 -1.5     -31.9    60     1287   09 24 01

09 25 20  AEAQR        19 15 38  52.6 143.2 -1.4     -31.0     7     1287   09 25 20
09 28 10  ---          19 18 29  52.9 144.2 -1.4     -30.2   170     1309   09 25 21

09 28 30  J2047-0236   19 18 49  50.6 143.3 -1.5     -30.9     7     1309   09 28 30
09 29 20  =2044-027    19 19 39  50.7 143.6 -1.5     -30.7    50     1315   09 28 31

09 29 50  J2050+0407   19 20 09  56.0 136.6 -1.5     -36.4    12     1315   09 29 50
09 30 50  =2047+039    19 21 09  56.1 136.9 -1.5     -36.1    60     1323   09 29 51

09 31 20  J2047-0236   19 21 39  51.0 144.3 -1.4     -30.2    12     1323   09 31 20
09 32 20  =2044-027    19 22 39  51.1 144.7 -1.4     -29.9    60     1331   09 31 21

09 32 40  AEAQR        19 22 59  53.5 145.9 -1.3     -28.9     7     1331   09 32 40
09 35 30  ---          19 25 50  53.8 146.9 -1.3     -28.0   170     1353   09 32 41

09 35 50  J2047-0236   19 26 10  51.5 145.9 -1.4     -28.9     7     1353   09 35 50
09 36 40  =2044-027    19 27 00  51.6 146.2 -1.3     -28.7    50     1359   09 35 51

09 37 10  J2050+0407   19 27 30  57.1 139.3 -1.4     -34.3    11     1359   09 37 10
09 38 10  =2047+039    19 28 30  57.2 139.6 -1.4     -34.0    60     1367   09 37 11

09 38 40  J2047-0236   19 29 00  51.8 146.9 -1.3     -28.1    11     1367   09 38 40
09 39 40  =2044-027    19 30 01  52.0 147.2 -1.3     -27.8    60     1375   09 38 41
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

09 40 00  AEAQR        19 30 21  54.3 148.6 -1.2     -26.6     7     1375   09 40 00
09 42 50  ---          19 33 11  54.7 149.7 -1.1     -25.7   170     1396   09 40 01

09 43 10  J2047-0236   19 33 31  52.4 148.5 -1.2     -26.7     7     1396   09 43 10
09 44 00  =2044-027    19 34 21  52.5 148.8 -1.2     -26.5    50     1403   09 43 11

09 44 30  J2050+0407   19 34 51  58.1 142.1 -1.3     -32.0    11     1403   09 44 30
09 45 30  =2047+039    19 35 52  58.2 142.5 -1.3     -31.7    60     1411   09 44 31

09 46 00  J2047-0236   19 36 22  52.7 149.6 -1.2     -25.9    11     1411   09 46 00
09 47 00  =2044-027    19 37 22  52.8 149.9 -1.2     -25.6    60     1418   09 46 01

09 47 20  AEAQR        19 37 42  55.1 151.5 -1.1     -24.2     7     1418   09 47 20
09 50 10  ---          19 40 32  55.4 152.7 -1.0     -23.3   170     1440   09 47 21

09 50 30  J2047-0236   19 40 52  53.2 151.2 -1.1     -24.5     7     1440   09 50 30
09 51 20  =2044-027    19 41 42  53.2 151.6 -1.1     -24.2    50     1447   09 50 31

09 51 50  J2050+0407   19 42 13  59.0 145.1 -1.1     -29.5    11     1447   09 51 50
09 52 50  =2047+039    19 43 13  59.1 145.6 -1.1     -29.2    60     1454   09 51 51

09 53 20  J2047-0236   19 43 43  53.5 152.3 -1.1     -23.6    11     1454   09 53 20
09 54 20  =2044-027    19 44 43  53.6 152.7 -1.1     -23.3    60     1462   09 53 21

09 54 40  AEAQR        19 45 03  55.9 154.5 -0.9     -21.7     7     1462   09 54 40
09 57 30  ---          19 47 54  56.1 155.7 -0.9     -20.7   170     1484   09 54 41

09 57 50  J2047-0236   19 48 14  53.9 154.1 -1.0     -22.1     8     1484   09 57 50
09 58 40  =2044-027    19 49 04  54.0 154.4 -1.0     -21.8    50     1490   09 57 51

09 59 10  J2050+0407   19 49 34  59.9 148.3 -1.0     -26.9    10     1490   09 59 10
10 00 10  =2047+039    19 50 34  60.0 148.8 -1.0     -26.6    60     1498   09 59 11

10 00 40  J2047-0236   19 51 04  54.2 155.2 -0.9     -21.2    10     1498   10 00 40
10 01 40  =2044-027    19 52 04  54.2 155.6 -0.9     -20.8    60     1506   10 00 41

10 02 00  AEAQR        19 52 24  56.5 157.6 -0.8     -19.1     8     1506   10 02 00
10 04 50  ---          19 55 15  56.7 158.8 -0.8     -18.1   170     1528   10 02 01

10 05 10  J2047-0236   19 55 35  54.5 157.0 -0.9     -19.6     8     1528   10 05 10
10 06 00  =2044-027    19 56 25  54.6 157.4 -0.9     -19.4    50     1534   10 05 11

10 06 30  J2050+0407   19 56 55  60.7 151.7 -0.9     -24.2    10     1534   10 06 30
10 07 30  =2047+039    19 57 55  60.8 152.1 -0.9     -23.8    60     1542   10 06 31
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

10 08 00  J2047-0236   19 58 25  54.8 158.2 -0.8     -18.7    10     1542   10 08 00
10 09 00  =2044-027    19 59 25  54.9 158.6 -0.8     -18.3    60     1550   10 08 01

10 09 20  AEAQR        19 59 45  57.1 160.8 -0.7     -16.4     8     1550   10 09 20
10 12 10  ---          20 02 36  57.3 162.1 -0.6     -15.4   170     1572   10 09 21

10 12 30  J2047-0236   20 02 56  55.1 160.0 -0.8     -17.1     8     1572   10 12 30
10 13 20  =2044-027    20 03 46  55.2 160.4 -0.7     -16.8    50     1578   10 12 31

10 13 50  J2050+0407   20 04 16  61.4 155.1 -0.8     -21.3    10     1578   10 13 50
10 14 50  =2047+039    20 05 16  61.5 155.6 -0.8     -20.9    60     1586   10 13 51

10 15 20  J2047-0236   20 05 46  55.3 161.2 -0.7     -16.1    10     1586   10 15 20
10 16 20  =2044-027    20 06 47  55.4 161.7 -0.7     -15.7    60     1593   10 15 21

10 16 40  AEAQR        20 07 07  57.5 164.1 -0.6     -13.6     8     1593   10 16 40
10 19 30  ---          20 09 57  57.7 165.4 -0.5     -12.5   170     1615   10 16 41

10 19 50  J2047-0236   20 10 17  55.6 163.2 -0.6     -14.5     8     1615   10 19 50
10 20 40  =2044-027    20 11 07  55.7 163.5 -0.6     -14.1    50     1622   10 19 51

10 21 10  J2050+0407   20 11 37  62.0 158.8 -0.7     -18.2    10     1622   10 21 10
10 22 10  =2047+039    20 12 38  62.1 159.3 -0.6     -17.8    60     1630   10 21 11

10 22 40  J2047-0236   20 13 08  55.8 164.4 -0.6     -13.4    10     1630   10 22 40
10 23 40  =2044-027    20 14 08  55.9 164.8 -0.6     -13.0    60     1637   10 22 41

10 24 00  AEAQR        20 14 28  57.9 167.5 -0.4     -10.8     8     1637   10 24 00
10 26 50  ---          20 17 18  58.1 168.8 -0.4      -9.6   170     1659   10 24 01

10 27 10  J2047-0236   20 17 38  56.0 166.3 -0.5     -11.7     8     1659   10 27 10
10 28 00  =2044-027    20 18 29  56.1 166.7 -0.5     -11.4    50     1666   10 27 11

10 28 30  J2050+0407   20 18 59  62.5 162.6 -0.5     -15.0     9     1666   10 28 30
10 29 30  =2047+039    20 19 59  62.6 163.1 -0.5     -14.5    60     1673   10 28 31

10 30 00  J2047-0236   20 20 29  56.2 167.6 -0.5     -10.7     9     1673   10 30 00
10 31 00  =2044-027    20 21 29  56.2 168.0 -0.4     -10.3    60     1681   10 30 01

10 31 20  AEAQR        20 21 49  58.2 170.9 -0.3      -7.8     8     1681   10 31 20
10 34 10  ---          20 24 40  58.3 172.2 -0.3      -6.7   170     1703   10 31 21

10 34 30  J2047-0236   20 25 00  56.4 169.6 -0.4      -9.0     8     1703   10 34 30
10 35 20  =2044-027    20 25 50  56.4 170.0 -0.4      -8.6    50     1709   10 34 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

10 35 50  J2050+0407   20 26 20  62.9 166.4 -0.4     -11.7     9     1709   10 35 50
10 36 50  =2047+039    20 27 20  63.0 167.0 -0.4     -11.2    60     1717   10 35 51

10 37 20  J2047-0236   20 27 50  56.5 170.9 -0.3      -7.9     9     1717   10 37 20
10 38 20  =2044-027    20 28 50  56.5 171.3 -0.3      -7.5    60     1725   10 37 21

10 38 40  AEAQR        20 29 10  58.4 174.4 -0.2      -4.8     8     1725   10 38 40
10 41 30  ---          20 32 01  58.5 175.7 -0.1      -3.7   170     1747   10 38 41

10 41 50  J2047-0236   20 32 21  56.6 172.9 -0.3      -6.1     8     1747   10 41 50
10 42 40  =2044-027    20 33 11  56.6 173.3 -0.2      -5.8    50     1753   10 41 51

10 43 10  J2050+0407   20 33 41  63.2 170.4 -0.3      -8.2     9     1753   10 43 10
10 44 10  =2047+039    20 34 41  63.3 171.0 -0.3      -7.8    60     1761   10 43 11

10 44 40  J2047-0236   20 35 11  56.7 174.2 -0.2      -5.0     9     1761   10 44 40
10 45 40  =2044-027    20 36 11  56.7 174.6 -0.2      -4.6    60     1769   10 44 41

10 46 00  AEAQR        20 36 31  58.5 177.9 -0.1      -1.8     8     1769   10 46 00
10 48 50  ---          20 39 22  58.5 179.2 -0.0      -0.7   170     1791   10 46 01

10 49 10  J2047-0236   20 39 42  56.8 176.2 -0.1      -3.3     8     1791   10 49 10
10 50 00  =2044-027    20 40 32  56.8 176.6 -0.1      -2.9    50     1797   10 49 11

10 50 30  J2050+0407   20 41 02  63.5 174.5 -0.2      -4.7     9     1797   10 50 30
10 51 30  =2047+039    20 42 02  63.5 175.1 -0.1      -4.3    60     1805   10 50 31

10 52 00  J2047-0236   20 42 32  56.8 177.5 -0.1      -2.1     9     1805   10 52 00
10 53 00  =2044-027    20 43 33  56.8 178.0 -0.1      -1.7    60     1812   10 52 01

10 53 20  AEAQR        20 43 53  58.5 181.4  0.0       1.2     9     1812   10 53 20
10 56 10  ---          20 46 43  58.5 182.8  0.1       2.4   170     1834   10 53 21

10 56 30  J2047-0236   20 47 03  56.8 179.6 -0.0      -0.4     9     1834   10 56 30
10 57 20  =2044-027    20 47 53  56.8 180.0 -0.0      -0.0    50     1841   10 56 31

10 57 50  J2050+0407   20 48 23  63.5 178.6 -0.0      -1.2     9     1841   10 57 50
10 58 50  =2047+039    20 49 24  63.6 179.2 -0.0      -0.7    60     1849   10 57 51

10 59 20  J2047-0236   20 49 54  56.8 180.9  0.0       0.7     9     1849   10 59 20
11 00 20  =2044-027    20 50 54  56.8 181.3  0.0       1.1    60     1856   10 59 21

11 00 40  AEAQR        20 51 14  58.5 184.9  0.2       4.2     9     1856   11 00 40
11 03 30  ---          20 54 04  58.4 186.3  0.2       5.4   170     1878   11 00 41
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

11 03 50  J2047-0236   20 54 24  56.8 182.9  0.1       2.5     9     1878   11 03 50
11 04 40  =2044-027    20 55 15  56.8 183.3  0.1       2.8    50     1885   11 03 51

11 05 10  J2050+0407   20 55 45  63.5 182.7  0.1       2.3     9     1885   11 05 10
11 06 10  =2047+039    20 56 45  63.5 183.3  0.1       2.8    60     1892   11 05 11

11 06 40  J2047-0236   20 57 15  56.7 184.2  0.2       3.6     9     1892   11 06 40
11 07 40  =2044-027    20 58 15  56.7 184.7  0.2       4.0    60     1900   11 06 41

11 08 00  AEAQR        20 58 35  58.3 188.4  0.3       7.2     9     1900   11 08 00
11 10 50  ---          21 01 26  58.2 189.7  0.3       8.4   170     1922   11 08 01

11 11 10  J2047-0236   21 01 46  56.7 186.3  0.2       5.4     9     1922   11 11 10
11 12 00  =2044-027    21 02 36  56.6 186.6  0.2       5.7    50     1928   11 11 11

11 12 30  J2050+0407   21 03 06  63.4 186.8  0.2       5.9     9     1928   11 12 30
11 13 30  =2047+039    21 04 06  63.4 187.4  0.2       6.3    60     1936   11 12 31

11 14 00  J2047-0236   21 04 36  56.6 187.5  0.3       6.5     9     1936   11 14 00
11 15 00  =2044-027    21 05 36  56.6 188.0  0.3       6.9    60     1944   11 14 01

11 15 20  AEAQR        21 05 56  58.0 191.8  0.4      10.2     9     1944   11 15 20
11 18 10  ---          21 08 47  57.9 193.2  0.5      11.3   170     1966   11 15 21

11 18 30  J2047-0236   21 09 07  56.4 189.6  0.4       8.2     9     1966   11 18 30
11 19 20  =2044-027    21 09 57  56.4 189.9  0.4       8.6    50     1972   11 18 31

11 19 50  J2050+0407   21 10 27  63.2 190.9  0.3       9.3     9     1972   11 19 50
11 20 50  =2047+039    21 11 27  63.1 191.4  0.3       9.8    60     1980   11 19 51

11 21 20  J2047-0236   21 11 57  56.3 190.8  0.4       9.3     9     1980   11 21 20
11 22 20  =2044-027    21 12 57  56.3 191.3  0.4       9.7    60     1988   11 21 21

11 22 40  AEAQR        21 13 17  57.6 195.2  0.5      13.1     9     1988   11 22 40
11 25 30  ---          21 16 08  57.5 196.5  0.6      14.2   170     2010   11 22 41

11 25 50  J2047-0236   21 16 28  56.1 192.8  0.5      11.0     9     2010   11 25 50
11 26 40  =2044-027    21 17 18  56.1 193.2  0.5      11.3    50     2016   11 25 51

11 27 10  J2050+0407   21 17 48  62.8 194.8  0.4      12.7     9     2016   11 27 10
11 28 10  =2047+039    21 18 48  62.7 195.3  0.5      13.2    60     2024   11 27 11

11 28 40  J2047-0236   21 19 18  56.0 194.1  0.5      12.1     9     2024   11 28 40
11 29 40  =2044-027    21 20 19  55.9 194.5  0.5      12.5    60     2031   11 28 41
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

11 30 00  AEAQR        21 20 39  57.2 198.5  0.7      15.9     9     2031   11 30 00
11 32 50  ---          21 23 29  57.0 199.8  0.7      16.9   170     2053   11 30 01

11 33 10  J2047-0236   21 23 49  55.7 196.0  0.6      13.8     9     2053   11 33 10
11 34 00  =2044-027    21 24 39  55.7 196.4  0.6      14.1    50     2060   11 33 11

11 34 30  J2050+0407   21 25 09  62.3 198.7  0.6      16.0     9     2060   11 34 30
11 35 30  =2047+039    21 26 10  62.3 199.2  0.6      16.5    60     2068   11 34 31

11 36 00  J2047-0236   21 26 40  55.6 197.3  0.6      14.8     9     2068   11 36 00
11 37 00  =2044-027    21 27 40  55.5 197.7  0.7      15.2    60     2075   11 36 01

11 37 20  AEAQR        21 28 00  56.6 201.7  0.8      18.6     9     2075   11 37 20
11 40 10  ---          21 30 50  56.4 203.0  0.8      19.6   170     2097   11 37 21

11 40 30  J2047-0236   21 31 10  55.3 199.2  0.7      16.4     9     2097   11 40 30
11 41 20  =2044-027    21 32 01  55.2 199.5  0.7      16.7    50     2104   11 40 31

11 41 50  J2050+0407   21 32 31  61.8 202.4  0.7      19.2     9     2104   11 41 50
11 42 50  =2047+039    21 33 31  61.7 202.9  0.7      19.6    60     2111   11 41 51

11 43 20  J2047-0236   21 34 01  55.1 200.4  0.8      17.4     9     2111   11 43 20
11 44 20  =2044-027    21 35 01  55.0 200.8  0.8      17.8    60     2119   11 43 21

11 44 40  AEAQR        21 35 21  56.0 204.9  0.9      21.2     9     2119   11 44 40
11 47 30  ---          21 38 12  55.7 206.0  1.0      22.2   170     2141   11 44 41

11 47 50  J2047-0236   21 38 32  54.7 202.2  0.8      19.0     9     2141   11 47 50
11 48 40  =2044-027    21 39 22  54.6 202.6  0.9      19.3    50     2147   11 47 51

11 49 10  J2050+0407   21 39 52  61.1 206.0  0.8      22.2     9     2147   11 49 10
11 50 10  =2047+039    21 40 52  61.0 206.5  0.8      22.6    60     2155   11 49 11

11 50 40  J2047-0236   21 41 22  54.5 203.4  0.9      20.0     9     2155   11 50 40
11 51 40  =2044-027    21 42 22  54.4 203.8  0.9      20.3    60     2163   11 50 41

11 52 00  AEAQR        21 42 42  55.3 207.9  1.0      23.7     9     2163   11 52 00
11 54 50  ---          21 45 33  55.0 209.0  1.1      24.7   170     2185   11 52 01

11 55 10  J2047-0236   21 45 53  54.1 205.2  1.0      21.5     9     2185   11 55 10
11 56 00  =2044-027    21 46 43  54.0 205.5  1.0      21.8    50     2191   11 55 11

11 56 30  J2050+0407   21 47 13  60.4 209.4  0.9      25.1     9     2191   11 56 30
11 57 30  =2047+039    21 48 13  60.3 209.9  1.0      25.5    60     2199   11 56 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

11 58 00  J2047-0236   21 48 43  53.8 206.3  1.0      22.4     9     2199   11 58 00
11 59 00  =2044-027    21 49 43  53.7 206.7  1.0      22.8    60     2207   11 58 01

11 59 20  AEAQR        21 50 04  54.5 210.8  1.2      26.1     9     2207   11 59 20
12 02 10  ---          21 52 54  54.2 211.9  1.2      27.0   170     2229   11 59 21

12 02 30  J2047-0236   21 53 14  53.4 208.0  1.1      23.9     9     2229   12 02 30
12 03 20  =2044-027    21 54 04  53.3 208.4  1.1      24.1    50     2235   12 02 31

12 03 50  J2050+0407   21 54 34  59.6 212.7  1.1      27.8     9     2235   12 03 50
12 04 50  =2047+039    21 55 34  59.5 213.2  1.1      28.2    60     2243   12 03 51

12 05 20  J2047-0236   21 56 05  53.1 209.1  1.1      24.8     9     2243   12 05 20
12 06 20  =2044-027    21 57 05  53.0 209.5  1.2      25.1    60     2250   12 05 21

12 06 40  AEAQR        21 57 25  53.7 213.6  1.3      28.4     9     2250   12 06 40
12 09 30  ---          22 00 15  53.3 214.6  1.3      29.3   170     2272   12 06 41

12 09 50  J2047-0236   22 00 35  52.6 210.8  1.2      26.2     9     2272   12 09 50
12 10 40  =2044-027    22 01 25  52.5 211.1  1.2      26.4    50     2279   12 09 51

12 11 10  J2050+0407   22 01 55  58.7 215.8  1.2      30.3    10     2279   12 11 10
12 12 10  =2047+039    22 02 56  58.6 216.3  1.2      30.7    60     2287   12 11 11

12 12 40  J2047-0236   22 03 26  52.3 211.8  1.3      27.0    10     2287   12 12 40
12 13 40  =2044-027    22 04 26  52.1 212.2  1.3      27.3    60     2294   12 12 41

12 14 00  AEAQR        22 04 46  52.8 216.2  1.4      30.6     9     2294   12 14 00
12 16 50  ---          22 07 36  52.4 217.2  1.4      31.4   170     2316   12 14 01

12 17 10  J2047-0236   22 07 56  51.7 213.5  1.3      28.4     9     2316   12 17 10
12 18 00  =2044-027    22 08 47  51.6 213.8  1.3      28.6    50     2323   12 17 11

12 18 30  J2050+0407   22 09 17  57.7 218.8  1.3      32.7    10     2323   12 18 30
12 19 30  =2047+039    22 10 17  57.6 219.2  1.3      33.0    60     2330   12 18 31

12 20 00  J2047-0236   22 10 47  51.4 214.5  1.4      29.2    10     2330   12 20 00
12 21 00  =2044-027    22 11 47  51.3 214.8  1.4      29.5    60     2338   12 20 01

12 21 20  AEAQR        22 12 07  51.8 218.8  1.5      32.6     9     2338   12 21 20
12 24 10  ---          22 14 58  51.4 219.7  1.6      33.4   170     2360   12 21 21

12 24 30  J2047-0236   22 15 18  50.8 216.0  1.5      30.4     9     2360   12 24 30
12 25 20  =2044-027    22 16 08  50.7 216.3  1.5      30.7    50     2366   12 24 31
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

12 25 50  J2050+0407   22 16 38  56.7 221.6  1.4      35.0    10     2366   12 25 50
12 26 50  =2047+039    22 17 38  56.6 222.0  1.4      35.3    60     2374   12 25 51

12 27 20  J2047-0236   22 18 08  50.5 217.0  1.5      31.2    10     2374   12 27 20
12 28 20  =2044-027    22 19 08  50.3 217.3  1.5      31.5    60     2382   12 27 21

12 28 40  AEAQR        22 19 28  50.8 221.2  1.6      34.6     9     2382   12 28 40
12 31 30  ---          22 22 19  50.4 222.2  1.7      35.3   170     2404   12 28 41

12 31 50  J2047-0236   22 22 39  49.9 218.5  1.6      32.4     9     2404   12 31 50
12 32 40  =2044-027    22 23 29  49.8 218.8  1.6      32.6    50     2410   12 31 51

12 33 10  J2050+0407   22 23 59  55.6 224.3  1.6      37.0    10     2410   12 33 10
12 34 10  =2047+039    22 24 59  55.5 224.6  1.6      37.3    60     2418   12 33 11

12 34 40  J2047-0236   22 25 29  49.5 219.4  1.6      33.1    10     2418   12 34 40
12 35 40  =2044-027    22 26 29  49.4 219.7  1.6      33.4    60     2426   12 34 41

12 36 00  AEAQR        22 26 50  49.7 223.6  1.8      36.4     9     2426   12 36 00
12 38 50  ---          22 29 40  49.3 224.5  1.8      37.1   170     2448   12 36 01

12 39 10  J2047-0236   22 30 00  48.9 220.8  1.7      34.3     9     2448   12 39 10
12 40 00  =2044-027    22 30 50  48.7 221.1  1.7      34.5    50     2454   12 39 11

12 40 30  J2050+0407   22 31 20  54.5 226.8  1.7      39.0    11     2454   12 40 30
12 41 30  =2047+039    22 32 20  54.4 227.1  1.7      39.2    60     2462   12 40 31

12 42 00  J2047-0236   22 32 51  48.5 221.7  1.7      35.0    10     2462   12 42 00
12 43 00  =2044-027    22 33 51  48.3 222.0  1.8      35.2    60     2469   12 42 01

12 43 20  AEAQR        22 34 11  48.6 225.8  1.9      38.1     9     2469   12 43 20
12 46 10  ---          22 37 01  48.2 226.7  1.9      38.7   170     2491   12 43 21

12 46 30  J2047-0236   22 37 21  47.8 223.1  1.8      36.0    10     2491   12 46 30
12 47 20  =2044-027    22 38 11  47.7 223.3  1.8      36.2    50     2498   12 46 31

12 47 50  J2050+0407   22 38 41  53.3 229.2  1.8      40.8    11     2498   12 47 50
12 48 50  =2047+039    22 39 42  53.2 229.5  1.8      41.0    60     2506   12 47 51

12 49 20  J2047-0236   22 40 12  47.4 223.9  1.9      36.7    11     2506   12 49 20
12 50 20  =2044-027    22 41 12  47.2 224.2  1.9      36.9    60     2513   12 49 21

12 50 40  AEAQR        22 41 32  47.5 228.0  2.0      39.7    10     2513   12 50 40
12 53 30  ---          22 44 22  47.0 228.8  2.1      40.3   170     2535   12 50 41
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

12 53 50  J2047-0236   22 44 42  46.7 225.3  1.9      37.7    10     2535   12 53 50
12 54 40  =2044-027    22 45 33  46.6 225.5  2.0      37.9    50     2542   12 53 51

12 55 10  J2050+0407   22 46 03  52.1 231.5  1.9      42.4    11     2542   12 55 10
12 56 10  =2047+039    22 47 03  52.0 231.8  1.9      42.7    60     2549   12 55 11

12 56 40  J2047-0236   22 47 33  46.3 226.1  2.0      38.3    11     2549   12 56 40
12 57 40  =2044-027    22 48 33  46.1 226.4  2.0      38.6    60     2557   12 56 41

12 58 00  AEAQR        22 48 53  46.3 230.0  2.1      41.2    10     2557   12 58 00
13 00 50  ---          22 51 44  45.8 230.8  2.2      41.8   170     2579   12 58 01

13 01 10  J2047-0236   22 52 04  45.6 227.3  2.1      39.3    10     2579   13 01 10
13 02 00  =2044-027    22 52 54  45.4 227.6  2.1      39.5    50     2585   13 01 11

13 02 30  J2050+0407   22 53 24  50.9 233.6  2.0      44.0    11     2585   13 02 30
13 03 30  =2047+039    22 54 24  50.7 233.9  2.1      44.2    60     2593   13 02 31

13 04 00  J2047-0236   22 54 54  45.1 228.1  2.1      39.9    11     2593   13 04 00
13 05 00  =2044-027    22 55 54  44.9 228.4  2.1      40.1    60     2601   13 04 01

13 05 20  AEAQR        22 56 14  45.0 232.0  2.3      42.7    10     2601   13 05 20
13 08 10  ---          22 59 05  44.6 232.7  2.3      43.2   170     2623   13 05 21

13 08 30  J2047-0236   22 59 25  44.4 229.3  2.2      40.8    10     2623   13 08 30
13 09 20  =2044-027    23 00 15  44.2 229.5  2.2      40.9    50     2629   13 08 31

13 09 50  J2050+0407   23 00 45  49.6 235.6  2.2      45.4    11     2629   13 09 50
13 10 50  =2047+039    23 01 45  49.4 235.9  2.2      45.6    60     2637   13 09 51

13 11 20  J2047-0236   23 02 15  43.9 230.1  2.2      41.3    11     2637   13 11 20
13 12 20  =2044-027    23 03 16  43.7 230.3  2.3      41.5    60     2645   13 11 21

13 12 40  AEAQR        23 03 36  43.8 233.8  2.4      44.0    10     2645   13 12 40
13 15 30  ---          23 06 26  43.3 234.5  2.4      44.5   170     2667   13 12 41

13 15 50  J2047-0236   23 06 46  43.2 231.2  2.3      42.2    10     2667   13 15 50
13 16 40  =2044-027    23 07 36  43.0 231.4  2.3      42.3    50     2673   13 15 51

13 17 10  J2050+0407   23 08 06  48.3 237.6  2.3      46.7    12     2673   13 17 10
13 18 10  =2047+039    23 09 06  48.1 237.8  2.3      46.9    60     2681   13 17 11

13 18 40  J2047-0236   23 09 37  42.7 231.9  2.4      42.7    11     2681   13 18 40
13 19 40  =2044-027    23 10 37  42.5 232.2  2.4      42.9    60     2688   13 18 41
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

13 20 00  AEAQR        23 10 57  42.5 235.6  2.5      45.2    10     2688   13 20 00
13 22 50  ---          23 13 47  42.0 236.3  2.5      45.7   170     2710   13 20 01

13 23 10  J2047-0236   23 14 07  41.9 233.1  2.4      43.5    10     2710   13 23 10
13 24 00  =2044-027    23 14 57  41.8 233.3  2.4      43.6    50     2717   13 23 11

13 24 30  J2050+0407   23 15 28  46.9 239.4  2.4      48.0    12     2717   13 24 30
13 25 30  =2047+039    23 16 28  46.7 239.7  2.4      48.1    60     2725   13 24 31

13 26 00  J2047-0236   23 16 58  41.4 233.7  2.5      44.0    12     2725   13 26 00
13 27 00  =2044-027    23 17 58  41.3 234.0  2.5      44.2    60     2732   13 26 01

13 27 20  AEAQR        23 18 18  41.2 237.3  2.6      46.4    10     2732   13 27 20
13 30 10  ---          23 21 08  40.6 238.0  2.7      46.9   170     2754   13 27 21

13 30 30  J2047-0236   23 21 28  40.6 234.8  2.6      44.7    10     2754   13 30 30
13 31 20  =2044-027    23 22 19  40.5 235.0  2.6      44.9    50     2761   13 30 31

13 31 50  J2050+0407   23 22 49  45.5 241.2  2.5      49.1    12     2761   13 31 50
13 32 50  =2047+039    23 23 49  45.3 241.4  2.5      49.2    60     2768   13 31 51

13 33 20  J2047-0236   23 24 19  40.1 235.5  2.6      45.2    12     2768   13 33 20
13 34 20  =2044-027    23 25 19  40.0 235.7  2.6      45.4    60     2776   13 33 21

13 34 40  AEAQR        23 25 39  39.8 239.0  2.7      47.5    10     2776   13 34 40
13 37 30  ---          23 28 30  39.3 239.6  2.8      47.9   170     2798   13 34 41

13 37 50  J2047-0236   23 28 50  39.3 236.5  2.7      45.9    10     2798   13 37 50
13 38 40  =2044-027    23 29 40  39.2 236.7  2.7      46.0    50     2804   13 37 51

13 39 10  J2050+0407   23 30 10  44.1 242.9  2.7      50.1    12     2804   13 39 10
13 40 10  =2047+039    23 31 10  43.9 243.1  2.7      50.3    60     2812   13 39 11

13 40 40  J2047-0236   23 31 40  38.8 237.1  2.7      46.3    12     2812   13 40 40
13 41 40  =2044-027    23 32 40  38.6 237.3  2.7      46.5    60     2820   13 40 41

13 42 00  AEAQR        23 33 00  38.5 240.6  2.9      48.5    10     2820   13 42 00
13 44 50  ---          23 35 51  37.9 241.2  2.9      48.9   170     2842   13 42 01

13 45 10  J2047-0236   23 36 11  38.0 238.1  2.8      47.0    10     2842   13 45 10
13 46 00  =2044-027    23 37 01  37.8 238.3  2.8      47.1    50     2848   13 45 11

13 46 30  J2050+0407   23 37 31  42.7 244.5  2.8      51.1    12     2848   13 46 30
13 47 30  =2047+039    23 38 31  42.5 244.7  2.8      51.2    60     2856   13 46 31
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GVLBI/JVLA 4cm Phase Referencing of Flares in AE Aqr
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   3 Jun 2015   Day 154 ---

13 48 00  J2047-0236   23 39 01  37.5 238.7  2.9      47.4    12     2856   13 48 00
13 49 00  =2044-027    23 40 02  37.3 238.9  2.9      47.5    60     2864   13 48 01

13 49 20  AEAQR        23 40 22  37.1 242.1  3.0      49.5    10     2864   13 49 20
13 52 10  ---          23 43 12  36.5 242.7  3.0      49.9   170     2886   13 49 21

13 52 30  J2047-0236   23 43 32  36.6 239.7  2.9      48.0    10     2886   13 52 30
13 53 20  =2044-027    23 44 22  36.5 239.8  2.9      48.1    50     2892   13 52 31

13 53 50  J2050+0407   23 44 52  41.3 246.0  2.9      52.0    12     2892   13 53 50
13 54 50  =2047+039    23 45 52  41.1 246.2  2.9      52.1    60     2900   13 53 51

13 55 20  J2047-0236   23 46 23  36.1 240.3  3.0      48.4    12     2900   13 55 20
13 56 20  =2044-027    23 47 23  35.9 240.5  3.0      48.5    60     2907   13 55 21

13 56 40  AEAQR        23 47 43  35.7 243.6  3.1      50.4    10     2907   13 56 40
13 59 30  ---          23 50 33  35.1 244.1  3.2      50.7   170     2929   13 56 41

13 59 50  J2047-0236   23 50 53  35.3 241.2  3.0      49.0    10     2929   13 59 50
14 00 40  =2044-027    23 51 43  35.1 241.3  3.1      49.1    50     2936   13 59 51

 ---------- Block 10: 14:00 -- 14:12 ----------

14 02 40  3C454.3      23 53 44  70.3 226.4  1.0      40.5    43     2936   14 02 40
14 12 40  ---          00 03 45  68.6 231.5  1.2      44.5   600     3013   14 02 41


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess215.X1024glob
   Matching groups in /afs/desy.de/user/a/alobanov/soft/sched/catalogs/freq.dat:
     v4cm_3

   Setup group:    4         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  13  Setup file default.  Used with PCAL = off
   LO sum=   8351.25  8351.25  8383.25  8383.25  8415.25  8415.25  8447.25  8447.25
   BBC fr=    751.25   751.25   783.25   783.25   815.25   815.25   847.25   847.25
   Bandwd=     32.00    32.00    32.00    32.00    32.00    32.00    32.00    32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     791.25    791.25    823.25    823.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  13  14  15  16  17  18  19  20  21  22

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * AEAQR             20 37 34.587380   * 20 40 09.233634     20 40 57.668541       0.00
                    -01 02 55.24289    *-00 52 14.86240     -00 48 50.19134        0.00
                     From catalog imbedded in main SCHED input file.

   J1642+3948        16 41 17.606228   * 16 42 58.809965     16 43 31.621121       0.77
 * 3C345             39 54 10.81496    * 39 48 36.99402      39 47 03.03515        0.52
   1641+399          /afs/desy.de/user/a/alobanov/soft/sched/catalogs/sources.vlba
   J1642+39          GSFC 2011B astro solution     52621 Observations

 * J2047-0236        20 44 34.222160   * 20 47 10.366577     20 47 59.213185       1.14
   2044-027         -02 47 25.79546    *-02 36 22.14654     -02 32 49.99127        2.36
   J2047-02          /afs/desy.de/user/a/alobanov/soft/sched/catalogs/sources.vlba
                     GSFC 2011B astro solution        12 Observations

 * J2050+0407        20 47 35.947689   * 20 50 06.240587     20 50 53.330079       0.20
   2047+039          03 56 35.55388    * 04 07 48.89013      04 11 21.85463        0.38
   J2050+04          /afs/desy.de/user/a/alobanov/soft/sched/catalogs/sources.vlba
                     rfc_2012b Petrov, 2012, unpublished 121 observations

   J2253+1608        22 51 29.519738   * 22 53 57.747937     22 54 43.706646       0.68
 * 3C454.3           15 52 54.34810    * 16 08 53.56093      16 13 45.15014        0.72
   2251+158          /afs/desy.de/user/a/alobanov/soft/sched/catalogs/sources.vlba
   J2253+16          GSFC 2011B astro solution     39747 Observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  AEAQR      sess215.X1024glob     1 2 3 4 5 6 7 10 12 13            6.306   330.350
  3C345      sess215.X1024glob     1 2 3 4 5 6 7 13                  0.367    28.250
  J2047-0236 sess215.X1024glob     1 2 3 4 5 6 7 10 12 13            2.897   163.858
  J2050+0407 sess215.X1024glob     1 2 3 4 5 6 7 12 13               1.003    66.853
  3C454.3    sess215.X1024glob     1 2 3 4 5 6 7 10 12 13            0.292    14.792

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J1331+3030        13 28 49.657778   * 13 31 08.288070     13 31 51.696429       0.20
 * 3C286             30 45 58.64061    * 30 30 32.95925      30 25 57.21816        0.19
   1328+307          /afs/desy.de/user/a/alobanov/soft/sched/catalogs/sources.vlba
   J1331+30          rfc_2012b Petrov, 2012, unpublished 542 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   AEAQR              118.5
   3C286              110.0
   3C345              117.9
   J2047-0236         117.7
   J2050+0407         114.1
   3C454.3             81.5

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

