  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The true nature of the jet base in 3C84
 Exp. Code:  GP061A  


Schedule Version:       9.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Georgios Filippos Paraschos

Address:  Max-Planck-Institute for Radiostronomy
          Auf dem Huegel, 69
          Bonn, NRW, 53121
          Germany

Phone:    +49228525292
EMAIL:    gfparaschos@mpifr-bonn.mpg.de
Fax:
Phone during observation: +492257301155

Observing mode:

Notes:    PHASECAL should be ON
          v9 adds KVNPC
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Jun 2024   Day 157 ---

 ---------- preempt no ----------

 Next scan frequencies:  22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
 Next BBC frequencies:     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

09 00 01  0716+714     19 01 22  12.0  -1.9 11.6       5.1     0        0   09 00 01
09 05 01  ---          19 06 23  12.0  -1.5 11.7       4.0   300       77   09 00 02

09 06 01  0716+714     19 07 23  12.0  -1.4 11.7       3.8    54       77   09 06 01
09 11 01  ---          19 12 24  12.0  -1.0 11.8       2.7   300      155   09 06 02

09 12 01  0716+714     19 13 24  12.0  -0.9 11.8       2.5    54      155   09 12 01
09 17 01  ---          19 18 25  11.9  -0.5 11.9       1.4   300      232   09 12 02

09 18 01  0716+714     19 19 25  11.9  -0.4 11.9       1.1    54      232   09 18 01
09 23 01  ---          19 24 26  11.9  -0.0 12.0       0.0   300      309   09 18 02

09 43 20  J0102+5824   19 44 48  30.9  36.8 -5.3     -80.8  1179      309   09 43 20
09 49 20  =0059+581    19 50 49  31.7  36.9 -5.2     -82.0   360      402   09 43 21

10 26 45  J0102+5824   20 28 20  36.6  37.4 -4.6     -89.8  2238      402   10 26 45
10 36 45  =0059+581    20 38 22  37.9  37.3 -4.4     -92.0   600      556   10 26 46

10 43 25  3C84         20 45 03  13.7  49.5 -6.6     -61.0   343      556   10 43 25
10 53 25  ---          20 55 05  15.3  50.4 -6.4     -62.4   600      711   10 43 26

10 54 10  3C84         20 55 50  15.5  50.5 -6.4     -62.5    39      711   10 54 10
11 04 10  ---          21 05 52  17.1  51.3 -6.3     -63.9   600      866   10 54 11

11 08 20  NRAO150      21 10 02  16.0  39.6 -6.9     -60.8   234      866   11 08 20
11 14 20  ---          21 16 03  16.9  40.1 -6.8     -61.8   360      958   11 08 21

 ---------- POINTING ----------

11 21 30  3C84         21 23 14  20.1  52.8 -6.0     -66.4   414      958   11 21 30
11 31 30  ---          21 33 16  21.8  53.6 -5.8     -67.8   600     1113   11 21 31

11 32 15  3C84         21 34 01  21.9  53.6 -5.8     -67.9    39     1113   11 32 15
11 42 15  ---          21 44 03  23.7  54.4 -5.6     -69.2   600     1268   11 32 16

11 46 55  J0102+5824   21 48 44  46.9  35.1 -3.3    -108.5   227     1268   11 46 55
11 52 55  =0059+581    21 54 45  47.6  34.7 -3.2    -110.0   360     1360   11 46 56

11 57 05  3C84         21 58 55  26.3  55.4 -5.4     -71.3   199     1360   11 57 05
12 07 05  ---          22 08 57  28.1  56.0 -5.2     -72.6   600     1515   11 57 06
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Jun 2024   Day 157 ---

12 07 50  3C84         22 09 42  28.2  56.1 -5.2     -72.7    39     1515   12 07 50
12 17 50  ---          22 19 44  30.0  56.7 -5.0     -74.1   600     1669   12 07 51

12 19 30  NRAO150      22 21 24  26.3  44.3 -5.7     -73.0    83     1669   12 19 30
12 25 30  ---          22 27 25  27.2  44.6 -5.6     -74.0   360     1762   12 19 31

 ---------- POINTING ----------

12 32 45  3C84         22 34 41  32.7  57.5 -4.8     -76.1   418     1762   12 32 45
12 42 45  ---          22 44 43  34.6  58.1 -4.6     -77.5   600     1917   12 32 46

12 43 30  3C84         22 45 28  34.7  58.1 -4.6     -77.6    39     1917   12 43 30
12 53 30  ---          22 55 30  36.5  58.6 -4.4     -79.0   600     2071   12 43 31

12 56 50  J0102+5824   22 58 50  54.9  28.2 -2.1    -128.9   156     2071   12 56 50
13 02 50  =0059+581    23 04 51  55.5  27.3 -2.0    -130.9   360     2164   12 56 51

13 06 10  3C84         23 08 12  38.9  59.1 -4.2     -80.8   158     2164   13 06 10
13 16 10  ---          23 18 13  40.7  59.4 -4.1     -82.2   600     2319   13 06 11

13 16 55  3C84         23 18 58  40.9  59.5 -4.0     -82.4    39     2319   13 16 55
13 26 55  ---          23 29 00  42.7  59.8 -3.9     -83.8   600     2473   13 16 56

13 29 25  NRAO150      23 31 30  37.1  46.8 -4.5     -85.4   130     2473   13 29 25
13 35 25  ---          23 37 31  38.1  46.8 -4.4     -86.5   360     2566   13 29 26

 ---------- POINTING ----------

13 42 45  3C84         23 44 53  45.7  60.1 -3.6     -86.2   420     2566   13 42 45
13 52 45  ---          23 54 54  47.5  60.3 -3.4     -87.8   600     2721   13 42 46

13 53 30  3C84         23 55 39  47.7  60.3 -3.4     -87.9    39     2721   13 53 30
14 03 30  ---          00 05 41  49.6  60.4 -3.3     -89.5   600     2875   13 53 31

14 06 50  J0102+5824   00 09 02  60.6  14.7 -0.9    -155.3   160     2875   14 06 50
14 12 50  =0059+581    00 15 03  60.9  13.2 -0.8    -157.9   360     2968   14 06 51

14 15 50  3C84         00 18 03  51.9  60.3 -3.1     -91.6   139     2968   14 15 50
14 25 50  ---          00 28 05  53.7  60.2 -2.9     -93.3   600     3123   14 15 51

14 26 35  3C84         00 28 50  53.9  60.2 -2.9     -93.5    39     3123   14 26 35
14 36 35  ---          00 38 52  55.8  59.9 -2.7     -95.3   600     3277   14 26 36

14 39 05  NRAO150      00 41 22  48.1  46.1 -3.3     -99.5   126     3277   14 39 05
14 45 05  ---          00 47 23  49.0  45.9 -3.2    -100.8   360     3370   14 39 06
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Jun 2024   Day 157 ---

 ---------- POINTING ----------

14 52 25  3C84         00 54 44  58.7  59.3 -2.4     -98.5   415     3370   14 52 25
15 02 25  ---          01 04 46  60.5  58.6 -2.3    -100.7   600     3524   14 52 26

15 03 05  3C84         01 05 26  60.7  58.6 -2.3    -100.9    34     3524   15 03 05
15 13 05  ---          01 15 28  62.5  57.8 -2.1    -103.3   600     3679   15 03 06

15 17 25  NRAO150      01 19 48  53.9  43.8 -2.7    -108.8   234     3679   15 17 25
15 23 25  ---          01 25 49  54.8  43.3 -2.6    -110.4   360     3772   15 17 26

15 28 25  3C84         01 30 50  65.3  56.0 -1.8    -107.4   273     3772   15 28 25
15 38 25  ---          01 40 52  67.0  54.5 -1.7    -110.4   600     3926   15 28 26

15 39 10  3C84         01 41 37  67.2  54.4 -1.7    -110.7    39     3926   15 39 10
15 49 10  ---          01 51 38  68.9  52.5 -1.5    -114.1   600     4081   15 39 11

15 52 30  NRAO150      01 54 59  59.0  39.7 -2.1    -119.0   172     4081   15 52 30
15 58 30  ---          02 01 00  59.8  38.8 -2.0    -120.9   360     4174   15 52 31

 ---------- POINTING ----------

16 05 50  3C84         02 08 21  71.7  48.2 -1.2    -120.9   411     4174   16 05 50
16 15 50  ---          02 18 23  73.3  44.8 -1.1    -125.8   600     4328   16 05 51

16 16 35  3C84         02 19 08  73.4  44.5 -1.0    -126.2    39     4328   16 16 35
16 26 35  ---          02 29 10  74.8  40.2 -0.9    -132.1   600     4483   16 16 36

16 29 55  J0102+5824   02 32 30  58.3 -21.9  1.5     142.0   148     4483   16 29 55
16 35 55  =0059+581    02 38 31  57.8 -23.1  1.6     139.8   360     4576   16 29 56

16 38 55  3C84         02 41 32  76.4  33.4 -0.7    -140.6   131     4576   16 38 55
16 48 55  ---          02 51 33  77.5  26.7 -0.5    -148.9   600     4730   16 38 56

16 49 40  3C84         02 52 18  77.6  26.1 -0.5    -149.6    39     4730   16 49 40
16 59 40  ---          03 02 20  78.4  18.0 -0.3    -159.2   600     4885   16 49 41

17 02 10  NRAO150      03 04 50  67.1  23.2 -0.9    -147.4   119     4885   17 02 10
17 08 10  ---          03 10 51  67.6  21.1 -0.8    -150.5   360     4978   17 02 11

 ---------- POINTING ----------

17 15 30  3C84         03 18 13  79.0   3.1 -0.1    -176.4   410     4978   17 15 30
17 25 30  ---          03 28 14  79.0  -6.7  0.1     172.3   600     5132   17 15 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Jun 2024   Day 157 ---

17 26 10  3C84         03 28 54  78.9  -7.3  0.1     171.5    34     5132   17 26 10
17 36 10  ---          03 38 56  78.5 -16.6  0.3     160.8   600     5287   17 26 11

17 40 30  NRAO150      03 43 17  69.3   8.0 -0.3    -169.0   233     5287   17 40 30
17 46 30  ---          03 49 18  69.5   5.4 -0.2    -172.6   360     5379   17 40 31

17 47 50  NRAO150      03 50 38  69.5   4.8 -0.2    -173.4    74     5379   17 47 50
17 53 50  ---          03 56 39  69.6   2.1 -0.1    -177.1   360     5472   17 47 51

 ---------- Segment (C). VLBA (1800-1900; EVNs out, KVN not yet back) ----------

17 56 00  3C84         03 58 49  76.7 -31.9  0.6     142.5    99     5472   17 56 00
18 06 00  ---          04 08 51  75.5 -37.8  0.8     135.2   600     5627   17 56 01

18 06 45  3C84         04 09 36  75.4 -38.2  0.8     134.7    39     5627   18 06 45
18 16 45  ---          04 19 38  74.0 -42.9  1.0     128.5   600     5781   18 06 46

18 20 05  J0102+5824   04 22 58  46.5 -35.3  3.3     107.6   139     5781   18 20 05
18 26 05  =0059+581    04 28 59  45.7 -35.7  3.4     106.1   360     5874   18 20 06

18 28 05  3C84         04 31 00  72.2 -47.1  1.2     122.5    60     5874   18 28 05
18 38 05  ---          04 41 01  70.6 -50.1  1.3     118.0   600     6029   18 28 06

18 38 50  3C84         04 41 46  70.5 -50.3  1.3     117.7    39     6029   18 38 50
18 48 50  ---          04 51 48  68.8 -52.6  1.5     113.9   600     6183   18 38 51

18 51 20  NRAO150      04 54 18  67.4 -22.0  0.9     149.2   120     6183   18 51 20
18 57 20  ---          05 00 19  66.8 -24.0  1.0     146.1   360     6276   18 51 21

 ---------- Segment (D). KVN+VLBA (1900-0200) ----------

19 00 00  3C84         05 03 00  66.9 -54.7  1.7     110.1   131     6276   19 00 00
19 10 00  ---          05 13 01  65.1 -56.2  1.9     107.1   600     6431   19 00 01

19 10 45  3C84         05 13 47  64.9 -56.3  1.9     106.9    39     6431   19 10 45
19 20 45  ---          05 23 48  63.1 -57.4  2.0     104.2   600     6585   19 10 46

19 23 15  J0102+5824   05 26 19  38.4 -37.3  4.4      92.8    94     6585   19 23 15
19 29 15  =0059+581    05 32 20  37.6 -37.3  4.5      91.5   360     6678   19 23 16

19 31 15  3C84         05 34 20  61.2 -58.4  2.2     101.6    65     6678   19 31 15
19 41 15  ---          05 44 22  59.4 -59.1  2.4      99.3   600     6833   19 31 16

19 42 00  3C84         05 45 07  59.2 -59.1  2.4      99.2    39     6833   19 42 00
19 52 00  ---          05 55 08  57.4 -59.6  2.6      97.1   600     6987   19 42 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Jun 2024   Day 157 ---

19 54 30  NRAO150      05 57 39  60.3 -38.2  1.9     122.3   127     6987   19 54 30
20 00 30  ---          06 03 40  59.5 -39.2  2.0     120.3   360     7080   19 54 31

20 02 30  3C84         06 05 40  55.4 -60.0  2.7      95.0    97     7080   20 02 30
20 12 30  ---          06 15 42  53.6 -60.2  2.9      93.2   600     7234   20 02 31

20 13 15  3C84         06 16 27  53.4 -60.2  2.9      93.0    39     7234   20 13 15
20 23 15  ---          06 26 28  51.5 -60.3  3.1      91.3   600     7389   20 13 16

20 25 45  J0102+5824   06 28 59  30.2 -36.7  5.4      79.8   100     7389   20 25 45
20 31 45  =0059+581    06 35 00  29.5 -36.5  5.5      78.6   360     7482   20 25 46

20 33 45  3C84         06 37 00  49.6 -60.4  3.3      89.5    72     7482   20 33 45
20 43 45  ---          06 47 02  47.7 -60.3  3.4      87.9   600     7636   20 33 46

20 44 30  3C84         06 47 47  47.6 -60.3  3.4      87.8    39     7636   20 44 30
20 54 30  ---          06 57 49  45.7 -60.1  3.6      86.2   600     7791   20 44 31

20 57 00  NRAO150      07 00 19  51.3 -45.1  3.0     104.3   130     7791   20 57 00
21 03 00  ---          07 06 20  50.4 -45.4  3.1     102.9   360     7884   20 57 01

21 05 00  3C84         07 08 20  43.7 -59.9  3.8      84.6   100     7884   21 05 00
21 15 00  ---          07 18 22  41.9 -59.6  3.9      83.1   600     8038   21 05 01

21 15 45  3C84         07 19 07  41.7 -59.6  4.0      83.0    39     8038   21 15 45
21 25 45  ---          07 29 09  39.9 -59.3  4.1      81.6   600     8193   21 15 46

21 28 15  NRAO150      07 31 39  46.5 -46.5  3.5      97.2   128     8193   21 28 15
21 34 15  ---          07 37 40  45.5 -46.6  3.6      95.9   360     8286   21 28 16

21 36 15  3C84         07 39 40  37.9 -58.9  4.3      80.1    98     8286   21 36 15
21 46 15  ---          07 49 42  36.1 -58.5  4.5      78.7   600     8440   21 36 16

21 47 00  3C84         07 50 27  35.9 -58.4  4.5      78.6    39     8440   21 47 00
21 57 00  ---          08 00 29  34.1 -57.9  4.7      77.2   600     8595   21 47 01

21 59 30  NRAO150      08 02 59  41.5 -47.0  4.0      90.7   127     8595   21 59 30
22 05 30  ---          08 09 00  40.6 -47.0  4.1      89.6   360     8688   21 59 31

22 07 30  3C84         08 11 01  32.2 -57.4  4.8      75.7    96     8688   22 07 30
22 17 30  ---          08 21 02  30.4 -56.8  5.0      74.4   600     8842   22 07 31

22 18 15  3C84         08 21 47  30.2 -56.8  5.0      74.3    39     8842   22 18 15
22 28 15  ---          08 31 49  28.4 -56.2  5.2      72.9   600     8997   22 18 16
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Jun 2024   Day 157 ---

22 30 45  J0102+5824   08 34 19  15.2 -30.0  7.5      55.5   116     8997   22 30 45
22 36 45  =0059+581    08 40 20  14.6 -29.5  7.6      54.3   360     9089   22 30 46

22 38 45  3C84         08 42 21  26.6 -55.5  5.3      71.5    88     9089   22 38 45
22 48 45  ---          08 52 22  24.8 -54.8  5.5      70.1   600     9244   22 38 46

22 49 30  3C84         08 53 07  24.7 -54.8  5.5      70.0    39     9244   22 49 30
22 59 30  ---          09 03 09  22.9 -54.0  5.7      68.6   600     9399   22 49 31

23 02 00  NRAO150      09 05 40  31.8 -45.9  5.1      79.2   124     9399   23 02 00
23 08 00  ---          09 11 41  30.8 -45.7  5.2      78.1   360     9491   23 02 01

23 10 00  3C84         09 13 41  21.1 -53.2  5.9      67.2    93     9491   23 10 00
23 20 00  ---          09 23 42  19.4 -52.4  6.0      65.8   600     9646   23 10 01

23 20 40  3C84         09 24 23  19.3 -52.4  6.0      65.7    34     9646   23 20 40
23 30 40  ---          09 34 24  17.6 -51.5  6.2      64.3   600     9801   23 20 41

23 33 10  NRAO150      09 36 55  27.0 -44.6  5.6      73.7   123     9801   23 33 10
23 39 10  ---          09 42 56  26.1 -44.3  5.7      72.7   360     9893   23 33 11

 ---------- preempt ok ----------

23 41 10  3C84         09 44 56  15.8 -50.6  6.4      62.8    92     9893   23 41 10
23 51 10  ---          09 54 58  14.1 -49.7  6.6      61.4   600    10048   23 41 11

 --- Start: Wed   5 Jun 2024   Day 157 -- Stop: Thu   6 Jun 2024   Day 158 ---

23 51 55  3C84         09 55 43  14.0 -49.7  6.6      61.3    39    10048   23 51 55
00 01 55  ---          10 05 44  12.4 -48.7  6.7      59.8   600    10202   23 51 56

00 35 35  NRAO150      10 39 30  17.8 -40.7  6.6      63.0  1992    10202   00 35 35
00 41 35  ---          10 45 31  17.0 -40.2  6.7      62.0   360    10295   00 35 36

00 55 00  0716+714     10 58 58  40.3 -19.8  3.6     114.8   749    10295   00 55 00
01 01 40  ---          11 05 39  39.8 -20.1  3.7     113.1   400    10398   00 55 01

01 03 20  0716+714     11 07 19  39.7 -20.1  3.7     112.6    94    10398   01 03 20
01 10 00  ---          11 14 01  39.2 -20.4  3.8     110.9   400    10501   01 03 21

01 11 40  0716+714     11 15 41  39.0 -20.4  3.9     110.4    94    10501   01 11 40
01 18 20  ---          11 22 22  38.5 -20.7  4.0     108.7   400    10604   01 11 41

01 20 00  0716+714     11 24 02  38.4 -20.7  4.0     108.3    94    10604   01 20 00
01 26 40  ---          11 30 43  37.9 -20.9  4.1     106.6   400    10707   01 20 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   6 Jun 2024   Day 158 ---

01 28 20  0716+714     11 32 24  37.8 -21.0  4.1     106.1    94    10707   01 28 20
01 35 00  ---          11 39 05  37.2 -21.2  4.2     104.5   400    10811   01 28 21

01 36 40  0716+714     11 40 45  37.1 -21.2  4.3     104.0    94    10811   01 36 40
01 43 20  ---          11 47 26  36.6 -21.3  4.4     102.4   400    10914   01 36 41

01 45 00  0716+714     11 49 06  36.5 -21.4  4.4     101.9    94    10914   01 45 00
01 51 40  ---          11 55 47  35.9 -21.5  4.5     100.3   400    11017   01 45 01

01 53 20  0716+714     11 57 28  35.8 -21.5  4.5      99.9    94    11017   01 53 20
02 00 00  ---          12 04 09  35.3 -21.6  4.7      98.2   400    11120   01 53 21


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess224.K2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    1         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  14  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
   BBC fr=     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     727.99    727.99    791.99    791.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  14  15  16  17  18  19  20  21  22  23

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   0059+581          00 59 43.470969   * 01 02 45.762377     01 04 12.915375       0.00
 * J0102+5824        58 08 04.84743    * 58 24 11.13658      58 31 46.66240        0.00
   J0102+58          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution, 399648 observations.

 * 3C84              03 16 29.567265   * 03 19 48.160096     03 21 23.184622       1.50
   J0319+4130        41 19 51.91692    * 41 30 42.10404      41 35 53.74929        2.86
   0316+413          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0319+41          GSFC 2016a X/S astro solution,  10291 observations.

 * NRAO150           03 55 45.261365   * 03 59 29.747266     04 01 16.989612       0.03
   J0359+5057        50 49 20.28574    * 50 57 50.16169      51 01 55.07231        0.02
   0355+508          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0359+50          GSFC 2016a X/S astro solution,  22807 observations.

 * 0716+714          07 16 13.029730   * 07 21 53.448465     07 24 35.369527       0.01
   J0721+7120        71 26 15.17409    * 71 20 36.36343      71 18 01.22650        0.00
   J0721+71          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  79366 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J0102+5824 sess224.K2048glob     1 2 3 4 5 6 8 11 14               2.033   169.764
  3C84       sess224.K2048glob     1 2 3 4 5 6 8 11 14              15.167  1240.703
  NRAO150    sess224.K2048glob     1 2 3 4 5 6 8 11 14               2.500   241.100
  0716+714   sess224.K2048glob     1 2 3 4 14                        2.422    37.089


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J0102+5824          54.3
   3C84                27.5
   NRAO150             30.4
   0716+714            53.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

