  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 43 GHz Precision Astrometry of the Jet in NRAO 150
 Exp. Code:  GA032D  


Schedule Version:       2.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       Ivan Agudo

Address:  IAA-CSIC
          Glorieta de la Astronomia s/n
          18008 Granada/Spain
 

Phone:    +34 958 230 632
EMAIL:    iagudo@iaa.es
Fax:
Phone during observation: +34 958 814 530

Observing mode: 43 GHz VLBI @ 1024 Mbps

Notes:    Q-band inverse phase-ref astrometry of NRAO150 with two
          position reference sources, J0350+5138 and J0350+5201
          DA193 and OJ287 also observed as polarization calibrators
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

 Next scan frequencies:  43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
 Next BBC frequencies:     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25
 Next scan bandwidths:      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00

16 30 00  J0350+5138   21 00 12  16.3  39.0 -6.9     -60.9     0        0   16 30 00
16 32 08  ---          21 00 42  16.4  39.1 -6.8     -61.0   129       17   16 30 01

16 32 19  NRAO150      21 02 32  15.1  39.1 -7.0     -59.6     0       17   16 32 19
16 32 49  ---          21 03 02  15.1  39.1 -7.0     -59.7    30       20   16 32 20

16 33 00  J0350+5201   21 03 13  16.9  38.9 -6.8     -61.5     0       20   16 33 00
16 33 30  ---          21 03 43  16.9  38.9 -6.8     -61.6    30       24   16 33 01

16 33 50  NRAO150      21 04 04  15.3  39.2 -6.9     -59.9     9       24   16 33 50
16 34 20  ---          21 04 34  15.3  39.3 -6.9     -59.9    30       28   16 33 51

16 34 32  J0350+5138   21 04 45  16.9  39.4 -6.8     -61.7     0       28   16 34 32
16 35 02  ---          21 05 15  17.0  39.4 -6.8     -61.8    30       32   16 34 33

16 35 13  NRAO150      21 05 26  15.5  39.3 -6.9     -60.1     0       32   16 35 13
16 35 43  ---          21 05 56  15.5  39.4 -6.9     -60.2    30       36   16 35 14

16 35 54  J0350+5201   21 06 08  17.3  39.1 -6.8     -62.0     0       36   16 35 54
16 36 24  ---          21 06 38  17.3  39.1 -6.8     -62.1    30       40   16 35 55

16 36 44  NRAO150      21 06 58  15.7  39.5 -6.9     -60.4     9       40   16 36 44
16 37 14  ---          21 07 28  15.7  39.5 -6.9     -60.4    30       44   16 36 45

16 37 26  J0350+5138   21 07 39  17.3  39.6 -6.7     -62.2     0       44   16 37 26
16 37 56  ---          21 08 09  17.4  39.6 -6.7     -62.3    30       48   16 37 27

16 38 07  NRAO150      21 08 21  15.9  39.6 -6.9     -60.6     0       48   16 38 07
16 38 37  ---          21 08 51  15.9  39.6 -6.9     -60.7    30       51   16 38 08

16 38 48  J0350+5201   21 09 02  17.7  39.3 -6.7     -62.5     0       51   16 38 48
16 39 18  ---          21 09 32  17.7  39.4 -6.7     -62.6    30       55   16 38 49

16 39 38  NRAO150      21 09 52  16.1  39.7 -6.8     -60.9     9       55   16 39 38
16 40 08  ---          21 10 22  16.1  39.7 -6.8     -60.9    30       59   16 39 39

16 40 20  J0350+5138   21 10 34  17.7  39.8 -6.7     -62.7     0       59   16 40 20
16 40 50  ---          21 11 04  17.8  39.9 -6.7     -62.8    30       63   16 40 21

16 41 05  NRAO150      21 11 19  16.3  39.8 -6.8     -61.1     4       63   16 41 05
16 41 42  ---          21 11 49  16.3  39.8 -6.8     -61.2    37       68   16 41 06
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

16 41 58  J0350+5201   21 12 13  18.1  39.6 -6.7     -63.1     5       68   16 41 58
16 42 47  ---          21 12 43  18.2  39.6 -6.7     -63.2    49       74   16 41 59

16 43 07  NRAO150      21 13 22  16.6  40.0 -6.8     -61.5     9       74   16 43 07
16 43 48  ---          21 13 52  16.6  40.0 -6.8     -61.5    40       79   16 43 08

16 44 03  J0350+5138   21 14 18  18.3  40.1 -6.6     -63.4     4       79   16 44 03
16 44 44  ---          21 14 48  18.3  40.1 -6.6     -63.5    41       85   16 44 04

16 44 59  NRAO150      21 15 14  16.8  40.1 -6.8     -61.8     4       85   16 44 59
16 45 36  ---          21 15 44  16.9  40.2 -6.8     -61.9    37       89   16 45 00

16 45 52  J0350+5201   21 16 07  18.6  39.8 -6.6     -63.8     5       89   16 45 52
16 46 40  ---          21 16 37  18.7  39.9 -6.6     -63.8    48       95   16 45 53

16 47 00  NRAO150      21 17 15  17.1  40.3 -6.7     -62.1     9       95   16 47 00
16 47 39  ---          21 17 45  17.2  40.3 -6.7     -62.2    39      100   16 47 01

16 47 54  J0350+5138   21 18 09  18.8  40.4 -6.6     -64.0     4      100   16 47 54
16 48 35  ---          21 18 39  18.9  40.4 -6.6     -64.1    41      106   16 47 55

16 48 50  NRAO150      21 19 05  17.3  40.4 -6.7     -62.4     4      106   16 48 50
16 49 26  ---          21 19 35  17.4  40.4 -6.7     -62.5    36      110   16 48 51

16 49 41  J0350+5201   21 19 57  19.2  40.1 -6.5     -64.4     4      110   16 49 41
16 50 29  ---          21 20 27  19.2  40.2 -6.5     -64.5    47      116   16 49 42

16 50 49  NRAO150      21 21 04  17.6  40.6 -6.7     -62.8     9      116   16 50 49
16 51 27  ---          21 21 35  17.7  40.6 -6.7     -62.9    38      121   16 50 50

16 51 41  J0350+5138   21 21 57  19.3  40.6 -6.5     -64.7     4      121   16 51 41
16 52 22  ---          21 22 27  19.4  40.7 -6.5     -64.8    40      127   16 51 42

16 52 36  NRAO150      21 22 52  17.9  40.7 -6.6     -63.1     3      127   16 52 36
16 53 12  ---          21 23 22  17.9  40.7 -6.6     -63.2    36      131   16 52 37

16 53 27  J0350+5201   21 23 44  19.7  40.4 -6.5     -65.1     4      131   16 53 27
16 54 14  ---          21 24 14  19.8  40.4 -6.5     -65.2    47      137   16 53 28

16 54 34  NRAO150      21 24 50  18.2  40.8 -6.6     -63.4     9      137   16 54 34
16 55 11  ---          21 25 20  18.2  40.9 -6.6     -63.5    37      142   16 54 35

16 55 25  J0350+5138   21 25 42  19.8  40.9 -6.4     -65.4     3      142   16 55 25
16 56 05  ---          21 26 12  19.9  40.9 -6.4     -65.4    40      147   16 55 26
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

16 56 19  NRAO150      21 26 36  18.4  41.0 -6.6     -63.7     3      147   16 56 19
16 56 55  ---          21 27 06  18.5  41.0 -6.6     -63.8    35      152   16 56 20

16 57 10  J0350+5201   21 27 27  20.2  40.6 -6.4     -65.7     4      152   16 57 10
16 57 56  ---          21 27 57  20.3  40.7 -6.4     -65.8    46      158   16 57 11

16 58 16  NRAO150      21 28 33  18.7  41.1 -6.5     -64.1     9      158   16 58 16
16 58 52  ---          21 29 03  18.7  41.2 -6.5     -64.2    36      162   16 58 17

16 59 06  J0350+5138   21 29 23  20.4  41.2 -6.4     -66.0     3      162   16 59 06
16 59 46  ---          21 29 53  20.4  41.2 -6.4     -66.1    40      167   16 59 07

17 00 00  NRAO150      21 30 17  18.9  41.2 -6.5     -64.4     3      167   17 00 00
17 00 34  ---          21 30 47  19.0  41.3 -6.5     -64.4    35      172   17 00 01

17 00 49  J0350+5201   21 31 07  20.7  40.9 -6.3     -66.4     4      172   17 00 49
17 01 35  ---          21 31 37  20.8  40.9 -6.3     -66.4    45      178   17 00 50

17 01 55  NRAO150      21 32 12  19.2  41.4 -6.5     -64.7     9      178   17 01 55
17 02 30  ---          21 32 42  19.3  41.4 -6.5     -64.8    35      182   17 01 56

17 02 44  J0350+5138   21 33 02  20.9  41.4 -6.3     -66.6     3      182   17 02 44
17 03 23  ---          21 33 32  21.0  41.4 -6.3     -66.7    39      187   17 02 45

17 03 37  NRAO150      21 33 55  19.4  41.5 -6.4     -65.0     3      187   17 03 37
17 04 11  ---          21 34 25  19.5  41.5 -6.4     -65.1    34      192   17 03 38

17 04 26  J0350+5201   21 34 44  21.2  41.1 -6.3     -67.0     4      192   17 04 26
17 05 11  ---          21 35 14  21.3  41.1 -6.3     -67.1    45      197   17 04 27

17 05 31  NRAO150      21 35 49  19.7  41.6 -6.4     -65.3     9      197   17 05 31
17 06 05  ---          21 36 19  19.8  41.7 -6.4     -65.4    34      202   17 05 32

17 06 19  J0350+5138   21 36 37  21.4  41.6 -6.3     -67.2     3      202   17 06 19
17 06 58  ---          21 37 07  21.5  41.7 -6.2     -67.3    39      207   17 06 20

17 07 12  NRAO150      21 37 30  20.0  41.7 -6.4     -65.6     3      207   17 07 12
17 07 45  ---          21 38 00  20.0  41.8 -6.4     -65.7    34      211   17 07 13

17 08 00  J0350+5201   21 38 19  21.7  41.3 -6.2     -67.6     3      211   17 08 00
17 08 44  ---          21 38 49  21.8  41.4 -6.2     -67.7    44      217   17 08 01

17 09 04  NRAO150      21 39 23  20.2  41.9 -6.4     -65.9     9      217   17 09 04
17 09 38  ---          21 39 53  20.3  41.9 -6.3     -66.0    34      221   17 09 05
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

17 09 52  J0350+5138   21 40 11  21.9  41.9 -6.2     -67.9     3      221   17 09 52
17 10 30  ---          21 40 41  22.0  41.9 -6.2     -67.9    39      226   17 09 53

17 10 44  NRAO150      21 41 03  20.5  42.0 -6.3     -66.2     2      226   17 10 44
17 11 17  ---          21 41 33  20.5  42.0 -6.3     -66.3    34      231   17 10 45

17 11 32  J0350+5201   21 41 51  22.2  41.6 -6.2     -68.2     3      231   17 11 32
17 12 16  ---          21 42 21  22.3  41.6 -6.2     -68.3    44      236   17 11 33

17 12 36  NRAO150      21 42 55  20.7  42.1 -6.3     -66.5     9      236   17 12 36
17 13 09  ---          21 43 25  20.8  42.2 -6.3     -66.6    33      241   17 12 37

17 13 22  J0350+5138   21 43 42  22.4  42.1 -6.1     -68.5     2      241   17 13 22
17 14 01  ---          21 44 12  22.5  42.1 -6.1     -68.5    38      245   17 13 23

17 14 14  NRAO150      21 44 34  21.0  42.2 -6.3     -66.8     2      245   17 14 14
17 14 47  ---          21 45 04  21.0  42.3 -6.3     -66.9    33      250   17 14 15

17 15 02  J0350+5201   21 45 21  22.7  41.8 -6.1     -68.8     3      250   17 15 02
17 15 45  ---          21 45 51  22.8  41.8 -6.1     -68.9    43      255   17 15 03

17 16 05  NRAO150      21 46 25  21.2  42.4 -6.2     -67.1     9      255   17 16 05
17 16 37  ---          21 46 55  21.3  42.4 -6.2     -67.2    32      259   17 16 06

17 16 51  J0350+5138   21 47 11  22.9  42.3 -6.1     -69.1     2      259   17 16 51
17 17 29  ---          21 47 41  23.0  42.3 -6.1     -69.1    38      264   17 16 52

17 17 42  NRAO150      21 48 02  21.5  42.5 -6.2     -67.4     2      264   17 17 42
17 18 15  ---          21 48 32  21.5  42.5 -6.2     -67.5    33      268   17 17 43

17 18 29  J0350+5201   21 48 50  23.2  42.0 -6.1     -69.4     3      268   17 18 29
17 19 12  ---          21 49 20  23.3  42.0 -6.0     -69.5    43      274   17 18 30

17 19 32  NRAO150      21 49 53  21.7  42.6 -6.2     -67.7     9      274   17 19 32
17 20 04  ---          21 50 23  21.8  42.6 -6.2     -67.8    32      278   17 19 33

17 20 17  J0350+5138   21 50 38  23.4  42.5 -6.0     -69.7     2      278   17 20 17
17 20 55  ---          21 51 08  23.5  42.5 -6.0     -69.7    38      283   17 20 18

17 21 08  NRAO150      21 51 29  22.0  42.7 -6.2     -68.0     2      283   17 21 08
17 21 41  ---          21 51 59  22.0  42.7 -6.1     -68.1    33      287   17 21 09

17 21 55  J0350+5201   21 52 16  23.7  42.2 -6.0     -70.0     3      287   17 21 55
17 22 37  ---          21 52 46  23.8  42.2 -6.0     -70.1    42      293   17 21 56
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

17 22 57  NRAO150      21 53 18  22.2  42.8 -6.1     -68.3     9      293   17 22 57
17 23 29  ---          21 53 49  22.3  42.8 -6.1     -68.4    31      297   17 22 58

17 23 42  J0350+5138   21 54 03  23.9  42.7 -6.0     -70.3     2      297   17 23 42
17 24 19  ---          21 54 33  24.0  42.7 -6.0     -70.3    38      302   17 23 43

17 24 32  NRAO150      21 54 54  22.5  42.9 -6.1     -68.6     2      302   17 24 32
17 25 05  ---          21 55 24  22.5  42.9 -6.1     -68.6    33      306   17 24 33

17 25 19  J0350+5201   21 55 40  24.2  42.4 -5.9     -70.6     3      306   17 25 19
17 26 01  ---          21 56 10  24.3  42.4 -5.9     -70.7    42      311   17 25 20

17 26 21  NRAO150      21 56 43  22.7  43.0 -6.1     -68.9     9      311   17 26 21
17 26 52  ---          21 57 13  22.8  43.0 -6.1     -69.0    31      315   17 26 22

17 27 05  J0350+5138   21 57 27  24.4  42.9 -5.9     -70.8     2      315   17 27 05
17 27 42  ---          21 57 57  24.5  42.9 -5.9     -70.9    37      320   17 27 06

17 27 55  NRAO150      21 58 17  23.0  43.1 -6.0     -69.1     2      320   17 27 55
17 28 27  ---          21 58 47  23.0  43.1 -6.0     -69.2    32      324   17 27 56

17 28 41  J0350+5201   21 59 03  24.7  42.6 -5.9     -71.2     2      324   17 28 41
17 29 23  ---          21 59 33  24.8  42.6 -5.9     -71.3    42      330   17 28 42

17 29 43  NRAO150      22 00 05  23.2  43.2 -6.0     -69.4     9      330   17 29 43
17 30 13  ---          22 00 35  23.3  43.2 -6.0     -69.5    30      333   17 29 44

17 30 24  J0350+5138   22 00 47  24.9  43.1 -5.8     -71.4     0      333   17 30 24
17 30 54  ---          22 01 17  25.0  43.1 -5.8     -71.5    30      337   17 30 25

17 31 06  NRAO150      22 01 28  23.4  43.3 -6.0     -69.7     0      337   17 31 06
17 31 36  ---          22 01 58  23.5  43.3 -6.0     -69.8    30      341   17 31 07

17 31 47  J0350+5201   22 02 10  25.2  42.7 -5.8     -71.8     0      341   17 31 47
17 32 17  ---          22 02 40  25.2  42.8 -5.8     -71.9    30      345   17 31 48

17 32 37  NRAO150      22 03 00  23.7  43.4 -6.0     -69.9     9      345   17 32 37
17 33 07  ---          22 03 30  23.7  43.4 -6.0     -70.0    30      349   17 32 38

17 33 18  J0350+5138   22 03 41  25.3  43.2 -5.8     -71.9     0      349   17 33 18
17 33 48  ---          22 04 11  25.4  43.2 -5.8     -72.0    30      353   17 33 19

17 33 59  NRAO150      22 04 22  23.9  43.5 -5.9     -70.2     0      353   17 33 59
17 34 29  ---          22 04 52  23.9  43.5 -5.9     -70.3    30      357   17 34 00
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

17 34 41  J0350+5201   22 05 04  25.6  42.9 -5.8     -72.3     0      357   17 34 41
17 35 11  ---          22 05 34  25.7  42.9 -5.8     -72.4    30      360   17 34 42

17 35 31  NRAO150      22 05 54  24.1  43.6 -5.9     -70.4     9      360   17 35 31
17 36 01  ---          22 06 24  24.2  43.6 -5.9     -70.5    30      364   17 35 32

17 36 12  J0350+5138   22 06 35  25.8  43.4 -5.8     -72.4     0      364   17 36 12
17 36 42  ---          22 07 06  25.8  43.4 -5.7     -72.5    30      368   17 36 13

17 36 53  NRAO150      22 07 17  24.3  43.6 -5.9     -70.7     0      368   17 36 53
17 37 23  ---          22 07 47  24.4  43.7 -5.9     -70.8    30      372   17 36 54

17 37 35  J0350+5201   22 07 58  26.0  43.0 -5.7     -72.8     0      372   17 37 35
17 38 05  ---          22 08 28  26.1  43.1 -5.7     -72.9    30      376   17 37 36

17 38 25  NRAO150      22 08 49  24.5  43.7 -5.9     -70.9     9      376   17 38 25
17 38 55  ---          22 09 19  24.6  43.7 -5.9     -71.0    30      380   17 38 26

17 39 06  J0350+5138   22 09 30  26.2  43.5 -5.7     -72.9     0      380   17 39 06
17 39 36  ---          22 10 00  26.3  43.5 -5.7     -73.0    30      384   17 39 07

17 39 49  NRAO150      22 10 12  24.7  43.8 -5.8     -71.2     1      384   17 39 49
17 40 20  ---          22 10 43  24.8  43.8 -5.8     -71.3    32      388   17 39 50

17 40 34  J0350+5201   22 10 58  26.5  43.2 -5.7     -73.3     2      388   17 40 34
17 41 14  ---          22 11 28  26.5  43.2 -5.7     -73.4    41      393   17 40 35

17 41 34  NRAO150      22 11 59  25.0  43.9 -5.8     -71.5     9      393   17 41 34
17 42 04  ---          22 12 29  25.1  43.9 -5.8     -71.6    30      397   17 41 35

17 42 17  J0350+5138   22 12 41  26.7  43.7 -5.7     -73.5     1      397   17 42 17
17 42 54  ---          22 13 11  26.7  43.7 -5.6     -73.6    37      402   17 42 18

17 43 06  NRAO150      22 13 30  25.2  44.0 -5.8     -71.7     1      402   17 43 06
17 43 37  ---          22 14 00  25.3  44.0 -5.8     -71.8    31      406   17 43 07

17 43 51  J0350+5201   22 14 15  26.9  43.3 -5.6     -73.9     2      406   17 43 51
17 44 31  ---          22 14 45  27.0  43.4 -5.6     -74.0    41      411   17 43 52

17 44 51  NRAO150      22 15 16  25.5  44.1 -5.8     -72.0     9      411   17 44 51
17 45 21  ---          22 15 46  25.6  44.1 -5.8     -72.1    30      415   17 44 52

17 45 34  J0350+5138   22 15 58  27.1  43.8 -5.6     -74.1     1      415   17 45 34
17 46 10  ---          22 16 29  27.2  43.9 -5.6     -74.1    37      420   17 45 35
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

17 46 22  NRAO150      22 16 47  25.7  44.2 -5.7     -72.3     1      420   17 46 22
17 46 54  ---          22 17 17  25.8  44.2 -5.7     -72.4    31      424   17 46 23

17 47 07  J0350+5201   22 17 32  27.4  43.5 -5.6     -74.5     2      424   17 47 07
17 47 47  ---          22 18 02  27.5  43.5 -5.6     -74.5    40      429   17 47 08

17 48 07  NRAO150      22 18 32  26.0  44.2 -5.7     -72.6     9      429   17 48 07
17 48 37  ---          22 19 03  26.1  44.3 -5.7     -72.7    30      433   17 48 08

17 48 50  J0350+5138   22 19 15  27.6  44.0 -5.5     -74.6     1      433   17 48 50
17 49 26  ---          22 19 45  27.7  44.0 -5.5     -74.7    36      437   17 48 51

17 49 38  NRAO150      22 20 04  26.2  44.3 -5.7     -72.9     1      437   17 49 38
17 50 09  ---          22 20 34  26.3  44.4 -5.7     -72.9    31      441   17 49 39

17 50 22  J0350+5201   22 20 48  27.9  43.6 -5.5     -75.0     2      441   17 50 22
17 51 02  ---          22 21 18  28.0  43.7 -5.5     -75.1    40      446   17 50 23

17 51 22  NRAO150      22 21 48  26.5  44.4 -5.6     -73.2     9      446   17 51 22
17 51 52  ---          22 22 18  26.5  44.4 -5.6     -73.2    30      450   17 51 23

17 52 05  J0350+5138   22 22 31  28.1  44.1 -5.5     -75.2     1      450   17 52 05
17 52 41  ---          22 23 01  28.2  44.2 -5.5     -75.3    36      455   17 52 06

17 52 53  NRAO150      22 23 19  26.7  44.5 -5.6     -73.4     1      455   17 52 53
17 53 24  ---          22 23 49  26.8  44.5 -5.6     -73.5    31      459   17 52 54

17 53 37  J0350+5201   22 24 03  28.4  43.8 -5.5     -75.6     2      459   17 53 37
17 54 17  ---          22 24 33  28.5  43.8 -5.5     -75.7    40      464   17 53 38

17 54 37  NRAO150      22 25 03  27.0  44.6 -5.6     -73.7     9      464   17 54 37
17 55 07  ---          22 25 33  27.0  44.6 -5.6     -73.8    30      468   17 54 38

17 55 19  J0350+5138   22 25 45  28.6  44.3 -5.4     -75.8     1      468   17 55 19
17 55 55  ---          22 26 16  28.7  44.3 -5.4     -75.9    36      473   17 55 20

17 56 07  NRAO150      22 26 34  27.2  44.7 -5.6     -74.0     1      473   17 56 07
17 56 38  ---          22 27 04  27.3  44.7 -5.6     -74.1    31      477   17 56 08

17 56 51  J0350+5201   22 27 18  28.9  43.9 -5.4     -76.2     2      477   17 56 51
17 57 31  ---          22 27 48  29.0  43.9 -5.4     -76.3    40      482   17 56 52

17 57 51  NRAO150      22 28 18  27.4  44.7 -5.5     -74.3     9      482   17 57 51
17 58 21  ---          22 28 48  27.5  44.8 -5.5     -74.4    30      486   17 57 52
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

17 58 33  J0350+5138   22 29 00  29.1  44.4 -5.4     -76.3     1      486   17 58 33
17 59 09  ---          22 29 30  29.2  44.4 -5.4     -76.4    36      490   17 58 34

17 59 21  NRAO150      22 29 48  27.7  44.8 -5.5     -74.5     1      490   17 59 21
17 59 51  ---          22 30 18  27.8  44.8 -5.5     -74.6    31      494   17 59 22

18 00 04  J0350+5201   22 30 31  29.4  44.1 -5.4     -76.8     2      494   18 00 04
18 00 44  ---          22 31 02  29.4  44.1 -5.3     -76.8    39      499   18 00 05

18 01 04  NRAO150      22 31 31  27.9  44.9 -5.5     -74.8     9      499   18 01 04
18 01 34  ---          22 32 01  28.0  44.9 -5.5     -74.9    30      503   18 01 05

18 01 46  J0350+5138   22 32 13  29.6  44.6 -5.3     -76.9     1      503   18 01 46
18 02 22  ---          22 32 43  29.7  44.6 -5.3     -77.0    36      508   18 01 47

18 02 34  NRAO150      22 33 01  28.2  45.0 -5.5     -75.1     1      508   18 02 34
18 03 04  ---          22 33 31  28.2  45.0 -5.5     -75.2    31      512   18 02 35

18 03 17  J0350+5201   22 33 45  29.8  44.2 -5.3     -77.3     2      512   18 03 17
18 03 56  ---          22 34 15  29.9  44.2 -5.3     -77.4    39      517   18 03 18

18 04 16  NRAO150      22 34 44  28.4  45.0 -5.4     -75.4     9      517   18 04 16
18 04 46  ---          22 35 14  28.5  45.1 -5.4     -75.5    30      521   18 04 17

18 04 58  J0350+5138   22 35 26  30.1  44.7 -5.3     -77.5     1      521   18 04 58
18 05 34  ---          22 35 56  30.1  44.7 -5.3     -77.6    36      525   18 04 59

18 05 46  NRAO150      22 36 14  28.7  45.1 -5.4     -75.6     1      525   18 05 46
18 06 16  ---          22 36 44  28.7  45.1 -5.4     -75.7    30      529   18 05 47

18 06 29  J0350+5201   22 36 57  30.3  44.3 -5.3     -77.9     2      529   18 06 29
18 07 08  ---          22 37 27  30.4  44.3 -5.2     -78.0    39      534   18 06 30

18 07 28  NRAO150      22 37 56  28.9  45.2 -5.4     -75.9     9      534   18 07 28
18 07 58  ---          22 38 26  29.0  45.2 -5.4     -76.0    30      538   18 07 29

18 08 10  J0350+5138   22 38 38  30.6  44.8 -5.2     -78.0     1      538   18 08 10
18 08 45  ---          22 39 08  30.6  44.8 -5.2     -78.1    36      543   18 08 11

18 08 57  NRAO150      22 39 26  29.1  45.2 -5.4     -76.2     1      543   18 08 57
18 09 28  ---          22 39 56  29.2  45.3 -5.3     -76.3    30      546   18 08 58

18 09 40  J0350+5201   22 40 09  30.8  44.4 -5.2     -78.5     1      546   18 09 40
18 10 19  ---          22 40 39  30.9  44.4 -5.2     -78.6    39      551   18 09 41
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

18 10 39  NRAO150      22 41 08  29.4  45.3 -5.3     -76.5     9      551   18 10 39
18 11 09  ---          22 41 38  29.5  45.3 -5.3     -76.6    30      555   18 10 40

18 11 21  J0350+5138   22 41 50  31.0  44.9 -5.2     -78.6     1      555   18 11 21
18 11 57  ---          22 42 20  31.1  44.9 -5.2     -78.7    36      560   18 11 22

18 12 08  NRAO150      22 42 37  29.6  45.4 -5.3     -76.8     1      560   18 12 08
18 12 39  ---          22 43 08  29.7  45.4 -5.3     -76.8    30      564   18 12 09

18 12 51  J0350+5201   22 43 20  31.3  44.5 -5.1     -79.0     1      564   18 12 51
18 13 30  ---          22 43 50  31.4  44.5 -5.1     -79.1    39      569   18 12 52

18 13 50  NRAO150      22 44 19  29.9  45.4 -5.3     -77.1     9      569   18 13 50
18 14 20  ---          22 44 49  30.0  45.5 -5.3     -77.1    30      573   18 13 51

18 14 32  J0350+5138   22 45 01  31.5  45.0 -5.1     -79.2     1      573   18 14 32
18 15 07  ---          22 45 31  31.6  45.1 -5.1     -79.3    35      577   18 14 33

18 15 19  NRAO150      22 45 48  30.1  45.5 -5.2     -77.3     1      577   18 15 19
18 15 49  ---          22 46 18  30.2  45.5 -5.2     -77.4    30      581   18 15 20

18 16 01  J0350+5201   22 46 31  31.8  44.6 -5.1     -79.6     1      581   18 16 01
18 16 40  ---          22 47 01  31.8  44.7 -5.1     -79.7    39      586   18 16 02

18 17 00  NRAO150      22 47 30  30.4  45.6 -5.2     -77.6     9      586   18 17 00
18 17 30  ---          22 48 00  30.5  45.6 -5.2     -77.7    30      590   18 17 01

18 17 42  J0350+5138   22 48 12  32.0  45.1 -5.1     -79.7     1      590   18 17 42
18 18 17  ---          22 48 42  32.1  45.2 -5.0     -79.8    35      595   18 17 43

18 18 29  NRAO150      22 48 59  30.6  45.6 -5.2     -77.9     1      595   18 18 29
18 18 59  ---          22 49 29  30.7  45.7 -5.2     -78.0    30      598   18 18 30

18 19 11  J0350+5201   22 49 41  32.3  44.7 -5.0     -80.2     1      598   18 19 11
18 19 50  ---          22 50 11  32.3  44.8 -5.0     -80.3    38      603   18 19 12

18 20 10  NRAO150      22 50 40  30.9  45.7 -5.2     -78.2     9      603   18 20 10
18 20 40  ---          22 51 10  30.9  45.7 -5.2     -78.2    30      607   18 20 11

18 21 38  DA193        22 52 08   8.2  48.2 -7.1     -56.6     5      607   18 21 38
18 28 28  ---          22 57 09   9.0  48.7 -7.0     -57.3   411      660   18 21 39

18 29 28  J0350+5138   23 00 00  33.8  45.5 -4.9     -81.9     3      660   18 29 28
18 29 58  ---          23 00 30  33.9  45.5 -4.9     -82.0    30      664   18 29 29
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

18 30 09  NRAO150      23 00 41  32.4  46.0 -5.0     -79.9     0      664   18 30 09
18 30 39  ---          23 01 11  32.5  46.1 -5.0     -80.0    30      668   18 30 10

18 30 51  J0350+5201   23 01 23  34.0  45.1 -4.8     -82.3     0      668   18 30 51
18 31 21  ---          23 01 53  34.1  45.1 -4.8     -82.4    30      672   18 30 52

18 31 41  NRAO150      23 02 13  32.6  46.1 -5.0     -80.2     9      672   18 31 41
18 32 11  ---          23 02 43  32.7  46.1 -5.0     -80.3    30      676   18 31 42

18 32 22  J0350+5138   23 02 54  34.3  45.6 -4.8     -82.4     0      676   18 32 22
18 32 52  ---          23 03 24  34.3  45.6 -4.8     -82.5    30      679   18 32 23

18 33 03  NRAO150      23 03 35  32.9  46.1 -5.0     -80.4     0      679   18 33 03
18 33 33  ---          23 04 06  32.9  46.2 -4.9     -80.5    30      683   18 33 04

18 33 44  J0350+5201   23 04 17  34.5  45.1 -4.8     -82.8     0      683   18 33 44
18 34 14  ---          23 04 47  34.5  45.1 -4.8     -82.9    30      687   18 33 45

18 34 34  NRAO150      23 05 07  33.1  46.2 -4.9     -80.7     9      687   18 34 34
18 35 04  ---          23 05 37  33.2  46.2 -4.9     -80.8    30      691   18 34 35

18 35 15  J0350+5138   23 05 48  34.7  45.6 -4.8     -82.9     0      691   18 35 15
18 35 45  ---          23 06 18  34.8  45.6 -4.8     -83.0    30      695   18 35 16

18 35 57  NRAO150      23 06 30  33.3  46.2 -4.9     -81.0     0      695   18 35 57
18 36 27  ---          23 07 00  33.4  46.2 -4.9     -81.0    30      699   18 35 58

18 36 38  J0350+5201   23 07 11  34.9  45.2 -4.7     -83.4     0      699   18 36 38
18 37 08  ---          23 07 41  35.0  45.2 -4.7     -83.5    30      703   18 36 39

18 37 28  NRAO150      23 08 01  33.5  46.3 -4.9     -81.2     9      703   18 37 28
18 37 58  ---          23 08 31  33.6  46.3 -4.9     -81.3    30      706   18 37 29

18 38 09  J0350+5138   23 08 43  35.2  45.7 -4.7     -83.5     0      706   18 38 09
18 38 39  ---          23 09 13  35.2  45.7 -4.7     -83.5    30      710   18 38 10

18 38 50  NRAO150      23 09 24  33.8  46.3 -4.9     -81.5     0      710   18 38 50
18 39 20  ---          23 09 54  33.8  46.3 -4.8     -81.6    30      714   18 38 51

18 39 32  J0350+5201   23 10 06  35.4  45.3 -4.7     -83.9     1      714   18 39 32
18 40 10  ---          23 10 36  35.4  45.3 -4.7     -84.0    38      719   18 39 33

18 40 30  NRAO150      23 11 04  34.0  46.4 -4.8     -81.8     9      719   18 40 30
18 41 00  ---          23 11 34  34.1  46.4 -4.8     -81.9    30      723   18 40 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

18 41 11  J0350+5138   23 11 45  35.6  45.8 -4.7     -84.0     0      723   18 41 11
18 41 46  ---          23 12 16  35.7  45.8 -4.7     -84.1    35      727   18 41 12

18 41 57  NRAO150      23 12 32  34.3  46.4 -4.8     -82.0     0      727   18 41 57
18 42 27  ---          23 13 02  34.3  46.4 -4.8     -82.1    30      731   18 41 58

18 42 39  J0350+5201   23 13 14  35.8  45.3 -4.6     -84.5     1      731   18 42 39
18 43 17  ---          23 13 44  35.9  45.3 -4.6     -84.6    38      736   18 42 40

18 43 37  NRAO150      23 14 11  34.5  46.4 -4.8     -82.3     9      736   18 43 37
18 44 07  ---          23 14 41  34.6  46.5 -4.8     -82.4    30      740   18 43 38

18 44 18  J0350+5138   23 14 53  36.1  45.8 -4.6     -84.6     0      740   18 44 18
18 44 53  ---          23 15 23  36.2  45.8 -4.6     -84.7    35      745   18 44 19

18 45 04  NRAO150      23 15 39  34.7  46.5 -4.8     -82.6     0      745   18 45 04
18 45 34  ---          23 16 09  34.8  46.5 -4.7     -82.7    30      748   18 45 05

18 45 46  J0350+5201   23 16 21  36.3  45.4 -4.6     -85.1     1      748   18 45 46
18 46 23  ---          23 16 51  36.4  45.4 -4.6     -85.2    37      753   18 45 47

18 46 43  NRAO150      23 17 18  35.0  46.5 -4.7     -82.9     9      753   18 46 43
18 47 13  ---          23 17 48  35.1  46.5 -4.7     -83.0    30      757   18 46 44

18 47 25  J0350+5138   23 18 00  36.6  45.9 -4.6     -85.2     0      757   18 47 25
18 47 59  ---          23 18 30  36.7  45.9 -4.6     -85.3    35      762   18 47 26

18 48 10  NRAO150      23 18 46  35.2  46.6 -4.7     -83.2     0      762   18 48 10
18 48 40  ---          23 19 16  35.3  46.6 -4.7     -83.2    30      765   18 48 11

18 48 52  J0350+5201   23 19 28  36.8  45.4 -4.5     -85.7     1      765   18 48 52
18 49 30  ---          23 19 58  36.9  45.4 -4.5     -85.8    37      770   18 48 53

18 49 50  NRAO150      23 20 25  35.5  46.6 -4.7     -83.5     9      770   18 49 50
18 50 20  ---          23 20 55  35.6  46.6 -4.7     -83.5    30      774   18 49 51

18 50 31  J0350+5138   23 21 06  37.1  45.9 -4.5     -85.8     0      774   18 50 31
18 51 05  ---          23 21 36  37.1  45.9 -4.5     -85.8    35      779   18 50 32

18 51 16  NRAO150      23 21 52  35.7  46.6 -4.6     -83.7     0      779   18 51 16
18 51 46  ---          23 22 22  35.8  46.6 -4.6     -83.8    30      782   18 51 17

18 51 58  J0350+5201   23 22 34  37.3  45.5 -4.5     -86.3     1      782   18 51 58
18 52 36  ---          23 23 04  37.3  45.5 -4.5     -86.4    37      787   18 51 59
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

18 52 56  NRAO150      23 23 31  36.0  46.7 -4.6     -84.0     9      787   18 52 56
18 53 26  ---          23 24 02  36.0  46.7 -4.6     -84.1    30      791   18 52 57

18 53 37  J0350+5138   23 24 13  37.5  46.0 -4.5     -86.3     0      791   18 53 37
18 54 11  ---          23 24 43  37.6  46.0 -4.4     -86.4    34      795   18 53 38

18 54 22  NRAO150      23 24 58  36.2  46.7 -4.6     -84.3     0      795   18 54 22
18 54 52  ---          23 25 29  36.3  46.7 -4.6     -84.4    30      799   18 54 23

18 55 04  J0350+5201   23 25 40  37.7  45.5 -4.4     -86.8     1      799   18 55 04
18 55 41  ---          23 26 10  37.8  45.5 -4.4     -86.9    37      804   18 55 05

18 56 01  NRAO150      23 26 38  36.5  46.7 -4.6     -84.6     9      804   18 56 01
18 56 31  ---          23 27 08  36.5  46.7 -4.6     -84.7    30      808   18 56 02

18 56 42  J0350+5138   23 27 19  38.0  46.0 -4.4     -86.9     0      808   18 56 42
18 57 17  ---          23 27 49  38.1  46.0 -4.4     -87.0    34      812   18 56 43

18 57 28  NRAO150      23 28 05  36.7  46.7 -4.5     -84.9     0      812   18 57 28
18 57 58  ---          23 28 35  36.8  46.7 -4.5     -84.9    30      816   18 57 29

18 58 10  J0350+5201   23 28 46  38.2  45.5 -4.4     -87.4     1      816   18 58 10
18 58 47  ---          23 29 16  38.3  45.5 -4.4     -87.5    37      821   18 58 11

18 59 07  NRAO150      23 29 44  36.9  46.8 -4.5     -85.2     9      821   18 59 07
18 59 37  ---          23 30 14  37.0  46.8 -4.5     -85.2    30      825   18 59 08

18 59 48  J0350+5138   23 30 25  38.5  46.0 -4.4     -87.5     0      825   18 59 48
19 00 22  ---          23 30 55  38.6  46.0 -4.3     -87.6    34      829   18 59 49

19 00 33  NRAO150      23 31 10  37.2  46.8 -4.5     -85.4     0      829   19 00 33
19 01 03  ---          23 31 40  37.2  46.8 -4.5     -85.5    30      833   19 00 34

19 01 15  J0350+5201   23 31 52  38.7  45.6 -4.3     -88.0     1      833   19 01 15
19 01 52  ---          23 32 22  38.8  45.6 -4.3     -88.1    37      838   19 01 16

19 02 12  NRAO150      23 32 49  37.4  46.8 -4.5     -85.7     9      838   19 02 12
19 02 42  ---          23 33 19  37.5  46.8 -4.5     -85.8    30      842   19 02 13

19 02 53  J0350+5138   23 33 31  39.0  46.1 -4.3     -88.1     0      842   19 02 53
19 03 27  ---          23 34 01  39.1  46.1 -4.3     -88.2    34      846   19 02 54

19 03 38  NRAO150      23 34 16  37.7  46.8 -4.4     -86.0     0      846   19 03 38
19 04 08  ---          23 34 46  37.7  46.8 -4.4     -86.1    30      850   19 03 39
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

19 04 20  J0350+5201   23 34 58  39.2  45.6 -4.3     -88.6     1      850   19 04 20
19 04 57  ---          23 35 28  39.2  45.6 -4.3     -88.7    37      855   19 04 21

19 05 17  NRAO150      23 35 55  37.9  46.9 -4.4     -86.3     9      855   19 05 17
19 05 47  ---          23 36 25  38.0  46.9 -4.4     -86.4    30      859   19 05 18

19 05 58  J0350+5138   23 36 36  39.5  46.1 -4.3     -88.7     0      859   19 05 58
19 06 32  ---          23 37 06  39.5  46.1 -4.2     -88.8    34      863   19 05 59

19 06 43  NRAO150      23 37 21  38.1  46.9 -4.4     -86.6     0      863   19 06 43
19 07 13  ---          23 37 51  38.2  46.9 -4.4     -86.7    30      867   19 06 44

19 07 25  J0350+5201   23 38 03  39.6  45.6 -4.2     -89.2     1      867   19 07 25
19 08 02  ---          23 38 33  39.7  45.6 -4.2     -89.3    37      872   19 07 26

19 08 22  NRAO150      23 39 00  38.4  46.9 -4.4     -86.9     9      872   19 08 22
19 08 52  ---          23 39 30  38.5  46.9 -4.4     -87.0    30      875   19 08 23

19 09 03  J0350+5138   23 39 41  39.9  46.1 -4.2     -89.3     0      875   19 09 03
19 09 37  ---          23 40 11  40.0  46.1 -4.2     -89.4    34      880   19 09 04

19 09 48  NRAO150      23 40 27  38.6  46.9 -4.3     -87.2     0      880   19 09 48
19 10 18  ---          23 40 57  38.7  46.9 -4.3     -87.2    30      884   19 09 49

19 10 29  J0350+5201   23 41 08  40.1  45.6 -4.2     -89.8     1      884   19 10 29
19 11 06  ---          23 41 38  40.2  45.6 -4.2     -89.9    37      888   19 10 30

19 11 26  NRAO150      23 42 05  38.9  46.9 -4.3     -87.5     9      888   19 11 26
19 11 56  ---          23 42 35  39.0  46.9 -4.3     -87.6    30      892   19 11 27

19 12 07  J0350+5138   23 42 46  40.4  46.1 -4.1     -89.9     0      892   19 12 07
19 12 41  ---          23 43 16  40.5  46.1 -4.1     -90.0    34      897   19 12 08

19 12 52  NRAO150      23 43 32  39.1  46.9 -4.3     -87.7     0      897   19 12 52
19 13 22  ---          23 44 02  39.2  46.9 -4.3     -87.8    30      901   19 12 53

19 13 34  J0350+5201   23 44 13  40.6  45.6 -4.1     -90.4     1      901   19 13 34
19 14 11  ---          23 44 43  40.7  45.6 -4.1     -90.5    37      905   19 13 35

19 14 31  NRAO150      23 45 10  39.4  47.0 -4.3     -88.0     9      905   19 14 31
19 15 01  ---          23 45 40  39.4  47.0 -4.3     -88.1    30      909   19 14 32

19 15 12  J0350+5138   23 45 51  40.9  46.1 -4.1     -90.5     0      909   19 15 12
19 15 46  ---          23 46 21  41.0  46.1 -4.1     -90.6    34      914   19 15 13
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

19 15 57  NRAO150      23 46 36  39.6  47.0 -4.2     -88.3     0      914   19 15 57
19 16 27  ---          23 47 06  39.7  47.0 -4.2     -88.4    30      917   19 15 58

19 16 38  J0350+5201   23 47 18  41.1  45.6 -4.1     -91.1     1      917   19 16 38
19 17 15  ---          23 47 48  41.1  45.6 -4.1     -91.2    36      922   19 16 39

19 17 35  NRAO150      23 48 15  39.8  47.0 -4.2     -88.6     9      922   19 17 35
19 18 05  ---          23 48 45  39.9  47.0 -4.2     -88.7    30      926   19 17 36

19 18 16  J0350+5138   23 48 56  41.4  46.1 -4.0     -91.1     0      926   19 18 16
19 18 50  ---          23 49 26  41.5  46.1 -4.0     -91.2    34      930   19 18 17

19 19 01  NRAO150      23 49 41  40.1  47.0 -4.2     -88.9     0      930   19 19 01
19 19 31  ---          23 50 11  40.2  47.0 -4.2     -89.0    30      934   19 19 02

19 19 42  J0350+5201   23 50 23  41.5  45.6 -4.0     -91.7     1      934   19 19 42
19 20 19  ---          23 50 53  41.6  45.6 -4.0     -91.8    36      939   19 19 43

19 20 39  NRAO150      23 51 19  40.3  47.0 -4.2     -89.2     9      939   19 20 39
19 21 09  ---          23 51 49  40.4  47.0 -4.1     -89.3    30      943   19 20 40

19 21 20  J0350+5138   23 52 00  41.8  46.1 -4.0     -91.7     0      943   19 21 20
19 21 54  ---          23 52 31  41.9  46.1 -4.0     -91.8    34      947   19 21 21

19 22 05  NRAO150      23 52 45  40.6  47.0 -4.1     -89.5     0      947   19 22 05
19 22 35  ---          23 53 15  40.6  47.0 -4.1     -89.6    30      951   19 22 06

19 22 46  J0350+5201   23 53 27  42.0  45.5 -4.0     -92.3     1      951   19 22 46
19 23 22  ---          23 53 57  42.1  45.5 -4.0     -92.4    36      956   19 22 47

19 23 42  NRAO150      23 54 23  40.8  47.0 -4.1     -89.8     9      956   19 23 42
19 24 12  ---          23 54 54  40.9  47.0 -4.1     -89.9    30      959   19 23 43

19 24 24  J0350+5138   23 55 05  42.3  46.0 -3.9     -92.4     0      959   19 24 24
19 24 57  ---          23 55 35  42.4  46.0 -3.9     -92.5    34      964   19 24 25

19 25 08  NRAO150      23 55 50  41.0  47.0 -4.1     -90.1     0      964   19 25 08
19 25 38  ---          23 56 20  41.1  47.0 -4.1     -90.2    30      968   19 25 09

19 25 50  J0350+5201   23 56 31  42.5  45.5 -3.9     -92.9     1      968   19 25 50
19 26 26  ---          23 57 01  42.6  45.5 -3.9     -93.0    36      972   19 25 51

19 26 46  NRAO150      23 57 28  41.3  47.0 -4.1     -90.4     9      972   19 26 46
19 27 16  ---          23 57 58  41.4  47.0 -4.0     -90.5    30      976   19 26 47
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

19 27 27  J0350+5138   23 58 09  42.8  46.0 -3.9     -93.0     0      976   19 27 27
19 28 01  ---          23 58 39  42.9  46.0 -3.9     -93.1    33      980   19 27 28

19 28 12  NRAO150      23 58 54  41.5  47.0 -4.0     -90.7     0      980   19 28 12
19 28 42  ---          23 59 24  41.6  47.0 -4.0     -90.8    30      984   19 28 13

19 28 54  J0350+5201   23 59 35  42.9  45.5 -3.9     -93.6     1      984   19 28 54
19 29 30  ---          00 00 05  43.0  45.5 -3.9     -93.7    36      989   19 28 55

19 29 50  NRAO150      00 00 32  41.8  47.0 -4.0     -91.0     9      989   19 29 50
19 30 20  ---          00 01 02  41.9  47.0 -4.0     -91.1    30      993   19 29 51

19 30 31  J0350+5138   00 01 13  43.3  46.0 -3.8     -93.6     0      993   19 30 31
19 31 01  ---          00 01 43  43.4  46.0 -3.8     -93.7    30      997   19 30 32

19 31 12  NRAO150      00 01 54  42.0  47.0 -4.0     -91.3     0      997   19 31 12
19 31 42  ---          00 02 24  42.1  47.0 -4.0     -91.4    30     1001   19 31 13

19 31 53  J0350+5201   00 02 36  43.4  45.4 -3.8     -94.2     1     1001   19 31 53
19 32 23  ---          00 03 06  43.5  45.4 -3.8     -94.3    30     1004   19 31 54

19 32 43  NRAO150      00 03 26  42.2  47.0 -4.0     -91.6     9     1004   19 32 43
19 33 13  ---          00 03 56  42.3  47.0 -3.9     -91.7    30     1008   19 32 44

19 33 24  J0350+5138   00 04 07  43.7  45.9 -3.8     -94.2     0     1008   19 33 24
19 33 54  ---          00 04 37  43.8  45.9 -3.8     -94.3    30     1012   19 33 25

19 34 05  NRAO150      00 04 48  42.5  47.0 -3.9     -91.9     0     1012   19 34 05
19 34 35  ---          00 05 18  42.5  47.0 -3.9     -92.0    30     1016   19 34 06

19 34 47  J0350+5201   00 05 30  43.9  45.4 -3.8     -94.8     1     1016   19 34 47
19 35 17  ---          00 06 00  43.9  45.4 -3.8     -94.9    30     1020   19 34 48

19 35 37  NRAO150      00 06 20  42.7  46.9 -3.9     -92.2     9     1020   19 35 37
19 36 07  ---          00 06 50  42.8  46.9 -3.9     -92.3    30     1024   19 35 38

19 36 18  J0350+5138   00 07 01  44.2  45.9 -3.7     -94.8     0     1024   19 36 18
19 36 48  ---          00 07 31  44.2  45.9 -3.7     -94.9    30     1028   19 36 19

19 36 59  NRAO150      00 07 42  42.9  46.9 -3.9     -92.4     0     1028   19 36 59
19 37 29  ---          00 08 12  43.0  46.9 -3.9     -92.5    30     1031   19 37 00

19 37 40  J0350+5201   00 08 24  44.3  45.3 -3.7     -95.4     1     1031   19 37 40
19 38 10  ---          00 08 54  44.4  45.3 -3.7     -95.5    30     1035   19 37 41
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

19 38 30  NRAO150      00 09 14  43.1  46.9 -3.9     -92.7     9     1035   19 38 30
19 39 00  ---          00 09 44  43.2  46.9 -3.9     -92.8    30     1039   19 38 31

19 39 12  J0350+5138   00 09 55  44.6  45.8 -3.7     -95.4     0     1039   19 39 12
19 39 42  ---          00 10 25  44.7  45.8 -3.7     -95.5    30     1043   19 39 13

19 39 53  NRAO150      00 10 36  43.4  46.9 -3.8     -93.0     1     1043   19 39 53
19 40 23  ---          00 11 06  43.4  46.9 -3.8     -93.1    30     1047   19 39 54

19 40 34  J0350+5201   00 11 18  44.7  45.3 -3.7     -96.0     1     1047   19 40 34
19 41 10  ---          00 11 48  44.8  45.3 -3.7     -96.1    36     1052   19 40 35

19 41 30  NRAO150      00 12 14  43.6  46.9 -3.8     -93.4    10     1052   19 41 30
19 42 00  ---          00 12 44  43.7  46.9 -3.8     -93.5    30     1055   19 41 31

19 42 11  J0350+5138   00 12 55  45.1  45.8 -3.6     -96.0     1     1055   19 42 11
19 42 44  ---          00 13 25  45.2  45.7 -3.6     -96.2    33     1060   19 42 12

19 42 56  NRAO150      00 13 40  43.8  46.9 -3.8     -93.6     1     1060   19 42 56
19 43 26  ---          00 14 10  43.9  46.9 -3.8     -93.7    30     1064   19 42 57

19 43 37  J0350+5201   00 14 21  45.2  45.2 -3.6     -96.7     1     1064   19 43 37
19 44 13  ---          00 14 51  45.3  45.2 -3.6     -96.8    36     1068   19 43 38

19 44 33  NRAO150      00 15 17  44.1  46.8 -3.8     -94.0    10     1068   19 44 33
19 45 03  ---          00 15 47  44.2  46.8 -3.7     -94.1    30     1072   19 44 34

19 45 14  J0350+5138   00 15 58  45.6  45.7 -3.6     -96.7     1     1072   19 45 14
19 45 47  ---          00 16 28  45.6  45.7 -3.6     -96.8    33     1076   19 45 15

19 45 58  NRAO150      00 16 43  44.3  46.8 -3.7     -94.3     1     1076   19 45 58
19 46 28  ---          00 17 13  44.4  46.8 -3.7     -94.4    30     1080   19 45 59

19 46 40  J0350+5201   00 17 24  45.7  45.1 -3.6     -97.3     1     1080   19 46 40
19 47 15  ---          00 17 54  45.8  45.1 -3.6     -97.4    36     1085   19 46 41

19 47 35  NRAO150      00 18 20  44.6  46.8 -3.7     -94.6    10     1085   19 47 35
19 48 05  ---          00 18 50  44.7  46.8 -3.7     -94.7    30     1089   19 47 36

19 48 16  J0350+5138   00 19 01  46.0  45.6 -3.5     -97.4     1     1089   19 48 16
19 48 50  ---          00 19 32  46.1  45.6 -3.5     -97.5    33     1093   19 48 17

19 49 01  NRAO150      00 19 46  44.8  46.8 -3.7     -94.9     1     1093   19 49 01
19 49 31  ---          00 20 16  44.9  46.8 -3.7     -95.0    30     1097   19 49 02
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

19 49 42  J0350+5201   00 20 27  46.1  45.0 -3.5     -98.0     1     1097   19 49 42
19 50 18  ---          00 20 58  46.2  45.0 -3.5     -98.1    35     1101   19 49 43

19 50 38  NRAO150      00 21 23  45.1  46.7 -3.7     -95.2    10     1101   19 50 38
19 51 08  ---          00 21 53  45.1  46.7 -3.6     -95.3    30     1105   19 50 39

19 51 19  J0350+5138   00 22 04  46.5  45.5 -3.5     -98.0     1     1105   19 51 19
19 51 52  ---          00 22 34  46.6  45.5 -3.5     -98.1    33     1109   19 51 20

19 52 03  NRAO150      00 22 49  45.3  46.7 -3.6     -95.5     1     1109   19 52 03
19 52 33  ---          00 23 19  45.4  46.7 -3.6     -95.6    30     1113   19 52 04

19 52 45  J0350+5201   00 23 30  46.6  44.9 -3.5     -98.7     1     1113   19 52 45
19 53 20  ---          00 24 01  46.7  44.9 -3.5     -98.8    35     1118   19 52 46

19 53 40  NRAO150      00 24 26  45.5  46.7 -3.6     -95.9    10     1118   19 53 40
19 54 10  ---          00 24 56  45.6  46.7 -3.6     -96.0    30     1122   19 53 41

19 54 21  J0350+5138   00 25 07  47.0  45.4 -3.4     -98.7     1     1122   19 54 21
19 54 54  ---          00 25 37  47.0  45.4 -3.4     -98.8    33     1126   19 54 22

19 55 05  NRAO150      00 25 51  45.8  46.6 -3.6     -96.2     1     1126   19 55 05
19 55 35  ---          00 26 22  45.8  46.6 -3.6     -96.3    30     1130   19 55 06

19 55 47  J0350+5201   00 26 33  47.1  44.8 -3.4     -99.3     1     1130   19 55 47
19 56 22  ---          00 27 03  47.1  44.8 -3.4     -99.5    35     1134   19 55 48

19 56 42  NRAO150      00 27 29  46.0  46.6 -3.6     -96.5    10     1134   19 56 42
19 57 12  ---          00 27 59  46.1  46.6 -3.5     -96.6    30     1138   19 56 43

19 57 23  J0350+5138   00 28 10  47.4  45.3 -3.4     -99.4     1     1138   19 57 23
19 57 56  ---          00 28 40  47.5  45.3 -3.4     -99.5    33     1142   19 57 24

19 58 07  NRAO150      00 28 54  46.2  46.6 -3.5     -96.8     1     1142   19 58 07
19 58 37  ---          00 29 24  46.3  46.5 -3.5     -96.9    30     1146   19 58 08

19 58 49  J0350+5201   00 29 36  47.5  44.7 -3.4    -100.0     2     1146   19 58 49
19 59 24  ---          00 30 06  47.6  44.7 -3.4    -100.1    35     1151   19 58 50

19 59 44  NRAO150      00 30 31  46.5  46.5 -3.5     -97.2    10     1151   19 59 44
20 00 14  ---          00 31 01  46.6  46.5 -3.5     -97.3    30     1155   19 59 45

20 00 25  J0350+5138   00 31 12  47.9  45.2 -3.3    -100.1     1     1155   20 00 25
20 00 58  ---          00 31 42  48.0  45.2 -3.3    -100.2    33     1159   20 00 26
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

20 01 09  NRAO150      00 31 57  46.7  46.5 -3.5     -97.5     1     1159   20 01 09
20 01 39  ---          00 32 27  46.8  46.5 -3.5     -97.6    30     1163   20 01 10

20 01 52  J0350+5201   00 32 39  48.0  44.6 -3.3    -100.7     2     1163   20 01 52
20 02 26  ---          00 33 09  48.1  44.6 -3.3    -100.8    35     1167   20 01 53

20 02 46  NRAO150      00 33 33  47.0  46.4 -3.5     -97.8    10     1167   20 02 46
20 03 16  ---          00 34 04  47.0  46.4 -3.4     -97.9    30     1171   20 02 47

20 03 27  J0350+5138   00 34 15  48.4  45.1 -3.3    -100.7     1     1171   20 03 27
20 04 00  ---          00 34 45  48.4  45.0 -3.3    -100.9    33     1175   20 03 28

20 04 11  NRAO150      00 34 59  47.2  46.4 -3.4     -98.1     1     1175   20 04 11
20 04 41  ---          00 35 29  47.3  46.4 -3.4     -98.2    30     1179   20 04 12

20 04 54  J0350+5201   00 35 41  48.4  44.4 -3.3    -101.4     2     1179   20 04 54
20 05 28  ---          00 36 12  48.5  44.4 -3.3    -101.5    34     1184   20 04 55

20 05 48  NRAO150      00 36 36  47.4  46.3 -3.4     -98.5    10     1184   20 05 48
20 06 18  ---          00 37 06  47.5  46.3 -3.4     -98.6    30     1187   20 05 49

20 06 30  J0350+5138   00 37 18  48.8  44.9 -3.2    -101.4     1     1187   20 06 30
20 07 02  ---          00 37 48  48.9  44.9 -3.2    -101.6    32     1192   20 06 31

20 07 14  NRAO150      00 38 02  47.7  46.3 -3.4     -98.8     1     1192   20 07 14
20 07 44  ---          00 38 32  47.7  46.3 -3.4     -98.9    30     1195   20 07 15

20 07 56  J0350+5201   00 38 44  48.9  44.3 -3.2    -102.1     2     1195   20 07 56
20 08 30  ---          00 39 14  49.0  44.3 -3.2    -102.2    34     1200   20 07 57

20 08 50  NRAO150      00 39 38  47.9  46.2 -3.4     -99.2    10     1200   20 08 50
20 09 20  ---          00 40 08  48.0  46.2 -3.3     -99.3    30     1204   20 08 51

20 09 32  J0350+5138   00 40 20  49.3  44.8 -3.2    -102.2     1     1204   20 09 32
20 10 04  ---          00 40 50  49.4  44.7 -3.2    -102.3    32     1208   20 09 33

20 10 16  NRAO150      00 41 04  48.1  46.2 -3.3     -99.5     1     1208   20 10 16
20 10 46  ---          00 41 34  48.2  46.1 -3.3     -99.6    30     1212   20 10 17

20 10 58  J0350+5201   00 41 47  49.4  44.1 -3.2    -102.8     2     1212   20 10 58
20 11 32  ---          00 42 17  49.4  44.1 -3.2    -103.0    34     1216   20 10 59

20 11 52  NRAO150      00 42 41  48.4  46.1 -3.3     -99.8    10     1216   20 11 52
20 12 22  ---          00 43 11  48.5  46.1 -3.3    -100.0    30     1220   20 11 53
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

20 12 34  J0350+5138   00 43 23  49.7  44.6 -3.1    -102.9     1     1220   20 12 34
20 13 06  ---          00 43 53  49.8  44.6 -3.1    -103.0    32     1224   20 12 35

20 13 18  NRAO150      00 44 07  48.6  46.0 -3.3    -100.2     1     1224   20 13 18
20 13 48  ---          00 44 37  48.7  46.0 -3.3    -100.3    30     1228   20 13 19

20 14 01  J0350+5201   00 44 50  49.8  44.0 -3.1    -103.6     3     1228   20 14 01
20 14 34  ---          00 45 20  49.9  44.0 -3.1    -103.7    33     1232   20 14 02

20 14 54  NRAO150      00 45 44  48.8  46.0 -3.3    -100.5    10     1232   20 14 54
20 15 24  ---          00 46 14  48.9  45.9 -3.2    -100.6    30     1236   20 14 55

20 15 36  J0350+5138   00 46 26  50.2  44.4 -3.1    -103.6     2     1236   20 15 36
20 16 08  ---          00 46 56  50.3  44.4 -3.1    -103.7    32     1240   20 15 37

20 16 20  NRAO150      00 47 10  49.1  45.9 -3.2    -100.9     2     1240   20 16 20
20 16 50  ---          00 47 40  49.1  45.9 -3.2    -101.0    30     1244   20 16 21

20 17 03  J0350+5201   00 47 53  50.3  43.8 -3.1    -104.3     3     1244   20 17 03
20 17 36  ---          00 48 23  50.3  43.8 -3.1    -104.4    33     1248   20 17 04

20 17 56  NRAO150      00 48 46  49.3  45.8 -3.2    -101.2    10     1248   20 17 56
20 18 26  ---          00 49 16  49.4  45.8 -3.2    -101.3    30     1252   20 17 57

20 18 39  J0350+5138   00 49 29  50.7  44.3 -3.0    -104.3     2     1252   20 18 39
20 19 10  ---          00 49 59  50.7  44.2 -3.0    -104.5    32     1256   20 18 40

20 19 22  NRAO150      00 50 13  49.5  45.8 -3.2    -101.6     2     1256   20 19 22
20 19 52  ---          00 50 43  49.6  45.7 -3.2    -101.7    30     1260   20 19 23

20 20 06  J0350+5201   00 50 56  50.7  43.6 -3.0    -105.1     3     1260   20 20 06
20 20 39  ---          00 51 26  50.8  43.6 -3.0    -105.2    33     1264   20 20 07

20 20 59  NRAO150      00 51 49  49.8  45.7 -3.1    -101.9    10     1264   20 20 59
20 21 29  ---          00 52 19  49.9  45.7 -3.1    -102.0    30     1268   20 21 00

20 22 24  DA193        00 53 15  29.2  58.6 -5.1     -72.9     6     1268   20 22 24
20 31 16  ---          00 58 15  30.1  58.9 -5.0     -73.5   532     1337   20 22 25

20 32 13  J0350+5138   01 03 05  52.7  43.3 -2.8    -107.7     5     1337   20 32 13
20 32 43  ---          01 03 35  52.8  43.3 -2.8    -107.9    30     1341   20 32 14

20 32 54  NRAO150      01 03 46  51.6  45.0 -2.9    -104.8     1     1341   20 32 54
20 33 24  ---          01 04 16  51.7  45.0 -2.9    -104.9    30     1344   20 32 55
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

20 33 35  J0350+5201   01 04 28  52.7  42.6 -2.8    -108.5     1     1344   20 33 35
20 34 05  ---          01 04 58  52.8  42.6 -2.8    -108.6    30     1348   20 33 36

20 34 25  NRAO150      01 05 18  51.8  44.9 -2.9    -105.2    10     1348   20 34 25
20 34 55  ---          01 05 48  51.9  44.9 -2.9    -105.3    30     1352   20 34 26

20 35 07  J0350+5138   01 05 59  53.1  43.1 -2.8    -108.5     1     1352   20 35 07
20 35 37  ---          01 06 29  53.2  43.1 -2.8    -108.6    30     1356   20 35 08

20 35 48  NRAO150      01 06 41  52.1  44.8 -2.9    -105.5     1     1356   20 35 48
20 36 18  ---          01 07 11  52.1  44.8 -2.9    -105.6    30     1360   20 35 49

20 36 29  J0350+5201   01 07 22  53.1  42.4 -2.7    -109.2     1     1360   20 36 29
20 36 59  ---          01 07 52  53.2  42.4 -2.7    -109.4    30     1364   20 36 30

20 37 19  NRAO150      01 08 12  52.3  44.7 -2.9    -105.9    10     1364   20 37 19
20 37 49  ---          01 08 42  52.4  44.7 -2.9    -106.0    30     1368   20 37 20

20 38 00  J0350+5138   01 08 53  53.5  42.8 -2.7    -109.3     1     1368   20 38 00
20 38 30  ---          01 09 24  53.6  42.8 -2.7    -109.4    30     1372   20 38 01

20 38 41  NRAO150      01 09 35  52.5  44.6 -2.9    -106.2     1     1372   20 38 41
20 39 11  ---          01 10 05  52.6  44.6 -2.8    -106.4    30     1375   20 38 42

20 39 23  J0350+5201   01 10 16  53.6  42.2 -2.7    -110.0     1     1375   20 39 23
20 39 53  ---          01 10 46  53.6  42.1 -2.7    -110.2    30     1379   20 39 24

20 40 13  NRAO150      01 11 06  52.7  44.5 -2.8    -106.6    10     1379   20 40 13
20 40 43  ---          01 11 36  52.8  44.4 -2.8    -106.7    30     1383   20 40 14

20 40 54  J0350+5138   01 11 48  54.0  42.6 -2.7    -110.0     1     1383   20 40 54
20 41 24  ---          01 12 18  54.0  42.5 -2.7    -110.2    30     1387   20 40 55

20 41 38  NRAO150      01 12 32  52.9  44.4 -2.8    -107.0     4     1387   20 41 38
20 42 08  ---          01 13 02  53.0  44.3 -2.8    -107.1    30     1391   20 41 39

20 42 23  J0350+5201   01 13 17  54.0  41.9 -2.6    -110.8     5     1391   20 42 23
20 42 54  ---          01 13 47  54.1  41.8 -2.6    -111.0    31     1395   20 42 24

20 43 14  NRAO150      01 14 08  53.2  44.3 -2.8    -107.4    10     1395   20 43 14
20 43 44  ---          01 14 38  53.3  44.2 -2.8    -107.5    30     1399   20 43 15

20 43 58  J0350+5138   01 14 52  54.4  42.3 -2.6    -110.9     4     1399   20 43 58
20 44 28  ---          01 15 22  54.5  42.3 -2.6    -111.0    30     1403   20 43 59
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

20 44 42  NRAO150      01 15 36  53.4  44.1 -2.8    -107.8     4     1403   20 44 42
20 45 12  ---          01 16 07  53.5  44.1 -2.7    -107.9    30     1406   20 44 43

20 45 27  J0350+5201   01 16 22  54.4  41.6 -2.6    -111.7     5     1406   20 45 27
20 45 58  ---          01 16 52  54.5  41.5 -2.6    -111.8    31     1410   20 45 28

20 46 18  NRAO150      01 17 12  53.6  44.0 -2.7    -108.2    10     1410   20 46 18
20 46 48  ---          01 17 42  53.7  44.0 -2.7    -108.3    30     1414   20 46 19

20 47 02  J0350+5138   01 17 57  54.8  42.0 -2.6    -111.7     4     1414   20 47 02
20 47 32  ---          01 18 27  54.9  42.0 -2.6    -111.9    30     1418   20 47 03

20 47 47  NRAO150      01 18 42  53.9  43.9 -2.7    -108.6     4     1418   20 47 47
20 48 17  ---          01 19 12  53.9  43.8 -2.7    -108.7    30     1422   20 47 48

20 48 32  J0350+5201   01 19 27  54.9  41.3 -2.5    -112.5     5     1422   20 48 32
20 49 03  ---          01 19 57  54.9  41.2 -2.5    -112.7    30     1426   20 48 33

20 49 23  NRAO150      01 20 18  54.1  43.7 -2.7    -109.0    10     1426   20 49 23
20 49 53  ---          01 20 48  54.2  43.7 -2.7    -109.1    30     1430   20 49 24

20 50 07  J0350+5138   01 21 02  55.3  41.7 -2.5    -112.6     5     1430   20 50 07
20 50 37  ---          01 21 33  55.4  41.6 -2.5    -112.7    30     1434   20 50 08

20 50 52  NRAO150      01 21 47  54.3  43.6 -2.6    -109.4     5     1434   20 50 52
20 51 22  ---          01 22 17  54.4  43.6 -2.6    -109.5    30     1437   20 50 53

20 51 37  J0350+5201   01 22 33  55.3  41.0 -2.5    -113.4     6     1437   20 51 37
20 52 08  ---          01 23 03  55.4  40.9 -2.5    -113.6    30     1441   20 51 38

20 52 28  NRAO150      01 23 23  54.6  43.5 -2.6    -109.8    10     1441   20 52 28
20 52 58  ---          01 23 53  54.6  43.4 -2.6    -110.0    30     1445   20 52 29

20 53 13  J0350+5138   01 24 08  55.7  41.4 -2.5    -113.5     5     1445   20 53 13
20 53 43  ---          01 24 38  55.8  41.3 -2.5    -113.6    30     1449   20 53 14

20 53 57  NRAO150      01 24 53  54.8  43.3 -2.6    -110.2     5     1449   20 53 57
20 54 27  ---          01 25 23  54.9  43.3 -2.6    -110.4    30     1453   20 53 58

20 54 43  J0350+5201   01 25 39  55.7  40.6 -2.4    -114.3     6     1453   20 54 43
20 55 13  ---          01 26 09  55.8  40.6 -2.4    -114.5    30     1457   20 54 44

20 55 33  NRAO150      01 26 29  55.0  43.2 -2.6    -110.7    10     1457   20 55 33
20 56 03  ---          01 26 59  55.1  43.1 -2.6    -110.8    30     1461   20 55 34
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

20 56 18  J0350+5138   01 27 14  56.2  41.0 -2.4    -114.4     5     1461   20 56 18
20 56 48  ---          01 27 44  56.2  41.0 -2.4    -114.5    30     1465   20 56 19

20 57 03  NRAO150      01 27 59  55.2  43.0 -2.5    -111.1     5     1465   20 57 03
20 57 33  ---          01 28 30  55.3  43.0 -2.5    -111.2    30     1468   20 57 04

20 57 49  J0350+5201   01 28 45  56.2  40.3 -2.4    -115.2     6     1468   20 57 49
20 58 19  ---          01 29 15  56.3  40.2 -2.4    -115.4    30     1472   20 57 50

20 58 39  NRAO150      01 29 35  55.5  42.9 -2.5    -111.5    10     1472   20 58 39
20 59 09  ---          01 30 05  55.5  42.8 -2.5    -111.7    30     1476   20 58 40

20 59 24  J0350+5138   01 30 21  56.6  40.6 -2.4    -115.3     5     1476   20 59 24
20 59 54  ---          01 30 51  56.7  40.6 -2.3    -115.4    30     1480   20 59 25

21 00 09  NRAO150      01 31 06  55.7  42.7 -2.5    -111.9     5     1480   21 00 09
21 00 39  ---          01 31 36  55.8  42.7 -2.5    -112.1    30     1484   21 00 10

21 00 55  J0350+5201   01 31 52  56.6  39.9 -2.3    -116.1     6     1484   21 00 55
21 01 25  ---          01 32 22  56.7  39.8 -2.3    -116.3    30     1488   21 00 56

21 01 45  NRAO150      01 32 42  55.9  42.5 -2.5    -112.4    10     1488   21 01 45
21 02 15  ---          01 33 12  56.0  42.5 -2.5    -112.5    30     1492   21 01 46

21 02 30  J0350+5138   01 33 27  57.0  40.3 -2.3    -116.2     5     1492   21 02 30
21 03 00  ---          01 33 57  57.1  40.2 -2.3    -116.4    30     1495   21 02 31

21 03 15  NRAO150      01 34 13  56.1  42.4 -2.4    -112.8     5     1495   21 03 15
21 03 45  ---          01 34 43  56.2  42.3 -2.4    -113.0    30     1499   21 03 16

21 04 01  J0350+5201   01 34 58  57.0  39.5 -2.3    -117.1     6     1499   21 04 01
21 04 31  ---          01 35 28  57.1  39.4 -2.3    -117.2    30     1503   21 04 02

21 04 51  NRAO150      01 35 49  56.4  42.2 -2.4    -113.3    10     1503   21 04 51
21 05 21  ---          01 36 19  56.4  42.1 -2.4    -113.4    30     1507   21 04 52

21 05 36  J0350+5138   01 36 34  57.5  39.9 -2.3    -117.2     5     1507   21 05 36
21 06 06  ---          01 37 04  57.5  39.8 -2.2    -117.3    30     1511   21 05 37

21 06 22  NRAO150      01 37 19  56.6  42.0 -2.4    -113.7     5     1511   21 06 22
21 06 52  ---          01 37 50  56.7  42.0 -2.4    -113.9    30     1515   21 06 23

21 07 07  J0350+5201   01 38 05  57.5  39.1 -2.2    -118.0     6     1515   21 07 07
21 07 37  ---          01 38 35  57.5  39.0 -2.2    -118.2    30     1519   21 07 08
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

21 07 57  NRAO150      01 38 55  56.8  41.8 -2.4    -114.2    10     1519   21 07 57
21 08 27  ---          01 39 25  56.9  41.8 -2.4    -114.3    30     1523   21 07 58

21 08 43  J0350+5138   01 39 41  57.9  39.4 -2.2    -118.1     5     1523   21 08 43
21 09 13  ---          01 40 11  58.0  39.4 -2.2    -118.3    30     1526   21 08 44

21 09 28  NRAO150      01 40 26  57.0  41.7 -2.3    -114.6     5     1526   21 09 28
21 09 58  ---          01 40 56  57.1  41.6 -2.3    -114.8    30     1530   21 09 29

21 10 13  J0350+5201   01 41 12  57.9  38.7 -2.2    -119.0     5     1530   21 10 13
21 10 43  ---          01 41 42  57.9  38.6 -2.2    -119.2    30     1534   21 10 14

21 11 03  NRAO150      01 42 02  57.3  41.5 -2.3    -115.1    10     1534   21 11 03
21 11 33  ---          01 42 32  57.3  41.4 -2.3    -115.2    30     1538   21 11 04

21 11 48  J0350+5138   01 42 47  58.3  39.0 -2.1    -119.1     5     1538   21 11 48
21 12 18  ---          01 43 17  58.4  38.9 -2.1    -119.3    30     1542   21 11 49

21 12 34  NRAO150      01 43 32  57.5  41.3 -2.3    -115.6     5     1542   21 12 34
21 13 04  ---          01 44 02  57.6  41.2 -2.3    -115.7    30     1546   21 12 35

21 13 19  J0350+5201   01 44 18  58.3  38.2 -2.1    -120.0     5     1546   21 13 19
21 13 49  ---          01 44 48  58.4  38.1 -2.1    -120.2    30     1550   21 13 20

21 14 09  NRAO150      01 45 08  57.7  41.1 -2.3    -116.0    10     1550   21 14 09
21 14 39  ---          01 45 38  57.8  41.0 -2.3    -116.2    30     1553   21 14 10

21 14 54  J0350+5138   01 45 53  58.7  38.6 -2.1    -120.1     5     1553   21 14 54
21 15 24  ---          01 46 23  58.8  38.5 -2.1    -120.3    30     1557   21 14 55

21 15 39  NRAO150      01 46 38  57.9  40.9 -2.2    -116.5     5     1557   21 15 39
21 16 09  ---          01 47 08  58.0  40.8 -2.2    -116.6    30     1561   21 15 40

21 16 24  J0350+5201   01 47 23  58.7  37.8 -2.1    -121.0     5     1561   21 16 24
21 16 54  ---          01 47 53  58.8  37.7 -2.1    -121.2    30     1565   21 16 25

21 17 14  NRAO150      01 48 14  58.1  40.7 -2.2    -117.0    10     1565   21 17 14
21 17 44  ---          01 48 44  58.2  40.6 -2.2    -117.1    30     1569   21 17 15

21 17 59  J0350+5138   01 48 59  59.2  38.1 -2.0    -121.1     5     1569   21 17 59
21 18 29  ---          01 49 29  59.2  38.0 -2.0    -121.3    30     1573   21 18 00

21 18 44  NRAO150      01 49 44  58.4  40.5 -2.2    -117.4     5     1573   21 18 44
21 19 14  ---          01 50 14  58.4  40.4 -2.2    -117.6    30     1577   21 18 45
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

21 19 28  J0350+5201   01 50 28  59.1  37.3 -2.0    -122.0     4     1577   21 19 28
21 19 59  ---          01 50 58  59.2  37.2 -2.0    -122.2    31     1581   21 19 29

21 20 19  NRAO150      01 51 19  58.6  40.2 -2.2    -117.9    10     1581   21 20 19
21 20 49  ---          01 51 49  58.6  40.2 -2.1    -118.1    30     1584   21 20 20

21 21 04  J0350+5138   01 52 04  59.6  37.6 -2.0    -122.1     5     1584   21 21 04
21 21 34  ---          01 52 34  59.6  37.5 -2.0    -122.3    30     1588   21 21 05

21 21 48  NRAO150      01 52 49  58.8  40.0 -2.1    -118.4     5     1588   21 21 48
21 22 18  ---          01 53 19  58.9  40.0 -2.1    -118.6    30     1592   21 21 49

21 22 32  J0350+5201   01 53 33  59.5  36.8 -2.0    -123.1     4     1592   21 22 32
21 23 04  ---          01 54 03  59.6  36.7 -2.0    -123.2    31     1596   21 22 33

21 23 24  NRAO150      01 54 24  59.0  39.8 -2.1    -118.9    10     1596   21 23 24
21 23 54  ---          01 54 54  59.1  39.7 -2.1    -119.1    30     1600   21 23 25

21 24 08  J0350+5138   01 55 09  60.0  37.1 -1.9    -123.2     5     1600   21 24 08
21 24 38  ---          01 55 39  60.0  37.0 -1.9    -123.4    30     1604   21 24 09

21 24 52  NRAO150      01 55 53  59.2  39.6 -2.1    -119.4     4     1604   21 24 52
21 25 22  ---          01 56 23  59.3  39.5 -2.1    -119.6    30     1608   21 24 53

21 25 36  J0350+5201   01 56 37  59.9  36.3 -1.9    -124.1     3     1608   21 25 36
21 26 07  ---          01 57 07  60.0  36.2 -1.9    -124.3    31     1612   21 25 37

21 26 27  NRAO150      01 57 28  59.4  39.3 -2.1    -119.9    10     1612   21 26 27
21 26 57  ---          01 57 58  59.5  39.3 -2.0    -120.1    30     1616   21 26 28

21 27 11  J0350+5138   01 58 13  60.4  36.6 -1.9    -124.2     4     1616   21 27 11
21 27 41  ---          01 58 43  60.4  36.5 -1.9    -124.4    30     1620   21 27 12

21 27 55  NRAO150      01 58 56  59.6  39.1 -2.0    -120.4     4     1620   21 27 55
21 28 25  ---          01 59 27  59.7  39.0 -2.0    -120.6    30     1623   21 27 56

21 28 38  J0350+5201   01 59 40  60.3  35.7 -1.9    -125.2     3     1623   21 28 38
21 29 10  ---          02 00 10  60.3  35.6 -1.9    -125.4    32     1628   21 28 39

21 29 30  NRAO150      02 00 32  59.8  38.8 -2.0    -120.9    10     1628   21 29 30
21 30 00  ---          02 01 02  59.9  38.8 -2.0    -121.1    30     1631   21 29 31

21 30 12  J0350+5138   02 01 14  60.7  36.0 -1.8    -125.3     2     1631   21 30 12
21 30 42  ---          02 01 44  60.8  35.9 -1.8    -125.5    30     1635   21 30 13
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

21 30 54  NRAO150      02 01 55  60.0  38.6 -2.0    -121.4     2     1635   21 30 54
21 31 24  ---          02 02 26  60.1  38.5 -2.0    -121.6    30     1639   21 30 55

21 31 36  J0350+5201   02 02 38  60.7  35.2 -1.8    -126.2     2     1639   21 31 36
21 32 06  ---          02 03 08  60.7  35.1 -1.8    -126.4    30     1643   21 31 37

21 32 26  NRAO150      02 03 28  60.2  38.4 -2.0    -121.9    10     1643   21 32 26
21 32 56  ---          02 03 58  60.3  38.3 -1.9    -122.1    30     1647   21 32 27

21 33 08  J0350+5138   02 04 10  61.1  35.5 -1.8    -126.4     2     1647   21 33 08
21 33 38  ---          02 04 40  61.2  35.4 -1.8    -126.5    30     1651   21 33 09

21 33 49  NRAO150      02 04 52  60.4  38.1 -1.9    -122.4     2     1651   21 33 49
21 34 19  ---          02 05 22  60.5  38.0 -1.9    -122.6    30     1655   21 33 50

21 34 32  J0350+5201   02 05 34  61.0  34.6 -1.8    -127.3     2     1655   21 34 32
21 35 02  ---          02 06 04  61.1  34.5 -1.8    -127.5    30     1658   21 34 33

21 35 22  NRAO150      02 06 24  60.6  37.9 -1.9    -122.9    10     1658   21 35 22
21 35 52  ---          02 06 54  60.7  37.8 -1.9    -123.1    30     1662   21 35 23

21 36 03  J0350+5138   02 07 06  61.5  34.9 -1.7    -127.4     2     1662   21 36 03
21 36 33  ---          02 07 36  61.5  34.8 -1.7    -127.6    30     1666   21 36 04

21 36 45  NRAO150      02 07 48  60.8  37.6 -1.9    -123.4     2     1666   21 36 45
21 37 15  ---          02 08 18  60.9  37.5 -1.9    -123.6    30     1670   21 36 46

21 37 27  J0350+5201   02 08 30  61.4  34.1 -1.7    -128.4     1     1670   21 37 27
21 37 57  ---          02 09 00  61.4  34.0 -1.7    -128.6    30     1674   21 37 28

21 38 17  NRAO150      02 09 20  61.0  37.3 -1.9    -123.9    10     1674   21 38 17
21 38 47  ---          02 09 50  61.1  37.3 -1.8    -124.1    30     1678   21 38 18

21 38 59  J0350+5138   02 10 02  61.8  34.3 -1.7    -128.5     2     1678   21 38 59
21 39 29  ---          02 10 32  61.9  34.2 -1.7    -128.7    30     1682   21 39 00

21 39 41  NRAO150      02 10 44  61.2  37.1 -1.8    -124.4     2     1682   21 39 41
21 40 11  ---          02 11 14  61.3  37.0 -1.8    -124.6    30     1685   21 39 42

21 40 24  J0350+5201   02 11 27  61.7  33.5 -1.7    -129.5     3     1685   21 40 24
21 40 56  ---          02 11 58  61.8  33.4 -1.7    -129.7    32     1690   21 40 25

21 41 16  NRAO150      02 12 19  61.4  36.8 -1.8    -125.0    10     1690   21 41 16
21 41 46  ---          02 12 49  61.5  36.7 -1.8    -125.2    30     1693   21 41 17
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

21 41 58  J0350+5138   02 13 02  62.2  33.7 -1.6    -129.7     2     1693   21 41 58
21 42 29  ---          02 13 32  62.3  33.6 -1.6    -129.9    31     1697   21 41 59

21 42 41  NRAO150      02 13 45  61.6  36.5 -1.8    -125.5     2     1697   21 42 41
21 43 11  ---          02 14 15  61.6  36.4 -1.8    -125.7    30     1701   21 42 42

21 43 25  J0350+5201   02 14 28  62.1  32.8 -1.6    -130.6     3     1701   21 43 25
21 43 56  ---          02 14 59  62.1  32.7 -1.6    -130.8    32     1705   21 43 26

21 44 16  NRAO150      02 15 20  61.8  36.2 -1.8    -126.1    10     1705   21 44 16
21 44 46  ---          02 15 50  61.8  36.1 -1.7    -126.3    30     1709   21 44 17

21 44 59  J0350+5138   02 16 03  62.6  33.0 -1.6    -130.8     3     1709   21 44 59
21 45 29  ---          02 16 33  62.6  32.9 -1.6    -131.0    30     1713   21 45 00

21 45 42  NRAO150      02 16 46  62.0  35.9 -1.7    -126.6     3     1713   21 45 42
21 46 12  ---          02 17 16  62.0  35.8 -1.7    -126.8    30     1717   21 45 43

21 46 25  J0350+5201   02 17 30  62.4  32.2 -1.6    -131.8     3     1717   21 46 25
21 46 57  ---          02 18 00  62.5  32.1 -1.6    -132.0    31     1721   21 46 26

21 47 17  NRAO150      02 18 21  62.2  35.6 -1.7    -127.2    10     1721   21 47 17
21 47 47  ---          02 18 51  62.2  35.5 -1.7    -127.4    30     1725   21 47 18

21 47 59  J0350+5138   02 19 04  62.9  32.4 -1.5    -132.0     3     1725   21 47 59
21 48 30  ---          02 19 34  63.0  32.2 -1.5    -132.2    30     1729   21 48 00

21 48 42  NRAO150      02 19 47  62.3  35.3 -1.7    -127.8     3     1729   21 48 42
21 49 12  ---          02 20 17  62.4  35.2 -1.7    -128.0    30     1733   21 48 43

21 49 26  J0350+5201   02 20 31  62.8  31.5 -1.5    -133.0     3     1733   21 49 26
21 49 57  ---          02 21 01  62.8  31.4 -1.5    -133.2    31     1737   21 49 27

21 50 17  NRAO150      02 21 22  62.5  35.0 -1.7    -128.4    10     1737   21 50 17
21 50 47  ---          02 21 52  62.6  34.9 -1.6    -128.6    30     1740   21 50 18

21 51 00  J0350+5138   02 22 05  63.2  31.7 -1.5    -133.2     3     1740   21 51 00
21 51 30  ---          02 22 35  63.3  31.5 -1.5    -133.5    30     1744   21 51 01

21 51 43  NRAO150      02 22 48  62.7  34.7 -1.6    -128.9     3     1744   21 51 43
21 52 13  ---          02 23 19  62.8  34.6 -1.6    -129.1    30     1748   21 51 44

21 52 27  J0350+5201   02 23 32  63.1  30.8 -1.5    -134.2     3     1748   21 52 27
21 52 58  ---          02 24 02  63.2  30.7 -1.5    -134.4    31     1752   21 52 28
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

21 53 18  NRAO150      02 24 23  62.9  34.3 -1.6    -129.5     9     1752   21 53 18
21 53 48  ---          02 24 54  63.0  34.2 -1.6    -129.7    30     1756   21 53 19

21 54 01  J0350+5138   02 25 07  63.6  30.9 -1.4    -134.5     3     1756   21 54 01
21 54 31  ---          02 25 37  63.6  30.8 -1.4    -134.7    30     1760   21 54 02

21 54 44  NRAO150      02 25 50  63.1  34.0 -1.6    -130.1     3     1760   21 54 44
21 55 14  ---          02 26 20  63.1  33.9 -1.6    -130.3    30     1764   21 54 45

21 55 28  J0350+5201   02 26 34  63.4  30.0 -1.4    -135.5     3     1764   21 55 28
21 55 59  ---          02 27 04  63.5  29.9 -1.4    -135.7    31     1768   21 55 29

21 56 19  NRAO150      02 27 25  63.3  33.7 -1.6    -130.7     9     1768   21 56 19
21 56 49  ---          02 27 55  63.3  33.5 -1.5    -130.9    30     1772   21 56 20

21 57 02  J0350+5138   02 28 09  63.9  30.2 -1.4    -135.8     3     1772   21 57 02
21 57 32  ---          02 28 39  64.0  30.0 -1.4    -136.0    30     1776   21 57 03

21 57 46  NRAO150      02 28 52  63.4  33.3 -1.5    -131.3     3     1776   21 57 46
21 58 16  ---          02 29 22  63.5  33.2 -1.5    -131.5    30     1779   21 57 47

21 58 30  J0350+5201   02 29 36  63.8  29.3 -1.4    -136.8     3     1779   21 58 30
21 59 00  ---          02 30 06  63.8  29.2 -1.4    -137.0    31     1783   21 58 31

21 59 20  NRAO150      02 30 27  63.6  32.9 -1.5    -131.9     9     1783   21 59 20
21 59 50  ---          02 30 57  63.7  32.8 -1.5    -132.2    30     1787   21 59 21

22 00 04  J0350+5138   02 31 11  64.2  29.4 -1.3    -137.1     3     1787   22 00 04
22 00 34  ---          02 31 41  64.3  29.3 -1.3    -137.3    30     1791   22 00 05

22 00 48  NRAO150      02 31 54  63.8  32.6 -1.5    -132.5     3     1791   22 00 48
22 01 18  ---          02 32 24  63.9  32.5 -1.5    -132.7    30     1795   22 00 49

22 01 32  J0350+5201   02 32 39  64.1  28.5 -1.3    -138.1     4     1795   22 01 32
22 02 02  ---          02 33 09  64.1  28.4 -1.3    -138.3    30     1799   22 01 33

22 02 22  NRAO150      02 33 29  64.0  32.2 -1.5    -133.2     9     1799   22 02 22
22 02 52  ---          02 33 59  64.0  32.1 -1.4    -133.4    30     1803   22 02 23

22 03 06  J0350+5138   02 34 13  64.6  28.6 -1.3    -138.4     3     1803   22 03 06
22 03 36  ---          02 34 43  64.6  28.5 -1.3    -138.6    30     1807   22 03 07

22 03 50  NRAO150      02 34 57  64.1  31.9 -1.4    -133.8     3     1807   22 03 50
22 04 20  ---          02 35 27  64.2  31.7 -1.4    -134.0    30     1810   22 03 51
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

22 04 34  J0350+5201   02 35 41  64.4  27.7 -1.3    -139.4     4     1810   22 04 34
22 05 04  ---          02 36 12  64.4  27.6 -1.3    -139.6    30     1814   22 04 35

22 05 24  NRAO150      02 36 32  64.3  31.5 -1.4    -134.5     9     1814   22 05 24
22 05 54  ---          02 37 02  64.4  31.3 -1.4    -134.7    30     1818   22 05 25

22 06 08  J0350+5138   02 37 16  64.9  27.8 -1.2    -139.7     4     1818   22 06 08
22 06 38  ---          02 37 46  64.9  27.6 -1.2    -140.0    30     1822   22 06 09

22 06 52  NRAO150      02 38 00  64.5  31.1 -1.4    -135.1     3     1822   22 06 52
22 07 22  ---          02 38 30  64.5  30.9 -1.4    -135.3    30     1826   22 06 53

22 07 37  J0350+5201   02 38 44  64.7  26.9 -1.2    -140.8     4     1826   22 07 37
22 08 07  ---          02 39 15  64.7  26.7 -1.2    -141.0    30     1830   22 07 38

22 08 27  NRAO150      02 39 35  64.7  30.7 -1.4    -135.8     9     1830   22 08 27
22 08 57  ---          02 40 05  64.7  30.5 -1.3    -136.0    30     1834   22 08 28

22 09 11  J0350+5138   02 40 19  65.2  26.9 -1.2    -141.1     4     1834   22 09 11
22 09 41  ---          02 40 49  65.2  26.7 -1.2    -141.3    30     1837   22 09 12

22 09 55  NRAO150      02 41 03  64.8  30.3 -1.3    -136.4     4     1837   22 09 55
22 10 25  ---          02 41 33  64.9  30.1 -1.3    -136.6    30     1841   22 09 56

22 10 39  J0350+5201   02 41 48  65.0  26.0 -1.2    -142.1     4     1841   22 10 39
22 11 09  ---          02 42 18  65.0  25.9 -1.2    -142.4    30     1845   22 10 40

22 11 29  NRAO150      02 42 38  65.0  29.8 -1.3    -137.1     9     1845   22 11 29
22 11 59  ---          02 43 08  65.0  29.7 -1.3    -137.3    30     1849   22 11 30

22 12 14  J0350+5138   02 43 22  65.5  26.0 -1.1    -142.5     4     1849   22 12 14
22 12 44  ---          02 43 52  65.5  25.8 -1.1    -142.8    30     1853   22 12 15

22 12 58  NRAO150      02 44 06  65.2  29.4 -1.3    -137.8     4     1853   22 12 58
22 13 28  ---          02 44 37  65.2  29.3 -1.3    -138.0    30     1857   22 12 59

22 13 42  J0350+5201   02 44 51  65.3  25.1 -1.1    -143.6     4     1857   22 13 42
22 14 12  ---          02 45 21  65.3  25.0 -1.1    -143.8    30     1861   22 13 43

22 14 32  NRAO150      02 45 41  65.3  29.0 -1.3    -138.5     9     1861   22 14 32
22 15 02  ---          02 46 11  65.4  28.9 -1.2    -138.7    30     1865   22 14 33

22 15 57  DA193        02 47 06  50.7  63.2 -3.2     -88.3    18     1865   22 15 57
22 20 57  ---          02 52 07  51.6  63.2 -3.1     -89.1   300     1903   22 15 58
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

22 24 07  OJ287        02 55 18  10.0  72.5 -6.0     -60.9    99     1903   22 24 07
22 32 09  ---          03 00 18  11.0  73.1 -5.9     -61.2   482     1965   22 24 08

22 34 21  J0350+5138   03 05 33  67.3  18.7 -0.8    -153.5    13     1965   22 34 21
22 34 51  ---          03 06 03  67.3  18.5 -0.8    -153.8    30     1969   22 34 22

22 35 02  NRAO150      03 06 15  67.2  22.5 -0.9    -148.4     1     1969   22 35 02
22 35 32  ---          03 06 45  67.3  22.4 -0.9    -148.6    30     1973   22 35 03

22 35 44  J0350+5201   03 06 56  67.0  17.9 -0.8    -154.5     1     1973   22 35 44
22 36 14  ---          03 07 26  67.0  17.7 -0.7    -154.8    30     1977   22 35 45

22 36 34  NRAO150      03 07 47  67.4  22.0 -0.9    -149.2     9     1977   22 36 34
22 37 04  ---          03 08 17  67.4  21.8 -0.9    -149.4    30     1981   22 36 35

22 37 15  J0350+5138   03 08 28  67.5  17.7 -0.7    -155.1     1     1981   22 37 15
22 37 45  ---          03 08 58  67.5  17.5 -0.7    -155.4    30     1985   22 37 16

22 37 57  NRAO150      03 09 09  67.5  21.5 -0.9    -149.9     1     1985   22 37 57
22 38 27  ---          03 09 40  67.5  21.3 -0.9    -150.2    30     1988   22 37 58

22 38 38  J0350+5201   03 09 51  67.2  16.9 -0.7    -156.0     1     1988   22 38 38
22 39 08  ---          03 10 21  67.2  16.7 -0.7    -156.3    30     1992   22 38 39

22 39 28  NRAO150      03 10 41  67.6  21.0 -0.8    -150.7     9     1992   22 39 28
22 39 58  ---          03 11 12  67.6  20.8 -0.8    -151.0    30     1996   22 39 29

22 40 10  J0350+5138   03 11 23  67.7  16.6 -0.7    -156.7     1     1996   22 40 10
22 40 40  ---          03 11 53  67.7  16.4 -0.7    -156.9    30     2000   22 40 11

22 40 51  NRAO150      03 12 05  67.7  20.5 -0.8    -151.4     1     2000   22 40 51
22 41 21  ---          03 12 35  67.7  20.3 -0.8    -151.7    30     2004   22 40 52

22 41 33  J0350+5201   03 12 47  67.4  15.8 -0.7    -157.6     1     2004   22 41 33
22 42 03  ---          03 13 17  67.4  15.6 -0.6    -157.9    30     2008   22 41 34

22 42 23  NRAO150      03 13 37  67.8  19.9 -0.8    -152.2     9     2008   22 42 23
22 42 53  ---          03 14 07  67.9  19.7 -0.8    -152.5    30     2012   22 42 24

22 43 05  J0350+5138   03 14 18  67.8  15.5 -0.6    -158.3     1     2012   22 43 05
22 43 35  ---          03 14 48  67.9  15.3 -0.6    -158.5    30     2016   22 43 06

22 43 48  NRAO150      03 15 02  67.9  19.4 -0.8    -153.0     3     2016   22 43 48
22 44 18  ---          03 15 32  68.0  19.2 -0.8    -153.3    30     2019   22 43 49
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

22 44 31  J0350+5201   03 15 45  67.5  14.7 -0.6    -159.2     2     2019   22 44 31
22 45 02  ---          03 16 15  67.6  14.5 -0.6    -159.5    31     2023   22 44 32

22 45 22  NRAO150      03 16 36  68.0  18.8 -0.7    -153.9     9     2023   22 45 22
22 45 52  ---          03 17 06  68.1  18.6 -0.7    -154.1    30     2027   22 45 23

22 46 05  J0350+5138   03 17 20  68.0  14.3 -0.6    -159.9     2     2027   22 46 05
22 46 35  ---          03 17 50  68.0  14.1 -0.6    -160.2    30     2031   22 46 06

22 46 49  NRAO150      03 18 03  68.1  18.2 -0.7    -154.7     2     2031   22 46 49
22 47 19  ---          03 18 33  68.2  18.1 -0.7    -154.9    30     2035   22 46 50

22 47 31  J0350+5201   03 18 45  67.7  13.6 -0.6    -160.9     1     2035   22 47 31
22 48 03  ---          03 19 16  67.7  13.4 -0.5    -161.1    32     2039   22 47 32

22 48 23  NRAO150      03 19 37  68.2  17.6 -0.7    -155.5     9     2039   22 48 23
22 48 53  ---          03 20 07  68.3  17.4 -0.7    -155.8    30     2043   22 48 24

22 49 06  J0350+5138   03 20 20  68.2  13.1 -0.5    -161.6     2     2043   22 49 06
22 49 36  ---          03 20 51  68.2  12.9 -0.5    -161.9    30     2047   22 49 07

22 49 49  NRAO150      03 21 03  68.3  17.1 -0.7    -156.3     2     2047   22 49 49
22 50 19  ---          03 21 33  68.4  16.9 -0.7    -156.6    30     2051   22 49 50

22 50 31  J0350+5201   03 21 46  67.9  12.4 -0.5    -162.5     1     2051   22 50 31
22 51 03  ---          03 22 16  67.9  12.2 -0.5    -162.8    32     2055   22 50 32

22 51 23  NRAO150      03 22 38  68.4  16.5 -0.6    -157.2     9     2055   22 51 23
22 51 53  ---          03 23 08  68.5  16.3 -0.6    -157.5    30     2059   22 51 24

22 52 05  J0350+5138   03 23 21  68.3  11.9 -0.5    -163.3     2     2059   22 52 05
22 52 35  ---          03 23 51  68.3  11.7 -0.5    -163.6    30     2063   22 52 06

22 52 48  NRAO150      03 24 03  68.5  15.9 -0.6    -158.0     2     2063   22 52 48
22 53 18  ---          03 24 33  68.5  15.7 -0.6    -158.3    30     2066   22 52 49

22 53 30  J0350+5201   03 24 46  68.0  11.2 -0.5    -164.2     1     2066   22 53 30
22 54 02  ---          03 25 16  68.0  11.0 -0.4    -164.5    32     2071   22 53 31

22 54 22  NRAO150      03 25 38  68.6  15.3 -0.6    -158.9     9     2071   22 54 22
22 54 52  ---          03 26 08  68.6  15.1 -0.6    -159.2    30     2074   22 54 23

22 55 04  J0350+5138   03 26 20  68.4  10.7 -0.4    -165.0     1     2074   22 55 04
22 55 35  ---          03 26 50  68.4  10.5 -0.4    -165.3    30     2078   22 55 05
Schedule for VLBA_FD   (Code Fd )                                   Page  32
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

22 55 47  NRAO150      03 27 03  68.7  14.7 -0.6    -159.7     1     2078   22 55 47
22 56 17  ---          03 27 33  68.7  14.5 -0.6    -160.0    30     2082   22 55 48

22 56 29  J0350+5201   03 27 45  68.1  10.0 -0.4    -165.9     1     2082   22 56 29
22 57 01  ---          03 28 15  68.1   9.8 -0.4    -166.2    32     2086   22 56 30

22 57 21  NRAO150      03 28 37  68.8  14.1 -0.5    -160.6     9     2086   22 57 21
22 57 51  ---          03 29 07  68.8  13.9 -0.5    -160.9    30     2090   22 57 22

22 58 03  J0350+5138   03 29 19  68.5   9.5 -0.4    -166.8     1     2090   22 58 03
22 58 34  ---          03 29 49  68.6   9.3 -0.4    -167.0    31     2094   22 58 04

22 58 46  NRAO150      03 30 02  68.8  13.5 -0.5    -161.4     1     2094   22 58 46
22 59 16  ---          03 30 32  68.9  13.3 -0.5    -161.7    30     2098   22 58 47

22 59 28  J0350+5201   03 30 44  68.2   8.8 -0.4    -167.6     1     2098   22 59 28
23 00 00  ---          03 31 15  68.2   8.6 -0.3    -167.9    32     2102   22 59 29

23 00 20  NRAO150      03 31 36  68.9  12.8 -0.5    -162.3     9     2102   23 00 20
23 00 50  ---          03 32 06  68.9  12.6 -0.5    -162.6    30     2106   23 00 21

23 01 02  J0350+5138   03 32 18  68.6   8.3 -0.3    -168.5     1     2106   23 01 02
23 01 33  ---          03 32 48  68.7   8.1 -0.3    -168.8    31     2110   23 01 03

23 01 44  NRAO150      03 33 01  69.0  12.2 -0.5    -163.2     1     2110   23 01 44
23 02 14  ---          03 33 31  69.0  12.0 -0.5    -163.5    30     2114   23 01 45

23 02 27  J0350+5201   03 33 44  68.3   7.6 -0.3    -169.3     1     2114   23 02 27
23 02 59  ---          03 34 14  68.3   7.4 -0.3    -169.6    32     2118   23 02 28

23 03 19  NRAO150      03 34 36  69.1  11.6 -0.4    -164.1     9     2118   23 03 19
23 03 49  ---          03 35 06  69.1  11.4 -0.4    -164.4    30     2122   23 03 20

23 04 00  J0350+5138   03 35 18  68.7   7.0 -0.3    -170.2     1     2122   23 04 00
23 04 31  ---          03 35 48  68.7   6.8 -0.3    -170.5    31     2126   23 04 01

23 04 43  NRAO150      03 36 00  69.1  11.0 -0.4    -164.9     1     2126   23 04 43
23 05 13  ---          03 36 30  69.1  10.8 -0.4    -165.2    30     2130   23 04 44

23 05 25  J0350+5201   03 36 43  68.4   6.4 -0.3    -171.0     1     2130   23 05 25
23 05 57  ---          03 37 13  68.4   6.2 -0.2    -171.3    32     2134   23 05 26

23 06 17  NRAO150      03 37 35  69.2  10.3 -0.4    -165.9     9     2134   23 06 17
23 06 47  ---          03 38 05  69.2  10.1 -0.4    -166.1    30     2138   23 06 18
Schedule for VLBA_FD   (Code Fd )                                   Page  33
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

23 06 59  J0350+5138   03 38 17  68.8   5.8 -0.2    -172.0     1     2138   23 06 59
23 07 30  ---          03 38 47  68.8   5.5 -0.2    -172.3    31     2142   23 07 00

23 07 42  NRAO150      03 39 00  69.2   9.7 -0.4    -166.7     1     2142   23 07 42
23 08 12  ---          03 39 30  69.2   9.5 -0.4    -167.0    30     2145   23 07 43

23 08 24  J0350+5201   03 39 42  68.4   5.2 -0.2    -172.8     1     2145   23 08 24
23 08 56  ---          03 40 12  68.5   4.9 -0.2    -173.1    32     2150   23 08 25

23 09 16  NRAO150      03 40 34  69.3   9.0 -0.3    -167.6     9     2150   23 09 16
23 09 46  ---          03 41 04  69.3   8.8 -0.3    -167.9    30     2153   23 09 17

23 09 58  J0350+5138   03 41 16  68.9   4.5 -0.2    -173.8     1     2153   23 09 58
23 10 29  ---          03 41 46  68.9   4.3 -0.2    -174.1    31     2157   23 09 59

23 10 40  NRAO150      03 41 59  69.3   8.4 -0.3    -168.5     1     2157   23 10 40
23 11 10  ---          03 42 29  69.3   8.2 -0.3    -168.8    30     2161   23 10 41

23 11 23  J0350+5201   03 42 41  68.5   3.9 -0.2    -174.5     1     2161   23 11 23
23 11 54  ---          03 43 11  68.5   3.7 -0.1    -174.8    32     2165   23 11 24

23 12 14  NRAO150      03 43 33  69.4   7.7 -0.3    -169.4     9     2165   23 12 14
23 12 44  ---          03 44 03  69.4   7.5 -0.3    -169.7    30     2169   23 12 15

23 12 56  J0350+5138   03 44 15  68.9   3.2 -0.1    -175.6     1     2169   23 12 56
23 13 27  ---          03 44 45  68.9   3.0 -0.1    -175.9    31     2173   23 12 57

23 13 39  NRAO150      03 44 58  69.4   7.1 -0.3    -170.3     1     2173   23 13 39
23 14 09  ---          03 45 28  69.4   6.9 -0.3    -170.6    30     2177   23 13 40

23 14 21  J0350+5201   03 45 40  68.5   2.7 -0.1    -176.3     1     2177   23 14 21
23 14 53  ---          03 46 10  68.5   2.5 -0.1    -176.6    32     2181   23 14 22

23 15 13  NRAO150      03 46 32  69.5   6.4 -0.2    -171.2     9     2181   23 15 13
23 15 43  ---          03 47 02  69.5   6.2 -0.2    -171.6    30     2185   23 15 14

23 15 55  J0350+5138   03 47 14  68.9   1.9 -0.1    -177.3     1     2185   23 15 55
23 16 26  ---          03 47 44  68.9   1.7 -0.1    -177.6    31     2189   23 15 56

23 16 38  NRAO150      03 47 57  69.5   5.8 -0.2    -172.1     1     2189   23 16 38
23 17 08  ---          03 48 27  69.5   5.5 -0.2    -172.4    30     2193   23 16 39

23 17 20  J0350+5201   03 48 39  68.6   1.4 -0.1    -178.0     2     2193   23 17 20
23 17 52  ---          03 49 09  68.6   1.2 -0.0    -178.3    32     2197   23 17 21
Schedule for VLBA_FD   (Code Fd )                                   Page  34
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

23 18 12  NRAO150      03 49 31  69.5   5.1 -0.2    -173.1     9     2197   23 18 12
23 18 42  ---          03 50 01  69.5   4.8 -0.2    -173.4    30     2201   23 18 13

23 18 54  J0350+5138   03 50 13  68.9   0.6 -0.0    -179.1     1     2201   23 18 54
23 19 24  ---          03 50 43  68.9   0.4 -0.0    -179.4    31     2205   23 18 55

23 19 36  NRAO150      03 50 56  69.5   4.4 -0.2    -173.9     1     2205   23 19 36
23 20 06  ---          03 51 26  69.5   4.2 -0.2    -174.2    30     2209   23 19 37

23 20 19  J0350+5201   03 51 39  68.6   0.2 -0.0    -179.8     2     2209   23 20 19
23 20 50  ---          03 52 09  68.6  -0.1  0.0     179.9    31     2213   23 20 20

23 21 10  NRAO150      03 52 30  69.6   3.7 -0.1    -174.9     9     2213   23 21 10
23 21 40  ---          03 53 00  69.6   3.5 -0.1    -175.2    30     2217   23 21 11

23 21 52  J0350+5138   03 53 12  68.9  -0.7  0.0     179.1     1     2217   23 21 52
23 22 23  ---          03 53 42  68.9  -0.9  0.0     178.8    31     2221   23 21 53

23 22 35  NRAO150      03 53 55  69.6   3.1 -0.1    -175.8     1     2221   23 22 35
23 23 05  ---          03 54 25  69.6   2.9 -0.1    -176.1    30     2225   23 22 36

23 23 17  J0350+5201   03 54 38  68.6  -1.1  0.0     178.5     2     2225   23 23 17
23 23 49  ---          03 55 08  68.6  -1.3  0.1     178.2    31     2229   23 23 18

23 24 09  NRAO150      03 55 29  69.6   2.4 -0.1    -176.7     9     2229   23 24 09
23 24 39  ---          03 55 59  69.6   2.2 -0.1    -177.0    30     2232   23 24 10

23 24 50  J0350+5138   03 56 11  68.9  -1.9  0.1     177.3     1     2232   23 24 50
23 25 21  ---          03 56 41  68.9  -2.2  0.1     177.0    31     2236   23 24 51

23 25 33  NRAO150      03 56 54  69.6   1.7 -0.1    -177.6     1     2236   23 25 33
23 26 03  ---          03 57 24  69.6   1.5 -0.1    -177.9    30     2240   23 25 34

23 26 16  J0350+5201   03 57 37  68.5  -2.4  0.1     176.7     3     2240   23 26 16
23 26 47  ---          03 58 07  68.5  -2.6  0.1     176.4    31     2244   23 26 17

23 27 07  NRAO150      03 58 28  69.6   1.0 -0.0    -178.6     9     2244   23 27 07
23 27 37  ---          03 58 58  69.6   0.8 -0.0    -178.9    30     2248   23 27 08

23 27 49  J0350+5138   03 59 10  68.9  -3.2  0.1     175.5     1     2248   23 27 49
23 28 20  ---          03 59 40  68.9  -3.4  0.1     175.2    31     2252   23 27 50

23 28 32  NRAO150      03 59 53  69.6   0.4 -0.0    -179.5     1     2252   23 28 32
23 29 02  ---          04 00 23  69.6   0.2 -0.0    -179.8    30     2256   23 28 33
Schedule for VLBA_FD   (Code Fd )                                   Page  35
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

23 29 15  J0350+5201   04 00 36  68.5  -3.6  0.1     175.0     3     2256   23 29 15
23 29 45  ---          04 01 06  68.5  -3.8  0.2     174.7    30     2260   23 29 16

23 30 05  NRAO150      04 01 27  69.6  -0.3  0.0     179.6    10     2260   23 30 05
23 30 35  ---          04 01 57  69.6  -0.5  0.0     179.3    30     2264   23 30 06

23 30 48  J0350+5138   04 02 09  68.9  -4.5  0.2     173.8     1     2264   23 30 48
23 31 18  ---          04 02 39  68.8  -4.7  0.2     173.5    31     2268   23 30 49

23 31 30  NRAO150      04 02 52  69.6  -0.9  0.0     178.7     2     2268   23 31 30
23 32 00  ---          04 03 22  69.6  -1.2  0.0     178.4    30     2272   23 31 31

23 32 14  J0350+5201   04 03 36  68.5  -4.8  0.2     173.2     3     2272   23 32 14
23 32 44  ---          04 04 06  68.4  -5.1  0.2     172.9    30     2275   23 32 15

23 33 04  NRAO150      04 04 26  69.6  -1.7  0.1     177.7    10     2275   23 33 04
23 33 34  ---          04 04 56  69.6  -1.9  0.1     177.4    30     2279   23 33 05

23 33 46  J0350+5138   04 05 08  68.8  -5.8  0.2     172.0     1     2279   23 33 46
23 34 16  ---          04 05 38  68.8  -6.0  0.2     171.7    30     2283   23 33 47

23 34 28  NRAO150      04 05 50  69.6  -2.3  0.1     176.9     1     2283   23 34 28
23 34 58  ---          04 06 20  69.6  -2.5  0.1     176.6    30     2287   23 34 29

23 35 10  J0350+5201   04 06 32  68.4  -6.1  0.2     171.5     2     2287   23 35 10
23 35 40  ---          04 07 02  68.4  -6.3  0.3     171.2    30     2291   23 35 11

23 36 00  NRAO150      04 07 22  69.6  -3.0  0.1     175.9    10     2291   23 36 00
23 36 30  ---          04 07 52  69.6  -3.2  0.1     175.6    30     2295   23 36 01

23 36 42  J0350+5138   04 08 04  68.7  -7.0  0.3     170.3     1     2295   23 36 42
23 37 12  ---          04 08 34  68.7  -7.2  0.3     170.0    30     2299   23 36 43

23 37 24  NRAO150      04 08 46  69.6  -3.6  0.1     175.1     1     2299   23 37 24
23 37 54  ---          04 09 16  69.6  -3.8  0.1     174.8    30     2303   23 37 25

23 38 06  J0350+5201   04 09 29  68.3  -7.3  0.3     169.8     2     2303   23 38 06
23 38 36  ---          04 09 59  68.3  -7.5  0.3     169.5    30     2306   23 38 07

23 38 56  NRAO150      04 10 19  69.5  -4.3  0.2     174.1    10     2306   23 38 56
23 39 26  ---          04 10 49  69.5  -4.5  0.2     173.8    30     2310   23 38 57

23 39 38  J0350+5138   04 11 01  68.6  -8.2  0.3     168.5     1     2310   23 39 38
23 40 08  ---          04 11 31  68.6  -8.4  0.3     168.2    30     2314   23 39 39
Schedule for VLBA_FD   (Code Fd )                                   Page  36
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

23 40 20  NRAO150      04 11 43  69.5  -4.9  0.2     173.3     1     2314   23 40 20
23 40 50  ---          04 12 13  69.5  -5.1  0.2     173.0    30     2318   23 40 21

23 41 02  J0350+5201   04 12 25  68.2  -8.5  0.3     168.1     2     2318   23 41 02
23 41 32  ---          04 12 55  68.2  -8.7  0.3     167.8    30     2322   23 41 03

23 41 52  NRAO150      04 13 15  69.5  -5.6  0.2     172.3     9     2322   23 41 52
23 42 22  ---          04 13 45  69.5  -5.8  0.2     172.0    30     2326   23 41 53

23 42 35  J0350+5138   04 13 59  68.5  -9.5  0.4     166.8     3     2326   23 42 35
23 43 05  ---          04 14 29  68.5  -9.7  0.4     166.5    30     2330   23 42 36

23 43 19  NRAO150      04 14 43  69.5  -6.3  0.2     171.4     3     2330   23 43 19
23 43 49  ---          04 15 13  69.4  -6.5  0.2     171.1    30     2333   23 43 20

23 44 05  J0350+5201   04 15 29  68.1  -9.7  0.4     166.3     5     2333   23 44 05
23 44 35  ---          04 15 59  68.1  -9.9  0.4     166.1    30     2337   23 44 06

23 44 55  NRAO150      04 16 19  69.4  -7.0  0.3     170.5     9     2337   23 44 55
23 45 25  ---          04 16 49  69.4  -7.2  0.3     170.1    30     2341   23 44 56

23 45 39  J0350+5138   04 17 03  68.4 -10.7  0.4     165.0     4     2341   23 45 39
23 46 09  ---          04 17 33  68.4 -10.9  0.4     164.7    30     2345   23 45 40

23 46 23  NRAO150      04 17 47  69.4  -7.6  0.3     169.6     4     2345   23 46 23
23 46 53  ---          04 18 17  69.4  -7.8  0.3     169.3    30     2349   23 46 24

23 47 10  J0350+5201   04 18 34  68.0 -10.9  0.4     164.6     6     2349   23 47 10
23 47 40  ---          04 19 04  68.0 -11.1  0.5     164.3    30     2353   23 47 11

23 48 00  NRAO150      04 19 24  69.3  -8.3  0.3     168.6     9     2353   23 48 00
23 48 30  ---          04 19 54  69.3  -8.5  0.3     168.3    30     2357   23 48 01

23 48 44  J0350+5138   04 20 09  68.3 -12.0  0.5     163.3     5     2357   23 48 44
23 49 14  ---          04 20 39  68.3 -12.2  0.5     163.0    30     2360   23 48 45

23 49 29  NRAO150      04 20 54  69.3  -9.0  0.3     167.7     5     2360   23 49 29
23 49 59  ---          04 21 24  69.3  -9.2  0.3     167.4    30     2364   23 49 30

23 50 16  J0350+5201   04 21 41  67.9 -12.2  0.5     162.8     6     2364   23 50 16
23 50 46  ---          04 22 11  67.9 -12.4  0.5     162.6    30     2368   23 50 17

23 51 06  NRAO150      04 22 31  69.2  -9.7  0.4     166.7     9     2368   23 51 06
23 51 36  ---          04 23 01  69.2  -9.9  0.4     166.4    30     2372   23 51 07
Schedule for VLBA_FD   (Code Fd )                                   Page  37
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  13 Mar 2017   Day  72 ---

23 51 52  J0350+5138   04 23 17  68.1 -13.2  0.5     161.5     5     2372   23 51 52
23 52 22  ---          04 23 47  68.1 -13.4  0.5     161.2    30     2376   23 51 53

23 52 37  NRAO150      04 24 02  69.2 -10.3  0.4     165.8     5     2376   23 52 37
23 53 07  ---          04 24 32  69.1 -10.5  0.4     165.5    30     2380   23 52 38

23 53 24  J0350+5201   04 24 49  67.7 -13.4  0.5     161.1     6     2380   23 53 24
23 53 54  ---          04 25 19  67.7 -13.6  0.6     160.8    30     2384   23 53 25

23 54 14  NRAO150      04 25 39  69.1 -11.0  0.4     164.8     9     2384   23 54 14
23 54 44  ---          04 26 09  69.1 -11.2  0.4     164.5    30     2388   23 54 15

23 55 00  J0350+5138   04 26 26  68.0 -14.5  0.6     159.7     6     2388   23 55 00
23 55 30  ---          04 26 56  68.0 -14.7  0.6     159.4    30     2391   23 55 01

23 55 47  NRAO150      04 27 12  69.0 -11.7  0.4     163.9     6     2391   23 55 47
23 56 17  ---          04 27 43  69.0 -11.9  0.4     163.6    30     2395   23 55 48

23 56 34  J0350+5201   04 27 59  67.6 -14.6  0.6     159.4     6     2395   23 56 34
23 57 04  ---          04 28 29  67.5 -14.8  0.6     159.1    30     2399   23 56 35

23 57 24  NRAO150      04 28 49  69.0 -12.4  0.5     163.0     9     2399   23 57 24
23 57 54  ---          04 29 20  68.9 -12.6  0.5     162.7    30     2403   23 57 25

23 58 10  J0350+5138   04 29 36  67.8 -15.7  0.6     158.0     6     2403   23 58 10
23 58 40  ---          04 30 06  67.8 -15.9  0.6     157.7    30     2407   23 58 11

23 58 57  NRAO150      04 30 23  68.9 -13.0  0.5     162.1     6     2407   23 58 57
23 59 27  ---          04 30 53  68.9 -13.2  0.5     161.8    30     2411   23 58 58

 --- Start: Mon  13 Mar 2017   Day  72 -- Stop: Tue  14 Mar 2017   Day  73 ---

23 59 43  J0350+5201   04 31 10  67.4 -15.8  0.7     157.6     6     2411   23 59 43
00 00 13  ---          04 31 40  67.4 -15.9  0.7     157.4    30     2415   23 59 44

00 00 33  NRAO150      04 32 00  68.8 -13.7  0.5     161.1     9     2415   00 00 33
00 01 03  ---          04 32 30  68.8 -13.9  0.5     160.8    30     2418   00 00 34

00 01 20  J0350+5138   04 32 47  67.6 -16.9  0.7     156.2     6     2418   00 01 20
00 01 50  ---          04 33 17  67.6 -17.1  0.7     156.0    30     2422   00 01 21

00 02 07  NRAO150      04 33 33  68.7 -14.3  0.5     160.2     6     2422   00 02 07
00 02 37  ---          04 34 03  68.7 -14.5  0.6     159.9    30     2426   00 02 08
Schedule for VLBA_FD   (Code Fd )                                   Page  38
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

00 02 53  J0350+5201   04 34 20  67.2 -16.9  0.7     155.9     6     2426   00 02 53
00 03 23  ---          04 34 50  67.2 -17.1  0.7     155.7    30     2430   00 02 54

00 03 43  NRAO150      04 35 10  68.6 -15.0  0.6     159.3     9     2430   00 03 43
00 04 13  ---          04 35 40  68.6 -15.2  0.6     159.0    30     2434   00 03 44

00 04 30  J0350+5138   04 35 57  67.4 -18.0  0.7     154.5     6     2434   00 04 30
00 05 00  ---          04 36 27  67.4 -18.2  0.7     154.3    30     2438   00 04 31

00 05 16  NRAO150      04 36 44  68.6 -15.6  0.6     158.4     6     2438   00 05 16
00 05 46  ---          04 37 14  68.5 -15.8  0.6     158.1    30     2442   00 05 17

00 06 03  J0350+5201   04 37 31  67.0 -18.1  0.8     154.3     6     2442   00 06 03
00 06 33  ---          04 38 01  67.0 -18.2  0.8     154.0    30     2446   00 06 04

00 06 53  NRAO150      04 38 21  68.5 -16.2  0.6     157.5     9     2446   00 06 53
00 07 23  ---          04 38 51  68.4 -16.4  0.6     157.2    30     2449   00 06 54

00 07 40  J0350+5138   04 39 07  67.2 -19.2  0.8     152.9     6     2449   00 07 40
00 08 10  ---          04 39 37  67.2 -19.4  0.8     152.6    30     2453   00 07 41

00 08 26  NRAO150      04 39 54  68.4 -16.9  0.7     156.6     6     2453   00 08 26
00 08 56  ---          04 40 24  68.3 -17.1  0.7     156.4    30     2457   00 08 27

00 09 13  J0350+5201   04 40 41  66.8 -19.2  0.8     152.6     6     2457   00 09 13
00 09 43  ---          04 41 11  66.7 -19.3  0.8     152.4    30     2461   00 09 14

00 10 03  NRAO150      04 41 31  68.3 -17.5  0.7     155.7     9     2461   00 10 03
00 10 33  ---          04 42 01  68.2 -17.7  0.7     155.5    30     2465   00 10 04

00 10 50  J0350+5138   04 42 18  67.0 -20.3  0.8     151.2     6     2465   00 10 50
00 11 20  ---          04 42 48  66.9 -20.5  0.9     151.0    30     2469   00 10 51

00 11 36  NRAO150      04 43 04  68.2 -18.1  0.7     154.9     6     2469   00 11 36
00 12 06  ---          04 43 35  68.1 -18.3  0.7     154.6    30     2473   00 11 37

00 12 23  J0350+5201   04 43 51  66.5 -20.3  0.9     151.0     6     2473   00 12 23
00 12 53  ---          04 44 21  66.5 -20.4  0.9     150.8    30     2476   00 12 24

00 13 13  NRAO150      04 44 41  68.1 -18.7  0.7     154.0     9     2476   00 13 13
00 13 43  ---          04 45 12  68.0 -18.9  0.7     153.7    30     2480   00 13 14

00 14 00  J0350+5138   04 45 28  66.7 -21.4  0.9     149.6     6     2480   00 14 00
00 14 30  ---          04 45 58  66.7 -21.6  0.9     149.3    30     2484   00 14 01
Schedule for VLBA_FD   (Code Fd )                                   Page  39
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

00 14 46  NRAO150      04 46 15  67.9 -19.3  0.8     153.1     6     2484   00 14 46
00 15 16  ---          04 46 45  67.9 -19.5  0.8     152.9    30     2488   00 14 47

00 15 33  J0350+5201   04 47 02  66.3 -21.3  0.9     149.4     6     2488   00 15 33
00 16 03  ---          04 47 32  66.3 -21.5  0.9     149.2    30     2492   00 15 34

00 16 23  NRAO150      04 47 52  67.8 -19.9  0.8     152.3     9     2492   00 16 23
00 16 53  ---          04 48 22  67.8 -20.1  0.8     152.0    30     2496   00 16 24

00 18 22  DA193        04 49 51  73.6  51.4 -1.1    -118.8    30     2496   00 18 22
00 24 57  ---          04 54 52  74.4  49.7 -1.0    -121.3   395     2547   00 18 23

00 26 33  OJ287        04 58 03  35.8  86.4 -4.0     -66.1    12     2547   00 26 33
00 30 00  ---          05 01 04  36.5  86.7 -3.9     -66.1   207     2573   00 26 34

00 32 03  J0350+5138   05 03 34  65.1 -27.0  1.2     140.9    34     2573   00 32 03
00 32 37  ---          05 04 04  65.1 -27.2  1.2     140.7    34     2578   00 32 04

00 32 48  NRAO150      05 04 20  66.5 -25.5  1.1     143.9     0     2578   00 32 48
00 33 19  ---          05 04 50  66.4 -25.7  1.1     143.6    31     2582   00 32 49

00 33 30  J0350+5201   05 05 02  64.7 -26.8  1.2     140.9     0     2582   00 33 30
00 34 00  ---          05 05 32  64.7 -26.9  1.2     140.7    30     2586   00 33 31

00 34 12  NRAO150      05 05 44  66.3 -26.0  1.1     143.2     0     2586   00 34 12
00 34 42  ---          05 06 14  66.3 -26.1  1.1     142.9    30     2589   00 34 13

00 34 53  J0350+5138   05 06 25  64.8 -27.8  1.2     139.6     0     2589   00 34 53
00 35 23  ---          05 06 55  64.8 -28.0  1.3     139.4    30     2593   00 34 54

00 35 34  NRAO150      05 07 07  66.2 -26.4  1.1     142.5     0     2593   00 35 34
00 36 04  ---          05 07 37  66.1 -26.6  1.1     142.3    30     2597   00 35 35

00 36 16  J0350+5201   05 07 48  64.4 -27.6  1.3     139.6     0     2597   00 36 16
00 36 46  ---          05 08 18  64.4 -27.7  1.3     139.4    30     2601   00 36 17

00 36 57  NRAO150      05 08 29  66.1 -26.8  1.1     141.9     0     2601   00 36 57
00 37 27  ---          05 09 00  66.0 -27.0  1.1     141.6    30     2605   00 36 58

00 37 38  J0350+5138   05 09 11  64.6 -28.6  1.3     138.4     0     2605   00 37 38
00 38 08  ---          05 09 41  64.5 -28.7  1.3     138.1    30     2609   00 37 39

00 38 19  NRAO150      05 09 52  65.9 -27.3  1.2     141.2     0     2609   00 38 19
00 38 49  ---          05 10 22  65.9 -27.4  1.2     141.0    30     2613   00 38 20
Schedule for VLBA_FD   (Code Fd )                                   Page  40
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

00 39 01  J0350+5201   05 10 33  64.2 -28.3  1.3     138.4     0     2613   00 39 01
00 39 31  ---          05 11 04  64.1 -28.4  1.3     138.2    30     2616   00 39 02

00 39 42  NRAO150      05 11 15  65.8 -27.7  1.2     140.6     0     2616   00 39 42
00 40 12  ---          05 11 45  65.7 -27.8  1.2     140.3    30     2620   00 39 43

00 40 23  J0350+5138   05 11 56  64.3 -29.3  1.3     137.2     0     2620   00 40 23
00 40 53  ---          05 12 26  64.2 -29.5  1.3     137.0    30     2624   00 40 24

00 41 04  NRAO150      05 12 37  65.6 -28.1  1.2     139.9     0     2624   00 41 04
00 41 34  ---          05 13 08  65.6 -28.2  1.2     139.7    30     2628   00 41 05

00 41 46  J0350+5201   05 13 19  63.9 -29.0  1.4     137.2     0     2628   00 41 46
00 42 16  ---          05 13 49  63.8 -29.1  1.4     137.0    30     2632   00 41 47

00 42 27  NRAO150      05 14 00  65.5 -28.5  1.2     139.3     0     2632   00 42 27
00 42 57  ---          05 14 31  65.5 -28.6  1.2     139.1    30     2636   00 42 28

00 43 08  J0350+5138   05 14 42  64.0 -30.0  1.4     136.0     0     2636   00 43 08
00 43 38  ---          05 15 12  63.9 -30.2  1.4     135.8    30     2640   00 43 09

00 43 49  NRAO150      05 15 23  65.4 -28.9  1.2     138.7     0     2640   00 43 49
00 44 19  ---          05 15 53  65.3 -29.0  1.3     138.5    30     2643   00 43 50

00 44 31  J0350+5201   05 16 04  63.6 -29.7  1.4     136.1     0     2643   00 44 31
00 45 01  ---          05 16 35  63.5 -29.8  1.4     135.9    30     2647   00 44 32

00 45 12  NRAO150      05 16 46  65.2 -29.3  1.3     138.1     0     2647   00 45 12
00 45 42  ---          05 17 16  65.2 -29.4  1.3     137.8    30     2651   00 45 13

00 45 53  J0350+5138   05 17 27  63.7 -30.7  1.4     134.8     0     2651   00 45 53
00 46 23  ---          05 17 57  63.6 -30.8  1.4     134.6    30     2655   00 45 54

00 46 34  NRAO150      05 18 08  65.1 -29.6  1.3     137.4     0     2655   00 46 34
00 47 04  ---          05 18 38  65.0 -29.8  1.3     137.2    30     2659   00 46 35

00 47 16  J0350+5201   05 18 50  63.3 -30.4  1.4     134.9     0     2659   00 47 16
00 47 46  ---          05 19 20  63.2 -30.5  1.5     134.7    30     2663   00 47 17

00 47 57  NRAO150      05 19 31  64.9 -30.0  1.3     136.8     0     2663   00 47 57
00 48 27  ---          05 20 01  64.9 -30.1  1.3     136.6    30     2667   00 47 58

00 48 38  J0350+5138   05 20 13  63.4 -31.4  1.5     133.7     0     2667   00 48 38
00 49 08  ---          05 20 43  63.3 -31.5  1.5     133.5    30     2671   00 48 39
Schedule for VLBA_FD   (Code Fd )                                   Page  41
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

00 49 19  NRAO150      05 20 54  64.8 -30.4  1.3     136.2     0     2671   00 49 19
00 49 49  ---          05 21 24  64.7 -30.5  1.3     136.0    30     2674   00 49 20

00 50 01  J0350+5201   05 21 35  63.0 -31.0  1.5     133.8     0     2674   00 50 01
00 50 31  ---          05 22 05  62.9 -31.2  1.5     133.6    30     2678   00 50 02

00 50 42  NRAO150      05 22 17  64.6 -30.7  1.4     135.6     0     2678   00 50 42
00 51 12  ---          05 22 47  64.6 -30.9  1.4     135.4    30     2682   00 50 43

00 51 23  J0350+5138   05 22 58  63.1 -32.0  1.5     132.6     0     2682   00 51 23
00 51 53  ---          05 23 28  63.0 -32.2  1.5     132.4    30     2686   00 51 24

00 52 04  NRAO150      05 23 39  64.5 -31.1  1.4     135.0     0     2686   00 52 04
00 52 34  ---          05 24 09  64.4 -31.2  1.4     134.8    30     2690   00 52 05

00 52 46  J0350+5201   05 24 21  62.7 -31.7  1.5     132.7     0     2690   00 52 46
00 53 16  ---          05 24 51  62.6 -31.8  1.5     132.5    30     2694   00 52 47

00 53 27  NRAO150      05 25 02  64.3 -31.5  1.4     134.5     0     2694   00 53 27
00 53 57  ---          05 25 32  64.3 -31.6  1.4     134.2    30     2698   00 53 28

00 54 08  J0350+5138   05 25 44  62.7 -32.7  1.6     131.5     0     2698   00 54 08
00 54 38  ---          05 26 14  62.7 -32.8  1.6     131.3    30     2701   00 54 09

00 54 49  NRAO150      05 26 25  64.2 -31.8  1.4     133.9     0     2701   00 54 49
00 55 19  ---          05 26 55  64.1 -31.9  1.4     133.7    30     2705   00 54 50

00 55 31  J0350+5201   05 27 06  62.4 -32.3  1.6     131.6     0     2705   00 55 31
00 56 01  ---          05 27 36  62.3 -32.4  1.6     131.4    30     2709   00 55 32

00 56 12  NRAO150      05 27 48  64.0 -32.2  1.5     133.3     0     2709   00 56 12
00 56 42  ---          05 28 18  64.0 -32.3  1.5     133.1    30     2713   00 56 13

00 56 53  J0350+5138   05 28 29  62.4 -33.3  1.6     130.4     0     2713   00 56 53
00 57 23  ---          05 28 59  62.4 -33.4  1.6     130.2    30     2717   00 56 54

00 57 34  NRAO150      05 29 10  63.9 -32.5  1.5     132.7     0     2717   00 57 34
00 58 04  ---          05 29 40  63.8 -32.6  1.5     132.5    30     2721   00 57 35

00 58 16  J0350+5201   05 29 52  62.0 -32.9  1.6     130.5     0     2721   00 58 16
00 58 46  ---          05 30 22  62.0 -33.0  1.6     130.3    30     2725   00 58 17

00 58 57  NRAO150      05 30 33  63.7 -32.8  1.5     132.2     0     2725   00 58 57
00 59 27  ---          05 31 04  63.6 -32.9  1.5     132.0    30     2729   00 58 58
Schedule for VLBA_FD   (Code Fd )                                   Page  42
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

00 59 39  J0350+5138   05 31 15  62.1 -33.9  1.7     129.3     0     2729   00 59 39
01 00 09  ---          05 31 45  62.0 -34.0  1.7     129.1    30     2732   00 59 40

01 00 20  NRAO150      05 31 56  63.5 -33.1  1.5     131.6     0     2732   01 00 20
01 00 50  ---          05 32 26  63.5 -33.3  1.5     131.4    30     2736   01 00 21

01 01 01  J0350+5201   05 32 37  61.7 -33.5  1.7     129.5     0     2736   01 01 01
01 01 31  ---          05 33 08  61.7 -33.6  1.7     129.3    30     2740   01 01 02

01 01 43  NRAO150      05 33 19  63.4 -33.5  1.5     131.0     0     2740   01 01 43
01 02 13  ---          05 33 49  63.3 -33.6  1.6     130.8    30     2744   01 01 44

01 02 24  J0350+5138   05 34 00  61.8 -34.4  1.7     128.3     0     2744   01 02 24
01 02 54  ---          05 34 30  61.7 -34.5  1.7     128.1    30     2748   01 02 25

01 03 05  NRAO150      05 34 41  63.2 -33.8  1.6     130.5     0     2748   01 03 05
01 03 35  ---          05 35 11  63.1 -33.9  1.6     130.3    30     2752   01 03 06

01 03 46  J0350+5201   05 35 23  61.4 -34.0  1.7     128.4     0     2752   01 03 46
01 04 16  ---          05 35 53  61.3 -34.1  1.7     128.3    30     2756   01 03 47

01 04 28  NRAO150      05 36 04  63.0 -34.1  1.6     130.0     0     2756   01 04 28
01 04 58  ---          05 36 35  63.0 -34.2  1.6     129.8    30     2759   01 04 29

01 05 09  J0350+5138   05 36 46  61.4 -35.0  1.8     127.3     0     2759   01 05 09
01 05 39  ---          05 37 16  61.4 -35.1  1.8     127.1    30     2763   01 05 10

01 05 50  NRAO150      05 37 27  62.9 -34.4  1.6     129.4     0     2763   01 05 50
01 06 20  ---          05 37 57  62.8 -34.5  1.6     129.2    30     2767   01 05 51

01 06 31  J0350+5201   05 38 08  61.1 -34.6  1.8     127.4     0     2767   01 06 31
01 07 01  ---          05 38 38  61.0 -34.7  1.8     127.2    30     2771   01 06 32

01 07 13  NRAO150      05 38 50  62.7 -34.7  1.6     128.9     0     2771   01 07 13
01 07 43  ---          05 39 20  62.6 -34.8  1.6     128.7    30     2775   01 07 14

01 07 54  J0350+5138   05 39 31  61.1 -35.5  1.8     126.2     0     2775   01 07 54
01 08 24  ---          05 40 01  61.0 -35.6  1.8     126.1    30     2779   01 07 55

01 08 35  NRAO150      05 40 12  62.5 -35.0  1.7     128.4     0     2779   01 08 35
01 09 05  ---          05 40 42  62.5 -35.1  1.7     128.2    30     2783   01 08 36

01 09 16  J0350+5201   05 40 54  60.7 -35.1  1.8     126.4     0     2783   01 09 16
01 09 46  ---          05 41 24  60.7 -35.2  1.8     126.2    30     2786   01 09 17
Schedule for VLBA_FD   (Code Fd )                                   Page  43
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

01 09 58  NRAO150      05 41 35  62.4 -35.3  1.7     127.8     0     2786   01 09 58
01 10 28  ---          05 42 05  62.3 -35.4  1.7     127.6    30     2790   01 09 59

01 10 39  J0350+5138   05 42 17  60.7 -36.0  1.8     125.3     0     2790   01 10 39
01 11 09  ---          05 42 47  60.7 -36.1  1.9     125.1    30     2794   01 10 40

01 11 20  NRAO150      05 42 58  62.2 -35.6  1.7     127.3     0     2794   01 11 20
01 11 50  ---          05 43 28  62.1 -35.7  1.7     127.1    30     2798   01 11 21

01 12 01  J0350+5201   05 43 39  60.4 -35.6  1.9     125.4     0     2798   01 12 01
01 12 31  ---          05 44 09  60.3 -35.7  1.9     125.3    30     2802   01 12 02

01 12 43  NRAO150      05 44 21  62.0 -35.8  1.7     126.8     0     2802   01 12 43
01 13 13  ---          05 44 51  62.0 -35.9  1.7     126.6    30     2806   01 12 44

01 13 24  J0350+5138   05 45 02  60.4 -36.5  1.9     124.3     0     2806   01 13 24
01 13 54  ---          05 45 32  60.3 -36.6  1.9     124.1    30     2810   01 13 25

01 14 05  NRAO150      05 45 43  61.8 -36.1  1.7     126.3     0     2810   01 14 05
01 14 35  ---          05 46 13  61.8 -36.2  1.8     126.1    30     2814   01 14 06

01 14 46  J0350+5201   05 46 25  60.0 -36.1  1.9     124.5     0     2814   01 14 46
01 15 16  ---          05 46 55  60.0 -36.2  1.9     124.3    30     2817   01 14 47

01 15 28  NRAO150      05 47 07  61.7 -36.4  1.8     125.8     0     2817   01 15 28
01 15 58  ---          05 47 37  61.6 -36.5  1.8     125.6    30     2821   01 15 29

01 16 09  J0350+5138   05 47 48  60.0 -37.0  1.9     123.3     0     2821   01 16 09
01 16 39  ---          05 48 18  60.0 -37.1  1.9     123.2    30     2825   01 16 10

01 16 50  NRAO150      05 48 29  61.5 -36.7  1.8     125.3     0     2825   01 16 50
01 17 20  ---          05 48 59  61.4 -36.7  1.8     125.1    30     2829   01 16 51

01 17 31  J0350+5201   05 49 11  59.7 -36.6  2.0     123.5     0     2829   01 17 31
01 18 01  ---          05 49 41  59.6 -36.6  2.0     123.3    30     2833   01 17 32

01 18 13  NRAO150      05 49 52  61.3 -36.9  1.8     124.8     0     2833   01 18 13
01 18 43  ---          05 50 22  61.2 -37.0  1.8     124.6    30     2837   01 18 14

01 18 54  J0350+5138   05 50 33  59.7 -37.5  2.0     122.4     0     2837   01 18 54
01 19 24  ---          05 51 03  59.6 -37.6  2.0     122.2    30     2841   01 18 55

01 19 35  NRAO150      05 51 15  61.1 -37.2  1.8     124.3     0     2841   01 19 35
01 20 05  ---          05 51 45  61.1 -37.3  1.8     124.1    30     2844   01 19 36
Schedule for VLBA_FD   (Code Fd )                                   Page  44
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

01 20 17  J0350+5201   05 51 56  59.3 -37.0  2.0     122.6     0     2844   01 20 17
01 20 47  ---          05 52 26  59.3 -37.1  2.0     122.4    30     2848   01 20 18

01 20 58  NRAO150      05 52 38  61.0 -37.4  1.9     123.8     0     2848   01 20 58
01 21 28  ---          05 53 08  60.9 -37.5  1.9     123.6    30     2852   01 20 59

01 21 39  J0350+5138   05 53 19  59.3 -37.9  2.0     121.5     0     2852   01 21 39
01 22 09  ---          05 53 49  59.2 -38.0  2.0     121.3    30     2856   01 21 40

01 22 20  NRAO150      05 54 00  60.8 -37.7  1.9     123.3     0     2856   01 22 20
01 22 50  ---          05 54 30  60.7 -37.8  1.9     123.1    30     2860   01 22 21

01 23 02  J0350+5201   05 54 42  59.0 -37.5  2.0     121.7     0     2860   01 23 02
01 23 32  ---          05 55 12  58.9 -37.5  2.1     121.5    30     2864   01 23 03

01 23 43  NRAO150      05 55 23  60.6 -37.9  1.9     122.8     0     2864   01 23 43
01 24 13  ---          05 55 53  60.5 -38.0  1.9     122.7    30     2868   01 23 44

01 24 24  J0350+5138   05 56 05  58.9 -38.3  2.1     120.6     0     2868   01 24 24
01 24 54  ---          05 56 35  58.9 -38.4  2.1     120.4    30     2872   01 24 25

01 25 06  NRAO150      05 56 46  60.4 -38.1  1.9     122.4     0     2872   01 25 06
01 25 36  ---          05 57 16  60.3 -38.2  1.9     122.2    30     2875   01 25 07

01 25 47  J0350+5201   05 57 27  58.6 -37.9  2.1     120.7     0     2875   01 25 47
01 26 17  ---          05 57 58  58.5 -38.0  2.1     120.6    30     2879   01 25 48

01 26 28  NRAO150      05 58 09  60.2 -38.4  2.0     121.9     0     2879   01 26 28
01 26 58  ---          05 58 39  60.2 -38.5  2.0     121.7    30     2883   01 26 29

01 27 10  J0350+5138   05 58 50  58.6 -38.8  2.1     119.7     0     2883   01 27 10
01 27 40  ---          05 59 20  58.5 -38.8  2.1     119.5    30     2887   01 27 11

01 27 51  NRAO150      05 59 31  60.0 -38.6  2.0     121.4     0     2887   01 27 51
01 28 21  ---          06 00 02  60.0 -38.7  2.0     121.3    30     2891   01 27 52

01 28 32  J0350+5201   06 00 13  58.2 -38.3  2.1     119.9     0     2891   01 28 32
01 29 02  ---          06 00 43  58.2 -38.4  2.1     119.7    30     2895   01 28 33

01 29 14  NRAO150      06 00 55  59.9 -38.8  2.0     121.0     0     2895   01 29 14
01 29 44  ---          06 01 25  59.8 -38.9  2.0     120.8    30     2899   01 29 15

01 29 55  J0350+5138   06 01 36  58.2 -39.2  2.2     118.8     0     2899   01 29 55
01 30 25  ---          06 02 06  58.1 -39.2  2.2     118.6    30     2902   01 29 56
Schedule for VLBA_FD   (Code Fd )                                   Page  45
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

01 30 36  NRAO150      06 02 17  59.7 -39.1  2.0     120.5     0     2902   01 30 36
01 31 06  ---          06 02 47  59.6 -39.1  2.0     120.3    30     2906   01 30 37

01 31 17  J0350+5201   06 02 59  57.9 -38.7  2.2     119.0     0     2906   01 31 17
01 31 47  ---          06 03 29  57.8 -38.7  2.2     118.8    30     2910   01 31 18

01 31 59  NRAO150      06 03 40  59.5 -39.3  2.0     120.0     0     2910   01 31 59
01 32 29  ---          06 04 10  59.4 -39.3  2.1     119.9    30     2914   01 32 00

01 32 40  J0350+5138   06 04 22  57.8 -39.5  2.2     117.9     0     2914   01 32 40
01 33 10  ---          06 04 52  57.7 -39.6  2.2     117.8    30     2918   01 32 41

01 33 21  NRAO150      06 05 03  59.3 -39.5  2.1     119.6     0     2918   01 33 21
01 33 51  ---          06 05 33  59.2 -39.6  2.1     119.4    30     2922   01 33 22

01 34 03  J0350+5201   06 05 44  57.5 -39.1  2.2     118.1     0     2922   01 34 03
01 34 33  ---          06 06 14  57.4 -39.1  2.2     118.0    30     2926   01 34 04

01 34 44  NRAO150      06 06 26  59.1 -39.7  2.1     119.2     0     2926   01 34 44
01 35 14  ---          06 06 56  59.0 -39.8  2.1     119.0    30     2929   01 34 45

01 35 25  J0350+5138   06 07 07  57.4 -39.9  2.3     117.1     0     2929   01 35 25
01 35 55  ---          06 07 37  57.4 -40.0  2.3     116.9    30     2933   01 35 26

01 36 06  NRAO150      06 07 48  58.9 -39.9  2.1     118.7     0     2933   01 36 06
01 36 36  ---          06 08 18  58.8 -40.0  2.1     118.6    30     2937   01 36 07

01 36 48  J0350+5201   06 08 30  57.1 -39.4  2.3     117.3     0     2937   01 36 48
01 37 18  ---          06 09 00  57.0 -39.5  2.3     117.1    30     2941   01 36 49

01 37 29  NRAO150      06 09 11  58.7 -40.1  2.1     118.3     0     2941   01 37 29
01 37 59  ---          06 09 42  58.6 -40.2  2.1     118.1    30     2945   01 37 30

01 38 10  J0350+5138   06 09 53  57.1 -40.3  2.3     116.2     0     2945   01 38 10
01 38 40  ---          06 10 23  57.0 -40.3  2.3     116.1    30     2949   01 38 11

01 38 51  NRAO150      06 10 34  58.5 -40.3  2.2     117.8     0     2949   01 38 51
01 39 21  ---          06 11 04  58.5 -40.4  2.2     117.7    30     2953   01 38 52

01 39 33  J0350+5201   06 11 15  56.7 -39.8  2.3     116.4     0     2953   01 39 33
01 40 03  ---          06 11 46  56.7 -39.8  2.3     116.3    30     2957   01 39 34

01 40 14  NRAO150      06 11 57  58.3 -40.5  2.2     117.4     0     2957   01 40 14
01 40 44  ---          06 12 27  58.3 -40.5  2.2     117.2    30     2960   01 40 15
Schedule for VLBA_FD   (Code Fd )                                   Page  46
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

01 40 55  J0350+5138   06 12 38  56.7 -40.6  2.3     115.4     0     2960   01 40 55
01 41 25  ---          06 13 08  56.6 -40.7  2.4     115.2    30     2964   01 40 56

01 41 36  NRAO150      06 13 19  58.1 -40.7  2.2     117.0     0     2964   01 41 36
01 42 06  ---          06 13 50  58.1 -40.7  2.2     116.8    30     2968   01 41 37

01 42 18  J0350+5201   06 14 01  56.4 -40.1  2.4     115.6     0     2968   01 42 18
01 42 48  ---          06 14 31  56.3 -40.2  2.4     115.4    30     2972   01 42 19

01 42 59  NRAO150      06 14 43  57.9 -40.9  2.2     116.5     0     2972   01 42 59
01 43 29  ---          06 15 13  57.9 -40.9  2.2     116.4    30     2976   01 43 00

01 43 40  J0350+5138   06 15 24  56.3 -40.9  2.4     114.6     0     2976   01 43 40
01 44 10  ---          06 15 54  56.2 -41.0  2.4     114.4    30     2980   01 43 41

01 44 22  NRAO150      06 16 05  57.8 -41.0  2.3     116.1     0     2980   01 44 22
01 44 52  ---          06 16 35  57.7 -41.1  2.3     116.0    30     2984   01 44 23

01 45 03  J0350+5201   06 16 47  56.0 -40.4  2.4     114.8     0     2984   01 45 03
01 45 33  ---          06 17 17  55.9 -40.5  2.4     114.6    30     2987   01 45 04

01 45 44  NRAO150      06 17 28  57.6 -41.2  2.3     115.7     0     2987   01 45 44
01 46 14  ---          06 17 58  57.5 -41.3  2.3     115.6    30     2991   01 45 45

01 46 26  J0350+5138   06 18 09  55.9 -41.2  2.4     113.8     0     2991   01 46 26
01 46 56  ---          06 18 39  55.8 -41.3  2.4     113.6    30     2995   01 46 27

01 47 07  NRAO150      06 18 51  57.4 -41.4  2.3     115.3     0     2995   01 47 07
01 47 37  ---          06 19 21  57.3 -41.4  2.3     115.1    30     2999   01 47 08

01 47 48  J0350+5201   06 19 32  55.6 -40.7  2.5     114.0     0     2999   01 47 48
01 48 18  ---          06 20 02  55.5 -40.8  2.5     113.8    30     3003   01 47 49

01 48 29  NRAO150      06 20 14  57.2 -41.6  2.3     114.9     0     3003   01 48 29
01 48 59  ---          06 20 44  57.1 -41.6  2.3     114.7    30     3007   01 48 30

01 49 11  J0350+5138   06 20 55  55.5 -41.5  2.5     113.0     0     3007   01 49 11
01 49 41  ---          06 21 25  55.4 -41.6  2.5     112.8    30     3011   01 49 12

01 49 52  NRAO150      06 21 36  57.0 -41.7  2.3     114.5     0     3011   01 49 52
01 50 22  ---          06 22 06  56.9 -41.8  2.4     114.3    30     3014   01 49 53

01 50 33  J0350+5201   06 22 18  55.2 -41.0  2.5     113.2     0     3014   01 50 33
01 51 03  ---          06 22 48  55.1 -41.1  2.5     113.0    30     3018   01 50 34
Schedule for VLBA_FD   (Code Fd )                                   Page  47
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

01 51 15  NRAO150      06 22 59  56.8 -41.9  2.4     114.1     0     3018   01 51 15
01 51 45  ---          06 23 29  56.7 -41.9  2.4     113.9    30     3022   01 51 16

01 51 56  J0350+5138   06 23 40  55.1 -41.8  2.5     112.2     0     3022   01 51 56
01 52 26  ---          06 24 11  55.0 -41.9  2.5     112.1    30     3026   01 51 57

01 52 37  NRAO150      06 24 22  56.6 -42.0  2.4     113.7     0     3026   01 52 37
01 53 07  ---          06 24 52  56.5 -42.1  2.4     113.5    30     3030   01 52 38

01 53 18  J0350+5201   06 25 03  54.8 -41.3  2.6     112.4     0     3030   01 53 18
01 53 48  ---          06 25 33  54.7 -41.4  2.6     112.3    30     3034   01 53 19

01 54 00  NRAO150      06 25 45  56.4 -42.2  2.4     113.3     0     3034   01 54 00
01 54 30  ---          06 26 15  56.3 -42.3  2.4     113.1    30     3038   01 54 01

01 54 41  J0350+5138   06 26 26  54.7 -42.1  2.6     111.4     0     3038   01 54 41
01 55 11  ---          06 26 56  54.6 -42.2  2.6     111.3    30     3042   01 54 42

01 55 22  NRAO150      06 27 07  56.2 -42.4  2.4     112.9     0     3042   01 55 22
01 55 52  ---          06 27 37  56.1 -42.4  2.4     112.7    30     3045   01 55 23

01 56 03  J0350+5201   06 27 49  54.4 -41.6  2.6     111.6     0     3045   01 56 03
01 56 33  ---          06 28 19  54.3 -41.7  2.6     111.5    30     3049   01 56 04

01 56 45  NRAO150      06 28 30  56.0 -42.5  2.5     112.5     0     3049   01 56 45
01 57 15  ---          06 29 00  55.9 -42.6  2.5     112.3    30     3053   01 56 46

01 57 26  J0350+5138   06 29 11  54.3 -42.4  2.6     110.7     0     3053   01 57 26
01 57 56  ---          06 29 42  54.2 -42.4  2.6     110.5    30     3057   01 57 27

01 58 07  NRAO150      06 29 53  55.8 -42.6  2.5     112.1     0     3057   01 58 07
01 58 37  ---          06 30 23  55.7 -42.7  2.5     112.0    30     3061   01 58 08

01 58 48  J0350+5201   06 30 34  54.0 -41.9  2.6     110.9     0     3061   01 58 48
01 59 18  ---          06 31 04  53.9 -41.9  2.7     110.8    30     3065   01 58 49

01 59 30  NRAO150      06 31 16  55.6 -42.8  2.5     111.7     0     3065   01 59 30
02 00 00  ---          06 31 46  55.5 -42.8  2.5     111.6    30     3069   01 59 31

02 00 11  J0350+5138   06 31 57  53.9 -42.6  2.7     109.9     0     3069   02 00 11
02 00 41  ---          06 32 27  53.8 -42.7  2.7     109.8    30     3072   02 00 12

02 00 52  NRAO150      06 32 38  55.4 -42.9  2.5     111.3     0     3072   02 00 52
02 01 22  ---          06 33 08  55.3 -43.0  2.5     111.2    30     3076   02 00 53
Schedule for VLBA_FD   (Code Fd )                                   Page  48
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

02 01 33  J0350+5201   06 33 20  53.6 -42.1  2.7     110.1     0     3076   02 01 33
02 02 03  ---          06 33 50  53.6 -42.2  2.7     110.0    30     3080   02 01 34

02 02 15  NRAO150      06 34 01  55.2 -43.1  2.6     110.9     0     3080   02 02 15
02 02 45  ---          06 34 31  55.1 -43.1  2.6     110.8    30     3084   02 02 16

02 02 56  J0350+5138   06 34 42  53.5 -42.9  2.7     109.2     0     3084   02 02 56
02 03 26  ---          06 35 12  53.4 -42.9  2.7     109.1    30     3088   02 02 57

02 03 37  NRAO150      06 35 24  55.0 -43.2  2.6     110.6     0     3088   02 03 37
02 04 07  ---          06 35 54  54.9 -43.3  2.6     110.4    30     3092   02 03 38

02 04 18  J0350+5201   06 36 05  53.2 -42.4  2.7     109.4     0     3092   02 04 18
02 04 48  ---          06 36 35  53.2 -42.4  2.7     109.3    30     3096   02 04 19

02 05 00  NRAO150      06 36 46  54.8 -43.3  2.6     110.2     0     3096   02 05 00
02 05 30  ---          06 37 17  54.7 -43.4  2.6     110.1    30     3100   02 05 01

02 05 41  J0350+5138   06 37 28  53.1 -43.1  2.8     108.5     0     3100   02 05 41
02 06 11  ---          06 37 58  53.0 -43.1  2.8     108.3    30     3103   02 05 42

02 06 22  NRAO150      06 38 09  54.6 -43.5  2.6     109.8     0     3103   02 06 22
02 06 52  ---          06 38 39  54.5 -43.5  2.6     109.7    30     3107   02 06 23

02 07 03  J0350+5201   06 38 50  52.8 -42.6  2.8     108.7     0     3107   02 07 03
02 07 33  ---          06 39 21  52.8 -42.6  2.8     108.5    30     3111   02 07 04

02 07 44  NRAO150      06 39 32  54.4 -43.6  2.6     109.4     0     3111   02 07 44
02 08 14  ---          06 40 02  54.3 -43.6  2.7     109.3    30     3115   02 07 45

02 08 26  J0350+5138   06 40 13  52.7 -43.3  2.8     107.8     0     3115   02 08 26
02 08 56  ---          06 40 43  52.6 -43.4  2.8     107.6    30     3119   02 08 27

02 09 07  NRAO150      06 40 54  54.2 -43.7  2.7     109.1     0     3119   02 09 07
02 09 37  ---          06 41 24  54.1 -43.8  2.7     108.9    30     3123   02 09 08

02 09 48  J0350+5201   06 41 36  52.4 -42.8  2.8     108.0     0     3123   02 09 48
02 10 18  ---          06 42 06  52.3 -42.8  2.8     107.8    30     3127   02 09 49

02 10 29  NRAO150      06 42 17  53.9 -43.8  2.7     108.7     0     3127   02 10 29
02 10 59  ---          06 42 47  53.9 -43.9  2.7     108.6    30     3130   02 10 30

02 11 11  J0350+5138   06 42 58  52.3 -43.5  2.9     107.1     0     3130   02 11 11
02 11 41  ---          06 43 28  52.2 -43.6  2.9     106.9    30     3134   02 11 12
Schedule for VLBA_FD   (Code Fd )                                   Page  49
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

02 11 52  NRAO150      06 43 40  53.7 -43.9  2.7     108.4     0     3134   02 11 52
02 12 22  ---          06 44 10  53.7 -44.0  2.7     108.2    30     3138   02 11 53

02 12 33  J0350+5201   06 44 21  52.0 -43.0  2.9     107.3     0     3138   02 12 33
02 13 03  ---          06 44 51  51.9 -43.1  2.9     107.1    30     3142   02 12 34

02 13 14  NRAO150      06 45 02  53.5 -44.1  2.7     108.0     0     3142   02 13 14
02 13 44  ---          06 45 32  53.5 -44.1  2.7     107.9    30     3146   02 13 15

02 13 55  J0350+5138   06 45 44  51.9 -43.7  2.9     106.4     0     3146   02 13 55
02 14 25  ---          06 46 14  51.8 -43.8  2.9     106.2    30     3150   02 13 56

02 14 36  NRAO150      06 46 25  53.3 -44.2  2.8     107.6     0     3150   02 14 36
02 15 06  ---          06 46 55  53.3 -44.2  2.8     107.5    30     3154   02 14 37

02 15 18  J0350+5201   06 47 06  51.6 -43.2  2.9     106.6     0     3154   02 15 18
02 15 48  ---          06 47 36  51.5 -43.3  2.9     106.4    30     3157   02 15 19

02 15 59  NRAO150      06 47 48  53.1 -44.3  2.8     107.3     0     3157   02 15 59
02 16 29  ---          06 48 18  53.0 -44.3  2.8     107.2    30     3161   02 16 00

02 17 24  DA193        06 49 13  75.9 -45.8  0.9     126.6     2     3161   02 17 24
02 22 24  ---          06 54 13  75.1 -48.0  1.0     123.7   300     3200   02 17 25

02 24 28  OJ287        06 56 18  61.1 104.4 -2.0     -62.5     8     3200   02 24 28
02 29 28  ---          07 01 18  62.1 105.6 -1.9     -61.9   300     3239   02 24 29

02 31 34  J0350+5138   07 03 25  49.2 -44.8  3.2     102.1    11     3239   02 31 34
02 32 10  ---          07 03 55  49.1 -44.8  3.2     101.9    37     3243   02 31 35

02 32 22  NRAO150      07 04 13  50.6 -45.4  3.1     103.2     0     3243   02 32 22
02 32 52  ---          07 04 43  50.6 -45.4  3.1     103.1    30     3247   02 32 23

02 33 03  J0350+5201   07 04 54  49.0 -44.3  3.2     102.2     0     3247   02 33 03
02 33 33  ---          07 05 24  48.9 -44.3  3.2     102.1    30     3251   02 33 04

02 33 44  NRAO150      07 05 35  50.4 -45.5  3.1     102.9     0     3251   02 33 44
02 34 14  ---          07 06 05  50.3 -45.5  3.1     102.8    30     3255   02 33 45

02 34 25  J0350+5138   07 06 17  48.8 -44.9  3.2     101.4     0     3255   02 34 25
02 34 55  ---          07 06 47  48.7 -44.9  3.3     101.3    30     3259   02 34 26

02 35 06  NRAO150      07 06 58  50.2 -45.5  3.1     102.6     0     3259   02 35 06
02 35 36  ---          07 07 28  50.1 -45.6  3.1     102.5    30     3263   02 35 07
Schedule for VLBA_FD   (Code Fd )                                   Page  50
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

02 35 47  J0350+5201   07 07 39  48.6 -44.4  3.3     101.6     0     3263   02 35 47
02 36 17  ---          07 08 09  48.5 -44.4  3.3     101.5    30     3267   02 35 48

02 36 28  NRAO150      07 08 20  50.0 -45.6  3.1     102.3     0     3267   02 36 28
02 36 58  ---          07 08 50  49.9 -45.6  3.1     102.1    30     3270   02 36 29

02 37 09  J0350+5138   07 09 01  48.4 -45.0  3.3     100.8     0     3270   02 37 09
02 37 39  ---          07 09 32  48.3 -45.1  3.3     100.7    30     3274   02 37 10

02 37 50  NRAO150      07 09 43  49.8 -45.7  3.1     101.9     0     3274   02 37 50
02 38 20  ---          07 10 13  49.7 -45.7  3.2     101.8    30     3278   02 37 51

02 38 31  J0350+5201   07 10 24  48.1 -44.5  3.3     100.9     0     3278   02 38 31
02 39 01  ---          07 10 54  48.1 -44.6  3.3     100.8    30     3282   02 38 32

02 39 13  NRAO150      07 11 05  49.6 -45.7  3.2     101.6     0     3282   02 39 13
02 39 43  ---          07 11 35  49.5 -45.8  3.2     101.5    30     3286   02 39 14

02 39 54  J0350+5138   07 11 46  47.9 -45.2  3.3     100.1     0     3286   02 39 54
02 40 24  ---          07 12 16  47.9 -45.2  3.3     100.0    30     3290   02 39 55

02 40 35  NRAO150      07 12 27  49.4 -45.8  3.2     101.3     0     3290   02 40 35
02 41 05  ---          07 12 57  49.3 -45.8  3.2     101.2    30     3294   02 40 36

02 41 16  J0350+5201   07 13 09  47.7 -44.7  3.4     100.3     0     3294   02 41 16
02 41 46  ---          07 13 39  47.6 -44.7  3.4     100.2    30     3298   02 41 17

02 41 57  NRAO150      07 13 50  49.2 -45.9  3.2     101.0     0     3298   02 41 57
02 42 27  ---          07 14 20  49.1 -45.9  3.2     100.9    30     3301   02 41 58

02 42 38  J0350+5138   07 14 31  47.5 -45.3  3.4      99.5     0     3301   02 42 38
02 43 08  ---          07 15 01  47.5 -45.3  3.4      99.4    30     3305   02 42 39

02 43 19  NRAO150      07 15 12  48.9 -45.9  3.2     100.7     0     3305   02 43 19
02 43 49  ---          07 15 42  48.9 -46.0  3.2     100.6    30     3309   02 43 20

02 44 00  J0350+5201   07 15 53  47.3 -44.8  3.4      99.7     0     3309   02 44 00
02 44 30  ---          07 16 23  47.2 -44.8  3.4      99.6    30     3313   02 44 01

02 44 41  NRAO150      07 16 34  48.7 -46.0  3.3     100.4     0     3313   02 44 41
02 45 11  ---          07 17 05  48.6 -46.0  3.3     100.2    30     3317   02 44 42

02 45 22  J0350+5138   07 17 16  47.1 -45.4  3.4      98.9     0     3317   02 45 22
02 45 52  ---          07 17 46  47.0 -45.4  3.4      98.8    30     3321   02 45 23
Schedule for VLBA_FD   (Code Fd )                                   Page  51
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

02 46 03  NRAO150      07 17 57  48.5 -46.1  3.3     100.0     0     3321   02 46 03
02 46 33  ---          07 18 27  48.4 -46.1  3.3      99.9    30     3325   02 46 04

02 46 44  J0350+5201   07 18 38  46.9 -44.9  3.4      99.1     0     3325   02 46 44
02 47 14  ---          07 19 08  46.8 -44.9  3.5      99.0    30     3328   02 46 45

02 47 25  NRAO150      07 19 19  48.3 -46.1  3.3      99.7     0     3328   02 47 25
02 47 55  ---          07 19 49  48.2 -46.1  3.3      99.6    30     3332   02 47 26

02 48 06  J0350+5138   07 20 00  46.7 -45.5  3.5      98.3     0     3332   02 48 06
02 48 36  ---          07 20 30  46.6 -45.5  3.5      98.2    30     3336   02 48 07

02 48 47  NRAO150      07 20 41  48.1 -46.2  3.3      99.4     0     3336   02 48 47
02 49 17  ---          07 21 11  48.0 -46.2  3.3      99.3    30     3340   02 48 48

02 49 28  J0350+5201   07 21 23  46.5 -45.0  3.5      98.5     0     3340   02 49 28
02 49 58  ---          07 21 53  46.4 -45.0  3.5      98.4    30     3344   02 49 29

02 50 09  NRAO150      07 22 04  47.9 -46.2  3.4      99.1     0     3344   02 50 09
02 50 39  ---          07 22 34  47.8 -46.2  3.4      99.0    30     3348   02 50 10

02 50 50  J0350+5138   07 22 45  46.3 -45.6  3.5      97.7     0     3348   02 50 50
02 51 20  ---          07 23 15  46.2 -45.6  3.5      97.6    30     3352   02 50 51

02 51 31  NRAO150      07 23 26  47.7 -46.3  3.4      98.8     0     3352   02 51 31
02 52 01  ---          07 23 56  47.6 -46.3  3.4      98.7    30     3355   02 51 32

02 52 12  J0350+5201   07 24 07  46.1 -45.0  3.5      97.9     0     3355   02 52 12
02 52 42  ---          07 24 37  46.0 -45.1  3.5      97.8    30     3359   02 52 13

02 52 53  NRAO150      07 24 48  47.5 -46.3  3.4      98.5     0     3359   02 52 53
02 53 23  ---          07 25 18  47.4 -46.3  3.4      98.4    30     3363   02 52 54

02 53 34  J0350+5138   07 25 29  45.8 -45.6  3.6      97.1     0     3363   02 53 34
02 54 04  ---          07 25 59  45.8 -45.6  3.6      97.0    30     3367   02 53 35

02 54 15  NRAO150      07 26 10  47.2 -46.4  3.4      98.2     0     3367   02 54 15
02 54 45  ---          07 26 40  47.2 -46.4  3.4      98.1    30     3371   02 54 16

02 54 56  J0350+5201   07 26 51  45.6 -45.1  3.6      97.3     0     3371   02 54 56
02 55 26  ---          07 27 22  45.6 -45.1  3.6      97.2    30     3375   02 54 57

02 55 37  NRAO150      07 27 33  47.0 -46.4  3.4      97.9     0     3375   02 55 37
02 56 07  ---          07 28 03  46.9 -46.4  3.5      97.8    30     3379   02 55 38
Schedule for VLBA_FD   (Code Fd )                                   Page  52
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

02 56 18  J0350+5138   07 28 14  45.4 -45.7  3.6      96.5     0     3379   02 56 18
02 56 48  ---          07 28 44  45.3 -45.7  3.6      96.4    30     3383   02 56 19

02 56 59  NRAO150      07 28 55  46.8 -46.4  3.5      97.6     0     3383   02 56 59
02 57 29  ---          07 29 25  46.7 -46.5  3.5      97.5    30     3386   02 57 00

02 57 40  J0350+5201   07 29 36  45.2 -45.2  3.6      96.7     0     3386   02 57 40
02 58 10  ---          07 30 06  45.1 -45.2  3.6      96.6    30     3390   02 57 41

02 58 21  NRAO150      07 30 17  46.6 -46.5  3.5      97.3     0     3390   02 58 21
02 58 51  ---          07 30 47  46.5 -46.5  3.5      97.2    30     3394   02 58 22

02 59 02  J0350+5138   07 30 58  45.0 -45.8  3.7      95.9     0     3394   02 59 02
02 59 32  ---          07 31 28  44.9 -45.8  3.7      95.8    30     3398   02 59 03

02 59 43  NRAO150      07 31 39  46.4 -46.5  3.5      97.0     0     3398   02 59 43
03 00 13  ---          07 32 09  46.3 -46.5  3.5      96.9    30     3402   02 59 44

03 00 24  J0350+5201   07 32 20  44.8 -45.3  3.7      96.1     0     3402   03 00 24
03 00 54  ---          07 32 50  44.7 -45.3  3.7      96.0    30     3406   03 00 25

03 01 05  NRAO150      07 33 01  46.2 -46.6  3.5      96.7     0     3406   03 01 05
03 01 35  ---          07 33 31  46.1 -46.6  3.5      96.6    30     3410   03 01 06

03 01 46  J0350+5138   07 33 42  44.6 -45.8  3.7      95.4     0     3410   03 01 46
03 02 16  ---          07 34 12  44.5 -45.8  3.7      95.3    30     3413   03 01 47

03 02 27  NRAO150      07 34 23  46.0 -46.6  3.6      96.5     0     3413   03 02 27
03 02 57  ---          07 34 54  45.9 -46.6  3.6      96.3    30     3417   03 02 28

03 03 08  J0350+5201   07 35 05  44.4 -45.3  3.7      95.5     0     3417   03 03 08
03 03 38  ---          07 35 35  44.3 -45.3  3.7      95.4    30     3421   03 03 09

03 03 49  NRAO150      07 35 46  45.7 -46.6  3.6      96.2     0     3421   03 03 49
03 04 19  ---          07 36 16  45.7 -46.6  3.6      96.1    30     3425   03 03 50

03 04 30  J0350+5138   07 36 27  44.2 -45.9  3.7      94.8     0     3425   03 04 30
03 05 00  ---          07 36 57  44.1 -45.9  3.8      94.7    30     3429   03 04 31

03 05 11  NRAO150      07 37 08  45.5 -46.7  3.6      95.9     0     3429   03 05 11
03 05 41  ---          07 37 38  45.4 -46.7  3.6      95.8    30     3433   03 05 12

03 05 52  J0350+5201   07 37 49  44.0 -45.4  3.8      94.9     0     3433   03 05 52
03 06 22  ---          07 38 19  43.9 -45.4  3.8      94.8    30     3437   03 05 53
Schedule for VLBA_FD   (Code Fd )                                   Page  53
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

03 06 33  NRAO150      07 38 30  45.3 -46.7  3.6      95.6     0     3437   03 06 33
03 07 03  ---          07 39 00  45.2 -46.7  3.6      95.5    30     3440   03 06 34

03 07 14  J0350+5138   07 39 11  43.7 -45.9  3.8      94.2     0     3440   03 07 14
03 07 44  ---          07 39 41  43.7 -45.9  3.8      94.1    30     3444   03 07 15

03 07 55  NRAO150      07 39 52  45.1 -46.7  3.7      95.3     0     3444   03 07 55
03 08 25  ---          07 40 22  45.0 -46.7  3.7      95.2    30     3448   03 07 56

03 08 36  J0350+5201   07 40 33  43.5 -45.4  3.8      94.4     0     3448   03 08 36
03 09 06  ---          07 41 03  43.5 -45.4  3.8      94.3    30     3452   03 08 37

03 09 16  NRAO150      07 41 14  44.9 -46.8  3.7      95.0     0     3452   03 09 16
03 09 46  ---          07 41 44  44.8 -46.8  3.7      94.9    30     3456   03 09 17

03 09 57  J0350+5138   07 41 55  43.3 -46.0  3.8      93.7     0     3456   03 09 57
03 10 27  ---          07 42 25  43.2 -46.0  3.8      93.6    30     3460   03 09 58

03 10 38  NRAO150      07 42 36  44.7 -46.8  3.7      94.7     0     3460   03 10 38
03 11 08  ---          07 43 06  44.6 -46.8  3.7      94.6    30     3464   03 10 39

03 11 19  J0350+5201   07 43 17  43.1 -45.5  3.9      93.8     0     3464   03 11 19
03 11 49  ---          07 43 47  43.1 -45.5  3.9      93.7    30     3468   03 11 20

03 12 00  NRAO150      07 43 58  44.5 -46.8  3.7      94.4     0     3468   03 12 00
03 12 30  ---          07 44 28  44.4 -46.8  3.7      94.3    30     3471   03 12 01

03 12 41  J0350+5138   07 44 39  42.9 -46.0  3.9      93.1     0     3471   03 12 41
03 13 11  ---          07 45 09  42.8 -46.0  3.9      93.0    30     3475   03 12 42

03 13 22  NRAO150      07 45 20  44.2 -46.8  3.7      94.2     0     3475   03 13 22
03 13 52  ---          07 45 50  44.2 -46.8  3.8      94.1    30     3479   03 13 23

03 14 03  J0350+5201   07 46 01  42.7 -45.5  3.9      93.2     0     3479   03 14 03
03 14 33  ---          07 46 31  42.6 -45.5  3.9      93.1    30     3483   03 14 04

03 14 44  NRAO150      07 46 42  44.0 -46.8  3.8      93.9     0     3483   03 14 44
03 15 14  ---          07 47 12  43.9 -46.9  3.8      93.8    30     3487   03 14 45

03 15 25  J0350+5138   07 47 23  42.5 -46.0  3.9      92.5     0     3487   03 15 25
03 15 55  ---          07 47 53  42.4 -46.0  3.9      92.4    30     3491   03 15 26

03 16 05  NRAO150      07 48 04  43.8 -46.9  3.8      93.6     0     3491   03 16 05
03 16 35  ---          07 48 34  43.7 -46.9  3.8      93.5    30     3495   03 16 06
Schedule for VLBA_FD   (Code Fd )                                   Page  54
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

03 16 46  J0350+5201   07 48 45  42.3 -45.5  3.9      92.7     0     3495   03 16 46
03 17 16  ---          07 49 15  42.2 -45.5  4.0      92.6    30     3498   03 16 47

03 17 27  NRAO150      07 49 26  43.6 -46.9  3.8      93.3     0     3498   03 17 27
03 17 57  ---          07 49 56  43.5 -46.9  3.8      93.2    30     3502   03 17 28

03 18 08  J0350+5138   07 50 07  42.0 -46.1  4.0      92.0     0     3502   03 18 08
03 18 38  ---          07 50 37  42.0 -46.1  4.0      91.9    30     3506   03 18 09

03 18 49  NRAO150      07 50 48  43.4 -46.9  3.8      93.0     0     3506   03 18 49
03 19 19  ---          07 51 18  43.3 -46.9  3.8      92.9    30     3510   03 18 50

03 19 30  J0350+5201   07 51 29  41.9 -45.5  4.0      92.1     0     3510   03 19 30
03 20 00  ---          07 51 59  41.8 -45.6  4.0      92.0    30     3514   03 19 31

03 20 11  NRAO150      07 52 10  43.2 -46.9  3.9      92.8     0     3514   03 20 11
03 20 41  ---          07 52 40  43.1 -46.9  3.9      92.7    30     3518   03 20 12

03 20 52  J0350+5138   07 52 51  41.6 -46.1  4.0      91.4     0     3518   03 20 52
03 21 22  ---          07 53 21  41.5 -46.1  4.0      91.3    30     3522   03 20 53

03 21 32  NRAO150      07 53 32  43.0 -46.9  3.9      92.5     0     3522   03 21 32
03 22 02  ---          07 54 02  42.9 -46.9  3.9      92.4    30     3526   03 21 33

03 22 13  J0350+5201   07 54 13  41.5 -45.6  4.0      91.6     0     3526   03 22 13
03 22 43  ---          07 54 43  41.4 -45.6  4.0      91.5    30     3529   03 22 14

03 22 54  NRAO150      07 54 54  42.7 -46.9  3.9      92.2     0     3529   03 22 54
03 23 24  ---          07 55 24  42.7 -46.9  3.9      92.1    30     3533   03 22 55

03 23 35  J0350+5138   07 55 35  41.2 -46.1  4.1      90.9     0     3533   03 23 35
03 24 05  ---          07 56 05  41.1 -46.1  4.1      90.8    30     3537   03 23 36

03 24 16  NRAO150      07 56 16  42.5 -47.0  3.9      92.0     0     3537   03 24 16
03 24 46  ---          07 56 46  42.4 -47.0  3.9      91.9    30     3541   03 24 17

03 24 57  J0350+5201   07 56 57  41.0 -45.6  4.1      91.0     0     3541   03 24 57
03 25 27  ---          07 57 27  41.0 -45.6  4.1      90.9    30     3545   03 24 58

03 25 37  NRAO150      07 57 37  42.3 -47.0  3.9      91.7     0     3545   03 25 37
03 26 07  ---          07 58 08  42.2 -47.0  4.0      91.6    30     3549   03 25 38

03 26 18  J0350+5138   07 58 18  40.8 -46.1  4.1      90.4     0     3549   03 26 18
03 26 48  ---          07 58 49  40.7 -46.1  4.1      90.3    30     3553   03 26 19
Schedule for VLBA_FD   (Code Fd )                                   Page  55
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

03 26 59  NRAO150      07 58 59  42.1 -47.0  4.0      91.4     0     3553   03 26 59
03 27 29  ---          07 59 30  42.0 -47.0  4.0      91.3    30     3556   03 27 00

03 27 40  J0350+5201   07 59 40  40.6 -45.6  4.1      90.5     0     3556   03 27 40
03 28 10  ---          08 00 10  40.5 -45.6  4.1      90.4    30     3560   03 27 41

03 28 21  NRAO150      08 00 21  41.9 -47.0  4.0      91.1     0     3560   03 28 21
03 28 51  ---          08 00 51  41.8 -47.0  4.0      91.0    30     3564   03 28 22

03 29 02  J0350+5138   08 01 02  40.4 -46.1  4.2      89.8     0     3564   03 29 02
03 29 32  ---          08 01 32  40.3 -46.1  4.2      89.7    30     3568   03 29 03

03 29 43  NRAO150      08 01 43  41.7 -47.0  4.0      90.9     0     3568   03 29 43
03 30 13  ---          08 02 13  41.6 -47.0  4.0      90.8    30     3572   03 29 44

03 30 23  J0350+5201   08 02 24  40.2 -45.6  4.2      89.9     0     3572   03 30 23
03 30 53  ---          08 02 54  40.1 -45.6  4.2      89.8    30     3576   03 30 24

03 31 04  NRAO150      08 03 05  41.5 -47.0  4.0      90.6     0     3576   03 31 04
03 31 34  ---          08 03 35  41.4 -47.0  4.0      90.5    30     3580   03 31 05

03 31 45  J0350+5138   08 03 46  39.9 -46.1  4.2      89.3     0     3580   03 31 45
03 32 15  ---          08 04 16  39.9 -46.1  4.2      89.2    30     3583   03 31 46

03 32 26  NRAO150      08 04 27  41.2 -47.0  4.1      90.3     0     3583   03 32 26
03 32 56  ---          08 04 57  41.2 -47.0  4.1      90.2    30     3587   03 32 27

03 33 07  J0350+5201   08 05 08  39.8 -45.6  4.2      89.4     0     3587   03 33 07
03 33 37  ---          08 05 38  39.7 -45.6  4.2      89.3    30     3591   03 33 08

03 33 48  NRAO150      08 05 49  41.0 -47.0  4.1      90.1     0     3591   03 33 48
03 34 18  ---          08 06 19  40.9 -47.0  4.1      90.0    30     3595   03 33 49

03 34 29  J0350+5138   08 06 30  39.5 -46.1  4.2      88.8     0     3595   03 34 29
03 34 59  ---          08 07 00  39.4 -46.1  4.3      88.7    30     3599   03 34 30

03 35 09  NRAO150      08 07 11  40.8 -47.0  4.1      89.8     0     3599   03 35 09
03 35 39  ---          08 07 41  40.7 -47.0  4.1      89.7    30     3603   03 35 10

03 35 50  J0350+5201   08 07 52  39.4 -45.6  4.3      88.9     0     3603   03 35 50
03 36 20  ---          08 08 22  39.3 -45.6  4.3      88.8    30     3607   03 35 51

03 36 31  NRAO150      08 08 33  40.6 -47.0  4.1      89.5     0     3607   03 36 31
03 37 01  ---          08 09 03  40.5 -47.0  4.1      89.4    30     3611   03 36 32
Schedule for VLBA_FD   (Code Fd )                                   Page  56
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

03 37 12  J0350+5138   08 09 14  39.1 -46.1  4.3      88.2     0     3611   03 37 12
03 37 42  ---          08 09 44  39.0 -46.1  4.3      88.1    30     3614   03 37 13

03 37 53  NRAO150      08 09 55  40.4 -47.0  4.2      89.3     0     3614   03 37 53
03 38 23  ---          08 10 25  40.3 -47.0  4.2      89.2    30     3618   03 37 54

03 38 34  J0350+5201   08 10 36  38.9 -45.6  4.3      88.3     0     3618   03 38 34
03 39 04  ---          08 11 06  38.9 -45.6  4.3      88.2    30     3622   03 38 35

03 39 15  NRAO150      08 11 17  40.2 -47.0  4.2      89.0     0     3622   03 39 15
03 39 45  ---          08 11 47  40.1 -47.0  4.2      88.9    30     3626   03 39 16

03 39 55  J0350+5138   08 11 58  38.7 -46.0  4.3      87.7     0     3626   03 39 55
03 40 25  ---          08 12 28  38.6 -46.0  4.3      87.6    30     3630   03 39 56

03 40 36  NRAO150      08 12 39  39.9 -47.0  4.2      88.8     0     3630   03 40 36
03 41 06  ---          08 13 09  39.9 -47.0  4.2      88.7    30     3634   03 40 37

03 41 17  J0350+5201   08 13 20  38.5 -45.5  4.4      87.8     0     3634   03 41 17
03 41 47  ---          08 13 50  38.4 -45.5  4.4      87.7    30     3638   03 41 18

03 41 58  NRAO150      08 14 01  39.7 -47.0  4.2      88.5     0     3638   03 41 58
03 42 28  ---          08 14 31  39.7 -47.0  4.2      88.4    30     3641   03 41 59

03 42 39  J0350+5138   08 14 42  38.2 -46.0  4.4      87.2     0     3641   03 42 39
03 43 09  ---          08 15 12  38.2 -46.0  4.4      87.1    30     3645   03 42 40

03 43 19  NRAO150      08 15 22  39.5 -47.0  4.2      88.2     0     3645   03 43 19
03 43 49  ---          08 15 53  39.4 -47.0  4.3      88.1    30     3649   03 43 20

03 44 00  J0350+5201   08 16 03  38.1 -45.5  4.4      87.3     0     3649   03 44 00
03 44 30  ---          08 16 34  38.0 -45.5  4.4      87.2    30     3653   03 44 01

03 44 41  NRAO150      08 16 44  39.3 -46.9  4.3      88.0     0     3653   03 44 41
03 45 11  ---          08 17 14  39.2 -46.9  4.3      87.9    30     3657   03 44 42

03 45 22  J0350+5138   08 17 25  37.8 -46.0  4.4      86.7     0     3657   03 45 22
03 45 52  ---          08 17 55  37.7 -46.0  4.4      86.6    30     3661   03 45 23

03 46 03  NRAO150      08 18 06  39.1 -46.9  4.3      87.7     0     3661   03 46 03
03 46 33  ---          08 18 36  39.0 -46.9  4.3      87.6    30     3665   03 46 04

03 46 43  J0350+5201   08 18 47  37.7 -45.5  4.4      86.8     0     3665   03 46 43
03 47 13  ---          08 19 17  37.6 -45.5  4.5      86.7    30     3668   03 46 44
Schedule for VLBA_FD   (Code Fd )                                   Page  57
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

03 47 24  NRAO150      08 19 28  38.9 -46.9  4.3      87.5     0     3668   03 47 24
03 47 54  ---          08 19 58  38.8 -46.9  4.3      87.4    30     3672   03 47 25

03 48 05  J0350+5138   08 20 09  37.4 -46.0  4.5      86.2     0     3672   03 48 05
03 48 35  ---          08 20 39  37.3 -45.9  4.5      86.1    30     3676   03 48 06

03 48 46  NRAO150      08 20 50  38.7 -46.9  4.3      87.2     0     3676   03 48 46
03 49 16  ---          08 21 20  38.6 -46.9  4.3      87.1    30     3680   03 48 47

03 49 27  J0350+5201   08 21 31  37.3 -45.5  4.5      86.2     0     3680   03 49 27
03 49 57  ---          08 22 01  37.2 -45.5  4.5      86.2    30     3684   03 49 28

03 50 07  NRAO150      08 22 11  38.4 -46.9  4.4      86.9     0     3684   03 50 07
03 50 37  ---          08 22 42  38.4 -46.9  4.4      86.9    30     3688   03 50 08

03 50 48  J0350+5138   08 22 52  37.0 -45.9  4.5      85.6     0     3688   03 50 48
03 51 18  ---          08 23 22  36.9 -45.9  4.5      85.5    30     3692   03 50 49

03 51 29  NRAO150      08 23 33  38.2 -46.9  4.4      86.7     0     3692   03 51 29
03 51 59  ---          08 24 03  38.2 -46.9  4.4      86.6    30     3696   03 51 30

03 52 10  J0350+5201   08 24 14  36.8 -45.4  4.5      85.7     0     3696   03 52 10
03 52 40  ---          08 24 44  36.8 -45.4  4.5      85.6    30     3699   03 52 11

03 52 50  NRAO150      08 24 55  38.0 -46.9  4.4      86.4     0     3699   03 52 50
03 53 20  ---          08 25 25  37.9 -46.9  4.4      86.3    30     3703   03 52 51

03 53 31  J0350+5138   08 25 36  36.6 -45.9  4.6      85.1     0     3703   03 53 31
03 54 01  ---          08 26 06  36.5 -45.9  4.6      85.0    30     3707   03 53 32

03 54 12  NRAO150      08 26 17  37.8 -46.9  4.4      86.2     0     3707   03 54 12
03 54 42  ---          08 26 47  37.7 -46.8  4.4      86.1    30     3711   03 54 13

03 54 53  J0350+5201   08 26 58  36.4 -45.4  4.6      85.2     0     3711   03 54 53
03 55 23  ---          08 27 28  36.3 -45.4  4.6      85.1    30     3715   03 54 54

03 55 33  NRAO150      08 27 38  37.6 -46.8  4.4      85.9     0     3715   03 55 33
03 56 03  ---          08 28 08  37.5 -46.8  4.5      85.8    30     3719   03 55 34

03 56 14  J0350+5138   08 28 19  36.1 -45.8  4.6      84.6     0     3719   03 56 14
03 56 44  ---          08 28 49  36.1 -45.8  4.6      84.5    30     3723   03 56 15

03 56 55  NRAO150      08 29 00  37.4 -46.8  4.5      85.7     0     3723   03 56 55
03 57 25  ---          08 29 30  37.3 -46.8  4.5      85.6    30     3726   03 56 56
Schedule for VLBA_FD   (Code Fd )                                   Page  58
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

03 57 35  J0350+5201   08 29 41  36.0 -45.3  4.6      84.7     0     3726   03 57 35
03 58 05  ---          08 30 11  35.9 -45.3  4.6      84.6    30     3730   03 57 36

03 58 16  NRAO150      08 30 22  37.2 -46.8  4.5      85.4     0     3730   03 58 16
03 58 46  ---          08 30 52  37.1 -46.8  4.5      85.3    30     3734   03 58 17

03 58 57  J0350+5138   08 31 02  35.7 -45.8  4.7      84.1     0     3734   03 58 57
03 59 27  ---          08 31 33  35.6 -45.8  4.7      84.0    30     3738   03 58 58

03 59 38  NRAO150      08 31 43  37.0 -46.8  4.5      85.2     0     3738   03 59 38
04 00 08  ---          08 32 13  36.9 -46.8  4.5      85.1    30     3742   03 59 39

04 00 18  J0350+5201   08 32 24  35.6 -45.3  4.7      84.2     0     3742   04 00 18
04 00 48  ---          08 32 54  35.5 -45.3  4.7      84.1    30     3746   04 00 19

04 00 59  NRAO150      08 33 05  36.7 -46.7  4.5      84.9     0     3746   04 00 59
04 01 29  ---          08 33 35  36.7 -46.7  4.5      84.8    30     3750   04 01 00

04 01 40  J0350+5138   08 33 46  35.3 -45.7  4.7      83.6     0     3750   04 01 40
04 02 10  ---          08 34 16  35.2 -45.7  4.7      83.5    30     3754   04 01 41

04 02 20  NRAO150      08 34 26  36.5 -46.7  4.6      84.7     0     3754   04 02 20
04 02 50  ---          08 34 57  36.4 -46.7  4.6      84.6    30     3757   04 02 21

04 03 01  J0350+5201   08 35 07  35.2 -45.2  4.7      83.7     0     3757   04 03 01
04 03 31  ---          08 35 37  35.1 -45.2  4.7      83.6    30     3761   04 03 02

04 03 42  NRAO150      08 35 48  36.3 -46.7  4.6      84.4     0     3761   04 03 42
04 04 12  ---          08 36 18  36.2 -46.7  4.6      84.3    30     3765   04 03 43

04 04 22  J0350+5138   08 36 29  34.9 -45.7  4.7      83.1     0     3765   04 04 22
04 04 52  ---          08 36 59  34.8 -45.6  4.8      83.0    30     3769   04 04 23

04 05 03  NRAO150      08 37 10  36.1 -46.7  4.6      84.2     0     3769   04 05 03
04 05 33  ---          08 37 40  36.0 -46.7  4.6      84.1    30     3773   04 05 04

04 05 44  J0350+5201   08 37 50  34.8 -45.2  4.8      83.2     0     3773   04 05 44
04 06 14  ---          08 38 21  34.7 -45.2  4.8      83.1    30     3777   04 05 45

04 06 24  NRAO150      08 38 31  35.9 -46.6  4.6      83.9     0     3777   04 06 24
04 06 54  ---          08 39 01  35.8 -46.6  4.6      83.8    30     3781   04 06 25

04 07 05  J0350+5138   08 39 12  34.5 -45.6  4.8      82.6     0     3781   04 07 05
04 07 35  ---          08 39 42  34.4 -45.6  4.8      82.5    30     3784   04 07 06
Schedule for VLBA_FD   (Code Fd )                                   Page  59
               43 GHz Precision Astrometry of the Jet in NRAO 150
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  14 Mar 2017   Day  73 ---

04 07 46  NRAO150      08 39 53  35.7 -46.6  4.7      83.7     0     3784   04 07 46
04 08 16  ---          08 40 23  35.6 -46.6  4.7      83.6    30     3788   04 07 47

04 08 27  J0350+5201   08 40 34  34.3 -45.1  4.8      82.7     0     3788   04 08 27
04 08 57  ---          08 41 04  34.3 -45.1  4.8      82.6    30     3792   04 08 28

04 09 07  NRAO150      08 41 14  35.5 -46.6  4.7      83.4     0     3792   04 09 07
04 09 37  ---          08 41 45  35.4 -46.6  4.7      83.3    30     3796   04 09 08

04 09 48  J0350+5138   08 41 55  34.0 -45.5  4.8      82.1     0     3796   04 09 48
04 10 18  ---          08 42 25  34.0 -45.5  4.8      82.0    30     3800   04 09 49

04 10 29  NRAO150      08 42 36  35.3 -46.6  4.7      83.2     0     3800   04 10 29
04 10 59  ---          08 43 06  35.2 -46.5  4.7      83.1    30     3804   04 10 30

04 11 09  J0350+5201   08 43 17  33.9 -45.1  4.9      82.2     0     3804   04 11 09
04 11 39  ---          08 43 47  33.9 -45.0  4.9      82.1    30     3808   04 11 10

04 11 50  NRAO150      08 43 58  35.0 -46.5  4.7      82.9     0     3808   04 11 50
04 12 20  ---          08 44 28  35.0 -46.5  4.7      82.8    30     3811   04 11 51

04 12 31  J0350+5138   08 44 39  33.6 -45.5  4.9      81.6     0     3811   04 12 31
04 13 01  ---          08 45 09  33.5 -45.4  4.9      81.5    30     3815   04 12 32

04 13 11  NRAO150      08 45 19  34.8 -46.5  4.7      82.7     0     3815   04 13 11
04 13 41  ---          08 45 49  34.7 -46.5  4.8      82.6    30     3819   04 13 12

04 13 52  J0350+5201   08 46 00  33.5 -45.0  4.9      81.7     0     3819   04 13 52
04 14 22  ---          08 46 30  33.4 -45.0  4.9      81.6    30     3823   04 13 53

04 14 33  NRAO150      08 46 41  34.6 -46.5  4.8      82.4     0     3823   04 14 33
04 15 03  ---          08 47 11  34.5 -46.4  4.8      82.4    30     3827   04 14 34

04 15 50  DA193        08 47 59  54.2 -63.2  2.9      91.2     1     3827   04 15 50
04 20 50  ---          08 52 59  53.2 -63.2  2.9      90.4   300     3866   04 15 51

04 23 48  OJ287        08 55 57  79.4 180.2  0.0       0.2    -4     3866   04 23 51
04 30 00  ---          09 02 10  79.3 188.1  0.1       7.4   368     3913   04 23 49


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess117.Q1024glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq.dat:
     v7mm_c8

   Setup group:    4         Station: VLBA_FD           Total bit rate:  1024
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   9  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43127.25  43127.25  43159.25  43159.25  43191.25  43191.25  43223.25  43223.25
   BBC fr=     727.25    727.25    759.25    759.25    791.25    791.25    823.25    823.25
   Bandwd=      32.00     32.00     32.00     32.00     32.00     32.00     32.00     32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     767.25    767.25    799.25    799.25
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   9  10  11  12  13  14  15  16  17  18

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * NRAO150           03 55 45.261371   * 03 59 29.747272     04 00 46.099621       0.00
                     50 49 20.28579    * 50 57 50.16174      51 00 42.84606        0.00
                     From catalog imbedded in main SCHED input file.

 * J0350+5138        03 46 40.589587   * 03 50 25.051489     03 51 41.359690       0.00
                     51 29 35.10800    * 51 38 38.73468      51 41 43.14411        0.00
                     From catalog imbedded in main SCHED input file.

 * J0350+5201        03 46 59.005870   * 03 50 44.499505     03 52 01.163353       0.00
                     51 52 19.27863    * 52 01 21.74506      52 04 25.85773        0.00
                     From catalog imbedded in main SCHED input file.

 * DA193             05 52 01.407172   * 05 55 30.805614     05 56 42.429612       0.00
                     39 48 21.94585    * 39 48 49.16500      39 48 53.16469        0.00
                     From catalog imbedded in main SCHED input file.

 * OJ287             08 51 57.250618   * 08 54 48.874930     08 55 48.230082       0.00
                     20 17 58.41741    * 20 06 30.64086      20 02 24.95527        0.00
                     From catalog imbedded in main SCHED input file.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  NRAO150    sess117.Q1024glob     1 4 5 6 7 8 9 19                  9.022   313.926
  J0350+5138 sess117.Q1024glob     1 4 5 6 7 8 9 19                  3.842   162.098
  J0350+5201 sess117.Q1024glob     1 4 5 6 7 8 9 19                  3.934   167.421
  DA193      sess117.Q1024glob     1 4 5 6 7 8 9 19                  1.207    59.009
  OJ287      sess117.Q1024glob     1 4 5 6 7 8 9 19                  0.784    26.707


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   NRAO150             77.5
   J0350+5138          76.5
   J0350+5201          76.6
   DA193               95.8
   OJ287              137.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

