  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Spectropolarimetric study of the jet and its termination region in 3C205
 Exp. Code:  GL046   


Schedule Version:       5.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Colin Lonsdale

Address:  MIT Haystack Observatory
          99 Millstone Rd.
          Westford, MA 01886
          USA

Phone:    +1 508 517 9106
EMAIL:    cjl@mit.edu
Fax:
Phone during observation: +1 508 517 9106

Observing mode: vlbi

Notes:    # Please, make sure PHASE CAL is OFF #
 
 
 


COVER LETTER:


{Any additional remarks you may want to write down}

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   7 Mar 2024   Day  67 ---

 Next scan frequencies:  1383.00  1383.00  1530.00  1530.00  1594.00  1594.00  1658.00  1658.00
 Next BBC frequencies:   1017.00  1017.00   870.00   870.00   806.00   806.00   742.00   742.00
 Next scan bandwidths:     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00

21 06 00  J0834+5534   01 14 30  14.4  33.2 -7.4     -56.3     0        0   21 06 00
21 09 00  =0831+557    01 17 31  14.8  33.4 -7.3     -56.8   180       46   21 06 01

21 09 30  3C205        01 18 01  15.6  31.1 -7.4     -56.7    20       46   21 09 30
21 18 30  ---          01 27 03  16.6  31.8 -7.2     -58.4   540      185   21 09 31

21 18 41  3C205        01 27 14  16.6  31.8 -7.2     -58.4     5      185   21 18 41
21 27 41  ---          01 36 15  17.7  32.5 -7.1     -60.1   540      325   21 18 42

21 27 52  3C205        01 36 26  17.7  32.5 -7.1     -60.2     5      325   21 27 52
21 29 11  ---          01 37 45  17.8  32.6 -7.1     -60.4    79      345   21 27 53

21 29 41  3C205        01 38 15  17.9  32.6 -7.0     -60.5    24      345   21 29 41
21 38 41  ---          01 47 17  19.0  33.2 -6.9     -62.2   540      484   21 29 42

21 38 52  3C205        01 47 28  19.0  33.2 -6.9     -62.3     5      484   21 38 52
21 47 52  ---          01 56 29  20.0  33.8 -6.7     -64.0   540      623   21 38 53

21 48 03  3C205        01 56 40  20.1  33.8 -6.7     -64.0     5      623   21 48 03
21 49 22  ---          01 58 00  20.2  33.9 -6.7     -64.3    79      644   21 48 04

21 50 22  J0818+4222   01 59 00  16.6  50.2 -6.3     -63.4    41      644   21 50 22
21 53 22  =0814+425    02 02 00  17.1  50.5 -6.3     -63.8   180      690   21 50 23

21 54 22  J0834+5534   02 03 00  20.4  36.7 -6.6     -65.2    42      690   21 54 22
21 57 22  =0831+557    02 06 01  20.8  36.9 -6.5     -65.8   180      736   21 54 23

21 57 52  3C205        02 06 31  21.3  34.4 -6.6     -65.9    20      736   21 57 52
22 06 52  ---          02 15 32  22.4  34.9 -6.4     -67.6   540      875   21 57 53

22 07 03  3C205        02 15 44  22.4  34.9 -6.4     -67.6     5      875   22 07 03
22 16 03  ---          02 24 45  23.5  35.4 -6.3     -69.4   540     1015   22 07 04

22 16 14  3C205        02 24 56  23.5  35.4 -6.3     -69.4     5     1015   22 16 14
22 17 33  ---          02 26 15  23.7  35.5 -6.2     -69.7    79     1035   22 16 15

22 18 03  3C205        02 26 45  23.8  35.5 -6.2     -69.8    24     1035   22 18 03
22 27 03  ---          02 35 47  24.9  35.9 -6.1     -71.5   540     1174   22 18 04

22 27 14  3C205        02 35 58  24.9  35.9 -6.1     -71.5     5     1174   22 27 14
22 36 14  ---          02 44 59  26.1  36.3 -5.9     -73.3   540     1313   22 27 15
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   7 Mar 2024   Day  67 ---

22 36 25  3C205        02 45 10  26.1  36.4 -5.9     -73.3     5     1313   22 36 25
22 37 44  ---          02 46 30  26.2  36.4 -5.9     -73.5    79     1334   22 36 26

22 38 14  3C205        02 47 00  26.3  36.4 -5.9     -73.6    24     1334   22 38 14
22 47 14  ---          02 56 01  27.5  36.8 -5.8     -75.4   540     1473   22 38 15

22 47 25  3C205        02 56 12  27.5  36.8 -5.7     -75.4     5     1473   22 47 25
22 56 25  ---          03 05 14  28.7  37.1 -5.6     -77.2   540     1612   22 47 26

22 56 36  3C205        03 05 25  28.7  37.1 -5.6     -77.2     5     1612   22 56 36
22 57 55  ---          03 06 44  28.9  37.2 -5.6     -77.5    79     1632   22 56 37

22 58 25  3C205        03 07 14  28.9  37.2 -5.6     -77.6    24     1632   22 58 25
23 07 25  ---          03 16 15  30.1  37.5 -5.4     -79.3   540     1771   22 58 26

23 07 36  3C205        03 16 26  30.1  37.5 -5.4     -79.4     5     1771   23 07 36
23 16 36  ---          03 25 28  31.3  37.7 -5.3     -81.2   540     1910   23 07 37

23 17 06  J0834+5534   03 25 58  31.6  40.5 -5.2     -80.7    20     1910   23 17 06
23 18 06  =0831+557    03 26 58  31.7  40.6 -5.2     -80.9    60     1926   23 17 07

23 18 36  3C205        03 27 28  31.6  37.8 -5.2     -81.6    20     1926   23 18 36
23 27 36  ---          03 36 30  32.8  37.9 -5.1     -83.4   540     2065   23 18 37

23 27 47  3C205        03 36 41  32.8  37.9 -5.1     -83.4     5     2065   23 27 47
23 36 47  ---          03 45 42  34.0  38.1 -4.9     -85.3   540     2204   23 27 48

23 36 58  3C205        03 45 53  34.0  38.1 -4.9     -85.3     5     2204   23 36 58
23 38 17  ---          03 47 13  34.2  38.1 -4.9     -85.6    79     2224   23 36 59

23 38 47  3C205        03 47 43  34.2  38.1 -4.9     -85.7    24     2224   23 38 47
23 47 47  ---          03 56 44  35.4  38.2 -4.7     -87.5   540     2364   23 38 48

23 47 58  3C205        03 56 55  35.5  38.2 -4.7     -87.6     5     2364   23 47 58
23 56 58  ---          04 05 57  36.7  38.2 -4.6     -89.4   540     2503   23 47 59

23 57 09  3C205        04 06 08  36.7  38.2 -4.6     -89.5     5     2503   23 57 09
23 58 28  ---          04 07 27  36.9  38.2 -4.6     -89.8    79     2523   23 57 10

 --- Start: Thu   7 Mar 2024   Day  67 -- Stop: Fri   8 Mar 2024   Day  68 ---

23 59 28  J0818+4222   04 08 27  39.3  58.3 -4.2     -81.6    38     2523   23 59 28
00 02 28  =0814+425    04 11 27  39.8  58.4 -4.1     -82.1   180     2569   23 59 29
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

00 03 28  J0834+5534   04 12 28  38.1  41.2 -4.4     -89.9    40     2569   00 03 28
00 05 28  =0831+557    04 14 28  38.4  41.2 -4.4     -90.3   120     2600   00 03 29

00 05 58  3C205        04 14 58  37.9  38.2 -4.4     -91.4    20     2600   00 05 58
00 14 58  ---          04 24 00  39.1  38.2 -4.3     -93.3   540     2739   00 05 59

00 15 09  3C205        04 24 11  39.1  38.2 -4.3     -93.4     5     2739   00 15 09
00 24 09  ---          04 33 12  40.3  38.0 -4.1     -95.3   540     2879   00 15 10

00 24 20  3C205        04 33 23  40.3  38.0 -4.1     -95.4     5     2879   00 24 20
00 25 39  ---          04 34 42  40.5  38.0 -4.1     -95.7    79     2899   00 24 21

00 26 09  3C205        04 35 12  40.6  38.0 -4.1     -95.8    24     2899   00 26 09
00 35 09  ---          04 44 14  41.8  37.8 -3.9     -97.8   540     3038   00 26 10

00 35 20  3C205        04 44 25  41.8  37.8 -3.9     -97.9     5     3038   00 35 20
00 44 20  ---          04 53 26  43.0  37.6 -3.8     -99.9   540     3177   00 35 21

00 44 31  3C205        04 53 37  43.0  37.6 -3.8    -100.0     5     3177   00 44 31
00 45 50  ---          04 54 57  43.2  37.5 -3.8    -100.3    79     3198   00 44 32

00 46 20  3C205        04 55 27  43.2  37.5 -3.8    -100.4    24     3198   00 46 20
00 55 20  ---          05 04 28  44.4  37.2 -3.6    -102.5   540     3337   00 46 21

00 55 31  3C205        05 04 39  44.4  37.2 -3.6    -102.6     5     3337   00 55 31
01 04 31  ---          05 13 41  45.6  36.8 -3.5    -104.8   540     3476   00 55 32

01 04 42  3C205        05 13 52  45.6  36.8 -3.5    -104.8     5     3476   01 04 42
01 06 01  ---          05 15 11  45.8  36.7 -3.4    -105.2    79     3496   01 04 43

01 06 31  3C205        05 15 41  45.9  36.7 -3.4    -105.3    24     3496   01 06 31
01 15 31  ---          05 24 42  47.0  36.2 -3.3    -107.5   540     3635   01 06 32

01 15 42  3C205        05 24 54  47.0  36.2 -3.3    -107.6     5     3635   01 15 42
01 24 42  ---          05 33 55  48.2  35.6 -3.1    -109.9   540     3774   01 15 43

01 25 12  J0834+5534   05 34 25  49.6  38.6 -3.0    -108.6    19     3774   01 25 12
01 26 12  =0831+557    05 35 25  49.7  38.5 -3.0    -108.9    60     3790   01 25 13

01 26 42  3C205        05 35 55  48.4  35.4 -3.1    -110.5    19     3790   01 26 42
01 35 42  ---          05 44 57  49.5  34.8 -2.9    -112.9   540     3929   01 26 43

01 35 53  3C205        05 45 08  49.6  34.8 -2.9    -112.9     5     3929   01 35 53
01 44 53  ---          05 54 09  50.7  34.0 -2.8    -115.4   540     4068   01 35 54
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

01 45 04  3C205        05 54 20  50.7  34.0 -2.8    -115.5     5     4068   01 45 04
01 46 23  ---          05 55 40  50.8  33.9 -2.8    -115.8    79     4088   01 45 05

01 46 53  3C205        05 56 10  50.9  33.8 -2.7    -116.0    24     4088   01 46 53
01 55 53  ---          06 05 11  52.0  32.9 -2.6    -118.6   540     4228   01 46 54

01 56 04  3C205        06 05 22  52.0  32.9 -2.6    -118.6     5     4228   01 56 04
02 05 04  ---          06 14 24  53.0  31.9 -2.4    -121.3   540     4367   01 56 05

02 05 15  3C205        06 14 35  53.0  31.9 -2.4    -121.4     5     4367   02 05 15
02 06 34  ---          06 15 54  53.2  31.7 -2.4    -121.8    79     4387   02 05 16

02 13 34  J0818+4222   06 22 55  63.9  55.3 -2.0    -107.0   393     4387   02 13 34
02 16 34  =0814+425    06 25 56  64.4  54.9 -1.9    -107.8   180     4433   02 13 35

02 17 04  J0834+5534   06 26 26  56.2  33.2 -2.2    -123.7     6     4433   02 17 04
02 19 04  =0831+557    06 28 26  56.4  32.9 -2.1    -124.3   120     4464   02 17 05

02 19 34  3C205        06 28 56  54.6  30.1 -2.2    -125.9    18     4464   02 19 34
02 28 34  ---          06 37 57  55.6  28.8 -2.1    -128.8   540     4603   02 19 35

02 28 45  3C205        06 38 09  55.6  28.8 -2.0    -128.9     5     4603   02 28 45
02 37 45  ---          06 47 10  56.5  27.4 -1.9    -132.0   540     4743   02 28 46

02 37 56  3C205        06 47 21  56.5  27.4 -1.9    -132.0     5     4743   02 37 56
02 39 15  ---          06 48 40  56.7  27.2 -1.9    -132.5    79     4763   02 37 57

02 39 45  3C205        06 49 10  56.7  27.1 -1.9    -132.7    24     4763   02 39 45
02 48 45  ---          06 58 12  57.6  25.5 -1.7    -135.9   540     4902   02 39 46

02 48 56  3C205        06 58 23  57.6  25.5 -1.7    -135.9     5     4902   02 48 56
02 57 56  ---          07 07 24  58.4  23.8 -1.6    -139.3   540     5041   02 48 57

02 58 07  3C205        07 07 35  58.4  23.8 -1.6    -139.3     5     5041   02 58 07
02 59 26  ---          07 08 55  58.5  23.5 -1.5    -139.8    79     5062   02 58 08

02 59 56  3C205        07 09 25  58.6  23.4 -1.5    -140.0    24     5062   02 59 56
03 08 56  ---          07 18 26  59.3  21.6 -1.4    -143.5   540     5201   02 59 57

03 09 07  3C205        07 18 37  59.3  21.6 -1.4    -143.6     5     5201   03 09 07
03 18 07  ---          07 27 39  60.0  19.6 -1.2    -147.2   540     5340   03 09 08

03 18 18  3C205        07 27 50  60.0  19.6 -1.2    -147.2     5     5340   03 18 18
03 19 37  ---          07 29 09  60.1  19.3 -1.2    -147.8    79     5360   03 18 19
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

03 20 07  3C205        07 29 39  60.2  19.2 -1.2    -148.0    24     5360   03 20 07
03 29 07  ---          07 38 40  60.8  17.0 -1.0    -151.7   540     5499   03 20 08

03 29 18  3C205        07 38 51  60.8  17.0 -1.0    -151.8     5     5499   03 29 18
03 38 18  ---          07 47 53  61.3  14.8 -0.9    -155.7   540     5638   03 29 19

03 38 48  J0834+5534   07 48 23  63.7  15.6 -0.8    -156.0    17     5638   03 38 48
03 39 48  =0831+557    07 49 23  63.8  15.3 -0.8    -156.4    60     5654   03 38 49

03 40 18  3C205        07 49 53  61.4  14.3 -0.9    -156.5    17     5654   03 40 18
03 49 18  ---          07 58 55  61.9  11.9 -0.7    -160.5   540     5793   03 40 19

03 49 29  3C205        07 59 06  61.9  11.9 -0.7    -160.6     5     5793   03 49 29
03 58 29  ---          08 08 07  62.2   9.4 -0.5    -164.7   540     5932   03 49 30

03 58 40  3C205        08 08 18  62.2   9.4 -0.5    -164.8     5     5932   03 58 40
03 59 59  ---          08 09 38  62.3   9.0 -0.5    -165.4    79     5952   03 58 41

04 00 29  3C205        08 10 08  62.3   8.9 -0.5    -165.6    24     5952   04 00 29
04 09 29  ---          08 19 09  62.6   6.3 -0.4    -169.7   540     6092   04 00 30

04 09 40  3C205        08 19 20  62.6   6.3 -0.4    -169.8     5     6092   04 09 40
04 18 40  ---          08 28 22  62.7   3.7 -0.2    -174.0   540     6231   04 09 41

04 18 51  3C205        08 28 33  62.7   3.6 -0.2    -174.1     5     6231   04 18 51
04 20 10  ---          08 29 52  62.7   3.2 -0.2    -174.7    79     6251   04 18 52

04 22 10  J0818+4222   08 31 52  78.1 -10.8  0.2     167.5    82     6251   04 22 10
04 25 10  =0814+425    08 34 53  78.0 -13.4  0.2     164.4   180     6297   04 22 11

04 25 40  J0834+5534   08 35 23  65.1   0.5 -0.0    -179.3    -3     6297   04 25 43
04 27 40  =0831+557    08 37 23  65.1  -0.2  0.0     179.7   117     6328   04 25 41

04 28 10  3C205        08 37 53  62.8   0.9 -0.1    -178.5    17     6328   04 28 10
04 37 10  ---          08 46 55  62.8  -1.7  0.1     177.2   540     6467   04 28 11

04 37 21  3C205        08 47 06  62.8  -1.8  0.1     177.2     5     6467   04 37 21
04 46 21  ---          08 56 07  62.7  -4.4  0.3     172.9   540     6606   04 37 22

04 46 32  3C205        08 56 18  62.7  -4.4  0.3     172.8     5     6606   04 46 32
04 47 51  ---          08 57 37  62.7  -4.8  0.3     172.2    79     6626   04 46 33

04 48 21  3C205        08 58 07  62.7  -5.0  0.3     172.0    24     6626   04 48 21
04 57 21  ---          09 07 09  62.4  -7.5  0.4     167.8   540     6765   04 48 22
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

04 57 32  3C205        09 07 20  62.4  -7.6  0.4     167.7     5     6765   04 57 32
05 06 32  ---          09 16 21  62.1 -10.1  0.6     163.6   540     6904   04 57 33

05 06 43  3C205        09 16 32  62.1 -10.1  0.6     163.5     5     6904   05 06 43
05 08 02  ---          09 17 52  62.1 -10.5  0.6     162.9    79     6925   05 06 44

05 08 32  3C205        09 18 22  62.1 -10.6  0.6     162.7    24     6925   05 08 32
05 17 32  ---          09 27 23  61.7 -13.0  0.8     158.6   540     7064   05 08 33

05 17 43  3C205        09 27 34  61.7 -13.1  0.8     158.6     5     7064   05 17 43
05 26 43  ---          09 36 36  61.2 -15.4  0.9     154.6   540     7203   05 17 44

05 26 54  3C205        09 36 47  61.2 -15.4  0.9     154.6     5     7203   05 26 54
05 28 13  ---          09 38 06  61.1 -15.8  1.0     154.0    79     7223   05 26 55

05 28 43  3C205        09 38 36  61.1 -15.9  1.0     153.8    24     7223   05 28 43
05 37 43  ---          09 47 38  60.5 -18.0  1.1     150.0   540     7363   05 28 44

05 37 54  3C205        09 47 49  60.5 -18.1  1.1     149.9     5     7363   05 37 54
05 46 54  ---          09 56 50  59.8 -20.1  1.3     146.2   540     7502   05 37 55

05 47 24  J0834+5534   09 57 20  61.4 -24.0  1.3     141.8    19     7502   05 47 24
05 48 24  =0831+557    09 58 20  61.3 -24.2  1.4     141.4    60     7517   05 47 25

05 48 54  3C205        09 58 50  59.7 -20.6  1.3     145.4    19     7517   05 48 54
05 57 54  ---          10 07 52  59.0 -22.5  1.4     141.9   540     7656   05 48 55

05 58 05  3C205        10 08 03  59.0 -22.5  1.5     141.8     5     7656   05 58 05
06 07 05  ---          10 17 04  58.2 -24.3  1.6     138.4   540     7795   05 58 06

06 07 16  3C205        10 17 15  58.2 -24.3  1.6     138.3     5     7795   06 07 16
06 08 35  ---          10 18 35  58.1 -24.6  1.6     137.8    79     7816   06 07 17

06 09 05  3C205        10 19 05  58.0 -24.7  1.6     137.6    24     7816   06 09 05
06 18 05  ---          10 28 06  57.2 -26.3  1.8     134.4   540     7955   06 09 06

06 18 16  3C205        10 28 17  57.2 -26.3  1.8     134.3     5     7955   06 18 16
06 27 16  ---          10 37 19  56.3 -27.8  1.9     131.1   540     8094   06 18 17

06 27 27  3C205        10 37 30  56.3 -27.8  1.9     131.1     5     8094   06 27 27
06 28 46  ---          10 38 49  56.1 -28.0  2.0     130.6    79     8114   06 27 28

06 29 46  J0818+4222   10 39 49  59.8 -57.5  2.3     101.2    31     8114   06 29 46
06 32 46  =0814+425    10 42 50  59.3 -57.7  2.4     100.5   180     8161   06 29 47
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

06 33 16  J0834+5534   10 43 20  56.6 -32.7  2.1     124.9     4     8161   06 33 16
06 35 16  =0831+557    10 45 20  56.4 -33.0  2.1     124.3   120     8192   06 33 17

06 35 46  3C205        10 45 50  55.4 -29.1  2.1     128.3    19     8192   06 35 46
06 44 46  ---          10 54 52  54.4 -30.3  2.2     125.3   540     8331   06 35 47

06 44 57  3C205        10 55 03  54.4 -30.4  2.2     125.3     5     8331   06 44 57
06 53 57  ---          11 04 04  53.4 -31.5  2.4     122.4   540     8470   06 44 58

06 54 08  3C205        11 04 15  53.4 -31.5  2.4     122.4     5     8470   06 54 08
06 55 27  ---          11 05 34  53.3 -31.7  2.4     122.0    79     8490   06 54 09

06 55 57  3C205        11 06 04  53.2 -31.7  2.4     121.8    24     8490   06 55 57
07 04 57  ---          11 15 06  52.2 -32.7  2.6     119.1   540     8629   06 55 58

07 05 08  3C205        11 15 17  52.1 -32.8  2.6     119.1     5     8629   07 05 08
07 14 08  ---          11 24 18  51.1 -33.7  2.7     116.4   540     8768   07 05 09

07 14 19  3C205        11 24 29  51.1 -33.7  2.7     116.4     5     8768   07 14 19
07 15 38  ---          11 25 49  50.9 -33.8  2.7     116.0    79     8789   07 14 20

07 16 08  3C205        11 26 19  50.8 -33.8  2.8     115.9    24     8789   07 16 08
07 25 08  ---          11 35 20  49.8 -34.6  2.9     113.4   540     8928   07 16 09

07 25 19  3C205        11 35 31  49.7 -34.6  2.9     113.3     5     8928   07 25 19
07 34 19  ---          11 44 33  48.6 -35.3  3.1     110.9   540     9067   07 25 20

07 34 30  3C205        11 44 44  48.6 -35.3  3.1     110.8     5     9067   07 34 30
07 35 49  ---          11 46 03  48.4 -35.4  3.1     110.5    79     9087   07 34 31

07 37 49  3C286        11 48 03  67.6  83.9 -1.7     -82.7    27     9087   07 37 49
07 41 49  ---          11 52 04  68.5  84.2 -1.7     -82.9   240     9149   07 37 50

07 43 49  J0818+4222   11 54 04  46.2 -59.2  3.6      87.3    10     9149   07 43 49
07 46 49  =0814+425    11 57 05  45.6 -59.1  3.6      86.8   180     9196   07 43 50

07 47 19  J0834+5534   11 57 35  47.1 -39.7  3.3     104.0     8     9196   07 47 19
07 48 49  =0831+557    11 59 05  46.8 -39.8  3.4     103.7    90     9219   07 47 20

07 49 19  3C205        11 59 35  46.7 -36.3  3.3     107.0    20     9219   07 49 19
07 58 19  ---          12 08 37  45.6 -36.8  3.5     104.7   540     9358   07 49 20

07 58 30  3C205        12 08 48  45.5 -36.8  3.5     104.7     5     9358   07 58 30
08 07 30  ---          12 17 49  44.4 -37.2  3.6     102.5   540     9497   07 58 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

08 07 41  3C205        12 18 00  44.4 -37.2  3.6     102.5     5     9497   08 07 41
08 09 00  ---          12 19 19  44.2 -37.2  3.6     102.1    79     9517   08 07 42

08 09 30  3C205        12 19 49  44.1 -37.3  3.6     102.0    24     9517   08 09 30
08 18 30  ---          12 28 51  42.9 -37.6  3.8      99.9   540     9657   08 09 31

08 18 41  3C205        12 29 02  42.9 -37.6  3.8      99.8     5     9657   08 18 41
08 27 41  ---          12 38 03  41.7 -37.8  4.0      97.8   540     9796   08 18 42

08 27 52  3C205        12 38 15  41.7 -37.8  4.0      97.7     5     9796   08 27 52
08 29 11  ---          12 39 34  41.5 -37.9  4.0      97.4    79     9816   08 27 53

08 29 41  3C205        12 40 04  41.5 -37.9  4.0      97.3    24     9816   08 29 41
08 38 41  ---          12 49 05  40.3 -38.0  4.1      95.3   540     9955   08 29 42

08 38 52  3C205        12 49 16  40.2 -38.1  4.1      95.3     5     9955   08 38 52
08 47 52  ---          12 58 18  39.0 -38.2  4.3      93.3   540    10094   08 38 53

08 48 03  3C205        12 58 29  39.0 -38.2  4.3      93.2     5    10094   08 48 03
08 49 22  ---          12 59 48  38.8 -38.2  4.3      92.9    79    10115   08 48 04

08 49 52  3C205        13 00 18  38.8 -38.2  4.3      92.8    24    10115   08 49 52
08 58 52  ---          13 09 20  37.6 -38.2  4.5      90.9   540    10254   08 49 53

08 59 03  3C205        13 09 31  37.6 -38.2  4.5      90.9     5    10254   08 59 03
09 08 03  ---          13 18 32  36.3 -38.2  4.6      88.9   540    10393   08 59 04

09 08 33  J0834+5534   13 19 02  35.6 -41.1  4.7      86.3    20    10393   09 08 33
09 09 33  =0831+557    13 20 02  35.5 -41.1  4.7      86.1    60    10408   09 08 34

09 10 03  3C205        13 20 32  36.1 -38.2  4.7      88.5    20    10408   09 10 03
09 19 03  ---          13 29 34  34.9 -38.2  4.8      86.7   540    10547   09 10 04

09 19 14  3C205        13 29 45  34.9 -38.2  4.8      86.6     5    10547   09 19 14
09 28 14  ---          13 38 46  33.7 -38.1  5.0      84.8   540    10687   09 19 15

09 28 25  3C205        13 38 57  33.6 -38.0  5.0      84.7     5    10687   09 28 25
09 29 44  ---          13 40 17  33.5 -38.0  5.0      84.5    79    10707   09 28 26

09 30 14  3C205        13 40 47  33.4 -38.0  5.0      84.4    24    10707   09 30 14
09 39 14  ---          13 49 48  32.2 -37.9  5.1      82.5   540    10846   09 30 15

09 39 25  3C205        13 49 59  32.2 -37.9  5.1      82.5     5    10846   09 39 25
09 47 45  ---          13 58 21  31.1 -37.7  5.3      80.8   500    10975   09 39 26
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

09 47 56  3C205        13 58 32  31.1 -37.7  5.3      80.8     5    10975   09 47 56
09 49 15  ---          13 59 51  30.9 -37.6  5.3      80.5    79    10995   09 47 57

09 49 45  3C205        14 00 21  30.8 -37.6  5.3      80.4    24    10995   09 49 45
09 58 45  ---          14 09 22  29.6 -37.4  5.5      78.6   540    11134   09 49 46

09 58 56  3C205        14 09 33  29.6 -37.4  5.5      78.6     5    11134   09 58 56
10 07 56  ---          14 18 35  28.4 -37.1  5.6      76.8   540    11273   09 58 57

10 08 26  J0834+5534   14 19 05  27.2 -39.4  5.7      74.7    20    11273   10 08 26
10 09 26  =0831+557    14 20 05  27.1 -39.4  5.7      74.6    60    11289   10 08 27

10 09 56  3C205        14 20 35  28.2 -37.0  5.7      76.5    20    11289   10 09 56
10 18 56  ---          14 29 37  27.0 -36.7  5.8      74.7   540    11428   10 09 57

10 19 07  3C205        14 29 48  27.0 -36.6  5.8      74.7     5    11428   10 19 07
10 28 07  ---          14 38 49  25.8 -36.3  6.0      72.9   540    11567   10 19 08

10 28 18  3C205        14 39 00  25.8 -36.3  6.0      72.9     5    11567   10 28 18
10 29 37  ---          14 40 20  25.6 -36.2  6.0      72.6    79    11588   10 28 19

10 30 07  3C205        14 40 50  25.6 -36.2  6.0      72.5    24    11588   10 30 07
10 39 07  ---          14 49 51  24.4 -35.8  6.1      70.8   540    11727   10 30 08

10 39 18  3C205        14 50 02  24.4 -35.8  6.1      70.8     5    11727   10 39 18
10 47 38  ---          14 58 23  23.4 -35.3  6.3      69.2   500    11855   10 39 19

10 47 49  3C205        14 58 35  23.3 -35.3  6.3      69.1     5    11855   10 47 49
10 49 08  ---          14 59 54  23.2 -35.3  6.3      68.9    79    11876   10 47 50

10 50 08  J0818+4222   15 00 54  13.3 -48.4  6.7      60.5    33    11876   10 50 08
10 53 08  =0814+425    15 03 54  12.8 -48.1  6.7      60.0   180    11922   10 50 09

10 53 38  J0834+5534   15 04 24  21.2 -37.1  6.5      66.4     5    11922   10 53 38
10 55 08  =0831+557    15 05 55  21.0 -37.0  6.5      66.1    90    11945   10 53 39

10 55 38  3C205        15 06 25  22.4 -34.9  6.4      67.6    19    11945   10 55 38
11 04 38  ---          15 15 26  21.3 -34.4  6.6      65.9   540    12085   10 55 39

11 04 49  3C205        15 15 37  21.2 -34.4  6.6      65.9     5    12085   11 04 49
11 13 49  ---          15 24 39  20.2 -33.9  6.7      64.2   540    12224   11 04 50

11 14 00  3C205        15 24 50  20.1 -33.8  6.7      64.1     5    12224   11 14 00
11 15 19  ---          15 26 09  20.0 -33.8  6.8      63.9    79    12244   11 14 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Spectropolarimetric study of the jet and its termination region in 3C205
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Mar 2024   Day  68 ---

11 15 49  3C205        15 26 39  19.9 -33.7  6.8      63.8    24    12244   11 15 49
11 24 49  ---          15 35 41  18.8 -33.1  6.9      62.1   540    12383   11 15 50

11 25 00  3C205        15 35 52  18.8 -33.1  6.9      62.0     5    12383   11 25 00
11 34 00  ---          15 44 53  17.8 -32.5  7.1      60.3   540    12522   11 25 01

11 34 11  3C205        15 45 04  17.8 -32.5  7.1      60.3     5    12522   11 34 11
11 35 30  ---          15 46 23  17.6 -32.4  7.1      60.0    79    12543   11 34 12

11 36 00  3C205        15 46 53  17.5 -32.4  7.1      59.9    24    12543   11 36 00
11 45 00  ---          15 55 55  16.5 -31.7  7.2      58.2   540    12682   11 36 01

11 45 11  3C205        15 56 06  16.5 -31.7  7.3      58.2     5    12682   11 45 11
11 53 31  ---          16 04 27  15.6 -31.1  7.4      56.6   500    12811   11 45 12

11 53 42  3C205        16 04 38  15.5 -31.1  7.4      56.5     5    12811   11 53 42
11 55 01  ---          16 05 58  15.4 -31.0  7.4      56.3    79    12831   11 53 43

11 55 31  3C205        16 06 28  15.3 -31.0  7.4      56.2    24    12831   11 55 31
12 04 31  ---          16 15 29  14.3 -30.2  7.6      54.5   540    12970   11 55 32

12 04 42  3C205        16 15 40  14.3 -30.2  7.6      54.4     5    12970   12 04 42
12 13 42  ---          16 24 42  13.4 -29.5  7.7      52.7   540    13109   12 04 43

12 14 12  J0834+5534   16 25 12  11.4 -31.0  7.8      51.4    18    13109   12 14 12
12 15 12  =0831+557    16 26 12  11.3 -30.9  7.8      51.2    60    13125   12 14 13

12 15 42  3C205        16 26 42  13.1 -29.3  7.8      52.3    18    13125   12 15 42
12 24 42  ---          16 35 43  12.2 -28.6  7.9      50.6   540    13264   12 15 43

12 24 53  3C205        16 35 54  12.2 -28.5  7.9      50.5     5    13264   12 24 53
12 26 12  ---          16 37 14  12.1 -28.4  7.9      50.3    79    13284   12 24 54

12 26 42  3C205        16 37 44  12.0 -28.4  7.9      50.2    24    13284   12 26 42
12 35 42  ---          16 46 45  11.1 -27.6  8.1      48.4   540    13423   12 26 43

12 35 53  3C205        16 46 56  11.1 -27.6  8.1      48.4     5    13423   12 35 53
12 44 53  ---          16 55 58  10.2 -26.7  8.2      46.6   540    13562   12 35 54

12 45 04  3C205        16 56 09  10.2 -26.7  8.3      46.6     5    13562   12 45 04
12 54 04  ---          17 05 10   9.3 -25.9  8.4      44.8   540    13701   12 45 05

12 56 00  3C286        17 07 07  44.2 -75.9  3.6      75.3    39    13701   12 56 00
13 00 00  ---          17 11 07  43.4 -75.6  3.6      75.0   240    13763   12 56 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess124.HL2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v20cm_2         FD filtered above 1760.  SC filtered above 1740.

   Setup group:    3         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  14.6      2.4     14.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  12  Setup file default.  Used with PCAL = off
   LO sum=   1383.00  1383.00  1530.00  1530.00  1594.00  1594.00  1658.00  1658.00
   BBC fr=   1017.00  1017.00   870.00   870.00   806.00   806.00   742.00   742.00
   Bandwd=     64.00    64.00    64.00    64.00    64.00    64.00    64.00    64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     846.00    846.00    782.00    782.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  12  13  14  15  16  17  18  19  20  21

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 3C205             08 35 09.955441   * 08 39 06.411500     08 41 02.339846       0.00
                     58 04 47.47266    * 57 54 13.10500      57 49 14.70621        0.00
                     From catalog imbedded in main SCHED input file.

   0814+425          08 14 51.669851   * 08 18 15.999611     08 19 55.826058       0.01
 * J0818+4222        42 32 07.73243    * 42 22 45.41493      42 18 19.97743        0.01
   J0818+42          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  13655 observations.

   0831+557          08 31 04.379584   * 08 34 54.903976     08 36 47.843879       0.19
 * J0834+5534        55 44 41.32199    * 55 34 21.07033      55 29 29.35118        0.09
   J0834+55          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,    621 observations.

 * 3C286             13 28 49.657769   * 13 31 08.288061     13 32 16.524378       0.17
   J1331+3030        30 45 58.64066    * 30 30 32.95930      30 22 51.78002        0.16
   1328+307          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J1331+30          GSFC 2016a X/S astro solution,    269 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  3C205      sess124.HL2048glob    1 2 3 4 5 6 7 8 9 10 11 12       13.957  2429.464
  J0818+4222 sess124.HL2048glob    1 2 3 4 5 6 7 8 9 10 11 12        0.350    36.542
  J0834+5534 sess124.HL2048glob    1 2 3 4 5 6 7 8 9 10 11 12        1.000    61.326
  3C286      sess124.HL2048glob    1 2 3 4 5 6 7 8 9 10 11 12        0.378    16.746


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   3C205              118.9
   J0818+4222         125.8
   J0834+5534         120.0
   3C286              139.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

