  COVER INFORMATION 
 
 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Proper motions of H2O masers in IRAS 20126+4104
 Exp. Code:  GM043A  

 
Schedule Version:       1.00                                              
Processed by SCHED version: Release of 28 April 2000                      
 
PI:       Luca Moscadelli                                                 
 
Address:  Stazione Astronomica di Cagliari                                
          Loc. Poggio dei Pini, strada 54                                 
          09012 - Capoterra (CA)                                          
          Italy                                                           
 
Phone:    +39 070 71180235                                                
EMAIL:    mosca@ca.astro.it (internet)                                    
Fax:      +39 070 71180222                                                
Phone during observation:                                                 
 
Observing mode: VLBA 128-2-2                                              
 
Notes:    This is a PHASE REF experiment, DO NOT INTERRUPT the SEQUENCE   
          SPECTRAL LINE observations: Make sure *** PHASE CAL is OFF***   
          Please make TSYS measurements whenever there is a gap           
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
 Next scan frequencies: 22227.48 22227.48
 Next BBC frequencies:    727.48   727.48
 Next scan bandwidths:     16.00    16.00
  
18 06 05  2002+472     14 27 11  26.0  48.4 -5.6     -72.1     0   1  1      0  18 06 05
18 09 05  ---          14 30 11  26.5  48.6 -5.5     -72.6   180   F  1   2400
  
18 10 05  2007+402     14 31 11  23.4  55.5 -5.6     -68.9    52   1  1   2400  18 09 48
18 10 40  ---          14 31 47  23.5  55.6 -5.6     -69.0    35   F  1   3093
  
18 10 40  IRAS2012     14 31 47  22.6  54.3 -5.7     -68.4    -4   1  1   3093  18 10 40
18 11 20  ---          14 32 27  22.7  54.4 -5.7     -68.5    36   F  1   3627
  
18 11 20  2007+402     14 32 27  23.7  55.6 -5.6     -69.1    -4   1  1   3627  18 11 20
18 11 50  ---          14 32 57  23.7  55.7 -5.6     -69.1    26   F  1   4027
  
18 11 50  IRAS2012     14 32 57  22.8  54.4 -5.7     -68.5    -4   1  1   4027  18 11 50
18 12 30  ---          14 33 37  22.9  54.5 -5.7     -68.6    36   F  1   4560
  
18 12 30  2007+402     14 33 37  23.9  55.7 -5.6     -69.2    -4   1  1   4560  18 12 30
18 13 00  ---          14 34 07  24.0  55.7 -5.6     -69.3    26   F  1   4960
  
18 13 00  IRAS2012     14 34 07  23.0  54.5 -5.7     -68.7    -4   1  1   4960  18 13 00
18 13 40  ---          14 34 47  23.2  54.6 -5.7     -68.8    36   F  1   5493
  
18 13 40  2007+402     14 34 47  24.1  55.8 -5.5     -69.4    -4   1  1   5493  18 13 40
18 14 10  ---          14 35 17  24.2  55.8 -5.5     -69.4    26   F  1   5893
  
18 14 10  IRAS2012     14 35 17  23.2  54.6 -5.7     -68.8    -4   1  1   5893  18 14 10
18 14 50  ---          14 35 57  23.4  54.6 -5.6     -68.9    36   F  1   6427
  
18 14 50  2007+402     14 35 57  24.3  55.9 -5.5     -69.5    -4   1  1   6427  18 14 50
18 15 20  ---          14 36 27  24.4  55.9 -5.5     -69.6    26   F  1   6827
  
18 15 20  IRAS2012     14 36 27  23.4  54.7 -5.6     -69.0    -4   1  1   6827  18 15 20
18 16 00  ---          14 37 07  23.6  54.7 -5.6     -69.1    36   F  1   7360
  
18 16 00  2007+402     14 37 07  24.5  56.0 -5.5     -69.7    -4   1  1   7360  18 16 00
18 16 30  ---          14 37 37  24.6  56.0 -5.5     -69.7    26   F  1   7760
  
18 16 30  IRAS2012     14 37 37  23.7  54.8 -5.6     -69.2    -4   1  1   7760  18 16 30
18 17 10  ---          14 38 18  23.8  54.8 -5.6     -69.2    36   F  1   8293
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
18 17 10  2007+402     14 38 18  24.7  56.0 -5.5     -69.8    -4   1  1   8293  18 17 10
18 17 40  ---          14 38 48  24.8  56.1 -5.5     -69.9    26   F  1   8693
  
18 18 40  IRAS2012     14 39 48  24.0  54.9 -5.6     -69.4    56   1  1   8693  18 18 22
18 19 25  ---          14 40 33  24.2  55.0 -5.6     -69.6    45   F  1   9533
  
18 20 25  2007+402     14 41 33  25.3  56.3 -5.4     -70.3    56   1  1   9533  18 20 07
18 21 00  ---          14 42 08  25.4  56.3 -5.4     -70.3    35   F  1  10240
  
18 21 00  IRAS2012     14 42 08  24.4  55.1 -5.5     -69.8    -4   1  1  10240  18 21 00
18 21 40  ---          14 42 48  24.6  55.1 -5.5     -69.9    36   F  1  10773
  
18 21 40  2007+402     14 42 48  25.5  56.4 -5.4     -70.4    -4   1  1  10773  18 21 40
18 22 10  ---          14 43 18  25.6  56.4 -5.4     -70.5    26   F  1  11173
  
18 22 10  IRAS2012     14 43 18  24.7  55.2 -5.5     -69.9    -4   1  1  11173  18 22 10
18 22 50  ---          14 43 59  24.8  55.2 -5.5     -70.0    36   F  1  11707
  
18 22 50  2007+402     14 43 59  25.7  56.5 -5.4     -70.6    -4   1  1  11707  18 22 50
18 23 20  ---          14 44 29  25.8  56.5 -5.4     -70.6    26   F  1  12107
  
18 23 20  IRAS2012     14 44 29  24.9  55.3 -5.5     -70.1    -4   1  1  12107  18 23 20
18 24 00  ---          14 45 09  25.0  55.3 -5.5     -70.2    36   F  1  12640
  
18 24 00  2007+402     14 45 09  25.9  56.5 -5.4     -70.7    -4   1  1  12640  18 24 00
18 24 30  ---          14 45 39  26.0  56.6 -5.4     -70.8    26   F  1  13040
  
18 24 30  IRAS2012     14 45 39  25.1  55.3 -5.5     -70.2    -4   1  1  13040  18 24 30
18 25 10  ---          14 46 19  25.2  55.4 -5.5     -70.3    36   F  1  13573
  
18 25 10  2007+402     14 46 19  26.1  56.6 -5.4     -70.9    -4   1  1  13573  18 25 10
18 25 40  ---          14 46 49  26.2  56.7 -5.3     -71.0    26   F  1  13973
  
18 25 40  IRAS2012     14 46 49  25.3  55.4 -5.5     -70.4    -4   1  1  13973  18 25 40
18 26 20  ---          14 47 29  25.4  55.5 -5.4     -70.5    36   F  1  14507
  
18 26 20  2007+402     14 47 29  26.3  56.7 -5.3     -71.0    -4   1  1  14507  18 26 20
18 26 50  ---          14 47 59  26.4  56.7 -5.3     -71.1    26   F  1  14907
  
18 26 50  IRAS2012     14 47 59  25.5  55.5 -5.4     -70.6    -4   1  1  14907  18 26 50
18 27 30  ---          14 48 39  25.6  55.6 -5.4     -70.6    36   F  1  15440
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
18 27 30  2007+402     14 48 39  26.6  56.8 -5.3     -71.2    -4   1  1  15440  18 27 30
18 28 00  ---          14 49 09  26.6  56.8 -5.3     -71.3    26   F  1  15840
  
18 28 00  IRAS2012     14 49 09  25.7  55.6 -5.4     -70.7    -4   1  1  15840  18 28 00
18 28 40  ---          14 49 49  25.8  55.6 -5.4     -70.8    36   F  1  16373
  
18 28 40  2007+402     14 49 49  26.8  56.9 -5.3     -71.4    -4   1  1  16373  18 28 40
18 29 10  ---          14 50 20  26.9  56.9 -5.3     -71.4    26   F  1  16773
  
18 30 10  IRAS2012     14 51 20  26.1  55.7 -5.4     -71.0    56   1  1  16773  18 29 53
18 30 55  ---          14 52 05  26.2  55.8 -5.4     -71.1    45   F  1  17600
  
18 31 55  2007+402     14 53 05  27.4  57.1 -5.2     -71.8    56   1  2  17600  18 31 55
18 32 40  ---          14 53 50  27.5  57.1 -5.2     -71.9    45   R  1  17000
  
18 32 40  IRAS2012     14 53 50  26.5  55.9 -5.3     -71.3    -4   1  2  17000  18 32 40
18 33 20  ---          14 54 30  26.6  55.9 -5.3     -71.4    36   R  1  16467
  
18 33 20  2007+402     14 54 30  27.6  57.2 -5.2     -72.0    -4   1  2  16467  18 33 20
18 33 50  ---          14 55 00  27.7  57.2 -5.2     -72.0    26   R  1  16067
  
18 33 50  IRAS2012     14 55 00  26.7  56.0 -5.3     -71.5    -4   1  2  16067  18 33 50
18 34 30  ---          14 55 40  26.8  56.0 -5.3     -71.6    36   R  1  15533
  
18 34 30  2007+402     14 55 40  27.8  57.3 -5.2     -72.1    -4   1  2  15533  18 34 30
18 35 00  ---          14 56 11  27.9  57.3 -5.2     -72.2    26   R  1  15133
  
18 35 00  IRAS2012     14 56 11  26.9  56.1 -5.3     -71.7    -4   1  2  15133  18 35 00
18 35 40  ---          14 56 51  27.1  56.1 -5.3     -71.7    36   R  1  14600
  
18 35 40  2007+402     14 56 51  28.0  57.3 -5.2     -72.3    -4   1  2  14600  18 35 40
18 36 10  ---          14 57 21  28.1  57.4 -5.2     -72.3    26   R  1  14200
  
18 36 10  IRAS2012     14 57 21  27.1  56.1 -5.3     -71.8    -4   1  2  14200  18 36 10
18 36 50  ---          14 58 01  27.3  56.2 -5.3     -71.9    36   R  1  13667
  
18 36 50  2007+402     14 58 01  28.2  57.4 -5.2     -72.4    -4   1  2  13667  18 36 50
18 37 20  ---          14 58 31  28.3  57.4 -5.2     -72.5    26   R  1  13267
  
18 37 20  IRAS2012     14 58 31  27.4  56.2 -5.3     -72.0    -4   1  2  13267  18 37 20
18 38 00  ---          14 59 11  27.5  56.3 -5.3     -72.1    36   R  1  12733
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
18 38 00  2007+402     14 59 11  28.5  57.5 -5.1     -72.6    -4   1  2  12733  18 38 00
18 38 30  ---          14 59 41  28.6  57.5 -5.1     -72.7    26   R  1  12333
  
18 38 30  IRAS2012     14 59 41  27.6  56.3 -5.2     -72.1    -4   1  2  12333  18 38 30
18 39 10  ---          15 00 21  27.7  56.3 -5.2     -72.2    36   R  1  11800
  
18 39 10  2007+402     15 00 21  28.7  57.6 -5.1     -72.7    -4   1  2  11800  18 39 10
18 39 40  ---          15 00 51  28.8  57.6 -5.1     -72.8    26   R  1  11400
  
18 39 40  IRAS2012     15 00 51  27.8  56.4 -5.2     -72.3    -4   1  2  11400  18 39 40
18 40 20  ---          15 01 31  27.9  56.4 -5.2     -72.4    36   R  1  10867
  
18 40 20  2007+402     15 01 31  28.9  57.6 -5.1     -72.9    -4   1  2  10867  18 40 20
18 40 50  ---          15 02 01  29.0  57.7 -5.1     -73.0    26   R  1  10467
  
18 40 50  IRAS2012     15 02 01  28.0  56.4 -5.2     -72.4    -4   1  2  10467  18 40 50
18 41 30  ---          15 02 42  28.1  56.5 -5.2     -72.5    36   R  1   9933
  
18 41 30  2007+402     15 02 42  29.1  57.7 -5.1     -73.0    -4   1  2   9933  18 41 30
18 42 00  ---          15 03 12  29.2  57.7 -5.1     -73.1    26   R  1   9533
  
18 43 00  IRAS2012     15 04 12  28.4  56.6 -5.2     -72.7    56   1  2   9533  18 43 00
18 43 55  ---          15 05 07  28.5  56.6 -5.2     -72.9    55   R  1   8800
  
18 44 55  2007+402     15 06 07  29.7  57.9 -5.0     -73.5    56   1  2   8800  18 44 55
18 45 40  ---          15 06 52  29.9  58.0 -5.0     -73.6    45   R  1   8200
  
18 45 40  IRAS2012     15 06 52  28.9  56.7 -5.1     -73.1    -4   1  2   8200  18 45 40
18 46 20  ---          15 07 32  29.0  56.8 -5.1     -73.2    36   R  1   7667
  
18 46 20  2007+402     15 07 32  30.0  58.0 -5.0     -73.7    -4   1  2   7667  18 46 20
18 46 50  ---          15 08 02  30.1  58.0 -5.0     -73.8    26   R  1   7267
  
18 46 50  IRAS2012     15 08 02  29.1  56.8 -5.1     -73.3    -4   1  2   7267  18 46 50
18 47 30  ---          15 08 43  29.2  56.9 -5.1     -73.3    36   R  1   6733
  
18 47 30  2007+402     15 08 43  30.2  58.1 -5.0     -73.8    -4   1  2   6733  18 47 30
18 48 00  ---          15 09 13  30.3  58.1 -5.0     -73.9    26   R  1   6333
  
18 48 00  IRAS2012     15 09 13  29.3  56.9 -5.1     -73.4    -4   1  2   6333  18 48 00
18 48 40  ---          15 09 53  29.4  56.9 -5.1     -73.5    36   R  1   5800
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
18 48 40  2007+402     15 09 53  30.4  58.2 -5.0     -74.0    -4   1  2   5800  18 48 40
18 49 10  ---          15 10 23  30.5  58.2 -5.0     -74.1    26   R  1   5400
  
18 49 10  IRAS2012     15 10 23  29.5  57.0 -5.1     -73.6    -4   1  2   5400  18 49 10
18 49 50  ---          15 11 03  29.6  57.0 -5.1     -73.7    36   R  1   4867
  
18 49 50  2007+402     15 11 03  30.6  58.2 -4.9     -74.1    -4   1  2   4867  18 49 50
18 50 20  ---          15 11 33  30.7  58.3 -4.9     -74.2    26   R  1   4467
  
18 50 20  IRAS2012     15 11 33  29.7  57.0 -5.0     -73.7    -4   1  2   4467  18 50 20
18 51 00  ---          15 12 13  29.8  57.1 -5.0     -73.8    36   R  1   3933
  
18 51 00  2007+402     15 12 13  30.8  58.3 -4.9     -74.3    -4   1  2   3933  18 51 00
18 51 30  ---          15 12 43  30.9  58.3 -4.9     -74.4    26   R  1   3533
  
18 51 30  IRAS2012     15 12 43  29.9  57.1 -5.0     -73.9    -4   1  2   3533  18 51 30
18 52 10  ---          15 13 23  30.0  57.1 -5.0     -74.0    36   R  1   3000
  
18 52 10  2007+402     15 13 23  31.0  58.4 -4.9     -74.5    -4   1  2   3000  18 52 10
18 52 40  ---          15 13 53  31.1  58.4 -4.9     -74.5    26   R  1   2600
  
18 52 40  IRAS2012     15 13 53  30.1  57.2 -5.0     -74.0    -4   1  2   2600  18 52 40
18 53 20  ---          15 14 34  30.2  57.2 -5.0     -74.1    36   R  1   2067
  
18 53 20  2007+402     15 14 34  31.3  58.4 -4.9     -74.6    -4   1  2   2067  18 53 20
18 53 50  ---          15 15 04  31.4  58.5 -4.9     -74.7    26   R  1   1667
  
18 53 50  IRAS2012     15 15 04  30.3  57.2 -5.0     -74.2    -4   1  2   1667  18 53 50
18 54 30  ---          15 15 44  30.5  57.3 -5.0     -74.3    36   R  1   1133
  
18 54 30  2007+402     15 15 44  31.5  58.5 -4.9     -74.8    -4   1  2   1133  18 54 30
18 55 00  ---          15 16 14  31.6  58.5 -4.9     -74.8    26   R  1    733
  
18 56 00  IRAS2012     15 17 14  30.7  57.4 -5.0     -74.5    56   1  2    733  18 56 00
18 56 55  ---          15 18 09  30.9  57.4 -4.9     -74.6    55   R  1      0
  
18 57 55  2007+402     15 19 09  32.1  58.7 -4.8     -75.2    56   1  1      0  18 57 55
18 58 40  ---          15 19 54  32.2  58.7 -4.8     -75.3    45   F  2    600
  
18 58 40  IRAS2012     15 19 54  31.2  57.5 -4.9     -74.9    -4   1  1    600  18 58 40
18 59 20  ---          15 20 35  31.3  57.6 -4.9     -74.9    36   F  2   1133
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
18 59 20  2007+402     15 20 35  32.4  58.8 -4.8     -75.4    -4   1  1   1133  18 59 20
18 59 50  ---          15 21 05  32.5  58.8 -4.8     -75.5    26   F  2   1533
  
18 59 50  IRAS2012     15 21 05  31.4  57.6 -4.9     -75.0    -4   1  1   1533  18 59 50
19 00 30  ---          15 21 45  31.5  57.6 -4.9     -75.1    36   F  2   2067
  
19 00 30  2007+402     15 21 45  32.6  58.8 -4.8     -75.6    -4   1  1   2067  19 00 30
19 01 00  ---          15 22 15  32.7  58.9 -4.8     -75.6    26   F  2   2467
  
19 01 00  IRAS2012     15 22 15  31.6  57.7 -4.9     -75.2    -4   1  1   2467  19 01 00
19 01 40  ---          15 22 55  31.8  57.7 -4.9     -75.3    36   F  2   3000
  
19 01 40  2007+402     15 22 55  32.8  58.9 -4.7     -75.7    -4   1  1   3000  19 01 40
19 02 10  ---          15 23 25  32.9  58.9 -4.7     -75.8    26   F  2   3400
  
19 02 10  IRAS2012     15 23 25  31.8  57.7 -4.9     -75.3    -4   1  1   3400  19 02 10
19 02 50  ---          15 24 05  32.0  57.8 -4.8     -75.4    36   F  2   3933
  
19 02 50  2007+402     15 24 05  33.0  59.0 -4.7     -75.9    -4   1  1   3933  19 02 50
19 03 20  ---          15 24 35  33.1  59.0 -4.7     -75.9    26   F  2   4333
  
19 03 20  IRAS2012     15 24 35  32.1  57.8 -4.8     -75.5    -4   1  1   4333  19 03 20
19 04 00  ---          15 25 15  32.2  57.8 -4.8     -75.6    36   F  2   4867
  
19 04 00  2007+402     15 25 15  33.2  59.0 -4.7     -76.0    -4   1  1   4867  19 04 00
19 04 30  ---          15 25 45  33.3  59.1 -4.7     -76.1    26   F  2   5267
  
19 04 30  IRAS2012     15 25 45  32.3  57.9 -4.8     -75.6    -4   1  1   5267  19 04 30
19 05 10  ---          15 26 25  32.4  57.9 -4.8     -75.7    36   F  2   5800
  
19 05 10  2007+402     15 26 25  33.4  59.1 -4.7     -76.2    -4   1  1   5800  19 05 10
19 05 40  ---          15 26 56  33.5  59.1 -4.7     -76.2    26   F  2   6200
  
19 05 40  IRAS2012     15 26 56  32.5  57.9 -4.8     -75.8    -4   1  1   6200  19 05 40
19 06 20  ---          15 27 36  32.6  58.0 -4.8     -75.9    36   F  2   6733
  
19 06 20  2007+402     15 27 36  33.7  59.2 -4.7     -76.3    -4   1  1   6733  19 06 20
19 06 50  ---          15 28 06  33.8  59.2 -4.7     -76.4    26   F  2   7133
  
19 06 50  IRAS2012     15 28 06  32.7  58.0 -4.8     -76.0    -4   1  1   7133  19 06 50
19 07 30  ---          15 28 46  32.8  58.0 -4.8     -76.1    36   F  2   7667
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
19 07 30  2007+402     15 28 46  33.9  59.2 -4.6     -76.5    -4   1  1   7667  19 07 30
19 08 00  ---          15 29 16  34.0  59.3 -4.6     -76.6    26   F  2   8067
  
19 09 00  IRAS2012     15 30 16  33.1  58.1 -4.7     -76.3    56   1  1   8067  19 09 00
19 09 55  ---          15 31 11  33.3  58.2 -4.7     -76.4    55   F  2   8800
  
19 10 55  2007+402     15 32 11  34.5  59.4 -4.6     -76.9    56   1  1   8800  19 10 55
19 11 40  ---          15 32 57  34.7  59.5 -4.6     -77.0    45   F  2   9400
  
19 11 40  IRAS2012     15 32 57  33.6  58.2 -4.7     -76.6    -4   1  1   9400  19 11 40
19 12 20  ---          15 33 37  33.7  58.3 -4.7     -76.7    36   F  2   9933
  
19 12 20  2007+402     15 33 37  34.8  59.5 -4.6     -77.1    -4   1  1   9933  19 12 20
19 12 50  ---          15 34 07  34.9  59.5 -4.6     -77.2    26   F  2  10333
  
19 12 50  IRAS2012     15 34 07  33.8  58.3 -4.7     -76.8    -4   1  1  10333  19 12 50
19 13 30  ---          15 34 47  33.9  58.3 -4.7     -76.9    36   F  2  10867
  
19 13 30  2007+402     15 34 47  35.0  59.5 -4.5     -77.3    -4   1  1  10867  19 13 30
19 14 00  ---          15 35 17  35.1  59.6 -4.5     -77.4    26   F  2  11267
  
19 14 00  IRAS2012     15 35 17  34.0  58.4 -4.7     -76.9    -4   1  1  11267  19 14 00
19 14 40  ---          15 35 57  34.1  58.4 -4.6     -77.0    36   F  2  11800
  
19 14 40  2007+402     15 35 57  35.2  59.6 -4.5     -77.4    -4   1  1  11800  19 14 40
19 15 10  ---          15 36 27  35.3  59.6 -4.5     -77.5    26   F  2  12200
  
19 15 10  IRAS2012     15 36 27  34.2  58.4 -4.6     -77.1    -4   1  1  12200  19 15 10
19 15 50  ---          15 37 07  34.4  58.5 -4.6     -77.2    36   F  2  12733
  
19 15 50  2007+402     15 37 07  35.4  59.7 -4.5     -77.6    -4   1  1  12733  19 15 50
19 16 20  ---          15 37 37  35.5  59.7 -4.5     -77.7    26   F  2  13133
  
19 16 20  IRAS2012     15 37 37  34.4  58.5 -4.6     -77.3    -4   1  1  13133  19 16 20
19 17 00  ---          15 38 17  34.6  58.5 -4.6     -77.4    36   F  2  13667
  
19 17 00  2007+402     15 38 17  35.6  59.7 -4.5     -77.8    -4   1  1  13667  19 17 00
19 17 30  ---          15 38 47  35.7  59.7 -4.5     -77.8    26   F  2  14067
  
19 17 30  IRAS2012     15 38 47  34.7  58.5 -4.6     -77.4    -4   1  1  14067  19 17 30
19 18 10  ---          15 39 28  34.8  58.6 -4.6     -77.5    36   F  2  14600
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
19 18 10  2007+402     15 39 28  35.9  59.8 -4.5     -77.9    -4   1  1  14600  19 18 10
19 18 40  ---          15 39 58  36.0  59.8 -4.5     -78.0    26   F  2  15000
  
19 18 40  IRAS2012     15 39 58  34.9  58.6 -4.6     -77.6    -4   1  1  15000  19 18 40
19 19 20  ---          15 40 38  35.0  58.6 -4.6     -77.7    36   F  2  15533
  
19 19 20  2007+402     15 40 38  36.1  59.8 -4.5     -78.1    -4   1  1  15533  19 19 20
19 19 50  ---          15 41 08  36.2  59.9 -4.4     -78.1    26   F  2  15933
  
19 19 50  IRAS2012     15 41 08  35.1  58.7 -4.6     -77.7    -4   1  1  15933  19 19 50
19 20 30  ---          15 41 48  35.2  58.7 -4.5     -77.8    36   F  2  16467
  
19 20 30  2007+402     15 41 48  36.3  59.9 -4.4     -78.2    -4   1  1  16467  19 20 30
19 21 00  ---          15 42 18  36.4  59.9 -4.4     -78.3    26   F  2  16867
  
19 22 00  IRAS2012     15 43 18  35.5  58.8 -4.5     -78.0    56   1  1  16867  19 22 00
19 22 55  ---          15 44 13  35.7  58.8 -4.5     -78.2    55   F  2  17600
  
19 26 15  2007+777     15 47 34  35.2  13.4 -4.3    -108.2   168   1  2  17600  19 26 15
19 29 15  ---          15 50 34  35.3  13.3 -4.2    -109.0   180   R  2  15200
  
19 32 45  2007+402     15 54 05  38.6  60.5 -4.2     -79.9   177   1  2  15200  19 32 28
19 33 20  ---          15 54 40  38.7  60.5 -4.2     -80.0    35   R  2  14507
  
19 33 20  IRAS2012     15 54 40  37.6  59.3 -4.3     -79.6    -4   1  2  14507  19 33 20
19 34 00  ---          15 55 20  37.7  59.3 -4.3     -79.7    36   R  2  13973
  
19 34 00  2007+402     15 55 20  38.8  60.5 -4.2     -80.0    -4   1  2  13973  19 34 00
19 34 30  ---          15 55 50  38.9  60.5 -4.2     -80.1    26   R  2  13573
  
19 34 30  IRAS2012     15 55 50  37.8  59.3 -4.3     -79.8    -4   1  2  13573  19 34 30
19 35 10  ---          15 56 30  37.9  59.4 -4.3     -79.9    36   R  2  13040
  
19 35 10  2007+402     15 56 30  39.0  60.6 -4.2     -80.2    -4   1  2  13040  19 35 10
19 35 40  ---          15 57 00  39.1  60.6 -4.2     -80.3    26   R  2  12640
  
19 35 40  IRAS2012     15 57 00  38.0  59.4 -4.3     -79.9    -4   1  2  12640  19 35 40
19 36 20  ---          15 57 41  38.1  59.4 -4.3     -80.0    36   R  2  12107
  
19 36 20  2007+402     15 57 41  39.3  60.6 -4.2     -80.4    -4   1  2  12107  19 36 20
19 36 50  ---          15 58 11  39.4  60.6 -4.2     -80.4    26   R  2  11707
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
19 36 50  IRAS2012     15 58 11  38.2  59.4 -4.3     -80.1    -4   1  2  11707  19 36 50
19 37 30  ---          15 58 51  38.4  59.5 -4.3     -80.2    36   R  2  11173
  
19 37 30  2007+402     15 58 51  39.5  60.7 -4.1     -80.5    -4   1  2  11173  19 37 30
19 38 00  ---          15 59 21  39.6  60.7 -4.1     -80.6    26   R  2  10773
  
19 38 00  IRAS2012     15 59 21  38.4  59.5 -4.3     -80.3    -4   1  2  10773  19 38 00
19 38 40  ---          16 00 01  38.6  59.5 -4.2     -80.3    36   R  2  10240
  
19 38 40  2007+402     16 00 01  39.7  60.7 -4.1     -80.7    -4   1  2  10240  19 38 40
19 39 10  ---          16 00 31  39.8  60.7 -4.1     -80.8    26   R  2   9840
  
19 39 10  IRAS2012     16 00 31  38.7  59.5 -4.2     -80.4    -4   1  2   9840  19 39 10
19 39 50  ---          16 01 11  38.8  59.5 -4.2     -80.5    36   R  2   9307
  
19 39 50  2007+402     16 01 11  39.9  60.7 -4.1     -80.8    -4   1  2   9307  19 39 50
19 40 20  ---          16 01 41  40.0  60.8 -4.1     -80.9    26   R  2   8907
  
19 41 20  IRAS2012     16 02 41  39.1  59.6 -4.2     -80.7    56   1  2   8907  19 41 02
19 42 05  ---          16 03 27  39.2  59.6 -4.2     -80.8    45   R  2   8067
  
19 43 05  2007+402     16 04 27  40.5  60.9 -4.1     -81.3    55   1  2   8067  19 42 47
19 43 40  ---          16 05 02  40.6  60.9 -4.0     -81.4    35   R  2   7360
  
19 43 40  IRAS2012     16 05 02  39.5  59.7 -4.2     -81.0    -4   1  2   7360  19 43 40
19 44 20  ---          16 05 42  39.6  59.7 -4.1     -81.1    36   R  2   6827
  
19 44 20  2007+402     16 05 42  40.8  60.9 -4.0     -81.5    -4   1  2   6827  19 44 20
19 44 50  ---          16 06 12  40.9  60.9 -4.0     -81.5    26   R  2   6427
  
19 44 50  IRAS2012     16 06 12  39.7  59.7 -4.1     -81.2    -4   1  2   6427  19 44 50
19 45 30  ---          16 06 52  39.8  59.8 -4.1     -81.3    36   R  2   5893
  
19 45 30  2007+402     16 06 52  41.0  61.0 -4.0     -81.6    -4   1  2   5893  19 45 30
19 46 00  ---          16 07 22  41.1  61.0 -4.0     -81.7    26   R  2   5493
  
19 46 00  IRAS2012     16 07 22  39.9  59.8 -4.1     -81.4    -4   1  2   5493  19 46 00
19 46 40  ---          16 08 02  40.1  59.8 -4.1     -81.5    36   R  2   4960
  
19 46 40  2007+402     16 08 02  41.2  61.0 -4.0     -81.8    -4   1  2   4960  19 46 40
19 47 10  ---          16 08 32  41.3  61.0 -4.0     -81.9    26   R  2   4560
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
19 47 10  IRAS2012     16 08 32  40.2  59.8 -4.1     -81.5    -4   1  2   4560  19 47 10
19 47 50  ---          16 09 12  40.3  59.9 -4.1     -81.6    36   R  2   4027
  
19 47 50  2007+402     16 09 12  41.4  61.0 -4.0     -82.0    -4   1  2   4027  19 47 50
19 48 20  ---          16 09 43  41.5  61.1 -4.0     -82.0    26   R  2   3627
  
19 48 20  IRAS2012     16 09 43  40.4  59.9 -4.1     -81.7    -4   1  2   3627  19 48 20
19 49 00  ---          16 10 23  40.5  59.9 -4.1     -81.8    36   R  2   3093
  
19 49 00  2007+402     16 10 23  41.6  61.1 -4.0     -82.1    -4   1  2   3093  19 49 00
19 49 30  ---          16 10 53  41.7  61.1 -3.9     -82.2    26   R  2   2693
  
19 49 30  IRAS2012     16 10 53  40.6  59.9 -4.1     -81.9    -4   1  2   2693  19 49 30
19 50 10  ---          16 11 33  40.7  59.9 -4.0     -82.0    36   R  2   2160
  
19 50 10  2007+402     16 11 33  41.9  61.1 -3.9     -82.3    -4   1  2   2160  19 50 10
19 50 40  ---          16 12 03  42.0  61.1 -3.9     -82.3    26   R  2   1760
  
19 50 40  IRAS2012     16 12 03  40.8  60.0 -4.0     -82.0    -4   1  2   1760  19 50 40
19 51 20  ---          16 12 43  40.9  60.0 -4.0     -82.1    36   R  2   1227
  
19 51 20  2007+402     16 12 43  42.1  61.2 -3.9     -82.4    -4   1  2   1227  19 51 20
19 51 50  ---          16 13 13  42.2  61.2 -3.9     -82.5    26   R  2    827
  
19 52 50  IRAS2012     16 14 13  41.2  60.0 -4.0     -82.4    56   1  2    827  19 52 33
19 53 35  ---          16 14 58  41.4  60.1 -4.0     -82.5    45   R  2      0
  
19 54 35  2002+472     16 15 59  44.1  51.8 -3.8     -90.4    52   1  3      0  19 54 35
19 57 35  ---          16 18 59  44.6  51.8 -3.7     -90.9   180   F  1   2400
  
19 58 35  2007+402     16 19 59  43.5  61.4 -3.8     -83.5    52   1  3   2400  19 58 18
19 59 10  ---          16 20 34  43.6  61.4 -3.8     -83.5    35   F  1   3093
  
19 59 10  IRAS2012     16 20 34  42.4  60.2 -3.9     -83.3    -4   1  3   3093  19 59 10
19 59 50  ---          16 21 14  42.5  60.2 -3.9     -83.4    36   F  1   3627
  
19 59 50  2007+402     16 21 14  43.7  61.4 -3.8     -83.6    -4   1  3   3627  19 59 50
20 00 20  ---          16 21 45  43.8  61.4 -3.8     -83.7    26   F  1   4027
  
20 00 20  IRAS2012     16 21 45  42.6  60.3 -3.9     -83.4    -4   1  3   4027  20 00 20
20 01 00  ---          16 22 25  42.7  60.3 -3.9     -83.5    36   F  1   4560
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
20 01 00  2007+402     16 22 25  43.9  61.5 -3.8     -83.8    -4   1  3   4560  20 01 00
20 01 30  ---          16 22 55  44.0  61.5 -3.7     -83.9    26   F  1   4960
  
20 01 30  IRAS2012     16 22 55  42.8  60.3 -3.9     -83.6    -4   1  3   4960  20 01 30
20 02 10  ---          16 23 35  43.0  60.3 -3.8     -83.7    36   F  1   5493
  
20 02 10  2007+402     16 23 35  44.1  61.5 -3.7     -84.0    -4   1  3   5493  20 02 10
20 02 40  ---          16 24 05  44.2  61.5 -3.7     -84.0    26   F  1   5893
  
20 02 40  IRAS2012     16 24 05  43.1  60.3 -3.8     -83.8    -4   1  3   5893  20 02 40
20 03 20  ---          16 24 45  43.2  60.3 -3.8     -83.9    36   F  1   6427
  
20 03 20  2007+402     16 24 45  44.4  61.5 -3.7     -84.1    -4   1  3   6427  20 03 20
20 03 50  ---          16 25 15  44.5  61.5 -3.7     -84.2    26   F  1   6827
  
20 03 50  IRAS2012     16 25 15  43.3  60.4 -3.8     -83.9    -4   1  3   6827  20 03 50
20 04 30  ---          16 25 55  43.4  60.4 -3.8     -84.0    36   F  1   7360
  
20 04 30  2007+402     16 25 55  44.6  61.6 -3.7     -84.3    -4   1  3   7360  20 04 30
20 05 00  ---          16 26 25  44.7  61.6 -3.7     -84.4    26   F  1   7760
  
20 05 00  IRAS2012     16 26 25  43.5  60.4 -3.8     -84.1    -4   1  3   7760  20 05 00
20 05 40  ---          16 27 05  43.6  60.4 -3.8     -84.2    36   F  1   8293
  
20 05 40  2007+402     16 27 05  44.8  61.6 -3.7     -84.5    -4   1  3   8293  20 05 40
20 06 10  ---          16 27 35  44.9  61.6 -3.7     -84.6    26   F  1   8693
  
20 07 10  IRAS2012     16 28 36  43.9  60.4 -3.8     -84.4    56   1  3   8693  20 06 52
20 07 55  ---          16 29 21  44.0  60.5 -3.8     -84.5    45   F  1   9533
  
20 08 55  2007+402     16 30 21  45.4  61.7 -3.6     -85.0    55   1  3   9533  20 08 37
20 09 30  ---          16 30 56  45.5  61.7 -3.6     -85.0    35   F  1  10240
  
20 09 30  IRAS2012     16 30 56  44.3  60.5 -3.7     -84.8    -4   1  3  10240  20 09 30
20 10 10  ---          16 31 36  44.5  60.5 -3.7     -84.9    36   F  1  10773
  
20 10 10  2007+402     16 31 36  45.7  61.7 -3.6     -85.1    -4   1  3  10773  20 10 10
20 10 40  ---          16 32 06  45.8  61.7 -3.6     -85.2    26   F  1  11173
  
20 10 40  IRAS2012     16 32 06  44.6  60.5 -3.7     -85.0    -4   1  3  11173  20 10 40
20 11 20  ---          16 32 46  44.7  60.5 -3.7     -85.1    36   F  1  11707
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
20 11 20  2007+402     16 32 46  45.9  61.7 -3.6     -85.3    -4   1  3  11707  20 11 20
20 11 50  ---          16 33 16  46.0  61.7 -3.6     -85.4    26   F  1  12107
  
20 11 50  IRAS2012     16 33 16  44.8  60.6 -3.7     -85.1    -4   1  3  12107  20 11 50
20 12 30  ---          16 33 57  44.9  60.6 -3.7     -85.2    36   F  1  12640
  
20 12 30  2007+402     16 33 57  46.1  61.8 -3.6     -85.5    -4   1  3  12640  20 12 30
20 13 00  ---          16 34 27  46.2  61.8 -3.6     -85.6    26   F  1  13040
  
20 13 00  IRAS2012     16 34 27  45.0  60.6 -3.7     -85.3    -4   1  3  13040  20 13 00
20 13 40  ---          16 35 07  45.1  60.6 -3.7     -85.4    36   F  1  13573
  
20 13 40  2007+402     16 35 07  46.3  61.8 -3.5     -85.6    -4   1  3  13573  20 13 40
20 14 10  ---          16 35 37  46.4  61.8 -3.5     -85.7    26   F  1  13973
  
20 14 10  IRAS2012     16 35 37  45.2  60.6 -3.6     -85.5    -4   1  3  13973  20 14 10
20 14 50  ---          16 36 17  45.3  60.6 -3.6     -85.6    36   F  1  14507
  
20 14 50  2007+402     16 36 17  46.5  61.8 -3.5     -85.8    -4   1  3  14507  20 14 50
20 15 20  ---          16 36 47  46.6  61.8 -3.5     -85.9    26   F  1  14907
  
20 15 20  IRAS2012     16 36 47  45.4  60.6 -3.6     -85.7    -4   1  3  14907  20 15 20
20 16 00  ---          16 37 27  45.6  60.6 -3.6     -85.8    36   F  1  15440
  
20 16 00  2007+402     16 37 27  46.8  61.8 -3.5     -86.0    -4   1  3  15440  20 16 00
20 16 30  ---          16 37 57  46.9  61.8 -3.5     -86.1    26   F  1  15840
  
20 16 30  IRAS2012     16 37 57  45.7  60.7 -3.6     -85.8    -4   1  3  15840  20 16 30
20 17 10  ---          16 38 37  45.8  60.7 -3.6     -85.9    36   F  1  16373
  
20 17 10  2007+402     16 38 37  47.0  61.9 -3.5     -86.2    -4   1  3  16373  20 17 10
20 17 40  ---          16 39 07  47.1  61.9 -3.5     -86.2    26   F  1  16773
  
20 18 40  IRAS2012     16 40 08  46.1  60.7 -3.6     -86.2    56   1  3  16773  20 18 23
20 19 25  ---          16 40 53  46.2  60.7 -3.6     -86.3    45   F  1  17600
  
20 20 25  2007+402     16 41 53  47.6  61.9 -3.4     -86.7    55   1  4  17600  20 20 25
20 21 10  ---          16 42 38  47.7  61.9 -3.4     -86.8    45   R  1  17000
  
20 21 10  IRAS2012     16 42 38  46.5  60.7 -3.5     -86.5    -4   1  4  17000  20 21 10
20 21 50  ---          16 43 18  46.7  60.8 -3.5     -86.6    36   R  1  16467
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
20 21 50  2007+402     16 43 18  47.9  61.9 -3.4     -86.9    -4   1  4  16467  20 21 50
20 22 20  ---          16 43 48  48.0  61.9 -3.4     -86.9    26   R  1  16067
  
20 22 20  IRAS2012     16 43 48  46.7  60.8 -3.5     -86.7    -4   1  4  16067  20 22 20
20 23 00  ---          16 44 28  46.9  60.8 -3.5     -86.8    36   R  1  15533
  
20 23 00  2007+402     16 44 28  48.1  61.9 -3.4     -87.0    -4   1  4  15533  20 23 00
20 23 30  ---          16 44 58  48.2  62.0 -3.4     -87.1    26   R  1  15133
  
20 23 30  IRAS2012     16 44 58  47.0  60.8 -3.5     -86.9    -4   1  4  15133  20 23 30
20 24 10  ---          16 45 38  47.1  60.8 -3.5     -87.0    36   R  1  14600
  
20 24 10  2007+402     16 45 38  48.3  62.0 -3.4     -87.2    -4   1  4  14600  20 24 10
20 24 40  ---          16 46 09  48.4  62.0 -3.4     -87.3    26   R  1  14200
  
20 24 40  IRAS2012     16 46 09  47.2  60.8 -3.5     -87.1    -4   1  4  14200  20 24 40
20 25 20  ---          16 46 49  47.3  60.8 -3.5     -87.2    36   R  1  13667
  
20 25 20  2007+402     16 46 49  48.5  62.0 -3.3     -87.4    -4   1  4  13667  20 25 20
20 25 50  ---          16 47 19  48.6  62.0 -3.3     -87.5    26   R  1  13267
  
20 25 50  IRAS2012     16 47 19  47.4  60.8 -3.5     -87.3    -4   1  4  13267  20 25 50
20 26 30  ---          16 47 59  47.5  60.8 -3.4     -87.4    36   R  1  12733
  
20 26 30  2007+402     16 47 59  48.8  62.0 -3.3     -87.6    -4   1  4  12733  20 26 30
20 27 00  ---          16 48 29  48.9  62.0 -3.3     -87.7    26   R  1  12333
  
20 27 00  IRAS2012     16 48 29  47.6  60.8 -3.4     -87.4    -4   1  4  12333  20 27 00
20 27 40  ---          16 49 09  47.8  60.8 -3.4     -87.5    36   R  1  11800
  
20 27 40  2007+402     16 49 09  49.0  62.0 -3.3     -87.8    -4   1  4  11800  20 27 40
20 28 10  ---          16 49 39  49.1  62.0 -3.3     -87.8    26   R  1  11400
  
20 28 10  IRAS2012     16 49 39  47.8  60.8 -3.4     -87.6    -4   1  4  11400  20 28 10
20 28 50  ---          16 50 19  48.0  60.8 -3.4     -87.7    36   R  1  10867
  
20 28 50  2007+402     16 50 19  49.2  62.0 -3.3     -87.9    -4   1  4  10867  20 28 50
20 29 20  ---          16 50 49  49.3  62.0 -3.3     -88.0    26   R  1  10467
  
20 29 20  IRAS2012     16 50 49  48.1  60.9 -3.4     -87.8    -4   1  4  10467  20 29 20
20 30 00  ---          16 51 29  48.2  60.9 -3.4     -87.9    36   R  1   9933
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
20 30 00  2007+402     16 51 29  49.4  62.0 -3.3     -88.1    -4   1  4   9933  20 30 00
20 30 30  ---          16 51 59  49.5  62.0 -3.3     -88.2    26   R  1   9533
  
20 31 30  IRAS2012     16 53 00  48.5  60.9 -3.4     -88.1    56   1  4   9533  20 31 30
20 32 25  ---          16 53 55  48.6  60.9 -3.3     -88.3    55   R  1   8800
  
20 33 25  2007+402     16 54 55  50.1  62.1 -3.2     -88.7    55   1  4   8800  20 33 25
20 34 10  ---          16 55 40  50.2  62.1 -3.2     -88.8    45   R  1   8200
  
20 34 10  IRAS2012     16 55 40  49.0  60.9 -3.3     -88.6    -4   1  4   8200  20 34 10
20 34 50  ---          16 56 20  49.1  60.9 -3.3     -88.7    36   R  1   7667
  
20 34 50  2007+402     16 56 20  50.4  62.1 -3.2     -88.9    -4   1  4   7667  20 34 50
20 35 20  ---          16 56 50  50.4  62.1 -3.2     -89.0    26   R  1   7267
  
20 35 20  IRAS2012     16 56 50  49.2  60.9 -3.3     -88.8    -4   1  4   7267  20 35 20
20 36 00  ---          16 57 30  49.3  60.9 -3.3     -88.9    36   R  1   6733
  
20 36 00  2007+402     16 57 30  50.6  62.1 -3.2     -89.1    -5   1  4   6733  20 36 00
20 36 30  ---          16 58 00  50.7  62.1 -3.2     -89.1    25   R  1   6333
  
20 36 30  IRAS2012     16 58 00  49.4  60.9 -3.3     -88.9    -5   1  4   6333  20 36 30
20 37 10  ---          16 58 41  49.5  60.9 -3.3     -89.1    35   R  1   5800
  
20 37 10  2007+402     16 58 41  50.8  62.1 -3.2     -89.3    -5   1  4   5800  20 37 10
20 37 40  ---          16 59 11  50.9  62.1 -3.1     -89.3    25   R  1   5400
  
20 37 40  IRAS2012     16 59 11  49.6  60.9 -3.3     -89.1    -5   1  4   5400  20 37 40
20 38 20  ---          16 59 51  49.8  60.9 -3.2     -89.2    35   R  1   4867
  
20 38 20  2007+402     16 59 51  51.0  62.1 -3.1     -89.4    -5   1  4   4867  20 38 20
20 38 50  ---          17 00 21  51.1  62.1 -3.1     -89.5    25   R  1   4467
  
20 38 50  IRAS2012     17 00 21  49.9  60.9 -3.2     -89.3    -5   1  4   4467  20 38 50
20 39 30  ---          17 01 01  50.0  60.9 -3.2     -89.4    35   R  1   3933
  
20 39 30  2007+402     17 01 01  51.2  62.1 -3.1     -89.6    -5   1  4   3933  20 39 30
20 40 00  ---          17 01 31  51.3  62.1 -3.1     -89.7    25   R  1   3533
  
20 40 00  IRAS2012     17 01 31  50.1  60.9 -3.2     -89.5    -5   1  4   3533  20 40 00
20 40 40  ---          17 02 11  50.2  60.9 -3.2     -89.6    35   R  1   3000
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
20 40 40  2007+402     17 02 11  51.5  62.1 -3.1     -89.8    -5   1  4   3000  20 40 40
20 41 10  ---          17 02 41  51.6  62.1 -3.1     -89.9    25   R  1   2600
  
20 41 10  IRAS2012     17 02 41  50.3  60.9 -3.2     -89.7    -5   1  4   2600  20 41 10
20 41 50  ---          17 03 21  50.4  60.9 -3.2     -89.8    35   R  1   2067
  
20 41 50  2007+402     17 03 21  51.7  62.1 -3.1     -90.0    -5   1  4   2067  20 41 50
20 42 20  ---          17 03 51  51.8  62.1 -3.1     -90.1    25   R  1   1667
  
20 42 20  IRAS2012     17 03 51  50.5  60.9 -3.2     -89.9    -5   1  4   1667  20 42 20
20 43 00  ---          17 04 32  50.6  60.9 -3.2     -90.0    35   R  1   1133
  
20 43 00  2007+402     17 04 32  51.9  62.1 -3.1     -90.2    -5   1  4   1133  20 43 00
20 43 30  ---          17 05 02  52.0  62.1 -3.0     -90.3    25   R  1    733
  
20 44 30  IRAS2012     17 06 02  50.9  60.9 -3.1     -90.3    56   1  4    733  20 44 30
20 45 25  ---          17 06 57  51.1  60.9 -3.1     -90.4    55   R  1      0
  
20 46 25  2007+402     17 07 57  52.6  62.1 -3.0     -90.8    55   1  3      0  20 46 25
20 47 10  ---          17 08 42  52.7  62.1 -3.0     -90.9    45   F  2    600
  
20 47 10  IRAS2012     17 08 42  51.4  60.9 -3.1     -90.7    -5   1  3    600  20 47 10
20 47 50  ---          17 09 22  51.6  60.9 -3.1     -90.8    35   F  2   1133
  
20 47 50  2007+402     17 09 22  52.8  62.1 -3.0     -91.0    -5   1  3   1133  20 47 50
20 48 20  ---          17 09 52  52.9  62.1 -3.0     -91.1    25   F  2   1533
  
20 48 20  IRAS2012     17 09 52  51.6  60.9 -3.1     -90.9    -5   1  3   1533  20 48 20
20 49 00  ---          17 10 33  51.8  60.9 -3.1     -91.0    35   F  2   2067
  
20 49 00  2007+402     17 10 33  53.1  62.1 -3.0     -91.2    -5   1  3   2067  20 49 00
20 49 30  ---          17 11 03  53.1  62.1 -2.9     -91.3    25   F  2   2467
  
20 49 30  IRAS2012     17 11 03  51.9  60.9 -3.1     -91.1    -5   1  3   2467  20 49 30
20 50 10  ---          17 11 43  52.0  60.9 -3.0     -91.2    35   F  2   3000
  
20 50 10  2007+402     17 11 43  53.3  62.1 -2.9     -91.4    -5   1  3   3000  20 50 10
20 50 40  ---          17 12 13  53.4  62.1 -2.9     -91.5    25   F  2   3400
  
20 50 40  IRAS2012     17 12 13  52.1  60.9 -3.0     -91.3    -5   1  3   3400  20 50 40
20 51 20  ---          17 12 53  52.2  60.9 -3.0     -91.4    35   F  2   3933
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
20 51 20  2007+402     17 12 53  53.5  62.1 -2.9     -91.6    -5   1  3   3933  20 51 20
20 51 50  ---          17 13 23  53.6  62.0 -2.9     -91.7    25   F  2   4333
  
20 51 50  IRAS2012     17 13 23  52.3  60.9 -3.0     -91.5    -5   1  3   4333  20 51 50
20 52 30  ---          17 14 03  52.4  60.9 -3.0     -91.6    35   F  2   4867
  
20 52 30  2007+402     17 14 03  53.7  62.0 -2.9     -91.8    -5   1  3   4867  20 52 30
20 53 00  ---          17 14 33  53.8  62.0 -2.9     -91.9    25   F  2   5267
  
20 53 00  IRAS2012     17 14 33  52.5  60.9 -3.0     -91.7    -5   1  3   5267  20 53 00
20 53 40  ---          17 15 13  52.7  60.9 -3.0     -91.8    35   F  2   5800
  
20 53 40  2007+402     17 15 13  53.9  62.0 -2.9     -92.0    -5   1  3   5800  20 53 40
20 54 10  ---          17 15 43  54.0  62.0 -2.9     -92.1    25   F  2   6200
  
20 54 10  IRAS2012     17 15 43  52.7  60.9 -3.0     -91.9    -5   1  3   6200  20 54 10
20 54 50  ---          17 16 23  52.9  60.9 -3.0     -92.0    35   F  2   6733
  
20 54 50  2007+402     17 16 23  54.2  62.0 -2.9     -92.2    -5   1  3   6733  20 54 50
20 55 20  ---          17 16 54  54.3  62.0 -2.8     -92.3    25   F  2   7133
  
20 55 20  IRAS2012     17 16 54  53.0  60.9 -3.0     -92.1    -5   1  3   7133  20 55 20
20 56 00  ---          17 17 34  53.1  60.9 -2.9     -92.2    35   F  2   7667
  
20 56 00  2007+402     17 17 34  54.4  62.0 -2.8     -92.4    -5   1  3   7667  20 56 00
20 56 30  ---          17 18 04  54.5  62.0 -2.8     -92.5    25   F  2   8067
  
20 57 30  IRAS2012     17 19 04  53.4  60.8 -2.9     -92.5    56   1  3   8067  20 57 30
20 58 25  ---          17 19 59  53.5  60.8 -2.9     -92.6    55   F  2   8800
  
20 59 25  2007+402     17 20 59  55.0  61.9 -2.8     -93.0    55   1  3   8800  20 59 25
21 00 10  ---          17 21 44  55.2  61.9 -2.8     -93.1    45   F  2   9400
  
21 00 10  IRAS2012     17 21 44  53.9  60.8 -2.9     -93.0    -5   1  3   9400  21 00 10
21 00 50  ---          17 22 24  54.0  60.8 -2.9     -93.1    35   F  2   9933
  
21 00 50  2007+402     17 22 24  55.3  61.9 -2.8     -93.2    -5   1  3   9933  21 00 50
21 01 20  ---          17 22 55  55.4  61.9 -2.7     -93.3    25   F  2  10333
  
21 01 20  IRAS2012     17 22 55  54.1  60.8 -2.9     -93.2    -5   1  3  10333  21 01 20
21 02 00  ---          17 23 35  54.2  60.8 -2.8     -93.3    35   F  2  10867
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
21 02 00  2007+402     17 23 35  55.5  61.9 -2.7     -93.4    -5   1  3  10867  21 02 00
21 02 30  ---          17 24 05  55.6  61.9 -2.7     -93.5    25   F  2  11267
  
21 02 30  IRAS2012     17 24 05  54.3  60.8 -2.8     -93.4    -5   1  3  11267  21 02 30
21 03 10  ---          17 24 45  54.4  60.7 -2.8     -93.5    35   F  2  11800
  
21 03 10  2007+402     17 24 45  55.7  61.9 -2.7     -93.7    -5   1  3  11800  21 03 10
21 03 40  ---          17 25 15  55.8  61.9 -2.7     -93.7    25   F  2  12200
  
21 03 40  IRAS2012     17 25 15  54.5  60.7 -2.8     -93.6    -5   1  3  12200  21 03 40
21 04 20  ---          17 25 55  54.7  60.7 -2.8     -93.7    35   F  2  12733
  
21 04 20  2007+402     17 25 55  56.0  61.8 -2.7     -93.9    -5   1  3  12733  21 04 20
21 04 50  ---          17 26 25  56.1  61.8 -2.7     -94.0    25   F  2  13133
  
21 04 50  IRAS2012     17 26 25  54.8  60.7 -2.8     -93.8    -5   1  3  13133  21 04 50
21 05 30  ---          17 27 05  54.9  60.7 -2.8     -93.9    35   F  2  13667
  
21 05 30  2007+402     17 27 05  56.2  61.8 -2.7     -94.1    -5   1  3  13667  21 05 30
21 06 00  ---          17 27 35  56.3  61.8 -2.7     -94.2    25   F  2  14067
  
21 06 00  IRAS2012     17 27 35  55.0  60.7 -2.8     -94.0    -5   1  3  14067  21 06 00
21 06 40  ---          17 28 15  55.1  60.7 -2.8     -94.1    35   F  2  14600
  
21 06 40  2007+402     17 28 15  56.4  61.8 -2.7     -94.3    -5   1  3  14600  21 06 40
21 07 10  ---          17 28 46  56.5  61.8 -2.7     -94.4    25   F  2  15000
  
21 07 10  IRAS2012     17 28 46  55.2  60.7 -2.8     -94.2    -5   1  3  15000  21 07 10
21 07 50  ---          17 29 26  55.3  60.6 -2.8     -94.3    35   F  2  15533
  
21 07 50  2007+402     17 29 26  56.6  61.8 -2.6     -94.5    -5   1  3  15533  21 07 50
21 08 20  ---          17 29 56  56.7  61.7 -2.6     -94.6    25   F  2  15933
  
21 08 20  IRAS2012     17 29 56  55.4  60.6 -2.7     -94.4    -5   1  3  15933  21 08 20
21 09 00  ---          17 30 36  55.5  60.6 -2.7     -94.6    35   F  2  16467
  
21 09 00  2007+402     17 30 36  56.9  61.7 -2.6     -94.7    -5   1  3  16467  21 09 00
21 09 30  ---          17 31 06  57.0  61.7 -2.6     -94.8    25   F  2  16867
  
21 10 30  IRAS2012     17 32 06  55.8  60.6 -2.7     -94.8    56   1  3  16867  21 10 30
21 11 25  ---          17 33 01  56.0  60.5 -2.7     -95.0    55   F  2  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
21 14 25  2007+777     17 36 02  39.9   9.6 -2.5    -137.1   144   1  4  17600  21 14 25
21 17 25  ---          17 39 02  40.0   9.4 -2.4    -137.9   180   R  2  15200
  
21 18 25  2007+402     17 40 02  58.6  61.4 -2.5     -96.5    21   1  4  15200  21 18 25
21 19 00  ---          17 40 37  58.8  61.4 -2.5     -96.7    35   R  2  14733
  
21 19 00  IRAS2012     17 40 37  57.4  60.3 -2.6     -96.5    -5   1  4  14733  21 19 00
21 19 40  ---          17 41 18  57.5  60.2 -2.6     -96.6    35   R  2  14200
  
21 19 40  2007+402     17 41 18  58.9  61.3 -2.4     -96.8    -5   1  4  14200  21 19 40
21 20 10  ---          17 41 48  59.0  61.3 -2.4     -96.9    25   R  2  13800
  
21 20 10  IRAS2012     17 41 48  57.6  60.2 -2.5     -96.7    -5   1  4  13800  21 20 10
21 20 50  ---          17 42 28  57.8  60.2 -2.5     -96.9    35   R  2  13267
  
21 20 50  2007+402     17 42 28  59.1  61.3 -2.4     -97.0    -5   1  4  13267  21 20 50
21 21 20  ---          17 42 58  59.2  61.3 -2.4     -97.1    25   R  2  12867
  
21 21 20  IRAS2012     17 42 58  57.9  60.2 -2.5     -97.0    -5   1  4  12867  21 21 20
21 22 00  ---          17 43 38  58.0  60.2 -2.5     -97.1    35   R  2  12333
  
21 22 00  2007+402     17 43 38  59.3  61.2 -2.4     -97.3    -5   1  4  12333  21 22 00
21 22 30  ---          17 44 08  59.4  61.2 -2.4     -97.4    25   R  2  11933
  
21 22 30  IRAS2012     17 44 08  58.1  60.1 -2.5     -97.2    -5   1  4  11933  21 22 30
21 23 10  ---          17 44 48  58.2  60.1 -2.5     -97.3    35   R  2  11400
  
21 23 10  2007+402     17 44 48  59.5  61.2 -2.4     -97.5    -5   1  4  11400  21 23 10
21 23 40  ---          17 45 18  59.6  61.2 -2.4     -97.6    25   R  2  11000
  
21 23 40  IRAS2012     17 45 18  58.3  60.1 -2.5     -97.4    -5   1  4  11000  21 23 40
21 24 20  ---          17 45 58  58.4  60.0 -2.5     -97.6    35   R  2  10467
  
21 24 20  2007+402     17 45 58  59.8  61.1 -2.4     -97.7    -5   1  4  10467  21 24 20
21 24 50  ---          17 46 28  59.9  61.1 -2.4     -97.8    25   R  2  10067
  
21 24 50  IRAS2012     17 46 28  58.5  60.0 -2.5     -97.7    -5   1  4  10067  21 24 50
21 25 30  ---          17 47 09  58.6  60.0 -2.5     -97.8    35   R  2   9533
  
21 25 30  2007+402     17 47 09  60.0  61.1 -2.3     -98.0    -5   1  4   9533  21 25 30
21 26 00  ---          17 47 39  60.1  61.0 -2.3     -98.1    25   R  2   9133
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
21 26 00  IRAS2012     17 47 39  58.7  60.0 -2.4     -97.9    -5   1  4   9133  21 26 00
21 26 40  ---          17 48 19  58.8  59.9 -2.4     -98.1    35   R  2   8600
  
21 26 40  2007+402     17 48 19  60.2  61.0 -2.3     -98.2    -5   1  4   8600  21 26 40
21 27 10  ---          17 48 49  60.3  61.0 -2.3     -98.3    25   R  2   8200
  
21 28 10  IRAS2012     17 49 49  59.1  59.9 -2.4     -98.4    56   1  4   8200  21 28 10
21 28 55  ---          17 50 34  59.3  59.8 -2.4     -98.5    45   R  2   7600
  
21 29 55  2007+402     17 51 34  60.8  60.8 -2.3     -98.9    55   1  4   7600  21 29 55
21 30 30  ---          17 52 09  60.9  60.8 -2.3     -99.0    35   R  2   7133
  
21 30 30  IRAS2012     17 52 09  59.6  59.7 -2.4     -98.9    -5   1  4   7133  21 30 30
21 31 10  ---          17 52 49  59.7  59.7 -2.4     -99.0    35   R  2   6600
  
21 31 10  2007+402     17 52 49  61.1  60.7 -2.2     -99.2    -5   1  4   6600  21 31 10
21 31 40  ---          17 53 20  61.1  60.7 -2.2     -99.3    25   R  2   6200
  
21 31 40  IRAS2012     17 53 20  59.8  59.7 -2.4     -99.1    -5   1  4   6200  21 31 40
21 32 20  ---          17 54 00  59.9  59.6 -2.3     -99.3    35   R  2   5667
  
21 32 20  2007+402     17 54 00  61.3  60.7 -2.2     -99.4    -5   1  4   5667  21 32 20
21 32 50  ---          17 54 30  61.4  60.6 -2.2     -99.6    25   R  2   5267
  
21 32 50  IRAS2012     17 54 30  60.0  59.6 -2.3     -99.4    -5   1  4   5267  21 32 50
21 33 30  ---          17 55 10  60.1  59.5 -2.3     -99.5    35   R  2   4733
  
21 33 30  2007+402     17 55 10  61.5  60.6 -2.2     -99.7    -5   1  4   4733  21 33 30
21 34 00  ---          17 55 40  61.6  60.5 -2.2     -99.8    25   R  2   4333
  
21 34 00  IRAS2012     17 55 40  60.2  59.5 -2.3     -99.6    -5   1  4   4333  21 34 00
21 34 40  ---          17 56 20  60.3  59.5 -2.3     -99.8    35   R  2   3800
  
21 34 40  2007+402     17 56 20  61.7  60.5 -2.2    -100.0    -5   1  4   3800  21 34 40
21 35 10  ---          17 56 50  61.8  60.5 -2.2    -100.1    25   R  2   3400
  
21 35 10  IRAS2012     17 56 50  60.4  59.4 -2.3     -99.9    -5   1  4   3400  21 35 10
21 35 50  ---          17 57 30  60.6  59.4 -2.3    -100.0    35   R  2   2867
  
21 35 50  2007+402     17 57 30  61.9  60.4 -2.2    -100.2    -5   1  4   2867  21 35 50
21 36 20  ---          17 58 00  62.0  60.4 -2.2    -100.3    25   R  2   2467
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
21 36 20  IRAS2012     17 58 00  60.6  59.4 -2.3    -100.1    -5   1  4   2467  21 36 20
21 37 00  ---          17 58 40  60.8  59.3 -2.3    -100.3    35   R  2   1933
  
21 37 00  2007+402     17 58 40  62.1  60.3 -2.2    -100.5    -5   1  4   1933  21 37 00
21 37 30  ---          17 59 10  62.2  60.3 -2.1    -100.6    25   R  2   1533
  
21 37 30  IRAS2012     17 59 10  60.9  59.3 -2.3    -100.4    -5   1  4   1533  21 37 30
21 38 10  ---          17 59 51  61.0  59.2 -2.2    -100.6    35   R  2   1000
  
21 38 10  2007+402     17 59 51  62.4  60.2 -2.1    -100.8    -5   1  4   1000  21 38 10
21 38 40  ---          18 00 21  62.5  60.2 -2.1    -100.9    25   R  2    600
  
21 39 40  IRAS2012     18 01 21  61.3  59.1 -2.2    -100.9    56   1  4    600  21 39 40
21 40 25  ---          18 02 06  61.4  59.1 -2.2    -101.1    45   R  2      0
  
21 41 25  2002+472     18 03 06  61.7  45.1 -2.0    -115.7    49   1  5      0  21 41 25
21 44 25  ---          18 06 07  62.2  44.6 -1.9    -116.6   180   F  1   2400
  
21 45 25  2007+402     18 07 07  63.7  59.6 -2.0    -102.5    48   1  5   2400  21 45 08
21 46 00  ---          18 07 42  63.8  59.6 -2.0    -102.6    35   F  1   3093
  
21 46 00  IRAS2012     18 07 42  62.4  58.6 -2.1    -102.4    -5   1  5   3093  21 46 00
21 46 40  ---          18 08 22  62.6  58.6 -2.1    -102.6    35   F  1   3627
  
21 46 40  2007+402     18 08 22  64.0  59.5 -2.0    -102.8    -5   1  5   3627  21 46 40
21 47 10  ---          18 08 52  64.0  59.5 -2.0    -102.9    25   F  1   4027
  
21 47 10  IRAS2012     18 08 52  62.6  58.5 -2.1    -102.7    -5   1  5   4027  21 47 10
21 47 50  ---          18 09 32  62.8  58.4 -2.1    -102.8    35   F  1   4560
  
21 47 50  2007+402     18 09 32  64.2  59.4 -2.0    -103.1    -5   1  5   4560  21 47 50
21 48 20  ---          18 10 02  64.3  59.4 -2.0    -103.2    25   F  1   4960
  
21 48 20  IRAS2012     18 10 02  62.9  58.4 -2.1    -103.0    -5   1  5   4960  21 48 20
21 49 00  ---          18 10 42  63.0  58.3 -2.1    -103.1    35   F  1   5493
  
21 49 00  2007+402     18 10 42  64.4  59.3 -2.0    -103.4    -5   1  5   5493  21 49 00
21 49 30  ---          18 11 12  64.5  59.2 -1.9    -103.5    25   F  1   5893
  
21 49 30  IRAS2012     18 11 12  63.1  58.3 -2.1    -103.3    -5   1  5   5893  21 49 30
21 50 10  ---          18 11 53  63.2  58.2 -2.0    -103.4    35   F  1   6427
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
21 50 10  2007+402     18 11 53  64.6  59.2 -1.9    -103.7    -5   1  5   6427  21 50 10
21 50 40  ---          18 12 23  64.7  59.1 -1.9    -103.8    25   F  1   6827
  
21 50 40  IRAS2012     18 12 23  63.3  58.2 -2.0    -103.6    -5   1  5   6827  21 50 40
21 51 20  ---          18 13 03  63.4  58.1 -2.0    -103.7    35   F  1   7360
  
21 51 20  2007+402     18 13 03  64.8  59.0 -1.9    -104.0    -5   1  5   7360  21 51 20
21 51 50  ---          18 13 33  64.9  59.0 -1.9    -104.1    25   F  1   7760
  
21 51 50  IRAS2012     18 13 33  63.5  58.1 -2.0    -103.9    -5   1  5   7760  21 51 50
21 52 30  ---          18 14 13  63.6  58.0 -2.0    -104.0    35   F  1   8293
  
21 52 30  2007+402     18 14 13  65.0  58.9 -1.9    -104.3    -5   1  5   8293  21 52 30
21 53 00  ---          18 14 43  65.1  58.9 -1.9    -104.4    25   F  1   8693
  
21 54 00  IRAS2012     18 15 43  63.9  57.8 -2.0    -104.4    56   1  5   8693  21 53 42
21 54 45  ---          18 16 28  64.0  57.8 -2.0    -104.6    45   F  1   9533
  
21 55 45  2007+402     18 17 28  65.6  58.5 -1.8    -105.2    55   1  5   9533  21 55 27
21 56 20  ---          18 18 04  65.7  58.5 -1.8    -105.3    35   F  1  10240
  
21 56 20  IRAS2012     18 18 04  64.3  57.6 -1.9    -105.0    -5   1  5  10240  21 56 20
21 57 00  ---          18 18 44  64.4  57.5 -1.9    -105.2    35   F  1  10773
  
21 57 00  2007+402     18 18 44  65.9  58.4 -1.8    -105.5    -5   1  5  10773  21 57 00
21 57 30  ---          18 19 14  66.0  58.3 -1.8    -105.6    25   F  1  11173
  
21 57 30  IRAS2012     18 19 14  64.5  57.4 -1.9    -105.3    -5   1  5  11173  21 57 30
21 58 10  ---          18 19 54  64.7  57.4 -1.9    -105.5    35   F  1  11707
  
21 58 10  2007+402     18 19 54  66.1  58.2 -1.8    -105.8    -5   1  5  11707  21 58 10
21 58 40  ---          18 20 24  66.2  58.2 -1.8    -106.0    25   F  1  12107
  
21 58 40  IRAS2012     18 20 24  64.8  57.3 -1.9    -105.7    -5   1  5  12107  21 58 40
21 59 20  ---          18 21 04  64.9  57.2 -1.9    -105.8    35   F  1  12640
  
21 59 20  2007+402     18 21 04  66.3  58.1 -1.8    -106.2    -5   1  5  12640  21 59 20
21 59 50  ---          18 21 34  66.4  58.0 -1.8    -106.3    25   F  1  13040
  
21 59 50  IRAS2012     18 21 34  65.0  57.2 -1.9    -106.0    -5   1  5  13040  21 59 50
22 00 30  ---          18 22 14  65.1  57.1 -1.9    -106.2    35   F  1  13573
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
22 00 30  2007+402     18 22 14  66.5  57.9 -1.8    -106.5    -5   1  5  13573  22 00 30
22 01 00  ---          18 22 44  66.6  57.9 -1.8    -106.6    25   F  1  13973
  
22 01 00  IRAS2012     18 22 44  65.2  57.0 -1.9    -106.3    -5   1  5  13973  22 01 00
22 01 40  ---          18 23 24  65.3  56.9 -1.9    -106.5    35   F  1  14507
  
22 01 40  2007+402     18 23 24  66.7  57.8 -1.7    -106.8    -5   1  5  14507  22 01 40
22 02 10  ---          18 23 55  66.8  57.7 -1.7    -107.0    25   F  1  14907
  
22 02 10  IRAS2012     18 23 55  65.4  56.9 -1.8    -106.6    -5   1  5  14907  22 02 10
22 02 50  ---          18 24 35  65.5  56.8 -1.8    -106.8    35   F  1  15440
  
22 02 50  2007+402     18 24 35  66.9  57.6 -1.7    -107.2    -5   1  5  15440  22 02 50
22 03 20  ---          18 25 05  67.0  57.5 -1.7    -107.3    25   F  1  15840
  
22 03 20  IRAS2012     18 25 05  65.6  56.7 -1.8    -107.0    -5   1  5  15840  22 03 20
22 04 00  ---          18 25 45  65.7  56.6 -1.8    -107.2    35   F  1  16373
  
22 04 00  2007+402     18 25 45  67.1  57.4 -1.7    -107.5    -5   1  5  16373  22 04 00
22 04 30  ---          18 26 15  67.2  57.4 -1.7    -107.7    25   F  1  16773
  
22 05 30  IRAS2012     18 27 15  66.0  56.4 -1.8    -107.6    56   1  5  16773  22 05 13
22 06 15  ---          18 28 00  66.1  56.3 -1.8    -107.8    45   F  1  17600
  
22 07 15  2007+402     18 29 00  67.7  56.9 -1.6    -108.5    55   1  6  17600  22 07 15
22 08 00  ---          18 29 46  67.9  56.8 -1.6    -108.7    45   R  1  17000
  
22 08 00  IRAS2012     18 29 46  66.4  56.1 -1.7    -108.3    -5   1  6  17000  22 08 00
22 08 40  ---          18 30 26  66.6  56.0 -1.7    -108.5    35   R  1  16467
  
22 08 40  2007+402     18 30 26  68.0  56.7 -1.6    -109.0    -5   1  6  16467  22 08 40
22 09 10  ---          18 30 56  68.1  56.6 -1.6    -109.1    25   R  1  16067
  
22 09 10  IRAS2012     18 30 56  66.6  55.9 -1.7    -108.7    -5   1  6  16067  22 09 10
22 09 50  ---          18 31 36  66.8  55.8 -1.7    -108.9    35   R  1  15533
  
22 09 50  2007+402     18 31 36  68.2  56.5 -1.6    -109.3    -5   1  6  15533  22 09 50
22 10 20  ---          18 32 06  68.3  56.4 -1.6    -109.5    25   R  1  15133
  
22 10 20  IRAS2012     18 32 06  66.9  55.7 -1.7    -109.0    -5   1  6  15133  22 10 20
22 11 00  ---          18 32 46  67.0  55.6 -1.7    -109.3    35   R  1  14600
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
22 11 00  2007+402     18 32 46  68.4  56.3 -1.6    -109.7    -5   1  6  14600  22 11 00
22 11 30  ---          18 33 16  68.5  56.2 -1.6    -109.9    25   R  1  14200
  
22 11 30  IRAS2012     18 33 16  67.1  55.5 -1.7    -109.4    -5   1  6  14200  22 11 30
22 12 10  ---          18 33 56  67.2  55.4 -1.7    -109.6    35   R  1  13667
  
22 12 10  2007+402     18 33 56  68.6  56.1 -1.6    -110.1    -5   1  6  13667  22 12 10
22 12 40  ---          18 34 26  68.7  56.0 -1.6    -110.2    25   R  1  13267
  
22 12 40  IRAS2012     18 34 26  67.3  55.3 -1.7    -109.8    -5   1  6  13267  22 12 40
22 13 20  ---          18 35 06  67.4  55.2 -1.7    -110.0    35   R  1  12733
  
22 13 20  2007+402     18 35 06  68.8  55.9 -1.5    -110.5    -5   1  6  12733  22 13 20
22 13 50  ---          18 35 36  68.9  55.8 -1.5    -110.6    25   R  1  12333
  
22 13 50  IRAS2012     18 35 36  67.5  55.1 -1.6    -110.2    -5   1  6  12333  22 13 50
22 14 30  ---          18 36 17  67.6  55.0 -1.6    -110.4    35   R  1  11800
  
22 14 30  2007+402     18 36 17  69.0  55.7 -1.5    -110.9    -5   1  6  11800  22 14 30
22 15 00  ---          18 36 47  69.1  55.6 -1.5    -111.0    25   R  1  11400
  
22 15 00  IRAS2012     18 36 47  67.7  54.9 -1.6    -110.5    -5   1  6  11400  22 15 00
22 15 40  ---          18 37 27  67.8  54.8 -1.6    -110.7    35   R  1  10867
  
22 15 40  2007+402     18 37 27  69.2  55.4 -1.5    -111.3    -5   1  6  10867  22 15 40
22 16 10  ---          18 37 57  69.3  55.3 -1.5    -111.4    25   R  1  10467
  
22 16 10  IRAS2012     18 37 57  67.9  54.7 -1.6    -110.9    -5   1  6  10467  22 16 10
22 16 50  ---          18 38 37  68.0  54.6 -1.6    -111.1    35   R  1   9933
  
22 16 50  2007+402     18 38 37  69.4  55.2 -1.5    -111.7    -5   1  6   9933  22 16 50
22 17 20  ---          18 39 07  69.5  55.1 -1.5    -111.8    25   R  1   9533
  
22 18 20  IRAS2012     18 40 07  68.3  54.3 -1.6    -111.6    55   1  6   9533  22 18 20
22 19 15  ---          18 41 02  68.4  54.2 -1.6    -112.0    55   R  1   8800
  
22 20 15  2007+402     18 42 03  70.0  54.5 -1.4    -112.9    55   1  6   8800  22 20 15
22 21 00  ---          18 42 48  70.2  54.3 -1.4    -113.2    45   R  1   8200
  
22 21 00  IRAS2012     18 42 48  68.7  53.8 -1.5    -112.6    -5   1  6   8200  22 21 00
22 21 40  ---          18 43 28  68.8  53.7 -1.5    -112.8    35   R  1   7667
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
22 21 40  2007+402     18 43 28  70.3  54.2 -1.4    -113.4    -5   1  6   7667  22 21 40
22 22 10  ---          18 43 58  70.4  54.1 -1.4    -113.6    25   R  1   7267
  
22 22 10  IRAS2012     18 43 58  68.9  53.6 -1.5    -113.0    -5   1  6   7267  22 22 10
22 22 50  ---          18 44 38  69.0  53.4 -1.5    -113.2    35   R  1   6733
  
22 22 50  2007+402     18 44 38  70.5  53.9 -1.4    -113.9    -5   1  6   6733  22 22 50
22 23 20  ---          18 45 08  70.6  53.8 -1.4    -114.1    25   R  1   6333
  
22 23 20  IRAS2012     18 45 08  69.1  53.3 -1.5    -113.4    -5   1  6   6333  22 23 20
22 24 00  ---          18 45 48  69.3  53.2 -1.5    -113.6    35   R  1   5800
  
22 24 00  2007+402     18 45 48  70.7  53.6 -1.4    -114.3    -5   1  6   5800  22 24 00
22 24 30  ---          18 46 18  70.8  53.5 -1.4    -114.5    25   R  1   5400
  
22 24 30  IRAS2012     18 46 18  69.3  53.1 -1.5    -113.8    -5   1  6   5400  22 24 30
22 25 10  ---          18 46 58  69.5  52.9 -1.5    -114.1    35   R  1   4867
  
22 25 10  2007+402     18 46 58  70.9  53.4 -1.3    -114.8    -5   1  6   4867  22 25 10
22 25 40  ---          18 47 28  71.0  53.2 -1.3    -115.0    25   R  1   4467
  
22 25 40  IRAS2012     18 47 28  69.5  52.8 -1.4    -114.2    -5   1  6   4467  22 25 40
22 26 20  ---          18 48 09  69.7  52.7 -1.4    -114.5    35   R  1   3933
  
22 26 20  2007+402     18 48 09  71.1  53.1 -1.3    -115.2    -5   1  6   3933  22 26 20
22 26 50  ---          18 48 39  71.2  52.9 -1.3    -115.4    25   R  1   3533
  
22 26 50  IRAS2012     18 48 39  69.7  52.6 -1.4    -114.7    -5   1  6   3533  22 26 50
22 27 30  ---          18 49 19  69.9  52.4 -1.4    -114.9    35   R  1   3000
  
22 27 30  2007+402     18 49 19  71.3  52.8 -1.3    -115.7    -5   1  6   3000  22 27 30
22 28 00  ---          18 49 49  71.4  52.6 -1.3    -115.9    25   R  1   2600
  
22 28 00  IRAS2012     18 49 49  69.9  52.3 -1.4    -115.1    -5   1  6   2600  22 28 00
22 28 40  ---          18 50 29  70.1  52.1 -1.4    -115.4    35   R  1   2067
  
22 28 40  2007+402     18 50 29  71.5  52.5 -1.3    -116.2    -5   1  6   2067  22 28 40
22 29 10  ---          18 50 59  71.6  52.3 -1.3    -116.4    25   R  1   1667
  
22 29 10  IRAS2012     18 50 59  70.1  52.0 -1.4    -115.6    -5   1  6   1667  22 29 10
22 29 50  ---          18 51 39  70.3  51.9 -1.4    -115.8    35   R  1   1133
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
22 29 50  2007+402     18 51 39  71.7  52.2 -1.3    -116.7    -5   1  6   1133  22 29 50
22 30 20  ---          18 52 09  71.8  52.0 -1.3    -116.9    25   R  1    733
  
22 31 20  IRAS2012     18 53 09  70.5  51.5 -1.4    -116.4    55   1  6    733  22 31 20
22 32 15  ---          18 54 04  70.7  51.3 -1.3    -116.8    55   R  1      0
  
22 33 15  2007+402     18 55 05  72.3  51.2 -1.2    -118.1    55   1  5      0  22 33 15
22 34 00  ---          18 55 50  72.4  51.0 -1.2    -118.5    45   F  2    600
  
22 34 00  IRAS2012     18 55 50  71.0  50.8 -1.3    -117.5    -5   1  5    600  22 34 00
22 34 40  ---          18 56 30  71.1  50.6 -1.3    -117.8    35   F  2   1133
  
22 34 40  2007+402     18 56 30  72.5  50.8 -1.2    -118.8    -5   1  5   1133  22 34 40
22 35 10  ---          18 57 00  72.6  50.6 -1.2    -119.0    25   F  2   1533
  
22 35 10  IRAS2012     18 57 00  71.1  50.5 -1.3    -118.0    -5   1  5   1533  22 35 10
22 35 50  ---          18 57 40  71.3  50.3 -1.3    -118.3    35   F  2   2067
  
22 35 50  2007+402     18 57 40  72.7  50.4 -1.2    -119.3    -5   1  5   2067  22 35 50
22 36 20  ---          18 58 10  72.8  50.2 -1.2    -119.5    25   F  2   2467
  
22 36 20  IRAS2012     18 58 10  71.3  50.2 -1.3    -118.5    -5   1  5   2467  22 36 20
22 37 00  ---          18 58 50  71.5  50.0 -1.3    -118.8    35   F  2   3000
  
22 37 00  2007+402     18 58 50  72.9  50.0 -1.1    -119.9    -5   1  5   3000  22 37 00
22 37 30  ---          18 59 20  73.0  49.9 -1.1    -120.1    25   F  2   3400
  
22 37 30  IRAS2012     18 59 20  71.5  49.8 -1.3    -119.0    -5   1  5   3400  22 37 30
22 38 10  ---          19 00 00  71.6  49.6 -1.2    -119.3    35   F  2   3933
  
22 38 10  2007+402     19 00 00  73.1  49.6 -1.1    -120.4    -5   1  5   3933  22 38 10
22 38 40  ---          19 00 31  73.2  49.5 -1.1    -120.7    25   F  2   4333
  
22 38 40  IRAS2012     19 00 31  71.7  49.5 -1.2    -119.6    -5   1  5   4333  22 38 40
22 39 20  ---          19 01 11  71.8  49.3 -1.2    -119.8    35   F  2   4867
  
22 39 20  2007+402     19 01 11  73.3  49.3 -1.1    -121.0    -5   1  5   4867  22 39 20
22 39 50  ---          19 01 41  73.4  49.1 -1.1    -121.2    25   F  2   5267
  
22 39 50  IRAS2012     19 01 41  71.9  49.1 -1.2    -120.1    -5   1  5   5267  22 39 50
22 40 30  ---          19 02 21  72.0  48.9 -1.2    -120.4    35   F  2   5800
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
22 40 30  2007+402     19 02 21  73.5  48.9 -1.1    -121.6    -5   1  5   5800  22 40 30
22 41 00  ---          19 02 51  73.6  48.7 -1.1    -121.8    25   F  2   6200
  
22 41 00  IRAS2012     19 02 51  72.1  48.8 -1.2    -120.6    -5   1  5   6200  22 41 00
22 41 40  ---          19 03 31  72.2  48.6 -1.2    -120.9    35   F  2   6733
  
22 41 40  2007+402     19 03 31  73.7  48.4 -1.1    -122.1    -5   1  5   6733  22 41 40
22 42 10  ---          19 04 01  73.8  48.3 -1.1    -122.4    25   F  2   7133
  
22 42 10  IRAS2012     19 04 01  72.3  48.4 -1.2    -121.2    -5   1  5   7133  22 42 10
22 42 50  ---          19 04 41  72.4  48.2 -1.2    -121.5    35   F  2   7667
  
22 42 50  2007+402     19 04 41  73.9  48.0 -1.1    -122.7    -5   1  5   7667  22 42 50
22 43 20  ---          19 05 11  73.9  47.8 -1.0    -123.0    25   F  2   8067
  
22 44 20  IRAS2012     19 06 11  72.6  47.7 -1.1    -122.2    55   1  5   8067  22 44 20
22 45 15  ---          19 07 07  72.8  47.4 -1.1    -122.6    55   F  2   8800
  
22 46 15  2007+402     19 08 07  74.4  46.7 -1.0    -124.6    55   1  5   8800  22 46 15
22 47 00  ---          19 08 52  74.5  46.4 -1.0    -125.0    45   F  2   9400
  
22 47 00  IRAS2012     19 08 52  73.1  46.8 -1.1    -123.5    -5   1  5   9400  22 47 00
22 47 40  ---          19 09 32  73.2  46.5 -1.1    -123.9    35   F  2   9933
  
22 47 40  2007+402     19 09 32  74.6  46.1 -1.0    -125.4    -5   1  5   9933  22 47 40
22 48 10  ---          19 10 02  74.7  45.9 -1.0    -125.6    25   F  2  10333
  
22 48 10  IRAS2012     19 10 02  73.2  46.4 -1.1    -124.1    -5   1  5  10333  22 48 10
22 48 50  ---          19 10 42  73.4  46.1 -1.1    -124.5    35   F  2  10867
  
22 48 50  2007+402     19 10 42  74.8  45.6 -1.0    -126.0    -5   1  5  10867  22 48 50
22 49 20  ---          19 11 12  74.9  45.4  -.9    -126.3    25   F  2  11267
  
22 49 20  IRAS2012     19 11 12  73.4  45.9 -1.1    -124.7    -5   1  5  11267  22 49 20
22 50 00  ---          19 11 52  73.5  45.7 -1.0    -125.1    35   F  2  11800
  
22 50 00  2007+402     19 11 52  75.0  45.1  -.9    -126.7    -5   1  5  11800  22 50 00
22 50 30  ---          19 12 22  75.1  44.9  -.9    -127.0    25   F  2  12200
  
22 50 30  IRAS2012     19 12 22  73.6  45.5 -1.0    -125.3    -5   1  5  12200  22 50 30
22 51 10  ---          19 13 03  73.7  45.2 -1.0    -125.7    35   F  2  12733
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
22 51 10  2007+402     19 13 03  75.2  44.6  -.9    -127.4    -5   1  5  12733  22 51 10
22 51 40  ---          19 13 33  75.2  44.4  -.9    -127.7    25   F  2  13133
  
22 51 40  IRAS2012     19 13 33  73.8  45.0 -1.0    -126.0    -5   1  5  13133  22 51 40
22 52 20  ---          19 14 13  73.9  44.8 -1.0    -126.3    35   F  2  13667
  
22 52 20  2007+402     19 14 13  75.3  44.1  -.9    -128.1    -5   1  5  13667  22 52 20
22 52 50  ---          19 14 43  75.4  43.8  -.9    -128.4    25   F  2  14067
  
22 52 50  IRAS2012     19 14 43  74.0  44.6 -1.0    -126.6    -5   1  5  14067  22 52 50
22 53 30  ---          19 15 23  74.1  44.3 -1.0    -127.0    35   F  2  14600
  
22 53 30  2007+402     19 15 23  75.5  43.5  -.9    -128.8    -5   1  5  14600  22 53 30
22 54 00  ---          19 15 53  75.6  43.3  -.9    -129.1    25   F  2  15000
  
22 54 00  IRAS2012     19 15 53  74.1  44.1 -1.0    -127.3    -5   1  5  15000  22 54 00
22 54 40  ---          19 16 33  74.2  43.8 -1.0    -127.7    35   F  2  15533
  
22 54 40  2007+402     19 16 33  75.7  42.9  -.9    -129.6    -5   1  5  15533  22 54 40
22 55 10  ---          19 17 03  75.8  42.7  -.8    -129.9    25   F  2  15933
  
22 55 10  IRAS2012     19 17 03  74.3  43.6 -1.0    -127.9    -5   1  5  15933  22 55 10
22 55 50  ---          19 17 43  74.4  43.3  -.9    -128.3    35   F  2  16467
  
22 55 50  2007+402     19 17 43  75.9  42.4  -.8    -130.3    -5   1  5  16467  22 55 50
22 56 20  ---          19 18 13  75.9  42.1  -.8    -130.6    25   F  2  16867
  
22 57 20  IRAS2012     19 19 14  74.6  42.6  -.9    -129.2    55   1  5  16867  22 57 20
22 58 15  ---          19 20 09  74.8  42.2  -.9    -129.8    55   F  2  17600
  
23 00 15  2007+777     19 22 09  42.5   3.1  -.7    -167.3    53   1  6  17600  23 00 15
23 03 15  ---          19 25 10  42.5   2.9  -.7    -168.2   180   R  2  15200
  
23 05 15  2007+402     19 27 10  77.2  37.1  -.7    -137.0    49   1  6  15200  23 04 58
23 05 50  ---          19 27 45  77.2  36.7  -.7    -137.5    35   R  2  14507
  
23 05 50  IRAS2012     19 27 45  75.8  38.4  -.8    -134.7    -5   1  6  14507  23 05 50
23 06 30  ---          19 28 25  75.9  38.1  -.8    -135.1    35   R  2  13973
  
23 06 30  2007+402     19 28 25  77.3  36.3  -.7    -138.0    -5   1  6  13973  23 06 30
23 07 00  ---          19 28 55  77.4  35.9  -.6    -138.4    25   R  2  13573
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
23 07 00  IRAS2012     19 28 55  76.0  37.8  -.8    -135.5    -5   1  6  13573  23 07 00
23 07 40  ---          19 29 35  76.1  37.4  -.7    -136.0    35   R  2  13040
  
23 07 40  2007+402     19 29 35  77.5  35.5  -.6    -138.9    -5   1  6  13040  23 07 40
23 08 10  ---          19 30 05  77.5  35.2  -.6    -139.3    25   R  2  12640
  
23 08 10  IRAS2012     19 30 05  76.1  37.1  -.7    -136.3    -5   1  6  12640  23 08 10
23 08 50  ---          19 30 45  76.2  36.7  -.7    -136.8    35   R  2  12107
  
23 08 50  2007+402     19 30 45  77.6  34.7  -.6    -139.9    -5   1  6  12107  23 08 50
23 09 20  ---          19 31 16  77.7  34.4  -.6    -140.3    25   R  2  11707
  
23 09 20  IRAS2012     19 31 16  76.3  36.5  -.7    -137.2    -5   1  6  11707  23 09 20
23 10 00  ---          19 31 56  76.4  36.1  -.7    -137.7    35   R  2  11173
  
23 10 00  2007+402     19 31 56  77.7  33.9  -.6    -140.9    -5   1  6  11173  23 10 00
23 10 30  ---          19 32 26  77.8  33.6  -.6    -141.3    25   R  2  10773
  
23 10 30  IRAS2012     19 32 26  76.4  35.8  -.7    -138.0    -5   1  6  10773  23 10 30
23 11 10  ---          19 33 06  76.5  35.4  -.7    -138.5    35   R  2  10240
  
23 11 10  2007+402     19 33 06  77.9  33.1  -.6    -141.8    -5   1  6  10240  23 11 10
23 11 40  ---          19 33 36  77.9  32.7  -.6    -142.3    25   R  2   9840
  
23 11 40  IRAS2012     19 33 36  76.6  35.1  -.7    -138.9    -5   1  6   9840  23 11 40
23 12 20  ---          19 34 16  76.7  34.6  -.7    -139.4    35   R  2   9307
  
23 12 20  2007+402     19 34 16  78.0  32.2  -.6    -142.9    -5   1  6   9307  23 12 20
23 12 50  ---          19 34 46  78.1  31.9  -.5    -143.3    25   R  2   8907
  
23 13 50  IRAS2012     19 35 46  76.8  33.7  -.6    -140.6    56   1  6   8907  23 13 32
23 14 35  ---          19 36 31  76.9  33.2  -.6    -141.2    45   R  2   8067
  
23 15 35  2007+402     19 37 32  78.4  29.8  -.5    -145.8    55   1  6   8067  23 15 17
23 16 10  ---          19 38 07  78.4  29.3  -.5    -146.3    35   R  2   7360
  
23 16 10  IRAS2012     19 38 07  77.1  32.2  -.6    -142.5    -5   1  6   7360  23 16 10
23 16 50  ---          19 38 47  77.2  31.7  -.6    -143.0    35   R  2   6827
  
23 16 50  2007+402     19 38 47  78.5  28.8  -.5    -147.0    -5   1  6   6827  23 16 50
23 17 20  ---          19 39 17  78.6  28.4  -.5    -147.5    25   R  2   6427
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
23 17 20  IRAS2012     19 39 17  77.2  31.4  -.6    -143.4    -5   1  6   6427  23 17 20
23 18 00  ---          19 39 57  77.3  30.9  -.6    -144.0    35   R  2   5893
  
23 18 00  2007+402     19 39 57  78.6  27.8  -.5    -148.1    -5   1  6   5893  23 18 00
23 18 30  ---          19 40 27  78.7  27.4  -.5    -148.6    25   R  2   5493
  
23 18 30  IRAS2012     19 40 27  77.4  30.6  -.6    -144.4    -5   1  6   5493  23 18 30
23 19 10  ---          19 41 07  77.5  30.1  -.6    -145.0    35   R  2   4960
  
23 19 10  2007+402     19 41 07  78.8  26.9  -.4    -149.2    -5   1  6   4960  23 19 10
23 19 40  ---          19 41 37  78.8  26.5  -.4    -149.7    25   R  2   4560
  
23 19 40  IRAS2012     19 41 37  77.5  29.7  -.5    -145.4    -5   1  6   4560  23 19 40
23 20 20  ---          19 42 17  77.6  29.3  -.5    -146.0    35   R  2   4027
  
23 20 20  2007+402     19 42 17  78.9  25.9  -.4    -150.4    -5   1  6   4027  23 20 20
23 20 50  ---          19 42 47  78.9  25.5  -.4    -150.9    25   R  2   3627
  
23 20 50  IRAS2012     19 42 47  77.6  28.9  -.5    -146.4    -5   1  6   3627  23 20 50
23 21 30  ---          19 43 28  77.7  28.4  -.5    -147.0    35   R  2   3093
  
23 21 30  2007+402     19 43 28  79.0  24.9  -.4    -151.6    -5   1  6   3093  23 21 30
23 22 00  ---          19 43 58  79.0  24.4  -.4    -152.1    25   R  2   2693
  
23 22 00  IRAS2012     19 43 58  77.7  28.0  -.5    -147.5    -5   1  6   2693  23 22 00
23 22 40  ---          19 44 38  77.8  27.5  -.5    -148.1    35   R  2   2160
  
23 22 40  2007+402     19 44 38  79.1  23.8  -.4    -152.8    -5   1  6   2160  23 22 40
23 23 10  ---          19 45 08  79.1  23.4  -.4    -153.3    25   R  2   1760
  
23 23 10  IRAS2012     19 45 08  77.9  27.2  -.5    -148.5    -5   1  6   1760  23 23 10
23 23 50  ---          19 45 48  77.9  26.6  -.5    -149.1    35   R  2   1227
  
23 23 50  2007+402     19 45 48  79.2  22.8  -.4    -154.0    -5   1  6   1227  23 23 50
23 24 20  ---          19 46 18  79.2  22.3  -.4    -154.5    25   R  2    827
  
23 25 20  IRAS2012     19 47 18  78.1  25.5  -.5    -150.5    56   1  6    827  23 25 03
23 26 05  ---          19 48 03  78.1  24.9  -.4    -151.2    45   R  2      0
  
23 27 05  2002+472     19 49 03  73.0   7.6  -.2    -170.3    47   1  7      0  23 27 05
23 30 05  ---          19 52 04  73.1   5.9  -.2    -172.5   180   F  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
23 31 05  2007+402     19 53 04  79.7  15.8  -.2    -162.1    45   1  7   2400  23 30 48
23 31 40  ---          19 53 39  79.7  15.2  -.2    -162.7    35   F  1   3093
  
23 31 40  IRAS2012     19 53 39  78.6  20.2  -.3    -156.8    -5   1  7   3093  23 31 40
23 32 20  ---          19 54 19  78.7  19.6  -.3    -157.5    35   F  1   3627
  
23 32 20  2007+402     19 54 19  79.8  14.5  -.2    -163.5    -5   1  7   3627  23 32 20
23 32 50  ---          19 54 49  79.8  14.0  -.2    -164.1    25   F  1   4027
  
23 32 50  IRAS2012     19 54 49  78.7  19.1  -.3    -158.0    -5   1  7   4027  23 32 50
23 33 30  ---          19 55 30  78.7  18.5  -.3    -158.7    35   F  1   4560
  
23 33 30  2007+402     19 55 30  79.8  13.3  -.2    -164.9    -5   1  7   4560  23 33 30
23 34 00  ---          19 56 00  79.8  12.8  -.2    -165.5    25   F  1   4960
  
23 34 00  IRAS2012     19 56 00  78.8  18.1  -.3    -159.2    -6   1  7   4960  23 34 00
23 34 40  ---          19 56 40  78.8  17.5  -.3    -159.9    34   F  1   5493
  
23 34 40  2007+402     19 56 40  79.9  12.1  -.2    -166.3    -6   1  7   5493  23 34 40
23 35 10  ---          19 57 10  79.9  11.6  -.2    -166.9    24   F  1   5893
  
23 35 10  IRAS2012     19 57 10  78.8  17.0  -.3    -160.4    -6   1  7   5893  23 35 10
23 35 50  ---          19 57 50  78.9  16.4  -.3    -161.1    34   F  1   6427
  
23 35 50  2007+402     19 57 50  79.9  10.9  -.2    -167.7    -6   1  7   6427  23 35 50
23 36 20  ---          19 58 20  79.9  10.3  -.2    -168.3    24   F  1   6827
  
23 36 20  IRAS2012     19 58 20  78.9  15.9  -.3    -161.7    -6   1  7   6827  23 36 20
23 37 00  ---          19 59 00  79.0  15.3  -.3    -162.4    34   F  1   7360
  
23 37 00  2007+402     19 59 00  80.0   9.6  -.1    -169.1    -6   1  7   7360  23 37 00
23 37 30  ---          19 59 30  80.0   9.1  -.1    -169.7    24   F  1   7760
  
23 37 30  IRAS2012     19 59 30  79.0  14.9  -.2    -162.9    -6   1  7   7760  23 37 30
23 38 10  ---          20 00 10  79.0  14.2  -.2    -163.7    34   F  1   8293
  
23 38 10  2007+402     20 00 10  80.0   8.3  -.1    -170.5    -6   1  7   8293  23 38 10
23 38 40  ---          20 00 40  80.0   7.8  -.1    -171.2    24   F  1   8693
  
23 39 40  IRAS2012     20 01 41  79.1  12.8  -.2    -165.3    55   1  7   8693  23 39 22
23 40 25  ---          20 02 26  79.1  12.1  -.2    -166.2    45   F  1   9533
Schedule for VLBA_FD   (Code Fd )                                   Page  32
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
23 41 25  2007+402     20 03 26  80.1   4.8  -.1    -174.6    53   1  7   9533  23 41 07
23 42 00  ---          20 04 01  80.1   4.1  -.1    -175.3    35   F  1  10240
  
23 42 00  IRAS2012     20 04 01  79.2  10.5  -.2    -167.9    -6   1  7  10240  23 42 00
23 42 40  ---          20 04 41  79.2   9.9  -.2    -168.7    34   F  1  10773
  
23 42 40  2007+402     20 04 41  80.1   3.4  -.1    -176.1    -6   1  7  10773  23 42 40
23 43 10  ---          20 05 11  80.1   2.9   .0    -176.8    24   F  1  11173
  
23 43 10  IRAS2012     20 05 11  79.2   9.4  -.2    -169.3    -6   1  7  11173  23 43 10
23 43 50  ---          20 05 51  79.3   8.7  -.1    -170.0    34   F  1  11707
  
23 43 50  2007+402     20 05 51  80.1   2.1   .0    -177.6    -6   1  7  11707  23 43 50
23 44 20  ---          20 06 21  80.1   1.6   .0    -178.2    24   F  1  12107
  
23 44 20  IRAS2012     20 06 21  79.3   8.2  -.1    -170.6    -6   1  7  12107  23 44 20
23 45 00  ---          20 07 01  79.3   7.5  -.1    -171.4    34   F  1  12640
  
23 45 00  2007+402     20 07 01  80.1    .8   .0    -179.1    -6   1  7  12640  23 45 00
23 45 30  ---          20 07 32  80.1    .3   .0    -179.7    24   F  1  13040
  
23 45 30  IRAS2012     20 07 32  79.3   7.0  -.1    -172.0    -7   1  7  13040  23 45 30
23 46 10  ---          20 08 12  79.3   6.4  -.1    -172.7    33   F  1  13573
  
23 46 10  2007+402     20 08 12  80.1   -.5   .0     179.5    -7   1  7  13573  23 46 10
23 46 40  ---          20 08 42  80.1  -1.0   .0     178.8    23   F  1  13973
  
23 46 40  IRAS2012     20 08 42  79.3   5.9  -.1    -173.3    -7   1  7  13973  23 46 40
23 47 20  ---          20 09 22  79.4   5.2  -.1    -174.1    33   F  1  14507
  
23 47 20  2007+402     20 09 22  80.1  -1.8   .0     178.0    -7   1  7  14507  23 47 20
23 47 50  ---          20 09 52  80.1  -2.3   .0     177.4    23   F  1  14907
  
23 47 50  IRAS2012     20 09 52  79.4   4.7  -.1    -174.7    -7   1  7  14907  23 47 50
23 48 30  ---          20 10 32  79.4   4.0  -.1    -175.4    33   F  1  15440
  
23 48 30  2007+402     20 10 32  80.1  -3.1   .0     176.5    -7   1  7  15440  23 48 30
23 49 00  ---          20 11 02  80.1  -3.6   .1     175.9    23   F  1  15840
  
23 49 00  IRAS2012     20 11 02  79.4   3.5  -.1    -176.0    -7   1  7  15840  23 49 00
23 49 40  ---          20 11 42  79.4   2.8   .0    -176.8    33   F  1  16373
Schedule for VLBA_FD   (Code Fd )                                   Page  33
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Thu   9 Nov 2000   Day 314 ---
  
23 49 40  2007+402     20 11 42  80.1  -4.4   .1     175.1    -7   1  7  16373  23 49 40
23 50 10  ---          20 12 12  80.1  -4.9   .1     174.4    23   F  1  16773
  
23 51 10  IRAS2012     20 13 12  79.4   1.3   .0    -178.6    54   1  7  16773  23 50 53
23 51 55  ---          20 13 58  79.4    .5   .0    -179.4    45   F  1  17600
  
23 52 55  2007+402     20 14 58  80.0  -7.9   .1     171.0    52   1  8  17600  23 52 55
23 53 40  ---          20 15 43  80.0  -8.7   .1     170.1    45   R  1  17000
  
23 53 40  IRAS2012     20 15 43  79.4  -1.3   .0     178.5    -7   1  8  17000  23 53 40
23 54 20  ---          20 16 23  79.4  -2.0   .0     177.7    33   R  1  16467
  
23 54 20  2007+402     20 16 23  80.0  -9.5   .1     169.3    -7   1  8  16467  23 54 20
23 54 50  ---          20 16 53  80.0 -10.0   .2     168.7    23   R  1  16067
  
23 54 50  IRAS2012     20 16 53  79.4  -2.5   .0     177.1    -7   1  8  16067  23 54 50
23 55 30  ---          20 17 33  79.4  -3.2   .1     176.4    33   R  1  15533
  
23 55 30  2007+402     20 17 33  79.9 -10.7   .2     167.9    -7   1  8  15533  23 55 30
23 56 00  ---          20 18 03  79.9 -11.2   .2     167.3    23   R  1  15133
  
23 56 00  IRAS2012     20 18 03  79.4  -3.7   .1     175.8    -7   1  8  15133  23 56 00
23 56 40  ---          20 18 43  79.4  -4.4   .1     175.0    33   R  1  14600
  
23 56 40  2007+402     20 18 43  79.9 -11.9   .2     166.5    -7   1  8  14600  23 56 40
23 57 10  ---          20 19 13  79.9 -12.5   .2     165.9    23   R  1  14200
  
23 57 10  IRAS2012     20 19 13  79.4  -4.9   .1     174.4    -7   1  8  14200  23 57 10
23 57 50  ---          20 19 54  79.3  -5.5   .1     173.6    33   R  1  13667
  
23 57 50  2007+402     20 19 54  79.8 -13.2   .2     165.1    -7   1  8  13667  23 57 50
23 58 20  ---          20 20 24  79.8 -13.7   .2     164.5    23   R  1  13267
  
23 58 20  IRAS2012     20 20 24  79.3  -6.1   .1     173.1    -7   1  8  13267  23 58 20
23 59 00  ---          20 21 04  79.3  -6.7   .1     172.3    33   R  1  12733
  
23 59 00  2007+402     20 21 04  79.8 -14.4   .2     163.7    -7   1  8  12733  23 59 00
23 59 30  ---          20 21 34  79.7 -14.9   .2     163.1    23   R  1  12333
  
 --- Start: Thu   9 Nov 2000   Day 314 -- Stop: Fri  10 Nov 2000   Day 315 ---
  
23 59 30  IRAS2012     20 21 34  79.3  -7.2   .1     171.7    -7   1  8  12333  23 59 30
00 00 10  ---          20 22 14  79.3  -7.9   .1     171.0    33   R  1  11800
Schedule for VLBA_FD   (Code Fd )                                   Page  34
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
00 00 10  2007+402     20 22 14  79.7 -15.6   .2     162.3    -7   1  8  11800  00 00 10
00 00 40  ---          20 22 44  79.7 -16.1   .2     161.7    23   R  1  11400
  
00 00 40  IRAS2012     20 22 44  79.3  -8.4   .1     170.4    -7   1  8  11400  00 00 40
00 01 20  ---          20 23 24  79.2  -9.1   .1     169.6    33   R  1  10867
  
00 01 20  2007+402     20 23 24  79.6 -16.8   .3     161.0    -7   1  8  10867  00 01 20
00 01 50  ---          20 23 54  79.6 -17.3   .3     160.4    23   R  1  10467
  
00 01 50  IRAS2012     20 23 54  79.2  -9.6   .2     169.0    -7   1  8  10467  00 01 50
00 02 30  ---          20 24 34  79.2 -10.2   .2     168.3    33   R  1   9933
  
00 02 30  2007+402     20 24 34  79.6 -17.9   .3     159.6    -7   1  8   9933  00 02 30
00 03 00  ---          20 25 04  79.5 -18.4   .3     159.1    23   R  1   9533
  
00 04 00  IRAS2012     20 26 05  79.1 -11.7   .2     166.6    54   1  8   9533  00 04 00
00 04 55  ---          20 27 00  79.1 -12.6   .2     165.6    55   R  1   8800
  
00 05 55  2007+402     20 28 00  79.3 -21.2   .3     155.8    52   1  8   8800  00 05 55
00 06 40  ---          20 28 45  79.3 -21.9   .3     155.0    45   R  1   8200
  
00 06 40  IRAS2012     20 28 45  79.0 -14.3   .2     163.6    -7   1  8   8200  00 06 40
00 07 20  ---          20 29 25  79.0 -14.9   .2     162.9    33   R  1   7667
  
00 07 20  2007+402     20 29 25  79.2 -22.5   .4     154.3    -7   1  8   7667  00 07 20
00 07 50  ---          20 29 55  79.2 -23.0   .4     153.8    23   R  1   7267
  
00 07 50  IRAS2012     20 29 55  79.0 -15.4   .3     162.4    -7   1  8   7267  00 07 50
00 08 30  ---          20 30 35  78.9 -16.0   .3     161.6    33   R  1   6733
  
00 08 30  2007+402     20 30 35  79.1 -23.6   .4     153.1    -7   1  8   6733  00 08 30
00 09 00  ---          20 31 05  79.1 -24.0   .4     152.6    23   R  1   6333
  
00 09 00  IRAS2012     20 31 05  78.9 -16.4   .3     161.1    -7   1  8   6333  00 09 00
00 09 40  ---          20 31 45  78.8 -17.1   .3     160.4    33   R  1   5800
  
00 09 40  2007+402     20 31 45  79.0 -24.6   .4     151.9    -7   1  8   5800  00 09 40
00 10 10  ---          20 32 16  79.0 -25.0   .4     151.4    23   R  1   5400
  
00 10 10  IRAS2012     20 32 16  78.8 -17.5   .3     159.9    -7   1  8   5400  00 10 10
00 10 50  ---          20 32 56  78.8 -18.1   .3     159.2    33   R  1   4867
Schedule for VLBA_FD   (Code Fd )                                   Page  35
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
00 10 50  2007+402     20 32 56  78.9 -25.6   .4     150.7    -7   1  8   4867  00 10 50
00 11 20  ---          20 33 26  78.8 -26.1   .4     150.2    23   R  1   4467
  
00 11 20  IRAS2012     20 33 26  78.7 -18.6   .3     158.6    -7   1  8   4467  00 11 20
00 12 00  ---          20 34 06  78.7 -19.2   .3     157.9    33   R  1   3933
  
00 12 00  2007+402     20 34 06  78.8 -26.6   .4     149.5    -7   1  8   3933  00 12 00
00 12 30  ---          20 34 36  78.7 -27.0   .4     149.0    23   R  1   3533
  
00 12 30  IRAS2012     20 34 36  78.6 -19.6   .3     157.4    -7   1  8   3533  00 12 30
00 13 10  ---          20 35 16  78.6 -20.2   .3     156.7    33   R  1   3000
  
00 13 10  2007+402     20 35 16  78.7 -27.6   .5     148.4    -7   1  8   3000  00 13 10
00 13 40  ---          20 35 46  78.6 -28.0   .5     147.9    23   R  1   2600
  
00 13 40  IRAS2012     20 35 46  78.6 -20.6   .4     156.2    -7   1  8   2600  00 13 40
00 14 20  ---          20 36 26  78.5 -21.2   .4     155.5    33   R  1   2067
  
00 14 20  2007+402     20 36 26  78.5 -28.6   .5     147.3    -7   1  8   2067  00 14 20
00 14 50  ---          20 36 56  78.5 -29.0   .5     146.8    23   R  1   1667
  
00 14 50  IRAS2012     20 36 56  78.5 -21.6   .4     155.0    -7   1  8   1667  00 14 50
00 15 30  ---          20 37 36  78.4 -22.2   .4     154.4    33   R  1   1133
  
00 15 30  2007+402     20 37 36  78.4 -29.5   .5     146.2    -7   1  8   1133  00 15 30
00 16 00  ---          20 38 07  78.4 -29.9   .5     145.7    23   R  1    733
  
00 17 00  IRAS2012     20 39 07  78.3 -23.5   .4     152.9    54   1  8    733  00 17 00
00 17 55  ---          20 40 02  78.2 -24.2   .4     152.0    55   R  1      0
  
00 18 40  2007+402     20 40 47  78.1 -31.9   .6     143.3    38   1  7      0  00 18 40
00 19 25  ---          20 41 32  78.0 -32.5   .6     142.6    45   F  2    600
  
00 19 25  IRAS2012     20 41 32  78.1 -25.4   .5     150.6    -7   1  7    600  00 19 25
00 20 05  ---          20 42 12  78.0 -26.0   .5     150.0    33   F  2   1133
  
00 20 05  2007+402     20 42 12  77.9 -32.9   .6     142.0    -7   1  7   1133  00 20 05
00 20 35  ---          20 42 42  77.9 -33.3   .6     141.6    23   F  2   1533
  
00 20 35  IRAS2012     20 42 42  78.0 -26.3   .5     149.5    -7   1  7   1533  00 20 35
00 21 15  ---          20 43 22  77.9 -26.9   .5     148.9    33   F  2   2067
Schedule for VLBA_FD   (Code Fd )                                   Page  36
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
00 21 15  2007+402     20 43 22  77.8 -33.8   .6     141.0    -7   1  7   2067  00 21 15
00 21 45  ---          20 43 52  77.7 -34.1   .6     140.6    23   F  2   2467
  
00 21 45  IRAS2012     20 43 52  77.9 -27.2   .5     148.4    -7   1  7   2467  00 21 45
00 22 25  ---          20 44 33  77.8 -27.7   .5     147.8    33   F  2   3000
  
00 22 25  2007+402     20 44 33  77.6 -34.6   .6     140.1    -7   1  7   3000  00 22 25
00 22 55  ---          20 45 03  77.6 -34.9   .6     139.6    23   F  2   3400
  
00 22 55  IRAS2012     20 45 03  77.7 -28.1   .5     147.4    -7   1  7   3400  00 22 55
00 23 35  ---          20 45 43  77.7 -28.6   .5     146.8    33   F  2   3933
  
00 23 35  2007+402     20 45 43  77.5 -35.4   .6     139.1    -6   1  7   3933  00 23 35
00 24 05  ---          20 46 13  77.4 -35.7   .6     138.7    24   F  2   4333
  
00 24 05  IRAS2012     20 46 13  77.6 -29.0   .5     146.3    -6   1  7   4333  00 24 05
00 24 45  ---          20 46 53  77.5 -29.5   .5     145.7    34   F  2   4867
  
00 24 45  2007+402     20 46 53  77.3 -36.1   .7     138.2    -6   1  7   4867  00 24 45
00 25 15  ---          20 47 23  77.3 -36.4   .7     137.8    24   F  2   5267
  
00 25 15  IRAS2012     20 47 23  77.5 -29.8   .5     145.3    -6   1  7   5267  00 25 15
00 25 55  ---          20 48 03  77.4 -30.3   .6     144.7    34   F  2   5800
  
00 25 55  2007+402     20 48 03  77.2 -36.9   .7     137.2    -6   1  7   5800  00 25 55
00 26 25  ---          20 48 33  77.1 -37.2   .7     136.9    24   F  2   6200
  
00 26 25  IRAS2012     20 48 33  77.4 -30.7   .6     144.3    -6   1  7   6200  00 26 25
00 27 05  ---          20 49 13  77.3 -31.1   .6     143.8    34   F  2   6733
  
00 27 05  2007+402     20 49 13  77.0 -37.6   .7     136.3    -6   1  7   6733  00 27 05
00 27 35  ---          20 49 43  77.0 -37.9   .7     136.0    24   F  2   7133
  
00 27 35  IRAS2012     20 49 43  77.2 -31.5   .6     143.3    -6   1  7   7133  00 27 35
00 28 15  ---          20 50 24  77.2 -31.9   .6     142.8    34   F  2   7667
  
00 28 15  2007+402     20 50 24  76.9 -38.3   .7     135.5    -6   1  7   7667  00 28 15
00 28 45  ---          20 50 54  76.8 -38.6   .7     135.1    24   F  2   8067
  
00 28 45  IRAS2012     20 50 54  77.1 -32.3   .6     142.4    -6   1  7   8067  00 28 45
00 29 40  ---          20 51 49  77.0 -32.9   .6     141.6    49   F  2   8800
Schedule for VLBA_FD   (Code Fd )                                   Page  37
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
00 29 40  2007+402     20 51 49  76.7 -39.1   .7     134.4    -6   1  7   8800  00 29 40
00 30 25  ---          20 52 34  76.6 -39.6   .7     133.9    39   F  2   9400
  
00 30 25  IRAS2012     20 52 34  76.9 -33.3   .6     141.0    -6   1  7   9400  00 30 25
00 31 05  ---          20 53 14  76.8 -33.8   .6     140.5    34   F  2   9933
  
00 31 05  2007+402     20 53 14  76.5 -39.9   .8     133.4    -6   1  7   9933  00 31 05
00 31 35  ---          20 53 44  76.4 -40.2   .8     133.1    24   F  2  10333
  
00 31 35  IRAS2012     20 53 44  76.8 -34.1   .7     140.1    -6   1  7  10333  00 31 35
00 32 15  ---          20 54 24  76.7 -34.5   .7     139.6    34   F  2  10867
  
00 32 15  2007+402     20 54 24  76.3 -40.6   .8     132.6    -6   1  7  10867  00 32 15
00 32 45  ---          20 54 54  76.3 -40.9   .8     132.2    24   F  2  11267
  
00 32 45  IRAS2012     20 54 54  76.6 -34.8   .7     139.2    -6   1  7  11267  00 32 45
00 33 25  ---          20 55 34  76.5 -35.2   .7     138.7    34   F  2  11800
  
00 33 25  2007+402     20 55 34  76.2 -41.2   .8     131.8    -6   1  7  11800  00 33 25
00 33 55  ---          20 56 04  76.1 -41.5   .8     131.4    24   F  2  12200
  
00 33 55  IRAS2012     20 56 04  76.5 -35.5   .7     138.3    -6   1  7  12200  00 33 55
00 34 35  ---          20 56 45  76.4 -35.9   .7     137.8    34   F  2  12733
  
00 34 35  2007+402     20 56 45  76.0 -41.8   .8     131.0    -6   1  7  12733  00 34 35
00 35 05  ---          20 57 15  75.9 -42.1   .8     130.7    24   F  2  13133
  
00 35 05  IRAS2012     20 57 15  76.3 -36.2   .7     137.5    -6   1  7  13133  00 35 05
00 35 45  ---          20 57 55  76.2 -36.6   .7     137.0    34   F  2  13667
  
00 35 45  2007+402     20 57 55  75.8 -42.4   .8     130.2    -6   1  7  13667  00 35 45
00 36 15  ---          20 58 25  75.8 -42.7   .8     129.9    24   F  2  14067
  
00 36 15  IRAS2012     20 58 25  76.2 -36.9   .7     136.6    -6   1  7  14067  00 36 15
00 36 55  ---          20 59 05  76.1 -37.3   .7     136.1    34   F  2  14600
  
00 36 55  2007+402     20 59 05  75.7 -43.0   .9     129.5    -6   1  7  14600  00 36 55
00 37 25  ---          20 59 35  75.6 -43.2   .9     129.2    24   F  2  15000
  
00 37 25  IRAS2012     20 59 35  76.0 -37.6   .8     135.8    -6   1  7  15000  00 37 25
00 38 05  ---          21 00 15  75.9 -37.9   .8     135.3    34   F  2  15533
Schedule for VLBA_FD   (Code Fd )                                   Page  38
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
00 38 05  2007+402     21 00 15  75.5 -43.6   .9     128.7    -6   1  7  15533  00 38 05
00 38 35  ---          21 00 45  75.4 -43.8   .9     128.4    24   F  2  15933
  
00 38 35  IRAS2012     21 00 45  75.9 -38.2   .8     134.9    -6   1  7  15933  00 38 35
00 39 15  ---          21 01 25  75.8 -38.6   .8     134.5    34   F  2  16467
  
00 39 15  2007+402     21 01 25  75.3 -44.1   .9     128.0    -6   1  7  16467  00 39 15
00 39 45  ---          21 01 55  75.2 -44.3   .9     127.7    24   F  2  16867
  
00 39 45  IRAS2012     21 01 55  75.7 -38.8   .8     134.1    -6   1  7  16867  00 39 45
00 40 40  ---          21 02 51  75.6 -39.3   .8     133.5    49   F  2  17600
  
00 42 40  2007+777     21 04 51  42.3  -4.2  1.0     162.7    51   1  8  17600  00 42 40
00 45 40  ---          21 07 51  42.2  -4.4  1.0     161.8   180   R  2  15200
  
00 47 40  2007+402     21 09 52  74.0 -47.6  1.0     123.2    54   1  8  15200  00 47 40
00 48 15  ---          21 10 27  73.9 -47.9  1.0     122.9    35   R  2  14733
  
00 48 15  IRAS2012     21 10 27  74.5 -43.0   .9     128.7    -5   1  8  14733  00 48 15
00 48 55  ---          21 11 07  74.4 -43.3   .9     128.4    35   R  2  14200
  
00 48 55  2007+402     21 11 07  73.8 -48.1  1.1     122.6    -5   1  8  14200  00 48 55
00 49 25  ---          21 11 37  73.7 -48.3  1.1     122.3    25   R  2  13800
  
00 49 25  IRAS2012     21 11 37  74.3 -43.5  1.0     128.1    -5   1  8  13800  00 49 25
00 50 05  ---          21 12 17  74.2 -43.8  1.0     127.7    35   R  2  13267
  
00 50 05  2007+402     21 12 17  73.6 -48.5  1.1     122.0    -5   1  8  13267  00 50 05
00 50 35  ---          21 12 47  73.5 -48.7  1.1     121.7    25   R  2  12867
  
00 50 35  IRAS2012     21 12 47  74.2 -44.0  1.0     127.4    -5   1  8  12867  00 50 35
00 51 15  ---          21 13 27  74.1 -44.3  1.0     127.0    35   R  2  12333
  
00 51 15  2007+402     21 13 27  73.4 -49.0  1.1     121.4    -5   1  8  12333  00 51 15
00 51 45  ---          21 13 57  73.4 -49.1  1.1     121.2    25   R  2  11933
  
00 51 45  IRAS2012     21 13 57  74.0 -44.5  1.0     126.7    -5   1  8  11933  00 51 45
00 52 25  ---          21 14 38  73.9 -44.7  1.0     126.4    35   R  2  11400
  
00 52 25  2007+402     21 14 38  73.2 -49.4  1.1     120.8    -5   1  8  11400  00 52 25
00 52 55  ---          21 15 08  73.2 -49.5  1.1     120.6    25   R  2  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  39
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
00 52 55  IRAS2012     21 15 08  73.8 -44.9  1.0     126.1    -5   1  8  11000  00 52 55
00 53 35  ---          21 15 48  73.7 -45.2  1.0     125.7    35   R  2  10467
  
00 53 35  2007+402     21 15 48  73.1 -49.7  1.1     120.3    -5   1  8  10467  00 53 35
00 54 05  ---          21 16 18  73.0 -49.9  1.1     120.0    25   R  2  10067
  
00 54 05  IRAS2012     21 16 18  73.6 -45.4  1.0     125.5    -5   1  8  10067  00 54 05
00 54 45  ---          21 16 58  73.5 -45.6  1.0     125.1    35   R  2   9533
  
00 54 45  2007+402     21 16 58  72.9 -50.1  1.2     119.7    -5   1  8   9533  00 54 45
00 55 15  ---          21 17 28  72.8 -50.3  1.2     119.5    25   R  2   9133
  
00 55 15  IRAS2012     21 17 28  73.5 -45.8  1.1     124.8    -5   1  8   9133  00 55 15
00 55 55  ---          21 18 08  73.4 -46.1  1.1     124.5    35   R  2   8600
  
00 55 55  2007+402     21 18 08  72.7 -50.5  1.2     119.2    -5   1  8   8600  00 55 55
00 56 25  ---          21 18 38  72.6 -50.6  1.2     119.0    25   R  2   8200
  
00 56 25  IRAS2012     21 18 38  73.3 -46.3  1.1     124.2    -5   1  8   8200  00 56 25
00 57 10  ---          21 19 23  73.2 -46.5  1.1     123.8    40   R  2   7600
  
00 57 10  2007+402     21 19 23  72.5 -50.9  1.2     118.6    -5   1  8   7600  00 57 10
00 57 45  ---          21 19 58  72.4 -51.1  1.2     118.3    30   R  2   7133
  
00 57 45  IRAS2012     21 19 58  73.1 -46.8  1.1     123.5    -5   1  8   7133  00 57 45
00 58 25  ---          21 20 38  73.0 -47.0  1.1     123.2    35   R  2   6600
  
00 58 25  2007+402     21 20 38  72.3 -51.2  1.2     118.1    -5   1  8   6600  00 58 25
00 58 55  ---          21 21 09  72.2 -51.4  1.2     117.8    25   R  2   6200
  
00 58 55  IRAS2012     21 21 09  72.9 -47.2  1.1     123.0    -5   1  8   6200  00 58 55
00 59 35  ---          21 21 49  72.8 -47.4  1.1     122.6    35   R  2   5667
  
00 59 35  2007+402     21 21 49  72.1 -51.6  1.2     117.5    -5   1  8   5667  00 59 35
01 00 05  ---          21 22 19  72.0 -51.7  1.2     117.3    25   R  2   5267
  
01 00 05  IRAS2012     21 22 19  72.7 -47.6  1.1     122.4    -5   1  8   5267  01 00 05
01 00 45  ---          21 22 59  72.6 -47.8  1.1     122.1    35   R  2   4733
  
01 00 45  2007+402     21 22 59  71.9 -51.9  1.3     117.0    -5   1  8   4733  01 00 45
01 01 15  ---          21 23 29  71.8 -52.1  1.3     116.8    25   R  2   4333
Schedule for VLBA_FD   (Code Fd )                                   Page  40
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
01 01 15  IRAS2012     21 23 29  72.5 -48.0  1.2     121.8    -5   1  8   4333  01 01 15
01 01 55  ---          21 24 09  72.4 -48.2  1.2     121.5    35   R  2   3800
  
01 01 55  2007+402     21 24 09  71.7 -52.2  1.3     116.5    -5   1  8   3800  01 01 55
01 02 25  ---          21 24 39  71.6 -52.4  1.3     116.3    25   R  2   3400
  
01 02 25  IRAS2012     21 24 39  72.3 -48.3  1.2     121.3    -5   1  8   3400  01 02 25
01 03 05  ---          21 25 19  72.2 -48.6  1.2     120.9    35   R  2   2867
  
01 03 05  2007+402     21 25 19  71.5 -52.5  1.3     116.1    -5   1  8   2867  01 03 05
01 03 35  ---          21 25 49  71.4 -52.7  1.3     115.9    25   R  2   2467
  
01 03 35  IRAS2012     21 25 49  72.1 -48.7  1.2     120.7    -5   1  8   2467  01 03 35
01 04 15  ---          21 26 29  72.0 -48.9  1.2     120.4    35   R  2   1933
  
01 04 15  2007+402     21 26 29  71.3 -52.9  1.3     115.6    -5   1  8   1933  01 04 15
01 04 45  ---          21 27 00  71.2 -53.0  1.3     115.4    25   R  2   1533
  
01 04 45  IRAS2012     21 27 00  72.0 -49.1  1.2     120.2    -5   1  8   1533  01 04 45
01 05 25  ---          21 27 40  71.8 -49.3  1.2     119.9    35   R  2   1000
  
01 05 25  2007+402     21 27 40  71.1 -53.1  1.3     115.1    -5   1  8   1000  01 05 25
01 05 55  ---          21 28 10  71.0 -53.3  1.3     114.9    25   R  2    600
  
01 05 55  IRAS2012     21 28 10  71.8 -49.4  1.2     119.6    -5   1  8    600  01 05 55
01 06 40  ---          21 28 55  71.6 -49.7  1.2     119.3    40   R  2      0
  
01 07 00  2002+472     21 29 15  66.3 -38.7  1.5     127.4     7   1  9      0  01 07 00
01 10 00  ---          21 32 15  65.9 -39.4  1.5     126.1   180   F  1   2400
  
01 10 20  2007+402     21 32 35  70.2 -54.3  1.4     113.2     8   1  9   2400  01 10 20
01 10 55  ---          21 33 11  70.1 -54.4  1.4     113.0    35   F  1   2867
  
01 10 55  IRAS2012     21 33 11  70.9 -50.8  1.3     117.5    -4   1  9   2867  01 10 55
01 11 35  ---          21 33 51  70.8 -51.0  1.3     117.2    36   F  1   3400
  
01 11 35  2007+402     21 33 51  70.0 -54.6  1.4     112.8    -4   1  9   3400  01 11 35
01 12 05  ---          21 34 21  69.9 -54.7  1.4     112.6    26   F  1   3800
  
01 12 05  IRAS2012     21 34 21  70.7 -51.1  1.3     117.0    -4   1  9   3800  01 12 05
01 12 45  ---          21 35 01  70.6 -51.3  1.3     116.7    36   F  1   4333
Schedule for VLBA_FD   (Code Fd )                                   Page  41
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
01 12 45  2007+402     21 35 01  69.8 -54.8  1.5     112.3    -4   1  9   4333  01 12 45
01 13 15  ---          21 35 31  69.7 -54.9  1.5     112.2    26   F  1   4733
  
01 13 15  IRAS2012     21 35 31  70.5 -51.4  1.4     116.5    -4   1  9   4733  01 13 15
01 13 55  ---          21 36 11  70.4 -51.6  1.4     116.3    36   F  1   5267
  
01 13 55  2007+402     21 36 11  69.6 -55.1  1.5     111.9    -4   1  9   5267  01 13 55
01 14 25  ---          21 36 41  69.5 -55.2  1.5     111.7    26   F  1   5667
  
01 14 25  IRAS2012     21 36 41  70.3 -51.7  1.4     116.1    -4   1  9   5667  01 14 25
01 15 05  ---          21 37 21  70.2 -51.9  1.4     115.8    36   F  1   6200
  
01 15 05  2007+402     21 37 21  69.4 -55.3  1.5     111.5    -4   1  9   6200  01 15 05
01 15 35  ---          21 37 51  69.3 -55.4  1.5     111.3    26   F  1   6600
  
01 15 35  IRAS2012     21 37 51  70.1 -52.0  1.4     115.6    -4   1  9   6600  01 15 35
01 16 15  ---          21 38 31  70.0 -52.2  1.4     115.3    36   F  1   7133
  
01 16 15  2007+402     21 38 31  69.2 -55.5  1.5     111.1    -4   1  9   7133  01 16 15
01 16 45  ---          21 39 02  69.1 -55.6  1.5     110.9    26   F  1   7533
  
01 16 45  IRAS2012     21 39 02  69.9 -52.3  1.4     115.1    -4   1  9   7533  01 16 45
01 17 25  ---          21 39 42  69.8 -52.4  1.4     114.9    36   F  1   8067
  
01 17 25  2007+402     21 39 42  68.9 -55.8  1.5     110.7    -4   1  9   8067  01 17 25
01 17 55  ---          21 40 12  68.9 -55.8  1.5     110.5    26   F  1   8467
  
01 17 55  IRAS2012     21 40 12  69.7 -52.6  1.4     114.7    -4   1  9   8467  01 17 55
01 18 35  ---          21 40 52  69.6 -52.7  1.4     114.5    36   F  1   9000
  
01 18 35  2007+402     21 40 52  68.7 -56.0  1.6     110.3    -4   1  9   9000  01 18 35
01 19 05  ---          21 41 22  68.7 -56.1  1.6     110.2    26   F  1   9400
  
01 19 05  IRAS2012     21 41 22  69.5 -52.8  1.4     114.3    -4   1  9   9400  01 19 05
01 19 50  ---          21 42 07  69.4 -53.0  1.5     114.0    41   F  1  10000
  
01 19 50  2007+402     21 42 07  68.5 -56.2  1.6     109.9    -4   1  9  10000  01 19 50
01 20 25  ---          21 42 42  68.4 -56.3  1.6     109.7    31   F  1  10467
  
01 20 25  IRAS2012     21 42 42  69.3 -53.1  1.5     113.8    -4   1  9  10467  01 20 25
01 21 05  ---          21 43 22  69.2 -53.3  1.5     113.5    36   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  42
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
01 21 05  2007+402     21 43 22  68.3 -56.4  1.6     109.5    -4   1  9  11000  01 21 05
01 21 35  ---          21 43 52  68.2 -56.5  1.6     109.3    26   F  1  11400
  
01 21 35  IRAS2012     21 43 52  69.1 -53.4  1.5     113.3    -4   1  9  11400  01 21 35
01 22 15  ---          21 44 32  69.0 -53.5  1.5     113.1    36   F  1  11933
  
01 22 15  2007+402     21 44 32  68.1 -56.6  1.6     109.1    -4   1  9  11933  01 22 15
01 22 45  ---          21 45 02  68.0 -56.7  1.6     109.0    26   F  1  12333
  
01 22 45  IRAS2012     21 45 02  68.9 -53.6  1.5     112.9    -4   1  9  12333  01 22 45
01 23 25  ---          21 45 43  68.8 -53.7  1.5     112.7    36   F  1  12867
  
01 23 25  2007+402     21 45 43  67.9 -56.8  1.6     108.8    -4   1  9  12867  01 23 25
01 23 55  ---          21 46 13  67.8 -56.9  1.6     108.6    26   F  1  13267
  
01 23 55  IRAS2012     21 46 13  68.7 -53.8  1.5     112.5    -4   1  9  13267  01 23 55
01 24 35  ---          21 46 53  68.6 -54.0  1.5     112.3    36   F  1  13800
  
01 24 35  2007+402     21 46 53  67.7 -57.0  1.7     108.4    -4   1  9  13800  01 24 35
01 25 05  ---          21 47 23  67.6 -57.1  1.7     108.2    26   F  1  14200
  
01 25 05  IRAS2012     21 47 23  68.5 -54.1  1.5     112.1    -4   1  9  14200  01 25 05
01 25 45  ---          21 48 03  68.4 -54.2  1.6     111.9    36   F  1  14733
  
01 25 45  2007+402     21 48 03  67.5 -57.2  1.7     108.0    -4   1  9  14733  01 25 45
01 26 15  ---          21 48 33  67.4 -57.2  1.7     107.9    26   F  1  15133
  
01 26 15  IRAS2012     21 48 33  68.3 -54.3  1.6     111.7    -4   1  9  15133  01 26 15
01 26 55  ---          21 49 13  68.2 -54.4  1.6     111.5    36   F  1  15667
  
01 26 55  2007+402     21 49 13  67.2 -57.3  1.7     107.7    -4   1  9  15667  01 26 55
01 27 25  ---          21 49 43  67.1 -57.4  1.7     107.5    26   F  1  16067
  
01 27 25  IRAS2012     21 49 43  68.1 -54.5  1.6     111.3    -4   1  9  16067  01 27 25
01 28 05  ---          21 50 23  68.0 -54.6  1.6     111.1    36   F  1  16600
  
01 28 05  2007+402     21 50 23  67.0 -57.5  1.7     107.3    -4   1  9  16600  01 28 05
01 28 35  ---          21 50 53  66.9 -57.6  1.7     107.2    26   F  1  17000
  
01 28 35  IRAS2012     21 50 53  67.9 -54.7  1.6     110.9    -4   1  9  17000  01 28 35
01 29 20  ---          21 51 39  67.8 -54.9  1.6     110.7    41   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  43
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
01 29 40  2007+402     21 51 59  66.7 -57.7  1.7     106.9    16   1 10  17600  01 29 40
01 30 25  ---          21 52 44  66.6 -57.8  1.7     106.7    45   R  1  17000
  
01 30 25  IRAS2012     21 52 44  67.6 -55.0  1.6     110.3    -4   1 10  17000  01 30 25
01 31 05  ---          21 53 24  67.5 -55.2  1.6     110.1    36   R  1  16467
  
01 31 05  2007+402     21 53 24  66.5 -57.9  1.8     106.5    -4   1 10  16467  01 31 05
01 31 35  ---          21 53 54  66.4 -58.0  1.8     106.3    26   R  1  16067
  
01 31 35  IRAS2012     21 53 54  67.4 -55.2  1.7     110.0    -4   1 10  16067  01 31 35
01 32 15  ---          21 54 34  67.2 -55.4  1.7     109.7    36   R  1  15533
  
01 32 15  2007+402     21 54 34  66.3 -58.1  1.8     106.1    -4   1 10  15533  01 32 15
01 32 45  ---          21 55 04  66.2 -58.2  1.8     106.0    26   R  1  15133
  
01 32 45  IRAS2012     21 55 04  67.2 -55.4  1.7     109.6    -4   1 10  15133  01 32 45
01 33 25  ---          21 55 44  67.0 -55.5  1.7     109.4    36   R  1  14600
  
01 33 25  2007+402     21 55 44  66.1 -58.2  1.8     105.8    -4   1 10  14600  01 33 25
01 33 55  ---          21 56 14  66.0 -58.3  1.8     105.7    26   R  1  14200
  
01 33 55  IRAS2012     21 56 14  66.9 -55.6  1.7     109.2    -4   1 10  14200  01 33 55
01 34 35  ---          21 56 54  66.8 -55.7  1.7     109.0    36   R  1  13667
  
01 34 35  2007+402     21 56 54  65.8 -58.4  1.8     105.5    -4   1 10  13667  01 34 35
01 35 05  ---          21 57 25  65.7 -58.5  1.8     105.3    26   R  1  13267
  
01 35 05  IRAS2012     21 57 25  66.7 -55.8  1.7     108.9    -4   1 10  13267  01 35 05
01 35 45  ---          21 58 05  66.6 -55.9  1.7     108.7    36   R  1  12733
  
01 35 45  2007+402     21 58 05  65.6 -58.5  1.8     105.2    -4   1 10  12733  01 35 45
01 36 15  ---          21 58 35  65.5 -58.6  1.8     105.0    26   R  1  12333
  
01 36 15  IRAS2012     21 58 35  66.5 -56.0  1.7     108.5    -4   1 10  12333  01 36 15
01 36 55  ---          21 59 15  66.4 -56.1  1.7     108.3    36   R  1  11800
  
01 36 55  2007+402     21 59 15  65.4 -58.7  1.9     104.8    -4   1 10  11800  01 36 55
01 37 25  ---          21 59 45  65.3 -58.7  1.9     104.7    26   R  1  11400
  
01 37 25  IRAS2012     21 59 45  66.3 -56.2  1.8     108.2    -4   1 10  11400  01 37 25
01 38 05  ---          22 00 25  66.2 -56.3  1.8     108.0    36   R  1  10867
Schedule for VLBA_FD   (Code Fd )                                   Page  44
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
01 38 05  2007+402     22 00 25  65.2 -58.8  1.9     104.5    -4   1 10  10867  01 38 05
01 38 35  ---          22 00 55  65.1 -58.9  1.9     104.4    26   R  1  10467
  
01 38 35  IRAS2012     22 00 55  66.1 -56.3  1.8     107.8    -4   1 10  10467  01 38 35
01 39 15  ---          22 01 35  66.0 -56.4  1.8     107.6    36   R  1   9933
  
01 39 15  2007+402     22 01 35  65.0 -58.9  1.9     104.2    -4   1 10   9933  01 39 15
01 39 45  ---          22 02 05  64.9 -59.0  1.9     104.1    26   R  1   9533
  
01 39 45  IRAS2012     22 02 05  65.9 -56.5  1.8     107.5    -4   1 10   9533  01 39 45
01 40 40  ---          22 03 00  65.7 -56.6  1.8     107.2    51   R  1   8800
  
01 40 40  2007+402     22 03 00  64.7 -59.1  1.9     103.8    -4   1 10   8800  01 40 40
01 41 25  ---          22 03 46  64.6 -59.2  1.9     103.7    41   R  1   8200
  
01 41 25  IRAS2012     22 03 46  65.6 -56.7  1.8     107.0    -4   1 10   8200  01 41 25
01 42 05  ---          22 04 26  65.5 -56.8  1.8     106.8    36   R  1   7667
  
01 42 05  2007+402     22 04 26  64.5 -59.2  1.9     103.5    -4   1 10   7667  01 42 05
01 42 35  ---          22 04 56  64.4 -59.3  2.0     103.4    26   R  1   7267
  
01 42 35  IRAS2012     22 04 56  65.4 -56.9  1.8     106.6    -4   1 10   7267  01 42 35
01 43 15  ---          22 05 36  65.3 -57.0  1.9     106.5    36   R  1   6733
  
01 43 15  2007+402     22 05 36  64.2 -59.4  2.0     103.2    -4   1 10   6733  01 43 15
01 43 45  ---          22 06 06  64.1 -59.4  2.0     103.1    26   R  1   6333
  
01 43 45  IRAS2012     22 06 06  65.2 -57.0  1.9     106.3    -4   1 10   6333  01 43 45
01 44 25  ---          22 06 46  65.1 -57.1  1.9     106.1    36   R  1   5800
  
01 44 25  2007+402     22 06 46  64.0 -59.5  2.0     102.9    -4   1 10   5800  01 44 25
01 44 55  ---          22 07 16  63.9 -59.5  2.0     102.8    26   R  1   5400
  
01 44 55  IRAS2012     22 07 16  65.0 -57.2  1.9     106.0    -4   1 10   5400  01 44 55
01 45 35  ---          22 07 56  64.9 -57.2  1.9     105.8    36   R  1   4867
  
01 45 35  2007+402     22 07 56  63.8 -59.6  2.0     102.6    -4   1 10   4867  01 45 35
01 46 05  ---          22 08 26  63.7 -59.6  2.0     102.5    26   R  1   4467
  
01 46 05  IRAS2012     22 08 26  64.8 -57.3  1.9     105.7    -4   1 10   4467  01 46 05
01 46 45  ---          22 09 06  64.6 -57.4  1.9     105.5    36   R  1   3933
Schedule for VLBA_FD   (Code Fd )                                   Page  45
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
01 46 45  2007+402     22 09 06  63.6 -59.7  2.0     102.3    -4   1 10   3933  01 46 45
01 47 15  ---          22 09 37  63.5 -59.7  2.0     102.2    26   R  1   3533
  
01 47 15  IRAS2012     22 09 37  64.5 -57.4  1.9     105.4    -4   1 10   3533  01 47 15
01 47 55  ---          22 10 17  64.4 -57.5  1.9     105.2    36   R  1   3000
  
01 47 55  2007+402     22 10 17  63.4 -59.8  2.0     102.0    -4   1 10   3000  01 47 55
01 48 25  ---          22 10 47  63.3 -59.8  2.1     101.9    26   R  1   2600
  
01 48 25  IRAS2012     22 10 47  64.3 -57.6  1.9     105.0    -4   1 10   2600  01 48 25
01 49 05  ---          22 11 27  64.2 -57.6  2.0     104.9    36   R  1   2067
  
01 49 05  2007+402     22 11 27  63.2 -59.9  2.1     101.7    -4   1 10   2067  01 49 05
01 49 35  ---          22 11 57  63.1 -59.9  2.1     101.6    26   R  1   1667
  
01 49 35  IRAS2012     22 11 57  64.1 -57.7  2.0     104.7    -4   1 10   1667  01 49 35
01 50 15  ---          22 12 37  64.0 -57.8  2.0     104.6    36   R  1   1133
  
01 50 15  2007+402     22 12 37  62.9 -60.0  2.1     101.5    -4   1 10   1133  01 50 15
01 50 45  ---          22 13 07  62.8 -60.0  2.1     101.4    26   R  1    733
  
01 50 45  IRAS2012     22 13 07  63.9 -57.8  2.0     104.4    -4   1 10    733  01 50 45
01 51 40  ---          22 14 02  63.7 -57.9  2.0     104.2    51   R  1      0
  
01 52 00  2007+402     22 14 22  62.6 -60.1  2.1     101.1    16   1  9      0  01 52 00
01 52 45  ---          22 15 07  62.5 -60.2  2.1     100.9    45   F  2    600
  
01 52 45  IRAS2012     22 15 07  63.5 -58.0  2.0     103.9    -4   1  9    600  01 52 45
01 53 25  ---          22 15 48  63.4 -58.1  2.0     103.7    36   F  2   1133
  
01 53 25  2007+402     22 15 48  62.3 -60.3  2.1     100.7    -4   1  9   1133  01 53 25
01 53 55  ---          22 16 18  62.2 -60.3  2.1     100.6    26   F  2   1533
  
01 53 55  IRAS2012     22 16 18  63.3 -58.2  2.0     103.6    -4   1  9   1533  01 53 55
01 54 35  ---          22 16 58  63.2 -58.2  2.0     103.4    36   F  2   2067
  
01 54 35  2007+402     22 16 58  62.1 -60.3  2.2     100.5    -4   1  9   2067  01 54 35
01 55 05  ---          22 17 28  62.0 -60.4  2.2     100.3    26   F  2   2467
  
01 55 05  IRAS2012     22 17 28  63.1 -58.3  2.1     103.3    -4   1  9   2467  01 55 05
01 55 45  ---          22 18 08  63.0 -58.3  2.1     103.2    36   F  2   3000
Schedule for VLBA_FD   (Code Fd )                                   Page  46
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
01 55 45  2007+402     22 18 08  61.9 -60.4  2.2     100.2    -4   1  9   3000  01 55 45
01 56 15  ---          22 18 38  61.8 -60.5  2.2     100.1    26   F  2   3400
  
01 56 15  IRAS2012     22 18 38  62.9 -58.4  2.1     103.0    -4   1  9   3400  01 56 15
01 56 55  ---          22 19 18  62.8 -58.4  2.1     102.9    36   F  2   3933
  
01 56 55  2007+402     22 19 18  61.7 -60.5  2.2      99.9    -4   1  9   3933  01 56 55
01 57 25  ---          22 19 48  61.6 -60.5  2.2      99.8    26   F  2   4333
  
01 57 25  IRAS2012     22 19 48  62.7 -58.5  2.1     102.7    -4   1  9   4333  01 57 25
01 58 05  ---          22 20 28  62.6 -58.5  2.1     102.6    36   F  2   4867
  
01 58 05  2007+402     22 20 28  61.5 -60.6  2.2      99.7    -4   1  9   4867  01 58 05
01 58 35  ---          22 20 58  61.4 -60.6  2.2      99.6    26   F  2   5267
  
01 58 35  IRAS2012     22 20 58  62.5 -58.6  2.1     102.5    -4   1  9   5267  01 58 35
01 59 15  ---          22 21 38  62.4 -58.6  2.1     102.3    36   F  2   5800
  
01 59 15  2007+402     22 21 38  61.2 -60.7  2.2      99.4    -4   1  9   5800  01 59 15
01 59 45  ---          22 22 09  61.2 -60.7  2.2      99.3    26   F  2   6200
  
01 59 45  IRAS2012     22 22 09  62.3 -58.7  2.1     102.2    -4   1  9   6200  01 59 45
02 00 25  ---          22 22 49  62.1 -58.7  2.1     102.0    36   F  2   6733
  
02 00 25  2007+402     22 22 49  61.0 -60.7  2.3      99.2    -4   1  9   6733  02 00 25
02 00 55  ---          22 23 19  60.9 -60.8  2.3      99.1    26   F  2   7133
  
02 00 55  IRAS2012     22 23 19  62.0 -58.8  2.1     101.9    -4   1  9   7133  02 00 55
02 01 35  ---          22 23 59  61.9 -58.8  2.2     101.7    36   F  2   7667
  
02 01 35  2007+402     22 23 59  60.8 -60.8  2.3      98.9    -4   1  9   7667  02 01 35
02 02 05  ---          22 24 29  60.7 -60.8  2.3      98.8    26   F  2   8067
  
02 02 05  IRAS2012     22 24 29  61.8 -58.9  2.2     101.6    -4   1  9   8067  02 02 05
02 03 00  ---          22 25 24  61.7 -59.0  2.2     101.4    51   F  2   8800
  
02 03 00  2007+402     22 25 24  60.5 -60.9  2.3      98.6    -4   1  9   8800  02 03 00
02 03 45  ---          22 26 09  60.4 -60.9  2.3      98.4    41   F  2   9400
  
02 03 45  IRAS2012     22 26 09  61.5 -59.0  2.2     101.2    -4   1  9   9400  02 03 45
02 04 25  ---          22 26 49  61.4 -59.1  2.2     101.1    36   F  2   9933
Schedule for VLBA_FD   (Code Fd )                                   Page  47
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
02 04 25  2007+402     22 26 49  60.3 -61.0  2.3      98.3    -4   1  9   9933  02 04 25
02 04 55  ---          22 27 19  60.2 -61.0  2.3      98.2    26   F  2  10333
  
02 04 55  IRAS2012     22 27 19  61.3 -59.1  2.2     101.0    -4   1  9  10333  02 04 55
02 05 35  ---          22 28 00  61.2 -59.2  2.2     100.8    36   F  2  10867
  
02 05 35  2007+402     22 28 00  60.1 -61.0  2.3      98.1    -4   1  9  10867  02 05 35
02 06 05  ---          22 28 30  60.0 -61.1  2.3      98.0    26   F  2  11267
  
02 06 05  IRAS2012     22 28 30  61.1 -59.2  2.2     100.7    -4   1  9  11267  02 06 05
02 06 45  ---          22 29 10  61.0 -59.2  2.2     100.5    36   F  2  11800
  
02 06 45  2007+402     22 29 10  59.8 -61.1  2.4      97.8    -4   1  9  11800  02 06 45
02 07 15  ---          22 29 40  59.7 -61.1  2.4      97.7    26   F  2  12200
  
02 07 15  IRAS2012     22 29 40  60.9 -59.3  2.3     100.4    -4   1  9  12200  02 07 15
02 07 55  ---          22 30 20  60.7 -59.3  2.3     100.3    36   F  2  12733
  
02 07 55  2007+402     22 30 20  59.6 -61.2  2.4      97.6    -4   1  9  12733  02 07 55
02 08 25  ---          22 30 50  59.5 -61.2  2.4      97.5    26   F  2  13133
  
02 08 25  IRAS2012     22 30 50  60.7 -59.4  2.3     100.2    -4   1  9  13133  02 08 25
02 09 05  ---          22 31 30  60.5 -59.4  2.3     100.0    36   F  2  13667
  
02 09 05  2007+402     22 31 30  59.4 -61.2  2.4      97.3    -4   1  9  13667  02 09 05
02 09 35  ---          22 32 00  59.3 -61.2  2.4      97.2    26   F  2  14067
  
02 09 35  IRAS2012     22 32 00  60.4 -59.4  2.3      99.9    -4   1  9  14067  02 09 35
02 10 15  ---          22 32 40  60.3 -59.5  2.3      99.7    36   F  2  14600
  
02 10 15  2007+402     22 32 40  59.2 -61.3  2.4      97.1    -4   1  9  14600  02 10 15
02 10 45  ---          22 33 10  59.1 -61.3  2.4      97.0    26   F  2  15000
  
02 10 45  IRAS2012     22 33 10  60.2 -59.5  2.3      99.6    -4   1  9  15000  02 10 45
02 11 25  ---          22 33 50  60.1 -59.5  2.3      99.5    36   F  2  15533
  
02 11 25  2007+402     22 33 50  59.0 -61.3  2.4      96.9    -4   1  9  15533  02 11 25
02 11 55  ---          22 34 21  58.9 -61.3  2.4      96.8    26   F  2  15933
  
02 11 55  IRAS2012     22 34 21  60.0 -59.6  2.3      99.4    -4   1  9  15933  02 11 55
02 12 35  ---          22 35 01  59.9 -59.6  2.3      99.2    36   F  2  16467
Schedule for VLBA_FD   (Code Fd )                                   Page  48
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
02 12 35  2007+402     22 35 01  58.7 -61.4  2.5      96.6    -4   1  9  16467  02 12 35
02 13 05  ---          22 35 31  58.6 -61.4  2.5      96.5    26   F  2  16867
  
02 13 05  IRAS2012     22 35 31  59.8 -59.7  2.4      99.1    -4   1  9  16867  02 13 05
02 14 00  ---          22 36 26  59.6 -59.7  2.4      98.9    51   F  2  17600
  
02 16 00  2007+777     22 38 26  39.8  -9.7  2.5     136.1    78   1 10  17600  02 16 00
02 19 00  ---          22 41 27  39.7  -9.9  2.6     135.3   180   R  2  15200
  
02 19 40  2007+402     22 42 07  57.4 -61.6  2.6      95.3     3   1 10  15200  02 19 40
02 20 15  ---          22 42 42  57.3 -61.7  2.6      95.1    35   R  2  14733
  
02 20 15  IRAS2012     22 42 42  58.5 -60.0  2.5      97.6    -4   1 10  14733  02 20 15
02 20 55  ---          22 43 22  58.3 -60.1  2.5      97.5    36   R  2  14200
  
02 20 55  2007+402     22 43 22  57.2 -61.7  2.6      95.0    -4   1 10  14200  02 20 55
02 21 25  ---          22 43 52  57.1 -61.7  2.6      94.9    26   R  2  13800
  
02 21 25  IRAS2012     22 43 52  58.2 -60.1  2.5      97.4    -4   1 10  13800  02 21 25
02 22 05  ---          22 44 32  58.1 -60.1  2.5      97.2    36   R  2  13267
  
02 22 05  2007+402     22 44 32  56.9 -61.7  2.6      94.8    -4   1 10  13267  02 22 05
02 22 35  ---          22 45 02  56.8 -61.7  2.6      94.7    26   R  2  12867
  
02 22 35  IRAS2012     22 45 02  58.0 -60.1  2.5      97.1    -4   1 10  12867  02 22 35
02 23 15  ---          22 45 42  57.9 -60.2  2.5      97.0    36   R  2  12333
  
02 23 15  2007+402     22 45 42  56.7 -61.7  2.6      94.6    -4   1 10  12333  02 23 15
02 23 45  ---          22 46 13  56.6 -61.8  2.6      94.5    26   R  2  11933
  
02 23 45  IRAS2012     22 46 13  57.8 -60.2  2.5      96.9    -4   1 10  11933  02 23 45
02 24 25  ---          22 46 53  57.7 -60.2  2.5      96.8    36   R  2  11400
  
02 24 25  2007+402     22 46 53  56.5 -61.8  2.7      94.4    -4   1 10  11400  02 24 25
02 24 55  ---          22 47 23  56.4 -61.8  2.7      94.3    26   R  2  11000
  
02 24 55  IRAS2012     22 47 23  57.6 -60.2  2.5      96.7    -4   1 10  11000  02 24 55
02 25 35  ---          22 48 03  57.5 -60.3  2.6      96.5    36   R  2  10467
  
02 25 35  2007+402     22 48 03  56.3 -61.8  2.7      94.2    -4   1 10  10467  02 25 35
02 26 05  ---          22 48 33  56.2 -61.8  2.7      94.1    26   R  2  10067
Schedule for VLBA_FD   (Code Fd )                                   Page  49
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
02 26 05  IRAS2012     22 48 33  57.4 -60.3  2.6      96.4    -4   1 10  10067  02 26 05
02 26 45  ---          22 49 13  57.2 -60.3  2.6      96.3    36   R  2   9533
  
02 26 45  2007+402     22 49 13  56.0 -61.8  2.7      93.9    -4   1 10   9533  02 26 45
02 27 15  ---          22 49 43  55.9 -61.8  2.7      93.8    26   R  2   9133
  
02 27 15  IRAS2012     22 49 43  57.1 -60.3  2.6      96.2    -4   1 10   9133  02 27 15
02 27 55  ---          22 50 23  57.0 -60.4  2.6      96.1    36   R  2   8600
  
02 27 55  2007+402     22 50 23  55.8 -61.9  2.7      93.7    -4   1 10   8600  02 27 55
02 28 25  ---          22 50 53  55.7 -61.9  2.7      93.6    26   R  2   8200
  
02 28 25  IRAS2012     22 50 53  56.9 -60.4  2.6      96.0    -4   1 10   8200  02 28 25
02 29 10  ---          22 51 38  56.8 -60.4  2.6      95.8    41   R  2   7600
  
02 29 10  2007+402     22 51 38  55.6 -61.9  2.7      93.5    -4   1 10   7600  02 29 10
02 29 45  ---          22 52 13  55.5 -61.9  2.7      93.4    31   R  2   7133
  
02 29 45  IRAS2012     22 52 13  56.7 -60.4  2.6      95.7    -4   1 10   7133  02 29 45
02 30 25  ---          22 52 54  56.5 -60.4  2.6      95.6    36   R  2   6600
  
02 30 25  2007+402     22 52 54  55.3 -61.9  2.8      93.3    -4   1 10   6600  02 30 25
02 30 55  ---          22 53 24  55.3 -61.9  2.8      93.2    26   R  2   6200
  
02 30 55  IRAS2012     22 53 24  56.5 -60.5  2.6      95.5    -4   1 10   6200  02 30 55
02 31 35  ---          22 54 04  56.3 -60.5  2.7      95.4    36   R  2   5667
  
02 31 35  2007+402     22 54 04  55.1 -61.9  2.8      93.1    -4   1 10   5667  02 31 35
02 32 05  ---          22 54 34  55.0 -61.9  2.8      93.0    26   R  2   5267
  
02 32 05  IRAS2012     22 54 34  56.2 -60.5  2.7      95.3    -4   1 10   5267  02 32 05
02 32 45  ---          22 55 14  56.1 -60.5  2.7      95.1    36   R  2   4733
  
02 32 45  2007+402     22 55 14  54.9 -62.0  2.8      92.9    -4   1 10   4733  02 32 45
02 33 15  ---          22 55 44  54.8 -62.0  2.8      92.8    26   R  2   4333
  
02 33 15  IRAS2012     22 55 44  56.0 -60.5  2.7      95.0    -4   1 10   4333  02 33 15
02 33 55  ---          22 56 24  55.9 -60.6  2.7      94.9    36   R  2   3800
  
02 33 55  2007+402     22 56 24  54.7 -62.0  2.8      92.7    -4   1 10   3800  02 33 55
02 34 25  ---          22 56 54  54.6 -62.0  2.8      92.6    26   R  2   3400
Schedule for VLBA_FD   (Code Fd )                                   Page  50
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
02 34 25  IRAS2012     22 56 54  55.8 -60.6  2.7      94.8    -4   1 10   3400  02 34 25
02 35 05  ---          22 57 34  55.7 -60.6  2.7      94.7    36   R  2   2867
  
02 35 05  2007+402     22 57 34  54.5 -62.0  2.8      92.5    -4   1 10   2867  02 35 05
02 35 35  ---          22 58 04  54.4 -62.0  2.8      92.4    26   R  2   2467
  
02 35 35  IRAS2012     22 58 04  55.6 -60.6  2.7      94.6    -4   1 10   2467  02 35 35
02 36 15  ---          22 58 45  55.5 -60.6  2.7      94.5    36   R  2   1933
  
02 36 15  2007+402     22 58 45  54.2 -62.0  2.8      92.2    -4   1 10   1933  02 36 15
02 36 45  ---          22 59 15  54.1 -62.0  2.9      92.2    26   R  2   1533
  
02 36 45  IRAS2012     22 59 15  55.4 -60.6  2.7      94.4    -4   1 10   1533  02 36 45
02 37 25  ---          22 59 55  55.2 -60.6  2.8      94.3    36   R  2   1000
  
02 37 25  2007+402     22 59 55  54.0 -62.0  2.9      92.0    -4   1 10   1000  02 37 25
02 37 55  ---          23 00 25  53.9 -62.0  2.9      92.0    26   R  2    600
  
02 37 55  IRAS2012     23 00 25  55.1 -60.7  2.8      94.2    -4   1 10    600  02 37 55
02 38 40  ---          23 01 10  55.0 -60.7  2.8      94.0    41   R  2      0
  
02 39 00  2002+472     23 01 30  52.0 -50.8  3.0      99.8    11   1 11      0  02 39 00
02 42 00  ---          23 04 31  51.5 -50.9  3.0      99.1   180   F  1   2400
  
02 42 20  2007+402     23 04 51  53.1 -62.1  3.0      91.2    11   1 11   2400  02 42 20
02 42 55  ---          23 05 26  53.0 -62.1  3.0      91.1    35   F  1   2867
  
02 42 55  IRAS2012     23 05 26  54.2 -60.8  2.8      93.3    -4   1 11   2867  02 42 55
02 43 35  ---          23 06 06  54.1 -60.8  2.9      93.1    36   F  1   3400
  
02 43 35  2007+402     23 06 06  52.8 -62.1  3.0      91.0    -4   1 11   3400  02 43 35
02 44 05  ---          23 06 36  52.7 -62.1  3.0      90.9    26   F  1   3800
  
02 44 05  IRAS2012     23 06 36  54.0 -60.8  2.9      93.1    -4   1 11   3800  02 44 05
02 44 45  ---          23 07 16  53.9 -60.8  2.9      92.9    36   F  1   4333
  
02 44 45  2007+402     23 07 16  52.6 -62.1  3.0      90.8    -4   1 11   4333  02 44 45
02 45 15  ---          23 07 46  52.5 -62.1  3.0      90.7    26   F  1   4733
  
02 45 15  IRAS2012     23 07 46  53.8 -60.8  2.9      92.8    -4   1 11   4733  02 45 15
02 45 55  ---          23 08 26  53.6 -60.8  2.9      92.7    36   F  1   5267
Schedule for VLBA_FD   (Code Fd )                                   Page  51
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
02 45 55  2007+402     23 08 26  52.4 -62.1  3.0      90.6    -4   1 11   5267  02 45 55
02 46 25  ---          23 08 56  52.3 -62.1  3.0      90.5    26   F  1   5667
  
02 46 25  IRAS2012     23 08 56  53.5 -60.8  2.9      92.6    -4   1 11   5667  02 46 25
02 47 05  ---          23 09 36  53.4 -60.8  2.9      92.5    36   F  1   6200
  
02 47 05  2007+402     23 09 36  52.2 -62.1  3.0      90.4    -4   1 11   6200  02 47 05
02 47 35  ---          23 10 06  52.1 -62.1  3.0      90.3    26   F  1   6600
  
02 47 35  IRAS2012     23 10 06  53.3 -60.8  2.9      92.4    -4   1 11   6600  02 47 35
02 48 15  ---          23 10 47  53.2 -60.8  2.9      92.3    36   F  1   7133
  
02 48 15  2007+402     23 10 47  51.9 -62.1  3.1      90.2    -4   1 11   7133  02 48 15
02 48 45  ---          23 11 17  51.9 -62.1  3.1      90.1    26   F  1   7533
  
02 48 45  IRAS2012     23 11 17  53.1 -60.9  2.9      92.2    -4   1 11   7533  02 48 45
02 49 25  ---          23 11 57  53.0 -60.9  3.0      92.1    36   F  1   8067
  
02 49 25  2007+402     23 11 57  51.7 -62.1  3.1      90.0    -5   1 11   8067  02 49 25
02 49 55  ---          23 12 27  51.6 -62.1  3.1      90.0    25   F  1   8467
  
02 49 55  IRAS2012     23 12 27  52.9 -60.9  3.0      92.0    -5   1 11   8467  02 49 55
02 50 35  ---          23 13 07  52.8 -60.9  3.0      91.9    35   F  1   9000
  
02 50 35  2007+402     23 13 07  51.5 -62.1  3.1      89.8    -5   1 11   9000  02 50 35
02 51 05  ---          23 13 37  51.4 -62.1  3.1      89.8    25   F  1   9400
  
02 51 05  IRAS2012     23 13 37  52.7 -60.9  3.0      91.8    -5   1 11   9400  02 51 05
02 51 50  ---          23 14 22  52.5 -60.9  3.0      91.7    40   F  1  10000
  
02 51 50  2007+402     23 14 22  51.3 -62.1  3.1      89.6    -5   1 11  10000  02 51 50
02 52 25  ---          23 14 57  51.2 -62.1  3.1      89.6    30   F  1  10467
  
02 52 25  IRAS2012     23 14 57  52.4 -60.9  3.0      91.6    -5   1 11  10467  02 52 25
02 53 05  ---          23 15 37  52.3 -60.9  3.0      91.5    35   F  1  11000
  
02 53 05  2007+402     23 15 37  51.0 -62.1  3.1      89.4    -5   1 11  11000  02 53 05
02 53 35  ---          23 16 07  50.9 -62.1  3.1      89.4    25   F  1  11400
  
02 53 35  IRAS2012     23 16 07  52.2 -60.9  3.0      91.4    -5   1 11  11400  02 53 35
02 54 15  ---          23 16 48  52.1 -60.9  3.0      91.3    35   F  1  11933
Schedule for VLBA_FD   (Code Fd )                                   Page  52
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
02 54 15  2007+402     23 16 48  50.8 -62.1  3.2      89.3    -5   1 11  11933  02 54 15
02 54 45  ---          23 17 18  50.7 -62.1  3.2      89.2    25   F  1  12333
  
02 54 45  IRAS2012     23 17 18  52.0 -60.9  3.0      91.2    -5   1 11  12333  02 54 45
02 55 25  ---          23 17 58  51.8 -60.9  3.1      91.1    35   F  1  12867
  
02 55 25  2007+402     23 17 58  50.6 -62.1  3.2      89.1    -5   1 11  12867  02 55 25
02 55 55  ---          23 18 28  50.5 -62.1  3.2      89.0    25   F  1  13267
  
02 55 55  IRAS2012     23 18 28  51.8 -60.9  3.1      91.0    -5   1 11  13267  02 55 55
02 56 35  ---          23 19 08  51.6 -60.9  3.1      90.9    35   F  1  13800
  
02 56 35  2007+402     23 19 08  50.4 -62.1  3.2      88.9    -5   1 11  13800  02 56 35
02 57 05  ---          23 19 38  50.3 -62.1  3.2      88.8    25   F  1  14200
  
02 57 05  IRAS2012     23 19 38  51.5 -60.9  3.1      90.8    -5   1 11  14200  02 57 05
02 57 45  ---          23 20 18  51.4 -60.9  3.1      90.7    35   F  1  14733
  
02 57 45  2007+402     23 20 18  50.1 -62.1  3.2      88.7    -5   1 11  14733  02 57 45
02 58 15  ---          23 20 48  50.0 -62.1  3.2      88.6    25   F  1  15133
  
02 58 15  IRAS2012     23 20 48  51.3 -60.9  3.1      90.6    -5   1 11  15133  02 58 15
02 58 55  ---          23 21 28  51.2 -60.9  3.1      90.5    35   F  1  15667
  
02 58 55  2007+402     23 21 28  49.9 -62.1  3.2      88.5    -5   1 11  15667  02 58 55
02 59 25  ---          23 21 58  49.8 -62.1  3.2      88.4    25   F  1  16067
  
02 59 25  IRAS2012     23 21 58  51.1 -60.9  3.1      90.4    -5   1 11  16067  02 59 25
03 00 05  ---          23 22 38  51.0 -60.9  3.1      90.3    35   F  1  16600
  
03 00 05  2007+402     23 22 38  49.7 -62.0  3.2      88.3    -5   1 11  16600  03 00 05
03 00 35  ---          23 23 09  49.6 -62.0  3.3      88.3    25   F  1  17000
  
03 00 35  IRAS2012     23 23 09  50.9 -60.9  3.1      90.2    -5   1 11  17000  03 00 35
03 01 20  ---          23 23 54  50.7 -60.9  3.2      90.1    40   F  1  17600
  
03 01 40  2007+402     23 24 14  49.4 -62.0  3.3      88.1    15   1 12  17600  03 01 40
03 02 25  ---          23 24 59  49.2 -62.0  3.3      88.0    45   R  1  17000
  
03 02 25  IRAS2012     23 24 59  50.5 -60.9  3.2      89.9    -5   1 12  17000  03 02 25
03 03 05  ---          23 25 39  50.4 -60.9  3.2      89.8    35   R  1  16467
Schedule for VLBA_FD   (Code Fd )                                   Page  53
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
03 03 05  2007+402     23 25 39  49.1 -62.0  3.3      87.9    -5   1 12  16467  03 03 05
03 03 35  ---          23 26 09  49.0 -62.0  3.3      87.8    25   R  1  16067
  
03 03 35  IRAS2012     23 26 09  50.3 -60.9  3.2      89.7    -5   1 12  16067  03 03 35
03 04 15  ---          23 26 49  50.2 -60.9  3.2      89.6    35   R  1  15533
  
03 04 15  2007+402     23 26 49  48.9 -62.0  3.3      87.7    -5   1 12  15533  03 04 15
03 04 45  ---          23 27 19  48.8 -62.0  3.3      87.6    25   R  1  15133
  
03 04 45  IRAS2012     23 27 19  50.1 -60.9  3.2      89.5    -5   1 12  15133  03 04 45
03 05 25  ---          23 27 59  50.0 -60.9  3.2      89.4    35   R  1  14600
  
03 05 25  2007+402     23 27 59  48.7 -62.0  3.3      87.5    -5   1 12  14600  03 05 25
03 05 55  ---          23 28 29  48.6 -62.0  3.3      87.4    25   R  1  14200
  
03 05 55  IRAS2012     23 28 29  49.9 -60.9  3.2      89.3    -5   1 12  14200  03 05 55
03 06 35  ---          23 29 10  49.7 -60.9  3.2      89.2    35   R  1  13667
  
03 06 35  2007+402     23 29 10  48.5 -62.0  3.4      87.3    -5   1 12  13667  03 06 35
03 07 05  ---          23 29 40  48.4 -62.0  3.4      87.3    25   R  1  13267
  
03 07 05  IRAS2012     23 29 40  49.6 -60.9  3.3      89.1    -5   1 12  13267  03 07 05
03 07 45  ---          23 30 20  49.5 -60.9  3.3      89.0    35   R  1  12733
  
03 07 45  2007+402     23 30 20  48.2 -62.0  3.4      87.2    -5   1 12  12733  03 07 45
03 08 15  ---          23 30 50  48.1 -62.0  3.4      87.1    25   R  1  12333
  
03 08 15  IRAS2012     23 30 50  49.4 -60.9  3.3      89.0    -5   1 12  12333  03 08 15
03 08 55  ---          23 31 30  49.3 -60.9  3.3      88.8    35   R  1  11800
  
03 08 55  2007+402     23 31 30  48.0 -61.9  3.4      87.0    -5   1 12  11800  03 08 55
03 09 25  ---          23 32 00  47.9 -61.9  3.4      86.9    25   R  1  11400
  
03 09 25  IRAS2012     23 32 00  49.2 -60.9  3.3      88.8    -5   1 12  11400  03 09 25
03 10 05  ---          23 32 40  49.1 -60.9  3.3      88.7    35   R  1  10867
  
03 10 05  2007+402     23 32 40  47.8 -61.9  3.4      86.8    -5   1 12  10867  03 10 05
03 10 35  ---          23 33 10  47.7 -61.9  3.4      86.7    25   R  1  10467
  
03 10 35  IRAS2012     23 33 10  49.0 -60.9  3.3      88.6    -5   1 12  10467  03 10 35
03 11 15  ---          23 33 50  48.9 -60.9  3.3      88.5    35   R  1   9933
Schedule for VLBA_FD   (Code Fd )                                   Page  54
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
03 11 15  2007+402     23 33 50  47.6 -61.9  3.4      86.6    -5   1 12   9933  03 11 15
03 11 45  ---          23 34 20  47.5 -61.9  3.4      86.5    25   R  1   9533
  
03 11 45  IRAS2012     23 34 20  48.8 -60.9  3.3      88.4    -5   1 12   9533  03 11 45
03 12 40  ---          23 35 16  48.6 -60.9  3.3      88.2    50   R  1   8800
  
03 12 40  2007+402     23 35 16  47.3 -61.9  3.5      86.4    -5   1 12   8800  03 12 40
03 13 25  ---          23 36 01  47.2 -61.9  3.5      86.3    40   R  1   8200
  
03 13 25  IRAS2012     23 36 01  48.5 -60.9  3.4      88.1    -5   1 12   8200  03 13 25
03 14 05  ---          23 36 41  48.3 -60.9  3.4      88.0    35   R  1   7667
  
03 14 05  2007+402     23 36 41  47.0 -61.9  3.5      86.2    -5   1 12   7667  03 14 05
03 14 35  ---          23 37 11  46.9 -61.8  3.5      86.1    25   R  1   7267
  
03 14 35  IRAS2012     23 37 11  48.2 -60.9  3.4      87.9    -5   1 12   7267  03 14 35
03 15 15  ---          23 37 51  48.1 -60.9  3.4      87.8    35   R  1   6733
  
03 15 15  2007+402     23 37 51  46.8 -61.8  3.5      86.0    -5   1 12   6733  03 15 15
03 15 45  ---          23 38 21  46.7 -61.8  3.5      86.0    25   R  1   6333
  
03 15 45  IRAS2012     23 38 21  48.0 -60.9  3.4      87.8    -5   1 12   6333  03 15 45
03 16 25  ---          23 39 01  47.9 -60.8  3.4      87.7    35   R  1   5800
  
03 16 25  2007+402     23 39 01  46.6 -61.8  3.5      85.9    -5   1 12   5800  03 16 25
03 16 55  ---          23 39 31  46.5 -61.8  3.5      85.8    25   R  1   5400
  
03 16 55  IRAS2012     23 39 31  47.8 -60.8  3.4      87.6    -5   1 12   5400  03 16 55
03 17 35  ---          23 40 11  47.7 -60.8  3.4      87.5    35   R  1   4867
  
03 17 35  2007+402     23 40 11  46.4 -61.8  3.5      85.7    -5   1 12   4867  03 17 35
03 18 05  ---          23 40 41  46.3 -61.8  3.5      85.6    25   R  1   4467
  
03 18 05  IRAS2012     23 40 41  47.6 -60.8  3.4      87.4    -5   1 12   4467  03 18 05
03 18 45  ---          23 41 22  47.4 -60.8  3.4      87.3    35   R  1   3933
  
03 18 45  2007+402     23 41 22  46.1 -61.8  3.6      85.5    -5   1 12   3933  03 18 45
03 19 15  ---          23 41 52  46.0 -61.8  3.6      85.4    25   R  1   3533
  
03 19 15  IRAS2012     23 41 52  47.4 -60.8  3.5      87.2    -5   1 12   3533  03 19 15
03 19 55  ---          23 42 32  47.2 -60.8  3.5      87.1    35   R  1   3000
Schedule for VLBA_FD   (Code Fd )                                   Page  55
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
03 19 55  2007+402     23 42 32  45.9 -61.7  3.6      85.3    -5   1 12   3000  03 19 55
03 20 25  ---          23 43 02  45.8 -61.7  3.6      85.3    25   R  1   2600
  
03 20 25  IRAS2012     23 43 02  47.1 -60.8  3.5      87.0    -5   1 12   2600  03 20 25
03 21 05  ---          23 43 42  47.0 -60.8  3.5      86.9    35   R  1   2067
  
03 21 05  2007+402     23 43 42  45.7 -61.7  3.6      85.2    -5   1 12   2067  03 21 05
03 21 35  ---          23 44 12  45.6 -61.7  3.6      85.1    25   R  1   1667
  
03 21 35  IRAS2012     23 44 12  46.9 -60.8  3.5      86.9    -5   1 12   1667  03 21 35
03 22 15  ---          23 44 52  46.8 -60.8  3.5      86.8    35   R  1   1133
  
03 22 15  2007+402     23 44 52  45.5 -61.7  3.6      85.0    -5   1 12   1133  03 22 15
03 22 45  ---          23 45 22  45.4 -61.7  3.6      84.9    25   R  1    733
  
03 22 45  IRAS2012     23 45 22  46.7 -60.8  3.5      86.7    -5   1 12    733  03 22 45
03 23 40  ---          23 46 17  46.5 -60.7  3.5      86.5    50   R  1      0
  
03 24 00  2007+402     23 46 37  45.1 -61.6  3.6      84.7    15   1 11      0  03 24 00
03 24 45  ---          23 47 23  45.0 -61.6  3.7      84.6    45   F  2    600
  
03 24 45  IRAS2012     23 47 23  46.3 -60.7  3.5      86.4    -5   1 11    600  03 24 45
03 25 25  ---          23 48 03  46.2 -60.7  3.6      86.3    35   F  2   1133
  
03 25 25  2007+402     23 48 03  44.9 -61.6  3.7      84.5    -5   1 11   1133  03 25 25
03 25 55  ---          23 48 33  44.8 -61.6  3.7      84.5    25   F  2   1533
  
03 25 55  IRAS2012     23 48 33  46.1 -60.7  3.6      86.2    -5   1 11   1533  03 25 55
03 26 35  ---          23 49 13  46.0 -60.7  3.6      86.1    35   F  2   2067
  
03 26 35  2007+402     23 49 13  44.7 -61.6  3.7      84.4    -5   1 11   2067  03 26 35
03 27 05  ---          23 49 43  44.6 -61.6  3.7      84.3    25   F  2   2467
  
03 27 05  IRAS2012     23 49 43  45.9 -60.7  3.6      86.0    -5   1 11   2467  03 27 05
03 27 45  ---          23 50 23  45.8 -60.7  3.6      85.9    35   F  2   3000
  
03 27 45  2007+402     23 50 23  44.4 -61.5  3.7      84.2    -5   1 11   3000  03 27 45
03 28 15  ---          23 50 53  44.3 -61.5  3.7      84.1    25   F  2   3400
  
03 28 15  IRAS2012     23 50 53  45.7 -60.7  3.6      85.8    -5   1 11   3400  03 28 15
03 28 55  ---          23 51 33  45.5 -60.6  3.6      85.7    35   F  2   3933
Schedule for VLBA_FD   (Code Fd )                                   Page  56
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
03 28 55  2007+402     23 51 33  44.2 -61.5  3.7      84.0    -5   1 11   3933  03 28 55
03 29 25  ---          23 52 03  44.1 -61.5  3.7      84.0    25   F  2   4333
  
03 29 25  IRAS2012     23 52 03  45.4 -60.6  3.6      85.7    -5   1 11   4333  03 29 25
03 30 05  ---          23 52 43  45.3 -60.6  3.6      85.6    35   F  2   4867
  
03 30 05  2007+402     23 52 43  44.0 -61.5  3.7      83.9    -5   1 11   4867  03 30 05
03 30 35  ---          23 53 13  43.9 -61.5  3.8      83.8    25   F  2   5267
  
03 30 35  IRAS2012     23 53 13  45.2 -60.6  3.6      85.5    -5   1 11   5267  03 30 35
03 31 15  ---          23 53 54  45.1 -60.6  3.7      85.4    35   F  2   5800
  
03 31 15  2007+402     23 53 54  43.8 -61.4  3.8      83.7    -5   1 11   5800  03 31 15
03 31 45  ---          23 54 24  43.7 -61.4  3.8      83.6    25   F  2   6200
  
03 31 45  IRAS2012     23 54 24  45.0 -60.6  3.7      85.3    -5   1 11   6200  03 31 45
03 32 25  ---          23 55 04  44.9 -60.6  3.7      85.2    35   F  2   6733
  
03 32 25  2007+402     23 55 04  43.5 -61.4  3.8      83.5    -5   1 11   6733  03 32 25
03 32 55  ---          23 55 34  43.5 -61.4  3.8      83.5    25   F  2   7133
  
03 32 55  IRAS2012     23 55 34  44.8 -60.6  3.7      85.1    -5   1 11   7133  03 32 55
03 33 35  ---          23 56 14  44.7 -60.5  3.7      85.0    35   F  2   7667
  
03 33 35  2007+402     23 56 14  43.3 -61.4  3.8      83.4    -5   1 11   7667  03 33 35
03 34 05  ---          23 56 44  43.2 -61.4  3.8      83.3    25   F  2   8067
  
03 34 05  IRAS2012     23 56 44  44.6 -60.5  3.7      85.0    -5   1 11   8067  03 34 05
03 35 00  ---          23 57 39  44.4 -60.5  3.7      84.8    50   F  2   8800
  
03 35 00  2007+402     23 57 39  43.1 -61.3  3.8      83.2    -5   1 11   8800  03 35 00
03 35 45  ---          23 58 24  42.9 -61.3  3.8      83.1    40   F  2   9400
  
03 35 45  IRAS2012     23 58 24  44.3 -60.5  3.7      84.7    -5   1 11   9400  03 35 45
03 36 25  ---          23 59 04  44.1 -60.5  3.7      84.6    35   F  2   9933
  
03 36 25  2007+402     23 59 04  42.8 -61.3  3.9      83.0    -5   1 11   9933  03 36 25
03 36 55  ---          23 59 35  42.7 -61.3  3.9      82.9    25   F  2  10333
  
03 36 55  IRAS2012     23 59 35  44.0 -60.5  3.8      84.5    -5   1 11  10333  03 36 55
03 37 35  ---          00 00 15  43.9 -60.4  3.8      84.4    35   F  2  10867
Schedule for VLBA_FD   (Code Fd )                                   Page  57
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
03 37 35  2007+402     00 00 15  42.6 -61.3  3.9      82.8    -5   1 11  10867  03 37 35
03 38 05  ---          00 00 45  42.5 -61.2  3.9      82.7    25   F  2  11267
  
03 38 05  IRAS2012     00 00 45  43.8 -60.4  3.8      84.4    -5   1 11  11267  03 38 05
03 38 45  ---          00 01 25  43.7 -60.4  3.8      84.3    35   F  2  11800
  
03 38 45  2007+402     00 01 25  42.3 -61.2  3.9      82.6    -5   1 11  11800  03 38 45
03 39 15  ---          00 01 55  42.3 -61.2  3.9      82.6    25   F  2  12200
  
03 39 15  IRAS2012     00 01 55  43.6 -60.4  3.8      84.2    -5   1 11  12200  03 39 15
03 39 55  ---          00 02 35  43.5 -60.4  3.8      84.1    35   F  2  12733
  
03 39 55  2007+402     00 02 35  42.1 -61.2  3.9      82.5    -5   1 11  12733  03 39 55
03 40 25  ---          00 03 05  42.0 -61.2  3.9      82.4    25   F  2  13133
  
03 40 25  IRAS2012     00 03 05  43.4 -60.4  3.8      84.0    -5   1 11  13133  03 40 25
03 41 05  ---          00 03 45  43.2 -60.4  3.8      83.9    35   F  2  13667
  
03 41 05  2007+402     00 03 45  41.9 -61.1  3.9      82.3    -5   1 11  13667  03 41 05
03 41 35  ---          00 04 15  41.8 -61.1  3.9      82.2    25   F  2  14067
  
03 41 35  IRAS2012     00 04 15  43.2 -60.3  3.8      83.9    -5   1 11  14067  03 41 35
03 42 15  ---          00 04 55  43.0 -60.3  3.8      83.8    35   F  2  14600
  
03 42 15  2007+402     00 04 55  41.7 -61.1  4.0      82.1    -5   1 11  14600  03 42 15
03 42 45  ---          00 05 25  41.6 -61.1  4.0      82.1    25   F  2  15000
  
03 42 45  IRAS2012     00 05 25  42.9 -60.3  3.8      83.7    -5   1 11  15000  03 42 45
03 43 25  ---          00 06 06  42.8 -60.3  3.9      83.6    35   F  2  15533
  
03 43 25  2007+402     00 06 06  41.5 -61.1  4.0      82.0    -5   1 11  15533  03 43 25
03 43 55  ---          00 06 36  41.4 -61.0  4.0      81.9    25   F  2  15933
  
03 43 55  IRAS2012     00 06 36  42.7 -60.3  3.9      83.5    -5   1 11  15933  03 43 55
03 44 35  ---          00 07 16  42.6 -60.3  3.9      83.4    35   F  2  16467
  
03 44 35  2007+402     00 07 16  41.2 -61.0  4.0      81.8    -5   1 11  16467  03 44 35
03 45 05  ---          00 07 46  41.2 -61.0  4.0      81.7    25   F  2  16867
  
03 45 05  IRAS2012     00 07 46  42.5 -60.2  3.9      83.3    -5   1 11  16867  03 45 05
03 46 00  ---          00 08 41  42.3 -60.2  3.9      83.2    50   F  2  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  58
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
03 48 00  2007+777     00 10 41  35.8 -13.1  4.1     111.5    87   1 12  17600  03 48 00
03 51 00  ---          00 13 42  35.7 -13.2  4.1     110.7   180   R  2  15200
  
03 51 40  2007+402     00 14 22  39.9 -60.7  4.1      80.8     6   1 12  15200  03 51 40
03 52 15  ---          00 14 57  39.8 -60.7  4.1      80.8    35   R  2  14733
  
03 52 15  IRAS2012     00 14 57  41.2 -60.0  4.0      82.3    -5   1 12  14733  03 52 15
03 52 55  ---          00 15 37  41.0 -60.0  4.0      82.2    35   R  2  14200
  
03 52 55  2007+402     00 15 37  39.7 -60.7  4.1      80.7    -5   1 12  14200  03 52 55
03 53 25  ---          00 16 07  39.6 -60.7  4.1      80.6    25   R  2  13800
  
03 53 25  IRAS2012     00 16 07  40.9 -60.0  4.0      82.1    -5   1 12  13800  03 53 25
03 54 05  ---          00 16 47  40.8 -60.0  4.0      82.0    35   R  2  13267
  
03 54 05  2007+402     00 16 47  39.5 -60.6  4.2      80.5    -5   1 12  13267  03 54 05
03 54 35  ---          00 17 17  39.4 -60.6  4.2      80.4    25   R  2  12867
  
03 54 35  IRAS2012     00 17 17  40.7 -59.9  4.0      82.0    -5   1 12  12867  03 54 35
03 55 15  ---          00 17 58  40.6 -59.9  4.1      81.9    35   R  2  12333
  
03 55 15  2007+402     00 17 58  39.2 -60.6  4.2      80.3    -5   1 12  12333  03 55 15
03 55 45  ---          00 18 28  39.1 -60.6  4.2      80.3    25   R  2  11933
  
03 55 45  IRAS2012     00 18 28  40.5 -59.9  4.1      81.8    -5   1 12  11933  03 55 45
03 56 25  ---          00 19 08  40.4 -59.9  4.1      81.7    35   R  2  11400
  
03 56 25  2007+402     00 19 08  39.0 -60.5  4.2      80.2    -5   1 12  11400  03 56 25
03 56 55  ---          00 19 38  38.9 -60.5  4.2      80.1    25   R  2  11000
  
03 56 55  IRAS2012     00 19 38  40.3 -59.9  4.1      81.6    -5   1 12  11000  03 56 55
03 57 35  ---          00 20 18  40.2 -59.8  4.1      81.6    35   R  2  10467
  
03 57 35  2007+402     00 20 18  38.8 -60.5  4.2      80.0    -5   1 12  10467  03 57 35
03 58 05  ---          00 20 48  38.7 -60.5  4.2      80.0    25   R  2  10067
  
03 58 05  IRAS2012     00 20 48  40.1 -59.8  4.1      81.5    -5   1 12  10067  03 58 05
03 58 45  ---          00 21 28  39.9 -59.8  4.1      81.4    35   R  2   9533
  
03 58 45  2007+402     00 21 28  38.6 -60.5  4.2      79.9    -5   1 12   9533  03 58 45
03 59 15  ---          00 21 58  38.5 -60.4  4.2      79.8    25   R  2   9133
Schedule for VLBA_FD   (Code Fd )                                   Page  59
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
03 59 15  IRAS2012     00 21 58  39.9 -59.8  4.1      81.3    -5   1 12   9133  03 59 15
03 59 55  ---          00 22 38  39.7 -59.7  4.1      81.2    35   R  2   8600
  
03 59 55  2007+402     00 22 38  38.4 -60.4  4.2      79.7    -5   1 12   8600  03 59 55
04 00 25  ---          00 23 08  38.3 -60.4  4.3      79.6    25   R  2   8200
  
04 00 25  IRAS2012     00 23 08  39.6 -59.7  4.1      81.1    -5   1 12   8200  04 00 25
04 01 10  ---          00 23 54  39.5 -59.7  4.2      81.0    40   R  2   7600
  
04 01 10  2007+402     00 23 54  38.1 -60.3  4.3      79.5    -5   1 12   7600  04 01 10
04 01 45  ---          00 24 29  38.0 -60.3  4.3      79.5    30   R  2   7133
  
04 01 45  IRAS2012     00 24 29  39.4 -59.7  4.2      81.0    -5   1 12   7133  04 01 45
04 02 25  ---          00 25 09  39.3 -59.6  4.2      80.9    35   R  2   6600
  
04 02 25  2007+402     00 25 09  37.9 -60.3  4.3      79.4    -5   1 12   6600  04 02 25
04 02 55  ---          00 25 39  37.8 -60.3  4.3      79.3    25   R  2   6200
  
04 02 55  IRAS2012     00 25 39  39.2 -59.6  4.2      80.8    -5   1 12   6200  04 02 55
04 03 35  ---          00 26 19  39.0 -59.6  4.2      80.7    35   R  2   5667
  
04 03 35  2007+402     00 26 19  37.7 -60.2  4.3      79.2    -5   1 12   5667  04 03 35
04 04 05  ---          00 26 49  37.6 -60.2  4.3      79.1    25   R  2   5267
  
04 04 05  IRAS2012     00 26 49  39.0 -59.6  4.2      80.6    -5   1 12   5267  04 04 05
04 04 45  ---          00 27 29  38.8 -59.6  4.2      80.5    35   R  2   4733
  
04 04 45  2007+402     00 27 29  37.5 -60.2  4.3      79.1    -5   1 12   4733  04 04 45
04 05 15  ---          00 27 59  37.4 -60.2  4.3      79.0    25   R  2   4333
  
04 05 15  IRAS2012     00 27 59  38.7 -59.5  4.2      80.5    -5   1 12   4333  04 05 15
04 05 55  ---          00 28 39  38.6 -59.5  4.2      80.4    35   R  2   3800
  
04 05 55  2007+402     00 28 39  37.2 -60.1  4.3      78.9    -5   1 12   3800  04 05 55
04 06 25  ---          00 29 09  37.1 -60.1  4.4      78.8    25   R  2   3400
  
04 06 25  IRAS2012     00 29 09  38.5 -59.5  4.2      80.3    -5   1 12   3400  04 06 25
04 07 05  ---          00 29 49  38.4 -59.5  4.3      80.2    35   R  2   2867
  
04 07 05  2007+402     00 29 49  37.0 -60.1  4.4      78.7    -5   1 12   2867  04 07 05
04 07 35  ---          00 30 20  36.9 -60.1  4.4      78.7    25   R  2   2467
Schedule for VLBA_FD   (Code Fd )                                   Page  60
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
04 07 35  IRAS2012     00 30 20  38.3 -59.4  4.3      80.1    -5   1 12   2467  04 07 35
04 08 15  ---          00 31 00  38.2 -59.4  4.3      80.0    35   R  2   1933
  
04 08 15  2007+402     00 31 00  36.8 -60.0  4.4      78.6    -5   1 12   1933  04 08 15
04 08 45  ---          00 31 30  36.7 -60.0  4.4      78.5    25   R  2   1533
  
04 08 45  IRAS2012     00 31 30  38.1 -59.4  4.3      80.0    -5   1 12   1533  04 08 45
04 09 25  ---          00 32 10  38.0 -59.4  4.3      79.9    35   R  2   1000
  
04 09 25  2007+402     00 32 10  36.6 -60.0  4.4      78.4    -5   1 12   1000  04 09 25
04 09 55  ---          00 32 40  36.5 -59.9  4.4      78.4    25   R  2    600
  
04 09 55  IRAS2012     00 32 40  37.9 -59.3  4.3      79.8    -5   1 12    600  04 09 55
04 10 40  ---          00 33 25  37.7 -59.3  4.3      79.7    40   R  2      0
  
04 11 00  2002+472     00 33 45  36.5 -51.2  4.5      82.4    13   1 13      0  04 11 00
04 14 00  ---          00 36 46  36.0 -51.1  4.6      81.9   180   F  1   2400
  
04 14 20  2007+402     00 37 06  35.7 -59.7  4.5      77.8    12   1 13   2400  04 14 20
04 14 55  ---          00 37 41  35.6 -59.7  4.5      77.7    35   F  1   2867
  
04 14 55  IRAS2012     00 37 41  36.9 -59.1  4.4      79.1    -5   1 13   2867  04 14 55
04 15 35  ---          00 38 21  36.8 -59.1  4.4      79.0    35   F  1   3400
  
04 15 35  2007+402     00 38 21  35.4 -59.7  4.5      77.6    -5   1 13   3400  04 15 35
04 16 05  ---          00 38 51  35.3 -59.6  4.5      77.5    25   F  1   3800
  
04 16 05  IRAS2012     00 38 51  36.7 -59.1  4.4      79.0    -5   1 13   3800  04 16 05
04 16 45  ---          00 39 31  36.6 -59.0  4.4      78.9    35   F  1   4333
  
04 16 45  2007+402     00 39 31  35.2 -59.6  4.5      77.4    -5   1 13   4333  04 16 45
04 17 15  ---          00 40 01  35.1 -59.6  4.5      77.4    25   F  1   4733
  
04 17 15  IRAS2012     00 40 01  36.5 -59.0  4.4      78.8    -5   1 13   4733  04 17 15
04 17 55  ---          00 40 41  36.4 -59.0  4.4      78.7    35   F  1   5267
  
04 17 55  2007+402     00 40 41  35.0 -59.5  4.5      77.3    -5   1 13   5267  04 17 55
04 18 25  ---          00 41 11  34.9 -59.5  4.6      77.2    25   F  1   5667
  
04 18 25  IRAS2012     00 41 11  36.3 -59.0  4.4      78.6    -5   1 13   5667  04 18 25
04 19 05  ---          00 41 51  36.2 -58.9  4.5      78.5    35   F  1   6200
Schedule for VLBA_FD   (Code Fd )                                   Page  61
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
04 19 05  2007+402     00 41 51  34.8 -59.5  4.6      77.1    -5   1 13   6200  04 19 05
04 19 35  ---          00 42 22  34.7 -59.5  4.6      77.1    25   F  1   6600
  
04 19 35  IRAS2012     00 42 22  36.1 -58.9  4.5      78.5    -5   1 13   6600  04 19 35
04 20 15  ---          00 43 02  36.0 -58.9  4.5      78.4    35   F  1   7133
  
04 20 15  2007+402     00 43 02  34.6 -59.4  4.6      77.0    -5   1 13   7133  04 20 15
04 20 45  ---          00 43 32  34.5 -59.4  4.6      76.9    25   F  1   7533
  
04 20 45  IRAS2012     00 43 32  35.9 -58.9  4.5      78.3    -5   1 13   7533  04 20 45
04 21 25  ---          00 44 12  35.7 -58.8  4.5      78.2    35   F  1   8067
  
04 21 25  2007+402     00 44 12  34.4 -59.4  4.6      76.8    -5   1 13   8067  04 21 25
04 21 55  ---          00 44 42  34.3 -59.3  4.6      76.8    25   F  1   8467
  
04 21 55  IRAS2012     00 44 42  35.6 -58.8  4.5      78.2    -5   1 13   8467  04 21 55
04 22 35  ---          00 45 22  35.5 -58.8  4.5      78.1    35   F  1   9000
  
04 22 35  2007+402     00 45 22  34.1 -59.3  4.6      76.7    -5   1 13   9000  04 22 35
04 23 05  ---          00 45 52  34.0 -59.3  4.6      76.6    25   F  1   9400
  
04 23 05  IRAS2012     00 45 52  35.4 -58.8  4.5      78.0    -5   1 13   9400  04 23 05
04 23 50  ---          00 46 37  35.3 -58.7  4.5      77.9    40   F  1  10000
  
04 23 50  2007+402     00 46 37  33.9 -59.2  4.6      76.5    -5   1 13  10000  04 23 50
04 24 25  ---          00 47 12  33.8 -59.2  4.7      76.4    30   F  1  10467
  
04 24 25  IRAS2012     00 47 12  35.2 -58.7  4.5      77.8    -5   1 13  10467  04 24 25
04 25 05  ---          00 47 52  35.1 -58.7  4.6      77.7    35   F  1  11000
  
04 25 05  2007+402     00 47 52  33.7 -59.2  4.7      76.3    -5   1 13  11000  04 25 05
04 25 35  ---          00 48 23  33.6 -59.1  4.7      76.3    25   F  1  11400
  
04 25 35  IRAS2012     00 48 23  35.0 -58.6  4.6      77.7    -5   1 13  11400  04 25 35
04 26 15  ---          00 49 03  34.9 -58.6  4.6      77.6    35   F  1  11933
  
04 26 15  2007+402     00 49 03  33.5 -59.1  4.7      76.2    -5   1 13  11933  04 26 15
04 26 45  ---          00 49 33  33.4 -59.1  4.7      76.1    25   F  1  12333
  
04 26 45  IRAS2012     00 49 33  34.8 -58.6  4.6      77.5    -5   1 13  12333  04 26 45
04 27 25  ---          00 50 13  34.6 -58.5  4.6      77.4    35   F  1  12867
Schedule for VLBA_FD   (Code Fd )                                   Page  62
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
04 27 25  2007+402     00 50 13  33.2 -59.0  4.7      76.0    -5   1 13  12867  04 27 25
04 27 55  ---          00 50 43  33.1 -59.0  4.7      76.0    25   F  1  13267
  
04 27 55  IRAS2012     00 50 43  34.5 -58.5  4.6      77.3    -5   1 13  13267  04 27 55
04 28 35  ---          00 51 23  34.4 -58.5  4.6      77.2    35   F  1  13800
  
04 28 35  2007+402     00 51 23  33.0 -59.0  4.7      75.9    -5   1 13  13800  04 28 35
04 29 05  ---          00 51 53  32.9 -59.0  4.7      75.8    25   F  1  14200
  
04 29 05  IRAS2012     00 51 53  34.3 -58.5  4.6      77.2    -5   1 13  14200  04 29 05
04 29 45  ---          00 52 33  34.2 -58.4  4.6      77.1    35   F  1  14733
  
04 29 45  2007+402     00 52 33  32.8 -58.9  4.7      75.7    -5   1 13  14733  04 29 45
04 30 15  ---          00 53 03  32.7 -58.9  4.8      75.7    25   F  1  15133
  
04 30 15  IRAS2012     00 53 03  34.1 -58.4  4.6      77.0    -5   1 13  15133  04 30 15
04 30 55  ---          00 53 43  34.0 -58.4  4.7      76.9    35   F  1  15667
  
04 30 55  2007+402     00 53 43  32.6 -58.8  4.8      75.6    -5   1 13  15667  04 30 55
04 31 25  ---          00 54 13  32.5 -58.8  4.8      75.5    25   F  1  16067
  
04 31 25  IRAS2012     00 54 13  33.9 -58.3  4.7      76.9    -5   1 13  16067  04 31 25
04 32 05  ---          00 54 54  33.8 -58.3  4.7      76.8    35   F  1  16600
  
04 32 05  2007+402     00 54 54  32.4 -58.8  4.8      75.4    -5   1 13  16600  04 32 05
04 32 35  ---          00 55 24  32.3 -58.8  4.8      75.3    25   F  1  17000
  
04 32 35  IRAS2012     00 55 24  33.7 -58.3  4.7      76.7    -5   1 13  17000  04 32 35
04 33 20  ---          00 56 09  33.5 -58.2  4.7      76.6    40   F  1  17600
  
04 33 40  2007+402     00 56 29  32.1 -58.7  4.8      75.2    15   1 14  17600  04 33 40
04 34 25  ---          00 57 14  31.9 -58.6  4.8      75.1    45   R  1  17000
  
04 34 25  IRAS2012     00 57 14  33.4 -58.2  4.7      76.4    -5   1 14  17000  04 34 25
04 35 05  ---          00 57 54  33.2 -58.1  4.7      76.4    35   R  1  16467
  
04 35 05  2007+402     00 57 54  31.8 -58.6  4.8      75.0    -5   1 14  16467  04 35 05
04 35 35  ---          00 58 24  31.7 -58.6  4.8      74.9    25   R  1  16067
  
04 35 35  IRAS2012     00 58 24  33.1 -58.1  4.7      76.3    -5   1 14  16067  04 35 35
04 36 15  ---          00 59 04  33.0 -58.1  4.7      76.2    35   R  1  15533
Schedule for VLBA_FD   (Code Fd )                                   Page  63
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
04 36 15  2007+402     00 59 04  31.6 -58.5  4.9      74.9    -5   1 14  15533  04 36 15
04 36 45  ---          00 59 34  31.5 -58.5  4.9      74.8    25   R  1  15133
  
04 36 45  IRAS2012     00 59 34  32.9 -58.1  4.8      76.1    -5   1 14  15133  04 36 45
04 37 25  ---          01 00 14  32.8 -58.0  4.8      76.0    35   R  1  14600
  
04 37 25  2007+402     01 00 14  31.4 -58.5  4.9      74.7    -5   1 14  14600  04 37 25
04 37 55  ---          01 00 45  31.3 -58.4  4.9      74.6    25   R  1  14200
  
04 37 55  IRAS2012     01 00 45  32.7 -58.0  4.8      76.0    -5   1 14  14200  04 37 55
04 38 35  ---          01 01 25  32.6 -58.0  4.8      75.9    35   R  1  13667
  
04 38 35  2007+402     01 01 25  31.2 -58.4  4.9      74.5    -5   1 14  13667  04 38 35
04 39 05  ---          01 01 55  31.1 -58.4  4.9      74.5    25   R  1  13267
  
04 39 05  IRAS2012     01 01 55  32.5 -57.9  4.8      75.8    -5   1 14  13267  04 39 05
04 39 45  ---          01 02 35  32.4 -57.9  4.8      75.7    35   R  1  12733
  
04 39 45  2007+402     01 02 35  31.0 -58.3  4.9      74.4    -5   1 14  12733  04 39 45
04 40 15  ---          01 03 05  30.9 -58.3  4.9      74.3    25   R  1  12333
  
04 40 15  IRAS2012     01 03 05  32.3 -57.9  4.8      75.7    -5   1 14  12333  04 40 15
04 40 55  ---          01 03 45  32.2 -57.8  4.8      75.6    35   R  1  11800
  
04 40 55  2007+402     01 03 45  30.8 -58.3  4.9      74.2    -5   1 14  11800  04 40 55
04 41 25  ---          01 04 15  30.7 -58.2  4.9      74.2    25   R  1  11400
  
04 41 25  IRAS2012     01 04 15  32.1 -57.8  4.8      75.5    -5   1 14  11400  04 41 25
04 42 05  ---          01 04 55  31.9 -57.8  4.8      75.4    35   R  1  10867
  
04 42 05  2007+402     01 04 55  30.5 -58.2  5.0      74.1    -5   1 14  10867  04 42 05
04 42 35  ---          01 05 25  30.4 -58.2  5.0      74.0    25   R  1  10467
  
04 42 35  IRAS2012     01 05 25  31.9 -57.7  4.8      75.3    -5   1 14  10467  04 42 35
04 43 15  ---          01 06 05  31.7 -57.7  4.9      75.2    35   R  1   9933
  
04 43 15  2007+402     01 06 05  30.3 -58.1  5.0      73.9    -5   1 14   9933  04 43 15
04 43 45  ---          01 06 36  30.2 -58.1  5.0      73.9    25   R  1   9533
  
04 43 45  IRAS2012     01 06 36  31.6 -57.7  4.9      75.2    -5   1 14   9533  04 43 45
04 44 40  ---          01 07 31  31.5 -57.6  4.9      75.1    50   R  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page  64
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
04 44 40  2007+402     01 07 31  30.1 -58.0  5.0      73.7    -5   1 14   8800  04 44 40
04 45 25  ---          01 08 16  29.9 -58.0  5.0      73.6    40   R  1   8200
  
04 45 25  IRAS2012     01 08 16  31.3 -57.6  4.9      75.0    -5   1 14   8200  04 45 25
04 46 05  ---          01 08 56  31.2 -57.5  4.9      74.9    35   R  1   7667
  
04 46 05  2007+402     01 08 56  29.8 -57.9  5.0      73.6    -5   1 14   7667  04 46 05
04 46 35  ---          01 09 26  29.7 -57.9  5.0      73.5    25   R  1   7267
  
04 46 35  IRAS2012     01 09 26  31.1 -57.5  4.9      74.8    -5   1 14   7267  04 46 35
04 47 15  ---          01 10 06  31.0 -57.5  4.9      74.7    35   R  1   6733
  
04 47 15  2007+402     01 10 06  29.6 -57.9  5.0      73.4    -5   1 14   6733  04 47 15
04 47 45  ---          01 10 36  29.5 -57.8  5.0      73.3    25   R  1   6333
  
04 47 45  IRAS2012     01 10 36  30.9 -57.4  4.9      74.6    -5   1 14   6333  04 47 45
04 48 25  ---          01 11 16  30.8 -57.4  4.9      74.5    35   R  1   5800
  
04 48 25  2007+402     01 11 16  29.4 -57.8  5.1      73.3    -5   1 14   5800  04 48 25
04 48 55  ---          01 11 46  29.3 -57.8  5.1      73.2    25   R  1   5400
  
04 48 55  IRAS2012     01 11 46  30.7 -57.4  5.0      74.5    -5   1 14   5400  04 48 55
04 49 35  ---          01 12 26  30.6 -57.3  5.0      74.4    35   R  1   4867
  
04 49 35  2007+402     01 12 26  29.2 -57.7  5.1      73.1    -5   1 14   4867  04 49 35
04 50 05  ---          01 12 57  29.1 -57.7  5.1      73.0    25   R  1   4467
  
04 50 05  IRAS2012     01 12 57  30.5 -57.3  5.0      74.3    -5   1 14   4467  04 50 05
04 50 45  ---          01 13 37  30.4 -57.3  5.0      74.2    35   R  1   3933
  
04 50 45  2007+402     01 13 37  29.0 -57.7  5.1      72.9    -5   1 14   3933  04 50 45
04 51 15  ---          01 14 07  28.9 -57.6  5.1      72.9    25   R  1   3533
  
04 51 15  IRAS2012     01 14 07  30.3 -57.2  5.0      74.2    -5   1 14   3533  04 51 15
04 51 55  ---          01 14 47  30.2 -57.2  5.0      74.1    35   R  1   3000
  
04 51 55  2007+402     01 14 47  28.7 -57.6  5.1      72.8    -5   1 14   3000  04 51 55
04 52 25  ---          01 15 17  28.7 -57.5  5.1      72.7    25   R  1   2600
  
04 52 25  IRAS2012     01 15 17  30.1 -57.2  5.0      74.0    -5   1 14   2600  04 52 25
04 53 05  ---          01 15 57  29.9 -57.1  5.0      73.9    35   R  1   2067
Schedule for VLBA_FD   (Code Fd )                                   Page  65
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
04 53 05  2007+402     01 15 57  28.5 -57.5  5.1      72.6    -5   1 14   2067  04 53 05
04 53 35  ---          01 16 27  28.4 -57.5  5.1      72.6    25   R  1   1667
  
04 53 35  IRAS2012     01 16 27  29.9 -57.1  5.0      73.8    -5   1 14   1667  04 53 35
04 54 15  ---          01 17 07  29.7 -57.1  5.0      73.8    35   R  1   1133
  
04 54 15  2007+402     01 17 07  28.3 -57.4  5.2      72.5    -5   1 14   1133  04 54 15
04 54 45  ---          01 17 37  28.2 -57.4  5.2      72.4    25   R  1    733
  
04 54 45  IRAS2012     01 17 37  29.6 -57.0  5.1      73.7    -5   1 14    733  04 54 45
04 55 40  ---          01 18 32  29.5 -57.0  5.1      73.6    50   R  1      0
  
04 56 00  2007+402     01 18 53  28.0 -57.3  5.2      72.3    15   1 13      0  04 56 00
04 56 45  ---          01 19 38  27.9 -57.3  5.2      72.2    45   F  2    600
  
04 56 45  IRAS2012     01 19 38  29.3 -56.9  5.1      73.4    -5   1 13    600  04 56 45
04 57 25  ---          01 20 18  29.2 -56.9  5.1      73.3    35   F  2   1133
  
04 57 25  2007+402     01 20 18  27.7 -57.2  5.2      72.1    -5   1 13   1133  04 57 25
04 57 55  ---          01 20 48  27.7 -57.2  5.2      72.0    25   F  2   1533
  
04 57 55  IRAS2012     01 20 48  29.1 -56.8  5.1      73.3    -5   1 13   1533  04 57 55
04 58 35  ---          01 21 28  29.0 -56.8  5.1      73.2    35   F  2   2067
  
04 58 35  2007+402     01 21 28  27.5 -57.1  5.2      71.9    -5   1 13   2067  04 58 35
04 59 05  ---          01 21 58  27.4 -57.1  5.2      71.8    25   F  2   2467
  
04 59 05  IRAS2012     01 21 58  28.9 -56.8  5.1      73.1    -5   1 13   2467  04 59 05
04 59 45  ---          01 22 38  28.7 -56.7  5.1      73.0    35   F  2   3000
  
04 59 45  2007+402     01 22 38  27.3 -57.1  5.2      71.8    -5   1 13   3000  04 59 45
05 00 15  ---          01 23 08  27.2 -57.0  5.3      71.7    25   F  2   3400
  
05 00 15  IRAS2012     01 23 08  28.7 -56.7  5.1      72.9    -5   1 13   3400  05 00 15
05 00 55  ---          01 23 48  28.5 -56.6  5.2      72.9    35   F  2   3933
  
05 00 55  2007+402     01 23 48  27.1 -57.0  5.3      71.6    -5   1 13   3933  05 00 55
05 01 25  ---          01 24 18  27.0 -57.0  5.3      71.5    25   F  2   4333
  
05 01 25  IRAS2012     01 24 18  28.4 -56.6  5.2      72.8    -5   1 13   4333  05 01 25
05 02 05  ---          01 24 59  28.3 -56.6  5.2      72.7    35   F  2   4867
Schedule for VLBA_FD   (Code Fd )                                   Page  66
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
05 02 05  2007+402     01 24 59  26.9 -56.9  5.3      71.4    -5   1 13   4867  05 02 05
05 02 35  ---          01 25 29  26.8 -56.9  5.3      71.4    25   F  2   5267
  
05 02 35  IRAS2012     01 25 29  28.2 -56.5  5.2      72.6    -5   1 13   5267  05 02 35
05 03 15  ---          01 26 09  28.1 -56.5  5.2      72.5    35   F  2   5800
  
05 03 15  2007+402     01 26 09  26.7 -56.8  5.3      71.3    -5   1 13   5800  05 03 15
05 03 45  ---          01 26 39  26.6 -56.8  5.3      71.2    25   F  2   6200
  
05 03 45  IRAS2012     01 26 39  28.0 -56.5  5.2      72.5    -5   1 13   6200  05 03 45
05 04 25  ---          01 27 19  27.9 -56.4  5.2      72.4    35   F  2   6733
  
05 04 25  2007+402     01 27 19  26.5 -56.7  5.3      71.1    -5   1 13   6733  05 04 25
05 04 55  ---          01 27 49  26.4 -56.7  5.3      71.1    25   F  2   7133
  
05 04 55  IRAS2012     01 27 49  27.8 -56.4  5.2      72.3    -5   1 13   7133  05 04 55
05 05 35  ---          01 28 29  27.7 -56.3  5.2      72.2    35   F  2   7667
  
05 05 35  2007+402     01 28 29  26.3 -56.7  5.3      71.0    -5   1 13   7667  05 05 35
05 06 05  ---          01 28 59  26.2 -56.6  5.4      70.9    25   F  2   8067
  
05 06 05  IRAS2012     01 28 59  27.6 -56.3  5.2      72.2    -5   1 13   8067  05 06 05
05 07 00  ---          01 29 54  27.4 -56.2  5.3      72.0    50   F  2   8800
  
05 07 00  2007+402     01 29 54  26.0 -56.6  5.4      70.8    -5   1 13   8800  05 07 00
05 07 45  ---          01 30 39  25.9 -56.5  5.4      70.7    40   F  2   9400
  
05 07 45  IRAS2012     01 30 39  27.3 -56.2  5.3      71.9    -5   1 13   9400  05 07 45
05 08 25  ---          01 31 20  27.2 -56.2  5.3      71.8    35   F  2   9933
  
05 08 25  2007+402     01 31 20  25.8 -56.5  5.4      70.6    -5   1 13   9933  05 08 25
05 08 55  ---          01 31 50  25.7 -56.4  5.4      70.5    25   F  2  10333
  
05 08 55  IRAS2012     01 31 50  27.1 -56.1  5.3      71.8    -5   1 13  10333  05 08 55
05 09 35  ---          01 32 30  27.0 -56.1  5.3      71.7    35   F  2  10867
  
05 09 35  2007+402     01 32 30  25.5 -56.4  5.4      70.5    -5   1 13  10867  05 09 35
05 10 05  ---          01 33 00  25.5 -56.4  5.4      70.4    25   F  2  11267
  
05 10 05  IRAS2012     01 33 00  26.9 -56.0  5.3      71.6    -5   1 13  11267  05 10 05
05 10 45  ---          01 33 40  26.8 -56.0  5.3      71.5    35   F  2  11800
Schedule for VLBA_FD   (Code Fd )                                   Page  67
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
05 10 45  2007+402     01 33 40  25.3 -56.3  5.4      70.3    -5   1 13  11800  05 10 45
05 11 15  ---          01 34 10  25.2 -56.3  5.4      70.2    25   F  2  12200
  
05 11 15  IRAS2012     01 34 10  26.7 -56.0  5.3      71.5    -5   1 13  12200  05 11 15
05 11 55  ---          01 34 50  26.6 -55.9  5.3      71.4    35   F  2  12733
  
05 11 55  2007+402     01 34 50  25.1 -56.2  5.5      70.1    -5   1 13  12733  05 11 55
05 12 25  ---          01 35 20  25.0 -56.2  5.5      70.1    25   F  2  13133
  
05 12 25  IRAS2012     01 35 20  26.5 -55.9  5.3      71.3    -5   1 13  13133  05 12 25
05 13 05  ---          01 36 00  26.4 -55.8  5.4      71.2    35   F  2  13667
  
05 13 05  2007+402     01 36 00  24.9 -56.1  5.5      70.0    -5   1 13  13667  05 13 05
05 13 35  ---          01 36 30  24.8 -56.1  5.5      69.9    25   F  2  14067
  
05 13 35  IRAS2012     01 36 30  26.3 -55.8  5.4      71.1    -5   1 13  14067  05 13 35
05 14 15  ---          01 37 11  26.1 -55.8  5.4      71.1    35   F  2  14600
  
05 14 15  2007+402     01 37 11  24.7 -56.1  5.5      69.8    -5   1 13  14600  05 14 15
05 14 45  ---          01 37 41  24.6 -56.0  5.5      69.8    25   F  2  15000
  
05 14 45  IRAS2012     01 37 41  26.1 -55.7  5.4      71.0    -5   1 13  15000  05 14 45
05 15 25  ---          01 38 21  25.9 -55.7  5.4      70.9    35   F  2  15533
  
05 15 25  2007+402     01 38 21  24.5 -56.0  5.5      69.7    -5   1 13  15533  05 15 25
05 15 55  ---          01 38 51  24.4 -55.9  5.5      69.6    25   F  2  15933
  
05 15 55  IRAS2012     01 38 51  25.8 -55.6  5.4      70.8    -5   1 13  15933  05 15 55
05 16 35  ---          01 39 31  25.7 -55.6  5.4      70.7    35   F  2  16467
  
05 16 35  2007+402     01 39 31  24.3 -55.9  5.5      69.5    -5   1 13  16467  05 16 35
05 17 05  ---          01 40 01  24.2 -55.8  5.5      69.5    25   F  2  16867
  
05 17 05  IRAS2012     01 40 01  25.6 -55.6  5.4      70.7    -5   1 13  16867  05 17 05
05 18 00  ---          01 40 56  25.5 -55.5  5.4      70.6    50   F  2  17600
  
05 20 00  2007+777     01 42 56  31.1 -14.1  5.6      88.4    90   1 14  17600  05 20 00
05 23 00  ---          01 45 57  30.9 -14.1  5.7      87.6   180   R  2  15200
  
05 23 40  2007+402     01 46 37  23.0 -55.4  5.6      68.6    10   1 14  15200  05 23 40
05 24 15  ---          01 47 12  22.9 -55.3  5.7      68.5    35   R  2  14733
Schedule for VLBA_FD   (Code Fd )                                   Page  68
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
05 24 15  IRAS2012     01 47 12  24.4 -55.1  5.5      69.7    -5   1 14  14733  05 24 15
05 24 55  ---          01 47 52  24.3 -55.0  5.6      69.6    35   R  2  14200
  
05 24 55  2007+402     01 47 52  22.8 -55.3  5.7      68.4    -5   1 14  14200  05 24 55
05 25 25  ---          01 48 22  22.7 -55.2  5.7      68.4    25   R  2  13800
  
05 25 25  IRAS2012     01 48 22  24.2 -55.0  5.6      69.5    -5   1 14  13800  05 25 25
05 26 05  ---          01 49 02  24.0 -54.9  5.6      69.5    35   R  2  13267
  
05 26 05  2007+402     01 49 02  22.6 -55.2  5.7      68.3    -5   1 14  13267  05 26 05
05 26 35  ---          01 49 33  22.5 -55.1  5.7      68.2    25   R  2  12867
  
05 26 35  IRAS2012     01 49 33  24.0 -54.9  5.6      69.4    -5   1 14  12867  05 26 35
05 27 15  ---          01 50 13  23.8 -54.8  5.6      69.3    35   R  2  12333
  
05 27 15  2007+402     01 50 13  22.4 -55.1  5.7      68.1    -5   1 14  12333  05 27 15
05 27 45  ---          01 50 43  22.3 -55.0  5.7      68.0    25   R  2  11933
  
05 27 45  IRAS2012     01 50 43  23.8 -54.8  5.6      69.2    -5   1 14  11933  05 27 45
05 28 25  ---          01 51 23  23.6 -54.8  5.6      69.1    35   R  2  11400
  
05 28 25  2007+402     01 51 23  22.2 -55.0  5.7      68.0    -5   1 14  11400  05 28 25
05 28 55  ---          01 51 53  22.1 -55.0  5.7      67.9    25   R  2  11000
  
05 28 55  IRAS2012     01 51 53  23.5 -54.7  5.6      69.1    -5   1 14  11000  05 28 55
05 29 35  ---          01 52 33  23.4 -54.7  5.6      69.0    35   R  2  10467
  
05 29 35  2007+402     01 52 33  22.0 -54.9  5.7      67.8    -5   1 14  10467  05 29 35
05 30 05  ---          01 53 03  21.9 -54.9  5.8      67.7    25   R  2  10067
  
05 30 05  IRAS2012     01 53 03  23.3 -54.6  5.6      68.9    -5   1 14  10067  05 30 05
05 30 45  ---          01 53 43  23.2 -54.6  5.7      68.8    35   R  2   9533
  
05 30 45  2007+402     01 53 43  21.8 -54.8  5.8      67.6    -5   1 14   9533  05 30 45
05 31 15  ---          01 54 13  21.7 -54.8  5.8      67.6    25   R  2   9133
  
05 31 15  IRAS2012     01 54 13  23.1 -54.5  5.7      68.8    -5   1 14   9133  05 31 15
05 31 55  ---          01 54 53  23.0 -54.5  5.7      68.7    35   R  2   8600
  
05 31 55  2007+402     01 54 53  21.6 -54.7  5.8      67.5    -5   1 14   8600  05 31 55
05 32 25  ---          01 55 24  21.5 -54.7  5.8      67.4    25   R  2   8200
Schedule for VLBA_FD   (Code Fd )                                   Page  69
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
05 32 25  IRAS2012     01 55 24  22.9 -54.5  5.7      68.6    -5   1 14   8200  05 32 25
05 33 10  ---          01 56 09  22.8 -54.4  5.7      68.5    40   R  2   7600
  
05 33 10  2007+402     01 56 09  21.4 -54.6  5.8      67.3    -5   1 14   7600  05 33 10
05 33 45  ---          01 56 44  21.2 -54.6  5.8      67.2    30   R  2   7133
  
05 33 45  IRAS2012     01 56 44  22.7 -54.4  5.7      68.4    -5   1 14   7133  05 33 45
05 34 25  ---          01 57 24  22.6 -54.3  5.7      68.3    35   R  2   6600
  
05 34 25  2007+402     01 57 24  21.1 -54.5  5.8      67.2    -5   1 14   6600  05 34 25
05 34 55  ---          01 57 54  21.0 -54.5  5.8      67.1    25   R  2   6200
  
05 34 55  IRAS2012     01 57 54  22.5 -54.3  5.7      68.3    -5   1 14   6200  05 34 55
05 35 35  ---          01 58 34  22.4 -54.2  5.7      68.2    35   R  2   5667
  
05 35 35  2007+402     01 58 34  20.9 -54.4  5.8      67.0    -5   1 14   5667  05 35 35
05 36 05  ---          01 59 04  20.8 -54.4  5.9      66.9    25   R  2   5267
  
05 36 05  IRAS2012     01 59 04  22.3 -54.2  5.7      68.1    -5   1 14   5267  05 36 05
05 36 45  ---          01 59 44  22.2 -54.1  5.8      68.0    35   R  2   4733
  
05 36 45  2007+402     01 59 44  20.7 -54.3  5.9      66.8    -5   1 14   4733  05 36 45
05 37 15  ---          02 00 14  20.6 -54.3  5.9      66.8    25   R  2   4333
  
05 37 15  IRAS2012     02 00 14  22.1 -54.1  5.8      67.9    -5   1 14   4333  05 37 15
05 37 55  ---          02 00 54  22.0 -54.0  5.8      67.8    35   R  2   3800
  
05 37 55  2007+402     02 00 54  20.5 -54.2  5.9      66.7    -5   1 14   3800  05 37 55
05 38 25  ---          02 01 24  20.4 -54.2  5.9      66.6    25   R  2   3400
  
05 38 25  IRAS2012     02 01 24  21.9 -54.0  5.8      67.8    -5   1 14   3400  05 38 25
05 39 05  ---          02 02 05  21.8 -54.0  5.8      67.7    35   R  2   2867
  
05 39 05  2007+402     02 02 05  20.3 -54.1  5.9      66.5    -5   1 14   2867  05 39 05
05 39 35  ---          02 02 35  20.2 -54.1  5.9      66.5    25   R  2   2467
  
05 39 35  IRAS2012     02 02 35  21.7 -53.9  5.8      67.6    -5   1 14   2467  05 39 35
05 40 15  ---          02 03 15  21.6 -53.9  5.8      67.5    35   R  2   1933
  
05 40 15  2007+402     02 03 15  20.1 -54.1  5.9      66.4    -5   1 14   1933  05 40 15
05 40 45  ---          02 03 45  20.0 -54.0  5.9      66.3    25   R  2   1533
Schedule for VLBA_FD   (Code Fd )                                   Page  70
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
05 40 45  IRAS2012     02 03 45  21.5 -53.8  5.8      67.5    -5   1 14   1533  05 40 45
05 41 25  ---          02 04 25  21.4 -53.8  5.8      67.4    35   R  2   1000
  
05 41 25  2007+402     02 04 25  19.9 -54.0  5.9      66.2    -5   1 14   1000  05 41 25
05 41 55  ---          02 04 55  19.8 -53.9  6.0      66.1    25   R  2    600
  
05 41 55  IRAS2012     02 04 55  21.3 -53.7  5.8      67.3    -5   1 14    600  05 41 55
05 42 40  ---          02 05 40  21.1 -53.7  5.9      67.2    40   R  2      0
  
-----------  Tape Change ------------
  
05 43 00  2002+472     02 06 00  21.4 -46.6  6.1      67.6    13   2  1      0  05 43 00
05 46 00  ---          02 09 01  21.0 -46.4  6.1      67.1   180   F  1   2400
  
05 46 20  2007+402     02 09 21  19.1 -53.6  6.0      65.5    13   2  1   2400  05 46 20
05 46 55  ---          02 09 56  19.0 -53.5  6.0      65.5    35   F  1   2867
  
05 46 55  IRAS2012     02 09 56  20.4 -53.3  5.9      66.6    -5   2  1   2867  05 46 55
05 47 35  ---          02 10 36  20.3 -53.3  5.9      66.5    35   F  1   3400
  
05 47 35  2007+402     02 10 36  18.8 -53.4  6.0      65.4    -5   2  1   3400  05 47 35
05 48 05  ---          02 11 06  18.7 -53.4  6.1      65.3    25   F  1   3800
  
05 48 05  IRAS2012     02 11 06  20.2 -53.2  5.9      66.5    -5   2  1   3800  05 48 05
05 48 45  ---          02 11 46  20.1 -53.2  6.0      66.4    35   F  1   4333
  
05 48 45  2007+402     02 11 46  18.6 -53.4  6.1      65.2    -5   2  1   4333  05 48 45
05 49 15  ---          02 12 16  18.5 -53.3  6.1      65.1    25   F  1   4733
  
05 49 15  IRAS2012     02 12 16  20.0 -53.2  6.0      66.3    -5   2  1   4733  05 49 15
05 49 55  ---          02 12 56  19.9 -53.1  6.0      66.2    35   F  1   5267
  
05 49 55  2007+402     02 12 56  18.4 -53.3  6.1      65.1    -5   2  1   5267  05 49 55
05 50 25  ---          02 13 26  18.3 -53.2  6.1      65.0    25   F  1   5667
  
05 50 25  IRAS2012     02 13 26  19.8 -53.1  6.0      66.1    -5   2  1   5667  05 50 25
05 51 05  ---          02 14 07  19.7 -53.0  6.0      66.0    35   F  1   6200
  
05 51 05  2007+402     02 14 07  18.2 -53.2  6.1      64.9    -5   2  1   6200  05 51 05
05 51 35  ---          02 14 37  18.1 -53.1  6.1      64.8    25   F  1   6600
  
05 51 35  IRAS2012     02 14 37  19.6 -53.0  6.0      66.0    -5   2  1   6600  05 51 35
05 52 15  ---          02 15 17  19.5 -52.9  6.0      65.9    35   F  1   7133
Schedule for VLBA_FD   (Code Fd )                                   Page  71
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
05 52 15  2007+402     02 15 17  18.0 -53.1  6.1      64.7    -5   2  1   7133  05 52 15
05 52 45  ---          02 15 47  17.9 -53.0  6.1      64.7    25   F  1   7533
  
05 52 45  IRAS2012     02 15 47  19.4 -52.9  6.0      65.8    -5   2  1   7533  05 52 45
05 53 25  ---          02 16 27  19.3 -52.8  6.0      65.7    35   F  1   8067
  
05 53 25  2007+402     02 16 27  17.8 -53.0  6.1      64.6    -5   2  1   8067  05 53 25
05 53 55  ---          02 16 57  17.7 -52.9  6.2      64.5    25   F  1   8467
  
05 53 55  IRAS2012     02 16 57  19.2 -52.8  6.0      65.6    -5   2  1   8467  05 53 55
05 54 35  ---          02 17 37  19.1 -52.7  6.1      65.6    35   F  1   9000
  
05 54 35  2007+402     02 17 37  17.6 -52.9  6.2      64.4    -5   2  1   9000  05 54 35
05 55 05  ---          02 18 07  17.5 -52.8  6.2      64.4    25   F  1   9400
  
05 55 05  IRAS2012     02 18 07  19.0 -52.7  6.1      65.5    -5   2  1   9400  05 55 05
05 55 50  ---          02 18 52  18.9 -52.6  6.1      65.4    40   F  1  10000
  
05 55 50  2007+402     02 18 52  17.4 -52.7  6.2      64.2    -5   2  1  10000  05 55 50
05 56 25  ---          02 19 27  17.3 -52.7  6.2      64.2    30   F  1  10467
  
05 56 25  IRAS2012     02 19 27  18.8 -52.6  6.1      65.3    -5   2  1  10467  05 56 25
05 57 05  ---          02 20 08  18.7 -52.5  6.1      65.2    35   F  1  11000
  
05 57 05  2007+402     02 20 08  17.2 -52.6  6.2      64.1    -5   2  1  11000  05 57 05
05 57 35  ---          02 20 38  17.1 -52.6  6.2      64.0    25   F  1  11400
  
05 57 35  IRAS2012     02 20 38  18.6 -52.5  6.1      65.1    -5   2  1  11400  05 57 35
05 58 15  ---          02 21 18  18.5 -52.4  6.1      65.0    35   F  1  11933
  
05 58 15  2007+402     02 21 18  17.0 -52.5  6.2      63.9    -5   2  1  11933  05 58 15
05 58 45  ---          02 21 48  16.9 -52.5  6.2      63.8    25   F  1  12333
  
05 58 45  IRAS2012     02 21 48  18.4 -52.4  6.1      65.0    -5   2  1  12333  05 58 45
05 59 25  ---          02 22 28  18.3 -52.3  6.1      64.9    35   F  1  12867
  
05 59 25  2007+402     02 22 28  16.8 -52.4  6.2      63.8    -5   2  1  12867  05 59 25
05 59 55  ---          02 22 58  16.7 -52.4  6.3      63.7    25   F  1  13267
  
05 59 55  IRAS2012     02 22 58  18.2 -52.3  6.1      64.8    -5   2  1  13267  05 59 55
06 00 35  ---          02 23 38  18.1 -52.2  6.2      64.7    35   F  1  13800
Schedule for VLBA_FD   (Code Fd )                                   Page  72
               Proper motions of H2O masers in IRAS 20126+4104
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Fri  10 Nov 2000   Day 315 ---
  
06 00 35  2007+402     02 23 38  16.6 -52.3  6.3      63.6    -5   2  1  13800  06 00 35
06 01 05  ---          02 24 08  16.5 -52.3  6.3      63.5    25   F  1  14200
  
06 01 05  IRAS2012     02 24 08  18.0 -52.2  6.2      64.7    -5   2  1  14200  06 01 05
06 01 45  ---          02 24 48  17.9 -52.1  6.2      64.6    35   F  1  14733
  
06 01 45  2007+402     02 24 48  16.4 -52.2  6.3      63.4    -5   2  1  14733  06 01 45
06 02 15  ---          02 25 18  16.3 -52.2  6.3      63.4    25   F  1  15133
  
06 02 15  IRAS2012     02 25 18  17.8 -52.1  6.2      64.5    -5   2  1  15133  06 02 15
06 02 55  ---          02 25 59  17.7 -52.0  6.2      64.4    35   F  1  15667
  
06 02 55  2007+402     02 25 59  16.2 -52.1  6.3      63.3    -5   2  1  15667  06 02 55
06 03 25  ---          02 26 29  16.1 -52.1  6.3      63.2    25   F  1  16067
  
06 03 25  IRAS2012     02 26 29  17.6 -52.0  6.2      64.3    -5   2  1  16067  06 03 25
06 04 05  ---          02 27 09  17.5 -51.9  6.2      64.2    35   F  1  16600
  
06 04 05  2007+402     02 27 09  16.0 -52.0  6.3      63.1    -5   2  1  16600  06 04 05
06 04 35  ---          02 27 39  15.9 -52.0  6.3      63.0    25   F  1  17000
  
06 04 35  IRAS2012     02 27 39  17.4 -51.9  6.2      64.2    -5   2  1  17000  06 04 35
06 05 20  ---          02 28 24  17.2 -51.8  6.2      64.1    40   F  1  17600
 
 
SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.
 
 
 Setup file: gm043a.set
   Matches group v1cm_b3 in /usr/local/sched/catalogs/freq.dat
 
   Setup group:    2         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 32.000
   Number of channels:  2    Passes/head pos:   2       Speedup factor:   1.00
 
   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00
 
   1st LO= 21500.00 21500.00
   Net SB=        U        U
   Pol.  =     RCP      LCP 
   BBC   =        1        2
   BBC SB=        U        U
   IF    =       B        D 
 
   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1     15.4     12.4
 
  The following frequency sets based on this setup were used.
 
  Frequency Set:   8  Based on FREQ, BW, and/or DOPPLER in schedule.  Used pcal sets:   1
   LO sum=  22227.48 22227.48
   BBC fr=    727.48   727.48
   Bandwd=    16.000   16.000
 
  The following pulse cal sets were used with this setup:
 
   Pulse cal detection set:   1  PCAL = OFF 
    PCALXB1=   S1    S2    OFF   OFF   OFF   OFF   OFF   OFF
    PCALXB2=   M1    M2    OFF   OFF   OFF   OFF   OFF   OFF
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0
 
   Track assignments are: 
    track1=   2, 18
    track2=   3, 19
    barrel=roll_8   
 SOURCE LIST -- Proper motions of H2O masers in IRAS 20126+4104
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
  
   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 
  
   2012+410        * 20 12 40.983000     20 14 26.030317     20 14 26.649683   
 * IRAS2012        * 41 04 21.19600      41 13 32.63748      41 13 57.20640    
                     From catalog imbedded in main SCHED input file.
 
 * 2007+402          20 05 59.559049   * 20 07 44.945000     20 07 45.518613   
                     40 21 01.80214    * 40 29 48.60400      40 30 12.71891    
                     From catalog imbedded in main SCHED input file.
 
 * 2007+777          20 07 20.429674   * 20 05 30.998000     20 05 28.248977   
                     77 43 58.12250    * 77 52 43.24700      77 53 10.41013    
                     From catalog imbedded in main SCHED input file.
 
 * 2002+472          20 00 39.216117   * 20 02 10.418300     20 02 10.754727   
                     47 17 02.42779    * 47 25 28.77700      47 25 53.78344    
                     From catalog imbedded in main SCHED input file.
 
 
 
  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   IRAS2012            92.8
   2007+402            91.3
   2007+777           103.9
   2002+472            93.0
 
  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

