  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
 Exp. Code:  GG060   


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 18 Sept. 2003                      

PI:       Mike Garrett                                                    

Address:  JIVE                                                            
          Postbus 2                                                       
          7990 AA Dwingeloo                                               
          Netherlands                                                     

Phone:    +31 521 596511                                                  
EMAIL:    garrett@jive.nfra.nl                                            
Fax:      +31 521 596539                                                  
Phone during observation: +31 528 220842                                  

Observing mode: 16-1-2 Single Pol, 2-bit sampling, 327 MHz                

Notes:    Please Note... Phase-referencing expt,                          
          Observing frequency is 327 MHz                                  
          Request only 1 SINGLE WSRT Antenna pleeeeeease                  
          Switch the phase-cal OFF during observations please             

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  24 Oct 2004   Day 298 ---

 Next scan frequencies:   328.49   328.49
 Next BBC frequencies:    828.49   828.49
 Next scan bandwidths:      4.00     4.00

02 00 00  J0958+6533   21 15 30   6.5  -4.5 11.3       9.4     0   1  1      0  02 00 00
02 02 45  ---          21 18 15   6.5  -4.2 11.3       8.8   165   F  1   1100

02 02 45  M81M82       21 18 15  10.2  -3.4 11.4       8.3   -13   1  1   1100  02 02 45
02 10 20  ---          21 25 51  10.1  -2.7 11.5       6.6   442   F  1   4133

02 10 20  J0958+6533   21 25 51   6.4  -3.5 11.4       7.2   -13   1  1   4133  02 10 20
02 13 05  ---          21 28 37   6.4  -3.2 11.5       6.6   152   F  1   5233

02 13 05  M81M82       21 28 37  10.1  -2.5 11.5       6.0   -14   1  1   5233  02 13 05
02 20 40  ---          21 36 13  10.0  -1.8 11.7       4.3   441   F  1   8267

02 20 40  J0958+6533   21 36 13   6.3  -2.4 11.6       5.0   -14   1  1   8267  02 20 40
02 23 25  ---          21 38 58   6.3  -2.1 11.7       4.4   151   F  1   9367

02 23 25  M81M82       21 38 58  10.0  -1.5 11.7       3.7   -14   1  1   9367  02 23 25
02 31 00  ---          21 46 35  10.0  -0.8 11.8       2.1   441   F  1  12400

02 31 00  J0958+6533   21 46 35   6.2  -1.3 11.8       2.7   -14   1  1  12400  02 31 00
02 33 45  ---          21 49 20   6.2  -1.0 11.8       2.1   151   F  1  13500

02 33 45  M81M82       21 49 20  10.0  -0.6 11.9       1.5   -14   1  1  13500  02 33 45
02 41 20  ---          21 56 56  10.0   0.1-12.0      -0.2   441   F  1  16533

02 41 20  J0958+6533   21 56 56   6.2  -0.2 12.0       0.5   -14   1  1  16533  02 41 20
02 44 00  ---          21 59 37   6.2   0.1-12.0      -0.1   146   F  1  17600

02 46 00  J0958+6533   22 01 37   6.2   0.3-12.0      -0.5   115   1  2  17600  02 46 00
02 48 45  ---          22 04 23   6.2   0.5-11.9      -1.1   165   R  1  16500

02 48 45  M81M82       22 04 23  10.0   0.7-11.9      -1.8   -14   1  2  16500  02 48 45
02 56 20  ---          22 11 59  10.0   1.4-11.7      -3.5   441   R  1  13467

02 56 20  J0958+6533   22 11 59   6.2   1.3-11.8      -2.8   -14   1  2  13467  02 56 20
02 59 05  ---          22 14 44   6.2   1.6-11.7      -3.4   151   R  1  12367

02 59 05  M81M82       22 14 44  10.0   1.7-11.7      -4.1   -14   1  2  12367  02 59 05
03 06 40  ---          22 22 21  10.1   2.3-11.6      -5.7   441   R  1   9333
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  24 Oct 2004   Day 298 ---

03 06 40  J0958+6533   22 22 21   6.3   2.4-11.6      -5.0   -14   1  2   9333  03 06 40
03 09 25  ---          22 25 06   6.3   2.7-11.6      -5.6   151   R  1   8233

03 09 25  M81M82       22 25 06  10.1   2.6-11.5      -6.3   -14   1  2   8233  03 09 25
03 17 00  ---          22 32 42  10.2   3.3-11.4      -8.0   441   R  1   5200

03 17 00  J0958+6533   22 32 42   6.4   3.5-11.4      -7.3   -14   1  2   5200  03 17 00
03 19 45  ---          22 35 28   6.4   3.8-11.4      -7.9   151   R  1   4100

03 19 45  M81M82       22 35 28  10.2   3.5-11.3      -8.6   -14   1  2   4100  03 19 45
03 27 20  ---          22 43 04  10.4   4.2-11.2     -10.3   441   R  1   1067

03 27 20  J0958+6533   22 43 04   6.6   4.6-11.3      -9.5   -14   1  2   1067  03 27 20
03 30 00  ---          22 45 44   6.6   4.8-11.2     -10.1   146   R  1      0

03 32 00  J0958+6533   22 47 45   6.6   5.0-11.2     -10.5   115   1  1      0  03 32 00
03 34 45  ---          22 50 30   6.7   5.3-11.1     -11.1   165   F  2   1100

03 34 45  M81M82       22 50 30  10.5   4.8-11.1     -11.9   -14   1  1   1100  03 34 45
03 42 20  ---          22 58 06  10.6   5.5-11.0     -13.5   441   F  2   4133

03 42 20  J0958+6533   22 58 06   6.9   6.1-11.0     -12.7   -14   1  1   4133  03 42 20
03 45 05  ---          23 00 52   6.9   6.4-11.0     -13.3   151   F  2   5233

03 45 05  M81M82       23 00 52  10.7   5.7-10.9     -14.1   -14   1  1   5233  03 45 05
03 52 40  ---          23 08 28  10.9   6.4-10.8     -15.8   441   F  2   8267

03 52 40  J0958+6533   23 08 28   7.1   7.1-10.8     -15.0   -13   1  1   8267  03 52 40
03 55 25  ---          23 11 14   7.2   7.4-10.8     -15.6   152   F  2   9367

03 55 25  M81M82       23 11 14  10.9   6.6-10.7     -16.4   -13   1  1   9367  03 55 25
04 03 00  ---          23 18 50  11.1   7.3-10.6     -18.0   442   F  2  12400

04 03 00  J0958+6533   23 18 50   7.4   8.2-10.7     -17.2   -13   1  1  12400  04 03 00
04 05 45  ---          23 21 35   7.5   8.5-10.6     -17.8   152   F  2  13500

04 05 45  M81M82       23 21 35  11.2   7.5-10.6     -18.6   -13   1  1  13500  04 05 45
04 13 20  ---          23 29 11  11.4   8.2-10.4     -20.3   442   F  2  16533

04 13 20  J0958+6533   23 29 11   7.7   9.2-10.5     -19.4   -13   1  1  16533  04 13 20
04 16 00  ---          23 31 52   7.8   9.5-10.5     -20.0   147   F  2  17600

04 18 00  J0958+6533   23 33 52   7.9   9.7-10.4     -20.4   115   1  2  17600  04 18 00
04 20 45  ---          23 36 38   8.0   9.9-10.4     -21.0   165   R  2  16500
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  24 Oct 2004   Day 298 ---

04 20 45  M81M82       23 36 38  11.7   8.8-10.3     -21.9   -13   1  2  16500  04 20 45
04 28 20  ---          23 44 14  11.9   9.4-10.2     -23.6   442   R  2  13467

04 28 20  J0958+6533   23 44 14   8.3  10.7-10.2     -22.6   -13   1  2  13467  04 28 20
04 31 05  ---          23 46 59   8.4  10.9-10.2     -23.2   152   R  2  12367

04 31 05  M81M82       23 46 59  12.0   9.7-10.2     -24.2   -13   1  2  12367  04 31 05
04 38 40  ---          23 54 36  12.3  10.3-10.0     -25.8   442   R  2   9333

04 38 40  J0958+6533   23 54 36   8.7  11.7-10.1     -24.9   -13   1  2   9333  04 38 40
04 41 25  ---          23 57 21   8.9  11.9-10.0     -25.4   152   R  2   8233

04 41 25  M81M82       23 57 21  12.4  10.5-10.0     -26.4   -13   1  2   8233  04 41 25
04 49 00  ---          00 04 57  12.7  11.1 -9.9     -28.1   442   R  2   5200

04 49 00  J0958+6533   00 04 57   9.2  12.6 -9.9     -27.1   -13   1  2   5200  04 49 00
04 51 45  ---          00 07 43   9.3  12.9 -9.9     -27.6   152   R  2   4100

04 51 45  M81M82       00 07 43  12.8  11.3 -9.8     -28.7   -13   1  2   4100  04 51 45
04 59 20  ---          00 15 19  13.2  11.9 -9.7     -30.3   442   R  2   1067

04 59 20  J0958+6533   00 15 19   9.7  13.6 -9.7     -29.3   -13   1  2   1067  04 59 20
05 02 00  ---          00 17 59   9.8  13.8 -9.7     -29.8   147   R  2      0

05 04 00  J0958+6533   00 20 00   9.9  14.0 -9.7     -30.2   115   1  1      0  05 04 00
05 06 45  ---          00 22 45  10.1  14.3 -9.6     -30.8   165   F  3   1100

05 06 45  M81M82       00 22 45  13.5  12.5 -9.6     -31.9   -13   1  1   1100  05 06 45
05 14 20  ---          00 30 21  13.9  13.1 -9.4     -33.5   442   F  3   4133

05 14 20  J0958+6533   00 30 21  10.5  15.0 -9.5     -32.4   -13   1  1   4133  05 14 20
05 17 05  ---          00 33 07  10.7  15.2 -9.4     -33.0   152   F  3   5233

05 17 05  M81M82       00 33 07  14.0  13.3 -9.4     -34.1   -13   1  1   5233  05 17 05
05 24 40  ---          00 40 43  14.4  13.9 -9.3     -35.8   442   F  3   8267

05 24 40  J0958+6533   00 40 43  11.1  15.9 -9.3     -34.6   -13   1  1   8267  05 24 40
05 27 25  ---          00 43 29  11.3  16.1 -9.3     -35.2   152   F  3   9367

05 27 25  M81M82       00 43 29  14.5  14.1 -9.2     -36.4   -13   1  1   9367  05 27 25
05 35 00  ---          00 51 05  14.9  14.6 -9.1     -38.0   442   F  3  12400

05 35 00  J0958+6533   00 51 05  11.7  16.8 -9.1     -36.8   -12   1  1  12400  05 35 00
05 37 45  ---          00 53 50  11.9  17.0 -9.1     -37.4   153   F  3  13500
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  24 Oct 2004   Day 298 ---

05 37 45  M81M82       00 53 50  15.1  14.8 -9.0     -38.6   -12   1  1  13500  05 37 45
05 45 20  ---          01 01 27  15.5  15.4 -8.9     -40.2   443   F  3  16533

05 45 20  J0958+6533   01 01 27  12.4  17.6 -9.0     -39.0   -12   1  1  16533  05 45 20
05 48 00  ---          01 04 07  12.6  17.8 -8.9     -39.5   148   F  3  17600

05 56 00  3C84         01 12 08  62.1  58.1 -2.1    -102.7   375   1  2  17600  05 56 00
06 06 15  ---          01 22 25  64.0  57.1 -2.0    -105.3   615   R  3  13500

06 14 15  J0958+6533   01 30 26  14.4  19.9 -8.5     -45.1   375   1  2  13500  06 14 15
06 17 00  ---          01 33 12  14.6  20.1 -8.4     -45.6   165   R  3  12400

06 17 00  M81M82       01 33 12  17.4  17.5 -8.4     -47.1   -12   1  2  12400  06 17 00
06 24 35  ---          01 40 48  17.9  17.9 -8.3     -48.7   443   R  3   9367

06 24 35  J0958+6533   01 40 48  15.2  20.7 -8.3     -47.2   -12   1  2   9367  06 24 35
06 27 20  ---          01 43 33  15.4  20.9 -8.3     -47.8   153   R  3   8267

06 27 20  M81M82       01 43 33  18.1  18.1 -8.2     -49.3   -11   1  2   8267  06 27 20
06 34 55  ---          01 51 10  18.6  18.6 -8.1     -50.9   444   R  3   5233

06 34 55  J0958+6533   01 51 10  16.0  21.4 -8.1     -49.4   -11   1  2   5233  06 34 55
06 37 40  ---          01 53 55  16.2  21.6 -8.1     -50.0   154   R  3   4133

06 37 40  M81M82       01 53 55  18.8  18.7 -8.0     -51.5   -11   1  2   4133  06 37 40
06 45 15  ---          02 01 31  19.4  19.2 -7.9     -53.2   444   R  3   1100

06 45 15  J0958+6533   02 01 31  16.8  22.1 -8.0     -51.5   -11   1  2   1100  06 45 15
06 48 00  ---          02 04 17  17.0  22.3 -7.9     -52.1   154   R  3      0

06 50 00  J0958+6533   02 06 17  17.2  22.5 -7.9     -52.5   114   1  1      0  06 50 00
06 52 45  ---          02 09 03  17.4  22.6 -7.8     -53.1   165   F  4   1100

06 52 45  M81M82       02 09 03  19.9  19.6 -7.8     -54.8   -11   1  1   1100  06 52 45
07 00 20  ---          02 16 39  20.4  20.0 -7.7     -56.4   444   F  4   4133

07 00 20  J0958+6533   02 16 39  18.0  23.1 -7.7     -54.7   -11   1  1   4133  07 00 20
07 03 05  ---          02 19 24  18.3  23.3 -7.7     -55.3   154   F  4   5233

07 03 05  M81M82       02 19 24  20.6  20.1 -7.6     -57.0   -11   1  1   5233  07 03 05
07 10 40  ---          02 27 01  21.2  20.5 -7.5     -58.7   444   F  4   8267

07 10 40  J0958+6533   02 27 01  18.9  23.8 -7.5     -56.8   -11   1  1   8267  07 10 40
07 13 25  ---          02 29 46  19.2  23.9 -7.5     -57.4   154   F  4   9367
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  24 Oct 2004   Day 298 ---

07 13 25  M81M82       02 29 46  21.4  20.6 -7.4     -59.3   -10   1  1   9367  07 13 25
07 21 00  ---          02 37 22  22.0  21.0 -7.3     -60.9   445   F  4  12400

07 21 00  J0958+6533   02 37 22  19.8  24.4 -7.4     -59.0   -10   1  1  12400  07 21 00
07 23 45  ---          02 40 08  20.1  24.5 -7.3     -59.6   155   F  4  13500

07 23 45  M81M82       02 40 08  22.2  21.1 -7.3     -61.5   -10   1  1  13500  07 23 45
07 31 20  ---          02 47 44  22.8  21.5 -7.1     -63.2   445   F  4  16533

07 31 20  J0958+6533   02 47 44  20.8  24.9 -7.2     -61.2   -10   1  1  16533  07 31 20
07 34 00  ---          02 50 24  21.0  25.1 -7.1     -61.7   150   F  4  17600

07 36 00  J0958+6533   02 52 25  21.2  25.2 -7.1     -62.1   114   1  2  17600  07 36 00
07 38 45  ---          02 55 10  21.5  25.3 -7.1     -62.7   165   R  4  16500

07 38 45  M81M82       02 55 10  23.4  21.8 -7.0     -64.8   -10   1  2  16500  07 38 45
07 46 20  ---          03 02 46  24.0  22.1 -6.9     -66.4   445   R  4  13467

07 46 20  J0958+6533   03 02 46  22.2  25.7 -6.9     -64.3   -10   1  2  13467  07 46 20
07 49 05  ---          03 05 32  22.4  25.8 -6.9     -64.9   155   R  4  12367

07 49 05  M81M82       03 05 32  24.2  22.2 -6.8     -67.0   -10   1  2  12367  07 49 05
07 56 40  ---          03 13 08  24.9  22.5 -6.7     -68.7   445   R  4   9333

07 56 40  J0958+6533   03 13 08  23.1  26.2 -6.8     -66.5    -9   1  2   9333  07 56 40
07 59 25  ---          03 15 54  23.4  26.3 -6.7     -67.1   156   R  4   8233

07 59 25  M81M82       03 15 54  25.1  22.5 -6.7     -69.3    -9   1  2   8233  07 59 25
08 07 00  ---          03 23 30  25.7  22.8 -6.5     -71.0   446   R  4   5200

08 07 00  J0958+6533   03 23 30  24.1  26.6 -6.6     -68.7    -9   1  2   5200  08 07 00
08 09 45  ---          03 26 15  24.4  26.7 -6.5     -69.2   156   R  4   4100

08 09 45  M81M82       03 26 15  25.9  22.9 -6.5     -71.6    -9   1  2   4100  08 09 45
08 17 20  ---          03 33 52  26.6  23.1 -6.4     -73.3   446   R  4   1067

08 17 20  J0958+6533   03 33 52  25.1  27.0 -6.4     -70.8    -9   1  2   1067  08 17 20
08 20 00  ---          03 36 32  25.4  27.1 -6.4     -71.4   151   R  4      0

08 22 00  J0958+6533   03 38 32  25.6  27.2 -6.3     -71.8   114   1  3      0  08 22 00
08 24 45  ---          03 41 18  25.9  27.3 -6.3     -72.4   165   F  1   1100

08 24 45  M81M82       03 41 18  27.2  23.3 -6.2     -74.9    -9   1  3   1100  08 24 45
08 32 20  ---          03 48 54  27.9  23.5 -6.1     -76.6   446   F  1   4133
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  24 Oct 2004   Day 298 ---

08 32 20  J0958+6533   03 48 54  26.6  27.6 -6.2     -74.0    -9   1  3   4133  08 32 20
08 35 05  ---          03 51 39  26.9  27.6 -6.1     -74.6   156   F  1   5233

08 35 05  M81M82       03 51 39  28.1  23.6 -6.1     -77.2    -9   1  3   5233  08 35 05
08 42 40  ---          03 59 16  28.8  23.7 -5.9     -78.9   446   F  1   8267

08 42 40  J0958+6533   03 59 16  27.6  27.9 -6.0     -76.3    -9   1  3   8267  08 42 40
08 45 25  ---          04 02 01  27.9  27.9 -6.0     -76.8   156   F  1   9367

08 45 25  M81M82       04 02 01  29.0  23.8 -5.9     -79.5    -9   1  3   9367  08 45 25
08 53 00  ---          04 09 37  29.7  23.9 -5.8     -81.3   446   F  1  12400

08 53 00  J0958+6533   04 09 37  28.7  28.1 -5.8     -78.5    -9   1  3  12400  08 53 00
08 55 45  ---          04 12 23  29.0  28.2 -5.8     -79.1   156   F  1  13500

08 55 45  M81M82       04 12 23  29.9  23.9 -5.7     -81.9    -9   1  3  13500  08 55 45
09 03 20  ---          04 19 59  30.6  24.0 -5.6     -83.6   446   F  1  16533

09 03 20  J0958+6533   04 19 59  29.7  28.4 -5.7     -80.7    -9   1  3  16533  09 03 20
09 06 00  ---          04 22 40  30.0  28.4 -5.6     -81.3   151   F  1  17600

09 08 00  J0958+6533   04 24 40  30.2  28.4 -5.6     -81.8   114   1  4  17600  09 08 00
09 10 45  ---          04 27 25  30.5  28.5 -5.5     -82.4   165   R  1  16500

09 10 45  M81M82       04 27 25  31.2  24.1 -5.5     -85.3    -9   1  4  16500  09 10 45
09 18 20  ---          04 35 02  31.9  24.2 -5.4     -87.1   446   R  1  13467

09 18 20  J0958+6533   04 35 02  31.3  28.6 -5.4     -84.0    -9   1  4  13467  09 18 20
09 21 05  ---          04 37 47  31.6  28.6 -5.4     -84.6   156   R  1  12367

09 21 05  M81M82       04 37 47  32.1  24.2 -5.3     -87.7    -9   1  4  12367  09 21 05
09 28 40  ---          04 45 23  32.8  24.2 -5.2     -89.5   446   R  1   9333

09 28 40  J0958+6533   04 45 23  32.4  28.7 -5.2     -86.3    -9   1  4   9333  09 28 40
09 31 25  ---          04 48 09  32.6  28.7 -5.2     -87.0   156   R  1   8233

09 31 25  M81M82       04 48 09  33.0  24.2 -5.1     -90.1    -9   1  4   8233  09 31 25
09 39 00  ---          04 55 45  33.7  24.2 -5.0     -91.9   446   R  1   5200

09 39 00  J0958+6533   04 55 45  33.4  28.8 -5.1     -88.7    -9   1  4   5200  09 39 00
09 41 45  ---          04 58 30  33.7  28.8 -5.0     -89.3   156   R  1   4100

09 41 45  M81M82       04 58 30  34.0  24.2 -5.0     -92.6    -9   1  4   4100  09 41 45
09 49 20  ---          05 06 07  34.6  24.1 -4.8     -94.4   446   R  1   1067
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  24 Oct 2004   Day 298 ---

09 49 20  J0958+6533   05 06 07  34.5  28.8 -4.9     -91.0    -9   1  4   1067  09 49 20
09 52 00  ---          05 08 47  34.8  28.8 -4.8     -91.6   151   R  1      0

09 54 00  J0958+6533   05 10 47  35.0  28.7 -4.8     -92.1   114   1  3      0  09 54 00
09 56 45  ---          05 13 33  35.3  28.7 -4.8     -92.7   165   F  2   1100

09 56 45  M81M82       05 13 33  35.3  24.1 -4.7     -96.1    -9   1  3   1100  09 56 45
10 04 20  ---          05 21 09  35.9  24.0 -4.6     -98.0   446   F  2   4133

10 04 20  J0958+6533   05 21 09  36.1  28.7 -4.6     -94.5    -9   1  3   4133  10 04 20
10 07 05  ---          05 23 55  36.3  28.6 -4.6     -95.1   156   F  2   5233

10 07 05  M81M82       05 23 55  36.2  23.9 -4.5     -98.6    -9   1  3   5233  10 07 05
10 14 40  ---          05 31 31  36.8  23.8 -4.4    -100.5   446   F  2   8267

10 14 40  J0958+6533   05 31 31  37.1  28.5 -4.5     -96.9    -9   1  3   8267  10 14 40
10 17 25  ---          05 34 16  37.4  28.5 -4.4     -97.6   156   F  2   9367

10 17 25  M81M82       05 34 16  37.1  23.7 -4.4    -101.2    -9   1  3   9367  10 17 25
10 25 00  ---          05 41 53  37.7  23.5 -4.2    -103.1   446   F  2  12400

10 25 00  J0958+6533   05 41 53  38.2  28.3 -4.3     -99.4    -9   1  3  12400  10 25 00
10 27 45  ---          05 44 38  38.5  28.3 -4.2    -100.1   156   F  2  13500

10 27 45  M81M82       05 44 38  38.0  23.5 -4.2    -103.8    -9   1  3  13500  10 27 45
10 35 20  ---          05 52 14  38.6  23.2 -4.1    -105.7   446   F  2  16533

10 35 20  J0958+6533   05 52 14  39.2  28.1 -4.1    -101.9    -9   1  3  16533  10 35 20
10 38 00  ---          05 54 55  39.5  28.0 -4.1    -102.6   151   F  2  17600

10 40 00  M81M82       05 56 55  39.0  23.1 -4.0    -106.9   111   1  4  17600  10 40 00
10 47 35  ---          06 04 31  39.7  22.8 -3.9    -108.8   455   R  2  14567

10 47 35  J0958+6533   06 04 31  40.5  27.7 -3.9    -105.0    -9   1  4  14567  10 47 35
10 50 20  ---          06 07 17  40.8  27.6 -3.9    -105.7   156   R  2  13467

10 50 20  M81M82       06 07 17  39.9  22.7 -3.8    -109.5    -9   1  4  13467  10 50 20
10 57 35  ---          06 14 33  40.5  22.4 -3.7    -111.4   426   R  2  10567

10 57 35  J0958+6533   06 14 33  41.5  27.3 -3.7    -107.5    -9   1  4  10567  10 57 35
11 00 00  ---          06 16 58  41.7  27.2 -3.7    -108.1   136   R  2   9600


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: GG060.90cm
   Matches group v5090n in /aps3/sched/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:   32
   Format: VLBA1:2           Bits per sample: 2         Sample rate:  8.000
   Number of channels:  2    Passes/head pos:   4       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=   -500.00   -500.00
   Net SB=         U         U
   Pol.  =      RCP       LCP 
   BBC   =         1         2
   BBC SB=         U         U
   IF    =        B         D 

   VLBA FE=     omit     90cm     omit     90cm
   VLBA Synth=  15.4     15.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=     328.49    328.49
   BBC fr=     828.49    828.49
   Bandwd=      4.000     4.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = OFF 
    PCALXB1=   S1    S2    OFF   OFF   OFF   OFF   OFF   OFF
    PCALXB2=   M1    M2    OFF   OFF   OFF   OFF   OFF   OFF
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0

   Track assignments are: 
    track1=   2, 10
    track2=  18, 26
    track3=   3, 11
    track4=  19, 27
    barrel=roll_off 
 SOURCE LIST -- Wide-field VLBI 327 MHz Observations of the M81/M82 Complex
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * M81M82            09 51 34.654386   * 09 55 41.933500     09 56 04.245779 
                     69 36 32.76608    * 69 22 19.37550      69 20 50.30297 
                     From catalog imbedded in main SCHED input file.

 * J0958+6533        09 54 57.847922   * 09 58 47.245102     09 59 07.942136 
                     65 48 15.53887    * 65 33 54.81806      65 32 25.99567 
                     From catalog imbedded in main SCHED input file.

   J0319+4130        03 16 29.567273   * 03 19 48.160103     03 20 07.879329 
   0316+413          41 19 51.91592    * 41 30 42.10305      41 31 49.47194 
 * 3C84              /aps3/sched/catalogs/sources.vlba
   J0319+41          ICRF - Ext.1 Source - 1998 IERS Annual Report



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   M81M82              91.2
   J0958+6533          88.9
   3C84               145.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

