  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Large Scale Jet of 0716+714
 Exp. Code:  gi002   


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 18 Sept. 2003                      

PI:       V. Impellizzeri/ T. Krichbaum                                   

Address:  Max-Planck-Institut fuer Radioastronomie                        
          Auf dem Huegel 69                                               
          53121 Bonn                                                      
          Germany                                                         

Phone:    0049-228-525-366                                                
EMAIL:    violette@mpifr-bonn.mpg.de                                      
Fax:      0049-228-525-229                                                
Phone during observation: 0049-228-525-366                                

Observing mode: 128-8-2                                                   

Notes:    VLBA at 90+50cm, EVN only at 90cm, all dual pol                 
          for EVPA calibration: 0836+71 and 1150+81                       
          All stations must record on TAPE - Socorro Correlator           
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Large Scale Jet of 0716+714
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  23 Oct 2004   Day 297 ---

 Next scan frequencies:   320.49   320.49   324.49   324.49   328.49   328.49
                          608.99   608.99
 Next BBC frequencies:    820.49   820.49   824.49   824.49   828.49   828.49
                          608.99   608.99
 Next scan bandwidths:      4.00     4.00     4.00     4.00     4.00     4.00
                            4.00     4.00

00 00 00  0716+714     19 11 13  12.0  -0.9 11.8       2.5     0   1  1      0  00 00 00
00 11 00  ---          19 22 15  12.0   0.0 12.0       0.0   660   F  1   4400

00 13 00  1150+812     19 24 15  26.8  -9.4  7.5      62.8    84   1  1   4400  00 13 00
00 18 30  ---          19 29 46  26.6  -9.2  7.6      61.5   330   F  1   6600

00 22 00  0836+710     19 33 17  12.2  -5.7 10.9      15.0   175   1  1   6600  00 22 00
00 27 30  ---          19 38 48  12.1  -5.2 10.9      13.8   330   F  1   8800

00 29 30  0716+714     19 40 48  12.0   1.5-11.7      -4.0   110   1  1   8800  00 29 30
00 40 30  ---          19 51 50  12.1   2.4-11.5      -6.5   660   F  1  13200

00 41 30  0716+714     19 52 50  12.1   2.5-11.5      -6.7    55   1  1  13200  00 41 30
00 52 30  ---          20 03 52  12.2   3.4-11.3      -9.1   660   F  1  17600

00 53 30  0716+714     20 04 52  12.2   3.5-11.3      -9.3    55   1  2  17600  00 53 30
01 04 30  ---          20 15 54  12.4   4.3-11.1     -11.8   660   R  1  13200

01 06 30  1150+812     20 17 54  25.0  -8.1  8.4      50.1    89   1  2  13200  01 06 30
01 12 00  ---          20 23 25  24.9  -7.9  8.5      48.8   330   R  1  11000

01 15 30  0836+710     20 26 56  11.5  -1.2 11.8       3.3   177   1  2  11000  01 15 30
01 21 00  ---          20 32 27  11.5  -0.8 11.8       2.1   330   R  1   8800

01 23 00  0716+714     20 34 27  12.8   5.8-10.8     -15.8   110   1  2   8800  01 23 00
01 34 00  ---          20 45 29  13.0   6.7-10.6     -18.2   660   R  1   4400

01 35 00  0716+714     20 46 29  13.0   6.8-10.6     -18.5    55   1  2   4400  01 35 00
01 46 00  ---          20 57 31  13.3   7.6-10.4     -20.9   660   R  1      0

01 47 00  0716+714     20 58 31  13.4   7.7-10.4     -21.1    55   1  3      0  01 47 00
01 58 00  ---          21 09 33  13.7   8.5-10.2     -23.5   660   F  1   4400

02 00 00  1150+812     21 11 33  23.6  -6.4  9.3      37.5    94   1  3   4400  02 00 00
02 05 30  ---          21 17 04  23.5  -6.2  9.4      36.3   330   F  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Large Scale Jet of 0716+714
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  23 Oct 2004   Day 297 ---

02 09 00  0836+710     21 20 34  11.7   3.2-11.4      -8.5   181   1  3   6600  02 09 00
02 14 30  ---          21 26 05  11.8   3.7-11.3      -9.7   330   F  1   8800

02 16 30  0716+714     21 28 06  14.3   9.9 -9.9     -27.6   109   1  3   8800  02 16 30
02 27 30  ---          21 39 08  14.8  10.7 -9.7     -30.0   660   F  1  13200

02 28 30  0716+714     21 40 08  14.8  10.8 -9.7     -30.2    55   1  3  13200  02 28 30
02 39 30  ---          21 51 09  15.3  11.6 -9.5     -32.6   660   F  1  17600

02 40 30  0716+714     21 52 10  15.3  11.6 -9.5     -32.8    55   1  4  17600  02 40 30
02 51 30  ---          22 03 11  15.8  12.4 -9.3     -35.2   660   R  1  13200

02 53 30  1150+812     22 05 12  22.5  -4.4 10.2      25.1   101   1  4  13200  02 53 30
02 59 00  ---          22 10 43  22.4  -4.2 10.3      23.8   330   R  1  11000

03 02 30  0836+710     22 14 13  12.8   7.6-10.5     -20.2   185   1  4  11000  03 02 30
03 08 00  ---          22 19 44  13.0   8.0-10.4     -21.5   330   R  1   8800

03 10 00  0716+714     22 21 45  16.7  13.6 -9.0     -39.3   107   1  4   8800  03 10 00
03 21 00  ---          22 32 46  17.3  14.3 -8.8     -41.7   660   R  1   4400

03 22 00  0716+714     22 33 46  17.3  14.4 -8.8     -41.9    55   1  4   4400  03 22 00
03 33 00  ---          22 44 48  17.9  15.1 -8.6     -44.3   660   R  1      0

03 34 00  0716+714     22 45 48  18.0  15.1 -8.6     -44.5    55   1  5      0  03 34 00
03 45 00  ---          22 56 50  18.6  15.8 -8.4     -47.0   660   F  1   4400

03 49 00  1150+812     23 00 51  21.8  -2.2 11.1      12.2   222   1  5   4400  03 49 00
03 54 30  ---          23 06 22  21.8  -2.0 11.2      10.9   330   F  1   6600

03 58 00  0836+710     23 09 52  14.9  11.8 -9.5     -32.4   190   1  5   6600  03 58 00
04 03 30  ---          23 15 23  15.1  12.2 -9.4     -33.6   330   F  1   8800

04 05 30  0716+714     23 17 24  19.9  16.9 -8.1     -51.4   104   1  5   8800  04 05 30
04 16 30  ---          23 28 25  20.6  17.5 -7.9     -53.9   660   F  1  13200

04 17 30  0716+714     23 29 26  20.6  17.5 -7.9     -54.1    55   1  5  13200  04 17 30
04 28 30  ---          23 40 27  21.4  18.1 -7.7     -56.5   660   F  1  17600

04 29 30  0716+714     23 41 28  21.4  18.1 -7.7     -56.7    55   1  6  17600  04 29 30
04 40 30  ---          23 52 29  22.2  18.6 -7.5     -59.1   660   R  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Large Scale Jet of 0716+714
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  23 Oct 2004   Day 297 ---

04 44 30  1150+812     23 56 30  21.6   0.1-11.9      -0.7   222   1  6  13200  04 44 30
04 50 00  ---          00 02 01  21.6   0.4-11.9      -2.0   330   R  1  11000

04 53 30  0836+710     00 05 32  17.7  15.5 -8.6     -44.5   194   1  6  11000  04 53 30
04 59 00  ---          00 11 02  18.0  15.8 -8.5     -45.7   330   R  1   8800

05 01 00  0716+714     00 13 03  23.6  19.5 -7.2     -63.7   103   1  6   8800  05 01 00
05 12 00  ---          00 24 05  24.4  19.9 -7.0     -66.1   660   R  1   4400

05 13 00  0716+714     00 25 05  24.5  19.9 -7.0     -66.4    55   1  6   4400  05 13 00
05 24 00  ---          00 36 07  25.3  20.3 -6.8     -68.8   660   R  1      0

05 25 00  0716+714     00 37 07  25.4  20.3 -6.8     -69.0    55   1  7      0  05 25 00
05 36 00  ---          00 48 08  26.2  20.7 -6.6     -71.5   660   F  1   4400

05 40 00  1150+812     00 52 09  21.9   2.5-11.0     -13.6   222   1  7   4400  05 40 00
05 45 30  ---          00 57 40  21.9   2.7-10.9     -14.9   330   F  1   6600

05 49 00  0836+710     01 01 11  21.2  18.5 -7.7     -56.6   193   1  7   6600  05 49 00
05 54 30  ---          01 06 42  21.6  18.8 -7.6     -57.8   330   F  1   8800

05 56 30  0716+714     01 08 42  27.8  21.2 -6.2     -76.1   102   1  7   8800  05 56 30
06 07 30  ---          01 19 44  28.7  21.4 -6.0     -78.6   660   F  1  13200

06 08 30  0716+714     01 20 44  28.7  21.4 -6.0     -78.9    55   1  7  13200  06 08 30
06 19 30  ---          01 31 46  29.6  21.6 -5.8     -81.4   660   F  1  17600

06 20 30  0716+714     01 32 46  29.7  21.6 -5.8     -81.6    55   1  8  17600  06 20 30
06 31 30  ---          01 43 48  30.6  21.7 -5.6     -84.2   660   R  1  13200

06 35 30  1150+812     01 47 48  22.6   4.7-10.1     -26.5   218   1  8  13200  06 35 30
06 41 00  ---          01 53 19  22.7   4.9-10.0     -27.8   330   R  1  11000

06 44 30  0836+710     01 56 50  25.2  20.8 -6.8     -68.9   193   1  8  11000  06 44 30
06 50 00  ---          02 02 21  25.7  21.0 -6.7     -70.1   330   R  1   8800

06 52 00  0716+714     02 04 21  32.2  21.8 -5.3     -89.0   101   1  8   8800  06 52 00
07 03 00  ---          02 15 23  33.1  21.8 -5.1     -91.6   660   R  1   4400

07 04 00  0716+714     02 16 23  33.2  21.8 -5.1     -91.8    55   1  8   4400  07 04 00
07 15 00  ---          02 27 25  34.0  21.8 -4.9     -94.5   660   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Large Scale Jet of 0716+714
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  23 Oct 2004   Day 297 ---

07 16 00  0716+714     02 28 25  34.1  21.8 -4.9     -94.7    55   1  9      0  07 16 00
07 27 00  ---          02 39 27  35.0  21.6 -4.7     -97.4   660   F  1   4400

07 31 00  1150+812     02 43 27  23.8   6.7 -9.2     -39.5   212   1  9   4400  07 31 00
07 36 30  ---          02 48 58  23.9   6.9 -9.1     -40.7   330   F  1   6600

07 40 00  0836+710     02 52 29  29.6  22.1 -5.8     -81.4   193   1  9   6600  07 40 00
07 45 30  ---          02 58 00  30.1  22.2 -5.7     -82.7   330   F  1   8800

07 47 30  0716+714     03 00 00  36.6  21.3 -4.4    -102.5   101   1  9   8800  07 47 30
07 58 30  ---          03 11 02  37.5  21.0 -4.2    -105.3   660   F  1  13200

07 59 30  0716+714     03 12 02  37.6  21.0 -4.2    -105.5    55   1  9  13200  07 59 30
08 10 30  ---          03 23 04  38.4  20.7 -4.0    -108.3   660   F  1  17600

08 11 30  0716+714     03 24 04  38.5  20.6 -4.0    -108.6    55   1 10  17600  08 11 30
08 22 30  ---          03 35 06  39.3  20.3 -3.8    -111.4   660   R  1  13200

08 26 30  1150+812     03 39 07  25.4   8.3 -8.2     -52.5   206   1 10  13200  08 26 30
08 32 00  ---          03 44 37  25.5   8.5 -8.1     -53.8   330   R  1  11000

08 35 30  0836+710     03 48 08  34.2  22.3 -4.9     -94.5   187   1 10  11000  08 35 30
08 41 00  ---          03 53 39  34.6  22.3 -4.8     -95.8   330   R  1   8800

08 43 00  0716+714     03 55 39  40.8  19.4 -3.4    -116.9   102   1 10   8800  08 43 00
08 54 00  ---          04 06 41  41.6  18.8 -3.3    -119.9   660   R  1   4400

08 55 00  0716+714     04 07 41  41.6  18.8 -3.2    -120.1    55   1 10   4400  08 55 00
09 06 00  ---          04 18 43  42.4  18.1 -3.1    -123.2   660   R  1      0

09 07 00  0716+714     04 19 43  42.5  18.1 -3.0    -123.4    55   1 11      0  09 07 00
09 18 00  ---          04 30 45  43.2  17.4 -2.9    -126.5   660   F  1   4400

09 22 00  1150+812     04 34 46  27.2   9.6 -7.3     -65.7   202   1 11   4400  09 22 00
09 27 30  ---          04 40 17  27.4   9.7 -7.2     -67.0   330   F  1   6600

09 31 00  0836+710     04 43 47  38.6  21.2 -4.0    -108.3   182   1 11   6600  09 31 00
09 36 30  ---          04 49 18  39.1  21.0 -3.9    -109.7   330   F  1   8800

09 38 30  0716+714     04 51 18  44.5  15.9 -2.5    -132.4   103   1 11   8800  09 38 30
09 49 30  ---          05 02 20  45.1  15.1 -2.3    -135.6   660   F  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Large Scale Jet of 0716+714
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  23 Oct 2004   Day 297 ---

09 50 30  0716+714     05 03 20  45.2  15.0 -2.3    -135.9    55   1 11  13200  09 50 30
10 01 30  ---          05 14 22  45.7  14.1 -2.1    -139.2   660   F  1  17600

10 02 30  0716+714     05 15 22  45.8  14.0 -2.1    -139.5    55   1 12  17600  10 02 30
10 13 30  ---          05 26 24  46.4  13.0 -1.9    -142.8   660   R  1  13200

10 17 30  1150+812     05 30 25  29.3  10.3 -6.4     -79.1   200   1 12  13200  10 17 30
10 23 00  ---          05 35 56  29.5  10.4 -6.3     -80.4   330   R  1  11000

10 26 30  0836+710     05 39 26  42.7  18.6 -3.0    -123.2   178   1 12  11000  10 26 30
10 32 00  ---          05 44 57  43.1  18.2 -2.9    -124.7   330   R  1   8800

10 34 00  0716+714     05 46 57  47.3  11.0 -1.6    -149.1   106   1 12   8800  10 34 00
10 45 00  ---          05 57 59  47.7   9.9 -1.4    -152.6   660   R  1   4400

10 46 00  0716+714     05 58 59  47.7   9.8 -1.4    -152.9    55   1 12   4400  10 46 00
10 57 00  ---          06 10 01  48.1   8.6 -1.2    -156.4   660   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: v9050cm
   Matches group v5090n in freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  128
   Format: VLBA1:2           Bits per sample: 2         Sample rate:  8.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=   -500.00   -500.00   -500.00   -500.00   -500.00   -500.00      0.00      0.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     90cm     omit     90cm
   VLBA Synth=  15.4     15.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=     320.49    320.49    324.49    324.49    328.49    328.49    608.99    608.99
   BBC fr=     820.49    820.49    824.49    824.49    828.49    828.49    608.99    608.99
   Bandwd=      4.000     4.000     4.000     4.000     4.000     4.000     4.000     4.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510    10  2510  2510  2510  3010
    PCALFR2=   510   510   510    10  2510  2510  2510  3010

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- Large Scale Jet of 0716+714
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

   J0721+7120        07 16 13.029725   * 07 21 53.448460     07 22 26.149165 
 * 0716+714          71 26 15.17405    * 71 20 36.36339      71 19 55.83740 
   J0721+71          /homes/vlbsoft/sched/catalogs/sources.vlba
                     ICRF - Ext.1 Source - 1998 IERS Annual Report

   J0841+7053        08 36 21.556642   * 08 41 24.365280     08 41 52.588367 
 * 0836+710          71 04 22.42747    * 70 53 42.17309      70 52 32.56061 
   J0841+70          /homes/vlbsoft/sched/catalogs/sources.vlba
                     ICRF - Ext.1 Source - 1998 IERS Annual Report

   J1153+8058        11 50 23.482288   * 11 53 12.499130     11 53 24.442535 
 * 1150+812          81 15 10.31168    * 80 58 29.15451      80 56 47.20426 
   J1153+80          /homes/vlbsoft/sched/catalogs/sources.vlba
                     ICRF - Ext.1 Source - 1998 IERS Annual Report



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0716+714           103.3
   0836+710            96.9
   1150+812            93.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

