  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1993J @ 6cm
 Exp. Code:  GM055A  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 18 Sept. 2003                      

PI:       J.M.Marcaide                                                    

Address:  Universitat de Valencia                                         
          C/ Dr. Moliner, 50                                              
          Burjassot, E 46100, Spain                                       
                                                                          

Phone:    34-96-398-3079/8 (work) or 34-96-337-1786 (home)                
EMAIL:    J.M.Marcaide@uv.es (internet)                                   
Fax:      34-96-398-3084                                                  
Phone during observation: 34-958-121311 (work) or 34-958-810928 (home)    

Observing mode: VLBA                                                      

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

 Next scan frequencies:  4966.49  4966.49  4982.49  4982.49  4998.49  4998.49
                         5014.49  5014.49
 Next BBC frequencies:    866.49   866.49   882.49   882.49   898.49   898.49
                          914.49   914.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

11 07 00  2007+777     06 51 35  19.1  -4.0 10.8      16.7     0   1  1      0  11 07 00
11 11 00  ---          06 55 36  19.0  -3.8 10.8      15.8   240   F  1   3200

11 12 48  1803+784     06 57 24  19.4   3.0-11.1     -13.0    97   1  1   3200  11 12 48
11 19 48  ---          07 04 25  19.5   3.4-10.9     -14.6   420   F  1   8800

11 21 32  2007+777     07 06 10  18.9  -3.2 11.0      13.4    94   1  1   8800  11 21 32
11 28 32  ---          07 13 11  18.8  -2.9 11.1      11.8   420   F  1  14400

11 30 20  1803+784     07 14 59  19.7   3.9-10.8     -17.0    97   1  1  14400  11 30 20
11 34 20  ---          07 18 59  19.7   4.1-10.7     -17.9   240   F  1  17600

11 41 11  M81          07 25 52  46.1  18.3 -2.5    -131.0   353   1  2  17600  11 41 11
11 45 11  ---          07 29 53  46.3  18.0 -2.4    -132.2   240   R  1  14400

11 45 26  SN1993J      07 30 08  46.4  18.0 -2.4    -132.2    10   1  2  14400  11 45 26
11 52 26  ---          07 37 09  46.8  17.3 -2.3    -134.3   420   R  1   8800

11 52 41  M81          07 37 24  46.8  17.3 -2.3    -134.4    10   1  2   8800  11 52 41
11 56 41  ---          07 41 25  47.1  16.9 -2.2    -135.6   240   R  1   5600

11 56 57  SN1993J      07 41 40  47.1  16.9 -2.2    -135.7    10   1  2   5600  11 56 57
12 03 57  ---          07 48 41  47.6  16.2 -2.1    -137.8   420   R  1      0

12 04 37  M81          07 49 21  47.6  16.1 -2.1    -138.0    35   1  3      0  12 04 37
12 09 37  ---          07 54 22  47.8  15.6 -2.0    -139.6   300   F  1   4000

12 09 52  SN1993J      07 54 37  47.9  15.6 -2.0    -139.7    10   1  3   4000  12 09 52
12 16 52  ---          08 01 38  48.3  14.9 -1.9    -141.8   420   F  1   9600

12 17 44  0917+624     08 02 31  55.9  16.4 -1.3    -148.6    31   1  3   9600  12 17 44
12 20 44  ---          08 05 32  56.1  15.8 -1.3    -149.7   180   F  1  12000

12 21 37  SN1993J      08 06 24  48.6  14.4 -1.8    -143.3    31   1  3  12000  12 21 37
12 28 37  ---          08 13 25  48.9  13.6 -1.7    -145.6   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

12 29 17  M81          08 14 05  48.9  13.5 -1.7    -145.7    35   1  4  17600  12 29 17
12 33 17  ---          08 18 06  49.1  13.1 -1.6    -147.0   240   R  1  14400

12 33 32  SN1993J      08 18 21  49.2  13.1 -1.6    -147.1    10   1  4  14400  12 33 32
12 40 32  ---          08 25 22  49.5  12.2 -1.5    -149.4   420   R  1   8800

12 40 47  M81          08 25 38  49.5  12.2 -1.5    -149.4    10   1  4   8800  12 40 47
12 44 47  ---          08 29 38  49.6  11.7 -1.4    -150.8   240   R  1   5600

12 45 02  SN1993J      08 29 53  49.7  11.7 -1.4    -150.9    10   1  4   5600  12 45 02
12 52 02  ---          08 36 55  50.0  10.8 -1.3    -153.1   420   R  1      0

12 52 43  0954+658     08 37 35  52.9  13.8 -1.4    -150.2    29   1  5      0  12 52 43
12 55 43  ---          08 40 36  53.1  13.4 -1.3    -151.2   180   F  1   2400

12 56 23  SN1993J      08 41 16  50.2  10.3 -1.2    -154.6    29   1  5   2400  12 56 23
13 03 23  ---          08 48 18  50.4   9.4 -1.1    -156.9   420   F  1   8000

13 03 38  M81          08 48 33  50.4   9.4 -1.1    -157.0    10   1  5   8000  13 03 38
13 08 38  ---          08 53 34  50.6   8.7 -1.0    -158.6   300   F  1  12000

13 08 53  SN1993J      08 53 49  50.6   8.7 -1.0    -158.8    10   1  5  12000  13 08 53
13 15 53  ---          09 00 50  50.8   7.7 -0.9    -161.1   420   F  1  17600

13 16 33  M81          09 01 30  50.8   7.7 -0.9    -161.3    35   1  6  17600  13 16 33
13 21 33  ---          09 06 31  50.9   7.0 -0.8    -163.0   300   R  1  13600

13 21 49  SN1993J      09 06 46  51.0   6.9 -0.8    -163.1    10   1  6  13600  13 21 49
13 28 49  ---          09 13 47  51.2   6.0 -0.7    -165.5   420   R  1   8000

13 29 46  0917+624     09 14 44  58.4   1.6 -0.1    -177.0    37   1  6   8000  13 29 46
13 32 46  ---          09 17 45  58.4   0.9 -0.1    -178.3   180   R  1   5600

13 33 42  SN1993J      09 18 41  51.3   5.3 -0.6    -167.2    36   1  6   5600  13 33 42
13 40 42  ---          09 25 43  51.4   4.3 -0.5    -169.6   420   R  1      0

13 41 22  M81          09 26 23  51.4   4.2 -0.5    -169.8    35   1  7      0  13 41 22
13 45 22  ---          09 30 23  51.4   3.7 -0.4    -171.2   240   F  1   3200

13 45 37  SN1993J      09 30 39  51.5   3.6 -0.4    -171.3    10   1  7   3200  13 45 37
13 52 37  ---          09 37 40  51.6   2.6 -0.3    -173.7   420   F  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

13 52 52  M81          09 37 55  51.5   2.6 -0.3    -173.8    10   1  7   8800  13 52 52
13 56 52  ---          09 41 56  51.5   2.0 -0.2    -175.2   240   F  1  12000

13 57 07  SN1993J      09 42 11  51.6   2.0 -0.2    -175.3    10   1  7  12000  13 57 07
14 04 07  ---          09 49 12  51.6   1.0 -0.1    -177.7   420   F  1  17600

14 04 47  0954+658     09 49 52  55.1   1.7 -0.2    -176.5    27   1  8  17600  14 04 47
14 07 47  ---          09 52 52  55.1   1.1 -0.1    -177.6   180   R  1  15200

14 08 24  SN1993J      09 53 29  51.6   0.3  0.0    -179.2    24   1  8  15200  14 08 24
14 15 24  ---          10 00 30  51.6  -0.7  0.1     178.4   420   R  1   9600

14 15 39  M81          10 00 46  51.6  -0.7  0.1     178.3    10   1  8   9600  14 15 39
14 20 39  ---          10 05 46  51.6  -1.4  0.2     176.6   300   R  1   5600

14 20 54  SN1993J      10 06 02  51.6  -1.5  0.2     176.5    10   1  8   5600  14 20 54
14 27 54  ---          10 13 03  51.6  -2.5  0.3     174.0   420   R  1      0

14 28 55  0917+624     10 14 03  57.3 -11.2  0.9     159.0    43   1  9      0  14 28 55
14 31 55  ---          10 17 04  57.2 -11.8  0.9     157.8   180   F  1   2400

14 32 55  SN1993J      10 18 04  51.5  -3.2  0.4     172.3    42   1  9   2400  14 32 55
14 39 55  ---          10 25 05  51.4  -4.2  0.5     169.9   420   F  1   8000

14 40 10  M81          10 25 20  51.4  -4.2  0.5     169.8    10   1  9   8000  14 40 10
14 45 10  ---          10 30 21  51.3  -4.9  0.6     168.1   300   F  1  12000

14 45 25  SN1993J      10 30 36  51.3  -5.0  0.6     168.0    10   1  9  12000  14 45 25
14 52 25  ---          10 37 37  51.2  -6.0  0.7     165.6   420   F  1  17600

14 53 05  M81          10 38 17  51.1  -6.0  0.7     165.4    35   1 10  17600  14 53 05
14 58 05  ---          10 43 18  51.0  -6.7  0.8     163.7   300   R  1  13600

14 58 20  SN1993J      10 43 33  51.0  -6.8  0.8     163.6    10   1 10  13600  14 58 20
15 05 20  ---          10 50 34  50.8  -7.7  0.9     161.2   420   R  1   8000

15 05 53  0954+658     10 51 08  54.2  -9.2  0.9     160.7    21   1 10   8000  15 05 53
15 08 53  ---          10 54 08  54.1  -9.7  0.9     159.6   180   R  1   5600

15 09 27  SN1993J      10 54 42  50.7  -8.3  1.0     159.8    21   1 10   5600  15 09 27
15 16 27  ---          11 01 43  50.5  -9.2  1.1     157.4   420   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

15 17 07  M81          11 02 23  50.4  -9.2  1.1     157.3    35   1 11      0  15 17 07
15 22 07  ---          11 07 24  50.2  -9.9  1.2     155.6   300   F  1   4000

15 22 22  SN1993J      11 07 39  50.3 -10.0  1.2     155.5    10   1 11   4000  15 22 22
15 29 22  ---          11 14 40  50.0 -10.8  1.3     153.1   420   F  1   9600

15 30 24  0917+624     11 15 43  53.4 -21.9  1.9     136.5    49   1 11   9600  15 30 24
15 33 24  ---          11 18 44  53.2 -22.3  1.9     135.5   180   F  1  12000

15 34 26  SN1993J      11 19 46  49.8 -11.5  1.4     151.5    49   1 11  12000  15 34 26
15 41 26  ---          11 26 47  49.5 -12.3  1.5     149.2   420   F  1  17600

15 42 06  M81          11 27 27  49.4 -12.3  1.5     149.1    35   1 12  17600  15 42 06
15 46 06  ---          11 31 27  49.2 -12.8  1.6     147.8   240   R  1  14400

15 46 21  SN1993J      11 31 43  49.2 -12.9  1.6     147.6    10   1 12  14400  15 46 21
15 53 21  ---          11 38 44  48.9 -13.7  1.7     145.4   420   R  1   8800

15 53 54  0954+658     11 39 17  51.9 -16.5  1.7     143.9    21   1 12   8800  15 53 54
15 57 54  ---          11 43 17  51.6 -17.0  1.7     142.5   240   R  1   5600

15 58 27  SN1993J      11 43 50  48.6 -14.3  1.8     143.8    21   1 12   5600  15 58 27
16 05 27  ---          11 50 51  48.3 -15.0  1.9     141.5   420   R  1      0

16 06 07  M81          11 51 31  48.2 -15.0  1.9     141.4    35   1 13      0  16 06 07
16 10 07  ---          11 55 32  48.0 -15.4  2.0     140.2   240   F  1   3200

16 10 22  SN1993J      11 55 47  48.0 -15.5  2.0     140.0    10   1 13   3200  16 10 22
16 17 22  ---          12 02 48  47.6 -16.2  2.1     137.9   420   F  1   8800

16 17 37  M81          12 03 04  47.5 -16.2  2.1     137.9    10   1 13   8800  16 17 37
16 21 37  ---          12 07 04  47.3 -16.6  2.2     136.6   240   F  1  12000

16 21 52  SN1993J      12 07 19  47.3 -16.7  2.2     136.5    10   1 13  12000  16 21 52
16 28 52  ---          12 14 21  46.8 -17.3  2.3     134.4   420   F  1  17600

16 29 32  M81          12 15 01  46.8 -17.3  2.3     134.2    35   1 14  17600  16 29 32
16 33 32  ---          12 19 01  46.5 -17.7  2.4     133.0   240   R  1  14400

16 33 48  SN1993J      12 19 17  46.5 -17.8  2.4     132.9    10   1 14  14400  16 33 48
16 38 48  ---          12 24 17  46.2 -18.2  2.5     131.4   300   R  1  10400
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

16 39 51  0917+624     12 25 21  46.9 -29.3  3.1     115.4    50   1 14  10400  16 39 51
16 42 51  ---          12 28 21  46.6 -29.5  3.1     114.6   180   R  1   8000

16 50 31  3C286        12 36 03  78.1  87.2 -0.9     -85.8   377   1 14   8000  16 50 31
17 00 31  ---          12 46 04  80.3  88.0 -0.8     -86.2   600   R  1      0

-----------  Tape Change ------------

17 15 31  0954+658     13 01 07  45.5 -24.9  3.0     118.8   819   2  1      0  17 15 31
17 18 31  ---          13 04 07  45.3 -25.1  3.1     118.0   180   F  1   2400

17 19 07  SN1993J      13 04 43  43.2 -21.2  3.1     119.9    26   2  1   2400  17 19 07
17 26 07  ---          13 11 44  42.7 -21.6  3.3     117.9   420   F  1   8000

17 26 47  M81          13 12 24  42.6 -21.6  3.3     117.8    35   2  1   8000  17 26 47
17 31 47  ---          13 17 25  42.2 -21.8  3.4     116.5   300   F  1  12000

17 32 02  SN1993J      13 17 40  42.2 -21.9  3.4     116.3    10   2  1  12000  17 32 02
17 39 02  ---          13 24 42  41.7 -22.3  3.5     114.5   420   F  1  17600

17 40 04  0917+624     13 25 44  40.2 -32.2  4.1     100.0    49   2  2  17600  17 40 04
17 44 04  ---          13 29 44  39.7 -32.3  4.1      99.0   240   R  1  14400

17 45 05  SN1993J      13 30 46  41.2 -22.6  3.6     112.9    49   2  2  14400  17 45 05
17 52 05  ---          13 37 47  40.6 -22.9  3.7     111.0   420   R  1   8800

17 52 20  M81          13 38 02  40.5 -22.8  3.7     111.0    10   2  2   8800  17 52 20
17 56 20  ---          13 42 03  40.2 -23.0  3.8     110.0   240   R  1   5600

17 56 35  SN1993J      13 42 18  40.2 -23.1  3.8     109.8    11   2  2   5600  17 56 35
18 03 35  ---          13 49 19  39.6 -23.3  3.9     108.0   420   R  1      0

18 04 15  M81          13 49 59  39.5 -23.3  3.9     107.9    35   2  3      0  18 04 15
18 07 15  ---          13 53 00  39.3 -23.4  4.0     107.2   180   F  1   2400

18 07 30  SN1993J      13 53 15  39.3 -23.5  4.0     107.0    11   2  3   2400  18 07 30
18 14 30  ---          14 00 16  38.7 -23.7  4.1     105.2   420   F  1   8000

18 14 45  M81          14 00 31  38.6 -23.6  4.1     105.3    10   2  3   8000  18 14 45
18 19 45  ---          14 05 32  38.2 -23.8  4.2     104.0   300   F  1  12000

18 20 01  SN1993J      14 05 47  38.2 -23.9  4.2     103.9    10   2  3  12000  18 20 01
18 27 01  ---          14 12 48  37.6 -24.0  4.3     102.1   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

18 27 41  M81          14 13 28  37.5 -24.0  4.3     102.0    35   2  4  17600  18 27 41
18 32 41  ---          14 18 29  37.1 -24.1  4.4     100.8   300   R  1  13600

18 32 56  SN1993J      14 18 44  37.0 -24.2  4.4     100.6    10   2  4  13600  18 32 56
18 39 56  ---          14 25 45  36.4 -24.3  4.5      98.9   420   R  1   8000

18 40 33  0954+658     14 26 23  37.2 -28.5  4.5      97.0    29   2  4   8000  18 40 33
18 43 33  ---          14 29 24  36.9 -28.6  4.5      96.3   180   R  1   5600

18 44 11  SN1993J      14 30 01  36.0 -24.4  4.6      97.9    29   2  4   5600  18 44 11
18 51 11  ---          14 37 02  35.4 -24.5  4.7      96.2   420   R  1      0

18 51 51  M81          14 37 42  35.4 -24.4  4.7      96.1    35   2  5      0  18 51 51
18 55 51  ---          14 41 43  35.0 -24.5  4.8      95.1   240   F  1   3200

18 56 06  SN1993J      14 41 58  35.0 -24.5  4.8      95.0    10   2  5   3200  18 56 06
19 04 06  ---          14 50 00  34.3 -24.6  4.9      93.1   480   F  1   9600

19 05 04  0917+624     14 50 58  30.3 -32.3  5.5      81.0    44   2  5   9600  19 05 04
19 08 04  ---          14 53 58  30.0 -32.3  5.5      80.4   180   F  1  12000

19 09 01  SN1993J      14 54 56  33.8 -24.6  5.0      91.9    44   2  5  12000  19 09 01
19 16 01  ---          15 01 57  33.2 -24.6  5.1      90.3   420   F  1  17600

19 16 41  M81          15 02 37  33.1 -24.6  5.1      90.2    35   2  6  17600  19 16 41
19 20 41  ---          15 06 38  32.8 -24.6  5.2      89.3   240   R  1  14400

19 20 56  SN1993J      15 06 53  32.8 -24.6  5.2      89.1    10   2  6  14400  19 20 56
19 27 56  ---          15 13 54  32.1 -24.6  5.3      87.5   420   R  1   8800

19 28 11  M81          15 14 09  32.1 -24.5  5.3      87.5    11   2  6   8800  19 28 11
19 32 11  ---          15 18 10  31.8 -24.5  5.4      86.6   240   R  1   5600

19 32 27  SN1993J      15 18 25  31.7 -24.6  5.4      86.5    10   2  6   5600  19 32 27
19 39 27  ---          15 25 26  31.1 -24.5  5.5      84.9   420   R  1      0

19 40 07  0954+658     15 26 06  31.0 -28.6  5.4      83.4    31   2  7      0  19 40 07
19 43 07  ---          15 29 07  30.7 -28.5  5.5      82.7   180   F  1   2400

19 43 45  SN1993J      15 29 45  30.7 -24.5  5.6      83.9    29   2  7   2400  19 43 45
19 50 45  ---          15 36 46  30.1 -24.4  5.7      82.3   420   F  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

19 51 00  M81          15 37 01  30.1 -24.3  5.7      82.3    11   2  7   8000  19 51 00
19 55 00  ---          15 41 02  29.7 -24.3  5.8      81.4   240   F  1  11200

19 55 15  SN1993J      15 41 17  29.7 -24.3  5.8      81.3    10   2  7  11200  19 55 15
20 03 15  ---          15 49 18  29.0 -24.2  5.9      79.5   480   F  1  17600

20 04 08  0917+624     15 50 12  23.7 -30.3  6.5      68.8    37   2  8  17600  20 04 08
20 07 08  ---          15 53 12  23.4 -30.2  6.5      68.2   180   R  1  15200

20 08 02  SN1993J      15 54 06  28.6 -24.1  6.0      78.4    37   2  8  15200  20 08 02
20 15 02  ---          16 01 07  27.9 -23.9  6.1      76.8   420   R  1   9600

20 15 17  M81          16 01 22  27.9 -23.9  6.1      76.8    11   2  8   9600  20 15 17
20 19 17  ---          16 05 23  27.6 -23.8  6.2      75.9   240   R  1   6400

20 19 32  SN1993J      16 05 38  27.5 -23.8  6.2      75.8    10   2  8   6400  20 19 32
20 27 32  ---          16 13 39  26.9 -23.6  6.3      74.0   480   R  1      0

20 28 12  M81          16 14 19  26.8 -23.5  6.3      74.0    35   2  9      0  20 28 12
20 33 12  ---          16 19 20  26.4 -23.4  6.4      72.8   300   F  1   4000

20 33 27  SN1993J      16 19 35  26.3 -23.4  6.4      72.7    10   2  9   4000  20 33 27
20 40 27  ---          16 26 37  25.7 -23.2  6.5      71.2   420   F  1   9600

20 41 05  0954+658     16 27 14  24.9 -26.9  6.5      70.2    29   2  9   9600  20 41 05
20 44 05  ---          16 30 15  24.6 -26.8  6.5      69.6   180   F  1  12000

20 44 43  SN1993J      16 30 53  25.4 -23.1  6.6      70.3    29   2  9  12000  20 44 43
20 51 43  ---          16 37 54  24.8 -22.8  6.7      68.7   420   F  1  17600

20 52 23  M81          16 38 34  24.8 -22.8  6.7      68.6    35   2 10  17600  20 52 23
20 56 23  ---          16 42 35  24.4 -22.6  6.8      67.8   240   R  1  14400

20 56 38  SN1993J      16 42 50  24.4 -22.7  6.8      67.6    10   2 10  14400  20 56 38
21 03 38  ---          16 49 51  23.8 -22.4  6.9      66.1   420   R  1   8800

21 03 53  M81          16 50 06  23.8 -22.3  6.9      66.1    11   2 10   8800  21 03 53
21 07 53  ---          16 54 07  23.5 -22.2  7.0      65.2   240   R  1   5600

21 08 08  SN1993J      16 54 22  23.4 -22.2  7.0      65.1    10   2 10   5600  21 08 08
21 15 08  ---          17 01 23  22.9 -21.9  7.1      63.6   420   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  31 Oct 2004   Day 305 ---

21 15 56  0917+624     17 02 11  16.3 -26.1  7.7      54.3    29   2 11      0  21 15 56
21 18 56  ---          17 05 12  16.0 -25.9  7.7      53.7   180   F  1   2400

21 19 44  SN1993J      17 06 00  22.5 -21.7  7.2      62.6    29   2 11   2400  21 19 44
21 26 44  ---          17 13 01  21.9 -21.4  7.3      61.1   420   F  1   8000

21 27 24  M81          17 13 41  21.9 -21.3  7.3      61.0    35   2 11   8000  21 27 24
21 31 24  ---          17 17 42  21.6 -21.1  7.4      60.1   240   F  1  11200

21 34 40  3C286        17 20 58  41.1 -74.6  3.8      74.3   151   2 11  11200  21 34 40
21 42 40  ---          17 29 00  39.5 -74.0  4.0      73.7   480   F  1  17600


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: GM055A.6cm
   Matches group v6cm_2 in /sched-2003/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         U         L         U         L         U         L         U
   Pol.  =      LCP       LCP       LCP       LCP       LCP       LCP       LCP       LCP 
   BBC   =         1         1         2         2         3         3         4         4
   BBC SB=         L         U         L         U         L         U         L         U
   IF    =        C         C         C         C         C         C         C         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4966.49   4966.49   4982.49   4982.49   4998.49   4998.49   5014.49   5014.49
   BBC fr=     866.49    866.49    882.49    882.49    898.49    898.49    914.49    914.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   490   490   490  6490  6490  6490  6490
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- SN1993J @ 6cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * 0917+624          09 17 40.306287   * 09 21 36.230500     09 21 58.272561 
                     62 28 38.63575    * 62 15 52.17600      62 14 31.45650 
                     From catalog imbedded in main SCHED input file.

 * 0954+658          09 54 57.847920   * 09 58 47.245100     09 59 08.330479 
                     65 48 15.53881    * 65 33 54.81800      65 32 24.31434 
                     From catalog imbedded in main SCHED input file.

 * SN1993J           09 51 19.039486   * 09 55 24.775500     09 55 47.401922 
                     69 15 26.47487    * 69 01 13.71000      68 59 43.12863 
                     From catalog imbedded in main SCHED input file.

 * M81               09 51 27.310854   * 09 55 33.173100     09 55 55.809379 
                     69 18 08.14534    * 69 03 55.06200      69 02 24.44071 
                     From catalog imbedded in main SCHED input file.

 * 1803+784          18 03 39.193244   * 18 00 45.683600     18 00 25.264404 
                     78 27 54.30008    * 78 28 04.02100      78 28 12.11852 
                     From catalog imbedded in main SCHED input file.

 * 2007+777          20 07 20.430477   * 20 05 30.998800     20 05 18.247564 
                     77 43 58.12445    * 77 52 43.24900      77 53 45.03684 
                     From catalog imbedded in main SCHED input file.

 * 3C286             13 28 49.657781   * 13 31 08.288074     13 31 19.946818 
                     30 45 58.64118    * 30 30 32.95982      30 29 06.72166 
                     From catalog imbedded in main SCHED input file.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0917+624            96.2
   0954+658            93.8
   SN1993J             95.6
   M81                 95.6
   1803+784            97.4
   2007+777           103.0
   3C286               46.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

