  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
 Exp. Code:  GB052   


Schedule Version:       1.00                                              
Processed by SCHED version: NRAO internal release of 4 October 2004       

PI:       N. Bartel                                                       

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@yorku.ca                                                 
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 256-8-2-ul 6cm                                       

Notes:    Fringe finder  : 3C84                                           
          Pol. Calibrator: 3C84                                           
          Amplitude check: 3C66A                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon  24 Oct 2005   Day 297 ---

 Next scan frequencies:  4979.49  4979.49  4979.49  4979.49  4995.49  4995.49
                         4995.49  4995.49
 Next BBC frequencies:    879.49   879.49   879.49   879.49   895.49   895.49
                          895.49   895.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

23 07 20  3C66A        18 25 20   2.2  39.6 -8.0  D  -48.6     0   1  1      0  23 07 20
23 08 30  ---          18 26 31   2.4  39.7 -7.9  H  -48.8     0   F  1    933

23 10 30  3C66A        18 28 31   2.7  39.9 -7.9  H  -49.1   114   1  1    933  23 10 30
23 11 40  ---          18 29 41   2.8  40.1 -7.9  H  -49.3     0   F  1   1867

23 11 40  SN1986J      18 29 41   2.4  40.6 -7.9  H  -49.3    -7   1  1   1867  23 11 40
23 13 40  ---          18 31 42   2.7  40.9 -7.9  H  -49.6     0   F  1   3467

23 13 40  3C66A        18 31 42   3.1  40.3 -7.9     -49.6    -7   1  1   3467  23 13 40
23 14 50  ---          18 32 52   3.3  40.5 -7.8     -49.8    63   F  1   4400

23 14 50  SN1986J      18 32 52   2.8  41.0 -7.8     -49.8    -7   1  1   4400  23 14 50
23 16 50  ---          18 34 52   3.1  41.2 -7.8     -50.2   113   F  1   6000

23 16 50  3C66A        18 34 52   3.6  40.7 -7.8     -50.2    -7   1  1   6000  23 16 50
23 18 00  ---          18 36 02   3.7  40.8 -7.8     -50.4    63   F  1   6933

23 18 00  SN1986J      18 36 02   3.3  41.4 -7.8     -50.3    -7   1  1   6933  23 18 00
23 20 00  ---          18 38 03   3.6  41.6 -7.7     -50.7   113   F  1   8533

23 20 00  3C66A        18 38 03   4.0  41.1 -7.8     -50.7    -7   1  1   8533  23 20 00
23 22 00  ---          18 40 03   4.3  41.3 -7.7     -51.0   113   F  1  10133

23 25 00  3C66A        18 43 03   4.7  41.6 -7.7     -51.5   173   1  1  10133  23 25 00
23 27 10  ---          18 45 14   5.0  41.9 -7.6     -51.8   130   F  1  11867

23 27 10  SN1986J      18 45 14   4.6  42.5 -7.6     -51.8    -7   1  1  11867  23 27 10
23 29 10  ---          18 47 14   4.9  42.7 -7.6     -52.1   113   F  1  13467

23 29 10  3C66A        18 47 14   5.3  42.1 -7.6     -52.2    -7   1  1  13467  23 29 10
23 30 20  ---          18 48 24   5.5  42.2 -7.6     -52.3    63   F  1  14400

23 30 20  SN1986J      18 48 24   5.1  42.8 -7.6     -52.3    -7   1  1  14400  23 30 20
23 32 20  ---          18 50 25   5.4  43.0 -7.5     -52.6   113   F  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon  24 Oct 2005   Day 297 ---

23 32 20  3C66A        18 50 25   5.8  42.5 -7.5     -52.7    -7   1  1  16000  23 32 20
23 33 30  ---          18 51 35   6.0  42.6 -7.5     -52.9    63   F  1  16933

23 33 30  SN1986J      18 51 35   5.5  43.2 -7.5     -52.8    -7   1  2  16933  23 33 30
23 35 30  ---          18 53 35   5.8  43.4 -7.5     -53.1   113   R  1  16667

23 35 30  3C66A        18 53 35   6.2  42.8 -7.5     -53.2    -7   1  2  16667  23 35 30
23 36 40  ---          18 54 45   6.4  42.9 -7.5     -53.4    63   R  1  15733

23 36 40  SN1986J      18 54 45   6.0  43.5 -7.5     -53.3    -7   1  2  15733  23 36 40
23 38 40  ---          18 56 46   6.3  43.8 -7.4     -53.6   113   R  1  14133

23 38 40  3C66A        18 56 46   6.7  43.2 -7.4     -53.7    -7   1  2  14133  23 38 40
23 39 50  ---          18 57 56   6.9  43.3 -7.4     -53.9    63   R  1  13200

23 39 50  SN1986J      18 57 56   6.5  43.9 -7.4     -53.8    -7   1  2  13200  23 39 50
23 41 50  ---          18 59 56   6.8  44.1 -7.4     -54.1   113   R  1  11600

23 41 50  3C66A        18 59 56   7.2  43.5 -7.4     -54.2    -7   1  2  11600  23 41 50
23 43 00  ---          19 01 06   7.4  43.6 -7.4     -54.4    63   R  1  10667

23 43 00  SN1986J      19 01 06   7.0  44.2 -7.4     -54.3    -6   1  2  10667  23 43 00
23 45 00  ---          19 03 07   7.3  44.4 -7.3     -54.6   114   R  1   9067

23 45 00  3C66A        19 03 07   7.6  43.8 -7.3     -54.7    -6   1  2   9067  23 45 00
23 47 00  ---          19 05 07   7.9  44.1 -7.3     -55.0   114   R  1   7467

23 50 00  3C66A        19 08 07   8.4  44.4 -7.2     -55.5   173   1  2   7467  23 50 00
23 52 10  ---          19 10 18   8.7  44.6 -7.2     -55.8   130   R  1   5733

23 52 10  SN1986J      19 10 18   8.4  45.2 -7.2     -55.7    -6   1  2   5733  23 52 10
23 54 10  ---          19 12 18   8.7  45.4 -7.2     -56.0   114   R  1   4133

23 54 10  3C66A        19 12 18   9.0  44.8 -7.2     -56.1    -6   1  2   4133  23 54 10
23 55 20  ---          19 13 28   9.2  44.9 -7.2     -56.3    64   R  1   3200

23 55 20  SN1986J      19 13 28   8.8  45.5 -7.2     -56.2    -6   1  2   3200  23 55 20
23 57 20  ---          19 15 29   9.1  45.7 -7.1     -56.5   114   R  1   1600

23 57 20  3C66A        19 15 29   9.5  45.1 -7.1     -56.6    -6   1  2   1600  23 57 20
23 58 30  ---          19 16 39   9.7  45.3 -7.1     -56.8    64   R  1    667
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Start: Mon  24 Oct 2005   Day 297 -- Stop: Tue  25 Oct 2005   Day 298 ---

23 58 30  SN1986J      19 16 39   9.3  45.9 -7.1     -56.7    -6   1  3    667  23 58 30
00 00 30  ---          19 18 39   9.6  46.1 -7.1     -57.0   114   F  1    933

00 00 30  3C66A        19 18 39  10.0  45.5 -7.1     -57.1    -6   1  3    933  00 00 30
00 01 40  ---          19 19 49  10.2  45.6 -7.1     -57.3    64   F  1   1867

00 01 40  SN1986J      19 19 49   9.8  46.2 -7.1     -57.2    -6   1  3   1867  00 01 40
00 03 40  ---          19 21 50  10.1  46.4 -7.0     -57.5   114   F  1   3467

00 03 40  3C66A        19 21 50  10.5  45.8 -7.0     -57.6    -6   1  3   3467  00 03 40
00 04 50  ---          19 23 00  10.7  45.9 -7.0     -57.7    64   F  1   4400

00 04 50  SN1986J      19 23 00  10.3  46.5 -7.0     -57.7    -6   1  3   4400  00 04 50
00 06 50  ---          19 25 00  10.6  46.7 -7.0     -58.0   114   F  1   6000

00 06 50  3C66A        19 25 00  11.0  46.1 -7.0     -58.1    -6   1  3   6000  00 06 50
00 08 00  ---          19 26 10  11.2  46.2 -6.9     -58.2    64   F  1   6933

00 08 00  SN1986J      19 26 10  10.8  46.8 -6.9     -58.1    -6   1  3   6933  00 08 00
00 10 00  ---          19 28 11  11.1  47.0 -6.9     -58.4   114   F  1   8533

00 10 00  3C66A        19 28 11  11.5  46.4 -6.9     -58.5    -6   1  3   8533  00 10 00
00 12 00  ---          19 30 11  11.8  46.6 -6.9     -58.8   114   F  1  10133

00 15 00  3C66A        19 33 12  12.3  46.9 -6.8     -59.3   173   1  3  10133  00 15 00
00 17 10  ---          19 35 22  12.6  47.1 -6.8     -59.6   130   F  1  11867

00 17 10  SN1986J      19 35 22  12.3  47.7 -6.8     -59.5    -6   1  3  11867  00 17 10
00 19 10  ---          19 37 22  12.6  47.9 -6.8     -59.8   114   F  1  13467

00 19 10  3C66A        19 37 22  12.9  47.3 -6.8     -59.9    -6   1  3  13467  00 19 10
00 20 20  ---          19 38 32  13.1  47.4 -6.7     -60.1    64   F  1  14400

00 20 20  SN1986J      19 38 32  12.8  48.0 -6.7     -60.0    -6   1  3  14400  00 20 20
00 22 20  ---          19 40 33  13.1  48.2 -6.7     -60.3   114   F  1  16000

00 22 20  3C66A        19 40 33  13.4  47.6 -6.7     -60.4    -6   1  3  16000  00 22 20
00 23 30  ---          19 41 43  13.6  47.7 -6.7     -60.6    64   F  1  16933

00 23 30  SN1986J      19 41 43  13.3  48.3 -6.7     -60.4    -6   1  4  16933  00 23 30
00 25 30  ---          19 43 43  13.6  48.5 -6.7     -60.7   114   R  1  16667
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

00 25 30  3C66A        19 43 43  13.9  47.9 -6.7     -60.9    -6   1  4  16667  00 25 30
00 26 40  ---          19 44 53  14.1  48.0 -6.6     -61.0    64   R  1  15733

00 26 40  SN1986J      19 44 53  13.8  48.6 -6.6     -60.9    -6   1  4  15733  00 26 40
00 28 40  ---          19 46 54  14.1  48.8 -6.6     -61.2   114   R  1  14133

00 28 40  3C66A        19 46 54  14.4  48.2 -6.6     -61.3    -6   1  4  14133  00 28 40
00 29 50  ---          19 48 04  14.6  48.3 -6.6     -61.5    64   R  1  13200

00 29 50  SN1986J      19 48 04  14.3  48.9 -6.6     -61.4    -6   1  4  13200  00 29 50
00 31 50  ---          19 50 04  14.6  49.1 -6.5     -61.7   114   R  1  11600

00 31 50  3C66A        19 50 04  14.9  48.4 -6.5     -61.8    -6   1  4  11600  00 31 50
00 33 00  ---          19 51 15  15.1  48.6 -6.5     -62.0    64   R  1  10667

00 33 00  SN1986J      19 51 15  14.8  49.2 -6.5     -61.8    -6   1  4  10667  00 33 00
00 35 00  ---          19 53 15  15.1  49.4 -6.5     -62.1   114   R  1   9067

00 35 00  3C66A        19 53 15  15.5  48.7 -6.5     -62.3    -6   1  4   9067  00 35 00
00 37 00  ---          19 55 15  15.8  48.9 -6.5     -62.6   114   R  1   7467

00 40 00  3C84         19 58 16   6.5  44.9 -7.4     -54.2   155   1  4   7467  00 40 00
00 42 00  ---          20 00 16   6.8  45.1 -7.3     -54.5   120   R  1   5867

00 42 00  3C66A        20 00 16  16.6  49.3 -6.4     -63.3   -26   1  4   5867  00 42 00
00 45 20  ---          20 03 37  17.1  49.6 -6.3     -63.8   174   R  1   3200

00 45 20  SN1986J      20 03 37  16.9  50.3 -6.3     -63.6    -6   1  4   3200  00 45 20
00 47 20  ---          20 05 37  17.2  50.5 -6.3     -63.9   114   R  1   1600

00 47 20  3C66A        20 05 37  17.5  49.8 -6.3     -64.1    -6   1  4   1600  00 47 20
00 48 30  ---          20 06 47  17.7  49.9 -6.3     -64.3    64   R  1    667

00 48 30  SN1986J      20 06 47  17.4  50.6 -6.3     -64.1    -6   1  5    667  00 48 30
00 50 30  ---          20 08 47  17.7  50.7 -6.2     -64.4   114   F  1    933

00 50 30  3C66A        20 08 47  18.0  50.1 -6.2     -64.5    -6   1  5    933  00 50 30
00 51 40  ---          20 09 58  18.2  50.2 -6.2     -64.7    64   F  1   1867

00 51 40  SN1986J      20 09 58  17.9  50.8 -6.2     -64.5    -6   1  5   1867  00 51 40
00 53 40  ---          20 11 58  18.2  51.0 -6.2     -64.8   114   F  1   3467
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

00 53 40  3C66A        20 11 58  18.5  50.3 -6.2     -65.0    -6   1  5   3467  00 53 40
00 54 50  ---          20 13 08  18.7  50.4 -6.2     -65.2    64   F  1   4400

00 54 50  SN1986J      20 13 08  18.4  51.1 -6.2     -65.0    -6   1  5   4400  00 54 50
00 56 50  ---          20 15 08  18.8  51.3 -6.1     -65.3   114   F  1   6000

00 56 50  3C66A        20 15 08  19.0  50.6 -6.1     -65.5    -6   1  5   6000  00 56 50
00 58 00  ---          20 16 19  19.2  50.7 -6.1     -65.6    64   F  1   6933

00 58 00  SN1986J      20 16 19  19.0  51.4 -6.1     -65.4    -6   1  5   6933  00 58 00
01 00 00  ---          20 18 19  19.3  51.5 -6.1     -65.7   114   F  1   8533

01 00 00  3C66A        20 18 19  19.6  50.8 -6.1     -65.9    -6   1  5   8533  01 00 00
01 02 00  ---          20 20 19  19.9  51.0 -6.0     -66.2   114   F  1  10133

01 05 00  3C66A        20 23 20  20.4  51.2 -6.0     -66.6   173   1  5  10133  01 05 00
01 07 10  ---          20 25 30  20.8  51.4 -6.0     -67.0   130   F  1  11867

01 07 10  SN1986J      20 25 30  20.5  52.1 -6.0     -66.7    -6   1  5  11867  01 07 10
01 09 10  ---          20 27 30  20.9  52.2 -5.9     -67.0   114   F  1  13467

01 09 10  3C66A        20 27 30  21.1  51.5 -5.9     -67.2    -6   1  5  13467  01 09 10
01 10 20  ---          20 28 41  21.3  51.6 -5.9     -67.4    64   F  1  14400

01 10 20  SN1986J      20 28 41  21.1  52.3 -5.9     -67.2    -6   1  5  14400  01 10 20
01 12 20  ---          20 30 41  21.4  52.5 -5.9     -67.5   114   F  1  16000

01 12 20  3C66A        20 30 41  21.6  51.8 -5.9     -67.7    -6   1  5  16000  01 12 20
01 13 30  ---          20 31 51  21.8  51.9 -5.9     -67.9    64   F  1  16933

01 13 30  SN1986J      20 31 51  21.6  52.6 -5.9     -67.6    -6   1  6  16933  01 13 30
01 15 30  ---          20 33 52  21.9  52.7 -5.8     -67.9   114   R  1  16667

01 15 30  3C66A        20 33 52  22.2  52.0 -5.8     -68.2    -6   1  6  16667  01 15 30
01 16 40  ---          20 35 02  22.4  52.1 -5.8     -68.3    64   R  1  15733

01 16 40  SN1986J      20 35 02  22.1  52.8 -5.8     -68.1    -6   1  6  15733  01 16 40
01 18 40  ---          20 37 02  22.5  53.0 -5.8     -68.4   114   R  1  14133

01 18 40  3C66A        20 37 02  22.7  52.2 -5.8     -68.6    -6   1  6  14133  01 18 40
01 19 50  ---          20 38 12  22.9  52.3 -5.7     -68.8    64   R  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

01 19 50  SN1986J      20 38 12  22.7  53.0 -5.7     -68.5    -6   1  6  13200  01 19 50
01 21 50  ---          20 40 13  23.0  53.2 -5.7     -68.8   114   R  1  11600

01 21 50  3C66A        20 40 13  23.3  52.5 -5.7     -69.1    -6   1  6  11600  01 21 50
01 23 00  ---          20 41 23  23.5  52.6 -5.7     -69.2    64   R  1  10667

01 23 00  SN1986J      20 41 23  23.2  53.3 -5.7     -69.0    -6   1  6  10667  01 23 00
01 25 00  ---          20 43 23  23.6  53.4 -5.7     -69.2   114   R  1   9067

01 25 00  3C66A        20 43 23  23.8  52.7 -5.7     -69.5    -6   1  6   9067  01 25 00
01 27 00  ---          20 45 23  24.2  52.8 -5.6     -69.8   114   R  1   7467

01 30 00  3C66A        20 48 24  24.7  53.0 -5.6     -70.2   173   1  6   7467  01 30 00
01 32 10  ---          20 50 34  25.0  53.2 -5.5     -70.5   130   R  1   5733

01 32 10  SN1986J      20 50 34  24.8  53.9 -5.5     -70.2    -6   1  6   5733  01 32 10
01 34 10  ---          20 52 35  25.2  54.1 -5.5     -70.5   114   R  1   4133

01 34 10  3C66A        20 52 35  25.4  53.3 -5.5     -70.8    -6   1  6   4133  01 34 10
01 35 20  ---          20 53 45  25.6  53.4 -5.5     -71.0    64   R  1   3200

01 35 20  SN1986J      20 53 45  25.4  54.1 -5.5     -70.7    -6   1  6   3200  01 35 20
01 37 20  ---          20 55 45  25.7  54.3 -5.5     -71.0   114   R  1   1600

01 37 20  3C66A        20 55 45  25.9  53.5 -5.5     -71.3    -6   1  6   1600  01 37 20
01 38 30  ---          20 56 55  26.1  53.6 -5.4     -71.4    64   R  1    667

01 38 30  SN1986J      20 56 55  25.9  54.4 -5.4     -71.1    -6   1  7    667  01 38 30
01 40 30  ---          20 58 56  26.3  54.5 -5.4     -71.4   114   F  1    933

01 40 30  3C66A        20 58 56  26.5  53.7 -5.4     -71.7    -6   1  7    933  01 40 30
01 41 40  ---          21 00 06  26.7  53.8 -5.4     -71.9    64   F  1   1867

01 41 40  SN1986J      21 00 06  26.5  54.6 -5.4     -71.6    -6   1  7   1867  01 41 40
01 43 40  ---          21 02 06  26.8  54.7 -5.3     -71.9   114   F  1   3467

01 43 40  3C66A        21 02 06  27.0  53.9 -5.3     -72.2    -6   1  7   3467  01 43 40
01 44 50  ---          21 03 16  27.2  54.0 -5.3     -72.3    64   F  1   4400

01 44 50  SN1986J      21 03 16  27.0  54.8 -5.3     -72.0    -6   1  7   4400  01 44 50
01 46 50  ---          21 05 17  27.4  54.9 -5.3     -72.3   114   F  1   6000
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

01 46 50  3C66A        21 05 17  27.6  54.1 -5.3     -72.6    -6   1  7   6000  01 46 50
01 48 00  ---          21 06 27  27.8  54.2 -5.3     -72.8    64   F  1   6933

01 48 00  SN1986J      21 06 27  27.6  55.0 -5.3     -72.5    -6   1  7   6933  01 48 00
01 50 00  ---          21 08 27  28.0  55.1 -5.2     -72.7   114   F  1   8533

01 50 00  3C66A        21 08 27  28.1  54.3 -5.2     -73.1    -6   1  7   8533  01 50 00
01 52 00  ---          21 10 28  28.5  54.4 -5.2     -73.4   114   F  1  10133

01 55 00  3C66A        21 13 28  29.0  54.6 -5.2     -73.8   173   1  7  10133  01 55 00
01 57 10  ---          21 15 38  29.4  54.7 -5.1     -74.1   130   F  1  11867

01 57 10  SN1986J      21 15 38  29.2  55.5 -5.1     -73.7    -6   1  7  11867  01 57 10
01 59 10  ---          21 17 39  29.6  55.6 -5.1     -74.0   114   F  1  13467

01 59 10  3C66A        21 17 39  29.8  54.9 -5.1     -74.4    -6   1  7  13467  01 59 10
02 00 20  ---          21 18 49  30.0  54.9 -5.1     -74.6    64   F  1  14400

02 00 20  SN1986J      21 18 49  29.8  55.7 -5.1     -74.2    -6   1  7  14400  02 00 20
02 02 20  ---          21 20 49  30.2  55.8 -5.0     -74.5   114   F  1  16000

02 02 20  3C66A        21 20 49  30.3  55.0 -5.0     -74.8    -6   1  7  16000  02 02 20
02 03 30  ---          21 21 59  30.5  55.1 -5.0     -75.0    64   F  1  16933

02 03 30  SN1986J      21 21 59  30.4  55.9 -5.0     -74.6    -6   1  8  16933  02 03 30
02 05 30  ---          21 24 00  30.7  56.0 -5.0     -74.9   114   R  1  16667

02 05 30  3C66A        21 24 00  30.9  55.2 -5.0     -75.3    -6   1  8  16667  02 05 30
02 06 40  ---          21 25 10  31.1  55.3 -5.0     -75.5    64   R  1  15733

02 06 40  SN1986J      21 25 10  30.9  56.1 -5.0     -75.1    -6   1  8  15733  02 06 40
02 08 40  ---          21 27 10  31.3  56.2 -4.9     -75.4   114   R  1  14133

02 08 40  3C66A        21 27 10  31.4  55.4 -4.9     -75.7    -6   1  8  14133  02 08 40
02 09 50  ---          21 28 20  31.6  55.4 -4.9     -75.9    64   R  1  13200

02 09 50  SN1986J      21 28 20  31.5  56.3 -4.9     -75.5    -6   1  8  13200  02 09 50
02 11 50  ---          21 30 21  31.9  56.4 -4.9     -75.8   114   R  1  11600

02 11 50  3C66A        21 30 21  32.0  55.5 -4.9     -76.2    -6   1  8  11600  02 11 50
02 13 00  ---          21 31 31  32.2  55.6 -4.9     -76.4    64   R  1  10667
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

02 13 00  SN1986J      21 31 31  32.1  56.4 -4.9     -76.0    -6   1  8  10667  02 13 00
02 15 00  ---          21 33 31  32.4  56.5 -4.8     -76.2   114   R  1   9067

02 15 00  3C66A        21 33 31  32.6  55.7 -4.8     -76.7    -6   1  8   9067  02 15 00
02 17 00  ---          21 35 32  32.9  55.8 -4.8     -76.9   114   R  1   7467

02 20 00  3C66A        21 38 32  33.5  56.0 -4.7     -77.4   173   1  8   7467  02 20 00
02 22 10  ---          21 40 42  33.8  56.1 -4.7     -77.7   130   R  1   5733

02 22 10  SN1986J      21 40 42  33.7  56.9 -4.7     -77.3    -6   1  8   5733  02 22 10
02 24 10  ---          21 42 43  34.1  57.0 -4.7     -77.5   114   R  1   4133

02 24 10  3C66A        21 42 43  34.2  56.2 -4.7     -78.0    -6   1  8   4133  02 24 10
02 25 20  ---          21 43 53  34.4  56.2 -4.7     -78.2    64   R  1   3200

02 25 20  SN1986J      21 43 53  34.3  57.0 -4.7     -77.7    -6   1  8   3200  02 25 20
02 27 20  ---          21 45 53  34.6  57.1 -4.6     -78.0   114   R  1   1600

02 27 20  3C66A        21 45 53  34.8  56.3 -4.6     -78.4    -6   1  8   1600  02 27 20
02 28 30  ---          21 47 04  35.0  56.3 -4.6     -78.6    64   R  1    667

02 28 30  SN1986J      21 47 04  34.9  57.2 -4.6     -78.2    -6   1  9    667  02 28 30
02 30 30  ---          21 49 04  35.2  57.3 -4.6     -78.4   114   F  1    933

02 30 30  3C66A        21 49 04  35.3  56.4 -4.6     -78.9    -6   1  9    933  02 30 30
02 31 40  ---          21 50 14  35.5  56.5 -4.5     -79.1    64   F  1   1867

02 31 40  SN1986J      21 50 14  35.4  57.3 -4.5     -78.6    -6   1  9   1867  02 31 40
02 33 40  ---          21 52 14  35.8  57.4 -4.5     -78.9   114   F  1   3467

02 33 40  3C66A        21 52 14  35.9  56.6 -4.5     -79.4    -6   1  9   3467  02 33 40
02 34 50  ---          21 53 25  36.1  56.6 -4.5     -79.5    64   F  1   4400

02 34 50  SN1986J      21 53 25  36.0  57.5 -4.5     -79.1    -6   1  9   4400  02 34 50
02 36 50  ---          21 55 25  36.4  57.6 -4.5     -79.3   114   F  1   6000

02 36 50  3C66A        21 55 25  36.5  56.7 -4.5     -79.8    -6   1  9   6000  02 36 50
02 38 00  ---          21 56 35  36.7  56.7 -4.4     -80.0    64   F  1   6933

02 38 00  SN1986J      21 56 35  36.6  57.6 -4.4     -79.5    -6   1  9   6933  02 38 00
02 40 00  ---          21 58 35  37.0  57.7 -4.4     -79.8   114   F  1   8533
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

02 40 00  3C66A        21 58 35  37.0  56.8 -4.4     -80.3    -6   1  9   8533  02 40 00
02 42 00  ---          22 00 36  37.4  56.9 -4.4     -80.6   114   F  1  10133

02 45 00  3C66A        22 03 36  38.0  57.0 -4.3     -81.0   173   1  9  10133  02 45 00
02 47 10  ---          22 05 47  38.3  57.1 -4.3     -81.4   130   F  1  11867

02 47 10  SN1986J      22 05 47  38.3  58.0 -4.3     -80.8    -6   1  9  11867  02 47 10
02 49 10  ---          22 07 47  38.6  58.1 -4.3     -81.1   114   F  1  13467

02 49 10  3C66A        22 07 47  38.7  57.2 -4.3     -81.7    -6   1  9  13467  02 49 10
02 50 20  ---          22 08 57  38.9  57.2 -4.2     -81.8    64   F  1  14400

02 50 20  SN1986J      22 08 57  38.8  58.1 -4.2     -81.3    -6   1  9  14400  02 50 20
02 52 20  ---          22 10 57  39.2  58.2 -4.2     -81.6   114   F  1  16000

02 52 20  3C66A        22 10 57  39.3  57.3 -4.2     -82.1    -6   1  9  16000  02 52 20
02 53 30  ---          22 12 08  39.5  57.3 -4.2     -82.3    64   F  1  16933

02 53 30  SN1986J      22 12 08  39.4  58.2 -4.2     -81.8    -6   1 10  16933  02 53 30
02 55 30  ---          22 14 08  39.8  58.3 -4.1     -82.1   114   R  1  16667

02 55 30  3C66A        22 14 08  39.9  57.4 -4.1     -82.6    -6   1 10  16667  02 55 30
02 56 40  ---          22 15 18  40.1  57.4 -4.1     -82.8    64   R  1  15733

02 56 40  SN1986J      22 15 18  40.0  58.3 -4.1     -82.2    -6   1 10  15733  02 56 40
02 58 40  ---          22 17 18  40.4  58.4 -4.1     -82.5   114   R  1  14133

02 58 40  3C66A        22 17 18  40.4  57.5 -4.1     -83.1    -6   1 10  14133  02 58 40
02 59 50  ---          22 18 29  40.6  57.5 -4.1     -83.3    64   R  1  13200

02 59 50  SN1986J      22 18 29  40.6  58.4 -4.1     -82.7    -6   1 10  13200  02 59 50
03 01 50  ---          22 20 29  41.0  58.5 -4.0     -83.0   114   R  1  11600

03 01 50  3C66A        22 20 29  41.0  57.5 -4.0     -83.6    -6   1 10  11600  03 01 50
03 03 00  ---          22 21 39  41.2  57.6 -4.0     -83.8    64   R  1  10667

03 03 00  SN1986J      22 21 39  41.2  58.5 -4.0     -83.2    -6   1 10  10667  03 03 00
03 05 00  ---          22 23 40  41.5  58.6 -4.0     -83.5   114   R  1   9067

03 05 00  3C66A        22 23 40  41.6  57.6 -4.0     -84.1    -6   1 10   9067  03 05 00
03 07 00  ---          22 25 40  41.9  57.7 -4.0     -84.4   114   R  1   7467
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

03 10 00  3C84         22 28 40  31.8  57.4 -4.9     -75.4   154   1 10   7467  03 10 00
03 12 00  ---          22 30 41  32.2  57.5 -4.8     -75.7   120   R  1   5867

03 12 00  3C66A        22 30 41  42.9  57.8 -3.9     -85.2   -27   1 10   5867  03 12 00
03 15 20  ---          22 34 01  43.5  57.9 -3.8     -85.7   173   R  1   3200

03 15 20  SN1986J      22 34 01  43.4  58.8 -3.8     -85.1    -6   1 10   3200  03 15 20
03 17 20  ---          22 36 02  43.8  58.9 -3.8     -85.4   114   R  1   1600

03 17 20  3C66A        22 36 02  43.8  57.9 -3.8     -86.0    -6   1 10   1600  03 17 20
03 18 30  ---          22 37 12  44.0  57.9 -3.8     -86.2    64   R  1    667

03 18 30  SN1986J      22 37 12  44.0  58.9 -3.8     -85.5    -6   1 11    667  03 18 30
03 20 30  ---          22 39 12  44.4  58.9 -3.7     -85.9   114   F  1    933

03 20 30  3C66A        22 39 12  44.4  57.9 -3.7     -86.5    -6   1 11    933  03 20 30
03 21 40  ---          22 40 22  44.6  58.0 -3.7     -86.7    64   F  1   1867

03 21 40  SN1986J      22 40 22  44.6  58.9 -3.7     -86.0    -6   1 11   1867  03 21 40
03 23 40  ---          22 42 23  45.0  59.0 -3.7     -86.3   114   F  1   3467

03 23 40  3C66A        22 42 23  45.0  58.0 -3.7     -87.0    -6   1 11   3467  03 23 40
03 24 50  ---          22 43 33  45.2  58.0 -3.7     -87.2    64   F  1   4400

03 24 50  SN1986J      22 43 33  45.2  59.0 -3.7     -86.5    -6   1 11   4400  03 24 50
03 26 50  ---          22 45 33  45.6  59.0 -3.6     -86.8   114   F  1   6000

03 26 50  3C66A        22 45 33  45.6  58.0 -3.6     -87.5    -6   1 11   6000  03 26 50
03 28 00  ---          22 46 43  45.8  58.0 -3.6     -87.7    64   F  1   6933

03 28 00  SN1986J      22 46 43  45.8  59.0 -3.6     -87.0    -6   1 11   6933  03 28 00
03 30 00  ---          22 48 44  46.1  59.1 -3.6     -87.4   114   F  1   8533

03 30 00  3C66A        22 48 44  46.2  58.1 -3.6     -88.1    -6   1 11   8533  03 30 00
03 32 00  ---          22 50 44  46.5  58.1 -3.5     -88.4   114   F  1  10133

03 35 00  3C66A        22 53 44  47.1  58.1 -3.5     -88.9   173   1 11  10133  03 35 00
03 37 10  ---          22 55 55  47.5  58.1 -3.5     -89.3   130   F  1  11867

03 37 10  SN1986J      22 55 55  47.5  59.1 -3.4     -88.5    -6   1 11  11867  03 37 10
03 39 10  ---          22 57 55  47.8  59.2 -3.4     -88.8   114   F  1  13467
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

03 39 10  3C66A        22 57 55  47.8  58.1 -3.4     -89.6    -6   1 11  13467  03 39 10
03 40 20  ---          22 59 05  48.0  58.1 -3.4     -89.8    64   F  1  14400

03 40 20  SN1986J      22 59 05  48.1  59.2 -3.4     -89.0    -6   1 11  14400  03 40 20
03 42 20  ---          23 01 06  48.4  59.2 -3.4     -89.4   114   F  1  16000

03 42 20  3C66A        23 01 06  48.4  58.1 -3.4     -90.1    -6   1 11  16000  03 42 20
03 43 30  ---          23 02 16  48.6  58.1 -3.3     -90.3    64   F  1  16933

03 43 30  SN1986J      23 02 16  48.6  59.2 -3.3     -89.6    -6   1 12  16933  03 43 30
03 45 30  ---          23 04 16  49.0  59.2 -3.3     -89.9   114   R  1  16667

03 45 30  3C66A        23 04 16  49.0  58.1 -3.3     -90.7    -6   1 12  16667  03 45 30
03 46 40  ---          23 05 26  49.2  58.1 -3.3     -90.9    64   R  1  15733

03 46 40  SN1986J      23 05 26  49.2  59.2 -3.3     -90.1    -6   1 12  15733  03 46 40
03 48 40  ---          23 07 27  49.6  59.2 -3.3     -90.4   114   R  1  14133

03 48 40  3C66A        23 07 27  49.6  58.1 -3.3     -91.2    -6   1 12  14133  03 48 40
03 49 50  ---          23 08 37  49.8  58.1 -3.2     -91.4    64   R  1  13200

03 49 50  SN1986J      23 08 37  49.8  59.2 -3.2     -90.6    -6   1 12  13200  03 49 50
03 51 50  ---          23 10 37  50.2  59.2 -3.2     -91.0   114   R  1  11600

03 51 50  3C66A        23 10 37  50.1  58.1 -3.2     -91.8    -6   1 12  11600  03 51 50
03 53 00  ---          23 11 47  50.4  58.1 -3.2     -92.0    64   R  1  10667

03 53 00  SN1986J      23 11 47  50.4  59.2 -3.2     -91.2    -6   1 12  10667  03 53 00
03 55 00  ---          23 13 48  50.8  59.1 -3.2     -91.5   114   R  1   9067

03 55 00  3C66A        23 13 48  50.7  58.0 -3.2     -92.4    -6   1 12   9067  03 55 00
03 57 00  ---          23 15 48  51.1  58.0 -3.1     -92.7   114   R  1   7467

04 12 00  3C66A        23 30 51  53.8  57.7 -2.9     -95.5   889   1 12   7467  04 12 00
04 14 10  ---          23 33 01  54.2  57.6 -2.8     -96.0   130   R  1   5733

04 14 10  SN1986J      23 33 01  54.3  58.8 -2.8     -95.0    -7   1 12   5733  04 14 10
04 16 10  ---          23 35 01  54.7  58.8 -2.8     -95.4   113   R  1   4133

04 16 10  3C66A        23 35 01  54.6  57.5 -2.8     -96.4    -7   1 12   4133  04 16 10
04 17 20  ---          23 36 11  54.8  57.5 -2.8     -96.6    63   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

04 17 20  SN1986J      23 36 11  54.9  58.7 -2.8     -95.6    -7   1 12   3200  04 17 20
04 19 20  ---          23 38 12  55.3  58.7 -2.7     -96.0   113   R  1   1600

04 19 20  3C66A        23 38 12  55.2  57.4 -2.7     -97.0    -7   1 12   1600  04 19 20
04 20 30  ---          23 39 22  55.4  57.4 -2.7     -97.2    63   R  1    667

04 20 30  SN1986J      23 39 22  55.5  58.6 -2.7     -96.3    -7   1 13    667  04 20 30
04 22 30  ---          23 41 22  55.9  58.5 -2.7     -96.7   113   F  1    933

04 22 30  3C66A        23 41 22  55.7  57.3 -2.7     -97.7    -7   1 13    933  04 22 30
04 23 40  ---          23 42 32  56.0  57.2 -2.7     -97.9    63   F  1   1867

04 23 40  SN1986J      23 42 32  56.1  58.5 -2.7     -96.9    -7   1 13   1867  04 23 40
04 25 40  ---          23 44 33  56.4  58.4 -2.6     -97.3   113   F  1   3467

04 25 40  3C66A        23 44 33  56.3  57.2 -2.6     -98.3    -7   1 13   3467  04 25 40
04 26 50  ---          23 45 43  56.5  57.1 -2.6     -98.6    63   F  1   4400

04 26 50  SN1986J      23 45 43  56.7  58.4 -2.6     -97.5    -7   1 13   4400  04 26 50
04 28 50  ---          23 47 43  57.0  58.3 -2.6     -98.0   113   F  1   6000

04 28 50  3C66A        23 47 43  56.9  57.0 -2.6     -99.0    -7   1 13   6000  04 28 50
04 30 00  ---          23 48 53  57.1  56.9 -2.6     -99.2    63   F  1   6933

04 30 00  SN1986J      23 48 53  57.2  58.2 -2.6     -98.2    -7   1 13   6933  04 30 00
04 32 00  ---          23 50 54  57.6  58.1 -2.5     -98.6   113   F  1   8533

04 32 00  3C66A        23 50 54  57.5  56.8 -2.5     -99.7    -7   1 13   8533  04 32 00
04 34 00  ---          23 52 54  57.8  56.7 -2.5    -100.1   113   F  1  10133

04 37 00  3C66A        23 55 55  58.4  56.5 -2.5    -100.8   173   1 13  10133  04 37 00
04 39 10  ---          23 58 05  58.8  56.4 -2.4    -101.3   130   F  1  11867

04 39 10  SN1986J      23 58 05  58.9  57.7 -2.4    -100.2    -7   1 13  11867  04 39 10
04 41 10  ---          00 00 05  59.3  57.6 -2.4    -100.6   113   F  1  13467

04 41 10  3C66A        00 00 05  59.1  56.2 -2.4    -101.8    -7   1 13  13467  04 41 10
04 42 20  ---          00 01 15  59.3  56.1 -2.4    -102.0    63   F  1  14400

04 42 20  SN1986J      00 01 15  59.5  57.5 -2.4    -100.9    -7   1 13  14400  04 42 20
04 44 20  ---          00 03 16  59.9  57.3 -2.3    -101.4   113   F  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

04 44 20  3C66A        00 03 16  59.7  56.0 -2.3    -102.5    -7   1 13  16000  04 44 20
04 45 30  ---          00 04 26  59.9  55.9 -2.3    -102.8    63   F  1  16933

04 45 30  SN1986J      00 04 26  60.1  57.3 -2.3    -101.6    -7   1 14  16933  04 45 30
04 47 30  ---          00 06 26  60.4  57.1 -2.3    -102.1   113   R  1  16667

04 47 30  3C66A        00 06 26  60.2  55.7 -2.3    -103.3    -7   1 14  16667  04 47 30
04 48 40  ---          00 07 37  60.5  55.6 -2.3    -103.6    63   R  1  15733

04 48 40  SN1986J      00 07 37  60.6  57.0 -2.3    -102.4    -7   1 14  15733  04 48 40
04 50 40  ---          00 09 37  61.0  56.8 -2.2    -102.9   113   R  1  14133

04 50 40  3C66A        00 09 37  60.8  55.5 -2.2    -104.1    -7   1 14  14133  04 50 40
04 51 50  ---          00 10 47  61.0  55.3 -2.2    -104.3    63   R  1  13200

04 51 50  SN1986J      00 10 47  61.2  56.7 -2.2    -103.1    -7   1 14  13200  04 51 50
04 53 50  ---          00 12 47  61.6  56.6 -2.2    -103.6   113   R  1  11600

04 53 50  3C66A        00 12 47  61.4  55.2 -2.2    -104.9    -7   1 14  11600  04 53 50
04 55 00  ---          00 13 58  61.6  55.0 -2.2    -105.2    63   R  1  10667

04 55 00  SN1986J      00 13 58  61.8  56.5 -2.1    -103.9    -7   1 14  10667  04 55 00
04 57 00  ---          00 15 58  62.1  56.3 -2.1    -104.4   113   R  1   9067

04 57 00  3C66A        00 15 58  61.9  54.8 -2.1    -105.7    -7   1 14   9067  04 57 00
04 59 00  ---          00 17 58  62.3  54.6 -2.1    -106.2   113   R  1   7467

05 02 00  3C66A        00 20 59  62.8  54.3 -2.0    -107.0   173   1 14   7467  05 02 00
05 04 10  ---          00 23 09  63.2  54.0 -2.0    -107.6   130   R  1   5733

05 04 10  SN1986J      00 23 09  63.4  55.5 -2.0    -106.3    -7   1 14   5733  05 04 10
05 06 10  ---          00 25 09  63.8  55.3 -2.0    -106.9   113   R  1   4133

05 06 10  3C66A        00 25 09  63.5  53.8 -2.0    -108.2    -7   1 14   4133  05 06 10
05 07 20  ---          00 26 20  63.7  53.6 -1.9    -108.5    63   R  1   3200

05 07 20  SN1986J      00 26 20  64.0  55.1 -1.9    -107.2    -7   1 14   3200  05 07 20
05 09 20  ---          00 28 20  64.3  54.9 -1.9    -107.8   113   R  1   1600

05 09 20  3C66A        00 28 20  64.1  53.3 -1.9    -109.1    -7   1 14   1600  05 09 20
05 10 30  ---          00 29 30  64.3  53.2 -1.9    -109.5    63   R  1    667
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

-----------  Tape Change ------------

05 10 30  SN1986J      00 29 30  64.5  54.7 -1.9    -108.1    -7   2  1    667  05 10 30
05 12 30  ---          00 31 30  64.9  54.4 -1.9    -108.7   113   F  1    933

05 12 30  3C66A        00 31 30  64.6  52.9 -1.9    -110.1    -7   2  1    933  05 12 30
05 13 40  ---          00 32 41  64.8  52.7 -1.8    -110.4    63   F  1   1867

05 13 40  SN1986J      00 32 41  65.1  54.3 -1.8    -109.1    -7   2  1   1867  05 13 40
05 15 40  ---          00 34 41  65.4  54.0 -1.8    -109.7   113   F  1   3467

05 15 40  3C66A        00 34 41  65.2  52.4 -1.8    -111.0    -7   2  1   3467  05 15 40
05 16 50  ---          00 35 51  65.4  52.2 -1.8    -111.4    63   F  1   4400

05 16 50  SN1986J      00 35 51  65.6  53.8 -1.8    -110.0    -7   2  1   4400  05 16 50
05 18 50  ---          00 37 51  66.0  53.5 -1.8    -110.6   113   F  1   6000

05 18 50  3C66A        00 37 51  65.7  51.9 -1.8    -112.1    -7   2  1   6000  05 18 50
05 20 00  ---          00 39 02  65.9  51.7 -1.7    -112.4    63   F  1   6933

05 20 00  SN1986J      00 39 02  66.2  53.3 -1.7    -111.0    -7   2  1   6933  05 20 00
05 22 00  ---          00 41 02  66.5  53.0 -1.7    -111.7   113   F  1   8533

05 22 00  3C66A        00 41 02  66.3  51.4 -1.7    -113.1    -7   2  1   8533  05 22 00
05 24 00  ---          00 43 02  66.6  51.0 -1.7    -113.8   113   F  1  10133

05 27 00  3C66A        00 46 03  67.1  50.4 -1.6    -114.8   173   2  1  10133  05 27 00
05 29 10  ---          00 48 13  67.4  50.0 -1.6    -115.6   130   F  1  11867

05 29 10  SN1986J      00 48 13  67.8  51.6 -1.6    -114.1    -7   2  1  11867  05 29 10
05 31 10  ---          00 50 14  68.1  51.2 -1.5    -114.8   113   F  1  13467

05 31 10  3C66A        00 50 14  67.8  49.6 -1.5    -116.3    -7   2  1  13467  05 31 10
05 32 20  ---          00 51 24  68.0  49.3 -1.5    -116.8    63   F  1  14400

05 32 20  SN1986J      00 51 24  68.3  51.0 -1.5    -115.2    -7   2  1  14400  05 32 20
05 34 20  ---          00 53 24  68.6  50.5 -1.5    -116.0   113   F  1  16000

05 34 20  3C66A        00 53 24  68.3  48.9 -1.5    -117.5    -7   2  1  16000  05 34 20
05 35 30  ---          00 54 34  68.5  48.6 -1.5    -118.0    63   F  1  16933

05 35 30  SN1986J      00 54 34  68.8  50.3 -1.5    -116.4    -7   2  2  16933  05 35 30
05 37 30  ---          00 56 35  69.2  49.8 -1.4    -117.2   113   R  1  16667
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

05 37 30  3C66A        00 56 35  68.8  48.1 -1.4    -118.8    -7   2  2  16667  05 37 30
05 38 40  ---          00 57 45  69.0  47.8 -1.4    -119.2    63   R  1  15734

05 38 40  SN1986J      00 57 45  69.3  49.5 -1.4    -117.7    -7   2  2  15734  05 38 40
05 40 40  ---          00 59 45  69.7  49.0 -1.4    -118.5   113   R  1  14134

05 40 40  3C66A        00 59 45  69.3  47.3 -1.4    -120.0    -7   2  2  14134  05 40 40
05 41 50  ---          01 00 55  69.5  47.0 -1.4    -120.5    63   R  1  13200

05 41 50  SN1986J      01 00 55  69.9  48.7 -1.4    -118.9    -7   2  2  13200  05 41 50
05 43 50  ---          01 02 56  70.2  48.2 -1.3    -119.8   113   R  1  11600

05 43 50  3C66A        01 02 56  69.8  46.5 -1.3    -121.4    -7   2  2  11600  05 43 50
05 45 00  ---          01 04 06  70.0  46.1 -1.3    -121.9    63   R  1  10667

05 45 00  SN1986J      01 04 06  70.4  47.9 -1.3    -120.3    -7   2  2  10667  05 45 00
05 47 00  ---          01 06 06  70.7  47.3 -1.3    -121.1   113   R  1   9067

05 47 00  3C66A        01 06 06  70.3  45.6 -1.3    -122.8    -7   2  2   9067  05 47 00
05 49 00  ---          01 08 06  70.6  45.0 -1.2    -123.7   113   R  1   7467

05 52 00  3C84         01 11 07  61.9  58.2 -2.2    -102.4   157   2  2   7467  05 52 00
05 54 00  ---          01 13 07  62.3  58.0 -2.1    -102.9   120   R  1   5867

05 54 00  3C66A        01 13 07  71.4  43.4 -1.2    -126.0   -24   2  2   5867  05 54 00
05 57 20  ---          01 16 28  71.8  42.2 -1.1    -127.7   176   R  1   3200

05 57 20  SN1986J      01 16 28  72.3  44.0 -1.1    -126.1    -7   2  2   3200  05 57 20
05 59 20  ---          01 18 28  72.6  43.2 -1.1    -127.1   113   R  1   1600

05 59 20  3C66A        01 18 28  72.1  41.5 -1.1    -128.8    -7   2  2   1600  05 59 20
06 00 30  ---          01 19 38  72.3  41.0 -1.1    -129.4    63   R  1    667

06 00 30  SN1986J      01 19 38  72.8  42.8 -1.1    -127.7    -7   2  3    667  06 00 30
06 02 30  ---          01 21 39  73.0  42.0 -1.0    -128.8   113   F  1    933

06 02 30  3C66A        01 21 39  72.6  40.2 -1.0    -130.5    -7   2  3    933  06 02 30
06 03 40  ---          01 22 49  72.7  39.8 -1.0    -131.1    63   F  1   1867

06 03 40  SN1986J      01 22 49  73.2  41.5 -1.0    -129.4    -7   2  3   1867  06 03 40
06 05 40  ---          01 24 49  73.5  40.7 -1.0    -130.6   113   F  1   3467
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

06 05 40  3C66A        01 24 49  73.0  38.9 -1.0    -132.2    -7   2  3   3467  06 05 40
06 06 50  ---          01 25 59  73.2  38.4 -1.0    -132.9    63   F  1   4400

06 06 50  SN1986J      01 25 59  73.7  40.2 -0.9    -131.2    -7   2  3   4400  06 06 50
06 08 50  ---          01 28 00  73.9  39.3 -0.9    -132.4   113   F  1   6000

06 08 50  3C66A        01 28 00  73.4  37.6 -0.9    -134.1    -7   2  3   6000  06 08 50
06 10 00  ---          01 29 10  73.6  37.0 -0.9    -134.8    63   F  1   6933

06 10 00  SN1986J      01 29 10  74.1  38.8 -0.9    -133.1    -7   2  3   6933  06 10 00
06 12 00  ---          01 31 10  74.4  37.9 -0.9    -134.4   113   F  1   8533

06 12 00  3C66A        01 31 10  73.8  36.1 -0.9    -136.0    -7   2  3   8533  06 12 00
06 14 00  ---          01 33 11  74.1  35.1 -0.8    -137.3   113   F  1  10133

06 17 00  3C66A        01 36 11  74.5  33.6 -0.8    -139.3   173   2  3  10133  06 17 00
06 19 10  ---          01 38 21  74.7  32.5 -0.7    -140.8   130   F  1  11867

06 19 10  SN1986J      01 38 21  75.3  34.2 -0.7    -139.2    -7   2  3  11867  06 19 10
06 21 10  ---          01 40 22  75.5  33.0 -0.7    -140.6   113   F  1  13467

06 21 10  3C66A        01 40 22  74.9  31.4 -0.7    -142.2    -7   2  3  13467  06 21 10
06 22 20  ---          01 41 32  75.1  30.7 -0.7    -143.0    63   F  1  14400

06 22 20  SN1986J      01 41 32  75.6  32.4 -0.7    -141.4    -7   2  3  14400  06 22 20
06 24 20  ---          01 43 32  75.9  31.2 -0.7    -142.9   113   F  1  16000

06 24 20  3C66A        01 43 32  75.3  29.6 -0.7    -144.4    -7   2  3  16000  06 24 20
06 25 30  ---          01 44 42  75.4  28.9 -0.6    -145.3    63   F  1  16933

06 25 30  SN1986J      01 44 42  76.0  30.5 -0.6    -143.8    -7   2  4  16933  06 25 30
06 27 30  ---          01 46 43  76.2  29.2 -0.6    -145.4   113   R  1  16667

06 27 30  3C66A        01 46 43  75.6  27.7 -0.6    -146.8    -7   2  4  16667  06 27 30
06 28 40  ---          01 47 53  75.7  26.9 -0.6    -147.7    63   R  1  15733

06 28 40  SN1986J      01 47 53  76.3  28.4 -0.6    -146.3    -7   2  4  15733  06 28 40
06 30 40  ---          01 49 53  76.5  27.1 -0.6    -147.9   113   R  1  14133

06 30 40  3C66A        01 49 53  75.9  25.7 -0.6    -149.3    -7   2  4  14133  06 30 40
06 31 50  ---          01 51 03  76.0  24.9 -0.5    -150.3    63   R  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

06 31 50  SN1986J      01 51 03  76.7  26.3 -0.5    -148.9    -7   2  4  13200  06 31 50
06 33 50  ---          01 53 04  76.8  24.9 -0.5    -150.6   113   R  1  11600

06 33 50  3C66A        01 53 04  76.2  23.6 -0.5    -151.9    -7   2  4  11600  06 33 50
06 35 00  ---          01 54 14  76.3  22.8 -0.5    -152.9    63   R  1  10667

06 35 00  SN1986J      01 54 14  76.9  24.1 -0.5    -151.6    -7   2  4  10667  06 35 00
06 37 00  ---          01 56 14  77.1  22.6 -0.4    -153.4   113   R  1   9067

06 37 00  3C66A        01 56 14  76.5  21.4 -0.4    -154.6    -7   2  4   9067  06 37 00
06 39 00  ---          01 58 15  76.6  19.9 -0.4    -156.3   113   R  1   7467

06 42 00  3C66A        02 01 15  76.8  17.7 -0.4    -159.0   173   2  4   7467  06 42 00
06 44 10  ---          02 03 26  77.0  16.1 -0.3    -161.0   130   R  1   5733

06 44 10  SN1986J      02 03 26  77.6  17.0 -0.3    -160.0    -7   2  4   5733  06 44 10
06 46 10  ---          02 05 26  77.8  15.4 -0.3    -162.0   113   R  1   4133

06 46 10  3C66A        02 05 26  77.1  14.5 -0.3    -162.8    -7   2  4   4133  06 46 10
06 47 20  ---          02 06 36  77.1  13.6 -0.3    -163.9    63   R  1   3200

06 47 20  SN1986J      02 06 36  77.8  14.4 -0.3    -163.1    -7   2  4   3200  06 47 20
06 49 20  ---          02 08 36  77.9  12.7 -0.2    -165.1   113   R  1   1600

06 49 20  3C66A        02 08 36  77.2  12.0 -0.2    -165.8    -7   2  4   1600  06 49 20
06 50 30  ---          02 09 47  77.3  11.1 -0.2    -166.9    63   R  1    667

06 50 30  SN1986J      02 09 47  78.0  11.7 -0.2    -166.3    -7   2  5    667  06 50 30
06 52 30  ---          02 11 47  78.1  10.0 -0.2    -168.4   113   F  1    933

06 52 30  3C66A        02 11 47  77.4   9.4 -0.2    -168.9    -7   2  5    933  06 52 30
06 53 40  ---          02 12 57  77.4   8.5 -0.2    -170.0    63   F  1   1867

06 53 40  SN1986J      02 12 57  78.1   9.0 -0.2    -169.6    -7   2  5   1867  06 53 40
06 55 40  ---          02 14 57  78.2   7.2 -0.1    -171.6   113   F  1   3467

06 55 40  3C66A        02 14 57  77.5   6.8 -0.1    -172.0    -7   2  5   3467  06 55 40
06 56 50  ---          02 16 08  77.5   5.8 -0.1    -173.1    63   F  1   4400

06 56 50  SN1986J      02 16 08  78.2   6.1 -0.1    -172.9    -7   2  5   4400  06 56 50
06 58 50  ---          02 18 08  78.2   4.3 -0.1    -175.0   113   F  1   6000
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

06 58 50  3C66A        02 18 08  77.5   4.2 -0.1    -175.1    -7   2  5   6000  06 58 50
07 00 00  ---          02 19 18  77.5   3.2 -0.1    -176.3    63   F  1   6933

07 00 00  SN1986J      02 19 18  78.3   3.3 -0.1    -176.2    -7   2  5   6933  07 00 00
07 02 00  ---          02 21 18  78.3   1.5  0.0    -178.3   113   F  1   8533

07 02 00  3C66A        02 21 18  77.6   1.5  0.0    -178.3    -7   2  5   8533  07 02 00
07 04 00  ---          02 23 19  77.6  -0.2  0.0     179.7   113   F  1  10133

07 07 00  3C66A        02 26 19  77.6  -2.8  0.1     176.7   172   2  5  10133  07 07 00
07 09 10  ---          02 28 30  77.5  -4.6  0.1     174.6   130   F  1  11867

07 09 10  SN1986J      02 28 30  78.2  -5.1  0.1     174.1    -7   2  5  11867  07 09 10
07 11 10  ---          02 30 30  78.2  -6.9  0.1     172.0   113   F  1  13467

07 11 10  3C66A        02 30 30  77.5  -6.3  0.1     172.6    -7   2  5  13467  07 11 10
07 12 20  ---          02 31 40  77.5  -7.3  0.1     171.4    63   F  1  14400

07 12 20  SN1986J      02 31 40  78.1  -7.9  0.1     170.8    -7   2  5  14400  07 12 20
07 14 20  ---          02 33 40  78.1  -9.7  0.2     168.7   113   F  1  16000

07 14 20  3C66A        02 33 40  77.4  -8.9  0.2     169.5    -7   2  5  16000  07 14 20
07 15 30  ---          02 34 51  77.4  -9.9  0.2     168.3    63   F  1  16933

07 15 30  SN1986J      02 34 51  78.0 -10.7  0.2     167.5    -7   2  6  16933  07 15 30
07 17 30  ---          02 36 51  77.9 -12.4  0.2     165.5   113   R  1  16667

07 17 30  3C66A        02 36 51  77.3 -11.5  0.2     166.4    -7   2  6  16667  07 17 30
07 18 40  ---          02 38 01  77.2 -12.5  0.2     165.3    63   R  1  15733

07 18 40  SN1986J      02 38 01  77.9 -13.4  0.3     164.3    -7   2  6  15733  07 18 40
07 20 40  ---          02 40 02  77.8 -15.1  0.3     162.3   113   R  1  14133

07 20 40  3C66A        02 40 02  77.1 -14.0  0.3     163.4    -7   2  6  14133  07 20 40
07 21 50  ---          02 41 12  77.1 -15.0  0.3     162.3    63   R  1  13200

07 21 50  SN1986J      02 41 12  77.7 -16.1  0.3     161.2    -7   2  6  13200  07 21 50
07 23 50  ---          02 43 12  77.6 -17.7  0.3     159.3   113   R  1  11600

07 23 50  3C66A        02 43 12  76.9 -16.5  0.3     160.5    -7   2  6  11600  07 23 50
07 25 00  ---          02 44 22  76.9 -17.4  0.4     159.4    63   R  1  10667
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

07 25 00  SN1986J      02 44 22  77.5 -18.6  0.4     158.2    -7   2  6  10667  07 25 00
07 27 00  ---          02 46 23  77.4 -20.2  0.4     156.3   113   R  1   9067

07 27 00  3C66A        02 46 23  76.7 -18.9  0.4     157.6    -7   2  6   9067  07 27 00
07 29 00  ---          02 48 23  76.6 -20.3  0.4     155.8   113   R  1   7467

07 32 00  3C66A        02 51 23  76.4 -22.5  0.5     153.3   173   2  6   7467  07 32 00
07 34 10  ---          02 53 34  76.2 -23.9  0.5     151.5   130   R  1   5733

07 34 10  SN1986J      02 53 34  76.8 -25.5  0.5     149.9    -7   2  6   5733  07 34 10
07 36 10  ---          02 55 34  76.6 -26.9  0.5     148.2   113   R  1   4133

07 36 10  3C66A        02 55 34  76.0 -25.3  0.5     149.8    -7   2  6   4133  07 36 10
07 37 20  ---          02 56 44  75.9 -26.0  0.6     148.9    63   R  1   3200

07 37 20  SN1986J      02 56 44  76.5 -27.7  0.6     147.3    -7   2  6   3200  07 37 20
07 39 20  ---          02 58 45  76.3 -29.0  0.6     145.7   113   R  1   1600

07 39 20  3C66A        02 58 45  75.7 -27.3  0.6     147.3    -7   2  6   1600  07 39 20
07 40 30  ---          02 59 55  75.6 -28.0  0.6     146.4    63   R  1    667

07 40 30  SN1986J      02 59 55  76.1 -29.7  0.6     144.7    -7   2  7    667  07 40 30
07 42 30  ---          03 01 55  75.9 -31.0  0.7     143.2   113   F  1    933

07 42 30  3C66A        03 01 55  75.4 -29.2  0.6     144.9    -7   2  7    933  07 42 30
07 43 40  ---          03 03 05  75.2 -29.9  0.7     144.1    63   F  1   1867

07 43 40  SN1986J      03 03 05  75.8 -31.7  0.7     142.3    -7   2  7   1867  07 43 40
07 45 40  ---          03 05 06  75.6 -32.8  0.7     140.8   113   F  1   3467

07 45 40  3C66A        03 05 06  75.0 -31.0  0.7     142.6    -7   2  7   3467  07 45 40
07 46 50  ---          03 06 16  74.9 -31.7  0.7     141.8    63   F  1   4400

07 46 50  SN1986J      03 06 16  75.4 -33.5  0.7     140.0    -7   2  7   4400  07 46 50
07 48 50  ---          03 08 16  75.2 -34.6  0.8     138.6   113   F  1   6000

07 48 50  3C66A        03 08 16  74.7 -32.8  0.8     140.4    -7   2  7   6000  07 48 50
07 50 00  ---          03 09 26  74.5 -33.4  0.8     139.6    63   F  1   6933

07 50 00  SN1986J      03 09 26  75.0 -35.2  0.8     137.8    -7   2  7   6933  07 50 00
07 52 00  ---          03 11 27  74.8 -36.3  0.8     136.5   113   F  1   8533
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

07 52 00  3C66A        03 11 27  74.3 -34.4  0.8     138.3    -7   2  7   8533  07 52 00
07 54 00  ---          03 13 27  74.0 -35.4  0.8     137.0   113   F  1  10133

07 57 00  3C66A        03 16 27  73.7 -36.8  0.9     135.1   173   2  7  10133  07 57 00
07 59 10  ---          03 18 38  73.4 -37.8  0.9     133.8   130   F  1  11867

07 59 10  SN1986J      03 18 38  73.8 -39.7  0.9     131.9    -7   2  7  11867  07 59 10
08 01 10  ---          03 20 38  73.5 -40.6  1.0     130.8   113   F  1  13467

08 01 10  3C66A        03 20 38  73.1 -38.7  1.0     132.6    -7   2  7  13467  08 01 10
08 02 20  ---          03 21 48  72.9 -39.2  1.0     131.9    63   F  1  14400

08 02 20  SN1986J      03 21 48  73.4 -41.1  1.0     130.1    -7   2  7  14400  08 02 20
08 04 20  ---          03 23 49  73.1 -41.9  1.0     129.0   113   F  1  16000

08 04 20  3C66A        03 23 49  72.7 -40.0  1.0     130.8    -7   2  7  16000  08 04 20
08 05 30  ---          03 24 59  72.5 -40.5  1.0     130.2    63   F  1  16934

08 05 30  SN1986J      03 24 59  72.9 -42.3  1.0     128.3    -7   2  8  16934  08 05 30
08 07 30  ---          03 26 59  72.6 -43.1  1.1     127.3   113   R  1  16667

08 07 30  3C66A        03 26 59  72.2 -41.2  1.1     129.1    -7   2  8  16667  08 07 30
08 08 40  ---          03 28 09  72.1 -41.7  1.1     128.5    63   R  1  15733

08 08 40  SN1986J      03 28 09  72.5 -43.5  1.1     126.7    -7   2  8  15733  08 08 40
08 10 40  ---          03 30 10  72.2 -44.3  1.1     125.6   113   R  1  14133

08 10 40  3C66A        03 30 10  71.8 -42.4  1.1     127.4    -7   2  8  14133  08 10 40
08 11 50  ---          03 31 20  71.6 -42.8  1.1     126.9    63   R  1  13200

08 11 50  SN1986J      03 31 20  72.0 -44.7  1.1     125.1    -7   2  8  13200  08 11 50
08 13 50  ---          03 33 20  71.7 -45.3  1.2     124.1   113   R  1  11600

08 13 50  3C66A        03 33 20  71.3 -43.5  1.2     125.9    -7   2  8  11600  08 13 50
08 15 00  ---          03 34 30  71.1 -43.9  1.2     125.3    63   R  1  10666

08 15 00  SN1986J      03 34 30  71.5 -45.7  1.2     123.5    -7   2  8  10666  08 15 00
08 17 00  ---          03 36 31  71.2 -46.4  1.2     122.6   113   R  1   9066

08 17 00  3C66A        03 36 31  70.8 -44.5  1.2     124.4    -7   2  8   9066  08 17 00
08 19 00  ---          03 38 31  70.5 -45.1  1.3     123.4   113   R  1   7466
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

08 22 00  3C84         03 41 32  78.3 -20.0  0.4     156.8   157   2  8   7466  08 22 00
08 24 00  ---          03 43 32  78.1 -21.7  0.4     154.8   120   R  1   5866

08 24 00  3C66A        03 43 32  69.8 -46.6  1.3     121.2   -23   2  8   5866  08 24 00
08 27 20  ---          03 46 52  69.2 -47.5  1.4     119.8   177   R  1   3200

08 27 20  SN1986J      03 46 52  69.5 -49.2  1.4     118.1    -7   2  8   3200  08 27 20
08 29 20  ---          03 48 53  69.2 -49.7  1.4     117.3   113   R  1   1600

08 29 20  3C66A        03 48 53  68.9 -48.0  1.4     119.0    -7   2  8   1600  08 29 20
08 30 30  ---          03 50 03  68.7 -48.2  1.5     118.5    63   R  1    666

08 30 30  SN1986J      03 50 03  69.0 -50.0  1.5     116.9    -7   2  9    666  08 30 30
08 32 30  ---          03 52 03  68.7 -50.5  1.5     116.1   113   F  1    934

08 32 30  3C66A        03 52 03  68.4 -48.7  1.5     117.8    -7   2  9    934  08 32 30
08 33 40  ---          03 53 13  68.2 -49.0  1.5     117.3    63   F  1   1867

08 33 40  SN1986J      03 53 13  68.5 -50.7  1.5     115.7    -7   2  9   1867  08 33 40
08 35 40  ---          03 55 14  68.2 -51.1  1.5     114.9   113   F  1   3467

08 35 40  3C66A        03 55 14  67.9 -49.4  1.5     116.6    -7   2  9   3467  08 35 40
08 36 50  ---          03 56 24  67.7 -49.7  1.6     116.1    63   F  1   4400

08 36 50  SN1986J      03 56 24  68.0 -51.4  1.6     114.5    -7   2  9   4400  08 36 50
08 38 50  ---          03 58 24  67.6 -51.8  1.6     113.8   113   F  1   6000

08 38 50  3C66A        03 58 24  67.4 -50.1  1.6     115.4    -7   2  9   6000  08 38 50
08 40 00  ---          03 59 35  67.2 -50.3  1.6     115.0    63   F  1   6934

08 40 00  SN1986J      03 59 35  67.4 -52.0  1.6     113.4    -7   2  9   6934  08 40 00
08 42 00  ---          04 01 35  67.1 -52.4  1.6     112.7   113   F  1   8534

08 42 00  3C66A        04 01 35  66.8 -50.7  1.6     114.3    -7   2  9   8534  08 42 00
08 44 00  ---          04 03 35  66.5 -51.1  1.7     113.6   113   F  1  10134

08 47 00  3C66A        04 06 36  66.0 -51.6  1.7     112.6   173   2  9  10134  08 47 00
08 49 10  ---          04 08 46  65.6 -52.0  1.8     111.9   130   F  1  11867

08 49 10  SN1986J      04 08 46  65.9 -53.6  1.8     110.4    -7   2  9  11867  08 49 10
08 51 10  ---          04 10 46  65.5 -53.9  1.8     109.8   113   F  1  13467
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

08 51 10  3C66A        04 10 46  65.3 -52.3  1.8     111.2    -7   2  9  13467  08 51 10
08 52 20  ---          04 11 57  65.1 -52.5  1.8     110.9    63   F  1  14400

08 52 20  SN1986J      04 11 57  65.3 -54.1  1.8     109.4    -7   2  9  14400  08 52 20
08 54 20  ---          04 13 57  65.0 -54.4  1.9     108.8   113   F  1  16000

08 54 20  3C66A        04 13 57  64.7 -52.8  1.8     110.3    -7   2  9  16000  08 54 20
08 55 30  ---          04 15 07  64.5 -53.0  1.9     109.9    63   F  1  16934

08 55 30  SN1986J      04 15 07  64.7 -54.5  1.9     108.5    -7   2 10  16934  08 55 30
08 57 30  ---          04 17 07  64.4 -54.8  1.9     107.9   113   R  1  16666

08 57 30  3C66A        04 17 07  64.2 -53.3  1.9     109.3    -7   2 10  16666  08 57 30
08 58 40  ---          04 18 18  64.0 -53.4  1.9     109.0    63   R  1  15733

08 58 40  SN1986J      04 18 18  64.2 -55.0  1.9     107.6    -7   2 10  15733  08 58 40
09 00 40  ---          04 20 18  63.8 -55.2  2.0     107.0   113   R  1  14133

09 00 40  3C66A        04 20 18  63.6 -53.7  2.0     108.4    -7   2 10  14133  09 00 40
09 01 50  ---          04 21 28  63.4 -53.8  2.0     108.1    63   R  1  13200

09 01 50  SN1986J      04 21 28  63.6 -55.4  2.0     106.7    -7   2 10  13200  09 01 50
09 03 50  ---          04 23 28  63.3 -55.6  2.0     106.1   113   R  1  11600

09 03 50  3C66A        04 23 28  63.1 -54.1  2.0     107.5    -7   2 10  11600  09 03 50
09 05 00  ---          04 24 39  62.9 -54.2  2.0     107.2    63   R  1  10666

09 05 00  SN1986J      04 24 39  63.1 -55.7  2.0     105.8    -7   2 10  10666  09 05 00
09 07 00  ---          04 26 39  62.7 -55.9  2.1     105.3   113   R  1   9066

09 07 00  3C66A        04 26 39  62.5 -54.5  2.1     106.6    -7   2 10   9066  09 07 00
09 09 00  ---          04 28 39  62.2 -54.7  2.1     106.1   113   R  1   7466

09 12 00  3C66A        04 31 40  61.7 -55.0  2.1     105.3   173   2 10   7466  09 12 00
09 14 10  ---          04 33 50  61.3 -55.2  2.2     104.7   130   R  1   5733

09 14 10  SN1986J      04 33 50  61.4 -56.6  2.2     103.4    -7   2 10   5733  09 14 10
09 16 10  ---          04 35 50  61.1 -56.8  2.2     102.9   113   R  1   4133

09 16 10  3C66A        04 35 50  60.9 -55.4  2.2     104.2    -7   2 10   4133  09 16 10
09 17 20  ---          04 37 01  60.7 -55.5  2.2     103.9    63   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

09 17 20  SN1986J      04 37 01  60.9 -56.9  2.2     102.7    -7   2 10   3200  09 17 20
09 19 20  ---          04 39 01  60.5 -57.1  2.3     102.2   113   R  1   1600

09 19 20  3C66A        04 39 01  60.4 -55.7  2.3     103.4    -7   2 10   1600  09 19 20
09 20 30  ---          04 40 11  60.2 -55.8  2.3     103.1    63   R  1    666

09 20 30  SN1986J      04 40 11  60.3 -57.2  2.3     101.9    -7   2 11    666  09 20 30
09 22 30  ---          04 42 12  59.9 -57.3  2.3     101.4   113   F  1    934

09 22 30  3C66A        04 42 12  59.8 -55.9  2.3     102.7    -7   2 11    934  09 22 30
09 23 40  ---          04 43 22  59.6 -56.0  2.3     102.4    63   F  1   1867

09 23 40  SN1986J      04 43 22  59.7 -57.4  2.3     101.2    -7   2 11   1867  09 23 40
09 25 40  ---          04 45 22  59.3 -57.5  2.4     100.7   113   F  1   3467

09 25 40  3C66A        04 45 22  59.2 -56.2  2.4     101.9    -7   2 11   3467  09 25 40
09 26 50  ---          04 46 32  59.0 -56.3  2.4     101.6    63   F  1   4400

09 26 50  SN1986J      04 46 32  59.1 -57.6  2.4     100.4    -7   2 11   4400  09 26 50
09 28 50  ---          04 48 33  58.8 -57.7  2.4     100.0   113   F  1   6000

09 28 50  3C66A        04 48 33  58.7 -56.4  2.4     101.2    -7   2 11   6000  09 28 50
09 30 00  ---          04 49 43  58.4 -56.5  2.4     100.9    63   F  1   6934

09 30 00  SN1986J      04 49 43  58.5 -57.8  2.4      99.7    -7   2 11   6934  09 30 00
09 32 00  ---          04 51 43  58.2 -57.9  2.5      99.3   113   F  1   8534

09 32 00  3C66A        04 51 43  58.1 -56.6  2.5     100.5    -7   2 11   8534  09 32 00
09 34 00  ---          04 53 43  57.7 -56.7  2.5     100.0   113   F  1  10134

09 37 00  3C66A        04 56 44  57.2 -56.9  2.6      99.3   173   2 11  10134  09 37 00
09 39 10  ---          04 58 54  56.8 -57.0  2.6      98.9   130   F  1  11867

09 39 10  SN1986J      04 58 54  56.9 -58.3  2.6      97.8    -7   2 11  11867  09 39 10
09 41 10  ---          05 00 55  56.5 -58.4  2.6      97.4   113   F  1  13467

09 41 10  3C66A        05 00 55  56.4 -57.1  2.6      98.5    -7   2 11  13467  09 41 10
09 42 20  ---          05 02 05  56.2 -57.2  2.7      98.2    63   F  1  14400

09 42 20  SN1986J      05 02 05  56.3 -58.4  2.7      97.1    -7   2 11  14400  09 42 20
09 44 20  ---          05 04 05  55.9 -58.5  2.7      96.7   113   F  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 Oct 2005   Day 298 ---

09 44 20  3C66A        05 04 05  55.9 -57.3  2.7      97.8    -7   2 11  16000  09 44 20
09 45 30  ---          05 05 15  55.6 -57.3  2.7      97.5    63   F  1  16934

09 45 30  SN1986J      05 05 15  55.7 -58.6  2.7      96.5    -7   2 12  16934  09 45 30
09 47 30  ---          05 07 16  55.3 -58.6  2.7      96.1   113   R  1  16666

09 47 30  3C66A        05 07 16  55.3 -57.4  2.7      97.1    -7   2 12  16666  09 47 30
09 48 40  ---          05 08 26  55.1 -57.5  2.8      96.9    63   R  1  15733

09 48 40  SN1986J      05 08 26  55.1 -58.7  2.8      95.9    -7   2 12  15733  09 48 40
09 50 40  ---          05 10 26  54.8 -58.7  2.8      95.5   113   R  1  14133

09 50 40  3C66A        05 10 26  54.7 -57.5  2.8      96.5    -7   2 12  14133  09 50 40
09 51 50  ---          05 11 36  54.5 -57.6  2.8      96.3    63   R  1  13200

09 51 50  SN1986J      05 11 36  54.5 -58.8  2.8      95.3    -7   2 12  13200  09 51 50
09 53 50  ---          05 13 37  54.2 -58.8  2.8      94.9   113   R  1  11600

09 53 50  3C66A        05 13 37  54.1 -57.6  2.8      95.9    -7   2 12  11600  09 53 50
09 55 00  ---          05 14 47  53.9 -57.7  2.9      95.6    63   R  1  10666

09 55 00  SN1986J      05 14 47  54.0 -58.9  2.9      94.6    -7   2 12  10666  09 55 00
09 57 00  ---          05 16 47  53.6 -58.9  2.9      94.3   113   R  1   9066

09 57 00  3C66A        05 16 47  53.6 -57.7  2.9      95.2    -7   2 12   9066  09 57 00
09 59 00  ---          05 18 48  53.2 -57.8  2.9      94.9   113   R  1   7466


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/sched.2004oct04/setups/v6cm-256-8-2-UL.set
   Matches group v6cm_2 in /usr/local/sched.2004oct04/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4979.49   4979.49   4979.49   4979.49   4995.49   4995.49   4995.49   4995.49
   BBC fr=     879.49    879.49    879.49    879.49    895.49    895.49    895.49    895.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   510   490   510  6490  6510  6490  6510
    PCALFR2=   490   510   490   510  6490  6510  6490  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- 8TH epoch of obs. of SN1986J in NGC891: VLBA/MkIV 6cm pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SN1986J           02 19 22.592220   * 02 22 31.320000     02 22 54.272068 
                     42 06 18.95870    * 42 19 57.28200      42 21 40.60344 
                     From catalog imbedded in main SCHED input file.
                        5.433 scan hours,    633.193 baseline hours above horizon.

 * 3C66A             02 19 29.982891   * 02 22 39.611477     02 23 02.677248 
                     42 48 29.80879    * 43 02 07.79928      43 03 51.01599 
                     From catalog imbedded in main SCHED input file.
                        4.667 scan hours,    517.153 baseline hours above horizon.

 * 3C84              03 16 29.567269   * 03 19 48.160100     03 20 12.253867 
                     41 19 51.91887    * 41 30 42.10600      41 32 04.54771 
                     From catalog imbedded in main SCHED input file.
                        0.167 scan hours,     21.385 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1986J            149.3
   3C66A              148.6
   3C84               145.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

