  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1993J @ 6cm
 Exp. Code:  GM057A  


Schedule Version:       1.00                                              
Processed by SCHED version:   6.01  Release: Late March 2005              

PI:       J.M.Marcaide                                                    

Address:  Universitat de Valencia                                         
          C/ Dr. Moliner, 50                                              
          Burjassot, E 46100, Spain                                       
                                                                          

Phone:    34-96-398-3079/8 (work) or 34-96-337-1786 (home)                
EMAIL:    J.M.Marcaide@uv.es (internet)                                   
Fax:      34-96-398-3084                                                  
Phone during observation: 34-958-121311 (work) or 34-958-810928 (home)    

Observing mode: VLBA                                                      

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

 Next scan frequencies:  4966.49  4966.49  4982.49  4982.49  4998.49  4998.49
                         5014.49  5014.49
 Next BBC frequencies:    866.49   866.49   882.49   882.49   898.49   898.49
                          914.49   914.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

09 40 00  1803+784     04 47 55  19.6  -3.8 10.8      16.5     0   1  1      0  09 40 00
09 44 00  ---          04 51 55  19.6  -3.6 10.9      15.6   240   F  1   3200

09 45 45  2007+777     04 53 40  22.2  -9.7  8.8      43.6    93   1  1   3200  09 45 45
09 52 45  ---          05 00 41  21.9  -9.4  8.9      42.0   420   F  1   8800

09 54 32  1803+784     05 02 29  19.4  -3.0 11.0      13.2    97   1  1   8800  09 54 32
10 01 32  ---          05 09 30  19.4  -2.7 11.2      11.6   420   F  1  14400

10 03 17  2007+777     05 11 15  21.6  -8.9  9.1      39.6    94   1  1  14400  10 03 17
10 07 17  ---          05 15 16  21.4  -8.8  9.2      38.6   240   F  1  17600

10 15 54  M81          05 23 54  36.2  24.3 -4.5     -98.4   481   1  2  17600  10 15 54
10 19 54  ---          05 27 55  36.6  24.2 -4.5     -99.4   240   R  1  14400

10 20 16  SN1993J      05 28 18  36.6  24.3 -4.5     -99.5    18   1  2  14400  10 20 16
10 27 16  ---          05 35 19  37.3  24.1 -4.3    -101.2   420   R  1   8800

10 27 39  M81          05 35 42  37.3  24.1 -4.3    -101.3    18   1  2   8800  10 27 39
10 31 39  ---          05 39 42  37.6  24.0 -4.3    -102.3   240   R  1   5600

10 32 02  SN1993J      05 40 05  37.7  24.0 -4.3    -102.4    18   1  2   5600  10 32 02
10 39 02  ---          05 47 06  38.3  23.8 -4.1    -104.2   420   R  1      0

10 39 42  M81          05 47 46  38.3  23.8 -4.1    -104.3    35   1  3      0  10 39 42
10 43 42  ---          05 51 47  38.7  23.6 -4.1    -105.3   240   F  1   3200

10 44 04  SN1993J      05 52 09  38.7  23.7 -4.1    -105.4    18   1  3   3200  10 44 04
10 51 04  ---          05 59 11  39.3  23.5 -3.9    -107.2   420   F  1   8800

10 51 27  M81          05 59 33  39.3  23.4 -3.9    -107.3    18   1  3   8800  10 51 27
10 55 27  ---          06 03 34  39.7  23.2 -3.9    -108.3   240   F  1  12000

10 55 49  SN1993J      06 03 57  39.7  23.3 -3.9    -108.4    18   1  3  12000  10 55 49
11 02 49  ---          06 10 58  40.3  23.0 -3.7    -110.2   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

11 03 29  M81          06 11 38  40.4  22.9 -3.7    -110.4    35   1  4  17600  11 03 29
11 07 29  ---          06 15 39  40.7  22.8 -3.7    -111.5   240   R  1  14400

11 07 52  SN1993J      06 16 01  40.8  22.8 -3.7    -111.6    18   1  4  14400  11 07 52
11 14 52  ---          06 23 02  41.3  22.5 -3.5    -113.4   420   R  1   8800

11 16 08  0917+624     06 24 18  47.5  28.9 -3.0    -117.0    57   1  4   8800  11 16 08
11 20 08  ---          06 28 19  47.9  28.5 -2.9    -118.1   240   R  1   5600

11 21 22  SN1993J      06 29 33  41.9  22.2 -3.4    -115.1    56   1  4   5600  11 21 22
11 28 22  ---          06 36 34  42.4  21.8 -3.3    -117.0   420   R  1      0

11 29 02  M81          06 37 15  42.5  21.7 -3.3    -117.2    35   1  5      0  11 29 02
11 33 02  ---          06 41 15  42.8  21.5 -3.2    -118.3   240   F  1   3200

11 33 25  SN1993J      06 41 38  42.8  21.5 -3.2    -118.4    18   1  5   3200  11 33 25
11 40 25  ---          06 48 39  43.4  21.1 -3.1    -120.3   420   F  1   8800

11 40 47  M81          06 49 02  43.4  21.0 -3.1    -120.4    18   1  5   8800  11 40 47
11 44 47  ---          06 53 02  43.7  20.8 -3.0    -121.6   240   F  1  12000

11 45 10  SN1993J      06 53 25  43.7  20.8 -3.0    -121.7    18   1  5  12000  11 45 10
11 52 10  ---          07 00 26  44.3  20.3 -2.9    -123.6   420   F  1  17600

11 54 10  M81          07 02 27  44.4  20.1 -2.9    -124.2   115   1  6  17600  11 54 10
11 58 10  ---          07 06 27  44.7  19.8 -2.8    -125.3   240   R  1  14400

11 58 33  SN1993J      07 06 50  44.7  19.8 -2.8    -125.4    18   1  6  14400  11 58 33
12 05 33  ---          07 13 51  45.3  19.3 -2.7    -127.5   420   R  1   8800

12 05 55  M81          07 14 14  45.2  19.2 -2.7    -127.6    18   1  6   8800  12 05 55
12 09 55  ---          07 18 15  45.5  18.9 -2.6    -128.7   240   R  1   5600

12 10 18  SN1993J      07 18 37  45.6  18.9 -2.6    -128.8    18   1  6   5600  12 10 18
12 17 18  ---          07 25 39  46.1  18.4 -2.5    -130.9   420   R  1      0

12 17 58  M81          07 26 19  46.1  18.3 -2.5    -131.1    35   1  7      0  12 17 58
12 21 58  ---          07 30 19  46.3  17.9 -2.4    -132.3   240   F  1   3200

12 22 21  SN1993J      07 30 42  46.4  17.9 -2.4    -132.4    18   1  7   3200  12 22 21
12 29 21  ---          07 37 43  46.9  17.3 -2.3    -134.5   420   F  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

12 29 43  M81          07 38 06  46.9  17.2 -2.3    -134.6    18   1  7   8800  12 29 43
12 33 43  ---          07 42 06  47.1  16.9 -2.2    -135.8   240   F  1  12000

12 34 06  SN1993J      07 42 29  47.2  16.9 -2.2    -135.9    18   1  7  12000  12 34 06
12 41 06  ---          07 49 31  47.6  16.2 -2.1    -138.1   420   F  1  17600

12 41 46  M81          07 50 11  47.6  16.1 -2.1    -138.2    35   1  8  17600  12 41 46
12 45 46  ---          07 54 11  47.8  15.7 -2.0    -139.5   240   R  1  14400

12 46 09  SN1993J      07 54 34  47.9  15.7 -2.0    -139.6    18   1  8  14400  12 46 09
12 53 09  ---          08 01 35  48.3  14.9 -1.9    -141.8   420   R  1   8800

12 53 52  0954+658     08 02 18  50.8  18.7 -1.9    -138.4    32   1  8   8800  12 53 52
12 57 52  ---          08 06 19  51.1  18.2 -1.9    -139.7   240   R  1   5600

12 58 34  SN1993J      08 07 02  48.6  14.4 -1.8    -143.5    32   1  8   5600  12 58 34
13 05 34  ---          08 14 03  49.0  13.6 -1.7    -145.7   420   R  1      0

13 06 14  M81          08 14 43  48.9  13.5 -1.7    -145.9    35   1  9      0  13 06 14
13 10 14  ---          08 18 44  49.1  13.0 -1.6    -147.2   240   F  1   3200

13 10 37  SN1993J      08 19 07  49.2  13.0 -1.6    -147.3    18   1  9   3200  13 10 37
13 17 37  ---          08 26 08  49.5  12.2 -1.5    -149.6   420   F  1   8800

13 18 00  M81          08 26 30  49.5  12.1 -1.5    -149.7    18   1  9   8800  13 18 00
13 22 00  ---          08 30 31  49.7  11.6 -1.4    -151.0   240   F  1  12000

13 22 22  SN1993J      08 30 54  49.7  11.6 -1.4    -151.2    18   1  9  12000  13 22 22
13 29 22  ---          08 37 55  50.0  10.7 -1.3    -153.5   420   F  1  17600

13 30 02  M81          08 38 35  50.0  10.6 -1.3    -153.6    35   1 10  17600  13 30 02
13 34 02  ---          08 42 36  50.2  10.1 -1.2    -155.0   240   R  1  14400

13 34 25  SN1993J      08 42 59  50.2  10.1 -1.2    -155.1    18   1 10  14400  13 34 25
13 41 25  ---          08 50 00  50.5   9.2 -1.1    -157.5   420   R  1   8800

13 41 48  M81          08 50 22  50.5   9.1 -1.1    -157.6    18   1 10   8800  13 41 48
13 45 48  ---          08 54 23  50.6   8.6 -1.0    -158.9   240   R  1   5600

13 46 11  SN1993J      08 54 46  50.6   8.6 -1.0    -159.0    18   1 10   5600  13 46 11
13 53 11  ---          09 01 47  50.9   7.6 -0.9    -161.4   420   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

13 53 51  M81          09 02 27  50.8   7.5 -0.9    -161.6    35   1 11      0  13 53 51
13 57 51  ---          09 06 28  50.9   7.0 -0.8    -163.0   240   F  1   3200

13 58 14  SN1993J      09 06 51  51.0   6.9 -0.8    -163.1    18   1 11   3200  13 58 14
14 05 14  ---          09 13 52  51.2   6.0 -0.7    -165.5   420   F  1   8800

14 05 36  M81          09 14 14  51.1   5.9 -0.7    -165.6    17   1 11   8800  14 05 36
14 09 36  ---          09 18 15  51.2   5.4 -0.6    -167.0   240   F  1  12000

14 09 59  SN1993J      09 18 38  51.3   5.3 -0.6    -167.1    18   1 11  12000  14 09 59
14 16 59  ---          09 25 39  51.4   4.3 -0.5    -169.6   420   F  1  17600

14 18 59  M81          09 27 39  51.4   4.1 -0.5    -170.2   115   1 12  17600  14 18 59
14 22 59  ---          09 31 40  51.4   3.5 -0.4    -171.6   240   R  1  14400

14 23 22  SN1993J      09 32 03  51.5   3.4 -0.4    -171.8    18   1 12  14400  14 23 22
14 30 22  ---          09 39 04  51.6   2.4 -0.3    -174.2   420   R  1   8800

14 31 21  0917+624     09 40 03  58.3  -4.0  0.3     172.6    39   1 12   8800  14 31 21
14 35 21  ---          09 44 04  58.2  -4.9  0.4     171.0   240   R  1   5600

14 36 19  SN1993J      09 45 02  51.6   1.6 -0.2    -176.2    39   1 12   5600  14 36 19
14 43 19  ---          09 52 03  51.6   0.6 -0.1    -178.7   420   R  1      0

14 43 59  M81          09 52 43  51.6   0.5 -0.1    -178.9    35   1 13      0  14 43 59
14 47 59  ---          09 56 44  51.6  -0.1  0.0     179.8   240   F  1   3200

14 48 22  SN1993J      09 57 07  51.6  -0.2  0.0     179.6    18   1 13   3200  14 48 22
14 55 22  ---          10 04 08  51.6  -1.2  0.1     177.1   420   F  1   8800

14 55 44  M81          10 04 30  51.6  -1.2  0.1     177.1    17   1 13   8800  14 55 44
14 59 44  ---          10 08 31  51.6  -1.8  0.2     175.7   240   F  1  12000

15 00 07  SN1993J      10 08 54  51.6  -1.9  0.2     175.5    18   1 13  12000  15 00 07
15 07 07  ---          10 15 55  51.5  -2.9  0.3     173.1   420   F  1  17600

15 07 47  M81          10 16 35  51.5  -3.0  0.3     172.9    35   1 14  17600  15 07 47
15 10 47  ---          10 19 36  51.4  -3.4  0.4     171.8   180   R  1  15200

15 10 47  SN1993J      10 19 36  51.5  -3.4  0.4     171.8    -5   1 14  15200  15 10 47
15 17 47  ---          10 26 37  51.4  -4.4  0.5     169.4   415   R  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

15 17 47  4C39.25      10 26 37  75.3 -51.3  1.0     120.2   -54   1 14   9600  15 17 47
15 29 47  ---          10 38 39  73.2 -55.3  1.2     114.5   666   R  1      0

-----------  Tape Change ------------

15 44 47  M81          10 53 41  50.7  -8.1  1.0     160.2   849   2  1      0  15 44 47
15 48 47  ---          10 57 42  50.6  -8.6  1.0     158.9   240   F  1   3200

15 49 10  SN1993J      10 58 05  50.6  -8.7  1.0     158.7    18   2  1   3200  15 49 10
15 56 10  ---          11 05 06  50.4  -9.6  1.2     156.3   420   F  1   8800

15 56 50  0954+658     11 05 46  53.6 -11.5  1.1     155.5    27   2  1   8800  15 56 50
16 00 50  ---          11 09 47  53.5 -12.2  1.2     154.0   240   F  1  12000

16 01 29  SN1993J      11 10 27  50.2 -10.3  1.2     154.6    27   2  1  12000  16 01 29
16 08 29  ---          11 17 28  49.9 -11.2  1.4     152.3   420   F  1  17600

16 09 09  M81          11 18 08  49.8 -11.2  1.4     152.1    35   2  2  17600  16 09 09
16 13 09  ---          11 22 09  49.7 -11.7  1.4     150.8   240   R  1  14400

16 13 32  SN1993J      11 22 31  49.7 -11.8  1.4     150.6    18   2  2  14400  16 13 32
16 20 32  ---          11 29 33  49.4 -12.6  1.6     148.3   420   R  1   8800

16 20 54  M81          11 29 55  49.3 -12.6  1.6     148.3    17   2  2   8800  16 20 54
16 24 54  ---          11 33 55  49.1 -13.1  1.6     147.0   240   R  1   5600

16 25 17  SN1993J      11 34 18  49.1 -13.2  1.6     146.8    18   2  2   5600  16 25 17
16 32 17  ---          11 41 19  48.8 -14.0  1.8     144.6   420   R  1      0

16 32 57  M81          11 42 00  48.7 -14.0  1.8     144.4    35   2  3      0  16 32 57
16 36 57  ---          11 46 00  48.5 -14.4  1.8     143.2   240   F  1   3200

16 36 57  SN1993J      11 46 00  48.5 -14.5  1.8     143.1    -5   2  3   3200  16 36 57
16 43 57  ---          11 53 01  48.1 -15.2  2.0     140.9   415   F  1   8800

16 43 57  M81          11 53 01  48.1 -15.2  2.0     141.0    -5   2  3   8800  16 43 57
16 47 57  ---          11 57 02  47.9 -15.6  2.0     139.7   235   F  1  12000

16 47 57  SN1993J      11 57 02  47.9 -15.7  2.0     139.7    -5   2  3  12000  16 47 57
16 54 57  ---          12 04 03  47.5 -16.4  2.1     137.5   415   F  1  17600

16 55 37  M81          12 04 43  47.4 -16.4  2.1     137.4    35   2  4  17600  16 55 37
16 59 37  ---          12 08 44  47.2 -16.7  2.2     136.1   240   R  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

17 00 00  SN1993J      12 09 07  47.2 -16.8  2.2     136.0    18   2  4  14400  17 00 00
17 07 00  ---          12 16 08  46.7 -17.5  2.3     133.8   420   R  1   8800

17 07 22  M81          12 16 30  46.7 -17.5  2.3     133.8    17   2  4   8800  17 07 22
17 11 22  ---          12 20 31  46.4 -17.8  2.4     132.6   240   R  1   5600

17 11 45  SN1993J      12 20 54  46.4 -17.9  2.4     132.4    18   2  4   5600  17 11 45
17 18 45  ---          12 27 55  46.0 -18.5  2.5     130.4   420   R  1      0

17 19 25  4C39.25      12 28 35  52.3 -64.5  3.0      88.6     3   2  5      0  17 19 25
17 28 25  ---          12 37 36  50.5 -64.4  3.2      87.3   540   F  1   7200

17 28 25  M81          12 37 36  45.3 -19.2  2.7     127.6   -36   2  5   7200  17 28 25
17 33 25  ---          12 42 37  44.9 -19.6  2.8     126.2   264   F  1  11200

17 33 25  SN1993J      12 42 37  44.9 -19.7  2.8     126.1    -5   2  5  11200  17 33 25
17 41 25  ---          12 50 38  44.3 -20.3  2.9     123.8   475   F  1  17600

17 42 05  M81          12 51 19  44.3 -20.2  2.9     123.7    35   2  6  17600  17 42 05
17 46 05  ---          12 55 19  44.0 -20.5  3.0     122.6   240   R  1  14400

17 46 27  SN1993J      12 55 42  43.9 -20.6  3.0     122.4    18   2  6  14400  17 46 27
17 53 27  ---          13 02 43  43.4 -21.1  3.1     120.4   420   R  1   8800

17 54 30  0917+624     13 03 46  42.7 -31.5  3.7     105.4    50   2  6   8800  17 54 30
17 58 30  ---          13 07 46  42.3 -31.6  3.8     104.4   240   R  1   5600

17 59 32  SN1993J      13 08 48  42.9 -21.4  3.2     118.8    49   2  6   5600  17 59 32
18 06 32  ---          13 15 50  42.4 -21.8  3.3     116.9   420   R  1      0

18 07 12  M81          13 16 30  42.3 -21.8  3.3     116.8    35   2  7      0  18 07 12
18 11 12  ---          13 20 30  42.0 -22.0  3.4     115.7   240   F  1   3200

18 11 52  SN1993J      13 21 11  41.9 -22.1  3.4     115.4    35   2  7   3200  18 11 52
18 18 52  ---          13 28 12  41.4 -22.5  3.5     113.5   420   F  1   8800

18 19 32  M81          13 28 52  41.3 -22.4  3.5     113.4    35   2  7   8800  18 19 32
18 23 32  ---          13 32 52  41.0 -22.6  3.6     112.4   240   F  1  12000

18 24 12  SN1993J      13 33 33  40.9 -22.7  3.6     112.1    35   2  7  12000  18 24 12
18 31 12  ---          13 40 34  40.3 -23.0  3.7     110.3   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

18 33 12  M81          13 42 34  40.2 -23.0  3.8     109.9   114   2  8  17600  18 33 12
18 37 12  ---          13 46 35  39.8 -23.2  3.8     108.8   240   R  1  14400

18 37 34  SN1993J      13 46 57  39.8 -23.3  3.9     108.7    18   2  8  14400  18 37 34
18 44 34  ---          13 53 58  39.2 -23.5  4.0     106.9   420   R  1   8800

18 44 57  M81          13 54 21  39.2 -23.5  4.0     106.8    18   2  8   8800  18 44 57
18 48 57  ---          13 58 22  38.8 -23.6  4.0     105.8   240   R  1   5600

18 49 19  SN1993J      13 58 44  38.8 -23.7  4.0     105.6    18   2  8   5600  18 49 19
18 56 19  ---          14 05 45  38.2 -23.9  4.2     103.9   420   R  1      0

18 56 59  M81          14 06 25  38.1 -23.8  4.2     103.8    35   2  9      0  18 56 59
19 00 59  ---          14 10 26  37.8 -23.9  4.2     102.8   240   F  1   3200

19 01 21  SN1993J      14 10 48  37.7 -24.0  4.2     102.6    18   2  9   3200  19 01 21
19 08 21  ---          14 17 49  37.1 -24.2  4.4     100.9   420   F  1   8800

19 09 03  0954+658     14 18 31  38.0 -28.4  4.3      98.9    33   2  9   8800  19 09 03
19 13 03  ---          14 22 32  37.6 -28.5  4.4      98.0   240   F  1  12000

19 13 45  SN1993J      14 23 14  36.7 -24.3  4.5      99.6    33   2  9  12000  19 13 45
19 20 45  ---          14 30 15  36.0 -24.4  4.6      97.9   420   F  1  17600

19 21 25  M81          14 30 55  36.0 -24.3  4.6      97.8    35   2 10  17600  19 21 25
19 25 25  ---          14 34 56  35.6 -24.4  4.6      96.8   240   R  1  14400

19 25 47  SN1993J      14 35 18  35.6 -24.4  4.7      96.6    17   2 10  14400  19 25 47
19 32 47  ---          14 42 19  35.0 -24.5  4.8      94.9   420   R  1   8800

19 33 10  M81          14 42 42  34.9 -24.5  4.8      94.9    18   2 10   8800  19 33 10
19 37 10  ---          14 46 43  34.6 -24.5  4.8      94.0   240   R  1   5600

19 37 32  SN1993J      14 47 05  34.5 -24.6  4.9      93.8    17   2 10   5600  19 37 32
19 44 32  ---          14 54 06  33.9 -24.6  5.0      92.2   420   R  1      0

19 45 12  M81          14 54 46  33.9 -24.6  5.0      92.1    35   2 11      0  19 45 12
19 49 12  ---          14 58 47  33.5 -24.6  5.0      91.1   240   F  1   3200

19 49 52  SN1993J      14 59 27  33.4 -24.6  5.1      90.9    35   2 11   3200  19 49 52
19 56 52  ---          15 06 28  32.8 -24.6  5.2      89.3   420   F  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  22 Oct 2005   Day 295 ---

19 57 32  M81          15 07 08  32.8 -24.6  5.2      89.2    35   2 11   8800  19 57 32
20 01 32  ---          15 11 09  32.4 -24.6  5.3      88.2   240   F  1  12000

20 02 12  SN1993J      15 11 49  32.3 -24.6  5.3      88.0    35   2 11  12000  20 02 12
20 09 12  ---          15 18 50  31.7 -24.6  5.4      86.4   420   F  1  17600

20 09 52  M81          15 19 30  31.6 -24.5  5.4      86.3    35   2 12  17600  20 09 52
20 13 52  ---          15 23 31  31.3 -24.5  5.5      85.4   240   R  1  14400

20 14 32  SN1993J      15 24 11  31.2 -24.5  5.5      85.2    35   2 12  14400  20 14 32
20 21 32  ---          15 31 12  30.6 -24.5  5.6      83.6   420   R  1   8800

20 22 12  M81          15 31 52  30.5 -24.4  5.6      83.5    35   2 12   8800  20 22 12
20 26 12  ---          15 35 53  30.2 -24.4  5.7      82.6   240   R  1   5600

20 26 52  SN1993J      15 36 33  30.1 -24.4  5.7      82.4    35   2 12   5600  20 26 52
20 33 52  ---          15 43 34  29.5 -24.3  5.8      80.8   420   R  1      0

20 34 32  M81          15 44 14  29.4 -24.2  5.8      80.7    35   2 13      0  20 34 32
20 38 32  ---          15 48 15  29.1 -24.2  5.9      79.8   240   F  1   3200

20 39 12  SN1993J      15 48 55  29.0 -24.2  5.9      79.6    35   2 13   3200  20 39 12
20 46 12  ---          15 55 56  28.4 -24.1  6.0      78.0   420   F  1   8800

20 47 05  0917+624     15 56 49  23.0 -30.0  6.6      67.5    36   2 13   8800  20 47 05
20 51 05  ---          16 00 50  22.5 -29.8  6.6      66.7   240   F  1  12000

20 51 58  SN1993J      16 01 43  27.9 -23.9  6.1      76.7    36   2 13  12000  20 51 58
20 58 58  ---          16 08 44  27.3 -23.8  6.2      75.2   420   F  1  17600

20 59 38  M81          16 09 24  27.2 -23.7  6.2      75.1    35   2 14  17600  20 59 38
21 03 38  ---          16 13 25  26.9 -23.6  6.3      74.2   240   R  1  14400

21 04 18  SN1993J      16 14 05  26.8 -23.6  6.3      74.0    35   2 14  14400  21 04 18
21 11 18  ---          16 21 06  26.2 -23.4  6.4      72.4   420   R  1   8800

21 11 58  M81          16 21 46  26.2 -23.3  6.4      72.3    35   2 14   8800  21 11 58
21 15 58  ---          16 25 47  25.8 -23.2  6.5      71.4   240   R  1   5600

21 16 38  SN1993J      16 26 27  25.8 -23.2  6.5      71.2    35   2 14   5600  21 16 38
21 23 38  ---          16 33 28  25.2 -23.0  6.6      69.7   420   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: GM057A.6cm
   Matches group v6cm_2 in /instalables/SCHED/catalogs/freq.dat

   Setup group:    2         Station: VLBA_FD           Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         U         L         U         L         U         L         U
   Pol.  =      LCP       LCP       LCP       LCP       LCP       LCP       LCP       LCP 
   BBC   =         1         1         2         2         3         3         4         4
   BBC SB=         L         U         L         U         L         U         L         U
   IF    =        C         C         C         C         C         C         C         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   2  Setup file default.  Used pcal sets:   1
   LO sum=    4966.49   4966.49   4982.49   4982.49   4998.49   4998.49   5014.49   5014.49
   BBC fr=     866.49    866.49    882.49    882.49    898.49    898.49    914.49    914.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   490   490   490  6490  6490  6490  6490
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- SN1993J @ 6cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 0917+624          09 17 40.306287   * 09 21 36.230500     09 22 03.033127       0.00
                     62 28 38.63575    * 62 15 52.17600      62 14 16.77725        0.00
                     From catalog imbedded in main SCHED input file.
                        0.267 scan hours,     40.867 baseline hours above horizon.

 * 0954+658          09 54 57.847920   * 09 58 47.245100     09 59 12.957828       0.00
                     65 48 15.53881    * 65 33 54.81800      65 32 07.88745        0.00
                     From catalog imbedded in main SCHED input file.
                        0.200 scan hours,     31.800 baseline hours above horizon.

 * SN1993J           09 51 19.039486   * 09 55 24.775500     09 55 52.324213       0.00
                     69 15 26.47487    * 69 01 13.71000      68 59 26.83455        0.00
                     From catalog imbedded in main SCHED input file.
                        6.083 scan hours,    946.049 baseline hours above horizon.

 * M81               09 51 27.310854   * 09 55 33.173100     09 56 00.733820       0.00
                     69 18 08.14534    * 69 03 55.06200      69 02 08.14066        0.00
                     From catalog imbedded in main SCHED input file.
                        3.000 scan hours,    463.261 baseline hours above horizon.

 * 1803+784          18 03 39.193244   * 18 00 45.683600     18 00 22.423475       0.00
                     78 27 54.30008    * 78 28 04.02100      78 28 12.71449        0.00
                     From catalog imbedded in main SCHED input file.
                        0.183 scan hours,     28.050 baseline hours above horizon.

 * 2007+777          20 07 20.430477   * 20 05 30.998800     20 05 16.642792       0.00
                     77 43 58.12445    * 77 52 43.24900      77 53 55.42065        0.00
                     From catalog imbedded in main SCHED input file.
                        0.183 scan hours,     24.933 baseline hours above horizon.

 * 4C39.25           09 23 55.319212   * 09 27 03.013933     09 27 24.218322       0.00
                     39 15 23.56648    * 39 02 20.85188      39 00 50.58409        0.00
                     From catalog imbedded in main SCHED input file.
                        0.350 scan hours,     30.623 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0917+624            89.6
   0954+658            87.6
   SN1993J             89.8
   M81                 89.9
   1803+784            95.8
   2007+777           101.8
   4C39.25             78.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

