  COVER INFORMATION 
 
 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1993J @ 6cm
 Exp. Code:  gm035f  

 
Schedule Version:       2.00                                              
Processed by SCHED version: Release of 28 April 2000                      
 
PI:       J.M.Marcaide                                                    
 
Address:  Universitat de Valencia                                         
          C/ Dr. Moliner, 50                                              
          Burjassot, E 46100, Spain                                       
                                                                          
 
Phone:    34-96-398-3079/8 (work) or 34-96-337-1786 (home)                
EMAIL:    jmm@vlbi.uv.es (internet)                                       
Fax:      34-96-398-3084                                                  
Phone during observation: 34-958-121311 (work) or 34-958-810928 (home)    
 
Observing mode: VLBA                                                      
 
Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
 Next scan frequencies:  4966.49  4966.49  4982.49  4982.49  4998.49  4998.49
                         5014.49  5014.49
 Next BBC frequencies:    866.49   866.49   882.49   882.49   898.49   898.49
                          914.49   914.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00
  
13 48 00  3C48         23 53 21  67.8  76.6 -1.7     -89.4     0   1  1      0  13 48 00
13 50 00  ---          23 55 21  68.2  76.6 -1.7     -89.7   120   F  1   1600
  
13 51 00  1803+784     23 56 21  30.2 -13.4  5.9      84.3   -18   1  1   1600  13 51 00
13 54 00  ---          23 59 22  30.0 -13.4  6.0      83.6   162   F  1   4000
  
13 55 00  2007+777     00 00 22  36.3 -12.9  3.9     114.2    45   1  1   4000  13 55 00
13 58 00  ---          00 03 22  36.2 -12.9  4.0     113.4   180   F  1   6400
  
13 59 00  1803+784     00 04 23  29.8 -13.3  6.1      82.4    45   1  1   6400  13 59 00
14 04 00  ---          00 09 23  29.5 -13.3  6.1      81.2   300   F  1  10400
  
14 05 00  2007+777     00 10 24  35.8 -13.1  4.1     111.6    45   1  1  10400  14 05 00
14 08 00  ---          00 13 24  35.7 -13.2  4.1     110.8   180   F  1  12800
  
14 14 00  3C48         00 19 25  73.2  76.2 -1.3     -93.3   283   1  1  12800  14 14 00
14 20 00  ---          00 25 26  74.5  75.9 -1.2     -94.5   360   F  1  17600
  
14 21 00  M81          00 26 26  13.5  13.0 -9.5     -32.8   -64   1  2  17600  14 21 00
14 25 00  ---          00 30 27  13.7  13.3 -9.4     -33.6   176   R  1  14400
  
14 26 00  SN1993J      00 31 27  13.7  13.4 -9.4     -33.9    58   1  2  14400  14 26 00
14 32 00  ---          00 37 28  14.0  13.9 -9.3     -35.2   360   R  1   9600
  
14 33 00  M81          00 38 28  14.1  13.9 -9.3     -35.4    58   1  2   9600  14 33 00
14 36 00  ---          00 41 29  14.2  14.1 -9.2     -36.0   180   R  1   7200
  
14 37 00  SN1993J      00 42 29  14.2  14.2 -9.2     -36.3    58   1  2   7200  14 37 00
14 43 00  ---          00 48 30  14.6  14.7 -9.1     -37.5   360   R  1   2400
  
14 45 00  0917+624     00 50 30  11.9  22.1 -8.5     -44.0   113   1  2   2400  14 45 00
14 48 00  ---          00 53 31  12.1  22.3 -8.5     -44.6   180   R  1      0
  
14 52 00  SN1993J      00 57 31  15.1  15.3 -9.0     -39.5   232   1  3      0  14 52 00
14 57 00  ---          01 02 32  15.4  15.7 -8.9     -40.6   300   F  1   4000
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
14 58 00  M81          01 03 32  15.4  15.7 -8.9     -40.8    58   1  3   4000  14 58 00
15 01 00  ---          01 06 33  15.6  15.9 -8.8     -41.4   180   F  1   6400
  
15 02 00  SN1993J      01 07 33  15.7  16.0 -8.8     -41.6    58   1  3   6400  15 02 00
15 07 00  ---          01 12 34  16.0  16.4 -8.7     -42.7   300   F  1  10400
  
15 08 00  M81          01 13 34  16.0  16.4 -8.7     -42.9    58   1  3  10400  15 08 00
15 11 00  ---          01 16 34  16.2  16.6 -8.6     -43.6   180   F  1  12800
  
15 12 00  SN1993J      01 17 35  16.3  16.7 -8.6     -43.8    58   1  3  12800  15 12 00
15 18 00  ---          01 23 36  16.6  17.1 -8.5     -45.1   360   F  1  17600
  
15 19 00  M81          01 24 36  16.7  17.2 -8.5     -45.3    58   1  4  17600  15 19 00
15 23 00  ---          01 28 36  17.0  17.4 -8.4     -46.1   240   R  1  14400
  
15 24 00  SN1993J      01 29 36  17.0  17.5 -8.4     -46.4    58   1  4  14400  15 24 00
15 30 00  ---          01 35 37  17.4  17.9 -8.3     -47.7   360   R  1   9600
  
15 31 00  M81          01 36 38  17.5  17.9 -8.3     -47.9    58   1  4   9600  15 31 00
15 34 00  ---          01 39 38  17.7  18.1 -8.3     -48.5   180   R  1   7200
  
15 35 00  SN1993J      01 40 38  17.8  18.2 -8.2     -48.7    58   1  4   7200  15 35 00
15 41 00  ---          01 46 39  18.2  18.6 -8.1     -50.0   360   R  1   2400
  
15 43 00  M81          01 48 40  18.3  18.7 -8.1     -50.4   118   1  4   2400  15 43 00
15 46 00  ---          01 51 40  18.5  18.8 -8.1     -51.1   180   R  1      0
  
15 47 00  SN1993J      01 52 40  18.6  19.0 -8.0     -51.3    58   1  5      0  15 47 00
15 53 00  ---          01 58 41  19.0  19.3 -7.9     -52.6   360   F  1   4800
  
15 54 00  0917+624     01 59 41  18.1  27.3 -7.4     -58.0    53   1  5   4800  15 54 00
15 57 00  ---          02 02 42  18.4  27.5 -7.3     -58.6   180   F  1   7200
  
16 01 00  SN1993J      02 06 43  19.6  19.8 -7.8     -54.3   233   1  5   7200  16 01 00
16 06 00  ---          02 11 43  19.9  20.0 -7.7     -55.4   300   F  1  11200
  
16 07 00  M81          02 12 44  20.0  20.0 -7.7     -55.6    58   1  5  11200  16 07 00
16 10 00  ---          02 15 44  20.3  20.2 -7.7     -56.3   180   F  1  13600
  
16 11 00  SN1993J      02 16 44  20.3  20.3 -7.6     -56.5    58   1  5  13600  16 11 00
16 16 00  ---          02 21 45  20.7  20.6 -7.6     -57.6   300   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
16 17 00  M81          02 22 45  20.8  20.6 -7.5     -57.8    58   1  6  17600  16 17 00
16 20 00  ---          02 25 46  21.0  20.7 -7.5     -58.4   180   R  1  15200
  
16 21 00  SN1993J      02 26 46  21.1  20.8 -7.5     -58.7    58   1  6  15200  16 21 00
16 27 00  ---          02 32 47  21.5  21.1 -7.4     -60.0   360   R  1  10400
  
16 28 00  M81          02 33 47  21.6  21.1 -7.4     -60.2    58   1  6  10400  16 28 00
16 32 00  ---          02 37 48  21.9  21.3 -7.3     -61.0   240   R  1   7200
  
16 33 00  SN1993J      02 38 48  22.0  21.4 -7.3     -61.2    58   1  6   7200  16 33 00
16 39 00  ---          02 44 49  22.5  21.7 -7.2     -62.5   360   R  1   2400
  
16 41 00  M81          02 46 49  22.7  21.7 -7.1     -63.0   118   1  6   2400  16 41 00
16 44 00  ---          02 49 50  22.9  21.8 -7.1     -63.6   180   R  1      0
  
16 45 00  SN1993J      02 50 50  23.0  21.9 -7.1     -63.9    58   1  7      0  16 45 00
16 51 00  ---          02 56 51  23.5  22.2 -7.0     -65.2   360   F  1   4800
  
16 52 00  0917+624     02 57 51  24.2  30.5 -6.4     -69.7    52   1  7   4800  16 52 00
16 55 00  ---          03 00 51  24.5  30.6 -6.3     -70.4   180   F  1   7200
  
16 59 00  SN1993J      03 04 52  24.1  22.5 -6.8     -66.9   233   1  7   7200  16 59 00
17 04 00  ---          03 09 53  24.5  22.7 -6.8     -68.0   300   F  1  11200
  
17 05 00  M81          03 10 53  24.6  22.7 -6.7     -68.2    58   1  7  11200  17 05 00
17 08 00  ---          03 13 54  24.9  22.8 -6.7     -68.9   180   F  1  13600
  
17 09 00  SN1993J      03 14 54  24.9  22.9 -6.7     -69.1    58   1  7  13600  17 09 00
17 14 00  ---          03 19 55  25.4  23.0 -6.6     -70.2   300   F  1  17600
  
17 15 00  M81          03 20 55  25.4  23.0 -6.6     -70.4    58   1  8  17600  17 15 00
17 18 00  ---          03 23 55  25.7  23.1 -6.5     -71.1   180   R  1  15200
  
17 19 00  SN1993J      03 24 55  25.8  23.2 -6.5     -71.3    58   1  8  15200  17 19 00
17 25 00  ---          03 30 56  26.3  23.4 -6.4     -72.6   360   R  1  10400
  
17 26 00  M81          03 31 57  26.4  23.4 -6.4     -72.8    58   1  8  10400  17 26 00
17 30 00  ---          03 35 57  26.7  23.5 -6.3     -73.7   240   R  1   7200
  
17 31 00  SN1993J      03 36 57  26.8  23.6 -6.3     -73.9    58   1  8   7200  17 31 00
17 37 00  ---          03 42 58  27.3  23.7 -6.2     -75.3   360   R  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
17 39 00  M81          03 44 59  27.5  23.7 -6.2     -75.7   118   1  8   2400  17 39 00
17 42 00  ---          03 47 59  27.8  23.8 -6.1     -76.4   180   R  1      0
  
17 43 00  SN1993J      03 48 59  27.9  23.9 -6.1     -76.6    58   1  9      0  17 43 00
17 49 00  ---          03 55 00  28.4  24.0 -6.0     -77.9   360   F  1   4800
  
17 50 00  0917+624     03 56 00  30.7  32.4 -5.4     -81.8    52   1  9   4800  17 50 00
17 53 00  ---          03 59 01  31.1  32.4 -5.4     -82.4   180   F  1   7200
  
17 57 00  SN1993J      04 03 02  29.1  24.2 -5.9     -79.7   232   1  9   7200  17 57 00
18 02 00  ---          04 08 02  29.5  24.3 -5.8     -80.9   300   F  1  11200
  
18 03 00  M81          04 09 03  29.6  24.2 -5.8     -81.1    58   1  9  11200  18 03 00
18 06 00  ---          04 12 03  29.9  24.3 -5.7     -81.8   180   F  1  13600
  
18 07 00  SN1993J      04 13 03  30.0  24.3 -5.7     -82.0    58   1  9  13600  18 07 00
18 12 00  ---          04 18 04  30.4  24.4 -5.6     -83.1   300   F  1  17600
  
18 13 00  M81          04 19 04  30.5  24.4 -5.6     -83.4    58   1 10  17600  18 13 00
18 16 00  ---          04 22 05  30.8  24.4 -5.6     -84.0   180   R  1  15200
  
18 17 00  SN1993J      04 23 05  30.9  24.5 -5.5     -84.3    58   1 10  15200  18 17 00
18 23 00  ---          04 29 06  31.4  24.5 -5.4     -85.7   360   R  1  10400
  
18 24 00  M81          04 30 06  31.5  24.5 -5.4     -85.9    58   1 10  10400  18 24 00
18 28 00  ---          04 34 07  31.8  24.5 -5.4     -86.8   240   R  1   7200
  
18 29 00  SN1993J      04 35 07  31.9  24.6 -5.3     -87.0    58   1 10   7200  18 29 00
18 35 00  ---          04 41 08  32.5  24.6 -5.2     -88.4   360   R  1   2400
  
18 37 00  M81          04 43 08  32.6  24.5 -5.2     -88.9   118   1 10   2400  18 37 00
18 40 00  ---          04 46 09  32.9  24.5 -5.2     -89.6   180   R  1      0
  
18 41 00  SN1993J      04 47 09  33.0  24.6 -5.1     -89.8    58   1 11      0  18 41 00
18 47 00  ---          04 53 10  33.5  24.6 -5.0     -91.2   360   F  1   4800
  
18 48 00  0917+624     04 54 10  37.5  32.6 -4.5     -94.5    50   1 11   4800  18 48 00
18 51 00  ---          04 57 11  37.8  32.6 -4.4     -95.2   180   F  1   7200
  
18 55 00  SN1993J      05 01 11  34.3  24.5 -4.9     -93.1   231   1 11   7200  18 55 00
19 00 00  ---          05 06 12  34.7  24.5 -4.8     -94.3   300   F  1  11200
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
19 01 00  M81          05 07 12  34.8  24.4 -4.8     -94.6    58   1 11  11200  19 01 00
19 04 00  ---          05 10 13  35.1  24.4 -4.8     -95.3   180   F  1  13600
  
19 05 00  SN1993J      05 11 13  35.2  24.5 -4.7     -95.5    58   1 11  13600  19 05 00
19 10 00  ---          05 16 14  35.6  24.4 -4.7     -96.7   300   F  1  17600
  
19 11 00  M81          05 17 14  35.7  24.3 -4.6     -97.0    58   1 12  17600  19 11 00
19 15 00  ---          05 21 14  36.0  24.3 -4.6     -97.9   240   R  1  14400
  
19 16 00  SN1993J      05 22 15  36.1  24.3 -4.6     -98.2    58   1 12  14400  19 16 00
19 22 00  ---          05 28 16  36.7  24.2 -4.5     -99.6   360   R  1   9600
  
19 23 00  M81          05 29 16  36.7  24.1 -4.4     -99.9    58   1 12   9600  19 23 00
19 26 00  ---          05 32 16  37.0  24.1 -4.4    -100.6   180   R  1   7200
  
19 27 00  SN1993J      05 33 16  37.1  24.1 -4.4    -100.9    58   1 12   7200  19 27 00
19 33 00  ---          05 39 17  37.6  24.0 -4.3    -102.4   360   R  1   2400
  
19 35 00  0917+624     05 41 18  42.9  31.4 -3.7    -105.7   108   1 12   2400  19 35 00
19 38 00  ---          05 44 18  43.2  31.2 -3.6    -106.5   180   R  1      0
  
19 39 00  SN1993J      05 45 18  38.2  23.8 -4.2    -103.9    48   1 13      0  19 39 00
19 44 00  ---          05 50 19  38.6  23.7 -4.1    -105.1   300   F  1   4000
  
19 45 00  M81          05 51 19  38.7  23.6 -4.1    -105.4    58   1 13   4000  19 45 00
19 48 00  ---          05 54 20  38.9  23.5 -4.0    -106.1   180   F  1   6400
  
19 49 00  SN1993J      05 55 20  39.0  23.5 -4.0    -106.4    58   1 13   6400  19 49 00
19 54 00  ---          06 00 21  39.5  23.4 -3.9    -107.7   300   F  1  10400
  
19 55 00  M81          06 01 21  39.5  23.3 -3.9    -107.9    58   1 13  10400  19 55 00
19 58 00  ---          06 04 22  39.8  23.2 -3.9    -108.7   180   F  1  12800
  
19 59 00  SN1993J      06 05 22  39.9  23.2 -3.8    -108.9    58   1 13  12800  19 59 00
20 05 00  ---          06 11 23  40.4  22.9 -3.7    -110.5   360   F  1  17600
  
20 06 00  M81          06 12 23  40.4  22.8 -3.7    -110.8    58   1 14  17600  20 06 00
20 10 00  ---          06 16 23  40.8  22.7 -3.7    -111.8   240   R  1  14400
  
20 10 00  SN1993J      06 16 23  40.8  22.7 -3.7    -111.8    -2   1 14  14400  20 10 00
20 16 00  ---          06 22 24  41.3  22.4 -3.5    -113.4   358   R  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
20 16 00  M81          06 22 24  41.3  22.4 -3.6    -113.4    -2   1 14   9600  20 16 00
20 19 00  ---          06 25 25  41.5  22.3 -3.5    -114.2   178   R  1   7200
  
20 19 00  SN1993J      06 25 25  41.6  22.3 -3.5    -114.2    -2   1 14   7200  20 19 00
20 25 00  ---          06 31 26  42.0  22.0 -3.4    -115.8   358   R  1   2400
  
20 25 00  0917+624     06 31 26  48.3  28.2 -2.8    -119.1   -14   1 14   2400  20 25 00
20 28 00  ---          06 34 26  48.6  27.9 -2.8    -120.0   166   R  1      0
  
-----------  Tape Change ------------
  
20 43 00  0917+624     06 49 29  50.0  26.5 -2.5    -124.4   895   2  1      0  20 43 00
20 47 00  ---          06 53 30  50.4  26.1 -2.5    -125.6   240   F  1   3200
  
20 48 00  2007+777     06 54 30  19.0  -3.9 10.8      16.1    -5   2  1   3200  20 48 00
20 52 00  ---          06 58 30  19.0  -3.7 10.9      15.2   235   F  1   6400
  
20 53 00  1803+784     06 59 31  19.4   3.1-11.0     -13.4    53   2  1   6400  20 53 00
20 58 00  ---          07 04 31  19.5   3.3-10.9     -14.5   300   F  1  10400
  
21 03 00  M81          07 09 32  44.9  19.5 -2.8    -126.4   247   2  1  10400  21 03 00
21 06 00  ---          07 12 33  45.1  19.3 -2.7    -127.2   180   F  1  12800
  
21 07 00  SN1993J      07 13 33  45.2  19.3 -2.7    -127.5    58   2  1  12800  21 07 00
21 13 00  ---          07 19 34  45.7  18.8 -2.6    -129.3   360   F  1  17600
  
21 14 00  M81          07 20 34  45.7  18.7 -2.6    -129.6    58   2  2  17600  21 14 00
21 18 00  ---          07 24 35  46.0  18.3 -2.5    -130.7   240   R  1  14400
  
21 19 00  SN1993J      07 25 35  46.1  18.3 -2.5    -131.0    58   2  2  14400  21 19 00
21 25 00  ---          07 31 36  46.5  17.8 -2.4    -132.8   360   R  1   9600
  
21 26 00  M81          07 32 36  46.5  17.6 -2.4    -133.1    58   2  2   9600  21 26 00
21 29 00  ---          07 35 36  46.7  17.4 -2.3    -134.0   180   R  1   7200
  
21 30 00  SN1993J      07 36 37  46.8  17.3 -2.3    -134.3    58   2  2   7200  21 30 00
21 36 00  ---          07 42 38  47.2  16.8 -2.2    -136.1   360   R  1   2400
  
21 38 00  0917+624     07 44 38  54.7  19.3 -1.6    -142.3   103   2  2   2400  21 38 00
21 41 00  ---          07 47 38  54.9  18.8 -1.6    -143.4   180   R  1      0
  
21 45 00  SN1993J      07 51 39  47.7  15.9 -2.1    -138.9   224   2  3      0  21 45 00
21 50 00  ---          07 56 40  48.0  15.4 -2.0    -140.4   300   F  1   4000
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
21 51 00  M81          07 57 40  48.0  15.2 -2.0    -140.7    58   2  3   4000  21 51 00
21 54 00  ---          08 00 41  48.2  14.9 -1.9    -141.7   180   F  1   6400
  
21 55 00  SN1993J      08 01 41  48.3  14.8 -1.9    -142.0    58   2  3   6400  21 55 00
22 00 00  ---          08 06 42  48.6  14.3 -1.8    -143.6   300   F  1  10400
  
22 01 00  M81          08 07 42  48.6  14.2 -1.8    -143.9    58   2  3  10400  22 01 00
22 04 00  ---          08 10 42  48.7  13.8 -1.7    -144.8   180   F  1  12800
  
22 05 00  SN1993J      08 11 42  48.8  13.8 -1.7    -145.2    58   2  3  12800  22 05 00
22 11 00  ---          08 17 43  49.1  13.1 -1.6    -147.1   360   F  1  17600
  
22 12 00  M81          08 18 44  49.1  12.9 -1.6    -147.4    58   2  4  17600  22 12 00
22 16 00  ---          08 22 44  49.3  12.5 -1.5    -148.7   240   R  1  14400
  
22 17 00  SN1993J      08 23 44  49.4  12.4 -1.5    -149.0    58   2  4  14400  22 17 00
22 23 00  ---          08 29 45  49.7  11.7 -1.4    -151.0   360   R  1   9600
  
22 24 00  M81          08 30 45  49.7  11.5 -1.4    -151.3    58   2  4   9600  22 24 00
22 27 00  ---          08 33 46  49.8  11.1 -1.4    -152.2   180   R  1   7200
  
22 28 00  SN1993J      08 34 46  49.9  11.0 -1.3    -152.6    58   2  4   7200  22 28 00
22 34 00  ---          08 40 47  50.1  10.3 -1.2    -154.6   360   R  1   2400
  
22 36 00  0917+624     08 42 47  57.7   8.4  -.6    -164.2   103   2  4   2400  22 36 00
22 39 00  ---          08 45 48  57.8   7.8  -.6    -165.4   180   R  1      0
  
22 43 00  SN1993J      08 49 49  50.5   9.1 -1.1    -157.6   223   2  5      0  22 43 00
22 48 00  ---          08 54 49  50.6   8.5 -1.0    -159.2   300   F  1   4000
  
22 49 00  M81          08 55 50  50.6   8.3 -1.0    -159.6    58   2  5   4000  22 49 00
22 52 00  ---          08 58 50  50.7   7.9  -.9    -160.6   180   F  1   6400
  
22 53 00  SN1993J      08 59 50  50.8   7.8  -.9    -160.9    58   2  5   6400  22 53 00
22 58 00  ---          09 04 51  50.9   7.1  -.8    -162.6   300   F  1  10400
  
22 59 00  M81          09 05 51  50.9   7.0  -.8    -162.9    58   2  5  10400  22 59 00
23 02 00  ---          09 08 52  51.0   6.6  -.8    -164.0   180   F  1  12800
  
23 03 00  SN1993J      09 09 52  51.1   6.5  -.8    -164.3    58   2  5  12800  23 03 00
23 09 00  ---          09 15 53  51.2   5.6  -.7    -166.4   360   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Tue   6 Jun 2000   Day 158 ---
  
23 10 00  M81          09 16 53  51.2   5.5  -.6    -166.7    58   2  6  17600  23 10 00
23 14 00  ---          09 20 54  51.2   4.9  -.6    -168.1   240   R  1  14400
  
23 15 00  SN1993J      09 21 54  51.3   4.8  -.6    -168.4    58   2  6  14400  23 15 00
23 21 00  ---          09 27 55  51.4   3.9  -.5    -170.5   360   R  1   9600
  
23 22 00  M81          09 28 55  51.4   3.8  -.4    -170.8    58   2  6   9600  23 22 00
23 25 00  ---          09 31 56  51.4   3.4  -.4    -171.8   180   R  1   7200
  
23 26 00  SN1993J      09 32 56  51.5   3.2  -.4    -172.2    58   2  6   7200  23 26 00
23 32 00  ---          09 38 57  51.5   2.4  -.3    -174.3   360   R  1   2400
  
23 34 00  0917+624     09 40 57  58.2  -4.3   .3     172.1   105   2  6   2400  23 34 00
23 37 00  ---          09 43 57  58.2  -4.9   .4     170.9   180   R  1      0
  
23 41 00  SN1993J      09 47 58  51.6   1.1  -.1    -177.4   225   2  7      0  23 41 00
23 46 00  ---          09 52 59  51.6    .3   .0    -179.2   300   F  1   4000
  
23 47 00  M81          09 53 59  51.6    .2   .0    -179.5    58   2  7   4000  23 47 00
23 50 00  ---          09 57 00  51.6   -.2   .0     179.5   180   F  1   6400
  
23 51 00  SN1993J      09 58 00  51.6   -.4   .0     179.1    58   2  7   6400  23 51 00
23 56 00  ---          10 03 01  51.6  -1.1   .1     177.4   300   F  1  10400
  
 --- Wed   7 Jun 2000   Day 159 ---
  
00 01 00  3C286        10 08 01  46.7  76.6 -3.4     -76.3   246   2  7  10400  00 01 00
00 04 00  ---          10 11 02  47.3  76.8 -3.3     -76.5   180   F  1  12800
  
00 05 00  1803+784     10 12 02  24.9  11.3 -7.8     -57.5    13   2  7  12800  00 05 00
00 08 00  ---          10 15 03  25.0  11.4 -7.8     -58.2   180   F  1  15200
  
00 10 00  2007+777     10 17 03  20.3   7.0 -9.8     -29.8   109   2  7  15200  00 10 00
00 13 00  ---          10 20 03  20.3   7.1 -9.8     -30.5   180   F  1  17600
 
 
SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.
 
 
 Setup file: gm35f.6cm
   Matches group v6cm_2 in /homes/ros/vlbi/sched/catalogs/freq.dat
 
   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00
 
   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00
 
   1st LO=  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00
   Net SB=        L        U        L        U        L        U        L        U
   Pol.  =     LCP      LCP      LCP      LCP      LCP      LCP      LCP      LCP 
   BBC   =        1        1        2        2        3        3        4        4
   BBC SB=        L        U        L        U        L        U        L        U
   IF    =       C        C        C        C        C        C        C        C 
 
   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4
 
  The following frequency sets based on this setup were used.
 
   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=   4966.49  4966.49  4982.49  4982.49  4998.49  4998.49  5014.49  5014.49
   BBC fr=    866.49   866.49   882.49   882.49   898.49   898.49   914.49   914.49
   Bandwd=     8.000    8.000    8.000    8.000    8.000    8.000    8.000    8.000
 
  The following pulse cal sets were used with this setup:
 
   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   490   490   490  6490  6490  6490  6490
    PCALFR2=   510   510   510   510  6510  6510  6510  6510
 
   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- SN1993J @ 6cm
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
  
   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 
  
 * 0917+624          09 17 40.306287   * 09 21 36.230500     09 21 35.043359   
                     62 28 38.63575    * 62 15 52.17600      62 16 02.43841    
                     From catalog imbedded in main SCHED input file.
 
 * SN1993J           09 51 19.039486   * 09 55 24.775500     09 55 23.499778   
                     69 15 26.47487    * 69 01 13.71000      69 01 26.46182    
                     From catalog imbedded in main SCHED input file.
 
 * M81               09 51 27.310854   * 09 55 33.173100     09 55 31.895608   
                     69 18 08.14534    * 69 03 55.06200      69 04 07.82584    
                     From catalog imbedded in main SCHED input file.
 
 * 1803+784          18 03 39.193244   * 18 00 45.683600     18 00 51.804473   
                     78 27 54.30008    * 78 28 04.02100      78 28 03.69944    
                     From catalog imbedded in main SCHED input file.
 
 * 2007+777          20 07 20.430477   * 20 05 30.998800     20 05 36.031242   
                     77 43 58.12445    * 77 52 43.24900      77 52 34.20481    
                     From catalog imbedded in main SCHED input file.
 
 * 3C48              01 34 49.826399   * 01 37 41.299465     01 37 40.905090   
                     32 54 20.26003    * 33 09 35.13422      33 09 24.97956    
                     From catalog imbedded in main SCHED input file.
 
 * 3C286             13 28 49.657781   * 13 31 08.288074     13 31 09.355518   
                     30 45 58.64118    * 30 30 32.95982      30 30 39.14468    
                     From catalog imbedded in main SCHED input file.
 
 
 
  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0917+624            58.5
   SN1993J             63.0
   M81                 63.0
   1803+784            78.4
   2007+777            75.9
   3C48                45.6
   3C286              106.8
 
  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

