  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Exploring the jets of a new microquasar
 Exp. Code:  gr021b  


Schedule Version:       2.00                                              
Processed by SCHED version: Release of 28 April 2000                      

PI:       Marc Ribo                                                       

Address:  Departament Astronomia i Meteorologia                           
          Facultat de Fisica (UB)                                         
          Av. Diagonal, 647                                               
          E-08028 Barcelona, SPAIN                                        

Phone:    +34-93-402-11-22                                                
EMAIL:    Internet: mribo@am.ub.es                                        
Fax:      +34-93-402-11-33                                                
Phone during observation: +34-93-302-17-43                                

Observing mode: v6cm-256-8-2-L VLBA/MKIV (modified for Hh)                

Notes:    Target source LS5039/J1826-14.   Phase-reference J1825-17       
          Phase-references or checks             J1837-15, J1911-20       
          Fringe-finder                              3C345/J1642+39       
          MERLIN compact calibrator               2134+004/J2136+00       

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

 Next scan frequencies:  4960.49  4968.49  4976.49  4984.49  4992.49  5000.49
                         5008.49  5016.49
 Next BBC frequencies:    860.49   868.49   876.49   884.49   892.49   900.49
                          908.49   916.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

02 59 08  LS5039       13 10 35   1.7 108.4 -5.3  D  -57.6     0   1  1      0  02 59 08
03 01 58  ---          13 13 26   2.3 108.7 -5.2  H  -57.5     0   F  1   2267

03 03 28  LS5039       13 14 56   2.6 108.9 -5.2  H  -57.3    87   1  1   2267  03 03 28
03 06 18  ---          13 17 46   3.1 109.3 -5.1  H  -57.1     0   F  1   4533

03 07 48  LS5039       13 19 17   3.4 109.5 -5.1     -57.0    87   1  1   4533  03 07 48
03 10 38  ---          13 22 07   4.0 109.9 -5.1     -56.8   170   F  1   6800

03 10 38  J1825-17     13 22 07   2.8 112.0 -5.1     -56.7    -4   1  1   6800  03 10 38
03 12 08  ---          13 23 37   3.1 112.2 -5.0     -56.5    86   F  1   8000

03 17 08  J1825-17     13 28 38   4.1 112.9 -5.0     -56.1   296   1  1   8000  03 17 08
03 18 38  ---          13 30 08   4.4 113.1 -4.9     -56.0    90   F  1   9200

03 18 38  LS5039       13 30 08   5.6 111.0 -4.9     -56.2    -4   1  1   9200  03 18 38
03 21 38  ---          13 33 09   6.2 111.4 -4.9     -56.0   176   F  1  11600

03 21 38  J1825-17     13 33 09   5.0 113.5 -4.9     -55.7    -5   1  1  11600  03 21 38
03 23 08  ---          13 34 39   5.3 113.7 -4.8     -55.6    85   F  1  12800

03 23 08  LS5039       13 34 39   6.5 111.6 -4.9     -55.9    -5   1  1  12800  03 23 08
03 25 58  ---          13 37 30   7.1 112.0 -4.8     -55.6   165   F  1  15067

03 25 58  J1825-17     13 37 30   5.8 114.1 -4.8     -55.4    -5   1  1  15067  03 25 58
03 27 28  ---          13 39 00   6.1 114.3 -4.8     -55.2    85   F  1  16267

03 27 28  LS5039       13 39 00   7.4 112.2 -4.8     -55.5    -5   1  2  16267  03 27 28
03 30 18  ---          13 41 50   8.0 112.6 -4.7     -55.3   165   R  1  16667

03 30 18  J1825-17     13 41 50   6.7 114.7 -4.7     -55.0    -5   1  2  16667  03 30 18
03 31 48  ---          13 43 21   7.0 114.9 -4.7     -54.8    85   R  1  15467

03 31 48  LS5039       13 43 21   8.3 112.8 -4.7     -55.2    -5   1  2  15467  03 31 48
03 34 38  ---          13 46 11   8.8 113.2 -4.7     -54.9   165   R  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

03 34 38  J1825-17     13 46 11   7.5 115.3 -4.7     -54.6    -5   1  2  13200  03 34 38
03 36 08  ---          13 47 41   7.8 115.5 -4.6     -54.4    85   R  1  12000

03 36 08  J1837-15     13 47 41   6.5 112.4 -4.8     -55.7    -5   1  2  12000  03 36 08
03 37 38  ---          13 49 12   6.8 112.6 -4.8     -55.5    85   R  1  10800

03 40 04  J1825-17     13 51 38   8.6 116.1 -4.6     -54.1   141   1  2  10800  03 40 04
03 41 34  ---          13 53 09   8.9 116.3 -4.5     -53.9    90   R  1   9600

03 41 34  LS5039       13 53 09  10.2 114.2 -4.6     -54.3    -5   1  2   9600  03 41 34
03 44 34  ---          13 56 09  10.8 114.6 -4.5     -54.0   175   R  1   7200

03 44 34  J1825-17     13 56 09   9.5 116.7 -4.5     -53.6    -5   1  2   7200  03 44 34
03 46 04  ---          13 57 39   9.8 116.9 -4.5     -53.5    85   R  1   6000

03 46 04  LS5039       13 57 39  11.1 114.8 -4.5     -53.9    -5   1  2   6000  03 46 04
03 49 04  ---          14 00 40  11.7 115.2 -4.4     -53.6   175   R  1   3600

03 49 04  J1825-17     14 00 40  10.3 117.4 -4.4     -53.2    -5   1  2   3600  03 49 04
03 50 34  ---          14 02 10  10.6 117.6 -4.4     -53.0    85   R  1   2400

03 50 34  J1837-15     14 02 10   9.3 114.4 -4.6     -54.4    -5   1  2   2400  03 50 34
03 52 04  ---          14 03 40   9.6 114.6 -4.6     -54.3    85   R  1   1200

04 02 30  J1825-17     14 14 08  12.9 119.4 -4.2     -51.8   617   1  3   1200  04 02 30
04 05 30  ---          14 17 08  13.4 119.8 -4.1     -51.4   180   F  1   1200

04 05 30  LS5039       14 17 08  14.8 117.7 -4.2     -52.0    -5   1  3   1200  04 05 30
04 08 30  ---          14 20 09  15.4 118.2 -4.1     -51.7   175   F  1   3600

04 08 30  J1825-17     14 20 09  14.0 120.3 -4.1     -51.1    -5   1  3   3600  04 08 30
04 10 00  ---          14 21 39  14.3 120.5 -4.1     -50.9    85   F  1   4800

04 10 00  LS5039       14 21 39  15.7 118.4 -4.1     -51.5    -5   1  3   4800  04 10 00
04 13 30  ---          14 25 09  16.4 119.0 -4.0     -51.2   205   F  1   7600

04 13 30  J1825-17     14 25 09  14.9 121.1 -4.0     -50.5    -5   1  3   7600  04 13 30
04 15 00  ---          14 26 40  15.2 121.3 -4.0     -50.4    85   F  1   8800

04 15 00  J1837-15     14 26 40  14.1 118.0 -4.2     -52.1    -4   1  3   8800  04 15 00
04 16 30  ---          14 28 10  14.4 118.2 -4.2     -51.9    86   F  1  10000
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

04 16 30  J1911-20     14 28 10   5.2 117.1 -4.7     -54.7   -20   1  3  10000  04 16 30
04 18 00  ---          14 29 40   5.5 117.3 -4.7     -54.5    70   F  1  11200

04 18 00  J1825-17     14 29 40  15.8 121.8 -3.9     -50.0   -22   1  3  11200  04 18 00
04 19 30  ---          14 31 10  16.0 122.0 -3.9     -49.8    68   F  1  12400

04 19 30  LS5039       14 31 10  17.5 119.9 -3.9     -50.5    -5   1  3  12400  04 19 30
04 22 30  ---          14 34 11  18.1 120.4 -3.9     -50.1   175   F  1  14800

04 22 30  J1825-17     14 34 11  16.6 122.5 -3.9     -49.5    -5   1  3  14800  04 22 30
04 24 00  ---          14 35 41  16.9 122.7 -3.8     -49.3    85   F  1  16000

04 24 00  LS5039       14 35 41  18.3 120.7 -3.8     -50.0    -5   1  4  16000  04 24 00
04 26 50  ---          14 38 32  18.9 121.1 -3.8     -49.6   165   R  1  16933

04 26 50  J1825-17     14 38 32  17.4 123.2 -3.8     -49.0    -5   1  4  16933  04 26 50
04 28 20  ---          14 40 02  17.6 123.4 -3.8     -48.8    85   R  1  15733

04 28 20  LS5039       14 40 02  19.1 121.4 -3.8     -49.5    -5   1  4  15733  04 28 20
04 31 10  ---          14 42 52  19.7 121.9 -3.7     -49.1   165   R  1  13467

04 31 10  J1825-17     14 42 52  18.1 123.9 -3.7     -48.4    -5   1  4  13467  04 31 10
04 32 40  ---          14 44 23  18.4 124.2 -3.7     -48.2    85   R  1  12267

04 32 40  LS5039       14 44 23  19.9 122.1 -3.7     -48.9    -5   1  4  12267  04 32 40
04 35 30  ---          14 47 13  20.4 122.6 -3.7     -48.6   165   R  1  10000

04 35 30  J1825-17     14 47 13  18.9 124.6 -3.6     -47.9    -5   1  4  10000  04 35 30
04 37 00  ---          14 48 43  19.2 124.9 -3.6     -47.7    85   R  1   8800

04 37 00  J1837-15     14 48 43  18.2 121.5 -3.8     -49.6    -4   1  4   8800  04 37 00
04 38 30  ---          14 50 14  18.5 121.7 -3.8     -49.4    86   R  1   7600

04 38 30  J1911-20     14 50 14   9.4 120.2 -4.3     -52.4   -20   1  4   7600  04 38 30
04 40 00  ---          14 51 44   9.7 120.4 -4.3     -52.2    70   R  1   6400

04 44 10  3C345        14 55 54  66.4  59.8 -1.8    -104.5   134   1  4   6400  04 44 10
04 51 10  ---          15 02 55  67.7  58.9 -1.7    -106.5   420   R  1    800

04 55 08  J1825-17     15 06 54  22.3 128.1 -3.3     -45.2   146   1  5    800  04 55 08
04 58 08  ---          15 09 55  22.8 128.7 -3.3     -44.7   180   F  1   1600
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

04 58 08  LS5039       15 09 55  24.5 126.6 -3.3     -45.6    -5   1  5   1600  04 58 08
05 01 08  ---          15 12 55  25.0 127.2 -3.2     -45.2   175   F  1   4000

05 01 08  J1825-17     15 12 55  23.3 129.2 -3.2     -44.3    -5   1  5   4000  05 01 08
05 02 38  ---          15 14 26  23.6 129.5 -3.2     -44.1    85   F  1   5200

05 02 38  LS5039       15 14 26  25.2 127.5 -3.2     -44.9    -5   1  5   5200  05 02 38
05 05 38  ---          15 17 26  25.7 128.0 -3.1     -44.5   175   F  1   7600

05 05 38  J1825-17     15 17 26  24.1 130.1 -3.1     -43.6    -5   1  5   7600  05 05 38
05 07 08  ---          15 18 56  24.3 130.3 -3.1     -43.4    85   F  1   8800

05 07 08  J1837-15     15 18 56  23.6 126.7 -3.3     -45.7    -4   1  5   8800  05 07 08
05 08 38  ---          15 20 27  23.8 127.0 -3.3     -45.5    86   F  1  10000

05 08 38  J1911-20     15 20 27  14.9 124.8 -3.8     -48.8   -20   1  5  10000  05 08 38
05 10 08  ---          15 21 57  15.1 125.0 -3.8     -48.6    70   F  1  11200

05 11 05  J1825-17     15 22 54  25.0 131.1 -3.0     -42.8    35   1  5  11200  05 11 05
05 12 35  ---          15 24 24  25.2 131.4 -3.0     -42.5    90   F  1  12400

05 12 35  LS5039       15 24 24  26.9 129.4 -3.0     -43.5    -5   1  5  12400  05 12 35
05 15 35  ---          15 27 24  27.4 130.0 -3.0     -43.0   175   F  1  14800

05 15 35  J1825-17     15 27 24  25.7 132.0 -3.0     -42.1    -5   1  5  14800  05 15 35
05 17 05  ---          15 28 55  25.9 132.3 -2.9     -41.8    85   F  1  16000

05 17 05  LS5039       15 28 55  27.7 130.3 -3.0     -42.8    -5   1  6  16000  05 17 05
05 19 55  ---          15 31 45  28.1 130.9 -2.9     -42.3   165   R  1  16933

05 19 55  J1825-17     15 31 45  26.4 132.8 -2.9     -41.4    -5   1  6  16933  05 19 55
05 21 25  ---          15 33 15  26.6 133.1 -2.9     -41.1    85   R  1  15733

05 21 25  LS5039       15 33 15  28.4 131.2 -2.9     -42.1    -5   1  6  15733  05 21 25
05 24 15  ---          15 36 06  28.8 131.7 -2.8     -41.6   165   R  1  13467

05 24 15  J1825-17     15 36 06  27.1 133.7 -2.8     -40.6    -6   1  6  13467  05 24 15
05 25 45  ---          15 37 36  27.3 134.0 -2.8     -40.4    84   R  1  12267

05 25 45  LS5039       15 37 36  29.1 132.1 -2.8     -41.4    -6   1  6  12267  05 25 45
05 28 35  ---          15 40 26  29.5 132.7 -2.8     -40.9   164   R  1  10000
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

05 28 35  J1825-17     15 40 26  27.7 134.6 -2.8     -39.9    -6   1  6  10000  05 28 35
05 30 05  ---          15 41 57  28.0 134.9 -2.7     -39.7    84   R  1   8800

05 30 05  J1837-15     15 41 57  27.4 131.2 -2.9     -42.3    -5   1  6   8800  05 30 05
05 31 35  ---          15 43 27  27.7 131.5 -2.9     -42.0    85   R  1   7600

05 31 35  J1911-20     15 43 27  18.8 128.6 -3.5     -45.7   -20   1  6   7600  05 31 35
05 33 05  ---          15 44 57  19.1 128.9 -3.4     -45.5    70   R  1   6400

05 33 48  J1825-17     15 45 40  28.5 135.7 -2.7     -39.0    22   1  6   6400  05 33 48
05 35 48  ---          15 47 41  28.8 136.1 -2.6     -38.7   120   R  1   4800

05 35 48  LS5039       15 47 41  30.7 134.2 -2.6     -39.7    -6   1  6   4800  05 35 48
05 39 18  ---          15 51 11  31.2 135.0 -2.6     -39.0   204   R  1   2000

05 39 18  J1825-17     15 51 11  29.4 136.9 -2.6     -38.0    -6   1  6   2000  05 39 18
05 41 18  ---          15 53 12  29.6 137.3 -2.5     -37.7   114   R  1    400

05 41 18  LS5039       15 53 12  31.5 135.4 -2.6     -38.7    -6   1  7    400  05 41 18
05 44 48  ---          15 56 42  32.0 136.2 -2.5     -38.0   204   F  1   3200

05 44 48  J1825-17     15 56 42  30.2 138.1 -2.5     -37.0    -6   1  7   3200  05 44 48
05 46 48  ---          15 58 43  30.4 138.5 -2.4     -36.6   114   F  1   4800

05 46 48  LS5039       15 58 43  32.3 136.6 -2.5     -37.7    -6   1  7   4800  05 46 48
05 50 18  ---          16 02 13  32.8 137.4 -2.4     -37.0   204   F  1   7600

05 50 18  J1825-17     16 02 13  30.9 139.3 -2.4     -36.0    -6   1  7   7600  05 50 18
05 52 18  ---          16 04 14  31.2 139.8 -2.4     -35.6   114   F  1   9200

05 52 18  J1837-15     16 04 14  30.9 135.8 -2.6     -38.5    -5   1  7   9200  05 52 18
05 54 18  ---          16 06 14  31.2 136.3 -2.5     -38.1   115   F  1  10800

05 54 18  J1911-20     16 06 14  22.6 132.7 -3.1     -42.3   -19   1  7  10800  05 54 18
05 55 48  ---          16 07 44  22.8 133.0 -3.1     -42.1    71   F  1  12000

05 56 30  J1825-17     16 08 26  31.8 140.7 -2.3     -34.8    22   1  7  12000  05 56 30
05 58 30  ---          16 10 26  32.1 141.2 -2.3     -34.4   120   F  1  13600

05 58 30  LS5039       16 10 26  34.0 139.4 -2.3     -35.4    -6   1  7  13600  05 58 30
06 02 00  ---          16 13 57  34.5 140.2 -2.2     -34.7   204   F  1  16400
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

06 02 00  J1825-17     16 13 57  32.5 142.0 -2.2     -33.7    -6   1  8  16400  06 02 00
06 04 00  ---          16 15 57  32.8 142.5 -2.2     -33.3   114   R  1  17200

06 04 00  LS5039       16 15 57  34.8 140.7 -2.2     -34.3    -6   1  8  17200  06 04 00
06 07 30  ---          16 19 28  35.2 141.5 -2.1     -33.6   204   R  1  14400

06 07 30  J1825-17     16 19 28  33.3 143.3 -2.1     -32.6    -6   1  8  14400  06 07 30
06 09 30  ---          16 21 28  33.5 143.8 -2.1     -32.2   114   R  1  12800

06 09 30  LS5039       16 21 28  35.5 142.0 -2.1     -33.2    -6   1  8  12800  06 09 30
06 13 00  ---          16 24 59  36.0 142.9 -2.0     -32.5   204   R  1  10000

06 13 00  J1825-17     16 24 59  34.0 144.7 -2.0     -31.4    -6   1  8  10000  06 13 00
06 15 00  ---          16 26 59  34.2 145.2 -2.0     -31.0   114   R  1   8400

06 15 00  J1837-15     16 26 59  34.1 141.1 -2.2     -34.1    -5   1  8   8400  06 15 00
06 17 00  ---          16 29 00  34.4 141.6 -2.1     -33.7   115   R  1   6800

06 17 00  J1911-20     16 29 00  26.0 137.2 -2.7     -38.5   -19   1  8   6800  06 17 00
06 18 30  ---          16 30 30  26.2 137.5 -2.7     -38.2    71   R  1   5600

06 19 10  J1825-17     16 31 10  34.7 146.2 -1.9     -30.1    22   1  8   5600  06 19 10
06 21 10  ---          16 33 11  35.0 146.7 -1.9     -29.6   120   R  1   4000

06 21 10  LS5039       16 33 11  37.0 145.0 -1.9     -30.7    -6   1  8   4000  06 21 10
06 24 40  ---          16 36 41  37.4 145.9 -1.8     -29.9   204   R  1   1200

06 24 40  J1825-17     16 36 41  35.4 147.6 -1.8     -28.9    -6   1  9   1200  06 24 40
06 26 40  ---          16 38 42  35.6 148.1 -1.8     -28.4   114   F  1    400

06 26 40  LS5039       16 38 42  37.7 146.5 -1.8     -29.5    -6   1  9    400  06 26 40
06 30 10  ---          16 42 12  38.1 147.4 -1.7     -28.7   204   F  1   3200

06 30 10  J1825-17     16 42 12  36.0 149.0 -1.7     -27.6    -6   1  9   3200  06 30 10
06 32 10  ---          16 44 13  36.2 149.6 -1.7     -27.2   114   F  1   4800

06 32 10  LS5039       16 44 13  38.3 147.9 -1.7     -28.2    -6   1  9   4800  06 32 10
06 35 40  ---          16 47 43  38.7 148.9 -1.6     -27.4   204   F  1   7600

06 35 40  J1825-17     16 47 43  36.6 150.5 -1.6     -26.4    -6   1  9   7600  06 35 40
06 37 40  ---          16 49 43  36.8 151.0 -1.6     -25.9   114   F  1   9200
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

06 37 40  J1837-15     16 49 43  37.0 146.8 -1.8     -29.3    -5   1  9   9200  06 37 40
06 39 40  ---          16 51 44  37.3 147.3 -1.8     -28.8   115   F  1  10800

06 39 40  J1911-20     16 51 44  29.2 142.1 -2.3     -34.3   -18   1  9  10800  06 39 40
06 41 10  ---          16 53 14  29.4 142.4 -2.3     -34.0    72   F  1  12000

06 41 49  J1825-17     16 53 53  37.2 152.1 -1.5     -24.9    21   1  9  12000  06 41 49
06 43 49  ---          16 55 53  37.4 152.7 -1.5     -24.4   120   F  1  13600

06 43 49  LS5039       16 55 53  39.6 151.2 -1.5     -25.4    -6   1  9  13600  06 43 49
06 47 19  ---          16 59 24  39.9 152.2 -1.4     -24.5   204   F  1  16400

06 47 19  J1825-17     16 59 24  37.8 153.7 -1.4     -23.6    -6   1 10  16400  06 47 19
06 49 19  ---          17 01 24  37.9 154.2 -1.4     -23.1   114   R  1  17200

06 49 19  LS5039       17 01 24  40.1 152.8 -1.4     -24.0    -6   1 10  17200  06 49 19
06 52 49  ---          17 04 55  40.5 153.8 -1.4     -23.2   204   R  1  14400

06 52 49  J1825-17     17 04 55  38.3 155.2 -1.3     -22.2    -6   1 10  14400  06 52 49
06 54 49  ---          17 06 55  38.4 155.8 -1.3     -21.7   114   R  1  12800

06 54 49  LS5039       17 06 55  40.7 154.4 -1.3     -22.6    -6   1 10  12800  06 54 49
06 58 19  ---          17 10 26  41.0 155.4 -1.3     -21.7   204   R  1  10000

06 58 19  J1825-17     17 10 26  38.8 156.8 -1.3     -20.8    -6   1 10  10000  06 58 19
07 00 19  ---          17 12 26  38.9 157.3 -1.2     -20.3   114   R  1   8400

07 00 19  J1837-15     17 12 26  39.5 153.0 -1.4     -23.9    -5   1 10   8400  07 00 19
07 02 19  ---          17 14 26  39.7 153.6 -1.4     -23.4   115   R  1   6800

07 02 19  J1911-20     17 14 26  32.0 147.3 -1.9     -29.7   -17   1 10   6800  07 02 19
07 03 49  ---          17 15 57  32.2 147.7 -1.9     -29.3    73   R  1   5600

07 04 26  J1825-17     17 16 33  39.3 158.5 -1.2     -19.3    21   1 10   5600  07 04 26
07 06 26  ---          17 18 34  39.4 159.1 -1.1     -18.7   120   R  1   4000

07 06 26  LS5039       17 18 34  41.7 157.9 -1.1     -19.6    -7   1 10   4000  07 06 26
07 09 56  ---          17 22 04  42.0 158.9 -1.1     -18.7   203   R  1   1200

07 09 56  J1825-17     17 22 04  39.7 160.1 -1.1     -17.8    -7   1 11   1200  07 09 56
07 11 56  ---          17 24 05  39.8 160.7 -1.0     -17.3   113   F  1    400
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

07 11 56  LS5039       17 24 05  42.1 159.6 -1.0     -18.1    -7   1 11    400  07 11 56
07 15 26  ---          17 27 35  42.4 160.6 -1.0     -17.2   203   F  1   3200

07 15 26  J1825-17     17 27 35  40.1 161.8 -1.0     -16.4    -7   1 11   3200  07 15 26
07 17 26  ---          17 29 36  40.2 162.4 -0.9     -15.8   113   F  1   4800

07 17 26  LS5039       17 29 36  42.5 161.3 -0.9     -16.6    -7   1 11   4800  07 17 26
07 20 56  ---          17 33 06  42.8 162.4 -0.9     -15.6   203   F  1   7600

07 20 56  J1825-17     17 33 06  40.4 163.4 -0.9     -14.9    -7   1 11   7600  07 20 56
07 22 56  ---          17 35 06  40.5 164.1 -0.8     -14.3   113   F  1   9200

07 22 56  J1837-15     17 35 06  41.4 159.7 -1.0     -18.0    -5   1 11   9200  07 22 56
07 24 56  ---          17 37 07  41.6 160.3 -1.0     -17.5   115   F  1  10800

07 24 56  J1911-20     17 37 07  34.4 153.0 -1.6     -24.6   -16   1 11  10800  07 24 56
07 26 26  ---          17 38 37  34.6 153.4 -1.5     -24.3    74   F  1  12000

07 27 00  J1825-17     17 39 12  40.8 165.3 -0.8     -13.2    20   1 11  12000  07 27 00
07 29 00  ---          17 41 12  40.9 165.9 -0.7     -12.7   120   F  1  13600

07 29 00  LS5039       17 41 12  43.2 165.0 -0.8     -13.3    -7   1 11  13600  07 29 00
07 32 30  ---          17 44 43  43.4 166.1 -0.7     -12.3   203   F  1  16400

07 32 30  J1825-17     17 44 43  41.1 167.0 -0.7     -11.7    -7   1 12  16400  07 32 30
07 34 30  ---          17 46 43  41.1 167.6 -0.6     -11.1   113   R  1  17200

07 34 30  LS5039       17 46 43  43.5 166.8 -0.7     -11.8    -7   1 12  17200  07 34 30
07 38 00  ---          17 50 13  43.7 167.9 -0.6     -10.7   203   R  1  14400

07 38 00  J1825-17     17 50 13  41.3 168.7 -0.6     -10.2    -7   1 12  14400  07 38 00
07 40 00  ---          17 52 14  41.4 169.3 -0.6      -9.6   113   R  1  12800

07 40 00  LS5039       17 52 14  43.8 168.6 -0.6     -10.2    -7   1 12  12800  07 40 00
07 43 30  ---          17 55 44  43.9 169.7 -0.5      -9.1   203   R  1  10000

07 43 30  J1825-17     17 55 44  41.5 170.5 -0.5      -8.6    -7   1 12  10000  07 43 30
07 45 30  ---          17 57 45  41.6 171.1 -0.5      -8.0   113   R  1   8400

07 45 30  J1837-15     17 57 45  42.8 166.8 -0.7     -11.7    -5   1 12   8400  07 45 30
07 47 30  ---          17 59 45  42.9 167.5 -0.6     -11.2   115   R  1   6800
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

07 47 30  J1911-20     17 59 45  36.4 159.0 -1.2     -19.1   -15   1 12   6800  07 47 30
07 49 00  ---          18 01 15  36.5 159.4 -1.2     -18.8    75   R  1   5600

07 49 33  J1825-17     18 01 48  41.7 172.4 -0.4      -6.9    21   1 12   5600  07 49 33
07 51 33  ---          18 03 49  41.8 173.0 -0.4      -6.3   120   R  1   4000

07 51 33  LS5039       18 03 49  44.2 172.4 -0.4      -6.7    -7   1 12   4000  07 51 33
07 55 03  ---          18 07 19  44.3 173.6 -0.3      -5.7   203   R  1   1200

07 55 03  J1825-17     18 07 19  41.9 174.1 -0.3      -5.3    -7   1 13   1200  07 55 03
07 57 03  ---          18 09 19  41.9 174.8 -0.3      -4.7   113   F  1    400

07 57 03  LS5039       18 09 19  44.3 174.3 -0.3      -5.1    -7   1 13    400  07 57 03
08 00 33  ---          18 12 50  44.4 175.4 -0.2      -4.0   203   F  1   3200

08 00 33  J1825-17     18 12 50  42.0 175.9 -0.2      -3.7    -7   1 13   3200  08 00 33
08 02 33  ---          18 14 50  42.0 176.5 -0.2      -3.1   113   F  1   4800

08 02 33  LS5039       18 14 50  44.4 176.1 -0.2      -3.4    -7   1 13   4800  08 02 33
08 06 03  ---          18 18 21  44.5 177.3 -0.1      -2.4   203   F  1   7600

08 06 03  J1825-17     18 18 21  42.0 177.7 -0.1      -2.1    -7   1 13   7600  08 06 03
08 08 03  ---          18 20 21  42.0 178.3 -0.1      -1.5   113   F  1   9200

08 08 03  J1837-15     18 20 21  43.6 174.2 -0.3      -5.1    -5   1 13   9200  08 08 03
08 10 03  ---          18 22 22  43.7 174.9 -0.3      -4.6   115   F  1  10800

08 10 03  J1911-20     18 22 22  37.9 165.4 -0.8     -13.3   -14   1 13  10800  08 10 03
08 11 33  ---          18 23 52  38.0 165.9 -0.8     -12.9    76   F  1  12000

08 13 33  J1825-17     18 25 52  42.1 180.1  0.0       0.1   109   1 13  12000  08 13 33
08 15 33  ---          18 27 53  42.0 180.7  0.0       0.6   120   F  1  13600

08 15 33  LS5039       18 27 53  44.5 180.5  0.0       0.5    -7   1 13  13600  08 15 33
08 19 03  ---          18 31 23  44.5 181.7  0.1       1.5   203   F  1  16400

08 19 03  J1825-17     18 31 23  42.0 181.8  0.1       1.7    -7   1 14  16400  08 19 03
08 21 03  ---          18 33 23  42.0 182.5  0.1       2.2   113   R  1  17200

08 21 03  LS5039       18 33 23  44.5 182.4  0.1       2.1    -7   1 14  17200  08 21 03
08 24 33  ---          18 36 54  44.4 183.6  0.2       3.2   203   R  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

08 24 33  J1825-17     18 36 54  42.0 183.6  0.2       3.3    -7   1 14  14400  08 24 33
08 26 33  ---          18 38 54  41.9 184.3  0.2       3.8   113   R  1  12800

08 26 33  LS5039       18 38 54  44.4 184.3  0.2       3.8    -7   1 14  12800  08 26 33
08 30 03  ---          18 42 25  44.4 185.5  0.3       4.9   203   R  1  10000

08 30 03  J1825-17     18 42 25  41.9 185.4  0.3       4.8    -7   1 14  10000  08 30 03
08 32 03  ---          18 44 25  41.8 186.0  0.3       5.4   113   R  1   8400

08 32 03  J1837-15     18 44 25  43.8 182.3  0.1       2.0    -6   1 14   8400  08 32 03
08 34 03  ---          18 46 26  43.8 182.9  0.1       2.6   114   R  1   6800

08 34 03  J1911-20     18 46 26  38.9 172.5 -0.4      -6.8   -12   1 14   6800  08 34 03
08 35 33  ---          18 47 56  38.9 173.0 -0.4      -6.4    78   R  1   5600

08 36 08  J1825-17     18 48 31  41.7 187.3  0.4       6.6    24   1 14   5600  08 36 08
08 38 08  ---          18 50 31  41.7 188.0  0.4       7.2   120   R  1   4000

08 38 08  LS5039       18 50 31  44.1 188.2  0.4       7.3    -7   1 14   4000  08 38 08
08 41 38  ---          18 54 02  44.0 189.3  0.5       8.3   203   R  1   1200

-----------  Tape Change ------------

08 41 38  J1825-17     18 54 02  41.6 189.1  0.5       8.2    -7   2  1   1200  08 41 38
08 43 38  ---          18 56 02  41.5 189.7  0.5       8.7   113   F  1    400

08 43 38  LS5039       18 56 02  44.0 190.0  0.5       8.9    -7   2  1    400  08 43 38
08 47 08  ---          18 59 33  43.8 191.2  0.6       9.9   203   F  1   3200

08 47 08  J1825-17     18 59 33  41.4 190.8  0.6       9.7    -7   2  1   3200  08 47 08
08 49 08  ---          19 01 33  41.3 191.4  0.6      10.3   113   F  1   4800

08 49 08  LS5039       19 01 33  43.7 191.8  0.6      10.5    -7   2  1   4800  08 49 08
08 52 38  ---          19 05 04  43.6 193.0  0.6      11.5   203   F  1   7600

08 52 38  J1825-17     19 05 04  41.1 192.5  0.7      11.3    -7   2  1   7600  08 52 38
08 54 38  ---          19 07 04  41.0 193.2  0.7      11.8   113   F  1   9200

08 54 38  J1837-15     19 07 04  43.3 189.8  0.5       8.7    -7   2  1   9200  08 54 38
08 56 38  ---          19 09 04  43.2 190.4  0.5       9.3   113   F  1  10800

08 56 38  J1911-20     19 09 04  39.2 179.4  0.0      -0.6   -10   2  1  10800  08 56 38
08 58 08  ---          19 10 35  39.3 179.8  0.0      -0.2    80   F  1  12000
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

08 58 44  J1825-17     19 11 10  40.8 194.4  0.8      13.0    24   2  1  12000  08 58 44
09 00 44  ---          19 13 11  40.7 195.0  0.8      13.5   120   F  1  13600

09 00 44  LS5039       19 13 11  43.1 195.6  0.8      13.9    -7   2  1  13600  09 00 44
09 04 14  ---          19 16 41  42.9 196.7  0.8      14.9   203   F  1  16400

09 04 14  J1825-17     19 16 41  40.5 196.1  0.9      14.5    -7   2  2  16400  09 04 14
09 06 14  ---          19 18 42  40.4 196.7  0.9      15.0   113   R  1  17200

09 06 14  LS5039       19 18 42  42.8 197.4  0.9      15.4    -7   2  2  17200  09 06 14
09 09 44  ---          19 22 12  42.6 198.5  0.9      16.4   203   R  1  14400

09 09 44  J1825-17     19 22 12  40.2 197.8  0.9      16.0    -7   2  2  14400  09 09 44
09 11 44  ---          19 24 13  40.0 198.4  1.0      16.5   113   R  1  12800

09 11 44  LS5039       19 24 13  42.4 199.1  1.0      16.9    -7   2  2  12800  09 11 44
09 15 14  ---          19 27 43  42.2 200.2  1.0      17.9   203   R  1  10000

09 15 14  J1825-17     19 27 43  39.8 199.4  1.0      17.4    -7   2  2  10000  09 15 14
09 17 14  ---          19 29 43  39.6 200.0  1.1      18.0   113   R  1   8400

09 17 14  J1837-15     19 29 43  42.2 197.0  0.9      15.2    -7   2  2   8400  09 17 14
09 19 14  ---          19 31 44  42.0 197.6  0.9      15.7   113   R  1   6800

09 19 14  J1911-20     19 31 44  39.0 186.2  0.3       5.7   -10   2  2   6800  09 19 14
09 20 44  ---          19 33 14  39.0 186.7  0.4       6.1    80   R  1   5600

09 23 44  3C345        19 36 14  53.8 296.8  2.9      90.9   105   2  2   5600  09 23 44
09 29 14  ---          19 41 45  52.8 296.8  3.0      90.0   330   R  1   1200

09 31 49  J1825-17     19 44 20  38.5 204.2  1.3      21.7    91   2  3   1200  09 31 49
09 34 49  ---          19 47 21  38.2 205.1  1.4      22.5   180   F  1   1200

09 34 49  LS5039       19 47 21  40.5 206.1  1.4      23.1    -7   2  3   1200  09 34 49
09 37 49  ---          19 50 21  40.2 207.0  1.4      23.8   173   F  1   3600

09 37 49  J1825-17     19 50 21  37.9 205.9  1.4      23.2    -7   2  3   3600  09 37 49
09 39 49  ---          19 52 22  37.7 206.5  1.4      23.7   113   F  1   5200

09 39 49  LS5039       19 52 22  40.0 207.6  1.4      24.3    -7   2  3   5200  09 39 49
09 42 49  ---          19 55 22  39.7 208.4  1.5      25.1   173   F  1   7600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

09 42 49  J1825-17     19 55 22  37.4 207.3  1.5      24.4    -7   2  3   7600  09 42 49
09 44 49  ---          19 57 23  37.2 207.9  1.5      24.9   113   F  1   9200

09 44 49  J1837-15     19 57 23  40.0 205.4  1.3      22.5    -8   2  3   9200  09 44 49
09 46 49  ---          19 59 23  39.8 206.0  1.4      23.0   112   F  1  10800

09 46 49  J1911-20     19 59 23  37.9 194.4  0.8      13.2   -10   2  3  10800  09 46 49
09 48 19  ---          20 00 53  37.9 194.8  0.8      13.6    80   F  1  12000

09 48 54  J1825-17     20 01 29  36.8 209.0  1.6      25.9    24   2  3  12000  09 48 54
09 50 54  ---          20 03 29  36.6 209.5  1.6      26.3   120   F  1  13600

09 50 54  LS5039       20 03 29  38.9 210.7  1.6      27.0    -7   2  3  13600  09 50 54
09 54 24  ---          20 07 00  38.5 211.7  1.7      27.9   203   F  1  16400

09 54 24  J1825-17     20 07 00  36.2 210.4  1.7      27.2    -7   2  4  16400  09 54 24
09 56 24  ---          20 09 00  36.0 211.0  1.7      27.6   113   R  1  17200

09 56 24  LS5039       20 09 00  38.2 212.2  1.7      28.3    -6   2  4  17200  09 56 24
09 59 54  ---          20 12 31  37.8 213.2  1.8      29.1   204   R  1  14400

09 59 54  J1825-17     20 12 31  35.6 211.9  1.8      28.4    -6   2  4  14400  09 59 54
10 01 54  ---          20 14 31  35.4 212.4  1.8      28.9   114   R  1  12800

10 01 54  LS5039       20 14 31  37.6 213.7  1.8      29.6    -6   2  4  12800  10 01 54
10 05 24  ---          20 18 02  37.2 214.6  1.9      30.4   204   R  1  10000

10 05 24  J1825-17     20 18 02  35.0 213.3  1.9      29.6    -6   2  4  10000  10 05 24
10 07 24  ---          20 20 02  34.7 213.8  1.9      30.1   114   R  1   8400

10 07 24  J1837-15     20 20 02  37.7 211.7  1.7      28.0    -8   2  4   8400  10 07 24
10 09 24  ---          20 22 02  37.4 212.3  1.7      28.5   112   R  1   6800

10 09 24  J1911-20     20 22 02  36.5 200.8  1.2      19.0   -10   2  4   6800  10 09 24
10 10 54  ---          20 23 33  36.4 201.2  1.2      19.4    80   R  1   5600

10 11 30  J1825-17     20 24 08  34.2 214.8  2.0      31.0    24   2  4   5600  10 11 30
10 13 30  ---          20 26 08  34.0 215.3  2.0      31.4   120   R  1   4000

10 13 30  LS5039       20 26 08  36.2 216.7  2.0      32.2    -6   2  4   4000  10 13 30
10 17 00  ---          20 29 39  35.7 217.6  2.1      32.9   204   R  1   1200
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

10 17 00  J1825-17     20 29 39  33.5 216.2  2.1      32.1    -6   2  5   1200  10 17 00
10 19 00  ---          20 31 39  33.3 216.6  2.1      32.5   114   F  1    400

10 19 00  LS5039       20 31 39  35.4 218.1  2.1      33.3    -6   2  5    400  10 19 00
10 22 30  ---          20 35 10  35.0 219.0  2.1      34.0   204   F  1   3200

10 22 30  J1825-17     20 35 10  32.8 217.5  2.2      33.3    -6   2  5   3200  10 22 30
10 24 30  ---          20 37 10  32.6 218.0  2.2      33.7   114   F  1   4800

10 24 30  LS5039       20 37 10  34.7 219.5  2.2      34.4    -6   2  5   4800  10 24 30
10 28 00  ---          20 40 41  34.2 220.3  2.2      35.2   204   F  1   7600

10 28 00  J1825-17     20 40 41  32.1 218.8  2.3      34.4    -6   2  5   7600  10 28 00
10 30 00  ---          20 42 41  31.8 219.2  2.3      34.8   114   F  1   9200

10 30 00  J1837-15     20 42 41  34.9 217.6  2.1      33.0    -8   2  5   9200  10 30 00
10 32 00  ---          20 44 41  34.6 218.0  2.1      33.4   112   F  1  10800

10 32 00  J1911-20     20 44 41  34.5 206.9  1.6      24.5    -9   2  5  10800  10 32 00
10 33 30  ---          20 46 11  34.4 207.3  1.6      24.8    81   F  1  12000

10 34 04  J1825-17     20 46 46  31.3 220.2  2.4      35.5    24   2  5  12000  10 34 04
10 36 04  ---          20 48 46  31.0 220.6  2.4      35.9   120   F  1  13600

10 36 04  LS5039       20 48 46  33.1 222.2  2.4      36.7    -6   2  5  13600  10 36 04
10 39 34  ---          20 52 17  32.5 223.0  2.4      37.4   204   F  1  16400

10 39 34  J1825-17     20 52 17  30.5 221.4  2.4      36.6    -6   2  6  16400  10 39 34
10 41 34  ---          20 54 17  30.2 221.9  2.5      37.0   114   R  1  17200

10 41 34  LS5039       20 54 17  32.3 223.5  2.5      37.8    -6   2  6  17200  10 41 34
10 45 04  ---          20 57 48  31.7 224.2  2.5      38.4   204   R  1  14400

10 45 04  J1825-17     20 57 48  29.7 222.6  2.5      37.6    -6   2  6  14400  10 45 04
10 47 04  ---          20 59 48  29.4 223.1  2.6      38.0   114   R  1  12800

10 47 04  LS5039       20 59 48  31.4 224.7  2.6      38.8    -6   2  6  12800  10 47 04
10 50 34  ---          21 03 19  30.9 225.5  2.6      39.4   204   R  1  10000

10 50 34  J1825-17     21 03 19  28.9 223.8  2.6      38.6    -6   2  6  10000  10 50 34
10 52 34  ---          21 05 19  28.6 224.2  2.7      39.0   114   R  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

10 52 34  J1837-15     21 05 19  31.8 222.9  2.5      37.4    -8   2  6   8400  10 52 34
10 54 34  ---          21 07 19  31.5 223.3  2.5      37.8   112   R  1   6800

10 54 34  J1911-20     21 07 19  32.1 212.5  1.9      29.5    -9   2  6   6800  10 54 34
10 56 04  ---          21 08 50  31.9 212.9  2.0      29.9    81   R  1   5600

10 58 04  J1825-17     21 10 50  27.7 225.4  2.8      39.9   110   2  6   5600  10 58 04
11 00 04  ---          21 12 50  27.4 225.8  2.8      40.3   120   R  1   4000

11 00 04  LS5039       21 12 50  29.4 227.5  2.8      41.0    -6   2  6   4000  11 00 04
11 03 34  ---          21 16 21  28.8 228.2  2.8      41.6   204   R  1   1200

11 03 34  J1825-17     21 16 21  26.9 226.5  2.8      40.8    -6   2  7   1200  11 03 34
11 05 34  ---          21 18 21  26.6 226.9  2.9      41.2   114   F  1    400

11 05 34  LS5039       21 18 21  28.5 228.6  2.9      41.9    -6   2  7    400  11 05 34
11 09 04  ---          21 21 52  28.0 229.4  2.9      42.5   204   F  1   3200

11 09 04  J1825-17     21 21 52  26.0 227.6  2.9      41.7    -6   2  7   3200  11 09 04
11 11 04  ---          21 23 52  25.7 228.0  3.0      42.1   114   F  1   4800

11 11 04  LS5039       21 23 52  27.6 229.8  3.0      42.8    -6   2  7   4800  11 11 04
11 14 34  ---          21 27 23  27.0 230.5  3.0      43.3   204   F  1   7600

11 14 34  J1825-17     21 27 23  25.1 228.7  3.0      42.6    -6   2  7   7600  11 14 34
11 16 34  ---          21 29 23  24.8 229.1  3.1      42.9   114   F  1   9200

11 16 34  J1837-15     21 29 23  28.1 228.0  2.9      41.6    -8   2  7   9200  11 16 34
11 18 34  ---          21 31 23  27.7 228.4  2.9      41.9   112   F  1  10800

11 18 34  J1911-20     21 31 23  29.1 218.1  2.3      34.4    -9   2  7  10800  11 18 34
11 20 04  ---          21 32 54  28.9 218.4  2.4      34.7    81   F  1  12000

11 20 37  J1825-17     21 33 26  24.1 229.9  3.1      43.6    21   2  7  12000  11 20 37
11 22 37  ---          21 35 27  23.8 230.2  3.2      43.9   120   F  1  13600

11 22 37  LS5039       21 35 27  25.7 232.0  3.2      44.6    -6   2  7  13600  11 22 37
11 26 07  ---          21 38 57  25.1 232.7  3.2      45.1   204   F  1  16400

11 26 07  J1825-17     21 38 57  23.2 230.9  3.2      44.4    -6   2  8  16400  11 26 07
11 28 07  ---          21 40 58  22.9 231.3  3.3      44.7   114   R  1  17200
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

11 28 07  LS5039       21 40 58  24.8 233.1  3.2      45.4    -6   2  8  17200  11 28 07
11 31 37  ---          21 44 28  24.1 233.7  3.3      45.8   204   R  1  14400

11 31 37  J1825-17     21 44 28  22.3 231.9  3.3      45.2    -6   2  8  14400  11 31 37
11 33 37  ---          21 46 29  22.0 232.3  3.3      45.5   114   R  1  12800

11 33 37  LS5039       21 46 29  23.8 234.1  3.3      46.1    -6   2  8  12800  11 33 37
11 37 07  ---          21 49 59  23.2 234.7  3.4      46.6   204   R  1  10000

11 37 07  J1825-17     21 49 59  21.4 232.9  3.4      46.0    -6   2  8  10000  11 37 07
11 39 07  ---          21 51 59  21.0 233.3  3.4      46.2   114   R  1   8400

11 39 07  J1837-15     21 51 59  24.3 232.5  3.2      45.1    -9   2  8   8400  11 39 07
11 41 07  ---          21 54 00  24.0 232.8  3.3      45.4   111   R  1   6800

11 41 07  J1911-20     21 54 00  25.9 222.9  2.7      38.6    -9   2  8   6800  11 41 07
11 42 37  ---          21 55 30  25.7 223.2  2.7      38.9    81   R  1   5600

11 43 09  J1825-17     21 56 02  20.3 234.0  3.5      46.8    19   2  8   5600  11 43 09
11 45 09  ---          21 58 02  20.0 234.3  3.5      47.1   120   R  1   4000

11 45 09  LS5039       21 58 02  21.8 236.2  3.5      47.7    -6   2  8   4000  11 45 09
11 48 39  ---          22 01 33  21.1 236.8  3.6      48.1   204   R  1   1200

11 48 39  J1825-17     22 01 33  19.4 234.9  3.6      47.5    -6   2  9   1200  11 48 39
11 50 39  ---          22 03 33  19.0 235.3  3.6      47.8   114   F  1    400

11 50 39  LS5039       22 03 33  20.8 237.1  3.6      48.4    -6   2  9    400  11 50 39
11 54 09  ---          22 07 04  20.1 237.7  3.7      48.8   204   F  1   3200

11 54 09  J1825-17     22 07 04  18.4 235.9  3.7      48.2    -5   2  9   3200  11 54 09
11 56 09  ---          22 09 04  18.0 236.2  3.7      48.5   115   F  1   4800

11 56 09  LS5039       22 09 04  19.8 238.0  3.7      49.0    -5   2  9   4800  11 56 09
11 59 39  ---          22 12 35  19.1 238.6  3.8      49.5   205   F  1   7600

11 59 39  J1825-17     22 12 35  17.4 236.8  3.8      48.9    -5   2  9   7600  11 59 39
12 01 39  ---          22 14 35  17.0 237.1  3.8      49.2   115   F  1   9200

12 01 39  J1837-15     22 14 35  20.4 236.5  3.6      48.1    -9   2  9   9200  12 01 39
12 03 39  ---          22 16 35  20.0 236.8  3.6      48.4   111   F  1  10800
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Exploring the jets of a new microquasar
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu   8 Jun 2000   Day 160 ---

12 03 39  J1911-20     22 16 35  22.5 227.3  3.1      42.4    -8   2  9  10800  12 03 39
12 05 09  ---          22 18 06  22.2 227.6  3.1      42.6    82   F  1  12000

12 05 40  J1825-17     22 18 37  16.3 237.8  3.9      49.7    17   2  9  12000  12 05 40
12 07 40  ---          22 20 37  15.9 238.1  3.9      49.9   120   F  1  13600

12 07 40  LS5039       22 20 37  17.6 240.0  3.9      50.4    -5   2  9  13600  12 07 40
12 11 40  ---          22 24 38  16.9 240.6  4.0      50.8   235   F  1  16800

12 11 40  J1825-17     22 24 38  15.2 238.7  4.0      50.4    -5   2 10  16800  12 11 40
12 13 40  ---          22 26 38  14.8 239.0  4.0      50.6   115   R  1  16800

12 13 40  LS5039       22 26 38  16.5 240.9  4.0      51.1    -5   2 10  16800  12 13 40
12 17 40  ---          22 30 39  15.8 241.5  4.1      51.5   235   R  1  13600

12 17 40  J1825-17     22 30 39  14.1 239.7  4.1      51.1    -5   2 10  13600  12 17 40
12 19 40  ---          22 32 39  13.7 240.0  4.1      51.3   115   R  1  12000

12 19 40  LS5039       22 32 39  15.4 241.9  4.1      51.7    -5   2 10  12000  12 19 40
12 23 40  ---          22 36 40  14.6 242.5  4.2      52.1   235   R  1   8800

12 23 40  J1825-17     22 36 40  13.0 240.6  4.2      51.7    -5   2 10   8800  12 23 40
12 25 40  ---          22 38 40  12.6 240.9  4.2      51.9   115   R  1   7200

12 25 40  J1837-15     22 38 40  15.9 240.5  4.0      51.0    -9   2 10   7200  12 25 40
12 27 50  ---          22 40 50  15.5 240.8  4.1      51.2   121   R  1   5467

12 27 50  J1911-20     22 40 50  18.5 231.7  3.5      46.0    -8   2 10   5467  12 27 50
12 30 00  ---          22 43 01  18.2 232.1  3.5      46.3   122   R  1   3733


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gr021.set
   Matches group v6cm_2 in /usr/local/sched/catalogs/freq.dat

   Setup group:    8         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00
   Net SB=        U        U        U        U        U        U        U        U
   Pol.  =     LCP      LCP      LCP      LCP      LCP      LCP      LCP      LCP 
   BBC   =        1        2        3        4        5        6        7        8
   BBC SB=        U        U        U        U        U        U        U        U
   IF    =       C        C        C        C        C        C        C        C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   9  Setup file default.  Used pcal sets:   1
   LO sum=   4960.49  4968.49  4976.49  4984.49  4992.49  5000.49  5008.49  5016.49
   BBC fr=    860.49   868.49   876.49   884.49   892.49   900.49   908.49   916.49
   Bandwd=     8.000    8.000    8.000    8.000    8.000    8.000    8.000    8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510  6510  6510  6510  6510
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- Exploring the jets of a new microquasar
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * LS5039            18 23 23.640326   * 18 26 15.056000     18 26 16.776796 
                    -14 52 42.58697    *-14 50 54.24000     -14 50 49.54489 
                     From catalog imbedded in main SCHED input file.
                     This is our VLBI target source

 * J1825-17          18 22 42.021602   * 18 25 36.540000     18 25 38.284642 
                    -17 20 35.14168    *-17 18 49.70000     -17 18 44.74095 
                     From catalog imbedded in main SCHED input file.
                     This is the phase-reference

 * J1837-15          18 34 45.502261   * 18 37 37.672000     18 37 39.370814 
                    -15 35 21.60577    *-15 32 43.98000     -15 32 38.86439 
                     From catalog imbedded in main SCHED input file.
                     This is a possible phase-reference

   J1911-2006        19 08 12.464444   * 19 11 09.652892     19 11 11.287347 
   1908-201         -20 11 55.17861    *-20 06 55.10920     -20 06 48.29216 
 * J1911-20          From catalog imbedded in main SCHED input file.
                     USNO - Ref Frame 1998-6, Eubanks June 1998

   J1642+3948        16 41 17.606463   * 16 42 58.810200     16 43 00.702098 
   1641+399          39 54 10.81592    * 39 48 36.99500      39 48 40.75083 
 * 3C345             From catalog imbedded in main SCHED input file.
   J1642+39          JVAS-Patnaik et al. 1992, mnras, 254, 655; S8.4GHz=5182 mJy

   J2136+0041        21 34 05.207384   * 21 36 38.586319     21 36 39.503228 
   2134+00           00 28 25.08063    * 00 41 54.21345      00 41 56.82659 
 * 2134+004          From catalog imbedded in main SCHED input file.
   J2136+00          USNO - Ref Frame 1998-6, Eubanks June 1998



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   LS5039             159.6
   J1825-17           160.7
   J1837-15           157.3
   J1911-20           151.0
   3C345              117.1
   2134+004           110.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

