  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GM044 6cm global observation of M82
 Exp. Code:  GM044   


Schedule Version:       1.10                                              
Processed by SCHED version: Short term release of 12 Feb. 2001            

PI:       Andrew McDonald                                                 

Address:  Jodrell Bank Observatory                                        
          Macclesfield                                                    
          Cheshire, England                                               
                                                                          

Phone:    (+44) 1477 571321                                               
EMAIL:    amd@jb.man.ac.uk                                                
Fax:                                                                      
Phone during observation: (+44) 1477 571321                               

Observing mode: 256-8-2                                                   

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

 Next scan frequencies:  4971.49  4971.49  4979.49  4979.49  4987.49  4987.49
                         4995.49  4995.49
 Next BBC frequencies:    871.49   871.49   879.49   879.49   887.49   887.49
                          895.49   895.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

13 00 00  J0958+65     23 04 16   7.0   6.7-10.9     -14.1     0   1  1      0  13 00 00
13 10 00  ---          23 14 17   7.3   7.7-10.7     -16.3   600   F  1   8000

13 10 00  4195         23 14 17  11.3   6.8-10.7     -17.1   -10   1  1   8000  13 10 00
13 13 00  ---          23 17 18  11.4   7.1-10.6     -17.8   170   F  1  10400

13 13 00  J0958+65     23 17 18   7.4   8.0-10.7     -16.9   -10   1  1  10400  13 13 00
13 14 30  ---          23 18 48   7.4   8.2-10.7     -17.3    80   F  1  11600

13 14 30  4195         23 18 48  11.4   7.2-10.6     -18.1   -10   1  1  11600  13 14 30
13 17 30  ---          23 21 48  11.5   7.5-10.6     -18.8   170   F  1  14000

13 17 30  J0958+65     23 21 48   7.5   8.5-10.6     -17.9   -10   1  1  14000  13 17 30
13 19 00  ---          23 23 19   7.6   8.6-10.6     -18.2    80   F  1  15200

13 19 00  4195         23 23 19  11.6   7.6-10.5     -19.1   -10   1  1  15200  13 19 00
13 22 00  ---          23 26 19  11.7   7.8-10.5     -19.7   170   F  1  17600

13 22 40  J0958+65     23 26 59   7.7   9.0-10.5     -19.0    30   1  2  17600  13 22 40
13 24 10  ---          23 28 30   7.8   9.2-10.5     -19.3    90   R  1  16400

13 24 10  4195         23 28 30  11.7   8.0-10.5     -20.2   -10   1  2  16400  13 24 10
13 27 10  ---          23 31 30  11.8   8.3-10.4     -20.9   170   R  1  14000

13 27 10  J0958+65     23 31 30   7.9   9.5-10.5     -20.0   -10   1  2  14000  13 27 10
13 28 40  ---          23 33 00   7.9   9.6-10.4     -20.3    80   R  1  12800

13 28 40  4195         23 33 00  11.9   8.4-10.4     -21.2   -10   1  2  12800  13 28 40
13 31 40  ---          23 36 01  12.0   8.6-10.3     -21.8   170   R  1  10400

13 31 40  J0958+65     23 36 01   8.0   9.9-10.4     -20.9   -10   1  2  10400  13 31 40
13 33 10  ---          23 37 31   8.1  10.0-10.4     -21.3    80   R  1   9200

13 33 10  4195         23 37 31  12.0   8.8-10.3     -22.2   -10   1  2   9200  13 33 10
13 36 10  ---          23 40 31  12.1   9.0-10.3     -22.8   170   R  1   6800
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

13 36 10  J0958+65     23 40 31   8.2  10.3-10.3     -21.9   -10   1  2   6800  13 36 10
13 37 40  ---          23 42 02   8.2  10.5-10.3     -22.2    80   R  1   5600

13 37 40  4195         23 42 02  12.2   9.1-10.2     -23.1   -10   1  2   5600  13 37 40
13 40 40  ---          23 45 02  12.3   9.4-10.2     -23.8   170   R  1   3200

13 40 40  J0958+65     23 45 02   8.4  10.8-10.2     -22.9   -10   1  2   3200  13 40 40
13 42 10  ---          23 46 32   8.4  10.9-10.2     -23.2    80   R  1   2000

13 42 10  4195         23 46 32  12.3   9.5-10.2     -24.1   -10   1  2   2000  13 42 10
13 44 40  ---          23 49 03  12.4   9.7-10.1     -24.7   140   R  1      0

13 45 20  J0958+65     23 49 43   8.6  11.2-10.2     -23.9    30   1  3      0  13 45 20
13 46 50  ---          23 51 13   8.6  11.4-10.1     -24.2    90   F  1   1200

13 46 50  4195         23 51 13  12.5   9.9-10.1     -25.1   -10   1  3   1200  13 46 50
13 49 50  ---          23 54 14  12.6  10.1-10.0     -25.8   170   F  1   3600

13 49 50  J0958+65     23 54 14   8.8  11.6-10.1     -24.8   -10   1  3   3600  13 49 50
13 51 20  ---          23 55 44   8.8  11.8-10.1     -25.2    80   F  1   4800

13 51 20  4195         23 55 44  12.6  10.2-10.0     -26.1   -10   1  3   4800  13 51 20
13 54 20  ---          23 58 44  12.8  10.5-10.0     -26.8   170   F  1   7200

13 54 20  J0958+65     23 58 44   9.0  12.1-10.0     -25.8   -10   1  3   7200  13 54 20
13 55 50  ---          00 00 15   9.0  12.2-10.0     -26.1    80   F  1   8400

13 55 50  4195         00 00 15  12.8  10.6 -9.9     -27.1   -10   1  3   8400  13 55 50
13 58 50  ---          00 03 15  12.9  10.8 -9.9     -27.8   170   F  1  10800

13 58 50  J0958+65     00 03 15   9.2  12.5 -9.9     -26.8   -10   1  3  10800  13 58 50
14 00 20  ---          00 04 45   9.2  12.6 -9.9     -27.1    80   F  1  12000

14 00 20  4195         00 04 45  13.0  11.0 -9.9     -28.1   -10   1  3  12000  14 00 20
14 03 20  ---          00 07 46  13.1  11.2 -9.8     -28.7   170   F  1  14400

14 03 20  J0958+65     00 07 46   9.4  12.9 -9.9     -27.7   -10   1  3  14400  14 03 20
14 04 50  ---          00 09 16   9.4  13.1 -9.8     -28.0    80   F  1  15600

14 04 50  4195         00 09 16  13.2  11.3 -9.8     -29.1    -9   1  3  15600  14 04 50
14 07 20  ---          00 11 47  13.3  11.5 -9.7     -29.6   141   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

14 08 00  J0958+65     00 12 27   9.6  13.4 -9.8     -28.7    31   1  4  17600  14 08 00
14 09 30  ---          00 13 57   9.7  13.5 -9.7     -29.0    90   R  1  16400

14 09 30  4195         00 13 57  13.4  11.7 -9.7     -30.1    -9   1  4  16400  14 09 30
14 12 30  ---          00 16 57  13.5  11.9 -9.6     -30.7   171   R  1  14000

14 12 30  J0958+65     00 16 57   9.8  13.8 -9.7     -29.7    -9   1  4  14000  14 12 30
14 14 00  ---          00 18 28   9.9  13.9 -9.7     -30.0    81   R  1  12800

14 14 00  4195         00 18 28  13.6  12.0 -9.6     -31.0    -9   1  4  12800  14 14 00
14 17 00  ---          00 21 28  13.7  12.2 -9.6     -31.7   171   R  1  10400

14 17 00  J0958+65     00 21 28  10.1  14.2 -9.6     -30.6    -9   1  4  10400  14 17 00
14 18 30  ---          00 22 58  10.1  14.3 -9.6     -30.9    81   R  1   9200

14 18 30  4195         00 22 58  13.8  12.4 -9.5     -32.0    -9   1  4   9200  14 18 30
14 21 30  ---          00 25 59  13.9  12.6 -9.5     -32.7   171   R  1   6800

14 21 30  J0958+65     00 25 59  10.3  14.6 -9.5     -31.6    -9   1  4   6800  14 21 30
14 23 00  ---          00 27 29  10.4  14.7 -9.5     -31.9    81   R  1   5600

14 23 00  4195         00 27 29  14.0  12.7 -9.5     -33.0    -9   1  4   5600  14 23 00
14 26 00  ---          00 30 30  14.2  12.9 -9.4     -33.7   171   R  1   3200

14 26 00  J0958+65     00 30 30  10.6  15.0 -9.5     -32.5    -9   1  4   3200  14 26 00
14 27 30  ---          00 32 00  10.6  15.1 -9.4     -32.9    81   R  1   2000

14 27 30  4195         00 32 00  14.2  13.0 -9.4     -34.0    -9   1  4   2000  14 27 30
14 30 00  ---          00 34 30  14.3  13.2 -9.4     -34.5   141   R  1      0

14 30 40  J0958+65     00 35 10  10.8  15.4 -9.4     -33.5    31   1  5      0  14 30 40
14 32 10  ---          00 36 41  10.9  15.5 -9.4     -33.8    90   F  1   1200

14 32 10  4195         00 36 41  14.5  13.4 -9.3     -35.0    -9   1  5   1200  14 32 10
14 35 10  ---          00 39 41  14.6  13.6 -9.3     -35.6   171   F  1   3600

14 35 10  J0958+65     00 39 41  11.1  15.8 -9.3     -34.5    -9   1  5   3600  14 35 10
14 36 40  ---          00 41 11  11.2  15.9 -9.3     -34.8    81   F  1   4800

14 36 40  4195         00 41 11  14.7  13.7 -9.2     -36.0    -9   1  5   4800  14 36 40
14 39 40  ---          00 44 12  14.8  13.9 -9.2     -36.6   171   F  1   7200
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

14 39 40  J0958+65     00 44 12  11.3  16.2 -9.2     -35.4    -9   1  5   7200  14 39 40
14 41 10  ---          00 45 42  11.4  16.3 -9.2     -35.7    81   F  1   8400

14 41 10  4195         00 45 42  14.9  14.0 -9.2     -36.9    -9   1  5   8400  14 41 10
14 44 10  ---          00 48 43  15.1  14.3 -9.1     -37.6   171   F  1  10800

14 44 10  J0958+65     00 48 43  11.6  16.6 -9.2     -36.4    -9   1  5  10800  14 44 10
14 45 40  ---          00 50 13  11.7  16.7 -9.1     -36.7    81   F  1  12000

14 45 40  4195         00 50 13  15.2  14.4 -9.1     -37.9    -9   1  5  12000  14 45 40
14 48 40  ---          00 53 13  15.3  14.6 -9.0     -38.6   171   F  1  14400

14 48 40  J0958+65     00 53 13  11.9  16.9 -9.1     -37.3    -9   1  5  14400  14 48 40
14 50 10  ---          00 54 44  12.0  17.1 -9.1     -37.6    81   F  1  15600

14 50 10  4195         00 54 44  15.4  14.7 -9.0     -38.9    -9   1  5  15600  14 50 10
14 52 40  ---          00 57 14  15.5  14.9 -9.0     -39.4   141   F  1  17600

14 53 20  J0958+65     00 57 54  12.2  17.3 -9.0     -38.3    31   1  6  17600  14 53 20
14 54 50  ---          00 59 24  12.3  17.5 -9.0     -38.6    90   R  1  16400

14 54 50  4195         00 59 24  15.7  15.0 -8.9     -39.9    -9   1  6  16400  14 54 50
14 57 50  ---          01 02 25  15.8  15.2 -8.9     -40.5   171   R  1  14000

14 57 50  J0958+65     01 02 25  12.5  17.7 -8.9     -39.3    -9   1  6  14000  14 57 50
14 59 20  ---          01 03 55  12.6  17.8 -8.9     -39.6    81   R  1  12800

14 59 20  4195         01 03 55  15.9  15.3 -8.9     -40.9    -9   1  6  12800  14 59 20
15 02 20  ---          01 06 56  16.1  15.5 -8.8     -41.5   171   R  1  10400

15 02 20  J0958+65     01 06 56  12.8  18.1 -8.9     -40.2    -9   1  6  10400  15 02 20
15 03 50  ---          01 08 26  12.9  18.2 -8.8     -40.5    81   R  1   9200

15 03 50  4195         01 08 26  16.2  15.6 -8.8     -41.8    -9   1  6   9200  15 03 50
15 06 50  ---          01 11 26  16.3  15.8 -8.7     -42.5   171   R  1   6800

15 06 50  J0958+65     01 11 26  13.1  18.4 -8.8     -41.1    -9   1  6   6800  15 06 50
15 08 20  ---          01 12 57  13.2  18.6 -8.8     -41.5    81   R  1   5600

15 08 20  4195         01 12 57  16.4  15.9 -8.7     -42.8    -8   1  6   5600  15 08 20
15 11 20  ---          01 15 57  16.6  16.1 -8.7     -43.5   172   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

15 11 20  J0958+65     01 15 57  13.4  18.8 -8.7     -42.1    -8   1  6   3200  15 11 20
15 12 50  ---          01 17 27  13.5  18.9 -8.7     -42.4    82   R  1   2000

15 12 50  4195         01 17 27  16.7  16.2 -8.6     -43.8    -8   1  6   2000  15 12 50
15 15 20  ---          01 19 58  16.8  16.4 -8.6     -44.3   142   R  1      0

15 16 00  J0958+65     01 20 38  13.7  19.2 -8.6     -43.1    32   1  7      0  15 16 00
15 17 30  ---          01 22 08  13.8  19.3 -8.6     -43.4    90   F  1   1200

15 17 30  4195         01 22 08  17.0  16.5 -8.6     -44.8    -8   1  7   1200  15 17 30
15 20 30  ---          01 25 09  17.2  16.7 -8.5     -45.4   172   F  1   3600

15 20 30  J0958+65     01 25 09  14.0  19.5 -8.6     -44.0    -8   1  7   3600  15 20 30
15 22 00  ---          01 26 39  14.2  19.6 -8.5     -44.3    82   F  1   4800

15 22 00  4195         01 26 39  17.3  16.8 -8.5     -45.8    -8   1  7   4800  15 22 00
15 25 00  ---          01 29 39  17.4  17.0 -8.4     -46.4   172   F  1   7200

15 25 00  J0958+65     01 29 39  14.4  19.9 -8.5     -45.0    -8   1  7   7200  15 25 00
15 26 30  ---          01 31 10  14.5  20.0 -8.5     -45.3    82   F  1   8400

15 26 30  4195         01 31 10  17.5  17.1 -8.4     -46.7    -8   1  7   8400  15 26 30
15 29 30  ---          01 34 10  17.7  17.3 -8.4     -47.4   172   F  1  10800

15 29 30  J0958+65     01 34 10  14.7  20.2 -8.4     -45.9    -8   1  7  10800  15 29 30
15 31 00  ---          01 35 40  14.8  20.3 -8.4     -46.2    82   F  1  12000

15 31 00  4195         01 35 40  17.8  17.4 -8.3     -47.7    -8   1  7  12000  15 31 00
15 34 00  ---          01 38 41  18.0  17.6 -8.3     -48.4   172   F  1  14400

15 34 00  J0958+65     01 38 41  15.0  20.5 -8.3     -46.8    -8   1  7  14400  15 34 00
15 35 30  ---          01 40 11  15.2  20.6 -8.3     -47.2    82   F  1  15600

15 35 30  4195         01 40 11  18.1  17.6 -8.3     -48.7    -8   1  7  15600  15 35 30
15 38 00  ---          01 42 42  18.3  17.8 -8.2     -49.2   142   F  1  17600

15 38 40  J0958+65     01 43 22  15.4  20.9 -8.3     -47.8    32   1  8  17600  15 38 40
15 40 10  ---          01 44 52  15.5  21.0 -8.2     -48.1    90   R  1  16400

15 40 10  4195         01 44 52  18.4  17.9 -8.2     -49.7    -8   1  8  16400  15 40 10
15 43 10  ---          01 47 52  18.6  18.1 -8.1     -50.4   172   R  1  14000
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

15 43 10  J0958+65     01 47 52  15.7  21.2 -8.2     -48.8    -8   1  8  14000  15 43 10
15 44 40  ---          01 49 23  15.9  21.3 -8.2     -49.1    82   R  1  12800

15 44 40  4195         01 49 23  18.7  18.2 -8.1     -50.7    -8   1  8  12800  15 44 40
15 47 40  ---          01 52 23  18.9  18.4 -8.1     -51.3   172   R  1  10400

15 47 40  J0958+65     01 52 23  16.1  21.5 -8.1     -49.7    -8   1  8  10400  15 47 40
15 49 10  ---          01 53 53  16.2  21.6 -8.1     -50.0    82   R  1   9200

15 49 10  4195         01 53 53  19.0  18.5 -8.0     -51.6    -8   1  8   9200  15 49 10
15 52 10  ---          01 56 54  19.2  18.6 -8.0     -52.3   172   R  1   6800

15 52 10  J0958+65     01 56 54  16.5  21.8 -8.0     -50.6    -8   1  8   6800  15 52 10
15 53 40  ---          01 58 24  16.6  21.9 -8.0     -51.0    82   R  1   5600

15 53 40  4195         01 58 24  19.3  18.7 -8.0     -52.6    -8   1  8   5600  15 53 40
15 56 40  ---          02 01 25  19.6  18.9 -7.9     -53.3   172   R  1   3200

15 56 40  J0958+65     02 01 25  16.8  22.1 -8.0     -51.6    -7   1  8   3200  15 56 40
15 58 10  ---          02 02 55  16.9  22.2 -7.9     -51.9    83   R  1   2000

15 58 10  4195         02 02 55  19.7  19.0 -7.9     -53.6    -7   1  8   2000  15 58 10
16 00 40  ---          02 05 25  19.8  19.1 -7.8     -54.1   143   R  1      0

16 01 20  J0958+65     02 06 05  17.2  22.4 -7.9     -52.6    33   1  9      0  16 01 20
16 02 50  ---          02 07 36  17.3  22.5 -7.9     -52.9    90   F  1   1200

16 02 50  4195         02 07 36  20.0  19.2 -7.8     -54.6    -7   1  9   1200  16 02 50
16 05 50  ---          02 10 36  20.2  19.4 -7.8     -55.3   173   F  1   3600

16 05 50  J0958+65     02 10 36  17.6  22.7 -7.8     -53.5    -7   1  9   3600  16 05 50
16 07 20  ---          02 12 06  17.7  22.8 -7.8     -53.8    83   F  1   4800

16 07 20  4195         02 12 06  20.3  19.4 -7.7     -55.6    -7   1  9   4800  16 07 20
16 10 20  ---          02 15 07  20.5  19.6 -7.7     -56.2   173   F  1   7200

16 10 20  J0958+65     02 15 07  18.0  23.0 -7.7     -54.4    -7   1  9   7200  16 10 20
16 11 50  ---          02 16 37  18.1  23.1 -7.7     -54.7    83   F  1   8400

16 11 50  4195         02 16 37  20.6  19.7 -7.7     -56.6    -7   1  9   8400  16 11 50
16 14 50  ---          02 19 38  20.9  19.8 -7.6     -57.2   173   F  1  10800
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

16 14 50  J0958+65     02 19 38  18.3  23.3 -7.7     -55.4    -7   1  9  10800  16 14 50
16 16 20  ---          02 21 08  18.5  23.4 -7.6     -55.7    83   F  1  12000

16 16 20  4195         02 21 08  21.0  19.9 -7.6     -57.5    -7   1  9  12000  16 16 20
16 19 20  ---          02 24 08  21.2  20.1 -7.5     -58.2   173   F  1  14400

16 19 20  J0958+65     02 24 08  18.7  23.6 -7.6     -56.3    -7   1  9  14400  16 19 20
16 20 50  ---          02 25 39  18.9  23.7 -7.6     -56.6    83   F  1  15600

16 20 50  4195         02 25 39  21.3  20.1 -7.5     -58.5    -7   1  9  15600  16 20 50
16 23 20  ---          02 28 09  21.5  20.3 -7.5     -59.1   143   F  1  17600

16 24 00  J0958+65     02 28 49  19.1  23.9 -7.5     -57.3    33   1 10  17600  16 24 00
16 25 30  ---          02 30 19  19.3  23.9 -7.5     -57.6    90   R  1  16400

16 25 30  4195         02 30 19  21.6  20.4 -7.4     -59.5    -7   1 10  16400  16 25 30
16 28 30  ---          02 33 20  21.9  20.5 -7.4     -60.2   173   R  1  14000

16 28 30  J0958+65     02 33 20  19.5  24.1 -7.4     -58.2    -7   1 10  14000  16 28 30
16 30 00  ---          02 34 50  19.7  24.2 -7.4     -58.5    83   R  1  12800

16 30 00  4195         02 34 50  22.0  20.6 -7.4     -60.5    -7   1 10  12800  16 30 00
16 33 00  ---          02 37 51  22.2  20.7 -7.3     -61.2   173   R  1  10400

16 33 00  J0958+65     02 37 51  19.9  24.4 -7.4     -59.2    -7   1 10  10400  16 33 00
16 34 30  ---          02 39 21  20.1  24.5 -7.3     -59.5    83   R  1   9200

16 34 30  4195         02 39 21  22.3  20.8 -7.3     -61.5    -7   1 10   9200  16 34 30
16 37 30  ---          02 42 21  22.6  20.9 -7.2     -62.1   173   R  1   6800

16 37 30  J0958+65     02 42 21  20.3  24.6 -7.3     -60.1    -6   1 10   6800  16 37 30
16 39 00  ---          02 43 52  20.5  24.7 -7.2     -60.4    84   R  1   5600

16 39 00  4195         02 43 52  22.7  21.0 -7.2     -62.5    -6   1 10   5600  16 39 00
16 42 00  ---          02 46 52  22.9  21.1 -7.2     -63.1   174   R  1   3200

16 42 00  J0958+65     02 46 52  20.7  24.9 -7.2     -61.0    -6   1 10   3200  16 42 00
16 43 30  ---          02 48 22  20.9  25.0 -7.2     -61.4    84   R  1   2000

16 43 30  4195         02 48 22  23.0  21.2 -7.1     -63.5    -6   1 10   2000  16 43 30
16 46 00  ---          02 50 53  23.2  21.3 -7.1     -64.0   144   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

16 46 40  J0958+65     02 51 33  21.2  25.1 -7.1     -62.0    34   1 11      0  16 46 40
16 48 10  ---          02 53 03  21.3  25.2 -7.1     -62.3    90   F  1   1200

16 48 10  4195         02 53 03  23.4  21.4 -7.0     -64.5    -6   1 11   1200  16 48 10
16 51 10  ---          02 56 04  23.6  21.5 -7.0     -65.1   174   F  1   3600

16 51 10  J0958+65     02 56 04  21.6  25.4 -7.0     -63.0    -6   1 11   3600  16 51 10
16 52 40  ---          02 57 34  21.7  25.4 -7.0     -63.3    84   F  1   4800

16 52 40  4195         02 57 34  23.7  21.5 -7.0     -65.5    -6   1 11   4800  16 52 40
16 55 40  ---          03 00 34  24.0  21.7 -6.9     -66.1   174   F  1   7200

16 55 40  J0958+65     03 00 34  22.0  25.6 -7.0     -63.9    -6   1 11   7200  16 55 40
16 57 10  ---          03 02 05  22.1  25.7 -6.9     -64.2    84   F  1   8400

16 57 10  4195         03 02 05  24.1  21.7 -6.9     -66.4    -6   1 11   8400  16 57 10
17 00 10  ---          03 05 05  24.3  21.8 -6.8     -67.1   174   F  1  10800

17 00 10  J0958+65     03 05 05  22.4  25.8 -6.9     -64.9    -6   1 11  10800  17 00 10
17 01 40  ---          03 06 35  22.5  25.9 -6.9     -65.2    84   F  1  12000

17 01 40  4195         03 06 35  24.5  21.9 -6.8     -67.4    -6   1 11  12000  17 01 40
17 04 40  ---          03 09 36  24.7  22.0 -6.8     -68.1   174   F  1  14400

17 04 40  J0958+65     03 09 36  22.8  26.0 -6.8     -65.8    -6   1 11  14400  17 04 40
17 06 10  ---          03 11 06  23.0  26.1 -6.8     -66.1    84   F  1  15600

17 06 10  4195         03 11 06  24.8  22.0 -6.7     -68.4    -6   1 11  15600  17 06 10
17 08 40  ---          03 13 36  25.0  22.1 -6.7     -69.0   144   F  1  17600

17 09 20  J0958+65     03 14 17  23.3  26.2 -6.7     -66.8    34   1 12  17600  17 09 20
17 10 50  ---          03 15 47  23.4  26.3 -6.7     -67.1    90   R  1  16400

17 10 50  4195         03 15 47  25.2  22.2 -6.7     -69.5    -6   1 12  16400  17 10 50
17 13 50  ---          03 18 47  25.4  22.3 -6.6     -70.1   174   R  1  14000

17 13 50  J0958+65     03 18 47  23.7  26.4 -6.7     -67.7    -5   1 12  14000  17 13 50
17 15 20  ---          03 20 17  23.8  26.5 -6.6     -68.0    85   R  1  12800

17 15 20  4195         03 20 17  25.6  22.4 -6.6     -70.4    -5   1 12  12800  17 15 20
17 18 20  ---          03 23 18  25.8  22.5 -6.5     -71.1   175   R  1  10400
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

17 18 20  J0958+65     03 23 18  24.1  26.6 -6.6     -68.7    -5   1 12  10400  17 18 20
17 19 50  ---          03 24 48  24.3  26.7 -6.6     -69.0    85   R  1   9200

17 19 50  4195         03 24 48  25.9  22.5 -6.5     -71.4    -5   1 12   9200  17 19 50
17 22 50  ---          03 27 49  26.2  22.6 -6.5     -72.1   175   R  1   6800

17 22 50  J0958+65     03 27 49  24.6  26.8 -6.5     -69.6    -5   1 12   6800  17 22 50
17 24 20  ---          03 29 19  24.7  26.8 -6.5     -69.9    85   R  1   5600

17 24 20  4195         03 29 19  26.3  22.6 -6.4     -72.4    -5   1 12   5600  17 24 20
17 27 20  ---          03 32 19  26.6  22.7 -6.4     -73.1   175   R  1   3200

17 27 20  J0958+65     03 32 19  25.0  27.0 -6.4     -70.6    -5   1 12   3200  17 27 20
17 28 50  ---          03 33 50  25.2  27.0 -6.4     -70.9    85   R  1   2000

17 28 50  4195         03 33 50  26.7  22.8 -6.4     -73.4    -5   1 12   2000  17 28 50
17 31 20  ---          03 36 20  26.9  22.8 -6.3     -74.0   145   R  1      0

17 32 00  J0958+65     03 37 00  25.5  27.1 -6.4     -71.6    35   1 13      0  17 32 00
17 33 30  ---          03 38 30  25.6  27.2 -6.3     -71.9    90   F  1   1200

17 33 30  4195         03 38 30  27.1  22.9 -6.3     -74.5    -5   1 13   1200  17 33 30
17 36 30  ---          03 41 31  27.3  23.0 -6.2     -75.2   175   F  1   3600

17 36 30  J0958+65     03 41 31  25.9  27.3 -6.3     -72.5    -5   1 13   3600  17 36 30
17 38 00  ---          03 43 01  26.1  27.3 -6.3     -72.9    85   F  1   4800

17 38 00  4195         03 43 01  27.5  23.0 -6.2     -75.5    -5   1 13   4800  17 38 00
17 41 00  ---          03 46 02  27.7  23.1 -6.2     -76.2   175   F  1   7200

17 41 00  J0958+65     03 46 02  26.4  27.4 -6.2     -73.5    -5   1 13   7200  17 41 00
17 42 30  ---          03 47 32  26.5  27.5 -6.2     -73.8    85   F  1   8400

17 47 00  J0555+39     03 52 03  63.3  61.4 -2.1    -100.4   194   1 13   8400  17 47 00
17 58 30  ---          04 03 35  65.5  60.3 -1.9    -103.2   690   F  1  17600

18 00 30  J0958+65     04 05 35  28.3  28.0 -5.9     -77.7    44   1 14  17600  18 00 30
18 02 00  ---          04 07 05  28.5  28.1 -5.9     -78.0    90   R  1  16400

18 02 00  4195         04 07 05  29.5  23.5 -5.8     -80.9    -5   1 14  16400  18 02 00
18 05 00  ---          04 10 06  29.8  23.5 -5.8     -81.6   175   R  1  14000
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

18 05 00  J0958+65     04 10 06  28.8  28.1 -5.8     -78.7    -5   1 14  14000  18 05 00
18 06 30  ---          04 11 36  28.9  28.2 -5.8     -79.0    85   R  1  12800

18 06 30  4195         04 11 36  29.9  23.6 -5.7     -81.9    -5   1 14  12800  18 06 30
18 09 00  ---          04 14 06  30.1  23.6 -5.7     -82.5   145   R  1  10800

18 09 00  J0958+65     04 14 06  29.2  28.2 -5.7     -79.5    -5   1 14  10800  18 09 00
18 10 30  ---          04 15 37  29.3  28.2 -5.7     -79.9    85   R  1   9600

18 10 30  4195         04 15 37  30.2  23.6 -5.7     -82.8    -5   1 14   9600  18 10 30
18 13 00  ---          04 18 07  30.4  23.6 -5.6     -83.4   145   R  1   7600

18 13 00  J0958+65     04 18 07  29.6  28.3 -5.7     -80.4    -5   1 14   7600  18 13 00
18 14 30  ---          04 19 37  29.7  28.3 -5.7     -80.7    85   R  1   6400

18 14 30  4195         04 19 37  30.6  23.7 -5.6     -83.8    -5   1 14   6400  18 14 30
18 17 00  ---          04 22 08  30.8  23.7 -5.6     -84.3   145   R  1   4400

18 17 00  J0958+65     04 22 08  30.0  28.4 -5.6     -81.3    -5   1 14   4400  18 17 00
18 18 30  ---          04 23 38  30.2  28.4 -5.6     -81.6    85   R  1   3200

18 18 30  4195         04 23 38  30.9  23.7 -5.5     -84.7    -5   1 14   3200  18 18 30
18 21 00  ---          04 26 08  31.1  23.7 -5.5     -85.3   145   R  1   1200

18 21 00  J0958+65     04 26 08  30.4  28.4 -5.5     -82.2    -5   1 14   1200  18 21 00
18 22 30  ---          04 27 39  30.6  28.5 -5.5     -82.5    85   R  1      0

-----------  Tape Change ------------

18 37 30  J0958+65     04 42 41  32.1  28.7 -5.3     -85.8   895   2  1      0  18 37 30
18 39 00  ---          04 44 11  32.3  28.7 -5.2     -86.1    90   F  1   1200

18 39 00  4195         04 44 11  32.7  23.8 -5.2     -89.4    -5   2  1   1200  18 39 00
18 42 00  ---          04 47 12  33.0  23.8 -5.1     -90.1   175   F  1   3600

18 42 00  J0958+65     04 47 12  32.6  28.7 -5.2     -86.8    -5   2  1   3600  18 42 00
18 43 30  ---          04 48 42  32.7  28.7 -5.2     -87.2    85   F  1   4800

18 43 30  4195         04 48 42  33.1  23.8 -5.1     -90.5    -5   2  1   4800  18 43 30
18 46 30  ---          04 51 42  33.4  23.8 -5.1     -91.2   175   F  1   7200

18 46 30  J0958+65     04 51 42  33.0  28.7 -5.1     -87.8    -5   2  1   7200  18 46 30
18 48 00  ---          04 53 13  33.2  28.7 -5.1     -88.2    85   F  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

18 48 00  4195         04 53 13  33.5  23.8 -5.0     -91.6    -5   2  1   8400  18 48 00
18 51 00  ---          04 56 13  33.8  23.8 -5.0     -92.3   175   F  1  10800

18 51 00  J0958+65     04 56 13  33.5  28.7 -5.0     -88.8    -5   2  1  10800  18 51 00
18 52 30  ---          04 57 43  33.7  28.7 -5.0     -89.2    85   F  1  12000

18 52 30  4195         04 57 43  33.9  23.8 -5.0     -92.6    -5   2  1  12000  18 52 30
18 55 30  ---          05 00 44  34.1  23.8 -4.9     -93.3   175   F  1  14400

18 55 30  J0958+65     05 00 44  34.0  28.7 -5.0     -89.9    -5   2  1  14400  18 55 30
18 57 00  ---          05 02 14  34.1  28.7 -4.9     -90.2    85   F  1  15600

18 57 00  4195         05 02 14  34.3  23.8 -4.9     -93.7    -5   2  1  15600  18 57 00
18 59 30  ---          05 04 45  34.5  23.7 -4.9     -94.3   145   F  1  17600

19 00 10  J0958+65     05 05 25  34.5  28.7 -4.9     -90.9    35   2  2  17600  19 00 10
19 01 40  ---          05 06 55  34.6  28.7 -4.9     -91.3    90   R  1  16400

19 01 40  4195         05 06 55  34.7  23.7 -4.8     -94.8    -5   2  2  16400  19 01 40
19 04 40  ---          05 09 55  34.9  23.7 -4.8     -95.5   175   R  1  14000

19 04 40  J0958+65     05 09 55  34.9  28.7 -4.8     -92.0    -5   2  2  14000  19 04 40
19 06 10  ---          05 11 26  35.1  28.7 -4.8     -92.3    85   R  1  12800

19 06 10  4195         05 11 26  35.1  23.7 -4.7     -95.9    -5   2  2  12800  19 06 10
19 09 10  ---          05 14 26  35.3  23.6 -4.7     -96.6   175   R  1  10400

19 09 10  J0958+65     05 14 26  35.4  28.7 -4.7     -93.0    -5   2  2  10400  19 09 10
19 10 40  ---          05 15 56  35.5  28.7 -4.7     -93.4    85   R  1   9200

19 10 40  4195         05 15 56  35.5  23.6 -4.7     -97.0    -5   2  2   9200  19 10 40
19 13 40  ---          05 18 57  35.7  23.6 -4.6     -97.7   175   R  1   6800

19 13 40  J0958+65     05 18 57  35.9  28.7 -4.7     -94.1    -5   2  2   6800  19 13 40
19 15 10  ---          05 20 27  36.0  28.6 -4.6     -94.4    85   R  1   5600

19 15 10  4195         05 20 27  35.8  23.6 -4.6     -98.1    -5   2  2   5600  19 15 10
19 18 10  ---          05 23 28  36.1  23.5 -4.5     -98.8   175   R  1   3200

19 18 10  J0958+65     05 23 28  36.3  28.6 -4.6     -95.1    -5   2  2   3200  19 18 10
19 19 40  ---          05 24 58  36.5  28.6 -4.6     -95.5    85   R  1   2000
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

19 19 40  4195         05 24 58  36.2  23.5 -4.5     -99.2    -5   2  2   2000  19 19 40
19 22 10  ---          05 27 28  36.4  23.4 -4.5     -99.8   145   R  1      0

19 22 50  J0958+65     05 28 08  36.8  28.6 -4.5     -96.2    35   2  3      0  19 22 50
19 24 20  ---          05 29 39  37.0  28.5 -4.5     -96.6    90   F  1   1200

19 24 20  4195         05 29 39  36.6  23.4 -4.4    -100.3    -5   2  3   1200  19 24 20
19 27 20  ---          05 32 39  36.9  23.3 -4.4    -101.1   175   F  1   3600

19 27 20  J0958+65     05 32 39  37.3  28.5 -4.4     -97.3    -5   2  3   3600  19 27 20
19 28 50  ---          05 34 09  37.4  28.5 -4.4     -97.6    85   F  1   4800

19 28 50  4195         05 34 09  37.0  23.3 -4.4    -101.4    -5   2  3   4800  19 28 50
19 31 50  ---          05 37 10  37.3  23.2 -4.3    -102.2   175   F  1   7200

19 31 50  J0958+65     05 37 10  37.7  28.4 -4.4     -98.4    -5   2  3   7200  19 31 50
19 33 20  ---          05 38 40  37.9  28.4 -4.3     -98.7    85   F  1   8400

19 33 20  4195         05 38 40  37.4  23.2 -4.3    -102.6    -5   2  3   8400  19 33 20
19 36 20  ---          05 41 41  37.7  23.1 -4.2    -103.3   175   F  1  10800

19 36 20  J0958+65     05 41 41  38.2  28.3 -4.3     -99.4    -5   2  3  10800  19 36 20
19 37 50  ---          05 43 11  38.3  28.3 -4.3     -99.8    85   F  1  12000

19 37 50  4195         05 43 11  37.8  23.1 -4.2    -103.7    -5   2  3  12000  19 37 50
19 40 50  ---          05 46 11  38.0  23.0 -4.2    -104.4   175   F  1  14400

19 40 50  J0958+65     05 46 11  38.7  28.2 -4.2    -100.5    -5   2  3  14400  19 40 50
19 42 20  ---          05 47 42  38.8  28.2 -4.2    -100.9    85   F  1  15600

19 42 20  4195         05 47 42  38.2  23.0 -4.1    -104.8    -5   2  3  15600  19 42 20
19 44 50  ---          05 50 12  38.4  22.9 -4.1    -105.5   145   F  1  17600

19 45 30  J0958+65     05 50 52  39.1  28.1 -4.1    -101.7    35   2  4  17600  19 45 30
19 47 00  ---          05 52 22  39.3  28.0 -4.1    -102.0    90   R  1  16400

19 47 00  4195         05 52 22  38.6  22.8 -4.1    -106.0    -5   2  4  16400  19 47 00
19 50 00  ---          05 55 23  38.8  22.7 -4.0    -106.8   175   R  1  14000

19 50 00  J0958+65     05 55 23  39.6  28.0 -4.1    -102.8    -5   2  4  14000  19 50 00
19 51 30  ---          05 56 53  39.7  27.9 -4.0    -103.2    85   R  1  12800
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

19 51 30  4195         05 56 53  38.9  22.7 -4.0    -107.2    -5   2  4  12800  19 51 30
19 54 30  ---          05 59 54  39.2  22.6 -3.9    -107.9   175   R  1  10400

19 54 30  J0958+65     05 59 54  40.0  27.8 -4.0    -103.9    -5   2  4  10400  19 54 30
19 56 00  ---          06 01 24  40.2  27.8 -4.0    -104.3    85   R  1   9200

19 56 00  4195         06 01 24  39.3  22.5 -3.9    -108.3    -5   2  4   9200  19 56 00
19 59 00  ---          06 04 24  39.5  22.4 -3.9    -109.1   175   R  1   6800

19 59 00  J0958+65     06 04 24  40.5  27.7 -3.9    -105.0    -5   2  4   6800  19 59 00
20 00 30  ---          06 05 55  40.6  27.6 -3.9    -105.4    85   R  1   5600

20 00 30  4195         06 05 55  39.7  22.4 -3.8    -109.5    -5   2  4   5600  20 00 30
20 03 30  ---          06 08 55  39.9  22.3 -3.8    -110.3   175   R  1   3200

20 03 30  J0958+65     06 08 55  40.9  27.5 -3.8    -106.2    -5   2  4   3200  20 03 30
20 05 00  ---          06 10 25  41.1  27.4 -3.8    -106.5    85   R  1   2000

20 05 00  4195         06 10 25  40.0  22.2 -3.8    -110.6    -6   2  4   2000  20 05 00
20 07 30  ---          06 12 56  40.2  22.1 -3.7    -111.3   144   R  1      0

20 08 10  J0958+65     06 13 36  41.4  27.3 -3.8    -107.4    35   2  5      0  20 08 10
20 09 40  ---          06 15 06  41.6  27.3 -3.7    -107.7    90   F  1   1200

20 09 40  4195         06 15 06  40.4  22.0 -3.7    -111.9    -6   2  5   1200  20 09 40
20 12 40  ---          06 18 07  40.7  21.9 -3.6    -112.7   174   F  1   3600

20 12 40  J0958+65     06 18 07  41.8  27.1 -3.7    -108.5    -6   2  5   3600  20 12 40
20 14 10  ---          06 19 37  42.0  27.1 -3.7    -108.9    84   F  1   4800

20 14 10  4195         06 19 37  40.8  21.8 -3.6    -113.0    -6   2  5   4800  20 14 10
20 17 10  ---          06 22 37  41.0  21.7 -3.6    -113.8   174   F  1   7200

20 17 10  J0958+65     06 22 37  42.3  26.9 -3.6    -109.7    -6   2  5   7200  20 17 10
20 18 40  ---          06 24 08  42.4  26.8 -3.6    -110.1    84   F  1   8400

20 22 10  J0927+39     06 27 38  52.6  64.5 -3.0     -88.9   183   2  5   8400  20 22 10
20 33 40  ---          06 39 10  54.9  64.5 -2.8     -90.7   690   F  1  17600

20 35 40  J0958+65     06 41 10  44.1  25.9 -3.3    -114.6    92   2  6  17600  20 35 40
20 37 10  ---          06 42 41  44.2  25.8 -3.3    -115.0    90   R  1  16400
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

20 37 10  4195         06 42 41  42.6  20.6 -3.2    -119.2    -5   2  6  16400  20 37 10
20 40 10  ---          06 45 41  42.8  20.4 -3.2    -120.1   175   R  1  14000

20 40 10  J0958+65     06 45 41  44.5  25.7 -3.2    -115.8    -5   2  6  14000  20 40 10
20 41 40  ---          06 47 11  44.6  25.6 -3.2    -116.2    85   R  1  12800

20 41 40  4195         06 47 11  42.9  20.4 -3.1    -120.5    -5   2  6  12800  20 41 40
20 44 40  ---          06 50 12  43.1  20.2 -3.1    -121.3   175   R  1  10400

20 44 40  J0958+65     06 50 12  44.9  25.4 -3.1    -117.0    -6   2  6  10400  20 44 40
20 46 10  ---          06 51 42  45.0  25.3 -3.1    -117.4    84   R  1   9200

20 46 10  4195         06 51 42  43.3  20.1 -3.1    -121.7    -6   2  6   9200  20 46 10
20 49 10  ---          06 54 43  43.5  19.9 -3.0    -122.6   174   R  1   6800

20 49 10  J0958+65     06 54 43  45.3  25.1 -3.1    -118.3    -6   2  6   6800  20 49 10
20 50 40  ---          06 56 13  45.5  24.9 -3.0    -118.7    84   R  1   5600

20 50 40  4195         06 56 13  43.6  19.8 -3.0    -123.0    -6   2  6   5600  20 50 40
20 53 40  ---          06 59 13  43.8  19.6 -2.9    -123.8   174   R  1   3200

20 53 40  J0958+65     06 59 13  45.7  24.7 -3.0    -119.5    -6   2  6   3200  20 53 40
20 55 10  ---          07 00 44  45.9  24.6 -3.0    -119.9    84   R  1   2000

20 55 10  4195         07 00 44  43.9  19.5 -2.9    -124.2    -6   2  6   2000  20 55 10
20 57 40  ---          07 03 14  44.1  19.3 -2.9    -125.0   144   R  1      0

20 58 20  J0958+65     07 03 54  46.1  24.4 -2.9    -120.8    34   2  7      0  20 58 20
20 59 50  ---          07 05 24  46.3  24.3 -2.9    -121.3    90   F  1   1200

20 59 50  4195         07 05 24  44.2  19.2 -2.8    -125.6    -6   2  7   1200  20 59 50
21 02 50  ---          07 08 25  44.5  19.0 -2.8    -126.4   174   F  1   3600

21 02 50  J0958+65     07 08 25  46.5  24.0 -2.8    -122.1    -6   2  7   3600  21 02 50
21 04 20  ---          07 09 55  46.7  23.9 -2.8    -122.6    84   F  1   4800

21 04 20  4195         07 09 55  44.6  18.8 -2.8    -126.9    -6   2  7   4800  21 04 20
21 07 20  ---          07 12 56  44.8  18.6 -2.7    -127.7   174   F  1   7200

21 07 20  J0958+65     07 12 56  46.9  23.7 -2.8    -123.4    -6   2  7   7200  21 07 20
21 08 50  ---          07 14 26  47.1  23.5 -2.7    -123.9    84   F  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

21 08 50  4195         07 14 26  44.9  18.5 -2.7    -128.1    -6   2  7   8400  21 08 50
21 11 50  ---          07 17 26  45.1  18.3 -2.6    -129.0   174   F  1  10800

21 11 50  J0958+65     07 17 26  47.3  23.3 -2.7    -124.7    -6   2  7  10800  21 11 50
21 13 20  ---          07 18 57  47.4  23.1 -2.7    -125.2    84   F  1  12000

21 13 20  4195         07 18 57  45.2  18.2 -2.6    -129.5    -7   2  7  12000  21 13 20
21 16 20  ---          07 21 57  45.4  17.9 -2.6    -130.3   173   F  1  14400

21 16 20  J0958+65     07 21 57  47.7  22.9 -2.6    -126.1    -7   2  7  14400  21 16 20
21 17 50  ---          07 23 27  47.8  22.7 -2.6    -126.5    83   F  1  15600

21 17 50  4195         07 23 27  45.5  17.8 -2.5    -130.8    -7   2  7  15600  21 17 50
21 20 20  ---          07 25 58  45.6  17.6 -2.5    -131.5   143   F  1  17600

21 21 00  J0958+65     07 26 38  48.1  22.4 -2.5    -127.4    33   2  8  17600  21 21 00
21 22 30  ---          07 28 08  48.2  22.3 -2.5    -127.9    90   R  1  16400

21 22 30  4195         07 28 08  45.8  17.4 -2.5    -132.1    -7   2  8  16400  21 22 30
21 25 30  ---          07 31 09  46.0  17.2 -2.4    -133.0   173   R  1  14000

21 25 30  J0958+65     07 31 09  48.5  22.0 -2.5    -128.8    -7   2  8  14000  21 25 30
21 27 00  ---          07 32 39  48.6  21.9 -2.4    -129.2    83   R  1  12800

21 27 00  4195         07 32 39  46.1  17.0 -2.4    -133.5    -7   2  8  12800  21 27 00
21 30 00  ---          07 35 39  46.3  16.8 -2.3    -134.4   173   R  1  10400

21 30 00  J0958+65     07 35 39  48.8  21.6 -2.4    -130.2    -7   2  8  10400  21 30 00
21 31 30  ---          07 37 10  48.9  21.4 -2.4    -130.6    83   R  1   9200

21 31 30  4195         07 37 10  46.3  16.6 -2.3    -134.8    -7   2  8   9200  21 31 30
21 34 30  ---          07 40 10  46.5  16.4 -2.3    -135.7   173   R  1   6800

21 34 30  J0958+65     07 40 10  49.2  21.1 -2.3    -131.5    -7   2  8   6800  21 34 30
21 36 00  ---          07 41 40  49.3  20.9 -2.3    -132.0    83   R  1   5600

21 36 00  4195         07 41 40  46.6  16.2 -2.2    -136.2    -7   2  8   5600  21 36 00
21 39 00  ---          07 44 41  46.8  16.0 -2.2    -137.1   173   R  1   3200

21 39 00  J0958+65     07 44 41  49.5  20.6 -2.2    -132.9    -7   2  8   3200  21 39 00
21 40 30  ---          07 46 11  49.6  20.4 -2.2    -133.4    83   R  1   2000
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

21 40 30  4195         07 46 11  46.9  15.8 -2.2    -137.5    -7   2  8   2000  21 40 30
21 43 00  ---          07 48 41  47.0  15.6 -2.1    -138.3   143   R  1      0

21 43 40  J0958+65     07 49 22  49.9  20.1 -2.2    -134.4    32   2  9      0  21 43 40
21 45 10  ---          07 50 52  50.0  19.9 -2.1    -134.9    90   F  1   1200

21 45 10  4195         07 50 52  47.2  15.4 -2.1    -139.0    -8   2  9   1200  21 45 10
21 48 10  ---          07 53 52  47.3  15.1 -2.0    -139.9   172   F  1   3600

21 48 10  J0958+65     07 53 52  50.2  19.6 -2.1    -135.8    -8   2  9   3600  21 48 10
21 49 40  ---          07 55 23  50.3  19.4 -2.1    -136.3    82   F  1   4800

21 49 40  4195         07 55 23  47.4  14.9 -2.0    -140.3    -8   2  9   4800  21 49 40
21 52 40  ---          07 58 23  47.6  14.6 -2.0    -141.3   172   F  1   7200

21 52 40  J0958+65     07 58 23  50.5  19.1 -2.0    -137.2    -8   2  9   7200  21 52 40
21 54 10  ---          07 59 53  50.6  18.9 -2.0    -137.7    82   F  1   8400

21 54 10  4195         07 59 53  47.7  14.5 -1.9    -141.7    -8   2  9   8400  21 54 10
21 57 10  ---          08 02 54  47.8  14.2 -1.9    -142.7   172   F  1  10800

21 57 10  J0958+65     08 02 54  50.8  18.5 -1.9    -138.7    -8   2  9  10800  21 57 10
21 58 40  ---          08 04 24  50.9  18.3 -1.9    -139.2    82   F  1  12000

21 58 40  4195         08 04 24  47.9  14.0 -1.9    -143.1    -8   2  9  12000  21 58 40
22 01 40  ---          08 07 25  48.1  13.7 -1.8    -144.1   172   F  1  14400

22 01 40  J0958+65     08 07 25  51.1  17.9 -1.9    -140.2    -8   2  9  14400  22 01 40
22 03 10  ---          08 08 55  51.2  17.8 -1.8    -140.6    82   F  1  15600

22 03 10  4195         08 08 55  48.1  13.5 -1.8    -144.5    -8   2  9  15600  22 03 10
22 05 40  ---          08 11 25  48.3  13.3 -1.7    -145.3   142   F  1  17600

22 06 20  J0958+65     08 12 05  51.4  17.3 -1.8    -141.7    32   2 10  17600  22 06 20
22 07 50  ---          08 13 36  51.5  17.1 -1.8    -142.2    90   R  1  16400

22 07 50  4195         08 13 36  48.4  13.0 -1.7    -146.0    -8   2 10  16400  22 07 50
22 10 50  ---          08 16 36  48.5  12.7 -1.7    -147.0   172   R  1  14000

22 10 50  J0958+65     08 16 36  51.7  16.7 -1.7    -143.2    -8   2 10  14000  22 10 50
22 12 20  ---          08 18 06  51.8  16.5 -1.7    -143.7    82   R  1  12800
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

22 12 20  4195         08 18 06  48.6  12.5 -1.6    -147.4    -8   2 10  12800  22 12 20
22 15 20  ---          08 21 07  48.7  12.2 -1.6    -148.4   172   R  1  10400

22 15 20  J0958+65     08 21 07  52.0  16.1 -1.6    -144.7    -9   2 10  10400  22 15 20
22 16 50  ---          08 22 37  52.1  15.9 -1.6    -145.2    81   R  1   9200

22 16 50  4195         08 22 37  48.8  12.0 -1.6    -148.9    -9   2 10   9200  22 16 50
22 19 50  ---          08 25 38  48.9  11.7 -1.5    -149.8   171   R  1   6800

22 19 50  J0958+65     08 25 38  52.3  15.5 -1.6    -146.2    -9   2 10   6800  22 19 50
22 21 20  ---          08 27 08  52.3  15.3 -1.5    -146.7    81   R  1   5600

22 21 20  4195         08 27 08  49.0  11.5 -1.5    -150.3    -9   2 10   5600  22 21 20
22 24 20  ---          08 30 08  49.1  11.2 -1.4    -151.3   171   R  1   3200

22 24 20  J0958+65     08 30 08  52.5  14.9 -1.5    -147.7    -9   2 10   3200  22 24 20
22 25 50  ---          08 31 39  52.6  14.7 -1.5    -148.3    81   R  1   2000

22 25 50  4195         08 31 39  49.2  11.0 -1.4    -151.8    -9   2 10   2000  22 25 50
22 28 20  ---          08 34 09  49.3  10.7 -1.4    -152.6   141   R  1      0

22 29 00  J0958+65     08 34 49  52.8  14.2 -1.4    -149.3    31   2 11      0  22 29 00
22 30 30  ---          08 36 19  52.8  14.0 -1.4    -149.9    90   F  1   1200

22 30 30  4195         08 36 19  49.4  10.5 -1.3    -153.3    -9   2 11   1200  22 30 30
22 33 30  ---          08 39 20  49.5  10.1 -1.3    -154.3   171   F  1   3600

22 33 30  J0958+65     08 39 20  53.0  13.5 -1.3    -150.9    -9   2 11   3600  22 33 30
22 35 00  ---          08 40 50  53.1  13.3 -1.3    -151.4    81   F  1   4800

22 35 00  4195         08 40 50  49.5   9.9 -1.3    -154.7    -9   2 11   4800  22 35 00
22 38 00  ---          08 43 51  49.6   9.5 -1.2    -155.7   171   F  1   7200

22 38 00  J0958+65     08 43 51  53.2  12.8 -1.3    -152.5    -9   2 11   7200  22 38 00
22 39 30  ---          08 45 21  53.3  12.6 -1.2    -153.0    81   F  1   8400

22 39 30  4195         08 45 21  49.7   9.4 -1.2    -156.2    -9   2 11   8400  22 39 30
22 42 30  ---          08 48 21  49.8   9.0 -1.1    -157.2   171   F  1  10800

22 42 30  J0958+65     08 48 21  53.4  12.1 -1.2    -154.1    -9   2 11  10800  22 42 30
22 44 00  ---          08 49 51  53.5  11.9 -1.1    -154.6    81   F  1  12000
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

22 44 00  4195         08 49 51  49.8   8.8 -1.1    -157.7    -9   2 11  12000  22 44 00
22 47 00  ---          08 52 52  49.9   8.4 -1.1    -158.7   171   F  1  14400

22 47 00  J0958+65     08 52 52  53.6  11.4 -1.1    -155.7    -9   2 11  14400  22 47 00
22 48 30  ---          08 54 22  53.7  11.2 -1.1    -156.2    81   F  1  15600

22 48 30  4195         08 54 22  50.0   8.2 -1.0    -159.2    -9   2 11  15600  22 48 30
22 51 00  ---          08 56 53  50.1   7.9 -1.0    -160.0   141   F  1  17600

22 51 40  J0958+65     08 57 33  53.8  10.7 -1.0    -157.3    30   2 12  17600  22 51 40
22 53 10  ---          08 59 03  53.9  10.4 -1.0    -157.9    90   R  1  16400

22 53 10  4195         08 59 03  50.1   7.6 -0.9    -160.8   -10   2 12  16400  22 53 10
22 56 10  ---          09 02 03  50.2   7.3 -0.9    -161.8   170   R  1  14000

22 56 10  J0958+65     09 02 03  54.0   9.9 -0.9    -159.0   -10   2 12  14000  22 56 10
22 57 40  ---          09 03 34  54.1   9.7 -0.9    -159.5    80   R  1  12800

22 57 40  4195         09 03 34  50.3   7.1 -0.9    -162.3   -10   2 12  12800  22 57 40
23 00 40  ---          09 06 34  50.3   6.7 -0.8    -163.3   170   R  1  10400

23 00 40  J0958+65     09 06 34  54.2   9.2 -0.9    -160.6   -10   2 12  10400  23 00 40
23 02 10  ---          09 08 04  54.2   8.9 -0.8    -161.1    80   R  1   9200

23 02 10  4195         09 08 04  50.4   6.5 -0.8    -163.8   -10   2 12   9200  23 02 10
23 05 10  ---          09 11 05  50.4   6.1 -0.7    -164.8   170   R  1   6800

23 05 10  J0958+65     09 11 05  54.3   8.4 -0.8    -162.2   -10   2 12   6800  23 05 10
23 06 40  ---          09 12 35  54.4   8.2 -0.8    -162.8    80   R  1   5600

23 06 40  4195         09 12 35  50.5   5.9 -0.7    -165.3   -10   2 12   5600  23 06 40
23 09 40  ---          09 15 36  50.5   5.5 -0.7    -166.3   170   R  1   3200

23 09 40  J0958+65     09 15 36  54.4   7.7 -0.7    -163.9   -10   2 12   3200  23 09 40
23 11 10  ---          09 17 06  54.5   7.4 -0.7    -164.4    80   R  1   2000

23 11 10  4195         09 17 06  50.6   5.3 -0.6    -166.8   -10   2 12   2000  23 11 10
23 13 40  ---          09 19 36  50.6   5.0 -0.6    -167.6   140   R  1      0

23 14 20  J0958+65     09 20 16  54.6   6.9 -0.6    -165.6    30   2 13      0  23 14 20
23 15 50  ---          09 21 47  54.6   6.6 -0.6    -166.2    90   F  1   1200
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

23 15 50  4195         09 21 47  50.7   4.7 -0.6    -168.4   -10   2 13   1200  23 15 50
23 18 50  ---          09 24 47  50.7   4.3 -0.5    -169.4   170   F  1   3600

23 18 50  J0958+65     09 24 47  54.7   6.1 -0.6    -167.3   -10   2 13   3600  23 18 50
23 20 20  ---          09 26 17  54.7   5.8 -0.5    -167.8    80   F  1   4800

23 20 20  4195         09 26 17  50.7   4.1 -0.5    -169.9   -10   2 13   4800  23 20 20
23 23 20  ---          09 29 18  50.8   3.6 -0.4    -170.9   170   F  1   7200

23 23 20  J0958+65     09 29 18  54.8   5.3 -0.5    -168.9   -10   2 13   7200  23 23 20
23 24 50  ---          09 30 48  54.8   5.0 -0.5    -169.5    80   F  1   8400

23 24 50  4195         09 30 48  50.8   3.4 -0.4    -171.4   -10   2 13   8400  23 24 50
23 27 50  ---          09 33 49  50.8   3.0 -0.4    -172.5   170   F  1  10800

23 27 50  J0958+65     09 33 49  54.9   4.5 -0.4    -170.6   -10   2 13  10800  23 27 50
23 29 20  ---          09 35 19  54.9   4.2 -0.4    -171.2    80   F  1  12000

23 29 20  4195         09 35 19  50.8   2.8 -0.3    -173.0   -10   2 13  12000  23 29 20
23 32 20  ---          09 38 19  50.9   2.4 -0.3    -174.0   170   F  1  14400

23 32 20  J0958+65     09 38 19  54.9   3.7 -0.3    -172.3   -10   2 13  14400  23 32 20
23 33 50  ---          09 39 50  54.9   3.4 -0.3    -172.9    80   F  1  15600

23 33 50  4195         09 39 50  50.9   2.2 -0.3    -174.5   -10   2 13  15600  23 33 50
23 36 20  ---          09 42 20  50.9   1.9 -0.2    -175.4   140   F  1  17600

23 38 20  J0958+65     09 44 20  55.0   2.6 -0.2    -174.6   110   2 14  17600  23 38 20
23 39 50  ---          09 45 51  55.0   2.3 -0.2    -175.1    90   R  1  16400

23 39 50  4195         09 45 51  50.9   1.4 -0.2    -176.6   -10   2 14  16400  23 39 50
23 42 50  ---          09 48 51  50.9   1.0 -0.1    -177.6   170   R  1  14000

23 42 50  J0958+65     09 48 51  55.0   1.8 -0.2    -176.2   -10   2 14  14000  23 42 50
23 44 20  ---          09 50 21  55.0   1.5 -0.1    -176.8    80   R  1  12800

23 44 20  4195         09 50 21  50.9   0.8 -0.1    -178.1   -10   2 14  12800  23 44 20
23 46 50  ---          09 52 52  51.0   0.4 -0.1    -179.0   140   R  1  10800

23 46 50  J0958+65     09 52 52  55.1   1.1 -0.1    -177.8   -10   2 14  10800  23 46 50
23 48 20  ---          09 54 22  55.1   0.8 -0.1    -178.3    80   R  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GM044 6cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   6 Jun 2001   Day 157 ---

23 48 20  4195         09 54 22  51.0   0.2  0.0    -179.5   -10   2 14   9600  23 48 20
23 50 50  ---          09 56 52  51.0  -0.1  0.0     179.7   140   R  1   7600

23 50 50  J0958+65     09 56 52  55.1   0.4  0.0    -179.3   -10   2 14   7600  23 50 50
23 52 20  ---          09 58 23  55.1   0.1  0.0    -179.8    80   R  1   6400

23 52 20  4195         09 58 23  51.0  -0.3  0.0     179.2   -10   2 14   6400  23 52 20
23 54 50  ---          10 00 53  51.0  -0.7  0.1     178.3   140   R  1   4400

23 54 50  J0958+65     10 00 53  55.1  -0.4  0.0     179.2   -10   2 14   4400  23 54 50
23 56 20  ---          10 02 23  55.1  -0.6  0.1     178.7    80   R  1   3200

23 56 20  4195         10 02 23  50.9  -0.9  0.1     177.8   -10   2 14   3200  23 56 20
23 58 50  ---          10 04 54  50.9  -1.2  0.1     176.9   140   R  1   1200

23 58 50  J0958+65     10 04 54  55.1  -1.1  0.1     177.7   -10   2 14   1200  23 58 50
23 59 59  ---          10 06 04  55.1  -1.3  0.1     177.3    59   R  1    267


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /local/scratch/amd/sched/setups/v6cm-256-8-2.set
   Matches group v6cm_2 in /local/scratch/amd/sched/catalogs/freq.dat

   Setup group:    6         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   6  Setup file default.  Used pcal sets:   1
   LO sum=    4971.49   4971.49   4979.49   4979.49   4987.49   4987.49   4995.49   4995.49
   BBC fr=     871.49    871.49    879.49    879.49    887.49    887.49    895.49    895.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510  6510  6510  6510  6510
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- GM044 6cm global observation of M82
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * 4195              09 51 41.947830   * 09 55 50.685000     09 55 54.575587 
                     69 54 57.45641    * 69 40 43.76000      69 40 41.64118 
                     From catalog imbedded in main SCHED input file.

   J0555+3948        05 52 01.407168   * 05 55 30.805611     05 55 33.616671 
   0552+398          39 48 21.94582    * 39 48 49.16497      39 48 49.11169 
   DA193             /local/scratch/amd/sched/catalogs/sources.vlba
 * J0555+39          USNO - Ref Frame 1998-6, Eubanks June 1998

   J0927+3902        09 23 55.319194   * 09 27 03.013915     09 27 06.253486 
   0923+392          39 15 23.56652    * 39 02 20.85193      39 02 12.76131 
   4C39.25           /local/scratch/amd/sched/catalogs/sources.vlba
 * J0927+39          USNO - Ref Frame 1998-6, Eubanks June 1998

   J0958+6533        09 54 57.847929   * 09 58 47.245110     09 58 51.003193 
   0954+658          65 48 15.53887    * 65 33 54.81806      65 33 51.98843 
 * J0958+65          /local/scratch/amd/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   4195                63.2
   J0555+39            20.8
   J0927+39            58.3
   J0958+65            63.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

