  COVER INFORMATION 
 
 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Global VLBI
 Exp. Code:  gr016c  

 
Schedule Version:       1.00                                              
Processed by SCHED version: Short term release of 12 Feb. 2001            
 
PI:       Eduardo Ros                                                     
 
Address:  Max-Planck-Institut fuer Radioastronomie                        
          Auf dem Huegel 69                                               
          D-53121 Bonn                                                    
          Germany                                                         
 
Phone:    +49-228-525292                                                  
EMAIL:    ros@mpifr-bonn.mpg.de                                           
Fax:      +49-228-525229                                                  
Phone during observation: +49-228-525292                                  
 
Observing mode: 4cm 128-2-2                                               
 
Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
 ---------- **** Start with fringe finders ----------
  
 Next scan frequencies:  8416.99  8432.99
 Next BBC frequencies:    816.99   832.99
 Next scan bandwidths:     16.00    16.00
  
13 03 00  1928+738     22 51 30  39.8 343.8  3.4     119.7     0   1  1      0  13 03 00
13 10 30  ---          22 59 01  39.3 343.5  3.5     117.7   450   F  1   6000
  
 ---------- **** Target sources - 1st half ----------
  
13 21 19  0357+057     23 09 52  17.9  93.9 -4.8     -59.7   480   1  1   6000  13 21 19
13 23 19  ---          23 11 52  18.4  94.1 -4.8     -59.6   120   F  1   7600
  
13 24 04  0411+05      23 12 37  15.3  92.6 -5.0     -59.7    37   1  1   7600  13 24 04
13 29 34  ---          23 18 08  16.5  93.3 -4.9     -59.7   330   F  1  12000
  
13 30 19  0357+057     23 18 53  19.9  95.1 -4.7     -59.5    36   1  1  12000  13 30 19
13 32 19  ---          23 20 54  20.3  95.3 -4.7     -59.5   120   F  1  13600
  
13 33 04  0411+05      23 21 39  17.2  93.8 -4.9     -59.6    37   1  1  13600  13 33 04
13 38 04  ---          23 26 39  18.3  94.4 -4.8     -59.5   300   F  1  17600
  
13 42 04  0357+057     23 30 40  22.4  96.7 -4.5     -59.2   230   1  2  17600  13 42 04
13 44 04  ---          23 32 41  22.8  96.9 -4.5     -59.2   120   R  1  16000
  
13 44 49  0411+05      23 33 26  19.8  95.3 -4.7     -59.4    37   1  2  16000  13 44 49
13 50 19  ---          23 38 57  20.9  96.1 -4.6     -59.3   330   R  1  11600
  
 ---------- **** Target sources - 1st half ----------
  
13 51 04  0357+057     23 39 42  24.3  97.9 -4.3     -58.9    36   1  2  11600  13 51 04
13 53 04  ---          23 41 42  24.7  98.2 -4.3     -58.9   120   R  1  10000
  
13 53 49  0411+05      23 42 27  21.7  96.5 -4.5     -59.2    37   1  2  10000  13 53 49
13 59 19  ---          23 47 58  22.9  97.3 -4.4     -59.0   330   R  1   5600
  
14 00 04  0357+057     23 48 43  26.2  99.2 -4.2     -58.6    36   1  2   5600  14 00 04
14 02 04  ---          23 50 44  26.7  99.5 -4.2     -58.5   120   R  1   4000
  
14 02 49  0411+05      23 51 29  23.6  97.8 -4.4     -58.9    37   1  2   4000  14 02 49
14 07 49  ---          23 56 30  24.7  98.5 -4.3     -58.8   300   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
14 08 34  0357+057     23 57 15  28.0 100.4 -4.0     -58.3    36   1  1      0  14 08 34
14 10 34  ---          23 59 15  28.5 100.7 -4.0     -58.2   120   F  2   1600
  
14 11 19  0411+05      00 00 00  25.4  99.0 -4.2     -58.6    37   1  1   1600  14 11 19
14 16 49  ---          00 05 31  26.6  99.8 -4.2     -58.4   330   F  2   6000
  
 ---------- **** Target sources - 1st half ----------
  
14 17 34  0357+057     00 06 16  30.0 101.8 -3.9     -57.8    36   1  1   6000  14 17 34
14 19 34  ---          00 08 17  30.4 102.1 -3.9     -57.7   120   F  2   7600
  
14 20 19  0411+05      00 09 02  27.3 100.3 -4.1     -58.3    37   1  1   7600  14 20 19
14 25 49  ---          00 14 33  28.5 101.1 -4.0     -58.0   330   F  2  12000
  
14 26 34  0357+057     00 15 18  31.8 103.2 -3.7     -57.4    36   1  1  12000  14 26 34
14 28 34  ---          00 17 18  32.3 103.5 -3.7     -57.2   120   F  2  13600
  
14 29 19  0411+05      00 18 03  29.3 101.7 -3.9     -57.9    37   1  1  13600  14 29 19
14 34 19  ---          00 23 04  30.3 102.4 -3.9     -57.6   300   F  2  17600
  
14 35 04  0357+057     00 23 49  33.6 104.6 -3.6     -56.8    36   1  2  17600  14 35 04
14 37 04  ---          00 25 49  34.0 104.9 -3.6     -56.7   120   R  2  16000
  
14 37 49  0411+05      00 26 35  31.0 103.0 -3.8     -57.4    37   1  2  16000  14 37 49
14 43 19  ---          00 32 05  32.2 103.8 -3.7     -57.1   330   R  2  11600
  
14 45 19  0357+057     00 34 06  35.8 106.3 -3.4     -56.1   111   1  2  11600  14 45 19
14 47 19  ---          00 36 06  36.2 106.6 -3.4     -56.0   120   R  2  10000
  
14 48 04  0411+05      00 36 51  33.2 104.6 -3.6     -56.8    37   1  2  10000  14 48 04
14 53 04  ---          00 41 52  34.2 105.4 -3.5     -56.4   300   R  2   6000
  
14 53 49  0357+057     00 42 37  37.5 107.8 -3.3     -55.4    36   1  2   6000  14 53 49
14 55 49  ---          00 44 38  37.9 108.1 -3.3     -55.3   120   R  2   4400
  
14 56 34  0411+05      00 45 23  35.0 106.0 -3.5     -56.2    37   1  2   4400  14 56 34
15 02 04  ---          00 50 54  36.1 107.0 -3.4     -55.8   330   R  2      0
  
15 02 49  0357+057     00 51 39  39.4 109.4 -3.1     -54.7    36   1  3      0  15 02 49
15 04 49  ---          00 53 39  39.8 109.8 -3.1     -54.5   120   F  1   1600
  
15 05 34  0411+05      00 54 24  36.8 107.6 -3.3     -55.5    37   1  3   1600  15 05 34
15 11 04  ---          00 59 55  37.9 108.6 -3.2     -55.0   330   F  1   6000
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
15 11 49  0357+057     01 00 40  41.2 111.1 -3.0     -53.8    37   1  3   6000  15 11 49
15 13 49  ---          01 02 40  41.6 111.5 -3.0     -53.6   120   F  1   7600
  
15 14 34  0411+05      01 03 26  38.7 109.2 -3.2     -54.7    37   1  3   7600  15 14 34
15 19 34  ---          01 08 26  39.7 110.1 -3.1     -54.3   300   F  1  11600
  
15 20 19  0357+057     01 09 12  42.9 112.8 -2.9     -52.9    37   1  3  11600  15 20 19
15 22 19  ---          01 11 12  43.3 113.3 -2.8     -52.6   120   F  1  13200
  
15 23 04  0411+05      01 11 57  40.4 110.8 -3.0     -53.9    37   1  3  13200  15 23 04
15 28 34  ---          01 17 28  41.5 111.9 -3.0     -53.3   330   F  1  17600
  
15 29 19  0357+057     01 18 13  44.6 114.7 -2.7     -51.8    37   1  4  17600  15 29 19
15 31 19  ---          01 20 13  45.0 115.2 -2.7     -51.5   120   R  1  16000
  
15 32 04  0411+05      01 20 58  42.2 112.6 -2.9     -53.0    37   1  4  16000  15 32 04
15 37 34  ---          01 26 29  43.3 113.7 -2.8     -52.3   330   R  1  11600
  
15 38 19  0357+057     01 27 15  46.4 116.8 -2.5     -50.6    37   1  4  11600  15 38 19
15 40 19  ---          01 29 15  46.8 117.2 -2.5     -50.3   120   R  1  10000
  
15 41 04  0411+05      01 30 00  44.0 114.5 -2.7     -51.9    37   1  4  10000  15 41 04
15 46 04  ---          01 35 01  44.9 115.6 -2.7     -51.3   300   R  1   6000
  
15 48 04  0357+057     01 37 01  48.3 119.1 -2.4     -49.1   111   1  4   6000  15 48 04
15 50 04  ---          01 39 01  48.6 119.6 -2.4     -48.8   120   R  1   4400
  
15 50 49  0411+05      01 39 47  45.9 116.6 -2.6     -50.6    37   1  4   4400  15 50 49
15 56 19  ---          01 45 17  46.9 117.9 -2.5     -49.8   330   R  1      0
  
 ---------- **** EVN antennas move to 2nd half (1422/1434) ----------
  
15 57 04  0357+057     01 46 03  49.9 121.3 -2.2     -47.6    37   1  3      0  15 57 04
15 59 04  ---          01 48 03  50.3 121.9 -2.2     -47.3   120   F  2   1600
  
15 59 49  0411+05      01 48 48  47.6 118.7 -2.4     -49.3    38   1  3   1600  15 59 49
16 05 19  ---          01 54 19  48.6 120.1 -2.3     -48.4   330   F  2   6000
  
16 06 04  0357+057     01 55 04  51.6 123.8 -2.1     -46.0    37   1  3   6000  16 06 04
16 08 04  ---          01 57 04  51.9 124.3 -2.1     -45.6   120   F  2   7600
  
16 08 49  0411+05      01 57 50  49.3 121.0 -2.3     -47.8    38   1  3   7600  16 08 49
16 13 49  ---          02 02 50  50.2 122.3 -2.2     -47.0   300   F  2  11600
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
16 14 34  0357+057     02 03 35  53.1 126.2 -1.9     -44.2    37   1  3  11600  16 14 34
16 16 34  ---          02 05 36  53.4 126.8 -1.9     -43.8   120   F  2  13200
  
16 17 19  0411+05      02 06 21  50.8 123.2 -2.1     -46.3    38   1  3  13200  16 17 19
16 22 49  ---          02 11 52  51.8 124.7 -2.0     -45.3   330   F  2  17600
  
 ---------- **** EVN antennas move to 2nd half (1422/1434) ----------
  
16 23 34  0357+057     02 12 37  54.6 129.0 -1.8     -42.2    37   1  4  17600  16 23 34
16 25 34  ---          02 14 37  54.9 129.6 -1.8     -41.8   120   R  2  16000
  
16 26 19  0411+05      02 15 22  52.4 125.8 -2.0     -44.6    38   1  4  16000  16 26 19
16 31 49  ---          02 20 53  53.4 127.4 -1.9     -43.4   330   R  2  11600
  
16 32 34  0357+057     02 21 38  56.1 132.0 -1.6     -40.0    38   1  4  11600  16 32 34
16 34 34  ---          02 23 39  56.4 132.7 -1.6     -39.5   120   R  2  10000
  
16 35 19  0411+05      02 24 24  54.0 128.5 -1.8     -42.6    38   1  4  10000  16 35 19
16 40 19  ---          02 29 25  54.8 130.1 -1.8     -41.4   300   R  2   6000
  
16 41 04  0357+057     02 30 10  57.4 135.0 -1.5     -37.7    38   1  4   6000  16 41 04
16 43 04  ---          02 32 10  57.7 135.7 -1.5     -37.2   120   R  2   4400
  
16 43 49  0411+05      02 32 55  55.4 131.2 -1.7     -40.6    38   1  4   4400  16 43 49
16 49 19  ---          02 38 26  56.3 133.1 -1.6     -39.2   330   R  2      0
  
16 50 04  0357+057     02 39 11  58.7 138.4 -1.4     -35.1    38   1  5      0  16 50 04
16 52 04  ---          02 41 12  59.0 139.2 -1.3     -34.4   120   F  1   1600
  
16 52 49  0411+05      02 41 57  56.8 134.3 -1.5     -38.2    39   1  5   1600  16 52 49
16 58 19  ---          02 47 28  57.6 136.3 -1.5     -36.6   330   F  1   6000
  
17 00 19  0357+057     02 49 28  60.2 142.6 -1.2     -31.7   113   1  5   6000  17 00 19
17 02 19  ---          02 51 28  60.4 143.5 -1.1     -31.0   120   F  1   7600
  
17 03 04  0411+05      02 52 13  58.3 138.1 -1.4     -35.2    39   1  5   7600  17 03 04
17 08 04  ---          02 57 14  59.0 140.1 -1.3     -33.7   300   F  1  11600
  
17 08 49  0357+057     02 57 59  61.2 146.3 -1.0     -28.6    39   1  5  11600  17 08 49
17 10 49  ---          03 00 00  61.5 147.3 -1.0     -27.9   120   F  1  13200
  
17 11 34  0411+05      03 00 45  59.5 141.6 -1.2     -32.5    39   1  5  13200  17 11 34
17 17 04  ---          03 06 16  60.2 143.9 -1.1     -30.6   330   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
17 17 49  0357+057     03 07 01  62.2 150.6  -.9     -25.2    39   1  6  17600  17 17 49
17 19 49  ---          03 09 01  62.4 151.5  -.9     -24.3   120   R  1  16000
  
17 20 34  0411+05      03 09 46  60.7 145.4 -1.1     -29.4    39   1  6  16000  17 20 34
17 26 04  ---          03 15 17  61.3 147.9 -1.0     -27.3   330   R  1  11600
  
17 26 49  0357+057     03 16 02  63.1 155.1  -.7     -21.4    38   1  6  11600  17 26 49
17 28 49  ---          03 18 03  63.3 156.1  -.7     -20.5   120   R  1  10000
  
17 29 34  0411+05      03 18 48  61.7 149.5  -.9     -26.0    39   1  6  10000  17 29 34
17 34 34  ---          03 23 49  62.2 152.0  -.8     -24.0   300   R  1   6000
  
17 35 19  0357+057     03 24 34  63.8 159.5  -.6     -17.6    38   1  6   6000  17 35 19
17 37 19  ---          03 26 34  64.0 160.6  -.6     -16.7   120   R  1   4400
  
17 38 04  0411+05      03 27 19  62.6 153.7  -.8     -22.5    38   1  6   4400  17 38 04
17 43 34  ---          03 32 50  63.1 156.5  -.7     -20.2   330   R  1      0
  
17 44 19  0357+057     03 33 35  64.4 164.5  -.4     -13.4    38   1  5      0  17 44 19
17 46 19  ---          03 35 36  64.5 165.6  -.4     -12.4   120   F  2   1600
  
17 47 04  0411+05      03 36 21  63.4 158.3  -.6     -18.6    38   1  5   1600  17 47 04
17 52 34  ---          03 41 52  63.8 161.3  -.5     -16.1   330   F  2   6000
  
17 53 19  0357+057     03 42 37  64.9 169.6  -.3      -9.0    37   1  5   6000  17 53 19
17 55 19  ---          03 44 37  64.9 170.8  -.3      -7.9   120   F  2   7600
  
17 56 04  0411+05      03 45 22  64.0 163.2  -.5     -14.5    38   1  5   7600  17 56 04
18 01 04  ---          03 50 23  64.3 166.0  -.4     -12.1   300   F  2  11600
  
18 03 04  0357+057     03 52 23  65.1 175.4  -.1      -4.0   112   1  5  11600  18 03 04
18 05 04  ---          03 54 24  65.2 176.5  -.1      -3.0   120   F  2  13200
  
18 05 49  0411+05      03 55 09  64.5 168.7  -.3      -9.8    38   1  5  13200  18 05 49
18 11 19  ---          04 00 40  64.7 171.8  -.2      -7.1   330   F  2  17600
  
18 12 04  0357+057     04 01 25  65.2 180.7   .0        .6    37   1  6  17600  18 12 04
18 14 04  ---          04 03 25  65.2 181.9   .1       1.6   120   R  2  16000
  
18 14 49  0411+05      04 04 10  64.8 173.9  -.2      -5.3    38   1  6  16000  18 14 49
18 20 19  ---          04 09 41  64.9 177.1  -.1      -2.5   330   R  2  11600
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
18 21 04  0357+057     04 10 26  65.1 186.0   .2       5.2    37   1  6  11600  18 21 04
18 23 04  ---          04 12 27  65.0 187.2   .2       6.2   120   R  2  10000
  
18 23 49  0411+05      04 13 12  64.9 179.1   .0       -.7    38   1  6  10000  18 23 49
18 28 49  ---          04 18 13  64.9 182.1   .1       1.8   300   R  2   6000
  
18 29 34  0357+057     04 18 58  64.8 191.0   .3       9.5    37   1  6   6000  18 29 34
18 31 34  ---          04 20 58  64.7 192.2   .3      10.5   120   R  2   4400
  
18 32 19  0411+05      04 21 43  64.9 184.1   .1       3.6    38   1  6   4400  18 32 19
18 37 49  ---          04 27 14  64.8 187.4   .2       6.4   330   R  2      0
  
18 38 34  0357+057     04 27 59  64.4 196.1   .5      13.9    37   1  7      0  18 38 34
18 40 34  ---          04 29 59  64.2 197.2   .5      14.9   120   F  1   1600
  
18 41 19  0411+05      04 30 45  64.7 189.4   .3       8.1    38   1  7   1600  18 41 19
18 46 49  ---          04 36 15  64.4 192.5   .4      10.8   330   F  1   6000
  
18 47 34  0357+057     04 37 01  63.7 201.1   .6      18.1    37   1  7   6000  18 47 34
18 49 34  ---          04 39 01  63.6 202.1   .6      19.0   120   F  1   7600
  
18 50 19  0411+05      04 39 46  64.3 194.5   .4      12.5    38   1  7   7600  18 50 19
18 55 19  ---          04 44 47  64.0 197.3   .5      14.9   300   F  1  11600
  
18 56 04  0357+057     04 45 32  63.0 205.5   .8      21.9    38   1  7  11600  18 56 04
18 58 04  ---          04 47 32  62.8 206.5   .8      22.7   120   F  1  13200
  
18 58 49  0411+05      04 48 17  63.7 199.2   .6      16.5    38   1  7  13200  18 58 49
19 04 19  ---          04 53 48  63.3 202.1   .7      19.0   330   F  1  17600
  
19 06 19  0357+057     04 55 49  62.0 210.6   .9      26.1   112   1  8  17600  19 06 19
19 08 19  ---          04 57 49  61.8 211.5  1.0      26.9   120   R  1  16000
  
19 09 04  0411+05      04 58 34  62.9 204.6   .7      21.1    38   1  8  16000  19 09 04
19 14 34  ---          05 04 05  62.4 207.4   .8      23.4   330   R  1  11600
  
19 15 19  0357+057     05 04 50  60.9 214.7  1.1      29.5    38   1  8  11600  19 15 19
19 17 19  ---          05 06 50  60.7 215.6  1.1      30.2   120   R  1  10000
  
19 18 04  0411+05      05 07 36  62.0 209.1   .9      24.8    39   1  8  10000  19 18 04
19 23 04  ---          05 12 36  61.5 211.4  1.0      26.8   300   R  1   6000
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
19 23 49  0357+057     05 13 22  59.8 218.4  1.2      32.5    38   1  8   6000  19 23 49
19 25 49  ---          05 15 22  59.6 219.2  1.3      33.2   120   R  1   4400
  
19 26 34  0411+05      05 16 07  61.1 213.0  1.0      28.1    39   1  8   4400  19 26 34
19 32 04  ---          05 21 38  60.4 215.5  1.1      30.1   330   R  1      0
  
 ---------- **** SC, HN, NT move to 1422/1434 ----------
  
19 32 49  0357+057     05 22 23  58.6 222.0  1.4      35.4    39   1  7      0  19 32 49
19 34 49  ---          05 24 23  58.3 222.8  1.4      36.0   120   F  2   1600
  
19 35 34  0411+05      05 25 08  60.0 217.0  1.2      31.4    39   1  7   1600  19 35 34
19 41 04  ---          05 30 39  59.2 219.3  1.3      33.2   330   F  2   6000
  
19 41 49  0357+057     05 31 25  57.2 225.4  1.5      38.0    39   1  7   6000  19 41 49
19 43 49  ---          05 33 25  56.9 226.2  1.6      38.6   120   F  2   7600
  
19 44 34  0411+05      05 34 10  58.7 220.7  1.3      34.3    39   1  7   7600  19 44 34
19 49 34  ---          05 39 11  58.0 222.7  1.4      35.9   300   F  2  11600
  
19 50 19  0357+057     05 39 56  55.9 228.4  1.7      40.3    39   1  7  11600  19 50 19
19 52 19  ---          05 41 56  55.6 229.1  1.7      40.8   120   F  2  13200
  
19 53 04  0411+05      05 42 41  57.5 224.0  1.5      36.9    39   1  7  13200  19 53 04
19 58 34  ---          05 48 12  56.7 226.0  1.6      38.4   330   F  2  17600
  
19 59 19  0357+057     05 48 57  54.4 231.4  1.8      42.5    39   1  8  17600  19 59 19
20 01 19  ---          05 50 58  54.1 232.0  1.8      43.0   120   R  2  16000
  
20 02 04  0411+05      05 51 43  56.1 227.2  1.6      39.4    39   1  8  16000  20 02 04
20 07 34  ---          05 57 14  55.2 229.1  1.7      40.8   330   R  2  11600
  
20 09 34  0357+057     05 59 14  52.7 234.5  2.0      44.7   113   1  8  11600  20 09 34
20 11 34  ---          06 01 14  52.3 235.1  2.0      45.2   120   R  2  10000
  
20 12 19  0411+05      06 02 00  54.5 230.6  1.8      41.9    39   1  8  10000  20 12 19
20 17 19  ---          06 07 00  53.6 232.2  1.9      43.1   300   R  2   6000
  
20 18 04  0357+057     06 07 45  51.1 236.9  2.1      46.4    38   1  8   6000  20 18 04
20 20 04  ---          06 09 46  50.8 237.4  2.2      46.8   120   R  2   4400
  
20 20 49  0411+05      06 10 31  53.0 233.2  1.9      43.8    39   1  8   4400  20 20 49
20 26 19  ---          06 16 02  52.1 234.9  2.0      45.0   330   R  2      0
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
20 27 04  0357+057     06 16 47  49.5 239.3  2.3      48.0    38   1  9      0  20 27 04
20 29 04  ---          06 18 47  49.1 239.8  2.3      48.4   120   F  1   1600
  
20 29 49  0411+05      06 19 32  51.4 235.8  2.1      45.7    38   1  9   1600  20 29 49
20 35 19  ---          06 25 03  50.4 237.3  2.2      46.7   330   F  1   6000
  
20 36 04  0357+057     06 25 48  47.8 241.5  2.4      49.5    38   1  9   6000  20 36 04
20 38 04  ---          06 27 49  47.4 242.0  2.5      49.8   120   F  1   7600
  
20 38 49  0411+05      06 28 34  49.8 238.3  2.2      47.3    38   1  9   7600  20 38 49
20 43 49  ---          06 33 35  48.9 239.6  2.3      48.2   300   F  1  11600
  
20 44 34  0357+057     06 34 20  46.2 243.5  2.6      50.7    38   1  9  11600  20 44 34
20 46 34  ---          06 36 20  45.8 244.0  2.6      51.0   120   F  1  13200
  
20 47 19  0411+05      06 37 05  48.2 240.4  2.4      48.8    38   1  9  13200  20 47 19
20 52 49  ---          06 42 36  47.2 241.8  2.5      49.6   330   F  1  17600
  
20 53 34  0357+057     06 43 21  44.4 245.5  2.7      51.9    37   1 10  17600  20 53 34
20 55 34  ---          06 45 22  44.0 245.9  2.8      52.2   120   R  1  16000
  
20 56 19  0411+05      06 46 07  46.5 242.6  2.5      50.1    38   1 10  16000  20 56 19
21 01 49  ---          06 51 38  45.5 243.9  2.6      50.9   330   R  1  11600
  
21 02 34  0357+057     06 52 23  42.7 247.4  2.9      53.0    37   1 10  11600  21 02 34
21 04 34  ---          06 54 23  42.3 247.8  2.9      53.2   120   R  1  10000
  
21 05 19  0411+05      06 55 08  44.8 244.6  2.7      51.4    38   1 10  10000  21 05 19
21 10 19  ---          07 00 09  43.8 245.7  2.8      52.0   300   R  1   6000
  
21 12 19  0357+057     07 02 09  40.7 249.3  3.0      54.0   112   1 10   6000  21 12 19
21 14 19  ---          07 04 10  40.3 249.7  3.1      54.2   120   R  1   4400
  
21 15 04  0411+05      07 04 55  42.9 246.7  2.8      52.6    38   1 10   4400  21 15 04
21 20 34  ---          07 10 26  41.8 247.8  2.9      53.2   330   R  1      0
  
21 21 19  0357+057     07 11 11  38.9 251.0  3.2      54.9    37   1  9      0  21 21 19
21 23 19  ---          07 13 11  38.5 251.4  3.2      55.1   120   F  2   1600
  
21 24 04  0411+05      07 13 56  41.1 248.5  3.0      53.6    38   1  9   1600  21 24 04
21 29 34  ---          07 19 27  40.0 249.6  3.1      54.1   330   F  2   6000
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
21 30 19  0357+057     07 20 12  37.0 252.6  3.3      55.6    37   1  9   6000  21 30 19
21 32 19  ---          07 22 13  36.6 253.0  3.4      55.8   120   F  2   7600
  
21 33 04  0411+05      07 22 58  39.3 250.2  3.1      54.5    38   1  9   7600  21 33 04
21 38 04  ---          07 27 59  38.2 251.2  3.2      54.9   300   F  2  11600
  
21 38 49  0357+057     07 28 44  35.3 254.1  3.5      56.3    37   1  9  11600  21 38 49
21 40 49  ---          07 30 44  34.9 254.4  3.5      56.4   120   F  2  13200
  
21 41 34  0411+05      07 31 29  37.5 251.8  3.3      55.2    38   1  9  13200  21 41 34
21 47 04  ---          07 37 00  36.4 252.8  3.4      55.7   330   F  2  17600
  
21 47 49  0357+057     07 37 45  33.4 255.6  3.6      56.9    37   1 10  17600  21 47 49
21 49 49  ---          07 39 46  33.0 255.9  3.7      57.0   120   R  2  16000
  
21 50 34  0411+05      07 40 31  35.7 253.4  3.4      55.9    38   1 10  16000  21 50 34
21 56 04  ---          07 46 02  34.5 254.3  3.5      56.3   330   R  2  11600
  
21 56 49  0357+057     07 46 47  31.5 257.0  3.8      57.4    37   1 10  11600  21 56 49
21 58 49  ---          07 48 47  31.1 257.4  3.8      57.6   120   R  2  10000
  
21 59 34  0411+05      07 49 32  33.8 254.9  3.6      56.6    38   1 10  10000  21 59 34
22 04 34  ---          07 54 33  32.8 255.7  3.7      56.9   300   R  2   6000
  
22 05 19  0357+057     07 55 18  29.7 258.4  3.9      57.9    37   1 10   6000  22 05 19
22 07 19  ---          07 57 18  29.3 258.7  4.0      58.0   120   R  2   4400
  
22 08 04  0411+05      07 58 04  32.0 256.3  3.7      57.1    38   1 10   4400  22 08 04
22 13 34  ---          08 03 34  30.9 257.2  3.8      57.4   330   R  2      0
  
 ---------- **** all antennas in 1422/1434 ----------
  
22 44 33  1434+235     08 34 39  11.2 429.4 -6.0     -61.3  1742   1 11      0  22 44 33
22 46 33  ---          08 36 39  11.6 429.6 -6.0     -61.5   120   F  1   1600
  
22 47 18  1422+231     08 37 24  14.0 431.4 -5.8     -62.3    38   1 11   1600  22 47 18
22 52 48  ---          08 42 55  15.2 432.0 -5.7     -62.7   330   F  1   6000
  
22 53 33  1434+235     08 43 40  13.0 430.4 -5.9     -62.0    39   1 11   6000  22 53 33
22 55 33  ---          08 45 40  13.5 430.6 -5.9     -62.1   120   F  1   7600
  
22 56 18  1422+231     08 46 26  15.9 432.4 -5.6     -62.9    38   1 11   7600  22 56 18
23 01 18  ---          08 51 26  16.9 432.9 -5.6     -63.3   300   F  1  11600
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sat   2 Jun 2001   Day 153 ---
  
23 02 03  1434+235     08 52 12  14.8 431.3 -5.7     -62.6    39   1 11  11600  23 02 03
23 04 03  ---          08 54 12  15.2 431.6 -5.7     -62.7   120   F  1  13200
  
23 04 48  1422+231     08 54 57  17.6 433.3 -5.5     -63.5    38   1 11  13200  23 04 48
23 10 18  ---          09 00 28  18.8 433.9 -5.4     -63.9   330   F  1  17600
  
23 11 03  1434+235     09 01 13  16.6 432.3 -5.6     -63.2    39   1 12  17600  23 11 03
23 13 03  ---          09 03 13  17.0 432.5 -5.6     -63.4   120   R  1  16000
  
23 13 48  1422+231     09 03 58  19.5 434.3 -5.3     -64.1    38   1 12  16000  23 13 48
23 19 18  ---          09 09 29  20.6 434.9 -5.3     -64.4   330   R  1  11600
  
23 20 03  1434+235     09 10 15  18.5 433.3 -5.4     -63.8    39   1 12  11600  23 20 03
23 22 03  ---          09 12 15  18.9 433.5 -5.4     -64.0   120   R  1  10000
  
23 22 48  1422+231     09 13 00  21.4 435.3 -5.2     -64.6    38   1 12  10000  23 22 48
23 27 48  ---          09 18 01  22.4 435.8 -5.1     -64.9   300   R  1   6000
  
23 28 33  1434+235     09 18 46  20.2 434.2 -5.3     -64.4    39   1 12   6000  23 28 33
23 30 33  ---          09 20 46  20.7 434.4 -5.3     -64.5   120   R  1   4400
  
23 31 18  1422+231     09 21 31  23.1 436.2 -5.1     -65.1    38   1 12   4400  23 31 18
23 36 48  ---          09 27 02  24.3 436.7 -5.0     -65.4   330   R  1      0
  
23 37 33  1434+235     09 27 47  22.1 435.1 -5.1     -64.9    39   1 11      0  23 37 33
23 39 33  ---          09 29 48  22.5 435.3 -5.1     -65.1   120   F  2   1600
  
23 40 18  1422+231     09 30 33  25.0 437.1 -4.9     -65.6    38   1 11   1600  23 40 18
23 45 48  ---          09 36 04  26.2 437.7 -4.8     -65.9   330   F  2   6000
  
23 47 48  1434+235     09 38 04  24.3 436.2 -5.0     -65.5   114   1 11   6000  23 47 48
23 49 48  ---          09 40 04  24.7 436.4 -4.9     -65.6   120   F  2   7600
  
23 50 33  1422+231     09 40 50  27.2 438.2 -4.7     -66.1    38   1 11   7600  23 50 33
23 55 33  ---          09 45 50  28.2 438.7 -4.6     -66.4   300   F  2  11600
  
23 56 18  1434+235     09 46 35  26.0 437.1 -4.8     -66.0    39   1 11  11600  23 56 18
23 58 18  ---          09 48 36  26.5 437.3 -4.8     -66.1   120   F  2  13200
  
 --- Start: Sat   2 Jun 2001   Day 153 -- Stop: Sun   3 Jun 2001   Day 154 ---
  
23 59 03  1422+231     09 49 21  29.0 439.1 -4.6     -66.5    38   1 11  13200  23 59 03
00 04 33  ---          09 54 52  30.2 439.7 -4.5     -66.8   330   F  2  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sun   3 Jun 2001   Day 154 ---
  
00 05 18  1434+235     09 55 37  27.9 438.0 -4.7     -66.5    39   1 12  17600  00 05 18
00 07 18  ---          09 57 37  28.4 438.2 -4.7     -66.6   120   R  2  16000
  
00 08 03  1422+231     09 58 22  30.9 440.0 -4.4     -66.9    38   1 12  16000  00 08 03
00 13 33  ---          10 03 53  32.1 440.6 -4.3     -67.2   330   R  2  11600
  
00 14 18  1434+235     10 04 38  29.8 439.0 -4.5     -66.9    39   1 12  11600  00 14 18
00 16 18  ---          10 06 39  30.3 439.2 -4.5     -67.0   120   R  2  10000
  
00 17 03  1422+231     10 07 24  32.8 441.0 -4.3     -67.3    38   1 12  10000  00 17 03
00 22 03  ---          10 12 25  33.9 441.5 -4.2     -67.5   300   R  2   6000
  
00 22 48  1434+235     10 13 10  31.6 439.9 -4.4     -67.3    39   1 12   6000  00 22 48
00 24 48  ---          10 15 10  32.1 440.1 -4.4     -67.4   120   R  2   4400
  
00 25 33  1422+231     10 15 55  34.6 441.9 -4.1     -67.6    38   1 12   4400  00 25 33
00 31 03  ---          10 21 26  35.8 442.5 -4.1     -67.8   330   R  2      0
  
00 31 48  1434+235     10 22 11  33.6 440.8 -4.2     -67.7    39   1 13      0  00 31 48
00 33 48  ---          10 24 12  34.0 441.0 -4.2     -67.8   120   F  1   1600
  
00 34 33  1422+231     10 24 57  36.5 442.8 -4.0     -68.0    38   1 13   1600  00 34 33
00 40 03  ---          10 30 28  37.7 443.4 -3.9     -68.1   330   F  1   6000
  
00 40 48  1434+235     10 31 13  35.5 441.7 -4.1     -68.0    38   1 13   6000  00 40 48
00 42 48  ---          10 33 13  35.9 442.0 -4.1     -68.1   120   F  1   7600
  
00 51 59  1422+231     10 42 25  40.3 444.7 -3.7     -68.5   540   1 13   7600  00 51 59
00 56 59  ---          10 47 26  41.4 445.3 -3.6     -68.6   300   F  1  11600
  
00 58 59  1434+235     10 49 26  39.4 443.7 -3.8     -68.7   114   1 13  11600  00 58 59
01 00 59  ---          10 51 26  39.8 443.9 -3.8     -68.7   120   F  1  13200
  
01 04 59  1422+231     10 55 27  43.1 446.2 -3.5     -68.8   232   1 13  13200  01 04 59
01 10 29  ---          11 00 58  44.3 446.8 -3.4     -68.9   330   F  1  17600
  
01 11 14  1434+235     11 01 43  42.0 445.0 -3.6     -69.0    38   1 14  17600  01 11 14
01 13 14  ---          11 03 44  42.4 445.3 -3.6     -69.1   120   R  1  16000
  
01 13 59  1422+231     11 04 29  45.0 447.3 -3.3     -68.9    38   1 14  16000  01 13 59
01 19 29  ---          11 10 00  46.2 447.9 -3.2     -69.0   330   R  1  11600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Global VLBI
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------
  
 --- Sun   3 Jun 2001   Day 154 ---
  
01 20 14  1434+235     11 10 45  43.9 446.0 -3.4     -69.2    38   1 14  11600  01 20 14
01 22 14  ---          11 12 45  44.4 446.3 -3.4     -69.3   120   R  1  10000
  
01 26 14  1422+231     11 16 46  47.7 448.7 -3.1     -69.1   232   1 14  10000  01 26 14
01 31 14  ---          11 21 47  48.7 449.3 -3.0     -69.1   300   R  1   6000
  
01 31 59  1434+235     11 22 32  46.5 447.4 -3.2     -69.4    38   1 14   6000  01 31 59
01 33 59  ---          11 24 32  46.9 447.6 -3.2     -69.4   120   R  1   4400
  
01 37 59  1422+231     11 28 33  50.2  90.2 -2.9     -69.1     0   1 14   4400  01 37 59
01 43 29  ---          11 34 04  51.4  90.9 -2.8     -69.1   330   R  1      0
  
01 44 14  1434+235     11 34 49  49.1  88.9 -3.0     -69.6    38   1 13      0  01 44 14
01 46 14  ---          11 36 49  49.5  89.1 -3.0     -69.6   120   F  2   1600
  
01 46 59  1422+231     11 37 35  52.1  91.4 -2.8     -69.1    38   1 13   1600  01 46 59
01 52 29  ---          11 43 06  53.3  92.1 -2.7     -69.0   330   F  2   6000
  
01 53 14  1434+235     11 43 51  51.0  90.0 -2.9     -69.6    38   1 13   6000  01 53 14
01 55 14  ---          11 45 51  51.5  90.2 -2.8     -69.6   120   F  2   7600
  
01 59 15  1422+231     11 49 52  54.8  93.1 -2.6     -68.9   232   1 13   7600  01 59 15
02 04 15  ---          11 54 53  55.9  93.8 -2.5     -68.8   300   F  2  11600
  
02 05 00  1434+235     11 55 38  53.6  91.5 -2.7     -69.5    38   1 13  11600  02 05 00
02 07 00  ---          11 57 38  54.0  91.8 -2.7     -69.5   120   F  2  13200
  
02 07 45  1422+231     11 58 23  56.6  94.3 -2.4     -68.7    38   1 13  13200  02 07 45
02 13 15  ---          12 03 54  57.8  95.2 -2.3     -68.5   330   F  2  17600
  
02 36 26  1803+784     12 27 09  31.3  13.4 -5.6     -89.7  1335   1 14  17600  02 36 26
02 42 56  ---          12 33 40  31.6  13.4 -5.5     -91.3   390   R  2  12400
  
02 49 01  3C345        12 39 47  40.4  61.8 -4.1     -80.7   331   1 14  12400  02 49 01
02 58 01  ---          12 48 48  42.1  62.1 -3.9     -81.9   540   R  2   5200
 
 
SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.
 
 
 Setup file: v4cm-128-2-2-R
   Matches group v4cm_3 in /homes/ros/vlbi/sched/catalogs/freq.dat
 
   Setup group:    5         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 32.000
   Number of channels:  2    Passes/head pos:   2       Speedup factor:   1.00
 
   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00
 
   1st LO=   7600.00   7600.00
   Net SB=         U         U
   Pol.  =      RCP       RCP 
   BBC   =         1         2
   BBC SB=         U         U
   IF    =        B         B 
 
   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.4     15.4
 
  The following frequency sets based on this setup were used.
 
   Frequency Set:   5  Setup file default.  Used pcal sets:   1
   LO sum=    8416.99   8432.99
   BBC fr=     816.99    832.99
   Bandwd=     16.000    16.000
 
  The following pulse cal sets were used with this setup:
 
   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S1    S1    S2    S1    OFF   OFF   OFF
    PCALXB2=   S2    S2    M1    M2    S2    OFF   OFF   OFF
    PCALFR1=    10 13010     0     0  1010     0     0     0
    PCALFR2=    10 13010     0     0  1010     0     0     0
 
   Track assignments are: 
    track1=   2, 18
    track2=   3, 19
    barrel=roll_off 
 SOURCE LIST -- Global VLBI
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
  
   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 
  
 * 0411+05           04 11 57.895704   * 04 14 37.408000     04 14 39.477461   
                     05 27 12.42793    * 05 34 42.34700      05 34 47.57157    
                     From catalog imbedded in main SCHED input file.
 
 * 0357+057          03 57 32.152711   * 04 00 11.735800     04 00 13.823263   
                     05 42 17.77247    * 05 50 43.13500      05 50 49.45056    
                     From catalog imbedded in main SCHED input file.
 
 * 1422+231          14 22 20.922247   * 14 24 38.042500     14 24 42.081098   
                     23 09 32.86642    * 22 56 00.96800      22 55 47.00565    
                     From catalog imbedded in main SCHED input file.
 
   J1436+2321        14 34 25.408295   * 14 36 40.983200     14 36 45.037632   
 * 1434+235          23 34 03.17032    * 23 21 03.28700      23 20 49.81939    
   J1436+23          /homes/ros/vlbi/sched/catalogs/sources.vlba
                     JVAS - Wilkinson et al. 1998, mnras, 300, 790; S8.4GHz=   634 mJy
 
   J1642+3948        16 41 17.606463   * 16 42 58.810200     16 43 02.669490   
   1641+399          39 54 10.81592    * 39 48 36.99500      39 48 29.95622    
 * 3C345             /homes/ros/vlbi/sched/catalogs/sources.vlba
   J1642+39          JVAS - Patnaik et al. 1992, mnras, 254, 655;   S8.4GHz=  5182 mJy
 
   J1800+7828        18 03 39.193553   * 18 00 45.683929     18 00 48.376406   
 * 1803+784          78 27 54.29752    * 78 28 04.01847      78 27 59.29256    
   J1800+78          /homes/ros/vlbi/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998
 
   J1927+7358        19 28 49.350252   * 19 27 48.495205     19 27 51.071428   
 * 1928+738          73 51 44.92753    * 73 58 01.56997      73 57 58.12757    
   J1927+73          /homes/ros/vlbi/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998
 
 
 
  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0411+05             18.1
   0357+057            19.5
   1422+231           123.6
   1434+235           124.9
   3C345              117.9
   1803+784            78.6
   1928+738            80.1
 
  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

