  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
 Exp. Code:  GB080   


Schedule Version:       7.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       M. Bietenholz

Address:  York University
          Toronto, ON M3J 1P3
          Canada
 

Phone:    +27-12-301-3100 (work)
EMAIL:    michael@yorku.ca
Fax:      +1-416-736-5516
Phone during observation: +27-76-882-3872 (cell)

Observing mode: 22 GHz; 2 Gbps @ NRAO & EB, 1 Gbps @ EVN

Notes:
          Fringe finder  : 3C84, J0237+2848
          Pol. Calibrator: 3C84
          Amplitude check: 3C66A

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 Next scan frequencies:  22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
 Next BBC frequencies:     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

08 55 50  3C454.3      19 06 51  36.3  91.8 -3.8     -63.6     0        0   08 55 50
09 00 00  ---          19 11 02  37.2  92.4 -3.7     -63.6   250       64   08 55 50

 ---------- ***This a 10-min gap for EB Pointing/focus 8 ----------

09 02 00  3C66A        19 13 02   9.1  44.8 -7.2     -56.1    56       64   09 02 00
09 03 30  ---          19 14 32   9.3  44.9 -7.2     -56.3    90       88   09 02 00

09 04 10  SN1986J      19 15 12   9.0  45.6 -7.1     -56.4    32       88   09 04 10
09 05 40  ---          19 16 42   9.2  45.8 -7.1     -56.6    90      111   09 04 10

09 05 40  3C66A        19 16 42   9.6  45.1 -7.1     -56.7    -8      111   09 05 48
09 06 40  ---          19 17 43   9.8  45.2 -7.1     -56.8    52      124   09 05 48

09 06 40  SN1986J      19 17 43   9.4  45.9 -7.1     -56.8    -8      124   09 06 48
09 08 30  ---          19 19 33   9.7  46.0 -7.1     -57.0   102      150   09 06 48

09 08 30  3C66A        19 19 33  10.0  45.4 -7.1     -57.1    -8      150   09 08 38
09 09 30  ---          19 20 33  10.2  45.5 -7.1     -57.3    52      164   09 08 38

09 09 30  SN1986J      19 20 33   9.8  46.1 -7.1     -57.2    -8      164   09 09 38
09 11 20  ---          19 22 23  10.1  46.3 -7.0     -57.5   102      190   09 09 38

09 12 00  3C66A        19 23 03  10.6  45.8 -7.0     -57.6    32      190   09 12 00
09 13 30  ---          19 24 34  10.8  45.9 -7.0     -57.9    90      213   09 12 00

09 14 10  SN1986J      19 25 14  10.6  46.6 -7.0     -57.9    32      213   09 14 10
09 15 30  ---          19 26 34  10.8  46.8 -7.0     -58.1    80      234   09 14 10

09 15 30  3C66A        19 26 34  11.1  46.1 -7.0     -58.2    -8      234   09 15 38
09 16 50  ---          19 27 54  11.3  46.3 -6.9     -58.4    72      252   09 15 38

09 16 50  SN1986J      19 27 54  11.0  46.9 -6.9     -58.3    -8      252   09 16 58
09 18 40  ---          19 29 45  11.3  47.1 -6.9     -58.6   102      279   09 16 58

09 18 40  3C66A        19 29 45  11.6  46.4 -6.9     -58.7    -8      279   09 18 48
09 20 00  ---          19 31 05  11.8  46.6 -6.9     -58.9    72      297   09 18 48

09 20 00  SN1986J      19 31 05  11.5  47.2 -6.9     -58.8    -8      297   09 20 08
09 21 50  ---          19 32 55  11.8  47.4 -6.8     -59.0   102      324   09 20 08
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

09 21 50  3C66A        19 32 55  12.1  46.7 -6.8     -59.1    -8      324   09 21 58
09 23 10  ---          19 34 15  12.3  46.9 -6.8     -59.3    72      342   09 21 58

09 23 10  SN1986J      19 34 15  12.0  47.5 -6.8     -59.2    -8      342   09 23 18
09 25 00  ---          19 36 06  12.3  47.7 -6.8     -59.5   102      368   09 23 18

09 25 00  3C66A        19 36 06  12.6  47.0 -6.8     -59.6    -8      368   09 25 08
09 26 20  ---          19 37 26  12.8  47.2 -6.8     -59.8    72      387   09 25 08

09 26 20  SN1986J      19 37 26  12.5  47.8 -6.8     -59.7    -8      387   09 26 28
09 28 10  ---          19 39 16  12.8  48.0 -6.7     -60.0   102      413   09 26 28

09 28 50  3C66A        19 39 56  13.2  47.4 -6.7     -60.2    32      413   09 28 50
09 30 10  ---          19 41 16  13.4  47.5 -6.7     -60.4    80      434   09 28 50

09 30 50  SN1986J      19 41 57  13.2  48.2 -6.7     -60.4    32      434   09 30 50
09 32 40  ---          19 43 47  13.5  48.4 -6.7     -60.6   110      462   09 30 50

09 32 40  3C66A        19 43 47  13.8  47.8 -6.7     -60.8    -8      462   09 32 48
09 34 00  ---          19 45 07  14.0  47.9 -6.6     -61.0    72      481   09 32 48

09 34 00  SN1986J      19 45 07  13.7  48.5 -6.6     -60.8    -8      481   09 34 08
09 35 50  ---          19 46 57  14.0  48.7 -6.6     -61.1   102      507   09 34 08

09 35 50  3C66A        19 46 57  14.3  48.1 -6.6     -61.2    -8      507   09 35 58
09 37 10  ---          19 48 18  14.6  48.2 -6.6     -61.4    72      526   09 35 58

09 37 10  SN1986J      19 48 18  14.2  48.8 -6.6     -61.3    -8      526   09 37 18
09 39 00  ---          19 50 08  14.5  49.0 -6.6     -61.6   102      552   09 37 18

09 39 00  3C66A        19 50 08  14.9  48.3 -6.6     -61.7    -8      552   09 39 08
09 40 20  ---          19 51 28  15.1  48.5 -6.5     -61.9    72      570   09 39 08

09 40 20  SN1986J      19 51 28  14.8  49.1 -6.5     -61.8    -8      570   09 40 28
09 42 10  ---          19 53 18  15.1  49.3 -6.5     -62.0   102      597   09 40 28

 ---------- ***This a 10-min gap for EB Pointing/focus 9 ----------

09 42 50  3C66A        19 53 59  15.5  48.7 -6.5     -62.3    32      597   09 42 50
09 44 30  ---          19 55 39  15.7  48.8 -6.5     -62.5   100      622   09 42 50

09 45 10  SN1986J      19 56 19  15.6  49.5 -6.5     -62.5    32      622   09 45 10
09 47 10  ---          19 58 19  15.9  49.7 -6.4     -62.8   120      653   09 45 10
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

09 47 10  3C66A        19 58 19  16.2  49.1 -6.4     -62.9    -8      653   09 47 18
09 48 30  ---          19 59 39  16.4  49.2 -6.4     -63.1    72      672   09 47 18

09 48 30  SN1986J      19 59 39  16.1  49.8 -6.4     -63.0    -8      672   09 48 38
09 50 20  ---          20 01 30  16.4  50.0 -6.4     -63.2   102      698   09 48 38

09 50 20  3C66A        20 01 30  16.7  49.3 -6.4     -63.4    -8      698   09 50 28
09 51 40  ---          20 02 50  16.9  49.4 -6.3     -63.6    72      717   09 50 28

09 51 40  SN1986J      20 02 50  16.6  50.1 -6.3     -63.4    -8      717   09 51 48
09 53 30  ---          20 04 40  16.9  50.3 -6.3     -63.7   102      743   09 51 48

09 54 10  3C66A        20 05 20  17.3  49.7 -6.3     -63.9    32      743   09 54 10
09 55 40  ---          20 06 51  17.6  49.8 -6.3     -64.2    90      766   09 54 10

09 56 20  SN1986J      20 07 31  17.4  50.5 -6.3     -64.1    32      766   09 56 20
09 57 50  ---          20 09 01  17.6  50.6 -6.2     -64.3    90      789   09 56 20

09 57 50  3C66A        20 09 01  17.9  50.0 -6.2     -64.5    -8      789   09 57 58
09 59 10  ---          20 10 21  18.1  50.1 -6.2     -64.7    72      808   09 57 58

09 59 10  SN1986J      20 10 21  17.9  50.8 -6.2     -64.5    -8      808   09 59 18
10 01 00  ---          20 12 12  18.2  50.9 -6.2     -64.8   102      834   09 59 18

10 01 00  3C66A        20 12 12  18.5  50.2 -6.2     -64.9    -8      834   10 01 08
10 02 20  ---          20 13 32  18.7  50.3 -6.2     -65.1    72      853   10 01 08

10 02 20  SN1986J      20 13 32  18.4  51.0 -6.2     -64.9    -8      853   10 02 28
10 04 10  ---          20 15 22  18.7  51.2 -6.1     -65.2   102      879   10 02 28

10 04 10  3C66A        20 15 22  19.0  50.5 -6.1     -65.4    -8      879   10 04 18
10 05 30  ---          20 16 42  19.2  50.6 -6.1     -65.6    72      898   10 04 18

10 05 30  SN1986J      20 16 42  18.9  51.3 -6.1     -65.4    -8      898   10 05 38
10 07 20  ---          20 18 33  19.2  51.4 -6.1     -65.7   102      924   10 05 38

10 08 00  3C66A        20 19 13  19.6  50.8 -6.1     -66.0    32      924   10 08 00
10 09 20  ---          20 20 33  19.8  50.9 -6.1     -66.2    80      945   10 08 00

10 10 00  SN1986J      20 21 13  19.7  51.6 -6.0     -66.0    32      945   10 10 00
10 11 30  ---          20 22 43  19.9  51.8 -6.0     -66.3    90      968   10 10 00

10 11 30  3C66A        20 22 43  20.2  51.1 -6.0     -66.5    -8      968   10 11 38
10 12 50  ---          20 24 03  20.4  51.2 -6.0     -66.7    72      986   10 11 38
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

10 12 50  SN1986J      20 24 03  20.2  51.9 -6.0     -66.4    -8      986   10 12 58
10 14 40  ---          20 25 54  20.5  52.0 -6.0     -66.7   102     1013   10 12 58

10 14 40  3C66A        20 25 54  20.7  51.3 -6.0     -66.9    -8     1013   10 14 48
10 16 00  ---          20 27 14  21.0  51.4 -5.9     -67.1    72     1031   10 14 48

10 16 00  SN1986J      20 27 14  20.7  52.1 -5.9     -66.9    -8     1031   10 16 08
10 17 50  ---          20 29 04  21.0  52.3 -5.9     -67.1   102     1057   10 16 08

10 17 50  3C66A        20 29 04  21.3  51.5 -5.9     -67.4    -8     1057   10 17 58
10 19 10  ---          20 30 25  21.5  51.6 -5.9     -67.6    72     1076   10 17 58

10 19 10  SN1986J      20 30 25  21.2  52.4 -5.9     -67.3    -8     1076   10 19 18
10 21 00  ---          20 32 15  21.6  52.5 -5.9     -67.6   102     1102   10 19 18

10 21 40  3C66A        20 32 55  21.9  51.8 -5.8     -67.9    32     1102   10 21 40
10 23 00  ---          20 34 15  22.1  51.9 -5.8     -68.1    80     1123   10 21 40

10 23 40  SN1986J      20 34 55  22.0  52.7 -5.8     -68.0    32     1123   10 23 40
10 25 10  ---          20 36 26  22.3  52.8 -5.8     -68.2    90     1146   10 23 40

10 25 10  3C66A        20 36 26  22.5  52.1 -5.8     -68.4    -8     1146   10 25 18
10 26 30  ---          20 37 46  22.7  52.2 -5.8     -68.6    72     1165   10 25 18

10 26 30  SN1986J      20 37 46  22.5  52.9 -5.8     -68.4    -8     1165   10 26 38
10 28 20  ---          20 39 36  22.8  53.0 -5.7     -68.6   102     1191   10 26 38

10 28 20  3C66A        20 39 36  23.1  52.3 -5.7     -68.9    -8     1191   10 28 28
10 29 40  ---          20 40 56  23.3  52.4 -5.7     -69.1    72     1209   10 28 28

10 29 40  SN1986J      20 40 56  23.1  53.1 -5.7     -68.8    -8     1209   10 29 48
10 31 30  ---          20 42 47  23.4  53.3 -5.7     -69.1   102     1236   10 29 48

10 31 30  3C66A        20 42 47  23.6  52.5 -5.7     -69.3    -8     1236   10 31 38
10 32 50  ---          20 44 07  23.8  52.6 -5.7     -69.5    72     1254   10 31 38

10 32 50  SN1986J      20 44 07  23.6  53.4 -5.7     -69.3    -8     1254   10 32 58
10 34 40  ---          20 45 57  23.9  53.5 -5.6     -69.5   102     1280   10 32 58

 ---------- ***This a 10-min gap for EB Pointing/focus 10 ----------

10 35 20  3C66A        20 46 37  24.2  52.8 -5.6     -69.9    32     1280   10 35 20
10 36 50  ---          20 48 07  24.5  52.9 -5.6     -70.1    90     1304   10 35 20
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

10 37 30  SN1986J      20 48 48  24.4  53.7 -5.6     -69.9    32     1304   10 37 30
10 39 00  ---          20 50 18  24.7  53.8 -5.6     -70.1    90     1327   10 37 30

10 39 40  3C66A        20 50 58  25.0  53.1 -5.5     -70.5    32     1327   10 39 40
10 41 00  ---          20 52 18  25.2  53.2 -5.5     -70.7    80     1347   10 39 40

10 41 00  SN1986J      20 52 18  25.0  53.9 -5.5     -70.4    -8     1347   10 41 08
10 42 50  ---          20 54 08  25.3  54.1 -5.5     -70.7   102     1374   10 41 08

10 42 50  3C66A        20 54 08  25.5  53.3 -5.5     -71.0    -8     1374   10 42 58
10 44 10  ---          20 55 29  25.8  53.4 -5.5     -71.2    72     1392   10 42 58

10 44 10  SN1986J      20 55 29  25.6  54.2 -5.5     -70.9    -8     1392   10 44 18
10 46 00  ---          20 57 19  25.9  54.3 -5.4     -71.1   102     1419   10 44 18

10 46 30  3C66A        20 57 49  26.2  53.6 -5.4     -71.5    22     1419   10 46 30
10 47 50  ---          20 59 09  26.4  53.6 -5.4     -71.7    80     1439   10 46 30

10 48 20  SN1986J      20 59 39  26.3  54.4 -5.4     -71.4    22     1439   10 48 20
10 50 00  ---          21 01 20  26.6  54.5 -5.4     -71.7   100     1465   10 48 20

10 50 00  3C66A        21 01 20  26.8  53.8 -5.4     -72.0    -8     1465   10 50 08
10 51 20  ---          21 02 40  27.0  53.9 -5.4     -72.2    72     1483   10 50 08

10 51 20  SN1986J      21 02 40  26.8  54.6 -5.3     -71.9    -8     1483   10 51 28
10 53 10  ---          21 04 30  27.1  54.7 -5.3     -72.1   102     1510   10 51 28

10 53 10  3C66A        21 04 30  27.3  54.0 -5.3     -72.4    -8     1510   10 53 18
10 54 30  ---          21 05 50  27.6  54.1 -5.3     -72.6    72     1528   10 53 18

10 54 30  SN1986J      21 05 50  27.4  54.8 -5.3     -72.3    -8     1528   10 54 38
10 56 20  ---          21 07 41  27.7  54.9 -5.3     -72.6   102     1555   10 54 38

10 56 20  3C66A        21 07 41  27.9  54.2 -5.3     -72.9    -8     1555   10 56 28
10 57 40  ---          21 09 01  28.1  54.3 -5.2     -73.1    72     1573   10 56 28

10 57 40  SN1986J      21 09 01  27.9  55.0 -5.2     -72.7    -8     1573   10 57 48
10 59 30  ---          21 10 51  28.3  55.1 -5.2     -73.0   102     1599   10 57 48

11 00 00  3C66A        21 11 21  28.5  54.4 -5.2     -73.4    22     1599   11 00 00
11 01 20  ---          21 12 41  28.8  54.5 -5.2     -73.6    80     1620   11 00 00

11 01 50  SN1986J      21 13 12  28.7  55.3 -5.2     -73.3    22     1620   11 01 50
11 03 30  ---          21 14 52  29.0  55.4 -5.1     -73.6   100     1646   11 01 50
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

11 03 30  3C66A        21 14 52  29.1  54.6 -5.1     -73.9    -8     1646   11 03 38
11 04 50  ---          21 16 12  29.4  54.7 -5.1     -74.1    72     1664   11 03 38

11 04 50  SN1986J      21 16 12  29.2  55.5 -5.1     -73.7    -8     1664   11 04 58
11 06 40  ---          21 18 02  29.5  55.6 -5.1     -74.0   102     1691   11 04 58

11 06 40  3C66A        21 18 02  29.7  54.8 -5.1     -74.4    -8     1691   11 06 48
11 08 00  ---          21 19 23  29.9  54.9 -5.1     -74.6    72     1709   11 06 48

11 08 00  SN1986J      21 19 23  29.8  55.7 -5.1     -74.2    -8     1709   11 08 08
11 09 50  ---          21 21 13  30.1  55.8 -5.0     -74.4   102     1735   11 08 08

11 09 50  3C66A        21 21 13  30.3  55.0 -5.0     -74.8    -8     1735   11 09 58
11 11 10  ---          21 22 33  30.5  55.0 -5.0     -75.0    72     1754   11 09 58

11 11 10  SN1986J      21 22 33  30.3  55.8 -5.0     -74.6    -8     1754   11 11 18
11 13 00  ---          21 24 23  30.7  55.9 -5.0     -74.9   102     1780   11 11 18

11 13 30  3C66A        21 24 53  30.9  55.2 -5.0     -75.3    22     1780   11 13 30
11 14 50  ---          21 26 14  31.1  55.2 -5.0     -75.5    80     1801   11 13 30

11 15 20  SN1986J      21 26 44  31.1  56.1 -4.9     -75.2    22     1801   11 15 20
11 16 50  ---          21 28 14  31.4  56.1 -4.9     -75.4    90     1824   11 15 20

11 16 50  3C66A        21 28 14  31.5  55.3 -4.9     -75.8    -8     1824   11 16 58
11 18 10  ---          21 29 34  31.7  55.4 -4.9     -76.0    72     1843   11 16 58

11 18 10  SN1986J      21 29 34  31.6  56.2 -4.9     -75.6    -8     1843   11 18 18
11 20 00  ---          21 31 25  31.9  56.3 -4.9     -75.9   102     1869   11 18 18

11 20 00  3C66A        21 31 25  32.1  55.5 -4.9     -76.3    -8     1869   11 20 08
11 21 20  ---          21 32 45  32.3  55.6 -4.9     -76.5    72     1887   11 20 08

11 21 20  SN1986J      21 32 45  32.2  56.4 -4.8     -76.1    -8     1887   11 21 28
11 23 10  ---          21 34 35  32.5  56.5 -4.8     -76.3   102     1914   11 21 28

11 23 10  3C66A        21 34 35  32.6  55.7 -4.8     -76.7    -8     1914   11 23 18
11 24 30  ---          21 35 55  32.9  55.7 -4.8     -76.9    72     1932   11 23 18

11 24 30  SN1986J      21 35 55  32.7  56.6 -4.8     -76.5    -8     1932   11 24 38
11 26 20  ---          21 37 46  33.1  56.6 -4.8     -76.8   102     1959   11 24 38
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- ***This a 10-min gap for EB Pointing/focus 11 ----------

11 27 00  3C66A        21 38 26  33.3  55.9 -4.8     -77.3    32     1959   11 27 00
11 28 30  ---          21 39 56  33.6  55.9 -4.7     -77.5    90     1982   11 27 00

11 29 10  SN1986J      21 40 36  33.6  56.8 -4.7     -77.2    32     1982   11 29 10
11 30 40  ---          21 42 06  33.8  56.9 -4.7     -77.4    90     2005   11 29 10

11 31 20  3C66A        21 42 46  34.1  56.1 -4.7     -77.9    32     2005   11 31 20
11 32 40  ---          21 44 07  34.3  56.1 -4.7     -78.1    80     2026   11 31 20

11 32 40  SN1986J      21 44 07  34.2  57.0 -4.7     -77.7    -8     2026   11 32 48
11 34 30  ---          21 45 57  34.5  57.0 -4.6     -77.9   102     2052   11 32 48

11 34 30  3C66A        21 45 57  34.7  56.2 -4.6     -78.4    -8     2052   11 34 38
11 35 50  ---          21 47 17  34.9  56.3 -4.6     -78.6    72     2070   11 34 38

11 35 50  SN1986J      21 47 17  34.8  57.1 -4.6     -78.1    -8     2070   11 35 58
11 37 40  ---          21 49 07  35.1  57.2 -4.6     -78.4   102     2097   11 35 58

11 38 10  3C66A        21 49 37  35.3  56.4 -4.6     -78.9    22     2097   11 38 10
11 39 40  ---          21 51 08  35.6  56.4 -4.5     -79.1    90     2120   11 38 10

11 40 10  SN1986J      21 51 38  35.6  57.3 -4.5     -78.7    22     2120   11 40 10
11 41 50  ---          21 53 18  35.9  57.4 -4.5     -79.0   100     2146   11 40 10

11 41 50  3C66A        21 53 18  36.0  56.5 -4.5     -79.5    -8     2146   11 41 58
11 43 10  ---          21 54 38  36.2  56.6 -4.5     -79.7    72     2164   11 41 58

11 43 10  SN1986J      21 54 38  36.1  57.4 -4.5     -79.2    -8     2164   11 43 18
11 45 00  ---          21 56 29  36.4  57.5 -4.5     -79.4   102     2190   11 43 18

11 45 00  3C66A        21 56 29  36.5  56.6 -4.5     -79.9    -8     2190   11 45 08
11 46 20  ---          21 57 49  36.8  56.7 -4.4     -80.1    72     2209   11 45 08

11 46 20  SN1986J      21 57 49  36.7  57.6 -4.4     -79.6    -8     2209   11 46 28
11 48 10  ---          21 59 39  37.0  57.6 -4.4     -79.9   102     2235   11 46 28

11 48 10  3C66A        21 59 39  37.1  56.8 -4.4     -80.4    -8     2235   11 48 18
11 49 30  ---          22 00 59  37.4  56.8 -4.4     -80.6    72     2254   11 48 18

11 49 30  SN1986J      22 00 59  37.3  57.7 -4.4     -80.1    -8     2254   11 49 38
11 51 20  ---          22 02 50  37.6  57.8 -4.3     -80.3   102     2280   11 49 38
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

11 51 50  3C66A        22 03 20  37.8  56.9 -4.3     -80.9    22     2280   11 51 50
11 53 10  ---          22 04 40  38.0  57.0 -4.3     -81.1    80     2301   11 51 50

11 53 40  SN1986J      22 05 10  38.0  57.9 -4.3     -80.7    22     2301   11 53 40
11 55 10  ---          22 06 40  38.3  57.9 -4.3     -80.9    90     2324   11 53 40

11 55 10  3C66A        22 06 40  38.4  57.0 -4.3     -81.4    -8     2324   11 55 18
11 56 30  ---          22 08 01  38.6  57.1 -4.3     -81.6    72     2342   11 55 18

11 56 30  SN1986J      22 08 01  38.5  58.0 -4.3     -81.1    -8     2342   11 56 38
11 58 20  ---          22 09 51  38.9  58.0 -4.2     -81.4   102     2369   11 56 38

11 58 20  3C66A        22 09 51  39.0  57.1 -4.2     -81.9    -8     2369   11 58 28
11 59 40  ---          22 11 11  39.2  57.2 -4.2     -82.1    72     2387   11 58 28

11 59 40  SN1986J      22 11 11  39.1  58.1 -4.2     -81.6    -8     2387   11 59 48
12 01 30  ---          22 13 01  39.5  58.1 -4.2     -81.8   102     2414   11 59 48

12 01 30  3C66A        22 13 01  39.5  57.2 -4.2     -82.4    -8     2414   12 01 38
12 02 50  ---          22 14 22  39.8  57.3 -4.2     -82.6    72     2432   12 01 38

12 02 50  SN1986J      22 14 22  39.7  58.2 -4.2     -82.0    -8     2432   12 02 58
12 04 40  ---          22 16 12  40.0  58.3 -4.1     -82.3   102     2458   12 02 58

12 05 10  3C66A        22 16 42  40.2  57.4 -4.1     -82.9    22     2458   12 05 10
12 06 30  ---          22 18 02  40.4  57.4 -4.1     -83.1    80     2479   12 05 10

12 07 00  SN1986J      22 18 32  40.5  58.3 -4.1     -82.6    22     2479   12 07 00
12 08 30  ---          22 20 02  40.7  58.4 -4.1     -82.9    90     2502   12 07 00

12 08 30  3C66A        22 20 02  40.8  57.4 -4.1     -83.5    -8     2502   12 08 38
12 09 50  ---          22 21 23  41.0  57.5 -4.0     -83.7    72     2521   12 08 38

12 09 50  SN1986J      22 21 23  41.0  58.4 -4.0     -83.1    -8     2521   12 09 58
12 11 40  ---          22 23 13  41.3  58.5 -4.0     -83.3   102     2547   12 09 58

12 11 40  3C66A        22 23 13  41.4  57.5 -4.0     -83.9    -8     2547   12 11 48
12 13 00  ---          22 24 33  41.6  57.6 -4.0     -84.1    72     2566   12 11 48

12 13 00  SN1986J      22 24 33  41.6  58.5 -4.0     -83.5    -8     2566   12 13 08
12 14 50  ---          22 26 24  41.9  58.6 -4.0     -83.8   102     2592   12 13 08

12 14 50  3C66A        22 26 24  41.9  57.6 -4.0     -84.4    -8     2592   12 14 58
12 16 10  ---          22 27 44  42.2  57.6 -3.9     -84.6    72     2610   12 14 58
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

12 16 10  SN1986J      22 27 44  42.1  58.6 -3.9     -84.0    -8     2610   12 16 18
12 18 00  ---          22 29 34  42.5  58.6 -3.9     -84.3   102     2637   12 16 18

 ---------- ***This a 10-min gap for EB Pointing/focus 12 ----------

12 18 40  3C66A        22 30 14  42.6  57.7 -3.9     -85.0    32     2637   12 18 40
12 20 10  ---          22 31 44  42.9  57.7 -3.9     -85.3    90     2660   12 18 40

12 20 50  SN1986J      22 32 25  43.0  58.7 -3.9     -84.7    32     2660   12 20 50
12 22 20  ---          22 33 55  43.3  58.7 -3.8     -85.0    90     2683   12 20 50

12 23 00  3C66A        22 34 35  43.4  57.8 -3.8     -85.7    32     2683   12 23 00
12 24 20  ---          22 35 55  43.7  57.8 -3.8     -85.9    80     2704   12 23 00

12 24 20  SN1986J      22 35 55  43.7  58.8 -3.8     -85.3    -8     2704   12 24 28
12 26 10  ---          22 37 45  44.0  58.8 -3.8     -85.6   102     2730   12 24 28

12 26 10  3C66A        22 37 45  44.0  57.8 -3.8     -86.2    -8     2730   12 26 18
12 27 30  ---          22 39 06  44.3  57.9 -3.7     -86.4    72     2748   12 26 18

12 27 30  SN1986J      22 39 06  44.2  58.8 -3.7     -85.8    -8     2748   12 27 38
12 29 20  ---          22 40 56  44.6  58.9 -3.7     -86.1   102     2775   12 27 38

12 29 50  3C66A        22 41 26  44.7  57.9 -3.7     -86.8    22     2775   12 29 50
12 31 20  ---          22 42 56  45.0  57.9 -3.7     -87.0    90     2798   12 29 50

12 31 50  SN1986J      22 43 26  45.0  58.9 -3.7     -86.4    22     2798   12 31 50
12 33 20  ---          22 44 57  45.3  58.9 -3.6     -86.7    90     2821   12 31 50

12 33 20  3C66A        22 44 57  45.3  57.9 -3.6     -87.4    -8     2821   12 33 28
12 34 40  ---          22 46 17  45.6  58.0 -3.6     -87.6    72     2840   12 33 28

12 34 40  SN1986J      22 46 17  45.6  59.0 -3.6     -86.9    -8     2840   12 34 48
12 36 30  ---          22 48 07  45.9  59.0 -3.6     -87.2   102     2866   12 34 48

12 36 30  3C66A        22 48 07  45.9  58.0 -3.6     -87.9    -8     2866   12 36 38
12 37 50  ---          22 49 27  46.1  58.0 -3.6     -88.1    72     2885   12 36 38

12 37 50  SN1986J      22 49 27  46.1  59.0 -3.6     -87.4    -8     2885   12 37 58
12 39 40  ---          22 51 18  46.5  59.0 -3.5     -87.7   102     2911   12 37 58

12 39 40  3C66A        22 51 18  46.5  58.0 -3.5     -88.4    -8     2911   12 39 48
12 41 00  ---          22 52 38  46.7  58.0 -3.5     -88.6    72     2929   12 39 48
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

12 41 00  SN1986J      22 52 38  46.7  59.0 -3.5     -87.9    -8     2929   12 41 08
12 42 50  ---          22 54 28  47.1  59.1 -3.5     -88.2   102     2956   12 41 08

12 43 20  3C66A        22 54 58  47.2  58.0 -3.5     -89.0    22     2956   12 43 20
12 44 40  ---          22 56 18  47.4  58.0 -3.5     -89.2    80     2976   12 43 20

12 45 10  SN1986J      22 56 49  47.5  59.1 -3.4     -88.6    22     2976   12 45 10
12 46 40  ---          22 58 19  47.8  59.1 -3.4     -88.8    90     2999   12 45 10

12 46 40  3C66A        22 58 19  47.8  58.0 -3.4     -89.6    -8     2999   12 46 48
12 48 00  ---          22 59 39  48.0  58.0 -3.4     -89.8    72     3018   12 46 48

12 48 00  SN1986J      22 59 39  48.0  59.1 -3.4     -89.1    -8     3018   12 48 08
12 49 50  ---          23 01 29  48.4  59.1 -3.4     -89.4   102     3044   12 48 08

12 49 50  3C66A        23 01 29  48.3  58.0 -3.4     -90.1    -8     3044   12 49 58
12 51 10  ---          23 02 49  48.6  58.0 -3.3     -90.4    72     3063   12 49 58

12 51 10  SN1986J      23 02 49  48.6  59.1 -3.3     -89.6    -8     3063   12 51 18
12 53 00  ---          23 04 40  49.0  59.1 -3.3     -89.9   102     3089   12 51 18

12 53 00  3C66A        23 04 40  48.9  58.0 -3.3     -90.7    -8     3089   12 53 08
12 54 20  ---          23 06 00  49.2  58.0 -3.3     -90.9    72     3108   12 53 08

12 54 20  SN1986J      23 06 00  49.2  59.1 -3.3     -90.1    -8     3108   12 54 28
12 56 10  ---          23 07 50  49.5  59.1 -3.3     -90.4   102     3134   12 54 28

12 56 40  3C66A        23 08 20  49.6  58.0 -3.3     -91.3    22     3134   12 56 40
12 58 00  ---          23 09 41  49.8  58.0 -3.2     -91.6    80     3155   12 56 40

12 58 30  SN1986J      23 10 11  50.0  59.1 -3.2     -90.8    22     3155   12 58 30
13 00 00  ---          23 11 41  50.2  59.1 -3.2     -91.1    90     3178   12 58 30

13 00 00  3C66A        23 11 41  50.2  58.0 -3.2     -91.9    -8     3178   13 00 08
13 01 20  ---          23 13 01  50.4  58.0 -3.2     -92.1    72     3196   13 00 08

13 01 20  SN1986J      23 13 01  50.5  59.1 -3.2     -91.3    -8     3196   13 01 28
13 03 10  ---          23 14 51  50.8  59.1 -3.1     -91.6   102     3223   13 01 28

13 03 10  3C66A        23 14 51  50.8  58.0 -3.1     -92.5    -8     3223   13 03 18
13 04 30  ---          23 16 12  51.0  57.9 -3.1     -92.7    72     3241   13 03 18

13 04 30  SN1986J      23 16 12  51.1  59.1 -3.1     -91.9    -8     3241   13 04 38
13 06 20  ---          23 18 02  51.4  59.0 -3.1     -92.2   102     3267   13 04 38
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

13 06 20  3C66A        23 18 02  51.4  57.9 -3.1     -93.1    -8     3267   13 06 28
13 07 40  ---          23 19 22  51.6  57.9 -3.1     -93.3    72     3286   13 06 28

13 07 40  SN1986J      23 19 22  51.7  59.0 -3.1     -92.4    -8     3286   13 07 48
13 09 30  ---          23 21 13  52.0  59.0 -3.0     -92.8   102     3312   13 07 48

 ---------- ***This a 10-min gap for EB Pointing/focus 13 ----------

13 10 10  3C66A        23 21 53  52.1  57.8 -3.0     -93.8    32     3312   13 10 10
13 11 40  ---          23 23 23  52.3  57.8 -3.0     -94.0    90     3335   13 10 10

13 12 20  SN1986J      23 24 03  52.5  58.9 -3.0     -93.3    32     3335   13 12 20
13 13 50  ---          23 25 33  52.8  58.9 -3.0     -93.6    90     3359   13 12 20

13 14 30  3C66A        23 26 13  52.9  57.7 -3.0     -94.6    32     3359   13 14 30
13 15 50  ---          23 27 34  53.1  57.7 -2.9     -94.8    80     3379   13 14 30

13 15 50  SN1986J      23 27 34  53.2  58.9 -2.9     -93.9    -8     3379   13 15 58
13 17 40  ---          23 29 24  53.5  58.8 -2.9     -94.3   102     3405   13 15 58

13 17 40  3C66A        23 29 24  53.4  57.7 -2.9     -95.2    -9     3405   13 17 49
13 19 00  ---          23 30 44  53.7  57.6 -2.9     -95.4    71     3424   13 17 49

13 19 00  SN1986J      23 30 44  53.8  58.8 -2.9     -94.5    -9     3424   13 19 09
13 20 50  ---          23 32 34  54.1  58.8 -2.9     -94.9   101     3450   13 19 09

13 21 20  3C66A        23 33 04  54.1  57.6 -2.8     -95.9    21     3450   13 21 20
13 22 50  ---          23 34 35  54.4  57.5 -2.8     -96.2    90     3473   13 21 20

13 23 20  SN1986J      23 35 05  54.6  58.7 -2.8     -95.3    21     3473   13 23 20
13 24 50  ---          23 36 35  54.8  58.6 -2.8     -95.6    90     3496   13 23 20

13 24 50  3C66A        23 36 35  54.7  57.4 -2.8     -96.6    -9     3496   13 24 59
13 26 10  ---          23 37 55  55.0  57.4 -2.8     -96.9    71     3514   13 24 59

13 26 10  SN1986J      23 37 55  55.1  58.6 -2.8     -95.9    -9     3514   13 26 19
13 28 00  ---          23 39 46  55.4  58.5 -2.7     -96.3   101     3540   13 26 19

13 28 00  3C66A        23 39 46  55.3  57.3 -2.7     -97.2    -9     3540   13 28 09
13 29 20  ---          23 41 06  55.6  57.3 -2.7     -97.5    71     3559   13 28 09

13 29 20  SN1986J      23 41 06  55.7  58.5 -2.7     -96.5    -9     3559   13 29 29
13 31 10  ---          23 42 56  56.0  58.4 -2.7     -96.9   101     3585   13 29 29
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

13 31 10  3C66A        23 42 56  55.9  57.2 -2.7     -97.9    -9     3585   13 31 19
13 32 30  ---          23 44 16  56.1  57.1 -2.7     -98.2    71     3603   13 31 19

13 32 30  SN1986J      23 44 16  56.2  58.4 -2.7     -97.2    -9     3603   13 32 39
13 34 20  ---          23 46 07  56.6  58.3 -2.6     -97.5   101     3629   13 32 39

13 34 50  3C66A        23 46 37  56.5  57.0 -2.6     -98.7    21     3629   13 34 50
13 36 10  ---          23 47 57  56.8  56.9 -2.6     -99.0    80     3650   13 34 50

13 36 40  SN1986J      23 48 27  57.0  58.2 -2.6     -98.0    21     3650   13 36 40
13 38 10  ---          23 49 57  57.3  58.1 -2.6     -98.3    90     3673   13 36 40

13 38 10  3C66A        23 49 57  57.2  56.8 -2.6     -99.4    -9     3673   13 38 19
13 39 30  ---          23 51 17  57.4  56.8 -2.5     -99.7    71     3691   13 38 19

13 39 30  SN1986J      23 51 17  57.5  58.0 -2.5     -98.6    -9     3691   13 39 39
13 41 20  ---          23 53 08  57.9  57.9 -2.5     -99.0   101     3717   13 39 39

13 41 20  3C66A        23 53 08  57.7  56.6 -2.5    -100.1    -9     3717   13 41 29
13 42 40  ---          23 54 28  58.0  56.6 -2.5    -100.4    71     3736   13 41 29

13 42 40  SN1986J      23 54 28  58.1  57.9 -2.5     -99.3    -9     3736   13 42 49
13 44 30  ---          23 56 18  58.4  57.8 -2.5     -99.7   101     3762   13 42 49

13 44 30  3C66A        23 56 18  58.3  56.4 -2.5    -100.8    -9     3762   13 44 39
13 45 50  ---          23 57 38  58.5  56.4 -2.4    -101.1    71     3780   13 44 39

13 45 50  SN1986J      23 57 38  58.7  57.7 -2.4    -100.0    -9     3780   13 45 59
13 47 40  ---          23 59 29  59.0  57.6 -2.4    -100.4   101     3806   13 45 59

13 48 10  3C66A        23 59 59  59.0  56.2 -2.4    -101.6    21     3806   13 48 10
13 49 30  ---          00 01 19  59.2  56.1 -2.4    -101.9    80     3826   13 48 10

13 50 00  SN1986J      00 01 49  59.4  57.4 -2.4    -100.9    21     3826   13 50 00
13 51 30  ---          00 03 19  59.7  57.3 -2.3    -101.3    90     3850   13 50 00

13 51 30  3C66A        00 03 19  59.5  56.0 -2.3    -102.4    -9     3850   13 51 39
13 52 50  ---          00 04 40  59.8  55.8 -2.3    -102.7    71     3868   13 51 39

13 52 50  SN1986J      00 04 40  60.0  57.2 -2.3    -101.6    -9     3868   13 52 59
13 54 40  ---          00 06 30  60.3  57.1 -2.3    -102.0   101     3894   13 52 59

13 54 40  3C66A        00 06 30  60.1  55.7 -2.3    -103.2    -9     3894   13 54 49
13 56 00  ---          00 07 50  60.3  55.6 -2.3    -103.5    71     3912   13 54 49
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

13 56 00  SN1986J      00 07 50  60.5  57.0 -2.3    -102.3    -9     3912   13 56 09
13 57 50  ---          00 09 40  60.9  56.8 -2.2    -102.8   101     3938   13 56 09

 ---------- ***This a 10-min gap for EB Pointing/focus 14 ----------

13 58 30  3C66A        00 10 21  60.8  55.4 -2.2    -104.1    31     3938   13 58 30
14 00 00  ---          00 11 51  61.1  55.2 -2.2    -104.5    90     3961   13 58 30

14 00 40  SN1986J      00 12 31  61.4  56.6 -2.2    -103.5    31     3961   14 00 40
14 02 10  ---          00 14 01  61.6  56.4 -2.2    -103.9    90     3985   14 00 40

14 02 50  3C66A        00 14 41  61.6  54.9 -2.2    -105.2    31     3985   14 02 50
14 04 10  ---          00 16 01  61.8  54.8 -2.1    -105.6    80     4005   14 02 50

14 04 10  SN1986J      00 16 01  62.0  56.2 -2.1    -104.4    -9     4005   14 04 19
14 06 00  ---          00 17 52  62.3  56.0 -2.1    -104.8   101     4031   14 04 19

14 06 00  3C66A        00 17 52  62.1  54.6 -2.1    -106.1    -9     4031   14 06 09
14 07 20  ---          00 19 12  62.4  54.5 -2.1    -106.4    71     4050   14 06 09

14 07 20  SN1986J      00 19 12  62.6  55.9 -2.1    -105.2    -9     4050   14 07 29
14 09 10  ---          00 21 02  62.9  55.7 -2.0    -105.7   101     4076   14 07 29

14 09 40  3C66A        00 21 32  62.8  54.2 -2.0    -107.1    21     4076   14 09 40
14 11 10  ---          00 23 03  63.0  54.0 -2.0    -107.5    90     4099   14 09 40

14 11 40  SN1986J      00 23 33  63.3  55.4 -2.0    -106.3    21     4099   14 11 40
14 13 10  ---          00 25 03  63.6  55.3 -2.0    -106.7    90     4122   14 11 40

14 13 10  3C66A        00 25 03  63.4  53.8 -2.0    -108.1    -9     4122   14 13 19
14 14 30  ---          00 26 23  63.6  53.6 -2.0    -108.4    71     4140   14 13 19

14 14 30  SN1986J      00 26 23  63.8  55.1 -2.0    -107.1    -9     4140   14 14 39
14 16 20  ---          00 28 13  64.2  54.9 -1.9    -107.6   101     4166   14 14 39

14 16 20  3C66A        00 28 13  63.9  53.4 -1.9    -109.0    -9     4166   14 16 29
14 17 40  ---          00 29 34  64.2  53.2 -1.9    -109.4    71     4185   14 16 29

14 17 40  SN1986J      00 29 34  64.4  54.7 -1.9    -108.0    -9     4185   14 17 49
14 19 30  ---          00 31 24  64.7  54.4 -1.9    -108.6   101     4211   14 17 49

14 19 30  3C66A        00 31 24  64.5  52.9 -1.9    -109.9    -9     4211   14 19 39
14 20 50  ---          00 32 44  64.7  52.7 -1.9    -110.3    71     4229   14 19 39
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

14 20 50  SN1986J      00 32 44  65.0  54.3 -1.8    -108.9    -9     4229   14 20 59
14 22 40  ---          00 34 35  65.3  54.0 -1.8    -109.5   101     4255   14 20 59

14 23 10  3C66A        00 35 05  65.1  52.4 -1.8    -111.0    21     4255   14 23 10
14 24 30  ---          00 36 25  65.3  52.2 -1.8    -111.5    80     4276   14 23 10

14 25 00  SN1986J      00 36 55  65.7  53.6 -1.8    -110.2    21     4276   14 25 00
14 26 30  ---          00 38 25  65.9  53.4 -1.8    -110.7    90     4299   14 25 00

14 26 30  3C66A        00 38 25  65.7  51.8 -1.8    -112.1    -9     4299   14 26 39
14 27 50  ---          00 39 45  65.9  51.6 -1.7    -112.5    71     4317   14 26 39

14 27 50  SN1986J      00 39 45  66.2  53.2 -1.7    -111.1    -9     4317   14 27 59
14 29 40  ---          00 41 36  66.5  52.9 -1.7    -111.7   101     4343   14 27 59

14 29 40  3C66A        00 41 36  66.2  51.3 -1.7    -113.1    -9     4343   14 29 49
14 31 00  ---          00 42 56  66.4  51.0 -1.7    -113.6    71     4361   14 29 49

14 31 00  SN1986J      00 42 56  66.7  52.6 -1.7    -112.1    -9     4361   14 31 09
14 32 50  ---          00 44 46  67.0  52.3 -1.6    -112.8   101     4387   14 31 09

14 32 50  3C66A        00 44 46  66.7  50.7 -1.7    -114.2    -9     4387   14 32 59
14 34 10  ---          00 46 06  67.0  50.4 -1.6    -114.7    71     4406   14 32 59

14 34 10  SN1986J      00 46 06  67.3  52.1 -1.6    -113.2    -9     4406   14 34 19
14 36 00  ---          00 47 57  67.6  51.7 -1.6    -113.8   101     4432   14 34 19

14 36 30  3C66A        00 48 27  67.3  50.0 -1.6    -115.5    21     4432   14 36 30
14 37 50  ---          00 49 47  67.6  49.7 -1.6    -116.0    80     4452   14 36 30

14 38 20  SN1986J      00 50 17  68.0  51.2 -1.6    -114.7    21     4452   14 38 20
14 39 50  ---          00 51 47  68.2  50.9 -1.5    -115.2    90     4475   14 38 20

14 39 50  3C66A        00 51 47  67.9  49.3 -1.5    -116.7    -9     4475   14 39 59
14 41 10  ---          00 53 08  68.1  49.0 -1.5    -117.2    71     4494   14 39 59

14 41 10  SN1986J      00 53 08  68.4  50.6 -1.5    -115.7    -9     4494   14 41 19
14 43 00  ---          00 54 58  68.7  50.2 -1.5    -116.4   101     4520   14 41 19

14 43 00  3C66A        00 54 58  68.4  48.6 -1.5    -117.9    -9     4520   14 43 09
14 44 20  ---          00 56 18  68.6  48.2 -1.5    -118.5    71     4538   14 43 09

14 44 20  SN1986J      00 56 18  69.0  49.9 -1.5    -116.9    -9     4538   14 44 29
14 46 10  ---          00 58 08  69.3  49.5 -1.4    -117.6   101     4564   14 44 29
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- ***This a 10-min gap for EB Pointing/focus 15 ----------

14 46 50  3C66A        00 58 48  69.0  47.6 -1.4    -119.5    31     4564   14 46 50
14 48 20  ---          01 00 19  69.3  47.2 -1.4    -120.1    90     4587   14 46 50

14 49 00  SN1986J      01 00 59  69.7  48.8 -1.4    -118.8    31     4587   14 49 00
14 50 30  ---          01 02 29  70.0  48.4 -1.4    -119.4    90     4610   14 49 00

14 51 10  3C66A        01 03 09  69.7  46.5 -1.3    -121.3    31     4610   14 51 10
14 52 10  ---          01 04 09  69.9  46.2 -1.3    -121.7    60     4626   14 51 10

14 52 10  SN1986J      01 04 09  70.2  47.9 -1.3    -120.1    -9     4626   14 52 19
14 54 00  ---          01 06 00  70.5  47.4 -1.3    -120.9   101     4652   14 52 19

14 54 00  3C66A        01 06 00  70.1  45.7 -1.3    -122.5    -9     4652   14 54 09
14 55 00  ---          01 07 00  70.3  45.4 -1.3    -122.9    51     4665   14 54 09

14 55 00  SN1986J      01 07 00  70.7  47.1 -1.3    -121.3    -9     4665   14 55 09
14 56 50  ---          01 08 50  71.0  46.6 -1.2    -122.2   101     4691   14 55 09

14 57 20  3C66A        01 09 20  70.7  44.7 -1.2    -124.0    21     4691   14 57 20
14 58 50  ---          01 10 50  70.9  44.2 -1.2    -124.7    90     4714   14 57 20

14 59 20  SN1986J      01 11 21  71.4  45.8 -1.2    -123.3    21     4714   14 59 20
15 00 50  ---          01 12 51  71.6  45.3 -1.2    -124.0    90     4737   14 59 20

15 00 50  3C66A        01 12 51  71.2  43.6 -1.2    -125.7    -9     4737   15 00 59
15 02 10  ---          01 14 11  71.4  43.1 -1.2    -126.3    71     4756   15 00 59

15 02 10  SN1986J      01 14 11  71.8  44.9 -1.2    -124.7    -9     4756   15 02 19
15 04 00  ---          01 16 01  72.1  44.3 -1.1    -125.6   101     4782   15 02 19

15 04 00  3C66A        01 16 01  71.6  42.5 -1.1    -127.2    -9     4782   15 04 09
15 05 20  ---          01 17 22  71.8  42.0 -1.1    -127.9    71     4800   15 04 09

15 05 20  SN1986J      01 17 22  72.3  43.8 -1.1    -126.3    -9     4800   15 05 29
15 07 10  ---          01 19 12  72.6  43.1 -1.1    -127.2   101     4826   15 05 29

15 07 10  3C66A        01 19 12  72.1  41.3 -1.1    -128.9    -9     4826   15 07 19
15 08 30  ---          01 20 32  72.3  40.8 -1.1    -129.6    71     4844   15 07 19

15 08 30  SN1986J      01 20 32  72.7  42.6 -1.1    -127.9    -9     4844   15 08 39
15 10 20  ---          01 22 22  73.0  41.9 -1.0    -128.9   101     4870   15 08 39
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

15 10 50  3C66A        01 22 52  72.6  39.9 -1.0    -130.8    21     4870   15 10 50
15 12 10  ---          01 24 13  72.8  39.4 -1.0    -131.6    80     4891   15 10 50

15 12 40  SN1986J      01 24 43  73.3  40.9 -1.0    -130.2    21     4891   15 12 40
15 14 10  ---          01 26 13  73.6  40.3 -1.0    -131.1    90     4914   15 12 40

15 14 10  3C66A        01 26 13  73.1  38.5 -1.0    -132.7    -9     4914   15 14 19
15 15 30  ---          01 27 33  73.2  38.0 -0.9    -133.5    71     4932   15 14 19

15 15 30  SN1986J      01 27 33  73.7  39.7 -0.9    -131.9    -9     4932   15 15 39
15 17 20  ---          01 29 24  74.0  38.9 -0.9    -133.0   101     4959   15 15 39

15 17 20  3C66A        01 29 24  73.5  37.2 -0.9    -134.6    -9     4959   15 17 29
15 18 40  ---          01 30 44  73.7  36.5 -0.9    -135.4    71     4977   15 17 29

15 18 40  SN1986J      01 30 44  74.2  38.3 -0.9    -133.8    -9     4977   15 18 49
15 20 30  ---          01 32 34  74.4  37.4 -0.9    -134.9   101     5003   15 18 49

15 20 30  3C66A        01 32 34  73.9  35.7 -0.9    -136.6    -9     5003   15 20 39
15 21 50  ---          01 33 54  74.1  35.0 -0.8    -137.4    71     5021   15 20 39

15 21 50  SN1986J      01 33 54  74.6  36.8 -0.8    -135.8    -9     5021   15 21 59
15 23 40  ---          01 35 45  74.8  35.8 -0.8    -137.0   101     5047   15 21 59

15 24 10  3C66A        01 36 15  74.3  33.9 -0.8    -138.9    21     5047   15 24 10
15 25 30  ---          01 37 35  74.5  33.2 -0.8    -139.8    80     5068   15 24 10

15 26 00  SN1986J      01 38 05  75.1  34.6 -0.8    -138.6    21     5068   15 26 00
15 27 30  ---          01 39 35  75.3  33.8 -0.7    -139.6    90     5091   15 26 00

15 27 30  3C66A        01 39 35  74.7  32.1 -0.7    -141.2    -9     5091   15 27 39
15 28 50  ---          01 40 55  74.9  31.4 -0.7    -142.1    71     5109   15 27 39

15 28 50  SN1986J      01 40 55  75.5  33.0 -0.7    -140.6    -9     5109   15 28 59
15 30 40  ---          01 42 46  75.7  32.0 -0.7    -141.9   101     5135   15 28 59

15 30 40  3C66A        01 42 46  75.1  30.4 -0.7    -143.4    -9     5135   15 30 49
15 32 00  ---          01 44 06  75.2  29.6 -0.7    -144.4    71     5154   15 30 49

15 32 00  SN1986J      01 44 06  75.8  31.2 -0.7    -142.9    -9     5154   15 32 09
15 33 50  ---          01 45 56  76.0  30.0 -0.6    -144.3   101     5180   15 32 09
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- ***This a 10-min gap for EB Pointing/focus 16 ----------

15 34 30  3C66A        01 46 36  75.5  28.1 -0.6    -146.3    31     5180   15 34 30
15 36 00  ---          01 48 07  75.6  27.2 -0.6    -147.4    90     5203   15 34 30

15 36 40  SN1986J      01 48 47  76.3  28.2 -0.6    -146.5    31     5203   15 36 40
15 38 10  ---          01 50 17  76.5  27.2 -0.6    -147.8    90     5226   15 36 40

15 38 56  3C66A        01 51 03  75.9  25.3 -0.5    -149.8    37     5226   15 38 50
15 40 26  ---          01 52 33  76.1  24.3 -0.5    -151.0    90     5251   15 38 50

15 40 26  SN1986J      01 52 33  76.7  25.7 -0.5    -149.6    -9     5251   15 40 35
15 42 06  ---          01 54 14  76.8  24.5 -0.5    -151.1    91     5274   15 40 35

15 42 22  3C66A        01 54 29  76.2  23.0 -0.5    -152.6     6     5274   15 42 22
15 43 52  ---          01 55 59  76.4  22.0 -0.5    -153.8    90     5297   15 42 22

15 43 52  SN1986J      01 55 59  77.0  23.3 -0.5    -152.6    -9     5297   15 44 01
15 45 32  ---          01 57 40  77.1  22.0 -0.4    -154.1    91     5321   15 44 01

15 46 02  3C66A        01 58 10  76.5  20.5 -0.4    -155.7    21     5321   15 46 02
15 47 32  ---          01 59 40  76.6  19.4 -0.4    -157.0    90     5344   15 46 02

15 48 02  SN1986J      02 00 10  77.3  20.1 -0.4    -156.4    21     5344   15 48 02
15 49 42  ---          02 01 50  77.4  18.8 -0.4    -157.9   100     5370   15 48 02

15 49 42  3C66A        02 01 50  76.8  17.8 -0.4    -158.9    -9     5370   15 49 51
15 51 02  ---          02 03 11  76.9  16.8 -0.3    -160.1    71     5388   15 49 51

15 51 02  SN1986J      02 03 11  77.5  17.8 -0.3    -159.2    -9     5388   15 51 11
15 52 52  ---          02 05 01  77.6  16.3 -0.3    -160.9   101     5414   15 51 11

15 52 52  3C66A        02 05 01  77.0  15.4 -0.3    -161.8    -9     5414   15 53 01
15 54 12  ---          02 06 21  77.0  14.3 -0.3    -163.0    71     5432   15 53 01

15 54 12  SN1986J      02 06 21  77.7  15.2 -0.3    -162.2    -9     5432   15 54 21
15 56 02  ---          02 08 11  77.8  13.6 -0.3    -164.0   101     5458   15 54 21

15 56 02  3C66A        02 08 11  77.1  12.9 -0.3    -164.8    -9     5458   15 56 11
15 57 22  ---          02 09 32  77.2  11.8 -0.2    -166.0    71     5477   15 56 11

15 57 22  SN1986J      02 09 32  77.9  12.5 -0.2    -165.4    -9     5477   15 57 31
15 59 12  ---          02 11 22  78.0  10.9 -0.2    -167.2   101     5503   15 57 31
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

15 59 42  3C66A        02 11 52  77.3   9.9 -0.2    -168.3    21     5503   15 59 42
16 01 02  ---          02 13 12  77.3   8.9 -0.2    -169.5    80     5523   15 59 42

16 01 32  SN1986J      02 13 42  78.1   8.9 -0.2    -169.6    21     5523   16 01 32
16 03 02  ---          02 15 13  78.1   7.6 -0.1    -171.2    90     5546   16 01 32

16 03 02  3C66A        02 15 13  77.4   7.2 -0.1    -171.5    -9     5546   16 03 11
16 04 22  ---          02 16 33  77.4   6.1 -0.1    -172.8    71     5565   16 03 11

16 04 22  SN1986J      02 16 33  78.1   6.4 -0.1    -172.5    -9     5565   16 04 31
16 06 12  ---          02 18 23  78.2   4.7 -0.1    -174.5   101     5591   16 04 31

16 06 12  3C66A        02 18 23  77.5   4.6 -0.1    -174.6    -9     5591   16 06 21
16 07 32  ---          02 19 43  77.5   3.4 -0.1    -176.0    71     5609   16 06 21

16 07 32  SN1986J      02 19 43  78.2   3.5 -0.1    -175.9    -9     5609   16 07 41
16 09 22  ---          02 21 34  78.2   1.9 -0.0    -177.8   101     5635   16 07 41

16 09 22  3C66A        02 21 34  77.5   1.9 -0.0    -177.8    -9     5635   16 09 31
16 10 42  ---          02 22 54  77.5   0.8 -0.0    -179.1    71     5653   16 09 31

16 10 42  SN1986J      02 22 54  78.2   0.7 -0.0    -179.2    -9     5653   16 10 51
16 12 32  ---          02 24 44  78.2  -1.0  0.0     178.9   101     5679   16 10 51

16 13 02  3C66A        02 25 14  77.5  -1.2  0.0     178.6    21     5679   16 13 02
16 14 22  ---          02 26 34  77.5  -2.3  0.0     177.2    80     5700   16 13 02

16 14 52  SN1986J      02 27 05  78.2  -3.1  0.1     176.4    21     5700   16 14 52
16 16 22  ---          02 28 35  78.2  -4.4  0.1     174.8    90     5723   16 14 52

16 16 22  3C66A        02 28 35  77.5  -4.0  0.1     175.2    -9     5723   16 16 31
16 17 42  ---          02 29 55  77.5  -5.2  0.1     173.9    71     5741   16 16 31

16 17 42  SN1986J      02 29 55  78.2  -5.6  0.1     173.4    -9     5741   16 17 51
16 19 32  ---          02 31 45  78.1  -7.3  0.1     171.5   101     5767   16 17 51

16 19 32  3C66A        02 31 45  77.4  -6.7  0.1     172.1    -9     5767   16 19 41
16 20 52  ---          02 33 06  77.4  -7.8  0.2     170.8    71     5786   16 19 41

16 20 52  SN1986J      02 33 06  78.1  -8.5  0.2     170.1    -9     5786   16 21 01
16 22 42  ---          02 34 56  78.0 -10.1  0.2     168.2   101     5812   16 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- ***This a 10-min gap for EB Pointing/focus 17 ----------

16 23 22  3C66A        02 35 36  77.3  -9.8  0.2     168.4    31     5812   16 23 22
16 24 52  ---          02 37 06  77.2 -11.1  0.2     166.9    90     5835   16 23 22

16 25 32  SN1986J      02 37 46  77.9 -12.5  0.2     165.4    31     5835   16 25 32
16 27 02  ---          02 39 17  77.8 -13.8  0.3     163.9    90     5858   16 25 32

16 27 42  3C66A        02 39 57  77.1 -13.3  0.3     164.2    31     5858   16 27 42
16 29 02  ---          02 41 17  77.0 -14.4  0.3     163.0    80     5879   16 27 42

16 29 02  SN1986J      02 41 17  77.7 -15.5  0.3     161.9    -9     5879   16 29 11
16 30 52  ---          02 43 07  77.6 -17.0  0.3     160.1   101     5905   16 29 11

16 30 52  3C66A        02 43 07  76.9 -15.8  0.3     161.3    -9     5905   16 31 01
16 32 12  ---          02 44 27  76.9 -16.8  0.3     160.1    71     5923   16 31 01

16 32 12  SN1986J      02 44 27  77.5 -18.0  0.3     158.9    -9     5923   16 32 21
16 34 02  ---          02 46 18  77.4 -19.5  0.4     157.1   101     5949   16 32 21

16 34 32  3C66A        02 46 48  76.7 -18.6  0.4     158.0    21     5949   16 34 32
16 35 52  ---          02 48 08  76.6 -19.5  0.4     156.8    80     5970   16 34 32

16 36 22  SN1986J      02 48 38  77.2 -21.3  0.4     155.0    21     5970   16 36 22
16 38 02  ---          02 50 18  77.1 -22.5  0.4     153.5   100     5996   16 36 22

16 38 02  3C66A        02 50 18  76.5 -21.1  0.4     154.9    -9     5996   16 38 11
16 39 22  ---          02 51 39  76.3 -22.0  0.5     153.8    71     6014   16 38 11

16 39 22  SN1986J      02 51 39  77.0 -23.5  0.5     152.3    -9     6014   16 39 31
16 41 12  ---          02 53 29  76.8 -24.8  0.5     150.7   101     6040   16 39 31

16 41 12  3C66A        02 53 29  76.2 -23.3  0.5     152.2    -9     6040   16 41 21
16 42 32  ---          02 54 49  76.1 -24.2  0.5     151.1    71     6058   16 41 21

16 42 32  SN1986J      02 54 49  76.7 -25.7  0.5     149.6    -9     6058   16 42 41
16 44 22  ---          02 56 39  76.5 -27.0  0.6     148.1   101     6084   16 42 41

16 44 22  3C66A        02 56 39  75.9 -25.4  0.5     149.7    -9     6084   16 44 31
16 45 42  ---          02 58 00  75.8 -26.2  0.6     148.6    71     6102   16 44 31

16 45 42  SN1986J      02 58 00  76.4 -27.9  0.6     147.0    -9     6102   16 45 51
16 47 32  ---          02 59 50  76.2 -29.1  0.6     145.5   101     6128   16 45 51
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

16 47 32  3C66A        02 59 50  75.6 -27.4  0.6     147.2    -9     6128   16 47 41
16 48 52  ---          03 01 10  75.5 -28.2  0.6     146.1    71     6147   16 47 41

16 48 52  SN1986J      03 01 10  76.0 -29.9  0.6     144.5    -9     6147   16 49 01
16 50 42  ---          03 03 00  75.8 -31.0  0.7     143.1   101     6173   16 49 01

16 50 42  3C66A        03 03 00  75.3 -29.3  0.7     144.8    -9     6173   16 50 51
16 52 02  ---          03 04 21  75.1 -30.1  0.7     143.8    71     6191   16 50 51

16 52 02  SN1986J      03 04 21  75.7 -31.8  0.7     142.1    -9     6191   16 52 11
16 53 50  ---          03 06 09  75.5 -32.9  0.7     140.7    99     6217   16 52 11

16 54 20  3C66A        03 06 39  74.9 -31.4  0.7     142.1    21     6217   16 54 20
16 56 00  ---          03 08 19  74.7 -32.3  0.7     141.0   100     6242   16 54 20

16 56 30  3C84         03 08 49  78.8  11.8 -0.2    -166.4    -9     6242   16 56 39
17 00 00  ---          03 12 20  78.9   8.5 -0.1    -170.3   201     6294   16 56 39

 ---------- EVN out ----------

17 00 30  3C66A        03 12 50  74.2 -34.6  0.8     138.0    -9     6294   17 00 38
17 03 30  ---          03 15 51  73.8 -36.1  0.9     136.1   171     6338   17 00 38

17 03 30  3C66A        03 15 51  73.8 -36.1  0.9     136.1    -6     6338   17 03 36
17 04 50  ---          03 17 11  73.6 -36.7  0.9     135.2    74     6357   17 03 36

17 04 50  SN1986J      03 17 11  74.1 -38.6  0.9     133.4    -9     6357   17 04 59
17 06 40  ---          03 19 01  73.8 -39.4  0.9     132.3   101     6383   17 04 59

17 06 40  3C66A        03 19 01  73.4 -37.5  0.9     134.1    -9     6383   17 06 49
17 08 00  ---          03 20 21  73.2 -38.1  0.9     133.3    71     6402   17 06 49

17 08 00  SN1986J      03 20 21  73.7 -40.0  0.9     131.5    -9     6402   17 08 09
17 09 50  ---          03 22 12  73.4 -40.8  1.0     130.4   101     6428   17 08 09

17 09 50  3C66A        03 22 12  73.0 -38.9  1.0     132.3    -9     6428   17 09 59
17 11 10  ---          03 23 32  72.8 -39.4  1.0     131.5    71     6446   17 09 59

17 11 10  SN1986J      03 23 32  73.2 -41.3  1.0     129.7    -9     6446   17 11 19
17 13 00  ---          03 25 22  73.0 -42.1  1.0     128.7   101     6472   17 11 19

17 13 00  3C66A        03 25 22  72.5 -40.2  1.0     130.5    -9     6472   17 13 09
17 14 20  ---          03 26 42  72.3 -40.7  1.0     129.8    71     6490   17 13 09
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- start of phase-ref block; pointing for VLA 1 ----------

17 14 20  SN1986J      03 26 42  72.8 -42.6  1.1     127.9    -9     6490   17 14 29
17 16 10  ---          03 28 33  72.5 -43.3  1.1     127.0   101     6516   17 14 29

17 16 10  3C66A        03 28 33  72.1 -41.4  1.1     128.8    -9     6516   17 16 19
17 17 20  ---          03 29 43  71.9 -41.8  1.1     128.2    61     6532   17 16 19

17 17 20  3C66A        03 29 43  71.9 -41.8  1.1     128.2    -6     6532   17 17 26
17 18 50  ---          03 31 13  71.7 -42.4  1.1     127.4    84     6554   17 17 26

17 18 50  3C66A        03 31 13  71.7 -42.4  1.1     127.4    -6     6554   17 18 56
17 20 10  ---          03 32 33  71.5 -42.8  1.1     126.7    74     6573   17 18 56

17 20 10  SN1986J      03 32 33  71.9 -44.7  1.1     124.9    -9     6573   17 20 19
17 22 00  ---          03 34 24  71.6 -45.3  1.2     124.1   101     6599   17 20 19

17 22 00  3C66A        03 34 24  71.2 -43.5  1.2     125.8    -9     6599   17 22 09
17 23 20  ---          03 35 44  71.0 -43.9  1.2     125.2    71     6617   17 22 09

17 23 20  SN1986J      03 35 44  71.4 -45.7  1.2     123.4    -9     6617   17 23 29
17 25 10  ---          03 37 34  71.1 -46.3  1.2     122.6   101     6643   17 23 29

17 25 10  3C66A        03 37 34  70.8 -44.5  1.2     124.3    -9     6643   17 25 19
17 26 30  ---          03 38 54  70.6 -44.9  1.3     123.7    71     6661   17 25 19

17 26 30  SN1986J      03 38 54  70.9 -46.7  1.3     122.0    -9     6661   17 26 39
17 28 20  ---          03 40 45  70.6 -47.3  1.3     121.1   101     6687   17 26 39

17 28 20  3C66A        03 40 45  70.3 -45.4  1.3     122.9    -9     6687   17 28 29
17 29 40  ---          03 42 05  70.1 -45.8  1.3     122.3    71     6706   17 28 29

17 29 40  SN1986J      03 42 05  70.4 -47.6  1.3     120.6    -9     6706   17 29 49
17 31 30  ---          03 43 55  70.1 -48.1  1.3     119.8   101     6732   17 29 49

17 31 30  3C66A        03 43 55  69.8 -46.3  1.3     121.5    -9     6732   17 31 39
17 32 50  ---          03 45 15  69.6 -46.7  1.4     120.9    71     6750   17 31 39

17 32 50  SN1986J      03 45 15  69.9 -48.5  1.4     119.2    -9     6750   17 32 59
17 34 40  ---          03 47 06  69.6 -49.0  1.4     118.5   101     6776   17 32 59

17 34 40  3C66A        03 47 06  69.3 -47.2  1.4     120.1    -9     6776   17 34 49
17 36 00  ---          03 48 26  69.1 -47.5  1.4     119.6    71     6794   17 34 49
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

17 36 00  SN1986J      03 48 26  69.4 -49.3  1.4     117.9    -9     6794   17 36 09
17 37 50  ---          03 50 16  69.1 -49.8  1.4     117.2   101     6820   17 36 09

17 37 50  3C66A        03 50 16  68.8 -48.0  1.4     118.9    -9     6820   17 37 59
17 39 10  ---          03 51 36  68.6 -48.3  1.5     118.3    71     6839   17 37 59

17 39 10  SN1986J      03 51 36  68.9 -50.1  1.5     116.7    -9     6839   17 39 19
17 41 00  ---          03 53 27  68.6 -50.5  1.5     116.0   101     6865   17 39 19

17 41 00  3C66A        03 53 27  68.3 -48.7  1.5     117.6    -9     6865   17 41 09
17 42 20  ---          03 54 47  68.1 -49.0  1.5     117.1    71     6883   17 41 09

17 42 20  SN1986J      03 54 47  68.3 -50.8  1.5     115.5    -9     6883   17 42 29
17 44 10  ---          03 56 37  68.0 -51.2  1.5     114.8   101     6909   17 42 29

17 44 10  3C66A        03 56 37  67.8 -49.4  1.5     116.4    -9     6909   17 44 19
17 45 30  ---          03 57 57  67.5 -49.7  1.6     115.9    71     6927   17 44 19

17 45 30  SN1986J      03 57 57  67.8 -51.4  1.6     114.3    -9     6927   17 45 39
17 47 20  ---          03 59 48  67.5 -51.8  1.6     113.7   101     6953   17 45 39

17 47 20  3C66A        03 59 48  67.2 -50.1  1.6     115.3    -9     6953   17 47 29
17 48 40  ---          04 01 08  67.0 -50.4  1.6     114.8    71     6971   17 47 29

17 48 40  SN1986J      04 01 08  67.3 -52.0  1.6     113.2    -9     6971   17 48 49
17 50 30  ---          04 02 58  67.0 -52.4  1.7     112.6   101     6997   17 48 49

17 50 30  3C66A        04 02 58  66.7 -50.7  1.7     114.2    -9     6997   17 50 39
17 51 50  ---          04 04 19  66.5 -51.0  1.7     113.7    71     7016   17 50 39

17 51 50  SN1986J      04 04 19  66.7 -52.6  1.7     112.2    -9     7016   17 51 59
17 53 40  ---          04 06 09  66.4 -52.9  1.7     111.6   101     7042   17 51 59

17 53 40  3C66A        04 06 09  66.2 -51.3  1.7     113.1    -9     7042   17 53 49
17 55 00  ---          04 07 29  65.9 -51.5  1.7     112.6    71     7060   17 53 49

17 55 00  SN1986J      04 07 29  66.2 -53.2  1.7     111.1    -9     7060   17 55 09
17 56 50  ---          04 09 19  65.9 -53.5  1.8     110.5   101     7086   17 55 09

17 56 50  3C66A        04 09 19  65.6 -51.8  1.8     112.0    -9     7086   17 56 59
17 58 10  ---          04 10 40  65.4 -52.1  1.8     111.6    71     7104   17 56 59

17 58 10  SN1986J      04 10 40  65.6 -53.7  1.8     110.1    -9     7104   17 58 19
18 00 00  ---          04 12 30  65.3 -54.0  1.8     109.6   101     7130   17 58 19
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- start of phase-ref block; pointing for VLA 2 ----------

18 00 00  SN1986J      04 12 30  65.3 -54.0  1.8     109.6    -6     7130   18 00 06
18 01 50  ---          04 14 20  65.0 -54.2  1.8     109.0   104     7157   18 00 06

18 01 50  3C66A        04 14 20  64.8 -52.6  1.8     110.5    -9     7157   18 01 59
18 03 00  ---          04 15 30  64.6 -52.8  1.9     110.1    61     7173   18 01 59

18 03 00  3C66A        04 15 30  64.6 -52.8  1.9     110.1    -6     7173   18 03 06
18 04 30  ---          04 17 01  64.3 -53.0  1.9     109.7    84     7195   18 03 06

18 04 30  3C66A        04 17 01  64.3 -53.0  1.9     109.7    -6     7195   18 04 36
18 05 50  ---          04 18 21  64.1 -53.2  1.9     109.3    74     7214   18 04 36

18 05 50  SN1986J      04 18 21  64.3 -54.8  1.9     107.8    -9     7214   18 05 59
18 07 40  ---          04 20 11  64.0 -55.0  1.9     107.3   101     7240   18 05 59

18 07 40  3C66A        04 20 11  63.8 -53.5  1.9     108.7    -9     7240   18 07 48
18 09 00  ---          04 21 31  63.5 -53.6  2.0     108.3    71     7258   18 07 48

18 09 00  SN1986J      04 21 31  63.7 -55.2  2.0     107.0    -9     7258   18 09 08
18 10 50  ---          04 23 22  63.4 -55.4  2.0     106.4   101     7284   18 09 08

18 10 50  3C66A        04 23 22  63.2 -53.9  2.0     107.8    -9     7284   18 10 58
18 12 10  ---          04 24 42  63.0 -54.0  2.0     107.4    71     7302   18 10 58

18 12 10  SN1986J      04 24 42  63.2 -55.5  2.0     106.1    -9     7302   18 12 18
18 14 00  ---          04 26 32  62.8 -55.7  2.0     105.6   101     7328   18 12 18

18 14 00  3C66A        04 26 32  62.7 -54.3  2.0     106.9    -9     7328   18 14 08
18 15 20  ---          04 27 52  62.4 -54.4  2.1     106.6    71     7347   18 14 08

18 15 20  SN1986J      04 27 52  62.6 -55.9  2.1     105.2    -9     7347   18 15 28
18 17 10  ---          04 29 43  62.3 -56.1  2.1     104.8   101     7373   18 15 28

18 17 10  3C66A        04 29 43  62.1 -54.6  2.1     106.1    -9     7373   18 17 18
18 18 30  ---          04 31 03  61.9 -54.8  2.1     105.7    71     7391   18 17 18

18 18 30  SN1986J      04 31 03  62.0 -56.2  2.1     104.4    -9     7391   18 18 38
18 20 20  ---          04 32 53  61.7 -56.4  2.2     103.9   101     7417   18 18 38

18 20 20  3C66A        04 32 53  61.6 -54.9  2.2     105.2    -9     7417   18 20 28
18 21 40  ---          04 34 13  61.3 -55.1  2.2     104.9    71     7435   18 20 28
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

18 21 40  SN1986J      04 34 13  61.5 -56.5  2.2     103.6    -9     7435   18 21 48
18 23 30  ---          04 36 04  61.1 -56.7  2.2     103.2   101     7461   18 21 48

18 23 30  3C66A        04 36 04  61.0 -55.2  2.2     104.4    -9     7461   18 23 38
18 24 50  ---          04 37 24  60.8 -55.4  2.2     104.1    71     7480   18 23 38

18 24 50  SN1986J      04 37 24  60.9 -56.8  2.2     102.8    -9     7480   18 24 58
18 26 40  ---          04 39 14  60.6 -56.9  2.3     102.4   101     7506   18 24 58

18 26 40  3C66A        04 39 14  60.4 -55.5  2.3     103.6    -9     7506   18 26 48
18 28 00  ---          04 40 34  60.2 -55.7  2.3     103.3    71     7524   18 26 48

18 28 00  SN1986J      04 40 34  60.3 -57.0  2.3     102.1    -9     7524   18 28 08
18 29 50  ---          04 42 25  60.0 -57.2  2.3     101.6   101     7550   18 28 08

18 29 50  3C66A        04 42 25  59.9 -55.8  2.3     102.9    -9     7550   18 29 58
18 31 10  ---          04 43 45  59.6 -55.9  2.3     102.5    71     7568   18 29 58

18 31 10  SN1986J      04 43 45  59.8 -57.3  2.3     101.3    -9     7568   18 31 18
18 33 00  ---          04 45 35  59.4 -57.4  2.4     100.9   101     7594   18 31 18

18 33 00  3C66A        04 45 35  59.3 -56.1  2.4     102.1    -9     7594   18 33 08
18 34 20  ---          04 46 55  59.1 -56.1  2.4     101.8    71     7612   18 33 08

18 34 20  SN1986J      04 46 55  59.2 -57.5  2.4     100.6    -9     7612   18 34 28
18 36 10  ---          04 48 46  58.8 -57.6  2.4     100.2   101     7638   18 34 28

18 36 10  3C66A        04 48 46  58.7 -56.3  2.4     101.4    -9     7638   18 36 18
18 37 30  ---          04 50 06  58.5 -56.4  2.4     101.1    71     7657   18 36 18

18 37 30  SN1986J      04 50 06  58.6 -57.7  2.4      99.9    -9     7657   18 37 38
18 39 20  ---          04 51 56  58.3 -57.8  2.5      99.5   101     7683   18 37 38

18 39 20  3C66A        04 51 56  58.2 -56.5  2.5     100.6    -9     7683   18 39 28
18 40 40  ---          04 53 17  57.9 -56.6  2.5     100.3    71     7701   18 39 28

18 40 40  SN1986J      04 53 17  58.0 -57.9  2.5      99.2    -9     7701   18 40 48
18 42 30  ---          04 55 07  57.7 -58.0  2.5      98.8   101     7727   18 40 48

18 42 30  3C66A        04 55 07  57.6 -56.7  2.5      99.9    -9     7727   18 42 38
18 43 50  ---          04 56 27  57.4 -56.8  2.5      99.6    71     7745   18 42 38

18 43 50  SN1986J      04 56 27  57.4 -58.1  2.5      98.5    -9     7745   18 43 58
18 45 40  ---          04 58 17  57.1 -58.2  2.6      98.1   101     7771   18 43 58
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- start of phase-ref block; pointing for VLA 3 ----------

18 45 40  SN1986J      04 58 17  57.1 -58.2  2.6      98.1    -6     7771   18 45 46
18 47 30  ---          05 00 08  56.8 -58.2  2.6      97.8   104     7798   18 45 46

18 47 30  3C66A        05 00 08  56.7 -57.0  2.6      98.9    -9     7798   18 47 38
18 48 40  ---          05 01 18  56.5 -57.0  2.6      98.6    61     7814   18 47 38

18 48 40  3C66A        05 01 18  56.5 -57.0  2.6      98.6    -6     7814   18 48 46
18 50 40  ---          05 03 18  56.1 -57.1  2.7      98.2   114     7843   18 48 46

18 50 40  3C66A        05 03 18  56.1 -57.1  2.7      98.2    -6     7843   18 50 46
18 52 00  ---          05 04 38  55.9 -57.2  2.7      97.9    74     7862   18 50 46

18 52 00  SN1986J      05 04 38  56.0 -58.4  2.7      96.8    -9     7862   18 52 08
18 53 50  ---          05 06 29  55.6 -58.5  2.7      96.5   101     7888   18 52 08

18 53 50  3C66A        05 06 29  55.6 -57.3  2.7      97.5    -9     7888   18 53 58
18 55 10  ---          05 07 49  55.3 -57.3  2.7      97.2    71     7907   18 53 58

18 55 10  SN1986J      05 07 49  55.4 -58.5  2.7      96.2    -9     7907   18 55 18
18 57 00  ---          05 09 39  55.0 -58.6  2.8      95.8   101     7933   18 55 18

18 57 00  3C66A        05 09 39  55.0 -57.4  2.8      96.9    -9     7933   18 57 08
18 58 20  ---          05 10 59  54.7 -57.4  2.8      96.6    71     7951   18 57 08

18 58 20  SN1986J      05 10 59  54.8 -58.7  2.8      95.6    -9     7951   18 58 28
19 00 10  ---          05 12 50  54.4 -58.7  2.8      95.2   101     7977   18 58 28

19 00 10  3C66A        05 12 50  54.4 -57.5  2.8      96.2    -9     7977   19 00 18
19 01 30  ---          05 14 10  54.2 -57.5  2.8      96.0    71     7995   19 00 18

19 01 30  SN1986J      05 14 10  54.2 -58.7  2.8      95.0    -9     7995   19 01 38
19 03 20  ---          05 16 00  53.9 -58.8  2.9      94.6   101     8021   19 01 38

19 03 20  3C66A        05 16 00  53.8 -57.6  2.9      95.6    -9     8021   19 03 28
19 04 40  ---          05 17 20  53.6 -57.6  2.9      95.4    71     8040   19 03 28

19 04 40  SN1986J      05 17 20  53.6 -58.8  2.9      94.4    -9     8040   19 04 48
19 06 30  ---          05 19 11  53.3 -58.9  2.9      94.0   101     8066   19 04 48

19 06 30  3C66A        05 19 11  53.3 -57.7  2.9      95.0    -9     8066   19 06 38
19 07 50  ---          05 20 31  53.0 -57.7  2.9      94.7    71     8084   19 06 38
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

19 07 50  SN1986J      05 20 31  53.0 -58.9  2.9      93.8    -8     8084   19 07 58
19 09 40  ---          05 22 21  52.7 -58.9  3.0      93.4   102     8110   19 07 58

19 09 40  3C66A        05 22 21  52.7 -57.8  3.0      94.4    -8     8110   19 09 48
19 11 00  ---          05 23 42  52.4 -57.8  3.0      94.1    72     8129   19 09 48

19 11 00  SN1986J      05 23 42  52.4 -59.0  3.0      93.2    -8     8129   19 11 08
19 12 50  ---          05 25 32  52.1 -59.0  3.0      92.9   102     8155   19 11 08

19 12 50  3C66A        05 25 32  52.1 -57.8  3.0      93.8    -8     8155   19 12 58
19 14 10  ---          05 26 52  51.9 -57.9  3.1      93.5    72     8174   19 12 58

19 14 10  SN1986J      05 26 52  51.9 -59.0  3.1      92.6    -8     8174   19 14 18
19 16 00  ---          05 28 42  51.5 -59.0  3.1      92.3   102     8200   19 14 18

19 16 00  3C66A        05 28 42  51.5 -57.9  3.1      93.2    -8     8200   19 16 08
19 17 20  ---          05 30 03  51.3 -57.9  3.1      93.0    72     8218   19 16 08

19 17 20  SN1986J      05 30 03  51.3 -59.0  3.1      92.1    -8     8218   19 17 28
19 19 10  ---          05 31 53  50.9 -59.1  3.1      91.7   102     8245   19 17 28

19 19 10  3C66A        05 31 53  50.9 -57.9  3.1      92.6    -8     8245   19 19 18
19 20 30  ---          05 33 13  50.7 -58.0  3.2      92.4    72     8263   19 19 18

19 20 30  SN1986J      05 33 13  50.7 -59.1  3.2      91.5    -8     8263   19 20 38
19 22 20  ---          05 35 03  50.4 -59.1  3.2      91.2   102     8290   19 20 38

19 22 20  3C66A        05 35 03  50.4 -58.0  3.2      92.1    -8     8290   19 22 28
19 23 40  ---          05 36 24  50.1 -58.0  3.2      91.8    72     8308   19 22 28

19 23 40  SN1986J      05 36 24  50.1 -59.1  3.2      91.0    -8     8308   19 23 48
19 25 30  ---          05 38 14  49.8 -59.1  3.2      90.6   102     8334   19 23 48

19 25 30  3C66A        05 38 14  49.8 -58.0  3.2      91.5    -8     8334   19 25 38
19 26 50  ---          05 39 34  49.5 -58.0  3.3      91.3    72     8353   19 25 38

19 26 50  SN1986J      05 39 34  49.5 -59.1  3.3      90.4    -8     8353   19 26 58
19 28 40  ---          05 41 24  49.2 -59.1  3.3      90.1   102     8379   19 26 58

19 28 40  3C66A        05 41 24  49.2 -58.0  3.3      90.9    -8     8379   19 28 48
19 30 00  ---          05 42 45  49.0 -58.0  3.3      90.7    72     8398   19 28 48

19 30 00  SN1986J      05 42 45  48.9 -59.1  3.3      89.9    -8     8398   19 30 08
19 31 50  ---          05 44 35  48.6 -59.1  3.3      89.6   102     8424   19 30 08
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- start of phase-ref block; pointing for VLA 4 ----------

19 31 50  SN1986J      05 44 35  48.6 -59.1  3.3      89.6    -6     8424   19 31 56
19 33 40  ---          05 46 25  48.3 -59.1  3.4      89.3   104     8451   19 31 56

19 33 40  3C66A        05 46 25  48.3 -58.0  3.4      90.1    -8     8451   19 33 48
19 34 50  ---          05 47 35  48.1 -58.0  3.4      89.9    62     8467   19 33 48

19 34 50  3C66A        05 47 35  48.1 -58.0  3.4      89.9    -6     8467   19 34 56
19 36 50  ---          05 49 36  47.7 -58.0  3.4      89.5   114     8496   19 34 56

19 36 50  3C66A        05 49 36  47.7 -58.0  3.4      89.5    -6     8496   19 36 56
19 38 10  ---          05 50 56  47.5 -58.0  3.5      89.3    74     8515   19 36 56

19 38 10  SN1986J      05 50 56  47.4 -59.1  3.5      88.5    -8     8515   19 38 18
19 40 00  ---          05 52 46  47.1 -59.1  3.5      88.2   102     8541   19 38 18

19 40 00  3C66A        05 52 46  47.1 -58.0  3.5      89.0    -8     8541   19 40 08
19 41 20  ---          05 54 06  46.9 -58.0  3.5      88.8    72     8560   19 40 08

19 41 20  SN1986J      05 54 06  46.8 -59.0  3.5      88.0    -8     8560   19 41 28
19 43 10  ---          05 55 57  46.5 -59.0  3.5      87.7   102     8586   19 41 28

19 43 10  3C66A        05 55 57  46.5 -58.0  3.5      88.5    -8     8586   19 43 18
19 44 30  ---          05 57 17  46.3 -58.0  3.6      88.2    72     8605   19 43 18

19 44 30  SN1986J      05 57 17  46.3 -59.0  3.6      87.5    -8     8605   19 44 38
19 46 20  ---          05 59 07  45.9 -59.0  3.6      87.2   102     8631   19 44 38

19 46 20  3C66A        05 59 07  46.0 -58.0  3.6      87.9    -8     8631   19 46 28
19 47 40  ---          06 00 28  45.7 -58.0  3.6      87.7    72     8650   19 46 28

19 47 40  SN1986J      06 00 28  45.7 -59.0  3.6      87.0    -8     8650   19 47 48
19 49 30  ---          06 02 18  45.3 -58.9  3.6      86.7   102     8676   19 47 48

19 49 30  3C66A        06 02 18  45.4 -57.9  3.6      87.4    -8     8676   19 49 38
19 50 50  ---          06 03 38  45.1 -57.9  3.7      87.2    72     8695   19 49 38

19 50 50  SN1986J      06 03 38  45.1 -58.9  3.7      86.5    -8     8695   19 50 58
19 52 40  ---          06 05 28  44.7 -58.9  3.7      86.2   102     8721   19 50 58

19 52 40  3C66A        06 05 28  44.8 -57.9  3.7      86.9    -8     8721   19 52 48
19 54 00  ---          06 06 49  44.6 -57.9  3.7      86.7    72     8739   19 52 48
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

19 54 00  SN1986J      06 06 49  44.5 -58.9  3.7      86.0    -8     8739   19 54 08
19 55 50  ---          06 08 39  44.2 -58.8  3.7      85.7   102     8766   19 54 08

19 55 50  3C66A        06 08 39  44.2 -57.9  3.7      86.4    -8     8766   19 55 58
19 57 10  ---          06 09 59  44.0 -57.8  3.8      86.2    72     8784   19 55 58

19 57 10  SN1986J      06 09 59  43.9 -58.8  3.8      85.5    -8     8784   19 57 18
19 59 00  ---          06 11 49  43.6 -58.8  3.8      85.2   102     8810   19 57 18

19 59 00  3C66A        06 11 49  43.7 -57.8  3.8      85.9    -8     8810   19 59 08
20 00 20  ---          06 13 10  43.4 -57.8  3.8      85.7    72     8829   19 59 08

20 00 20  SN1986J      06 13 10  43.3 -58.7  3.8      85.0    -8     8829   20 00 28
20 02 10  ---          06 15 00  43.0 -58.7  3.9      84.7   102     8855   20 00 28

20 02 10  3C66A        06 15 00  43.1 -57.7  3.9      85.4    -8     8855   20 02 18
20 03 30  ---          06 16 20  42.8 -57.7  3.9      85.2    72     8874   20 02 18

20 03 30  SN1986J      06 16 20  42.7 -58.7  3.9      84.5    -8     8874   20 03 38
20 05 20  ---          06 18 10  42.4 -58.6  3.9      84.2   102     8900   20 03 38

20 05 20  3C66A        06 18 10  42.5 -57.7  3.9      84.9    -8     8900   20 05 28
20 06 40  ---          06 19 31  42.3 -57.6  3.9      84.7    72     8919   20 05 28

20 06 40  SN1986J      06 19 31  42.2 -58.6  3.9      84.0    -8     8919   20 06 48
20 08 30  ---          06 21 21  41.8 -58.5  4.0      83.8   102     8945   20 06 48

20 08 30  3C66A        06 21 21  41.9 -57.6  4.0      84.4    -8     8945   20 08 38
20 09 50  ---          06 22 41  41.7 -57.6  4.0      84.2    72     8964   20 08 38

20 09 50  SN1986J      06 22 41  41.6 -58.5  4.0      83.6    -8     8964   20 09 58
20 11 40  ---          06 24 31  41.2 -58.5  4.0      83.3   102     8990   20 09 58

20 11 40  3C66A        06 24 31  41.3 -57.5  4.0      83.9    -8     8990   20 11 48
20 13 00  ---          06 25 52  41.1 -57.5  4.0      83.7    72     9008   20 11 48

20 13 00  SN1986J      06 25 52  41.0 -58.4  4.0      83.1    -8     9008   20 13 08
20 14 50  ---          06 27 42  40.7 -58.4  4.1      82.8   102     9035   20 13 08

20 14 50  3C66A        06 27 42  40.8 -57.4  4.1      83.4    -8     9035   20 14 58
20 16 10  ---          06 29 02  40.5 -57.4  4.1      83.2    72     9053   20 14 58

20 16 10  SN1986J      06 29 02  40.4 -58.3  4.1      82.6    -8     9053   20 16 18
20 18 00  ---          06 30 53  40.1 -58.3  4.1      82.3   102     9079   20 16 18
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

 ---------- start of phase-ref block; pointing for VLA 5 ----------

20 18 00  SN1986J      06 30 53  40.1 -58.3  4.1      82.3    -6     9079   20 18 06
20 19 50  ---          06 32 43  39.7 -58.2  4.2      82.1   104     9106   20 18 06

20 19 50  3C66A        06 32 43  39.9 -57.3  4.1      82.7    -8     9106   20 19 58
20 21 00  ---          06 33 53  39.6 -57.3  4.2      82.5    62     9122   20 19 58

20 21 00  3C66A        06 33 53  39.6 -57.3  4.2      82.5    -6     9122   20 21 06
20 23 00  ---          06 35 53  39.3 -57.2  4.2      82.2   114     9152   20 21 06

20 23 00  3C66A        06 35 53  39.3 -57.2  4.2      82.2    -6     9152   20 23 06
20 24 20  ---          06 37 14  39.0 -57.2  4.2      82.0    74     9171   20 23 06

20 24 20  SN1986J      06 37 14  38.9 -58.0  4.2      81.4    -8     9171   20 24 28
20 26 10  ---          06 39 04  38.6 -58.0  4.3      81.1   102     9197   20 24 28

20 26 10  3C66A        06 39 04  38.7 -57.1  4.3      81.7    -8     9197   20 26 18
20 27 30  ---          06 40 24  38.5 -57.0  4.3      81.5    72     9215   20 26 18

20 27 30  SN1986J      06 40 24  38.3 -57.9  4.3      80.9    -8     9215   20 27 38
20 29 20  ---          06 42 14  38.0 -57.9  4.3      80.7   102     9242   20 27 38

20 29 20  3C66A        06 42 14  38.1 -57.0  4.3      81.2    -8     9242   20 29 28
20 30 40  ---          06 43 35  37.9 -56.9  4.3      81.0    72     9260   20 29 28

20 30 40  SN1986J      06 43 35  37.8 -57.8  4.3      80.5    -8     9260   20 30 48
20 32 30  ---          06 45 25  37.4 -57.7  4.4      80.2   102     9287   20 30 48

20 32 30  3C66A        06 45 25  37.6 -56.9  4.4      80.8    -8     9287   20 32 38
20 33 50  ---          06 46 45  37.3 -56.8  4.4      80.6    72     9305   20 32 38

20 33 50  SN1986J      06 46 45  37.2 -57.7  4.4      80.0    -8     9305   20 33 58
20 35 40  ---          06 48 35  36.8 -57.6  4.4      79.8   102     9331   20 33 58

20 35 40  3C66A        06 48 35  37.0 -56.7  4.4      80.3    -8     9331   20 35 48
20 37 00  ---          06 49 56  36.8 -56.7  4.4      80.1    72     9350   20 35 48

20 37 00  SN1986J      06 49 56  36.6 -57.6  4.4      79.6    -8     9350   20 37 08
20 38 50  ---          06 51 46  36.3 -57.5  4.5      79.3   102     9376   20 37 08

20 38 50  3C66A        06 51 46  36.4 -56.6  4.5      79.8    -8     9376   20 38 58
20 40 10  ---          06 53 06  36.2 -56.6  4.5      79.6    72     9395   20 38 58
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

20 40 10  SN1986J      06 53 06  36.0 -57.4  4.5      79.1    -8     9395   20 40 18
20 42 00  ---          06 54 56  35.7 -57.3  4.5      78.8   102     9421   20 40 18

20 42 00  3C66A        06 54 56  35.9 -56.5  4.5      79.4    -8     9421   20 42 08
20 43 20  ---          06 56 17  35.6 -56.4  4.5      79.2    72     9440   20 42 08

20 43 20  SN1986J      06 56 17  35.5 -57.3  4.5      78.6    -8     9440   20 43 28
20 45 10  ---          06 58 07  35.1 -57.2  4.6      78.4   102     9466   20 43 28

20 45 10  3C66A        06 58 07  35.3 -56.4  4.6      78.9    -8     9466   20 45 18
20 46 30  ---          06 59 27  35.0 -56.3  4.6      78.7    72     9484   20 45 18

20 46 30  SN1986J      06 59 27  34.9 -57.1  4.6      78.2    -8     9484   20 46 38
20 48 20  ---          07 01 18  34.5 -57.0  4.6      77.9   102     9511   20 46 38

20 48 20  3C66A        07 01 18  34.7 -56.2  4.6      78.4    -8     9511   20 48 28
20 49 40  ---          07 02 38  34.5 -56.2  4.6      78.2    72     9529   20 48 28

20 49 40  SN1986J      07 02 38  34.3 -57.0  4.6      77.7    -8     9529   20 49 48
20 51 30  ---          07 04 28  34.0 -56.9  4.7      77.5   102     9556   20 49 48

20 51 30  3C66A        07 04 28  34.1 -56.1  4.7      78.0    -8     9556   20 51 38
20 52 50  ---          07 05 48  33.9 -56.0  4.7      77.8    72     9574   20 51 38

20 52 50  SN1986J      07 05 48  33.7 -56.8  4.7      77.3    -8     9574   20 52 58
20 54 40  ---          07 07 39  33.4 -56.7  4.7      77.0   102     9600   20 52 58

20 54 40  3C66A        07 07 39  33.6 -55.9  4.7      77.5    -8     9600   20 54 48
20 56 00  ---          07 08 59  33.3 -55.9  4.8      77.3    72     9619   20 54 48

20 56 00  SN1986J      07 08 59  33.2 -56.7  4.8      76.8    -8     9619   20 56 08
20 57 50  ---          07 10 49  32.8 -56.6  4.8      76.6   102     9645   20 56 08

20 57 50  3C66A        07 10 49  33.0 -55.8  4.8      77.1    -8     9645   20 57 58
20 59 10  ---          07 12 09  32.8 -55.7  4.8      76.9    72     9664   20 57 58

20 59 10  SN1986J      07 12 09  32.6 -56.5  4.8      76.4    -8     9664   20 59 18
21 01 00  ---          07 14 00  32.3 -56.4  4.8      76.1   102     9690   20 59 18

 ---------- start of phase-ref block; pointing for VLA 6 ----------

21 01 00  SN1986J      07 14 00  32.3 -56.4  4.8      76.1    -6     9690   21 01 06
21 02 50  ---          07 15 50  31.9 -56.3  4.9      75.9   104     9717   21 01 06
Schedule for VLBA_FD   (Code Fd )                                   Page  32
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

21 02 50  3C66A        07 15 50  32.1 -55.5  4.9      76.3    -8     9717   21 02 58
21 04 00  ---          07 17 00  31.9 -55.5  4.9      76.2    62     9733   21 02 58

21 04 00  3C66A        07 17 00  31.9 -55.5  4.9      76.2    -6     9733   21 04 06
21 06 00  ---          07 19 00  31.6 -55.4  4.9      75.9   114     9762   21 04 06

21 06 00  3C66A        07 19 00  31.6 -55.4  4.9      75.9    -6     9762   21 06 06
21 07 20  ---          07 20 21  31.3 -55.3  4.9      75.7    74     9781   21 06 06

21 07 20  SN1986J      07 20 21  31.1 -56.1  4.9      75.2    -8     9781   21 07 28
21 09 10  ---          07 22 11  30.8 -56.0  5.0      75.0   102     9808   21 07 28

21 09 10  3C66A        07 22 11  31.0 -55.2  5.0      75.4    -8     9808   21 09 18
21 10 30  ---          07 23 31  30.8 -55.1  5.0      75.2    72     9826   21 09 18

21 10 30  SN1986J      07 23 31  30.6 -55.9  5.0      74.8    -8     9826   21 10 38
21 12 20  ---          07 25 21  30.2 -55.8  5.0      74.5   102     9852   21 10 38

21 12 20  3C66A        07 25 21  30.4 -55.0  5.0      75.0    -8     9852   21 12 28
21 13 40  ---          07 26 42  30.2 -54.9  5.0      74.8    72     9871   21 12 28

21 13 40  SN1986J      07 26 42  30.0 -55.7  5.1      74.4    -8     9871   21 13 48
21 15 30  ---          07 28 32  29.7 -55.6  5.1      74.1   102     9897   21 13 48

21 15 30  3C66A        07 28 32  29.9 -54.8  5.1      74.5    -8     9897   21 15 38
21 16 50  ---          07 29 52  29.6 -54.8  5.1      74.3    72     9916   21 15 38

21 16 50  SN1986J      07 29 52  29.4 -55.5  5.1      73.9    -8     9916   21 16 58
21 18 40  ---          07 31 42  29.1 -55.4  5.1      73.7   102     9942   21 16 58

21 18 40  3C66A        07 31 42  29.3 -54.7  5.1      74.1    -8     9942   21 18 48
21 20 00  ---          07 33 03  29.1 -54.6  5.2      73.9    72     9961   21 18 48

21 20 00  SN1986J      07 33 03  28.9 -55.3  5.2      73.5    -8     9961   21 20 08
21 21 50  ---          07 34 53  28.5 -55.2  5.2      73.2   102     9987   21 20 08

21 21 50  3C66A        07 34 53  28.8 -54.5  5.2      73.6    -8     9987   21 21 58
21 23 10  ---          07 36 13  28.5 -54.4  5.2      73.4    72    10005   21 21 58

21 23 10  SN1986J      07 36 13  28.3 -55.2  5.2      73.0    -8    10005   21 23 18
21 25 00  ---          07 38 04  28.0 -55.0  5.2      72.8   102    10032   21 23 18

21 25 00  3C66A        07 38 04  28.2 -54.3  5.2      73.2    -8    10032   21 25 08
21 26 20  ---          07 39 24  28.0 -54.2  5.3      73.0    72    10050   21 25 08
Schedule for VLBA_FD   (Code Fd )                                   Page  33
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

21 26 20  SN1986J      07 39 24  27.7 -55.0  5.3      72.6    -8    10050   21 26 28
21 28 10  ---          07 41 14  27.4 -54.8  5.3      72.3   102    10077   21 26 28

21 28 10  3C66A        07 41 14  27.7 -54.1  5.3      72.7    -8    10077   21 28 18
21 29 30  ---          07 42 34  27.4 -54.0  5.3      72.5    72    10095   21 28 18

21 29 30  SN1986J      07 42 34  27.2 -54.8  5.3      72.1    -8    10095   21 29 38
21 31 20  ---          07 44 25  26.9 -54.6  5.3      71.9   102    10121   21 29 38

21 31 20  3C66A        07 44 25  27.1 -53.9  5.3      72.2    -8    10121   21 31 28
21 32 40  ---          07 45 45  26.9 -53.8  5.4      72.1    72    10140   21 31 28

21 32 40  SN1986J      07 45 45  26.6 -54.6  5.4      71.7    -8    10140   21 32 48
21 34 30  ---          07 47 35  26.3 -54.4  5.4      71.4   102    10166   21 32 48

21 34 30  3C66A        07 47 35  26.6 -53.7  5.4      71.8    -8    10166   21 34 38
21 35 50  ---          07 48 55  26.3 -53.6  5.4      71.6    72    10185   21 34 38

21 35 50  SN1986J      07 48 55  26.1 -54.3  5.4      71.3    -8    10185   21 35 58
21 37 40  ---          07 50 46  25.8 -54.2  5.5      71.0   102    10211   21 35 58

 ---------- start of phase-ref block; pointing for VLA 7 ----------

21 37 40  SN1986J      07 50 46  25.8 -54.2  5.5      71.0    -6    10211   21 37 46
21 39 30  ---          07 52 36  25.4 -54.1  5.5      70.7   104    10238   21 37 46

21 39 30  3C66A        07 52 36  25.7 -53.4  5.5      71.1    -8    10238   21 39 38
21 40 40  ---          07 53 46  25.5 -53.3  5.5      70.9    62    10254   21 39 38

21 40 40  3C66A        07 53 46  25.5 -53.3  5.5      70.9    -6    10254   21 40 46
21 42 10  ---          07 55 16  25.2 -53.2  5.5      70.7    84    10275   21 40 46

21 42 10  3C66A        07 55 16  25.2 -53.2  5.5      70.7    -6    10275   21 42 16
21 43 30  ---          07 56 37  25.0 -53.1  5.5      70.5    74    10294   21 42 16

21 43 30  SN1986J      07 56 37  24.7 -53.8  5.5      70.2    -8    10294   21 43 38
21 45 20  ---          07 58 27  24.4 -53.7  5.6      69.9   102    10321   21 43 38

21 45 20  3C66A        07 58 27  24.7 -53.0  5.6      70.2    -8    10321   21 45 28
21 46 40  ---          07 59 47  24.5 -52.9  5.6      70.1    72    10339   21 45 28

21 46 40  SN1986J      07 59 47  24.2 -53.6  5.6      69.7    -8    10339   21 46 48
21 48 30  ---          08 01 37  23.9 -53.5  5.6      69.5   102    10366   21 46 48
Schedule for VLBA_FD   (Code Fd )                                   Page  34
               SN1986J in NGC891: VLBA/MkIV 1.4cm pol.
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Fri   8 Jun 2018   Day 159 ---

21 48 30  3C66A        08 01 37  24.1 -52.8  5.6      69.8    -8    10366   21 48 38
21 49 50  ---          08 02 58  23.9 -52.7  5.7      69.6    72    10384   21 48 38

21 49 50  SN1986J      08 02 58  23.6 -53.4  5.7      69.3    -8    10384   21 49 58
21 51 40  ---          08 04 48  23.3 -53.3  5.7      69.0   102    10410   21 49 58

21 51 40  3C66A        08 04 48  23.6 -52.5  5.7      69.3    -8    10410   21 51 48
21 53 00  ---          08 06 08  23.4 -52.5  5.7      69.2    72    10429   21 51 48

21 53 00  SN1986J      08 06 08  23.1 -53.2  5.7      68.8    -8    10429   21 53 08
21 54 50  ---          08 07 58  22.8 -53.0  5.7      68.6   102    10455   21 53 08

21 54 50  3C66A        08 07 58  23.1 -52.3  5.7      68.9    -8    10455   21 54 58
21 56 30  ---          08 09 39  22.8 -52.2  5.8      68.6    92    10479   21 54 58

21 56 30  3C84         08 09 39  32.4 -57.5  4.8      75.9   -27    10479   21 56 56
22 00 00  ---          08 13 09  31.7 -57.3  4.9      75.4   183    10526   21 56 56


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess218.K2048glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    7         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  14  Setup file default.  Used with PCAL = off
   LO sum=   22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
   BBC fr=     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     728.00    728.00    792.00    792.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  14  15  16  17  18  21  22  23  24  25

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * SN1986J           02 19 22.592220   * 02 22 31.320000     02 23 39.013501       0.00
                     42 06 18.95870    * 42 19 57.28200      42 24 38.37363        0.00
                     From catalog imbedded in main SCHED input file.

 * 3C66A             02 19 29.982891   * 02 22 39.611477     02 23 47.629821       0.00
                     42 48 29.80879    * 43 02 07.79928      43 06 48.65770        0.00
                     From catalog imbedded in main SCHED input file.

   J0319+4130        03 16 29.567260   * 03 19 48.160090     03 20 59.097460       1.30
   0316+413          41 19 51.91699    * 41 30 42.10412      41 34 23.13954        2.72
 * 3C84              /home/guest/rmc/SCHED/sched11.4/catalogs/sources.vlba.2012jul
   J0319+41          GSFC 2011B astro solution      9957 Observations

   J1331+3030        13 28 49.657778   * 13 31 08.288070     13 31 59.220478       0.20
 * 3C286             30 45 58.64061    * 30 30 32.95925      30 25 07.00819        0.19
   1328+307          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.vlba.2012jul
   J1331+30          rfc_2012b Petrov, 2012, unpublished 542 observations

   J2253+1608        22 51 29.519738   * 22 53 57.747937     22 54 51.783140       0.68
 * 3C454.3           15 52 54.34810    * 16 08 53.56093      16 14 36.87134        0.72
   2251+158          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.vlba.2012jul
   J2253+16          GSFC 2011B astro solution     39747 Observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  SN1986J    sess218.K2048glob     1 2 3 4 5 6 8 10 12 13 14 1 +    10.649  1202.556
  3C66A      sess218.K2048glob     1 2 3 4 5 6 8 10 12 13 14 1 +     7.714   859.721
             ps/vla_x_pointing.set 20                                1.125     0.000
  3C84       sess218.K2048glob     1 2 3 4 5 6 8 10 12 14 19         0.183    17.025
             ps/vla_x_pointing.set 20                                0.056     0.000
  3C286      sess218.K2048glob     19                                0.067     0.000
             ps/vla_x_pointing.set 20                                0.217     0.000
  3C454.3    sess218.K2048glob     1 2 4 5 6 8 10 12 14 19           0.069    11.439
             ps/vla_x_pointing.set 20                                0.111     0.000


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1986J             38.9
   3C66A               39.1
   3C84                28.9
   3C286              106.0
   3C454.3             86.3

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

