  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
 Exp. Code:  GI001C  


Schedule Version:       1.00                                              
Processed by SCHED version: NRAO internal release of 4 October 2004       

PI:       Hiroshi Imai                                                    

Address:  Department of Physics                                           
          Kagoshima University                                            
          Japan                                                           
          1-21-35 Korimoto, Kagoshima 890-0065                            

Phone:    81-99-285-8960                                                  
EMAIL:    hiroimai@sci.kagoshima-u.ac.jp                                  
Fax:      81-99-285-8960                                                  
Phone during observation: 81-99-285-8960                                  

Observing mode: VLBA/MKIV                                                 

Notes:    P-cal signal should be off.                                     
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

 Next scan frequencies:  1611.76  1611.76  1614.28  1614.28  1618.28  1618.28
                         1622.28  1622.28
 Next BBC frequencies:    788.24   788.24   785.72   785.72   781.72   781.72
                          777.72   777.72
 Next scan bandwidths:      1.00     1.00     4.00     4.00     4.00     4.00
                            4.00     4.00

10 06 00  1830+139     13 51 25  23.8  87.4 -4.7     -62.3     0   1  1      0  10 06 00
10 13 00  ---          13 58 26  25.3  88.3 -4.6     -62.4   420   F  1   5600

10 14 00  W43AOH       13 59 26  14.4 100.9 -4.8     -57.7    32   1  1   5600  10 14 00
10 29 00  ---          14 14 29  17.5 103.0 -4.6     -57.0   900   F  1  17600

10 30 00  W43AOH       14 15 29  17.8 103.1 -4.5     -57.0    54   1  2  17600  10 30 00
10 52 00  ---          14 37 33  22.3 106.4 -4.2     -55.7  1320   R  1      0

10 54 00  1830+139     14 39 33  34.1  93.6 -3.9     -62.2    90   1  1      0  10 54 00
11 01 00  ---          14 46 34  35.6  94.6 -3.8     -62.1   420   F  2   5600

11 02 00  OT081        14 47 34  42.4 106.1 -3.1     -57.0    41   1  1   5600  11 02 00
11 09 00  ---          14 54 35  43.8 107.4 -3.0     -56.4   420   F  2  11200

11 10 00  2145+067     14 55 36  -7.6  77.2 -6.9  D  -57.7   -29   1  1  11200  11 10 00
11 18 00  ---          15 03 37  -5.9  78.2 -6.7  D  -58.1     0   F  2  17600

11 20 00  W43AOH       15 05 37  28.1 110.9 -3.7     -53.6    62   1  2  17600  11 20 00
11 42 00  ---          15 27 41  32.4 114.7 -3.3     -51.4  1320   R  2      0

11 43 00  W43AOH       15 28 41  32.6 114.9 -3.3     -51.3    54   1  3      0  11 43 00
12 05 00  ---          15 50 45  36.9 119.2 -3.0     -48.7  1320   F  1  17600

12 06 00  W43AOH       15 51 45  37.1 119.5 -2.9     -48.6    54   1  4  17600  12 06 00
12 21 00  ---          16 06 47  39.8 122.7 -2.7     -46.4   900   R  1   5600

12 23 00  2145+067     16 08 48   7.9  86.6 -5.7     -59.9    50   1  4   5600  12 23 00
12 30 00  ---          16 15 49   9.4  87.4 -5.5     -60.0   420   R  1      0

12 32 00  OT081        16 17 49  59.7 128.9 -1.6     -42.8    14   1  3      0  12 32 00
12 37 00  ---          16 22 50  60.5 130.7 -1.5     -41.4   300   F  2   4000

12 38 00  TXS1843      16 23 50  44.3 125.5 -2.4     -44.5    22   1  3   4000  12 38 00
12 40 00  ---          16 25 50  44.7 126.0 -2.3     -44.1   120   F  2   5600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

12 40 00  TXS1843      16 25 50  44.7 126.0 -2.3     -44.1    -4   1  3   5600  12 40 00
12 42 30  ---          16 28 21  45.1 126.6 -2.3     -43.7   146   F  2   7600

12 42 30  W43AOH       16 28 21  43.6 127.8 -2.3     -42.8    -9   1  3   7600  12 42 30
12 45 00  ---          16 30 51  44.0 128.5 -2.3     -42.4   141   F  2   9600

12 45 00  TXS1843      16 30 51  45.6 127.3 -2.3     -43.2    -9   1  3   9600  12 45 00
12 47 30  ---          16 33 22  46.0 127.9 -2.2     -42.7   141   F  2  11600

12 47 30  W43AOH       16 33 22  44.5 129.1 -2.2     -41.9    -9   1  3  11600  12 47 30
12 50 00  ---          16 35 52  44.9 129.8 -2.2     -41.4   141   F  2  13600

12 50 00  TXS1843      16 35 52  46.4 128.6 -2.2     -42.3    -9   1  3  13600  12 50 00
12 52 30  ---          16 38 22  46.8 129.3 -2.1     -41.8   141   F  2  15600

12 52 30  W43AOH       16 38 22  45.3 130.4 -2.2     -40.9    -9   1  3  15600  12 52 30
12 55 00  ---          16 40 53  45.7 131.1 -2.1     -40.4   141   F  2  17600

12 56 00  TXS1843      16 41 53  47.4 130.2 -2.1     -41.1    51   1  4  17600  12 56 00
12 58 00  ---          16 43 53  47.7 130.8 -2.0     -40.6   120   R  2  16000

12 58 00  TXS1843      16 43 53  47.7 130.8 -2.0     -40.6    -4   1  4  16000  12 58 00
13 00 30  ---          16 46 24  48.1 131.5 -2.0     -40.1   146   R  2  14000

13 00 30  W43AOH       16 46 24  46.6 132.6 -2.0     -39.3    -9   1  4  14000  13 00 30
13 03 00  ---          16 48 54  47.0 133.4 -2.0     -38.7   141   R  2  12000

13 03 00  TXS1843      16 48 54  48.5 132.2 -2.0     -39.6    -9   1  4  12000  13 03 00
13 05 30  ---          16 51 25  48.9 133.0 -1.9     -39.0   141   R  2  10000

13 05 30  W43AOH       16 51 25  47.4 134.1 -1.9     -38.2    -9   1  4  10000  13 05 30
13 08 00  ---          16 53 55  47.7 134.8 -1.9     -37.6   141   R  2   8000

13 08 00  TXS1843      16 53 55  49.3 133.7 -1.9     -38.5    -9   1  4   8000  13 08 00
13 10 30  ---          16 56 25  49.7 134.5 -1.8     -37.9   141   R  2   6000

13 10 30  W43AOH       16 56 25  48.1 135.6 -1.9     -37.1    -9   1  4   6000  13 10 30
13 13 00  ---          16 58 56  48.5 136.3 -1.8     -36.5   141   R  2   4000

13 13 00  TXS1843      16 58 56  50.1 135.2 -1.8     -37.3    -9   1  4   4000  13 13 00
13 15 30  ---          17 01 26  50.5 136.0 -1.7     -36.7   141   R  2   2000

13 15 30  W43AOH       17 01 26  48.9 137.1 -1.8     -35.9    -9   1  4   2000  13 15 30
13 18 00  ---          17 03 57  49.2 137.9 -1.7     -35.3   141   R  2      0
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

13 20 00  OT081        17 05 57  66.5 150.6 -0.8     -25.3    80   1  5      0  13 20 00
13 25 00  ---          17 10 58  67.0 153.5 -0.7     -22.9   300   F  1   4000

13 26 00  TXS1843      17 11 58  52.0 139.5 -1.6     -34.0    24   1  5   4000  13 26 00
13 28 00  ---          17 13 58  52.3 140.1 -1.5     -33.5   120   F  1   5600

13 28 00  TXS1843      17 13 58  52.3 140.1 -1.5     -33.5    -4   1  5   5600  13 28 00
13 30 30  ---          17 16 29  52.6 141.0 -1.5     -32.8   146   F  1   7600

13 30 30  W43AOH       17 16 29  51.0 141.9 -1.5     -32.1    -9   1  5   7600  13 30 30
13 33 00  ---          17 18 59  51.3 142.8 -1.5     -31.4   141   F  1   9600

13 33 00  TXS1843      17 18 59  53.0 141.9 -1.5     -32.1    -9   1  5   9600  13 33 00
13 35 30  ---          17 21 29  53.3 142.8 -1.4     -31.4   141   F  1  11600

13 35 30  W43AOH       17 21 29  51.6 143.6 -1.4     -30.7    -9   1  5  11600  13 35 30
13 38 00  ---          17 24 00  51.9 144.5 -1.4     -30.0   141   F  1  13600

13 38 00  TXS1843      17 24 00  53.6 143.7 -1.4     -30.6    -9   1  5  13600  13 38 00
13 40 30  ---          17 26 30  53.9 144.6 -1.3     -29.9   141   F  1  15600

13 40 30  W43AOH       17 26 30  52.3 145.4 -1.4     -29.3    -9   1  5  15600  13 40 30
13 43 00  ---          17 29 01  52.6 146.3 -1.3     -28.5   141   F  1  17600

13 44 00  TXS1843      17 30 01  54.4 145.9 -1.3     -28.9    50   1  6  17600  13 44 00
13 46 00  ---          17 32 01  54.6 146.6 -1.2     -28.2   120   R  1  16000

13 46 00  TXS1843      17 32 01  54.6 146.6 -1.2     -28.2    -4   1  6  16000  13 46 00
13 48 30  ---          17 34 32  54.9 147.6 -1.2     -27.4   146   R  1  14000

13 48 30  W43AOH       17 34 32  53.2 148.3 -1.2     -26.9    -9   1  6  14000  13 48 30
13 51 00  ---          17 37 02  53.5 149.2 -1.2     -26.1   141   R  1  12000

13 51 00  TXS1843      17 37 02  55.2 148.6 -1.2     -26.6    -9   1  6  12000  13 51 00
13 53 30  ---          17 39 32  55.5 149.6 -1.1     -25.8   141   R  1  10000

13 53 30  W43AOH       17 39 32  53.7 150.2 -1.1     -25.3    -9   1  6  10000  13 53 30
13 56 00  ---          17 42 03  54.0 151.2 -1.1     -24.5   141   R  1   8000

13 56 00  TXS1843      17 42 03  55.7 150.6 -1.1     -25.0    -9   1  6   8000  13 56 00
13 58 30  ---          17 44 33  56.0 151.6 -1.0     -24.2   141   R  1   6000

13 58 30  W43AOH       17 44 33  54.3 152.1 -1.1     -23.7    -9   1  6   6000  13 58 30
14 01 00  ---          17 47 04  54.5 153.1 -1.0     -22.9   141   R  1   4000
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

14 01 00  TXS1843      17 47 04  56.2 152.6 -1.0     -23.3    -9   1  6   4000  14 01 00
14 03 30  ---          17 49 34  56.5 153.7 -0.9     -22.4   141   R  1   2000

14 03 30  W43AOH       17 49 34  54.8 154.1 -1.0     -22.1    -9   1  6   2000  14 03 30
14 06 00  ---          17 52 04  55.0 155.1 -0.9     -21.2   141   R  1      0

14 08 00  OT081        17 54 05  69.0 181.6  0.0       1.4    86   1  5      0  14 08 00
14 13 00  ---          17 59 06  68.9 185.0  0.1       4.4   300   F  2   4000

14 14 00  TXS1843      18 00 06  57.4 158.2 -0.8     -18.7    31   1  5   4000  14 14 00
14 16 00  ---          18 02 06  57.6 159.1 -0.7     -17.9   120   F  2   5600

14 16 00  TXS1843      18 02 06  57.6 159.1 -0.7     -17.9    -4   1  5   5600  14 16 00
14 18 30  ---          18 04 37  57.7 160.2 -0.7     -17.0   146   F  2   7600

14 18 30  W43AOH       18 04 37  56.0 160.4 -0.7     -16.8    -9   1  5   7600  14 18 30
14 21 00  ---          18 07 07  56.2 161.4 -0.7     -15.9   141   F  2   9600

14 21 00  TXS1843      18 07 07  57.9 161.3 -0.7     -16.0    -9   1  5   9600  14 21 00
14 23 30  ---          18 09 37  58.1 162.4 -0.6     -15.0   141   F  2  11600

14 23 30  W43AOH       18 09 37  56.4 162.5 -0.6     -15.0    -9   1  5  11600  14 23 30
14 26 00  ---          18 12 08  56.5 163.6 -0.6     -14.0   141   F  2  13600

14 26 00  TXS1843      18 12 08  58.2 163.6 -0.6     -14.1    -9   1  5  13600  14 26 00
14 28 30  ---          18 14 38  58.4 164.8 -0.5     -13.1   141   F  2  15600

14 28 30  W43AOH       18 14 38  56.7 164.7 -0.6     -13.1    -9   1  5  15600  14 28 30
14 31 00  ---          18 17 09  56.8 165.8 -0.5     -12.1   141   F  2  17600

14 32 00  TXS1843      18 18 09  58.6 166.4 -0.5     -11.7    50   1  6  17600  14 32 00
14 34 00  ---          18 20 09  58.7 167.3 -0.4     -10.9   120   R  2  16000

14 34 00  TXS1843      18 20 09  58.7 167.3 -0.4     -10.9    -4   1  6  16000  14 34 00
14 36 30  ---          18 22 39  58.8 168.5 -0.4      -9.9   146   R  2  14000

14 36 30  W43AOH       18 22 39  57.1 168.3 -0.4     -10.0    -9   1  6  14000  14 36 30
14 39 00  ---          18 25 10  57.2 169.5 -0.4      -9.1   141   R  2  12000

14 39 00  TXS1843      18 25 10  58.9 169.7 -0.4      -8.8    -9   1  6  12000  14 39 00
14 41 30  ---          18 27 40  59.0 170.9 -0.3      -7.8   141   R  2  10000

14 41 30  W43AOH       18 27 40  57.3 170.6 -0.3      -8.1    -9   1  6  10000  14 41 30
14 44 00  ---          18 30 11  57.3 171.8 -0.3      -7.1   141   R  2   8000
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

14 44 00  TXS1843      18 30 11  59.1 172.1 -0.3      -6.8    -9   1  6   8000  14 44 00
14 46 30  ---          18 32 41  59.1 173.3 -0.2      -5.7   141   R  2   6000

14 46 30  W43AOH       18 32 41  57.4 172.9 -0.3      -6.1    -9   1  6   6000  14 46 30
14 49 00  ---          18 35 12  57.5 174.1 -0.2      -5.1   141   R  2   4000

14 49 00  TXS1843      18 35 12  59.2 174.6 -0.2      -4.7    -9   1  6   4000  14 49 00
14 51 30  ---          18 37 42  59.2 175.8 -0.1      -3.6   141   R  2   2000

14 51 30  W43AOH       18 37 42  57.5 175.2 -0.2      -4.1    -9   1  6   2000  14 51 30
14 54 00  ---          18 40 12  57.6 176.4 -0.1      -3.1   141   R  2      0

14 56 00  OT081        18 42 13  65.9 211.9  0.8      27.4    90   1  7      0  14 56 00
15 01 00  ---          18 47 14  65.4 214.5  0.9      29.6   300   F  1   4000

15 02 00  TXS1843      18 48 14  59.3 180.9  0.0       0.8    32   1  7   4000  15 02 00
15 04 00  ---          18 50 14  59.3 181.9  0.1       1.7   120   F  1   5600

15 04 00  TXS1843      18 50 14  59.3 181.9  0.1       1.7    -4   1  7   5600  15 04 00
15 06 30  ---          18 52 44  59.3 183.1  0.1       2.7   146   F  1   7600

15 06 30  W43AOH       18 52 44  57.6 182.2  0.1       1.9    -9   1  7   7600  15 06 30
15 09 00  ---          18 55 15  57.6 183.4  0.1       2.9   141   F  1   9600

15 09 00  TXS1843      18 55 15  59.2 184.4  0.1       3.8    -9   1  7   9600  15 09 00
15 11 30  ---          18 57 45  59.2 185.6  0.2       4.8   141   F  1  11600

15 11 30  W43AOH       18 57 45  57.5 184.6  0.2       3.9    -9   1  7  11600  15 11 30
15 14 00  ---          19 00 16  57.5 185.7  0.2       4.9   141   F  1  13600

15 14 00  TXS1843      19 00 16  59.1 186.8  0.2       5.9    -9   1  7  13600  15 14 00
15 16 30  ---          19 02 46  59.1 188.0  0.3       6.9   141   F  1  15600

15 16 30  W43AOH       19 02 46  57.4 186.9  0.2       5.9    -9   1  7  15600  15 16 30
15 19 00  ---          19 05 16  57.4 188.0  0.3       6.9   141   F  1  17600

15 20 00  TXS1843      19 06 17  58.9 189.7  0.3       8.3    51   1  8  17600  15 20 00
15 22 00  ---          19 08 17  58.9 190.7  0.4       9.2   120   R  1  16000

15 22 00  TXS1843      19 08 17  58.9 190.7  0.4       9.2    -4   1  8  16000  15 22 00
15 24 30  ---          19 10 47  58.8 191.9  0.4      10.2   146   R  1  14000

15 24 30  W43AOH       19 10 47  57.2 190.6  0.4       9.1    -9   1  8  14000  15 24 30
15 27 00  ---          19 13 18  57.1 191.7  0.4      10.1   141   R  1  12000
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

15 27 00  TXS1843      19 13 18  58.6 193.0  0.4      11.2    -9   1  8  12000  15 27 00
15 29 30  ---          19 15 48  58.5 194.2  0.5      12.2   141   R  1  10000

15 29 30  W43AOH       19 15 48  56.9 192.8  0.5      11.0    -9   1  8  10000  15 29 30
15 32 00  ---          19 18 19  56.8 194.0  0.5      12.0   141   R  1   8000

15 32 00  TXS1843      19 18 19  58.4 195.4  0.5      13.2    -9   1  8   8000  15 32 00
15 34 30  ---          19 20 49  58.2 196.6  0.6      14.2   141   R  1   6000

15 34 30  W43AOH       19 20 49  56.7 195.1  0.5      12.9    -9   1  8   6000  15 34 30
15 37 00  ---          19 23 19  56.5 196.2  0.6      13.9   141   R  1   4000

15 37 00  TXS1843      19 23 19  58.1 197.7  0.6      15.2    -9   1  8   4000  15 37 00
15 39 30  ---          19 25 50  57.9 198.8  0.7      16.1   141   R  1   2000

15 39 30  W43AOH       19 25 50  56.4 197.3  0.6      14.8    -9   1  8   2000  15 39 30
15 42 00  ---          19 28 20  56.2 198.4  0.7      15.7   141   R  1      0

15 44 00  OT081        19 30 21  58.9 232.8  1.6      44.0    91   1  7      0  15 44 00
15 49 00  ---          19 35 21  58.0 234.4  1.7      45.2   300   F  2   4000

15 50 00  TXS1843      19 36 22  57.1 203.5  0.8      20.1    33   1  7   4000  15 50 00
15 52 00  ---          19 38 22  56.9 204.4  0.9      20.8   120   F  2   5600

15 52 00  TXS1843      19 38 22  56.9 204.4  0.9      20.8    -4   1  7   5600  15 52 00
15 54 30  ---          19 40 52  56.7 205.4  0.9      21.7   146   F  2   7600

15 54 30  W43AOH       19 40 52  55.2 203.7  0.9      20.2    -9   1  7   7600  15 54 30
15 57 00  ---          19 43 23  55.0 204.7  0.9      21.1   141   F  2   9600

15 57 00  TXS1843      19 43 23  56.4 206.5  1.0      22.6    -9   1  7   9600  15 57 00
15 59 30  ---          19 45 53  56.2 207.5  1.0      23.4   141   F  2  11600

15 59 30  W43AOH       19 45 53  54.8 205.7  1.0      21.9    -9   1  7  11600  15 59 30
16 02 00  ---          19 48 24  54.6 206.7  1.0      22.8   141   F  2  13600

16 02 00  TXS1843      19 48 24  55.9 208.5  1.0      24.3    -9   1  7  13600  16 02 00
16 04 30  ---          19 50 54  55.7 209.6  1.1      25.1   141   F  2  15600

16 04 30  W43AOH       19 50 54  54.3 207.7  1.0      23.6    -9   1  7  15600  16 04 30
16 07 00  ---          19 53 24  54.1 208.7  1.1      24.4   141   F  2  17600

16 08 00  TXS1843      19 54 25  55.3 211.0  1.1      26.3    52   1  8  17600  16 08 00
16 10 00  ---          19 56 25  55.1 211.7  1.2      26.9   120   R  2  16000
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

16 10 00  TXS1843      19 56 25  55.1 211.7  1.2      26.9    -4   1  8  16000  16 10 00
16 12 30  ---          19 58 55  54.8 212.7  1.2      27.7   146   R  2  14000

16 12 30  W43AOH       19 58 55  53.5 210.8  1.2      26.1    -9   1  8  14000  16 12 30
16 15 00  ---          20 01 26  53.2 211.7  1.2      26.9   141   R  2  12000

16 15 00  TXS1843      20 01 26  54.5 213.7  1.3      28.5    -9   1  8  12000  16 15 00
16 17 30  ---          20 03 56  54.2 214.6  1.3      29.3   141   R  2  10000

16 17 30  W43AOH       20 03 56  52.9 212.6  1.3      27.7    -9   1  8  10000  16 17 30
16 20 00  ---          20 06 26  52.6 213.6  1.3      28.4   141   R  2   8000

16 20 00  TXS1843      20 06 26  53.9 215.5  1.3      30.0    -9   1  8   8000  16 20 00
16 22 30  ---          20 08 57  53.6 216.4  1.4      30.7   141   R  2   6000

16 22 30  W43AOH       20 08 57  52.3 214.5  1.4      29.2    -9   1  8   6000  16 22 30
16 25 00  ---          20 11 27  52.0 215.4  1.4      29.9   141   R  2   4000

16 25 00  TXS1843      20 11 27  53.2 217.3  1.4      31.5    -8   1  8   4000  16 25 00
16 27 30  ---          20 13 58  52.9 218.2  1.5      32.2   142   R  2   2000

16 27 30  W43AOH       20 13 58  51.7 216.2  1.4      30.6    -8   1  8   2000  16 27 30
16 30 00  ---          20 16 28  51.4 217.1  1.5      31.3   142   R  2      0

16 32 00  OT081        20 18 28  50.0 246.3  2.4      53.0    95   1  9      0  16 32 00
16 37 00  ---          20 23 29  49.0 247.4  2.5      53.7   300   F  1   4000

16 38 00  W43AOH       20 24 29  50.3 219.8  1.6      33.4    36   1  9   4000  16 38 00
16 55 00  ---          20 41 32  47.8 225.1  1.9      37.5  1020   F  1  17600

16 56 00  W43AOH       20 42 32  47.7 225.4  1.9      37.8    54   1 10  17600  16 56 00
17 18 00  ---          21 04 36  44.1 231.4  2.3      42.3  1320   R  1      0

17 20 00  OT081        21 06 36  40.2 255.8  3.2      57.8    98   1  9      0  17 20 00
17 25 00  ---          21 11 37  39.1 256.7  3.3      58.1   300   F  2   4000

17 26 00  W43AOH       21 12 37  42.7 233.4  2.4      43.7    39   1  9   4000  17 26 00
17 43 00  ---          21 29 40  39.7 237.4  2.7      46.5  1020   F  2  17600

17 44 00  W43AOH       21 30 40  39.5 237.7  2.7      46.7    54   1 10  17600  17 44 00
18 06 00  ---          21 52 44  35.4 242.3  3.1      49.7  1320   R  2      0

18 07 00  OT081        21 53 44  30.2 263.1  4.0      60.1    40   1 11      0  18 07 00
18 12 00  ---          21 58 45  29.1 263.8  4.1      60.2   300   F  1   4000
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed   2 Mar 2005   Day  61 ---

18 13 00  W43AOH       21 59 45  34.1 243.7  3.2      50.5    41   1 11   4000  18 13 00
18 30 00  ---          22 16 48  30.8 246.8  3.5      52.3  1020   F  1  17600

18 32 00  W43AOH       22 18 48  30.4 247.2  3.5      52.5   113   1 12  17600  18 32 00
18 54 00  ---          22 40 52  25.9 250.9  3.9      54.4  1320   R  1      0

18 56 00  OT081        22 42 52  19.7 269.7  4.9      60.8   101   1 11      0  18 56 00
19 01 00  ---          22 47 53  18.6 270.4  4.9      60.8   300   F  2   4000

19 02 00  W43AOH       22 48 53  24.3 252.2  4.0      55.0    42   1 11   4000  19 02 00
19 19 00  ---          23 05 56  20.8 254.8  4.3      56.2  1020   F  2  17600

19 21 00  W43AOH       23 07 56  20.4 255.1  4.3      56.3   113   1 12  17600  19 21 00
19 43 00  ---          23 30 00  15.7 258.2  4.7      57.4  1320   R  2      0

19 44 00  W43AOH       23 31 00  15.5 258.4  4.7      57.5    54   1 13      0  19 44 00
20 06 00  ---          23 53 04  10.9 261.4  5.1      58.3  1320   F  1  17600

20 07 00  OT081        23 54 04   4.4 278.6  6.0      59.6    41   1 14  17600  20 07 00
20 18 00  ---          00 05 06   2.1 280.0  6.2  D   59.3     0   R  1   8800

20 19 00  2145+067     00 06 06  50.0 240.9  2.3      49.2   -42   1 14   8800  20 19 00
20 30 00  ---          00 17 08  47.9 243.6  2.5      50.9   618   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gw43a-oh.set
   Matches group v20cm_2 in /usr/local/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    1         Station: VLBA              Total bit rate:  128
   Format: VLBA1:1           Bits per sample: 2         Sample rate:  8.000
   Number of channels:  8    Passes/head pos:   2       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

  Frequency Set:   8  Based on FREQ, BW, and/or DOPPLER in schedule.  Used pcal sets:   1
   LO sum=    1611.76   1611.76   1614.28   1614.28   1618.28   1618.28   1622.28   1622.28
   BBC fr=     788.24    788.24    785.72    785.72    781.72    781.72    777.72    777.72
   Bandwd=      1.000     1.000     4.000     4.000     4.000     4.000     4.000     4.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = OFF 
    PCALXB1=   S1    S2    S3    S4    S5    S6    S7    S8 
    PCALXB2=   M1    M2    M3    M4    M5    M6    M7    M8 
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0

   Track assignments are: 
    track1=   2,  6, 10, 14, 18, 22, 26, 30
    track2=   3,  7, 11, 15, 19, 23, 27, 31
    barrel=roll_off 
 SOURCE LIST -- GI10C: 1612 MHz OH masers in W43A (H. Imai and P.J. Diamond)
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

   J1751+0939        17 49 10.387930   * 17 51 32.818573     17 51 46.744239 
   1749+096          09 39 42.82582    * 09 39 00.72837      09 38 37.66032 
   J1751+09          From catalog imbedded in main SCHED input file.
 * OT081             USNO - Ref Frame 1998-6, Eubanks June 1998
                     Doppler based on other sources.

   J1832+1357        18 30 26.112214   * 18 32 43.471123     18 32 56.637427 
 * 1830+139          13 55 26.71680    * 13 57 44.40030      13 57 38.61481 
                     From catalog imbedded in main SCHED input file.
                     VLBA Calib. Survey - ICRF Frame - reduced by GSFC group
                     Doppler based on other sources.

   J2148+0657        21 45 36.078481   * 21 48 05.458679     21 48 19.174511 
 * 2145+067          06 43 40.90462    * 06 57 38.60422      06 58 50.37709 
   J2148+06          From catalog imbedded in main SCHED input file.
                     ICRF - Ext.1 Source - 1998 IERS Annual Report
                     Doppler based on other sources.

 * W43AOH            18 45 05.339856   * 18 47 41.163000     18 47 56.157477 
                    -01 48 32.70202    *-01 45 11.22000     -01 45 06.10776 
                     From catalog imbedded in main SCHED input file.
                     Doppler based on LSR frame and radio definition.  Velocities:
                         35.00    35.00    35.00    35.00    35.00    35.00    35.00    35.00


 * TXS1843           18 43 30.011769   * 18 46 03.900000     18 46 18.704387 
   TXS1843-001      -00 06 52.60264    *-00 03 38.00000     -00 03 34.07885 
                     From catalog imbedded in main SCHED input file.
                     Doppler based on other sources.

 * 1851+005          18 49 13.574417   * 18 51 46.723100     18 52 01.424519 
   J1851+0035        00 31 53.27360    * 00 35 32.34800      00 35 38.59231 
                     From catalog imbedded in main SCHED input file.
                     Cataloged in JVAS and having a flux of 0.45 Jy a the X-band
                     Doppler based on other sources.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   OT081               77.0
   1830+139            68.0
   2145+067            21.5
   W43AOH              61.4
   TXS1843             62.0
   1851+005            60.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

