  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: M82 transient (ToO)
 Exp. Code:  GB071B  


Schedule Version:       2.00
Processed by SCHED version:   9.30  Release near March 23, 2010

PI:       Andreas Brunthaler

Address:  MPIfR
          Auf dem Huegel 69
          53121 Bonn
          Germany

Phone:    +49 228 525 377
EMAIL:    brunthal@mpifr-bonn.mpg.de
Fax:      +49 228 525 229
Phone during observation: +49 228 525 377

Observing mode: VLBA+EVN at 6 cm

Notes:    VLBA 512 Mbps; EVN 1 Gbps
          CORRELATION IN SOCORRO
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

 Next scan frequencies:  4942.49  4942.49  4942.49  4942.49  4974.49  4974.49
                         4974.49  4974.49  5006.49  5006.49  5006.49  5006.49
                         5038.49  5038.49  5038.49  5038.49
 Next BBC frequencies:    842.49   842.49   842.49   842.49   874.49   874.49
                          874.49   874.49   906.49   906.49   906.49   906.49
                          938.49   938.49   938.49   938.49
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00    16.00    16.00    16.00    16.00
                           16.00    16.00    16.00    16.00

10 30 00  3C454.3      20 01 36  48.1 100.0 -2.9     -61.9     0   1  1      0  10 30 00
10 34 00  ---          20 05 37  48.9 100.7 -2.8     -61.7   240   F  1     15  10 30 00

10 34 30  J1048+7143   20 06 07  16.2 -12.3  9.3      35.8   -51   1  1     15  10 34 30
10 38 30  =1044+719    20 10 07  16.0 -12.1  9.3      34.9   189   F  1     31  10 34 30

10 38 30  M81          20 10 07  11.6  -9.4 10.2      23.1   -15   1  1     31  No stop 
10 40 30  ---          20 12 08  11.5  -9.2 10.3      22.7   105   F  1     39  10 38 30

10 40 30  M82          20 12 08  12.1  -9.0 10.3      22.8    -7   1  1     39  No stop 
10 42 30  ---          20 14 08  12.0  -8.9 10.3      22.4   113   F  1     46  10 40 30

10 42 30  M81          20 14 08  11.4  -9.1 10.3      22.3    -7   1  1     46  No stop 
10 44 00  ---          20 15 38  11.4  -8.9 10.3      21.9    83   F  1     52  10 42 30

10 44 00  M82          20 15 38  11.9  -8.7 10.3      22.1    -7   1  1     52  No stop 
10 46 00  ---          20 17 39  11.9  -8.6 10.3      21.6   113   F  1     60  10 44 00

10 46 30  M81          20 18 09  11.3  -8.7 10.4      21.4    23   1  1     60  10 46 30
10 47 30  ---          20 19 09  11.2  -8.6 10.4      21.2    60   F  1     64  10 46 30

10 47 30  M82          20 19 09  11.8  -8.4 10.4      21.3    -7   1  1     64  No stop 
10 49 30  ---          20 21 09  11.8  -8.3 10.4      20.9   113   F  1     72  10 47 30

10 49 30  M81          20 21 09  11.2  -8.5 10.4      20.7    -7   1  1     72  No stop 
10 51 00  ---          20 22 39  11.1  -8.3 10.4      20.4    83   F  1     77  10 49 30

10 51 00  M82          20 22 39  11.7  -8.2 10.4      20.5    -7   1  1     77  No stop 
10 53 00  ---          20 24 40  11.7  -8.0 10.5      20.1   113   F  1     85  10 51 00

10 53 00  M81          20 24 40  11.1  -8.2 10.5      20.0    -7   1  1     85  No stop 
10 54 30  ---          20 26 10  11.0  -8.0 10.5      19.7    83   F  1     91  10 53 00
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

10 54 30  M82          20 26 10  11.6  -7.9 10.5      19.8    -7   1  1     91  No stop 
10 56 30  ---          20 28 10  11.6  -7.7 10.5      19.3   113   F  1     99  10 54 30

10 57 00  M81          20 28 40  11.0  -7.8 10.5      19.1    23   1  1     99  10 57 00
10 58 00  ---          20 29 41  10.9  -7.7 10.6      18.9    60   F  1    103  10 57 00

10 58 00  M82          20 29 41  11.5  -7.6 10.5      19.0    -7   1  1    103  No stop 
11 00 00  ---          20 31 41  11.5  -7.4 10.6      18.6   113   F  1    110  10 58 00

11 00 00  M81          20 31 41  10.9  -7.6 10.6      18.5    -7   1  1    110  No stop 
11 01 30  ---          20 33 11  10.8  -7.4 10.6      18.1    83   F  1    116  11 00 00

11 01 30  M82          20 33 11  11.4  -7.3 10.6      18.2    -7   1  1    116  No stop 
11 03 30  ---          20 35 11  11.4  -7.1 10.6      17.8   113   F  1    124  11 01 30

11 04 00  M81          20 35 42  10.8  -7.2 10.7      17.6    23   1  1    124  11 04 00
11 05 00  ---          20 36 42  10.7  -7.1 10.7      17.4    60   F  1    128  11 04 00

11 05 00  M82          20 36 42  11.3  -7.0 10.7      17.5    -7   1  1    128  No stop 
11 07 00  ---          20 38 42  11.3  -6.8 10.7      17.0   113   F  1    135  11 05 00

11 07 00  M81          20 38 42  10.7  -7.0 10.7      16.9    -7   1  1    135  No stop 
11 08 30  ---          20 40 12  10.6  -6.8 10.7      16.6    83   F  1    141  11 07 00

11 08 30  M82          20 40 12  11.2  -6.7 10.7      16.7    -7   1  1    141  No stop 
11 10 30  ---          20 42 13  11.2  -6.5 10.8      16.3   113   F  1    149  11 08 30

11 10 30  M81          20 42 13  10.6  -6.7 10.8      16.2    -7   1  1    149  No stop 
11 12 00  ---          20 43 43  10.5  -6.5 10.8      15.8    83   F  1    155  11 10 30

11 12 00  M82          20 43 43  11.1  -6.4 10.8      15.9    -7   1  1    155  No stop 
11 14 00  ---          20 45 43  11.1  -6.2 10.8      15.5   113   F  1    163  11 12 00

11 14 30  M81          20 46 13  10.5  -6.3 10.8      15.3    23   1  1    163  11 14 30
11 15 30  ---          20 47 13  10.5  -6.2 10.8      15.1    60   F  1    166  11 14 30

11 15 30  M82          20 47 13  11.1  -6.1 10.8      15.2    -7   1  1    166  No stop 
11 17 30  ---          20 49 14  11.0  -5.9 10.9      14.7   113   F  1    174  11 15 30

11 17 30  M81          20 49 14  10.4  -6.0 10.9      14.6    -7   1  1    174  No stop 
11 19 00  ---          20 50 44  10.4  -5.9 10.9      14.3    83   F  1    180  11 17 30

11 19 00  M82          20 50 44  11.0  -5.8 10.9      14.4    -7   1  1    180  No stop 
11 21 00  ---          20 52 44  10.9  -5.6 10.9      14.0   113   F  1    188  11 19 00
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

11 21 30  M81          20 53 14  10.3  -5.7 10.9      13.8    23   1  1    188  11 21 30
11 22 30  ---          20 54 15  10.3  -5.6 11.0      13.6    60   F  1    192  11 21 30

11 22 30  M82          20 54 15  10.9  -5.5 11.0      13.6    -7   1  1    192  No stop 
11 24 30  ---          20 56 15  10.9  -5.3 11.0      13.2   113   F  1    199  11 22 30

11 24 30  M81          20 56 15  10.3  -5.4 11.0      13.1    -7   1  1    199  No stop 
11 26 00  ---          20 57 45  10.2  -5.3 11.0      12.8    83   F  1    205  11 24 30

11 26 00  M82          20 57 45  10.8  -5.2 11.0      12.9    -7   1  1    205  No stop 
11 28 00  ---          20 59 45  10.8  -5.0 11.1      12.4   113   F  1    213  11 26 00

11 28 00  M81          20 59 45  10.2  -5.1 11.1      12.4    -7   1  1    213  No stop 
11 29 30  ---          21 01 16  10.2  -5.0 11.1      12.0    83   F  1    219  11 28 00

11 29 30  M82          21 01 16  10.8  -4.9 11.1      12.1    -7   1  1    219  No stop 
11 31 30  ---          21 03 16  10.7  -4.7 11.1      11.7   113   F  1    226  11 29 30

11 32 00  M81          21 03 46  10.1  -4.8 11.1      11.5    23   1  1    226  11 32 00
11 33 00  ---          21 04 46  10.1  -4.7 11.1      11.3    60   F  1    230  11 32 00

11 33 30  J1048+7143   21 05 16  13.9  -8.2 10.3      22.9    16   1  1    230  11 33 30
11 36 30  =1044+719    21 08 17  13.8  -7.9 10.3      22.2   180   F  1    242  11 33 30

11 36 30  M81          21 08 17  10.0  -4.3 11.2      10.5   -14   1  1    242  No stop 
11 38 30  ---          21 10 17  10.0  -4.2 11.2      10.1   106   F  1    250  11 36 30

11 38 30  M82          21 10 17  10.6  -4.1 11.2      10.1    -7   1  1    250  No stop 
11 40 30  ---          21 12 18  10.6  -3.9 11.3       9.7   113   F  1    257  11 38 30

11 40 30  M81          21 12 18  10.0  -4.0 11.3       9.6    -7   1  1    257  No stop 
11 42 00  ---          21 13 48  10.0  -3.9 11.3       9.3    83   F  1    263  11 40 30

11 42 00  M82          21 13 48  10.6  -3.8 11.3       9.4    -7   1  1    263  No stop 
11 44 00  ---          21 15 48  10.5  -3.6 11.3       8.9   113   F  1    271  11 42 00

11 44 30  M81          21 16 18   9.9  -3.6 11.3       8.7    23   1  1    271  11 44 30
11 45 30  ---          21 17 18   9.9  -3.5 11.3       8.5    60   F  1    275  11 44 30

11 45 30  M82          21 17 18  10.5  -3.5 11.3       8.6    -7   1  1    275  No stop 
11 47 30  ---          21 19 19  10.5  -3.3 11.4       8.2   113   F  1    283  11 45 30

11 47 30  M81          21 19 19   9.9  -3.4 11.4       8.1    -7   1  1    283  No stop 
11 49 00  ---          21 20 49   9.9  -3.2 11.4       7.8    83   F  1    288  11 47 30
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

11 49 00  M82          21 20 49  10.5  -3.2 11.4       7.8    -7   1  1    288  No stop 
11 51 00  ---          21 22 49  10.5  -3.0 11.4       7.4   113   F  1    296  11 49 00

11 51 00  M81          21 22 49   9.8  -3.0 11.4       7.3    -7   1  1    296  No stop 
11 52 30  ---          21 24 20   9.8  -2.9 11.5       7.0    83   F  1    302  11 51 00

11 52 30  M82          21 24 20  10.4  -2.9 11.5       7.1    -7   1  1    302  No stop 
11 54 30  ---          21 26 20  10.4  -2.7 11.5       6.6   113   F  1    310  11 52 30

11 55 00  M81          21 26 50   9.8  -2.7 11.5       6.5    23   1  1    310  11 55 00
11 56 00  ---          21 27 50   9.8  -2.6 11.5       6.2    60   F  1    314  11 55 00

11 56 00  M82          21 27 50  10.4  -2.6 11.5       6.3    -7   1  1    314  No stop 
11 58 00  ---          21 29 50  10.4  -2.4 11.6       5.9   113   F  1    321  11 56 00

11 58 00  M81          21 29 50   9.8  -2.4 11.6       5.8    -7   1  1    321  No stop 
11 59 30  ---          21 31 21   9.8  -2.3 11.6       5.5    83   F  1    327  11 58 00

11 59 30  M82          21 31 21  10.4  -2.2 11.6       5.5    -7   1  1    327  No stop 
12 01 30  ---          21 33 21  10.4  -2.1 11.6       5.1   113   F  1    335  11 59 30

12 02 00  M81          21 33 51   9.7  -2.0 11.6       4.9    23   1  1    335  12 02 00
12 03 00  ---          21 34 51   9.7  -2.0 11.6       4.7    60   F  1    339  12 02 00

12 03 00  M82          21 34 51  10.3  -1.9 11.6       4.8    -7   1  1    339  No stop 
12 05 00  ---          21 36 52  10.3  -1.8 11.7       4.3   113   F  1    346  12 03 00

12 05 00  M81          21 36 52   9.7  -1.8 11.7       4.3    -7   1  1    346  No stop 
12 06 30  ---          21 38 22   9.7  -1.6 11.7       3.9    83   F  1    352  12 05 00

12 06 30  M82          21 38 22  10.3  -1.6 11.7       4.0    -7   1  1    352  No stop 
12 08 30  ---          21 40 22  10.3  -1.4 11.7       3.6   113   F  1    360  12 06 30

12 08 30  M81          21 40 22   9.7  -1.5 11.7       3.5    -7   1  1    360  No stop 
12 10 00  ---          21 41 52   9.7  -1.3 11.8       3.2    83   F  1    366  12 08 30

12 10 00  M82          21 41 52  10.3  -1.3 11.8       3.2    -7   1  1    366  No stop 
12 12 00  ---          21 43 53  10.3  -1.1 11.8       2.8   113   F  1    374  12 10 00

12 12 30  M81          21 44 23   9.7  -1.1 11.8       2.6    23   1  1    374  12 12 30
12 13 30  ---          21 45 23   9.7  -1.0 11.8       2.4    60   F  1    377  12 12 30

12 13 30  M82          21 45 23  10.3  -1.0 11.8       2.5    -7   1  1    377  No stop 
12 15 30  ---          21 47 23  10.3  -0.8 11.8       2.0   113   F  1    385  12 13 30
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

12 15 30  M81          21 47 23   9.7  -0.8 11.8       2.0    -7   1  1    385  No stop 
12 17 00  ---          21 48 54   9.7  -0.7 11.9       1.6    83   F  1    391  12 15 30

12 17 00  M82          21 48 54  10.3  -0.7 11.9       1.7    -7   1  1    391  No stop 
12 19 00  ---          21 50 54  10.3  -0.5 11.9       1.3   113   F  1    399  12 17 00

12 19 30  M81          21 51 24   9.7  -0.5 11.9       1.1    23   1  1    399  12 19 30
12 20 30  ---          21 52 24   9.7  -0.4 11.9       0.9    60   F  1    403  12 19 30

12 20 30  M82          21 52 24  10.3  -0.4 11.9       0.9    -7   1  1    403  No stop 
12 22 30  ---          21 54 24  10.3  -0.2 12.0       0.5   113   F  1    410  12 20 30

12 22 30  M81          21 54 24   9.7  -0.2 12.0       0.4    -7   1  1    410  No stop 
12 24 00  ---          21 55 55   9.7   0.0 12.0       0.1    83   F  1    416  12 22 30

12 24 00  M82          21 55 55  10.3  -0.1 12.0       0.2    -7   1  1    416  No stop 
12 26 00  ---          21 57 55  10.3   0.1-12.0      -0.3   113   F  1    424  12 24 00

12 26 00  M81          21 57 55   9.7   0.1-12.0      -0.3    -7   1  1    424  No stop 
12 27 30  ---          21 59 25   9.7   0.3-11.9      -0.7    83   F  1    430  12 26 00

12 27 30  M82          21 59 25  10.3   0.2-12.0      -0.6    -7   1  1    430  No stop 
12 29 30  ---          22 01 26  10.3   0.4-11.9      -1.0   113   F  1    437  12 27 30

12 30 00  M81          22 01 56   9.7   0.5-11.9      -1.2    23   1  1    437  12 30 00
12 31 00  ---          22 02 56   9.7   0.6-11.9      -1.4    60   F  1    441  12 30 00

12 31 30  J1048+7143   22 03 26  12.6  -3.7 11.2      10.1    18   1  1    441  12 31 30
12 34 30  =1044+719    22 06 26  12.6  -3.4 11.3       9.4   180   F  1    453  12 31 30

12 34 30  M81          22 06 26   9.7   0.9-11.8      -2.2   -12   1  1    453  No stop 
12 36 30  ---          22 08 27   9.7   1.1-11.8      -2.6   108   F  1    461  12 34 30

12 36 30  M82          22 08 27  10.3   1.0-11.8      -2.6    -7   1  1    461  No stop 
12 38 30  ---          22 10 27  10.3   1.2-11.8      -3.0   113   F  1    468  12 36 30

12 38 30  M81          22 10 27   9.7   1.3-11.8      -3.1    -7   1  1    468  No stop 
12 40 00  ---          22 11 57   9.7   1.4-11.7      -3.4    83   F  1    474  12 38 30

12 40 00  M82          22 11 57  10.3   1.3-11.7      -3.3    -7   1  1    474  No stop 
12 42 00  ---          22 13 58  10.3   1.5-11.7      -3.8   113   F  1    482  12 40 00

12 42 30  M81          22 14 28   9.7   1.6-11.7      -3.9    23   1  1    482  12 42 30
12 43 30  ---          22 15 28   9.7   1.7-11.7      -4.2    60   F  1    486  12 42 30
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

12 43 30  M82          22 15 28  10.3   1.7-11.7      -4.1    -7   1  1    486  No stop 
12 45 30  ---          22 17 28  10.3   1.8-11.7      -4.5   113   F  1    494  12 43 30

12 45 30  M81          22 17 28   9.7   1.9-11.6      -4.6    -7   1  1    494  No stop 
12 47 00  ---          22 18 58   9.7   2.0-11.6      -4.9    83   F  1    499  12 45 30

12 47 00  M82          22 18 58  10.4   2.0-11.6      -4.9    -7   1  1    499  No stop 
12 49 00  ---          22 20 59  10.4   2.1-11.6      -5.3   113   F  1    507  12 47 00

12 49 00  M81          22 20 59   9.8   2.2-11.6      -5.4    -7   1  1    507  No stop 
12 50 30  ---          22 22 29   9.8   2.4-11.6      -5.7    83   F  1    513  12 49 00

12 50 30  M82          22 22 29  10.4   2.3-11.6      -5.6    -7   1  1    513  No stop 
12 52 30  ---          22 24 29  10.4   2.5-11.5      -6.1   113   F  1    521  12 50 30

12 53 00  M81          22 24 59   9.8   2.6-11.5      -6.2    23   1  1    521  12 53 00
12 54 00  ---          22 26 00   9.8   2.7-11.5      -6.5    60   F  1    524  12 53 00

12 54 00  M82          22 26 00  10.4   2.6-11.5      -6.4    -7   1  1    524  No stop 
12 56 00  ---          22 28 00  10.4   2.8-11.5      -6.8   113   F  1    532  12 54 00

12 56 00  M81          22 28 00   9.8   2.9-11.5      -6.9    -7   1  1    532  No stop 
12 57 30  ---          22 29 30   9.8   3.0-11.4      -7.2    83   F  1    538  12 56 00

12 57 30  M82          22 29 30  10.4   2.9-11.5      -7.2    -7   1  1    538  No stop 
12 59 30  ---          22 31 31  10.5   3.1-11.4      -7.6   113   F  1    546  12 57 30

13 00 00  M81          22 32 01   9.9   3.2-11.4      -7.8    23   1  1    546  13 00 00
13 01 00  ---          22 33 01   9.9   3.3-11.4      -8.0    60   F  1    550  13 00 00

13 01 00  M82          22 33 01  10.5   3.2-11.4      -7.9    -7   1  1    550  No stop 
13 03 00  ---          22 35 01  10.5   3.4-11.4      -8.4   113   F  1    557  13 01 00

13 03 00  M81          22 35 01   9.9   3.5-11.4      -8.4    -7   1  1    557  No stop 
13 04 30  ---          22 36 31   9.9   3.6-11.3      -8.7    83   F  1    563  13 03 00

13 04 30  M82          22 36 31  10.5   3.5-11.3      -8.7    -7   1  1    563  No stop 
13 06 30  ---          22 38 32  10.6   3.7-11.3      -9.1   113   F  1    571  13 04 30

13 06 30  M81          22 38 32  10.0   3.8-11.3      -9.2    -7   1  1    571  No stop 
13 08 00  ---          22 40 02  10.0   3.9-11.3      -9.5    83   F  1    577  13 06 30

13 08 00  M82          22 40 02  10.6   3.8-11.3      -9.5    -7   1  1    577  No stop 
13 10 00  ---          22 42 02  10.6   4.0-11.2      -9.9   113   F  1    584  13 08 00
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

13 10 30  M81          22 42 32  10.0   4.2-11.2     -10.1    23   1  1    584  13 10 30
13 11 30  ---          22 43 32  10.0   4.3-11.2     -10.3    60   F  1    588  13 10 30

13 11 30  M82          22 43 32  10.6   4.1-11.2     -10.2    -7   1  1    588  No stop 
13 13 30  ---          22 45 33  10.7   4.3-11.2     -10.7   113   F  1    596  13 11 30

13 13 30  M81          22 45 33  10.1   4.4-11.2     -10.7    -7   1  1    596  No stop 
13 15 00  ---          22 47 03  10.1   4.6-11.2     -11.0    83   F  1    602  13 13 30

13 15 00  M82          22 47 03  10.7   4.4-11.2     -11.0    -7   1  1    602  No stop 
13 17 00  ---          22 49 03  10.7   4.6-11.1     -11.4   113   F  1    610  13 15 00

13 17 30  M81          22 49 33  10.1   4.8-11.1     -11.6    23   1  1    610  13 17 30
13 18 30  ---          22 50 34  10.2   4.9-11.1     -11.8    60   F  1    614  13 17 30

13 18 30  M82          22 50 34  10.7   4.7-11.1     -11.8    -7   1  1    614  No stop 
13 20 30  ---          22 52 34  10.8   4.9-11.1     -12.2   113   F  1    621  13 18 30

13 20 30  M81          22 52 34  10.2   5.1-11.1     -12.2    -7   1  1    621  No stop 
13 22 00  ---          22 54 04  10.2   5.2-11.0     -12.6    83   F  1    627  13 20 30

13 22 00  M82          22 54 04  10.8   5.0-11.0     -12.5    -7   1  1    627  No stop 
13 24 00  ---          22 56 05  10.9   5.2-11.0     -13.0   113   F  1    635  13 22 00

13 24 00  M81          22 56 05  10.3   5.4-11.0     -13.0    -7   1  1    635  No stop 
13 25 30  ---          22 57 35  10.3   5.5-11.0     -13.3    83   F  1    641  13 24 00

13 25 30  M82          22 57 35  10.9   5.3-11.0     -13.3    -7   1  1    641  No stop 
13 27 30  ---          22 59 35  10.9   5.5-11.0     -13.7   113   F  1    648  13 25 30

13 28 00  M81          23 00 05  10.3   5.7-10.9     -13.9    23   1  1    648  13 28 00
13 29 00  ---          23 01 05  10.4   5.8-10.9     -14.1    60   F  1    652  13 28 00

13 29 30  J1048+7143   23 01 35  12.3   1.0-11.8      -2.7    20   1  1    652  13 29 30
13 32 30  =1044+719    23 04 36  12.3   1.2-11.7      -3.4   180   F  1    664  13 29 30

13 32 30  M81          23 04 36  10.4   6.1-10.9     -14.9   -10   1  1    664  No stop 
13 34 30  ---          23 06 36  10.5   6.3-10.8     -15.3   110   F  1    672  13 32 30

13 34 30  M82          23 06 36  11.1   6.1-10.8     -15.3    -7   1  1    672  No stop 
13 36 30  ---          23 08 37  11.1   6.3-10.8     -15.7   113   F  1    679  13 34 30

13 36 30  M81          23 08 37  10.5   6.5-10.8     -15.7    -7   1  1    679  No stop 
13 38 00  ---          23 10 07  10.6   6.6-10.8     -16.1    83   F  1    685  13 36 30
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

13 38 00  M82          23 10 07  11.2   6.4-10.8     -16.0    -7   1  1    685  No stop 
13 40 00  ---          23 12 07  11.2   6.6-10.7     -16.5   113   F  1    693  13 38 00

13 40 30  M81          23 12 37  10.6   6.8-10.7     -16.6    23   1  1    693  13 40 30
13 41 30  ---          23 13 37  10.7   6.9-10.7     -16.8    60   F  1    697  13 40 30

13 41 30  M82          23 13 37  11.2   6.7-10.7     -16.8    -7   1  1    697  No stop 
13 43 30  ---          23 15 38  11.3   6.9-10.7     -17.2   113   F  1    704  13 41 30

13 43 30  M81          23 15 38  10.7   7.1-10.7     -17.3    -7   1  1    704  No stop 
13 45 00  ---          23 17 08  10.8   7.2-10.7     -17.6    83   F  1    710  13 43 30

13 45 00  M82          23 17 08  11.3   7.0-10.7     -17.6    -7   1  1    710  No stop 
13 47 00  ---          23 19 08  11.4   7.2-10.6     -18.0   113   F  1    718  13 45 00

13 47 00  M81          23 19 08  10.8   7.4-10.6     -18.0    -7   1  1    718  No stop 
13 48 30  ---          23 20 39  10.9   7.5-10.6     -18.3    83   F  1    724  13 47 00

13 48 30  M82          23 20 39  11.4   7.3-10.6     -18.3    -7   1  1    724  No stop 
13 50 30  ---          23 22 39  11.5   7.5-10.6     -18.8   113   F  1    732  13 48 30

13 51 00  M81          23 23 09  10.9   7.7-10.6     -18.9    23   1  1    732  13 51 00
13 52 00  ---          23 24 09  11.0   7.8-10.5     -19.1    60   F  1    735  13 51 00

13 52 00  M82          23 24 09  11.5   7.6-10.5     -19.1    -7   1  1    735  No stop 
13 54 00  ---          23 26 09  11.6   7.8-10.5     -19.5   113   F  1    743  13 52 00

13 54 00  M81          23 26 09  11.0   8.0-10.5     -19.5    -7   1  1    743  No stop 
13 55 30  ---          23 27 40  11.1   8.1-10.5     -19.9    83   F  1    749  13 54 00

13 55 30  M82          23 27 40  11.6   7.9-10.5     -19.8    -7   1  1    749  No stop 
13 57 30  ---          23 29 40  11.7   8.1-10.5     -20.3   113   F  1    757  13 55 30

13 58 00  M81          23 30 10  11.1   8.3-10.4     -20.4    23   1  1    757  13 58 00
13 59 00  ---          23 31 10  11.2   8.4-10.4     -20.6    60   F  1    761  13 58 00

13 59 00  M82          23 31 10  11.7   8.2-10.4     -20.6    -7   1  1    761  No stop 
14 01 00  ---          23 33 11  11.8   8.4-10.4     -21.0   113   F  1    768  13 59 00

14 01 00  M81          23 33 11  11.2   8.6-10.4     -21.1    -7   1  1    768  No stop 
14 02 30  ---          23 34 41  11.3   8.7-10.4     -21.4    83   F  1    774  14 01 00

14 02 30  M82          23 34 41  11.8   8.5-10.4     -21.4    -7   1  1    774  No stop 
14 04 30  ---          23 36 41  11.9   8.6-10.3     -21.8   113   F  1    782  14 02 30
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

14 04 30  M81          23 36 41  11.3   8.9-10.3     -21.8    -7   1  1    782  No stop 
14 06 00  ---          23 38 11  11.4   9.0-10.3     -22.2    83   F  1    788  14 04 30

14 06 00  M82          23 38 11  12.0   8.8-10.3     -22.1    -7   1  1    788  No stop 
14 08 00  ---          23 40 12  12.0   8.9-10.3     -22.6   113   F  1    795  14 06 00

14 08 30  M81          23 40 42  11.5   9.2-10.3     -22.7    23   1  1    795  14 08 30
14 09 30  ---          23 41 42  11.5   9.3-10.2     -22.9    60   F  1    799  14 08 30

14 09 30  M82          23 41 42  12.1   9.1-10.3     -22.9    -7   1  1    799  No stop 
14 11 30  ---          23 43 42  12.1   9.2-10.2     -23.3   113   F  1    807  14 09 30

14 11 30  M81          23 43 42  11.6   9.5-10.2     -23.3    -7   1  1    807  No stop 
14 13 00  ---          23 45 13  11.6   9.6-10.2     -23.7    83   F  1    813  14 11 30

14 13 00  M82          23 45 13  12.2   9.3-10.2     -23.7    -7   1  1    813  No stop 
14 15 00  ---          23 47 13  12.3   9.5-10.2     -24.1   113   F  1    821  14 13 00

14 15 30  M81          23 47 43  11.7   9.8-10.1     -24.2    23   1  1    821  14 15 30
14 16 30  ---          23 48 43  11.8   9.9-10.1     -24.4    60   F  1    824  14 15 30

14 16 30  M82          23 48 43  12.3   9.6-10.1     -24.4    -7   1  1    824  No stop 
14 18 30  ---          23 50 43  12.4   9.8-10.1     -24.9   113   F  1    832  14 16 30

14 18 30  M81          23 50 43  11.8  10.1-10.1     -24.9    -7   1  1    832  No stop 
14 20 00  ---          23 52 14  11.9  10.2-10.1     -25.2    83   F  1    838  14 18 30

14 20 00  M82          23 52 14  12.4   9.9-10.1     -25.2    -7   1  1    838  No stop 
14 22 00  ---          23 54 14  12.5  10.1-10.0     -25.6   113   F  1    846  14 20 00

14 22 00  M81          23 54 14  12.0  10.4-10.0     -25.6    -7   1  1    846  No stop 
14 23 30  ---          23 55 44  12.0  10.5-10.0     -26.0    83   F  1    852  14 22 00

14 23 30  M82          23 55 44  12.6  10.2-10.0     -25.9    -7   1  1    852  No stop 
14 25 30  ---          23 57 45  12.7  10.4-10.0     -26.4   113   F  1    859  14 23 30

14 26 00  M81          23 58 15  12.1  10.7-10.0     -26.5    23   1  1    859  14 26 00
14 27 00  ---          23 59 15  12.2  10.8-10.0     -26.7    60   F  1    863  14 26 00

14 27 30  J1048+7143   23 59 45  13.1   5.6-10.8     -15.5    21   1  1    863  14 27 30
14 30 30  =1044+719    00 02 45  13.1   5.8-10.8     -16.2   180   F  1    875  14 27 30

14 30 30  M81          00 02 45  12.3  11.1 -9.9     -27.5    -9   1  1    875  No stop 
14 32 30  ---          00 04 46  12.4  11.2 -9.9     -27.9   111   F  1    883  14 30 30
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

14 32 30  M82          00 04 46  12.9  10.9 -9.9     -27.9    -7   1  1    883  No stop 
14 34 30  ---          00 06 46  13.0  11.1 -9.8     -28.3   113   F  1    890  14 32 30

14 34 30  M81          00 06 46  12.5  11.4 -9.8     -28.3    -7   1  1    890  No stop 
14 36 00  ---          00 08 16  12.6  11.5 -9.8     -28.7    83   F  1    896  14 34 30

14 36 00  M82          00 08 16  13.1  11.2 -9.8     -28.7    -7   1  1    896  No stop 
14 38 00  ---          00 10 17  13.2  11.3 -9.8     -29.1   113   F  1    904  14 36 00

14 38 30  M81          00 10 47  12.7  11.7 -9.8     -29.2    23   1  1    904  14 38 30
14 39 30  ---          00 11 47  12.7  11.8 -9.7     -29.4    60   F  1    908  14 38 30

14 39 30  M82          00 11 47  13.2  11.5 -9.7     -29.4    -7   1  1    908  No stop 
14 41 30  ---          00 13 47  13.3  11.6 -9.7     -29.9   113   F  1    915  14 39 30

14 41 30  M81          00 13 47  12.8  12.0 -9.7     -29.9    -7   1  1    915  No stop 
14 43 00  ---          00 15 18  12.9  12.1 -9.7     -30.2    83   F  1    921  14 41 30

14 43 00  M82          00 15 18  13.4  11.7 -9.7     -30.2    -7   1  1    921  No stop 
14 45 00  ---          00 17 18  13.5  11.9 -9.7     -30.6   113   F  1    929  14 43 00

14 45 00  M81          00 17 18  12.9  12.2 -9.7     -30.6    -7   1  1    929  No stop 
14 46 30  ---          00 18 48  13.0  12.4 -9.6     -30.9    83   F  1    935  14 45 00

14 46 30  M82          00 18 48  13.5  12.0 -9.6     -30.9    -7   1  1    935  No stop 
14 48 30  ---          00 20 48  13.6  12.2 -9.6     -31.4   113   F  1    943  14 46 30

14 49 00  M81          00 21 19  13.1  12.5 -9.6     -31.5    23   1  1    943  14 49 00
14 50 00  ---          00 22 19  13.2  12.6 -9.6     -31.7    60   F  1    946  14 49 00

14 50 00  M82          00 22 19  13.7  12.3 -9.6     -31.7    -7   1  1    946  No stop 
14 52 00  ---          00 24 19  13.8  12.4 -9.5     -32.1   113   F  1    954  14 50 00

14 52 00  M81          00 24 19  13.3  12.8 -9.5     -32.1    -7   1  1    954  No stop 
14 53 30  ---          00 25 49  13.3  12.9 -9.5     -32.4    83   F  1    960  14 52 00

14 53 30  M82          00 25 49  13.9  12.5 -9.5     -32.5    -7   1  1    960  No stop 
14 55 30  ---          00 27 50  13.9  12.7 -9.5     -32.9   113   F  1    968  14 53 30

14 56 00  M81          00 28 20  13.5  13.1 -9.5     -33.0    23   1  1    968  14 56 00
14 57 00  ---          00 29 20  13.5  13.2 -9.5     -33.2    60   F  1    972  14 56 00

14 57 00  M82          00 29 20  14.0  12.8 -9.5     -33.2    -7   1  1    972  No stop 
14 59 00  ---          00 31 20  14.1  13.0 -9.4     -33.7   113   F  1    979  14 57 00
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

14 59 00  M81          00 31 20  13.6  13.3 -9.4     -33.6    -7   1  1    979  No stop 
15 00 30  ---          00 32 50  13.7  13.4 -9.4     -34.0    83   F  1    985  14 59 00

15 00 30  M82          00 32 50  14.2  13.1 -9.4     -34.0    -7   1  1    985  No stop 
15 02 30  ---          00 34 51  14.3  13.2 -9.4     -34.4   113   F  1    993  15 00 30

15 02 30  M81          00 34 51  13.8  13.6 -9.4     -34.4    -7   1  1    993  No stop 
15 04 00  ---          00 36 21  13.9  13.7 -9.3     -34.7    83   F  1    999  15 02 30

15 04 00  M82          00 36 21  14.4  13.3 -9.3     -34.7    -7   1  1    999  No stop 
15 06 00  ---          00 38 21  14.5  13.5 -9.3     -35.2   113   F  1   1006  15 04 00

15 06 30  M81          00 38 51  14.0  13.9 -9.3     -35.3    23   1  1   1006  15 06 30
15 07 30  ---          00 39 52  14.1  14.0 -9.3     -35.5    60   F  1   1010  15 06 30

15 07 30  M82          00 39 52  14.5  13.6 -9.3     -35.5    -7   1  1   1010  No stop 
15 09 30  ---          00 41 52  14.6  13.7 -9.2     -35.9   113   F  1   1018  15 07 30

15 09 30  M81          00 41 52  14.2  14.1 -9.2     -35.9    -7   1  1   1018  No stop 
15 11 00  ---          00 43 22  14.2  14.2 -9.2     -36.2    83   F  1   1024  15 09 30

15 11 00  M82          00 43 22  14.7  13.8 -9.2     -36.3    -7   1  1   1024  No stop 
15 13 00  ---          00 45 22  14.8  14.0 -9.2     -36.7   113   F  1   1032  15 11 00

15 13 30  M81          00 45 53  14.4  14.4 -9.2     -36.8    23   1  1   1032  15 13 30
15 14 30  ---          00 46 53  14.4  14.5 -9.2     -37.0    60   F  1   1035  15 13 30

15 14 30  M82          00 46 53  14.9  14.1 -9.2     -37.0    -7   1  1   1035  No stop 
15 16 30  ---          00 48 53  15.0  14.2 -9.1     -37.4   113   F  1   1043  15 14 30

15 16 30  M81          00 48 53  14.5  14.6 -9.1     -37.4    -7   1  1   1043  No stop 
15 18 00  ---          00 50 23  14.6  14.8 -9.1     -37.7    83   F  1   1049  15 16 30

15 18 00  M82          00 50 23  15.1  14.3 -9.1     -37.8    -7   1  1   1049  No stop 
15 20 00  ---          00 52 24  15.2  14.5 -9.1     -38.2   113   F  1   1057  15 18 00

15 20 00  M81          00 52 24  14.7  14.9 -9.1     -38.2    -7   1  1   1057  No stop 
15 21 30  ---          00 53 54  14.8  15.0 -9.0     -38.5    83   F  1   1063  15 20 00

15 21 30  M82          00 53 54  15.3  14.6 -9.0     -38.5    -7   1  1   1063  No stop 
15 23 30  ---          00 55 54  15.4  14.7 -9.0     -39.0   113   F  1   1070  15 21 30

15 24 00  M81          00 56 24  14.9  15.2 -9.0     -39.0    23   1  1   1070  15 24 00
15 25 00  ---          00 57 24  15.0  15.3 -9.0     -39.2    60   F  1   1074  15 24 00
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

15 25 30  J1048+7143   00 57 55  14.8  10.0 -9.9     -28.3    20   1  1   1074  15 25 30
15 28 30  =1044+719    01 00 55  14.9  10.2 -9.8     -28.9   180   F  1   1086  15 25 30

15 28 30  M81          01 00 55  15.2  15.5 -8.9     -40.0   -10   1  1   1086  No stop 
15 30 30  ---          01 02 55  15.3  15.7 -8.9     -40.4   110   F  1   1093  15 28 30

15 30 30  M82          01 02 55  15.8  15.2 -8.9     -40.5    -7   1  1   1093  No stop 
15 32 30  ---          01 04 56  15.9  15.4 -8.9     -40.9   113   F  1   1101  15 30 30

15 32 30  M81          01 04 56  15.4  15.8 -8.9     -40.9    -7   1  1   1101  No stop 
15 34 00  ---          01 06 26  15.5  15.9 -8.8     -41.2    83   F  1   1107  15 32 30

15 34 00  M82          01 06 26  16.0  15.5 -8.8     -41.2    -7   1  1   1107  No stop 
15 36 00  ---          01 08 26  16.1  15.6 -8.8     -41.7   113   F  1   1115  15 34 00

15 36 30  M81          01 08 56  15.7  16.1 -8.8     -41.7    23   1  1   1115  15 36 30
15 37 30  ---          01 09 56  15.7  16.1 -8.8     -41.9    60   F  1   1119  15 36 30

15 37 30  M82          01 09 56  16.2  15.7 -8.8     -42.0    -7   1  1   1119  No stop 
15 39 30  ---          01 11 57  16.3  15.8 -8.7     -42.4   113   F  1   1126  15 37 30

15 39 30  M81          01 11 57  15.9  16.3 -8.7     -42.4    -7   1  1   1126  No stop 
15 41 00  ---          01 13 27  15.9  16.4 -8.7     -42.7    83   F  1   1132  15 39 30

15 41 00  M82          01 13 27  16.4  15.9 -8.7     -42.7    -7   1  1   1132  No stop 
15 43 00  ---          01 15 27  16.5  16.1 -8.7     -43.2   113   F  1   1140  15 41 00

15 43 00  M81          01 15 27  16.1  16.5 -8.7     -43.1    -7   1  1   1140  No stop 
15 44 30  ---          01 16 58  16.2  16.6 -8.7     -43.4    83   F  1   1146  15 43 00

15 44 30  M82          01 16 58  16.6  16.2 -8.7     -43.5    -7   1  1   1146  No stop 
15 46 30  ---          01 18 58  16.7  16.3 -8.6     -43.9   113   F  1   1153  15 44 30

15 47 00  M81          01 19 28  16.3  16.8 -8.6     -44.0    23   1  1   1153  15 47 00
15 48 00  ---          01 20 28  16.4  16.9 -8.6     -44.2    60   F  1   1157  15 47 00

15 48 00  M82          01 20 28  16.8  16.4 -8.6     -44.3    -7   1  1   1157  No stop 
15 50 00  ---          01 22 29  16.9  16.5 -8.6     -44.7   113   F  1   1165  15 48 00

15 50 00  M81          01 22 29  16.5  17.0 -8.6     -44.6    -7   1  1   1165  No stop 
15 51 30  ---          01 23 59  16.6  17.1 -8.5     -44.9    83   F  1   1171  15 50 00

15 51 30  M82          01 23 59  17.0  16.6 -8.5     -45.0    -7   1  1   1171  No stop 
15 53 30  ---          01 25 59  17.1  16.8 -8.5     -45.4   113   F  1   1179  15 51 30
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

15 54 00  M81          01 26 29  16.8  17.3 -8.5     -45.5    24   1  1   1179  15 54 00
15 55 00  ---          01 27 29  16.8  17.3 -8.5     -45.7    60   F  1   1183  15 54 00

15 55 00  M82          01 27 29  17.2  16.8 -8.5     -45.8    -7   1  1   1183  No stop 
15 57 00  ---          01 29 30  17.4  17.0 -8.5     -46.2   113   F  1   1190  15 55 00

15 57 00  M81          01 29 30  16.9  17.5 -8.4     -46.1    -7   1  1   1190  No stop 
15 58 30  ---          01 31 00  17.0  17.6 -8.4     -46.5    83   F  1   1196  15 57 00

15 58 30  M82          01 31 00  17.4  17.1 -8.4     -46.5    -7   1  1   1196  No stop 
16 00 30  ---          01 33 00  17.6  17.2 -8.4     -47.0   113   F  1   1204  15 58 30

16 00 30  M81          01 33 00  17.2  17.7 -8.4     -46.9    -7   1  1   1204  No stop 
16 02 00  ---          01 34 31  17.3  17.8 -8.4     -47.2    83   F  1   1210  16 00 30

16 02 00  M82          01 34 31  17.7  17.3 -8.4     -47.3    -7   1  1   1210  No stop 
16 04 00  ---          01 36 31  17.8  17.4 -8.3     -47.7   113   F  1   1217  16 02 00

16 04 30  M81          01 37 01  17.4  17.9 -8.3     -47.7    24   1  1   1217  16 04 30
16 05 30  ---          01 38 01  17.5  18.0 -8.3     -48.0    60   F  1   1221  16 04 30

16 05 30  M82          01 38 01  17.9  17.5 -8.3     -48.0    -6   1  1   1221  No stop 
16 07 30  ---          01 40 01  18.0  17.6 -8.3     -48.5   114   F  1   1229  16 05 30

16 07 30  M81          01 40 01  17.6  18.1 -8.3     -48.4    -6   1  1   1229  No stop 
16 09 00  ---          01 41 32  17.7  18.2 -8.2     -48.7    84   F  1   1235  16 07 30

16 09 00  M82          01 41 32  18.1  17.7 -8.3     -48.8    -6   1  1   1235  No stop 
16 11 00  ---          01 43 32  18.3  17.8 -8.2     -49.2   114   F  1   1243  16 09 00

16 11 30  M81          01 44 02  17.9  18.4 -8.2     -49.2    24   1  1   1243  16 11 30
16 12 30  ---          01 45 02  18.0  18.4 -8.2     -49.5    60   F  1   1246  16 11 30

16 12 30  M82          01 45 02  18.4  17.9 -8.2     -49.5    -6   1  1   1246  No stop 
16 14 30  ---          01 47 03  18.5  18.0 -8.2     -50.0   114   F  1   1254  16 12 30

16 14 30  M81          01 47 03  18.1  18.6 -8.2     -49.9    -6   1  1   1254  No stop 
16 16 00  ---          01 48 33  18.2  18.7 -8.1     -50.2    84   F  1   1260  16 14 30

16 16 00  M82          01 48 33  18.6  18.1 -8.1     -50.3    -6   1  1   1260  No stop 
16 18 00  ---          01 50 33  18.7  18.3 -8.1     -50.7   114   F  1   1268  16 16 00

16 18 00  M81          01 50 33  18.4  18.8 -8.1     -50.6    -6   1  1   1268  No stop 
16 19 30  ---          01 52 03  18.5  18.9 -8.1     -51.0    84   F  1   1273  16 18 00
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

16 19 30  M82          01 52 03  18.8  18.3 -8.1     -51.1    -6   1  1   1273  No stop 
16 21 30  ---          01 54 04  19.0  18.5 -8.0     -51.5   114   F  1   1281  16 19 30

16 22 00  M81          01 54 34  18.6  19.0 -8.0     -51.5    24   1  1   1281  16 22 00
16 23 00  ---          01 55 34  18.7  19.1 -8.0     -51.7    60   F  1   1285  16 22 00

16 23 30  J1048+7143   01 56 04  17.4  13.9 -8.9     -41.0    21   1  1   1285  16 23 30
16 26 30  =1044+719    01 59 05  17.5  14.1 -8.8     -41.7   180   F  1   1297  16 23 30

16 26 30  M81          01 59 05  19.0  19.3 -8.0     -52.5    -9   1  1   1297  No stop 
16 28 30  ---          02 01 05  19.1  19.4 -7.9     -52.9   111   F  1   1304  16 26 30

16 28 30  M82          02 01 05  19.4  18.8 -7.9     -53.0    -6   1  1   1304  No stop 
16 30 30  ---          02 03 05  19.6  19.0 -7.9     -53.4   114   F  1   1312  16 28 30

16 30 30  M81          02 03 05  19.2  19.5 -7.9     -53.3    -6   1  1   1312  No stop 
16 32 00  ---          02 04 35  19.4  19.6 -7.9     -53.7    84   F  1   1318  16 30 30

16 32 00  M82          02 04 35  19.7  19.0 -7.9     -53.8    -6   1  1   1318  No stop 
16 34 00  ---          02 06 36  19.8  19.2 -7.8     -54.2   114   F  1   1326  16 32 00

16 34 30  M81          02 07 06  19.5  19.7 -7.8     -54.2    24   1  1   1326  16 34 30
16 35 30  ---          02 08 06  19.6  19.8 -7.8     -54.4    60   F  1   1330  16 34 30

16 35 30  M82          02 08 06  19.9  19.2 -7.8     -54.5    -6   1  1   1330  No stop 
16 37 30  ---          02 10 06  20.1  19.3 -7.8     -55.0   114   F  1   1337  16 35 30

16 37 30  M81          02 10 06  19.8  19.9 -7.8     -54.8    -6   1  1   1337  No stop 
16 39 00  ---          02 11 37  19.9  20.0 -7.7     -55.2    84   F  1   1343  16 37 30

16 39 00  M82          02 11 37  20.2  19.4 -7.8     -55.3    -6   1  1   1343  No stop 
16 41 00  ---          02 13 37  20.3  19.5 -7.7     -55.7   114   F  1   1351  16 39 00

16 41 00  M81          02 13 37  20.0  20.1 -7.7     -55.6    -6   1  1   1351  No stop 
16 42 30  ---          02 15 07  20.1  20.2 -7.7     -55.9    84   F  1   1357  16 41 00

16 42 30  M82          02 15 07  20.4  19.6 -7.7     -56.0    -6   1  1   1357  No stop 
16 44 30  ---          02 17 07  20.6  19.7 -7.7     -56.5   114   F  1   1364  16 42 30

16 45 00  M81          02 17 38  20.3  20.3 -7.6     -56.5    24   1  1   1364  16 45 00
16 46 00  ---          02 18 38  20.4  20.3 -7.6     -56.7    60   F  1   1368  16 45 00

16 46 00  M82          02 18 38  20.7  19.8 -7.6     -56.8    -6   1  1   1368  No stop 
16 48 00  ---          02 20 38  20.8  19.9 -7.6     -57.2   114   F  1   1376  16 46 00
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

16 48 00  M81          02 20 38  20.5  20.5 -7.6     -57.1    -6   1  1   1376  No stop 
16 49 30  ---          02 22 08  20.6  20.5 -7.6     -57.4    84   F  1   1382  16 48 00

16 49 30  M82          02 22 08  21.0  20.0 -7.6     -57.6    -6   1  1   1382  No stop 
16 51 30  ---          02 24 09  21.1  20.1 -7.5     -58.0   114   F  1   1390  16 49 30

16 52 00  M81          02 24 39  20.8  20.7 -7.5     -58.0    24   1  1   1390  16 52 00
16 53 00  ---          02 25 39  20.9  20.7 -7.5     -58.2    60   F  1   1393  16 52 00

16 53 00  M82          02 25 39  21.2  20.1 -7.5     -58.3    -6   1  1   1393  No stop 
16 55 00  ---          02 27 39  21.4  20.2 -7.5     -58.8   114   F  1   1401  16 53 00

16 55 00  M81          02 27 39  21.1  20.8 -7.5     -58.6    -6   1  1   1401  No stop 
16 56 30  ---          02 29 09  21.2  20.9 -7.5     -58.9    84   F  1   1407  16 55 00

16 56 30  M82          02 29 09  21.5  20.3 -7.5     -59.1    -6   1  1   1407  No stop 
16 58 30  ---          02 31 10  21.6  20.4 -7.4     -59.5   114   F  1   1415  16 56 30

16 58 30  M81          02 31 10  21.3  21.0 -7.4     -59.4    -6   1  1   1415  No stop 
17 00 00  ---          02 32 40  21.5  21.1 -7.4     -59.7    84   F  1   1421  16 58 30

17 00 00  M82          02 32 40  21.7  20.5 -7.4     -59.8    -6   1  1   1421  No stop 
17 02 00  ---          02 34 40  21.9  20.6 -7.4     -60.3   114   F  1   1428  17 00 00

17 02 30  M81          02 35 10  21.6  21.2 -7.4     -60.2    24   1  1   1428  17 02 30
17 03 30  ---          02 36 11  21.7  21.2 -7.3     -60.5    60   F  1   1432  17 02 30

17 03 30  M82          02 36 11  22.0  20.6 -7.3     -60.6    -6   1  1   1432  No stop 
17 05 30  ---          02 38 11  22.2  20.7 -7.3     -61.0   114   F  1   1440  17 03 30

17 05 30  M81          02 38 11  21.9  21.3 -7.3     -60.9    -6   1  1   1440  No stop 
17 07 00  ---          02 39 41  22.0  21.4 -7.3     -61.2    84   F  1   1446  17 05 30

17 07 00  M82          02 39 41  22.3  20.8 -7.3     -61.4    -6   1  1   1446  No stop 
17 09 00  ---          02 41 42  22.4  20.9 -7.3     -61.8   114   F  1   1453  17 07 00

17 09 30  M81          02 42 12  22.2  21.5 -7.2     -61.8    24   1  1   1453  17 09 30
17 10 30  ---          02 43 12  22.3  21.6 -7.2     -62.0    60   F  1   1457  17 09 30

17 10 30  M82          02 43 12  22.5  21.0 -7.2     -62.1    -6   1  1   1457  No stop 
17 12 30  ---          02 45 12  22.7  21.0 -7.2     -62.6   114   F  1   1465  17 10 30

17 12 30  M81          02 45 12  22.4  21.6 -7.2     -62.4    -6   1  1   1465  No stop 
17 14 00  ---          02 46 42  22.6  21.7 -7.2     -62.7    84   F  1   1471  17 12 30
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

17 14 00  M82          02 46 42  22.8  21.1 -7.2     -62.9    -6   1  1   1471  No stop 
17 16 00  ---          02 48 43  23.0  21.2 -7.1     -63.3   114   F  1   1479  17 14 00

17 16 00  M81          02 48 43  22.7  21.8 -7.1     -63.2    -6   1  1   1479  No stop 
17 17 30  ---          02 50 13  22.8  21.9 -7.1     -63.5    84   F  1   1484  17 16 00

17 17 30  M82          02 50 13  23.1  21.3 -7.1     -63.7    -6   1  1   1484  No stop 
17 19 30  ---          02 52 13  23.2  21.3 -7.1     -64.1   114   F  1   1492  17 17 30

17 20 00  M81          02 52 43  23.0  22.0 -7.1     -64.0    24   1  1   1492  17 20 00
17 21 00  ---          02 53 43  23.1  22.0 -7.0     -64.3    60   F  1   1496  17 20 00

17 21 30  J1048+7143   02 54 14  20.7  17.1 -7.9     -53.7    19   1  1   1496  17 21 30
17 24 30  =1044+719    02 57 14  20.9  17.3 -7.9     -54.4   180   F  1   1508  17 21 30

17 24 30  M81          02 57 14  23.4  22.2 -7.0     -65.0   -11   1  1   1508  No stop 
17 26 30  ---          02 59 14  23.6  22.2 -7.0     -65.5   109   F  1   1515  17 24 30

17 26 30  M82          02 59 14  23.8  21.6 -7.0     -65.6    -6   1  1   1515  No stop 
17 28 30  ---          03 01 15  23.9  21.7 -6.9     -66.1   114   F  1   1523  17 26 30

17 28 30  M81          03 01 15  23.7  22.3 -6.9     -65.9    -6   1  1   1523  No stop 
17 30 00  ---          03 02 45  23.8  22.4 -6.9     -66.2    84   F  1   1529  17 28 30

17 30 00  M82          03 02 45  24.1  21.8 -6.9     -66.4    -6   1  1   1529  No stop 
17 32 00  ---          03 04 45  24.2  21.8 -6.9     -66.8   114   F  1   1537  17 30 00

17 32 30  M81          03 05 15  24.1  22.5 -6.9     -66.8    24   1  1   1537  17 32 30
17 33 30  ---          03 06 16  24.1  22.5 -6.8     -67.0    60   F  1   1541  17 32 30

17 33 30  M82          03 06 16  24.3  21.9 -6.8     -67.2    -6   1  1   1541  No stop 
17 35 30  ---          03 08 16  24.5  22.0 -6.8     -67.6   114   F  1   1548  17 33 30

17 35 30  M81          03 08 16  24.3  22.6 -6.8     -67.4    -6   1  1   1548  No stop 
17 37 00  ---          03 09 46  24.4  22.7 -6.8     -67.7    84   F  1   1554  17 35 30

17 37 00  M82          03 09 46  24.6  22.0 -6.8     -67.9    -6   1  1   1554  No stop 
17 39 00  ---          03 11 46  24.8  22.1 -6.7     -68.4   114   F  1   1562  17 37 00

17 39 00  M81          03 11 46  24.6  22.7 -6.7     -68.2    -6   1  1   1562  No stop 
17 40 30  ---          03 13 17  24.7  22.8 -6.7     -68.5    84   F  1   1568  17 39 00

17 40 30  M82          03 13 17  24.9  22.1 -6.7     -68.7    -6   1  1   1568  No stop 
17 42 30  ---          03 15 17  25.1  22.2 -6.7     -69.1   114   F  1   1575  17 40 30
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

17 43 00  M81          03 15 47  24.9  22.9 -6.7     -69.1    24   1  1   1575  17 43 00
17 44 00  ---          03 16 47  25.0  22.9 -6.7     -69.3    60   F  1   1579  17 43 00

17 44 00  M82          03 16 47  25.2  22.3 -6.7     -69.5    -6   1  1   1579  No stop 
17 46 00  ---          03 18 48  25.4  22.3 -6.6     -69.9   114   F  1   1587  17 44 00

17 46 00  M81          03 18 48  25.2  23.0 -6.6     -69.7    -6   1  1   1587  No stop 
17 47 30  ---          03 20 18  25.3  23.0 -6.6     -70.0    84   F  1   1593  17 46 00

17 47 30  M82          03 20 18  25.5  22.4 -6.6     -70.2    -6   1  1   1593  No stop 
17 49 30  ---          03 22 18  25.7  22.4 -6.6     -70.7   114   F  1   1601  17 47 30

17 50 00  M81          03 22 48  25.5  23.1 -6.6     -70.6    24   1  1   1601  17 50 00
17 51 00  ---          03 23 48  25.6  23.1 -6.5     -70.8    60   F  1   1604  17 50 00

17 51 00  M82          03 23 48  25.8  22.5 -6.5     -71.0    -6   1  1   1604  No stop 
17 53 00  ---          03 25 49  25.9  22.6 -6.5     -71.5   114   F  1   1612  17 51 00

17 53 00  M81          03 25 49  25.8  23.2 -6.5     -71.3    -6   1  1   1612  No stop 
17 54 30  ---          03 27 19  25.9  23.3 -6.5     -71.6    84   F  1   1618  17 53 00

17 54 30  M82          03 27 19  26.1  22.6 -6.5     -71.8    -6   1  1   1618  No stop 
17 56 30  ---          03 29 19  26.2  22.7 -6.5     -72.2   114   F  1   1626  17 54 30

17 56 30  M81          03 29 19  26.1  23.3 -6.5     -72.0    -6   1  1   1626  No stop 
17 58 00  ---          03 30 50  26.2  23.4 -6.4     -72.4    84   F  1   1632  17 56 30

17 58 00  M82          03 30 50  26.4  22.7 -6.4     -72.6    -6   1  1   1632  No stop 
18 00 00  ---          03 32 50  26.5  22.8 -6.4     -73.0   114   F  1   1639  17 58 00

18 00 30  M81          03 33 20  26.4  23.4 -6.4     -72.9    24   1  1   1639  18 00 30
18 01 30  ---          03 34 20  26.5  23.5 -6.4     -73.1    60   F  1   1643  18 00 30

18 01 30  M82          03 34 20  26.6  22.8 -6.4     -73.4    -6   1  1   1643  No stop 
18 03 30  ---          03 36 20  26.8  22.9 -6.3     -73.8   114   F  1   1651  18 01 30

18 03 30  M81          03 36 20  26.7  23.5 -6.3     -73.6    -6   1  1   1651  No stop 
18 05 00  ---          03 37 51  26.8  23.6 -6.3     -73.9    84   F  1   1657  18 03 30

18 05 00  M82          03 37 51  26.9  22.9 -6.3     -74.1    -6   1  1   1657  No stop 
18 07 00  ---          03 39 51  27.1  22.9 -6.3     -74.6   114   F  1   1664  18 05 00

18 07 30  M81          03 40 21  27.0  23.6 -6.3     -74.5    24   1  1   1664  18 07 30
18 08 30  ---          03 41 21  27.1  23.7 -6.3     -74.7    60   F  1   1668  18 07 30
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

18 08 30  M82          03 41 21  27.2  23.0 -6.3     -74.9    -6   1  1   1668  No stop 
18 10 30  ---          03 43 22  27.4  23.0 -6.2     -75.4   114   F  1   1676  18 08 30

18 10 30  M81          03 43 22  27.3  23.7 -6.2     -75.1    -6   1  1   1676  No stop 
18 12 00  ---          03 44 52  27.4  23.8 -6.2     -75.5    84   F  1   1682  18 10 30

18 12 00  M82          03 44 52  27.5  23.1 -6.2     -75.7    -6   1  1   1682  No stop 
18 14 00  ---          03 46 52  27.7  23.1 -6.2     -76.1   114   F  1   1690  18 12 00

18 14 00  M81          03 46 52  27.6  23.8 -6.2     -75.9    -6   1  1   1690  No stop 
18 15 30  ---          03 48 22  27.7  23.8 -6.1     -76.2    84   F  1   1695  18 14 00

18 15 30  M82          03 48 22  27.8  23.2 -6.1     -76.5    -6   1  1   1695  No stop 
18 17 30  ---          03 50 23  28.0  23.2 -6.1     -76.9   114   F  1   1703  18 15 30

18 18 00  M81          03 50 53  27.9  23.9 -6.1     -76.8    24   1  1   1703  18 18 00
18 19 00  ---          03 51 53  28.0  23.9 -6.1     -77.0    60   F  1   1707  18 18 00

18 19 30  J1048+7143   03 52 23  24.7  19.6 -6.9     -66.6    17   1  1   1707  18 19 30
18 22 30  =1044+719    03 55 24  24.9  19.7 -6.9     -67.3   180   F  1   1719  18 19 30

18 22 30  M81          03 55 24  28.3  24.0 -6.0     -77.8   -13   1  1   1719  No stop 
18 24 30  ---          03 57 24  28.5  24.0 -6.0     -78.2   107   F  1   1726  18 22 30

18 24 30  M82          03 57 24  28.6  23.4 -6.0     -78.5    -6   1  1   1726  No stop 
18 26 30  ---          03 59 24  28.8  23.4 -6.0     -79.0   114   F  1   1734  18 24 30

18 26 30  M81          03 59 24  28.7  24.1 -6.0     -78.7    -6   1  1   1734  No stop 
18 28 00  ---          04 00 54  28.8  24.1 -5.9     -79.0    84   F  1   1740  18 26 30

18 28 00  M82          04 00 54  28.9  23.4 -5.9     -79.3    -6   1  1   1740  No stop 
18 30 00  ---          04 02 55  29.1  23.5 -5.9     -79.7   114   F  1   1748  18 28 00

18 30 30  M81          04 03 25  29.0  24.2 -5.9     -79.6    24   1  1   1748  18 30 30
18 31 30  ---          04 04 25  29.1  24.2 -5.9     -79.8    60   F  1   1752  18 30 30

18 31 30  M82          04 04 25  29.2  23.5 -5.9     -80.1    -6   1  1   1752  No stop 
18 33 30  ---          04 06 25  29.4  23.5 -5.8     -80.5   114   F  1   1759  18 31 30

18 33 30  M81          04 06 25  29.3  24.2 -5.8     -80.3    -6   1  1   1759  No stop 
18 35 00  ---          04 07 56  29.4  24.2 -5.8     -80.6    84   F  1   1765  18 33 30

18 35 00  M82          04 07 56  29.5  23.5 -5.8     -80.9    -6   1  1   1765  No stop 
18 37 00  ---          04 09 56  29.7  23.6 -5.8     -81.3   114   F  1   1773  18 35 00
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

18 37 00  M81          04 09 56  29.6  24.3 -5.8     -81.1    -6   1  1   1773  No stop 
18 38 30  ---          04 11 26  29.7  24.3 -5.7     -81.4    84   F  1   1779  18 37 00

18 38 30  M82          04 11 26  29.8  23.6 -5.8     -81.7    -6   1  1   1779  No stop 
18 40 30  ---          04 13 27  30.0  23.6 -5.7     -82.1   114   F  1   1786  18 38 30

18 41 00  M81          04 13 57  30.0  24.3 -5.7     -82.0    24   1  1   1786  18 41 00
18 42 00  ---          04 14 57  30.0  24.3 -5.7     -82.2    60   F  1   1790  18 41 00

18 42 00  M82          04 14 57  30.1  23.6 -5.7     -82.5    -6   1  1   1790  No stop 
18 44 00  ---          04 16 57  30.3  23.7 -5.7     -82.9   114   F  1   1798  18 42 00

18 44 00  M81          04 16 57  30.2  24.4 -5.7     -82.6    -6   1  1   1798  No stop 
18 45 30  ---          04 18 27  30.4  24.4 -5.6     -83.0    84   F  1   1804  18 44 00

18 45 30  M82          04 18 27  30.4  23.7 -5.6     -83.3    -6   1  1   1804  No stop 
18 47 30  ---          04 20 28  30.6  23.7 -5.6     -83.7   114   F  1   1811  18 45 30

18 48 00  M81          04 20 58  30.6  24.4 -5.6     -83.6    24   1  1   1811  18 48 00
18 49 00  ---          04 21 58  30.7  24.4 -5.6     -83.8    60   F  1   1815  18 48 00

18 49 00  M82          04 21 58  30.7  23.7 -5.6     -84.1    -6   1  1   1815  No stop 
18 51 00  ---          04 23 58  30.9  23.7 -5.5     -84.5   114   F  1   1823  18 49 00

18 51 00  M81          04 23 58  30.8  24.5 -5.5     -84.2    -6   1  1   1823  No stop 
18 52 30  ---          04 25 29  31.0  24.5 -5.5     -84.6    84   F  1   1829  18 51 00

18 52 30  M82          04 25 29  31.0  23.8 -5.5     -84.9    -6   1  1   1829  No stop 
18 54 30  ---          04 27 29  31.2  23.8 -5.5     -85.3   114   F  1   1837  18 52 30

18 54 30  M81          04 27 29  31.2  24.5 -5.5     -85.0    -6   1  1   1837  No stop 
18 56 00  ---          04 28 59  31.3  24.5 -5.5     -85.4    84   F  1   1842  18 54 30

18 56 00  M82          04 28 59  31.3  23.8 -5.5     -85.7    -6   1  1   1842  No stop 
18 58 00  ---          04 30 59  31.5  23.8 -5.4     -86.2   114   F  1   1850  18 56 00

18 58 30  M81          04 31 29  31.5  24.5 -5.4     -86.0    24   1  1   1850  18 58 30
18 59 30  ---          04 32 30  31.6  24.5 -5.4     -86.2    60   F  1   1854  18 58 30

18 59 30  M82          04 32 30  31.6  23.8 -5.4     -86.5    -6   1  1   1854  No stop 
19 01 30  ---          04 34 30  31.8  23.8 -5.4     -87.0   114   F  1   1862  18 59 30

19 01 30  M81          04 34 30  31.8  24.5 -5.4     -86.7    -6   1  1   1862  No stop 
19 03 00  ---          04 36 00  31.9  24.6 -5.3     -87.0    84   F  1   1868  19 01 30
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

19 03 00  M82          04 36 00  31.9  23.8 -5.3     -87.3    -6   1  1   1868  No stop 
19 05 00  ---          04 38 01  32.1  23.8 -5.3     -87.8   114   F  1   1875  19 03 00

19 05 30  M81          04 38 31  32.1  24.6 -5.3     -87.6    24   1  1   1875  19 05 30
19 06 30  ---          04 39 31  32.2  24.6 -5.3     -87.8    60   F  1   1879  19 05 30

19 06 30  M82          04 39 31  32.2  23.8 -5.3     -88.1    -6   1  1   1879  No stop 
19 08 30  ---          04 41 31  32.4  23.9 -5.3     -88.6   114   F  1   1887  19 06 30

19 08 30  M81          04 41 31  32.4  24.6 -5.2     -88.3    -6   1  1   1887  No stop 
19 10 00  ---          04 43 01  32.5  24.6 -5.2     -88.6    84   F  1   1893  19 08 30

19 10 00  M82          04 43 01  32.5  23.9 -5.2     -88.9    -6   1  1   1893  No stop 
19 12 00  ---          04 45 02  32.7  23.9 -5.2     -89.4   114   F  1   1901  19 10 00

19 12 00  M81          04 45 02  32.7  24.6 -5.2     -89.1    -6   1  1   1901  No stop 
19 13 30  ---          04 46 32  32.9  24.6 -5.2     -89.4    84   F  1   1906  19 12 00

19 13 30  M82          04 46 32  32.8  23.9 -5.2     -89.8    -6   1  1   1906  No stop 
19 15 30  ---          04 48 32  33.0  23.9 -5.1     -90.2   114   F  1   1914  19 13 30

19 16 00  M81          04 49 02  33.1  24.6 -5.1     -90.0    24   1  1   1914  19 16 00
19 17 00  ---          04 50 03  33.2  24.6 -5.1     -90.3    60   F  1   1918  19 16 00

19 17 30  J1048+7143   04 50 33  29.0  21.1 -6.0     -79.8    16   1  1   1918  19 17 30
19 20 30  =1044+719    04 53 33  29.3  21.1 -5.9     -80.4   180   F  1   1930  19 17 30

19 20 30  M81          04 53 33  33.5  24.6 -5.0     -91.1   -14   1  1   1930  No stop 
19 22 30  ---          04 55 33  33.7  24.6 -5.0     -91.6   106   F  1   1937  19 20 30

19 22 30  M82          04 55 33  33.6  23.8 -5.0     -91.9    -6   1  1   1937  No stop 
19 24 30  ---          04 57 34  33.8  23.8 -5.0     -92.4   114   F  1   1945  19 22 30

19 24 30  M81          04 57 34  33.8  24.6 -5.0     -92.0    -6   1  1   1945  No stop 
19 26 00  ---          04 59 04  34.0  24.6 -5.0     -92.4    84   F  1   1951  19 24 30

19 26 00  M82          04 59 04  33.9  23.8 -5.0     -92.7    -6   1  1   1951  No stop 
19 28 00  ---          05 01 04  34.1  23.8 -4.9     -93.2   114   F  1   1959  19 26 00

19 28 30  M81          05 01 34  34.2  24.6 -4.9     -93.0    24   1  1   1959  19 28 30
19 29 30  ---          05 02 35  34.3  24.5 -4.9     -93.2    60   F  1   1962  19 28 30

19 29 30  M82          05 02 35  34.2  23.8 -4.9     -93.6    -6   1  1   1962  No stop 
19 31 30  ---          05 04 35  34.4  23.8 -4.9     -94.0   114   F  1   1970  19 29 30
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

19 31 30  M81          05 04 35  34.5  24.5 -4.9     -93.7    -6   1  1   1970  No stop 
19 33 00  ---          05 06 05  34.6  24.5 -4.8     -94.0    84   F  1   1976  19 31 30

19 33 00  M82          05 06 05  34.5  23.8 -4.8     -94.4    -6   1  1   1976  No stop 
19 35 00  ---          05 08 05  34.7  23.8 -4.8     -94.9   114   F  1   1984  19 33 00

19 35 00  M81          05 08 05  34.8  24.5 -4.8     -94.5    -6   1  1   1984  No stop 
19 36 30  ---          05 09 36  34.9  24.5 -4.8     -94.9    84   F  1   1990  19 35 00

19 36 30  M82          05 09 36  34.8  23.8 -4.8     -95.2    -6   1  1   1990  No stop 
19 38 30  ---          05 11 36  35.0  23.7 -4.8     -95.7   114   F  1   1997  19 36 30

19 39 00  M81          05 12 06  35.1  24.5 -4.7     -95.5    24   1  1   1997  19 39 00
19 40 00  ---          05 13 06  35.2  24.5 -4.7     -95.7    60   F  1   2001  19 39 00

19 40 00  M82          05 13 06  35.1  23.7 -4.7     -96.1    -6   1  1   2001  No stop 
19 42 00  ---          05 15 07  35.3  23.7 -4.7     -96.6   114   F  1   2009  19 40 00

19 42 00  M81          05 15 07  35.4  24.4 -4.7     -96.2    -6   1  1   2009  No stop 
19 43 30  ---          05 16 37  35.5  24.4 -4.7     -96.6    84   F  1   2015  19 42 00

19 43 30  M82          05 16 37  35.4  23.7 -4.7     -96.9    -6   1  1   2015  No stop 
19 45 30  ---          05 18 37  35.6  23.6 -4.6     -97.4   114   F  1   2022  19 43 30

19 46 00  M81          05 19 07  35.8  24.4 -4.6     -97.2    24   1  1   2022  19 46 00
19 47 00  ---          05 20 07  35.9  24.4 -4.6     -97.4    60   F  1   2026  19 46 00

19 47 00  M82          05 20 07  35.8  23.6 -4.6     -97.8    -6   1  1   2026  No stop 
19 49 00  ---          05 22 08  35.9  23.6 -4.6     -98.3   114   F  1   2034  19 47 00

19 49 00  M81          05 22 08  36.0  24.3 -4.6     -97.9    -6   1  1   2034  No stop 
19 50 30  ---          05 23 38  36.2  24.3 -4.5     -98.3    84   F  1   2040  19 49 00

19 50 30  M82          05 23 38  36.1  23.6 -4.6     -98.6    -6   1  1   2040  No stop 
19 52 30  ---          05 25 38  36.2  23.5 -4.5     -99.1   114   F  1   2048  19 50 30

19 52 30  M81          05 25 38  36.3  24.3 -4.5     -98.7    -6   1  1   2048  No stop 
19 54 00  ---          05 27 09  36.5  24.3 -4.5     -99.1    84   F  1   2053  19 52 30

19 54 00  M82          05 27 09  36.4  23.5 -4.5     -99.5    -6   1  1   2053  No stop 
19 56 00  ---          05 29 09  36.5  23.5 -4.5    -100.0   114   F  1   2061  19 54 00

19 56 30  M81          05 29 39  36.7  24.2 -4.4     -99.7    24   1  1   2061  19 56 30
19 57 30  ---          05 30 39  36.8  24.2 -4.4    -100.0    60   F  1   2065  19 56 30
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               M82 transient (ToO)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  29 May 2010   Day 149 ---

19 57 30  M82          05 30 39  36.7  23.4 -4.4    -100.3    -6   1  1   2065  No stop 
19 59 30  ---          05 32 40  36.8  23.4 -4.4    -100.8   114   F  1   2073  19 57 30

19 59 30  M81          05 32 40  37.0  24.2 -4.4    -100.5    -6   1  1   2073  No stop 
20 01 00  ---          05 34 10  37.1  24.1 -4.4    -100.8    84   F  1   2079  19 59 30

20 01 00  M82          05 34 10  37.0  23.4 -4.4    -101.2    -6   1  1   2079  No stop 
20 03 00  ---          05 36 10  37.1  23.3 -4.3    -101.7   114   F  1   2086  20 01 00

20 03 30  M81          05 36 40  37.3  24.1 -4.3    -101.5    24   1  1   2086  20 03 30
20 04 30  ---          05 37 40  37.4  24.0 -4.3    -101.7    60   F  1   2090  20 03 30

20 04 30  M82          05 37 40  37.3  23.3 -4.3    -102.1    -6   1  1   2090  No stop 
20 06 30  ---          05 39 41  37.4  23.3 -4.3    -102.6   114   F  1   2098  20 04 30

20 06 30  M81          05 39 41  37.6  24.0 -4.3    -102.2    -6   1  1   2098  No stop 
20 08 00  ---          05 41 11  37.7  24.0 -4.3    -102.6    84   F  1   2104  20 06 30

20 08 00  M82          05 41 11  37.6  23.2 -4.3    -103.0    -6   1  1   2104  No stop 
20 10 00  ---          05 43 11  37.7  23.2 -4.2    -103.5   114   F  1   2111  20 08 00

20 10 00  M81          05 43 11  37.9  23.9 -4.2    -103.1    -6   1  1   2111  No stop 
20 11 30  ---          05 44 41  38.0  23.9 -4.2    -103.4    84   F  1   2117  20 10 00

20 11 30  M82          05 44 41  37.9  23.1 -4.2    -103.8    -6   1  1   2117  No stop 
20 13 30  ---          05 46 42  38.0  23.1 -4.2    -104.3   114   F  1   2125  20 11 30

20 14 00  M81          05 47 12  38.2  23.8 -4.2    -104.1    24   1  1   2125  20 14 00
20 15 00  ---          05 48 12  38.3  23.8 -4.1    -104.3    60   F  1   2129  20 14 00

20 15 30  J1048+7143   05 48 42  33.6  21.4 -5.0     -93.4    15   1  1   2129  20 15 30
20 18 30  =1044+719    05 51 43  33.8  21.4 -5.0     -94.1   180   F  1   2141  20 15 30

20 19 30  4C39.25      05 52 43  45.7  63.9 -3.6     -83.8    26   1  1   2141  20 19 30
20 28 30  ---          06 01 44  47.5  64.1 -3.4     -85.0   540   F  1   2175  20 19 30


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gb071.6cm
   Matching groups in /aps3/sched9.3/catalogs/freq.dat:
     v6cm_2

   Setup group:   11         Station: VLBA_FD           Total bit rate:  512
   Format: VLBA1:4           Bits per sample: 1         Sample rate: 32.000
   Number of channels: 16                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
             4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
                   5         6         5         6         7         8         7         8
   BBC SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 
                  A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:  11  Setup file default.  Used pcal sets:   1
   LO sum=    4942.49   4942.49   4942.49   4942.49   4974.49   4974.49   4974.49   4974.49
              5006.49   5006.49   5006.49   5006.49   5038.49   5038.49   5038.49   5038.49
   BBC fr=     842.49    842.49    842.49    842.49    874.49    874.49    874.49    874.49
               906.49    906.49    906.49    906.49    938.49    938.49    938.49    938.49
   Bandwd=     16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000
               16.000    16.000    16.000    16.000    16.000    16.000    16.000    16.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S9    S11   S13   S15
    PCALXB2=   S2    S4    S6    S8    S10   S12   S14   S16
    PCALFR1=   490   510   490   510   490   510   490   510
    PCALFR2=   490   510   490   510   490   510   490   510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27, 66, 74, 82, 90, 67, 75, 83, 91
    barrel=roll_off 
 SOURCE LIST -- M82 transient (ToO)
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * M82               09 51 42.820698   * 09 55 51.551000     09 56 43.985903       0.00
                     69 54 59.52156    * 69 40 45.79200      69 37 59.74072        0.00
                     From catalog imbedded in main SCHED input file.
                        5.000 scan hours,    534.852 baseline hours above horizon.

   J0927+3902        09 23 55.319215   * 09 27 03.013936     09 27 42.722175       0.01
   0923+392          39 15 23.56644    * 39 02 20.85184      38 59 42.57979        0.01
 * 4C39.25           /aps3/sched9.3/catalogs/sources.vlba
   J0927+39          GSFC Nov. 2009 Solution 2009a    226075 Observations
                        0.150 scan hours,     14.547 baseline hours above horizon.

   J0955+6903        09 51 27.310825   * 09 55 33.173069     09 56 25.021626       0.11
   0951+693          69 18 08.14426    * 69 03 55.06092      69 01 09.05193        0.03
 * M81               /aps3/sched9.3/catalogs/sources.vlba
                     GSFC Nov. 2009 Solution 2009a      2054 Observations
                        3.583 scan hours,    378.792 baseline hours above horizon.

 * J1048+7143        10 44 49.735104   * 10 48 27.619920     10 49 14.396117       0.02
   1044+719          71 59 26.88537    * 71 43 35.93840      71 40 29.83488        0.01
   J1048+71          /aps3/sched9.3/catalogs/sources.vlba
                     GSFC Nov. 2009 Solution 2009a    118344 Observations
                        0.567 scan hours,     59.469 baseline hours above horizon.

   J2253+1608        22 51 29.519743   * 22 53 57.747942     22 54 29.397075       0.01
 * 3C454.3           15 52 54.34806    * 16 08 53.56089      16 12 10.61631        0.01
   2251+158          /aps3/sched9.3/catalogs/sources.vlba
   J2253+16          GSFC Nov. 2009 Solution 2009a     39040 Observations
                        0.067 scan hours,      8.000 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   M82                 67.2
   4C39.25             65.6
   M81                 67.2
   J1048+7143          71.3
   3C454.3             77.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

