  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
 Exp. Code:  GI001A  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 18 Sept. 2003                      

PI:       Hiroshi Imai                                                    

Address:  Department of Physics                                           
          Kagoshima University                                            
          Japan                                                           
          1-21-35 Korimoto, Kagoshima 890-0065                            

Phone:    81-99-285-8960                                                  
EMAIL:    hiroimai@sci.kagoshima-u.ac.jp                                  
Fax:      81-99-285-8960                                                  
Phone during observation: 81-99-285-8960                                  

Observing mode: VLBA/MKIV                                                 

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   7 Nov 2003   Day 311 ---

 Next scan frequencies:  1611.76  1611.76  1614.02  1614.02  1618.02  1618.02
                         1622.02  1622.02
 Next BBC frequencies:    788.24   788.24   785.98   785.98   781.98   781.98
                          777.98   777.98
 Next scan bandwidths:      0.50     0.50     4.00     4.00     4.00     4.00
                            4.00     4.00

17 37 00  1830+139     13 47 16  22.9  86.9 -4.8     -62.3     0   1  1      0  17 37 00
17 43 00  ---          13 53 17  24.2  87.6 -4.7     -62.4   360   F  1   4800

17 44 00  W43AOH       13 54 17  13.3 100.2 -4.9     -57.9    32   1  1   4800  17 44 00
18 00 00  ---          14 10 20  16.7 102.4 -4.6     -57.2   960   F  1  17600

18 01 00  W43AOH       14 11 20  16.9 102.5 -4.6     -57.2    54   1  2  17600  18 01 00
18 23 00  ---          14 33 24  21.5 105.8 -4.2     -55.9  1320   R  1      0

18 25 00  1830+139     14 35 24  33.3  93.0 -4.0     -62.3    90   1  1      0  18 25 00
18 31 00  ---          14 41 25  34.6  93.9 -3.9     -62.2   360   F  2   4800

18 33 00  OT081        14 43 25  41.5 105.3 -3.1     -57.3   100   1  1   4800  18 33 00
18 39 00  ---          14 49 26  42.8 106.4 -3.0     -56.8   360   F  2   9600

18 41 00  2145+067     14 51 27  -8.5  76.6 -6.9  D  -57.5    33   1  1   9600  18 41 00
18 46 00  ---          14 56 27  -7.4  77.3 -6.9  D  -57.7     0   F  2  13600

18 47 00  W43AOH       14 57 27  26.4 109.5 -3.8     -54.2     6   1  1  13600  18 47 00
18 52 00  ---          15 02 28  27.5 110.3 -3.8     -53.8   300   F  2  17600

18 53 00  W43AOH       15 03 28  27.7 110.5 -3.7     -53.7    54   1  2  17600  18 53 00
19 15 00  ---          15 25 32  32.0 114.4 -3.4     -51.6  1320   R  2      0

19 16 00  W43AOH       15 26 32  32.2 114.5 -3.4     -51.5    54   1  3      0  19 16 00
19 38 00  ---          15 48 36  36.5 118.8 -3.0     -49.0  1320   F  1  17600

19 39 00  W43AOH       15 49 36  36.7 119.0 -3.0     -48.8    54   1  4  17600  19 39 00
19 50 00  ---          16 00 38  38.7 121.3 -2.8     -47.3   660   R  1   8800

19 51 00  OT081        16 01 38  56.9 123.5 -1.8     -46.7    18   1  4   8800  19 51 00
19 57 00  ---          16 07 39  58.0 125.4 -1.7     -45.4   360   R  1   4000

19 59 00  2145+067     16 09 39   8.1  86.7 -5.6     -59.9    14   1  4   4000  19 59 00
20 04 00  ---          16 14 40   9.2  87.3 -5.6     -60.0   300   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   7 Nov 2003   Day 311 ---

20 04 00  OT081        16 14 40  59.2 127.8 -1.6     -43.6  -106   1  3      0  20 04 00
20 05 00  ---          16 15 40  59.4 128.1 -1.6     -43.4   -46   F  2    800

20 06 00  TXS1843      16 16 40  43.1 123.7 -2.5     -45.7    21   1  3    800  20 06 00
20 08 00  ---          16 18 41  43.4 124.2 -2.5     -45.3   120   F  2   2400

20 08 00  TXS1843      16 18 41  43.4 124.2 -2.5     -45.3    -4   1  3   2400  20 08 00
20 10 30  ---          16 21 11  43.9 124.8 -2.4     -44.9   146   F  2   4400

20 10 30  W43AOH       16 21 11  42.4 126.1 -2.4     -44.1    -9   1  3   4400  20 10 30
20 13 00  ---          16 23 42  42.8 126.7 -2.4     -43.7   141   F  2   6400

20 13 00  TXS1843      16 23 42  44.3 125.5 -2.4     -44.5    -9   1  3   6400  20 13 00
20 15 30  ---          16 26 12  44.8 126.1 -2.3     -44.1   141   F  2   8400

20 15 30  W43AOH       16 26 12  43.3 127.3 -2.4     -43.2    -9   1  3   8400  20 15 30
20 18 00  ---          16 28 42  43.7 127.9 -2.3     -42.8   141   F  2  10400

20 18 00  TXS1843      16 28 42  45.2 126.7 -2.3     -43.6    -9   1  3  10400  20 18 00
20 20 30  ---          16 31 13  45.6 127.4 -2.3     -43.1   141   F  2  12400

20 20 30  W43AOH       16 31 13  44.1 128.6 -2.3     -42.3    -9   1  3  12400  20 20 30
20 23 00  ---          16 33 43  44.5 129.2 -2.2     -41.8   141   F  2  14400

20 24 00  TXS1843      16 34 43  46.2 128.3 -2.2     -42.5    51   1  3  14400  20 24 00
20 26 00  ---          16 36 44  46.6 128.8 -2.2     -42.1   120   F  2  16000

20 26 00  TXS1843      16 36 44  46.6 128.8 -2.2     -42.1    -4   1  4  16000  20 26 00
20 28 30  ---          16 39 14  47.0 129.5 -2.1     -41.6   146   R  2  14000

20 28 30  W43AOH       16 39 14  45.4 130.7 -2.1     -40.7    -9   1  4  14000  20 28 30
20 31 00  ---          16 41 45  45.8 131.4 -2.1     -40.2   141   R  2  12000

20 31 00  TXS1843      16 41 45  47.4 130.2 -2.1     -41.1    -9   1  4  12000  20 31 00
20 33 30  ---          16 44 15  47.8 130.9 -2.0     -40.6   141   R  2  10000

20 33 30  W43AOH       16 44 15  46.3 132.1 -2.1     -39.7    -9   1  4  10000  20 33 30
20 36 00  ---          16 46 45  46.7 132.8 -2.0     -39.2   141   R  2   8000

20 36 00  TXS1843      16 46 45  48.2 131.6 -2.0     -40.0    -9   1  4   8000  20 36 00
20 38 30  ---          16 49 16  48.6 132.4 -1.9     -39.5   141   R  2   6000

20 38 30  W43AOH       16 49 16  47.0 133.5 -2.0     -38.7    -9   1  4   6000  20 38 30
20 41 00  ---          16 51 46  47.4 134.2 -1.9     -38.1   141   R  2   4000
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   7 Nov 2003   Day 311 ---

20 41 00  TXS1843      16 51 46  49.0 133.1 -1.9     -38.9    -9   1  4   4000  20 41 00
20 43 30  ---          16 54 17  49.4 133.8 -1.9     -38.4   141   R  2   2000

20 43 30  W43AOH       16 54 17  47.8 134.9 -1.9     -37.5    -9   1  4   2000  20 43 30
20 46 00  ---          16 56 47  48.2 135.7 -1.9     -37.0   141   R  2      0

20 48 00  OT081        16 58 47  65.7 146.8 -0.9     -28.5    79   1  5      0  20 48 00
20 53 00  ---          17 03 48  66.2 149.5 -0.8     -26.3   300   F  1   4000

20 54 00  TXS1843      17 04 48  51.0 137.1 -1.7     -35.8    24   1  5   4000  20 54 00
20 56 00  ---          17 06 49  51.3 137.8 -1.7     -35.3   120   F  1   5600

20 56 00  TXS1843      17 06 49  51.3 137.8 -1.7     -35.3    -4   1  5   5600  20 56 00
20 58 30  ---          17 09 19  51.6 138.6 -1.6     -34.7   146   F  1   7600

20 58 30  W43AOH       17 09 19  50.0 139.6 -1.6     -33.9    -9   1  5   7600  20 58 30
21 01 00  ---          17 11 50  50.4 140.4 -1.6     -33.3   141   F  1   9600

21 01 00  TXS1843      17 11 50  52.0 139.4 -1.6     -34.0    -9   1  5   9600  21 01 00
21 03 30  ---          17 14 20  52.3 140.3 -1.5     -33.3   141   F  1  11600

21 03 30  W43AOH       17 14 20  50.7 141.2 -1.6     -32.6    -9   1  5  11600  21 03 30
21 06 00  ---          17 16 50  51.0 142.1 -1.5     -32.0   141   F  1  13600

21 06 00  TXS1843      17 16 50  52.7 141.2 -1.5     -32.7    -9   1  5  13600  21 06 00
21 08 30  ---          17 19 21  53.0 142.0 -1.4     -32.0   141   F  1  15600

21 08 30  W43AOH       17 19 21  51.4 142.9 -1.5     -31.3    -9   1  5  15600  21 08 30
21 11 00  ---          17 21 51  51.7 143.8 -1.4     -30.6   141   F  1  17600

21 12 00  TXS1843      17 22 51  53.5 143.3 -1.4     -31.0    50   1  6  17600  21 12 00
21 14 00  ---          17 24 52  53.7 144.0 -1.4     -30.4   120   R  1  16000

21 14 00  TXS1843      17 24 52  53.7 144.0 -1.4     -30.4    -4   1  6  16000  21 14 00
21 16 30  ---          17 27 22  54.0 144.9 -1.3     -29.6   146   R  1  14000

21 16 30  W43AOH       17 27 22  52.4 145.7 -1.3     -29.0    -9   1  6  14000  21 16 30
21 19 00  ---          17 29 52  52.7 146.6 -1.3     -28.3   141   R  1  12000

21 19 00  TXS1843      17 29 52  54.4 145.9 -1.3     -28.9    -9   1  6  12000  21 19 00
21 21 30  ---          17 32 23  54.7 146.8 -1.2     -28.1   141   R  1  10000

21 21 30  W43AOH       17 32 23  53.0 147.5 -1.3     -27.5    -9   1  6  10000  21 21 30
21 24 00  ---          17 34 53  53.2 148.5 -1.2     -26.8   141   R  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   7 Nov 2003   Day 311 ---

21 24 00  TXS1843      17 34 53  54.9 147.8 -1.2     -27.3    -9   1  6   8000  21 24 00
21 26 30  ---          17 37 24  55.2 148.8 -1.1     -26.5   141   R  1   6000

21 26 30  W43AOH       17 37 24  53.5 149.4 -1.2     -26.0    -9   1  6   6000  21 26 30
21 29 00  ---          17 39 54  53.8 150.4 -1.1     -25.2   141   R  1   4000

21 29 00  TXS1843      17 39 54  55.5 149.7 -1.1     -25.7    -9   1  6   4000  21 29 00
21 31 30  ---          17 42 25  55.8 150.7 -1.1     -24.9   141   R  1   2000

21 31 30  W43AOH       17 42 25  54.1 151.3 -1.1     -24.4    -9   1  6   2000  21 31 30
21 34 00  ---          17 44 55  54.3 152.3 -1.0     -23.6   141   R  1      0

21 36 00  OT081        17 46 55  69.0 176.7 -0.1      -2.9    85   1  5      0  21 36 00
21 41 00  ---          17 51 56  69.0 180.2  0.0       0.1   300   F  2   4000

21 42 00  TXS1843      17 52 56  56.8 155.1 -0.9     -21.2    30   1  5   4000  21 42 00
21 44 00  ---          17 54 57  57.0 156.0 -0.9     -20.5   120   F  2   5600

21 44 00  TXS1843      17 54 57  57.0 156.0 -0.9     -20.5    -4   1  5   5600  21 44 00
21 46 30  ---          17 57 27  57.2 157.1 -0.8     -19.6   146   F  2   7600

21 46 30  W43AOH       17 57 27  55.5 157.4 -0.8     -19.3    -9   1  5   7600  21 46 30
21 49 00  ---          17 59 57  55.7 158.4 -0.8     -18.5   141   F  2   9600

21 49 00  TXS1843      17 59 57  57.4 158.1 -0.8     -18.7    -9   1  5   9600  21 49 00
21 51 30  ---          18 02 28  57.6 159.3 -0.7     -17.7   141   F  2  11600

21 51 30  W43AOH       18 02 28  55.9 159.5 -0.8     -17.6    -9   1  5  11600  21 51 30
21 54 00  ---          18 04 58  56.0 160.6 -0.7     -16.7   141   F  2  13600

21 54 00  TXS1843      18 04 58  57.8 160.4 -0.7     -16.8    -9   1  5  13600  21 54 00
21 56 30  ---          18 07 29  58.0 161.5 -0.6     -15.8   141   F  2  15600

21 56 30  W43AOH       18 07 29  56.2 161.6 -0.7     -15.7    -9   1  5  15600  21 56 30
21 59 00  ---          18 09 59  56.4 162.7 -0.6     -14.8   141   F  2  17600

22 00 00  TXS1843      18 10 59  58.2 163.1 -0.6     -14.5    50   1  6  17600  22 00 00
22 02 00  ---          18 13 00  58.3 164.0 -0.6     -13.7   120   R  2  16000

22 02 00  TXS1843      18 13 00  58.3 164.0 -0.6     -13.7    -4   1  6  16000  22 02 00
22 04 30  ---          18 15 30  58.5 165.2 -0.5     -12.7   146   R  2  14000

22 04 30  W43AOH       18 15 30  56.7 165.2 -0.5     -12.7    -9   1  6  14000  22 04 30
22 07 00  ---          18 18 00  56.8 166.3 -0.5     -11.8   141   R  2  12000
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   7 Nov 2003   Day 311 ---

22 07 00  TXS1843      18 18 00  58.6 166.4 -0.5     -11.7    -9   1  6  12000  22 07 00
22 09 30  ---          18 20 31  58.7 167.5 -0.4     -10.7   141   R  2  10000

22 09 30  W43AOH       18 20 31  57.0 167.4 -0.5     -10.8    -9   1  6  10000  22 09 30
22 12 00  ---          18 23 01  57.1 168.5 -0.4      -9.9   141   R  2   8000

22 12 00  TXS1843      18 23 01  58.8 168.7 -0.4      -9.7    -9   1  6   8000  22 12 00
22 14 30  ---          18 25 32  58.9 169.9 -0.3      -8.6   141   R  2   6000

22 14 30  W43AOH       18 25 32  57.2 169.7 -0.4      -8.9    -9   1  6   6000  22 14 30
22 17 00  ---          18 28 02  57.3 170.8 -0.3      -7.9   141   R  2   4000

22 17 00  TXS1843      18 28 02  59.0 171.1 -0.3      -7.6    -9   1  6   4000  22 17 00
22 19 30  ---          18 30 32  59.1 172.3 -0.3      -6.6   141   R  2   2000

22 19 30  W43AOH       18 30 32  57.4 172.0 -0.3      -6.9    -9   1  6   2000  22 19 30
22 22 00  ---          18 33 03  57.4 173.1 -0.2      -5.9   141   R  2      0

22 24 00  OT081        18 35 03  66.7 208.0  0.7      24.2    91   1  7      0  22 24 00
22 29 00  ---          18 40 04  66.2 210.8  0.8      26.5   300   F  1   4000

22 30 00  TXS1843      18 41 04  59.3 177.5 -0.1      -2.2    32   1  7   4000  22 30 00
22 32 00  ---          18 43 04  59.3 178.5 -0.1      -1.3   120   F  1   5600

22 32 00  TXS1843      18 43 04  59.3 178.5 -0.1      -1.3    -4   1  7   5600  22 32 00
22 34 30  ---          18 45 35  59.3 179.7  0.0      -0.3   146   F  1   7600

22 34 30  W43AOH       18 45 35  57.6 178.9  0.0      -0.9    -9   1  7   7600  22 34 30
22 37 00  ---          18 48 05  57.6 180.1  0.0       0.1   141   F  1   9600

22 37 00  TXS1843      18 48 05  59.3 180.9  0.0       0.8    -9   1  7   9600  22 37 00
22 39 30  ---          18 50 36  59.3 182.1  0.1       1.8   141   F  1  11600

22 39 30  W43AOH       18 50 36  57.6 181.3  0.0       1.1    -9   1  7  11600  22 39 30
22 42 00  ---          18 53 06  57.6 182.4  0.1       2.1   141   F  1  13600

22 42 00  TXS1843      18 53 06  59.3 183.4  0.1       2.9    -9   1  7  13600  22 42 00
22 44 30  ---          18 55 37  59.2 184.6  0.2       3.9   141   F  1  15600

22 44 30  W43AOH       18 55 37  57.6 183.6  0.1       3.1    -9   1  7  15600  22 44 30
22 47 00  ---          18 58 07  57.5 184.8  0.2       4.1   141   F  1  17600

22 48 00  TXS1843      18 59 07  59.2 186.3  0.2       5.4    51   1  8  17600  22 48 00
22 50 00  ---          19 01 07  59.1 187.3  0.2       6.2   120   R  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   7 Nov 2003   Day 311 ---

22 50 00  TXS1843      19 01 07  59.1 187.3  0.2       6.2    -4   1  8  16000  22 50 00
22 52 30  ---          19 03 38  59.0 188.5  0.3       7.3   146   R  1  14000

22 52 30  W43AOH       19 03 38  57.4 187.3  0.3       6.3    -9   1  8  14000  22 52 30
22 55 00  ---          19 06 08  57.3 188.5  0.3       7.3   141   R  1  12000

22 55 00  TXS1843      19 06 08  58.9 189.7  0.3       8.3    -9   1  8  12000  22 55 00
22 57 30  ---          19 08 39  58.9 190.9  0.4       9.3   141   R  1  10000

22 57 30  W43AOH       19 08 39  57.2 189.6  0.3       8.3    -9   1  8  10000  22 57 30
23 00 00  ---          19 11 09  57.1 190.8  0.4       9.3   141   R  1   8000

23 00 00  TXS1843      19 11 09  58.7 192.1  0.4      10.4    -9   1  8   8000  23 00 00
23 02 30  ---          19 13 39  58.6 193.3  0.5      11.4   141   R  1   6000

23 02 30  W43AOH       19 13 39  57.0 191.9  0.4      10.2    -9   1  8   6000  23 02 30
23 05 00  ---          19 16 10  56.9 193.0  0.5      11.2   141   R  1   4000

23 05 00  TXS1843      19 16 10  58.5 194.4  0.5      12.4    -9   1  8   4000  23 05 00
23 07 30  ---          19 18 40  58.4 195.6  0.5      13.4   141   R  1   2000

23 07 30  W43AOH       19 18 40  56.8 194.2  0.5      12.2    -9   1  8   2000  23 07 30
23 10 00  ---          19 21 11  56.7 195.3  0.6      13.1   141   R  1      0

23 12 00  OT081        19 23 11  60.1 230.3  1.5      42.1    91   1  7      0  23 12 00
23 17 00  ---          19 28 12  59.3 232.0  1.6      43.5   300   F  2   4000

23 18 00  TXS1843      19 29 12  57.7 200.4  0.7      17.4    33   1  7   4000  23 18 00
23 20 00  ---          19 31 12  57.5 201.3  0.7      18.2   120   F  2   5600

23 20 00  TXS1843      19 31 12  57.5 201.3  0.7      18.2    -4   1  7   5600  23 20 00
23 22 30  ---          19 33 43  57.3 202.4  0.8      19.1   146   F  2   7600

23 22 30  W43AOH       19 33 43  55.8 200.7  0.8      17.7    -9   1  7   7600  23 22 30
23 25 00  ---          19 36 13  55.6 201.8  0.8      18.6   141   F  2   9600

23 25 00  TXS1843      19 36 13  57.1 203.5  0.8      20.0    -9   1  7   9600  23 25 00
23 27 30  ---          19 38 44  56.9 204.5  0.9      20.9   141   F  2  11600

23 27 30  W43AOH       19 38 44  55.4 202.8  0.8      19.5    -9   1  7  11600  23 27 30
23 30 00  ---          19 41 14  55.2 203.8  0.9      20.4   141   F  2  13600

23 30 00  TXS1843      19 41 14  56.6 205.6  0.9      21.8    -9   1  7  13600  23 30 00
23 32 30  ---          19 43 44  56.4 206.7  1.0      22.7   141   F  2  15600
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri   7 Nov 2003   Day 311 ---

23 32 30  W43AOH       19 43 44  55.0 204.9  0.9      21.2    -9   1  7  15600  23 32 30
23 35 00  ---          19 46 15  54.8 205.9  1.0      22.1   141   F  2  17600

23 36 00  TXS1843      19 47 15  56.1 208.1  1.0      23.9    51   1  8  17600  23 36 00
23 38 00  ---          19 49 15  55.9 208.9  1.1      24.6   120   R  2  16000

23 38 00  TXS1843      19 49 15  55.9 208.9  1.1      24.6    -4   1  8  16000  23 38 00
23 40 30  ---          19 51 46  55.6 209.9  1.1      25.4   146   R  2  14000

23 40 30  W43AOH       19 51 46  54.2 208.1  1.1      23.9    -9   1  8  14000  23 40 30
23 43 00  ---          19 54 16  54.0 209.0  1.1      24.7   141   R  2  12000

23 43 00  TXS1843      19 54 16  55.3 210.9  1.1      26.2    -9   1  8  12000  23 43 00
23 45 30  ---          19 56 47  55.0 211.9  1.2      27.1   141   R  2  10000

23 45 30  W43AOH       19 56 47  53.7 210.0  1.1      25.5    -9   1  8  10000  23 45 30
23 48 00  ---          19 59 17  53.4 211.0  1.2      26.3   141   R  2   8000

23 48 00  TXS1843      19 59 17  54.7 212.9  1.2      27.8    -9   1  8   8000  23 48 00
23 50 30  ---          20 01 47  54.4 213.8  1.3      28.6   141   R  2   6000

23 50 30  W43AOH       20 01 47  53.1 211.9  1.2      27.0    -9   1  8   6000  23 50 30
23 53 00  ---          20 04 18  52.9 212.8  1.3      27.8   141   R  2   4000

23 53 00  TXS1843      20 04 18  54.1 214.8  1.3      29.4    -9   1  8   4000  23 53 00
23 55 30  ---          20 06 48  53.8 215.7  1.3      30.1   141   R  2   2000

23 55 30  W43AOH       20 06 48  52.6 213.7  1.3      28.5    -9   1  8   2000  23 55 30
23 58 00  ---          20 09 19  52.3 214.6  1.4      29.3   141   R  2      0

 --- Sat   8 Nov 2003   Day 312 ---

00 00 00  OT081        20 11 19  51.4 244.6  2.3      52.0    94   1  9      0  00 00 00
00 05 00  ---          20 16 20  50.4 245.8  2.4      52.8   300   F  1   4000

00 06 00  TXS1843      20 17 20  52.5 219.4  1.5      33.1    36   1  9   4000  00 06 00
00 08 00  ---          20 19 20  52.2 220.1  1.6      33.7   120   F  1   5600

00 08 00  TXS1843      20 19 20  52.2 220.1  1.6      33.7    -4   1  9   5600  00 08 00
00 10 30  ---          20 21 51  51.8 221.0  1.6      34.3   146   F  1   7600

00 10 30  W43AOH       20 21 51  50.6 218.9  1.6      32.7    -8   1  9   7600  00 10 30
00 13 00  ---          20 24 21  50.3 219.8  1.6      33.4   142   F  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Nov 2003   Day 312 ---

00 13 00  TXS1843      20 24 21  51.5 221.8  1.6      35.0    -8   1  9   9600  00 13 00
00 15 30  ---          20 26 51  51.1 222.6  1.7      35.6   142   F  1  11600

00 15 30  W43AOH       20 26 51  49.9 220.6  1.6      34.0    -8   1  9  11600  00 15 30
00 18 00  ---          20 29 22  49.6 221.4  1.7      34.7   142   F  1  13600

00 18 00  TXS1843      20 29 22  50.7 223.4  1.7      36.3    -8   1  9  13600  00 18 00
00 20 30  ---          20 31 52  50.4 224.2  1.8      36.9   142   F  1  15600

00 20 30  W43AOH       20 31 52  49.2 222.2  1.7      35.3    -8   1  9  15600  00 20 30
00 23 00  ---          20 34 23  48.9 222.9  1.8      35.9   142   F  1  17600

00 24 00  TXS1843      20 35 23  49.8 225.3  1.8      37.7    52   1 10  17600  00 24 00
00 26 00  ---          20 37 23  49.5 225.9  1.9      38.2   120   R  1  16000

00 26 00  TXS1843      20 37 23  49.5 225.9  1.9      38.2    -4   1 10  16000  00 26 00
00 28 30  ---          20 39 54  49.1 226.7  1.9      38.7   146   R  1  14000

00 28 30  W43AOH       20 39 54  48.1 224.6  1.9      37.2    -8   1 10  14000  00 28 30
00 31 00  ---          20 42 24  47.7 225.3  1.9      37.8   142   R  1  12000

00 31 00  TXS1843      20 42 24  48.7 227.4  1.9      39.3    -8   1 10  12000  00 31 00
00 33 30  ---          20 44 54  48.3 228.1  2.0      39.8   142   R  1  10000

00 33 30  W43AOH       20 44 54  47.3 226.1  2.0      38.3    -8   1 10  10000  00 33 30
00 36 00  ---          20 47 25  46.9 226.8  2.0      38.9   142   R  1   8000

00 36 00  TXS1843      20 47 25  47.9 228.9  2.0      40.4    -8   1 10   8000  00 36 00
00 38 30  ---          20 49 55  47.5 229.6  2.1      40.9   142   R  1   6000

00 38 30  W43AOH       20 49 55  46.5 227.5  2.0      39.4    -8   1 10   6000  00 38 30
00 41 00  ---          20 52 26  46.1 228.2  2.1      39.9   142   R  1   4000

00 41 00  TXS1843      20 52 26  47.1 230.3  2.1      41.4    -8   1 10   4000  00 41 00
00 43 30  ---          20 54 56  46.7 230.9  2.1      41.9   142   R  1   2000

00 43 30  W43AOH       20 54 56  45.7 228.9  2.1      40.4    -8   1 10   2000  00 43 30
00 46 00  ---          20 57 26  45.3 229.6  2.2      40.9   142   R  1      0

00 47 00  OT081        20 58 27  41.9 254.4  3.1      57.2    37   1  9      0  00 47 00
00 52 00  ---          21 03 27  40.8 255.3  3.2      57.6   300   F  2   4000

00 53 00  TXS1843      21 04 28  45.1 233.4  2.3      43.7    39   1  9   4000  00 53 00
00 55 00  ---          21 06 28  44.7 234.0  2.3      44.1   120   F  2   5600
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Nov 2003   Day 312 ---

00 55 00  TXS1843      21 06 28  44.7 234.0  2.3      44.1    -4   1  9   5600  00 55 00
00 57 30  ---          21 08 58  44.3 234.6  2.4      44.5   146   F  2   7600

00 57 30  W43AOH       21 08 58  43.4 232.6  2.4      43.1    -8   1  9   7600  00 57 30
01 00 00  ---          21 11 29  42.9 233.2  2.4      43.6   142   F  2   9600

01 00 00  TXS1843      21 11 29  43.9 235.2  2.4      45.0    -8   1  9   9600  01 00 00
01 02 30  ---          21 13 59  43.4 235.8  2.5      45.4   142   F  2  11600

01 02 30  W43AOH       21 13 59  42.5 233.8  2.4      44.0    -8   1  9  11600  01 02 30
01 05 00  ---          21 16 30  42.1 234.4  2.5      44.4   142   F  2  13600

01 05 00  TXS1843      21 16 30  43.0 236.4  2.5      45.8    -8   1  9  13600  01 05 00
01 07 30  ---          21 19 00  42.5 237.0  2.5      46.2   142   F  2  15600

01 07 30  W43AOH       21 19 00  41.6 235.0  2.5      44.8    -8   1  9  15600  01 07 30
01 10 00  ---          21 21 30  41.2 235.6  2.6      45.3   142   F  2  17600

01 11 00  TXS1843      21 22 31  41.9 237.8  2.6      46.7    53   1 10  17600  01 11 00
01 13 00  ---          21 24 31  41.5 238.3  2.6      47.1   120   R  2  16000

01 13 00  TXS1843      21 24 31  41.5 238.3  2.6      47.1    -4   1 10  16000  01 13 00
01 15 30  ---          21 27 01  41.1 238.9  2.7      47.4   146   R  2  14000

01 15 30  W43AOH       21 27 01  40.2 236.9  2.7      46.1    -8   1 10  14000  01 15 30
01 18 00  ---          21 29 32  39.7 237.4  2.7      46.5   142   R  2  12000

01 18 00  TXS1843      21 29 32  40.6 239.4  2.7      47.8    -8   1 10  12000  01 18 00
01 20 30  ---          21 32 02  40.1 240.0  2.8      48.1   142   R  2  10000

01 20 30  W43AOH       21 32 02  39.3 238.0  2.7      46.9    -8   1 10  10000  01 20 30
01 23 00  ---          21 34 33  38.8 238.5  2.8      47.2   142   R  2   8000

01 23 00  TXS1843      21 34 33  39.7 240.5  2.8      48.5    -8   1 10   8000  01 23 00
01 25 30  ---          21 37 03  39.2 241.0  2.8      48.8   142   R  2   6000

01 25 30  W43AOH       21 37 03  38.4 239.1  2.8      47.6    -8   1 10   6000  01 25 30
01 28 00  ---          21 39 33  37.9 239.6  2.9      47.9   142   R  2   4000

01 28 00  TXS1843      21 39 33  38.7 241.6  2.9      49.2    -8   1 10   4000  01 28 00
01 30 30  ---          21 42 04  38.2 242.1  2.9      49.5   142   R  2   2000

01 30 30  W43AOH       21 42 04  37.4 240.1  2.9      48.3    -8   1 10   2000  01 30 30
01 33 00  ---          21 44 34  37.0 240.7  2.9      48.6   142   R  2      0
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Nov 2003   Day 312 ---

01 34 00  OT081        21 45 34  31.9 262.0  3.9      59.8    40   1 11      0  01 34 00
01 39 00  ---          21 50 35  30.9 262.7  4.0      60.0   300   F  1   4000

01 40 00  TXS1843      21 51 35  36.4 244.0  3.1      50.7    42   1 11   4000  01 40 00
01 42 00  ---          21 53 36  36.0 244.4  3.1      50.9   120   F  1   5600

01 42 00  TXS1843      21 53 36  36.0 244.4  3.1      50.9    -4   1 11   5600  01 42 00
01 44 30  ---          21 56 06  35.5 244.9  3.2      51.2   146   F  1   7600

01 44 30  W43AOH       21 56 06  34.8 243.0  3.1      50.1    -7   1 11   7600  01 44 30
01 47 00  ---          21 58 36  34.3 243.5  3.2      50.4   143   F  1   9600

01 47 00  TXS1843      21 58 36  35.0 245.4  3.2      51.5    -7   1 11   9600  01 47 00
01 49 30  ---          22 01 07  34.6 245.8  3.2      51.7   143   F  1  11600

01 49 30  W43AOH       22 01 07  33.8 243.9  3.2      50.7    -7   1 11  11600  01 49 30
01 52 00  ---          22 03 37  33.3 244.4  3.3      50.9   143   F  1  13600

01 52 00  TXS1843      22 03 37  34.1 246.3  3.3      52.0    -7   1 11  13600  01 52 00
01 54 30  ---          22 06 08  33.6 246.8  3.3      52.3   143   F  1  15600

01 54 30  W43AOH       22 06 08  32.8 244.9  3.3      51.2    -7   1 11  15600  01 54 30
01 57 00  ---          22 08 38  32.3 245.4  3.3      51.5   143   F  1  17600

01 57 00  W43AOH       22 08 38  32.3 245.4  3.3      51.5    -4   1 12  17600  01 57 00
02 05 00  ---          22 16 39  30.8 246.8  3.5      52.3   476   R  1  11200

02 06 00  OT081        22 17 40  25.1 266.4  4.4      60.6    41   1 12  11200  02 06 00
02 13 00  ---          22 24 41  23.6 267.4  4.5      60.7   420   R  1   5600

02 15 00  2145+067     22 26 41  64.7 202.8  0.6      19.6    32   1 12   5600  02 15 00
02 22 00  ---          22 33 42  64.1 206.5  0.8      22.8   420   R  1      0

02 24 00  TXS1843      22 35 43  27.6 251.9  3.8      54.9    41   1 11      0  02 24 00
02 26 00  ---          22 37 43  27.2 252.2  3.9      55.0   120   F  2   1600

02 26 00  TXS1843      22 37 43  27.2 252.2  3.9      55.0    -4   1 11   1600  02 26 00
02 28 30  ---          22 40 13  26.7 252.6  3.9      55.2   146   F  2   3600

02 28 30  W43AOH       22 40 13  26.0 250.8  3.9      54.4    -7   1 11   3600  02 28 30
02 31 00  ---          22 42 44  25.5 251.2  3.9      54.6   143   F  2   5600

02 31 00  TXS1843      22 42 44  26.2 253.0  3.9      55.4    -7   1 11   5600  02 31 00
02 33 30  ---          22 45 14  25.7 253.4  4.0      55.5   143   F  2   7600
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Nov 2003   Day 312 ---

02 33 30  W43AOH       22 45 14  25.0 251.6  4.0      54.8    -7   1 11   7600  02 33 30
02 36 00  ---          22 47 45  24.5 252.0  4.0      55.0   143   F  2   9600

02 36 00  TXS1843      22 47 45  25.1 253.8  4.0      55.7    -7   1 11   9600  02 36 00
02 38 30  ---          22 50 15  24.6 254.2  4.1      55.9   143   F  2  11600

02 38 30  W43AOH       22 50 15  24.0 252.4  4.0      55.1    -7   1 11  11600  02 38 30
02 41 00  ---          22 52 45  23.5 252.8  4.1      55.3   143   F  2  13600

02 41 00  TXS1843      22 52 45  24.1 254.6  4.1      56.0    -7   1 11  13600  02 41 00
02 43 30  ---          22 55 16  23.6 254.9  4.2      56.2   143   F  2  15600

02 43 30  W43AOH       22 55 16  23.0 253.2  4.1      55.5    -7   1 11  15600  02 43 30
02 46 00  ---          22 57 46  22.4 253.6  4.2      55.7   143   F  2  17600

02 47 00  TXS1843      22 58 46  22.9 255.5  4.2      56.4    53   1 12  17600  02 47 00
02 49 00  ---          23 00 47  22.4 255.8  4.2      56.5   120   R  2  16000

02 49 00  TXS1843      23 00 47  22.4 255.8  4.2      56.5    -4   1 12  16000  02 49 00
02 51 30  ---          23 03 17  21.9 256.1  4.3      56.7   146   R  2  14000

02 51 30  W43AOH       23 03 17  21.3 254.4  4.3      56.0    -7   1 12  14000  02 51 30
02 54 00  ---          23 05 48  20.8 254.8  4.3      56.2   143   R  2  12000

02 54 00  TXS1843      23 05 48  21.4 256.5  4.3      56.8    -7   1 12  12000  02 54 00
02 56 30  ---          23 08 18  20.9 256.9  4.4      56.9   143   R  2  10000

02 56 30  W43AOH       23 08 18  20.3 255.1  4.3      56.3    -7   1 12  10000  02 56 30
02 59 00  ---          23 10 48  19.7 255.5  4.4      56.5   143   R  2   8000

02 59 00  TXS1843      23 10 48  20.3 257.2  4.4      57.1    -7   1 12   8000  02 59 00
03 01 30  ---          23 13 19  19.8 257.6  4.5      57.2   143   R  2   6000

03 01 30  W43AOH       23 13 19  19.2 255.9  4.4      56.6    -7   1 12   6000  03 01 30
03 04 00  ---          23 15 49  18.7 256.2  4.5      56.7   143   R  2   4000

03 06 00  2145+067     23 17 49  58.4 226.2  1.5      38.7    35   1 12   4000  03 06 00
03 11 00  ---          23 22 50  57.6 228.0  1.6      40.1   300   R  2      0

03 12 00  W43AOH       23 23 50  17.0 257.4  4.6      57.1   -27   1 13      0  03 12 00
03 23 00  ---          23 34 52  14.7 258.9  4.8      57.7   633   F  1   8800

03 23 00  W43AOH       23 34 52  14.7 258.9  4.8      57.7    -4   1 13   8800  03 23 00
03 34 00  ---          23 45 54  12.4 260.4  5.0      58.1   656   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Nov 2003   Day 312 ---

03 35 00  W43AOH       23 46 54  12.2 260.6  5.0      58.1    54   1 14  17600  03 35 00
03 46 00  ---          23 57 56   9.8 262.0  5.2      58.5   660   R  1   8800

03 46 00  W43AOH       23 57 56   9.8 262.0  5.2      58.5    -4   1 14   8800  03 46 00
03 52 00  ---          00 03 57   8.5 262.8  5.3      58.7   356   R  1   4000

03 54 00  2145+067     00 05 57  50.0 240.9  2.3      49.2    31   1 14   4000  03 54 00
03 59 00  ---          00 10 58  49.1 242.1  2.4      50.0   300   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gw43a-oh.set
   Matches group v20cm_2 in /home/imai/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    1         Station: VLBA              Total bit rate:  128
   Format: VLBA1:1           Bits per sample: 2         Sample rate:  8.000
   Number of channels:  8    Passes/head pos:   2       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

  Frequency Set:   8  Based on FREQ, BW, and/or DOPPLER in schedule.  Used pcal sets:   1
   LO sum=    1611.76   1611.76   1614.02   1614.02   1618.02   1618.02   1622.02   1622.02
   BBC fr=     788.24    788.24    785.98    785.98    781.98    781.98    777.98    777.98
   Bandwd=      0.500     0.500     4.000     4.000     4.000     4.000     4.000     4.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = OFF 
    PCALXB1=   S1    S2    S3    S4    S5    S6    S7    S8 
    PCALXB2=   M1    M2    M3    M4    M5    M6    M7    M8 
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0

   Track assignments are: 
    track1=   2,  6, 10, 14, 18, 22, 26, 30
    track2=   3,  7, 11, 15, 19, 23, 27, 31
    barrel=roll_off 
 SOURCE LIST -- GI100: 1612 MHz OH masers in W43A (H. Imai & P.J. Diamond)
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

   J1751+0939        17 49 10.387930   * 17 51 32.818573     17 51 41.925822 
   1749+096          09 39 42.82582    * 09 39 00.72837      09 39 00.03070 
   J1751+09          From catalog imbedded in main SCHED input file.
 * OT081             USNO - Ref Frame 1998-6, Eubanks June 1998
                     Doppler based on other sources.

   J1832+1357        18 30 26.112214   * 18 32 43.471123     18 32 52.356879 
 * 1830+139          13 55 26.71680    * 13 57 44.40030      13 57 57.99375 
                     From catalog imbedded in main SCHED input file.
                     Doppler based on other sources.

   J2148+0657        21 45 36.078481   * 21 48 05.458679     21 48 16.254800 
 * 2145+067          06 43 40.90462    * 06 57 38.60422      06 58 43.32894 
   J2148+06          From catalog imbedded in main SCHED input file.
                     ICRF - Ext.1 Source - 1998 IERS Annual Report
                     Doppler based on other sources.

 * W43AOH            18 45 05.339856   * 18 47 41.163000     18 47 51.471400 
                    -01 48 32.70202    *-01 45 11.22000     -01 44 56.98528 
                     From catalog imbedded in main SCHED input file.
                     Doppler based on LSR frame and radio definition.  Velocities:
                         35.00    35.00    35.00    35.00    35.00    35.00    35.00    35.00


 * TXS1843           18 43 30.011769   * 18 46 03.900000     18 46 14.061318 
   TXS1843-001      -00 06 52.60264    *-00 03 38.00000     -00 03 23.79023 
                     From catalog imbedded in main SCHED input file.
                     Doppler based on other sources.

 * 1851+005          18 49 13.574417   * 18 51 46.723100     18 51 56.857347 
   J1851+0035        00 31 53.27360    * 00 35 32.34800      00 35 48.51155 
                     From catalog imbedded in main SCHED input file.
                     Doppler based on other sources.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   OT081               51.9
   1830+139            62.8
   2145+067           105.9
   W43AOH              60.3
   TXS1843             60.4
   1851+005            62.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

