  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: RadioAstron visibility tracking of H2O maser spots
 Exp. Code:  ga042   


Schedule Version:       1.10
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Alexey Alakoz & Hiroshi Imai

Address:  ASC Lebedev
          Profsoyuznaya 84/32
          117997 Moscow, Russia
 

Phone:    +79165452842
EMAIL:    alexey.alakoz@gmail.com
Fax:      +74953332378
Phone during observation: +79165452842

Observing mode: K-band dual-pol

Notes:    K-band, Radioastron-compatible frequency setup
          P-CAL is OFF
          Tsys is ON
          auto-level (AGC) is ON

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

 ---------- K-band VLBI scans. Space segment 01: target source W3IRS5 ----------

 Next scan frequencies:  22228.00  22228.00  22228.00  22228.00
 Next BBC frequencies:     728.00    728.00    728.00    728.00
 Next scan bandwidths:      16.00     16.00     16.00     16.00

11 00 00  W3IRS5_H2O   10 39 35  13.4 -23.7  8.2      47.8     0        0   11 00 00
11 21 20  ---          11 00 59  11.6 -21.9  8.6      43.5  1280       41   11 00 01

11 21 50  W3IRS5_H2O   11 01 29  11.6 -21.9  8.6      43.4    24       41   11 21 50
11 43 10  ---          11 22 52   9.9 -19.9  8.9      39.0  1280       82   11 21 51

11 43 40  W3IRS5_H2O   11 23 22   9.9 -19.9  8.9      38.9    24       82   11 43 40
12 05 00  ---          11 44 46   8.4 -17.9  9.3      34.5  1280      124   11 43 41

 ---------- K-band VLBI scans. Ground segment 02 : Delay/D-term cal. NRAO150 scan 1 ----------

12 06 00  NRAO150      11 45 46   9.0 -34.9  7.7      51.4    40      124   12 06 00
12 20 00  ---          11 59 48   7.3 -33.4  8.0      48.9   840      151   12 06 01

 ---------- K-band VLBI scans. Space segment 02: space-ground FF source 0716+714 ----------

12 22 00  0716+714     12 01 49  35.4 -21.6  4.6      98.7    57      151   12 22 00
12 35 00  ---          12 14 51  34.4 -21.8  4.8      95.5   780      176   12 22 01

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 ----------

12 37 00  0241+622     12 16 51   7.9 -16.4  9.5      31.8    60      176   12 37 00
12 38 00  ---          12 17 51   7.8 -16.3  9.5      31.6    60      178   12 37 01

12 38 00  W3IRS5_H2O   12 17 51   6.4 -14.5  9.8      27.6   -11      178   12 38 11
12 39 00  ---          12 18 51   6.3 -14.4  9.9      27.4    49      179   12 38 01

12 39 00  0241+622     12 18 51   7.8 -16.2  9.5      31.4   -11      179   12 39 11
12 40 00  ---          12 19 52   7.7 -16.1  9.6      31.2    49      181   12 39 01

12 40 00  W3IRS5_H2O   12 19 52   6.3 -14.3  9.9      27.2   -11      181   12 40 11
12 41 00  ---          12 20 52   6.2 -14.2  9.9      26.9    49      183   12 40 01

12 41 00  0241+622     12 20 52   7.6 -16.0  9.6      31.0   -11      183   12 41 11
12 42 00  ---          12 21 52   7.6 -15.9  9.6      30.8    49      184   12 41 01

12 42 00  W3IRS5_H2O   12 21 52   6.2 -14.1  9.9      26.7   -11      184   12 42 11
12 43 00  ---          12 22 52   6.1 -14.0  9.9      26.5    49      186   12 42 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

12 43 00  0241+622     12 22 52   7.5 -15.8  9.6      30.6   -11      186   12 43 11
12 44 00  ---          12 23 52   7.5 -15.7  9.6      30.4    49      187   12 43 01

12 44 00  W3IRS5_H2O   12 23 52   6.1 -13.9  9.9      26.3   -11      187   12 44 11
12 45 00  ---          12 24 52   6.0 -13.8 10.0      26.1    49      189   12 44 01

12 45 00  0241+622     12 24 52   7.4 -15.6  9.6      30.2   -11      189   12 45 11
12 46 00  ---          12 25 52   7.3 -15.5  9.7      30.0    49      190   12 45 01

12 46 00  W3IRS5_H2O   12 25 52   6.0 -13.7 10.0      25.9   -11      190   12 46 11
12 47 00  ---          12 26 53   5.9 -13.6 10.0      25.7    49      192   12 46 01

12 47 30  0241+622     12 27 23   7.3 -15.4  9.7      29.7    19      192   12 47 30
12 48 00  ---          12 27 53   7.2 -15.3  9.7      29.5    30      193   12 47 31

12 48 00  W3IRS5_H2O   12 27 53   5.9 -13.5 10.0      25.5   -11      193   12 48 11
12 49 00  ---          12 28 53   5.8 -13.4 10.0      25.3    49      195   12 48 01

12 49 00  0241+622     12 28 53   7.2 -15.2  9.7      29.3   -11      195   12 49 11
12 50 00  ---          12 29 53   7.1 -15.1  9.7      29.1    49      196   12 49 01

12 50 00  W3IRS5_H2O   12 29 53   5.8 -13.3 10.0      25.0   -11      196   12 50 11
12 51 00  ---          12 30 53   5.7 -13.2 10.1      24.8    49      198   12 50 01

12 51 00  0241+622     12 30 53   7.1 -15.0  9.7      28.9   -11      198   12 51 11
12 52 00  ---          12 31 53   7.0 -14.9  9.8      28.7    49      199   12 51 01

12 52 00  W3IRS5_H2O   12 31 53   5.7 -13.1 10.1      24.6   -11      199   12 52 11
12 53 00  ---          12 32 54   5.6 -13.0 10.1      24.4    49      201   12 52 01

12 53 00  0241+622     12 32 54   7.0 -14.8  9.8      28.5   -11      201   12 53 11
12 54 00  ---          12 33 54   6.9 -14.7  9.8      28.3    49      202   12 53 01

12 54 00  W3IRS5_H2O   12 33 54   5.6 -12.8 10.1      24.2   -11      202   12 54 11
12 55 00  ---          12 34 54   5.5 -12.7 10.1      24.0    49      204   12 54 01

12 55 00  0241+622     12 34 54   6.8 -14.6  9.8      28.1   -11      204   12 55 11
12 56 00  ---          12 35 54   6.8 -14.5  9.8      27.9    49      206   12 55 01

12 56 00  W3IRS5_H2O   12 35 54   5.5 -12.6 10.1      23.8   -11      206   12 56 11
12 57 00  ---          12 36 54   5.4 -12.5 10.2      23.6    49      207   12 56 01

12 57 30  0241+622     12 37 24   6.7 -14.3  9.8      27.6    19      207   12 57 30
12 58 00  ---          12 37 54   6.7 -14.3  9.9      27.4    30      208   12 57 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

12 58 00  W3IRS5_H2O   12 37 54   5.4 -12.4 10.2      23.4   -11      208   12 58 11
12 59 00  ---          12 38 55   5.3 -12.3 10.2      23.1    49      210   12 58 01

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 in parallel to GBT/Eff pointing scan ----------

13 00 00  0241+622     12 39 55   6.6 -14.1  9.9      27.0    49      210   13 00 00
13 01 00  ---          12 40 55   6.5 -14.0  9.9      26.8    60      212   13 00 01

13 01 00  W3IRS5_H2O   12 40 55   5.3 -12.1 10.2      22.7   -11      212   13 01 11
13 02 00  ---          12 41 55   5.2 -12.0 10.2      22.5    49      213   13 01 01

13 02 00  0241+622     12 41 55   6.5 -13.9  9.9      26.6   -11      213   13 02 11
13 03 00  ---          12 42 55   6.4 -13.8  9.9      26.4    49      215   13 02 01

13 03 00  W3IRS5_H2O   12 42 55   5.2 -11.9 10.3      22.3   -11      215   13 03 11
13 04 00  ---          12 43 55   5.1 -11.8 10.3      22.1    49      216   13 03 01

13 04 00  0241+622     12 43 55   6.4 -13.7 10.0      26.2   -10      216   13 04 10
13 05 00  ---          12 44 56   6.3 -13.6 10.0      26.0    50      218   13 04 01

13 05 00  W3IRS5_H2O   12 44 56   5.1 -11.7 10.3      21.9   -10      218   13 05 10
13 06 00  ---          12 45 56   5.0 -11.5 10.3      21.7    50      220   13 05 01

13 06 00  0241+622     12 45 56   6.3 -13.5 10.0      25.8   -10      220   13 06 10
13 07 00  ---          12 46 56   6.2 -13.4 10.0      25.5    50      221   13 06 01

13 07 00  W3IRS5_H2O   12 46 56   5.0 -11.4 10.3  H   21.5   -10      221   13 07 10
13 08 00  ---          12 47 56   4.9 -11.3 10.3  H   21.2     0      223   13 07 01

13 08 00  0241+622     12 47 56   6.2 -13.3 10.0      25.3   -10      223   13 08 10
13 09 00  ---          12 48 56   6.1 -13.1 10.0      25.1    50      224   13 08 01

13 09 00  W3IRS5_H2O   12 48 56   4.9 -11.2 10.4  H   21.0   -10      224   13 09 10
13 10 00  ---          12 49 56   4.9 -11.1 10.4  H   20.8     0      226   13 09 01

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 ----------

13 20 00  0241+622     12 59 58   5.6 -12.0 10.2      22.8   590      226   13 20 00
13 21 00  ---          13 00 58   5.6 -11.9 10.2      22.6    60      228   13 20 01

13 21 00  W3IRS5_H2O   13 00 58   4.4  -9.9 10.6  H   18.5   -10      228   13 21 10
13 22 00  ---          13 01 58   4.4  -9.8 10.6  H   18.3     0      230   13 21 01

13 22 30  0241+622     13 02 28   5.5 -11.7 10.3      22.3    20      230   13 22 30
13 23 00  ---          13 02 59   5.5 -11.7 10.3      22.2    30      231   13 22 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

13 23 00  W3IRS5_H2O   13 02 59   4.4  -9.7 10.6  H   18.0   -10      231   13 23 10
13 24 00  ---          13 03 59   4.3  -9.6 10.6  H   17.8     0      232   13 23 01

13 24 00  0241+622     13 03 59   5.4 -11.6 10.3      22.0   -10      232   13 24 10
13 25 00  ---          13 04 59   5.4 -11.4 10.3      21.7    50      234   13 24 01

13 25 00  W3IRS5_H2O   13 04 59   4.3  -9.4 10.6  H   17.6   -10      234   13 25 10
13 26 00  ---          13 05 59   4.3  -9.3 10.6  H   17.4     0      235   13 25 01

13 26 00  0241+622     13 05 59   5.3 -11.3 10.3      21.5   -10      235   13 26 10
13 27 00  ---          13 06 59   5.3 -11.2 10.3      21.3    50      237   13 26 01

13 27 00  W3IRS5_H2O   13 06 59   4.2  -9.2 10.7  H   17.2   -10      237   13 27 10
13 28 00  ---          13 07 59   4.2  -9.1 10.7  H   17.0     0      239   13 27 01

13 28 00  0241+622     13 07 59   5.3 -11.1 10.4      21.1   -10      239   13 28 10
13 29 00  ---          13 09 00   5.2 -11.0 10.4      20.9    50      240   13 28 01

13 29 00  W3IRS5_H2O   13 09 00   4.1  -9.0 10.7  H   16.8   -10      240   13 29 10
13 30 00  ---          13 10 00   4.1  -8.9 10.7  H   16.6     0      242   13 29 01

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. VLBA+GB scans on W3IRS5 ----------

13 43 00  0241+622     13 23 02   4.7  -9.5 10.6  H   17.9   770      242   13 43 00
13 44 00  ---          13 24 02   4.6  -9.4 10.6  H   17.7     0      244   13 43 01

13 44 00  W3IRS5_H2O   13 24 02   3.7  -7.3 10.9  H   13.6   -10      244   13 44 10
13 45 00  ---          13 25 02   3.7  -7.2 11.0  H   13.3     0      245   13 44 01

13 45 30  0241+622     13 25 32   4.6  -9.2 10.7  H   17.4    20      245   13 45 30
13 46 30  ---          13 26 32   4.6  -9.1 10.7  H   17.2     0      247   13 45 31

13 46 30  W3IRS5_H2O   13 26 32   3.6  -7.0 11.0  H   13.0   -10      247   13 46 40
13 47 30  ---          13 27 33   3.6  -6.9 11.0  H   12.8     0      249   13 46 31

13 48 00  0241+622     13 28 03   4.5  -8.9 10.7  H   16.8    20      249   13 48 00
13 49 00  ---          13 29 03   4.5  -8.8 10.7  H   16.6     0      251   13 48 01

13 49 00  W3IRS5_H2O   13 29 03   3.6  -6.7 11.0  H   12.5   -10      251   13 49 10
13 50 00  ---          13 30 03   3.5  -6.6 11.0  H   12.3     0      252   13 49 01

13 50 30  0241+622     13 30 33   4.4  -8.7 10.7  H   16.3    20      252   13 50 30
13 51 30  ---          13 31 33   4.4  -8.5 10.8  H   16.1     0      254   13 50 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

13 51 30  W3IRS5_H2O   13 31 33   3.5  -6.4 11.1  H   11.9   -10      254   13 51 40
13 52 30  ---          13 32 33   3.5  -6.3 11.1  H   11.7     0      256   13 51 31

13 53 00  0241+622     13 33 03   4.3  -8.4 10.8  H   15.8    20      256   13 53 00
13 54 00  ---          13 34 04   4.3  -8.3 10.8  H   15.6     0      258   13 53 01

13 54 00  W3IRS5_H2O   13 34 04   3.4  -6.2 11.1  H   11.4   -10      258   13 54 10
13 55 00  ---          13 35 04   3.4  -6.0 11.1  H   11.2     0      260   13 54 01

 ---------- K-band VLBI scans. Ground segment 02 :  scans on W3IRS5 ----------

14 24 00  0241+622     14 04 09   3.6  -4.9 11.3  H    9.1  1730      260   14 24 00
14 25 00  ---          14 05 09   3.6  -4.8 11.3  H    8.9     0      261   14 24 01

14 25 00  W3IRS5_H2O   14 05 09   2.9  -2.6 11.6  H    4.7    -9      261   14 25 09
14 26 00  ---          14 06 09   2.9  -2.4 11.7  H    4.5     0      263   14 25 01

14 26 30  0241+622     14 06 39   3.5  -4.6 11.3  H    8.6    21      263   14 26 30
14 27 00  ---          14 07 09   3.5  -4.5 11.3  H    8.5     0      264   14 26 31

14 27 00  W3IRS5_H2O   14 07 09   2.9  -2.3 11.7  H    4.3    -9      264   14 27 09
14 28 00  ---          14 08 09   2.9  -2.2 11.7  H    4.1     0      266   14 27 01

14 28 00  0241+622     14 08 09   3.5  -4.4 11.4  H    8.3    -9      266   14 28 09
14 29 00  ---          14 09 09   3.5  -4.3 11.4  H    8.0     0      267   14 28 01

14 29 00  W3IRS5_H2O   14 09 09   2.9  -2.1 11.7  H    3.9    -9      267   14 29 09
14 30 00  ---          14 10 10   2.9  -2.0 11.7  H    3.7     0      269   14 29 01

14 30 00  0241+622     14 10 10   3.5  -4.2 11.4  H    7.8    -9      269   14 30 09
14 31 00  ---          14 11 10   3.5  -4.1 11.4  H    7.6     0      271   14 30 01

14 31 00  W3IRS5_H2O   14 11 10   2.9  -1.9 11.7  H    3.4    -9      271   14 31 09
14 32 00  ---          14 12 10   2.9  -1.7 11.8  H    3.2     0      272   14 31 01

14 32 00  0241+622     14 12 10   3.4  -4.0 11.4  H    7.4    -9      272   14 32 09
14 33 00  ---          14 13 10   3.4  -3.8 11.4  H    7.2     0      274   14 32 01

14 33 00  W3IRS5_H2O   14 13 10   2.9  -1.6 11.8  H    3.0    -9      274   14 33 09
14 34 00  ---          14 14 10   2.9  -1.5 11.8  H    2.8     0      276   14 33 01

 ----------  Ground-only scan on 0716+714 ----------

16 50 00  0716+714     16 30 33  16.4 -13.3  9.1      38.0  8108      276   16 50 00
16 58 00  ---          16 38 34  16.0 -12.7  9.2      36.3   480      291   16 50 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 in parallel to GBT/Eff pointing scan ----------

17 00 00  0241+622     16 40 34   6.0  12.8-10.1     -24.4    92      291   17 00 00
17 01 00  ---          16 41 34   6.0  12.9-10.1     -24.6    60      293   17 00 01

17 01 00  W3IRS5_H2O   16 41 34   6.7  15.1 -9.8     -28.7    -9      293   17 01 09
17 02 00  ---          16 42 35   6.7  15.2 -9.7     -28.9    51      295   17 01 01

17 02 30  0241+622     16 43 05   6.1  13.0-10.1     -24.9    21      295   17 02 30
17 03 00  ---          16 43 35   6.1  13.1-10.0     -25.0    30      296   17 02 31

17 03 00  W3IRS5_H2O   16 43 35   6.8  15.3 -9.7     -29.1    -9      296   17 03 09
17 04 00  ---          16 44 35   6.8  15.4 -9.7     -29.3    51      297   17 03 01

17 04 00  0241+622     16 44 35   6.1  13.2-10.0     -25.2    -9      297   17 04 09
17 05 00  ---          16 45 35   6.2  13.3-10.0     -25.5    51      299   17 04 01

17 05 00  W3IRS5_H2O   16 45 35   6.9  15.5 -9.7     -29.5    -9      299   17 05 09
17 06 00  ---          16 46 35   7.0  15.6 -9.7     -29.7    51      300   17 05 01

17 06 00  0241+622     16 46 35   6.2  13.4-10.0     -25.7    -9      300   17 06 09
17 07 00  ---          16 47 35   6.3  13.5-10.0     -25.9    51      302   17 06 01

17 07 00  W3IRS5_H2O   16 47 35   7.0  15.7 -9.7     -29.9    -9      302   17 07 09
17 08 00  ---          16 48 36   7.1  15.8 -9.6     -30.1    51      304   17 07 01

17 08 00  0241+622     16 48 36   6.3  13.6-10.0     -26.1    -9      304   17 08 09
17 09 00  ---          16 49 36   6.4  13.7 -9.9     -26.3    51      305   17 08 01

17 09 00  W3IRS5_H2O   16 49 36   7.1  15.9 -9.6     -30.3    -9      305   17 09 09
17 10 00  ---          16 50 36   7.2  16.0 -9.6     -30.5    51      307   17 09 01

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 +GBT/EFLSBERG ----------

17 10 30  0241+622     16 51 06   6.5  13.9 -9.9     -26.6    21      307   17 10 30
17 11 30  ---          16 52 06   6.5  14.0 -9.9     -26.8    60      309   17 10 31

17 11 30  W3IRS5_H2O   16 52 06   7.3  16.1 -9.6     -30.9   -10      309   17 11 40
17 12 30  ---          16 53 06   7.3  16.2 -9.6     -31.1    50      311   17 11 31

17 12 30  0241+622     16 53 06   6.6  14.1 -9.9     -27.0   -10      311   17 12 40
17 13 30  ---          16 54 06   6.6  14.2 -9.9     -27.2    50      312   17 12 31

17 13 30  W3IRS5_H2O   16 54 06   7.4  16.3 -9.6     -31.3   -10      312   17 13 40
17 14 30  ---          16 55 07   7.5  16.4 -9.5     -31.5    50      314   17 13 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

17 14 30  0241+622     16 55 07   6.7  14.3 -9.9     -27.5   -10      314   17 14 40
17 15 30  ---          16 56 07   6.7  14.4 -9.8     -27.7    50      315   17 14 31

17 15 30  W3IRS5_H2O   16 56 07   7.5  16.6 -9.5     -31.7   -10      315   17 15 40
17 16 30  ---          16 57 07   7.6  16.7 -9.5     -31.9    50      317   17 15 31

17 16 30  0241+622     16 57 07   6.8  14.5 -9.8     -27.9   -10      317   17 16 40
17 17 30  ---          16 58 07   6.8  14.6 -9.8     -28.1    50      319   17 16 31

17 17 30  W3IRS5_H2O   16 58 07   7.7  16.8 -9.5     -32.1   -10      319   17 17 40
17 18 30  ---          16 59 07   7.7  16.9 -9.5     -32.3    50      320   17 17 31

17 18 30  0241+622     16 59 07   6.9  14.7 -9.8     -28.3   -10      320   17 18 40
17 19 30  ---          17 00 07   7.0  14.8 -9.8     -28.5    50      322   17 18 31

17 19 30  W3IRS5_H2O   17 00 07   7.8  17.0 -9.5     -32.5   -10      322   17 19 40
17 20 30  ---          17 01 08   7.8  17.0 -9.4     -32.7    50      323   17 19 31

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 /all stations ----------

17 20 30  0241+622     17 01 08   7.0  14.9 -9.8     -28.7   -10      323   17 20 40
17 21 30  ---          17 02 08   7.1  15.0 -9.7     -28.9    50      325   17 20 31

17 21 30  W3IRS5_H2O   17 02 08   7.9  17.1 -9.4     -32.9   -10      325   17 21 40
17 22 30  ---          17 03 08   8.0  17.2 -9.4     -33.1    50      327   17 21 31

17 23 00  0241+622     17 03 38   7.2  15.2 -9.7     -29.2    20      327   17 23 00
17 23 30  ---          17 04 08   7.2  15.2 -9.7     -29.3    30      328   17 23 01

17 23 30  W3IRS5_H2O   17 04 08   8.0  17.3 -9.4     -33.4   -10      328   17 23 40
17 24 30  ---          17 05 08   8.1  17.4 -9.4     -33.6    50      329   17 23 31

17 24 30  0241+622     17 05 08   7.2  15.3 -9.7     -29.6   -10      329   17 24 40
17 25 30  ---          17 06 08   7.3  15.4 -9.7     -29.8    50      331   17 24 31

17 25 30  W3IRS5_H2O   17 06 08   8.2  17.5 -9.3     -33.8   -10      331   17 25 40
17 26 30  ---          17 07 09   8.2  17.6 -9.3     -34.0    50      332   17 25 31

17 26 30  0241+622     17 07 09   7.4  15.5 -9.7     -30.0   -10      332   17 26 40
17 27 30  ---          17 08 09   7.4  15.6 -9.6     -30.2    50      334   17 26 31

17 27 30  W3IRS5_H2O   17 08 09   8.3  17.7 -9.3     -34.2   -10      334   17 27 40
17 28 30  ---          17 09 09   8.4  17.8 -9.3     -34.4    50      336   17 27 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

17 28 30  0241+622     17 09 09   7.5  15.7 -9.6     -30.4   -10      336   17 28 40
17 29 30  ---          17 10 09   7.5  15.8 -9.6     -30.6    50      337   17 28 31

17 29 30  W3IRS5_H2O   17 10 09   8.4  17.9 -9.3     -34.6   -10      337   17 29 40
17 30 30  ---          17 11 09   8.5  18.0 -9.3     -34.8    50      339   17 29 31

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 /all stations ----------

17 31 00  0241+622     17 11 39   7.6  16.0 -9.6     -30.9    20      339   17 31 00
17 32 00  ---          17 12 39   7.7  16.1 -9.6     -31.1    60      341   17 31 01

17 32 00  W3IRS5_H2O   17 12 39   8.6  18.2 -9.2     -35.1   -10      341   17 32 10
17 33 00  ---          17 13 40   8.7  18.3 -9.2     -35.3    50      342   17 32 01

17 33 00  0241+622     17 13 40   7.7  16.2 -9.5     -31.3   -10      342   17 33 10
17 34 00  ---          17 14 40   7.8  16.3 -9.5     -31.5    50      344   17 33 01

17 34 00  W3IRS5_H2O   17 14 40   8.7  18.4 -9.2     -35.5   -10      344   17 34 10
17 35 00  ---          17 15 40   8.8  18.5 -9.2     -35.7    50      346   17 34 01

17 35 00  0241+622     17 15 40   7.9  16.4 -9.5     -31.8   -10      346   17 35 10
17 36 00  ---          17 16 40   7.9  16.5 -9.5     -32.0    50      347   17 35 01

17 36 00  W3IRS5_H2O   17 16 40   8.9  18.6 -9.2     -35.9   -10      347   17 36 10
17 37 00  ---          17 17 40   8.9  18.7 -9.2     -36.2    50      349   17 36 01

17 37 00  0241+622     17 17 40   8.0  16.6 -9.5     -32.2   -10      349   17 37 10
17 38 00  ---          17 18 40   8.0  16.7 -9.5     -32.4    50      351   17 37 01

17 38 00  W3IRS5_H2O   17 18 40   9.0  18.8 -9.1     -36.4   -10      351   17 38 10
17 39 00  ---          17 19 41   9.1  18.8 -9.1     -36.6    50      352   17 38 01

17 39 00  0241+622     17 19 41   8.1  16.8 -9.4     -32.6   -10      352   17 39 10
17 40 00  ---          17 20 41   8.2  16.9 -9.4     -32.8    50      354   17 39 01

17 40 00  W3IRS5_H2O   17 20 41   9.1  18.9 -9.1     -36.8   -10      354   17 40 10
17 41 00  ---          17 21 41   9.2  19.0 -9.1     -37.0    50      355   17 40 01

17 41 30  0241+622     17 22 11   8.3  17.0 -9.4     -33.1    20      355   17 41 30
17 42 00  ---          17 22 41   8.3  17.1 -9.4     -33.2    30      356   17 41 31

17 42 00  W3IRS5_H2O   17 22 41   9.3  19.1 -9.1     -37.2   -10      356   17 42 10
17 43 00  ---          17 23 41   9.4  19.2 -9.1     -37.4    50      358   17 42 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

17 43 00  0241+622     17 23 41   8.4  17.2 -9.4     -33.4   -10      358   17 43 10
17 44 00  ---          17 24 41   8.4  17.3 -9.4     -33.6    50      360   17 43 01

17 44 00  W3IRS5_H2O   17 24 41   9.4  19.3 -9.0     -37.6   -10      360   17 44 10
17 45 00  ---          17 25 42   9.5  19.4 -9.0     -37.8    50      361   17 44 01

17 45 00  0241+622     17 25 42   8.5  17.4 -9.3     -33.8   -10      361   17 45 10
17 46 00  ---          17 26 42   8.5  17.5 -9.3     -34.0    50      363   17 45 01

17 46 00  W3IRS5_H2O   17 26 42   9.6  19.5 -9.0     -38.0   -10      363   17 46 10
17 47 00  ---          17 27 42   9.6  19.6 -9.0     -38.2    50      364   17 46 01

17 47 00  0241+622     17 27 42   8.6  17.6 -9.3     -34.3   -10      364   17 47 10
17 48 00  ---          17 28 42   8.7  17.6 -9.3     -34.5    50      366   17 47 01

17 48 00  W3IRS5_H2O   17 28 42   9.7  19.7 -9.0     -38.4   -10      366   17 48 10
17 49 00  ---          17 29 42   9.8  19.8 -9.0     -38.6    50      368   17 48 01

 ---------- K-band VLBI scans. Space segment 03: target source W3IRS5 ----------

17 50 00  W3IRS5_H2O   17 30 42   9.9  19.9 -8.9     -38.8    54      368   17 50 00
18 12 15  ---          17 53 01  11.6  21.9 -8.6     -43.4  1335      411   17 50 01

18 12 45  W3IRS5_H2O   17 53 31  11.6  21.9 -8.6     -43.5    24      411   18 12 45
18 35 00  ---          18 15 50  13.5  23.8 -8.2     -48.0  1335      454   18 12 46

 ---------- K-band VLBI scans. Ground segment 02 : Phase-ref. scans on W3IRS5 /all stations ----------

18 37 00  0241+622     18 17 50  12.3  22.1 -8.5     -44.6   109      454   18 37 00
18 38 00  ---          18 18 50  12.4  22.2 -8.5     -44.8    60      456   18 37 01

18 38 00  W3IRS5_H2O   18 18 50  13.7  24.0 -8.1     -48.6   -11      456   18 38 11
18 39 00  ---          18 19 50  13.8  24.1 -8.1     -48.8    49      457   18 38 01

18 39 30  0241+622     18 20 21  12.5  22.3 -8.4     -45.1    19      457   18 39 30
18 40 00  ---          18 20 51  12.5  22.3 -8.4     -45.2    30      458   18 39 31

18 40 00  W3IRS5_H2O   18 20 51  13.9  24.2 -8.1     -49.0   -11      458   18 40 11
18 41 00  ---          18 21 51  14.0  24.3 -8.1     -49.2    49      460   18 40 01

18 41 00  0241+622     18 21 51  12.6  22.4 -8.4     -45.4   -11      460   18 41 11
18 42 00  ---          18 22 51  12.7  22.5 -8.4     -45.6    49      461   18 41 01

18 42 00  W3IRS5_H2O   18 22 51  14.1  24.3 -8.1     -49.4   -11      461   18 42 11
18 43 00  ---          18 23 51  14.2  24.4 -8.1     -49.7    49      463   18 42 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

18 43 00  0241+622     18 23 51  12.8  22.6 -8.4     -45.8   -11      463   18 43 11
18 44 00  ---          18 24 51  12.8  22.7 -8.4     -46.0    49      464   18 43 01

18 44 00  W3IRS5_H2O   18 24 51  14.3  24.5 -8.0     -49.9   -11      464   18 44 11
18 45 00  ---          18 25 51  14.4  24.6 -8.0     -50.1    49      466   18 44 01

18 45 00  0241+622     18 25 51  12.9  22.7 -8.3     -46.2   -11      466   18 45 11
18 46 00  ---          18 26 52  13.0  22.8 -8.3     -46.4    49      468   18 45 01

18 46 00  W3IRS5_H2O   18 26 52  14.4  24.6 -8.0     -50.3   -11      468   18 46 11
18 47 00  ---          18 27 52  14.5  24.7 -8.0     -50.5    49      469   18 46 01

18 47 00  0241+622     18 27 52  13.1  22.9 -8.3     -46.6   -11      469   18 47 11
18 48 00  ---          18 28 52  13.2  23.0 -8.3     -46.8    49      471   18 47 01

18 48 00  W3IRS5_H2O   18 28 52  14.6  24.8 -8.0     -50.7   -11      471   18 48 11
18 49 00  ---          18 29 52  14.7  24.9 -8.0     -50.9    49      472   18 48 01

 ---------- K-band VLBI scans. Space segment 04: space-ground observations  0716+714 ----------

18 52 00  0716+714     18 32 53  12.3  -4.2 11.1      11.3   151      472   18 52 00
19 05 00  ---          18 45 55  12.2  -3.1 11.4       8.4   780      497   18 52 01

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 in parallel to GBT/Eff pointing scan ----------

19 06 00  0241+622     18 46 55  14.7  24.4 -8.0     -50.5    33      497   19 06 00
19 07 00  ---          18 47 55  14.8  24.5 -8.0     -50.7    60      499   19 06 01

19 07 00  W3IRS5_H2O   18 47 55  16.4  26.2 -7.7     -54.5   -11      499   19 07 11
19 08 00  ---          18 48 55  16.5  26.3 -7.6     -54.7    49      501   19 07 01

19 08 30  0241+622     18 49 25  15.0  24.6 -8.0     -51.0    19      501   19 08 30
19 09 00  ---          18 49 55  15.0  24.6 -7.9     -51.1    30      502   19 08 31

19 09 00  W3IRS5_H2O   18 49 55  16.6  26.3 -7.6     -54.9   -11      502   19 09 11
19 10 00  ---          18 50 56  16.7  26.4 -7.6     -55.1    49      503   19 09 01

19 10 00  0241+622     18 50 56  15.1  24.7 -7.9     -51.3   -11      503   19 10 11
19 11 00  ---          18 51 56  15.2  24.8 -7.9     -51.5    49      505   19 10 01

19 11 00  W3IRS5_H2O   18 51 56  16.8  26.5 -7.6     -55.3   -11      505   19 11 11
19 12 00  ---          18 52 56  16.9  26.6 -7.6     -55.5    49      507   19 11 01

19 12 00  0241+622     18 52 56  15.3  24.9 -7.9     -51.7   -11      507   19 12 11
19 13 00  ---          18 53 56  15.4  24.9 -7.9     -51.9    49      508   19 12 01
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

19 13 00  W3IRS5_H2O   18 53 56  17.0  26.6 -7.6     -55.7   -11      508   19 13 11
19 14 00  ---          18 54 56  17.1  26.7 -7.5     -55.9    49      510   19 13 01

19 14 00  0241+622     18 54 56  15.5  25.0 -7.9     -52.1   -11      510   19 14 11
19 15 00  ---          18 55 56  15.6  25.1 -7.8     -52.3    49      511   19 14 01

19 15 00  W3IRS5_H2O   18 55 56  17.2  26.8 -7.5     -56.1   -11      511   19 15 11
19 16 00  ---          18 56 57  17.3  26.8 -7.5     -56.3    49      513   19 15 01

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 +GBT/EFLSBERG ----------

19 16 30  0241+622     18 57 27  15.7  25.2 -7.8     -52.6    19      513   19 16 30
19 17 30  ---          18 58 27  15.8  25.3 -7.8     -52.8    60      515   19 16 31

19 17 30  W3IRS5_H2O   18 58 27  17.4  26.9 -7.5     -56.6   -11      515   19 17 41
19 18 30  ---          18 59 27  17.5  27.0 -7.5     -56.8    49      516   19 17 31

19 19 00  0241+622     18 59 57  15.9  25.4 -7.8     -53.1    19      516   19 19 00
19 19 30  ---          19 00 27  16.0  25.4 -7.8     -53.2    30      517   19 19 01

19 19 30  W3IRS5_H2O   19 00 27  17.6  27.1 -7.4     -57.0   -11      517   19 19 41
19 20 30  ---          19 01 27  17.7  27.1 -7.4     -57.2    49      519   19 19 31

19 20 30  0241+622     19 01 27  16.1  25.5 -7.8     -53.4   -11      519   19 20 41
19 21 30  ---          19 02 27  16.2  25.6 -7.7     -53.6    49      521   19 20 31

19 21 30  W3IRS5_H2O   19 02 27  17.8  27.2 -7.4     -57.4   -11      521   19 21 41
19 22 30  ---          19 03 28  17.9  27.3 -7.4     -57.6    49      522   19 21 31

19 22 30  0241+622     19 03 28  16.3  25.6 -7.7     -53.8   -11      522   19 22 41
19 23 30  ---          19 04 28  16.3  25.7 -7.7     -54.0    49      524   19 22 31

19 23 30  W3IRS5_H2O   19 04 28  18.0  27.3 -7.4     -57.8   -11      524   19 23 41
19 24 30  ---          19 05 28  18.1  27.4 -7.4     -58.0    49      525   19 23 31

19 24 30  0241+622     19 05 28  16.4  25.8 -7.7     -54.2   -11      525   19 24 41
19 25 30  ---          19 06 28  16.5  25.8 -7.7     -54.4    49      527   19 24 31

19 25 30  W3IRS5_H2O   19 06 28  18.2  27.5 -7.3     -58.2   -11      527   19 25 41
19 26 30  ---          19 07 28  18.3  27.5 -7.3     -58.4    49      528   19 25 31

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 /all stations ----------

19 26 30  0241+622     19 07 28  16.6  25.9 -7.7     -54.6   -11      528   19 26 41
19 27 30  ---          19 08 28  16.7  26.0 -7.6     -54.8    49      530   19 26 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

19 27 30  W3IRS5_H2O   19 08 28  18.4  27.6 -7.3     -58.6   -11      530   19 27 41
19 28 30  ---          19 09 29  18.5  27.6 -7.3     -58.8    49      532   19 27 31

19 29 00  0241+622     19 09 59  16.9  26.1 -7.6     -55.1    19      532   19 29 00
19 29 30  ---          19 10 29  16.9  26.1 -7.6     -55.2    30      533   19 29 01

19 29 30  W3IRS5_H2O   19 10 29  18.6  27.7 -7.3     -59.0   -11      533   19 29 41
19 30 30  ---          19 11 29  18.7  27.8 -7.3     -59.2    49      534   19 29 31

19 30 30  0241+622     19 11 29  17.0  26.2 -7.6     -55.4   -11      534   19 30 41
19 31 30  ---          19 12 29  17.1  26.3 -7.6     -55.6    49      536   19 30 31

19 31 30  W3IRS5_H2O   19 12 29  18.8  27.8 -7.2     -59.4   -11      536   19 31 41
19 32 30  ---          19 13 29  18.9  27.9 -7.2     -59.6    49      537   19 31 31

19 32 30  0241+622     19 13 29  17.2  26.3 -7.5     -55.8   -11      537   19 32 41
19 33 30  ---          19 14 29  17.3  26.4 -7.5     -56.1    49      539   19 32 31

19 33 30  W3IRS5_H2O   19 14 29  19.0  28.0 -7.2     -59.8   -11      539   19 33 41
19 34 30  ---          19 15 30  19.1  28.0 -7.2     -60.0    49      540   19 33 31

19 34 30  0241+622     19 15 30  17.4  26.5 -7.5     -56.3   -11      540   19 34 41
19 35 30  ---          19 16 30  17.5  26.5 -7.5     -56.5    49      542   19 34 31

19 35 30  W3IRS5_H2O   19 16 30  19.2  28.1 -7.2     -60.2   -11      542   19 35 41
19 36 30  ---          19 17 30  19.3  28.1 -7.2     -60.4    49      544   19 35 31

19 37 00  0241+622     19 18 00  17.6  26.6 -7.5     -56.8    19      544   19 37 00
19 38 00  ---          19 19 00  17.7  26.7 -7.5     -57.0    60      546   19 37 01

19 38 00  W3IRS5_H2O   19 19 00  19.5  28.2 -7.1     -60.8   -11      546   19 38 11
19 39 00  ---          19 20 00  19.6  28.3 -7.1     -61.0    49      547   19 38 01

19 39 00  0241+622     19 20 00  17.8  26.8 -7.4     -57.2   -11      547   19 39 11
19 40 00  ---          19 21 01  17.9  26.8 -7.4     -57.4    49      549   19 39 01

19 40 00  W3IRS5_H2O   19 21 01  19.7  28.4 -7.1     -61.2   -11      549   19 40 11
19 41 00  ---          19 22 01  19.8  28.4 -7.1     -61.4    49      550   19 40 01

19 41 00  0241+622     19 22 01  18.0  26.9 -7.4     -57.6   -11      550   19 41 11
19 42 00  ---          19 23 01  18.1  26.9 -7.4     -57.8    49      552   19 41 01

19 42 00  W3IRS5_H2O   19 23 01  19.9  28.5 -7.1     -61.6   -11      552   19 42 11
19 43 00  ---          19 24 01  20.0  28.5 -7.1     -61.8    49      553   19 42 01
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

19 43 00  0241+622     19 24 01  18.2  27.0 -7.4     -58.0   -11      553   19 43 11
19 44 00  ---          19 25 01  18.3  27.1 -7.4     -58.2    49      555   19 43 01

19 44 00  W3IRS5_H2O   19 25 01  20.1  28.6 -7.0     -62.0   -12      555   19 44 12
19 45 00  ---          19 26 01  20.2  28.7 -7.0     -62.2    48      557   19 44 01

19 45 00  0241+622     19 26 01  18.4  27.1 -7.3     -58.4   -11      557   19 45 11
19 46 00  ---          19 27 01  18.5  27.2 -7.3     -58.6    49      558   19 45 01

19 46 00  W3IRS5_H2O   19 27 01  20.3  28.7 -7.0     -62.4   -12      558   19 46 12
19 47 00  ---          19 28 02  20.4  28.8 -7.0     -62.6    48      560   19 46 01

19 47 30  0241+622     19 28 32  18.7  27.3 -7.3     -58.9    18      560   19 47 30
19 48 30  ---          19 29 32  18.8  27.4 -7.3     -59.1    60      562   19 47 31

19 48 30  W3IRS5_H2O   19 29 32  20.5  28.9 -7.0     -62.9   -12      562   19 48 42
19 49 30  ---          19 30 32  20.6  28.9 -6.9     -63.1    48      563   19 48 31

19 49 30  0241+622     19 30 32  18.9  27.4 -7.3     -59.3   -12      563   19 49 42
19 50 30  ---          19 31 32  19.0  27.5 -7.2     -59.5    48      565   19 49 31

19 50 30  W3IRS5_H2O   19 31 32  20.7  29.0 -6.9     -63.3   -12      565   19 50 42
19 51 30  ---          19 32 32  20.9  29.0 -6.9     -63.5    48      566   19 50 31

19 51 30  0241+622     19 32 32  19.1  27.6 -7.2     -59.7   -12      566   19 51 42
19 52 30  ---          19 33 33  19.2  27.6 -7.2     -59.9    48      568   19 51 31

19 52 30  W3IRS5_H2O   19 33 33  21.0  29.1 -6.9     -63.7   -12      568   19 52 42
19 53 30  ---          19 34 33  21.1  29.1 -6.9     -63.9    48      569   19 52 31

19 53 30  0241+622     19 34 33  19.3  27.7 -7.2     -60.1   -12      569   19 53 42
19 54 30  ---          19 35 33  19.4  27.7 -7.2     -60.3    48      571   19 53 31

19 54 30  W3IRS5_H2O   19 35 33  21.2  29.2 -6.9     -64.1   -12      571   19 54 42
19 55 30  ---          19 36 33  21.3  29.2 -6.8     -64.3    48      572   19 54 31

19 55 30  0241+622     19 36 33  19.5  27.8 -7.2     -60.5   -12      572   19 55 42
19 56 30  ---          19 37 33  19.6  27.9 -7.1     -60.7    48      574   19 55 31

19 56 30  W3IRS5_H2O   19 37 33  21.4  29.3 -6.8     -64.5   -12      574   19 56 42
19 57 30  ---          19 38 33  21.5  29.4 -6.8     -64.7    48      576   19 56 31

19 58 00  0241+622     19 39 03  19.7  27.9 -7.1     -61.0    18      576   19 58 00
19 59 00  ---          19 40 04  19.8  28.0 -7.1     -61.2    60      577   19 58 01
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

19 59 00  W3IRS5_H2O   19 40 04  21.6  29.4 -6.8     -65.0   -12      577   19 59 12
20 00 00  ---          19 41 04  21.7  29.5 -6.8     -65.2    48      579   19 59 01

20 00 00  0241+622     19 41 04  19.9  28.1 -7.1     -61.4   -12      579   20 00 12
20 01 00  ---          19 42 04  20.0  28.1 -7.1     -61.6    48      581   20 00 01

20 01 00  W3IRS5_H2O   19 42 04  21.9  29.5 -6.8     -65.4   -12      581   20 01 12
20 02 00  ---          19 43 04  22.0  29.6 -6.7     -65.6    48      582   20 01 01

20 02 00  0241+622     19 43 04  20.1  28.2 -7.1     -61.8   -12      582   20 02 12
20 03 00  ---          19 44 04  20.2  28.2 -7.0     -62.0    48      584   20 02 01

20 03 00  W3IRS5_H2O   19 44 04  22.1  29.6 -6.7     -65.8   -12      584   20 03 12
20 04 00  ---          19 45 04  22.2  29.7 -6.7     -66.0    48      585   20 03 01

20 04 00  0241+622     19 45 04  20.3  28.3 -7.0     -62.2   -12      585   20 04 12
20 05 00  ---          19 46 05  20.4  28.4 -7.0     -62.4    48      587   20 04 01

20 05 00  W3IRS5_H2O   19 46 05  22.3  29.7 -6.7     -66.2   -12      587   20 05 12
20 06 00  ---          19 47 05  22.4  29.8 -6.7     -66.4    48      588   20 05 01

20 06 00  0241+622     19 47 05  20.5  28.4 -7.0     -62.6   -12      588   20 06 12
20 07 00  ---          19 48 05  20.6  28.5 -7.0     -62.8    48      590   20 06 01

20 07 00  W3IRS5_H2O   19 48 05  22.5  29.8 -6.7     -66.6   -12      590   20 07 12
20 08 00  ---          19 49 05  22.6  29.9 -6.6     -66.8    48      591   20 07 01

20 08 30  0241+622     19 49 35  20.8  28.5 -6.9     -63.1    18      591   20 08 30
20 09 30  ---          19 50 35  20.9  28.6 -6.9     -63.3    60      593   20 08 31

20 09 30  W3IRS5_H2O   19 50 35  22.8  30.0 -6.6     -67.1   -12      593   20 09 42
20 10 30  ---          19 51 36  22.9  30.0 -6.6     -67.3    48      595   20 09 31

20 10 30  0241+622     19 51 36  21.0  28.7 -6.9     -63.5   -12      595   20 10 42
20 11 30  ---          19 52 36  21.1  28.7 -6.9     -63.7    48      596   20 10 31

20 11 30  W3IRS5_H2O   19 52 36  23.0  30.1 -6.6     -67.5   -12      596   20 11 42
20 12 30  ---          19 53 36  23.1  30.1 -6.6     -67.7    48      598   20 11 31

20 12 30  0241+622     19 53 36  21.2  28.8 -6.9     -63.9   -12      598   20 12 42
20 13 30  ---          19 54 36  21.3  28.8 -6.9     -64.1    48      599   20 12 31

20 13 30  W3IRS5_H2O   19 54 36  23.2  30.2 -6.5     -67.9   -12      599   20 13 42
20 14 30  ---          19 55 36  23.3  30.2 -6.5     -68.1    48      601   20 13 31
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

20 14 30  0241+622     19 55 36  21.4  28.9 -6.8     -64.4   -12      601   20 14 42
20 15 30  ---          19 56 36  21.5  28.9 -6.8     -64.6    48      603   20 14 31

20 15 30  W3IRS5_H2O   19 56 36  23.4  30.3 -6.5     -68.3   -12      603   20 15 42
20 16 30  ---          19 57 36  23.5  30.3 -6.5     -68.5    48      604   20 15 31

20 16 30  0241+622     19 57 36  21.6  29.0 -6.8     -64.8   -12      604   20 16 42
20 17 30  ---          19 58 37  21.7  29.0 -6.8     -65.0    48      606   20 16 31

20 17 30  W3IRS5_H2O   19 58 37  23.6  30.4 -6.5     -68.7   -12      606   20 17 42
20 18 30  ---          19 59 37  23.7  30.4 -6.5     -68.9    48      607   20 17 31

20 18 33  0241+622     19 59 40  21.8  29.1 -6.8     -65.2    -9      607   20 18 42
20 19 33  ---          20 00 40  21.9  29.1 -6.8     -65.4    51      609   20 18 34

20 19 33  W3IRS5_H2O   20 00 40  23.9  30.5 -6.4     -69.2   -12      609   20 19 45
20 20 33  ---          20 01 40  24.0  30.5 -6.4     -69.4    48      610   20 19 34

20 20 33  0241+622     20 01 40  22.0  29.2 -6.7     -65.6   -12      610   20 20 45
20 21 33  ---          20 02 40  22.1  29.2 -6.7     -65.8    48      612   20 20 34

20 21 33  W3IRS5_H2O   20 02 40  24.1  30.5 -6.4     -69.6   -12      612   20 21 45
20 22 33  ---          20 03 40  24.2  30.6 -6.4     -69.8    48      613   20 21 34

20 22 33  0241+622     20 03 40  22.2  29.3 -6.7     -66.0   -12      613   20 22 45
20 23 33  ---          20 04 41  22.3  29.4 -6.7     -66.2    48      615   20 22 34

20 23 33  W3IRS5_H2O   20 04 41  24.3  30.6 -6.4     -70.0   -12      615   20 23 45
20 24 33  ---          20 05 41  24.4  30.7 -6.4     -70.2    48      617   20 23 34

20 24 33  0241+622     20 05 41  22.5  29.4 -6.7     -66.4   -12      617   20 24 45
20 25 33  ---          20 06 41  22.6  29.5 -6.7     -66.6    48      618   20 24 34

20 25 33  W3IRS5_H2O   20 06 41  24.5  30.7 -6.3     -70.4   -12      618   20 25 45
20 26 33  ---          20 07 41  24.6  30.8 -6.3     -70.6    48      620   20 25 34

20 26 33  0241+622     20 07 41  22.7  29.5 -6.6     -66.8   -12      620   20 26 45
20 27 33  ---          20 08 41  22.8  29.5 -6.6     -67.0    48      621   20 26 34

20 27 33  W3IRS5_H2O   20 08 41  24.7  30.8 -6.3     -70.8   -12      621   20 27 45
20 28 33  ---          20 09 41  24.8  30.8 -6.3     -71.0    48      623   20 27 34

20 28 33  0241+622     20 09 41  22.9  29.6 -6.6     -67.2   -12      623   20 28 45
20 29 33  ---          20 10 42  23.0  29.6 -6.6     -67.4    48      624   20 28 34
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

 ---------- K-band VLBI scans. Ground segment 02 : Delay/D-term cal. 3C84, scan 4 ----------

20 31 33  3C84         20 12 42   8.6  46.3 -7.1     -56.3    83      624   20 31 33
20 41 33  ---          20 22 44  10.1  47.3 -7.0     -57.8   600      644   20 31 34

 ----------  Ground-only scan on 0716+714 ----------

20 47 00  0716+714     20 28 12  12.6   5.2-10.9     -14.1   289      644   20 47 00
20 57 00  ---          20 38 13  12.8   6.0-10.8     -16.3   600      663   20 47 01

 ---------- K-band VLBI scans. Ground segment 03 : Phase-ref. scans on W3IRS5 without VLA/GBT/Effelsberg ----------

21 00 00  0241+622     20 41 14  26.3  30.9 -6.1     -73.6   146      663   21 00 00
21 01 00  ---          20 42 14  26.4  31.0 -6.1     -73.9    60      665   21 00 01

21 01 00  W3IRS5_H2O   20 42 14  28.5  32.0 -5.7     -77.7   -12      665   21 01 12
21 02 00  ---          20 43 14  28.6  32.0 -5.7     -77.9    48      666   21 01 01

21 02 30  0241+622     20 43 44  26.6  31.0 -6.0     -74.2    18      666   21 02 30
21 03 30  ---          20 44 44  26.7  31.1 -6.0     -74.4    60      668   21 02 31

21 03 30  W3IRS5_H2O   20 44 44  28.8  32.1 -5.7     -78.2   -12      668   21 03 42
21 04 30  ---          20 45 44  28.9  32.1 -5.7     -78.4    48      670   21 03 31

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 without GBT/Effelsberg ----------

21 05 00  0241+622     20 46 14  26.9  31.1 -6.0     -74.7    18      670   21 05 00
21 06 00  ---          20 47 15  27.0  31.1 -6.0     -74.9    60      672   21 05 01

21 06 00  W3IRS5_H2O   20 47 15  29.1  32.1 -5.7     -78.7   -12      672   21 06 12
21 07 00  ---          20 48 15  29.2  32.2 -5.6     -78.9    48      673   21 06 01

21 07 00  0241+622     20 48 15  27.1  31.2 -6.0     -75.1   -12      673   21 07 12
21 08 00  ---          20 49 15  27.2  31.2 -6.0     -75.3    48      675   21 07 01

21 08 00  W3IRS5_H2O   20 49 15  29.3  32.2 -5.6     -79.1   -12      675   21 08 12
21 09 00  ---          20 50 15  29.4  32.2 -5.6     -79.3    48      676   21 08 01

21 09 00  0241+622     20 50 15  27.3  31.2 -5.9     -75.5   -12      676   21 09 12
21 10 00  ---          20 51 15  27.4  31.3 -5.9     -75.7    48      678   21 09 01

21 10 00  W3IRS5_H2O   20 51 15  29.5  32.2 -5.6     -79.5   -12      678   21 10 12
21 11 00  ---          20 52 15  29.6  32.3 -5.6     -79.8    48      680   21 10 01
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

21 11 00  0241+622     20 52 15  27.5  31.3 -5.9     -75.9   -12      680   21 11 12
21 12 00  ---          20 53 16  27.6  31.3 -5.9     -76.1    48      681   21 11 01

21 12 00  W3IRS5_H2O   20 53 16  29.8  32.3 -5.6     -80.0   -12      681   21 12 12
21 13 00  ---          20 54 16  29.9  32.3 -5.5     -80.2    48      683   21 12 01

21 13 00  0241+622     20 54 16  27.8  31.4 -5.9     -76.3   -12      683   21 13 12
21 14 00  ---          20 55 16  27.9  31.4 -5.9     -76.5    48      684   21 13 01

21 14 00  W3IRS5_H2O   20 55 16  30.0  32.3 -5.5     -80.4   -12      684   21 14 12
21 15 00  ---          20 56 16  30.1  32.3 -5.5     -80.6    48      686   21 14 01

21 17 30  0241+622     20 58 47  28.3  31.5 -5.8     -77.3   138      686   21 17 30
21 18 30  ---          20 59 47  28.4  31.5 -5.8     -77.5    60      688   21 17 31

21 18 30  W3IRS5_H2O   20 59 47  30.5  32.4 -5.5     -81.3   -12      688   21 18 42
21 19 30  ---          21 00 47  30.6  32.4 -5.4     -81.5    48      689   21 18 31

21 19 30  0241+622     21 00 47  28.5  31.6 -5.8     -77.7   -12      689   21 19 42
21 20 30  ---          21 01 47  28.6  31.6 -5.7     -77.9    48      691   21 19 31

21 20 30  W3IRS5_H2O   21 01 47  30.7  32.5 -5.4     -81.8   -12      691   21 20 42
21 21 30  ---          21 02 47  30.9  32.5 -5.4     -82.0    48      692   21 20 31

21 21 30  0241+622     21 02 47  28.7  31.6 -5.7     -78.1   -12      692   21 21 42
21 22 30  ---          21 03 47  28.8  31.6 -5.7     -78.3    48      694   21 21 31

21 22 30  W3IRS5_H2O   21 03 47  31.0  32.5 -5.4     -82.2   -12      694   21 22 42
21 23 30  ---          21 04 48  31.1  32.5 -5.4     -82.4    48      695   21 22 31

21 23 30  0241+622     21 04 48  28.9  31.7 -5.7     -78.5   -12      695   21 23 42
21 24 30  ---          21 05 48  29.1  31.7 -5.7     -78.7    48      697   21 23 31

21 24 30  W3IRS5_H2O   21 05 48  31.2  32.5 -5.4     -82.6   -12      697   21 24 42
21 25 30  ---          21 06 48  31.3  32.6 -5.3     -82.8    48      698   21 24 31

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 ----------

21 28 00  0241+622     21 09 18  29.4  31.8 -5.6     -79.5   138      698   21 28 00
21 29 00  ---          21 10 18  29.6  31.8 -5.6     -79.7    60      700   21 28 01

21 29 00  W3IRS5_H2O   21 10 18  31.7  32.6 -5.3     -83.6   -12      700   21 29 12
21 30 00  ---          21 11 19  31.8  32.6 -5.3     -83.8    48      702   21 29 01
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

21 30 00  0241+622     21 11 19  29.7  31.8 -5.6     -79.9   -12      702   21 30 12
21 31 00  ---          21 12 19  29.8  31.9 -5.6     -80.1    48      704   21 30 01

21 31 00  W3IRS5_H2O   21 12 19  32.0  32.6 -5.2     -84.0   -12      704   21 31 12
21 32 00  ---          21 13 19  32.1  32.7 -5.2     -84.2    48      705   21 31 01

21 32 00  0241+622     21 13 19  29.9  31.9 -5.6     -80.3   -12      705   21 32 12
21 33 00  ---          21 14 19  30.0  31.9 -5.5     -80.5    48      707   21 32 01

21 33 00  W3IRS5_H2O   21 14 19  32.2  32.7 -5.2     -84.4   -12      707   21 33 12
21 34 00  ---          21 15 19  32.3  32.7 -5.2     -84.6    48      708   21 33 01

21 34 00  0241+622     21 15 19  30.1  31.9 -5.5     -80.7   -12      708   21 34 12
21 35 00  ---          21 16 19  30.2  31.9 -5.5     -81.0    48      710   21 34 01

21 35 00  W3IRS5_H2O   21 16 19  32.4  32.7 -5.2     -84.9   -12      710   21 35 12
21 36 00  ---          21 17 20  32.5  32.7 -5.2     -85.1    48      711   21 35 01

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 without VLA ----------

21 36 00  0241+622     21 17 20  30.4  32.0 -5.5     -81.2   -12      711   21 36 12
21 37 00  ---          21 18 20  30.5  32.0 -5.5     -81.4    48      713   21 36 01

21 37 00  W3IRS5_H2O   21 18 20  32.7  32.7 -5.1     -85.3   -12      713   21 37 12
21 38 00  ---          21 19 20  32.8  32.7 -5.1     -85.5    48      714   21 37 01

21 38 00  0241+622     21 19 20  30.6  32.0 -5.5     -81.6   -12      714   21 38 12
21 39 00  ---          21 20 20  30.7  32.0 -5.4     -81.8    48      716   21 38 01

 ---------- K-band VLBI scans. Ground segment 04 : Delay/D-term cal. 3C84 scan 5 ----------

21 40 50  3C84         21 22 10  20.0  52.7 -6.0     -66.3    80      716   21 40 50
21 49 50  ---          21 31 12  21.5  53.4 -5.8     -67.5   540      733   21 40 51

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 ----------

21 52 30  0241+622     21 33 52  32.3  32.2 -5.2     -84.7   131      733   21 52 30
21 53 30  ---          21 34 52  32.4  32.3 -5.2     -84.9    60      735   21 52 31

21 53 30  W3IRS5_H2O   21 34 52  34.6  32.8 -4.9     -88.9   -12      735   21 53 42
21 54 30  ---          21 35 53  34.7  32.8 -4.9     -89.1    48      737   21 53 31

21 54 30  0241+622     21 35 53  32.5  32.3 -5.2     -85.1   -12      737   21 54 42
21 55 30  ---          21 36 53  32.6  32.3 -5.2     -85.3    48      738   21 54 31
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

21 55 30  W3IRS5_H2O   21 36 53  34.8  32.8 -4.8     -89.3   -12      738   21 55 42
21 56 30  ---          21 37 53  34.9  32.8 -4.8     -89.5    48      740   21 55 31

21 56 30  0241+622     21 37 53  32.7  32.3 -5.1     -85.6   -12      740   21 56 42
21 57 30  ---          21 38 53  32.8  32.3 -5.1     -85.8    48      741   21 56 31

21 57 30  W3IRS5_H2O   21 38 53  35.1  32.8 -4.8     -89.8   -12      741   21 57 42
21 58 30  ---          21 39 53  35.2  32.8 -4.8     -90.0    48      743   21 57 31

21 58 45  0241+622     21 40 08  33.0  32.3 -5.1     -86.1     3      743   21 58 45
21 59 45  ---          21 41 08  33.1  32.3 -5.1     -86.3    60      745   21 58 46

21 59 45  W3IRS5_H2O   21 41 08  35.3  32.8 -4.8     -90.3   -12      745   21 59 57
22 00 45  ---          21 42 09  35.4  32.8 -4.7     -90.5    48      746   21 59 46

22 00 45  0241+622     21 42 09  33.2  32.3 -5.1     -86.5   -12      746   22 00 57
22 01 45  ---          21 43 09  33.3  32.3 -5.1     -86.7    48      748   22 00 46

22 01 45  W3IRS5_H2O   21 43 09  35.6  32.8 -4.7     -90.7   -12      748   22 01 57
22 02 45  ---          21 44 09  35.7  32.8 -4.7     -90.9    48      750   22 01 46

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 ----------

22 03 00  0241+622     21 44 24  33.5  32.3 -5.0     -87.0     3      750   22 03 00
22 04 00  ---          21 45 24  33.6  32.4 -5.0     -87.2    60      751   22 03 01

22 04 00  W3IRS5_H2O   21 45 24  35.8  32.8 -4.7     -91.2   -12      751   22 04 12
22 05 00  ---          21 46 24  35.9  32.8 -4.7     -91.4    48      753   22 04 01

22 05 00  0241+622     21 46 24  33.7  32.4 -5.0     -87.4   -12      753   22 05 12
22 06 00  ---          21 47 24  33.8  32.4 -5.0     -87.6    48      755   22 05 01

22 06 00  W3IRS5_H2O   21 47 24  36.0  32.8 -4.7     -91.7   -12      755   22 06 12
22 07 00  ---          21 48 25  36.2  32.8 -4.6     -91.9    48      756   22 06 01

22 07 00  0241+622     21 48 25  33.9  32.4 -5.0     -87.9   -12      756   22 07 12
22 08 00  ---          21 49 25  34.0  32.4 -5.0     -88.1    48      758   22 07 01

22 08 00  W3IRS5_H2O   21 49 25  36.3  32.8 -4.6     -92.1   -12      758   22 08 12
22 09 00  ---          21 50 25  36.4  32.8 -4.6     -92.3    48      759   22 08 01

22 09 00  0241+622     21 50 25  34.2  32.4 -4.9     -88.3   -12      759   22 09 12
22 10 00  ---          21 51 25  34.3  32.4 -4.9     -88.5    48      761   22 09 01
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

22 10 00  W3IRS5_H2O   21 51 25  36.5  32.8 -4.6     -92.6   -12      761   22 10 12
22 11 00  ---          21 52 25  36.6  32.8 -4.6     -92.8    48      762   22 10 01

22 12 45  0241+622     21 54 11  34.6  32.4 -4.9     -89.1    93      762   22 12 45
22 13 45  ---          21 55 11  34.7  32.4 -4.9     -89.3    60      764   22 12 46

22 13 45  W3IRS5_H2O   21 55 11  37.0  32.8 -4.5     -93.4   -12      764   22 13 57
22 14 45  ---          21 56 11  37.1  32.8 -4.5     -93.6    48      766   22 13 46

22 14 45  0241+622     21 56 11  34.8  32.4 -4.8     -89.6   -12      766   22 14 57
22 15 45  ---          21 57 11  34.9  32.4 -4.8     -89.8    48      767   22 14 46

22 15 45  W3IRS5_H2O   21 57 11  37.2  32.8 -4.5     -93.9   -12      767   22 15 57
22 16 45  ---          21 58 11  37.3  32.7 -4.5     -94.1    48      769   22 15 46

22 16 45  0241+622     21 58 11  35.0  32.4 -4.8     -90.0   -12      769   22 16 57
22 17 45  ---          21 59 11  35.2  32.4 -4.8     -90.2    48      770   22 16 46

22 17 45  W3IRS5_H2O   21 59 11  37.4  32.7 -4.5     -94.3   -12      770   22 17 57
22 18 45  ---          22 00 12  37.5  32.7 -4.4     -94.5    48      772   22 17 46

22 18 45  0241+622     22 00 12  35.3  32.4 -4.8     -90.5   -12      772   22 18 57
22 19 45  ---          22 01 12  35.4  32.4 -4.8     -90.7    48      773   22 18 46

22 19 45  W3IRS5_H2O   22 01 12  37.7  32.7 -4.4     -94.8   -12      773   22 19 57
22 20 45  ---          22 02 12  37.8  32.7 -4.4     -95.0    48      775   22 19 46

22 20 45  0241+622     22 02 12  35.5  32.4 -4.7     -90.9   -12      775   22 20 57
22 21 45  ---          22 03 12  35.6  32.4 -4.7     -91.1    48      777   22 20 46

22 21 45  W3IRS5_H2O   22 03 12  37.9  32.7 -4.4     -95.2   -13      777   22 21 58
22 22 45  ---          22 04 12  38.0  32.7 -4.4     -95.5    47      778   22 21 46

22 23 45  0241+622     22 05 12  35.9  32.4 -4.7     -91.6    48      778   22 23 45
22 24 45  ---          22 06 13  36.0  32.4 -4.7     -91.8    60      780   22 23 46

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 ----------

22 25 15  0241+622     22 06 43  36.0  32.4 -4.7     -91.9    24      780   22 25 15
22 26 15  ---          22 07 43  36.1  32.4 -4.6     -92.1    60      782   22 25 16

22 26 15  W3IRS5_H2O   22 07 43  38.4  32.6 -4.3     -96.3   -13      782   22 26 28
22 27 15  ---          22 08 43  38.5  32.6 -4.3     -96.5    47      783   22 26 16
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

22 27 15  0241+622     22 08 43  36.3  32.4 -4.6     -92.4   -12      783   22 27 27
22 28 15  ---          22 09 43  36.4  32.4 -4.6     -92.6    48      785   22 27 16

22 28 15  W3IRS5_H2O   22 09 43  38.6  32.6 -4.3     -96.7   -13      785   22 28 28
22 29 15  ---          22 10 43  38.8  32.6 -4.3     -97.0    47      787   22 28 16

22 29 15  0241+622     22 10 43  36.5  32.4 -4.6     -92.8   -12      787   22 29 27
22 30 15  ---          22 11 43  36.6  32.3 -4.6     -93.0    48      788   22 29 16

22 30 15  W3IRS5_H2O   22 11 43  38.9  32.5 -4.3     -97.2   -13      788   22 30 28
22 31 15  ---          22 12 44  39.0  32.5 -4.2     -97.4    47      790   22 30 16

 ---------- K-band VLBI scans. Ground segment 04 : Delay/D-term cal. 3C84, scan 6 ----------

22 34 30  3C84         22 15 59  29.4  56.5 -5.1     -73.6   167      790   22 34 30
22 44 30  ---          22 26 01  31.2  57.1 -4.9     -75.0   600      809   22 34 31

 ----------  Ground-only scan  0716+714 ----------

22 52 00  0716+714     22 33 32  17.2  14.3 -8.8     -41.5   411      809   22 52 00
22 58 00  ---          22 39 33  17.5  14.7 -8.7     -42.8   360      820   22 52 01

23 00 00  0241+622     22 41 33  40.0  31.8 -4.1    -100.0    68      820   23 00 00
23 01 00  ---          22 42 34  40.1  31.8 -4.1    -100.2    60      822   23 00 01

23 01 00  W3IRS5_H2O   22 42 34  42.4  31.7 -3.7    -104.6   -13      822   23 01 13
23 02 00  ---          22 43 34  42.5  31.6 -3.7    -104.9    47      824   23 01 01

23 02 00  0241+622     22 43 34  40.2  31.8 -4.0    -100.4   -12      824   23 02 12
23 03 00  ---          22 44 34  40.4  31.8 -4.0    -100.7    48      825   23 02 01

23 03 00  W3IRS5_H2O   22 44 34  42.6  31.6 -3.7    -105.1   -13      825   23 03 13
23 04 00  ---          22 45 34  42.7  31.5 -3.7    -105.4    47      827   23 03 01

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 without GBT/Effelsberg ----------

23 04 30  0241+622     22 46 04  40.5  31.7 -4.0    -101.1    18      827   23 04 30
23 05 30  ---          22 47 04  40.6  31.7 -4.0    -101.3    60      829   23 04 31

23 05 30  W3IRS5_H2O   22 47 04  42.9  31.5 -3.7    -105.7   -13      829   23 05 43
23 06 30  ---          22 48 04  43.0  31.4 -3.7    -106.0    47      830   23 05 31

23 06 30  0241+622     22 48 04  40.8  31.7 -4.0    -101.5   -12      830   23 06 42
23 07 30  ---          22 49 05  40.9  31.6 -4.0    -101.8    48      832   23 06 31
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

23 07 30  W3IRS5_H2O   22 49 05  43.1  31.4 -3.6    -106.2   -13      832   23 07 43
23 08 30  ---          22 50 05  43.2  31.3 -3.6    -106.5    47      833   23 07 31

23 08 30  0241+622     22 50 05  41.0  31.6 -3.9    -102.0   -12      833   23 08 42
23 09 30  ---          22 51 05  41.1  31.6 -3.9    -102.3    48      835   23 08 31

23 09 30  W3IRS5_H2O   22 51 05  43.4  31.3 -3.6    -106.7   -13      835   23 09 43
23 10 30  ---          22 52 05  43.5  31.2 -3.6    -107.0    47      837   23 09 31

 ---------- K-band VLBI scans. Ground segment 04 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

23 11 45  0241+622     22 53 20  41.4  31.5 -3.9    -102.8    63      837   23 11 45
23 12 45  ---          22 54 20  41.5  31.5 -3.9    -103.1    60      838   23 11 46

23 12 45  W3IRS5_H2O   22 54 20  43.7  31.1 -3.5    -107.6   -13      838   23 12 58
23 13 45  ---          22 55 21  43.8  31.1 -3.5    -107.8    47      840   23 12 46

23 14 15  0241+622     22 55 51  41.6  31.4 -3.8    -103.4    18      840   23 14 15
23 15 15  ---          22 56 51  41.7  31.4 -3.8    -103.7    60      842   23 14 16

23 15 15  W3IRS5_H2O   22 56 51  44.0  31.0 -3.5    -108.2   -12      842   23 15 27
23 16 15  ---          22 57 51  44.1  31.0 -3.5    -108.5    48      843   23 15 16

23 16 15  0241+622     22 57 51  41.9  31.3 -3.8    -103.9   -12      843   23 16 27
23 17 15  ---          22 58 51  42.0  31.3 -3.8    -104.2    48      845   23 16 16

23 17 15  W3IRS5_H2O   22 58 51  44.2  30.9 -3.5    -108.7   -12      845   23 17 27
23 18 15  ---          22 59 51  44.3  30.9 -3.5    -109.0    48      847   23 17 16

23 18 15  0241+622     22 59 51  42.1  31.3 -3.8    -104.4   -12      847   23 18 27
23 19 15  ---          23 00 52  42.2  31.2 -3.8    -104.7    48      848   23 18 16

23 19 15  W3IRS5_H2O   23 00 52  44.4  30.8 -3.4    -109.2   -12      848   23 19 27
23 20 15  ---          23 01 52  44.6  30.7 -3.4    -109.5    48      850   23 19 16

23 20 15  0241+622     23 01 52  42.3  31.2 -3.7    -104.9   -12      850   23 20 27
23 21 15  ---          23 02 52  42.4  31.1 -3.7    -105.2    48      851   23 20 16

23 21 15  W3IRS5_H2O   23 02 52  44.7  30.7 -3.4    -109.8   -12      851   23 21 27
23 22 15  ---          23 03 52  44.8  30.6 -3.4    -110.0    48      853   23 21 16

23 22 15  0241+622     23 03 52  42.5  31.1 -3.7    -105.4   -12      853   23 22 27
23 23 15  ---          23 04 52  42.6  31.1 -3.7    -105.7    48      854   23 22 16
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Dec 2018   Day 364 ---

23 23 15  W3IRS5_H2O   23 04 52  44.9  30.6 -3.4    -110.3   -12      854   23 23 27
23 24 15  ---          23 05 52  45.0  30.5 -3.4    -110.5    48      856   23 23 16

 ---------- K-band VLBI scans. Ground segment 04 : DA193, scan 1 ----------

23 27 00  0552+398     23 08 38  10.9  49.9 -6.8     -59.0    89      856   23 27 00
23 35 00  ---          23 16 39  12.2  50.7 -6.7     -60.1   480      871   23 27 01

23 36 00  0241+622     23 17 39  44.0  30.5 -3.5    -108.9   -11      871   23 36 11
23 37 00  ---          23 18 39  44.2  30.4 -3.5    -109.2    49      873   23 36 01

23 37 00  W3IRS5_H2O   23 18 39  46.4  29.7 -3.1    -114.0   -12      873   23 37 12
23 38 00  ---          23 19 40  46.5  29.6 -3.1    -114.2    48      874   23 37 01

23 38 00  0241+622     23 19 40  44.3  30.3 -3.4    -109.4   -12      874   23 38 12
23 39 00  ---          23 20 40  44.4  30.3 -3.4    -109.7    48      876   23 38 01

23 39 00  W3IRS5_H2O   23 20 40  46.6  29.6 -3.1    -114.5   -12      876   23 39 12
23 40 00  ---          23 21 40  46.7  29.5 -3.1    -114.8    48      878   23 39 01

 ---------- All stations: 3C48 ----------

23 41 30  3C48         23 23 10  61.2  75.8 -2.3     -85.9    49      878   23 41 30
23 51 30  ---          23 33 12  63.3  76.1 -2.1     -87.0   600      897   23 41 31

23 53 00  0241+622     23 34 42  45.9  29.5 -3.2    -113.4    47      897   23 53 00
23 54 00  ---          23 35 42  46.0  29.4 -3.2    -113.7    60      899   23 53 01

23 54 00  W3IRS5_H2O   23 35 42  48.2  28.4 -2.9    -118.7   -12      899   23 54 12
23 55 00  ---          23 36 42  48.3  28.3 -2.8    -119.0    48      900   23 54 01

23 55 00  0241+622     23 36 42  46.1  29.3 -3.2    -113.9   -12      900   23 55 12
23 56 00  ---          23 37 43  46.2  29.2 -3.1    -114.2    48      902   23 55 01

23 56 00  W3IRS5_H2O   23 37 43  48.4  28.2 -2.8    -119.2   -12      902   23 56 12
23 57 00  ---          23 38 43  48.5  28.2 -2.8    -119.5    48      903   23 56 01

23 57 00  0241+622     23 38 43  46.3  29.2 -3.1    -114.5   -12      903   23 57 12
23 58 00  ---          23 39 43  46.4  29.1 -3.1    -114.8    48      905   23 57 01
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Start: Sun  30 Dec 2018   Day 364 -- Stop: Mon  31 Dec 2018   Day 365 ---

 ---------- K-band VLBI scans. Space segment 05: target source W3IRS5 ----------

23 59 00  W3IRS5_H2O   23 40 43  48.7  28.0 -2.8    -120.1    48      905   23 59 00
00 07 50  ---          23 49 35  49.6  27.2 -2.6    -122.7   530      922   23 59 01

00 09 20  W3IRS5_H2O   23 51 05  49.7  27.0 -2.6    -123.1    84      922   00 09 20
00 18 10  ---          23 59 56  50.5  26.1 -2.5    -125.8   530      939   00 09 21

00 19 40  W3IRS5_H2O   00 01 26  50.7  25.9 -2.4    -126.2    84      939   00 19 40
00 28 30  ---          00 10 18  51.5  24.9 -2.3    -129.0   530      956   00 19 41

00 30 00  W3IRS5_H2O   00 11 48  51.6  24.8 -2.3    -129.5    84      956   00 30 00
00 39 00  ---          00 20 50  52.4  23.6 -2.1    -132.3   540      974   00 30 01

00 40 00  W3IRS5_H2O   00 21 50  52.5  23.5 -2.1    -132.7    54      974   00 40 00
00 43 00  ---          00 24 50  52.8  23.1 -2.0    -133.6   180      979   00 40 01

 ---------- K-band VLBI scans. Ground segment 05 : DA193, scan 2 ----------

00 44 50  0552+398     00 26 41  24.3  56.7 -5.5     -69.4    46      979   00 44 50
00 50 50  ---          00 32 42  25.4  57.1 -5.4     -70.2   360      991   00 44 51

00 50 50  W3IRS5_H2O   00 32 42  53.4  22.0 -1.9    -136.2   -63      991   00 51 53
00 53 50  ---          00 35 42  53.7  21.6 -1.9    -137.3   117      995   00 50 51

 ---------- K-band VLBI scans. Space segment 06: 0716+714 ----------

00 56 00  0716+714     00 37 52  25.3  20.3 -6.8     -68.8    66      995   00 56 00
01 09 00  ---          00 50 55  26.3  20.7 -6.6     -71.7   780     1020   00 56 01

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 without GBT/Effelsberg ----------

01 10 00  0241+622     00 51 55  53.2  21.6 -1.9    -136.5    -1     1020   01 10 01
01 11 00  ---          00 52 55  53.2  21.5 -1.9    -136.9    59     1022   01 10 01

01 11 00  W3IRS5_H2O   00 52 55  55.0  19.0 -1.6    -143.2   -11     1022   01 11 11
01 12 00  ---          00 53 55  55.0  18.8 -1.6    -143.6    49     1023   01 11 01

01 12 00  0241+622     00 53 55  53.3  21.3 -1.9    -137.2   -11     1023   01 12 11
01 13 00  ---          00 54 55  53.4  21.2 -1.9    -137.5    49     1025   01 12 01

01 13 00  W3IRS5_H2O   00 54 55  55.1  18.6 -1.5    -143.9   -11     1025   01 13 11
01 14 00  ---          00 55 55  55.2  18.5 -1.5    -144.3    49     1026   01 13 01
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  31 Dec 2018   Day 365 ---

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 without GBT/Effelsberg ----------

01 14 30  0241+622     00 56 25  53.5  21.0 -1.8    -138.1    19     1026   01 14 30
01 15 30  ---          00 57 26  53.6  20.8 -1.8    -138.4    60     1028   01 14 31

01 15 30  W3IRS5_H2O   00 57 26  55.3  18.2 -1.5    -144.8   -11     1028   01 15 41
01 16 30  ---          00 58 26  55.3  18.0 -1.5    -145.2    49     1030   01 15 31

01 16 30  0241+622     00 58 26  53.7  20.7 -1.8    -138.7   -11     1030   01 16 41
01 17 30  ---          00 59 26  53.7  20.5 -1.8    -139.1    49     1032   01 16 31

01 17 30  W3IRS5_H2O   00 59 26  55.4  17.9 -1.5    -145.5   -11     1032   01 17 41
01 18 30  ---          01 00 26  55.5  17.7 -1.4    -145.9    49     1033   01 17 31

01 18 30  0241+622     01 00 26  53.8  20.4 -1.8    -139.4   -11     1033   01 18 41
01 19 30  ---          01 01 26  53.9  20.2 -1.8    -139.8    49     1035   01 18 31

01 19 30  W3IRS5_H2O   01 01 26  55.5  17.5 -1.4    -146.3   -11     1035   01 19 41
01 20 30  ---          01 02 26  55.6  17.4 -1.4    -146.6    49     1036   01 19 31

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

01 20 30  0241+622     01 02 26  54.0  20.1 -1.7    -140.1   -11     1036   01 20 41
01 21 30  ---          01 03 27  54.0  19.9 -1.7    -140.4    49     1038   01 20 31

01 21 30  W3IRS5_H2O   01 03 27  55.7  17.2 -1.4    -147.0   -11     1038   01 21 41
01 22 30  ---          01 04 27  55.7  17.0 -1.4    -147.4    49     1039   01 21 31

01 24 15  0241+622     01 06 12  54.2  19.5 -1.7    -141.4    94     1039   01 24 15
01 25 15  ---          01 07 12  54.3  19.4 -1.7    -141.7    60     1041   01 24 16

01 25 15  W3IRS5_H2O   01 07 12  55.9  16.5 -1.3    -148.4   -11     1041   01 25 26
01 26 15  ---          01 08 12  56.0  16.3 -1.3    -148.7    49     1043   01 25 16

01 26 15  0241+622     01 08 12  54.4  19.2 -1.6    -142.1   -11     1043   01 26 26
01 27 15  ---          01 09 13  54.5  19.1 -1.6    -142.4    49     1045   01 26 16

01 27 15  W3IRS5_H2O   01 09 13  56.0  16.2 -1.3    -149.1   -11     1045   01 27 26
01 28 15  ---          01 10 13  56.1  16.0 -1.3    -149.5    49     1046   01 27 16

01 28 15  0241+622     01 10 13  54.5  18.9 -1.6    -142.8   -11     1046   01 28 26
01 29 15  ---          01 11 13  54.6  18.7 -1.6    -143.2    49     1048   01 28 16

01 29 15  W3IRS5_H2O   01 11 13  56.1  15.8 -1.3    -149.9   -11     1048   01 29 26
01 30 15  ---          01 12 13  56.2  15.6 -1.2    -150.2    49     1049   01 29 16
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  31 Dec 2018   Day 365 ---

01 30 15  0241+622     01 12 13  54.7  18.6 -1.6    -143.5   -11     1049   01 30 26
01 31 15  ---          01 13 13  54.7  18.4 -1.6    -143.9    49     1051   01 30 16

01 31 15  W3IRS5_H2O   01 13 13  56.3  15.4 -1.2    -150.6   -11     1051   01 31 26
01 32 15  ---          01 14 13  56.3  15.3 -1.2    -151.0    49     1052   01 31 16

01 32 15  0241+622     01 14 13  54.8  18.3 -1.5    -144.2   -11     1052   01 32 26
01 33 15  ---          01 15 14  54.9  18.1 -1.5    -144.6    49     1054   01 32 16

01 33 15  W3IRS5_H2O   01 15 14  56.4  15.1 -1.2    -151.3   -11     1054   01 33 26
01 34 15  ---          01 16 14  56.4  14.9 -1.2    -151.7    49     1056   01 33 16

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

01 36 00  0241+622     01 17 59  55.0  17.6 -1.5    -145.6    94     1056   01 36 00
01 37 00  ---          01 18 59  55.1  17.5 -1.5    -145.9    60     1058   01 36 01

01 37 00  W3IRS5_H2O   01 18 59  56.6  14.4 -1.1    -152.8   -11     1058   01 37 11
01 38 00  ---          01 19 59  56.6  14.2 -1.1    -153.1    49     1059   01 37 01

01 38 00  0241+622     01 19 59  55.2  17.3 -1.4    -146.3   -11     1059   01 38 11
01 39 00  ---          01 20 59  55.2  17.1 -1.4    -146.6    49     1061   01 38 01

01 39 00  W3IRS5_H2O   01 20 59  56.7  14.0 -1.1    -153.5   -11     1061   01 39 11
01 40 00  ---          01 22 00  56.7  13.8 -1.1    -153.9    49     1062   01 39 01

01 40 00  0241+622     01 22 00  55.3  17.0 -1.4    -147.0   -11     1062   01 40 11
01 41 00  ---          01 23 00  55.4  16.8 -1.4    -147.4    49     1064   01 40 01

01 41 00  W3IRS5_H2O   01 23 00  56.8  13.6 -1.1    -154.3   -11     1064   01 41 11
01 42 00  ---          01 24 00  56.8  13.4 -1.1    -154.7    49     1065   01 41 01

01 42 00  0241+622     01 24 00  55.4  16.6 -1.4    -147.7   -11     1065   01 42 11
01 43 00  ---          01 25 00  55.5  16.5 -1.4    -148.1    49     1067   01 42 01

01 43 00  W3IRS5_H2O   01 25 00  56.9  13.2 -1.0    -155.1   -11     1067   01 43 11
01 44 00  ---          01 26 00  56.9  13.0 -1.0    -155.4    49     1069   01 43 01

01 44 00  0241+622     01 26 00  55.6  16.3 -1.3    -148.5   -11     1069   01 44 11
01 45 00  ---          01 27 00  55.6  16.1 -1.3    -148.8    49     1070   01 44 01

01 45 00  W3IRS5_H2O   01 27 00  57.0  12.8 -1.0    -155.8   -11     1070   01 45 11
01 46 00  ---          01 28 01  57.0  12.6 -1.0    -156.2    49     1072   01 45 01
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  31 Dec 2018   Day 365 ---

01 46 00  0241+622     01 28 01  55.7  15.9 -1.3    -149.2   -11     1072   01 46 11
01 47 00  ---          01 29 01  55.7  15.8 -1.3    -149.6    49     1073   01 46 01

01 47 00  W3IRS5_H2O   01 29 01  57.1  12.4 -1.0    -156.6   -11     1073   01 47 11
01 48 00  ---          01 30 01  57.1  12.2 -1.0    -157.0    49     1075   01 47 01

01 48 00  0241+622     01 30 01  55.8  15.6 -1.3    -149.9   -11     1075   01 48 11
01 49 00  ---          01 31 01  55.8  15.4 -1.3    -150.3    49     1076   01 48 01

 ---------- K-band VLBI scans. Ground segment 07 : DA193 scan 3 ----------

01 51 00  0552+398     01 33 01  36.6  60.8 -4.4     -78.0    74     1076   01 51 00
01 59 00  ---          01 41 03  38.1  61.2 -4.3     -79.1   480     1092   01 51 01

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

02 00 30  0241+622     01 42 33  56.5  13.3 -1.1    -154.6    46     1092   02 00 30
02 01 30  ---          01 43 33  56.5  13.1 -1.0    -155.0    60     1094   02 00 31

02 01 30  W3IRS5_H2O   01 43 33  57.7   9.5 -0.7    -162.3   -10     1094   02 01 40
02 02 30  ---          01 44 33  57.7   9.3 -0.7    -162.7    50     1095   02 01 31

02 02 30  0241+622     01 44 33  56.6  12.9 -1.0    -155.4   -10     1095   02 02 40
02 03 30  ---          01 45 34  56.6  12.7 -1.0    -155.8    50     1097   02 02 31

02 03 30  W3IRS5_H2O   01 45 34  57.7   9.1 -0.7    -163.1   -10     1097   02 03 40
02 04 30  ---          01 46 34  57.8   8.9 -0.7    -163.5    50     1099   02 03 31

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

02 04 30  0241+622     01 46 34  56.7  12.5 -1.0    -156.1   -10     1099   02 04 40
02 05 30  ---          01 47 34  56.7  12.3 -1.0    -156.5    50     1100   02 04 31

02 05 30  W3IRS5_H2O   01 47 34  57.8   8.7 -0.7    -163.9   -10     1100   02 05 40
02 06 30  ---          01 48 34  57.8   8.4 -0.6    -164.3    50     1102   02 05 31

02 06 30  0241+622     01 48 34  56.7  12.1 -1.0    -156.9   -10     1102   02 06 40
02 07 30  ---          01 49 34  56.8  11.9 -0.9    -157.3    50     1103   02 06 31

02 07 30  W3IRS5_H2O   01 49 34  57.9   8.2 -0.6    -164.7   -11     1103   02 07 41
02 08 30  ---          01 50 34  57.9   8.0 -0.6    -165.1    49     1105   02 07 31

02 08 30  0241+622     01 50 34  56.8  11.7 -0.9    -157.7   -11     1105   02 08 41
02 09 30  ---          01 51 34  56.9  11.5 -0.9    -158.1    49     1107   02 08 31
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  31 Dec 2018   Day 365 ---

02 09 30  W3IRS5_H2O   01 51 34  57.9   7.8 -0.6    -165.5   -11     1107   02 09 41
02 10 30  ---          01 52 35  58.0   7.6 -0.6    -165.9    49     1108   02 09 31

02 10 30  0241+622     01 52 35  56.9  11.4 -0.9    -158.4   -11     1108   02 10 41
02 11 30  ---          01 53 35  57.0  11.2 -0.9    -158.8    49     1110   02 10 31

02 11 30  W3IRS5_H2O   01 53 35  58.0   7.4 -0.6    -166.3   -11     1110   02 11 41
02 12 30  ---          01 54 35  58.0   7.2 -0.5    -166.7    49     1111   02 11 31

02 12 30  0241+622     01 54 35  57.0  11.0 -0.9    -159.2   -11     1111   02 12 41
02 13 30  ---          01 55 35  57.0  10.8 -0.8    -159.6    49     1113   02 12 31

02 13 30  W3IRS5_H2O   01 55 35  58.0   6.9 -0.5    -167.1   -11     1113   02 13 41
02 14 30  ---          01 56 35  58.1   6.7 -0.5    -167.5    49     1115   02 13 31

02 14 30  0241+622     01 56 35  57.1  10.6 -0.8    -160.0   -11     1115   02 14 41
02 15 30  ---          01 57 35  57.1  10.4 -0.8    -160.4    49     1116   02 14 31

02 15 30  W3IRS5_H2O   01 57 35  58.1   6.5 -0.5    -167.9   -11     1116   02 15 41
02 16 30  ---          01 58 36  58.1   6.3 -0.5    -168.3    49     1118   02 15 31

02 16 30  0241+622     01 58 36  57.2  10.2 -0.8    -160.8   -11     1118   02 16 41
02 17 30  ---          01 59 36  57.2  10.0 -0.8    -161.2    49     1119   02 16 31

02 17 30  W3IRS5_H2O   01 59 36  58.1   6.1 -0.5    -168.7   -11     1119   02 17 41
02 18 30  ---          02 00 36  58.2   5.9 -0.4    -169.1    49     1121   02 17 31

02 18 30  0241+622     02 00 36  57.2   9.8 -0.8    -161.6   -11     1121   02 18 41
02 19 30  ---          02 01 36  57.3   9.6 -0.7    -162.0    49     1122   02 18 31

02 19 30  W3IRS5_H2O   02 01 36  58.2   5.6 -0.4    -169.5   -11     1122   02 19 41
02 20 30  ---          02 02 36  58.2   5.4 -0.4    -170.0    49     1124   02 19 31

 ---------- K-band VLBI scans. Ground segment 07 : DA193, scan 4 ----------

02 22 30  0552+398     02 04 37  42.5  62.2 -3.9     -82.2    72     1124   02 22 30
02 32 30  ---          02 14 38  44.4  62.5 -3.7     -83.6   600     1143   02 22 31

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

02 32 30  0241+622     02 14 38  57.7   6.9 -0.5    -167.1   -48     1143   02 33 18
02 33 30  ---          02 15 38  57.7   6.6 -0.5    -167.5    12     1144   02 32 31

02 33 30  W3IRS5_H2O   02 15 38  58.4   2.6 -0.2    -175.3   -11     1144   02 33 41
02 34 30  ---          02 16 39  58.4   2.3 -0.2    -175.7    49     1145   02 33 31
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               RadioAstron visibility tracking of H2O maser spots
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  31 Dec 2018   Day 365 ---

02 34 30  0241+622     02 16 39  57.7   6.4 -0.5    -167.9   -11     1145   02 34 41
02 35 30  ---          02 17 39  57.7   6.2 -0.5    -168.3    49     1147   02 34 31

02 35 30  W3IRS5_H2O   02 17 39  58.4   2.1 -0.2    -176.1   -11     1147   02 35 41
02 36 30  ---          02 18 39  58.4   1.9 -0.1    -176.5    49     1148   02 35 31

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

02 37 45  0241+622     02 19 54  57.8   5.7 -0.4    -169.2    64     1148   02 37 45
02 38 45  ---          02 20 54  57.8   5.5 -0.4    -169.6    60     1150   02 37 46

02 38 45  W3IRS5_H2O   02 20 54  58.4   1.4 -0.1    -177.4   -11     1150   02 38 56
02 39 45  ---          02 21 54  58.4   1.2 -0.1    -177.8    49     1152   02 38 46

02 39 45  0241+622     02 21 54  57.8   5.3 -0.4    -170.0   -11     1152   02 39 56
02 40 45  ---          02 22 55  57.9   5.1 -0.4    -170.4    49     1154   02 39 46

02 40 45  W3IRS5_H2O   02 22 55  58.4   0.9 -0.1    -178.3   -11     1154   02 40 56
02 41 45  ---          02 23 55  58.4   0.7 -0.1    -178.7    49     1155   02 40 46

02 41 45  0241+622     02 23 55  57.9   4.9 -0.4    -170.8   -11     1155   02 41 56
02 42 45  ---          02 24 55  57.9   4.7 -0.4    -171.2    49     1157   02 41 46

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

02 42 45  W3IRS5_H2O   02 24 55  58.4   0.5 -0.0    -179.1   -11     1157   02 42 56
02 43 45  ---          02 25 55  58.4   0.3 -0.0    -179.5    49     1158   02 42 46

02 43 45  0241+622     02 25 55  57.9   4.5 -0.3    -171.7   -11     1158   02 43 56
02 44 45  ---          02 26 55  57.9   4.2 -0.3    -172.1    49     1160   02 43 46

 ---------- K-band VLBI scans. Ground segment 07 : Phase-ref. scans on W3IRS5 with  GBT/Effelsberg ----------

02 44 45  0241+622     02 26 55  57.9   4.2 -0.3    -172.1    -6     1160   02 44 51
02 45 45  ---          02 27 55  57.9   4.0 -0.3    -172.5    54     1162   02 44 46

02 45 45  W3IRS5_H2O   02 27 55  58.4  -0.2  0.0     179.7   -11     1162   02 45 56
02 46 45  ---          02 28 56  58.4  -0.4  0.0     179.3    49     1163   02 45 46

02 46 45  0241+622     02 28 56  58.0   3.8 -0.3    -172.9   -11     1163   02 46 56
02 47 45  ---          02 29 56  58.0   3.6 -0.3    -173.3    49     1165   02 46 46

02 50 00  0518+165     02 32 11  48.9  99.9 -2.8     -62.2    59     1165   02 50 00
03 00 00  ---          02 42 13  51.0 101.7 -2.7     -61.6   600     1184   02 50 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./ga042_freq.dat:
     v1cm_b3

   Setup group:    7         Station: VLBA_FD           Total bit rate:   256
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  12  Setup file default.  Used with PCAL = off
   LO sum=   22228.00  22228.00  22228.00  22228.00
   BBC fr=     728.00    728.00    728.00    728.00
   Bandwd=      16.00     16.00     16.00     16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     728.00    728.00    728.00    728.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  12  13  14  15  16  17  18  19  20  27

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 55.507293       0.00
                     85 16 41.77889    * 85 00 00.00000      84 53 24.69683        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

 * 0241+622          02 41 00.673424   * 02 44 57.696744     02 46 29.056178       0.33
   J0244+6228        62 15 27.54311    * 62 28 06.51562      62 32 59.13195        0.14
                     From catalog imbedded in main SCHED input file.
                     rfc_2018c Petrov and Kovalev, in preparation  874 observations

   3C138             05 18 16.514082   * 05 21 09.885964     05 22 16.133039       0.12
 * 0518+165          16 35 26.83410    * 16 38 22.05157      16 39 20.31716        0.12
   J0521+1638        From catalog imbedded in main SCHED input file.
                     rfc_2018c Petrov and Kovalev, in preparation  412 observations. No flux informat

 * W3IRS5_H2O        02 21 53.326396   * 02 25 40.785000     02 27 08.349616       0.00
                     61 52 21.52150    * 62 05 52.56000      62 11 06.09706        0.00
                     ./ga042_sources.radioastron
                     H2O maser; positions from proposal, RA-AO2-08

 * 0716+714          07 16 13.029739   * 07 21 53.448474     07 24 03.933519       0.00
   J0721+7120        71 26 15.17406    * 71 20 36.36340      71 18 14.48302        0.00
                     ./ga042_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 42370 observations, RA-AO4-07, RA-AO3-0

   0316+413          03 16 29.567283   * 03 19 48.160114     03 21 04.051607       0.00
   J0319+4130        41 19 51.91847    * 41 30 42.10559      41 34 48.08248        0.00
 * 3C84              ./ga042_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 15448 observations, RA-AO4-04, RA-AO3-0

   0355+508          03 55 45.261370   * 03 59 29.747271     04 00 55.884074       0.00
   J0359+5057        50 49 20.28584    * 50 57 50.16179      51 01 02.26361        0.00
 * NRAO150           ./ga042_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 19270 observations, RA-AO3-04, RA-AO2-1

 * 0552+398          05 52 01.407174   * 05 55 30.805616     05 56 50.898153       0.00
   J0555+3948        39 48 21.94579    * 39 48 49.16494      39 48 51.81108        0.00
                     ./ga042_sources.radioastron
                     AGN, rfc_2013d Petrov, 2013, unpublished 392026 observations, RA-AO3-04, RA-AO2-

   0134+329          01 34 49.826374   * 01 37 41.299440     01 38 46.241861       0.00
   J0137+3309        32 54 20.25881    * 33 09 35.13299      33 15 23.83881        0.00
 * 3C48              ./ga042_sources.radioastron
                     WSRT calibrator, rfc_2013d Petrov, 2013, unpublished 140 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra1cm2.set            26                                3.800     0.000
  0241+622   ra1cm2.set            1 2 3 4 5 6 9 12 21 22 24 2 +     4.633   621.548
  0518+165   ra1cm2.set            1 2 3 5 12 21 22 24 25 29         0.167    27.769
  W3IRS5_H2O ra1cm2.set            1 2 3 4 5 6 9 12 21 22 24 2 +     6.933  1225.023
  0716+714   ra1cm2.set            1 2 3 4 5 6 9 12 21 22 24 2 +     1.433   276.681
  3C84       ra1cm2.set            1 2 3 4 5 6 9 12 21 22 24 2 +     0.983   126.613
  NRAO150    ra1cm2.set            2 3 4 5 6 9 12 21 22 24 25        0.900   155.212
  0552+398   ra1cm2.set            1 2 3 4 5 12 21 22 24 25 29       0.600    82.241
  3C48       ra1cm2.set            1 2 3 4 5 6 9 12 21 22 24 2 +     0.333    44.353

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 0528+134          05 28 06.759218   * 05 30 56.416749     05 32 01.257298       0.00
   J0530+1331        13 29 42.28878    * 13 31 55.14945      13 32 37.05063        0.00
                     ./ga042_sources.radioastron
                     AGN, MASIV, rfc_2013d Petrov, 2013, unpublished 139206 observations, RA-AO3-04,



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA             113.9
   0241+622           124.9
   0518+165           160.8
   W3IRS5_H2O         122.8
   0716+714           131.4
   3C84               135.0
   NRAO150            138.7
   0528+134           161.4
   0552+398           161.1
   3C48               114.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

