  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Evolution of the smallest radio sources
 Exp. Code:  GD014   


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 1 July 1999                        

PI:       J. Dennett-Thorpe                                               

Address:  RuG                                                             
          Postbus 800, 9700AV                                             
          Groningen The Netherlands                                       
                                                                          

Phone:    31--50--3634090                                                 
EMAIL:    jdt@astro.rug.nl                                                
Fax:      31--50--3636100                                                 
Phone during observation: 31--50--3122795/3634090                         

Observing mode: VLBA, 22 GHz continuum, 128-4-2                           

Notes:    Please note i have included the file freq.dat which has entry fo
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

 Next scan frequencies: 22207.49 22207.49 22223.49 22223.49
 Next BBC frequencies:    707.49   707.49   723.49   723.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00

05 30 00  J0943+3614   08 40 01  75.7  62.7 -1.1    -108.5     0   1  1      0  05 30 00
05 35 30  ---          08 45 32  76.7  61.2 -1.0    -110.8   330   F  1   2200

05 35 30  J1000+4223   08 45 32  71.0  46.6 -1.2    -122.2   -13   1  1   2200  05 35 30
05 41 00  ---          08 51 02  71.8  44.8 -1.2    -124.8   317   F  1   4400

05 41 00  J0955+5728   08 51 02  60.9  17.9 -1.1    -150.5   -24   1  1   4400  05 41 00
05 46 30  ---          08 56 33  61.3  16.5 -1.0    -152.9   306   F  1   6600

05 46 30  J1026+5141   08 56 33  63.2  31.7 -1.5    -133.1   -12   1  1   6600  05 46 30
05 52 00  ---          09 02 04  63.8  30.4 -1.4    -135.4   318   F  1   8800

05 52 00  J1109+3830   09 02 04  62.7  64.5 -2.1     -97.1   -25   1  1   8800  05 52 00
05 57 30  ---          09 07 35  63.8  64.2 -2.0     -98.2   305   F  1  11000

05 57 30  J1137+3442   09 07 35  58.4  72.6 -2.5     -86.7   -13   1  1  11000  05 57 30
06 03 00  ---          09 13 06  59.6  72.7 -2.4     -87.4   317   F  1  13200

06 05 00  J1425+3946   09 15 06  27.8  58.1 -5.2     -71.9    55   1  1  13200  06 05 00
06 10 30  ---          09 20 37  28.9  58.5 -5.1     -72.6   330   F  1  15400

06 32 00  J0027+599    09 42 11   6.7 -19.4  9.3      34.8  1236   1  1  15400  06 32 00
06 37 30  ---          09 47 42   6.4 -18.8  9.3      33.7   330   F  1  17600

06 43 00  J0202+420    09 53 13   2.6 -41.2  7.8  H   49.7   313   1  2  17600  06 43 00
06 48 30  ---          09 58 43   1.8 -40.5  7.9  D   48.8     0   R  1  15400

07 17 00  J0943+3614   10 27 18  79.3 -55.6  0.7     118.3  1554   1  2  15400  07 17 00
07 22 30  ---          10 32 49  78.3 -58.2  0.8     115.0   330   R  1  13200

07 22 30  J1000+4223   10 32 49  76.6 -26.7  0.5     148.4   -23   1  2  13200  07 22 30
07 28 00  ---          10 38 20  76.0 -30.3  0.6     144.0   307   R  1  11000

07 28 00  J0955+5728   10 38 20  62.2 -12.3  0.7     160.0   -30   1  2  11000  07 28 00
07 33 30  ---          10 43 51  61.9 -13.8  0.8     157.5   300   R  1   8800

07 33 30  J1026+5141   10 43 51  68.7  -7.4  0.3     169.7   -16   1  2   8800  07 33 30
07 39 00  ---          10 49 22  68.5  -9.7  0.4     166.4   314   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

07 41 00  J1109+3830   10 51 22  81.3  24.3 -0.3    -153.1    93   1  2   6600  07 41 00
07 46 30  ---          10 56 53  81.7  17.6 -0.2    -160.6   330   R  1   4400

07 46 30  J1137+3442   10 56 53  80.6  61.7 -0.7    -112.8   -31   1  2   4400  07 46 30
07 52 00  ---          11 02 24  81.6  58.7 -0.6    -116.6   299   R  1   2200

07 54 00  J1425+3946   11 04 24  48.4  63.1 -3.4     -86.5    52   1  2   2200  07 54 00
07 59 30  ---          11 09 55  49.5  63.2 -3.3     -87.3   330   R  1      0

08 01 30  1611+343     11 11 55  27.7  64.7 -5.0     -70.2    75   1  3      0  08 01 30
08 07 00  ---          11 17 26  28.8  65.2 -4.9     -70.8   330   F  1   2200

08 09 00  J1719+4803   11 19 27  22.2  46.2 -6.0     -68.4   105   1  3   2200  08 09 00
08 14 30  ---          11 24 58  23.1  46.6 -5.9     -69.3   330   F  1   4400

08 14 30  J1745+4059   11 24 58  16.0  51.5 -6.3     -63.1   -16   1  3   4400  08 14 30
08 21 00  ---          11 31 29  17.1  52.0 -6.2     -64.0   374   F  1   7000

08 21 00  J1800+388    11 31 29  13.6  52.7 -6.5     -61.4    -9   1  3   7000  08 21 00
08 26 30  ---          11 37 00  14.5  53.2 -6.4     -62.2   321   F  1   9200

08 26 30  J1819+3845   11 37 00  11.3  51.4 -6.7     -59.6    -9   1  3   9200  08 26 30
08 32 00  ---          11 42 31  12.2  52.0 -6.6     -60.3   321   F  1  11400

08 32 00  J1923+3941   11 42 31   2.4  44.1 -7.7     -51.1   -22   1  3  11400  08 32 00
08 39 30  ---          11 50 02   3.6  45.0 -7.6     -52.3   428   F  1  14400

08 39 30  J1810+5029   11 50 02  20.1  42.5 -6.3     -65.9   -35   1  3  14400  08 39 30
08 47 30  ---          11 58 03  21.3  43.0 -6.2     -67.2   445   F  1  17600

08 50 30  J1942+5154   12 01 04  10.0  34.5 -7.7     -52.2   155   1  4  17600  08 50 30
08 56 00  ---          12 06 34  10.7  35.0 -7.6     -53.2   330   R  1  15400

08 58 00  J1949+506    12 08 35   9.3  35.5 -7.7     -52.0   115   1  4  15400  08 58 00
09 03 30  ---          12 14 06  10.0  36.0 -7.6     -53.0   330   R  1  13200

09 03 30  J1950+6108   12 14 06  16.0  27.3 -7.6     -54.8   -14   1  4  13200  09 03 30
09 09 00  ---          12 19 37  16.6  27.7 -7.5     -55.9   316   R  1  11000

09 09 00  J2248+7054   12 19 37  12.9   7.5-10.5     -20.1   -15   1  4  11000  09 09 00
09 14 30  ---          12 25 07  13.0   7.9-10.4     -21.3   315   R  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

09 17 30  J0943+3614   12 28 08  55.4 -69.4  2.7      87.2    93   1  4   8800  09 17 30
09 23 00  ---          12 33 39  54.3 -69.3  2.8      86.4   330   R  1   6600

09 23 00  J1000+4223   12 33 39  57.3 -58.1  2.6      98.4    -9   1  4   6600  09 23 00
09 28 30  ---          12 39 10  56.3 -58.4  2.6      97.3   321   R  1   4400

09 28 30  J0955+5728   12 39 10  51.2 -34.2  2.7     116.0   -18   1  4   4400  09 28 30
09 34 00  ---          12 44 41  50.5 -34.7  2.8     114.4   312   R  1   2200

09 34 00  J1026+5141   12 44 41  57.1 -40.3  2.3     116.2   -15   1  4   2200  09 34 00
09 39 30  ---          12 50 12  56.3 -40.9  2.4     114.6   315   R  1      0

09 39 30  J1109+3830   12 50 12  67.9 -62.2  1.7     103.3   -25   1  5      0  09 39 30
09 45 00  ---          12 55 42  66.9 -62.8  1.8     101.9   305   F  1   2200

09 48 00  J1137+3442   12 58 43  72.4 -71.3  1.4      97.6   167   1  5   2200  09 48 00
09 53 30  ---          13 04 14  71.3 -71.7  1.5      96.4   330   F  1   4400

09 55 30  J1425+3946   13 06 14  71.4  55.1 -1.3    -113.3    33   1  5   4400  09 55 30
10 01 00  ---          13 11 45  72.4  53.7 -1.2    -115.5   330   F  1   6600

10 03 00  1611+343     13 13 45  52.2  72.4 -3.0     -82.6    78   1  5   6600  10 03 00
10 08 30  ---          13 19 16  53.3  72.6 -2.9     -83.2   330   F  1   8800

10 08 30  J1719+4803   13 19 16  41.7  50.9 -4.0     -88.4   -25   1  5   8800  10 08 30
10 14 00  ---          13 24 47  42.7  51.0 -3.9     -89.4   305   F  1  11000

10 14 00  J1745+4059   13 24 47  37.4  59.5 -4.3     -79.3   -13   1  5  11000  10 14 00
10 19 30  ---          13 30 18  38.4  59.8 -4.3     -80.1   317   F  1  13200

10 19 30  J1800+388    13 30 18  35.1  61.7 -4.5     -76.5    -9   1  5  13200  10 19 30
10 25 00  ---          13 35 49  36.2  62.0 -4.4     -77.2   321   F  1  15400

10 25 00  J1819+3845   13 35 49  32.6  61.0 -4.7     -74.8    -9   1  5  15400  10 25 00
10 30 30  ---          13 41 20  33.6  61.3 -4.6     -75.5   321   F  1  17600

10 30 30  J1923+3941   13 41 20  22.1  55.9 -5.7     -67.8   -25   1  6  17600  10 30 30
10 36 00  ---          13 46 51  23.1  56.3 -5.6     -68.5   305   R  1  15400

10 44 00  J1810+5029   13 54 52  39.3  47.6 -4.3     -87.6   445   1  6  15400  10 44 00
10 49 30  ---          14 00 23  40.2  47.7 -4.2     -88.6   330   R  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

10 52 30  J0943+3614   14 03 24  36.5 -65.4  4.3      75.9   103   1  6  13200  10 52 30
10 58 00  ---          14 08 54  35.4 -65.0  4.4      75.3   330   R  1  11000

10 58 00  J1000+4223   14 08 54  39.8 -58.2  4.1      82.1   -11   1  6  11000  10 58 00
11 03 30  ---          14 14 25  38.8 -58.0  4.2      81.3   319   R  1   8800

11 03 30  J0955+5728   14 14 25  38.8 -38.6  4.3      92.6   -15   1  6   8800  11 03 30
11 09 00  ---          14 19 56  38.1 -38.7  4.4      91.4   315   R  1   6600

11 09 00  J1026+5141   14 19 56  42.8 -46.0  3.9      93.0   -11   1  6   6600  11 09 00
11 14 30  ---          14 25 27  42.0 -46.1  4.0      91.9   319   R  1   4400

11 14 30  J1109+3830   14 25 27  49.4 -65.1  3.3      85.9   -17   1  6   4400  11 14 30
11 20 00  ---          14 30 58  48.3 -65.0  3.4      85.1   313   R  1   2200

11 20 00  J1137+3442   14 30 58  53.5 -71.8  2.9      83.9   -12   1  6   2200  11 20 00
11 25 30  ---          14 36 29  52.4 -71.6  3.0      83.3   318   R  1      0

11 25 30  J1425+3946   14 36 29  80.6 -12.6  0.2     165.8   -59   1  7      0  11 25 30
11 31 00  ---          14 42 00  80.3 -18.7  0.3     158.9   271   F  1   2200

11 33 00  J1745+4059   14 44 00  52.2  61.3 -3.0     -91.1    62   1  7   2200  11 33 00
11 38 30  ---          14 49 31  53.3  61.2 -2.9     -92.1   330   F  1   4400

11 38 30  J1719+4803   14 49 31  56.6  47.7 -2.5    -107.7   -11   1  7   4400  11 38 30
11 44 00  ---          14 55 02  57.5  47.2 -2.4    -109.2   319   F  1   6600

11 44 00  J1800+388    14 55 02  51.5  64.8 -3.1     -87.7   -14   1  7   6600  11 44 00
11 49 30  ---          15 00 33  52.5  64.9 -3.0     -88.5   316   F  1   8800

11 49 30  J1819+3845   15 00 33  48.8  64.7 -3.3     -85.7    -9   1  7   8800  11 49 30
11 55 00  ---          15 06 04  49.9  64.8 -3.2     -86.5   321   F  1  11000

11 55 00  J1923+3941   15 06 04  37.7  61.3 -4.3     -78.7   -26   1  7  11000  11 55 00
12 00 30  ---          15 11 35  38.7  61.6 -4.2     -79.4   304   F  1  13200

12 02 30  J1810+5029   15 13 35  51.8  45.8 -2.9    -104.1    92   1  7  13200  12 02 30
12 08 00  ---          15 19 06  52.6  45.5 -2.9    -105.5   330   F  1  15400

12 08 00  J1942+5154   15 19 06  38.2  45.7 -4.4     -87.3   -31   1  7  15400  12 08 00
12 13 30  ---          15 24 37  39.1  45.8 -4.3     -88.4   299   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

12 13 30  J1949+506    15 24 37  37.9  47.3 -4.4     -86.0    -4   1  8  17600  12 13 30
12 19 00  ---          15 30 08  38.7  47.3 -4.3     -87.0   326   R  1  15400

12 21 00  J1950+6108   15 32 08  38.6  33.9 -4.3     -95.6   109   1  8  15400  12 21 00
12 26 30  ---          15 37 39  39.3  33.8 -4.2     -96.9   330   R  1  13200

12 26 30  J2248+7054   15 37 39  23.4  19.9 -7.2     -63.3   -34   1  8  13200  12 26 30
12 37 30  ---          15 48 41  24.2  20.3 -7.0     -65.8   626   R  1   8800

12 39 30  J0943+3614   15 50 41  16.2 -57.1  6.1      63.6    66   1  8   8800  12 39 30
12 45 00  ---          15 56 12  15.2 -56.6  6.2      62.9   330   R  1   6600

12 45 00  J1000+4223   15 56 12  20.8 -52.2  5.9      67.0   -13   1  8   6600  12 45 00
12 50 30  ---          16 01 43  19.9 -51.7  6.0      66.2   317   R  1   4400

12 52 30  J0955+5728   16 03 43  24.4 -36.2  6.1      70.8   108   1  8   4400  12 52 30
12 58 00  ---          16 09 14  23.7 -35.9  6.2      69.7   330   R  1   2200

12 58 00  J1026+5141   16 09 14  26.1 -43.5  5.7      72.8    -7   1  8   2200  12 58 00
13 03 30  ---          16 14 45  25.3 -43.2  5.8      71.9   323   R  1      0

13 03 30  J1109+3830   16 14 45  28.5 -59.9  5.1      72.0   -13   1  9      0  13 03 30
13 09 00  ---          16 20 16  27.5 -59.5  5.2      71.3   317   F  1   2200

13 11 00  J1137+3442   16 22 16  31.1 -65.5  4.8      72.2   111   1  9   2200  13 11 00
13 16 30  ---          16 27 47  30.1 -65.1  4.8      71.6   330   F  1   4400

13 18 30  J1425+3946   16 29 48  63.2 -61.5  2.1     100.3    52   1  9   4400  13 18 30
13 24 00  ---          16 35 18  62.2 -61.9  2.2      99.0   330   F  1   6600

13 26 00  1611+343     16 37 19  83.9 -52.8  0.4     124.0    75   1  9   6600  13 26 00
13 31 30  ---          16 42 50  82.9 -57.9  0.5     118.2   330   F  1   8800

13 31 30  J1719+4803   16 42 50  71.2  19.4 -0.6    -154.7   -54   1  9   8800  13 31 30
13 37 00  ---          16 48 21  71.6  16.7 -0.5    -158.3   276   F  1  11000

13 37 00  J1745+4059   16 48 21  74.5  44.2 -1.0    -127.4   -20   1  9  11000  13 37 00
13 42 30  ---          16 53 52  75.3  41.6 -0.9    -130.8   310   F  1  13200

13 42 30  J1800+388    16 53 52  74.1  54.6 -1.1    -115.9   -11   1  9  13200  13 42 30
13 48 00  ---          16 59 22  75.1  52.7 -1.0    -118.5   319   F  1  15400
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

13 48 00  J1819+3845   16 59 22  71.7  58.3 -1.3    -110.2    -9   1  9  15400  13 48 00
13 53 30  ---          17 04 53  72.7  57.0 -1.2    -112.3   321   F  1  17600

13 53 30  J1923+3941   17 04 53  60.4  62.6 -2.3     -96.9   -27   1 10  17600  13 53 30
13 59 00  ---          17 10 24  61.5  62.3 -2.2     -98.0   303   R  1  15400

14 01 00  J1810+5029   17 12 25  67.4  24.5 -1.0    -145.8    93   1 10  15400  14 01 00
14 06 30  ---          17 17 55  67.9  22.6 -0.9    -148.7   330   R  1  13200

14 06 30  J1942+5154   17 17 55  56.1  40.7 -2.4    -114.7   -26   1 10  13200  14 06 30
14 12 00  ---          17 23 26  56.9  40.0 -2.3    -116.3   304   R  1  11000

14 12 00  J1949+506    17 23 26  56.3  42.9 -2.4    -112.5    -4   1 10  11000  14 12 00
14 17 30  ---          17 28 57  57.1  42.2 -2.3    -114.1   326   R  1   8800

14 19 30  J1950+6108   17 30 58  51.9  26.6 -2.3    -127.0   108   1 10   8800  14 19 30
14 25 00  ---          17 36 28  52.4  25.9 -2.2    -128.8   330   R  1   6600

14 27 00  J2248+7054   17 38 29  32.9  22.3 -5.2     -90.8    79   1 10   6600  14 27 00
14 32 30  ---          17 44 00  33.3  22.3 -5.1     -92.1   330   R  1   4400

14 34 30  J0955+5728   17 46 00  12.4 -29.2  7.8      51.3    76   1 10   4400  14 34 30
14 40 00  ---          17 51 31  11.8 -28.7  7.9      50.3   330   R  1   2200

14 53 00  J1026+5141   18 04 33  10.3 -35.0  7.6      52.7   774   1 10   2200  14 53 00
14 58 30  ---          18 10 04   9.6 -34.4  7.7      51.7   330   R  1      0

14 58 30  J1109+3830   18 10 04   8.2 -49.7  7.0      57.1   -12   1 11      0  14 58 30
15 05 00  ---          18 16 35   7.1 -49.0  7.1      56.1   378   F  1   2600

15 05 00  J1137+3442   18 16 35   9.7 -55.3  6.7      59.3    -7   1 11   2600  15 05 00
15 11 30  ---          18 23 06   8.6 -54.6  6.8      58.5   383   F  1   5200

15 14 30  J1425+3946   18 26 07  41.0 -61.9  4.0      81.1   113   1 11   5200  15 14 30
15 23 30  ---          18 35 08  39.3 -61.6  4.2      79.9   540   F  1   8800

15 23 30  1611+343     18 35 08  60.1 -73.7  2.4      86.9   -44   1 11   8800  15 23 30
15 33 30  ---          18 45 10  58.0 -73.4  2.5      85.7   556   F  1  12800

15 33 30  J1719+4803   18 45 10  66.1 -37.0  1.4     129.2   -26   1 11  12800  15 33 30
15 40 00  ---          18 51 41  65.3 -38.7  1.5     126.5   364   F  1  15400
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

15 42 00  J1745+4059   18 53 41  72.8 -48.4  1.1     121.6   103   1 11  15400  15 42 00
15 47 30  ---          18 59 12  71.9 -50.1  1.2     119.0   330   F  1  17600

15 47 30  J1800+388    18 59 12  75.4 -51.9  1.0     119.7    -9   1 12  17600  15 47 30
15 53 00  ---          19 04 43  74.5 -53.9  1.1     116.9   321   R  1  15400

15 53 00  J1819+3845   19 04 43  77.7 -45.8  0.8     127.7    -8   1 12  15400  15 53 00
15 58 30  ---          19 10 14  76.8 -48.7  0.8     124.1   322   R  1  13200

15 58 30  J1923+3941   19 10 14  80.5  16.1 -0.2    -162.0   -45   1 12  13200  15 58 30
16 07 30  ---          19 19 15  80.9   5.5 -0.1    -173.8   495   R  1   9600

16 09 30  J1810+5029   19 21 16  66.2 -28.6  1.2     139.7    89   1 12   9600  16 09 30
16 16 00  ---          19 27 47  65.5 -30.5  1.3     136.7   390   R  1   7000

16 16 00  J1942+5154   19 27 47  68.6   6.1 -0.2    -171.4   -26   1 12   7000  16 16 00
16 22 30  ---          19 34 18  68.7   3.4 -0.1    -175.2   364   R  1   4400

16 22 30  J1949+506    19 34 18  69.7   7.1 -0.3    -170.4    -4   1 12   4400  16 22 30
16 28 00  ---          19 39 49  69.9   4.6 -0.2    -173.8   326   R  1   2200

16 32 00  J2248+7054   19 43 49  42.6  18.6 -3.1    -122.7   183   1 12   2200  16 32 00
16 37 30  ---          19 49 20  43.0  18.3 -3.0    -124.3   330   R  1      0

16 37 30  J1950+6108   19 49 20  59.5   0.3  0.0    -179.4   -35   1 13      0  16 37 30
16 43 00  ---          19 54 51  59.5  -1.0  0.1     178.3   295   F  1   2200

16 43 00  J1810+5029   19 54 51  62.2 -36.9  1.7     125.7   -26   1 13   2200  16 43 00
16 48 30  ---          20 00 22  61.5 -38.0  1.8     123.7   304   F  1   4400

16 48 30  J1923+3941   20 00 22  78.3 -37.0  0.6     137.7   -36   1 13   4400  16 48 30
16 54 00  ---          20 05 53  77.5 -40.6  0.7     133.3   294   F  1   6600

16 54 00  J1819+3845   20 05 53  66.8 -62.3  1.8     102.3   -24   1 13   6600  16 54 00
16 59 30  ---          20 11 24  65.7 -62.9  1.9     100.9   306   F  1   8800

16 59 30  J1800+388    20 11 24  62.0 -64.0  2.2      96.9    -9   1 13   8800  16 59 30
17 05 00  ---          20 16 55  61.0 -64.3  2.3      95.8   321   F  1  11000

17 05 00  J1745+4059   20 16 55  57.9 -60.6  2.5      96.6    -8   1 13  11000  17 05 00
17 10 30  ---          20 22 26  56.8 -60.8  2.6      95.5   322   F  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

17 10 30  J1719+4803   20 22 26  51.3 -49.9  3.0      99.8   -13   1 13  13200  17 10 30
17 16 00  ---          20 27 57  50.4 -50.2  3.1      98.6   317   F  1  15400

17 31 00  J2248+7054   20 42 59  46.2  14.2 -2.1    -139.8   855   1 13  15400  17 31 00
17 36 30  ---          20 48 30  46.5  13.7 -2.0    -141.5   330   F  1  17600

17 39 30  J2256+4309   20 51 30  62.2  54.4 -2.1    -106.3   147   1 14  17600  17 39 30
17 45 00  ---          20 57 01  63.1  53.8 -2.0    -107.8   330   R  1  15400

17 45 00  J2339+5003   20 57 01  54.2  45.4 -2.7    -107.3   -20   1 14  15400  17 45 00
17 50 30  ---          21 02 32  55.0  44.9 -2.6    -108.8   310   R  1  13200

17 50 30  J0005+544    21 02 32  49.9  40.1 -3.0    -107.5   -12   1 14  13200  17 50 30
17 56 00  ---          21 08 03  50.6  39.7 -2.9    -108.9   318   R  1  11000

17 56 00  J0027+599    21 08 03  46.0  33.3 -3.3    -109.0   -11   1 14  11000  17 56 00
18 01 30  ---          21 13 34  46.7  33.0 -3.2    -110.5   319   R  1   8800

18 03 30  J0044+3919   21 15 34  46.9  63.6 -3.5     -84.9    98   1 14   8800  18 03 30
18 09 00  ---          21 21 05  48.0  63.7 -3.4     -85.7   330   R  1   6600

18 11 00  J0139+3928   21 23 06  38.0  61.7 -4.3     -78.8    98   1 14   6600  18 11 00
18 16 30  ---          21 28 37  39.0  61.9 -4.2     -79.5   330   R  1   4400

18 16 30  J0148+4215   21 28 37  37.7  58.0 -4.3     -80.3    -5   1 14   4400  18 16 30
18 22 00  ---          21 34 07  38.7  58.2 -4.2     -81.1   325   R  1   2200

18 24 00  J0202+420    21 36 08  36.5  57.9 -4.4     -79.3   114   1 14   2200  18 24 00
18 29 30  ---          21 41 39  37.5  58.2 -4.4     -80.1   330   R  1      0

-----------  Tape Change ------------

18 29 30  J0204+4005   21 41 39  36.9  60.6 -4.4     -78.4    -4   2  1      0  18 29 30
18 35 00  ---          21 47 10  37.9  60.8 -4.3     -79.1   326   F  1   2200

18 43 00  J1719+4803   21 55 11  35.9 -50.3  4.6      82.2   404   2  1   2200  18 43 00
18 48 30  ---          22 00 42  35.0 -50.1  4.7      81.3   330   F  1   4400

18 48 30  J1745+4059   22 00 42  38.4 -59.8  4.3      80.0    -9   2  1   4400  18 48 30
18 54 00  ---          22 06 13  37.4 -59.5  4.3      79.3   321   F  1   6600

18 54 00  J1800+388    22 06 13  39.8 -63.0  4.1      79.5    -7   2  1   6600  18 54 00
18 59 30  ---          22 11 44  38.7 -62.7  4.2      78.8   323   F  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

18 59 30  J1819+3845   22 11 44  42.4 -63.6  3.9      81.2    -9   2  1   8800  18 59 30
19 05 00  ---          22 17 14  41.3 -63.4  4.0      80.5   321   F  1  11000

19 05 00  J1923+3941   22 17 14  53.8 -63.4  2.9      90.7   -27   2  1  11000  19 05 00
19 10 30  ---          22 22 45  52.7 -63.4  3.0      89.8   303   F  1  13200

19 10 30  J1810+5029   22 22 45  39.9 -47.7  4.2      88.2   -28   2  1  13200  19 10 30
19 16 00  ---          22 28 16  39.0 -47.6  4.3      87.2   302   F  1  15400

19 18 00  J1942+5154   22 30 17  52.7 -42.9  2.8     108.2    91   2  1  15400  19 18 00
19 23 30  ---          22 35 48  51.9 -43.4  2.9     106.8   330   F  1  17600

19 23 30  J1949+506    22 35 48  53.4 -44.7  2.8     107.1    -5   2  2  17600  19 23 30
19 29 00  ---          22 41 18  52.5 -45.1  2.9     105.7   325   R  1  15400

19 29 00  J1950+6108   22 41 18  48.7 -29.7  2.8     117.9   -12   2  2  15400  19 29 00
19 34 30  ---          22 46 49  48.1 -30.2  2.9     116.3   318   R  1  13200

19 37 30  J2248+7054   22 49 50  49.7  -0.2  0.0     179.4   158   2  2  13200  19 37 30
19 43 00  ---          22 55 21  49.7  -0.9  0.1     177.5   330   R  1  11000

19 43 00  J2256+4309   22 55 21  77.5   1.4  0.0    -178.4   -58   2  2  11000  19 43 00
19 48 30  ---          23 00 52  77.4  -3.3  0.1     176.1   272   R  1   8800

19 48 30  J2339+5003   23 00 52  69.3  17.5 -0.6    -156.2   -18   2  2   8800  19 48 30
19 54 00  ---          23 06 23  69.6  15.2 -0.5    -159.4   312   R  1   6600

19 54 00  J0005+544    23 06 23  63.9  19.6 -1.0    -150.3   -13   2  2   6600  19 54 00
19 59 30  ---          23 11 53  64.3  18.0 -0.9    -152.8   317   R  1   4400

19 59 30  J0027+599    23 11 53  58.1  17.7 -1.3    -148.4   -15   2  2   4400  19 59 30
20 05 00  ---          23 17 24  58.4  16.6 -1.2    -150.6   315   R  1   2200

20 07 00  J0044+3919   23 19 25  70.6  57.6 -1.4    -110.0    91   2  2   2200  20 07 00
20 12 30  ---          23 24 56  71.6  56.5 -1.3    -112.0   330   R  1      0

20 12 30  J0139+3928   23 24 56  61.4  62.8 -2.2     -97.5   -22   2  3      0  20 12 30
20 18 00  ---          23 30 26  62.4  62.5 -2.1     -98.7   308   F  1   2200

20 18 00  J0148+4215   23 30 26  60.1  57.5 -2.3    -101.5    -7   2  3   2200  20 18 00
20 23 30  ---          23 35 57  61.1  57.0 -2.2    -102.8   323   F  1   4400
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

20 23 30  J0202+420    23 35 57  58.6  58.3 -2.4     -99.3    -7   2  3   4400  20 23 30
20 29 00  ---          23 41 28  59.6  58.0 -2.4    -100.5   323   F  1   6600

20 29 00  J0204+4005   23 41 28  59.7  62.0 -2.4     -96.9    -5   2  3   6600  20 29 00
20 34 30  ---          23 46 59  60.7  61.7 -2.3     -98.0   325   F  1   8800

20 39 30  DA193        23 52 00  18.4  54.1 -6.1     -65.1   213   2  3   8800  20 39 30
20 45 00  ---          23 57 31  19.4  54.5 -6.0     -65.8   330   F  1  11000

20 53 00  J1719+4803   00 05 32  15.3 -42.8  6.8      61.0   413   2  3  11000  20 53 00
20 58 30  ---          00 11 03  14.5 -42.3  6.9      60.1   330   F  1  13200

20 58 30  J1745+4059   00 11 03  15.2 -51.0  6.4      62.4    -8   2  3  13200  20 58 30
21 04 00  ---          00 16 34  14.3 -50.5  6.5      61.6   322   F  1  15400

21 06 00  J1800+388    00 18 34  15.4 -53.7  6.3      62.9   116   2  3  15400  21 06 00
21 11 30  ---          00 24 05  14.5 -53.2  6.4      62.1   330   F  1  17600

21 11 30  J1819+3845   00 24 05  17.8 -55.0  6.1      64.6    -9   2  4  17600  21 11 30
21 17 00  ---          00 29 36  16.8 -54.5  6.2      63.9   321   R  1  15400

21 17 00  J1923+3941   00 29 36  28.7 -58.6  5.1      72.5   -26   2  4  15400  21 17 00
21 22 30  ---          00 35 07  27.7 -58.2  5.2      71.8   304   R  1  13200

21 22 30  J1810+5029   00 35 07  19.5 -42.2  6.4      65.2   -18   2  4  13200  21 22 30
21 28 00  ---          00 40 38  18.7 -41.8  6.5      64.3   312   R  1  11000

21 28 00  J1942+5154   00 40 38  32.8 -45.1  5.0      80.8   -30   2  4  11000  21 28 00
21 33 30  ---          00 46 09  32.0 -44.9  5.1      79.8   300   R  1   8800

21 33 30  J1949+506    00 46 09  32.9 -46.5  4.9      80.4    -4   2  4   8800  21 33 30
21 39 00  ---          00 51 40  32.1 -46.4  5.0      79.4   326   R  1   6600

21 39 00  J1950+6108   00 51 40  33.5 -34.0  5.0      86.3   -10   2  4   6600  21 39 00
21 44 30  ---          00 57 11  32.9 -34.0  5.1      85.1   320   R  1   4400

21 44 30  J2248+7054   00 57 11  46.0 -14.6  2.2     138.5   -28   2  4   4400  21 44 30
21 50 00  ---          01 02 42  45.7 -15.0  2.2     136.9   302   R  1   2200

21 52 00  J2256+4309   01 04 42  61.8 -54.7  2.1     105.7    86   2  4   2200  21 52 00
21 57 30  ---          01 10 13  60.8 -55.2  2.2     104.3   330   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

21 57 30  J2339+5003   01 10 13  64.1 -34.8  1.5     130.2   -16   2  5      0  21 57 30
22 03 00  ---          01 15 44  63.5 -36.0  1.6     128.0   314   F  1   2200

22 03 00  J0005+544    01 15 44  63.0 -22.9  1.2     144.9   -11   2  5   2200  22 03 00
22 08 30  ---          01 21 15  62.5 -24.3  1.3     142.5   319   F  1   4400

22 08 30  J0027+599    01 21 15  59.3 -13.3  0.9     156.7    -9   2  5   4400  22 08 30
22 14 00  ---          01 26 46  59.0 -14.5  1.0     154.5   321   F  1   6600

22 14 00  J0044+3919   01 26 46  77.8 -41.9  0.7     132.1   -40   2  5   6600  22 14 00
22 19 30  ---          01 32 16  76.9 -45.0  0.8     128.1   290   F  1   8800

22 19 30  J0139+3928   01 32 16  81.1   8.4 -0.1    -170.6   -38   2  5   8800  22 19 30
22 25 00  ---          01 37 47  81.2   1.5  0.0    -178.3   292   F  1  11000

22 25 00  J0148+4215   01 37 47  78.2   9.9 -0.2    -168.4    -8   2  5  11000  22 25 00
22 30 30  ---          01 43 18  78.3   5.0 -0.1    -174.2   322   F  1  13200

22 30 30  J0202+420    01 43 18  77.9  17.4 -0.3    -159.7   -10   2  5  13200  22 30 30
22 36 00  ---          01 48 49  78.2  12.7 -0.2    -165.2   320   F  1  15400

22 40 00  J1942+5154   01 52 50  22.1 -41.7  6.2      68.1   126   2  5  15400  22 40 00
22 45 30  ---          01 58 21  21.3 -41.4  6.3      67.2   330   F  1  17600

22 45 30  J1949+506    01 58 21  21.9 -43.0  6.1      68.0    -3   2  6  17600  22 45 30
22 51 00  ---          02 03 52  21.1 -42.7  6.2      67.0   327   R  1  15400

22 51 00  J1950+6108   02 03 52  25.0 -32.1  6.2      71.4   -10   2  6  15400  22 51 00
22 56 30  ---          02 09 23  24.4 -31.9  6.3      70.3   320   R  1  13200

22 56 30  J2248+7054   02 09 23  41.4 -19.6  3.4     118.0   -36   2  6  13200  22 56 30
23 02 00  ---          02 14 53  41.0 -19.9  3.4     116.5   294   R  1  11000

23 02 00  J2256+4309   02 14 53  49.1 -57.9  3.3      90.9   -27   2  6  11000  23 02 00
23 07 30  ---          02 20 24  48.1 -58.0  3.4      90.0   303   R  1   8800

23 07 30  J2339+5003   02 20 24  54.3 -45.3  2.7     107.5   -14   2  6   8800  23 07 30
23 13 00  ---          02 25 55  53.4 -45.8  2.8     106.1   316   R  1   6600

23 13 00  J0005+544    02 25 55  55.4 -36.2  2.3     119.1    -8   2  6   6600  23 13 00
23 18 30  ---          02 31 26  54.7 -36.8  2.4     117.4   322   R  1   4400
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  22 Feb 2000   Day  53 ---

23 18 30  J0204+4005   02 31 26  79.0 -28.6  0.5     147.4   -51   2  6   4400  23 18 30
23 24 00  ---          02 36 57  78.4 -33.0  0.5     142.2   279   R  1   2200

23 26 00  J0027+599    02 38 57  53.3 -27.1  2.2     128.3    68   2  6   2200  23 26 00
23 31 30  ---          02 44 28  52.8 -27.8  2.3     126.6   330   R  1      0

23 31 30  J0044+3919   02 44 28  64.1 -62.2  2.0     100.3   -25   2  7      0  23 31 30
23 37 00  ---          02 49 59  63.0 -62.6  2.1      99.1   305   F  1   2200

23 37 00  J0139+3928   02 49 59  73.0 -53.8  1.2     115.9   -22   2  7   2200  23 37 00
23 42 30  ---          02 55 30  72.1 -55.3  1.3     113.6   308   F  1   4400

23 42 30  J0148+4215   02 55 30  72.3 -44.4  1.1     125.6    -9   2  7   4400  23 42 30
23 48 00  ---          03 01 01  71.5 -46.2  1.2     122.9   321   F  1   6600

23 48 00  J0202+420    03 01 01  73.6 -41.5  1.0     129.7    -6   2  7   6600  23 48 00
23 53 30  ---          03 06 32  72.8 -43.7  1.1     126.7   324   F  1   8800

23 53 30  J0204+4005   03 06 32  74.2 -49.1  1.0     121.8    -6   2  7   8800  23 53 30
23 59 00  ---          03 12 03  73.3 -51.0  1.1     119.1   324   F  1  11000

 --- Wed  23 Feb 2000   Day  54 ---

00 04 00  DA193        03 17 04  56.7  63.0 -2.6     -93.4   222   2  7  11000  00 04 00
00 09 30  ---          03 22 35  57.7  62.9 -2.5     -94.4   330   F  1  13200

00 17 30  J0943+3614   03 30 36  15.2  56.6 -6.2     -62.9   393   2  7  13200  00 17 30
00 23 00  ---          03 36 07  16.2  57.1 -6.1     -63.6   330   F  1  15400

00 26 00  J0955+5728   03 39 07  23.4  35.7 -6.3     -69.2   164   2  7  15400  00 26 00
00 31 30  ---          03 44 38  24.1  36.0 -6.2     -70.3   330   F  1  17600

00 31 30  J1000+4223   03 44 38  17.5  50.6 -6.3     -64.2   -15   2  8  17600  00 31 30
00 37 00  ---          03 50 09  18.4  51.0 -6.2     -64.9   315   R  1  15400

00 37 00  J1026+5141   03 50 09  18.4  40.2 -6.6     -63.6    -9   2  8  15400  00 37 00
00 42 30  ---          03 55 40  19.2  40.6 -6.5     -64.5   321   R  1  13200

00 42 30  J1109+3830   03 55 40   6.0  48.2 -7.2     -55.1   -28   2  8  13200  00 42 30
00 48 00  ---          04 01 11   6.8  48.9 -7.1     -55.9   302   R  1  11000

01 09 00  J1942+5154   04 22 14   3.4 -28.3  8.7  H   41.3  1207   2  8  11000  01 09 00
01 14 30  ---          04 27 45   2.9 -27.6  8.8  H   40.3     0   R  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  23 Feb 2000   Day  54 ---

01 14 30  J1949+506    04 27 45   2.7 -29.3  8.6  H   41.6    -3   2  8   8800  01 14 30
01 20 00  ---          04 33 16   2.1 -28.6  8.7  D   40.6     0   R  1   6600

01 22 00  J1950+6108   04 35 16  10.0 -21.7  8.7      41.1   103   2  8   6600  01 22 00
01 27 30  ---          04 40 47   9.5 -21.1  8.8      40.0   330   R  1   4400

01 27 30  J2248+7054   04 40 47  29.4 -22.0  5.9      80.7   -42   2  8   4400  01 27 30
01 33 00  ---          04 46 18  28.9 -21.9  6.0      79.4   288   R  1   2200

01 33 00  J2256+4309   04 46 18  22.2 -51.9  5.8      68.2   -22   2  8   2200  01 33 00
01 38 30  ---          04 51 49  21.3 -51.5  5.9      67.4   308   R  1      0

01 38 30  J2339+5003   04 51 49  30.2 -46.7  5.2      77.2   -20   2  9      0  01 38 30
01 44 00  ---          04 57 20  29.4 -46.4  5.3      76.2   310   F  1   2200

01 44 00  J0005+544    04 57 20  34.1 -42.2  4.9      83.6   -11   2  9   2200  01 44 00
01 49 30  ---          05 02 51  33.3 -42.0  5.0      82.6   319   F  1   4400

01 49 30  J0027+599    05 02 51  36.6 -35.5  4.6      90.9    -9   2  9   4400  01 49 30
01 55 00  ---          05 08 22  35.9 -35.5  4.7      89.7   321   F  1   6600

01 57 00  J0044+3919   05 10 22  36.1 -61.3  4.4      77.4   101   2  9   6600  01 57 00
02 02 30  ---          05 15 53  35.0 -61.0  4.5      76.7   330   F  1   8800

02 02 30  J0139+3928   05 15 53  45.4 -63.2  3.6      84.0   -23   2  9   8800  02 02 30
02 08 00  ---          05 21 24  44.4 -63.0  3.7      83.2   307   F  1  11000

02 10 00  J0148+4215   05 23 24  46.0 -59.2  3.6      87.2   115   2  9  11000  02 10 00
02 15 30  ---          05 28 55  45.0 -59.1  3.7      86.3   330   F  1  13200

02 15 30  J0202+420    05 28 55  47.6 -59.6  3.4      88.3    -7   2  9  13200  02 15 30
02 21 00  ---          05 34 26  46.6 -59.5  3.5      87.5   323   F  1  15400

02 21 00  J0204+4005   05 34 26  46.7 -62.4  3.5      85.5    -4   2  9  15400  02 21 00
02 26 30  ---          05 39 57  45.7 -62.3  3.6      84.7   326   F  1  17600

02 31 30  DA193        05 44 58  80.6  12.5 -0.2    -166.0   228   2 10  17600  02 31 30
02 37 00  ---          05 50 29  80.8   6.0 -0.1    -173.2   330   R  1  15400

02 42 00  J0943+3614   05 55 30  42.8  67.2 -3.8     -79.5   222   2 10  15400  02 42 00
02 47 30  ---          06 01 00  43.9  67.4 -3.7     -80.1   330   R  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  23 Feb 2000   Day  54 ---

02 47 30  J1000+4223   06 01 00  41.5  58.5 -4.0     -83.5    -8   2 10  13200  02 47 30
02 53 00  ---          06 06 31  42.5  58.7 -3.9     -84.3   322   R  1  11000

02 53 00  J0955+5728   06 06 31  42.8  38.1 -3.8     -99.3   -16   2 10  11000  02 53 00
02 58 30  ---          06 12 02  43.6  37.9 -3.7    -100.6   314   R  1   8800

02 58 30  J1026+5141   06 12 02  39.6  46.1 -4.2     -88.8   -10   2 10   8800  02 58 30
03 04 00  ---          06 17 33  40.4  46.1 -4.1     -89.9   320   R  1   6600

03 06 00  J1109+3830   06 19 34  31.3  60.9 -4.8     -73.8   100   2 10   6600  03 06 00
03 11 30  ---          06 25 04  32.3  61.2 -4.7     -74.5   330   R  1   4400

03 11 30  J1137+3442   06 25 04  25.9  63.4 -5.2     -69.3   -15   2 10   4400  03 11 30
03 17 00  ---          06 30 35  27.0  63.8 -5.1     -69.9   315   R  1   2200

03 30 30  J2256+4309   06 44 08   3.8 -40.7  7.8  H   50.3   738   2 10   2200  03 30 30
03 36 00  ---          06 49 38   3.0 -40.1  7.9  H   49.4     0   R  1      0

03 36 00  J2339+5003   06 49 38  12.9 -38.9  7.2      57.3   -22   2 11      0  03 36 00
03 41 30  ---          06 55 09  12.2 -38.4  7.3      56.3   308   F  1   2200

03 41 30  J0005+544    06 55 09  17.8 -36.6  6.8      61.9   -13   2 11   2200  03 41 30
03 47 00  ---          07 00 40  17.1 -36.2  6.9      60.9   317   F  1   4400

03 47 00  J0027+599    07 00 40  22.2 -32.3  6.6      66.9   -12   2 11   4400  03 47 00
03 52 30  ---          07 06 11  21.6 -32.0  6.7      65.8   318   F  1   6600

03 52 30  J0044+3919   07 06 11  15.1 -52.9  6.4      62.5   -16   2 11   6600  03 52 30
03 58 00  ---          07 11 42  14.1 -52.4  6.5      61.8   314   F  1   8800

04 00 00  J0139+3928   07 13 42  23.4 -56.7  5.6      68.7   100   2 11   8800  04 00 00
04 05 30  ---          07 19 13  22.4 -56.3  5.7      68.0   330   F  1  11000

04 05 30  J0148+4215   07 19 13  25.1 -54.2  5.5      70.5    -7   2 11  11000  04 05 30
04 11 00  ---          07 24 44  24.2 -53.8  5.6      69.7   323   F  1  13200

04 11 00  J0202+420    07 24 44  26.5 -54.9  5.4      71.6    -7   2 11  13200  04 11 00
04 16 30  ---          07 30 15  25.6 -54.5  5.5      70.8   323   F  1  15400

04 16 30  J0204+4005   07 30 15  25.1 -56.7  5.4      70.1    -3   2 11  15400  04 16 30
04 22 00  ---          07 35 46  24.2 -56.3  5.5      69.4   327   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Evolution of the smallest radio sources
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  23 Feb 2000   Day  54 ---

04 43 30  J2339+5003   07 57 20   4.4 -32.0  8.3  H   45.3  1249   2 12  17600  04 43 30
04 49 00  ---          08 02 50   3.8 -31.4  8.4  H   44.3     0   R  1  15400

04 51 00  J0005+544    08 04 51   9.5 -30.7  8.0      49.1   107   2 12  15400  04 51 00
04 56 30  ---          08 10 22   8.9 -30.2  8.1      48.1   330   R  1  13200

04 56 30  J0027+599    08 10 22  14.7 -27.7  7.7      53.2   -14   2 12  13200  04 56 30
05 02 00  ---          08 15 53  14.1 -27.3  7.8      52.1   316   R  1  11000

05 02 00  J0044+3919   08 15 53   3.7 -45.6  7.5  H   52.6   -23   2 12  11000  05 02 00
05 07 30  ---          08 21 23   2.9 -44.9  7.6  H   51.8     0   R  1   8800

05 07 30  J0139+3928   08 21 23  11.6 -50.8  6.7      59.7   -20   2 12   8800  05 07 30
05 13 00  ---          08 26 54  10.7 -50.2  6.8      58.9   310   R  1   6600

05 13 00  J0148+4215   08 26 54  13.7 -48.7  6.6      60.9    -8   2 12   6600  05 13 00
05 18 30  ---          08 32 25  12.8 -48.2  6.7      60.0   322   R  1   4400

05 18 30  J0202+420    08 32 25  15.0 -49.6  6.5      62.0    -6   2 12   4400  05 18 30
05 24 00  ---          08 37 56  14.1 -49.1  6.6      61.3   324   R  1   2200

05 24 00  J0204+4005   08 37 56  13.4 -51.1  6.6      61.0    -3   2 12   2200  05 24 00
05 29 30  ---          08 43 27  12.4 -50.5  6.7      60.2   327   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: jdt.1cm
   Matches group v1cm_b3 in ./freq.dat

   Setup group:    8         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO= 21500.00 21500.00 21500.00 21500.00
   Net SB=        L        U        L        U
   Pol.  =     LCP      LCP      LCP      LCP 
   BBC   =        1        1        2        2
   BBC SB=        L        U        L        U
   IF    =       D        D        D        D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1     15.4     12.4

  The following frequency sets based on this setup were used.

   Frequency Set:   8  Setup file default.  Used pcal sets:   1
   LO sum=  22207.49 22207.49 22223.49 22223.49
   BBC fr=    707.49   707.49   723.49   723.49
   Bandwd=     8.000    8.000    8.000    8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=   490   490  6490  6490     0     0     0     0
    PCALFR2=   510   510  6510  6510     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- Evolution of the smallest radio sources
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * J0005+544         00 02 29.052923   * 00 05 04.360000     00 05 02.478137 
                     54 11 43.20071    * 54 28 24.94000      54 28 26.26210 
                     From catalog imbedded in main SCHED input file.

 * J0027+599         00 24 16.670114   * 00 27 03.290000     00 27 01.304161 
                     59 42 17.40578    * 59 58 52.98000      59 58 56.34036 
                     From catalog imbedded in main SCHED input file.

 * J0044+3919        00 41 53.554105   * 00 44 37.541100     00 44 36.104819 
                     39 03 23.74561    * 39 19 47.88500      39 19 46.99627 
                     From catalog imbedded in main SCHED input file.

 * J0139+3928        01 36 05.375440   * 01 39 01.745800     01 39 00.553190 
                     39 12 42.23949    * 39 27 54.75000      39 27 55.03631 
                     From catalog imbedded in main SCHED input file.

 * J0148+4215        01 45 43.563051   * 01 48 44.576000     01 48 43.409068 
                     42 00 25.18999    * 42 15 19.41200      42 15 20.70028 
                     From catalog imbedded in main SCHED input file.

 * J0202+420         01 59 39.580574   * 02 02 43.650000     02 02 42.559531 
                     41 50 51.28327    * 42 05 16.34000      42 05 17.82610 
                     From catalog imbedded in main SCHED input file.

 * J0204+4005        02 01 02.904562   * 02 04 05.196000     02 04 04.128100 
                     39 50 41.49608    * 40 05 03.51600      40 05 04.41074 
                     From catalog imbedded in main SCHED input file.

 * J0943+3614        09 40 17.512476   * 09 43 19.152300     09 43 20.114589 
                     36 28 37.30558    * 36 14 52.06900      36 14 46.63297 
                     From catalog imbedded in main SCHED input file.

 * J0955+5728        09 51 59.925945   * 09 55 28.760600     09 55 30.243630 
                     57 42 50.93365    * 57 28 37.29800      57 28 33.58869 
                     From catalog imbedded in main SCHED input file.

 * J1000+4223        09 57 10.521336   * 10 00 15.195800     10 00 16.248183 
                     42 38 29.71907    * 42 24 04.86600      42 23 59.45698 
                     From catalog imbedded in main SCHED input file.

 * J1026+5141        10 23 19.684123   * 10 26 27.674600     10 26 28.930677 
                     51 56 30.83963    * 51 41 14.00000      51 41 08.30208 
                     From catalog imbedded in main SCHED input file.

 * J1109+3830        11 06 53.319482   * 11 09 39.033900     11 09 39.964744 
                     38 47 38.81261    * 38 31 22.31900      38 31 14.51045 
                     From catalog imbedded in main SCHED input file.

 * J1137+3442        11 34 30.513521   * 11 37 09.165000     11 37 09.996263 
                     34 58 32.26116    * 34 41 55.90800      34 41 47.45403 
                     From catalog imbedded in main SCHED input file.

 * J1425+3946        14 23 48.399587   * 14 25 49.189700     14 25 49.361583 
                     40 00 23.43167    * 39 46 55.00600      39 46 42.69984 
                     From catalog imbedded in main SCHED input file.

 * J1719+4803        17 18 17.710790   * 17 19 38.251500     17 19 37.334383 
                     48 07 10.61134    * 48 04 12.25600      48 03 58.62479 
                     From catalog imbedded in main SCHED input file.

 * J1745+4059        17 43 52.618572   * 17 45 28.452300     17 45 27.435798 
                     41 00 58.69948    * 40 59 51.82200      40 59 39.50405 
                     From catalog imbedded in main SCHED input file.

 * J1800+388         17 58 44.708592   * 18 00 24.770000     18 00 23.688107 
                     38 48 32.47568    * 38 48 30.70000      38 48 18.93180 
                     From catalog imbedded in main SCHED input file.

 * J1810+5029        18 09 20.647427   * 18 10 33.547200     18 10 32.286441 
                     50 28 12.51248    * 50 28 56.07300      50 28 43.14404 
                     From catalog imbedded in main SCHED input file.

 * J1819+3845        18 17 46.174716   * 18 19 26.546400     18 19 25.367898 
                     38 43 40.45829    * 38 45 01.77400      38 44 50.32971 
                     From catalog imbedded in main SCHED input file.

 * J1923+3941        19 22 06.665161   * 19 23 48.706200     19 23 47.233504 
                     39 35 11.86247    * 39 41 06.73900      39 40 56.56131 
                     From catalog imbedded in main SCHED input file.

 * J1942+5154        19 41 04.505757   * 19 42 21.493200     19 42 19.734808 
                     51 47 27.48584    * 51 54 37.75100      51 54 27.52724 
                     From catalog imbedded in main SCHED input file.

 * J1949+506         19 48 22.063767   * 19 49 43.490000     19 49 41.732820 
                     50 33 53.00185    * 50 41 31.98000      50 41 22.04726 
                     From catalog imbedded in main SCHED input file.

 * J1950+6108        19 50 00.436962   * 19 50 47.049000     19 50 44.918559 
                     61 01 23.27837    * 61 09 07.48000      61 08 57.62397 
                     From catalog imbedded in main SCHED input file.

 * J2248+7054        22 46 26.806932   * 22 48 00.771100     22 47 57.478263 
                     70 38 57.51106    * 70 54 49.28000      70 54 49.65589 
                     From catalog imbedded in main SCHED input file.

 * J2256+4309        22 54 43.496872   * 22 57 00.047700     22 56 58.251437 
                     42 54 02.22428    * 43 10 05.18400      43 10 01.90068 
                     From catalog imbedded in main SCHED input file.

 * J2339+5003        23 36 38.334361   * 23 39 04.448000     23 39 02.600668 
                     49 47 31.46783    * 50 04 08.69400      50 04 08.12522 
                     From catalog imbedded in main SCHED input file.

   J0555+3948        05 52 01.407168   * 05 55 30.805611     05 55 31.093263 
   0552+398          39 48 21.94582    * 39 48 49.16497      39 48 49.96209 
 * DA193             /aps3/sched/catalogs/sources.vlba
   J0555+39          USNO - Ref Frame 1998-6, Eubanks June 1998

   J1613+3412        16 11 47.914260   * 16 13 41.064251     16 13 40.598066 
 * 1611+343          34 20 19.83400    * 34 12 47.90902      34 12 36.09265 
   J1613+34          /aps3/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J0005+544           68.3
   J0027+599           74.6
   J0044+3919          59.7
   J0139+3928          67.6
   J0148+4215          70.7
   J0202+420           72.8
   J0204+4005          72.0
   J0943+3614         152.6
   J0955+5728         132.5
   J1000+4223         147.5
   J1026+5141         138.6
   J1109+3830         149.7
   J1137+3442         150.1
   J1425+3946         118.6
   J1719+4803          88.1
   J1745+4059          81.4
   J1800+388           77.9
   J1810+5029          81.4
   J1819+3845          74.5
   J1923+3941          64.7
   J1942+5154          70.9
   J1949+506           69.3
   J1950+6108          77.3
   J2248+7054          81.3
   J2256+4309          54.0
   J2339+5003          62.7
   DA193              114.6
   1611+343            97.3

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

