  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GP 34 = Water masers in Mrk 1066
 Exp. Code:  GP034   


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 02 July 2002                       

PI:       Alison Peck                                                     

Address:  SAO/SMA Project, Punahele Prof. Bldg, Ste 210                   
          82 Puuhonu Place                                                
          Hilo, HI  96720  USA                                            
                                                                          

Phone:    +1 808 933 6962                                                 
EMAIL:    apeck@cfa.harvard.edu                                           
Fax:      +1 808 933 6948                                                 
Phone during observation: +1 808 933 6962                                 

Observing mode: 1.3 cm spectral line observations                         

Notes:    Spectral Line Observations - Pulse Cals OFF                     
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

 Next scan frequencies: 21959.02 21959.02
 Next BBC frequencies:    759.02   759.02
 Next scan bandwidths:      8.00     8.00

18 00 00  MRK1066      20 17 57  10.3  53.1 -6.7     -59.3     0   1  1      0  18 00 00
18 01 10  ---          20 19 07  10.5  53.2 -6.7     -59.5    70   F  1    933

18 01 10  J0253+3835   20 19 07  12.6  52.4 -6.6     -60.7   -10   1  1    933  18 01 10
18 01 50  ---          20 19 47  12.7  52.4 -6.6     -60.8    30   F  1   1467

18 01 50  MRK1066      20 19 47  10.7  53.3 -6.7     -59.5   -10   1  1   1467  18 01 50
18 03 00  ---          20 20 57  10.9  53.4 -6.7     -59.7    60   F  1   2400

18 03 00  J0253+3835   20 20 57  12.9  52.5 -6.5     -60.9   -10   1  1   2400  18 03 00
18 03 40  ---          20 21 37  13.0  52.6 -6.5     -61.0    30   F  1   2933

18 03 40  MRK1066      20 21 37  11.0  53.5 -6.6     -59.8   -10   1  1   2933  18 03 40
18 04 50  ---          20 22 48  11.2  53.6 -6.6     -59.9    60   F  1   3867

18 04 50  J0253+3835   20 22 48  13.2  52.7 -6.5     -61.2   -10   1  1   3867  18 04 50
18 05 30  ---          20 23 28  13.3  52.8 -6.5     -61.3    30   F  1   4400

18 05 30  MRK1066      20 23 28  11.3  53.7 -6.6     -60.0   -10   1  1   4400  18 05 30
18 06 40  ---          20 24 38  11.5  53.8 -6.6     -60.2    60   F  1   5333

18 06 40  J0253+3835   20 24 38  13.5  52.9 -6.5     -61.4   -10   1  1   5333  18 06 40
18 07 20  ---          20 25 18  13.6  53.0 -6.5     -61.5    30   F  1   5867

18 07 20  MRK1066      20 25 18  11.6  53.9 -6.6     -60.3   -10   1  1   5867  18 07 20
18 08 30  ---          20 26 28  11.8  54.0 -6.6     -60.4    60   F  1   6800

18 08 30  J0253+3835   20 26 28  13.8  53.1 -6.4     -61.7   -10   1  1   6800  18 08 30
18 09 10  ---          20 27 08  14.0  53.1 -6.4     -61.7    30   F  1   7333

18 09 10  MRK1066      20 27 08  11.9  54.1 -6.6     -60.5   -10   1  1   7333  18 09 10
18 10 20  ---          20 28 18  12.1  54.2 -6.5     -60.6    60   F  1   8267

18 10 20  J0253+3835   20 28 18  14.2  53.2 -6.4     -61.9   -10   1  1   8267  18 10 20
18 11 00  ---          20 28 59  14.3  53.3 -6.4     -62.0    30   F  1   8800

18 11 00  MRK1066      20 28 59  12.2  54.2 -6.5     -60.7   -10   1  1   8800  18 11 00
18 12 10  ---          20 30 09  12.4  54.4 -6.5     -60.9    60   F  1   9733
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

18 12 10  J0253+3835   20 30 09  14.5  53.4 -6.4     -62.1   -10   1  1   9733  18 12 10
18 12 50  ---          20 30 49  14.6  53.5 -6.4     -62.2    30   F  1  10267

18 12 50  MRK1066      20 30 49  12.6  54.4 -6.5     -61.0   -10   1  1  10267  18 12 50
18 14 00  ---          20 31 59  12.8  54.5 -6.5     -61.1    60   F  1  11200

18 14 00  J0253+3835   20 31 59  14.8  53.6 -6.4     -62.4   -10   1  1  11200  18 14 00
18 14 40  ---          20 32 39  14.9  53.7 -6.3     -62.5    30   F  1  11733

18 14 40  MRK1066      20 32 39  12.9  54.6 -6.5     -61.2   -10   1  1  11733  18 14 40
18 15 50  ---          20 33 49  13.1  54.7 -6.4     -61.4    60   F  1  12667

18 15 50  J0253+3835   20 33 49  15.1  53.8 -6.3     -62.6   -10   1  1  12667  18 15 50
18 16 30  ---          20 34 29  15.2  53.8 -6.3     -62.7    30   F  1  13200

18 16 30  MRK1066      20 34 29  13.2  54.8 -6.4     -61.4   -10   1  1  13200  18 16 30
18 17 40  ---          20 35 40  13.4  54.9 -6.4     -61.6    60   F  1  14133

18 17 40  J0253+3835   20 35 40  15.4  53.9 -6.3     -62.9   -10   1  1  14133  18 17 40
18 18 20  ---          20 36 20  15.6  54.0 -6.3     -63.0    30   F  1  14667

18 18 20  MRK1066      20 36 20  13.5  55.0 -6.4     -61.7   -10   1  1  14667  18 18 20
18 19 30  ---          20 37 30  13.7  55.1 -6.4     -61.8    60   F  1  15600

18 19 30  J0253+3835   20 37 30  15.8  54.1 -6.3     -63.1   -10   1  1  15600  18 19 30
18 20 10  ---          20 38 10  15.9  54.2 -6.3     -63.2    30   F  1  16133

18 20 10  MRK1066      20 38 10  13.9  55.1 -6.4     -61.9   -10   1  1  16133  18 20 10
18 21 20  ---          20 39 20  14.1  55.3 -6.3     -62.1    60   F  1  17067

18 21 20  J0253+3835   20 39 20  16.1  54.3 -6.2     -63.4   -10   1  1  17067  18 21 20
18 22 00  ---          20 40 00  16.2  54.3 -6.2     -63.4    30   F  1  17600

18 22 37  MRK1066      20 40 37  14.3  55.4 -6.3     -62.2    27   1  2  17600  18 22 37
18 23 47  ---          20 41 48  14.5  55.5 -6.3     -62.4    70   R  1  16667

18 23 47  J0253+3835   20 41 48  16.5  54.5 -6.2     -63.7   -10   1  2  16667  18 23 47
18 24 27  ---          20 42 28  16.6  54.6 -6.2     -63.8    30   R  1  16133

18 24 27  MRK1066      20 42 28  14.6  55.6 -6.3     -62.4   -10   1  2  16133  18 24 27
18 25 37  ---          20 43 38  14.8  55.7 -6.3     -62.6    60   R  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

18 25 37  J0253+3835   20 43 38  16.8  54.7 -6.2     -63.9   -10   1  2  15200  18 25 37
18 26 17  ---          20 44 18  16.9  54.7 -6.2     -64.0    30   R  1  14667

18 26 17  MRK1066      20 44 18  14.9  55.7 -6.3     -62.7   -10   1  2  14667  18 26 17
18 27 27  ---          20 45 28  15.2  55.8 -6.2     -62.8    60   R  1  13733

18 27 27  J0253+3835   20 45 28  17.2  54.8 -6.1     -64.2   -10   1  2  13733  18 27 27
18 28 07  ---          20 46 08  17.3  54.9 -6.1     -64.2    30   R  1  13200

18 28 07  MRK1066      20 46 08  15.3  55.9 -6.2     -62.9   -10   1  2  13200  18 28 07
18 29 17  ---          20 47 19  15.5  56.0 -6.2     -63.1    60   R  1  12267

18 29 17  J0253+3835   20 47 19  17.5  55.0 -6.1     -64.4   -10   1  2  12267  18 29 17
18 29 57  ---          20 47 59  17.6  55.0 -6.1     -64.5    30   R  1  11733

18 29 57  MRK1066      20 47 59  15.6  56.1 -6.2     -63.1   -10   1  2  11733  18 29 57
18 31 07  ---          20 49 09  15.8  56.2 -6.2     -63.3    60   R  1  10800

18 31 07  J0253+3835   20 49 09  17.8  55.1 -6.1     -64.6   -10   1  2  10800  18 31 07
18 31 47  ---          20 49 49  17.9  55.2 -6.1     -64.7    30   R  1  10267

18 31 47  MRK1066      20 49 49  15.9  56.3 -6.2     -63.4   -10   1  2  10267  18 31 47
18 32 57  ---          20 50 59  16.1  56.4 -6.2     -63.5    60   R  1   9333

18 32 57  J0253+3835   20 50 59  18.1  55.3 -6.0     -64.9   -10   1  2   9333  18 32 57
18 33 37  ---          20 51 39  18.2  55.4 -6.0     -65.0    30   R  1   8800

18 33 37  MRK1066      20 51 39  16.3  56.4 -6.1     -63.6   -10   1  2   8800  18 33 37
18 34 47  ---          20 52 49  16.5  56.5 -6.1     -63.7    60   R  1   7867

18 34 47  J0253+3835   20 52 49  18.4  55.5 -6.0     -65.1   -10   1  2   7867  18 34 47
18 35 27  ---          20 53 30  18.6  55.5 -6.0     -65.2    30   R  1   7333

18 35 27  MRK1066      20 53 30  16.6  56.6 -6.1     -63.8   -10   1  2   7333  18 35 27
18 36 37  ---          20 54 40  16.8  56.7 -6.1     -64.0    60   R  1   6400

18 36 37  J0253+3835   20 54 40  18.8  55.6 -6.0     -65.3   -10   1  2   6400  18 36 37
18 37 17  ---          20 55 20  18.9  55.7 -6.0     -65.4    30   R  1   5867

18 37 17  MRK1066      20 55 20  16.9  56.8 -6.1     -64.0   -10   1  2   5867  18 37 17
18 38 27  ---          20 56 30  17.1  56.9 -6.1     -64.2    60   R  1   4933
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

18 38 27  J0253+3835   20 56 30  19.1  55.8 -5.9     -65.6   -10   1  2   4933  18 38 27
18 39 07  ---          20 57 10  19.2  55.8 -5.9     -65.7    30   R  1   4400

18 39 07  MRK1066      20 57 10  17.2  56.9 -6.0     -64.3   -10   1  2   4400  18 39 07
18 40 17  ---          20 58 20  17.5  57.0 -6.0     -64.4    60   R  1   3467

18 40 17  J0253+3835   20 58 20  19.4  55.9 -5.9     -65.8   -10   1  2   3467  18 40 17
18 40 57  ---          20 59 00  19.5  56.0 -5.9     -65.9    30   R  1   2933

18 41 17  J0319+4130   20 59 20  16.3  51.0 -6.3     -63.2     7   1  2   2933  18 41 17
18 44 57  ---          21 03 01  16.9  51.3 -6.3     -63.7   220   R  1      0

18 46 57  J0253+3835   21 05 01  20.6  56.5 -5.8     -66.7   106   1  1      0  18 46 57
18 47 37  ---          21 05 42  20.7  56.6 -5.8     -66.7    40   F  2    533

18 47 37  MRK1066      21 05 42  18.8  57.7 -5.9     -65.3   -10   1  1    533  18 47 37
18 48 47  ---          21 06 52  19.0  57.8 -5.9     -65.5    60   F  2   1467

18 48 47  J0253+3835   21 06 52  21.0  56.7 -5.8     -66.9   -10   1  1   1467  18 48 47
18 49 27  ---          21 07 32  21.1  56.7 -5.8     -67.0    30   F  2   2000

18 49 27  MRK1066      21 07 32  19.1  57.9 -5.9     -65.5   -10   1  1   2000  18 49 27
18 50 37  ---          21 08 42  19.3  58.0 -5.9     -65.7    60   F  2   2933

18 50 37  J0253+3835   21 08 42  21.3  56.8 -5.7     -67.1   -10   1  1   2933  18 50 37
18 51 17  ---          21 09 22  21.4  56.9 -5.7     -67.2    30   F  2   3467

18 51 17  MRK1066      21 09 22  19.5  58.0 -5.8     -65.8   -10   1  1   3467  18 51 17
18 52 27  ---          21 10 32  19.7  58.1 -5.8     -65.9    60   F  2   4400

18 52 27  J0253+3835   21 10 32  21.6  57.0 -5.7     -67.4   -10   1  1   4400  18 52 27
18 53 07  ---          21 11 12  21.7  57.0 -5.7     -67.4    30   F  2   4933

18 53 07  MRK1066      21 11 12  19.8  58.2 -5.8     -66.0   -10   1  1   4933  18 53 07
18 54 17  ---          21 12 23  20.0  58.3 -5.8     -66.1    60   F  2   5867

18 54 17  J0253+3835   21 12 23  21.9  57.1 -5.7     -67.6   -10   1  1   5867  18 54 17
18 54 57  ---          21 13 03  22.1  57.2 -5.7     -67.7    30   F  2   6400

18 54 57  MRK1066      21 13 03  20.1  58.3 -5.8     -66.2   -10   1  1   6400  18 54 57
18 56 07  ---          21 14 13  20.3  58.4 -5.8     -66.3    60   F  2   7333
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

18 56 07  J0253+3835   21 14 13  22.3  57.2 -5.7     -67.8   -10   1  1   7333  18 56 07
18 56 47  ---          21 14 53  22.4  57.3 -5.6     -67.9    30   F  2   7867

18 56 47  MRK1066      21 14 53  20.5  58.5 -5.8     -66.4   -10   1  1   7867  18 56 47
18 57 57  ---          21 16 03  20.7  58.6 -5.7     -66.6    60   F  2   8800

18 57 57  J0253+3835   21 16 03  22.6  57.4 -5.6     -68.1   -10   1  1   8800  18 57 57
18 58 37  ---          21 16 43  22.7  57.4 -5.6     -68.1    30   F  2   9333

18 58 37  MRK1066      21 16 43  20.8  58.6 -5.7     -66.6   -10   1  1   9333  18 58 37
18 59 47  ---          21 17 54  21.0  58.7 -5.7     -66.8    60   F  2  10267

18 59 47  J0253+3835   21 17 54  22.9  57.5 -5.6     -68.3   -10   1  1  10267  18 59 47
19 00 27  ---          21 18 34  23.1  57.6 -5.6     -68.4    30   F  2  10800

19 00 27  MRK1066      21 18 34  21.1  58.8 -5.7     -66.9   -10   1  1  10800  19 00 27
19 01 37  ---          21 19 44  21.4  58.9 -5.7     -67.0    60   F  2  11733

19 01 37  J0253+3835   21 19 44  23.3  57.7 -5.6     -68.5   -10   1  1  11733  19 01 37
19 02 17  ---          21 20 24  23.4  57.7 -5.5     -68.6    30   F  2  12267

19 02 17  MRK1066      21 20 24  21.5  59.0 -5.7     -67.1   -10   1  1  12267  19 02 17
19 03 27  ---          21 21 34  21.7  59.1 -5.6     -67.2    60   F  2  13200

19 03 27  J0253+3835   21 21 34  23.6  57.8 -5.5     -68.7   -10   1  1  13200  19 03 27
19 04 07  ---          21 22 14  23.7  57.9 -5.5     -68.8    30   F  2  13733

19 04 07  MRK1066      21 22 14  21.8  59.1 -5.6     -67.3   -10   1  1  13733  19 04 07
19 05 17  ---          21 23 24  22.0  59.2 -5.6     -67.4    60   F  2  14667

19 05 17  J0253+3835   21 23 24  24.0  58.0 -5.5     -69.0   -10   1  1  14667  19 05 17
19 05 57  ---          21 24 05  24.1  58.0 -5.5     -69.1    30   F  2  15200

19 05 57  MRK1066      21 24 05  22.2  59.3 -5.6     -67.5   -10   1  1  15200  19 05 57
19 07 07  ---          21 25 15  22.4  59.4 -5.6     -67.7    60   F  2  16133

19 07 07  J0253+3835   21 25 15  24.3  58.1 -5.5     -69.2   -10   1  1  16133  19 07 07
19 07 47  ---          21 25 55  24.4  58.2 -5.5     -69.3    30   F  2  16667

19 07 47  MRK1066      21 25 55  22.5  59.4 -5.6     -67.7   -10   1  1  16667  19 07 47
19 08 57  ---          21 27 05  22.7  59.5 -5.6     -67.9    60   F  2  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

19 09 34  J0253+3835   21 27 42  24.7  58.3 -5.4     -69.5    27   1  2  17600  19 09 34
19 10 14  ---          21 28 22  24.9  58.3 -5.4     -69.6    40   R  2  17067

19 10 14  MRK1066      21 28 22  23.0  59.6 -5.5     -68.0   -10   1  2  17067  19 10 14
19 11 24  ---          21 29 32  23.2  59.7 -5.5     -68.2    60   R  2  16133

19 11 24  J0253+3835   21 29 32  25.1  58.4 -5.4     -69.7   -10   1  2  16133  19 11 24
19 12 04  ---          21 30 13  25.2  58.5 -5.4     -69.8    30   R  2  15600

19 12 04  MRK1066      21 30 13  23.3  59.8 -5.5     -68.2   -10   1  2  15600  19 12 04
19 13 14  ---          21 31 23  23.5  59.9 -5.5     -68.4    60   R  2  14667

19 13 14  J0253+3835   21 31 23  25.4  58.6 -5.4     -70.0   -10   1  2  14667  19 13 14
19 13 54  ---          21 32 03  25.5  58.6 -5.4     -70.0    30   R  2  14133

19 13 54  MRK1066      21 32 03  23.6  59.9 -5.5     -68.5   -10   1  2  14133  19 13 54
19 15 04  ---          21 33 13  23.9  60.0 -5.4     -68.6    60   R  2  13200

19 15 04  J0253+3835   21 33 13  25.7  58.7 -5.3     -70.2   -10   1  2  13200  19 15 04
19 15 44  ---          21 33 53  25.9  58.8 -5.3     -70.3    30   R  2  12667

19 15 44  MRK1066      21 33 53  24.0  60.1 -5.4     -68.7   -10   1  2  12667  19 15 44
19 16 54  ---          21 35 03  24.2  60.2 -5.4     -68.8    60   R  2  11733

19 16 54  J0253+3835   21 35 03  26.1  58.8 -5.3     -70.4   -10   1  2  11733  19 16 54
19 17 34  ---          21 35 43  26.2  58.9 -5.3     -70.5    30   R  2  11200

19 17 34  MRK1066      21 35 43  24.3  60.2 -5.4     -68.9   -10   1  2  11200  19 17 34
19 18 44  ---          21 36 54  24.5  60.3 -5.4     -69.0    60   R  2  10267

19 18 44  J0253+3835   21 36 54  26.4  59.0 -5.3     -70.6   -10   1  2  10267  19 18 44
19 19 24  ---          21 37 34  26.5  59.0 -5.3     -70.7    30   R  2   9733

19 19 24  MRK1066      21 37 34  24.7  60.3 -5.4     -69.1   -10   1  2   9733  19 19 24
19 20 34  ---          21 38 44  24.9  60.4 -5.4     -69.2    60   R  2   8800

19 20 34  J0253+3835   21 38 44  26.8  59.1 -5.2     -70.9   -10   1  2   8800  19 20 34
19 21 14  ---          21 39 24  26.9  59.2 -5.2     -71.0    30   R  2   8267

19 21 14  MRK1066      21 39 24  25.0  60.5 -5.3     -69.3   -10   1  2   8267  19 21 14
19 22 24  ---          21 40 34  25.2  60.6 -5.3     -69.5    60   R  2   7333
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

19 22 24  J0253+3835   21 40 34  27.1  59.2 -5.2     -71.1   -10   1  2   7333  19 22 24
19 23 04  ---          21 41 14  27.2  59.3 -5.2     -71.2    30   R  2   6800

19 23 04  MRK1066      21 41 14  25.4  60.6 -5.3     -69.5   -10   1  2   6800  19 23 04
19 24 14  ---          21 42 25  25.6  60.7 -5.3     -69.7    60   R  2   5867

19 24 14  J0253+3835   21 42 25  27.4  59.4 -5.2     -71.3   -10   1  2   5867  19 24 14
19 24 54  ---          21 43 05  27.6  59.4 -5.2     -71.4    30   R  2   5333

19 24 54  MRK1066      21 43 05  25.7  60.8 -5.3     -69.8   -10   1  2   5333  19 24 54
19 26 04  ---          21 44 15  25.9  60.9 -5.3     -69.9    60   R  2   4400

19 26 04  J0253+3835   21 44 15  27.8  59.5 -5.2     -71.6   -10   1  2   4400  19 26 04
19 26 44  ---          21 44 55  27.9  59.5 -5.1     -71.6    30   R  2   3867

19 26 44  MRK1066      21 44 55  26.0  60.9 -5.3     -70.0   -10   1  2   3867  19 26 44
19 27 54  ---          21 46 05  26.3  61.0 -5.2     -70.1    60   R  2   2933

19 28 54  J0319+4130   21 47 05  24.4  54.7 -5.5     -69.8    50   1  2   2933  19 28 54
19 32 34  ---          21 50 46  25.1  55.0 -5.5     -70.3   220   R  2      0

19 34 34  J0253+3835   21 52 46  29.4  60.1 -5.0     -72.6   105   1  3      0  19 34 34
19 35 14  ---          21 53 26  29.5  60.1 -5.0     -72.7    40   F  1    533

19 35 14  MRK1066      21 53 26  27.7  61.6 -5.1     -71.0   -10   1  3    533  19 35 14
19 36 24  ---          21 54 37  27.9  61.6 -5.1     -71.1    60   F  1   1467

19 36 24  J0253+3835   21 54 37  29.7  60.2 -5.0     -72.8   -10   1  3   1467  19 36 24
19 37 04  ---          21 55 17  29.8  60.2 -5.0     -72.9    30   F  1   2000

19 37 04  MRK1066      21 55 17  28.0  61.7 -5.1     -71.2   -10   1  3   2000  19 37 04
19 38 14  ---          21 56 27  28.2  61.8 -5.1     -71.3    60   F  1   2933

19 38 14  J0253+3835   21 56 27  30.1  60.3 -4.9     -73.1   -10   1  3   2933  19 38 14
19 38 54  ---          21 57 07  30.2  60.4 -4.9     -73.1    30   F  1   3467

19 38 54  MRK1066      21 57 07  28.4  61.8 -5.1     -71.4   -10   1  3   3467  19 38 54
19 40 04  ---          21 58 17  28.6  61.9 -5.0     -71.5    60   F  1   4400

19 40 04  J0253+3835   21 58 17  30.4  60.4 -4.9     -73.3   -10   1  3   4400  19 40 04
19 40 44  ---          21 58 57  30.5  60.5 -4.9     -73.4    30   F  1   4933
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

19 40 44  MRK1066      21 58 57  28.7  62.0 -5.0     -71.6   -10   1  3   4933  19 40 44
19 41 54  ---          22 00 07  28.9  62.0 -5.0     -71.7    60   F  1   5867

19 41 54  J0253+3835   22 00 07  30.7  60.6 -4.9     -73.5   -10   1  3   5867  19 41 54
19 42 34  ---          22 00 48  30.9  60.6 -4.9     -73.6    30   F  1   6400

19 42 34  MRK1066      22 00 48  29.1  62.1 -5.0     -71.8   -10   1  3   6400  19 42 34
19 43 44  ---          22 01 58  29.3  62.2 -5.0     -71.9    60   F  1   7333

19 43 44  J0253+3835   22 01 58  31.1  60.7 -4.9     -73.7   -10   1  3   7333  19 43 44
19 44 24  ---          22 02 38  31.2  60.7 -4.8     -73.8    30   F  1   7867

19 44 24  MRK1066      22 02 38  29.4  62.2 -5.0     -72.0   -10   1  3   7867  19 44 24
19 45 34  ---          22 03 48  29.6  62.3 -4.9     -72.2    60   F  1   8800

19 45 34  J0253+3835   22 03 48  31.4  60.8 -4.8     -74.0   -10   1  3   8800  19 45 34
19 46 14  ---          22 04 28  31.6  60.8 -4.8     -74.0    30   F  1   9333

19 46 14  MRK1066      22 04 28  29.8  62.4 -4.9     -72.2   -10   1  3   9333  19 46 14
19 47 24  ---          22 05 38  30.0  62.4 -4.9     -72.4    60   F  1  10267

19 47 24  J0253+3835   22 05 38  31.8  60.9 -4.8     -74.2   -10   1  3  10267  19 47 24
19 48 04  ---          22 06 18  31.9  61.0 -4.8     -74.3    30   F  1  10800

19 48 04  MRK1066      22 06 18  30.1  62.5 -4.9     -72.4   -10   1  3  10800  19 48 04
19 49 14  ---          22 07 29  30.3  62.6 -4.9     -72.6    60   F  1  11733

19 49 14  J0253+3835   22 07 29  32.1  61.0 -4.8     -74.4   -10   1  3  11733  19 49 14
19 49 54  ---          22 08 09  32.2  61.1 -4.8     -74.5    30   F  1  12267

19 49 54  MRK1066      22 08 09  30.5  62.6 -4.9     -72.7   -10   1  3  12267  19 49 54
19 51 04  ---          22 09 19  30.7  62.7 -4.8     -72.8    60   F  1  13200

19 51 04  J0253+3835   22 09 19  32.5  61.1 -4.7     -74.6   -10   1  3  13200  19 51 04
19 51 44  ---          22 09 59  32.6  61.2 -4.7     -74.7    30   F  1  13733

19 51 44  MRK1066      22 09 59  30.8  62.7 -4.8     -72.9   -10   1  3  13733  19 51 44
19 52 54  ---          22 11 09  31.0  62.8 -4.8     -73.0    60   F  1  14667

19 52 54  J0253+3835   22 11 09  32.8  61.3 -4.7     -74.9   -10   1  3  14667  19 52 54
19 53 34  ---          22 11 49  32.9  61.3 -4.7     -75.0    30   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

19 53 34  MRK1066      22 11 49  31.2  62.9 -4.8     -73.1   -10   1  3  15200  19 53 34
19 54 44  ---          22 13 00  31.4  62.9 -4.8     -73.2    60   F  1  16133

19 54 44  J0253+3835   22 13 00  33.2  61.4 -4.7     -75.1   -10   1  3  16133  19 54 44
19 55 24  ---          22 13 40  33.3  61.4 -4.7     -75.2    30   F  1  16667

19 55 24  MRK1066      22 13 40  31.5  63.0 -4.8     -73.3   -10   1  3  16667  19 55 24
19 56 34  ---          22 14 50  31.7  63.1 -4.8     -73.4    60   F  1  17600

19 57 11  J0253+3835   22 15 27  33.6  61.5 -4.6     -75.4    27   1  4  17600  19 57 11
19 57 51  ---          22 16 07  33.8  61.5 -4.6     -75.5    40   R  1  17067

19 57 51  MRK1066      22 16 07  32.0  63.2 -4.7     -73.6   -10   1  4  17067  19 57 51
19 59 01  ---          22 17 17  32.2  63.2 -4.7     -73.7    60   R  1  16133

19 59 01  J0253+3835   22 17 17  34.0  61.6 -4.6     -75.6   -10   1  4  16133  19 59 01
19 59 41  ---          22 17 57  34.1  61.7 -4.6     -75.7    30   R  1  15600

19 59 41  MRK1066      22 17 57  32.3  63.3 -4.7     -73.8   -10   1  4  15600  19 59 41
20 00 51  ---          22 19 08  32.6  63.3 -4.7     -73.9    60   R  1  14667

20 00 51  J0253+3835   22 19 08  34.3  61.7 -4.6     -75.9   -10   1  4  14667  20 00 51
20 01 31  ---          22 19 48  34.4  61.8 -4.6     -75.9    30   R  1  14133

20 01 31  MRK1066      22 19 48  32.7  63.4 -4.7     -74.0   -10   1  4  14133  20 01 31
20 02 41  ---          22 20 58  32.9  63.5 -4.7     -74.1    60   R  1  13200

20 02 41  J0253+3835   22 20 58  34.7  61.8 -4.5     -76.1   -10   1  4  13200  20 02 41
20 03 21  ---          22 21 38  34.8  61.9 -4.5     -76.2    30   R  1  12667

20 03 21  MRK1066      22 21 38  33.0  63.5 -4.6     -74.2   -10   1  4  12667  20 03 21
20 04 31  ---          22 22 48  33.3  63.6 -4.6     -74.3    60   R  1  11733

20 04 31  J0253+3835   22 22 48  35.0  61.9 -4.5     -76.3   -10   1  4  11733  20 04 31
20 05 11  ---          22 23 28  35.1  62.0 -4.5     -76.4    30   R  1  11200

20 05 11  MRK1066      22 23 28  33.4  63.6 -4.6     -74.4   -10   1  4  11200  20 05 11
20 06 21  ---          22 24 38  33.6  63.7 -4.6     -74.5    60   R  1  10267

20 06 21  J0253+3835   22 24 38  35.4  62.0 -4.5     -76.5    -9   1  4  10267  20 06 21
20 07 01  ---          22 25 19  35.5  62.1 -4.5     -76.6    31   R  1   9733
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

20 07 01  MRK1066      22 25 19  33.7  63.8 -4.6     -74.6    -9   1  4   9733  20 07 01
20 08 11  ---          22 26 29  34.0  63.8 -4.6     -74.8    61   R  1   8800

20 08 11  J0253+3835   22 26 29  35.7  62.1 -4.4     -76.8    -9   1  4   8800  20 08 11
20 08 51  ---          22 27 09  35.8  62.2 -4.4     -76.8    31   R  1   8267

20 08 51  MRK1066      22 27 09  34.1  63.9 -4.6     -74.8    -9   1  4   8267  20 08 51
20 10 01  ---          22 28 19  34.3  63.9 -4.5     -75.0    61   R  1   7333

20 10 01  J0253+3835   22 28 19  36.1  62.2 -4.4     -77.0    -9   1  4   7333  20 10 01
20 10 41  ---          22 28 59  36.2  62.3 -4.4     -77.1    31   R  1   6800

20 10 41  MRK1066      22 28 59  34.5  64.0 -4.5     -75.0    -9   1  4   6800  20 10 41
20 11 51  ---          22 30 09  34.7  64.1 -4.5     -75.2    61   R  1   5867

20 11 51  J0253+3835   22 30 09  36.4  62.3 -4.4     -77.2    -9   1  4   5867  20 11 51
20 12 31  ---          22 30 49  36.5  62.4 -4.4     -77.3    31   R  1   5333

20 12 31  MRK1066      22 30 49  34.8  64.1 -4.5     -75.2    -9   1  4   5333  20 12 31
20 13 41  ---          22 32 00  35.0  64.2 -4.5     -75.4    61   R  1   4400

20 14 41  J0319+4130   22 33 00  32.7  57.6 -4.8     -76.1    49   1  4   4400  20 14 41
20 20 11  ---          22 38 31  33.7  57.9 -4.7     -76.8   330   R  1      0

20 22 11  J0253+3835   22 40 31  38.4  62.9 -4.2     -78.5   105   1  3      0  20 22 11
20 22 51  ---          22 41 11  38.5  62.9 -4.2     -78.6    40   F  2    533

20 22 51  MRK1066      22 41 11  36.8  64.7 -4.3     -76.4    -9   1  3    533  20 22 51
20 24 01  ---          22 42 21  37.1  64.8 -4.3     -76.6    61   F  2   1467

20 24 01  J0253+3835   22 42 21  38.7  63.0 -4.2     -78.7    -9   1  3   1467  20 24 01
20 24 41  ---          22 43 01  38.9  63.0 -4.2     -78.8    31   F  2   2000

20 24 41  MRK1066      22 43 01  37.2  64.8 -4.3     -76.6    -9   1  3   2000  20 24 41
20 25 51  ---          22 44 12  37.4  64.9 -4.3     -76.8    61   F  2   2933

20 25 51  J0253+3835   22 44 12  39.1  63.1 -4.2     -79.0    -9   1  3   2933  20 25 51
20 26 31  ---          22 44 52  39.2  63.1 -4.1     -79.1    31   F  2   3467

20 26 31  MRK1066      22 44 52  37.5  64.9 -4.3     -76.9    -9   1  3   3467  20 26 31
20 27 41  ---          22 46 02  37.8  65.0 -4.2     -77.0    61   F  2   4400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

20 27 41  J0253+3835   22 46 02  39.5  63.1 -4.1     -79.2    -9   1  3   4400  20 27 41
20 28 21  ---          22 46 42  39.6  63.2 -4.1     -79.3    31   F  2   4933

20 28 21  MRK1066      22 46 42  37.9  65.0 -4.2     -77.1    -9   1  3   4933  20 28 21
20 29 31  ---          22 47 52  38.1  65.1 -4.2     -77.2    61   F  2   5867

20 29 31  J0253+3835   22 47 52  39.8  63.2 -4.1     -79.4    -9   1  3   5867  20 29 31
20 30 11  ---          22 48 32  39.9  63.3 -4.1     -79.5    31   F  2   6400

20 30 11  MRK1066      22 48 32  38.3  65.1 -4.2     -77.3    -9   1  3   6400  20 30 11
20 31 21  ---          22 49 43  38.5  65.2 -4.2     -77.4    61   F  2   7333

20 31 21  J0253+3835   22 49 43  40.2  63.3 -4.1     -79.7    -9   1  3   7333  20 31 21
20 32 01  ---          22 50 23  40.3  63.3 -4.0     -79.7    31   F  2   7867

20 32 01  MRK1066      22 50 23  38.6  65.2 -4.2     -77.5    -9   1  3   7867  20 32 01
20 33 11  ---          22 51 33  38.8  65.3 -4.1     -77.6    61   F  2   8800

20 33 11  J0253+3835   22 51 33  40.5  63.4 -4.0     -79.9    -9   1  3   8800  20 33 11
20 33 51  ---          22 52 13  40.6  63.4 -4.0     -80.0    31   F  2   9333

20 33 51  MRK1066      22 52 13  39.0  65.3 -4.1     -77.7    -9   1  3   9333  20 33 51
20 35 01  ---          22 53 23  39.2  65.4 -4.1     -77.8    61   F  2  10267

20 35 01  J0253+3835   22 53 23  40.9  63.5 -4.0     -80.1    -9   1  3  10267  20 35 01
20 35 41  ---          22 54 03  41.0  63.5 -4.0     -80.2    31   F  2  10800

20 35 41  MRK1066      22 54 03  39.3  65.4 -4.1     -77.9    -9   1  3  10800  20 35 41
20 36 51  ---          22 55 13  39.6  65.5 -4.1     -78.1    61   F  2  11733

20 36 51  J0253+3835   22 55 13  41.2  63.6 -4.0     -80.4    -9   1  3  11733  20 36 51
20 37 31  ---          22 55 54  41.3  63.6 -4.0     -80.4    31   F  2  12267

20 37 31  MRK1066      22 55 54  39.7  65.5 -4.1     -78.1    -9   1  3  12267  20 37 31
20 38 41  ---          22 57 04  39.9  65.6 -4.1     -78.3    61   F  2  13200

20 38 41  J0253+3835   22 57 04  41.6  63.6 -3.9     -80.6    -9   1  3  13200  20 38 41
20 39 21  ---          22 57 44  41.7  63.7 -3.9     -80.7    31   F  2  13733

20 39 21  MRK1066      22 57 44  40.1  65.6 -4.0     -78.3    -9   1  3  13733  20 39 21
20 40 31  ---          22 58 54  40.3  65.7 -4.0     -78.5    61   F  2  14667
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

20 40 31  J0253+3835   22 58 54  41.9  63.7 -3.9     -80.8    -9   1  3  14667  20 40 31
20 41 11  ---          22 59 34  42.1  63.7 -3.9     -80.9    31   F  2  15200

20 41 11  MRK1066      22 59 34  40.4  65.7 -4.0     -78.6    -9   1  3  15200  20 41 11
20 42 21  ---          23 00 44  40.6  65.8 -4.0     -78.7    61   F  2  16133

20 42 21  J0253+3835   23 00 44  42.3  63.8 -3.9     -81.1    -9   1  3  16133  20 42 21
20 43 01  ---          23 01 24  42.4  63.8 -3.9     -81.2    31   F  2  16667

20 43 01  MRK1066      23 01 24  40.8  65.8 -4.0     -78.8    -9   1  3  16667  20 43 01
20 44 11  ---          23 02 35  41.0  65.9 -4.0     -78.9    61   F  2  17600

20 44 48  J0253+3835   23 03 12  42.8  63.9 -3.8     -81.4    27   1  4  17600  20 44 48
20 45 28  ---          23 03 52  42.9  63.9 -3.8     -81.5    40   R  2  17067

20 45 28  MRK1066      23 03 52  41.3  66.0 -3.9     -79.1    -9   1  4  17067  20 45 28
20 46 38  ---          23 05 02  41.5  66.0 -3.9     -79.2    61   R  2  16133

20 46 38  J0253+3835   23 05 02  43.1  64.0 -3.8     -81.6    -9   1  4  16133  20 46 38
20 47 18  ---          23 05 42  43.2  64.0 -3.8     -81.7    31   R  2  15600

20 47 18  MRK1066      23 05 42  41.6  66.1 -3.9     -79.3    -9   1  4  15600  20 47 18
20 48 28  ---          23 06 52  41.8  66.1 -3.9     -79.4    61   R  2  14667

20 48 28  J0253+3835   23 06 52  43.5  64.0 -3.8     -81.9    -9   1  4  14667  20 48 28
20 49 08  ---          23 07 33  43.6  64.1 -3.8     -81.9    31   R  2  14133

20 49 08  MRK1066      23 07 33  42.0  66.1 -3.9     -79.5    -9   1  4  14133  20 49 08
20 50 18  ---          23 08 43  42.2  66.2 -3.9     -79.6    61   R  2  13200

20 50 18  J0253+3835   23 08 43  43.8  64.1 -3.7     -82.1    -9   1  4  13200  20 50 18
20 50 58  ---          23 09 23  44.0  64.1 -3.7     -82.2    31   R  2  12667

20 50 58  MRK1066      23 09 23  42.3  66.2 -3.8     -79.7    -9   1  4  12667  20 50 58
20 52 08  ---          23 10 33  42.6  66.3 -3.8     -79.8    61   R  2  11733

20 52 08  J0253+3835   23 10 33  44.2  64.2 -3.7     -82.3    -9   1  4  11733  20 52 08
20 52 48  ---          23 11 13  44.3  64.2 -3.7     -82.4    31   R  2  11200

20 52 48  MRK1066      23 11 13  42.7  66.3 -3.8     -79.9    -9   1  4  11200  20 52 48
20 53 58  ---          23 12 23  42.9  66.4 -3.8     -80.1    61   R  2  10267
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

20 53 58  J0253+3835   23 12 23  44.5  64.2 -3.7     -82.6    -9   1  4  10267  20 53 58
20 54 38  ---          23 13 03  44.7  64.3 -3.7     -82.7    31   R  2   9733

20 54 38  MRK1066      23 13 03  43.1  66.4 -3.8     -80.1    -9   1  4   9733  20 54 38
20 55 48  ---          23 14 14  43.3  66.5 -3.8     -80.3    61   R  2   8800

20 55 48  J0253+3835   23 14 14  44.9  64.3 -3.7     -82.8    -9   1  4   8800  20 55 48
20 56 28  ---          23 14 54  45.0  64.3 -3.6     -82.9    31   R  2   8267

20 56 28  MRK1066      23 14 54  43.4  66.5 -3.8     -80.3    -9   1  4   8267  20 56 28
20 57 38  ---          23 16 04  43.7  66.6 -3.7     -80.5    61   R  2   7333

20 57 38  J0253+3835   23 16 04  45.2  64.4 -3.6     -83.1    -9   1  4   7333  20 57 38
20 58 18  ---          23 16 44  45.4  64.4 -3.6     -83.2    31   R  2   6800

20 58 18  MRK1066      23 16 44  43.8  66.6 -3.7     -80.6    -9   1  4   6800  20 58 18
20 59 28  ---          23 17 54  44.0  66.6 -3.7     -80.7    61   R  2   5867

20 59 28  J0253+3835   23 17 54  45.6  64.4 -3.6     -83.3    -9   1  4   5867  20 59 28
21 00 08  ---          23 18 34  45.7  64.4 -3.6     -83.4    31   R  2   5333

21 00 08  MRK1066      23 18 34  44.2  66.7 -3.7     -80.8    -9   1  4   5333  21 00 08
21 01 18  ---          23 19 45  44.4  66.7 -3.7     -80.9    61   R  2   4400

21 01 18  J0253+3835   23 19 45  46.0  64.5 -3.6     -83.5    -9   1  4   4400  21 01 18
21 01 58  ---          23 20 25  46.1  64.5 -3.5     -83.6    31   R  2   3867

21 01 58  MRK1066      23 20 25  44.5  66.7 -3.7     -81.0    -9   1  4   3867  21 01 58
21 03 08  ---          23 21 35  44.7  66.8 -3.6     -81.1    61   R  2   2933

21 03 08  J0319+4130   23 21 35  41.6  59.7 -4.0     -82.9   -12   1  4   2933  21 03 08
21 06 48  ---          23 25 15  42.3  59.8 -3.9     -83.4   208   R  2      0

21 08 48  J0253+3835   23 27 16  47.4  64.7 -3.4     -84.6   104   1  5      0  21 08 48
21 09 28  ---          23 27 56  47.6  64.7 -3.4     -84.7    40   F  1    533

21 09 28  MRK1066      23 27 56  46.0  67.1 -3.5     -81.9    -9   1  5    533  21 09 28
21 10 38  ---          23 29 06  46.2  67.1 -3.5     -82.0    61   F  1   1467

21 10 38  J0253+3835   23 29 06  47.8  64.8 -3.4     -84.8    -9   1  5   1467  21 10 38
21 11 18  ---          23 29 46  47.9  64.8 -3.4     -84.9    31   F  1   2000
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

21 11 18  MRK1066      23 29 46  46.4  67.1 -3.5     -82.1    -9   1  5   2000  21 11 18
21 12 28  ---          23 30 56  46.6  67.2 -3.5     -82.3    61   F  1   2933

21 12 28  J0253+3835   23 30 56  48.1  64.8 -3.4     -85.1    -9   1  5   2933  21 12 28
21 13 08  ---          23 31 36  48.3  64.8 -3.4     -85.2    31   F  1   3467

21 13 08  MRK1066      23 31 36  46.7  67.2 -3.5     -82.4    -9   1  5   3467  21 13 08
21 14 18  ---          23 32 47  47.0  67.3 -3.5     -82.5    61   F  1   4400

21 14 18  J0253+3835   23 32 47  48.5  64.9 -3.3     -85.3    -9   1  5   4400  21 14 18
21 14 58  ---          23 33 27  48.6  64.9 -3.3     -85.4    31   F  1   4933

21 14 58  MRK1066      23 33 27  47.1  67.3 -3.4     -82.6    -9   1  5   4933  21 14 58
21 16 08  ---          23 34 37  47.3  67.3 -3.4     -82.7    61   F  1   5867

21 16 08  J0253+3835   23 34 37  48.9  64.9 -3.3     -85.6    -9   1  5   5867  21 16 08
21 16 48  ---          23 35 17  49.0  64.9 -3.3     -85.7    31   F  1   6400

21 16 48  MRK1066      23 35 17  47.5  67.3 -3.4     -82.8    -9   1  5   6400  21 16 48
21 17 58  ---          23 36 27  47.7  67.4 -3.4     -82.9    61   F  1   7333

21 17 58  J0253+3835   23 36 27  49.2  64.9 -3.3     -85.8    -9   1  5   7333  21 17 58
21 18 38  ---          23 37 07  49.3  64.9 -3.3     -85.9    31   F  1   7867

21 18 38  MRK1066      23 37 07  47.8  67.4 -3.4     -83.0    -9   1  5   7867  21 18 38
21 19 48  ---          23 38 18  48.1  67.5 -3.4     -83.2    61   F  1   8800

21 19 48  J0253+3835   23 38 18  49.6  65.0 -3.3     -86.1    -9   1  5   8800  21 19 48
21 20 28  ---          23 38 58  49.7  65.0 -3.2     -86.2    31   F  1   9333

21 20 28  MRK1066      23 38 58  48.2  67.5 -3.4     -83.3    -9   1  5   9333  21 20 28
21 21 38  ---          23 40 08  48.4  67.5 -3.3     -83.4    61   F  1  10267

21 21 38  J0253+3835   23 40 08  49.9  65.0 -3.2     -86.3    -9   1  5  10267  21 21 38
21 22 18  ---          23 40 48  50.1  65.0 -3.2     -86.4    31   F  1  10800

21 22 18  MRK1066      23 40 48  48.6  67.5 -3.3     -83.5    -9   1  5  10800  21 22 18
21 23 28  ---          23 41 58  48.8  67.6 -3.3     -83.6    61   F  1  11733

21 23 28  J0253+3835   23 41 58  50.3  65.0 -3.2     -86.6    -9   1  5  11733  21 23 28
21 24 08  ---          23 42 38  50.4  65.1 -3.2     -86.7    31   F  1  12267
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

21 24 08  MRK1066      23 42 38  48.9  67.6 -3.3     -83.7    -9   1  5  12267  21 24 08
21 25 18  ---          23 43 48  49.2  67.6 -3.3     -83.9    61   F  1  13200

21 25 18  J0253+3835   23 43 48  50.6  65.1 -3.2     -86.9    -9   1  5  13200  21 25 18
21 25 58  ---          23 44 29  50.8  65.1 -3.1     -87.0    31   F  1  13733

21 25 58  MRK1066      23 44 29  49.3  67.7 -3.3     -83.9    -9   1  5  13733  21 25 58
21 27 08  ---          23 45 39  49.5  67.7 -3.2     -84.1    61   F  1  14667

21 27 08  J0253+3835   23 45 39  51.0  65.1 -3.1     -87.1    -9   1  5  14667  21 27 08
21 27 48  ---          23 46 19  51.1  65.1 -3.1     -87.2    31   F  1  15200

21 27 48  MRK1066      23 46 19  49.7  67.7 -3.2     -84.2    -9   1  5  15200  21 27 48
21 28 58  ---          23 47 29  49.9  67.8 -3.2     -84.3    61   F  1  16133

21 28 58  J0253+3835   23 47 29  51.4  65.1 -3.1     -87.4    -9   1  5  16133  21 28 58
21 29 38  ---          23 48 09  51.5  65.1 -3.1     -87.5    31   F  1  16667

21 29 38  MRK1066      23 48 09  50.0  67.8 -3.2     -84.4    -9   1  5  16667  21 29 38
21 30 48  ---          23 49 19  50.3  67.8 -3.2     -84.5    61   F  1  17600

21 31 25  J0253+3835   23 49 56  51.8  65.2 -3.1     -87.8    28   1  6  17600  21 31 25
21 32 05  ---          23 50 37  52.0  65.2 -3.0     -87.8    40   R  1  17067

21 32 05  MRK1066      23 50 37  50.5  67.9 -3.2     -84.7    -9   1  6  17067  21 32 05
21 33 15  ---          23 51 47  50.7  67.9 -3.1     -84.9    61   R  1  16133

21 33 15  J0253+3835   23 51 47  52.2  65.2 -3.0     -88.0    -9   1  6  16133  21 33 15
21 33 55  ---          23 52 27  52.3  65.2 -3.0     -88.1    31   R  1  15600

21 33 55  MRK1066      23 52 27  50.9  67.9 -3.1     -84.9    -9   1  6  15600  21 33 55
21 35 05  ---          23 53 37  51.1  67.9 -3.1     -85.1    61   R  1  14667

21 35 05  J0253+3835   23 53 37  52.6  65.2 -3.0     -88.3    -9   1  6  14667  21 35 05
21 35 45  ---          23 54 17  52.7  65.2 -3.0     -88.4    31   R  1  14133

21 35 45  MRK1066      23 54 17  51.2  68.0 -3.1     -85.2    -9   1  6  14133  21 35 45
21 36 55  ---          23 55 27  51.5  68.0 -3.1     -85.3    61   R  1  13200

21 36 55  J0253+3835   23 55 27  52.9  65.2 -3.0     -88.6    -9   1  6  13200  21 36 55
21 37 35  ---          23 56 07  53.1  65.2 -3.0     -88.7    31   R  1  12667
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

21 37 35  MRK1066      23 56 07  51.6  68.0 -3.1     -85.4    -9   1  6  12667  21 37 35
21 38 45  ---          23 57 18  51.8  68.0 -3.0     -85.6    61   R  1  11733

21 38 45  J0253+3835   23 57 18  53.3  65.2 -2.9     -88.8    -9   1  6  11733  21 38 45
21 39 25  ---          23 57 58  53.4  65.2 -2.9     -88.9    31   R  1  11200

21 39 25  MRK1066      23 57 58  52.0  68.1 -3.0     -85.7    -9   1  6  11200  21 39 25
21 40 35  ---          23 59 08  52.2  68.1 -3.0     -85.8    61   R  1  10267

21 40 35  J0253+3835   23 59 08  53.6  65.2 -2.9     -89.1    -9   1  6  10267  21 40 35
21 41 15  ---          23 59 48  53.8  65.3 -2.9     -89.2    31   R  1   9733

21 41 15  MRK1066      23 59 48  52.3  68.1 -3.0     -85.9    -9   1  6   9733  21 41 15
21 42 25  ---          00 00 58  52.6  68.1 -3.0     -86.1    61   R  1   8800

21 42 25  J0253+3835   00 00 58  54.0  65.3 -2.9     -89.4    -9   1  6   8800  21 42 25
21 43 05  ---          00 01 38  54.1  65.3 -2.9     -89.5    31   R  1   8267

21 43 05  MRK1066      00 01 38  52.7  68.1 -3.0     -86.1    -9   1  6   8267  21 43 05
21 44 15  ---          00 02 49  52.9  68.2 -3.0     -86.3    61   R  1   7333

21 44 15  J0253+3835   00 02 49  54.4  65.3 -2.8     -89.7    -9   1  6   7333  21 44 15
21 44 55  ---          00 03 29  54.5  65.3 -2.8     -89.8    31   R  1   6800

21 44 55  MRK1066      00 03 29  53.1  68.2 -2.9     -86.4    -9   1  6   6800  21 44 55
21 46 05  ---          00 04 39  53.3  68.2 -2.9     -86.5    61   R  1   5867

21 46 05  J0253+3835   00 04 39  54.7  65.3 -2.8     -90.0    -9   1  6   5867  21 46 05
21 46 45  ---          00 05 19  54.8  65.3 -2.8     -90.1    31   R  1   5333

21 46 45  MRK1066      00 05 19  53.4  68.2 -2.9     -86.6    -9   1  6   5333  21 46 45
21 47 55  ---          00 06 29  53.7  68.2 -2.9     -86.8    61   R  1   4400

21 47 55  J0253+3835   00 06 29  55.1  65.3 -2.8     -90.3    -9   1  6   4400  21 47 55
21 48 35  ---          00 07 09  55.2  65.3 -2.8     -90.4    31   R  1   3867

21 48 35  MRK1066      00 07 09  53.8  68.3 -2.9     -86.9    -9   1  6   3867  21 48 35
21 49 45  ---          00 08 19  54.0  68.3 -2.9     -87.0    61   R  1   2933

21 49 45  J0319+4130   00 08 19  50.3  60.5 -3.2     -90.1   -13   1  6   2933  21 49 45
21 53 25  ---          00 12 00  51.0  60.5 -3.1     -90.7   207   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

21 55 25  J0253+3835   00 14 00  56.5  65.2 -2.7     -91.5   103   1  5      0  21 55 25
21 56 05  ---          00 14 41  56.7  65.2 -2.6     -91.6    40   F  2    533

21 56 05  MRK1066      00 14 41  55.3  68.4 -2.8     -87.9    -9   1  5    533  21 56 05
21 57 15  ---          00 15 51  55.6  68.4 -2.7     -88.1    61   F  2   1467

21 57 15  J0253+3835   00 15 51  56.9  65.2 -2.6     -91.8    -9   1  5   1467  21 57 15
21 57 55  ---          00 16 31  57.0  65.2 -2.6     -91.9    31   F  2   2000

21 57 55  MRK1066      00 16 31  55.7  68.4 -2.7     -88.2    -9   1  5   2000  21 57 55
21 59 05  ---          00 17 41  55.9  68.4 -2.7     -88.3    61   F  2   2933

21 59 05  J0253+3835   00 17 41  57.3  65.2 -2.6     -92.1    -9   1  5   2933  21 59 05
21 59 45  ---          00 18 21  57.4  65.2 -2.6     -92.2    31   F  2   3467

21 59 45  MRK1066      00 18 21  56.1  68.4 -2.7     -88.4    -9   1  5   3467  21 59 45
22 00 55  ---          00 19 31  56.3  68.4 -2.7     -88.6    61   F  2   4400

22 00 55  J0253+3835   00 19 31  57.6  65.2 -2.6     -92.4    -9   1  5   4400  22 00 55
22 01 35  ---          00 20 11  57.8  65.1 -2.6     -92.5    31   F  2   4933

22 01 35  MRK1066      00 20 11  56.4  68.4 -2.7     -88.7    -9   1  5   4933  22 01 35
22 02 45  ---          00 21 22  56.7  68.4 -2.6     -88.9    61   F  2   5867

22 02 45  J0253+3835   00 21 22  58.0  65.1 -2.5     -92.7    -9   1  5   5867  22 02 45
22 03 25  ---          00 22 02  58.1  65.1 -2.5     -92.8    31   F  2   6400

22 03 25  MRK1066      00 22 02  56.8  68.4 -2.6     -89.0    -9   1  5   6400  22 03 25
22 04 35  ---          00 23 12  57.0  68.4 -2.6     -89.1    61   F  2   7333

22 04 35  J0253+3835   00 23 12  58.3  65.1 -2.5     -93.0    -9   1  5   7333  22 04 35
22 05 15  ---          00 23 52  58.5  65.1 -2.5     -93.1    31   F  2   7867

22 05 15  MRK1066      00 23 52  57.2  68.5 -2.6     -89.2    -9   1  5   7867  22 05 15
22 06 25  ---          00 25 02  57.4  68.5 -2.6     -89.4    61   F  2   8800

22 06 25  J0253+3835   00 25 02  58.7  65.1 -2.5     -93.3    -9   1  5   8800  22 06 25
22 07 05  ---          00 25 42  58.8  65.0 -2.5     -93.4    31   F  2   9333

22 07 05  MRK1066      00 25 42  57.5  68.5 -2.6     -89.5    -9   1  5   9333  22 07 05
22 08 15  ---          00 26 52  57.8  68.5 -2.6     -89.7    61   F  2  10267
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

22 08 15  J0253+3835   00 26 52  59.1  65.0 -2.4     -93.6    -9   1  5  10267  22 08 15
22 08 55  ---          00 27 33  59.2  65.0 -2.4     -93.8    31   F  2  10800

22 08 55  MRK1066      00 27 33  57.9  68.5 -2.5     -89.8    -9   1  5  10800  22 08 55
22 10 05  ---          00 28 43  58.1  68.5 -2.5     -89.9    61   F  2  11733

22 10 05  J0253+3835   00 28 43  59.4  65.0 -2.4     -94.0    -9   1  5  11733  22 10 05
22 10 45  ---          00 29 23  59.5  64.9 -2.4     -94.1    31   F  2  12267

22 10 45  MRK1066      00 29 23  58.3  68.5 -2.5     -90.0    -9   1  5  12267  22 10 45
22 11 55  ---          00 30 33  58.5  68.5 -2.5     -90.2    61   F  2  13200

22 11 55  J0253+3835   00 30 33  59.8  64.9 -2.4     -94.3    -9   1  5  13200  22 11 55
22 12 35  ---          00 31 13  59.9  64.9 -2.4     -94.4    31   F  2  13733

22 12 35  MRK1066      00 31 13  58.6  68.5 -2.5     -90.3    -9   1  5  13733  22 12 35
22 13 45  ---          00 32 23  58.9  68.5 -2.5     -90.5    61   F  2  14667

22 13 45  J0253+3835   00 32 23  60.1  64.9 -2.3     -94.6    -9   1  5  14667  22 13 45
22 14 25  ---          00 33 04  60.3  64.8 -2.3     -94.8    31   F  2  15200

22 14 25  MRK1066      00 33 04  59.0  68.5 -2.5     -90.6    -9   1  5  15200  22 14 25
22 15 35  ---          00 34 14  59.2  68.5 -2.4     -90.8    61   F  2  16133

22 15 35  J0253+3835   00 34 14  60.5  64.8 -2.3     -95.0    -9   1  5  16133  22 15 35
22 16 15  ---          00 34 54  60.6  64.8 -2.3     -95.1    31   F  2  16667

22 16 15  MRK1066      00 34 54  59.4  68.4 -2.4     -90.9    -9   1  5  16667  22 16 15
22 17 25  ---          00 36 04  59.6  68.4 -2.4     -91.1    61   F  2  17600

22 18 02  J0253+3835   00 36 41  61.0  64.7 -2.3     -95.4    28   1  6  17600  22 18 02
22 18 42  ---          00 37 21  61.1  64.7 -2.3     -95.6    40   R  2  17067

22 18 42  MRK1066      00 37 21  59.9  68.4 -2.4     -91.3    -8   1  6  17067  22 18 42
22 19 52  ---          00 38 31  60.1  68.4 -2.4     -91.4    62   R  2  16133

22 19 52  J0253+3835   00 38 31  61.3  64.6 -2.2     -95.8    -9   1  6  16133  22 19 52
22 20 32  ---          00 39 12  61.5  64.6 -2.2     -95.9    31   R  2  15600

22 20 32  MRK1066      00 39 12  60.2  68.4 -2.3     -91.6    -9   1  6  15600  22 20 32
22 21 42  ---          00 40 22  60.5  68.4 -2.3     -91.7    61   R  2  14667
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

22 21 42  J0253+3835   00 40 22  61.7  64.6 -2.2     -96.1    -9   1  6  14667  22 21 42
22 22 22  ---          00 41 02  61.8  64.5 -2.2     -96.3    31   R  2  14133

22 22 22  MRK1066      00 41 02  60.6  68.4 -2.3     -91.8    -9   1  6  14133  22 22 22
22 23 32  ---          00 42 12  60.8  68.4 -2.3     -92.0    61   R  2  13200

22 23 32  J0253+3835   00 42 12  62.0  64.5 -2.2     -96.5    -9   1  6  13200  22 23 32
22 24 12  ---          00 42 52  62.2  64.4 -2.2     -96.6    31   R  2  12667

22 24 12  MRK1066      00 42 52  61.0  68.4 -2.3     -92.1    -9   1  6  12667  22 24 12
22 25 22  ---          00 44 02  61.2  68.3 -2.3     -92.3    61   R  2  11733

22 25 22  J0253+3835   00 44 02  62.4  64.4 -2.2     -96.9    -9   1  6  11733  22 25 22
22 26 02  ---          00 44 42  62.5  64.3 -2.1     -97.0    31   R  2  11200

22 26 02  MRK1066      00 44 42  61.3  68.3 -2.3     -92.4    -9   1  6  11200  22 26 02
22 27 12  ---          00 45 53  61.6  68.3 -2.2     -92.6    61   R  2  10267

22 27 12  J0253+3835   00 45 53  62.8  64.3 -2.1     -97.2    -9   1  6  10267  22 27 12
22 27 52  ---          00 46 33  62.9  64.3 -2.1     -97.4    31   R  2   9733

22 27 52  MRK1066      00 46 33  61.7  68.3 -2.2     -92.8    -9   1  6   9733  22 27 52
22 29 02  ---          00 47 43  61.9  68.3 -2.2     -93.0    61   R  2   8800

22 29 02  J0253+3835   00 47 43  63.1  64.2 -2.1     -97.6    -9   1  6   8800  22 29 02
22 29 42  ---          00 48 23  63.2  64.1 -2.1     -97.8    31   R  2   8267

22 29 42  MRK1066      00 48 23  62.1  68.3 -2.2     -93.1    -9   1  6   8267  22 29 42
22 30 52  ---          00 49 33  62.3  68.2 -2.2     -93.3    61   R  2   7333

22 30 52  J0253+3835   00 49 33  63.5  64.1 -2.1     -98.0    -9   1  6   7333  22 30 52
22 31 32  ---          00 50 13  63.6  64.0 -2.1     -98.1    31   R  2   6800

22 31 32  MRK1066      00 50 13  62.4  68.2 -2.2     -93.4    -9   1  6   6800  22 31 32
22 32 42  ---          00 51 24  62.7  68.2 -2.1     -93.6    61   R  2   5867

22 32 42  J0253+3835   00 51 24  63.8  64.0 -2.0     -98.4    -9   1  6   5867  22 32 42
22 33 22  ---          00 52 04  63.9  63.9 -2.0     -98.5    31   R  2   5333

22 33 22  MRK1066      00 52 04  62.8  68.2 -2.1     -93.7    -9   1  6   5333  22 33 22
22 34 32  ---          00 53 14  63.0  68.1 -2.1     -93.9    61   R  2   4400
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

22 35 32  J0530+1331   00 54 14  24.6  88.4 -4.6     -62.2   -23   1  6   4400  22 35 32
22 41 02  ---          00 59 45  25.8  89.1 -4.5     -62.2   307   R  2      0

22 43 02  J0253+3835   01 01 45  65.8  63.2 -1.9    -100.7    34   1  7      0  22 43 02
22 43 42  ---          01 02 25  65.9  63.1 -1.8    -100.9    40   F  1    533

22 43 42  MRK1066      01 02 25  64.9  67.8 -2.0     -95.6    -9   1  7    533  22 43 42
22 44 52  ---          01 03 36  65.1  67.7 -1.9     -95.8    61   F  1   1467

22 44 52  J0253+3835   01 03 36  66.2  63.0 -1.8    -101.2    -9   1  7   1467  22 44 52
22 45 32  ---          01 04 16  66.3  62.9 -1.8    -101.3    31   F  1   2000

22 45 32  MRK1066      01 04 16  65.2  67.7 -1.9     -95.9    -9   1  7   2000  22 45 32
22 46 42  ---          01 05 26  65.5  67.6 -1.9     -96.2    61   F  1   2933

22 46 42  J0253+3835   01 05 26  66.5  62.8 -1.8    -101.6    -9   1  7   2933  22 46 42
22 47 22  ---          01 06 06  66.6  62.8 -1.8    -101.8    31   F  1   3467

22 47 22  MRK1066      01 06 06  65.6  67.6 -1.9     -96.3    -9   1  7   3467  22 47 22
22 48 32  ---          01 07 16  65.8  67.5 -1.9     -96.5    61   F  1   4400

22 48 32  J0253+3835   01 07 16  66.9  62.6 -1.8    -102.1    -9   1  7   4400  22 48 32
22 49 12  ---          01 07 56  67.0  62.6 -1.8    -102.2    31   F  1   4933

22 49 12  MRK1066      01 07 56  66.0  67.5 -1.9     -96.7    -9   1  7   4933  22 49 12
22 50 22  ---          01 09 06  66.2  67.4 -1.9     -96.9    61   F  1   5867

22 50 22  J0253+3835   01 09 06  67.2  62.4 -1.7    -102.5    -9   1  7   5867  22 50 22
22 51 02  ---          01 09 47  67.3  62.4 -1.7    -102.7    31   F  1   6400

22 51 02  MRK1066      01 09 47  66.3  67.4 -1.8     -97.1    -9   1  7   6400  22 51 02
22 52 12  ---          01 10 57  66.6  67.3 -1.8     -97.3    61   F  1   7333

22 52 12  J0253+3835   01 10 57  67.6  62.2 -1.7    -103.0    -9   1  7   7333  22 52 12
22 52 52  ---          01 11 37  67.7  62.2 -1.7    -103.2    31   F  1   7867

22 52 52  MRK1066      01 11 37  66.7  67.3 -1.8     -97.4    -9   1  7   7867  22 52 52
22 54 02  ---          01 12 47  66.9  67.2 -1.8     -97.7    61   F  1   8800

22 54 02  J0253+3835   01 12 47  67.9  62.0 -1.7    -103.5    -9   1  7   8800  22 54 02
22 54 42  ---          01 13 27  68.0  61.9 -1.7    -103.7    31   F  1   9333
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

22 54 42  MRK1066      01 13 27  67.1  67.2 -1.8     -97.8    -9   1  7   9333  22 54 42
22 55 52  ---          01 14 37  67.3  67.1 -1.8     -98.1    61   F  1  10267

22 55 52  J0253+3835   01 14 37  68.3  61.8 -1.6    -104.0   -10   1  7  10267  22 55 52
22 56 32  ---          01 15 17  68.4  61.7 -1.6    -104.2    30   F  1  10800

22 56 32  MRK1066      01 15 17  67.4  67.0 -1.7     -98.2   -10   1  7  10800  22 56 32
22 57 42  ---          01 16 28  67.6  66.9 -1.7     -98.5    60   F  1  11733

22 57 42  J0253+3835   01 16 28  68.6  61.5 -1.6    -104.5   -10   1  7  11733  22 57 42
22 58 22  ---          01 17 08  68.7  61.5 -1.6    -104.7    30   F  1  12267

22 58 22  MRK1066      01 17 08  67.8  66.9 -1.7     -98.6   -10   1  7  12267  22 58 22
22 59 32  ---          01 18 18  68.0  66.8 -1.7     -98.9    60   F  1  13200

22 59 32  J0253+3835   01 18 18  69.0  61.3 -1.6    -105.0   -10   1  7  13200  22 59 32
23 00 12  ---          01 18 58  69.1  61.2 -1.6    -105.2    30   F  1  13733

23 00 12  MRK1066      01 18 58  68.1  66.7 -1.7     -99.0   -10   1  7  13733  23 00 12
23 01 22  ---          01 20 08  68.4  66.6 -1.7     -99.3    60   F  1  14667

23 01 22  J0253+3835   01 20 08  69.3  61.0 -1.6    -105.6   -10   1  7  14667  23 01 22
23 02 02  ---          01 20 48  69.4  60.9 -1.5    -105.8    30   F  1  15200

23 02 02  MRK1066      01 20 48  68.5  66.6 -1.7     -99.5   -10   1  7  15200  23 02 02
23 03 12  ---          01 21 59  68.7  66.5 -1.6     -99.7    60   F  1  16133

23 03 12  J0253+3835   01 21 59  69.7  60.7 -1.5    -106.1   -10   1  7  16133  23 03 12
23 03 52  ---          01 22 39  69.8  60.6 -1.5    -106.3    30   F  1  16667

23 03 52  MRK1066      01 22 39  68.9  66.4 -1.6     -99.9   -10   1  7  16667  23 03 52
23 05 02  ---          01 23 49  69.1  66.3 -1.6    -100.2    60   F  1  17600

23 05 39  J0253+3835   01 24 26  70.1  60.4 -1.5    -106.9    27   1  8  17600  23 05 39
23 06 19  ---          01 25 06  70.2  60.2 -1.5    -107.1    40   R  1  17067

23 06 19  MRK1066      01 25 06  69.4  66.2 -1.6    -100.5   -10   1  8  17067  23 06 19
23 07 29  ---          01 26 16  69.6  66.0 -1.6    -100.8    60   R  1  16133

23 07 29  J0253+3835   01 26 16  70.5  60.0 -1.5    -107.5   -10   1  8  16133  23 07 29
23 08 09  ---          01 26 56  70.6  59.9 -1.4    -107.7    30   R  1  15600
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

23 08 09  MRK1066      01 26 56  69.7  66.0 -1.6    -101.0   -10   1  8  15600  23 08 09
23 09 19  ---          01 28 07  69.9  65.8 -1.5    -101.3    60   R  1  14667

23 09 19  J0253+3835   01 28 07  70.8  59.7 -1.4    -108.1   -10   1  8  14667  23 09 19
23 09 59  ---          01 28 47  70.9  59.6 -1.4    -108.3    30   R  1  14133

23 09 59  MRK1066      01 28 47  70.1  65.7 -1.5    -101.4   -10   1  8  14133  23 09 59
23 11 09  ---          01 29 57  70.3  65.6 -1.5    -101.7    60   R  1  13200

23 11 09  J0253+3835   01 29 57  71.1  59.4 -1.4    -108.7   -10   1  8  13200  23 11 09
23 11 49  ---          01 30 37  71.3  59.2 -1.4    -108.9    30   R  1  12667

23 11 49  MRK1066      01 30 37  70.4  65.5 -1.5    -101.9   -10   1  8  12667  23 11 49
23 12 59  ---          01 31 47  70.7  65.4 -1.5    -102.2    60   R  1  11733

23 12 59  J0253+3835   01 31 47  71.5  59.0 -1.4    -109.3   -10   1  8  11733  23 12 59
23 13 39  ---          01 32 27  71.6  58.9 -1.3    -109.5    30   R  1  11200

23 13 39  MRK1066      01 32 27  70.8  65.3 -1.5    -102.4   -10   1  8  11200  23 13 39
23 14 49  ---          01 33 37  71.0  65.1 -1.4    -102.7    60   R  1  10267

23 14 49  J0253+3835   01 33 37  71.8  58.6 -1.3    -110.0   -10   1  8  10267  23 14 49
23 15 29  ---          01 34 18  71.9  58.5 -1.3    -110.2    30   R  1   9733

23 15 29  MRK1066      01 34 18  71.2  65.0 -1.4    -102.9   -10   1  8   9733  23 15 29
23 16 39  ---          01 35 28  71.4  64.9 -1.4    -103.2    60   R  1   8800

23 16 39  J0253+3835   01 35 28  72.2  58.2 -1.3    -110.6   -10   1  8   8800  23 16 39
23 17 19  ---          01 36 08  72.3  58.1 -1.3    -110.9    30   R  1   8267

23 17 19  MRK1066      01 36 08  71.5  64.8 -1.4    -103.4   -10   1  8   8267  23 17 19
23 18 29  ---          01 37 18  71.7  64.6 -1.4    -103.8    60   R  1   7333

23 18 29  J0253+3835   01 37 18  72.5  57.8 -1.3    -111.3   -11   1  8   7333  23 18 29
23 19 09  ---          01 37 58  72.6  57.6 -1.3    -111.6    29   R  1   6800

23 19 09  MRK1066      01 37 58  71.9  64.5 -1.4    -104.0   -11   1  8   6800  23 19 09
23 20 19  ---          01 39 08  72.1  64.3 -1.4    -104.3    59   R  1   5867

23 20 19  J0253+3835   01 39 08  72.8  57.3 -1.2    -112.0   -11   1  8   5867  23 20 19
23 20 59  ---          01 39 48  72.9  57.2 -1.2    -112.3    29   R  1   5333
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

23 20 59  MRK1066      01 39 48  72.2  64.2 -1.3    -104.5   -11   1  8   5333  23 20 59
23 22 09  ---          01 40 59  72.5  64.0 -1.3    -104.9    59   R  1   4400

23 22 09  J0253+3835   01 40 59  73.2  56.9 -1.2    -112.8   -11   1  8   4400  23 22 09
23 22 49  ---          01 41 39  73.3  56.7 -1.2    -113.0    29   R  1   3867

23 22 49  MRK1066      01 41 39  72.6  63.9 -1.3    -105.1   -11   1  8   3867  23 22 49
23 23 59  ---          01 42 49  72.8  63.7 -1.3    -105.5    59   R  1   2933

23 24 59  J0530+1331   01 43 49  35.2  94.9 -3.8     -61.9   -21   1  8   2933  23 24 59
23 28 39  ---          01 47 30  36.0  95.4 -3.7     -61.8   199   R  1      0

23 30 39  J0253+3835   01 49 30  74.7  54.4 -1.1    -116.5    37   1  7      0  23 30 39
23 31 19  ---          01 50 10  74.8  54.1 -1.1    -116.8    40   F  2    533

23 31 19  MRK1066      01 50 10  74.2  62.2 -1.2    -108.0   -11   1  7    533  23 31 19
23 32 29  ---          01 51 20  74.4  61.9 -1.1    -108.5    59   F  2   1467

23 32 29  J0253+3835   01 51 20  75.0  53.7 -1.0    -117.4   -11   1  7   1467  23 32 29
23 33 09  ---          01 52 00  75.1  53.5 -1.0    -117.7    29   F  2   2000

23 33 09  MRK1066      01 52 00  74.6  61.8 -1.1    -108.7   -12   1  7   2000  23 33 09
23 34 19  ---          01 53 11  74.8  61.5 -1.1    -109.2    58   F  2   2933

23 34 19  J0253+3835   01 53 11  75.3  53.1 -1.0    -118.3   -12   1  7   2933  23 34 19
23 34 59  ---          01 53 51  75.4  52.8 -1.0    -118.7    28   F  2   3467

23 34 59  MRK1066      01 53 51  74.9  61.3 -1.1    -109.4   -12   1  7   3467  23 34 59
23 36 09  ---          01 55 01  75.1  61.0 -1.1    -109.9    58   F  2   4400

23 36 09  J0253+3835   01 55 01  75.6  52.4 -1.0    -119.3   -12   1  7   4400  23 36 09
23 36 49  ---          01 55 41  75.7  52.1 -1.0    -119.6    28   F  2   4933

23 36 49  MRK1066      01 55 41  75.3  60.8 -1.1    -110.2   -12   1  7   4933  23 36 49
23 37 59  ---          01 56 51  75.5  60.5 -1.1    -110.7    58   F  2   5867

23 37 59  J0253+3835   01 56 51  75.9  51.7 -0.9    -120.3   -12   1  7   5867  23 37 59
23 38 39  ---          01 57 31  76.1  51.4 -0.9    -120.6    28   F  2   6400

23 38 39  MRK1066      01 57 31  75.6  60.3 -1.0    -110.9   -12   1  7   6400  23 38 39
23 39 49  ---          01 58 42  75.8  60.0 -1.0    -111.4    58   F  2   7333
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

23 39 49  J0253+3835   01 58 42  76.2  50.9 -0.9    -121.3   -12   1  7   7333  23 39 49
23 40 29  ---          01 59 22  76.4  50.6 -0.9    -121.7    28   F  2   7867

23 40 29  MRK1066      01 59 22  75.9  59.8 -1.0    -111.7   -12   1  7   7867  23 40 29
23 41 39  ---          02 00 32  76.2  59.4 -1.0    -112.3    58   F  2   8800

23 41 39  J0253+3835   02 00 32  76.6  50.1 -0.9    -122.4   -12   1  7   8800  23 41 39
23 42 19  ---          02 01 12  76.7  49.8 -0.9    -122.8    28   F  2   9333

23 42 19  MRK1066      02 01 12  76.3  59.2 -1.0    -112.6   -12   1  7   9333  23 42 19
23 43 29  ---          02 02 22  76.5  58.8 -1.0    -113.1    58   F  2  10267

23 43 29  J0253+3835   02 02 22  76.9  49.3 -0.8    -123.5   -12   1  7  10267  23 43 29
23 44 09  ---          02 03 02  77.0  48.9 -0.8    -123.9    28   F  2  10800

23 44 09  MRK1066      02 03 02  76.6  58.6 -1.0    -113.5   -12   1  7  10800  23 44 09
23 45 19  ---          02 04 12  76.8  58.2 -0.9    -114.0    58   F  2  11733

23 45 19  J0253+3835   02 04 12  77.2  48.4 -0.8    -124.6   -13   1  7  11733  23 45 19
23 45 59  ---          02 04 53  77.3  48.0 -0.8    -125.1    27   F  2  12267

23 45 59  MRK1066      02 04 53  77.0  57.9 -0.9    -114.4   -13   1  7  12267  23 45 59
23 47 09  ---          02 06 03  77.2  57.5 -0.9    -115.0    57   F  2  13200

23 47 09  J0253+3835   02 06 03  77.4  47.4 -0.8    -125.8   -13   1  7  13200  23 47 09
23 47 49  ---          02 06 43  77.6  47.1 -0.8    -126.3    27   F  2  13733

23 47 49  MRK1066      02 06 43  77.3  57.2 -0.9    -115.3   -13   1  7  13733  23 47 49
23 48 59  ---          02 07 53  77.5  56.8 -0.9    -115.9    57   F  2  14667

23 48 59  J0253+3835   02 07 53  77.7  46.4 -0.8    -127.1   -13   1  7  14667  23 48 59
23 49 39  ---          02 08 33  77.8  46.1 -0.7    -127.6    27   F  2  15200

23 49 39  MRK1066      02 08 33  77.6  56.5 -0.9    -116.3   -13   1  7  15200  23 49 39
23 50 49  ---          02 09 43  77.8  56.0 -0.8    -117.0    57   F  2  16133

23 50 49  J0253+3835   02 09 43  78.0  45.4 -0.7    -128.4   -13   1  7  16133  23 50 49
23 51 29  ---          02 10 23  78.1  45.0 -0.7    -128.9    27   F  2  16667

23 51 29  MRK1066      02 10 23  78.0  55.7 -0.8    -117.4   -13   1  7  16667  23 51 29
23 52 39  ---          02 11 34  78.2  55.2 -0.8    -118.0    57   F  2  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat   8 Feb 2003   Day  39 ---

23 53 16  J0253+3835   02 12 11  78.4  43.9 -0.7    -130.2    23   1  8  17600  23 53 16
23 53 56  ---          02 12 51  78.5  43.5 -0.7    -130.8    40   R  2  17067

23 53 56  MRK1066      02 12 51  78.4  54.6 -0.8    -118.8   -13   1  8  17067  23 53 56
23 55 06  ---          02 14 01  78.6  54.0 -0.8    -119.6    57   R  2  16133

23 55 06  J0253+3835   02 14 01  78.7  42.7 -0.7    -131.7   -14   1  8  16133  23 55 06
23 55 46  ---          02 14 41  78.8  42.3 -0.6    -132.2    26   R  2  15600

23 55 46  MRK1066      02 14 41  78.7  53.7 -0.8    -120.0   -14   1  8  15600  23 55 46
23 56 56  ---          02 15 51  78.9  53.1 -0.7    -120.8    56   R  2  14667

23 56 56  J0253+3835   02 15 51  78.9  41.5 -0.6    -133.2   -14   1  8  14667  23 56 56
23 57 36  ---          02 16 31  79.0  41.0 -0.6    -133.8    26   R  2  14133

23 57 36  MRK1066      02 16 31  79.0  52.7 -0.7    -121.2   -14   1  8  14133  23 57 36
23 58 46  ---          02 17 42  79.2  52.1 -0.7    -122.0    56   R  2  13200

23 58 46  J0253+3835   02 17 42  79.2  40.1 -0.6    -134.8   -14   1  8  13200  23 58 46
23 59 26  ---          02 18 22  79.3  39.7 -0.6    -135.4    26   R  2  12667

 --- Start: Sat   8 Feb 2003   Day  39 -- Stop: Sun   9 Feb 2003   Day  40 ---

23 59 26  MRK1066      02 18 22  79.3  51.7 -0.7    -122.5   -14   1  8  12667  23 59 26
00 00 36  ---          02 19 32  79.5  51.0 -0.7    -123.4    56   R  2  11733

00 00 36  J0253+3835   02 19 32  79.4  38.8 -0.6    -136.4   -14   1  8  11733  00 00 36
00 01 16  ---          02 20 12  79.5  38.2 -0.6    -137.0    26   R  2  11200

00 01 16  MRK1066      02 20 12  79.6  50.6 -0.7    -123.9   -14   1  8  11200  00 01 16
00 02 26  ---          02 21 22  79.8  49.8 -0.6    -124.8    56   R  2  10266

00 02 26  J0253+3835   02 21 22  79.7  37.3 -0.5    -138.1   -14   1  8  10266  00 02 26
00 03 06  ---          02 22 02  79.8  36.8 -0.5    -138.8    26   R  2   9733

00 03 06  MRK1066      02 22 02  79.9  49.4 -0.6    -125.3   -14   1  8   9733  00 03 06
00 04 16  ---          02 23 13  80.1  48.6 -0.6    -126.3    56   R  2   8800

00 04 16  J0253+3835   02 23 13  79.9  35.8 -0.5    -139.9   -15   1  8   8800  00 04 16
00 04 56  ---          02 23 53  80.0  35.2 -0.5    -140.6    25   R  2   8266

00 04 56  MRK1066      02 23 53  80.2  48.1 -0.6    -126.8   -15   1  8   8266  00 04 56
00 06 06  ---          02 25 03  80.4  47.3 -0.6    -127.8    55   R  2   7333
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   9 Feb 2003   Day  40 ---

00 06 06  J0253+3835   02 25 03  80.1  34.2 -0.5    -141.8   -15   1  8   7333  00 06 06
00 06 46  ---          02 25 43  80.2  33.6 -0.5    -142.5    25   R  2   6800

00 06 46  MRK1066      02 25 43  80.5  46.8 -0.6    -128.4   -15   1  8   6800  00 06 46
00 07 56  ---          02 26 53  80.7  45.9 -0.6    -129.5    55   R  2   5866

00 07 56  J0253+3835   02 26 53  80.4  32.5 -0.4    -143.8   -15   1  8   5866  00 07 56
00 08 36  ---          02 27 33  80.4  31.8 -0.4    -144.5    25   R  2   5333

00 08 36  MRK1066      02 27 33  80.8  45.3 -0.5    -130.1   -15   1  8   5333  00 08 36
00 09 46  ---          02 28 43  81.0  44.4 -0.5    -131.2    55   R  2   4400

00 09 46  J0253+3835   02 28 43  80.6  30.7 -0.4    -145.8   -15   1  8   4400  00 09 46
00 10 26  ---          02 29 24  80.6  30.0 -0.4    -146.5    25   R  2   3866

00 10 26  MRK1066      02 29 24  81.1  43.8 -0.5    -131.9   -15   1  8   3866  00 10 26
00 11 36  ---          02 30 34  81.3  42.8 -0.5    -133.1    55   R  2   2933

00 12 36  J0319+4130   02 31 34  75.4  38.5 -0.8    -134.3    42   1  8   2933  00 12 36
00 16 16  ---          02 35 15  75.9  36.5 -0.7    -136.9   220   R  2      0

00 18 16  J0253+3835   02 37 15  81.4  21.4 -0.3    -156.3   103   1  9      0  00 18 16
00 18 56  ---          02 37 55  81.4  20.6 -0.3    -157.2    40   F  1    533

00 18 56  MRK1066      02 37 55  82.3  35.2 -0.4    -141.7   -16   1  9    533  00 18 56
00 20 06  ---          02 39 05  82.4  33.8 -0.4    -143.3    54   F  1   1466

00 20 06  J0253+3835   02 39 05  81.5  19.2 -0.2    -158.8   -16   1  9   1466  00 20 06
00 20 46  ---          02 39 45  81.6  18.4 -0.2    -159.7    24   F  1   2000

00 20 46  MRK1066      02 39 45  82.5  33.0 -0.3    -144.2   -16   1  9   2000  00 20 46
00 21 56  ---          02 40 55  82.6  31.5 -0.3    -145.8    54   F  1   2933

00 21 56  J0253+3835   02 40 55  81.6  16.9 -0.2    -161.4   -16   1  9   2933  00 21 56
00 22 36  ---          02 41 36  81.7  16.0 -0.2    -162.3    24   F  1   3466

00 22 36  MRK1066      02 41 36  82.7  30.6 -0.3    -146.8   -16   1  9   3466  00 22 36
00 23 46  ---          02 42 46  82.8  29.1 -0.3    -148.5    54   F  1   4400

00 23 46  J0253+3835   02 42 46  81.7  14.5 -0.2    -164.0   -16   1  9   4400  00 23 46
00 24 26  ---          02 43 26  81.8  13.6 -0.2    -165.0    24   F  1   4933
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   9 Feb 2003   Day  40 ---

00 24 26  MRK1066      02 43 26  82.9  28.1 -0.3    -149.5   -16   1  9   4933  00 24 26
00 25 36  ---          02 44 36  83.0  26.5 -0.3    -151.4    54   F  1   5866

00 25 36  J0253+3835   02 44 36  81.8  12.1 -0.1    -166.7   -16   1  9   5866  00 25 36
00 26 16  ---          02 45 16  81.9  11.2 -0.1    -167.7    24   F  1   6400

00 26 16  MRK1066      02 45 16  83.1  25.5 -0.2    -152.4   -16   1  9   6400  00 26 16
00 27 26  ---          02 46 26  83.2  23.8 -0.2    -154.3    54   F  1   7333

00 27 26  J0253+3835   02 46 26  81.9   9.6 -0.1    -169.4   -15   1  9   7333  00 27 26
00 28 06  ---          02 47 06  81.9   8.7 -0.1    -170.4    25   F  1   7866

00 28 06  MRK1066      02 47 06  83.2  22.7 -0.2    -155.5   -15   1  9   7866  00 28 06
00 29 16  ---          02 48 17  83.3  20.9 -0.2    -157.4    55   F  1   8800

00 29 16  J0253+3835   02 48 17  82.0   7.1 -0.1    -172.2   -15   1  9   8800  00 29 16
00 29 56  ---          02 48 57  82.0   6.1 -0.1    -173.2    25   F  1   9333

00 29 56  MRK1066      02 48 57  83.4  19.8 -0.2    -158.6   -15   1  9   9333  00 29 56
00 31 06  ---          02 50 07  83.5  17.9 -0.2    -160.7    55   F  1  10267

00 31 06  J0253+3835   02 50 07  82.0   4.5 -0.1    -175.0   -15   1  9  10267  00 31 06
00 31 46  ---          02 50 47  82.0   3.6  0.0    -176.1    25   F  1  10800

00 31 46  MRK1066      02 50 47  83.5  16.8 -0.2    -161.9   -15   1  9  10800  00 31 46
00 32 56  ---          02 51 57  83.6  14.8 -0.1    -164.1    55   F  1  11733

00 32 56  J0253+3835   02 51 57  82.0   1.9  0.0    -177.9   -15   1  9  11733  00 32 56
00 33 36  ---          02 52 37  82.0   1.0  0.0    -178.9    25   F  1  12267

00 33 36  MRK1066      02 52 37  83.6  13.7 -0.1    -165.3   -14   1  9  12267  00 33 36
00 34 46  ---          02 53 48  83.7  11.6 -0.1    -167.5    56   F  1  13200

00 34 46  J0253+3835   02 53 48  82.0  -0.7  0.0     179.3   -14   1  9  13200  00 34 46
00 35 26  ---          02 54 28  82.0  -1.6  0.0     178.2    26   F  1  13733

00 35 26  MRK1066      02 54 28  83.7  10.4 -0.1    -168.8   -14   1  9  13733  00 35 26
00 36 36  ---          02 55 38  83.7   8.3 -0.1    -171.1    56   F  1  14667

00 36 36  J0253+3835   02 55 38  82.0  -3.2  0.0     176.4   -14   1  9  14667  00 36 36
00 37 16  ---          02 56 18  82.0  -4.2  0.0     175.4    26   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   9 Feb 2003   Day  40 ---

00 37 16  MRK1066      02 56 18  83.7   7.1 -0.1    -172.4   -14   1  9  15200  00 37 16
00 38 26  ---          02 57 28  83.8   5.0  0.0    -174.7    56   F  1  16133

00 38 26  J0253+3835   02 57 28  82.0  -5.8  0.1     173.6   -13   1  9  16133  00 38 26
00 39 06  ---          02 58 08  82.0  -6.7  0.1     172.6    27   F  1  16667

00 39 06  MRK1066      02 58 08  83.8   3.7  0.0    -176.0   -13   1  9  16667  00 39 06
00 40 16  ---          02 59 18  83.8   1.6  0.0    -178.3    57   F  1  17600

00 40 53  J0253+3835   02 59 56  81.9  -9.2  0.1     169.8    24   1 10  17600  00 40 53
00 41 33  ---          03 00 36  81.9 -10.1  0.1     168.8    40   R  1  17067

00 41 33  MRK1066      03 00 36  83.8  -0.8  0.0     179.1   -12   1 10  17067  00 41 33
00 42 43  ---          03 01 46  83.8  -3.0  0.0     176.8    58   R  1  16133

00 42 43  J0253+3835   03 01 46  81.8 -11.7  0.1     167.1   -12   1 10  16133  00 42 43
00 43 23  ---          03 02 26  81.8 -12.6  0.2     166.1    28   R  1  15600

00 43 23  MRK1066      03 02 26  83.8  -4.2  0.0     175.5   -12   1 10  15600  00 43 23
00 44 33  ---          03 03 36  83.8  -6.4  0.1     173.2    58   R  1  14667

00 44 33  J0253+3835   03 03 36  81.8 -14.1  0.2     164.4   -11   1 10  14667  00 44 33
00 45 13  ---          03 04 16  81.7 -15.0  0.2     163.4    29   R  1  14133

00 45 13  MRK1066      03 04 16  83.7  -7.6  0.1     171.8   -11   1 10  14133  00 45 13
00 46 23  ---          03 05 26  83.7  -9.7  0.1     169.6    59   R  1  13200

00 46 23  J0253+3835   03 05 26  81.7 -16.5  0.2     161.7   -11   1 10  13200  00 46 23
00 47 03  ---          03 06 07  81.6 -17.4  0.2     160.8    29   R  1  12667

00 47 03  MRK1066      03 06 07  83.7 -10.9  0.1     168.3   -10   1 10  12667  00 47 03
00 48 13  ---          03 07 17  83.6 -13.0  0.1     166.1    60   R  1  11733

00 48 13  J0253+3835   03 07 17  81.5 -18.8  0.2     159.2   -10   1 10  11733  00 48 13
00 48 53  ---          03 07 57  81.5 -19.7  0.2     158.3    30   R  1  11200

00 48 53  MRK1066      03 07 57  83.6 -14.1  0.1     164.8   -10   1 10  11200  00 48 53
00 50 03  ---          03 09 07  83.5 -16.1  0.1     162.6    60   R  1  10267

00 50 03  J0253+3835   03 09 07  81.4 -21.1  0.3     156.7   -10   1 10  10267  00 50 03
00 50 43  ---          03 09 47  81.3 -21.9  0.3     155.8    30   R  1   9733
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   9 Feb 2003   Day  40 ---

00 50 43  MRK1066      03 09 47  83.5 -17.2  0.2     161.4   -10   1 10   9733  00 50 43
00 51 53  ---          03 10 57  83.4 -19.2  0.2     159.3    60   R  1   8800

00 51 53  J0253+3835   03 10 57  81.2 -23.2  0.3     154.2   -10   1 10   8800  00 51 53
00 52 33  ---          03 11 37  81.2 -24.0  0.3     153.4    30   R  1   8266

00 52 33  MRK1066      03 11 37  83.4 -20.3  0.2     158.1   -10   1 10   8266  00 52 33
00 53 43  ---          03 12 48  83.3 -22.1  0.2     156.1    60   R  1   7333

00 53 43  J0253+3835   03 12 48  81.1 -25.3  0.3     151.9   -10   1 10   7333  00 53 43
00 54 23  ---          03 13 28  81.0 -26.1  0.3     151.1    30   R  1   6800

00 54 23  MRK1066      03 13 28  83.2 -23.1  0.2     155.0   -10   1 10   6800  00 54 23
00 55 33  ---          03 14 38  83.1 -24.9  0.2     153.1    60   R  1   5866

00 55 33  J0253+3835   03 14 38  80.9 -27.3  0.4     149.6   -10   1 10   5866  00 55 33
00 56 13  ---          03 15 18  80.8 -28.0  0.4     148.8    30   R  1   5333

00 56 13  MRK1066      03 15 18  83.0 -25.9  0.3     152.0   -10   1 10   5333  00 56 13
00 57 23  ---          03 16 28  82.9 -27.6  0.3     150.2    60   R  1   4400

00 58 23  J0319+4130   03 17 28  79.1   2.5  0.0    -177.1    34   1 10   4400  00 58 23
01 03 53  ---          03 22 59  79.1  -3.0  0.1     176.6   330   R  1      0

01 05 53  J0253+3835   03 25 00  79.7 -37.1  0.5     138.4    91   1  9      0  01 05 53
01 06 33  ---          03 25 40  79.6 -37.6  0.5     137.8    40   F  2    533

01 06 33  MRK1066      03 25 40  81.8 -38.8  0.4     137.6   -10   1  9    533  01 06 33
01 07 43  ---          03 26 50  81.7 -40.0  0.4     136.3    60   F  2   1466

01 07 43  J0253+3835   03 26 50  79.5 -38.5  0.6     136.7   -10   1  9   1466  01 07 43
01 08 23  ---          03 27 30  79.4 -39.1  0.6     136.1    30   F  2   2000

01 08 23  MRK1066      03 27 30  81.6 -40.7  0.5     135.5   -10   1  9   2000  01 08 23
01 09 33  ---          03 28 40  81.4 -41.8  0.5     134.2    60   F  2   2933

01 09 33  J0253+3835   03 28 40  79.2 -39.9  0.6     135.0   -10   1  9   2933  01 09 33
01 10 13  ---          03 29 20  79.1 -40.4  0.6     134.4    30   F  2   3466

01 10 13  MRK1066      03 29 20  81.3 -42.4  0.5     133.5   -10   1  9   3466  01 10 13
01 11 23  ---          03 30 31  81.2 -43.5  0.5     132.3    60   F  2   4400
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   9 Feb 2003   Day  40 ---

01 11 23  J0253+3835   03 30 31  79.0 -41.3  0.6     133.4   -10   1  9   4400  01 11 23
01 12 03  ---          03 31 11  78.9 -41.7  0.6     132.9    30   F  2   4933

01 12 03  MRK1066      03 31 11  81.1 -44.0  0.5     131.6   -10   1  9   4933  01 12 03
01 13 13  ---          03 32 21  80.9 -45.0  0.5     130.5    60   F  2   5867

01 13 13  J0253+3835   03 32 21  78.7 -42.5  0.7     131.9   -10   1  9   5867  01 13 13
01 13 53  ---          03 33 01  78.6 -43.0  0.7     131.4    30   F  2   6400

01 13 53  MRK1066      03 33 01  80.8 -45.6  0.5     129.9   -10   1  9   6400  01 13 53
01 15 03  ---          03 34 11  80.6 -46.5  0.6     128.8    60   F  2   7333

01 15 03  J0253+3835   03 34 11  78.4 -43.7  0.7     130.5   -10   1  9   7333  01 15 03
01 15 43  ---          03 34 51  78.3 -44.1  0.7     129.9    30   F  2   7867

01 15 43  MRK1066      03 34 51  80.5 -47.0  0.6     128.2   -10   1  9   7867  01 15 43
01 16 53  ---          03 36 01  80.3 -47.8  0.6     127.2    60   F  2   8800

01 16 53  J0253+3835   03 36 01  78.2 -44.8  0.7     129.1   -10   1  9   8800  01 16 53
01 17 33  ---          03 36 42  78.1 -45.2  0.7     128.6    30   F  2   9333

01 17 33  MRK1066      03 36 42  80.2 -48.3  0.6     126.6   -10   1  9   9333  01 17 33
01 18 43  ---          03 37 52  80.0 -49.1  0.6     125.6    60   F  2  10267

01 18 43  J0253+3835   03 37 52  77.9 -45.9  0.7     127.7   -10   1  9  10267  01 18 43
01 19 23  ---          03 38 32  77.8 -46.3  0.8     127.3    30   F  2  10800

01 19 23  MRK1066      03 38 32  79.9 -49.6  0.6     125.1   -10   1  9  10800  01 19 23
01 20 33  ---          03 39 42  79.7 -50.3  0.7     124.2    60   F  2  11733

01 20 33  J0253+3835   03 39 42  77.6 -46.9  0.8     126.4   -10   1  9  11733  01 20 33
01 21 13  ---          03 40 22  77.5 -47.3  0.8     126.0    30   F  2  12267

01 21 13  MRK1066      03 40 22  79.6 -50.7  0.7     123.7   -10   1  9  12267  01 21 13
01 22 23  ---          03 41 32  79.4 -51.4  0.7     122.8    60   F  2  13200

01 22 23  J0253+3835   03 41 32  77.3 -47.9  0.8     125.2   -10   1  9  13200  01 22 23
01 23 03  ---          03 42 12  77.2 -48.2  0.8     124.8    30   F  2  13733

01 23 03  MRK1066      03 42 12  79.3 -51.8  0.7     122.3   -10   1  9  13733  01 23 03
01 24 13  ---          03 43 23  79.1 -52.5  0.7     121.5    60   F  2  14667
Schedule for VLBA_FD   (Code Fd )                                   Page  32
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   9 Feb 2003   Day  40 ---

01 24 13  J0253+3835   03 43 23  77.0 -48.8  0.8     124.0   -10   1  9  14667  01 24 13
01 24 53  ---          03 44 03  76.9 -49.1  0.8     123.6    30   F  2  15200

01 24 53  MRK1066      03 44 03  79.0 -52.8  0.7     121.0   -10   1  9  15200  01 24 53
01 26 03  ---          03 45 13  78.8 -53.5  0.8     120.3    60   F  2  16133

01 26 03  J0253+3835   03 45 13  76.7 -49.7  0.9     122.9   -10   1  9  16133  01 26 03
01 26 43  ---          03 45 53  76.6 -50.0  0.9     122.5    30   F  2  16667

01 26 43  MRK1066      03 45 53  78.7 -53.8  0.8     119.8   -10   1  9  16667  01 26 43
01 27 53  ---          03 47 03  78.5 -54.4  0.8     119.1    60   F  2  17600

01 28 53  J0530+1331   03 48 03  60.8 120.1 -1.7     -50.0   -62   1 10  17600  01 28 53
01 32 33  ---          03 51 44  61.4 121.3 -1.7     -49.1   158   R  2  14667

01 33 33  J0253+3835   03 52 44  75.4 -52.8  1.0     118.7   -62   1 10  14667  01 33 33
01 34 13  ---          03 53 24  75.3 -53.1  1.0     118.3   -22   R  2  14133

01 34 13  MRK1066      03 53 24  77.3 -57.2  0.9     115.4   -10   1 10  14133  01 34 13
01 35 23  ---          03 54 35  77.1 -57.6  0.9     114.8    60   R  2  13200

01 35 23  J0253+3835   03 54 35  75.1 -53.5  1.0     117.8   -10   1 10  13200  01 35 23
01 36 03  ---          03 55 15  75.0 -53.7  1.0     117.4    30   R  2  12667

01 36 03  MRK1066      03 55 15  77.0 -57.9  0.9     114.5   -10   1 10  12667  01 36 03
01 37 13  ---          03 56 25  76.8 -58.3  0.9     113.9    60   R  2  11733

01 37 13  J0253+3835   03 56 25  74.8 -54.1  1.1     116.9   -10   1 10  11733  01 37 13
01 37 53  ---          03 57 05  74.7 -54.3  1.1     116.5    30   R  2  11200

01 37 53  MRK1066      03 57 05  76.7 -58.5  0.9     113.5   -10   1 10  11200  01 37 53
01 39 03  ---          03 58 15  76.4 -58.9  1.0     113.0    60   R  2  10267

01 39 03  J0253+3835   03 58 15  74.5 -54.7  1.1     116.0   -10   1 10  10267  01 39 03
01 39 43  ---          03 58 55  74.4 -54.9  1.1     115.7    30   R  2   9733

01 39 43  MRK1066      03 58 55  76.3 -59.1  1.0     112.7   -10   1 10   9733  01 39 43
01 40 53  ---          04 00 05  76.1 -59.5  1.0     112.1    60   R  2   8800

01 40 53  J0253+3835   04 00 05  74.2 -55.3  1.1     115.1   -10   1 10   8800  01 40 53
01 41 33  ---          04 00 46  74.0 -55.5  1.1     114.9    30   R  2   8267
Schedule for VLBA_FD   (Code Fd )                                   Page  33
               GP 34 = Water masers in Mrk 1066
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   9 Feb 2003   Day  40 ---

01 41 33  MRK1066      04 00 46  76.0 -59.7  1.0     111.8   -10   1 10   8267  01 41 33
01 42 43  ---          04 01 56  75.8 -60.1  1.0     111.3    60   R  2   7333

01 42 43  J0253+3835   04 01 56  73.8 -55.8  1.1     114.3   -10   1 10   7333  01 42 43
01 43 23  ---          04 02 36  73.7 -56.0  1.2     114.1    30   R  2   6800

01 43 23  MRK1066      04 02 36  75.6 -60.3  1.0     111.0   -10   1 10   6800  01 43 23
01 44 33  ---          04 03 46  75.4 -60.6  1.1     110.5    60   R  2   5867

01 44 33  J0253+3835   04 03 46  73.5 -56.4  1.2     113.6   -10   1 10   5867  01 44 33
01 45 13  ---          04 04 26  73.4 -56.5  1.2     113.3    30   R  2   5333

01 45 13  MRK1066      04 04 26  75.3 -60.8  1.1     110.2   -10   1 10   5333  01 45 13
01 46 23  ---          04 05 36  75.1 -61.1  1.1     109.8    60   R  2   4400

01 46 23  J0253+3835   04 05 36  73.2 -56.9  1.2     112.8   -10   1 10   4400  01 46 23
01 47 03  ---          04 06 16  73.1 -57.0  1.2     112.5    30   R  2   3867

01 47 03  MRK1066      04 06 16  74.9 -61.3  1.1     109.5   -10   1 10   3867  01 47 03
01 48 13  ---          04 07 27  74.7 -61.6  1.1     109.0    60   R  2   2933

01 48 13  J0253+3835   04 07 27  72.8 -57.3  1.2     112.1   -10   1 10   2933  01 48 13
01 48 53  ---          04 08 07  72.7 -57.5  1.2     111.8    30   R  2   2400

01 48 53  MRK1066      04 08 07  74.6 -61.7  1.1     108.8   -10   1 10   2400  01 48 53
01 50 03  ---          04 09 17  74.4 -62.0  1.2     108.3    60   R  2   1466

01 50 03  J0253+3835   04 09 17  72.5 -57.8  1.3     111.3   -10   1 10   1466  01 50 03
01 50 43  ---          04 09 57  72.4 -57.9  1.3     111.1    30   R  2    933

01 50 43  MRK1066      04 09 57  74.3 -62.2  1.2     108.1   -10   1 10    933  01 50 43
01 51 53  ---          04 11 07  74.0 -62.4  1.2     107.7    60   R  2      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gp034.set
   Matches group v1cm_b2 in /data/AU_1/ali/SCHED/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 32.000
   Number of channels:  2    Passes/head pos:   2       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=  21200.00  21200.00
   Net SB=         U         U
   Pol.  =      RCP       LCP 
   BBC   =         1         2
   BBC SB=         U         U
   IF    =        B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1     15.4     12.1

  The following frequency sets based on this setup were used.

  Frequency Set:   1  Based on FREQ, BW, and/or DOPPLER in schedule.  Used pcal sets:   1
   LO sum=   21959.02  21959.02
   BBC fr=     759.02    759.02
   Bandwd=      8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = OFF 
    PCALXB1=   S1    S2    OFF   OFF   OFF   OFF   OFF   OFF
    PCALXB2=   M1    M2    OFF   OFF   OFF   OFF   OFF   OFF
    PCALFR1=     0     0     0     0     0     0     0     0
    PCALFR2=     0     0     0     0     0     0     0     0

   Track assignments are: 
    track1=   2, 18
    track2=   3, 19
    barrel=roll_off 
 SOURCE LIST -- GP 34 = Water masers in Mrk 1066
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * MRK1066           02 56 49.847541   * 02 59 58.591000     03 00 09.076426 
                     36 37 20.88339    * 36 49 14.27000      36 50 04.01294 
                     From catalog imbedded in main SCHED input file.

 * J0253+3835        02 49 58.983977   * 02 53 08.888121     02 53 19.375574 
                     38 23 10.94904    * 38 35 24.99892      38 36 16.41524 
                     From catalog imbedded in main SCHED input file.

 * J0319+4130        03 16 29.567273   * 03 19 48.160103     03 19 59.343203 
                     41 19 51.91592    * 41 30 42.10305      41 31 30.03631 
                     From catalog imbedded in main SCHED input file.

 * J0530+1331        05 28 06.759213   * 05 30 56.416744     05 31 06.786948 
                     13 29 42.28888    * 13 31 55.14955      13 32 03.99888 
                     From catalog imbedded in main SCHED input file.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   MRK1066             93.3
   J0253+3835          92.6
   J0319+4130          98.2
   J0530+1331         122.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

