  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
 Exp. Code:  GB053   


Schedule Version:       1.00                                              
Processed by SCHED version: NRAO internal release of 4 October 2004       

PI:       Norbert Bartel                                                  

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@yorku.ca                                                 
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 256-8-2-ul 6cm                                       

Notes:    Fringe finder  : OQ208, OJ287, 3C273                            
          Pol. Calibrator: OQ208, OJ287                                   
          Amplitude check: OQ208, OJ287                                   
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

 Next scan frequencies:  4979.49  4979.49  4979.49  4979.49  4995.49  4995.49
                         4995.49  4995.49
 Next BBC frequencies:    879.49   879.49   879.49   879.49   895.49   895.49
                          895.49   895.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

03 18 09  J1215+17     06 42 44  14.2  78.6 -5.5     -61.8     0   1  1      0  03 18 09
03 19 19  ---          06 43 54  14.5  78.7 -5.5     -61.9    70   F  1    933

03 19 19  SN1979C      06 43 54  12.3  78.8 -5.7     -61.3   -10   1  1    933  03 19 19
03 22 09  ---          06 46 45  12.9  79.1 -5.6     -61.4   160   F  1   3200

03 22 09  J1215+17     06 46 45  15.1  79.1 -5.5     -62.0   -10   1  1   3200  03 22 09
03 23 29  ---          06 48 05  15.4  79.2 -5.5     -62.0    70   F  1   4267

03 23 29  SN1979C      06 48 05  13.2  79.3 -5.6     -61.5   -10   1  1   4267  03 23 29
03 26 19  ---          06 50 56  13.8  79.6 -5.5     -61.6   160   F  1   6533

03 26 19  J1215+17     06 50 56  16.0  79.5 -5.4     -62.2   -10   1  1   6533  03 26 19
03 27 39  ---          06 52 16  16.3  79.7 -5.4     -62.2    70   F  1   7600

03 27 39  SN1979C      06 52 16  14.1  79.8 -5.5     -61.6   -10   1  1   7600  03 27 39
03 30 29  ---          06 55 06  14.7  80.1 -5.5     -61.7   160   F  1   9867

03 30 29  J1215+17     06 55 06  16.9  80.0 -5.3     -62.3   -10   1  1   9867  03 30 29
03 31 49  ---          06 56 27  17.1  80.2 -5.3     -62.4    70   F  1  10933

03 31 49  SN1979C      06 56 27  14.9  80.3 -5.4     -61.8   -10   1  1  10933  03 31 49
03 34 39  ---          06 59 17  15.6  80.6 -5.4     -61.9   160   F  1  13200

03 34 39  J1215+17     06 59 17  17.7  80.5 -5.3     -62.5   -10   1  1  13200  03 34 39
03 35 59  ---          07 00 37  18.0  80.7 -5.2     -62.5    70   F  1  14267

03 35 59  SN1979C      07 00 37  15.8  80.8 -5.4     -61.9   -10   1  1  14267  03 35 59
03 38 49  ---          07 03 28  16.4  81.1 -5.3     -62.0   160   F  1  16533

03 38 49  J1215+17     07 03 28  18.6  81.0 -5.2     -62.6   -10   1  1  16533  03 38 49
03 40 09  ---          07 04 48  18.9  81.2 -5.2     -62.7    70   F  1  17600

03 40 46  J1215+17     07 05 25  19.1  81.2 -5.2     -62.7    32   1  2  17600  03 40 46
03 41 56  ---          07 06 35  19.3  81.4 -5.1     -62.7    70   R  1  16667
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

03 41 56  SN1979C      07 06 35  17.1  81.5 -5.3     -62.2   -10   1  2  16667  03 41 56
03 44 46  ---          07 09 26  17.7  81.8 -5.2     -62.2   160   R  1  14400

03 44 46  J1215+17     07 09 26  19.9  81.7 -5.1     -62.8   -10   1  2  14400  03 44 46
03 46 06  ---          07 10 46  20.2  81.8 -5.1     -62.9    70   R  1  13333

03 46 06  SN1979C      07 10 46  18.0  82.0 -5.2     -62.3   -10   1  2  13333  03 46 06
03 48 56  ---          07 13 36  18.6  82.3 -5.2     -62.4   160   R  1  11067

03 48 56  J1215+17     07 13 36  20.8  82.2 -5.0     -63.0   -10   1  2  11067  03 48 56
03 50 16  ---          07 14 57  21.1  82.3 -5.0     -63.0    70   R  1  10000

03 50 16  SN1979C      07 14 57  18.9  82.5 -5.1     -62.4   -10   1  2  10000  03 50 16
03 53 06  ---          07 17 47  19.5  82.8 -5.1     -62.5   160   R  1   7733

03 53 06  J1215+17     07 17 47  21.7  82.7 -5.0     -63.1   -10   1  2   7733  03 53 06
03 54 26  ---          07 19 07  22.0  82.8 -4.9     -63.1    70   R  1   6667

03 54 26  SN1979C      07 19 07  19.8  83.0 -5.1     -62.5   -10   1  2   6667  03 54 26
03 57 16  ---          07 21 58  20.4  83.3 -5.0     -62.6   160   R  1   4400

03 57 16  J1215+17     07 21 58  22.6  83.2 -4.9     -63.2   -10   1  2   4400  03 57 16
03 58 36  ---          07 23 18  22.9  83.3 -4.9     -63.3    70   R  1   3333

03 58 36  SN1979C      07 23 18  20.7  83.4 -5.0     -62.7   -10   1  2   3333  03 58 36
04 01 26  ---          07 26 08  21.3  83.8 -5.0     -62.7   160   R  1   1067

04 01 26  J1215+17     07 26 08  23.5  83.6 -4.8     -63.3   -10   1  2   1067  04 01 26
04 02 46  ---          07 27 29  23.8  83.8 -4.8     -63.4    70   R  1      0

04 03 23  J1215+17     07 28 06  23.9  83.9 -4.8     -63.4    32   1  3      0  04 03 23
04 04 33  ---          07 29 16  24.1  84.0 -4.8     -63.4    70   F  1    933

04 04 33  SN1979C      07 29 16  21.9  84.2 -4.9     -62.8   -10   1  3    933  04 04 33
04 07 23  ---          07 32 06  22.6  84.5 -4.9     -62.9   160   F  1   3200

04 07 23  J1215+17     07 32 06  24.7  84.3 -4.7     -63.5   -10   1  3   3200  04 07 23
04 08 43  ---          07 33 27  25.0  84.5 -4.7     -63.5    70   F  1   4267

04 08 43  SN1979C      07 33 27  22.8  84.6 -4.8     -62.9   -10   1  3   4267  04 08 43
04 11 33  ---          07 36 17  23.4  85.0 -4.8     -63.0   160   F  1   6533
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

04 11 33  J1215+17     07 36 17  25.6  84.8 -4.7     -63.6   -10   1  3   6533  04 11 33
04 12 53  ---          07 37 37  25.9  85.0 -4.6     -63.6    70   F  1   7600

04 12 53  SN1979C      07 37 37  23.7  85.1 -4.8     -63.0   -10   1  3   7600  04 12 53
04 15 43  ---          07 40 28  24.3  85.5 -4.7     -63.0   160   F  1   9867

04 15 43  J1215+17     07 40 28  26.5  85.3 -4.6     -63.7   -10   1  3   9867  04 15 43
04 17 03  ---          07 41 48  26.8  85.5 -4.6     -63.7    70   F  1  10933

04 17 03  SN1979C      07 41 48  24.6  85.6 -4.7     -63.1   -10   1  3  10933  04 17 03
04 19 53  ---          07 44 38  25.2  86.0 -4.6     -63.1   160   F  1  13200

04 19 53  J1215+17     07 44 38  27.4  85.8 -4.5     -63.7   -10   1  3  13200  04 19 53
04 21 13  ---          07 45 59  27.7  86.0 -4.5     -63.8    70   F  1  14267

04 21 13  SN1979C      07 45 59  25.5  86.1 -4.6     -63.1   -10   1  3  14267  04 21 13
04 24 03  ---          07 48 49  26.1  86.5 -4.6     -63.2   160   F  1  16533

04 24 03  J1215+17     07 48 49  28.3  86.3 -4.4     -63.8   -10   1  3  16533  04 24 03
04 25 23  ---          07 50 09  28.6  86.5 -4.4     -63.8    70   F  1  17600

04 26 00  J1215+17     07 50 46  28.7  86.6 -4.4     -63.8    32   1  4  17600  04 26 00
04 27 10  ---          07 51 57  29.0  86.7 -4.4     -63.9    70   R  1  16667

04 27 10  SN1979C      07 51 57  26.8  86.9 -4.5     -63.2   -10   1  4  16667  04 27 10
04 30 00  ---          07 54 47  27.4  87.2 -4.5     -63.3   160   R  1  14400

04 30 00  J1215+17     07 54 47  29.6  87.0 -4.3     -63.9   -10   1  4  14400  04 30 00
04 31 20  ---          07 56 07  29.9  87.2 -4.3     -63.9    70   R  1  13333

04 31 20  SN1979C      07 56 07  27.7  87.4 -4.5     -63.3   -10   1  4  13333  04 31 20
04 34 10  ---          07 58 58  28.3  87.7 -4.4     -63.3   160   R  1  11067

04 34 10  J1215+17     07 58 58  30.5  87.6 -4.3     -63.9   -10   1  4  11067  04 34 10
04 35 30  ---          08 00 18  30.8  87.7 -4.3     -64.0    70   R  1  10000

04 35 30  SN1979C      08 00 18  28.6  87.9 -4.4     -63.3   -10   1  4  10000  04 35 30
04 38 20  ---          08 03 08  29.2  88.2 -4.3     -63.3   160   R  1   7733

04 38 20  J1215+17     08 03 08  31.4  88.1 -4.2     -64.0   -10   1  4   7733  04 38 20
04 39 40  ---          08 04 29  31.7  88.2 -4.2     -64.0    70   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

04 39 40  SN1979C      08 04 29  29.5  88.4 -4.3     -63.3   -10   1  4   6667  04 39 40
04 42 30  ---          08 07 19  30.1  88.8 -4.3     -63.4   160   R  1   4400

04 42 30  J1215+17     08 07 19  32.3  88.6 -4.1     -64.0   -10   1  4   4400  04 42 30
04 43 50  ---          08 08 39  32.6  88.7 -4.1     -64.0    70   R  1   3333

04 43 50  SN1979C      08 08 39  30.4  88.9 -4.2     -63.4   -10   1  4   3333  04 43 50
04 46 40  ---          08 11 30  31.0  89.3 -4.2     -63.4   160   R  1   1067

04 46 40  J1215+17     08 11 30  33.2  89.1 -4.1     -64.0   -10   1  4   1067  04 46 40
04 48 00  ---          08 12 50  33.5  89.3 -4.0     -64.0    70   R  1      0

04 51 00  3C273        08 15 51  23.8 102.5 -4.2     -57.2   155   1  5      0  04 51 00
04 54 00  ---          08 18 51  24.4 102.9 -4.2     -57.0   180   F  1   2400

04 54 00  J1215+17     08 18 51  34.8  90.0 -3.9     -64.0   -27   1  5   2400  04 54 00
04 57 00  ---          08 21 52  35.4  90.4 -3.9     -64.0   153   F  1   4800

04 57 00  SN1979C      08 21 52  33.2  90.6 -4.0     -63.4   -10   1  5   4800  04 57 00
04 59 10  ---          08 24 02  33.7  90.9 -4.0     -63.4   120   F  1   6533

04 59 10  J1215+17     08 24 02  35.9  90.7 -3.9     -64.0   -10   1  5   6533  04 59 10
05 00 30  ---          08 25 22  36.2  90.9 -3.8     -64.0    70   F  1   7600

05 00 30  SN1979C      08 25 22  34.0  91.1 -4.0     -63.4   -10   1  5   7600  05 00 30
05 03 20  ---          08 28 13  34.6  91.4 -3.9     -63.4   160   F  1   9867

05 03 20  J1215+17     08 28 13  36.8  91.2 -3.8     -64.0   -10   1  5   9867  05 03 20
05 04 40  ---          08 29 33  37.1  91.4 -3.8     -64.0    70   F  1  10933

05 04 40  SN1979C      08 29 33  34.9  91.6 -3.9     -63.3   -10   1  5  10933  05 04 40
05 07 30  ---          08 32 23  35.5  92.0 -3.8     -63.3   160   F  1  13200

05 07 30  J1215+17     08 32 23  37.7  91.8 -3.7     -64.0   -10   1  5  13200  05 07 30
05 08 50  ---          08 33 43  38.0  92.0 -3.7     -64.0    70   F  1  14267

05 08 50  SN1979C      08 33 43  35.8  92.2 -3.8     -63.3   -10   1  5  14267  05 08 50
05 11 40  ---          08 36 34  36.4  92.5 -3.8     -63.3   160   F  1  16533

05 11 40  J1215+17     08 36 34  38.6  92.3 -3.6     -64.0   -10   1  5  16533  05 11 40
05 13 00  ---          08 37 54  38.9  92.5 -3.6     -63.9    70   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

05 15 00  J1215+17     08 39 54  39.3  92.8 -3.6     -63.9   113   1  6  17600  05 15 00
05 16 40  ---          08 41 35  39.7  93.0 -3.6     -63.9   100   R  1  16267

05 16 40  SN1979C      08 41 35  37.5  93.2 -3.7     -63.2   -10   1  6  16267  05 16 40
05 19 55  ---          08 44 50  38.2  93.7 -3.6     -63.2   185   R  1  13667

05 19 55  J1215+17     08 44 50  40.4  93.5 -3.5     -63.8   -10   1  6  13667  05 19 55
05 21 45  ---          08 46 41  40.8  93.7 -3.5     -63.8   100   R  1  12200

05 21 45  SN1979C      08 46 41  38.6  93.9 -3.6     -63.1   -10   1  6  12200  05 21 45
05 25 00  ---          08 49 56  39.3  94.4 -3.6     -63.1   185   R  1   9600

05 25 00  J1215+17     08 49 56  41.5  94.2 -3.4     -63.7   -10   1  6   9600  05 25 00
05 26 50  ---          08 51 46  41.9  94.4 -3.4     -63.7   100   R  1   8133

05 26 50  SN1979C      08 51 46  39.7  94.6 -3.5     -63.0   -10   1  6   8133  05 26 50
05 30 05  ---          08 55 02  40.4  95.1 -3.5     -62.9   185   R  1   5533

05 30 05  J1215+17     08 55 02  42.6  94.9 -3.3     -63.6   -10   1  6   5533  05 30 05
05 31 55  ---          08 56 52  43.0  95.2 -3.3     -63.6   100   R  1   4067

05 31 55  SN1979C      08 56 52  40.8  95.4 -3.4     -62.9   -10   1  6   4067  05 31 55
05 35 10  ---          09 00 08  41.5  95.8 -3.4     -62.8   185   R  1   1467

05 35 10  J1215+17     09 00 08  43.7  95.7 -3.3     -63.5   -10   1  6   1467  05 35 10
05 37 00  ---          09 01 58  44.0  95.9 -3.2     -63.4   100   R  1      0

05 52 00  3C273        09 17 01  36.3 112.6 -3.2     -52.6   879   1  7      0  05 52 00
05 53 20  ---          09 18 21  36.6 112.9 -3.2     -52.5    80   F  1   1067

05 53 20  J1215+17     09 18 21  47.5  98.5 -2.9     -62.8   -28   1  7   1067  05 53 20
05 59 40  ---          09 24 42  48.9  99.5 -2.8     -62.5   352   F  1   6133

05 59 40  SN1979C      09 24 42  46.7  99.7 -3.0     -61.8   -10   1  7   6133  05 59 40
06 02 40  ---          09 27 42  47.3 100.2 -2.9     -61.6   170   F  1   8533

06 02 40  J1215+17     09 27 42  49.5 100.0 -2.8     -62.3   -10   1  7   8533  06 02 40
06 04 30  ---          09 29 33  49.9 100.3 -2.8     -62.2   100   F  1  10000

06 04 30  SN1979C      09 29 33  47.7 100.5 -2.9     -61.5   -10   1  7  10000  06 04 30
06 07 30  ---          09 32 33  48.4 101.0 -2.8     -61.4   170   F  1  12400
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

06 07 30  J1215+17     09 32 33  50.6 100.9 -2.7     -62.0   -10   1  7  12400  06 07 30
06 09 20  ---          09 34 23  50.9 101.2 -2.7     -61.9   100   F  1  13867

06 09 20  SN1979C      09 34 23  48.7 101.3 -2.8     -61.2   -10   1  7  13867  06 09 20
06 12 10  ---          09 37 14  49.3 101.8 -2.8     -61.1   160   F  1  16133

06 12 10  J1215+17     09 37 14  51.5 101.7 -2.6     -61.7   -10   1  7  16133  06 12 10
06 14 00  ---          09 39 04  51.9 102.0 -2.6     -61.6   100   F  1  17600

06 14 37  J1215+17     09 39 41  52.1 102.2 -2.6     -61.5    32   1  8  17600  06 14 37
06 16 17  ---          09 41 22  52.4 102.5 -2.6     -61.4   100   R  1  16267

06 16 17  SN1979C      09 41 22  50.2 102.6 -2.7     -60.8   -10   1  8  16267  06 16 17
06 19 22  ---          09 44 27  50.9 103.1 -2.6     -60.5   175   R  1  13800

06 19 22  J1215+17     09 44 27  53.1 103.1 -2.5     -61.2   -10   1  8  13800  06 19 22
06 21 02  ---          09 46 07  53.4 103.4 -2.5     -61.0    90   R  1  12467

06 21 02  SN1979C      09 46 07  51.2 103.5 -2.6     -60.4   -10   1  8  12467  06 21 02
06 24 07  ---          09 49 13  51.9 104.0 -2.6     -60.2   175   R  1  10000

06 24 07  J1215+17     09 49 13  54.1 104.0 -2.4     -60.7   -10   1  8  10000  06 24 07
06 27 07  ---          09 52 13  54.7 104.6 -2.4     -60.5   170   R  1   7600

06 27 07  SN1979C      09 52 13  52.5 104.6 -2.5     -59.9   -10   1  8   7600  06 27 07
06 30 27  ---          09 55 34  53.2 105.3 -2.5     -59.6   190   R  1   4933

06 30 27  J1215+17     09 55 34  55.4 105.3 -2.3     -60.2   -10   1  8   4933  06 30 27
06 33 27  ---          09 58 34  56.0 105.9 -2.3     -59.8   170   R  1   2533

06 33 27  SN1979C      09 58 34  53.8 105.9 -2.4     -59.3   -10   1  8   2533  06 33 27
06 36 37  ---          10 01 45  54.5 106.6 -2.4     -59.0   180   R  1      0

06 37 14  J1215+17     10 02 22  56.8 106.8 -2.2     -59.4    26   1  9      0  06 37 14
06 38 54  ---          10 04 02  57.1 107.1 -2.2     -59.2   100   F  1   1333

06 38 54  SN1979C      10 04 02  54.9 107.1 -2.3     -58.7   -10   1  9   1333  06 38 54
06 42 09  ---          10 07 18  55.6 107.8 -2.3     -58.3   185   F  1   3933

06 42 09  J1215+17     10 07 18  57.8 107.9 -2.1     -58.8   -10   1  9   3933  06 42 09
06 43 59  ---          10 09 08  58.2 108.3 -2.1     -58.6   100   F  1   5400
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

06 43 59  SN1979C      10 09 08  56.0 108.2 -2.2     -58.1   -10   1  9   5400  06 43 59
06 47 14  ---          10 12 24  56.6 109.0 -2.2     -57.7   185   F  1   8000

06 47 14  J1215+17     10 12 24  58.8 109.1 -2.0     -58.2   -10   1  9   8000  06 47 14
06 49 04  ---          10 14 14  59.2 109.5 -2.0     -57.9   100   F  1   9467

06 49 04  SN1979C      10 14 14  57.0 109.4 -2.2     -57.5   -10   1  9   9467  06 49 04
06 52 19  ---          10 17 29  57.7 110.2 -2.1     -57.0   185   F  1  12067

06 52 19  J1215+17     10 17 29  59.9 110.4 -2.0     -57.5   -10   1  9  12067  06 52 19
06 54 09  ---          10 19 20  60.2 110.8 -1.9     -57.2   100   F  1  13533

06 54 09  SN1979C      10 19 20  58.0 110.6 -2.1     -56.8   -10   1  9  13533  06 54 09
06 57 24  ---          10 22 35  58.7 111.5 -2.0     -56.3   185   F  1  16133

06 57 24  J1215+17     10 22 35  60.9 111.7 -1.9     -56.7   -10   1  9  16133  06 57 24
06 59 14  ---          10 24 26  61.3 112.2 -1.8     -56.4   100   F  1  17600

07 14 13  J1215+17     10 39 27  64.2 116.7 -1.6     -53.4   887   1 10  17600  07 14 13
07 15 53  ---          10 41 07  64.5 117.3 -1.6     -53.1   100   R  1  16267

07 15 53  SN1979C      10 41 07  62.3 116.7 -1.7     -53.0   -10   1 10  16267  07 15 53
07 19 08  ---          10 44 23  63.0 117.7 -1.6     -52.3   185   R  1  13667

07 19 08  J1215+17     10 44 23  65.1 118.4 -1.5     -52.3   -10   1 10  13667  07 19 08
07 20 58  ---          10 46 13  65.5 119.0 -1.5     -51.8   100   R  1  12200

07 20 58  SN1979C      10 46 13  63.3 118.3 -1.6     -51.9   -10   1 10  12200  07 20 58
07 24 13  ---          10 49 29  63.9 119.4 -1.6     -51.1   185   R  1   9600

07 24 13  J1215+17     10 49 29  66.1 120.2 -1.4     -51.0   -10   1 10   9600  07 24 13
07 26 03  ---          10 51 19  66.4 120.9 -1.4     -50.5   100   R  1   8133

07 26 03  SN1979C      10 51 19  64.3 120.1 -1.5     -50.7   -10   1 10   8133  07 26 03
07 29 18  ---          10 54 35  64.9 121.2 -1.5     -49.9   185   R  1   5533

07 29 18  J1215+17     10 54 35  67.0 122.2 -1.3     -49.6   -10   1 10   5533  07 29 18
07 31 08  ---          10 56 25  67.4 122.9 -1.3     -49.0   100   R  1   4067

07 31 08  SN1979C      10 56 25  65.2 121.9 -1.4     -49.4   -10   1 10   4067  07 31 08
07 34 23  ---          10 59 40  65.8 123.2 -1.4     -48.5   185   R  1   1467
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

07 34 23  J1215+17     10 59 40  67.9 124.3 -1.3     -48.0   -10   1 10   1467  07 34 23
07 36 13  ---          11 01 31  68.3 125.1 -1.2     -47.4   100   R  1      0

07 36 50  J1215+17     11 02 08  68.4 125.3 -1.2     -47.2    32   1 11      0  07 36 50
07 38 10  ---          11 03 28  68.6 125.9 -1.2     -46.7    80   F  1   1067

07 38 10  SN1979C      11 03 28  66.5 124.7 -1.3     -47.3   -10   1 11   1067  07 38 10
07 40 50  ---          11 06 08  66.9 125.8 -1.3     -46.5   150   F  1   3200

07 40 50  J1215+17     11 06 08  69.1 127.2 -1.2     -45.8   -10   1 11   3200  07 40 50
07 42 20  ---          11 07 39  69.3 127.9 -1.1     -45.2    80   F  1   4400

07 42 20  SN1979C      11 07 39  67.2 126.4 -1.3     -46.0   -10   1 11   4400  07 42 20
07 45 00  ---          11 10 19  67.7 127.6 -1.2     -45.1   150   F  1   6533

07 45 00  J1215+17     11 10 19  69.8 129.2 -1.1     -44.2   -10   1 11   6533  07 45 00
07 46 20  ---          11 11 39  70.0 129.8 -1.1     -43.7    70   F  1   7600

07 46 20  SN1979C      11 11 39  67.9 128.2 -1.2     -44.6   -10   1 11   7600  07 46 20
07 49 10  ---          11 14 30  68.4 129.5 -1.1     -43.6   160   F  1   9867

07 49 10  J1215+17     11 14 30  70.5 131.3 -1.0     -42.5   -10   1 11   9867  07 49 10
07 50 30  ---          11 15 50  70.7 132.0 -1.0     -41.9    70   F  1  10933

07 50 30  SN1979C      11 15 50  68.6 130.2 -1.1     -43.1   -10   1 11  10933  07 50 30
07 53 20  ---          11 18 40  69.0 131.6 -1.1     -42.0   160   F  1  13200

07 53 20  J1215+17     11 18 40  71.1 133.6 -0.9     -40.6   -10   1 11  13200  07 53 20
07 54 40  ---          11 20 01  71.3 134.3 -0.9     -40.0    70   F  1  14267

07 54 40  SN1979C      11 20 01  69.3 132.2 -1.1     -41.5   -10   1 11  14267  07 54 40
07 57 30  ---          11 22 51  69.7 133.7 -1.0     -40.3   160   F  1  16533

07 57 30  J1215+17     11 22 51  71.8 136.0 -0.9     -38.6   -10   1 11  16533  07 57 30
07 58 50  ---          11 24 11  72.0 136.8 -0.9     -38.0    70   F  1  17600

07 59 27  J1215+17     11 24 48  72.1 137.2 -0.8     -37.7    32   1 12  17600  07 59 27
08 00 37  ---          11 25 59  72.2 137.9 -0.8     -37.1    70   R  1  16667

08 00 37  SN1979C      11 25 59  70.2 135.4 -1.0     -38.9   -10   1 12  16667  08 00 37
08 03 27  ---          11 28 49  70.6 137.0 -0.9     -37.6   160   R  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

08 03 27  J1215+17     11 28 49  72.6 139.7 -0.8     -35.5   -10   1 12  14400  08 03 27
08 04 47  ---          11 30 09  72.8 140.6 -0.8     -34.8    70   R  1  13333

08 04 47  SN1979C      11 30 09  70.8 137.8 -0.9     -36.9   -10   1 12  13333  08 04 47
08 07 37  ---          11 33 00  71.2 139.5 -0.8     -35.5   160   R  1  11067

08 07 37  J1215+17     11 33 00  73.2 142.5 -0.7     -33.2   -10   1 12  11067  08 07 37
08 08 57  ---          11 34 20  73.4 143.5 -0.7     -32.4    70   R  1  10000

08 08 57  SN1979C      11 34 20  71.4 140.3 -0.8     -34.8   -10   1 12  10000  08 08 57
08 11 47  ---          11 37 11  71.8 142.1 -0.8     -33.3   160   R  1   7733

08 11 47  J1215+17     11 37 11  73.7 145.5 -0.6     -30.6   -10   1 12   7733  08 11 47
08 13 07  ---          11 38 31  73.9 146.5 -0.6     -29.7    70   R  1   6667

08 13 07  SN1979C      11 38 31  72.0 142.9 -0.7     -32.6   -10   1 12   6667  08 13 07
08 15 57  ---          11 41 21  72.3 144.8 -0.7     -31.0   160   R  1   4400

08 15 57  J1215+17     11 41 21  74.2 148.7 -0.6     -27.9   -10   1 12   4400  08 15 57
08 17 17  ---          11 42 41  74.4 149.7 -0.5     -27.0    70   R  1   3333

08 17 17  SN1979C      11 42 41  72.5 145.8 -0.7     -30.2   -10   1 12   3333  08 17 17
08 20 07  ---          11 45 32  72.8 147.8 -0.6     -28.5   160   R  1   1067

08 20 07  J1215+17     11 45 32  74.7 152.0 -0.5     -25.0   -10   1 12   1067  08 20 07
08 21 27  ---          11 46 52  74.8 153.1 -0.5     -24.0    70   R  1      0

08 23 27  J1215+17     11 48 52  75.0 154.8 -0.4     -22.5   113   1 13      0  08 23 27
08 24 37  ---          11 50 03  75.1 155.8 -0.4     -21.6    70   F  1    933

08 24 37  SN1979C      11 50 03  73.3 151.1 -0.6     -25.6   -10   1 13    933  08 24 37
08 27 27  ---          11 52 53  73.6 153.3 -0.5     -23.7   160   F  1   3200

08 27 27  J1215+17     11 52 53  75.3 158.3 -0.4     -19.4    -9   1 13   3200  08 27 27
08 28 47  ---          11 54 13  75.4 159.5 -0.4     -18.3    71   F  1   4267

08 28 47  SN1979C      11 54 13  73.7 154.3 -0.5     -22.8    -9   1 13   4267  08 28 47
08 31 37  ---          11 57 04  74.0 156.6 -0.4     -20.8   161   F  1   6533

08 31 37  J1215+17     11 57 04  75.6 162.1 -0.3     -16.0   -10   1 13   6533  08 31 37
08 32 57  ---          11 58 24  75.7 163.4 -0.3     -14.9    70   F  1   7600
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

08 32 57  SN1979C      11 58 24  74.1 157.7 -0.4     -19.8   -10   1 13   7600  08 32 57
08 35 47  ---          12 01 14  74.3 160.1 -0.4     -17.8   160   F  1   9867

08 35 47  J1215+17     12 01 14  75.9 166.0 -0.2     -12.5   -10   1 13   9867  08 35 47
08 37 07  ---          12 02 35  75.9 167.3 -0.2     -11.4    70   F  1  10933

08 37 07  SN1979C      12 02 35  74.4 161.2 -0.3     -16.8   -10   1 13  10933  08 37 07
08 39 57  ---          12 05 25  74.6 163.7 -0.3     -14.6   160   F  1  13200

08 39 57  J1215+17     12 05 25  76.1 170.1 -0.2      -8.9   -10   1 13  13200  08 39 57
08 41 17  ---          12 06 45  76.1 171.4 -0.1      -7.7    70   F  1  14267

08 41 17  SN1979C      12 06 45  74.7 164.8 -0.3     -13.5   -10   1 13  14267  08 41 17
08 44 07  ---          12 09 36  74.8 167.4 -0.2     -11.3   160   F  1  16533

08 44 07  J1215+17     12 09 36  76.2 174.2 -0.1      -5.2   -11   1 13  16533  08 44 07
08 45 27  ---          12 10 56  76.2 175.6 -0.1      -4.0    69   F  1  17600

08 46 04  J1215+17     12 11 33  76.2 176.2 -0.1      -3.4    31   1 14  17600  08 46 04
08 47 14  ---          12 12 43  76.2 177.4  0.0      -2.4    70   R  1  16667

08 47 14  SN1979C      12 12 43  74.9 170.2 -0.2      -8.7   -11   1 14  16667  08 47 14
08 50 04  ---          12 15 34  75.0 172.8 -0.1      -6.4   159   R  1  14400

08 50 04  J1215+17     12 15 34  76.2 180.2  0.0       0.2   -11   1 14  14400  08 50 04
08 51 24  ---          12 16 54  76.2 181.6  0.0       1.4    69   R  1  13333

08 51 24  SN1979C      12 16 54  75.1 174.1 -0.1      -5.3   -11   1 14  13333  08 51 24
08 54 14  ---          12 19 44  75.1 176.7 -0.1      -2.9   159   R  1  11067

08 54 14  J1215+17     12 19 44  76.2 184.4  0.1       4.0   -11   1 14  11067  08 54 14
08 55 34  ---          12 21 05  76.2 185.8  0.1       5.2    69   R  1  10000

08 55 34  SN1979C      12 21 05  75.1 178.0  0.0      -1.8   -11   1 14  10000  08 55 34
08 58 24  ---          12 23 55  75.1 180.6  0.0       0.6   159   R  1   7733

08 58 24  J1215+17     12 23 55  76.1 188.6  0.1       7.7   -11   1 14   7733  08 58 24
08 59 44  ---          12 25 15  76.1 189.9  0.2       8.9    69   R  1   6667

08 59 44  SN1979C      12 25 15  75.1 181.9  0.0       1.7   -11   1 14   6667  08 59 44
09 02 34  ---          12 28 06  75.1 184.5  0.1       4.1   159   R  1   4400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

09 02 34  J1215+17     12 28 06  75.9 192.7  0.2      11.4   -11   1 14   4400  09 02 34
09 03 54  ---          12 29 26  75.9 193.9  0.2      12.5    69   R  1   3333

09 03 54  SN1979C      12 29 26  75.1 185.8  0.1       5.2   -11   1 14   3333  09 03 54
09 06 44  ---          12 32 17  75.0 188.4  0.2       7.5   159   R  1   1067

09 06 44  J1215+17     12 32 17  75.7 196.6  0.3      14.9   -11   1 14   1067  09 06 44
09 08 04  ---          12 33 37  75.6 197.9  0.3      16.0    69   R  1      0

-----------  Tape Change ------------

09 23 04  J1215+17     12 48 39  74.3 210.8  0.6      27.4   885   2  1      0  09 23 04
09 24 14  ---          12 49 49  74.2 211.7  0.6      28.2    70   F  1    933

09 24 14  SN1979C      12 49 49  73.9 203.7  0.4      21.1   -11   2  1    933  09 24 14
09 27 04  ---          12 52 40  73.7 206.0  0.5      23.1   159   F  1   3200

09 27 04  J1215+17     12 52 40  73.8 213.8  0.6      30.1   -11   2  1   3200  09 27 04
09 28 24  ---          12 54 00  73.7 214.8  0.6      30.9    69   F  1   4267

09 28 24  SN1979C      12 54 00  73.6 207.0  0.5      24.0   -11   2  1   4267  09 28 24
09 31 14  ---          12 56 51  73.3 209.2  0.6      25.9   159   F  1   6533

09 31 14  J1215+17     12 56 51  73.3 216.9  0.7      32.6   -11   2  1   6533  09 31 14
09 32 34  ---          12 58 11  73.1 217.8  0.7      33.4    69   F  1   7600

09 32 34  SN1979C      12 58 11  73.1 210.2  0.6      26.7   -11   2  1   7600  09 32 34
09 35 24  ---          13 01 01  72.8 212.3  0.6      28.5   159   F  1   9867

09 35 24  J1215+17     13 01 01  72.8 219.7  0.8      35.1   -11   2  1   9867  09 35 24
09 36 44  ---          13 02 21  72.6 220.6  0.8      35.8    69   F  1  10933

09 36 44  SN1979C      13 02 21  72.6 213.2  0.7      29.3   -11   2  1  10933  09 36 44
09 39 34  ---          13 05 12  72.3 215.2  0.7      31.0   159   F  1  13200

09 39 34  J1215+17     13 05 12  72.2 222.4  0.8      37.3   -11   2  1  13200  09 39 34
09 40 54  ---          13 06 32  72.0 223.2  0.9      38.0    69   F  1  14267

09 40 54  SN1979C      13 06 32  72.1 216.1  0.7      31.8   -11   2  1  14267  09 40 54
09 43 44  ---          13 09 23  71.8 217.9  0.8      33.4   159   F  1  16533

09 43 44  J1215+17     13 09 23  71.5 224.9  0.9      39.4   -11   2  1  16533  09 43 44
09 45 04  ---          13 10 43  71.3 225.7  0.9      40.0    69   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

09 45 41  OQ208        13 11 20  77.6  96.8 -0.9     -76.3   -55   2  2  17600  09 45 41
09 48 41  ---          13 14 20  78.3  97.6 -0.9     -75.9   125   R  1  15200

09 51 41  J1215+17     13 17 21  70.3 229.3  1.0      43.0    86   2  2  15200  09 51 41
09 54 41  ---          13 20 21  69.8 230.8  1.1      44.2   180   R  1  12800

09 54 41  SN1979C      13 20 21  70.2 224.5  1.0      38.8   -10   2  2  12800  09 54 41
09 56 51  ---          13 22 32  69.9 225.7  1.0      39.8   120   R  1  11067

09 56 51  J1215+17     13 22 32  69.4 231.9  1.1      45.0   -10   2  2  11067  09 56 51
09 58 11  ---          13 23 52  69.2 232.5  1.1      45.5    70   R  1  10000

09 58 11  SN1979C      13 23 52  69.7 226.4  1.0      40.4   -10   2  2  10000  09 58 11
10 01 01  ---          13 26 42  69.2 227.9  1.1      41.5   160   R  1   7733

10 01 01  J1215+17     13 26 42  68.7 233.8  1.2      46.5   -10   2  2   7733  10 01 01
10 02 21  ---          13 28 03  68.5 234.4  1.2      47.0    70   R  1   6667

10 02 21  SN1979C      13 28 03  69.0 228.5  1.1      42.1   -10   2  2   6667  10 02 21
10 05 11  ---          13 30 53  68.5 229.9  1.1      43.2   160   R  1   4400

10 05 11  J1215+17     13 30 53  68.0 235.7  1.3      47.9   -10   2  2   4400  10 05 11
10 06 31  ---          13 32 13  67.7 236.2  1.3      48.4    70   R  1   3333

10 06 31  SN1979C      13 32 13  68.3 230.6  1.1      43.7   -10   2  2   3333  10 06 31
10 09 21  ---          13 35 04  67.9 231.9  1.2      44.7   160   R  1   1067

10 09 21  J1215+17     13 35 04  67.2 237.4  1.3      49.2   -10   2  2   1067  10 09 21
10 10 41  ---          13 36 24  67.0 237.9  1.4      49.6    70   R  1      0

10 11 18  J1215+17     13 37 01  66.9 238.2  1.4      49.8    32   2  3      0  10 11 18
10 12 28  ---          13 38 11  66.7 238.6  1.4      50.2    70   F  1    933

10 12 28  SN1979C      13 38 11  67.3 233.3  1.2      45.8   -10   2  3    933  10 12 28
10 15 18  ---          13 41 02  66.8 234.5  1.3      46.7   160   F  1   3200

10 15 18  J1215+17     13 41 02  66.1 239.7  1.4      50.9    -9   2  3   3200  10 15 18
10 16 38  ---          13 42 22  65.9 240.2  1.5      51.3    71   F  1   4267

10 16 38  SN1979C      13 42 22  66.6 235.0  1.3      47.1    -9   2  3   4267  10 16 38
10 19 28  ---          13 45 12  66.1 236.2  1.4      48.0   161   F  1   6533
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

10 19 28  J1215+17     13 45 12  65.3 241.2  1.5      52.0    -9   2  3   6533  10 19 28
10 20 48  ---          13 46 33  65.1 241.7  1.5      52.3    71   F  1   7600

10 20 48  SN1979C      13 46 33  65.8 236.7  1.4      48.4    -9   2  3   7600  10 20 48
10 23 38  ---          13 49 23  65.3 237.8  1.4      49.2   161   F  1   9867

10 23 38  J1215+17     13 49 23  64.6 242.7  1.6      53.0    -9   2  3   9867  10 23 38
10 24 58  ---          13 50 43  64.3 243.1  1.6      53.3    71   F  1  10933

10 24 58  SN1979C      13 50 43  65.1 238.3  1.5      49.5    -9   2  3  10933  10 24 58
10 27 48  ---          13 53 34  64.6 239.3  1.5      50.3   161   F  1  13200

10 27 48  J1215+17     13 53 34  63.7 244.0  1.6      53.9    -9   2  3  13200  10 27 48
10 29 08  ---          13 54 54  63.5 244.5  1.7      54.2    71   F  1  14267

10 29 08  SN1979C      13 54 54  64.3 239.8  1.5      50.6    -9   2  3  14267  10 29 08
10 31 58  ---          13 57 45  63.8 240.8  1.6      51.3   161   F  1  16533

10 31 58  J1215+17     13 57 45  62.9 245.3  1.7      54.8    -9   2  3  16533  10 31 58
10 33 18  ---          13 59 05  62.7 245.7  1.7      55.1    71   F  1  17600

10 33 55  J1215+17     13 59 42  62.6 245.9  1.7      55.2    32   2  4  17600  10 33 55
10 35 05  ---          14 00 52  62.3 246.3  1.8      55.4    70   R  1  16667

10 35 05  SN1979C      14 00 52  63.2 241.8  1.6      52.0    -9   2  4  16667  10 35 05
10 37 55  ---          14 03 43  62.7 242.8  1.7      52.6   161   R  1  14400

10 37 55  J1215+17     14 03 43  61.8 247.1  1.8      55.9    -9   2  4  14400  10 37 55
10 39 15  ---          14 05 03  61.5 247.5  1.8      56.1    71   R  1  13333

10 39 15  SN1979C      14 05 03  62.4 243.2  1.7      52.9    -9   2  4  13333  10 39 15
10 42 05  ---          14 07 53  61.8 244.1  1.7      53.5   161   R  1  11067

10 42 05  J1215+17     14 07 53  60.9 248.2  1.9      56.6    -9   2  4  11067  10 42 05
10 43 25  ---          14 09 13  60.7 248.6  1.9      56.8    71   R  1  10000

10 43 25  SN1979C      14 09 13  61.6 244.5  1.8      53.8    -9   2  4  10000  10 43 25
10 46 15  ---          14 12 04  61.0 245.3  1.8      54.3   161   R  1   7733

10 46 15  J1215+17     14 12 04  60.1 249.3  1.9      57.3    -9   2  4   7733  10 46 15
10 47 35  ---          14 13 24  59.8 249.7  2.0      57.5    71   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

10 47 35  SN1979C      14 13 24  60.8 245.7  1.8      54.6    -9   2  4   6667  10 47 35
10 50 25  ---          14 16 15  60.2 246.5  1.9      55.1   161   R  1   4400

10 50 25  J1215+17     14 16 15  59.2 250.4  2.0      57.9    -9   2  4   4400  10 50 25
10 51 45  ---          14 17 35  59.0 250.7  2.0      58.1    71   R  1   3333

10 51 45  SN1979C      14 17 35  60.0 246.9  1.9      55.3    -9   2  4   3333  10 51 45
10 54 35  ---          14 20 25  59.4 247.6  2.0      55.8   161   R  1   1067

10 54 35  J1215+17     14 20 25  58.4 251.4  2.1      58.5    -9   2  4   1067  10 54 35
10 55 55  ---          14 21 45  58.1 251.7  2.1      58.6    71   R  1      0

10 56 32  J1215+17     14 22 23  58.0 251.9  2.1      58.7    32   2  5      0  10 56 32
10 57 42  ---          14 23 33  57.8 252.2  2.1      58.9    70   F  1    933

10 57 42  SN1979C      14 23 33  58.8 248.4  2.0      56.3    -8   2  5    933  10 57 42
11 00 32  ---          14 26 23  58.2 249.2  2.1      56.7   162   F  1   3200

11 00 32  J1215+17     14 26 23  57.2 252.8  2.2      59.2    -8   2  5   3200  11 00 32
11 01 52  ---          14 27 43  56.9 253.1  2.2      59.4    72   F  1   4267

11 01 52  SN1979C      14 27 43  57.9 249.5  2.1      56.9    -8   2  5   4267  11 01 52
11 04 42  ---          14 30 34  57.4 250.2  2.1      57.3   162   F  1   6533

11 04 42  J1215+17     14 30 34  56.3 253.7  2.3      59.7    -8   2  5   6533  11 04 42
11 06 02  ---          14 31 54  56.0 254.0  2.3      59.8    72   F  1   7600

11 06 02  SN1979C      14 31 54  57.1 250.5  2.1      57.4    -8   2  5   7600  11 06 02
11 08 52  ---          14 34 45  56.5 251.2  2.2      57.8   162   F  1   9867

11 08 52  J1215+17     14 34 45  55.5 254.6  2.3      60.1    -8   2  5   9867  11 08 52
11 10 12  ---          14 36 05  55.2 254.9  2.3      60.2    72   F  1  10933

11 10 12  SN1979C      14 36 05  56.2 251.5  2.2      58.0    -8   2  5  10933  11 10 12
11 13 02  ---          14 38 55  55.7 252.1  2.3      58.3   162   F  1  13200

11 13 02  J1215+17     14 38 55  54.6 255.5  2.4      60.5    -8   2  5  13200  11 13 02
11 14 22  ---          14 40 15  54.3 255.8  2.4      60.6    72   F  1  14267

11 14 22  SN1979C      14 40 15  55.4 252.4  2.3      58.5    -8   2  5  14267  11 14 22
11 17 12  ---          14 43 06  54.8 253.0  2.3      58.8   162   F  1  16533
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

11 17 12  J1215+17     14 43 06  53.7 256.3  2.5      60.9    -8   2  5  16533  11 17 12
11 18 32  ---          14 44 26  53.4 256.6  2.5      61.0    72   F  1  17600

11 19 09  J1215+17     14 45 03  53.3 256.7  2.5      61.1    32   2  6  17600  11 19 09
11 20 19  ---          14 46 13  53.1 256.9  2.5      61.2    70   R  1  16667

11 20 19  SN1979C      14 46 13  54.2 253.7  2.4      59.1    -8   2  6  16667  11 20 19
11 23 09  ---          14 49 04  53.6 254.3  2.4      59.4   162   R  1  14400

11 23 09  J1215+17     14 49 04  52.5 257.5  2.6      61.4    -8   2  6  14400  11 23 09
11 24 29  ---          14 50 24  52.2 257.7  2.6      61.5    72   R  1  13333

11 24 29  SN1979C      14 50 24  53.3 254.6  2.5      59.5    -8   2  6  13333  11 24 29
11 27 19  ---          14 53 15  52.7 255.2  2.5      59.8   162   R  1  11067

11 27 19  J1215+17     14 53 15  51.6 258.2  2.6      61.7    -8   2  6  11067  11 27 19
11 28 39  ---          14 54 35  51.3 258.5  2.7      61.8    72   R  1  10000

11 28 39  SN1979C      14 54 35  52.4 255.4  2.5      59.9    -8   2  6  10000  11 28 39
11 31 29  ---          14 57 25  51.8 256.0  2.6      60.2   162   R  1   7733

11 31 29  J1215+17     14 57 25  50.7 259.0  2.7      62.0    -8   2  6   7733  11 31 29
11 32 49  ---          14 58 46  50.4 259.2  2.7      62.0    72   R  1   6667

11 32 49  SN1979C      14 58 46  51.5 256.2  2.6      60.3    -8   2  6   6667  11 32 49
11 35 39  ---          15 01 36  51.0 256.8  2.6      60.5   162   R  1   4400

11 35 39  J1215+17     15 01 36  49.8 259.7  2.8      62.2    -8   2  6   4400  11 35 39
11 36 59  ---          15 02 56  49.5 260.0  2.8      62.3    72   R  1   3333

11 36 59  SN1979C      15 02 56  50.7 257.0  2.7      60.6    -8   2  6   3333  11 36 59
11 39 49  ---          15 05 47  50.1 257.5  2.7      60.8   162   R  1   1067

11 39 49  J1215+17     15 05 47  48.9 260.4  2.8      62.5    -8   2  6   1067  11 39 49
11 41 09  ---          15 07 07  48.7 260.7  2.9      62.5    72   R  1      0

11 43 09  J1215+17     15 09 07  48.2 261.0  2.9      62.6   113   2  7      0  11 43 09
11 44 19  ---          15 10 17  48.0 261.2  2.9      62.7    70   F  1    933

11 44 19  SN1979C      15 10 17  49.1 258.4  2.8      61.1    -8   2  7    933  11 44 19
11 47 09  ---          15 13 08  48.5 258.9  2.8      61.3   162   F  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

11 47 09  J1215+17     15 13 08  47.4 261.7  3.0      62.8    -8   2  7   3200  11 47 09
11 48 29  ---          15 14 28  47.1 261.9  3.0      62.9    72   F  1   4267

11 48 29  SN1979C      15 14 28  48.2 259.1  2.9      61.4    -8   2  7   4267  11 48 29
11 51 19  ---          15 17 19  47.6 259.6  2.9      61.6   162   F  1   6533

11 51 19  J1215+17     15 17 19  46.5 262.3  3.0      63.0    -8   2  7   6533  11 51 19
11 52 39  ---          15 18 39  46.2 262.5  3.1      63.1    72   F  1   7600

11 52 39  SN1979C      15 18 39  47.4 259.8  2.9      61.6    -8   2  7   7600  11 52 39
11 55 29  ---          15 21 29  46.8 260.3  3.0      61.8   162   F  1   9867

11 55 29  J1215+17     15 21 29  45.6 263.0  3.1      63.2    -8   2  7   9867  11 55 29
11 56 49  ---          15 22 49  45.3 263.2  3.1      63.2    72   F  1  10933

11 56 49  SN1979C      15 22 49  46.5 260.5  3.0      61.9    -8   2  7  10933  11 56 49
11 59 39  ---          15 25 40  45.9 261.0  3.0      62.0   162   F  1  13200

11 59 39  J1215+17     15 25 40  44.7 263.6  3.2      63.3    -8   2  7  13200  11 59 39
12 00 59  ---          15 27 00  44.4 263.8  3.2      63.4    72   F  1  14267

12 00 59  SN1979C      15 27 00  45.6 261.2  3.1      62.1    -8   2  7  14267  12 00 59
12 03 49  ---          15 29 51  45.0 261.6  3.1      62.2   162   F  1  16533

12 03 49  J1215+17     15 29 51  43.8 264.2  3.2      63.5    -8   2  7  16533  12 03 49
12 05 09  ---          15 31 11  43.5 264.4  3.3      63.5    72   F  1  17600

12 05 46  J1215+17     15 31 48  43.4 264.5  3.3      63.5    32   2  8  17600  12 05 46
12 06 56  ---          15 32 58  43.1 264.7  3.3      63.5    70   R  1  16667

12 06 56  SN1979C      15 32 58  44.3 262.1  3.2      62.3    -8   2  8  16667  12 06 56
12 09 46  ---          15 35 49  43.7 262.6  3.2      62.4   162   R  1  14400

12 09 46  J1215+17     15 35 49  42.5 265.1  3.3      63.6    -8   2  8  14400  12 09 46
12 11 06  ---          15 37 09  42.2 265.3  3.4      63.7    72   R  1  13333

12 11 06  SN1979C      15 37 09  43.4 262.8  3.2      62.5    -8   2  8  13333  12 11 06
12 13 56  ---          15 39 59  42.8 263.2  3.3      62.6   162   R  1  11067

12 13 56  J1215+17     15 39 59  41.6 265.7  3.4      63.7    -8   2  8  11067  12 13 56
12 15 16  ---          15 41 20  41.3 265.9  3.4      63.7    72   R  1  10000
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

12 15 16  SN1979C      15 41 20  42.5 263.4  3.3      62.6    -8   2  8  10000  12 15 16
12 18 06  ---          15 44 10  41.9 263.8  3.3      62.7   162   R  1   7733

12 18 06  J1215+17     15 44 10  40.7 266.3  3.5      63.8    -8   2  8   7733  12 18 06
12 19 26  ---          15 45 30  40.4 266.5  3.5      63.8    72   R  1   6667

12 19 26  SN1979C      15 45 30  41.6 264.0  3.4      62.8    -8   2  8   6667  12 19 26
12 22 16  ---          15 48 21  41.0 264.4  3.4      62.9   162   R  1   4400

12 22 16  J1215+17     15 48 21  39.8 266.9  3.5      63.9    -8   2  8   4400  12 22 16
12 23 36  ---          15 49 41  39.5 267.1  3.6      63.9    72   R  1   3333

12 23 36  SN1979C      15 49 41  40.7 264.6  3.4      62.9    -8   2  8   3333  12 23 36
12 26 26  ---          15 52 31  40.1 265.0  3.5      63.0   162   R  1   1067

12 26 26  J1215+17     15 52 31  38.9 267.4  3.6      63.9    -8   2  8   1067  12 26 26
12 27 46  ---          15 53 52  38.7 267.6  3.6      63.9    72   R  1      0

12 28 23  J1215+17     15 54 29  38.5 267.7  3.7      64.0    32   2  9      0  12 28 23
12 29 33  ---          15 55 39  38.3 267.9  3.7      64.0    70   F  1    933

12 29 33  SN1979C      15 55 39  39.5 265.5  3.5      63.0    -8   2  9    933  12 29 33
12 32 23  ---          15 58 29  38.9 265.9  3.6      63.1   162   F  1   3200

12 32 23  J1215+17     15 58 29  37.7 268.2  3.7      64.0    -8   2  9   3200  12 32 23
12 33 43  ---          15 59 50  37.4 268.4  3.7      64.0    72   F  1   4267

12 33 43  SN1979C      15 59 50  38.6 266.1  3.6      63.1    -8   2  9   4267  12 33 43
12 36 33  ---          16 02 40  38.0 266.5  3.7      63.2   162   F  1   6533

12 36 33  J1215+17     16 02 40  36.8 268.8  3.8      64.0    -8   2  9   6533  12 36 33
12 37 53  ---          16 04 00  36.5 269.0  3.8      64.0    72   F  1   7600

12 37 53  SN1979C      16 04 00  37.7 266.7  3.7      63.2    -8   2  9   7600  12 37 53
12 40 43  ---          16 06 51  37.1 267.0  3.7      63.2   162   F  1   9867

12 40 43  J1215+17     16 06 51  35.9 269.3  3.9      64.0    -8   2  9   9867  12 40 43
12 42 03  ---          16 08 11  35.6 269.5  3.9      64.0    72   F  1  10933

12 42 03  SN1979C      16 08 11  36.8 267.2  3.7      63.3    -8   2  9  10933  12 42 03
12 44 53  ---          16 11 01  36.2 267.6  3.8      63.3   162   F  1  13200
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

12 44 53  J1215+17     16 11 01  35.0 269.9  3.9      64.0    -8   2  9  13200  12 44 53
12 46 13  ---          16 12 22  34.7 270.0  4.0      64.0    72   F  1  14267

12 46 13  SN1979C      16 12 22  35.9 267.8  3.8      63.3    -8   2  9  14267  12 46 13
12 49 03  ---          16 15 12  35.3 268.2  3.9      63.3   162   F  1  16533

12 49 03  J1215+17     16 15 12  34.1 270.4  4.0      64.0    -8   2  9  16533  12 49 03
12 50 23  ---          16 16 32  33.8 270.6  4.0      64.0    72   F  1  17600

12 51 00  J1215+17     16 17 09  33.6 270.6  4.0      64.0    32   2 10  17600  12 51 00
12 52 10  ---          16 18 20  33.4 270.8  4.0      64.0    70   R  1  16667

12 52 10  SN1979C      16 18 20  34.6 268.6  3.9      63.4    -8   2 10  16667  12 52 10
12 55 00  ---          16 21 10  34.0 268.9  4.0      63.4   162   R  1  14400

12 55 00  J1215+17     16 21 10  32.8 271.1  4.1      64.0    -8   2 10  14400  12 55 00
12 56 20  ---          16 22 30  32.5 271.3  4.1      64.0    72   R  1  13333

12 56 20  SN1979C      16 22 30  33.7 269.1  4.0      63.4    -8   2 10  13333  12 56 20
12 59 10  ---          16 25 21  33.1 269.5  4.0      63.4   162   R  1  11067

12 59 10  J1215+17     16 25 21  31.9 271.7  4.2      64.0    -8   2 10  11067  12 59 10
13 00 30  ---          16 26 41  31.6 271.8  4.2      64.0    72   R  1  10000

13 00 30  SN1979C      16 26 41  32.8 269.7  4.1      63.4    -8   2 10  10000  13 00 30
13 03 20  ---          16 29 31  32.2 270.0  4.1      63.4   162   R  1   7733

13 03 20  J1215+17     16 29 31  31.0 272.2  4.2      64.0    -8   2 10   7733  13 03 20
13 04 40  ---          16 30 52  30.7 272.3  4.3      64.0    72   R  1   6667

13 04 40  SN1979C      16 30 52  31.9 270.2  4.1      63.4    -8   2 10   6667  13 04 40
13 07 30  ---          16 33 42  31.3 270.6  4.2      63.4   162   R  1   4400

13 07 30  J1215+17     16 33 42  30.1 272.7  4.3      63.9    -8   2 10   4400  13 07 30
13 08 50  ---          16 35 02  29.8 272.9  4.3      63.9    72   R  1   3333

13 08 50  SN1979C      16 35 02  31.0 270.7  4.2      63.4    -8   2 10   3333  13 08 50
13 11 40  ---          16 37 53  30.4 271.1  4.2      63.4   162   R  1   1067

13 11 40  J1215+17     16 37 53  29.2 273.2  4.4      63.9    -8   2 10   1067  13 11 40
13 13 00  ---          16 39 13  28.9 273.4  4.4      63.8    72   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

13 13 37  J1215+17     16 39 50  28.8 273.4  4.4      63.8    32   2 11      0  13 13 37
13 14 47  ---          16 41 00  28.5 273.6  4.4      63.8    70   F  1    933

13 14 47  SN1979C      16 41 00  29.7 271.5  4.3      63.4    -8   2 11    933  13 14 47
13 17 37  ---          16 43 51  29.1 271.8  4.3      63.3   162   F  1   3200

13 17 37  J1215+17     16 43 51  27.9 273.9  4.5      63.8    -8   2 11   3200  13 17 37
13 18 57  ---          16 45 11  27.6 274.1  4.5      63.8    72   F  1   4267

13 18 57  SN1979C      16 45 11  28.8 272.0  4.4      63.3    -8   2 11   4267  13 18 57
13 21 47  ---          16 48 01  28.2 272.3  4.4      63.3   162   F  1   6533

13 21 47  J1215+17     16 48 01  27.0 274.4  4.5      63.7    -8   2 11   6533  13 21 47
13 23 07  ---          16 49 22  26.7 274.6  4.6      63.7    72   F  1   7600

13 23 07  SN1979C      16 49 22  27.9 272.5  4.4      63.3    -8   2 11   7600  13 23 07
13 25 57  ---          16 52 12  27.3 272.8  4.5      63.2   162   F  1   9867

13 25 57  J1215+17     16 52 12  26.1 274.9  4.6      63.6    -8   2 11   9867  13 25 57
13 27 17  ---          16 53 32  25.8 275.1  4.6      63.6    72   F  1  10933

13 27 17  SN1979C      16 53 32  27.0 273.0  4.5      63.2    -8   2 11  10933  13 27 17
13 30 07  ---          16 56 23  26.4 273.3  4.6      63.2   162   F  1  13200

13 30 07  J1215+17     16 56 23  25.2 275.4  4.7      63.5    -8   2 11  13200  13 30 07
13 31 27  ---          16 57 43  24.9 275.6  4.7      63.5    72   F  1  14267

13 31 27  SN1979C      16 57 43  26.1 273.5  4.6      63.2    -8   2 11  14267  13 31 27
13 34 17  ---          17 00 33  25.5 273.9  4.6      63.1   162   F  1  16533

13 34 17  J1215+17     17 00 33  24.3 275.9  4.8      63.4    -8   2 11  16533  13 34 17
13 35 37  ---          17 01 54  24.0 276.0  4.8      63.4    72   F  1  17600

13 36 14  J1215+17     17 02 31  23.9 276.1  4.8      63.4    32   2 12  17600  13 36 14
13 37 24  ---          17 03 41  23.7 276.3  4.8      63.4    70   R  1  16667

13 37 24  SN1979C      17 03 41  24.8 274.2  4.7      63.1    -8   2 12  16667  13 37 24
13 40 14  ---          17 06 31  24.2 274.6  4.7      63.0   162   R  1  14400

13 40 14  J1215+17     17 06 31  23.0 276.6  4.9      63.3    -8   2 12  14400  13 40 14
13 41 34  ---          17 07 52  22.8 276.7  4.9      63.2    72   R  1  13333
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

13 41 34  SN1979C      17 07 52  24.0 274.7  4.7      63.0    -8   2 12  13333  13 41 34
13 44 24  ---          17 10 42  23.3 275.1  4.8      62.9   162   R  1  11067

13 44 24  J1215+17     17 10 42  22.2 277.1  4.9      63.2    -8   2 12  11067  13 44 24
13 45 44  ---          17 12 02  21.9 277.2  4.9      63.1    72   R  1  10000

13 45 44  SN1979C      17 12 02  23.1 275.2  4.8      62.9    -8   2 12  10000  13 45 44
13 48 34  ---          17 14 53  22.4 275.6  4.9      62.9   162   R  1   7733

13 48 34  J1215+17     17 14 53  21.3 277.6  5.0      63.0    -8   2 12   7733  13 48 34
13 49 54  ---          17 16 13  21.0 277.7  5.0      63.0    72   R  1   6667

13 49 54  SN1979C      17 16 13  22.2 275.7  4.9      62.8    -8   2 12   6667  13 49 54
13 52 44  ---          17 19 04  21.6 276.1  4.9      62.8   162   R  1   4400

13 52 44  J1215+17     17 19 04  20.4 278.1  5.1      62.9    -8   2 12   4400  13 52 44
13 54 04  ---          17 20 24  20.1 278.2  5.1      62.9    72   R  1   3333

13 54 04  SN1979C      17 20 24  21.3 276.2  5.0      62.7    -8   2 12   3333  13 54 04
13 56 54  ---          17 23 14  20.7 276.6  5.0      62.7   162   R  1   1067

13 56 54  J1215+17     17 23 14  19.5 278.5  5.1      62.8    -8   2 12   1067  13 56 54
13 58 14  ---          17 24 34  19.2 278.7  5.2      62.7    72   R  1      0

14 00 14  J1215+17     17 26 35  18.8 278.9  5.2      62.7   113   2 13      0  14 00 14
14 01 24  ---          17 27 45  18.5 279.1  5.2      62.6    70   F  1    933

14 01 24  SN1979C      17 27 45  19.7 277.1  5.1      62.5    -8   2 13    933  14 01 24
14 04 14  ---          17 30 35  19.1 277.4  5.1      62.4   162   F  1   3200

14 04 14  J1215+17     17 30 35  17.9 279.4  5.3      62.5    -8   2 13   3200  14 04 14
14 05 34  ---          17 31 56  17.6 279.5  5.3      62.5    72   F  1   4267

14 05 34  SN1979C      17 31 56  18.8 277.6  5.1      62.4    -8   2 13   4267  14 05 34
14 08 24  ---          17 34 46  18.2 277.9  5.2      62.3   162   F  1   6533

14 08 24  J1215+17     17 34 46  17.0 279.9  5.3      62.4    -8   2 13   6533  14 08 24
14 09 44  ---          17 36 06  16.8 280.0  5.3      62.3    72   F  1   7600

14 09 44  SN1979C      17 36 06  17.9 278.1  5.2      62.3    -8   2 13   7600  14 09 44
14 12 34  ---          17 38 57  17.3 278.4  5.3      62.2   162   F  1   9867
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

14 12 34  J1215+17     17 38 57  16.2 280.4  5.4      62.2    -8   2 13   9867  14 12 34
14 13 54  ---          17 40 17  15.9 280.5  5.4      62.1    72   F  1  10933

14 13 54  SN1979C      17 40 17  17.0 278.6  5.3      62.1    -8   2 13  10933  14 13 54
14 16 44  ---          17 43 07  16.4 278.9  5.3      62.0   162   F  1  13200

14 16 44  J1215+17     17 43 07  15.3 280.8  5.5      62.0    -8   2 13  13200  14 16 44
14 18 04  ---          17 44 28  15.0 281.0  5.5      62.0    72   F  1  14267

14 18 04  SN1979C      17 44 28  16.1 279.1  5.4      62.0    -8   2 13  14267  14 18 04
14 20 54  ---          17 47 18  15.5 279.4  5.4      61.9   162   F  1  16533

14 20 54  J1215+17     17 47 18  14.4 281.3  5.5      61.8    -8   2 13  16533  14 20 54
14 22 14  ---          17 48 38  14.1 281.5  5.6      61.8    72   F  1  17600

14 24 14  J1215+17     17 50 39  13.7 281.7  5.6      61.7   113   2 14  17600  14 24 14
14 25 24  ---          17 51 49  13.4 281.9  5.6      61.6    70   R  1  16667

14 25 24  SN1979C      17 51 49  14.6 279.9  5.5      61.7    -8   2 14  16667  14 25 24
14 28 14  ---          17 54 39  14.0 280.3  5.5      61.6   162   R  1  14400

14 28 14  J1215+17     17 54 39  12.8 282.2  5.7      61.5    -8   2 14  14400  14 28 14
14 29 34  ---          17 56 00  12.6 282.3  5.7      61.4    72   R  1  13333

14 29 34  SN1979C      17 56 00  13.7 280.4  5.5      61.6    -8   2 14  13333  14 29 34
14 32 24  ---          17 58 50  13.1 280.7  5.6      61.4   162   R  1  11067

14 32 24  J1215+17     17 58 50  12.0 282.7  5.7      61.3    -8   2 14  11067  14 32 24
14 33 44  ---          18 00 10  11.7 282.8  5.7      61.2    72   R  1  10000

14 33 44  SN1979C      18 00 10  12.8 280.9  5.6      61.4    -8   2 14  10000  14 33 44
14 36 34  ---          18 03 01  12.2 281.2  5.7      61.3   162   R  1   7733

14 36 34  J1215+17     18 03 01  11.1 283.2  5.8      61.1    -8   2 14   7733  14 36 34
14 37 54  ---          18 04 21  10.8 283.3  5.8      61.0    72   R  1   6667

14 37 54  SN1979C      18 04 21  11.9 281.4  5.7      61.2    -8   2 14   6667  14 37 54
14 40 44  ---          18 07 11  11.3 281.7  5.7      61.1   162   R  1   4400

14 40 44  J1215+17     18 07 11  10.2 283.7  5.9      60.9    -8   2 14   4400  14 40 44
14 42 04  ---          18 08 32   9.9 283.8  5.9      60.8    72   R  1   3333
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  25 Feb 2005   Day  56 ---

14 42 04  SN1979C      18 08 32  11.0 281.9  5.8      61.0    -8   2 14   3333  14 42 04
14 44 54  ---          18 11 22  10.5 282.2  5.8      60.9   162   R  1   1067

14 44 54  J1215+17     18 11 22   9.3 284.2  5.9      60.7    -8   2 14   1067  14 44 54
14 46 14  ---          18 12 42   9.1 284.3  6.0      60.6    72   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/sched.2004oct04/setups/v6cm-256-8-2-UL.set
   Matches group v6cm_2 in /usr/local/sched.2004oct04/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4979.49   4979.49   4979.49   4979.49   4995.49   4995.49   4995.49   4995.49
   BBC fr=     879.49    879.49    879.49    879.49    895.49    895.49    895.49    895.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   510   490   510  6490  6510  6490  6510
    PCALFR2=   490   510   490   510  6490  6510  6490  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- 10th epoch of obs. of SN1979C in M100: VLBA/MkIV 6cm pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SN1979C           12 20 26.708149   * 12 22 58.666427     12 23 15.241506 
                     16 04 29.46765    * 15 47 51.95179      15 46 00.74582 
                     From catalog imbedded in main SCHED input file.
                        8.619 scan hours,    572.105 baseline hours above horizon.

 * 3C273             12 26 33.246145   * 12 29 06.700041     12 29 23.231979 
                     02 19 43.30589    * 02 03 08.59840      02 01 19.59005 
                     From catalog imbedded in main SCHED input file.
                        0.072 scan hours,     12.350 baseline hours above horizon.

 * J1215+17          12 12 31.449683   * 12 15 03.979124     12 15 20.653261 
                     17 11 18.14600    * 16 54 37.95736      16 52 46.77782 
                     From catalog imbedded in main SCHED input file.
                        5.142 scan hours,    331.555 baseline hours above horizon.

 * OQ208             14 04 45.615152   * 14 07 00.394411     14 07 14.989338 
                     28 41 29.23491    * 28 27 14.68994      28 25 29.98071 
                     From catalog imbedded in main SCHED input file.
                        0.050 scan hours,      1.938 baseline hours above horizon.

 * OJ287             08 51 57.250620   * 08 54 48.874931     08 55 07.555469 
                     20 17 58.41739    * 20 06 30.64084      20 05 22.46270 
                     From catalog imbedded in main SCHED input file.
                        0.050 scan hours,      2.250 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1979C            152.6
   3C273              150.5
   J1215+17           154.2
   OQ208              126.4
   OJ287              153.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

