  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1993J @ 6cm
 Exp. Code:  GM059A  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 18 Sept. 2003                      

PI:       J.M.Marcaide                                                    

Address:  Universitat de Valencia                                         
          C/ Dr. Moliner, 50                                              
          Burjassot, E 46100, Spain                                       
                                                                          

Phone:    34-96-398-3079/8 (work) or 34-96-337-1786 (home)                
EMAIL:    J.M.Marcaide@uv.es (internet)                                   
Fax:      34-96-398-3084                                                  
Phone during observation: 34-958-121311 (work) or 34-958-810928 (home)    

Observing mode: VLBA                                                      

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

 Next scan frequencies:  8383.49  8399.49  8399.49  8415.49  8415.49  8431.49
                         8431.49  8447.49
 Next BBC frequencies:    783.49   799.49   799.49   815.49   815.49   831.49
                          831.49   847.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

14 07 00  J2022+61     17 13 39  46.6  30.5 -3.1    -113.4     0   1  1      0  14 07 00
14 07 45  ---          17 14 24  46.7  30.4 -3.1    -113.6    45   F  1    600

14 08 19  SN2004ET     17 14 58  45.8  33.2 -3.3    -108.8    26   1  1    600  14 08 19
14 10 34  ---          17 17 14  46.0  33.1 -3.3    -109.4   135   F  1   2400

14 11 08  J2022+61     17 17 48  47.0  30.2 -3.1    -114.5    26   1  1   2400  14 11 08
14 11 53  ---          17 18 33  47.1  30.1 -3.1    -114.7    45   F  1   3000

14 12 27  SN2004ET     17 19 07  46.3  33.0 -3.3    -109.9    26   1  1   3000  14 12 27
14 14 42  ---          17 21 22  46.5  32.8 -3.2    -110.5   135   F  1   4800

14 15 16  J2022+61     17 21 56  47.5  29.9 -3.0    -115.7    26   1  1   4800  14 15 16
14 16 01  ---          17 22 41  47.6  29.8 -3.0    -115.9    45   F  1   5400

14 16 35  SN2004ET     17 23 15  46.7  32.7 -3.2    -110.9    26   1  1   5400  14 16 35
14 18 50  ---          17 25 31  47.0  32.6 -3.2    -111.5   135   F  1   7200

14 19 24  J2022+61     17 26 05  47.9  29.5 -2.9    -116.8    26   1  1   7200  14 19 24
14 20 09  ---          17 26 50  48.0  29.5 -2.9    -117.0    45   F  1   7800

14 20 42  SN2004ET     17 27 24  47.2  32.4 -3.1    -112.0    26   1  1   7800  14 20 42
14 22 57  ---          17 29 39  47.5  32.3 -3.1    -112.7   135   F  1   9600

14 23 31  J2022+61     17 30 13  48.4  29.2 -2.9    -118.0    26   1  1   9600  14 23 31
14 24 16  ---          17 30 58  48.5  29.1 -2.9    -118.2    45   F  1  10200

14 24 50  SN2004ET     17 31 32  47.7  32.1 -3.1    -113.2    26   1  1  10200  14 24 50
14 27 05  ---          17 33 47  48.0  32.0 -3.0    -113.8   135   F  1  12000

14 27 39  J2022+61     17 34 21  48.8  28.8 -2.8    -119.2    26   1  1  12000  14 27 39
14 28 24  ---          17 35 07  48.9  28.8 -2.8    -119.4    45   F  1  12600

14 28 58  SN2004ET     17 35 40  48.2  31.8 -3.0    -114.3    26   1  1  12600  14 28 58
14 31 13  ---          17 37 56  48.4  31.7 -3.0    -114.9   135   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

14 31 45  J2035+58     17 38 28  49.2  34.1 -2.9    -113.2    25   1  1  14400  14 31 45
14 32 45  ---          17 39 28  49.3  34.0 -2.9    -113.5    60   F  1  15200

14 33 18  SN2004ET     17 40 01  48.7  31.5 -2.9    -115.5    25   1  1  15200  14 33 18
14 36 18  ---          17 43 02  49.0  31.2 -2.9    -116.3   180   F  1  17600

14 36 58  J2022+61     17 43 42  49.8  28.0 -2.6    -121.9    32   1  2  17600  14 36 58
14 37 43  ---          17 44 27  49.8  27.9 -2.6    -122.1    45   R  1  17000

14 38 16  SN2004ET     17 45 00  49.2  31.1 -2.8    -116.9    25   1  2  17000  14 38 16
14 40 31  ---          17 47 16  49.5  30.9 -2.8    -117.5   135   R  1  15200

14 41 05  J2022+61     17 47 50  50.2  27.6 -2.6    -123.1    26   1  2  15200  14 41 05
14 41 50  ---          17 48 35  50.2  27.5 -2.6    -123.3    45   R  1  14600

14 42 24  SN2004ET     17 49 08  49.7  30.7 -2.8    -118.1    25   1  2  14600  14 42 24
14 44 39  ---          17 51 24  49.9  30.5 -2.7    -118.7   135   R  1  12800

14 45 12  J2022+61     17 51 58  50.6  27.1 -2.5    -124.3    26   1  2  12800  14 45 12
14 45 57  ---          17 52 43  50.7  27.1 -2.5    -124.6    45   R  1  12200

14 46 31  SN2004ET     17 53 16  50.1  30.3 -2.7    -119.2    25   1  2  12200  14 46 31
14 48 46  ---          17 55 32  50.4  30.1 -2.7    -119.9   135   R  1  10400

14 49 20  J2022+61     17 56 06  51.0  26.7 -2.4    -125.6    25   1  2  10400  14 49 20
14 50 05  ---          17 56 51  51.1  26.6 -2.4    -125.8    45   R  1   9800

14 50 38  SN2004ET     17 57 24  50.6  29.9 -2.6    -120.4    25   1  2   9800  14 50 38
14 52 53  ---          17 59 40  50.8  29.7 -2.6    -121.1   135   R  1   8000

14 53 27  J2022+61     18 00 13  51.4  26.2 -2.4    -126.9    25   1  2   8000  14 53 27
14 54 12  ---          18 00 58  51.5  26.1 -2.4    -127.1    45   R  1   7400

14 54 45  SN2004ET     18 01 32  51.0  29.5 -2.6    -121.7    25   1  2   7400  14 54 45
14 57 00  ---          18 03 47  51.3  29.3 -2.5    -122.3   135   R  1   5600

14 57 34  J2022+61     18 04 21  51.8  25.7 -2.3    -128.1    25   1  2   5600  14 57 34
14 58 19  ---          18 05 06  51.8  25.7 -2.3    -128.4    45   R  1   5000

14 58 52  SN2004ET     18 05 40  51.4  29.1 -2.5    -122.9    25   1  2   5000  14 58 52
15 01 07  ---          18 07 55  51.7  28.8 -2.5    -123.6   135   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

15 01 41  J2022+61     18 08 29  52.2  25.2 -2.2    -129.4    25   1  2   3200  15 01 41
15 02 41  ---          18 09 29  52.2  25.1 -2.2    -129.8    60   R  1   2400

15 03 14  SN2004ET     18 10 02  51.9  28.6 -2.4    -124.2    25   1  2   2400  15 03 14
15 06 14  ---          18 13 03  52.2  28.2 -2.4    -125.2   180   R  1      0

15 06 54  J2022+61     18 13 43  52.6  24.6 -2.1    -131.1    32   1  3      0  15 06 54
15 07 39  ---          18 14 28  52.7  24.5 -2.1    -131.4    45   F  1    600

15 08 12  SN2004ET     18 15 01  52.4  28.0 -2.3    -125.8    25   1  3    600  15 08 12
15 10 27  ---          18 17 17  52.6  27.7 -2.3    -126.5   135   F  1   2400

15 11 01  J2022+61     18 17 50  53.0  24.0 -2.1    -132.4    25   1  3   2400  15 11 01
15 11 46  ---          18 18 35  53.1  23.9 -2.1    -132.7    45   F  1   3000

15 12 19  SN2004ET     18 19 09  52.8  27.5 -2.3    -127.1    25   1  3   3000  15 12 19
15 14 34  ---          18 21 24  53.0  27.2 -2.2    -127.8   135   F  1   4800

15 15 07  J2022+61     18 21 58  53.3  23.5 -2.0    -133.8    25   1  3   4800  15 15 07
15 15 52  ---          18 22 43  53.4  23.4 -2.0    -134.1    45   F  1   5400

15 16 26  SN2004ET     18 23 16  53.2  27.0 -2.2    -128.4    25   1  3   5400  15 16 26
15 18 41  ---          18 25 32  53.4  26.7 -2.2    -129.1   135   F  1   7200

15 19 14  J2022+61     18 26 05  53.7  22.9 -1.9    -135.2    25   1  3   7200  15 19 14
15 19 59  ---          18 26 50  53.8  22.8 -1.9    -135.4    45   F  1   7800

15 20 32  SN2004ET     18 27 23  53.6  26.4 -2.1    -129.7    25   1  3   7800  15 20 32
15 22 47  ---          18 29 39  53.8  26.1 -2.1    -130.4   135   F  1   9600

15 23 21  J2022+61     18 30 12  54.0  22.3 -1.9    -136.6    25   1  3   9600  15 23 21
15 24 06  ---          18 30 57  54.1  22.2 -1.9    -136.8    45   F  1  10200

15 24 39  SN2004ET     18 31 31  54.0  25.9 -2.1    -131.1    25   1  3  10200  15 24 39
15 26 54  ---          18 33 46  54.2  25.6 -2.0    -131.8   135   F  1  12000

15 27 27  J2022+61     18 34 19  54.4  21.7 -1.8    -138.0    25   1  3  12000  15 27 27
15 28 12  ---          18 35 05  54.4  21.6 -1.8    -138.2    45   F  1  12600

15 28 45  SN2004ET     18 35 38  54.4  25.3 -2.0    -132.4    25   1  3  12600  15 28 45
15 31 00  ---          18 37 53  54.6  25.0 -2.0    -133.2   135   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

15 31 30  J2035+58     18 38 23  55.8  27.2 -2.0    -131.5    22   1  3  14400  15 31 30
15 32 30  ---          18 39 23  55.9  27.0 -1.9    -131.8    60   F  1  15200

15 33 01  SN2004ET     18 39 54  54.8  24.7 -1.9    -133.9    22   1  3  15200  15 33 01
15 36 01  ---          18 42 54  55.1  24.2 -1.9    -134.9   180   F  1  17600

15 36 41  J2022+61     18 43 34  55.1  20.3 -1.6    -141.2    31   1  4  17600  15 36 41
15 37 26  ---          18 44 19  55.1  20.1 -1.6    -141.4    45   R  1  17000

15 37 58  SN2004ET     18 44 52  55.2  23.9 -1.8    -135.6    24   1  4  17000  15 37 58
15 40 13  ---          18 47 08  55.4  23.5 -1.8    -136.3   135   R  1  15200

15 40 47  J2022+61     18 47 41  55.4  19.6 -1.6    -142.6    25   1  4  15200  15 40 47
15 41 32  ---          18 48 26  55.4  19.5 -1.6    -142.9    45   R  1  14600

15 42 05  SN2004ET     18 48 59  55.6  23.3 -1.8    -137.0    24   1  4  14600  15 42 05
15 44 20  ---          18 51 15  55.8  22.9 -1.7    -137.8   135   R  1  12800

15 44 53  J2022+61     18 51 48  55.7  18.9 -1.5    -144.1    25   1  4  12800  15 44 53
15 45 38  ---          18 52 33  55.7  18.8 -1.5    -144.4    45   R  1  12200

15 46 11  SN2004ET     18 53 06  55.9  22.6 -1.7    -138.4    24   1  4  12200  15 46 11
15 48 26  ---          18 55 21  56.1  22.2 -1.7    -139.2   135   R  1  10400

15 48 59  J2022+61     18 55 55  56.0  18.2 -1.4    -145.6    25   1  4  10400  15 48 59
15 49 44  ---          18 56 40  56.0  18.0 -1.4    -145.9    45   R  1   9800

15 50 17  SN2004ET     18 57 13  56.3  21.9 -1.6    -139.9    24   1  4   9800  15 50 17
15 52 32  ---          18 59 28  56.4  21.5 -1.6    -140.7   135   R  1   8000

15 53 05  J2022+61     19 00 01  56.2  17.4 -1.4    -147.1    24   1  4   8000  15 53 05
15 53 50  ---          19 00 46  56.3  17.3 -1.4    -147.4    45   R  1   7400

15 54 23  SN2004ET     19 01 19  56.6  21.2 -1.6    -141.4    24   1  4   7400  15 54 23
15 56 38  ---          19 03 35  56.8  20.8 -1.5    -142.2   135   R  1   5600

15 57 11  J2022+61     19 04 08  56.5  16.7 -1.3    -148.6    24   1  4   5600  15 57 11
15 57 56  ---          19 04 53  56.5  16.6 -1.3    -148.9    45   R  1   5000

15 58 28  SN2004ET     19 05 26  56.9  20.4 -1.5    -142.9    24   1  4   5000  15 58 28
16 00 43  ---          19 07 41  57.1  20.0 -1.5    -143.7   135   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

16 01 16  J2022+61     19 08 14  56.7  15.9 -1.2    -150.2    24   1  4   3200  16 01 16
16 02 16  ---          19 09 15  56.8  15.7 -1.2    -150.6    60   R  1   2400

16 02 49  SN2004ET     19 09 47  57.2  19.6 -1.4    -144.5    24   1  4   2400  16 02 49
16 05 49  ---          19 12 48  57.4  19.1 -1.4    -145.6   180   R  1      0

16 06 29  J2022+61     19 13 28  57.0  14.9 -1.1    -152.2    31   1  5      0  16 06 29
16 07 14  ---          19 14 13  57.1  14.8 -1.1    -152.5    45   F  1    600

16 07 47  SN2004ET     19 14 46  57.6  18.7 -1.3    -146.4    24   1  5    600  16 07 47
16 10 02  ---          19 17 01  57.7  18.2 -1.3    -147.3   135   F  1   2400

16 10 35  J2022+61     19 17 34  57.3  14.1 -1.1    -153.7    24   1  5   2400  16 10 35
16 11 20  ---          19 18 19  57.3  14.0 -1.1    -154.0    45   F  1   3000

16 11 52  SN2004ET     19 18 52  57.8  17.9 -1.3    -148.0    24   1  5   3000  16 11 52
16 14 07  ---          19 21 07  58.0  17.4 -1.2    -148.8   135   F  1   4800

16 14 40  J2022+61     19 21 40  57.5  13.3 -1.0    -155.3    24   1  5   4800  16 14 40
16 15 25  ---          19 22 25  57.5  13.2 -1.0    -155.6    45   F  1   5400

16 15 58  SN2004ET     19 22 58  58.1  17.1 -1.2    -149.6    24   1  5   5400  16 15 58
16 18 13  ---          19 25 13  58.3  16.6 -1.2    -150.4   135   F  1   7200

16 18 46  J2022+61     19 25 46  57.7  12.5 -0.9    -156.9    24   1  5   7200  16 18 46
16 19 31  ---          19 26 32  57.7  12.3 -0.9    -157.2    45   F  1   7800

16 20 03  SN2004ET     19 27 04  58.4  16.2 -1.1    -151.2    24   1  5   7800  16 20 03
16 22 18  ---          19 29 20  58.5  15.7 -1.1    -152.0   135   F  1   9600

16 22 51  J2022+61     19 29 53  57.8  11.6 -0.9    -158.6    24   1  5   9600  16 22 51
16 23 36  ---          19 30 38  57.9  11.5 -0.9    -158.9    45   F  1  10200

16 24 09  SN2004ET     19 31 10  58.6  15.4 -1.1    -152.8    24   1  5  10200  16 24 09
16 26 24  ---          19 33 26  58.7  14.9 -1.0    -153.7   135   F  1  12000

16 26 56  J2022+61     19 33 59  58.0  10.8 -0.8    -160.2    24   1  5  12000  16 26 56
16 27 41  ---          19 34 44  58.1  10.6 -0.8    -160.5    45   F  1  12600

16 28 14  SN2004ET     19 35 16  58.8  14.5 -1.0    -154.4    24   1  5  12600  16 28 14
16 30 29  ---          19 37 31  59.0  14.0 -1.0    -155.3   135   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

16 30 57  J2035+58     19 38 00  60.6  15.4 -1.0    -154.2    19   1  5  14400  16 30 57
16 31 57  ---          19 39 00  60.6  15.1 -0.9    -154.7    60   F  1  15200

16 33 57  SN2004ET     19 41 00  59.1  13.2 -0.9    -156.7   111   1  5  15200  16 33 57
16 36 57  ---          19 44 00  59.3  12.5 -0.9    -158.0   180   F  1  17600

16 37 37  J2022+61     19 44 41  58.4   8.5 -0.6    -164.5    31   1  6  17600  16 37 37
16 38 22  ---          19 45 26  58.4   8.3 -0.6    -164.8    45   R  1  17000

16 38 54  SN2004ET     19 45 58  59.4  12.1 -0.8    -158.8    24   1  6  17000  16 38 54
16 41 09  ---          19 48 13  59.5  11.6 -0.8    -159.7   135   R  1  15200

16 41 42  J2022+61     19 48 46  58.5   7.6 -0.6    -166.2    24   1  6  15200  16 41 42
16 42 27  ---          19 49 31  58.6   7.4 -0.5    -166.5    45   R  1  14600

16 42 59  SN2004ET     19 50 04  59.5  11.1 -0.8    -160.5    24   1  6  14600  16 42 59
16 45 14  ---          19 52 19  59.6  10.6 -0.7    -161.4   135   R  1  12800

16 45 47  J2022+61     19 52 52  58.6   6.7 -0.5    -167.8    24   1  6  12800  16 45 47
16 46 32  ---          19 53 37  58.7   6.5 -0.5    -168.1    45   R  1  12200

16 47 04  SN2004ET     19 54 09  59.7  10.2 -0.7    -162.2    24   1  6  12200  16 47 04
16 49 19  ---          19 56 25  59.8   9.7 -0.7    -163.1   135   R  1  10400

16 49 52  J2022+61     19 56 57  58.7   5.8 -0.4    -169.5    24   1  6  10400  16 49 52
16 50 37  ---          19 57 43  58.7   5.6 -0.4    -169.8    45   R  1   9800

16 51 09  SN2004ET     19 58 15  59.9   9.2 -0.6    -163.9    24   1  6   9800  16 51 09
16 53 24  ---          20 00 30  59.9   8.7 -0.6    -164.9   135   R  1   8000

16 53 56  J2022+61     20 01 03  58.8   4.8 -0.4    -171.2    24   1  6   8000  16 53 56
16 54 41  ---          20 01 48  58.8   4.7 -0.3    -171.5    45   R  1   7400

16 55 13  SN2004ET     20 02 20  60.0   8.2 -0.6    -165.6    24   1  6   7400  16 55 13
16 57 28  ---          20 04 36  60.1   7.7 -0.5    -166.6   135   R  1   5600

16 58 01  J2022+61     20 05 08  58.9   3.9 -0.3    -172.9    24   1  6   5600  16 58 01
16 58 46  ---          20 05 53  58.9   3.7 -0.3    -173.2    45   R  1   5000

16 59 18  SN2004ET     20 06 25  60.1   7.3 -0.5    -167.4    24   1  6   5000  16 59 18
17 01 33  ---          20 08 41  60.2   6.7 -0.4    -168.4   135   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

17 02 06  J2022+61     20 09 13  58.9   3.0 -0.2    -174.6    24   1  6   3200  17 02 06
17 03 06  ---          20 10 14  58.9   2.7 -0.2    -175.0    60   R  1   2400

17 03 38  SN2004ET     20 10 46  60.2   6.2 -0.4    -169.3    24   1  6   2400  17 03 38
17 06 38  ---          20 13 46  60.3   5.5 -0.4    -170.6   180   R  1      0

17 07 18  J2022+61     20 14 26  59.0   1.8 -0.1    -176.8    31   1  7      0  17 07 18
17 08 03  ---          20 15 11  59.0   1.6 -0.1    -177.1    45   F  1    600

17 08 35  SN2004ET     20 15 44  60.3   5.0 -0.3    -171.4    23   1  7    600  17 08 35
17 10 50  ---          20 17 59  60.4   4.4 -0.3    -172.4   135   F  1   2400

17 11 22  J2022+61     20 18 31  59.0   0.8 -0.1    -178.5    24   1  7   2400  17 11 22
17 12 07  ---          20 19 17  59.0   0.7  0.0    -178.8    45   F  1   3000

17 12 39  SN2004ET     20 19 49  60.4   3.9 -0.3    -173.2    23   1  7   3000  17 12 39
17 14 54  ---          20 22 04  60.4   3.4 -0.2    -174.1   135   F  1   4800

17 15 26  J2022+61     20 22 36  59.0  -0.1  0.0     179.8    24   1  7   4800  17 15 26
17 16 11  ---          20 23 22  59.0  -0.3  0.0     179.5    45   F  1   5400

17 16 43  SN2004ET     20 23 54  60.4   2.9 -0.2    -174.9    23   1  7   5400  17 16 43
17 18 58  ---          20 26 09  60.5   2.4 -0.2    -175.9   135   F  1   7200

17 19 31  J2022+61     20 26 41  59.0  -1.0  0.1     178.1    23   1  7   7200  17 19 31
17 20 16  ---          20 27 26  59.0  -1.2  0.1     177.8    45   F  1   7800

17 20 48  SN2004ET     20 27 58  60.5   1.9 -0.1    -176.7    23   1  7   7800  17 20 48
17 23 03  ---          20 30 14  60.5   1.3 -0.1    -177.7   135   F  1   9600

17 23 35  J2022+61     20 30 46  59.0  -2.0  0.1     176.4    23   1  7   9600  17 23 35
17 24 20  ---          20 31 31  59.0  -2.2  0.2     176.1    45   F  1  10200

17 24 52  SN2004ET     20 32 03  60.5   0.9 -0.1    -178.5    23   1  7  10200  17 24 52
17 27 07  ---          20 34 19  60.5   0.3  0.0    -179.5   135   F  1  12000

17 27 39  J2022+61     20 34 51  58.9  -2.9  0.2     174.7    23   1  7  12000  17 27 39
17 28 24  ---          20 35 36  58.9  -3.1  0.2     174.4    45   F  1  12600

17 28 56  SN2004ET     20 36 08  60.5  -0.2  0.0     179.7    23   1  7  12600  17 28 56
17 31 11  ---          20 38 23  60.5  -0.7  0.0     178.7   135   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

17 31 37  J2035+58     20 38 49  62.3  -0.9  0.1     178.4    16   1  7  14400  17 31 37
17 32 37  ---          20 39 49  62.3  -1.2  0.1     178.0    60   F  1  15200

17 33 03  SN2004ET     20 40 16  60.5  -1.2  0.1     177.9    17   1  7  15200  17 33 03
17 36 03  ---          20 43 16  60.5  -2.0  0.1     176.6   180   F  1  17600

17 36 43  J2022+61     20 43 57  58.8  -5.0  0.4     170.9    31   1  8  17600  17 36 43
17 37 28  ---          20 44 42  58.8  -5.2  0.4     170.6    45   R  1  17000

17 38 00  SN2004ET     20 45 13  60.5  -2.5  0.2     175.7    22   1  8  17000  17 38 00
17 40 15  ---          20 47 29  60.4  -3.0  0.2     174.8   135   R  1  15200

17 40 47  J2022+61     20 48 01  58.7  -5.9  0.4     169.2    23   1  8  15200  17 40 47
17 41 32  ---          20 48 46  58.7  -6.1  0.4     168.9    45   R  1  14600

17 42 03  SN2004ET     20 49 18  60.4  -3.5  0.2     174.0    22   1  8  14600  17 42 03
17 44 18  ---          20 51 33  60.4  -4.0  0.3     173.0   135   R  1  12800

17 44 51  J2022+61     20 52 05  58.6  -6.8  0.5     167.6    23   1  8  12800  17 44 51
17 45 36  ---          20 52 51  58.6  -7.0  0.5     167.3    45   R  1  12200

17 46 07  SN2004ET     20 53 22  60.3  -4.5  0.3     172.2    22   1  8  12200  17 46 07
17 48 22  ---          20 55 38  60.3  -5.1  0.3     171.2   135   R  1  10400

17 48 54  J2022+61     20 56 10  58.5  -7.7  0.6     165.9    22   1  8  10400  17 48 54
17 49 39  ---          20 56 55  58.5  -7.9  0.6     165.6    45   R  1   9800

17 50 11  SN2004ET     20 57 27  60.3  -5.5  0.4     170.4    22   1  8   9800  17 50 11
17 52 26  ---          20 59 42  60.2  -6.1  0.4     169.5   135   R  1   8000

17 52 58  J2022+61     21 00 14  58.4  -8.6  0.6     164.2    22   1  8   8000  17 52 58
17 53 43  ---          21 00 59  58.4  -8.8  0.6     163.9    45   R  1   7400

17 54 14  SN2004ET     21 01 31  60.2  -6.5  0.4     168.7    22   1  8   7400  17 54 14
17 56 29  ---          21 03 46  60.1  -7.1  0.5     167.7   135   R  1   5600

17 57 01  J2022+61     21 04 18  58.2  -9.5  0.7     162.6    22   1  8   5600  17 57 01
17 57 46  ---          21 05 03  58.2  -9.7  0.7     162.3    45   R  1   5000

17 58 18  SN2004ET     21 05 35  60.1  -7.5  0.5     166.9    22   1  8   5000  17 58 18
18 00 33  ---          21 07 50  60.0  -8.1  0.5     166.0   135   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

18 01 05  J2022+61     21 08 22  58.1 -10.4  0.8     161.0    22   1  8   3200  18 01 05
18 02 05  ---          21 09 22  58.1 -10.6  0.8     160.6    60   R  1   2400

18 02 36  SN2004ET     21 09 54  59.9  -8.6  0.6     165.1    22   1  8   2400  18 02 36
18 05 36  ---          21 12 54  59.8  -9.3  0.6     163.8   180   R  1      0

18 06 16  J2022+61     21 13 34  57.9 -11.5  0.9     158.9    30   1  9      0  18 06 16
18 07 01  ---          21 14 20  57.9 -11.6  0.9     158.6    45   F  1    600

18 07 32  SN2004ET     21 14 51  59.8  -9.7  0.7     163.0    22   1  9    600  18 07 32
18 09 47  ---          21 17 06  59.7 -10.3  0.7     162.1   135   F  1   2400

18 10 19  J2022+61     21 17 38  57.7 -12.3  0.9     157.3    22   1  9   2400  18 10 19
18 11 04  ---          21 18 23  57.7 -12.5  0.9     157.0    45   F  1   3000

18 11 36  SN2004ET     21 18 55  59.6 -10.7  0.7     161.3    21   1  9   3000  18 11 36
18 13 51  ---          21 21 10  59.5 -11.2  0.8     160.4   135   F  1   4800

18 14 22  J2022+61     21 21 42  57.5 -13.1  1.0     155.7    22   1  9   4800  18 14 22
18 15 07  ---          21 22 27  57.5 -13.3  1.0     155.4    45   F  1   5400

18 15 39  SN2004ET     21 22 58  59.5 -11.6  0.8     159.6    21   1  9   5400  18 15 39
18 17 54  ---          21 25 14  59.4 -12.1  0.8     158.7   135   F  1   7200

18 18 25  J2022+61     21 25 46  57.3 -13.9  1.1     154.1    22   1  9   7200  18 18 25
18 19 10  ---          21 26 31  57.3 -14.1  1.1     153.8    45   F  1   7800

18 19 41  SN2004ET     21 27 02  59.3 -12.6  0.9     157.9    21   1  9   7800  18 19 41
18 21 56  ---          21 29 17  59.2 -13.1  0.9     157.0   135   F  1   9600

18 22 28  J2022+61     21 29 49  57.1 -14.7  1.1     152.6    22   1  9   9600  18 22 28
18 23 13  ---          21 30 34  57.0 -14.9  1.1     152.3    45   F  1  10200

18 23 44  SN2004ET     21 31 06  59.1 -13.5  0.9     156.3    21   1  9  10200  18 23 44
18 25 59  ---          21 33 21  59.0 -14.0  1.0     155.4   135   F  1  12000

18 26 31  J2022+61     21 33 53  56.9 -15.5  1.2     151.0    21   1  9  12000  18 26 31
18 27 16  ---          21 34 38  56.8 -15.7  1.2     150.7    45   F  1  12600

18 27 47  SN2004ET     21 35 09  58.9 -14.4  1.0     154.6    21   1  9  12600  18 27 47
18 30 02  ---          21 37 24  58.7 -14.8  1.0     153.7   135   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

18 30 28  J2035+58     21 37 51  60.3 -16.5  1.0     152.2    17   1  9  14400  18 30 28
18 31 28  ---          21 38 51  60.2 -16.8  1.1     151.8    60   F  1  15200

18 31 54  SN2004ET     21 39 17  58.6 -15.2  1.1     153.0    17   1  9  15200  18 31 54
18 34 54  ---          21 42 17  58.5 -15.9  1.1     151.8   180   F  1  17600

18 35 34  J2022+61     21 42 57  56.3 -17.2  1.3     147.6    30   1 10  17600  18 35 34
18 36 19  ---          21 43 42  56.3 -17.3  1.4     147.3    45   R  1  17000

18 36 50  SN2004ET     21 44 13  58.3 -16.3  1.1     151.0    21   1 10  17000  18 36 50
18 39 05  ---          21 46 29  58.2 -16.7  1.2     150.1   135   R  1  15200

18 39 37  J2022+61     21 47 00  56.0 -17.9  1.4     146.1    21   1 10  15200  18 39 37
18 40 22  ---          21 47 46  56.0 -18.1  1.4     145.8    45   R  1  14600

18 40 52  SN2004ET     21 48 17  58.1 -17.1  1.2     149.4    21   1 10  14600  18 40 52
18 43 07  ---          21 50 32  58.0 -17.6  1.3     148.6   135   R  1  12800

18 43 39  J2022+61     21 51 03  55.8 -18.6  1.5     144.6    21   1 10  12800  18 43 39
18 44 24  ---          21 51 49  55.7 -18.8  1.5     144.4    45   R  1  12200

18 44 55  SN2004ET     21 52 20  57.8 -17.9  1.3     147.9    21   1 10  12200  18 44 55
18 47 10  ---          21 54 35  57.7 -18.4  1.3     147.0   135   R  1  10400

18 47 41  J2022+61     21 55 06  55.5 -19.3  1.5     143.2    21   1 10  10400  18 47 41
18 48 26  ---          21 55 52  55.4 -19.5  1.6     142.9    45   R  1   9800

18 48 57  SN2004ET     21 56 22  57.6 -18.7  1.3     146.3    21   1 10   9800  18 48 57
18 51 12  ---          21 58 38  57.4 -19.2  1.4     145.5   135   R  1   8000

18 51 43  J2022+61     21 59 09  55.2 -20.0  1.6     141.7    21   1 10   8000  18 51 43
18 52 28  ---          21 59 54  55.1 -20.1  1.6     141.5    45   R  1   7400

18 52 59  SN2004ET     22 00 25  57.3 -19.5  1.4     144.8    21   1 10   7400  18 52 59
18 55 14  ---          22 02 41  57.1 -19.9  1.5     144.0   135   R  1   5600

18 55 46  J2022+61     22 03 12  54.9 -20.7  1.7     140.3    21   1 10   5600  18 55 46
18 56 31  ---          22 03 57  54.8 -20.8  1.7     140.1    45   R  1   5000

18 57 01  SN2004ET     22 04 28  57.0 -20.2  1.5     143.3    20   1 10   5000  18 57 01
18 59 16  ---          22 06 43  56.8 -20.7  1.5     142.5   135   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

18 59 48  J2022+61     22 07 15  54.6 -21.3  1.8     138.9    21   1 10   3200  18 59 48
19 00 48  ---          22 08 15  54.5 -21.4  1.8     138.6    60   R  1   2400

19 02 48  SN2004ET     22 10 15  56.5 -21.3  1.6     141.2   110   1 10   2400  19 02 48
19 05 48  ---          22 13 16  56.3 -21.8  1.6     140.1   180   R  1      0

19 06 28  J2022+61     22 13 56  54.1 -22.3  1.9     136.6    30   1 11      0  19 06 28
19 07 13  ---          22 14 41  54.0 -22.4  1.9     136.4    45   F  1    600

19 07 43  SN2004ET     22 15 12  56.1 -22.1  1.7     139.4    20   1 11    600  19 07 43
19 09 58  ---          22 17 27  56.0 -22.5  1.7     138.6   135   F  1   2400

19 10 29  J2022+61     22 17 58  53.7 -22.9  1.9     135.3    21   1 11   2400  19 10 29
19 11 14  ---          22 18 43  53.7 -23.0  1.9     135.0    45   F  1   3000

19 11 45  SN2004ET     22 19 14  55.8 -22.8  1.7     137.9    20   1 11   3000  19 11 45
19 14 00  ---          22 21 29  55.6 -23.2  1.8     137.2   135   F  1   4800

19 14 31  J2022+61     22 22 00  53.4 -23.4  2.0     133.9    21   1 11   4800  19 14 31
19 15 16  ---          22 22 46  53.3 -23.5  2.0     133.7    45   F  1   5400

19 15 46  SN2004ET     22 23 16  55.5 -23.5  1.8     136.5    20   1 11   5400  19 15 46
19 18 01  ---          22 25 31  55.3 -23.8  1.8     135.8   135   F  1   7200

19 18 32  J2022+61     22 26 03  53.0 -24.0  2.1     132.6    21   1 11   7200  19 18 32
19 19 17  ---          22 26 48  53.0 -24.1  2.1     132.3    45   F  1   7800

19 19 48  SN2004ET     22 27 18  55.1 -24.1  1.9     135.1    20   1 11   7800  19 19 48
19 22 03  ---          22 29 34  54.9 -24.4  1.9     134.4   135   F  1   9600

19 22 34  J2022+61     22 30 05  52.7 -24.5  2.1     131.3    20   1 11   9600  19 22 34
19 23 19  ---          22 30 50  52.6 -24.6  2.1     131.0    45   F  1  10200

19 23 49  SN2004ET     22 31 20  54.8 -24.7  1.9     133.8    20   1 11  10200  19 23 49
19 26 04  ---          22 33 36  54.6 -25.0  2.0     133.0   135   F  1  12000

19 26 35  J2022+61     22 34 06  52.3 -25.0  2.2     130.0    20   1 11  12000  19 26 35
19 27 20  ---          22 34 52  52.2 -25.1  2.2     129.7    45   F  1  12600

19 27 50  SN2004ET     22 35 22  54.4 -25.3  2.0     132.4    20   1 11  12600  19 27 50
19 30 05  ---          22 37 37  54.2 -25.6  2.0     131.7   135   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

19 30 32  J2035+58     22 38 04  55.3 -28.0  2.0     129.6    19   1 11  14400  19 30 32
19 31 32  ---          22 39 05  55.2 -28.2  2.1     129.3    60   F  1  15200

19 31 59  SN2004ET     22 39 31  54.0 -25.9  2.1     131.0    18   1 11  15200  19 31 59
19 34 59  ---          22 42 32  53.7 -26.3  2.1     130.0   180   F  1  17600

19 35 39  J2022+61     22 43 12  51.5 -26.1  2.4     127.1    29   1 12  17600  19 35 39
19 36 24  ---          22 43 57  51.4 -26.2  2.4     126.9    45   R  1  17000

19 36 54  SN2004ET     22 44 27  53.5 -26.6  2.1     129.4    20   1 12  17000  19 36 54
19 39 09  ---          22 46 43  53.3 -26.9  2.2     128.7   135   R  1  15200

19 39 40  J2022+61     22 47 14  51.1 -26.6  2.4     125.9    20   1 12  15200  19 39 40
19 40 25  ---          22 47 59  51.0 -26.7  2.4     125.7    45   R  1  14600

19 40 55  SN2004ET     22 48 29  53.2 -27.1  2.2     128.1    20   1 12  14600  19 40 55
19 43 10  ---          22 50 44  52.9 -27.4  2.3     127.4   135   R  1  12800

19 43 41  J2022+61     22 51 15  50.7 -27.0  2.5     124.7    20   1 12  12800  19 43 41
19 44 26  ---          22 52 00  50.6 -27.1  2.5     124.4    45   R  1  12200

19 44 56  SN2004ET     22 52 30  52.8 -27.6  2.3     126.8    20   1 12  12200  19 44 56
19 47 11  ---          22 54 46  52.5 -27.9  2.3     126.1   135   R  1  10400

19 47 41  J2022+61     22 55 16  50.3 -27.4  2.6     123.5    20   1 12  10400  19 47 41
19 48 26  ---          22 56 01  50.2 -27.5  2.6     123.2    45   R  1   9800

19 48 56  SN2004ET     22 56 31  52.3 -28.1  2.4     125.6    20   1 12   9800  19 48 56
19 51 11  ---          22 58 47  52.1 -28.3  2.4     124.9   135   R  1   8000

19 51 42  J2022+61     22 59 17  49.9 -27.8  2.6     122.3    20   1 12   8000  19 51 42
19 52 27  ---          23 00 03  49.8 -27.9  2.6     122.0    45   R  1   7400

19 52 57  SN2004ET     23 00 33  51.9 -28.5  2.4     124.4    20   1 12   7400  19 52 57
19 55 12  ---          23 02 48  51.7 -28.8  2.5     123.7   135   R  1   5600

19 55 42  J2022+61     23 03 18  49.5 -28.2  2.7     121.1    20   1 12   5600  19 55 42
19 56 27  ---          23 04 04  49.4 -28.3  2.7     120.9    45   R  1   5000

19 56 57  SN2004ET     23 04 33  51.5 -29.0  2.5     123.1    20   1 12   5000  19 56 57
19 59 12  ---          23 06 49  51.3 -29.2  2.5     122.4   135   R  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

19 59 42  J2022+61     23 07 19  49.1 -28.6  2.8     119.9    20   1 12   3200  19 59 42
20 00 42  ---          23 08 19  49.0 -28.7  2.8     119.6    60   R  1   2400

20 01 12  SN2004ET     23 08 49  51.1 -29.4  2.6     121.8    20   1 12   2400  20 01 12
20 04 12  ---          23 11 50  50.8 -29.8  2.6     121.0   180   R  1      0

20 04 52  J2022+61     23 12 30  48.5 -29.1  2.8     118.4    30   1 13      0  20 04 52
20 05 37  ---          23 13 15  48.5 -29.1  2.9     118.2    45   F  1    600

20 06 07  SN2004ET     23 13 45  50.6 -29.9  2.6     120.4    20   1 13    600  20 06 07
20 08 22  ---          23 16 00  50.3 -30.2  2.7     119.7   135   F  1   2400

20 08 52  J2022+61     23 16 31  48.1 -29.4  2.9     117.3    20   1 13   2400  20 08 52
20 09 37  ---          23 17 16  48.0 -29.5  2.9     117.1    45   F  1   3000

20 10 07  SN2004ET     23 17 45  50.1 -30.3  2.7     119.2    19   1 13   3000  20 10 07
20 12 22  ---          23 20 01  49.9 -30.5  2.7     118.6   135   F  1   4800

20 12 52  J2022+61     23 20 31  47.7 -29.7  3.0     116.2    20   1 13   4800  20 12 52
20 13 37  ---          23 21 16  47.6 -29.8  3.0     116.0    45   F  1   5400

20 14 06  SN2004ET     23 21 46  49.7 -30.7  2.8     118.1    19   1 13   5400  20 14 06
20 16 21  ---          23 24 01  49.4 -30.9  2.8     117.4   135   F  1   7200

20 16 52  J2022+61     23 24 31  47.3 -30.0  3.0     115.1    20   1 13   7200  20 16 52
20 17 37  ---          23 25 16  47.2 -30.1  3.1     114.9    45   F  1   7800

20 18 06  SN2004ET     23 25 46  49.2 -31.1  2.8     116.9    19   1 13   7800  20 18 06
20 20 21  ---          23 28 01  49.0 -31.3  2.9     116.3   135   F  1   9600

20 20 51  J2022+61     23 28 32  46.8 -30.3  3.1     114.0    20   1 13   9600  20 20 51
20 21 36  ---          23 29 17  46.7 -30.4  3.1     113.8    45   F  1  10200

20 22 05  SN2004ET     23 29 46  48.8 -31.4  2.9     115.8    19   1 13  10200  20 22 05
20 24 20  ---          23 32 02  48.5 -31.6  2.9     115.2   135   F  1  12000

20 24 50  J2022+61     23 32 32  46.4 -30.6  3.2     112.9    20   1 13  12000  20 24 50
20 25 35  ---          23 33 17  46.3 -30.6  3.2     112.7    45   F  1  12600

20 26 05  SN2004ET     23 33 46  48.3 -31.7  3.0     114.7    19   1 13  12600  20 26 05
20 28 20  ---          23 36 02  48.1 -31.9  3.0     114.1   135   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

20 28 47  J2035+58     23 36 29  48.7 -34.4  3.0     112.1    20   1 13  14400  20 28 47
20 29 47  ---          23 37 29  48.6 -34.5  3.0     111.9    60   F  1  15200

20 30 15  SN2004ET     23 37 57  47.9 -32.0  3.0     113.6    20   1 13  15200  20 30 15
20 33 15  ---          23 40 57  47.5 -32.3  3.1     112.7   180   F  1  17600

20 33 55  J2022+61     23 41 37  45.4 -31.2  3.3     110.5    30   1 14  17600  20 33 55
20 35 25  ---          23 43 08  45.2 -31.2  3.3     110.1    90   R  1  16400

20 35 25  SN2004ET     23 43 08  47.3 -32.4  3.1     112.2   -10   1 14  16400  20 35 25
20 38 25  ---          23 46 08  46.9 -32.6  3.2     111.4   170   R  1  14000

20 38 25  J2022+61     23 46 08  44.9 -31.4  3.4     109.3   -10   1 14  14000  20 38 25
20 39 55  ---          23 47 38  44.7 -31.5  3.4     108.9    80   R  1  12800

20 39 55  SN2004ET     23 47 38  46.7 -32.7  3.2     111.0   -10   1 14  12800  20 39 55
20 42 55  ---          23 50 39  46.4 -32.9  3.3     110.2   170   R  1  10400

20 42 55  J2022+61     23 50 39  44.4 -31.7  3.5     108.2   -10   1 14  10400  20 42 55
20 44 25  ---          23 52 09  44.2 -31.7  3.5     107.8    80   R  1   9200

20 44 25  SN2004ET     23 52 09  46.2 -33.0  3.3     109.8   -10   1 14   9200  20 44 25
20 47 25  ---          23 55 10  45.9 -33.2  3.3     109.0   170   R  1   6800

20 47 25  2007+777     23 55 10  36.5 -12.7  3.8     115.4   -25   1 14   6800  20 47 25
20 55 55  ---          00 03 41  36.1 -12.9  4.0     113.2   485   R  1      0

-----------  Tape Change ------------

21 10 55  3C48         00 18 43  73.0  76.2 -1.3     -93.3   820   2  1      0  21 10 55
21 17 55  ---          00 25 45  74.5  75.8 -1.2     -94.6   420   F  1   5600

21 27 57  J2022+61     00 35 49  39.1 -33.2  4.2      97.2   524   2  1   5600  21 27 57
21 28 42  ---          00 36 34  39.1 -33.2  4.2      97.0    45   F  1   6200

21 29 10  SN2004ET     00 37 02  40.8 -34.9  4.0      98.7    19   2  1   6200  21 29 10
21 31 25  ---          00 39 17  40.5 -34.9  4.1      98.2   135   F  1   8000

21 31 54  J2022+61     00 39 46  38.7 -33.3  4.3      96.2    19   2  1   8000  21 31 54
21 32 39  ---          00 40 31  38.6 -33.3  4.3      96.1    45   F  1   8600

21 33 07  SN2004ET     00 40 59  40.3 -35.0  4.1      97.8    18   2  1   8600  21 33 07
21 35 22  ---          00 43 14  40.0 -35.0  4.1      97.3   135   F  1  10400
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

21 35 50  J2022+61     00 43 43  38.2 -33.4  4.4      95.3    19   2  1  10400  21 35 50
21 36 35  ---          00 44 28  38.1 -33.4  4.4      95.2    45   F  1  11000

21 37 03  SN2004ET     00 44 56  39.8 -35.1  4.2      96.9    18   2  1  11000  21 37 03
21 39 18  ---          00 47 11  39.6 -35.1  4.2      96.4   135   F  1  12800

21 39 46  J2022+61     00 47 40  37.7 -33.4  4.4      94.4    19   2  1  12800  21 39 46
21 40 31  ---          00 48 25  37.7 -33.4  4.4      94.3    45   F  1  13400

21 40 59  SN2004ET     00 48 53  39.4 -35.1  4.2      96.0    18   2  1  13400  21 40 59
21 43 14  ---          00 51 08  39.1 -35.2  4.3      95.5   135   F  1  15200

21 43 42  J2022+61     00 51 37  37.3 -33.5  4.5      93.5    19   2  1  15200  21 43 42
21 44 27  ---          00 52 22  37.2 -33.5  4.5      93.4    45   F  1  15800

21 44 55  SN2004ET     00 52 49  38.9 -35.2  4.3      95.1    18   2  1  15800  21 44 55
21 47 10  ---          00 55 05  38.6 -35.2  4.3      94.6   135   F  1  17600

21 47 50  J2022+61     00 55 45  36.8 -33.5  4.6      92.6    30   2  2  17600  21 47 50
21 48 35  ---          00 56 30  36.7 -33.5  4.6      92.4    45   R  1  17000

21 49 03  SN2004ET     00 56 58  38.3 -35.3  4.4      94.2    18   2  2  17000  21 49 03
21 51 18  ---          00 59 13  38.1 -35.3  4.4      93.7   135   R  1  15200

21 51 46  J2022+61     00 59 41  36.3 -33.5  4.6      91.7    19   2  2  15200  21 51 46
21 52 31  ---          01 00 26  36.2 -33.5  4.6      91.6    45   R  1  14600

21 52 58  SN2004ET     01 00 54  37.9 -35.3  4.4      93.3    18   2  2  14600  21 52 58
21 55 13  ---          01 03 09  37.6 -35.3  4.5      92.8   135   R  1  12800

21 55 41  J2022+61     01 03 37  35.9 -33.5  4.7      90.9    19   2  2  12800  21 55 41
21 56 26  ---          01 04 23  35.8 -33.5  4.7      90.7    45   R  1  12200

21 56 54  SN2004ET     01 04 50  37.4 -35.3  4.5      92.4    18   2  2  12200  21 56 54
21 59 09  ---          01 07 05  37.1 -35.3  4.5      91.9   135   R  1  10400

21 59 37  J2022+61     01 07 33  35.4 -33.5  4.8      90.0    19   2  2  10400  21 59 37
22 00 22  ---          01 08 18  35.3 -33.5  4.8      89.8    45   R  1   9800

22 00 49  SN2004ET     01 08 46  36.9 -35.3  4.6      91.6    18   2  2   9800  22 00 49
22 03 04  ---          01 11 01  36.6 -35.4  4.6      91.1   135   R  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

22 03 32  J2022+61     01 11 29  34.9 -33.5  4.8      89.1    18   2  2   8000  22 03 32
22 04 17  ---          01 12 14  34.8 -33.5  4.8      89.0    45   R  1   7400

22 04 44  SN2004ET     01 12 41  36.4 -35.4  4.6      90.7    18   2  2   7400  22 04 44
22 06 59  ---          01 14 57  36.1 -35.4  4.7      90.2   135   R  1   5600

22 07 27  J2022+61     01 15 25  34.5 -33.5  4.9      88.3    18   2  2   5600  22 07 27
22 08 12  ---          01 16 10  34.4 -33.5  4.9      88.1    45   R  1   5000

22 08 39  SN2004ET     01 16 37  35.9 -35.4  4.7      89.9    18   2  2   5000  22 08 39
22 10 54  ---          01 18 52  35.6 -35.4  4.7      89.4   135   R  1   3200

22 11 21  J2035+58     01 19 20  35.5 -37.5  4.7      88.0    20   2  2   3200  22 11 21
22 12 21  ---          01 20 20  35.4 -37.5  4.7      87.8    60   R  1   2400

22 12 49  SN2004ET     01 20 48  35.4 -35.4  4.8      89.0    20   2  2   2400  22 12 49
22 15 49  ---          01 23 49  35.0 -35.3  4.8      88.3   180   R  1      0

22 16 29  J2022+61     01 24 29  33.4 -33.4  5.0      86.3    31   2  3      0  22 16 29
22 17 14  ---          01 25 14  33.3 -33.4  5.1      86.2    45   F  1    600

22 17 41  SN2004ET     01 25 41  34.8 -35.3  4.8      87.9    18   2  3    600  22 17 41
22 19 56  ---          01 27 56  34.5 -35.3  4.9      87.4   135   F  1   2400

22 20 23  J2022+61     01 28 24  32.9 -33.4  5.1      85.5    18   2  3   2400  22 20 23
22 21 08  ---          01 29 09  32.8 -33.4  5.1      85.3    45   F  1   3000

22 21 35  SN2004ET     01 29 36  34.3 -35.3  4.9      87.1    18   2  3   3000  22 21 35
22 23 50  ---          01 31 51  34.0 -35.3  4.9      86.6   135   F  1   4800

22 24 18  J2022+61     01 32 18  32.5 -33.4  5.2      84.6    18   2  3   4800  22 24 18
22 25 03  ---          01 33 03  32.4 -33.3  5.2      84.5    45   F  1   5400

22 25 30  SN2004ET     01 33 31  33.8 -35.3  5.0      86.2    18   2  3   5400  22 25 30
22 27 45  ---          01 35 46  33.5 -35.3  5.0      85.8   135   F  1   7200

22 28 12  J2022+61     01 36 13  32.0 -33.3  5.2      83.8    18   2  3   7200  22 28 12
22 28 57  ---          01 36 58  31.9 -33.3  5.2      83.7    45   F  1   7800

22 29 24  SN2004ET     01 37 25  33.3 -35.2  5.0      85.4    18   2  3   7800  22 29 24
22 31 39  ---          01 39 41  33.0 -35.2  5.1      84.9   135   F  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

22 32 06  J2022+61     01 40 08  31.5 -33.2  5.3      83.0    18   2  3   9600  22 32 06
22 32 51  ---          01 40 53  31.4 -33.2  5.3      82.8    45   F  1  10200

22 33 18  SN2004ET     01 41 20  32.8 -35.2  5.1      84.6    18   2  3  10200  22 33 18
22 35 33  ---          01 43 36  32.6 -35.1  5.1      84.1   135   F  1  12000

22 36 00  J2022+61     01 44 03  31.1 -33.2  5.4      82.2    18   2  3  12000  22 36 00
22 36 45  ---          01 44 48  31.0 -33.2  5.4      82.0    45   F  1  12600

22 37 13  SN2004ET     01 45 16  32.3 -35.1  5.2      83.8    19   2  3  12600  22 37 13
22 39 28  ---          01 47 31  32.1 -35.1  5.2      83.3   135   F  1  14400

22 39 55  J2035+58     01 47 59  31.8 -37.1  5.2      82.1    20   2  3  14400  22 39 55
22 40 55  ---          01 48 59  31.7 -37.1  5.2      81.9    60   F  1  15200

22 41 23  SN2004ET     01 49 27  31.8 -35.1  5.2      82.9    20   2  3  15200  22 41 23
22 44 23  ---          01 52 27  31.5 -35.0  5.3      82.3   180   F  1  17600

22 45 03  J2022+61     01 53 07  30.0 -33.0  5.5      80.3    31   2  4  17600  22 45 03
22 45 48  ---          01 53 53  29.9 -33.0  5.5      80.1    45   R  1  17000

22 46 16  SN2004ET     01 54 20  31.2 -35.0  5.3      81.9    19   2  4  17000  22 46 16
22 48 31  ---          01 56 35  30.9 -34.9  5.4      81.4   135   R  1  15200

22 48 58  J2022+61     01 57 03  29.5 -32.9  5.6      79.4    19   2  4  15200  22 48 58
22 49 43  ---          01 57 48  29.5 -32.9  5.6      79.3    45   R  1  14600

22 50 11  SN2004ET     01 58 16  30.7 -34.9  5.4      81.1    19   2  4  14600  22 50 11
22 52 26  ---          02 00 31  30.5 -34.8  5.4      80.6   135   R  1  12800

22 52 54  J2022+61     02 00 59  29.1 -32.8  5.6      78.6    19   2  4  12800  22 52 54
22 53 39  ---          02 01 44  29.0 -32.8  5.7      78.5    45   R  1  12200

22 54 06  SN2004ET     02 02 12  30.3 -34.8  5.4      80.3    19   2  4  12200  22 54 06
22 56 21  ---          02 04 27  30.0 -34.7  5.5      79.8   135   R  1  10400

22 56 49  J2022+61     02 04 55  28.6 -32.7  5.7      77.8    19   2  4  10400  22 56 49
22 57 34  ---          02 05 40  28.5 -32.7  5.7      77.7    45   R  1   9800

22 58 02  SN2004ET     02 06 08  29.8 -34.7  5.5      79.5    19   2  4   9800  22 58 02
23 00 17  ---          02 08 23  29.5 -34.6  5.5      79.0   135   R  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

23 00 44  J2022+61     02 08 51  28.2 -32.6  5.8      77.0    19   2  4   8000  23 00 44
23 01 29  ---          02 09 36  28.1 -32.5  5.8      76.8    45   R  1   7400

23 01 57  SN2004ET     02 10 04  29.3 -34.6  5.6      78.7    19   2  4   7400  23 01 57
23 04 12  ---          02 12 20  29.0 -34.5  5.6      78.2   135   R  1   5600

23 04 40  J2022+61     02 12 48  27.7 -32.4  5.8      76.2    19   2  4   5600  23 04 40
23 05 25  ---          02 13 33  27.6 -32.4  5.9      76.0    45   R  1   5000

23 05 53  SN2004ET     02 14 01  28.8 -34.5  5.6      77.9    19   2  4   5000  23 05 53
23 08 08  ---          02 16 16  28.5 -34.4  5.7      77.4   135   R  1   3200

23 08 36  J2022+61     02 16 44  27.3 -32.3  5.9      75.4    19   2  4   3200  23 08 36
23 09 36  ---          02 17 44  27.1 -32.3  5.9      75.2    60   R  1   2400

23 10 04  SN2004ET     02 18 12  28.3 -34.3  5.7      77.0    20   2  4   2400  23 10 04
23 13 04  ---          02 21 13  27.9 -34.2  5.8      76.4   180   R  1      0

23 13 44  J2022+61     02 21 53  26.7 -32.1  6.0      74.3    31   2  5      0  23 13 44
23 14 29  ---          02 22 38  26.6 -32.1  6.0      74.2    45   F  1    600

23 14 57  SN2004ET     02 23 06  27.7 -34.2  5.8      76.0    20   2  5    600  23 14 57
23 17 12  ---          02 25 22  27.4 -34.1  5.8      75.6   135   F  1   2400

23 17 40  J2022+61     02 25 50  26.2 -32.0  6.1      73.5    20   2  5   2400  23 17 40
23 18 25  ---          02 26 35  26.1 -32.0  6.1      73.4    45   F  1   3000

23 18 53  SN2004ET     02 27 03  27.2 -34.0  5.9      75.3    20   2  5   3000  23 18 53
23 21 08  ---          02 29 18  27.0 -34.0  5.9      74.8   135   F  1   4800

23 21 37  J2022+61     02 29 47  25.8 -31.8  6.1      72.7    20   2  5   4800  23 21 37
23 22 22  ---          02 30 32  25.7 -31.8  6.1      72.6    45   F  1   5400

23 22 50  SN2004ET     02 31 00  26.8 -33.9  5.9      74.5    20   2  5   5400  23 22 50
23 25 05  ---          02 33 16  26.5 -33.8  6.0      74.0   135   F  1   7200

23 25 33  J2022+61     02 33 44  25.3 -31.7  6.2      71.9    20   2  5   7200  23 25 33
23 26 18  ---          02 34 29  25.2 -31.6  6.2      71.8    45   F  1   7800

23 26 46  SN2004ET     02 34 57  26.3 -33.7  6.0      73.7    20   2  5   7800  23 26 46
23 29 01  ---          02 37 13  26.0 -33.6  6.0      73.2   135   F  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  20 Feb 2005   Day  51 ---

23 29 30  J2022+61     02 37 41  24.9 -31.5  6.3      71.1    20   2  5   9600  23 29 30
23 30 15  ---          02 38 27  24.8 -31.5  6.3      71.0    45   F  1  10200

23 30 43  SN2004ET     02 38 55  25.8 -33.6  6.1      72.9    20   2  5  10200  23 30 43
23 32 58  ---          02 41 10  25.5 -33.5  6.1      72.4   135   F  1  12000

23 33 27  J2022+61     02 41 39  24.4 -31.3  6.3      70.3    20   2  5  12000  23 33 27
23 34 12  ---          02 42 24  24.3 -31.3  6.3      70.2    45   F  1  12600

23 34 40  SN2004ET     02 42 52  25.3 -33.4  6.1      72.1    20   2  5  12600  23 34 40
23 36 55  ---          02 45 08  25.1 -33.3  6.2      71.6   135   F  1  14400

23 37 22  J2035+58     02 45 35  24.5 -35.1  6.2      70.8    20   2  5  14400  23 37 22
23 38 22  ---          02 46 35  24.3 -35.1  6.2      70.6    60   F  1  15200

23 40 22  SN2004ET     02 48 36  24.7 -33.2  6.2      71.0   113   2  5  15200  23 40 22
23 43 22  ---          02 51 36  24.3 -33.0  6.3      70.4   180   F  1  17600

23 44 02  J2022+61     02 52 16  23.3 -30.8  6.5      68.2    32   2  6  17600  23 44 02
23 44 47  ---          02 53 01  23.2 -30.8  6.5      68.0    45   R  1  17000

23 45 16  SN2004ET     02 53 30  24.1 -32.9  6.3      70.0    21   2  6  17000  23 45 16
23 47 31  ---          02 55 45  23.8 -32.8  6.3      69.5   135   R  1  15200

23 48 00  J2022+61     02 56 14  22.8 -30.7  6.6      67.4    21   2  6  15200  23 48 00
23 48 45  ---          02 56 59  22.7 -30.6  6.6      67.2    45   R  1  14600

23 49 13  SN2004ET     02 57 28  23.6 -32.8  6.4      69.2    21   2  6  14600  23 49 13
23 51 28  ---          02 59 43  23.4 -32.6  6.4      68.8   135   R  1  12800

23 51 57  J2022+61     03 00 12  22.4 -30.5  6.6      66.6    21   2  6  12800  23 51 57
23 52 42  ---          03 00 57  22.3 -30.4  6.6      66.4    45   R  1  12200

23 53 11  SN2004ET     03 01 26  23.2 -32.6  6.4      68.4    21   2  6  12200  23 53 11
23 55 26  ---          03 03 42  22.9 -32.4  6.5      68.0   135   R  1  10400

23 55 55  J2022+61     03 04 11  22.0 -30.2  6.7      65.8    21   2  6  10400  23 55 55
23 56 40  ---          03 04 56  21.9 -30.2  6.7      65.6    45   R  1   9800

23 57 08  SN2004ET     03 05 24  22.7 -32.4  6.5      67.6    21   2  6   9800  23 57 08
23 59 23  ---          03 07 40  22.5 -32.2  6.5      67.2   135   R  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Start: Sun  20 Feb 2005   Day  51 -- Stop: Mon  21 Feb 2005   Day  52 ---

23 59 52  J2022+61     03 08 09  21.5 -30.0  6.8      65.0    21   2  6   8000  23 59 52
00 00 37  ---          03 08 54  21.4 -30.0  6.8      64.9    45   R  1   7400

00 01 06  SN2004ET     03 09 23  22.3 -32.2  6.6      66.9    21   2  6   7400  00 01 06
00 03 21  ---          03 11 38  22.0 -32.0  6.6      66.4   135   R  1   5600

00 03 50  J2022+61     03 12 07  21.1 -29.8  6.8      64.2    21   2  6   5600  00 03 50
00 04 35  ---          03 12 52  21.0 -29.8  6.8      64.1    45   R  1   5000

00 05 04  SN2004ET     03 13 21  21.8 -31.9  6.6      66.1    21   2  6   5000  00 05 04
00 07 19  ---          03 15 37  21.5 -31.8  6.7      65.6   135   R  1   3200

00 07 48  J2022+61     03 16 06  20.7 -29.6  6.9      63.4    21   2  6   3200  00 07 48
00 08 48  ---          03 17 06  20.6 -29.5  6.9      63.2    60   R  1   2400

00 09 17  SN2004ET     03 17 35  21.3 -31.7  6.7      65.2    21   2  6   2400  00 09 17
00 12 17  ---          03 20 35  21.0 -31.5  6.8      64.7   180   R  1      0

00 12 57  J2022+61     03 21 16  20.1 -29.3  7.0      62.4    32   2  7      0  00 12 57
00 13 42  ---          03 22 01  20.0 -29.3  7.0      62.2    45   F  1    600

00 14 11  SN2004ET     03 22 30  20.8 -31.4  6.8      64.3    22   2  7    600  00 14 11
00 16 26  ---          03 24 45  20.5 -31.3  6.8      63.8   135   F  1   2400

00 16 55  J2022+61     03 25 14  19.7 -29.1  7.1      61.6    22   2  7   2400  00 16 55
00 17 40  ---          03 25 59  19.6 -29.0  7.1      61.4    45   F  1   3000

00 18 09  SN2004ET     03 26 29  20.3 -31.2  6.8      63.5    22   2  7   3000  00 18 09
00 20 24  ---          03 28 44  20.1 -31.1  6.9      63.1   135   F  1   4800

00 20 53  J2022+61     03 29 13  19.3 -28.8  7.1      60.8    22   2  7   4800  00 20 53
00 21 38  ---          03 29 58  19.2 -28.8  7.1      60.6    45   F  1   5400

00 22 07  SN2004ET     03 30 27  19.9 -31.0  6.9      62.7    22   2  7   5400  00 22 07
00 24 22  ---          03 32 43  19.6 -30.8  7.0      62.3   135   F  1   7200

00 24 52  J2022+61     03 33 12  18.9 -28.6  7.2      60.0    22   2  7   7200  00 24 52
00 25 37  ---          03 33 57  18.8 -28.5  7.2      59.8    45   F  1   7800

00 26 06  SN2004ET     03 34 27  19.4 -30.7  7.0      61.9    22   2  7   7800  00 26 06
00 28 21  ---          03 36 42  19.2 -30.6  7.0      61.5   135   F  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon  21 Feb 2005   Day  52 ---

00 28 50  J2022+61     03 37 11  18.5 -28.3  7.3      59.2    22   2  7   9600  00 28 50
00 29 35  ---          03 37 56  18.4 -28.3  7.3      59.1    45   F  1  10200

00 30 04  SN2004ET     03 38 26  19.0 -30.5  7.0      61.2    22   2  7  10200  00 30 04
00 32 19  ---          03 40 41  18.8 -30.3  7.1      60.7   135   F  1  12000

00 32 49  J2022+61     03 41 10  18.1 -28.1  7.3      58.4    22   2  7  12000  00 32 49
00 33 34  ---          03 41 56  18.0 -28.0  7.3      58.3    45   F  1  12600

00 34 03  SN2004ET     03 42 25  18.6 -30.2  7.1      60.4    22   2  7  12600  00 34 03
00 36 18  ---          03 44 40  18.3 -30.1  7.2      59.9   135   F  1  14400

00 36 44  J2035+58     03 45 07  17.4 -31.6  7.2      59.4    19   2  7  14400  00 36 44
00 37 44  ---          03 46 07  17.3 -31.6  7.2      59.2    60   F  1  15200

00 38 11  SN2004ET     03 46 34  18.1 -29.9  7.2      59.6    19   2  7  15200  00 38 11
00 41 11  ---          03 49 35  17.8 -29.7  7.2      59.0   180   F  1  17600

00 41 51  J2022+61     03 50 15  17.2 -27.5  7.5      56.6    33   2  8  17600  00 41 51
00 42 36  ---          03 51 00  17.1 -27.4  7.5      56.4    45   R  1  17000

00 43 06  SN2004ET     03 51 29  17.6 -29.6  7.3      58.6    22   2  8  17000  00 43 06
00 45 21  ---          03 53 45  17.4 -29.4  7.3      58.2   135   R  1  15200

00 45 50  J2022+61     03 54 14  16.8 -27.2  7.5      55.8    22   2  8  15200  00 45 50
00 46 35  ---          03 54 59  16.7 -27.1  7.5      55.6    45   R  1  14600

00 47 05  SN2004ET     03 55 29  17.2 -29.3  7.3      57.8    22   2  8  14600  00 47 05
00 49 20  ---          03 57 44  16.9 -29.2  7.4      57.4   135   R  1  12800

00 49 49  J2022+61     03 58 14  16.4 -26.9  7.6      55.0    22   2  8  12800  00 49 49
00 50 34  ---          03 58 59  16.3 -26.8  7.6      54.8    45   R  1  12200

00 51 03  SN2004ET     03 59 28  16.8 -29.0  7.4      57.0    22   2  8  12200  00 51 03
00 53 18  ---          04 01 44  16.5 -28.9  7.4      56.6   135   R  1  10400

00 53 48  J2022+61     04 02 13  16.0 -26.6  7.7      54.2    22   2  8  10400  00 53 48
00 54 33  ---          04 02 59  15.9 -26.6  7.7      54.0    45   R  1   9800

00 55 02  SN2004ET     04 03 28  16.3 -28.8  7.5      56.2    22   2  8   9800  00 55 02
00 57 17  ---          04 05 43  16.1 -28.6  7.5      55.8   135   R  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon  21 Feb 2005   Day  52 ---

00 57 47  J2022+61     04 06 13  15.6 -26.3  7.7      53.4    22   2  8   8000  00 57 47
00 58 32  ---          04 06 58  15.5 -26.3  7.7      53.3    45   R  1   7400

00 59 02  SN2004ET     04 07 28  15.9 -28.5  7.5      55.5    22   2  8   7400  00 59 02
01 01 17  ---          04 09 43  15.7 -28.3  7.6      55.0   135   R  1   5600

01 01 46  J2022+61     04 10 13  15.2 -26.0  7.8      52.6    22   2  8   5600  01 01 46
01 02 31  ---          04 10 58  15.2 -26.0  7.8      52.4    45   R  1   5000

01 03 01  SN2004ET     04 11 28  15.5 -28.2  7.6      54.7    22   2  8   5000  01 03 01
01 05 16  ---          04 13 43  15.3 -28.0  7.6      54.2   135   R  1   3200

01 05 45  J2022+61     04 14 13  14.9 -25.7  7.9      51.8    22   2  8   3200  01 05 45
01 06 45  ---          04 15 13  14.8 -25.6  7.9      51.6    60   R  1   2400

01 07 15  SN2004ET     04 15 42  15.1 -27.9  7.7      53.8    22   2  8   2400  01 07 15
01 10 15  ---          04 18 43  14.8 -27.6  7.7      53.2   180   R  1      0

01 10 55  J2022+61     04 19 23  14.4 -25.3  8.0      50.8    32   2  9      0  01 10 55
01 11 40  ---          04 20 08  14.3 -25.3  8.0      50.6    45   F  1    600

01 12 09  SN2004ET     04 20 38  14.6 -27.5  7.8      52.9    22   2  9    600  01 12 09
01 14 24  ---          04 22 53  14.4 -27.3  7.8      52.4   135   F  1   2400

01 14 54  J2022+61     04 23 23  14.0 -25.0  8.0      50.0    22   2  9   2400  01 14 54
01 15 39  ---          04 24 08  13.9 -25.0  8.0      49.8    45   F  1   3000

01 16 09  SN2004ET     04 24 38  14.2 -27.2  7.8      52.1    22   2  9   3000  01 16 09
01 18 24  ---          04 26 53  14.0 -27.0  7.9      51.6   135   F  1   4800

01 18 54  J2022+61     04 27 23  13.6 -24.7  8.1      49.2    22   2  9   4800  01 18 54
01 19 39  ---          04 28 08  13.6 -24.6  8.1      49.0    45   F  1   5400

01 20 08  SN2004ET     04 28 38  13.8 -26.8  7.9      51.3    22   2  9   5400  01 20 08
01 22 23  ---          04 30 53  13.6 -26.7  7.9      50.8   135   F  1   7200

01 22 53  J2022+61     04 31 23  13.3 -24.4  8.2      48.3    22   2  9   7200  01 22 53
01 23 38  ---          04 32 08  13.2 -24.3  8.2      48.2    45   F  1   7800

01 24 08  SN2004ET     04 32 38  13.4 -26.5  8.0      50.5    22   2  9   7800  01 24 08
01 26 23  ---          04 34 53  13.2 -26.3  8.0      50.0   135   F  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon  21 Feb 2005   Day  52 ---

01 26 53  J2022+61     04 35 23  12.9 -24.0  8.2      47.5    22   2  9   9600  01 26 53
01 27 38  ---          04 36 08  12.9 -24.0  8.2      47.4    45   F  1  10200

01 28 07  SN2004ET     04 36 38  13.0 -26.2  8.0      49.7    22   2  9  10200  01 28 07
01 30 22  ---          04 38 54  12.8 -26.0  8.1      49.3   135   F  1  12000

01 30 52  J2022+61     04 39 24  12.6 -23.7  8.3      46.7    22   2  9  12000  01 30 52
01 31 37  ---          04 40 09  12.5 -23.7  8.3      46.6    45   F  1  12600

01 32 07  SN2004ET     04 40 38  12.7 -25.9  8.1      48.9    22   2  9  12600  01 32 07
01 34 22  ---          04 42 54  12.5 -25.7  8.1      48.5   135   F  1  14400

01 34 48  J2035+58     04 43 20  11.2 -27.0  8.1      48.1    17   2  9  14400  01 34 48
01 35 48  ---          04 44 20  11.1 -26.9  8.1      47.9    60   F  1  15200

01 36 14  SN2004ET     04 44 46  12.3 -25.5  8.2      48.1    18   2  9  15200  01 36 14
01 39 14  ---          04 47 47  12.0 -25.3  8.2      47.5   180   F  1  17600

01 39 54  J2022+61     04 48 27  11.8 -22.9  8.4      44.9    32   2 10  17600  01 39 54
01 40 39  ---          04 49 12  11.8 -22.9  8.5      44.8    45   R  1  17000

01 41 08  SN2004ET     04 49 42  11.8 -25.1  8.2      47.1    22   2 10  17000  01 41 08
01 43 23  ---          04 51 57  11.6 -24.9  8.3      46.7   135   R  1  15200

01 43 53  J2022+61     04 52 27  11.5 -22.6  8.5      44.1    23   2 10  15200  01 43 53
01 44 38  ---          04 53 12  11.4 -22.5  8.5      43.9    45   R  1  14600

01 45 08  SN2004ET     04 53 42  11.5 -24.7  8.3      46.3    22   2 10  14600  01 45 08
01 47 23  ---          04 55 57  11.3 -24.5  8.3      45.9   135   R  1  12800

01 51 53  3C48         05 00 28  47.4 -72.8  3.4      79.1   192   2 10  12800  01 51 53
01 55 53  ---          05 04 29  46.5 -72.5  3.4      78.8   240   R  1   9600


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: GM059A.4cm
   Matches group v4cm_3 in /sched-2003/catalogs/freq.dat.2004sep27

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         L         U         L         U         L         U         L
   Pol.  =      RCP       RCP       RCP       RCP       RCP       RCP       RCP       RCP 
   BBC   =         1         2         2         3         3         4         4         5
   BBC SB=         U         L         U         L         U         L         U         L
   IF    =        B         B         B         B         B         B         B         B 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    8383.49   8399.49   8399.49   8415.49   8415.49   8431.49   8431.49   8447.49
   BBC fr=     783.49    799.49    799.49    815.49    815.49    831.49    831.49    847.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510  6510  6510  6510  6510
    PCALFR2=   490   490   490   490  6490  6490  6490  6490

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- SN1993J @ 6cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SN2004ET          20 34 21.958890   * 20 35 25.359900     20 35 28.650019 
                     59 56 50.95521    * 60 07 17.73500      60 08 04.85444 
                     From catalog imbedded in main SCHED input file.

 * J2035+58          20 34 14.260136   * 20 35 23.752100     20 35 27.823206 
                     58 10 52.22792    * 58 21 18.74600      58 22 05.77157 
                     From catalog imbedded in main SCHED input file.

 * J2022+61          20 21 13.300181   * 20 22 06.681700     20 22 08.911650 
                     61 27 18.15499    * 61 36 58.80400      61 37 40.12421 
                     From catalog imbedded in main SCHED input file.

 * 2007+777          20 07 20.430477   * 20 05 30.998800     20 05 12.920371 
                     77 43 58.12445    * 77 52 43.24900      77 53 17.98859 
                     From catalog imbedded in main SCHED input file.

 * 3C48              01 34 49.826399   * 01 37 41.299465     01 37 57.341525 
                     32 54 20.26003    * 33 09 35.13422      33 11 12.96540 
                     From catalog imbedded in main SCHED input file.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN2004ET            73.6
   J2035+58            72.1
   J2022+61            75.7
   2007+777            90.4
   3C48                64.8

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

