  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
 Exp. Code:  GB049B  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 02 July 2002                       

PI:       N. Bartel, M.P. Rupen                                           

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@polaris.phys.yorku.ca                                    
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 256-8-2-ul 18cm                                      

Notes:    Fringe finder  : J1407+28, J1642+39, J0927+39, 0954+658         
          Pol. Calibrator: 0954+658, J1407+28                             
          Amplitude check: 0954+658, J1407+28                             
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

 Next scan frequencies:  1659.49  1659.49  1659.49  1659.49  1675.49  1675.49
                         1675.49  1675.49
 Next BBC frequencies:    740.51   740.51   740.51   740.51   724.51   724.51
                          724.51   724.51
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

18 05 00  M81          04 11 10  29.8  24.3 -5.7     -81.5     0   1  1      0  18 05 00
18 08 00  ---          04 14 11  30.0  24.3 -5.7     -82.2   180   F  1   2400

18 08 00  SN1993J      04 14 11  30.0  24.4 -5.7     -82.2    -6   1  1   2400  18 08 00
18 10 00  ---          04 16 11  30.2  24.4 -5.7     -82.6   114   F  1   4000

18 10 00  M81          04 16 11  30.2  24.3 -5.7     -82.6    -6   1  1   4000  18 10 00
18 11 10  ---          04 17 21  30.3  24.4 -5.6     -82.9    64   F  1   4933

18 11 10  SN1993J      04 17 21  30.3  24.4 -5.6     -82.9    -6   1  1   4933  18 11 10
18 13 10  ---          04 19 22  30.5  24.4 -5.6     -83.3   114   F  1   6533

18 13 10  M81          04 19 22  30.5  24.4 -5.6     -83.3    -6   1  1   6533  18 13 10
18 14 20  ---          04 20 32  30.6  24.4 -5.6     -83.6    64   F  1   7467

18 14 20  SN1993J      04 20 32  30.6  24.4 -5.6     -83.6    -6   1  1   7467  18 14 20
18 16 20  ---          04 22 32  30.8  24.5 -5.6     -84.1   114   F  1   9067

18 16 20  M81          04 22 32  30.8  24.4 -5.6     -84.1    -6   1  1   9067  18 16 20
18 17 30  ---          04 23 42  30.9  24.4 -5.5     -84.3    64   F  1  10000

18 17 30  SN1993J      04 23 42  30.9  24.5 -5.5     -84.3    -6   1  1  10000  18 17 30
18 19 30  ---          04 25 43  31.1  24.5 -5.5     -84.8   114   F  1  11600

18 19 30  M81          04 25 43  31.1  24.4 -5.5     -84.8    -6   1  1  11600  18 19 30
18 20 40  ---          04 26 53  31.2  24.5 -5.5     -85.0    64   F  1  12533

18 20 40  SN1993J      04 26 53  31.2  24.5 -5.5     -85.1    -6   1  1  12533  18 20 40
18 22 40  ---          04 28 53  31.3  24.5 -5.4     -85.5   114   F  1  14133

18 22 40  M81          04 28 53  31.3  24.5 -5.5     -85.5    -6   1  1  14133  18 22 40
18 23 50  ---          04 30 03  31.4  24.5 -5.4     -85.8    64   F  1  15067

18 23 50  SN1993J      04 30 03  31.4  24.5 -5.4     -85.8    -6   1  1  15067  18 23 50
18 25 50  ---          04 32 04  31.6  24.6 -5.4     -86.2   114   F  1  16667
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

18 25 50  M81          04 32 04  31.6  24.5 -5.4     -86.2    -6   1  1  16667  18 25 50
18 27 00  ---          04 33 14  31.7  24.5 -5.4     -86.5    64   F  1  17600

18 31 00  J0927+39     04 37 15  31.4  60.3 -4.8     -74.1   210   1  2  17600  18 31 00
18 33 50  ---          04 40 05  32.0  60.5 -4.8     -74.5   170   R  1  15333

18 37 50  0954+658     04 44 06  32.2  28.7 -5.3     -86.1   213   1  2  15333  18 37 50
18 40 50  ---          04 47 06  32.5  28.7 -5.2     -86.7   180   R  1  12933

18 40 50  M81          04 47 06  33.0  24.6 -5.1     -89.7    -9   1  2  12933  18 40 50
18 43 30  ---          04 49 47  33.2  24.6 -5.1     -90.3   151   R  1  10800

18 43 30  SN1993J      04 49 47  33.2  24.6 -5.1     -90.3    -6   1  2  10800  18 43 30
18 45 30  ---          04 51 47  33.4  24.6 -5.1     -90.8   114   R  1   9200

18 45 30  M81          04 51 47  33.4  24.6 -5.1     -90.8    -6   1  2   9200  18 45 30
18 46 40  ---          04 52 57  33.5  24.5 -5.0     -91.1    64   R  1   8267

18 46 40  SN1993J      04 52 57  33.5  24.6 -5.0     -91.1    -6   1  2   8267  18 46 40
18 48 40  ---          04 54 58  33.7  24.6 -5.0     -91.6   114   R  1   6667

18 48 40  M81          04 54 58  33.7  24.5 -5.0     -91.6    -6   1  2   6667  18 48 40
18 49 50  ---          04 56 08  33.8  24.5 -5.0     -91.8    64   R  1   5733

18 49 50  SN1993J      04 56 08  33.8  24.6 -5.0     -91.8    -6   1  2   5733  18 49 50
18 51 50  ---          04 58 08  34.0  24.6 -5.0     -92.3   114   R  1   4133

18 51 50  M81          04 58 08  33.9  24.5 -5.0     -92.3    -6   1  2   4133  18 51 50
18 53 00  ---          04 59 18  34.1  24.5 -4.9     -92.6    64   R  1   3200

18 53 00  SN1993J      04 59 18  34.1  24.6 -4.9     -92.6    -6   1  2   3200  18 53 00
18 55 00  ---          05 01 19  34.2  24.6 -4.9     -93.1   114   R  1   1600

18 55 00  M81          05 01 19  34.2  24.5 -4.9     -93.1    -6   1  2   1600  18 55 00
18 56 10  ---          05 02 29  34.3  24.5 -4.9     -93.3    64   R  1    667

18 59 10  M81          05 05 29  34.6  24.5 -4.8     -94.0   173   1  3    667  18 59 10
19 01 20  ---          05 07 40  34.8  24.5 -4.8     -94.6   130   F  1   1067

19 01 20  SN1993J      05 07 40  34.8  24.5 -4.8     -94.6    -6   1  3   1067  19 01 20
19 03 20  ---          05 09 40  35.0  24.5 -4.8     -95.0   114   F  1   2667
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

19 03 20  M81          05 09 40  35.0  24.5 -4.8     -95.0    -6   1  3   2667  19 03 20
19 04 30  ---          05 10 50  35.1  24.4 -4.8     -95.3    64   F  1   3600

19 04 30  SN1993J      05 10 50  35.1  24.5 -4.7     -95.3    -6   1  3   3600  19 04 30
19 06 30  ---          05 12 50  35.3  24.5 -4.7     -95.8   114   F  1   5200

19 06 30  M81          05 12 50  35.3  24.4 -4.7     -95.8    -6   1  3   5200  19 06 30
19 07 40  ---          05 14 01  35.4  24.4 -4.7     -96.1    64   F  1   6133

19 07 40  SN1993J      05 14 01  35.4  24.5 -4.7     -96.1    -6   1  3   6133  19 07 40
19 09 40  ---          05 16 01  35.6  24.4 -4.7     -96.6   114   F  1   7733

19 09 40  M81          05 16 01  35.5  24.4 -4.7     -96.6    -6   1  3   7733  19 09 40
19 10 50  ---          05 17 11  35.6  24.4 -4.6     -96.8    64   F  1   8667

19 10 50  SN1993J      05 17 11  35.7  24.4 -4.6     -96.8    -6   1  3   8667  19 10 50
19 12 50  ---          05 19 11  35.8  24.4 -4.6     -97.3   114   F  1  10267

19 12 50  M81          05 19 11  35.8  24.3 -4.6     -97.3    -6   1  3  10267  19 12 50
19 14 00  ---          05 20 22  35.9  24.3 -4.6     -97.6    64   F  1  11200

19 14 00  SN1993J      05 20 22  35.9  24.4 -4.6     -97.6    -6   1  3  11200  19 14 00
19 16 00  ---          05 22 22  36.1  24.3 -4.6     -98.1   114   F  1  12800

19 16 00  M81          05 22 22  36.1  24.3 -4.6     -98.1    -6   1  3  12800  19 16 00
19 17 10  ---          05 23 32  36.2  24.3 -4.5     -98.4    64   F  1  13733

19 17 10  SN1993J      05 23 32  36.2  24.3 -4.5     -98.4    -6   1  3  13733  19 17 10
19 19 10  ---          05 25 33  36.4  24.3 -4.5     -98.9   114   F  1  15333

19 19 10  M81          05 25 33  36.4  24.2 -4.5     -98.9    -6   1  3  15333  19 19 10
19 20 20  ---          05 26 43  36.5  24.2 -4.5     -99.2    64   F  1  16267

19 23 20  M81          05 29 43  36.8  24.2 -4.4     -99.9   173   1  4  16267  19 23 20
19 25 30  ---          05 31 54  36.9  24.1 -4.4    -100.4   130   R  1  17200

19 25 30  SN1993J      05 31 54  37.0  24.2 -4.4    -100.4    -6   1  4  17200  19 25 30
19 27 30  ---          05 33 54  37.1  24.1 -4.4    -100.9   114   R  1  15600

19 27 30  M81          05 33 54  37.1  24.1 -4.4    -100.9    -6   1  4  15600  19 27 30
19 28 40  ---          05 35 04  37.2  24.1 -4.3    -101.2    64   R  1  14667
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

19 28 40  SN1993J      05 35 04  37.2  24.1 -4.3    -101.2    -6   1  4  14667  19 28 40
19 30 40  ---          05 37 04  37.4  24.1 -4.3    -101.7   114   R  1  13067

19 30 40  M81          05 37 04  37.4  24.0 -4.3    -101.7    -6   1  4  13067  19 30 40
19 31 50  ---          05 38 15  37.5  24.0 -4.3    -102.0    64   R  1  12133

19 31 50  SN1993J      05 38 15  37.5  24.0 -4.3    -102.0    -6   1  4  12133  19 31 50
19 33 50  ---          05 40 15  37.7  24.0 -4.3    -102.5   114   R  1  10533

19 33 50  M81          05 40 15  37.7  23.9 -4.3    -102.5    -6   1  4  10533  19 33 50
19 35 00  ---          05 41 25  37.8  23.9 -4.2    -102.8    64   R  1   9600

19 35 00  SN1993J      05 41 25  37.8  24.0 -4.2    -102.8    -6   1  4   9600  19 35 00
19 37 00  ---          05 43 25  38.0  23.9 -4.2    -103.3   114   R  1   8000

19 37 00  M81          05 43 25  38.0  23.9 -4.2    -103.3    -6   1  4   8000  19 37 00
19 38 10  ---          05 44 36  38.1  23.8 -4.2    -103.6    64   R  1   7067

19 38 10  SN1993J      05 44 36  38.1  23.9 -4.2    -103.6    -6   1  4   7067  19 38 10
19 40 10  ---          05 46 36  38.2  23.8 -4.2    -104.1   114   R  1   5467

19 40 10  M81          05 46 36  38.2  23.8 -4.2    -104.1    -6   1  4   5467  19 40 10
19 41 20  ---          05 47 46  38.3  23.7 -4.1    -104.4    64   R  1   4533

19 41 20  SN1993J      05 47 46  38.4  23.8 -4.1    -104.4    -6   1  4   4533  19 41 20
19 43 20  ---          05 49 46  38.5  23.7 -4.1    -104.9   114   R  1   2933

19 43 20  M81          05 49 46  38.5  23.7 -4.1    -104.9    -6   1  4   2933  19 43 20
19 44 30  ---          05 50 57  38.6  23.6 -4.1    -105.2    64   R  1   2000

19 47 30  M81          05 53 57  38.9  23.6 -4.0    -105.9   173   1  4   2000  19 47 30
19 49 40  ---          05 56 08  39.0  23.5 -4.0    -106.5   130   R  1    267

19 49 40  SN1993J      05 56 08  39.1  23.5 -4.0    -106.5    -6   1  5    267  19 49 40
19 51 40  ---          05 58 08  39.2  23.5 -4.0    -107.0   114   F  1   1867

19 51 40  M81          05 58 08  39.2  23.4 -4.0    -107.0    -6   1  5   1867  19 51 40
19 52 50  ---          05 59 18  39.3  23.4 -3.9    -107.3    64   F  1   2800

19 52 50  SN1993J      05 59 18  39.3  23.4 -3.9    -107.3    -6   1  5   2800  19 52 50
19 54 50  ---          06 01 18  39.5  23.4 -3.9    -107.8   114   F  1   4400
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

19 54 50  M81          06 01 18  39.5  23.3 -3.9    -107.8    -6   1  5   4400  19 54 50
19 56 00  ---          06 02 29  39.6  23.3 -3.9    -108.1    64   F  1   5333

19 56 00  SN1993J      06 02 29  39.6  23.3 -3.9    -108.1    -6   1  5   5333  19 56 00
19 58 00  ---          06 04 29  39.8  23.2 -3.9    -108.6   114   F  1   6933

19 58 00  M81          06 04 29  39.8  23.2 -3.9    -108.6    -6   1  5   6933  19 58 00
19 59 10  ---          06 05 39  39.9  23.1 -3.8    -108.9    64   F  1   7867

19 59 10  SN1993J      06 05 39  39.9  23.2 -3.8    -108.9    -6   1  5   7867  19 59 10
20 01 10  ---          06 07 39  40.1  23.1 -3.8    -109.4   114   F  1   9467

20 01 10  M81          06 07 39  40.0  23.1 -3.8    -109.4    -6   1  5   9467  20 01 10
20 02 20  ---          06 08 50  40.1  23.0 -3.8    -109.7    64   F  1  10400

20 02 20  SN1993J      06 08 50  40.2  23.1 -3.8    -109.7    -6   1  5  10400  20 02 20
20 04 20  ---          06 10 50  40.3  23.0 -3.7    -110.3   114   F  1  12000

20 04 20  M81          06 10 50  40.3  22.9 -3.8    -110.3    -6   1  5  12000  20 04 20
20 05 30  ---          06 12 00  40.4  22.9 -3.7    -110.6    64   F  1  12933

20 05 30  SN1993J      06 12 00  40.4  22.9 -3.7    -110.6    -6   1  5  12933  20 05 30
20 07 30  ---          06 14 00  40.6  22.9 -3.7    -111.1   114   F  1  14533

20 07 30  M81          06 14 00  40.6  22.8 -3.7    -111.1    -6   1  5  14533  20 07 30
20 08 40  ---          06 15 11  40.7  22.8 -3.7    -111.4    64   F  1  15467

20 11 40  M81          06 18 11  40.9  22.6 -3.6    -112.2   174   1  5  15467  20 11 40
20 13 50  ---          06 20 22  41.1  22.5 -3.6    -112.7   130   F  1  17200

20 13 50  SN1993J      06 20 22  41.1  22.6 -3.6    -112.7    -6   1  6  17200  20 13 50
20 15 50  ---          06 22 22  41.3  22.5 -3.6    -113.3   114   R  1  15600

20 15 50  M81          06 22 22  41.3  22.4 -3.6    -113.3    -6   1  6  15600  20 15 50
20 17 00  ---          06 23 32  41.3  22.4 -3.5    -113.6    64   R  1  14667

20 17 00  SN1993J      06 23 32  41.4  22.4 -3.5    -113.6    -6   1  6  14667  20 17 00
20 19 00  ---          06 25 32  41.5  22.3 -3.5    -114.1   114   R  1  13067

20 19 00  M81          06 25 32  41.5  22.3 -3.5    -114.1    -6   1  6  13067  20 19 00
20 20 10  ---          06 26 43  41.6  22.2 -3.5    -114.4    64   R  1  12133
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

20 20 10  SN1993J      06 26 43  41.6  22.3 -3.5    -114.4    -6   1  6  12133  20 20 10
20 22 10  ---          06 28 43  41.8  22.2 -3.5    -115.0   114   R  1  10533

20 22 10  M81          06 28 43  41.8  22.1 -3.5    -115.0    -6   1  6  10533  20 22 10
20 23 20  ---          06 29 53  41.9  22.1 -3.4    -115.3    64   R  1   9600

20 23 20  SN1993J      06 29 53  41.9  22.1 -3.4    -115.3    -6   1  6   9600  20 23 20
20 25 20  ---          06 31 53  42.1  22.0 -3.4    -115.8   114   R  1   8000

20 25 20  M81          06 31 53  42.0  22.0 -3.4    -115.8    -6   1  6   8000  20 25 20
20 26 30  ---          06 33 04  42.1  21.9 -3.4    -116.1    64   R  1   7067

20 26 30  SN1993J      06 33 04  42.2  22.0 -3.4    -116.1    -6   1  6   7067  20 26 30
20 28 30  ---          06 35 04  42.3  21.8 -3.3    -116.7   114   R  1   5467

20 28 30  M81          06 35 04  42.3  21.8 -3.3    -116.7    -6   1  6   5467  20 28 30
20 29 40  ---          06 36 14  42.4  21.7 -3.3    -117.0    64   R  1   4533

20 29 40  SN1993J      06 36 14  42.4  21.8 -3.3    -117.0    -6   1  6   4533  20 29 40
20 31 40  ---          06 38 14  42.6  21.7 -3.3    -117.5   114   R  1   2933

20 31 40  M81          06 38 14  42.5  21.6 -3.3    -117.5    -6   1  6   2933  20 31 40
20 32 50  ---          06 39 25  42.6  21.6 -3.3    -117.8    64   R  1   2000

20 36 50  J0927+39     06 43 25  55.6  64.5 -2.7     -91.3   205   1  7   2000  20 36 50
20 39 40  ---          06 46 16  56.2  64.5 -2.7     -91.8   170   F  1    267

20 43 40  0954+658     06 50 16  44.9  25.4 -3.1    -117.0   208   1  7    267  20 43 40
20 46 40  ---          06 53 17  45.2  25.2 -3.1    -117.8   180   F  1   2667

20 46 40  M81          06 53 17  43.7  20.7 -3.0    -121.7    -9   1  7   2667  20 46 40
20 49 20  ---          06 55 57  43.9  20.5 -3.0    -122.4   151   F  1   4800

20 49 20  SN1993J      06 55 57  43.9  20.6 -3.0    -122.4    -6   1  7   4800  20 49 20
20 51 20  ---          06 57 58  44.1  20.4 -3.0    -123.0   114   F  1   6400

20 51 20  M81          06 57 58  44.1  20.4 -3.0    -123.0    -6   1  7   6400  20 51 20
20 52 30  ---          06 59 08  44.1  20.3 -2.9    -123.3    64   F  1   7333

20 52 30  SN1993J      06 59 08  44.2  20.4 -2.9    -123.3    -6   1  7   7333  20 52 30
20 54 30  ---          07 01 08  44.3  20.2 -2.9    -123.9   114   F  1   8933
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

20 54 30  M81          07 01 08  44.3  20.2 -2.9    -123.9    -6   1  7   8933  20 54 30
20 55 40  ---          07 02 18  44.4  20.1 -2.9    -124.2    64   F  1   9867

20 55 40  SN1993J      07 02 18  44.4  20.1 -2.9    -124.2    -6   1  7   9867  20 55 40
20 57 40  ---          07 04 19  44.6  20.0 -2.9    -124.8   114   F  1  11467

20 57 40  M81          07 04 19  44.5  20.0 -2.9    -124.8    -6   1  7  11467  20 57 40
20 58 50  ---          07 05 29  44.6  19.9 -2.8    -125.1    64   F  1  12400

20 58 50  SN1993J      07 05 29  44.6  19.9 -2.8    -125.1    -6   1  7  12400  20 58 50
21 00 50  ---          07 07 29  44.8  19.8 -2.8    -125.7   114   F  1  14000

21 00 50  M81          07 07 29  44.8  19.7 -2.8    -125.7    -6   1  7  14000  21 00 50
21 02 00  ---          07 08 39  44.8  19.6 -2.8    -126.0    64   F  1  14933

21 05 00  M81          07 11 40  45.1  19.4 -2.7    -126.9   174   1  7  14933  21 05 00
21 07 10  ---          07 13 50  45.2  19.3 -2.7    -127.5   130   F  1  16667

21 07 10  SN1993J      07 13 50  45.3  19.3 -2.7    -127.5    -6   1  8  16667  21 07 10
21 09 10  ---          07 15 51  45.4  19.1 -2.7    -128.1   114   R  1  16933

21 09 10  M81          07 15 51  45.4  19.1 -2.7    -128.1    -6   1  8  16933  21 09 10
21 10 20  ---          07 17 01  45.4  19.0 -2.6    -128.4    64   R  1  16000

21 10 20  SN1993J      07 17 01  45.5  19.0 -2.6    -128.4    -6   1  8  16000  21 10 20
21 12 20  ---          07 19 01  45.6  18.9 -2.6    -129.0   114   R  1  14400

21 12 20  M81          07 19 01  45.6  18.8 -2.6    -129.0    -6   1  8  14400  21 12 20
21 13 30  ---          07 20 11  45.7  18.7 -2.6    -129.3    64   R  1  13467

21 13 30  SN1993J      07 20 11  45.7  18.8 -2.6    -129.3    -6   1  8  13467  21 13 30
21 15 30  ---          07 22 12  45.8  18.6 -2.6    -129.9   114   R  1  11867

21 15 30  M81          07 22 12  45.8  18.6 -2.6    -129.9    -6   1  8  11867  21 15 30
21 16 40  ---          07 23 22  45.9  18.5 -2.5    -130.3    64   R  1  10933

21 16 40  SN1993J      07 23 22  45.9  18.5 -2.5    -130.3    -6   1  8  10933  21 16 40
21 18 40  ---          07 25 22  46.1  18.4 -2.5    -130.9   114   R  1   9333

21 18 40  M81          07 25 22  46.0  18.3 -2.5    -130.8    -6   1  8   9333  21 18 40
21 19 50  ---          07 26 32  46.1  18.2 -2.5    -131.2    64   R  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

21 19 50  SN1993J      07 26 32  46.1  18.3 -2.5    -131.2    -6   1  8   8400  21 19 50
21 21 50  ---          07 28 33  46.3  18.1 -2.5    -131.8   114   R  1   6800

21 21 50  M81          07 28 33  46.2  18.1 -2.5    -131.8    -6   1  8   6800  21 21 50
21 23 00  ---          07 29 43  46.3  17.9 -2.4    -132.1    64   R  1   5867

21 23 00  SN1993J      07 29 43  46.3  18.0 -2.4    -132.1    -6   1  8   5867  21 23 00
21 25 00  ---          07 31 43  46.5  17.8 -2.4    -132.7   114   R  1   4267

21 25 00  M81          07 31 43  46.4  17.8 -2.4    -132.7    -6   1  8   4267  21 25 00
21 26 10  ---          07 32 53  46.5  17.7 -2.4    -133.1    64   R  1   3333

21 29 10  M81          07 35 54  46.7  17.4 -2.3    -134.0   174   1  8   3333  21 29 10
21 31 20  ---          07 38 04  46.8  17.2 -2.3    -134.6   130   R  1   1600

21 31 20  SN1993J      07 38 04  46.9  17.2 -2.3    -134.6    -6   1  8   1600  21 31 20
21 33 20  ---          07 40 05  47.0  17.1 -2.3    -135.2   114   R  1      0

21 33 20  M81          07 40 05  47.0  17.0 -2.3    -135.2    -6   1  9      0  21 33 20
21 34 30  ---          07 41 15  47.0  16.9 -2.2    -135.6    64   F  1    933

21 34 30  SN1993J      07 41 15  47.1  16.9 -2.2    -135.6    -6   1  9    933  21 34 30
21 36 30  ---          07 43 15  47.2  16.8 -2.2    -136.2   114   F  1   2533

21 36 30  M81          07 43 15  47.2  16.7 -2.2    -136.2    -6   1  9   2533  21 36 30
21 37 40  ---          07 44 25  47.2  16.6 -2.2    -136.5    64   F  1   3467

21 37 40  SN1993J      07 44 25  47.3  16.6 -2.2    -136.5    -6   1  9   3467  21 37 40
21 39 40  ---          07 46 26  47.4  16.4 -2.2    -137.2   114   F  1   5067

21 39 40  M81          07 46 26  47.4  16.4 -2.2    -137.1    -6   1  9   5067  21 39 40
21 40 50  ---          07 47 36  47.4  16.3 -2.1    -137.5    64   F  1   6000

21 40 50  SN1993J      07 47 36  47.5  16.3 -2.1    -137.5    -6   1  9   6000  21 40 50
21 42 50  ---          07 49 36  47.6  16.1 -2.1    -138.1   114   F  1   7600

21 42 50  M81          07 49 36  47.6  16.1 -2.1    -138.1    -6   1  9   7600  21 42 50
21 44 00  ---          07 50 46  47.6  16.0 -2.1    -138.5    64   F  1   8533

21 44 00  SN1993J      07 50 46  47.7  16.0 -2.1    -138.5    -6   1  9   8533  21 44 00
21 46 00  ---          07 52 47  47.8  15.8 -2.0    -139.1   114   F  1  10133
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

21 46 00  M81          07 52 47  47.7  15.8 -2.1    -139.1    -6   1  9  10133  21 46 00
21 47 10  ---          07 53 57  47.8  15.7 -2.0    -139.5    64   F  1  11067

21 47 10  SN1993J      07 53 57  47.9  15.7 -2.0    -139.5    -6   1  9  11067  21 47 10
21 49 10  ---          07 55 57  48.0  15.5 -2.0    -140.1   114   F  1  12667

21 49 10  M81          07 55 57  47.9  15.5 -2.0    -140.1    -6   1  9  12667  21 49 10
21 50 20  ---          07 57 07  48.0  15.3 -2.0    -140.4    64   F  1  13600

21 53 20  M81          08 00 08  48.2  15.0 -1.9    -141.4   174   1  9  13600  21 53 20
21 55 30  ---          08 02 18  48.3  14.8 -1.9    -142.0   130   F  1  15333

21 55 30  SN1993J      08 02 18  48.3  14.8 -1.9    -142.1    -6   1  9  15333  21 55 30
21 57 30  ---          08 04 19  48.4  14.6 -1.9    -142.7   114   F  1  16933

21 57 30  M81          08 04 19  48.4  14.6 -1.9    -142.7    -6   1 10  16933  21 57 30
21 58 40  ---          08 05 29  48.5  14.5 -1.8    -143.0    64   R  1  17333

21 58 40  SN1993J      08 05 29  48.5  14.5 -1.8    -143.1    -6   1 10  17333  21 58 40
22 00 40  ---          08 07 29  48.6  14.3 -1.8    -143.7   114   R  1  15733

22 00 40  M81          08 07 29  48.6  14.2 -1.8    -143.7    -6   1 10  15733  22 00 40
22 01 50  ---          08 08 39  48.6  14.1 -1.8    -144.0    64   R  1  14800

22 01 50  SN1993J      08 08 39  48.7  14.1 -1.8    -144.1    -6   1 10  14800  22 01 50
22 03 50  ---          08 10 40  48.8  13.9 -1.8    -144.7   114   R  1  13200

22 03 50  M81          08 10 40  48.7  13.9 -1.8    -144.7    -6   1 10  13200  22 03 50
22 05 00  ---          08 11 50  48.8  13.8 -1.7    -145.0    64   R  1  12267

22 05 00  SN1993J      08 11 50  48.8  13.8 -1.7    -145.1    -6   1 10  12267  22 05 00
22 07 00  ---          08 13 50  48.9  13.6 -1.7    -145.7   114   R  1  10667

22 07 00  M81          08 13 50  48.9  13.5 -1.7    -145.7    -6   1 10  10667  22 07 00
22 08 10  ---          08 15 00  49.0  13.4 -1.7    -146.1    64   R  1   9733

22 08 10  SN1993J      08 15 00  49.0  13.4 -1.7    -146.1    -6   1 10   9733  22 08 10
22 10 10  ---          08 17 01  49.1  13.2 -1.6    -146.7   114   R  1   8133

22 10 10  M81          08 17 01  49.1  13.2 -1.6    -146.7    -6   1 10   8133  22 10 10
22 11 20  ---          08 18 11  49.1  13.1 -1.6    -147.1    64   R  1   7200
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

22 11 20  SN1993J      08 18 11  49.2  13.1 -1.6    -147.1    -6   1 10   7200  22 11 20
22 13 20  ---          08 20 11  49.3  12.8 -1.6    -147.7   114   R  1   5600

22 13 20  M81          08 20 11  49.2  12.8 -1.6    -147.7    -6   1 10   5600  22 13 20
22 14 30  ---          08 21 21  49.3  12.7 -1.6    -148.1    64   R  1   4667

22 17 30  M81          08 24 22  49.4  12.3 -1.5    -149.1   174   1 10   4667  22 17 30
22 19 40  ---          08 26 32  49.5  12.1 -1.5    -149.8   130   R  1   2933

22 19 40  SN1993J      08 26 32  49.5  12.1 -1.5    -149.8    -6   1 10   2933  22 19 40
22 21 40  ---          08 28 33  49.6  11.9 -1.5    -150.4   114   R  1   1333

22 21 40  M81          08 28 33  49.6  11.8 -1.5    -150.4    -6   1 10   1333  22 21 40
22 22 50  ---          08 29 43  49.6  11.7 -1.4    -150.8    64   R  1    400

22 22 50  SN1993J      08 29 43  49.7  11.7 -1.4    -150.8    -6   1 11    400  22 22 50
22 24 50  ---          08 31 43  49.8  11.5 -1.4    -151.5   114   F  1   2000

22 24 50  M81          08 31 43  49.7  11.5 -1.4    -151.4    -6   1 11   2000  22 24 50
22 26 00  ---          08 32 53  49.8  11.3 -1.4    -151.8    64   F  1   2933

22 26 00  SN1993J      08 32 53  49.8  11.3 -1.4    -151.8    -6   1 11   2933  22 26 00
22 28 00  ---          08 34 54  49.9  11.1 -1.3    -152.5   114   F  1   4533

22 28 00  M81          08 34 54  49.9  11.1 -1.3    -152.5    -6   1 11   4533  22 28 00
22 29 10  ---          08 36 04  49.9  10.9 -1.3    -152.9    64   F  1   5467

22 29 10  SN1993J      08 36 04  50.0  10.9 -1.3    -152.9    -6   1 11   5467  22 29 10
22 31 10  ---          08 38 04  50.0  10.7 -1.3    -153.5   114   F  1   7067

22 31 10  M81          08 38 04  50.0  10.7 -1.3    -153.5    -6   1 11   7067  22 31 10
22 32 20  ---          08 39 14  50.0  10.5 -1.3    -153.9    64   F  1   8000

22 32 20  SN1993J      08 39 14  50.1  10.5 -1.3    -153.9    -6   1 11   8000  22 32 20
22 34 20  ---          08 41 15  50.2  10.3 -1.2    -154.6   114   F  1   9600

22 34 20  M81          08 41 15  50.1  10.3 -1.2    -154.6    -6   1 11   9600  22 34 20
22 35 30  ---          08 42 25  50.2  10.1 -1.2    -155.0    64   F  1  10533

22 35 30  SN1993J      08 42 25  50.2  10.1 -1.2    -155.0    -6   1 11  10533  22 35 30
22 37 30  ---          08 44 25  50.3   9.9 -1.2    -155.6   114   F  1  12133
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

22 37 30  M81          08 44 25  50.2   9.9 -1.2    -155.6    -6   1 11  12133  22 37 30
22 38 40  ---          08 45 35  50.3   9.7 -1.2    -156.0    64   F  1  13067

22 41 40  M81          08 48 36  50.4   9.3 -1.1    -157.0   174   1 11  13067  22 41 40
22 43 50  ---          08 50 46  50.5   9.1 -1.1    -157.7   130   F  1  14800

22 43 50  SN1993J      08 50 46  50.5   9.1 -1.1    -157.8    -6   1 11  14800  22 43 50
22 45 50  ---          08 52 46  50.6   8.8 -1.0    -158.4   114   F  1  16400

22 45 50  M81          08 52 46  50.5   8.8 -1.1    -158.4    -6   1 11  16400  22 45 50
22 47 00  ---          08 53 57  50.6   8.6 -1.0    -158.8    64   F  1  17333

22 47 00  SN1993J      08 53 57  50.6   8.7 -1.0    -158.8    -6   1 12  17333  22 47 00
22 49 00  ---          08 55 57  50.7   8.4 -1.0    -159.5   114   R  1  15733

22 49 00  M81          08 55 57  50.6   8.4 -1.0    -159.5    -6   1 12  15733  22 49 00
22 50 10  ---          08 57 07  50.7   8.2 -1.0    -159.9    64   R  1  14800

22 50 10  SN1993J      08 57 07  50.7   8.2 -1.0    -159.9    -6   1 12  14800  22 50 10
22 52 10  ---          08 59 08  50.8   8.0 -0.9    -160.6   114   R  1  13200

22 52 10  M81          08 59 08  50.7   8.0 -0.9    -160.5    -6   1 12  13200  22 52 10
22 53 20  ---          09 00 18  50.8   7.8 -0.9    -160.9    64   R  1  12267

22 53 20  SN1993J      09 00 18  50.8   7.8 -0.9    -161.0    -6   1 12  12267  22 53 20
22 55 20  ---          09 02 18  50.9   7.5 -0.9    -161.6   114   R  1  10667

22 55 20  M81          09 02 18  50.8   7.5 -0.9    -161.6    -6   1 12  10667  22 55 20
22 56 30  ---          09 03 28  50.9   7.4 -0.9    -162.0    64   R  1   9733

22 56 30  SN1993J      09 03 28  50.9   7.4 -0.9    -162.0    -6   1 12   9733  22 56 30
22 58 30  ---          09 05 29  51.0   7.1 -0.8    -162.7   114   R  1   8133

22 58 30  M81          09 05 29  50.9   7.1 -0.8    -162.7    -6   1 12   8133  22 58 30
22 59 40  ---          09 06 39  50.9   6.9 -0.8    -163.1    64   R  1   7200

22 59 40  SN1993J      09 06 39  51.0   7.0 -0.8    -163.1    -6   1 12   7200  22 59 40
23 01 40  ---          09 08 39  51.0   6.7 -0.8    -163.8   114   R  1   5600

23 01 40  M81          09 08 39  51.0   6.7 -0.8    -163.8    -6   1 12   5600  23 01 40
23 02 50  ---          09 09 49  51.0   6.5 -0.8    -164.2    64   R  1   4667
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

23 05 50  M81          09 12 50  51.1   6.1 -0.7    -165.2   174   1 12   4667  23 05 50
23 08 00  ---          09 15 00  51.1   5.8 -0.7    -165.9   130   R  1   2933

23 08 00  SN1993J      09 15 00  51.2   5.8 -0.7    -165.9    -6   1 12   2933  23 08 00
23 10 00  ---          09 17 00  51.2   5.5 -0.6    -166.6   114   R  1   1333

23 10 00  M81          09 17 00  51.2   5.5 -0.6    -166.6    -6   1 12   1333  23 10 00
23 11 10  ---          09 18 11  51.2   5.4 -0.6    -167.0    64   R  1    400

23 11 10  SN1993J      09 18 11  51.2   5.4 -0.6    -167.0    -6   1 13    400  23 11 10
23 13 10  ---          09 20 11  51.3   5.1 -0.6    -167.7   114   F  1   2000

23 13 10  M81          09 20 11  51.2   5.1 -0.6    -167.7    -6   1 13   2000  23 13 10
23 14 20  ---          09 21 21  51.3   4.9 -0.6    -168.1    64   F  1   2933

23 14 20  SN1993J      09 21 21  51.3   4.9 -0.6    -168.1    -6   1 13   2933  23 14 20
23 16 20  ---          09 23 21  51.3   4.6 -0.5    -168.8   114   F  1   4533

23 16 20  M81          09 23 21  51.3   4.6 -0.5    -168.8    -6   1 13   4533  23 16 20
23 17 30  ---          09 24 32  51.3   4.5 -0.5    -169.2    64   F  1   5467

23 17 30  SN1993J      09 24 32  51.4   4.5 -0.5    -169.2    -6   1 13   5467  23 17 30
23 19 30  ---          09 26 32  51.4   4.2 -0.5    -169.9   114   F  1   7067

23 19 30  M81          09 26 32  51.4   4.2 -0.5    -169.9    -6   1 13   7067  23 19 30
23 20 40  ---          09 27 42  51.4   4.0 -0.5    -170.3    64   F  1   8000

23 20 40  SN1993J      09 27 42  51.4   4.0 -0.5    -170.3    -6   1 13   8000  23 20 40
23 22 40  ---          09 29 43  51.4   3.7 -0.4    -171.0   114   F  1   9600

23 22 40  M81          09 29 43  51.4   3.7 -0.4    -171.0    -6   1 13   9600  23 22 40
23 23 50  ---          09 30 53  51.4   3.6 -0.4    -171.4    64   F  1  10533

23 23 50  SN1993J      09 30 53  51.5   3.6 -0.4    -171.4    -6   1 13  10533  23 23 50
23 25 50  ---          09 32 53  51.5   3.3 -0.4    -172.1   114   F  1  12133

23 25 50  M81          09 32 53  51.4   3.3 -0.4    -172.0    -6   1 13  12133  23 25 50
23 27 00  ---          09 34 03  51.5   3.1 -0.4    -172.5    64   F  1  13067

23 30 00  M81          09 37 04  51.5   2.7 -0.3    -173.5   174   1 13  13067  23 30 00
23 32 10  ---          09 39 14  51.5   2.4 -0.3    -174.2   130   F  1  14800
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Jun 2004   Day 158 ---

23 32 10  SN1993J      09 39 14  51.6   2.4 -0.3    -174.3    -6   1 13  14800  23 32 10
23 34 10  ---          09 41 14  51.6   2.1 -0.2    -175.0   114   F  1  16400

23 34 10  M81          09 41 14  51.5   2.1 -0.2    -174.9    -6   1 13  16400  23 34 10
23 35 20  ---          09 42 25  51.5   1.9 -0.2    -175.3    64   F  1  17333

23 35 20  SN1993J      09 42 25  51.6   1.9 -0.2    -175.4    -6   1 14  17333  23 35 20
23 37 20  ---          09 44 25  51.6   1.6 -0.2    -176.1   114   R  1  15733

23 37 20  M81          09 44 25  51.5   1.6 -0.2    -176.0    -6   1 14  15733  23 37 20
23 38 30  ---          09 45 35  51.6   1.5 -0.2    -176.4    64   R  1  14800

23 38 30  SN1993J      09 45 35  51.6   1.5 -0.2    -176.5    -6   1 14  14800  23 38 30
23 40 30  ---          09 47 35  51.6   1.2 -0.1    -177.2   114   R  1  13200

23 40 30  M81          09 47 35  51.6   1.2 -0.1    -177.1    -6   1 14  13200  23 40 30
23 41 40  ---          09 48 46  51.6   1.0 -0.1    -177.5    64   R  1  12267

23 41 40  SN1993J      09 48 46  51.6   1.0 -0.1    -177.6    -6   1 14  12267  23 41 40
23 43 40  ---          09 50 46  51.6   0.7 -0.1    -178.3   114   R  1  10667

23 43 40  M81          09 50 46  51.6   0.7 -0.1    -178.2    -6   1 14  10667  23 43 40
23 44 50  ---          09 51 56  51.6   0.6 -0.1    -178.6    64   R  1   9733

23 44 50  SN1993J      09 51 56  51.6   0.6 -0.1    -178.7    -6   1 14   9733  23 44 50
23 46 50  ---          09 53 56  51.6   0.3  0.0    -179.4   114   R  1   8133

23 46 50  M81          09 53 56  51.6   0.3  0.0    -179.3    -6   1 14   8133  23 46 50
23 48 00  ---          09 55 07  51.6   0.1  0.0    -179.7    64   R  1   7200

23 48 00  SN1993J      09 55 07  51.6   0.1  0.0    -179.8    -6   1 14   7200  23 48 00
23 50 00  ---          09 57 07  51.6  -0.2  0.0     179.5   114   R  1   5600

23 50 00  M81          09 57 07  51.6  -0.2  0.0     179.6    -6   1 14   5600  23 50 00
23 51 10  ---          09 58 17  51.6  -0.3  0.0     179.2    64   R  1   4667

 --- Mon   7 Jun 2004   Day 159 ---

00 06 10  M81          10 13 20  51.5  -2.5  0.3     174.0   893   1 14   4667  00 06 10
00 08 20  ---          10 15 30  51.5  -2.8  0.3     173.2   130   R  1   2933

00 08 20  SN1993J      10 15 30  51.5  -2.8  0.3     173.2    -6   1 14   2933  00 08 20
00 10 20  ---          10 17 30  51.5  -3.1  0.4     172.5   114   R  1   1333
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

00 10 20  M81          10 17 30  51.5  -3.1  0.4     172.5    -6   1 14   1333  00 10 20
00 11 30  ---          10 18 41  51.4  -3.3  0.4     172.1    64   R  1    400

-----------  Tape Change ------------

00 11 30  SN1993J      10 18 41  51.5  -3.3  0.4     172.1    -6   2  1    400  00 11 30
00 13 30  ---          10 20 41  51.5  -3.6  0.4     171.4   114   F  1   2000

00 13 30  M81          10 20 41  51.4  -3.5  0.4     171.4    -6   2  1   2000  00 13 30
00 14 40  ---          10 21 51  51.4  -3.7  0.4     171.0    64   F  1   2933

00 14 40  SN1993J      10 21 51  51.4  -3.7  0.4     171.0    -6   2  1   2933  00 14 40
00 16 40  ---          10 23 51  51.4  -4.0  0.5     170.3   114   F  1   4533

00 16 40  M81          10 23 51  51.4  -4.0  0.5     170.3    -6   2  1   4533  00 16 40
00 17 50  ---          10 25 02  51.4  -4.2  0.5     169.9    64   F  1   5467

00 17 50  SN1993J      10 25 02  51.4  -4.2  0.5     169.9    -6   2  1   5467  00 17 50
00 19 50  ---          10 27 02  51.4  -4.5  0.5     169.2   114   F  1   7067

00 19 50  M81          10 27 02  51.3  -4.4  0.5     169.3    -6   2  1   7067  00 19 50
00 21 00  ---          10 28 12  51.3  -4.6  0.5     168.8    64   F  1   8000

00 21 00  SN1993J      10 28 12  51.3  -4.6  0.5     168.8    -6   2  1   8000  00 21 00
00 23 00  ---          10 30 12  51.3  -4.9  0.6     168.1   114   F  1   9600

00 23 00  M81          10 30 12  51.3  -4.9  0.6     168.2    -6   2  1   9600  00 23 00
00 24 10  ---          10 31 23  51.2  -5.1  0.6     167.8    64   F  1  10533

00 24 10  SN1993J      10 31 23  51.3  -5.1  0.6     167.7    -6   2  1  10533  00 24 10
00 26 10  ---          10 33 23  51.2  -5.4  0.6     167.0   114   F  1  12133

00 26 10  M81          10 33 23  51.2  -5.3  0.6     167.1    -6   2  1  12133  00 26 10
00 27 20  ---          10 34 33  51.2  -5.5  0.6     166.7    64   F  1  13067

00 30 20  M81          10 37 34  51.1  -5.9  0.7     165.6   174   2  1  13067  00 30 20
00 32 30  ---          10 39 44  51.1  -6.2  0.7     164.9   130   F  1  14800

00 32 30  SN1993J      10 39 44  51.1  -6.2  0.7     164.8    -6   2  1  14800  00 32 30
00 34 30  ---          10 41 44  51.1  -6.5  0.8     164.2   114   F  1  16400

00 34 30  M81          10 41 44  51.0  -6.5  0.8     164.2    -6   2  1  16400  00 34 30
00 35 40  ---          10 42 55  51.0  -6.6  0.8     163.8    64   F  1  17333
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

00 35 40  SN1993J      10 42 55  51.0  -6.7  0.8     163.8    -6   2  2  17333  00 35 40
00 37 40  ---          10 44 55  51.0  -7.0  0.8     163.1   114   R  1  15733

00 37 40  M81          10 44 55  50.9  -6.9  0.8     163.2    -6   2  2  15733  00 37 40
00 38 50  ---          10 46 05  50.9  -7.1  0.8     162.8    64   R  1  14800

00 38 50  SN1993J      10 46 05  51.0  -7.1  0.8     162.7    -6   2  2  14800  00 38 50
00 40 50  ---          10 48 05  50.9  -7.4  0.9     162.0   114   R  1  13200

00 40 50  M81          10 48 05  50.9  -7.3  0.9     162.1    -6   2  2  13200  00 40 50
00 42 00  ---          10 49 16  50.8  -7.5  0.9     161.7    64   R  1  12267

00 42 00  SN1993J      10 49 16  50.9  -7.5  0.9     161.6    -6   2  2  12267  00 42 00
00 44 00  ---          10 51 16  50.8  -7.8  0.9     160.9   114   R  1  10667

00 44 00  M81          10 51 16  50.8  -7.8  0.9     161.0    -6   2  2  10667  00 44 00
00 45 10  ---          10 52 26  50.7  -7.9  0.9     160.6    64   R  1   9733

00 45 10  SN1993J      10 52 26  50.8  -8.0  0.9     160.5    -6   2  2   9733  00 45 10
00 47 10  ---          10 54 26  50.7  -8.2  1.0     159.9   114   R  1   8133

00 47 10  M81          10 54 26  50.7  -8.2  1.0     159.9    -6   2  2   8133  00 47 10
00 48 20  ---          10 55 37  50.6  -8.4  1.0     159.5    64   R  1   7200

00 48 20  SN1993J      10 55 37  50.7  -8.4  1.0     159.5    -6   2  2   7200  00 48 20
00 50 20  ---          10 57 37  50.6  -8.7  1.0     158.8   114   R  1   5600

00 50 20  M81          10 57 37  50.6  -8.6  1.0     158.9    -6   2  2   5600  00 50 20
00 51 30  ---          10 58 47  50.5  -8.8  1.0     158.5    64   R  1   4667

00 59 30  J1407+28     11 06 48  51.0  81.5 -3.0     -75.4   414   2  2   4667  00 59 30
01 03 40  ---          11 10 59  51.8  81.8 -2.9     -75.6   250   R  1   1333

01 07 40  0954+658     11 15 00  53.2 -13.0  1.3     152.2   171   2  2   1333  01 07 40
01 09 20  ---          11 16 40  53.1 -13.2  1.3     151.6   100   R  1      0

01 09 20  M81          11 16 40  49.9 -11.0  1.3     152.6   -12   2  3      0  01 09 20
01 12 00  ---          11 19 20  49.8 -11.4  1.4     151.7   148   F  1   2133

01 12 00  SN1993J      11 19 20  49.8 -11.4  1.4     151.6    -6   2  3   2133  01 12 00
01 14 00  ---          11 21 21  49.7 -11.7  1.4     151.0   114   F  1   3733
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

01 14 00  M81          11 21 21  49.7 -11.6  1.4     151.0    -6   2  3   3733  01 14 00
01 15 10  ---          11 22 31  49.6 -11.8  1.4     150.6    64   F  1   4667

01 15 10  SN1993J      11 22 31  49.7 -11.8  1.4     150.6    -6   2  3   4667  01 15 10
01 17 10  ---          11 24 31  49.6 -12.0  1.5     149.9   114   F  1   6267

01 17 10  M81          11 24 31  49.5 -12.0  1.5     150.0    -6   2  3   6267  01 17 10
01 18 20  ---          11 25 42  49.5 -12.1  1.5     149.6    64   F  1   7200

01 18 20  SN1993J      11 25 42  49.5 -12.2  1.5     149.5    -6   2  3   7200  01 18 20
01 20 20  ---          11 27 42  49.4 -12.4  1.5     148.9   114   F  1   8800

01 20 20  M81          11 27 42  49.4 -12.4  1.5     149.0    -6   2  3   8800  01 20 20
01 21 30  ---          11 28 52  49.3 -12.5  1.5     148.6    64   F  1   9733

01 21 30  SN1993J      11 28 52  49.4 -12.6  1.6     148.5    -6   2  3   9733  01 21 30
01 23 30  ---          11 30 52  49.3 -12.8  1.6     147.9   114   F  1  11333

01 23 30  M81          11 30 52  49.2 -12.7  1.6     147.9    -6   2  3  11333  01 23 30
01 24 40  ---          11 32 03  49.2 -12.9  1.6     147.6    64   F  1  12267

01 27 40  M81          11 35 03  49.0 -13.2  1.7     146.6   174   2  3  12267  01 27 40
01 29 50  ---          11 37 13  48.9 -13.5  1.7     145.9   130   F  1  14000

01 29 50  SN1993J      11 37 13  49.0 -13.5  1.7     145.8    -6   2  3  14000  01 29 50
01 31 50  ---          11 39 14  48.9 -13.7  1.7     145.2   114   F  1  15600

01 31 50  M81          11 39 14  48.8 -13.7  1.7     145.3    -6   2  3  15600  01 31 50
01 33 00  ---          11 40 24  48.8 -13.8  1.7     144.9    64   F  1  16533

01 33 00  SN1993J      11 40 24  48.8 -13.9  1.7     144.8    -6   2  4  16533  01 33 00
01 35 00  ---          11 42 24  48.7 -14.1  1.8     144.2   114   R  1  17067

01 35 00  M81          11 42 24  48.7 -14.0  1.8     144.3    -6   2  4  17067  01 35 00
01 36 10  ---          11 43 34  48.6 -14.2  1.8     143.9    64   R  1  16133

01 36 10  SN1993J      11 43 34  48.6 -14.2  1.8     143.8    -6   2  4  16133  01 36 10
01 38 10  ---          11 45 35  48.5 -14.4  1.8     143.2   114   R  1  14533

01 38 10  M81          11 45 35  48.5 -14.4  1.8     143.3    -6   2  4  14533  01 38 10
01 39 20  ---          11 46 45  48.4 -14.5  1.8     142.9    64   R  1  13600
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

01 39 20  SN1993J      11 46 45  48.5 -14.6  1.8     142.8    -6   2  4  13600  01 39 20
01 41 20  ---          11 48 45  48.4 -14.8  1.9     142.2   114   R  1  12000

01 41 20  M81          11 48 45  48.3 -14.7  1.9     142.3    -6   2  4  12000  01 41 20
01 42 30  ---          11 49 55  48.3 -14.9  1.9     141.9    64   R  1  11067

01 42 30  SN1993J      11 49 55  48.3 -14.9  1.9     141.8    -6   2  4  11067  01 42 30
01 44 30  ---          11 51 56  48.2 -15.1  1.9     141.2   114   R  1   9467

01 44 30  M81          11 51 56  48.2 -15.1  1.9     141.3    -6   2  4   9467  01 44 30
01 45 40  ---          11 53 06  48.1 -15.2  2.0     140.9    64   R  1   8533

01 45 40  SN1993J      11 53 06  48.1 -15.2  2.0     140.8    -6   2  4   8533  01 45 40
01 47 40  ---          11 55 06  48.0 -15.5  2.0     140.2   114   R  1   6933

01 47 40  M81          11 55 06  48.0 -15.4  2.0     140.3    -6   2  4   6933  01 47 40
01 48 50  ---          11 56 17  47.9 -15.5  2.0     139.9    64   R  1   6000

01 51 50  M81          11 59 17  47.7 -15.8  2.1     139.0   174   2  4   6000  01 51 50
01 54 00  ---          12 01 27  47.6 -16.0  2.1     138.3   130   R  1   4267

01 54 00  SN1993J      12 01 27  47.6 -16.1  2.1     138.3    -6   2  4   4267  01 54 00
01 56 00  ---          12 03 28  47.5 -16.3  2.1     137.7   114   R  1   2667

01 56 00  M81          12 03 28  47.5 -16.2  2.1     137.7    -6   2  4   2667  01 56 00
01 57 10  ---          12 04 38  47.4 -16.3  2.1     137.4    64   R  1   1733

01 57 10  SN1993J      12 04 38  47.4 -16.4  2.1     137.3    -6   2  4   1733  01 57 10
01 59 10  ---          12 06 38  47.3 -16.6  2.2     136.7   114   R  1    133

01 59 10  M81          12 06 38  47.3 -16.5  2.2     136.8    -6   2  5    133  01 59 10
02 00 20  ---          12 07 48  47.2 -16.7  2.2     136.4    64   F  1   1067

02 00 20  SN1993J      12 07 48  47.2 -16.7  2.2     136.3    -6   2  5   1067  02 00 20
02 02 20  ---          12 09 49  47.1 -16.9  2.2     135.7   114   F  1   2667

02 02 20  M81          12 09 49  47.1 -16.8  2.2     135.8    -6   2  5   2667  02 02 20
02 03 30  ---          12 10 59  47.0 -17.0  2.3     135.4    64   F  1   3600

02 03 30  SN1993J      12 10 59  47.0 -17.0  2.3     135.4    -6   2  5   3600  02 03 30
02 05 30  ---          12 12 59  46.9 -17.2  2.3     134.8   114   F  1   5200
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

02 05 30  M81          12 12 59  46.9 -17.1  2.3     134.8    -6   2  5   5200  02 05 30
02 06 40  ---          12 14 09  46.8 -17.2  2.3     134.5    64   F  1   6133

02 06 40  SN1993J      12 14 09  46.8 -17.3  2.3     134.4    -6   2  5   6133  02 06 40
02 08 40  ---          12 16 10  46.7 -17.5  2.3     133.8   114   F  1   7733

02 08 40  M81          12 16 10  46.7 -17.4  2.3     133.9    -6   2  5   7733  02 08 40
02 09 50  ---          12 17 20  46.6 -17.5  2.4     133.5    64   F  1   8667

02 09 50  SN1993J      12 17 20  46.6 -17.6  2.4     133.5    -6   2  5   8667  02 09 50
02 11 50  ---          12 19 20  46.5 -17.8  2.4     132.9   114   F  1  10267

02 11 50  M81          12 19 20  46.5 -17.7  2.4     132.9    -6   2  5  10267  02 11 50
02 13 00  ---          12 20 31  46.4 -17.8  2.4     132.6    64   F  1  11200

02 16 00  M81          12 23 31  46.2 -18.1  2.5     131.7   174   2  5  11200  02 16 00
02 18 10  ---          12 25 41  46.1 -18.3  2.5     131.1   130   F  1  12933

02 18 10  SN1993J      12 25 41  46.1 -18.3  2.5     131.0    -6   2  5  12933  02 18 10
02 20 10  ---          12 27 42  45.9 -18.5  2.5     130.4   114   F  1  14533

02 20 10  M81          12 27 42  45.9 -18.4  2.5     130.5    -6   2  5  14533  02 20 10
02 21 20  ---          12 28 52  45.8 -18.5  2.5     130.1    64   F  1  15467

02 21 20  SN1993J      12 28 52  45.9 -18.6  2.6     130.1    -6   2  5  15467  02 21 20
02 23 20  ---          12 30 52  45.7 -18.8  2.6     129.5   114   F  1  17067

02 23 20  M81          12 30 52  45.7 -18.7  2.6     129.5    -6   2  6  17067  02 23 20
02 24 30  ---          12 32 02  45.6 -18.8  2.6     129.2    64   R  1  17200

02 24 30  SN1993J      12 32 02  45.6 -18.8  2.6     129.1    -6   2  6  17200  02 24 30
02 26 30  ---          12 34 03  45.5 -19.0  2.6     128.5   114   R  1  15600

02 26 30  M81          12 34 03  45.5 -18.9  2.6     128.6    -6   2  6  15600  02 26 30
02 27 40  ---          12 35 13  45.4 -19.0  2.7     128.3    64   R  1  14667

02 27 40  SN1993J      12 35 13  45.4 -19.1  2.7     128.2    -6   2  6  14667  02 27 40
02 29 40  ---          12 37 13  45.3 -19.3  2.7     127.6   114   R  1  13067

02 29 40  M81          12 37 13  45.3 -19.2  2.7     127.7    -6   2  6  13067  02 29 40
02 30 50  ---          12 38 23  45.2 -19.3  2.7     127.4    64   R  1  12133
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

02 30 50  SN1993J      12 38 23  45.2 -19.3  2.7     127.3    -6   2  6  12133  02 30 50
02 32 50  ---          12 40 24  45.1 -19.5  2.7     126.7   114   R  1  10533

02 32 50  M81          12 40 24  45.0 -19.4  2.7     126.8    -6   2  6  10533  02 32 50
02 34 00  ---          12 41 34  45.0 -19.5  2.8     126.4    64   R  1   9600

02 34 00  SN1993J      12 41 34  45.0 -19.6  2.8     126.4    -6   2  6   9600  02 34 00
02 36 00  ---          12 43 34  44.8 -19.7  2.8     125.8   114   R  1   8000

02 36 00  M81          12 43 34  44.8 -19.7  2.8     125.9    -6   2  6   8000  02 36 00
02 37 10  ---          12 44 44  44.7 -19.8  2.8     125.5    64   R  1   7067

02 40 10  M81          12 47 45  44.5 -20.0  2.9     124.7   174   2  6   7067  02 40 10
02 42 20  ---          12 49 55  44.3 -20.1  2.9     124.1   130   R  1   5333

02 42 20  SN1993J      12 49 55  44.4 -20.2  2.9     124.0    -6   2  6   5333  02 42 20
02 44 20  ---          12 51 56  44.2 -20.3  2.9     123.4   114   R  1   3733

02 44 20  M81          12 51 56  44.2 -20.3  2.9     123.5    -6   2  6   3733  02 44 20
02 45 30  ---          12 53 06  44.1 -20.4  3.0     123.2    64   R  1   2800

02 45 30  SN1993J      12 53 06  44.1 -20.4  3.0     123.1    -6   2  6   2800  02 45 30
02 47 30  ---          12 55 06  44.0 -20.5  3.0     122.5   114   R  1   1200

02 47 30  M81          12 55 06  44.0 -20.5  3.0     122.6    -6   2  6   1200  02 47 30
02 48 40  ---          12 56 16  43.9 -20.6  3.0     122.3    64   R  1    267

02 48 40  SN1993J      12 56 16  43.9 -20.6  3.0     122.2    -6   2  7    267  02 48 40
02 50 40  ---          12 58 17  43.7 -20.8  3.0     121.7   114   F  1   1867

02 50 40  M81          12 58 17  43.7 -20.7  3.0     121.7    -6   2  7   1867  02 50 40
02 51 50  ---          12 59 27  43.6 -20.8  3.1     121.4    64   F  1   2800

02 51 50  SN1993J      12 59 27  43.6 -20.8  3.1     121.3    -6   2  7   2800  02 51 50
02 53 50  ---          13 01 27  43.5 -21.0  3.1     120.8   114   F  1   4400

02 53 50  M81          13 01 27  43.5 -20.9  3.1     120.8    -6   2  7   4400  02 53 50
02 55 00  ---          13 02 37  43.4 -21.0  3.1     120.5    64   F  1   5333

02 55 00  SN1993J      13 02 37  43.4 -21.0  3.1     120.4    -6   2  7   5333  02 55 00
02 57 00  ---          13 04 38  43.2 -21.2  3.1     119.9   114   F  1   6933
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

02 57 00  M81          13 04 38  43.2 -21.1  3.1     120.0    -6   2  7   6933  02 57 00
02 58 10  ---          13 05 48  43.1 -21.2  3.2     119.6    64   F  1   7867

02 58 10  SN1993J      13 05 48  43.2 -21.2  3.2     119.6    -6   2  7   7867  02 58 10
03 00 10  ---          13 07 48  43.0 -21.4  3.2     119.0   114   F  1   9467

03 00 10  M81          13 07 48  43.0 -21.3  3.2     119.1    -6   2  7   9467  03 00 10
03 01 20  ---          13 08 58  42.9 -21.4  3.2     118.8    64   F  1  10400

03 04 20  0954+658     13 11 59  44.5 -25.6  3.2     115.9   171   2  7  10400  03 04 20
03 06 30  ---          13 14 09  44.3 -25.8  3.3     115.3   130   F  1  12133

03 06 30  M81          13 14 09  42.5 -21.7  3.3     117.4   -10   2  7  12133  03 06 30
03 09 40  ---          13 17 20  42.2 -21.8  3.4     116.5   180   F  1  14667

03 09 40  SN1993J      13 17 20  42.2 -21.9  3.4     116.4    -6   2  7  14667  03 09 40
03 11 40  ---          13 19 20  42.1 -22.0  3.4     115.9   114   F  1  16267

03 11 40  M81          13 19 20  42.1 -21.9  3.4     116.0    -6   2  7  16267  03 11 40
03 12 50  ---          13 20 30  42.0 -22.0  3.4     115.7    64   F  1  17200

03 12 50  SN1993J      13 20 30  42.0 -22.1  3.4     115.6    -6   2  8  17200  03 12 50
03 14 50  ---          13 22 31  41.8 -22.2  3.4     115.0   114   R  1  15600

03 14 50  M81          13 22 31  41.8 -22.1  3.4     115.1    -6   2  8  15600  03 14 50
03 16 00  ---          13 23 41  41.7 -22.2  3.5     114.8    64   R  1  14667

03 16 00  SN1993J      13 23 41  41.7 -22.2  3.5     114.7    -6   2  8  14667  03 16 00
03 18 00  ---          13 25 41  41.6 -22.3  3.5     114.2   114   R  1  13067

03 18 00  M81          13 25 41  41.6 -22.3  3.5     114.3    -6   2  8  13067  03 18 00
03 19 10  ---          13 26 51  41.5 -22.3  3.5     114.0    64   R  1  12133

03 19 10  SN1993J      13 26 51  41.5 -22.4  3.5     113.9    -6   2  8  12133  03 19 10
03 21 10  ---          13 28 52  41.3 -22.5  3.6     113.4   114   R  1  10533

03 21 10  M81          13 28 52  41.3 -22.4  3.5     113.4    -6   2  8  10533  03 21 10
03 22 20  ---          13 30 02  41.2 -22.5  3.6     113.1    64   R  1   9600

03 22 20  SN1993J      13 30 02  41.2 -22.5  3.6     113.0    -6   2  8   9600  03 22 20
03 24 20  ---          13 32 02  41.0 -22.6  3.6     112.5   114   R  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

03 24 20  M81          13 32 02  41.0 -22.6  3.6     112.6    -6   2  8   8000  03 24 20
03 25 30  ---          13 33 12  40.9 -22.6  3.6     112.3    64   R  1   7067

03 31 00  J1642+39     13 38 43  51.7  63.2 -3.1     -89.1   267   2  8   7067  03 31 00
03 35 10  ---          13 42 54  52.5  63.2 -3.0     -89.8   250   R  1   3733

03 40 10  0954+658     13 47 55  41.1 -27.5  3.8     106.4   234   2  8   3733  03 40 10
03 41 50  ---          13 49 35  40.9 -27.5  3.8     106.0   100   R  1   2400

03 41 50  M81          13 49 35  39.6 -23.3  3.9     108.0    -9   2  8   2400  03 41 50
03 44 30  ---          13 52 16  39.3 -23.4  3.9     107.3   151   R  1    267

03 44 30  SN1993J      13 52 16  39.3 -23.4  3.9     107.3    -6   2  9    267  03 44 30
03 46 30  ---          13 54 16  39.2 -23.5  4.0     106.8   114   F  1   1867

03 46 30  M81          13 54 16  39.2 -23.4  4.0     106.8    -6   2  9   1867  03 46 30
03 47 40  ---          13 55 26  39.1 -23.5  4.0     106.5    64   F  1   2800

03 47 40  SN1993J      13 55 26  39.1 -23.5  4.0     106.5    -6   2  9   2800  03 47 40
03 49 40  ---          13 57 26  38.9 -23.6  4.0     106.0   114   F  1   4400

03 49 40  M81          13 57 26  38.9 -23.5  4.0     106.0    -6   2  9   4400  03 49 40
03 50 50  ---          13 58 37  38.8 -23.6  4.0     105.7    64   F  1   5333

03 50 50  SN1993J      13 58 37  38.8 -23.6  4.0     105.7    -6   2  9   5333  03 50 50
03 52 50  ---          14 00 37  38.6 -23.7  4.1     105.2   114   F  1   6933

03 52 50  M81          14 00 37  38.6 -23.6  4.1     105.2    -6   2  9   6933  03 52 50
03 54 00  ---          14 01 47  38.5 -23.7  4.1     104.9    64   F  1   7867

03 54 00  SN1993J      14 01 47  38.5 -23.7  4.1     104.9    -6   2  9   7867  03 54 00
03 56 00  ---          14 03 47  38.3 -23.8  4.1     104.4   114   F  1   9467

03 56 00  M81          14 03 47  38.3 -23.7  4.1     104.4    -6   2  9   9467  03 56 00
03 57 10  ---          14 04 58  38.2 -23.8  4.2     104.1    64   F  1  10400

04 00 10  M81          14 07 58  38.0 -23.8  4.2     103.4   173   2  9  10400  04 00 10
04 02 20  ---          14 10 08  37.8 -23.9  4.2     102.8   130   F  1  12133

04 02 20  SN1993J      14 10 08  37.8 -24.0  4.2     102.8    -6   2  9  12133  04 02 20
04 04 20  ---          14 12 09  37.6 -24.0  4.3     102.3   114   F  1  13733
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

04 04 20  M81          14 12 09  37.6 -23.9  4.3     102.3    -6   2  9  13733  04 04 20
04 05 30  ---          14 13 19  37.5 -24.0  4.3     102.0    64   F  1  14667

04 05 30  SN1993J      14 13 19  37.5 -24.0  4.3     102.0    -6   2  9  14667  04 05 30
04 07 30  ---          14 15 19  37.3 -24.1  4.3     101.5   114   F  1  16267

04 07 30  M81          14 15 19  37.3 -24.0  4.3     101.6    -6   2  9  16267  04 07 30
04 08 40  ---          14 16 30  37.2 -24.0  4.3     101.3    64   F  1  17200

04 08 40  SN1993J      14 16 30  37.2 -24.1  4.3     101.2    -6   2 10  17200  04 08 40
04 10 40  ---          14 18 30  37.1 -24.2  4.4     100.7   114   R  1  15600

04 10 40  M81          14 18 30  37.1 -24.1  4.4     100.8    -6   2 10  15600  04 10 40
04 11 50  ---          14 19 40  37.0 -24.1  4.4     100.5    64   R  1  14667

04 11 50  SN1993J      14 19 40  37.0 -24.2  4.4     100.4    -6   2 10  14667  04 11 50
04 13 50  ---          14 21 40  36.8 -24.2  4.4      99.9   114   R  1  13067

04 13 50  M81          14 21 40  36.8 -24.2  4.4     100.0    -6   2 10  13067  04 13 50
04 15 00  ---          14 22 51  36.7 -24.2  4.4      99.7    64   R  1  12133

04 15 00  SN1993J      14 22 51  36.7 -24.2  4.5      99.6    -6   2 10  12133  04 15 00
04 17 00  ---          14 24 51  36.5 -24.3  4.5      99.1   114   R  1  10533

04 17 00  M81          14 24 51  36.5 -24.2  4.5      99.2    -6   2 10  10533  04 17 00
04 18 10  ---          14 26 01  36.4 -24.2  4.5      98.9    64   R  1   9600

04 18 10  SN1993J      14 26 01  36.4 -24.3  4.5      98.9    -6   2 10   9600  04 18 10
04 20 10  ---          14 28 01  36.2 -24.3  4.5      98.4   114   R  1   8000

04 20 10  M81          14 28 01  36.2 -24.3  4.5      98.4    -6   2 10   8000  04 20 10
04 21 20  ---          14 29 12  36.1 -24.3  4.6      98.2    64   R  1   7067

04 24 20  M81          14 32 12  35.9 -24.3  4.6      97.4   173   2 10   7067  04 24 20
04 26 30  ---          14 34 22  35.7 -24.4  4.6      96.9   130   R  1   5333

04 26 30  SN1993J      14 34 22  35.7 -24.4  4.6      96.8    -6   2 10   5333  04 26 30
04 28 30  ---          14 36 23  35.5 -24.4  4.7      96.4   114   R  1   3733

04 28 30  M81          14 36 23  35.5 -24.4  4.7      96.4    -6   2 10   3733  04 28 30
04 29 40  ---          14 37 33  35.4 -24.4  4.7      96.1    64   R  1   2800
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

04 29 40  SN1993J      14 37 33  35.4 -24.5  4.7      96.1    -6   2 10   2800  04 29 40
04 31 40  ---          14 39 33  35.2 -24.5  4.7      95.6   114   R  1   1200

04 31 40  M81          14 39 33  35.2 -24.4  4.7      95.7    -6   2 10   1200  04 31 40
04 32 50  ---          14 40 43  35.1 -24.4  4.7      95.4    64   R  1    267

04 32 50  SN1993J      14 40 43  35.1 -24.5  4.7      95.3    -6   2 11    267  04 32 50
04 34 50  ---          14 42 44  34.9 -24.5  4.8      94.8   114   F  1   1867

04 34 50  M81          14 42 44  34.9 -24.5  4.8      94.9    -6   2 11   1867  04 34 50
04 36 00  ---          14 43 54  34.8 -24.5  4.8      94.6    64   F  1   2800

04 36 00  SN1993J      14 43 54  34.8 -24.5  4.8      94.6    -6   2 11   2800  04 36 00
04 38 00  ---          14 45 54  34.6 -24.5  4.8      94.1   114   F  1   4400

04 38 00  M81          14 45 54  34.6 -24.5  4.8      94.1    -6   2 11   4400  04 38 00
04 39 10  ---          14 47 05  34.5 -24.5  4.9      93.9    64   F  1   5333

04 39 10  SN1993J      14 47 05  34.5 -24.5  4.9      93.8    -6   2 11   5333  04 39 10
04 41 10  ---          14 49 05  34.3 -24.6  4.9      93.3   114   F  1   6933

04 41 10  M81          14 49 05  34.4 -24.5  4.9      93.4    -6   2 11   6933  04 41 10
04 42 20  ---          14 50 15  34.2 -24.5  4.9      93.1    64   F  1   7867

04 42 20  SN1993J      14 50 15  34.2 -24.6  4.9      93.0    -6   2 11   7867  04 42 20
04 44 20  ---          14 52 15  34.1 -24.6  4.9      92.6   114   F  1   9467

04 44 20  M81          14 52 15  34.1 -24.5  4.9      92.6    -6   2 11   9467  04 44 20
04 45 30  ---          14 53 26  34.0 -24.5  5.0      92.4    64   F  1  10400

04 48 30  M81          14 56 26  33.7 -24.5  5.0      91.6   173   2 11  10400  04 48 30
04 50 40  ---          14 58 36  33.5 -24.5  5.0      91.1   130   F  1  12133

04 50 40  SN1993J      14 58 36  33.5 -24.6  5.0      91.1    -6   2 11  12133  04 50 40
04 52 40  ---          15 00 37  33.3 -24.6  5.1      90.6   114   F  1  13733

04 52 40  M81          15 00 37  33.3 -24.6  5.1      90.7    -6   2 11  13733  04 52 40
04 53 50  ---          15 01 47  33.2 -24.6  5.1      90.4    64   F  1  14667

04 53 50  SN1993J      15 01 47  33.2 -24.6  5.1      90.3    -6   2 11  14667  04 53 50
04 55 50  ---          15 03 47  33.0 -24.6  5.1      89.9   114   F  1  16267
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

04 55 50  M81          15 03 47  33.0 -24.6  5.1      89.9    -6   2 11  16267  04 55 50
04 57 00  ---          15 04 57  32.9 -24.6  5.2      89.7    64   F  1  17200

04 57 00  SN1993J      15 04 57  32.9 -24.6  5.2      89.6    -6   2 12  17200  04 57 00
04 59 00  ---          15 06 58  32.7 -24.6  5.2      89.1   114   R  1  15600

04 59 00  M81          15 06 58  32.8 -24.6  5.2      89.2    -6   2 12  15600  04 59 00
05 00 10  ---          15 08 08  32.7 -24.5  5.2      88.9    64   R  1  14667

05 00 10  SN1993J      15 08 08  32.6 -24.6  5.2      88.9    -6   2 12  14667  05 00 10
05 02 10  ---          15 10 08  32.5 -24.6  5.2      88.4   114   R  1  13067

05 02 10  M81          15 10 08  32.5 -24.5  5.2      88.4    -6   2 12  13067  05 02 10
05 03 20  ---          15 11 18  32.4 -24.5  5.3      88.2    64   R  1  12133

05 03 20  SN1993J      15 11 18  32.4 -24.6  5.3      88.1    -6   2 12  12133  05 03 20
05 05 20  ---          15 13 19  32.2 -24.6  5.3      87.7   114   R  1  10533

05 05 20  M81          15 13 19  32.2 -24.5  5.3      87.7    -6   2 12  10533  05 05 20
05 06 30  ---          15 14 29  32.1 -24.5  5.3      87.4    64   R  1   9600

05 06 30  SN1993J      15 14 29  32.1 -24.6  5.3      87.4    -6   2 12   9600  05 06 30
05 08 30  ---          15 16 29  31.9 -24.6  5.3      86.9   114   R  1   8000

05 08 30  M81          15 16 29  31.9 -24.5  5.3      87.0    -6   2 12   8000  05 08 30
05 09 40  ---          15 17 40  31.8 -24.5  5.4      86.7    64   R  1   7067

05 12 40  0954+658     15 20 40  31.6 -28.6  5.4      84.6   171   2 12   7067  05 12 40
05 14 50  ---          15 22 50  31.3 -28.6  5.4      84.1   130   R  1   5333

05 14 50  M81          15 22 50  31.3 -24.5  5.4      85.5    -9   2 12   5333  05 14 50
05 18 00  ---          15 26 01  31.1 -24.4  5.5      84.8   181   R  1   2800

05 18 00  SN1993J      15 26 01  31.0 -24.5  5.5      84.7    -6   2 12   2800  05 18 00
05 20 00  ---          15 28 01  30.9 -24.5  5.5      84.3   114   R  1   1200

05 20 00  M81          15 28 01  30.9 -24.4  5.5      84.3    -6   2 12   1200  05 20 00
05 21 10  ---          15 29 11  30.8 -24.4  5.6      84.1    64   R  1    267

05 21 10  SN1993J      15 29 11  30.8 -24.5  5.6      84.0    -6   2 13    267  05 21 10
05 23 10  ---          15 31 12  30.6 -24.4  5.6      83.6   114   F  1   1867
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

05 23 10  M81          15 31 12  30.6 -24.4  5.6      83.6    -6   2 13   1867  05 23 10
05 24 20  ---          15 32 22  30.5 -24.4  5.6      83.3    64   F  1   2800

05 24 20  SN1993J      15 32 22  30.5 -24.4  5.6      83.3    -6   2 13   2800  05 24 20
05 26 20  ---          15 34 22  30.3 -24.4  5.6      82.8   114   F  1   4400

05 26 20  M81          15 34 22  30.3 -24.4  5.6      82.9    -6   2 13   4400  05 26 20
05 27 30  ---          15 35 32  30.2 -24.3  5.7      82.6    64   F  1   5333

05 27 30  SN1993J      15 35 32  30.2 -24.4  5.7      82.6    -6   2 13   5333  05 27 30
05 29 30  ---          15 37 33  30.0 -24.4  5.7      82.1   114   F  1   6933

05 29 30  M81          15 37 33  30.0 -24.3  5.7      82.2    -6   2 13   6933  05 29 30
05 30 40  ---          15 38 43  29.9 -24.3  5.7      81.9    64   F  1   7867

05 30 40  SN1993J      15 38 43  29.9 -24.3  5.7      81.8    -6   2 13   7867  05 30 40
05 32 40  ---          15 40 43  29.7 -24.3  5.7      81.4   114   F  1   9467

05 32 40  M81          15 40 43  29.8 -24.3  5.7      81.5    -6   2 13   9467  05 32 40
05 33 50  ---          15 41 53  29.6 -24.2  5.8      81.2    64   F  1  10400

05 36 50  M81          15 44 54  29.4 -24.2  5.8      80.5   173   2 13  10400  05 36 50
05 39 00  ---          15 47 04  29.2 -24.2  5.9      80.0   130   F  1  12133

05 39 00  SN1993J      15 47 04  29.2 -24.2  5.9      80.0    -6   2 13  12133  05 39 00
05 41 00  ---          15 49 05  29.0 -24.2  5.9      79.5   114   F  1  13733

05 41 00  M81          15 49 05  29.0 -24.1  5.9      79.6    -6   2 13  13733  05 41 00
05 42 10  ---          15 50 15  28.9 -24.1  5.9      79.3    64   F  1  14667

05 42 10  SN1993J      15 50 15  28.9 -24.1  5.9      79.3    -6   2 13  14667  05 42 10
05 44 10  ---          15 52 15  28.7 -24.1  5.9      78.8   114   F  1  16267

05 44 10  M81          15 52 15  28.7 -24.1  5.9      78.9    -6   2 13  16267  05 44 10
05 45 20  ---          15 53 25  28.6 -24.0  6.0      78.6    64   F  1  17200

05 45 20  SN1993J      15 53 25  28.6 -24.1  6.0      78.5    -6   2 14  17200  05 45 20
05 47 20  ---          15 55 26  28.4 -24.0  6.0      78.1   114   R  1  15600

05 47 20  M81          15 55 26  28.5 -24.0  6.0      78.1    -6   2 14  15600  05 47 20
05 48 30  ---          15 56 36  28.4 -24.0  6.0      77.9    64   R  1  14667
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Mon   7 Jun 2004   Day 159 ---

05 48 30  SN1993J      15 56 36  28.3 -24.0  6.0      77.8    -6   2 14  14667  05 48 30
05 50 30  ---          15 58 36  28.2 -24.0  6.0      77.4   114   R  1  13067

05 50 30  M81          15 58 36  28.2 -23.9  6.0      77.4    -6   2 14  13067  05 50 30
05 51 40  ---          15 59 46  28.1 -23.9  6.1      77.2    64   R  1  12133

05 51 40  SN1993J      15 59 46  28.1 -23.9  6.1      77.1    -6   2 14  12133  05 51 40
05 53 40  ---          16 01 47  27.9 -23.9  6.1      76.7   114   R  1  10533

05 53 40  M81          16 01 47  27.9 -23.9  6.1      76.7    -6   2 14  10533  05 53 40
05 54 50  ---          16 02 57  27.8 -23.8  6.1      76.5    64   R  1   9600

05 54 50  SN1993J      16 02 57  27.8 -23.9  6.1      76.4    -6   2 14   9600  05 54 50
05 56 50  ---          16 04 57  27.6 -23.8  6.2      76.0   114   R  1   8000

05 56 50  M81          16 04 57  27.6 -23.8  6.2      76.0    -6   2 14   8000  05 56 50
05 58 00  ---          16 06 07  27.5 -23.8  6.2      75.8    64   R  1   7067


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/sched.2002Jul02a/setups/v18cm-256-8-2-UL.set
   Matches group v20cm_2 in /usr/local/sched.2002Jul02a/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
   BBC SB=         U         U         L         L         U         U         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    1659.49   1659.49   1659.49   1659.49   1675.49   1675.49   1675.49   1675.49
   BBC fr=     740.51    740.51    740.51    740.51    724.51    724.51    724.51    724.51
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   510   490   510  6490  6510  6490  6510
    PCALFR2=   490   510   490   510  6490  6510  6490  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- 33th epoch of obs. of SN1993J in M81: VLBA/MkIV 18 pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SN1993J           09 51 19.038889   * 09 55 24.774900     09 55 45.128121 
                     69 15 26.46784    * 69 01 13.70300      69 00 21.88735 
                     From catalog imbedded in main SCHED input file.

 * M81               09 51 27.310854   * 09 55 33.173100     09 55 53.538842 
                     69 18 08.14534    * 69 03 55.06200      69 03 03.22660 
                     From catalog imbedded in main SCHED input file.

 * 0954+658          09 54 57.847119   * 09 58 47.244300     09 59 06.314627 
                     65 48 15.53178    * 65 33 54.81100      65 33 01.80804 
                     From catalog imbedded in main SCHED input file.

   J0927+3902        09 23 55.319195   * 09 27 03.013916     09 27 18.338573 
   0923+392          39 15 23.56655    * 39 02 20.85195      39 01 28.45120 
   4C39.25           /usr/local/sched.2002Jul02a/catalogs/sources.vlba
 * J0927+39          ICRF - Ext.1 Source - 1998 IERS Annual Report

   J1407+2827        14 04 45.615151   * 14 07 00.394410     14 07 13.018785 
   1404+286          28 41 29.23495    * 28 27 14.68998      28 26 04.50752 
 * J1407+28          /usr/local/sched.2002Jul02a/catalogs/sources.vlba
   OQ208             ICRF - Ext.1 Source - 1998 IERS Annual Report

   J1642+3948        16 41 17.606214   * 16 42 58.809952     16 43 09.189214 
   1641+399          39 54 10.81489    * 39 48 36.99395      39 48 02.88151 
   3C345             /usr/local/sched.2002Jul02a/catalogs/sources.vlba
 * J1642+39          ICRF - Ext.1 Source - 1998 IERS Annual Report



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1993J             62.9
   M81                 62.9
   0954+658            62.9
   J0927+39            58.0
   J1407+28           113.7
   J1642+39           117.3

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

