  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Radio AGN feedback
 Exp. Code:  GM081B  


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Suma Murthy

Address:  JIVE
          Oude Hoogeveensedijk 4
          7991 PD Dwingeloo
          The Netherlands

Phone:    +31 521 596 508
EMAIL:    murthy@jive.eu
Fax:
Phone during observation: +31 521 596 508

Observing mode: vlbi

Notes:    # Please, make sure PHASE CAL is OFF #
          v2: fixed (mixed-BW) tunings, line at 1292.50 with DOPINCR 250kHz
            line centered in USB of 2nd DBBC BBC per pol
 


COVER LETTER:


Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   1 Jun 2022   Day 152 ---

 Next scan frequencies:  1264.50  1264.50  1280.50  1280.50  1296.50  1296.50  1312.50  1312.50
 Next BBC frequencies:    835.50   835.50   819.50   819.50   803.50   803.50   787.50   787.50
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

22 00 00  J1407+2827   07 45 41   9.7  62.7 -6.4     -60.3     0        0   22 00 00
22 05 00  =OQ208       07 50 42  10.6  63.2 -6.3     -60.8   300       19   22 00 01

22 06 30  J1439+4958   07 52 12  15.9  40.9 -6.8     -61.0    66       19   22 06 30
22 08 30  ---          07 54 13  16.2  41.1 -6.8     -61.3   120       27   22 06 31

22 08 30  J1435+5051   07 54 13  17.2  40.6 -6.7     -62.3   -10       27   22 08 40
22 13 30  ---          07 59 13  17.9  41.0 -6.6     -63.2   290       46   22 08 31

22 14 00  J1439+4958   07 59 43  16.9  41.5 -6.7     -62.3    20       46   22 14 00
22 15 30  ---          08 01 14  17.2  41.6 -6.7     -62.5    90       52   22 14 01

22 15 30  J1435+5051   08 01 14  18.2  41.2 -6.6     -63.5   -10       52   22 15 40
22 20 30  ---          08 06 15  18.9  41.5 -6.5     -64.4   290       70   22 15 31

22 21 00  J1439+4958   08 06 45  17.9  42.1 -6.6     -63.5    20       70   22 21 00
22 22 30  ---          08 08 15  18.2  42.2 -6.5     -63.7    90       76   22 21 01

22 22 30  J1435+5051   08 08 15  19.2  41.7 -6.5     -64.7   -10       76   22 22 40
22 27 30  ---          08 13 16  19.9  42.0 -6.4     -65.6   290       95   22 22 31

22 28 00  J1439+4958   08 13 46  19.0  42.6 -6.4     -64.6    20       95   22 28 00
22 29 30  ---          08 15 16  19.2  42.7 -6.4     -64.9    90      100   22 28 01

22 29 30  J1435+5051   08 15 16  20.2  42.2 -6.3     -65.9   -10      100   22 29 40
22 34 30  ---          08 20 17  20.9  42.5 -6.3     -66.8   290      119   22 29 31

22 35 00  J1439+4958   08 20 47  20.0  43.1 -6.3     -65.8    20      119   22 35 00
22 36 30  ---          08 22 17  20.2  43.2 -6.3     -66.1    90      125   22 35 01

22 36 30  J1435+5051   08 22 17  21.2  42.6 -6.2     -67.1   -10      125   22 36 40
22 41 30  ---          08 27 18  21.9  43.0 -6.1     -68.0   290      144   22 36 31

22 42 00  J1439+4958   08 27 48  21.0  43.6 -6.2     -67.0    20      144   22 42 00
22 43 30  ---          08 29 18  21.2  43.7 -6.2     -67.2    90      149   22 42 01

22 43 30  J1435+5051   08 29 18  22.2  43.1 -6.1     -68.3   -10      149   22 43 40
22 48 30  ---          08 34 19  23.0  43.4 -6.0     -69.2   290      168   22 43 31

22 49 00  J1439+4958   08 34 49  22.1  44.0 -6.1     -68.1    20      168   22 49 00
22 50 30  ---          08 36 19  22.3  44.1 -6.1     -68.4    90      174   22 49 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   1 Jun 2022   Day 152 ---

22 50 30  J1435+5051   08 36 19  23.3  43.5 -6.0     -69.5   -10      174   22 50 40
22 55 30  ---          08 41 20  24.0  43.8 -5.9     -70.3   290      193   22 50 31

22 56 00  J1439+4958   08 41 50  23.1  44.5 -6.0     -69.3    20      193   22 56 00
22 57 30  ---          08 43 21  23.3  44.6 -6.0     -69.6    90      198   22 56 01

22 57 30  J1435+5051   08 43 21  24.3  43.9 -5.9     -70.7   -10      198   22 57 40
23 02 30  ---          08 48 21  25.1  44.2 -5.8     -71.5   290      217   22 57 31

23 03 00  J1439+4958   08 48 52  24.2  44.9 -5.9     -70.5    20      217   23 03 00
23 04 30  ---          08 50 22  24.4  45.0 -5.8     -70.7    90      223   23 03 01

23 04 30  J1435+5051   08 50 22  25.4  44.3 -5.8     -71.9   -10      223   23 04 40
23 09 30  ---          08 55 23  26.1  44.6 -5.7     -72.7   290      242   23 04 31

23 10 00  J1439+4958   08 55 53  25.3  45.3 -5.7     -71.7    20      242   23 10 00
23 11 30  ---          08 57 23  25.5  45.4 -5.7     -71.9    90      247   23 10 01

23 11 30  J1435+5051   08 57 23  26.4  44.7 -5.6     -73.1   -10      247   23 11 40
23 16 30  ---          09 02 24  27.2  44.9 -5.6     -73.9   290      266   23 11 31

23 17 00  J1439+4958   09 02 54  26.3  45.7 -5.6     -72.8    20      266   23 17 00
23 18 30  ---          09 04 24  26.6  45.8 -5.6     -73.1    90      272   23 17 01

23 18 30  J1435+5051   09 04 24  27.5  45.0 -5.5     -74.3   -10      272   23 18 40
23 23 30  ---          09 09 25  28.3  45.3 -5.4     -75.1   290      290   23 18 31

23 24 00  J1439+4958   09 09 55  27.4  46.1 -5.5     -74.0    20      290   23 24 00
23 25 30  ---          09 11 25  27.6  46.1 -5.5     -74.3    90      296   23 24 01

23 25 30  J1435+5051   09 11 25  28.6  45.4 -5.4     -75.5   -10      296   23 25 40
23 30 30  ---          09 16 26  29.3  45.6 -5.3     -76.3   290      315   23 25 31

23 31 00  J1439+4958   09 16 56  28.5  46.4 -5.4     -75.2    20      315   23 31 00
23 32 30  ---          09 18 26  28.7  46.5 -5.4     -75.5    90      321   23 31 01

23 32 30  J1435+5051   09 18 26  29.6  45.7 -5.3     -76.7   -10      321   23 32 40
23 37 30  ---          09 23 27  30.4  45.9 -5.2     -77.6   290      339   23 32 31

23 38 00  J1439+4958   09 23 57  29.6  46.7 -5.3     -76.4    20      339   23 38 00
23 39 30  ---          09 25 28  29.8  46.8 -5.3     -76.6    90      345   23 38 01

23 39 30  J1435+5051   09 25 28  30.7  46.0 -5.2     -77.9   -10      345   23 39 40
23 44 30  ---          09 30 28  31.5  46.1 -5.1     -78.8   290      364   23 39 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   1 Jun 2022   Day 152 ---

23 45 00  J1439+4958   09 30 58  30.7  47.0 -5.2     -77.6    20      364   23 45 00
23 46 30  ---          09 32 29  30.9  47.1 -5.1     -77.8    90      370   23 45 01

23 46 30  J1435+5051   09 32 29  31.8  46.2 -5.1     -79.1   -10      370   23 46 40
23 51 30  ---          09 37 29  32.6  46.4 -5.0     -80.0   290      388   23 46 31

23 52 00  J1439+4958   09 38 00  31.8  47.3 -5.0     -78.8    20      388   23 52 00
23 53 30  ---          09 39 30  32.0  47.3 -5.0     -79.0    90      394   23 52 01

23 53 30  J1435+5051   09 39 30  32.9  46.5 -4.9     -80.4   -10      394   23 53 40
23 58 30  ---          09 44 31  33.7  46.6 -4.9     -81.3   290      413   23 53 31

 --- Start: Wed   1 Jun 2022   Day 152 -- Stop: Thu   2 Jun 2022   Day 153 ---

23 59 00  J1439+4958   09 45 01  32.9  47.5 -4.9     -80.0    20      413   23 59 00
00 00 30  ---          09 46 31  33.2  47.6 -4.9     -80.3    90      419   23 59 01

00 00 30  J1435+5051   09 46 31  34.0  46.7 -4.8     -81.6   -10      419   00 00 40
00 05 30  ---          09 51 32  34.8  46.8 -4.7     -82.5   290      437   00 00 31

00 06 00  J1439+4958   09 52 02  34.0  47.7 -4.8     -81.2    20      437   00 06 00
00 07 30  ---          09 53 32  34.3  47.8 -4.8     -81.5    90      443   00 06 01

00 07 30  J1435+5051   09 53 32  35.1  46.8 -4.7     -82.9   -10      443   00 07 40
00 12 30  ---          09 58 33  35.9  47.0 -4.6     -83.8   290      462   00 07 31

00 13 00  J1439+4958   09 59 03  35.2  47.9 -4.7     -82.4    20      462   00 13 00
00 14 30  ---          10 00 33  35.4  48.0 -4.7     -82.7    90      468   00 13 01

00 16 00  J1407+2827   10 02 03  37.1  75.9 -4.1     -71.5    62      468   00 16 00
00 21 00  =OQ208       10 07 04  38.2  76.3 -4.0     -71.8   300      487   00 16 01

00 23 00  J1439+4958   10 09 05  36.8  48.2 -4.5     -84.2    92      487   00 23 00
00 25 30  ---          10 11 35  37.2  48.2 -4.5     -84.7   150      497   00 23 01

00 25 30  J1435+5051   10 11 35  37.9  47.2 -4.4     -86.2   -10      497   00 25 40
00 30 30  ---          10 16 36  38.7  47.2 -4.3     -87.1   290      515   00 25 31

00 31 00  J1439+4958   10 17 06  38.0  48.3 -4.4     -85.7    21      515   00 31 00
00 32 30  ---          10 18 36  38.3  48.3 -4.4     -85.9    90      521   00 31 01

00 32 30  J1435+5051   10 18 36  39.0  47.3 -4.3     -87.5    -9      521   00 32 39
00 37 30  ---          10 23 37  39.8  47.3 -4.2     -88.4   291      540   00 32 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

00 38 00  J1439+4958   10 24 07  39.2  48.4 -4.3     -87.0    21      540   00 38 00
00 39 30  ---          10 25 37  39.4  48.4 -4.2     -87.2    90      546   00 38 01

00 39 30  J1435+5051   10 25 37  40.2  47.3 -4.2     -88.8    -9      546   00 39 39
00 44 30  ---          10 30 38  40.9  47.3 -4.1     -89.8   291      564   00 39 31

00 45 00  J1439+4958   10 31 08  40.3  48.5 -4.2     -88.3    21      564   00 45 00
00 46 30  ---          10 32 39  40.5  48.5 -4.1     -88.5    90      570   00 45 01

00 46 30  J1435+5051   10 32 39  41.3  47.3 -4.1     -90.2    -9      570   00 46 39
00 51 30  ---          10 37 39  42.1  47.3 -4.0     -91.1   291      589   00 46 31

00 52 00  J1439+4958   10 38 09  41.4  48.5 -4.0     -89.6    21      589   00 52 00
00 53 30  ---          10 39 40  41.7  48.5 -4.0     -89.9    90      595   00 52 01

00 53 30  J1435+5051   10 39 40  42.4  47.3 -3.9     -91.5    -9      595   00 53 39
00 58 30  ---          10 44 40  43.2  47.3 -3.9     -92.5   291      613   00 53 31

00 59 00  J1439+4958   10 45 11  42.6  48.5 -3.9     -90.9    21      613   00 59 00
01 00 30  ---          10 46 41  42.8  48.5 -3.9     -91.2    90      619   00 59 01

01 00 30  J1435+5051   10 46 41  43.5  47.2 -3.8     -92.9    -9      619   01 00 39
01 05 30  ---          10 51 42  44.3  47.2 -3.7     -93.9   291      638   01 00 31

01 06 00  J1439+4958   10 52 12  43.7  48.5 -3.8     -92.3    21      638   01 06 00
01 07 30  ---          10 53 42  43.9  48.4 -3.8     -92.6    90      644   01 06 01

01 07 30  J1435+5051   10 53 42  44.6  47.1 -3.7     -94.4    -9      644   01 07 39
01 12 30  ---          10 58 43  45.4  47.0 -3.6     -95.4   291      663   01 07 31

01 13 00  J1439+4958   10 59 13  44.8  48.4 -3.7     -93.7    21      663   01 13 00
01 14 30  ---          11 00 43  45.1  48.3 -3.7     -94.0    90      668   01 13 01

01 14 30  J1435+5051   11 00 43  45.7  47.0 -3.6     -95.8    -9      668   01 14 39
01 19 30  ---          11 05 44  46.5  46.9 -3.5     -96.9   291      687   01 14 31

01 20 00  J1439+4958   11 06 14  46.0  48.2 -3.6     -95.1    21      687   01 20 00
01 21 30  ---          11 07 44  46.2  48.2 -3.5     -95.4    90      693   01 20 01

01 21 30  J1435+5051   11 07 44  46.8  46.8 -3.5     -97.3    -9      693   01 21 39
01 26 30  ---          11 12 45  47.6  46.7 -3.4     -98.4   291      712   01 21 31

01 27 00  J1439+4958   11 13 15  47.1  48.1 -3.5     -96.6    21      712   01 27 00
01 28 30  ---          11 14 45  47.3  48.0 -3.4     -96.9    90      717   01 27 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

01 28 30  J1435+5051   11 14 45  47.9  46.6 -3.4     -98.8    -9      717   01 28 39
01 33 30  ---          11 19 46  48.7  46.4 -3.3     -99.9   291      736   01 28 31

01 34 00  J1439+4958   11 20 16  48.2  47.9 -3.3     -98.1    21      736   01 34 00
01 35 30  ---          11 21 47  48.4  47.8 -3.3     -98.4    90      742   01 34 01

01 35 30  J1435+5051   11 21 47  49.0  46.3 -3.2    -100.4    -9      742   01 35 39
01 40 30  ---          11 26 47  49.8  46.1 -3.2    -101.5   291      761   01 35 31

01 41 00  J1439+4958   11 27 17  49.3  47.6 -3.2     -99.6    21      761   01 41 00
01 42 30  ---          11 28 48  49.6  47.5 -3.2    -100.0    90      766   01 41 01

01 42 30  J1435+5051   11 28 48  50.1  46.0 -3.1    -102.0    -9      766   01 42 39
01 47 30  ---          11 33 49  50.9  45.7 -3.0    -103.2   291      785   01 42 31

01 48 00  J1439+4958   11 34 19  50.4  47.3 -3.1    -101.2    21      785   01 48 00
01 49 30  ---          11 35 49  50.7  47.2 -3.1    -101.6    90      791   01 48 01

01 49 30  J1435+5051   11 35 49  51.2  45.6 -3.0    -103.7    -9      791   01 49 39
01 54 30  ---          11 40 50  51.9  45.3 -2.9    -104.9   291      810   01 49 31

01 55 00  J1439+4958   11 41 20  51.5  46.9 -3.0    -102.9    21      810   01 55 00
01 56 30  ---          11 42 50  51.8  46.8 -3.0    -103.2    90      816   01 55 01

01 56 30  J1435+5051   11 42 50  52.2  45.1 -2.9    -105.4    -9      816   01 56 39
02 01 30  ---          11 47 51  53.0  44.8 -2.8    -106.6   291      834   01 56 31

02 02 00  J1439+4958   11 48 21  52.6  46.5 -2.9    -104.5    21      834   02 02 00
02 03 30  ---          11 49 51  52.9  46.4 -2.8    -104.9    90      840   02 02 01

02 03 30  J1435+5051   11 49 51  53.3  44.6 -2.8    -107.2    -9      840   02 03 39
02 08 30  ---          11 54 52  54.1  44.2 -2.7    -108.5   291      859   02 03 31

02 09 00  J1439+4958   11 55 22  53.7  46.0 -2.8    -106.3    21      859   02 09 00
02 10 30  ---          11 56 52  54.0  45.9 -2.7    -106.7    90      865   02 09 01

02 10 30  J1435+5051   11 56 52  54.4  44.0 -2.7    -109.0    -9      865   02 10 39
02 15 30  ---          12 01 53  55.1  43.6 -2.6    -110.3   291      883   02 10 31

02 16 00  J1439+4958   12 02 23  54.8  45.4 -2.6    -108.1    21      883   02 16 00
02 17 30  ---          12 03 53  55.0  45.3 -2.6    -108.5    90      889   02 16 01

02 17 30  J1435+5051   12 03 53  55.4  43.4 -2.5    -110.9    -9      889   02 17 39
02 22 30  ---          12 08 54  56.1  42.9 -2.5    -112.3   291      908   02 17 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

02 23 00  J1439+4958   12 09 24  55.9  44.7 -2.5    -110.0    21      908   02 23 00
02 24 30  ---          12 10 55  56.1  44.6 -2.5    -110.4    90      914   02 23 01

02 24 30  J1435+5051   12 10 55  56.4  42.6 -2.4    -112.8    -9      914   02 24 39
02 29 30  ---          12 15 55  57.2  42.1 -2.3    -114.3   291      932   02 24 31

02 30 00  J1439+4958   12 16 26  56.9  44.0 -2.4    -111.9    21      932   02 30 00
02 31 30  ---          12 17 56  57.2  43.9 -2.4    -112.3    90      938   02 30 01

02 33 00  J1407+2827   12 19 26  66.3  88.6 -1.8     -77.8    50      938   02 33 00
02 38 00  =OQ208       12 24 27  67.4  89.2 -1.7     -77.9   300      958   02 33 01

02 40 00  J1439+4958   12 26 27  58.4  42.8 -2.2    -114.8    79      958   02 40 00
02 42 30  ---          12 28 58  58.8  42.5 -2.2    -115.6   150      967   02 40 01

02 42 30  J1435+5051   12 28 58  59.0  40.3 -2.1    -118.3    -9      967   02 42 39
02 47 30  ---          12 33 58  59.7  39.6 -2.0    -119.9   291      986   02 42 31

02 48 00  J1439+4958   12 34 28  59.6  41.7 -2.1    -117.3    21      986   02 48 00
02 49 30  ---          12 35 59  59.8  41.5 -2.1    -117.8    90      992   02 48 01

02 49 30  J1435+5051   12 35 59  60.0  39.3 -2.0    -120.6    -9      992   02 49 39
02 54 30  ---          12 41 00  60.7  38.4 -1.9    -122.3   291     1011   02 49 31

02 55 00  J1439+4958   12 41 30  60.6  40.6 -2.0    -119.6    21     1011   02 55 00
02 56 30  ---          12 43 00  60.8  40.4 -2.0    -120.1    90     1016   02 55 01

02 56 30  J1435+5051   12 43 00  60.9  38.1 -1.9    -123.0   -10     1016   02 56 40
03 01 30  ---          12 48 01  61.6  37.2 -1.8    -124.7   290     1035   02 56 31

03 02 00  J1439+4958   12 48 31  61.5  39.4 -1.9    -122.0    20     1035   03 02 00
03 03 30  ---          12 50 01  61.7  39.2 -1.8    -122.5    90     1041   03 02 01

03 03 30  J1435+5051   12 50 01  61.8  36.8 -1.8    -125.5   -10     1041   03 03 40
03 08 30  ---          12 55 02  62.5  35.8 -1.7    -127.3   290     1059   03 03 31

03 09 00  J1439+4958   12 55 32  62.5  38.1 -1.8    -124.5    20     1059   03 09 00
03 10 30  ---          12 57 02  62.7  37.8 -1.7    -125.1    90     1065   03 09 01

03 10 30  J1435+5051   12 57 02  62.7  35.3 -1.7    -128.1   -10     1065   03 10 40
03 15 30  ---          13 02 03  63.3  34.2 -1.6    -130.1   290     1084   03 10 31

03 16 00  J1439+4958   13 02 33  63.4  36.7 -1.6    -127.1    20     1084   03 16 00
03 17 30  ---          13 04 03  63.6  36.3 -1.6    -127.7    90     1090   03 16 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

03 17 30  J1435+5051   13 04 03  63.6  33.8 -1.5    -130.9   -10     1090   03 17 40
03 22 30  ---          13 09 04  64.2  32.6 -1.5    -132.9   290     1108   03 17 31

03 23 00  J1439+4958   13 09 34  64.3  35.1 -1.5    -129.9    20     1108   03 23 00
03 24 30  ---          13 11 04  64.5  34.7 -1.5    -130.5    90     1114   03 23 01

03 24 30  J1435+5051   13 11 04  64.4  32.1 -1.4    -133.7   -10     1114   03 24 40
03 29 30  ---          13 16 05  65.0  30.8 -1.3    -135.9   290     1133   03 24 31

03 30 00  J1439+4958   13 16 35  65.1  33.3 -1.4    -132.8    20     1133   03 30 00
03 31 30  ---          13 18 06  65.3  32.9 -1.4    -133.5    90     1139   03 30 01

03 31 30  J1435+5051   13 18 06  65.2  30.2 -1.3    -136.8   -10     1139   03 31 40
03 36 30  ---          13 23 06  65.7  28.8 -1.2    -139.0   290     1157   03 31 31

03 37 00  J1439+4958   13 23 37  65.9  31.4 -1.3    -135.9    20     1157   03 37 00
03 38 30  ---          13 25 07  66.1  31.0 -1.3    -136.6    90     1163   03 37 01

03 38 30  J1435+5051   13 25 07  65.9  28.2 -1.2    -140.0   -10     1163   03 38 40
03 43 30  ---          13 30 08  66.4  26.7 -1.1    -142.3   290     1182   03 38 31

03 44 00  J1439+4958   13 30 38  66.7  29.3 -1.2    -139.2    20     1182   03 44 00
03 45 30  ---          13 32 08  66.9  28.9 -1.1    -139.9    90     1188   03 44 01

03 45 30  J1435+5051   13 32 08  66.6  26.1 -1.1    -143.3   -10     1188   03 45 40
03 50 30  ---          13 37 09  67.1  24.4 -1.0    -145.8   290     1206   03 45 31

03 51 00  J1439+4958   13 37 39  67.4  27.1 -1.0    -142.6    20     1206   03 51 00
03 52 30  ---          13 39 09  67.6  26.6 -1.0    -143.3    90     1212   03 51 01

03 52 30  J1435+5051   13 39 09  67.2  23.7 -0.9    -146.8   -10     1212   03 52 40
03 58 00  ---          13 44 40  67.7  21.8 -0.9    -149.7   320     1233   03 52 31

03 58 00  J1439+4958   13 44 40  68.1  24.6 -0.9    -146.2   -10     1233   03 58 10
04 00 00  ---          13 46 40  68.3  23.9 -0.9    -147.2   110     1240   03 58 01

04 00 00  J1407+2827   13 46 40  84.8 114.9 -0.4     -62.5   -74     1240   04 01 14
04 05 00  =OQ208       13 51 41  85.8 121.7 -0.3     -56.3   226     1254   04 00 01

04 06 30  J1439+4958   13 53 11  68.8  21.5 -0.8    -150.8    11     1254   04 06 30
04 08 30  ---          13 55 12  69.0  20.7 -0.8    -151.9   120     1262   04 06 31

04 08 30  J1435+5051   13 55 12  68.5  17.8 -0.7    -155.4   -10     1262   04 08 40
04 13 30  ---          14 00 13  68.8  15.8 -0.6    -158.2   290     1281   04 08 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

04 14 00  J1439+4958   14 00 43  69.4  18.4 -0.7    -155.0    20     1281   04 14 00
04 15 30  ---          14 02 13  69.5  17.8 -0.6    -155.9    90     1287   04 14 01

04 15 30  J1435+5051   14 02 13  68.9  15.0 -0.6    -159.3   -10     1287   04 15 40
04 20 30  ---          14 07 14  69.2  12.9 -0.5    -162.3   290     1305   04 15 31

04 21 00  J1439+4958   14 07 44  69.8  15.5 -0.5    -159.2    20     1305   04 21 00
04 22 30  ---          14 09 14  69.9  14.8 -0.5    -160.1    90     1311   04 21 01

04 22 30  J1435+5051   14 09 14  69.3  12.1 -0.4    -163.5   -10     1311   04 22 40
04 27 30  ---          14 14 15  69.5   9.9 -0.4    -166.5   290     1330   04 22 31

04 28 00  J1439+4958   14 14 45  70.2  12.3 -0.4    -163.4    20     1330   04 28 00
04 29 30  ---          14 16 15  70.2  11.6 -0.4    -164.4    90     1336   04 28 01

04 29 30  J1435+5051   14 16 15  69.5   9.0 -0.3    -167.7   -10     1336   04 29 40
04 34 30  ---          14 21 16  69.7   6.8 -0.2    -170.7   290     1354   04 29 31

04 35 00  J1439+4958   14 21 46  70.4   9.1 -0.3    -167.8    20     1354   04 35 00
04 36 30  ---          14 23 16  70.5   8.4 -0.3    -168.8    90     1360   04 35 01

04 36 30  J1435+5051   14 23 16  69.7   5.9 -0.2    -172.0   -10     1360   04 36 40
04 41 30  ---          14 28 17  69.8   3.6 -0.1    -175.1   290     1379   04 36 31

04 42 00  J1439+4958   14 28 47  70.6   5.7 -0.2    -172.3    20     1379   04 42 00
04 43 30  ---          14 30 17  70.7   5.0 -0.2    -173.3    90     1384   04 42 01

04 43 30  J1435+5051   14 30 17  69.8   2.7 -0.1    -176.3   -10     1384   04 43 40
04 48 30  ---          14 35 18  69.9   0.4 -0.0    -179.5   290     1403   04 43 31

04 49 00  J1439+4958   14 35 48  70.7   2.3 -0.1    -176.9    20     1403   04 49 00
04 50 30  ---          14 37 19  70.8   1.6 -0.1    -177.9    90     1409   04 49 01

04 50 30  J1435+5051   14 37 19  69.9  -0.5  0.0     179.3   -10     1409   04 50 40
04 55 30  ---          14 42 19  69.8  -2.8  0.1     176.1   290     1428   04 50 31

04 56 00  J1439+4958   14 42 49  70.8  -1.1  0.0     178.5    20     1428   04 56 00
04 57 30  ---          14 44 20  70.7  -1.8  0.1     177.6    90     1433   04 56 01

04 57 30  J1435+5051   14 44 20  69.8  -3.8  0.1     174.9   -10     1433   04 57 40
05 02 30  ---          14 49 21  69.7  -6.0  0.2     171.8   290     1452   04 57 31

05 03 00  J1439+4958   14 49 51  70.7  -4.5  0.2     174.0    20     1452   05 03 00
05 04 30  ---          14 51 21  70.7  -5.2  0.2     173.0    90     1458   05 03 01
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

05 04 30  J1435+5051   14 51 21  69.7  -6.9  0.3     170.6   -10     1458   05 04 40
05 09 30  ---          14 56 22  69.5  -9.2  0.3     167.5   290     1477   05 04 31

05 10 00  J1439+4958   14 56 52  70.5  -7.9  0.3     169.4    20     1477   05 10 00
05 11 30  ---          14 58 22  70.5  -8.6  0.3     168.5    90     1482   05 10 01

05 11 30  J1435+5051   14 58 22  69.5 -10.0  0.4     166.3   -10     1482   05 11 40
05 16 30  ---          15 03 23  69.2 -12.2  0.5     163.3   290     1501   05 11 31

05 17 00  J1439+4958   15 03 53  70.3 -11.2  0.4     165.0    20     1501   05 17 00
05 18 30  ---          15 05 23  70.2 -11.9  0.4     164.1    90     1507   05 17 01

05 18 30  J1435+5051   15 05 23  69.1 -13.1  0.5     162.1   -10     1507   05 18 40
05 23 30  ---          15 10 24  68.9 -15.2  0.6     159.2   290     1526   05 18 31

05 24 00  J1439+4958   15 10 54  69.9 -14.3  0.5     160.7    20     1526   05 24 00
05 25 30  ---          15 12 24  69.9 -15.0  0.5     159.8    90     1531   05 24 01

05 25 30  J1435+5051   15 12 24  68.8 -16.0  0.6     158.0   -10     1531   05 25 40
05 30 30  ---          15 17 25  68.5 -18.0  0.7     155.2   290     1550   05 25 31

05 31 00  J1439+4958   15 17 55  69.5 -17.4  0.6     156.5    20     1550   05 31 00
05 32 30  ---          15 19 25  69.4 -18.0  0.6     155.6    90     1556   05 31 01

05 32 30  J1435+5051   15 19 25  68.3 -18.7  0.7     154.1   -10     1556   05 32 40
05 37 30  ---          15 24 26  68.0 -20.6  0.8     151.3   290     1574   05 32 31

05 38 00  J1439+4958   15 24 56  69.0 -20.3  0.7     152.4    20     1574   05 38 00
05 39 30  ---          15 26 27  68.9 -20.9  0.8     151.6    90     1580   05 38 01

05 39 30  J1435+5051   15 26 27  67.8 -21.4  0.8     150.3   -10     1580   05 39 40
05 44 30  ---          15 31 27  67.4 -23.2  0.9     147.7   290     1599   05 39 31

05 45 00  J1439+4958   15 31 58  68.5 -23.0  0.9     148.6    20     1599   05 45 00
05 46 30  ---          15 33 28  68.3 -23.5  0.9     147.8    90     1605   05 45 01

05 46 30  J1435+5051   15 33 28  67.2 -23.8  1.0     146.6   -10     1605   05 46 40
05 51 30  ---          15 38 29  66.8 -25.5  1.0     144.1   290     1623   05 46 31

05 52 00  J1439+4958   15 38 59  67.9 -25.5  1.0     144.9    20     1623   05 52 00
05 53 30  ---          15 40 29  67.7 -26.1  1.0     144.1    90     1629   05 52 01

05 53 30  J1435+5051   15 40 29  66.6 -26.2  1.1     143.1   -10     1629   05 53 40
05 58 30  ---          15 45 30  66.1 -27.7  1.2     140.8   290     1648   05 53 31
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

05 59 00  J1439+4958   15 46 00  67.2 -27.9  1.1     141.3    20     1648   05 59 00
06 00 30  ---          15 47 30  67.0 -28.4  1.1     140.6    90     1654   05 59 01

06 00 30  J1435+5051   15 47 30  65.9 -28.3  1.2     139.8   -10     1654   06 00 40
06 05 30  ---          15 52 31  65.4 -29.8  1.3     137.5   290     1672   06 00 31

06 06 00  J1439+4958   15 53 01  66.4 -30.1  1.2     138.0    20     1672   06 06 00
06 07 30  ---          15 54 31  66.3 -30.5  1.2     137.3    90     1678   06 06 01

06 07 30  J1435+5051   15 54 31  65.2 -30.3  1.3     136.6   -10     1678   06 07 40
06 12 30  ---          15 59 32  64.6 -31.6  1.4     134.5   290     1697   06 07 31

06 13 00  J1439+4958   16 00 02  65.7 -32.1  1.3     134.8    20     1697   06 13 00
06 14 30  ---          16 01 32  65.5 -32.5  1.3     134.1    90     1703   06 13 01

06 16 00  J1407+2827   16 03 03  64.9 -87.9  1.9      77.7    43     1703   06 16 00
06 21 00  =OQ208       16 08 03  63.9 -87.4  2.0      77.6   300     1722   06 16 01

06 23 00  J1439+4958   16 10 04  64.5 -34.7  1.5     130.5    74     1722   06 23 00
06 25 30  ---          16 12 34  64.2 -35.3  1.5     129.5   150     1732   06 23 01

06 25 30  J1435+5051   16 12 34  63.1 -34.8  1.6     129.1   -10     1732   06 25 40
06 30 30  ---          16 17 35  62.4 -35.8  1.7     127.2   290     1750   06 25 31

06 31 00  J1439+4958   16 18 05  63.5 -36.6  1.6     127.3    20     1750   06 31 00
06 32 30  ---          16 19 35  63.3 -36.9  1.7     126.8    90     1756   06 31 01

06 32 30  J1435+5051   16 19 35  62.2 -36.2  1.7     126.5   -10     1756   06 32 40
06 37 30  ---          16 24 36  61.5 -37.2  1.8     124.6   290     1775   06 32 31

06 38 00  J1439+4958   16 25 06  62.6 -38.0  1.7     124.7    20     1775   06 38 00
06 39 30  ---          16 26 36  62.4 -38.3  1.8     124.1    90     1781   06 38 01

06 39 30  J1435+5051   16 26 36  61.3 -37.6  1.8     123.9   -10     1781   06 39 40
06 44 30  ---          16 31 37  60.6 -38.5  1.9     122.2   290     1799   06 39 31

06 45 00  J1439+4958   16 32 07  61.6 -39.3  1.9     122.2    20     1799   06 45 00
06 46 30  ---          16 33 38  61.4 -39.6  1.9     121.6    90     1805   06 45 01

06 46 30  J1435+5051   16 33 38  60.3 -38.8  2.0     121.5   -10     1805   06 46 40
06 51 30  ---          16 38 38  59.7 -39.6  2.0     119.8   290     1824   06 46 31

06 52 00  J1439+4958   16 39 09  60.6 -40.6  2.0     119.8    20     1824   06 52 00
06 53 30  ---          16 40 39  60.4 -40.8  2.0     119.3    90     1830   06 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

06 53 30  J1435+5051   16 40 39  59.4 -39.9  2.1     119.2   -10     1830   06 53 40
06 58 30  ---          16 45 40  58.7 -40.7  2.2     117.6   290     1848   06 53 31

06 59 00  J1439+4958   16 46 10  59.7 -41.6  2.1     117.5    20     1848   06 59 00
07 00 30  ---          16 47 40  59.4 -41.9  2.1     117.0    90     1854   06 59 01

07 00 30  J1435+5051   16 47 40  58.4 -40.9  2.2     116.9   -10     1854   07 00 40
07 05 30  ---          16 52 41  57.7 -41.6  2.3     115.4   290     1873   07 00 31

07 06 00  J1439+4958   16 53 11  58.6 -42.6  2.2     115.3    20     1873   07 06 00
07 07 30  ---          16 54 41  58.4 -42.8  2.2     114.8    90     1879   07 06 01

07 07 30  J1435+5051   16 54 41  57.4 -41.9  2.3     114.8   -10     1879   07 07 40
07 12 30  ---          16 59 42  56.7 -42.5  2.4     113.3   290     1897   07 07 31

07 13 00  J1439+4958   17 00 12  57.6 -43.5  2.3     113.2    20     1897   07 13 00
07 14 30  ---          17 01 42  57.4 -43.7  2.4     112.8    90     1903   07 13 01

07 14 30  J1435+5051   17 01 42  56.4 -42.7  2.4     112.8   -10     1903   07 14 40
07 19 30  ---          17 06 43  55.7 -43.2  2.5     111.3   290     1922   07 14 31

07 20 00  J1439+4958   17 07 13  56.6 -44.3  2.4     111.2    20     1922   07 20 00
07 21 30  ---          17 08 43  56.3 -44.4  2.5     110.8    90     1927   07 20 01

07 21 30  J1435+5051   17 08 43  55.4 -43.4  2.5     110.8   -10     1927   07 21 40
07 26 30  ---          17 13 44  54.6 -43.9  2.6     109.4   290     1946   07 21 31

07 27 00  J1439+4958   17 14 14  55.5 -45.0  2.6     109.3    20     1946   07 27 00
07 28 30  ---          17 15 45  55.3 -45.1  2.6     108.9    90     1952   07 27 01

07 28 30  J1435+5051   17 15 45  54.3 -44.1  2.7     108.9   -10     1952   07 28 40
07 33 30  ---          17 20 45  53.6 -44.5  2.7     107.6   290     1971   07 28 31

07 34 00  J1439+4958   17 21 15  54.4 -45.6  2.7     107.4    20     1971   07 34 00
07 35 30  ---          17 22 46  54.2 -45.7  2.7     107.0    90     1976   07 34 01

07 35 30  J1435+5051   17 22 46  53.3 -44.6  2.8     107.1   -10     1976   07 35 40
07 40 30  ---          17 27 47  52.5 -45.0  2.9     105.8   290     1995   07 35 31

07 41 00  J1439+4958   17 28 17  53.3 -46.2  2.8     105.7    20     1995   07 41 00
07 42 30  ---          17 29 47  53.1 -46.3  2.8     105.3    90     2001   07 41 01

07 42 30  J1435+5051   17 29 47  52.2 -45.2  2.9     105.3   -10     2001   07 42 40
07 47 30  ---          17 34 48  51.4 -45.5  3.0     104.1   290     2020   07 42 31
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

07 48 00  J1439+4958   17 35 18  52.2 -46.6  2.9     103.9    20     2020   07 48 00
07 49 30  ---          17 36 48  52.0 -46.7  2.9     103.6    90     2025   07 48 01

07 49 30  J1435+5051   17 36 48  51.1 -45.6  3.0     103.6   -10     2025   07 49 40
07 54 30  ---          17 41 49  50.3 -45.9  3.1     102.4   290     2044   07 49 31

07 55 00  J1439+4958   17 42 19  51.1 -47.0  3.0     102.3    20     2044   07 55 00
07 56 30  ---          17 43 49  50.9 -47.1  3.1     101.9    90     2050   07 55 01

07 56 30  J1435+5051   17 43 49  50.0 -46.0  3.1     101.9   -10     2050   07 56 40
08 01 30  ---          17 48 50  49.3 -46.2  3.2     100.8   290     2069   07 56 31

08 02 00  J1439+4958   17 49 20  50.0 -47.4  3.1     100.7    20     2069   08 02 00
08 03 30  ---          17 50 50  49.8 -47.5  3.2     100.3    90     2074   08 02 01

08 03 30  J1435+5051   17 50 50  48.9 -46.3  3.2     100.3   -10     2074   08 03 40
08 08 30  ---          17 55 51  48.2 -46.5  3.3      99.2   290     2093   08 03 31

08 09 00  J1439+4958   17 56 21  48.9 -47.7  3.3      99.1    20     2093   08 09 00
08 10 30  ---          17 57 51  48.7 -47.8  3.3      98.8    90     2099   08 09 01

08 10 30  J1435+5051   17 57 51  47.9 -46.6  3.4      98.8   -10     2099   08 10 40
08 15 30  ---          18 02 52  47.1 -46.8  3.4      97.7   290     2117   08 10 31

08 16 00  J1439+4958   18 03 22  47.8 -47.9  3.4      97.6    20     2117   08 16 00
08 17 30  ---          18 04 53  47.6 -48.0  3.4      97.2    90     2123   08 16 01

08 17 30  J1435+5051   18 04 53  46.8 -46.8  3.5      97.2   -10     2123   08 17 40
08 22 30  ---          18 09 53  46.0 -47.0  3.6      96.2   290     2142   08 17 31

08 23 00  J1439+4958   18 10 24  46.7 -48.1  3.5      96.1    20     2142   08 23 00
08 24 30  ---          18 11 54  46.4 -48.2  3.5      95.8    90     2148   08 23 01

08 24 30  J1435+5051   18 11 54  45.6 -47.0  3.6      95.7   -10     2148   08 24 40
08 29 30  ---          18 16 55  44.9 -47.1  3.7      94.7   290     2166   08 24 31

08 30 00  J1439+4958   18 17 25  45.6 -48.3  3.6      94.6    20     2166   08 30 00
08 31 30  ---          18 18 55  45.3 -48.3  3.6      94.3    90     2172   08 30 01

08 33 00  J1407+2827   18 20 25  35.8 -75.3  4.2      71.0    63     2172   08 33 00
08 38 00  =OQ208       18 25 26  34.7 -74.9  4.3      70.7   300     2192   08 33 01

08 40 00  J1439+4958   18 27 26  43.9 -48.4  3.8      92.6    93     2192   08 40 00
08 42 30  ---          18 29 57  43.5 -48.5  3.8      92.1   150     2201   08 40 01
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

08 42 30  J1435+5051   18 29 57  42.8 -47.3  3.9      92.1    -9     2201   08 42 39
08 47 30  ---          18 34 58  42.0 -47.3  4.0      91.1   291     2220   08 42 31

08 48 00  J1439+4958   18 35 28  42.7 -48.5  3.9      91.0    21     2220   08 48 00
08 49 30  ---          18 36 58  42.4 -48.5  3.9      90.7    90     2226   08 48 01

08 49 30  J1435+5051   18 36 58  41.7 -47.3  4.0      90.7    -9     2226   08 49 39
08 54 30  ---          18 41 59  40.9 -47.3  4.1      89.7   291     2244   08 49 31

08 55 00  J1439+4958   18 42 29  41.5 -48.5  4.0      89.7    21     2244   08 55 00
08 56 30  ---          18 43 59  41.3 -48.5  4.1      89.4    90     2250   08 55 01

08 56 30  J1435+5051   18 43 59  40.6 -47.3  4.1      89.3    -9     2250   08 56 39
09 01 30  ---          18 49 00  39.8 -47.3  4.2      88.4   291     2269   08 56 31

09 02 00  J1439+4958   18 49 30  40.4 -48.5  4.1      88.4    21     2269   09 02 00
09 03 30  ---          18 51 00  40.1 -48.5  4.2      88.1    90     2275   09 02 01

09 03 30  J1435+5051   18 51 00  39.5 -47.3  4.2      88.0    -9     2275   09 03 39
09 08 30  ---          18 56 01  38.7 -47.2  4.3      87.0   291     2294   09 03 31

09 09 00  J1439+4958   18 56 31  39.3 -48.4  4.3      87.1    21     2294   09 09 00
09 10 30  ---          18 58 01  39.0 -48.4  4.3      86.8    90     2299   09 09 01

09 10 30  J1435+5051   18 58 01  38.4 -47.2  4.4      86.7    -9     2299   09 10 39
09 15 30  ---          19 03 02  37.6 -47.1  4.4      85.7   291     2318   09 10 31

09 16 00  J1439+4958   19 03 32  38.1 -48.3  4.4      85.8    21     2318   09 16 00
09 17 30  ---          19 05 02  37.9 -48.3  4.4      85.5    90     2324   09 16 01

09 17 30  J1435+5051   19 05 02  37.3 -47.1  4.5      85.4    -9     2324   09 17 39
09 22 30  ---          19 10 03  36.5 -47.0  4.6      84.4   291     2343   09 17 31

09 23 00  J1439+4958   19 10 33  37.0 -48.2  4.5      84.5    21     2343   09 23 00
09 24 30  ---          19 12 04  36.8 -48.2  4.5      84.2    90     2348   09 23 01

09 24 30  J1435+5051   19 12 04  36.2 -47.0  4.6      84.1    -9     2348   09 24 39
09 29 30  ---          19 17 04  35.4 -46.9  4.7      83.2   291     2367   09 24 31

09 30 00  J1439+4958   19 17 35  35.9 -48.1  4.6      83.2    21     2367   09 30 00
09 31 30  ---          19 19 05  35.6 -48.0  4.6      83.0    90     2373   09 30 01

09 31 30  J1435+5051   19 19 05  35.0 -46.8  4.7      82.8    -9     2373   09 31 39
09 36 30  ---          19 24 06  34.3 -46.7  4.8      81.9   291     2392   09 31 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu   2 Jun 2022   Day 153 ---

09 37 00  J1439+4958   19 24 36  34.8 -47.9  4.7      82.0    21     2392   09 37 00
09 38 30  ---          19 26 06  34.5 -47.8  4.8      81.7    90     2398   09 37 01

09 38 30  J1435+5051   19 26 06  33.9 -46.7  4.8      81.6    -9     2398   09 38 39
09 43 30  ---          19 31 07  33.2 -46.5  4.9      80.7   291     2416   09 38 31

09 44 00  J1439+4958   19 31 37  33.6 -47.7  4.9      80.8    21     2416   09 44 00
09 45 30  ---          19 33 07  33.4 -47.6  4.9      80.5    90     2422   09 44 01

09 45 30  J1435+5051   19 33 07  32.9 -46.4  4.9      80.3    -9     2422   09 45 39
09 50 30  ---          19 38 08  32.1 -46.3  5.0      79.4   291     2441   09 45 31

09 51 00  J1439+4958   19 38 38  32.5 -47.4  5.0      79.6    21     2441   09 51 00
09 52 30  ---          19 40 08  32.3 -47.4  5.0      79.3    90     2447   09 51 01

09 52 30  J1435+5051   19 40 08  31.8 -46.2  5.1      79.1    -9     2447   09 52 39
09 58 00  ---          19 45 39  30.9 -46.0  5.2      78.1   321     2467   09 52 31

09 58 00  J1439+4958   19 45 39  31.4 -47.2  5.1      78.4    -9     2467   09 58 09
10 00 00  ---          19 47 39  31.1 -47.1  5.1      78.0   111     2474   09 58 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess222H5globline.setini
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v20cm_1         FD and KP filtered below 1330. SC filtered above 1440

   Setup group:    4         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  12.9      2.1     12.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  11  Setup file default.  Used with PCAL = off
   LO sum=   1264.50  1264.50  1280.50  1280.50  1296.50  1296.50  1312.50  1312.50
   BBC fr=    835.50   835.50   819.50   819.50   803.50   803.50   787.50   787.50
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     819.50    819.50    803.50    803.50
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  11  12  13  14  15  16  17  19  20  21

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * J1435+5051        14 33 39.332909   * 14 35 21.677000     14 36 09.048726       0.00
                     51 04 25.55781    * 50 51 22.92000      50 45 41.33201        0.00
                     From catalog imbedded in main SCHED input file.

 * J1439+4958        14 38 04.222104   * 14 39 46.976000     14 40 34.505301       0.00
                     50 10 55.89403    * 49 58 05.45600      49 52 28.84641        0.00
                     From catalog imbedded in main SCHED input file.

   OQ208             14 04 45.615156   * 14 07 00.394415     14 08 01.337818       0.24
 * J1407+2827        28 41 29.23515    * 28 27 14.69019      28 20 58.97386        0.35
   1404+286          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J1407+28          GSFC 2016a X/S astro solution,  68278 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J1435+5051 s222H5globline.setini 1 2 3 4 5 6 11 18                11.775  1061.565
  J1439+4958 s222H5globline.setini 1 2 3 4 5 6 11 18                 3.900   368.173
  J1407+2827 s222H5globline.setini 1 2 3 4 5 6 11 18                 0.750    59.051


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J1435+5051         102.1
   J1439+4958         103.3
   J1407+2827         117.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

