  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
 Exp. Code:  GB042C  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 1 July 1999                        

PI:       N. Bartel, M.P. Rupen                                           

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@polaris.phys.yorku.ca                                    
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 256-8-2-ul 4cm                                       

Notes:    Fringe finder  : 0954+658                                       
          Pol. Calibrator: 0954+658, OQ208                                
          Amplitude check: 0954+658, OQ208                                
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

 Next scan frequencies:  4979.49  4979.49  4979.49  4979.49  4995.49  4995.49
                         4995.49  4995.49
 Next BBC frequencies:    879.49   879.49   879.49   879.49   895.49   895.49
                          895.49   895.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

17 11 00  0954+658     02 23 44  18.7  23.6 -7.6     -56.2     0   1  1      0  17 11 00
17 14 00  ---          02 26 45  18.9  23.7 -7.5     -56.8   180   F  1   2400

17 14 00  M81          02 26 45  21.1  20.8 -7.5     -58.6    -6   1  1   2400  17 14 00
17 16 20  ---          02 29 05  21.2  20.9 -7.4     -59.1   134   F  1   4267

17 16 20  SN1993J      02 29 05  21.2  20.9 -7.4     -59.1    -2   1  1   4267  17 16 20
17 18 20  ---          02 31 05  21.4  21.0 -7.4     -59.5   118   F  1   5867

17 18 20  M81          02 31 05  21.4  21.0 -7.4     -59.5    -2   1  1   5867  17 18 20
17 19 30  ---          02 32 16  21.5  21.0 -7.4     -59.8    68   F  1   6800

17 19 30  SN1993J      02 32 16  21.5  21.1 -7.4     -59.8    -2   1  1   6800  17 19 30
17 21 30  ---          02 34 16  21.6  21.2 -7.4     -60.2   118   F  1   8400

17 21 30  M81          02 34 16  21.6  21.1 -7.4     -60.2    -2   1  1   8400  17 21 30
17 22 40  ---          02 35 26  21.7  21.2 -7.3     -60.5    68   F  1   9333

17 22 40  SN1993J      02 35 26  21.7  21.2 -7.3     -60.5    -2   1  1   9333  17 22 40
17 24 40  ---          02 37 27  21.9  21.3 -7.3     -60.9   118   F  1  10933

17 24 40  M81          02 37 27  21.9  21.3 -7.3     -60.9    -2   1  1  10933  17 24 40
17 25 50  ---          02 38 37  22.0  21.3 -7.3     -61.2    68   F  1  11867

17 25 50  SN1993J      02 38 37  22.0  21.4 -7.3     -61.2    -2   1  1  11867  17 25 50
17 27 50  ---          02 40 37  22.1  21.5 -7.2     -61.6   118   F  1  13467

17 27 50  M81          02 40 37  22.1  21.4 -7.3     -61.6    -2   1  1  13467  17 27 50
17 29 00  ---          02 41 47  22.2  21.5 -7.2     -61.8    68   F  1  14400

17 29 00  SN1993J      02 41 47  22.2  21.5 -7.2     -61.9    -2   1  1  14400  17 29 00
17 31 00  ---          02 43 48  22.4  21.6 -7.2     -62.3   118   F  1  16000

17 31 00  M81          02 43 48  22.4  21.6 -7.2     -62.3    -2   1  1  16000  17 31 00
17 33 00  ---          02 45 48  22.6  21.7 -7.2     -62.7   118   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

17 36 00  M81          02 48 48  22.8  21.8 -7.1     -63.4   178   1  2  17600  17 36 00
17 38 10  ---          02 50 59  23.0  21.9 -7.1     -63.8   130   R  1  15867

17 38 10  SN1993J      02 50 59  23.0  21.9 -7.1     -63.8    -2   1  2  15867  17 38 10
17 40 10  ---          02 52 59  23.1  22.0 -7.0     -64.3   118   R  1  14267

17 40 10  M81          02 52 59  23.1  22.0 -7.0     -64.3    -2   1  2  14267  17 40 10
17 41 20  ---          02 54 09  23.2  22.0 -7.0     -64.5    68   R  1  13333

17 41 20  SN1993J      02 54 09  23.2  22.1 -7.0     -64.5    -2   1  2  13333  17 41 20
17 43 20  ---          02 56 10  23.4  22.2 -7.0     -65.0   118   R  1  11733

17 43 20  M81          02 56 10  23.4  22.1 -7.0     -65.0    -2   1  2  11733  17 43 20
17 44 30  ---          02 57 20  23.5  22.2 -7.0     -65.2    68   R  1  10800

17 44 30  SN1993J      02 57 20  23.5  22.2 -7.0     -65.2    -2   1  2  10800  17 44 30
17 46 30  ---          02 59 20  23.6  22.3 -6.9     -65.7   118   R  1   9200

17 46 30  M81          02 59 20  23.6  22.2 -6.9     -65.6    -2   1  2   9200  17 46 30
17 47 40  ---          03 00 30  23.7  22.3 -6.9     -65.9    68   R  1   8267

17 47 40  SN1993J      03 00 30  23.7  22.3 -6.9     -65.9    -2   1  2   8267  17 47 40
17 49 40  ---          03 02 31  23.9  22.4 -6.9     -66.3   118   R  1   6667

17 49 40  M81          03 02 31  23.9  22.4 -6.9     -66.3    -2   1  2   6667  17 49 40
17 50 50  ---          03 03 41  24.0  22.4 -6.9     -66.6    68   R  1   5733

17 50 50  SN1993J      03 03 41  24.0  22.5 -6.9     -66.6    -2   1  2   5733  17 50 50
17 52 50  ---          03 05 41  24.2  22.5 -6.8     -67.0   118   R  1   4133

17 52 50  M81          03 05 41  24.2  22.5 -6.8     -67.0    -2   1  2   4133  17 52 50
17 54 00  ---          03 06 51  24.3  22.5 -6.8     -67.3    68   R  1   3200

17 54 00  SN1993J      03 06 51  24.3  22.6 -6.8     -67.3    -2   1  2   3200  17 54 00
17 56 00  ---          03 08 52  24.4  22.7 -6.8     -67.7   118   R  1   1600

17 56 00  M81          03 08 52  24.4  22.6 -6.8     -67.7    -2   1  2   1600  17 56 00
17 58 00  ---          03 10 52  24.6  22.7 -6.7     -68.2   118   R  1      0

18 01 00  0954+658     03 13 52  23.2  26.2 -6.8     -66.7   175   1  3      0  18 01 00
18 04 00  ---          03 16 53  23.5  26.3 -6.7     -67.3   180   F  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

18 04 00  M81          03 16 53  25.1  22.9 -6.6     -69.5    -5   1  3   2400  18 04 00
18 06 20  ---          03 19 13  25.3  23.0 -6.6     -70.0   135   F  1   4267

18 06 20  SN1993J      03 19 13  25.3  23.0 -6.6     -70.0    -2   1  3   4267  18 06 20
18 08 20  ---          03 21 14  25.5  23.1 -6.6     -70.4   118   F  1   5867

18 08 20  M81          03 21 14  25.5  23.0 -6.6     -70.4    -2   1  3   5867  18 08 20
18 09 30  ---          03 22 24  25.6  23.1 -6.6     -70.7    68   F  1   6800

18 09 30  SN1993J      03 22 24  25.6  23.1 -6.6     -70.7    -2   1  3   6800  18 09 30
18 11 30  ---          03 24 24  25.7  23.2 -6.5     -71.1   118   F  1   8400

18 11 30  M81          03 24 24  25.7  23.1 -6.5     -71.1    -2   1  3   8400  18 11 30
18 12 40  ---          03 25 34  25.8  23.2 -6.5     -71.4    68   F  1   9333

18 12 40  SN1993J      03 25 34  25.8  23.2 -6.5     -71.4    -2   1  3   9333  18 12 40
18 14 40  ---          03 27 35  26.0  23.3 -6.5     -71.8   118   F  1  10933

18 14 40  M81          03 27 35  26.0  23.2 -6.5     -71.8    -2   1  3  10933  18 14 40
18 15 50  ---          03 28 45  26.1  23.3 -6.4     -72.1    68   F  1  11867

18 15 50  SN1993J      03 28 45  26.1  23.3 -6.4     -72.1    -2   1  3  11867  18 15 50
18 17 50  ---          03 30 45  26.3  23.4 -6.4     -72.5   118   F  1  13467

18 17 50  M81          03 30 45  26.3  23.3 -6.4     -72.5    -2   1  3  13467  18 17 50
18 19 00  ---          03 31 55  26.4  23.4 -6.4     -72.8    68   F  1  14400

18 19 00  SN1993J      03 31 55  26.4  23.4 -6.4     -72.8    -2   1  3  14400  18 19 00
18 21 00  ---          03 33 56  26.5  23.5 -6.4     -73.2   118   F  1  16000

18 21 00  M81          03 33 56  26.5  23.4 -6.4     -73.2    -2   1  3  16000  18 21 00
18 23 00  ---          03 35 56  26.7  23.5 -6.3     -73.7   118   F  1  17600

18 26 00  M81          03 38 57  27.0  23.6 -6.3     -74.3   177   1  4  17600  18 26 00
18 28 10  ---          03 41 07  27.2  23.6 -6.2     -74.8   130   R  1  15867

18 28 10  SN1993J      03 41 07  27.2  23.7 -6.2     -74.8    -2   1  4  15867  18 28 10
18 30 10  ---          03 43 07  27.3  23.7 -6.2     -75.3   118   R  1  14267

18 30 10  M81          03 43 07  27.3  23.7 -6.2     -75.2    -2   1  4  14267  18 30 10
18 31 20  ---          03 44 17  27.4  23.7 -6.2     -75.5    68   R  1  13333
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

18 31 20  SN1993J      03 44 17  27.4  23.8 -6.2     -75.5    -2   1  4  13333  18 31 20
18 33 20  ---          03 46 18  27.6  23.8 -6.2     -76.0   118   R  1  11733

18 33 20  M81          03 46 18  27.6  23.8 -6.2     -76.0    -2   1  4  11733  18 33 20
18 34 30  ---          03 47 28  27.7  23.8 -6.1     -76.2    68   R  1  10800

18 34 30  SN1993J      03 47 28  27.7  23.8 -6.1     -76.2    -2   1  4  10800  18 34 30
18 36 30  ---          03 49 28  27.9  23.9 -6.1     -76.7   118   R  1   9200

18 36 30  M81          03 49 28  27.9  23.8 -6.1     -76.7    -2   1  4   9200  18 36 30
18 37 40  ---          03 50 39  28.0  23.9 -6.1     -76.9    68   R  1   8267

18 37 40  SN1993J      03 50 39  28.0  23.9 -6.1     -76.9    -2   1  4   8267  18 37 40
18 39 40  ---          03 52 39  28.2  24.0 -6.0     -77.4   118   R  1   6667

18 39 40  M81          03 52 39  28.2  23.9 -6.1     -77.4    -2   1  4   6667  18 39 40
18 40 50  ---          03 53 49  28.3  23.9 -6.0     -77.6    68   R  1   5733

18 40 50  SN1993J      03 53 49  28.3  24.0 -6.0     -77.6    -2   1  4   5733  18 40 50
18 42 50  ---          03 55 49  28.4  24.0 -6.0     -78.1   118   R  1   4133

18 42 50  M81          03 55 49  28.4  24.0 -6.0     -78.1    -2   1  4   4133  18 42 50
18 44 00  ---          03 57 00  28.5  24.0 -6.0     -78.3    68   R  1   3200

18 44 00  SN1993J      03 57 00  28.5  24.1 -6.0     -78.3    -2   1  4   3200  18 44 00
18 46 00  ---          03 59 00  28.7  24.1 -5.9     -78.8   118   R  1   1600

18 46 00  M81          03 59 00  28.7  24.0 -5.9     -78.8    -2   1  4   1600  18 46 00
18 48 00  ---          04 01 00  28.9  24.1 -5.9     -79.2   118   R  1      0

18 51 00  M81          04 04 01  29.1  24.1 -5.9     -79.9   177   1  5      0  18 51 00
18 53 10  ---          04 06 11  29.3  24.2 -5.8     -80.4   130   F  1   1733

18 53 10  SN1993J      04 06 11  29.3  24.2 -5.8     -80.4    -2   1  5   1733  18 53 10
18 55 10  ---          04 08 11  29.5  24.3 -5.8     -80.9   118   F  1   3333

18 55 10  M81          04 08 11  29.5  24.2 -5.8     -80.8    -2   1  5   3333  18 55 10
18 56 20  ---          04 09 22  29.6  24.2 -5.8     -81.1    68   F  1   4267

18 56 20  SN1993J      04 09 22  29.6  24.3 -5.8     -81.1    -2   1  5   4267  18 56 20
18 58 20  ---          04 11 22  29.8  24.3 -5.7     -81.6   118   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

18 58 20  M81          04 11 22  29.8  24.3 -5.7     -81.6    -2   1  5   5867  18 58 20
18 59 30  ---          04 12 32  29.9  24.3 -5.7     -81.8    68   F  1   6800

18 59 30  SN1993J      04 12 32  29.9  24.3 -5.7     -81.8    -2   1  5   6800  18 59 30
19 01 30  ---          04 14 32  30.1  24.4 -5.7     -82.3   118   F  1   8400

19 01 30  M81          04 14 32  30.1  24.3 -5.7     -82.3    -2   1  5   8400  19 01 30
19 02 40  ---          04 15 43  30.2  24.3 -5.7     -82.5    68   F  1   9333

19 02 40  SN1993J      04 15 43  30.2  24.4 -5.7     -82.6    -2   1  5   9333  19 02 40
19 04 40  ---          04 17 43  30.4  24.4 -5.6     -83.0   118   F  1  10933

19 04 40  M81          04 17 43  30.4  24.3 -5.6     -83.0    -2   1  5  10933  19 04 40
19 05 50  ---          04 18 53  30.5  24.4 -5.6     -83.3    68   F  1  11867

19 05 50  SN1993J      04 18 53  30.5  24.4 -5.6     -83.3    -2   1  5  11867  19 05 50
19 07 50  ---          04 20 53  30.6  24.4 -5.6     -83.7   118   F  1  13467

19 07 50  M81          04 20 53  30.6  24.4 -5.6     -83.7    -2   1  5  13467  19 07 50
19 09 00  ---          04 22 04  30.7  24.4 -5.6     -84.0    68   F  1  14400

19 09 00  SN1993J      04 22 04  30.8  24.5 -5.6     -84.0    -2   1  5  14400  19 09 00
19 11 00  ---          04 24 04  30.9  24.5 -5.5     -84.5   118   F  1  16000

19 11 00  M81          04 24 04  30.9  24.4 -5.5     -84.5    -2   1  5  16000  19 11 00
19 13 00  ---          04 26 04  31.1  24.4 -5.5     -84.9   118   F  1  17600

19 16 00  M81          04 29 05  31.4  24.5 -5.4     -85.6   177   1  6  17600  19 16 00
19 18 10  ---          04 31 15  31.6  24.5 -5.4     -86.1   130   R  1  15867

19 18 10  SN1993J      04 31 15  31.6  24.5 -5.4     -86.1    -2   1  6  15867  19 18 10
19 20 10  ---          04 33 15  31.7  24.5 -5.4     -86.6   118   R  1  14267

19 20 10  M81          04 33 15  31.7  24.5 -5.4     -86.6    -2   1  6  14267  19 20 10
19 21 20  ---          04 34 26  31.8  24.5 -5.4     -86.8    68   R  1  13333

19 21 20  SN1993J      04 34 26  31.9  24.6 -5.4     -86.8    -2   1  6  13333  19 21 20
19 23 20  ---          04 36 26  32.0  24.6 -5.3     -87.3   118   R  1  11733

19 23 20  M81          04 36 26  32.0  24.5 -5.3     -87.3    -2   1  6  11733  19 23 20
19 24 30  ---          04 37 36  32.1  24.5 -5.3     -87.6    68   R  1  10800
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

19 24 30  SN1993J      04 37 36  32.1  24.6 -5.3     -87.6    -2   1  6  10800  19 24 30
19 26 30  ---          04 39 37  32.3  24.6 -5.3     -88.0   118   R  1   9200

19 26 30  M81          04 39 37  32.3  24.5 -5.3     -88.0    -2   1  6   9200  19 26 30
19 27 40  ---          04 40 47  32.4  24.5 -5.2     -88.3    68   R  1   8267

19 27 40  SN1993J      04 40 47  32.4  24.6 -5.2     -88.3    -2   1  6   8267  19 27 40
19 29 40  ---          04 42 47  32.6  24.6 -5.2     -88.8   118   R  1   6667

19 29 40  M81          04 42 47  32.6  24.5 -5.2     -88.8    -2   1  6   6667  19 29 40
19 30 50  ---          04 43 57  32.7  24.5 -5.2     -89.0    68   R  1   5733

19 30 50  SN1993J      04 43 57  32.7  24.6 -5.2     -89.0    -2   1  6   5733  19 30 50
19 32 50  ---          04 45 58  32.9  24.6 -5.2     -89.5   118   R  1   4133

19 32 50  M81          04 45 58  32.9  24.5 -5.2     -89.5    -2   1  6   4133  19 32 50
19 34 00  ---          04 47 08  33.0  24.5 -5.1     -89.8    68   R  1   3200

19 34 00  SN1993J      04 47 08  33.0  24.6 -5.1     -89.8    -2   1  6   3200  19 34 00
19 36 00  ---          04 49 08  33.2  24.6 -5.1     -90.2   118   R  1   1600

19 36 00  M81          04 49 08  33.2  24.5 -5.1     -90.2    -2   1  6   1600  19 36 00
19 38 00  ---          04 51 08  33.3  24.5 -5.1     -90.7   118   R  1      0

19 41 00  M81          04 54 09  33.6  24.5 -5.0     -91.4   177   1  7      0  19 41 00
19 43 10  ---          04 56 19  33.8  24.5 -5.0     -91.9   130   F  1   1733

19 43 10  SN1993J      04 56 19  33.8  24.6 -5.0     -91.9    -2   1  7   1733  19 43 10
19 45 10  ---          04 58 20  34.0  24.6 -5.0     -92.4   118   F  1   3333

19 45 10  M81          04 58 20  34.0  24.5 -5.0     -92.4    -2   1  7   3333  19 45 10
19 46 20  ---          04 59 30  34.1  24.5 -4.9     -92.7    68   F  1   4267

19 46 20  SN1993J      04 59 30  34.1  24.6 -4.9     -92.7    -2   1  7   4267  19 46 20
19 48 20  ---          05 01 30  34.3  24.6 -4.9     -93.2   118   F  1   5867

19 48 20  M81          05 01 30  34.3  24.5 -4.9     -93.1    -2   1  7   5867  19 48 20
19 49 30  ---          05 02 40  34.4  24.5 -4.9     -93.4    68   F  1   6800

19 49 30  SN1993J      05 02 40  34.4  24.5 -4.9     -93.4    -2   1  7   6800  19 49 30
19 51 30  ---          05 04 41  34.6  24.5 -4.8     -93.9   118   F  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

19 51 30  M81          05 04 41  34.5  24.5 -4.9     -93.9    -2   1  7   8400  19 51 30
19 52 40  ---          05 05 51  34.6  24.5 -4.8     -94.2    68   F  1   9333

19 52 40  SN1993J      05 05 51  34.7  24.5 -4.8     -94.2    -2   1  7   9333  19 52 40
19 54 40  ---          05 07 51  34.8  24.5 -4.8     -94.7   118   F  1  10933

19 54 40  M81          05 07 51  34.8  24.5 -4.8     -94.7    -2   1  7  10933  19 54 40
19 55 50  ---          05 09 01  34.9  24.4 -4.8     -94.9    68   F  1  11867

19 55 50  SN1993J      05 09 01  34.9  24.5 -4.8     -94.9    -2   1  7  11867  19 55 50
19 57 50  ---          05 11 02  35.1  24.5 -4.7     -95.4   118   F  1  13467

19 57 50  M81          05 11 02  35.1  24.4 -4.7     -95.4    -2   1  7  13467  19 57 50
19 59 00  ---          05 12 12  35.2  24.4 -4.7     -95.7    68   F  1  14400

19 59 00  SN1993J      05 12 12  35.2  24.5 -4.7     -95.7    -2   1  7  14400  19 59 00
20 01 00  ---          05 14 12  35.4  24.4 -4.7     -96.2   118   F  1  16000

20 01 00  M81          05 14 12  35.4  24.4 -4.7     -96.2    -2   1  7  16000  20 01 00
20 03 00  ---          05 16 13  35.6  24.4 -4.7     -96.7   118   F  1  17600

20 06 00  0954+658     05 19 13  35.9  28.7 -4.7     -94.1   175   1  8  17600  20 06 00
20 09 00  ---          05 22 14  36.2  28.6 -4.6     -94.8   180   R  1  15200

20 09 00  M81          05 22 14  36.1  24.3 -4.6     -98.1    -5   1  8  15200  20 09 00
20 11 20  ---          05 24 34  36.3  24.2 -4.5     -98.7   135   R  1  13333

20 11 20  SN1993J      05 24 34  36.3  24.3 -4.5     -98.7    -2   1  8  13333  20 11 20
20 13 20  ---          05 26 34  36.5  24.3 -4.5     -99.2   118   R  1  11733

20 13 20  M81          05 26 34  36.5  24.2 -4.5     -99.2    -2   1  8  11733  20 13 20
20 14 30  ---          05 27 44  36.6  24.2 -4.5     -99.5    68   R  1  10800

20 14 30  SN1993J      05 27 44  36.6  24.2 -4.5     -99.5    -2   1  8  10800  20 14 30
20 16 30  ---          05 29 45  36.8  24.2 -4.4    -100.0   118   R  1   9200

20 16 30  M81          05 29 45  36.8  24.1 -4.4    -100.0    -2   1  8   9200  20 16 30
20 17 40  ---          05 30 55  36.9  24.1 -4.4    -100.2    68   R  1   8267

20 17 40  SN1993J      05 30 55  36.9  24.2 -4.4    -100.2    -2   1  8   8267  20 17 40
20 19 40  ---          05 32 55  37.1  24.1 -4.4    -100.7   118   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

20 19 40  M81          05 32 55  37.0  24.1 -4.4    -100.7    -2   1  8   6667  20 19 40
20 20 50  ---          05 34 05  37.1  24.1 -4.4    -101.0    68   R  1   5733

20 20 50  SN1993J      05 34 05  37.2  24.1 -4.4    -101.0    -2   1  8   5733  20 20 50
20 22 50  ---          05 36 06  37.3  24.1 -4.3    -101.5   118   R  1   4133

20 22 50  M81          05 36 06  37.3  24.0 -4.3    -101.5    -2   1  8   4133  20 22 50
20 24 00  ---          05 37 16  37.4  24.0 -4.3    -101.8    68   R  1   3200

20 24 00  SN1993J      05 37 16  37.4  24.0 -4.3    -101.8    -2   1  8   3200  20 24 00
20 26 00  ---          05 39 16  37.6  24.0 -4.3    -102.3   118   R  1   1600

20 26 00  M81          05 39 16  37.6  23.9 -4.3    -102.3    -2   1  8   1600  20 26 00
20 28 00  ---          05 41 17  37.8  23.9 -4.2    -102.8   118   R  1      0

20 31 00  M81          05 44 17  38.0  23.8 -4.2    -103.5   177   1  9      0  20 31 00
20 33 10  ---          05 46 27  38.2  23.8 -4.2    -104.1   130   F  1   1733

20 33 10  SN1993J      05 46 27  38.3  23.8 -4.2    -104.1    -2   1  9   1733  20 33 10
20 35 10  ---          05 48 28  38.4  23.8 -4.1    -104.6   118   F  1   3333

20 35 10  M81          05 48 28  38.4  23.7 -4.1    -104.6    -2   1  9   3333  20 35 10
20 36 20  ---          05 49 38  38.5  23.7 -4.1    -104.9    68   F  1   4267

20 36 20  SN1993J      05 49 38  38.5  23.7 -4.1    -104.9    -2   1  9   4267  20 36 20
20 38 20  ---          05 51 38  38.7  23.7 -4.1    -105.4   118   F  1   5867

20 38 20  M81          05 51 38  38.7  23.6 -4.1    -105.4    -2   1  9   5867  20 38 20
20 39 30  ---          05 52 49  38.8  23.6 -4.0    -105.7    68   F  1   6800

20 39 30  SN1993J      05 52 49  38.8  23.6 -4.0    -105.7    -2   1  9   6800  20 39 30
20 41 30  ---          05 54 49  39.0  23.6 -4.0    -106.2   118   F  1   8400

20 41 30  M81          05 54 49  38.9  23.5 -4.0    -106.2    -2   1  9   8400  20 41 30
20 42 40  ---          05 55 59  39.0  23.5 -4.0    -106.5    68   F  1   9333

20 42 40  SN1993J      05 55 59  39.1  23.5 -4.0    -106.5    -2   1  9   9333  20 42 40
20 44 40  ---          05 57 59  39.2  23.5 -4.0    -107.0   118   F  1  10933

20 44 40  M81          05 57 59  39.2  23.4 -4.0    -107.0    -2   1  9  10933  20 44 40
20 45 50  ---          05 59 10  39.3  23.4 -3.9    -107.3    68   F  1  11867
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

20 45 50  SN1993J      05 59 10  39.3  23.4 -3.9    -107.3    -2   1  9  11867  20 45 50
20 47 50  ---          06 01 10  39.5  23.3 -3.9    -107.8   118   F  1  13467

20 47 50  M81          06 01 10  39.5  23.3 -3.9    -107.8    -2   1  9  13467  20 47 50
20 49 00  ---          06 02 20  39.6  23.3 -3.9    -108.1    68   F  1  14400

20 49 00  SN1993J      06 02 20  39.6  23.3 -3.9    -108.1    -2   1  9  14400  20 49 00
20 51 00  ---          06 04 20  39.8  23.2 -3.9    -108.6   118   F  1  16000

20 51 00  M81          06 04 20  39.8  23.2 -3.9    -108.6    -2   1  9  16000  20 51 00
20 53 00  ---          06 06 21  39.9  23.1 -3.8    -109.1   118   F  1  17600

20 56 00  M81          06 09 21  40.2  23.0 -3.8    -109.9   177   1 10  17600  20 56 00
20 58 10  ---          06 11 32  40.4  22.9 -3.7    -110.5   130   R  1  15867

20 58 10  SN1993J      06 11 32  40.4  22.9 -3.7    -110.5    -2   1 10  15867  20 58 10
21 00 10  ---          06 13 32  40.6  22.9 -3.7    -111.0   118   R  1  14267

21 00 10  M81          06 13 32  40.5  22.8 -3.7    -111.0    -2   1 10  14267  21 00 10
21 01 20  ---          06 14 42  40.6  22.8 -3.7    -111.3    68   R  1  13333

21 01 20  SN1993J      06 14 42  40.7  22.8 -3.7    -111.3    -2   1 10  13333  21 01 20
21 03 20  ---          06 16 42  40.8  22.7 -3.6    -111.8   118   R  1  11733

21 03 20  M81          06 16 42  40.8  22.7 -3.7    -111.8    -2   1 10  11733  21 03 20
21 04 30  ---          06 17 53  40.9  22.6 -3.6    -112.1    68   R  1  10800

21 04 30  SN1993J      06 17 53  40.9  22.7 -3.6    -112.2    -2   1 10  10800  21 04 30
21 06 30  ---          06 19 53  41.1  22.6 -3.6    -112.7   118   R  1   9200

21 06 30  M81          06 19 53  41.1  22.5 -3.6    -112.7    -2   1 10   9200  21 06 30
21 07 40  ---          06 21 03  41.2  22.5 -3.6    -113.0    68   R  1   8267

21 07 40  SN1993J      06 21 03  41.2  22.5 -3.6    -113.0    -2   1 10   8267  21 07 40
21 09 40  ---          06 23 03  41.3  22.4 -3.5    -113.5   118   R  1   6667

21 09 40  M81          06 23 03  41.3  22.4 -3.5    -113.5    -2   1 10   6667  21 09 40
21 10 50  ---          06 24 14  41.4  22.3 -3.5    -113.8    68   R  1   5733

21 10 50  SN1993J      06 24 14  41.4  22.4 -3.5    -113.8    -2   1 10   5733  21 10 50
21 12 50  ---          06 26 14  41.6  22.3 -3.5    -114.4   118   R  1   4133
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

21 12 50  M81          06 26 14  41.6  22.2 -3.5    -114.4    -2   1 10   4133  21 12 50
21 14 00  ---          06 27 24  41.7  22.2 -3.5    -114.7    68   R  1   3200

21 14 00  SN1993J      06 27 24  41.7  22.2 -3.5    -114.7    -2   1 10   3200  21 14 00
21 16 00  ---          06 29 25  41.9  22.1 -3.4    -115.2   118   R  1   1600

21 16 00  M81          06 29 25  41.8  22.1 -3.4    -115.2    -2   1 10   1600  21 16 00
21 18 00  ---          06 31 25  42.0  22.0 -3.4    -115.7   118   R  1      0

21 21 00  M81          06 34 25  42.2  21.8 -3.4    -116.6   178   1 11      0  21 21 00
21 23 10  ---          06 36 36  42.4  21.7 -3.3    -117.1   130   F  1   1733

21 23 10  SN1993J      06 36 36  42.4  21.7 -3.3    -117.1    -2   1 11   1733  21 23 10
21 25 10  ---          06 38 36  42.6  21.6 -3.3    -117.7   118   F  1   3333

21 25 10  M81          06 38 36  42.6  21.6 -3.3    -117.7    -2   1 11   3333  21 25 10
21 26 20  ---          06 39 46  42.7  21.5 -3.3    -118.0    68   F  1   4267

21 26 20  SN1993J      06 39 46  42.7  21.6 -3.3    -118.0    -2   1 11   4267  21 26 20
21 28 20  ---          06 41 47  42.9  21.4 -3.2    -118.6   118   F  1   5867

21 28 20  M81          06 41 47  42.8  21.4 -3.2    -118.5    -2   1 11   5867  21 28 20
21 29 30  ---          06 42 57  42.9  21.3 -3.2    -118.9    68   F  1   6800

21 29 30  SN1993J      06 42 57  42.9  21.4 -3.2    -118.9    -2   1 11   6800  21 29 30
21 31 30  ---          06 44 57  43.1  21.3 -3.2    -119.4   118   F  1   8400

21 31 30  M81          06 44 57  43.1  21.2 -3.2    -119.4    -2   1 11   8400  21 31 30
21 32 40  ---          06 46 07  43.2  21.1 -3.2    -119.7    68   F  1   9333

21 32 40  SN1993J      06 46 07  43.2  21.2 -3.2    -119.7    -2   1 11   9333  21 32 40
21 34 40  ---          06 48 08  43.4  21.1 -3.1    -120.3   118   F  1  10933

21 34 40  M81          06 48 08  43.3  21.0 -3.1    -120.3    -2   1 11  10933  21 34 40
21 35 50  ---          06 49 18  43.4  20.9 -3.1    -120.6    68   F  1  11867

21 35 50  SN1993J      06 49 18  43.4  21.0 -3.1    -120.6    -2   1 11  11867  21 35 50
21 37 50  ---          06 51 18  43.6  20.9 -3.1    -121.2   118   F  1  13467

21 37 50  M81          06 51 18  43.6  20.8 -3.1    -121.2    -2   1 11  13467  21 37 50
21 39 00  ---          06 52 28  43.7  20.7 -3.1    -121.5    68   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

21 39 00  SN1993J      06 52 28  43.7  20.8 -3.1    -121.5    -2   1 11  14400  21 39 00
21 41 00  ---          06 54 29  43.8  20.7 -3.0    -122.1   118   F  1  16000

21 41 00  M81          06 54 29  43.8  20.6 -3.0    -122.1    -2   1 11  16000  21 41 00
21 43 00  ---          06 56 29  44.0  20.5 -3.0    -122.6   118   F  1  17600

21 46 00  M81          06 59 29  44.2  20.3 -2.9    -123.5   178   1 12  17600  21 46 00
21 48 10  ---          07 01 40  44.3  20.1 -2.9    -124.1   130   R  1  15867

21 48 10  SN1993J      07 01 40  44.4  20.2 -2.9    -124.1    -2   1 12  15867  21 48 10
21 50 10  ---          07 03 40  44.5  20.0 -2.9    -124.6   118   R  1  14267

21 50 10  M81          07 03 40  44.5  20.0 -2.9    -124.6    -2   1 12  14267  21 50 10
21 51 20  ---          07 04 50  44.6  19.9 -2.8    -125.0    68   R  1  13333

21 51 20  SN1993J      07 04 50  44.6  19.9 -2.8    -125.0    -2   1 12  13333  21 51 20
21 53 20  ---          07 06 51  44.8  19.8 -2.8    -125.5   118   R  1  11733

21 53 20  M81          07 06 51  44.7  19.8 -2.8    -125.5    -2   1 12  11733  21 53 20
21 54 30  ---          07 08 01  44.8  19.7 -2.8    -125.9    68   R  1  10800

21 54 30  SN1993J      07 08 01  44.8  19.7 -2.8    -125.9    -2   1 12  10800  21 54 30
21 56 30  ---          07 10 01  45.0  19.6 -2.8    -126.5   118   R  1   9200

21 56 30  M81          07 10 01  45.0  19.5 -2.8    -126.4    -2   1 12   9200  21 56 30
21 57 40  ---          07 11 11  45.0  19.4 -2.7    -126.8    68   R  1   8267

21 57 40  SN1993J      07 11 11  45.1  19.5 -2.7    -126.8    -2   1 12   8267  21 57 40
21 59 40  ---          07 13 12  45.2  19.3 -2.7    -127.4   118   R  1   6667

21 59 40  M81          07 13 12  45.2  19.3 -2.7    -127.4    -2   1 12   6667  21 59 40
22 00 50  ---          07 14 22  45.3  19.2 -2.7    -127.7    68   R  1   5733

22 00 50  SN1993J      07 14 22  45.3  19.2 -2.7    -127.7    -2   1 12   5733  22 00 50
22 02 50  ---          07 16 22  45.4  19.1 -2.7    -128.3   118   R  1   4133

22 02 50  M81          07 16 22  45.4  19.0 -2.7    -128.3    -2   1 12   4133  22 02 50
22 04 00  ---          07 17 32  45.5  18.9 -2.6    -128.6    68   R  1   3200

22 04 00  SN1993J      07 17 32  45.5  19.0 -2.6    -128.6    -2   1 12   3200  22 04 00
22 06 00  ---          07 19 33  45.7  18.8 -2.6    -129.2   118   R  1   1600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

22 06 00  M81          07 19 33  45.6  18.8 -2.6    -129.2    -2   1 12   1600  22 06 00
22 08 00  ---          07 21 33  45.8  18.6 -2.6    -129.8   118   R  1      0

22 11 00  0954+658     07 24 34  47.9  22.6 -2.6    -126.8   174   1 13      0  22 11 00
22 14 00  ---          07 27 34  48.2  22.4 -2.5    -127.7   180   F  1   2400

22 14 00  M81          07 27 34  46.2  18.1 -2.5    -131.6    -6   1 13   2400  22 14 00
22 16 20  ---          07 29 54  46.3  17.9 -2.4    -132.2   134   F  1   4267

22 16 20  SN1993J      07 29 54  46.4  17.9 -2.4    -132.3    -2   1 13   4267  22 16 20
22 18 20  ---          07 31 55  46.5  17.8 -2.4    -132.8   118   F  1   5867

22 18 20  M81          07 31 55  46.5  17.7 -2.4    -132.8    -2   1 13   5867  22 18 20
22 19 30  ---          07 33 05  46.5  17.6 -2.4    -133.2    68   F  1   6800

22 19 30  SN1993J      07 33 05  46.6  17.7 -2.4    -133.2    -2   1 13   6800  22 19 30
22 21 30  ---          07 35 05  46.7  17.5 -2.3    -133.8   118   F  1   8400

22 21 30  M81          07 35 05  46.7  17.4 -2.3    -133.8    -2   1 13   8400  22 21 30
22 22 40  ---          07 36 15  46.7  17.3 -2.3    -134.1    68   F  1   9333

22 22 40  SN1993J      07 36 15  46.8  17.4 -2.3    -134.1    -2   1 13   9333  22 22 40
22 24 40  ---          07 38 16  46.9  17.2 -2.3    -134.7   118   F  1  10933

22 24 40  M81          07 38 16  46.9  17.2 -2.3    -134.7    -2   1 13  10933  22 24 40
22 25 50  ---          07 39 26  46.9  17.1 -2.3    -135.1    68   F  1  11867

22 25 50  SN1993J      07 39 26  47.0  17.1 -2.3    -135.1    -2   1 13  11867  22 25 50
22 27 50  ---          07 41 26  47.1  16.9 -2.2    -135.7   118   F  1  13467

22 27 50  M81          07 41 26  47.1  16.9 -2.2    -135.7    -2   1 13  13467  22 27 50
22 29 00  ---          07 42 37  47.1  16.8 -2.2    -136.0    68   F  1  14400

22 29 00  SN1993J      07 42 37  47.2  16.8 -2.2    -136.1    -2   1 13  14400  22 29 00
22 31 00  ---          07 44 37  47.3  16.6 -2.2    -136.7   118   F  1  16000

22 31 00  M81          07 44 37  47.3  16.6 -2.2    -136.7    -2   1 13  16000  22 31 00
22 33 00  ---          07 46 37  47.4  16.4 -2.2    -137.3   118   F  1  17600

22 36 00  M81          07 49 38  47.6  16.1 -2.1    -138.2   178   1 14  17600  22 36 00
22 38 10  ---          07 51 48  47.7  15.9 -2.1    -138.9   130   R  1  15867
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

22 38 10  SN1993J      07 51 48  47.7  15.9 -2.1    -138.9    -2   1 14  15867  22 38 10
22 40 10  ---          07 53 48  47.9  15.7 -2.0    -139.5   118   R  1  14267

22 40 10  M81          07 53 48  47.8  15.7 -2.0    -139.5    -2   1 14  14267  22 40 10
22 41 20  ---          07 54 59  47.9  15.5 -2.0    -139.8    68   R  1  13333

22 41 20  SN1993J      07 54 59  47.9  15.6 -2.0    -139.8    -2   1 14  13333  22 41 20
22 43 20  ---          07 56 59  48.0  15.4 -2.0    -140.5   118   R  1  11733

22 43 20  M81          07 56 59  48.0  15.3 -2.0    -140.5    -2   1 14  11733  22 43 20
22 44 30  ---          07 58 09  48.1  15.2 -2.0    -140.8    68   R  1  10800

22 44 30  SN1993J      07 58 09  48.1  15.2 -2.0    -140.8    -2   1 14  10800  22 44 30
22 46 30  ---          08 00 09  48.2  15.0 -1.9    -141.5   118   R  1   9200

22 46 30  M81          08 00 09  48.2  15.0 -1.9    -141.4    -2   1 14   9200  22 46 30
22 47 40  ---          08 01 20  48.2  14.9 -1.9    -141.8    68   R  1   8267

22 47 40  SN1993J      08 01 20  48.3  14.9 -1.9    -141.8    -2   1 14   8267  22 47 40
22 49 40  ---          08 03 20  48.4  14.7 -1.9    -142.4   118   R  1   6667

22 49 40  M81          08 03 20  48.3  14.7 -1.9    -142.4    -2   1 14   6667  22 49 40
22 50 50  ---          08 04 30  48.4  14.5 -1.9    -142.8    68   R  1   5733

22 50 50  SN1993J      08 04 30  48.5  14.6 -1.9    -142.8    -2   1 14   5733  22 50 50
22 52 50  ---          08 06 30  48.6  14.4 -1.8    -143.4   118   R  1   4133

22 52 50  M81          08 06 30  48.5  14.3 -1.8    -143.4    -2   1 14   4133  22 52 50
22 54 00  ---          08 07 41  48.6  14.2 -1.8    -143.8    68   R  1   3200

22 54 00  SN1993J      08 07 41  48.6  14.2 -1.8    -143.8    -2   1 14   3200  22 54 00
22 56 00  ---          08 09 41  48.7  14.0 -1.8    -144.4   118   R  1   1600

22 56 00  M81          08 09 41  48.7  14.0 -1.8    -144.4    -2   1 14   1600  22 56 00
22 58 00  ---          08 11 41  48.8  13.8 -1.7    -145.1   118   R  1      0

-----------  Tape Change ------------

23 13 00  M81          08 26 44  49.5  12.0 -1.5    -149.9   897   2  1      0  23 13 00
23 15 10  ---          08 28 54  49.6  11.8 -1.4    -150.6   130   F  1   1733

23 15 10  SN1993J      08 28 54  49.7  11.8 -1.4    -150.6    -2   2  1   1733  23 15 10
23 17 10  ---          08 30 54  49.7  11.5 -1.4    -151.3   118   F  1   3333
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

23 17 10  M81          08 30 54  49.7  11.5 -1.4    -151.2    -2   2  1   3333  23 17 10
23 18 20  ---          08 32 05  49.7  11.4 -1.4    -151.6    68   F  1   4267

23 18 20  SN1993J      08 32 05  49.8  11.4 -1.4    -151.6    -2   2  1   4267  23 18 20
23 20 20  ---          08 34 05  49.9  11.2 -1.4    -152.3   118   F  1   5867

23 20 20  M81          08 34 05  49.8  11.1 -1.4    -152.3    -2   2  1   5867  23 20 20
23 21 30  ---          08 35 15  49.9  11.0 -1.3    -152.7    68   F  1   6800

23 21 30  SN1993J      08 35 15  49.9  11.0 -1.3    -152.7    -2   2  1   6800  23 21 30
23 23 30  ---          08 37 15  50.0  10.8 -1.3    -153.3   118   F  1   8400

23 23 30  M81          08 37 15  50.0  10.7 -1.3    -153.3    -2   2  1   8400  23 23 30
23 24 40  ---          08 38 26  50.0  10.6 -1.3    -153.7    68   F  1   9333

23 24 40  SN1993J      08 38 26  50.1  10.6 -1.3    -153.7    -2   2  1   9333  23 24 40
23 26 40  ---          08 40 26  50.1  10.4 -1.3    -154.4   118   F  1  10933

23 26 40  M81          08 40 26  50.1  10.4 -1.3    -154.4    -2   2  1  10933  23 26 40
23 27 50  ---          08 41 36  50.1  10.2 -1.2    -154.8    68   F  1  11867

23 27 50  SN1993J      08 41 36  50.2  10.2 -1.2    -154.8    -2   2  1  11867  23 27 50
23 29 50  ---          08 43 37  50.2  10.0 -1.2    -155.4   118   F  1  13467

23 29 50  M81          08 43 37  50.2  10.0 -1.2    -155.4    -2   2  1  13467  23 29 50
23 31 00  ---          08 44 47  50.2   9.8 -1.2    -155.8    68   F  1  14400

23 31 00  SN1993J      08 44 47  50.3   9.8 -1.2    -155.8    -2   2  1  14400  23 31 00
23 33 00  ---          08 46 47  50.4   9.6 -1.1    -156.5   118   F  1  16000

23 33 00  M81          08 46 47  50.3   9.5 -1.1    -156.5    -2   2  1  16000  23 33 00
23 35 00  ---          08 48 47  50.4   9.3 -1.1    -157.1   118   F  1  17600

23 50 00  M81          09 03 50  50.9   7.3 -0.9    -162.2   897   2  2  17600  23 50 00
23 52 10  ---          09 06 00  50.9   7.0 -0.8    -162.9   130   R  1  15867

23 52 10  SN1993J      09 06 00  51.0   7.0 -0.8    -163.0    -2   2  2  15867  23 52 10
23 54 10  ---          09 08 01  51.0   6.7 -0.8    -163.6   118   R  1  14267

23 54 10  M81          09 08 01  51.0   6.7 -0.8    -163.6    -2   2  2  14267  23 54 10
23 55 20  ---          09 09 11  51.0   6.6 -0.8    -164.0    68   R  1  13333
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Fri  24 May 2002   Day 144 ---

23 55 20  SN1993J      09 09 11  51.0   6.6 -0.8    -164.0    -2   2  2  13333  23 55 20
23 57 20  ---          09 11 11  51.1   6.3 -0.7    -164.7   118   R  1  11733

23 57 20  M81          09 11 11  51.0   6.3 -0.7    -164.7    -2   2  2  11733  23 57 20
23 58 30  ---          09 12 21  51.1   6.1 -0.7    -165.1    68   R  1  10800

 --- Start: Fri  24 May 2002   Day 144 -- Stop: Sat  25 May 2002   Day 145 ---

23 58 30  SN1993J      09 12 21  51.1   6.1 -0.7    -165.1    -2   2  2  10800  23 58 30
00 00 30  ---          09 14 22  51.2   5.9 -0.7    -165.8   118   R  1   9200

00 00 30  M81          09 14 22  51.1   5.9 -0.7    -165.8    -2   2  2   9200  00 00 30
00 01 40  ---          09 15 32  51.1   5.7 -0.7    -166.2    68   R  1   8267

00 01 40  SN1993J      09 15 32  51.2   5.7 -0.7    -166.2    -2   2  2   8267  00 01 40
00 03 40  ---          09 17 32  51.2   5.4 -0.6    -166.9   118   R  1   6667

00 03 40  M81          09 17 32  51.2   5.4 -0.6    -166.8    -2   2  2   6667  00 03 40
00 04 50  ---          09 18 42  51.2   5.3 -0.6    -167.2    68   R  1   5733

00 04 50  SN1993J      09 18 42  51.3   5.3 -0.6    -167.3    -2   2  2   5733  00 04 50
00 06 50  ---          09 20 43  51.3   5.0 -0.6    -168.0   118   R  1   4133

00 06 50  M81          09 20 43  51.2   5.0 -0.6    -167.9    -2   2  2   4133  00 06 50
00 08 00  ---          09 21 53  51.3   4.8 -0.6    -168.3    68   R  1   3200

00 08 00  SN1993J      09 21 53  51.3   4.8 -0.6    -168.4    -2   2  2   3200  00 08 00
00 10 00  ---          09 23 53  51.3   4.5 -0.5    -169.1   118   R  1   1600

00 10 00  M81          09 23 53  51.3   4.5 -0.5    -169.0    -2   2  2   1600  00 10 00
00 12 00  ---          09 25 53  51.3   4.3 -0.5    -169.7   118   R  1      0

00 27 00  M81          09 40 56  51.5   2.1 -0.2    -174.9   897   2  3      0  00 27 00
00 29 10  ---          09 43 06  51.5   1.8 -0.2    -175.6   130   F  1   1733

00 29 10  SN1993J      09 43 06  51.6   1.8 -0.2    -175.7    -2   2  3   1733  00 29 10
00 31 10  ---          09 45 07  51.6   1.5 -0.2    -176.4   118   F  1   3333

00 31 10  M81          09 45 07  51.5   1.5 -0.2    -176.3    -2   2  3   3333  00 31 10
00 32 20  ---          09 46 17  51.6   1.4 -0.2    -176.7    68   F  1   4267

00 32 20  SN1993J      09 46 17  51.6   1.3 -0.2    -176.8    -2   2  3   4267  00 32 20
00 34 20  ---          09 48 17  51.6   1.1 -0.1    -177.5   118   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

00 34 20  M81          09 48 17  51.6   1.1 -0.1    -177.4    -2   2  3   5867  00 34 20
00 35 30  ---          09 49 27  51.6   0.9 -0.1    -177.8    68   F  1   6800

00 35 30  SN1993J      09 49 27  51.6   0.9 -0.1    -177.9    -2   2  3   6800  00 35 30
00 37 30  ---          09 51 28  51.6   0.6 -0.1    -178.6   118   F  1   8400

00 37 30  M81          09 51 28  51.6   0.6 -0.1    -178.5    -2   2  3   8400  00 37 30
00 38 40  ---          09 52 38  51.6   0.4 -0.1    -178.9    68   F  1   9333

00 38 40  SN1993J      09 52 38  51.6   0.4  0.0    -179.0    -2   2  3   9333  00 38 40
00 40 40  ---          09 54 38  51.6   0.1  0.0    -179.7   118   F  1  10933

00 40 40  M81          09 54 38  51.6   0.2  0.0    -179.6    -2   2  3  10933  00 40 40
00 41 50  ---          09 55 48  51.6   0.0  0.0     180.0    68   F  1  11867

00 41 50  SN1993J      09 55 48  51.6   0.0  0.0     179.9    -2   2  3  11867  00 41 50
00 43 50  ---          09 57 49  51.6  -0.3  0.0     179.2   118   F  1  13467

00 43 50  M81          09 57 49  51.6  -0.3  0.0     179.3    -2   2  3  13467  00 43 50
00 45 00  ---          09 58 59  51.6  -0.5  0.1     178.9    68   F  1  14400

00 45 00  SN1993J      09 58 59  51.6  -0.5  0.1     178.8    -2   2  3  14400  00 45 00
00 47 00  ---          10 00 59  51.6  -0.8  0.1     178.1   118   F  1  16000

00 47 00  M81          10 00 59  51.6  -0.8  0.1     178.2    -2   2  3  16000  00 47 00
00 49 00  ---          10 03 00  51.6  -1.0  0.1     177.5   118   F  1  17600

00 54 00  OQ208        10 08 00  38.6  76.4 -4.0     -72.0   246   2  4  17600  00 54 00
00 56 10  ---          10 10 11  39.0  76.6 -3.9     -72.1   130   R  1  15867

00 56 10  M81          10 10 11  51.5  -2.1  0.2     175.0   -54   2  4  15867  00 56 10
00 59 20  ---          10 13 21  51.5  -2.5  0.3     173.9   136   R  1  13333

00 59 20  SN1993J      10 13 21  51.5  -2.6  0.3     173.8    -2   2  4  13333  00 59 20
01 01 20  ---          10 15 22  51.5  -2.8  0.3     173.2   118   R  1  11733

01 01 20  M81          10 15 22  51.5  -2.8  0.3     173.2    -2   2  4  11733  01 01 20
01 02 30  ---          10 16 32  51.5  -3.0  0.3     172.8    68   R  1  10800

01 02 30  SN1993J      10 16 32  51.5  -3.0  0.3     172.8    -2   2  4  10800  01 02 30
01 04 30  ---          10 18 32  51.5  -3.3  0.4     172.1   118   R  1   9200
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

01 04 30  M81          10 18 32  51.4  -3.3  0.4     172.1    -2   2  4   9200  01 04 30
01 05 40  ---          10 19 42  51.4  -3.4  0.4     171.7    68   R  1   8267

01 05 40  SN1993J      10 19 42  51.5  -3.5  0.4     171.7    -2   2  4   8267  01 05 40
01 07 40  ---          10 21 43  51.4  -3.7  0.4     171.0   118   R  1   6667

01 07 40  M81          10 21 43  51.4  -3.7  0.4     171.0    -2   2  4   6667  01 07 40
01 08 50  ---          10 22 53  51.4  -3.9  0.5     170.6    68   R  1   5733

01 08 50  SN1993J      10 22 53  51.4  -3.9  0.5     170.6    -2   2  4   5733  01 08 50
01 10 50  ---          10 24 53  51.4  -4.2  0.5     169.9   118   R  1   4133

01 10 50  M81          10 24 53  51.3  -4.2  0.5     169.9    -2   2  4   4133  01 10 50
01 12 00  ---          10 26 03  51.3  -4.3  0.5     169.5    68   R  1   3200

01 12 00  SN1993J      10 26 03  51.4  -4.4  0.5     169.5    -2   2  4   3200  01 12 00
01 14 00  ---          10 28 04  51.3  -4.6  0.5     168.8   118   R  1   1600

01 14 00  M81          10 28 04  51.3  -4.6  0.5     168.8    -2   2  4   1600  01 14 00
01 16 00  ---          10 30 04  51.3  -4.9  0.6     168.2   118   R  1      0

01 19 00  M81          10 33 04  51.2  -5.3  0.6     167.1   178   2  5      0  01 19 00
01 21 10  ---          10 35 15  51.2  -5.6  0.7     166.4   130   F  1   1733

01 21 10  SN1993J      10 35 15  51.2  -5.6  0.7     166.3    -2   2  5   1733  01 21 10
01 23 10  ---          10 37 15  51.2  -5.9  0.7     165.6   118   F  1   3333

01 23 10  M81          10 37 15  51.1  -5.9  0.7     165.7    -2   2  5   3333  01 23 10
01 24 20  ---          10 38 25  51.1  -6.1  0.7     165.3    68   F  1   4267

01 24 20  SN1993J      10 38 25  51.1  -6.1  0.7     165.2    -2   2  5   4267  01 24 20
01 26 20  ---          10 40 26  51.1  -6.4  0.7     164.6   118   F  1   5867

01 26 20  M81          10 40 26  51.0  -6.3  0.7     164.6    -2   2  5   5867  01 26 20
01 27 30  ---          10 41 36  51.0  -6.5  0.8     164.2    68   F  1   6800

01 27 30  SN1993J      10 41 36  51.1  -6.5  0.8     164.2    -2   2  5   6800  01 27 30
01 29 30  ---          10 43 36  51.0  -6.8  0.8     163.5   118   F  1   8400

01 29 30  M81          10 43 36  51.0  -6.8  0.8     163.5    -2   2  5   8400  01 29 30
01 30 40  ---          10 44 46  50.9  -6.9  0.8     163.1    68   F  1   9333
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

01 30 40  SN1993J      10 44 46  51.0  -7.0  0.8     163.1    -2   2  5   9333  01 30 40
01 32 40  ---          10 46 47  50.9  -7.2  0.9     162.4   118   F  1  10933

01 32 40  M81          10 46 47  50.9  -7.2  0.9     162.5    -2   2  5  10933  01 32 40
01 33 50  ---          10 47 57  50.8  -7.3  0.9     162.1    68   F  1  11867

01 33 50  SN1993J      10 47 57  50.9  -7.4  0.9     162.0    -2   2  5  11867  01 33 50
01 35 50  ---          10 49 57  50.8  -7.7  0.9     161.3   118   F  1  13467

01 35 50  M81          10 49 57  50.8  -7.6  0.9     161.4    -2   2  5  13467  01 35 50
01 37 00  ---          10 51 07  50.8  -7.8  0.9     161.0    68   F  1  14400

01 37 00  SN1993J      10 51 07  50.8  -7.8  0.9     160.9    -2   2  5  14400  01 37 00
01 39 00  ---          10 53 08  50.7  -8.1  1.0     160.3   118   F  1  16000

01 39 00  M81          10 53 08  50.7  -8.0  1.0     160.3    -2   2  5  16000  01 39 00
01 41 00  ---          10 55 08  50.6  -8.3  1.0     159.6   118   F  1  17600

01 44 00  M81          10 58 09  50.5  -8.7  1.0     158.6   178   2  6  17600  01 44 00
01 46 10  ---          11 00 19  50.5  -9.0  1.1     157.9   130   R  1  15867

01 46 10  SN1993J      11 00 19  50.5  -9.0  1.1     157.8    -2   2  6  15867  01 46 10
01 48 10  ---          11 02 19  50.4  -9.3  1.1     157.2   118   R  1  14267

01 48 10  M81          11 02 19  50.4  -9.2  1.1     157.2    -2   2  6  14267  01 48 10
01 49 20  ---          11 03 29  50.4  -9.4  1.1     156.9    68   R  1  13333

01 49 20  SN1993J      11 03 29  50.4  -9.4  1.1     156.8    -2   2  6  13333  01 49 20
01 51 20  ---          11 05 30  50.3  -9.7  1.2     156.1   118   R  1  11733

01 51 20  M81          11 05 30  50.3  -9.7  1.2     156.2    -2   2  6  11733  01 51 20
01 52 30  ---          11 06 40  50.2  -9.8  1.2     155.8    68   R  1  10800

01 52 30  SN1993J      11 06 40  50.3  -9.8  1.2     155.7    -2   2  6  10800  01 52 30
01 54 30  ---          11 08 40  50.2 -10.1  1.2     155.1   118   R  1   9200

01 54 30  M81          11 08 40  50.2 -10.1  1.2     155.1    -2   2  6   9200  01 54 30
01 55 40  ---          11 09 50  50.1 -10.2  1.2     154.8    68   R  1   8267

01 55 40  SN1993J      11 09 50  50.2 -10.3  1.2     154.7    -2   2  6   8267  01 55 40
01 57 40  ---          11 11 51  50.1 -10.5  1.3     154.0   118   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

01 57 40  M81          11 11 51  50.1 -10.5  1.3     154.1    -2   2  6   6667  01 57 40
01 58 50  ---          11 13 01  50.0 -10.6  1.3     153.7    68   R  1   5733

01 58 50  SN1993J      11 13 01  50.0 -10.7  1.3     153.6    -2   2  6   5733  01 58 50
02 00 50  ---          11 15 01  50.0 -10.9  1.3     153.0   118   R  1   4133

02 00 50  M81          11 15 01  49.9 -10.9  1.3     153.0    -2   2  6   4133  02 00 50
02 02 00  ---          11 16 12  49.9 -11.0  1.3     152.7    68   R  1   3200

02 02 00  SN1993J      11 16 12  49.9 -11.0  1.3     152.6    -2   2  6   3200  02 02 00
02 04 00  ---          11 18 12  49.8 -11.3  1.4     151.9   118   R  1   1600

02 04 00  M81          11 18 12  49.8 -11.2  1.4     152.0    -2   2  6   1600  02 04 00
02 06 00  ---          11 20 12  49.7 -11.5  1.4     151.4   118   R  1      0

02 09 00  M81          11 23 13  49.6 -11.8  1.5     150.4   178   2  7      0  02 09 00
02 11 10  ---          11 25 23  49.5 -12.1  1.5     149.7   130   F  1   1733

02 11 10  SN1993J      11 25 23  49.5 -12.2  1.5     149.6    -2   2  7   1733  02 11 10
02 13 10  ---          11 27 23  49.4 -12.4  1.5     148.9   118   F  1   3333

02 13 10  M81          11 27 23  49.4 -12.3  1.5     149.0    -2   2  7   3333  02 13 10
02 14 20  ---          11 28 34  49.3 -12.5  1.5     148.6    68   F  1   4267

02 14 20  SN1993J      11 28 34  49.4 -12.5  1.5     148.6    -2   2  7   4267  02 14 20
02 16 20  ---          11 30 34  49.3 -12.8  1.6     147.9   118   F  1   5867

02 16 20  M81          11 30 34  49.2 -12.7  1.6     148.0    -2   2  7   5867  02 16 20
02 17 30  ---          11 31 44  49.2 -12.9  1.6     147.6    68   F  1   6800

02 17 30  SN1993J      11 31 44  49.2 -12.9  1.6     147.5    -2   2  7   6800  02 17 30
02 19 30  ---          11 33 44  49.1 -13.1  1.6     146.9   118   F  1   8400

02 19 30  M81          11 33 44  49.1 -13.1  1.6     147.0    -2   2  7   8400  02 19 30
02 20 40  ---          11 34 55  49.0 -13.2  1.7     146.6    68   F  1   9333

02 20 40  SN1993J      11 34 55  49.1 -13.3  1.7     146.5    -2   2  7   9333  02 20 40
02 22 40  ---          11 36 55  49.0 -13.5  1.7     145.9   118   F  1  10933

02 22 40  M81          11 36 55  48.9 -13.4  1.7     146.0    -2   2  7  10933  02 22 40
02 23 50  ---          11 38 05  48.9 -13.6  1.7     145.6    68   F  1  11867
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

02 23 50  SN1993J      11 38 05  48.9 -13.6  1.7     145.5    -2   2  7  11867  02 23 50
02 25 50  ---          11 40 05  48.8 -13.9  1.7     144.9   118   F  1  13467

02 25 50  M81          11 40 05  48.8 -13.8  1.7     145.0    -2   2  7  13467  02 25 50
02 27 00  ---          11 41 16  48.7 -13.9  1.8     144.6    68   F  1  14400

02 27 00  SN1993J      11 41 16  48.7 -14.0  1.8     144.5    -2   2  7  14400  02 27 00
02 29 00  ---          11 43 16  48.6 -14.2  1.8     143.9   118   F  1  16000

02 29 00  M81          11 43 16  48.6 -14.1  1.8     144.0    -2   2  7  16000  02 29 00
02 31 00  ---          11 45 16  48.5 -14.4  1.8     143.3   118   F  1  17600

02 34 00  M81          11 48 17  48.3 -14.7  1.9     142.4   178   2  8  17600  02 34 00
02 36 10  ---          11 50 27  48.2 -14.9  1.9     141.7   130   R  1  15867

02 36 10  SN1993J      11 50 27  48.2 -15.0  1.9     141.6    -2   2  8  15867  02 36 10
02 38 10  ---          11 52 27  48.1 -15.2  1.9     141.0   118   R  1  14267

02 38 10  M81          11 52 27  48.1 -15.1  1.9     141.1    -2   2  8  14267  02 38 10
02 39 20  ---          11 53 38  48.0 -15.2  2.0     140.7    68   R  1  13333

02 39 20  SN1993J      11 53 38  48.1 -15.3  2.0     140.6    -2   2  8  13333  02 39 20
02 41 20  ---          11 55 38  48.0 -15.5  2.0     140.0   118   R  1  11733

02 41 20  M81          11 55 38  47.9 -15.5  2.0     140.1    -2   2  8  11733  02 41 20
02 42 30  ---          11 56 48  47.9 -15.6  2.0     139.7    68   R  1  10800

02 42 30  SN1993J      11 56 48  47.9 -15.6  2.0     139.7    -2   2  8  10800  02 42 30
02 44 30  ---          11 58 48  47.8 -15.8  2.1     139.0   118   R  1   9200

02 44 30  M81          11 58 48  47.7 -15.8  2.1     139.1    -2   2  8   9200  02 44 30
02 45 40  ---          11 59 59  47.7 -15.9  2.1     138.7    68   R  1   8267

02 45 40  SN1993J      11 59 59  47.7 -16.0  2.1     138.7    -2   2  8   8267  02 45 40
02 47 40  ---          12 01 59  47.6 -16.2  2.1     138.1   118   R  1   6667

02 47 40  M81          12 01 59  47.6 -16.1  2.1     138.1    -2   2  8   6667  02 47 40
02 48 50  ---          12 03 09  47.5 -16.2  2.1     137.8    68   R  1   5733

02 48 50  SN1993J      12 03 09  47.5 -16.3  2.1     137.7    -2   2  8   5733  02 48 50
02 50 50  ---          12 05 10  47.4 -16.5  2.2     137.1   118   R  1   4133
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

02 50 50  M81          12 05 10  47.4 -16.4  2.2     137.2    -2   2  8   4133  02 50 50
02 52 00  ---          12 06 20  47.3 -16.5  2.2     136.8    68   R  1   3200

02 52 00  SN1993J      12 06 20  47.3 -16.6  2.2     136.7    -2   2  8   3200  02 52 00
02 54 00  ---          12 08 20  47.2 -16.8  2.2     136.1   118   R  1   1600

02 54 00  M81          12 08 20  47.2 -16.7  2.2     136.2    -2   2  8   1600  02 54 00
02 56 00  ---          12 10 20  47.0 -16.9  2.2     135.6   118   R  1      0

03 01 00  0954+658     12 15 21  49.3 -20.9  2.3     132.2   293   2  9      0  03 01 00
03 04 00  ---          12 18 22  49.1 -21.2  2.3     131.3   180   F  1   2400

03 04 00  M81          12 18 22  46.5 -17.6  2.4     133.2    -7   2  9   2400  03 04 00
03 06 20  ---          12 20 42  46.4 -17.8  2.4     132.5   133   F  1   4267

03 06 20  SN1993J      12 20 42  46.4 -17.9  2.4     132.4    -2   2  9   4267  03 06 20
03 08 20  ---          12 22 42  46.3 -18.1  2.5     131.8   118   F  1   5867

03 08 20  M81          12 22 42  46.2 -18.0  2.4     131.9    -2   2  9   5867  03 08 20
03 09 30  ---          12 23 53  46.2 -18.1  2.5     131.5    68   F  1   6800

03 09 30  SN1993J      12 23 53  46.2 -18.2  2.5     131.5    -2   2  9   6800  03 09 30
03 11 30  ---          12 25 53  46.1 -18.3  2.5     130.9   118   F  1   8400

03 11 30  M81          12 25 53  46.0 -18.3  2.5     131.0    -2   2  9   8400  03 11 30
03 12 40  ---          12 27 03  46.0 -18.4  2.5     130.6    68   F  1   9333

03 12 40  SN1993J      12 27 03  46.0 -18.4  2.5     130.5    -2   2  9   9333  03 12 40
03 14 40  ---          12 29 03  45.8 -18.6  2.6     129.9   118   F  1  10933

03 14 40  M81          12 29 03  45.8 -18.5  2.6     130.0    -2   2  9  10933  03 14 40
03 15 50  ---          12 30 14  45.7 -18.6  2.6     129.7    68   F  1  11867

03 15 50  SN1993J      12 30 14  45.8 -18.7  2.6     129.6    -2   2  9  11867  03 15 50
03 17 50  ---          12 32 14  45.6 -18.9  2.6     129.0   118   F  1  13467

03 17 50  M81          12 32 14  45.6 -18.8  2.6     129.1    -2   2  9  13467  03 17 50
03 19 00  ---          12 33 24  45.5 -18.9  2.6     128.8    68   F  1  14400

03 19 00  SN1993J      12 33 24  45.5 -19.0  2.6     128.7    -2   2  9  14400  03 19 00
03 21 00  ---          12 35 24  45.4 -19.1  2.7     128.1   118   F  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

03 21 00  M81          12 35 24  45.4 -19.1  2.7     128.2    -2   2  9  16000  03 21 00
03 23 00  ---          12 37 25  45.2 -19.2  2.7     127.6   118   F  1  17600

03 26 00  M81          12 40 25  45.0 -19.4  2.7     126.7   178   2 10  17600  03 26 00
03 28 10  ---          12 42 36  44.9 -19.6  2.8     126.1   130   R  1  15867

03 28 10  SN1993J      12 42 36  44.9 -19.7  2.8     126.0    -2   2 10  15867  03 28 10
03 30 10  ---          12 44 36  44.7 -19.8  2.8     125.5   118   R  1  14267

03 30 10  M81          12 44 36  44.7 -19.8  2.8     125.5    -2   2 10  14267  03 30 10
03 31 20  ---          12 45 46  44.6 -19.8  2.8     125.2    68   R  1  13333

03 31 20  SN1993J      12 45 46  44.6 -19.9  2.8     125.1    -2   2 10  13333  03 31 20
03 33 20  ---          12 47 47  44.5 -20.0  2.9     124.6   118   R  1  11733

03 33 20  M81          12 47 47  44.5 -20.0  2.9     124.6    -2   2 10  11733  03 33 20
03 34 30  ---          12 48 57  44.4 -20.1  2.9     124.3    68   R  1  10800

03 34 30  SN1993J      12 48 57  44.4 -20.1  2.9     124.2    -2   2 10  10800  03 34 30
03 36 30  ---          12 50 57  44.3 -20.3  2.9     123.7   118   R  1   9200

03 36 30  M81          12 50 57  44.3 -20.2  2.9     123.7    -2   2 10   9200  03 36 30
03 37 40  ---          12 52 07  44.2 -20.3  2.9     123.4    68   R  1   8267

03 37 40  SN1993J      12 52 07  44.2 -20.3  2.9     123.3    -2   2 10   8267  03 37 40
03 39 40  ---          12 54 08  44.0 -20.5  3.0     122.8   118   R  1   6667

03 39 40  M81          12 54 08  44.0 -20.4  3.0     122.8    -2   2 10   6667  03 39 40
03 40 50  ---          12 55 18  43.9 -20.5  3.0     122.5    68   R  1   5733

03 40 50  SN1993J      12 55 18  43.9 -20.6  3.0     122.4    -2   2 10   5733  03 40 50
03 42 50  ---          12 57 18  43.8 -20.7  3.0     121.9   118   R  1   4133

03 42 50  M81          12 57 18  43.8 -20.6  3.0     122.0    -2   2 10   4133  03 42 50
03 44 00  ---          12 58 28  43.7 -20.7  3.0     121.6    68   R  1   3200

03 44 00  SN1993J      12 58 28  43.7 -20.8  3.0     121.6    -2   2 10   3200  03 44 00
03 46 00  ---          13 00 29  43.5 -20.9  3.1     121.0   118   R  1   1600

03 46 00  M81          13 00 29  43.5 -20.8  3.1     121.1    -2   2 10   1600  03 46 00
03 48 00  ---          13 02 29  43.4 -21.0  3.1     120.5   118   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

03 53 00  OQ208        13 07 30  76.9  95.8 -1.0     -76.8   220   2 11      0  03 53 00
03 55 10  ---          13 09 40  77.3  96.3 -1.0     -76.6   130   F  1   1733

03 55 10  M81          13 09 40  42.8 -21.4  3.2     118.5   -80   2 11   1733  03 55 10
03 58 20  ---          13 12 51  42.6 -21.6  3.3     117.7   110   F  1   4267

03 58 20  SN1993J      13 12 51  42.6 -21.6  3.3     117.6    -2   2 11   4267  03 58 20
04 00 20  ---          13 14 51  42.4 -21.8  3.3     117.1   118   F  1   5867

04 00 20  M81          13 14 51  42.4 -21.7  3.3     117.1    -2   2 11   5867  04 00 20
04 01 30  ---          13 16 01  42.3 -21.8  3.3     116.8    68   F  1   6800

04 01 30  SN1993J      13 16 01  42.3 -21.8  3.3     116.7    -2   2 11   6800  04 01 30
04 03 30  ---          13 18 01  42.2 -21.9  3.4     116.2   118   F  1   8400

04 03 30  M81          13 18 01  42.2 -21.9  3.4     116.3    -2   2 11   8400  04 03 30
04 04 40  ---          13 19 12  42.1 -21.9  3.4     116.0    68   F  1   9333

04 04 40  SN1993J      13 19 12  42.1 -22.0  3.4     115.9    -2   2 11   9333  04 04 40
04 06 40  ---          13 21 12  41.9 -22.1  3.4     115.4   118   F  1  10933

04 06 40  M81          13 21 12  41.9 -22.0  3.4     115.4    -2   2 11  10933  04 06 40
04 07 50  ---          13 22 22  41.8 -22.1  3.4     115.1    68   F  1  11867

04 07 50  SN1993J      13 22 22  41.8 -22.2  3.4     115.0    -2   2 11  11867  04 07 50
04 09 50  ---          13 24 23  41.7 -22.3  3.5     114.5   118   F  1  13467

04 09 50  M81          13 24 23  41.6 -22.2  3.5     114.6    -2   2 11  13467  04 09 50
04 11 00  ---          13 25 33  41.6 -22.3  3.5     114.3    68   F  1  14400

04 11 00  SN1993J      13 25 33  41.6 -22.3  3.5     114.2    -2   2 11  14400  04 11 00
04 13 00  ---          13 27 33  41.4 -22.4  3.5     113.7   118   F  1  16000

04 13 00  M81          13 27 33  41.4 -22.3  3.5     113.7    -2   2 11  16000  04 13 00
04 15 00  ---          13 29 33  41.2 -22.4  3.6     113.2   118   F  1  17600

04 18 00  M81          13 32 34  41.0 -22.6  3.6     112.4   178   2 12  17600  04 18 00
04 20 10  ---          13 34 44  40.8 -22.7  3.7     111.8   130   R  1  15867

04 20 10  SN1993J      13 34 44  40.8 -22.7  3.7     111.8    -2   2 12  15867  04 20 10
04 22 10  ---          13 36 45  40.6 -22.8  3.7     111.2   118   R  1  14267
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

04 22 10  M81          13 36 45  40.6 -22.8  3.7     111.3    -2   2 12  14267  04 22 10
04 23 20  ---          13 37 55  40.5 -22.8  3.7     111.0    68   R  1  13333

04 23 20  SN1993J      13 37 55  40.5 -22.9  3.7     110.9    -2   2 12  13333  04 23 20
04 25 20  ---          13 39 55  40.4 -23.0  3.7     110.4   118   R  1  11733

04 25 20  M81          13 39 55  40.4 -22.9  3.7     110.5    -2   2 12  11733  04 25 20
04 26 30  ---          13 41 05  40.3 -22.9  3.8     110.2    68   R  1  10800

04 26 30  SN1993J      13 41 05  40.3 -23.0  3.8     110.1    -2   2 12  10800  04 26 30
04 28 30  ---          13 43 06  40.1 -23.1  3.8     109.6   118   R  1   9200

04 28 30  M81          13 43 06  40.1 -23.0  3.8     109.7    -2   2 12   9200  04 28 30
04 29 40  ---          13 44 16  40.0 -23.1  3.8     109.4    68   R  1   8267

04 29 40  SN1993J      13 44 16  40.0 -23.1  3.8     109.3    -2   2 12   8267  04 29 40
04 31 40  ---          13 46 16  39.8 -23.2  3.8     108.8   118   R  1   6667

04 31 40  M81          13 46 16  39.8 -23.1  3.8     108.8    -2   2 12   6667  04 31 40
04 32 50  ---          13 47 26  39.7 -23.2  3.9     108.5    68   R  1   5733

04 32 50  SN1993J      13 47 26  39.7 -23.3  3.9     108.5    -2   2 12   5733  04 32 50
04 34 50  ---          13 49 27  39.6 -23.3  3.9     108.0   118   R  1   4133

04 34 50  M81          13 49 27  39.6 -23.3  3.9     108.0    -2   2 12   4133  04 34 50
04 36 00  ---          13 50 37  39.5 -23.3  3.9     107.7    68   R  1   3200

04 36 00  SN1993J      13 50 37  39.5 -23.4  3.9     107.7    -2   2 12   3200  04 36 00
04 38 00  ---          13 52 37  39.3 -23.4  4.0     107.1   118   R  1   1600

04 38 00  M81          13 52 37  39.3 -23.4  3.9     107.2    -2   2 12   1600  04 38 00
04 40 00  ---          13 54 37  39.1 -23.4  4.0     106.7   118   R  1      0

04 43 00  M81          13 57 38  38.9 -23.5  4.0     105.9   177   2 13      0  04 43 00
04 45 10  ---          13 59 48  38.7 -23.6  4.1     105.4   130   F  1   1733

04 45 10  SN1993J      13 59 48  38.7 -23.7  4.1     105.3    -2   2 13   1733  04 45 10
04 47 10  ---          14 01 49  38.5 -23.7  4.1     104.8   118   F  1   3333

04 47 10  M81          14 01 49  38.5 -23.7  4.1     104.9    -2   2 13   3333  04 47 10
04 48 20  ---          14 02 59  38.4 -23.7  4.1     104.6    68   F  1   4267
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

04 48 20  SN1993J      14 02 59  38.4 -23.8  4.1     104.5    -2   2 13   4267  04 48 20
04 50 20  ---          14 04 59  38.2 -23.8  4.2     104.0   118   F  1   5867

04 50 20  M81          14 04 59  38.2 -23.8  4.2     104.1    -2   2 13   5867  04 50 20
04 51 30  ---          14 06 09  38.1 -23.8  4.2     103.8    68   F  1   6800

04 51 30  SN1993J      14 06 09  38.1 -23.8  4.2     103.7    -2   2 13   6800  04 51 30
04 53 30  ---          14 08 10  37.9 -23.9  4.2     103.2   118   F  1   8400

04 53 30  M81          14 08 10  38.0 -23.8  4.2     103.3    -2   2 13   8400  04 53 30
04 54 40  ---          14 09 20  37.8 -23.9  4.2     103.0    68   F  1   9333

04 54 40  SN1993J      14 09 20  37.8 -23.9  4.2     102.9    -2   2 13   9333  04 54 40
04 56 40  ---          14 11 20  37.7 -24.0  4.3     102.4   118   F  1  10933

04 56 40  M81          14 11 20  37.7 -23.9  4.3     102.5    -2   2 13  10933  04 56 40
04 57 50  ---          14 12 30  37.6 -24.0  4.3     102.2    68   F  1  11867

04 57 50  SN1993J      14 12 30  37.6 -24.0  4.3     102.1    -2   2 13  11867  04 57 50
04 59 50  ---          14 14 31  37.4 -24.1  4.3     101.6   118   F  1  13467

04 59 50  M81          14 14 31  37.4 -24.0  4.3     101.7    -2   2 13  13467  04 59 50
05 01 00  ---          14 15 41  37.3 -24.0  4.3     101.4    68   F  1  14400

05 01 00  SN1993J      14 15 41  37.3 -24.1  4.3     101.4    -2   2 13  14400  05 01 00
05 03 00  ---          14 17 41  37.1 -24.1  4.4     100.9   118   F  1  16000

05 03 00  M81          14 17 41  37.1 -24.1  4.4     100.9    -2   2 13  16000  05 03 00
05 05 00  ---          14 19 42  36.9 -24.1  4.4     100.4   118   F  1  17600

05 08 00  M81          14 22 42  36.7 -24.2  4.4      99.7   177   2 14  17600  05 08 00
05 10 10  ---          14 24 52  36.5 -24.2  4.5      99.2   130   R  1  15867

05 10 10  SN1993J      14 24 52  36.5 -24.3  4.5      99.1    -2   2 14  15867  05 10 10
05 12 10  ---          14 26 53  36.3 -24.3  4.5      98.6   118   R  1  14267

05 12 10  M81          14 26 53  36.3 -24.2  4.5      98.7    -2   2 14  14267  05 12 10
05 13 20  ---          14 28 03  36.2 -24.3  4.5      98.4    68   R  1  13333

05 13 20  SN1993J      14 28 03  36.2 -24.3  4.5      98.3    -2   2 14  13333  05 13 20
05 15 20  ---          14 30 03  36.0 -24.3  4.6      97.8   118   R  1  11733
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  25 May 2002   Day 145 ---

05 15 20  M81          14 30 03  36.0 -24.3  4.6      97.9    -2   2 14  11733  05 15 20
05 16 30  ---          14 31 13  35.9 -24.3  4.6      97.6    68   R  1  10800

05 16 30  SN1993J      14 31 13  35.9 -24.4  4.6      97.6    -2   2 14  10800  05 16 30
05 18 30  ---          14 33 14  35.7 -24.4  4.6      97.1   118   R  1   9200

05 18 30  M81          14 33 14  35.7 -24.3  4.6      97.1    -2   2 14   9200  05 18 30
05 19 40  ---          14 34 24  35.6 -24.4  4.6      96.9    68   R  1   8267

05 19 40  SN1993J      14 34 24  35.6 -24.4  4.6      96.8    -2   2 14   8267  05 19 40
05 21 40  ---          14 36 24  35.5 -24.4  4.7      96.3   118   R  1   6667

05 21 40  M81          14 36 24  35.5 -24.4  4.7      96.4    -2   2 14   6667  05 21 40
05 22 50  ---          14 37 34  35.4 -24.4  4.7      96.1    68   R  1   5733

05 22 50  SN1993J      14 37 34  35.4 -24.4  4.7      96.0    -2   2 14   5733  05 22 50
05 24 50  ---          14 39 35  35.2 -24.5  4.7      95.6   118   R  1   4133

05 24 50  M81          14 39 35  35.2 -24.4  4.7      95.6    -2   2 14   4133  05 24 50
05 26 00  ---          14 40 45  35.1 -24.4  4.8      95.3    68   R  1   3200

05 26 00  SN1993J      14 40 45  35.1 -24.5  4.8      95.3    -2   2 14   3200  05 26 00
05 28 00  ---          14 42 45  34.9 -24.5  4.8      94.8   118   R  1   1600

05 28 00  M81          14 42 45  34.9 -24.4  4.8      94.9    -2   2 14   1600  05 28 00
05 30 00  ---          14 44 46  34.7 -24.5  4.8      94.4   118   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/sched.01jul99/setups/v6cm-256-8-2-UL.set
   Matches group v6cm_2 in /usr/local/sched.01jul99/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00  4100.00
   Net SB=        L        L        U        U        L        L        U        U
   Pol.  =     RCP      LCP      RCP      LCP      RCP      LCP      RCP      LCP 
   BBC   =        1        2        1        2        3        4        3        4
   BBC SB=        L        L        U        U        L        L        U        U
   IF    =       A        C        A        C        A        C        A        C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=   4979.49  4979.49  4979.49  4979.49  4995.49  4995.49  4995.49  4995.49
   BBC fr=    879.49   879.49   879.49   879.49   895.49   895.49   895.49   895.49
   Bandwd=     8.000    8.000    8.000    8.000    8.000    8.000    8.000    8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   510   490   510  6490  6510  6490  6510
    PCALFR2=   490   510   490   510  6490  6510  6490  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- 30rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SN1993J           09 51 19.038889   * 09 55 24.774900     09 55 34.565398 
                     69 15 26.46784    * 69 01 13.70300      69 00 56.72454 
                     From catalog imbedded in main SCHED input file.

 * M81               09 51 27.310854   * 09 55 33.173100     09 55 42.970605 
                     69 18 08.14534    * 69 03 55.06200      69 03 38.07920 
                     From catalog imbedded in main SCHED input file.

 * 0954+658          09 54 57.847119   * 09 58 47.244300     09 58 56.449032 
                     65 48 15.53178    * 65 33 54.81100      65 33 36.86534 
                     From catalog imbedded in main SCHED input file.

   J1407+2827        14 04 45.615152   * 14 07 00.394411     14 07 07.194363 
   1404+286          28 41 29.23491    * 28 27 14.68994      28 26 41.05558 
   J1407+28          /usr/local/sched.01jul99/catalogs/sources.vlba
 * OQ208             USNO - Ref Frame 1998-6, Eubanks June 1998



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1993J             69.6
   M81                 69.6
   0954+658            70.3
   OQ208              122.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

