  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
 Exp. Code:  GB049A  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 02 July 2002                       

PI:       N. Bartel, M.P. Rupen                                           

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@yorku.ca                                                 
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 256-8-2-ul 6cm                                       

Notes:    Fringe finder  : 0954+658                                       
          Pol. Calibrator: 0954+658, OQ208                                
          Amplitude check: 0954+658, OQ208                                
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

 Next scan frequencies:  4979.49  4979.49  4979.49  4979.49  4995.49  4995.49
                         4995.49  4995.49
 Next BBC frequencies:    879.49   879.49   879.49   879.49   895.49   895.49
                          895.49   895.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

19 08 32  0954+658     04 27 34  30.5  28.5 -5.5     -82.4     0   1  1      0  19 08 32
19 11 32  ---          04 30 35  30.8  28.5 -5.5     -83.1   180   F  1   2400

19 11 32  M81          04 30 35  31.5  24.5 -5.4     -85.9    -9   1  1   2400  19 11 32
19 13 52  ---          04 32 55  31.7  24.5 -5.4     -86.4   131   F  1   4267

19 13 52  SN1993J      04 32 55  31.7  24.6 -5.4     -86.4    -6   1  1   4267  19 13 52
19 15 52  ---          04 34 55  31.9  24.6 -5.3     -86.9   114   F  1   5867

19 15 52  M81          04 34 55  31.9  24.5 -5.3     -86.9    -6   1  1   5867  19 15 52
19 17 02  ---          04 36 06  32.0  24.5 -5.3     -87.2    64   F  1   6800

19 17 02  SN1993J      04 36 06  32.0  24.6 -5.3     -87.2    -6   1  1   6800  19 17 02
19 19 02  ---          04 38 06  32.2  24.6 -5.3     -87.6   114   F  1   8400

19 19 02  M81          04 38 06  32.2  24.5 -5.3     -87.6    -6   1  1   8400  19 19 02
19 20 12  ---          04 39 16  32.3  24.5 -5.3     -87.9    64   F  1   9333

19 20 12  SN1993J      04 39 16  32.3  24.6 -5.3     -87.9    -6   1  1   9333  19 20 12
19 22 12  ---          04 41 16  32.4  24.6 -5.2     -88.4   114   F  1  10933

19 22 12  M81          04 41 16  32.4  24.5 -5.2     -88.4    -6   1  1  10933  19 22 12
19 23 22  ---          04 42 27  32.5  24.5 -5.2     -88.6    64   F  1  11867

19 23 22  SN1993J      04 42 27  32.6  24.6 -5.2     -88.6    -6   1  1  11867  19 23 22
19 25 22  ---          04 44 27  32.7  24.6 -5.2     -89.1   114   F  1  13467

19 25 22  M81          04 44 27  32.7  24.5 -5.2     -89.1    -6   1  1  13467  19 25 22
19 26 32  ---          04 45 37  32.8  24.6 -5.2     -89.4    64   F  1  14400

19 26 32  SN1993J      04 45 37  32.8  24.6 -5.2     -89.4    -6   1  1  14400  19 26 32
19 28 32  ---          04 47 37  33.0  24.6 -5.1     -89.8   114   F  1  16000

19 28 32  M81          04 47 37  33.0  24.6 -5.1     -89.8    -6   1  1  16000  19 28 32
19 30 32  ---          04 49 38  33.2  24.6 -5.1     -90.3   114   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

19 31 12  M81          04 50 18  33.2  24.6 -5.1     -90.5    34   1  2  17600  19 31 12
19 33 22  ---          04 52 28  33.4  24.5 -5.1     -91.0   130   R  1  15867

19 33 22  SN1993J      04 52 28  33.5  24.6 -5.1     -91.0    -6   1  2  15867  19 33 22
19 35 22  ---          04 54 29  33.6  24.6 -5.0     -91.4   114   R  1  14267

19 35 22  M81          04 54 29  33.6  24.5 -5.0     -91.4    -6   1  2  14267  19 35 22
19 36 32  ---          04 55 39  33.7  24.5 -5.0     -91.7    64   R  1  13333

19 36 32  SN1993J      04 55 39  33.7  24.6 -5.0     -91.7    -6   1  2  13333  19 36 32
19 38 32  ---          04 57 39  33.9  24.6 -5.0     -92.2   114   R  1  11733

19 38 32  M81          04 57 39  33.9  24.5 -5.0     -92.2    -6   1  2  11733  19 38 32
19 39 42  ---          04 58 49  34.0  24.5 -5.0     -92.5    64   R  1  10800

19 39 42  SN1993J      04 58 49  34.0  24.6 -4.9     -92.5    -6   1  2  10800  19 39 42
19 41 42  ---          05 00 50  34.2  24.6 -4.9     -92.9   114   R  1   9200

19 41 42  M81          05 00 50  34.2  24.5 -4.9     -92.9    -6   1  2   9200  19 41 42
19 42 52  ---          05 02 00  34.3  24.5 -4.9     -93.2    64   R  1   8267

19 42 52  SN1993J      05 02 00  34.3  24.6 -4.9     -93.2    -6   1  2   8267  19 42 52
19 44 52  ---          05 04 00  34.5  24.6 -4.9     -93.7   114   R  1   6667

19 44 52  M81          05 04 00  34.5  24.5 -4.9     -93.7    -6   1  2   6667  19 44 52
19 46 02  ---          05 05 10  34.6  24.5 -4.8     -94.0    64   R  1   5733

19 46 02  SN1993J      05 05 10  34.6  24.5 -4.8     -94.0    -6   1  2   5733  19 46 02
19 48 02  ---          05 07 11  34.8  24.5 -4.8     -94.4   114   R  1   4133

19 48 02  M81          05 07 11  34.8  24.5 -4.8     -94.4    -6   1  2   4133  19 48 02
19 49 12  ---          05 08 21  34.9  24.5 -4.8     -94.7    64   R  1   3200

19 49 12  SN1993J      05 08 21  34.9  24.5 -4.8     -94.7    -6   1  2   3200  19 49 12
19 51 12  ---          05 10 21  35.1  24.5 -4.8     -95.2   114   R  1   1600

19 51 12  M81          05 10 21  35.0  24.4 -4.8     -95.2    -6   1  2   1600  19 51 12
19 53 12  ---          05 12 21  35.2  24.4 -4.7     -95.7   114   R  1      0

20 03 12  0954+658     05 22 23  36.2  28.6 -4.6     -94.8   591   1  3      0  20 03 12
20 06 12  ---          05 25 24  36.5  28.6 -4.6     -95.5   180   F  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

20 06 12  M81          05 25 24  36.4  24.2 -4.5     -98.8    -9   1  3   2400  20 06 12
20 08 32  ---          05 27 44  36.6  24.2 -4.5     -99.4   131   F  1   4267

20 08 32  SN1993J      05 27 44  36.6  24.3 -4.5     -99.4    -6   1  3   4267  20 08 32
20 10 32  ---          05 29 44  36.8  24.2 -4.4     -99.9   114   F  1   5867

20 10 32  M81          05 29 44  36.8  24.2 -4.4     -99.9    -6   1  3   5867  20 10 32
20 11 42  ---          05 30 54  36.9  24.1 -4.4    -100.2    64   F  1   6800

20 11 42  SN1993J      05 30 54  36.9  24.2 -4.4    -100.2    -6   1  3   6800  20 11 42
20 13 42  ---          05 32 55  37.1  24.2 -4.4    -100.7   114   F  1   8400

20 13 42  M81          05 32 55  37.0  24.1 -4.4    -100.7    -6   1  3   8400  20 13 42
20 14 52  ---          05 34 05  37.1  24.1 -4.4    -101.0    64   F  1   9333

20 14 52  SN1993J      05 34 05  37.2  24.1 -4.4    -101.0    -6   1  3   9333  20 14 52
20 16 52  ---          05 36 05  37.3  24.1 -4.3    -101.5   114   F  1  10933

20 16 52  M81          05 36 05  37.3  24.0 -4.3    -101.5    -6   1  3  10933  20 16 52
20 18 02  ---          05 37 16  37.4  24.0 -4.3    -101.7    64   F  1  11867

20 18 02  SN1993J      05 37 16  37.4  24.1 -4.3    -101.7    -6   1  3  11867  20 18 02
20 20 02  ---          05 39 16  37.6  24.0 -4.3    -102.2   114   F  1  13467

20 20 02  M81          05 39 16  37.6  24.0 -4.3    -102.2    -6   1  3  13467  20 20 02
20 21 12  ---          05 40 26  37.7  23.9 -4.3    -102.5    64   F  1  14400

20 21 12  SN1993J      05 40 26  37.7  24.0 -4.3    -102.5    -6   1  3  14400  20 21 12
20 23 12  ---          05 42 26  37.9  23.9 -4.2    -103.0   114   F  1  16000

20 23 12  M81          05 42 26  37.9  23.9 -4.2    -103.0    -6   1  3  16000  20 23 12
20 25 12  ---          05 44 27  38.0  23.8 -4.2    -103.5   114   F  1  17600

20 25 52  M81          05 45 07  38.1  23.8 -4.2    -103.7    34   1  4  17600  20 25 52
20 28 02  ---          05 47 17  38.3  23.8 -4.1    -104.2   130   R  1  15867

20 28 02  SN1993J      05 47 17  38.3  23.8 -4.1    -104.2    -6   1  4  15867  20 28 02
20 30 02  ---          05 49 17  38.5  23.7 -4.1    -104.8   114   R  1  14267

20 30 02  M81          05 49 17  38.5  23.7 -4.1    -104.7    -6   1  4  14267  20 30 02
20 31 12  ---          05 50 28  38.6  23.7 -4.1    -105.0    64   R  1  13333
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

20 31 12  SN1993J      05 50 28  38.6  23.7 -4.1    -105.0    -6   1  4  13333  20 31 12
20 33 12  ---          05 52 28  38.8  23.6 -4.1    -105.6   114   R  1  11733

20 33 12  M81          05 52 28  38.7  23.6 -4.1    -105.5    -6   1  4  11733  20 33 12
20 34 22  ---          05 53 38  38.8  23.6 -4.0    -105.8    64   R  1  10800

20 34 22  SN1993J      05 53 38  38.9  23.6 -4.0    -105.8    -6   1  4  10800  20 34 22
20 36 22  ---          05 55 39  39.0  23.5 -4.0    -106.4   114   R  1   9200

20 36 22  M81          05 55 39  39.0  23.5 -4.0    -106.4    -6   1  4   9200  20 36 22
20 37 32  ---          05 56 49  39.1  23.5 -4.0    -106.7    64   R  1   8267

20 37 32  SN1993J      05 56 49  39.1  23.5 -4.0    -106.7    -6   1  4   8267  20 37 32
20 39 32  ---          05 58 49  39.3  23.4 -3.9    -107.2   114   R  1   6667

20 39 32  M81          05 58 49  39.3  23.4 -4.0    -107.2    -6   1  4   6667  20 39 32
20 40 42  ---          05 59 59  39.4  23.4 -3.9    -107.5    64   R  1   5733

20 40 42  SN1993J      05 59 59  39.4  23.4 -3.9    -107.5    -6   1  4   5733  20 40 42
20 42 42  ---          06 02 00  39.6  23.3 -3.9    -108.0   114   R  1   4133

20 42 42  M81          06 02 00  39.5  23.3 -3.9    -108.0    -6   1  4   4133  20 42 42
20 43 52  ---          06 03 10  39.6  23.2 -3.9    -108.3    64   R  1   3200

20 43 52  SN1993J      06 03 10  39.7  23.3 -3.9    -108.3    -6   1  4   3200  20 43 52
20 45 52  ---          06 05 10  39.8  23.2 -3.8    -108.8   114   R  1   1600

20 45 52  M81          06 05 10  39.8  23.2 -3.8    -108.8    -6   1  4   1600  20 45 52
20 47 52  ---          06 07 10  40.0  23.1 -3.8    -109.3   114   R  1      0

20 48 32  M81          06 07 51  40.0  23.1 -3.8    -109.5    34   1  5      0  20 48 32
20 50 42  ---          06 10 01  40.2  23.0 -3.8    -110.0   130   F  1   1733

20 50 42  SN1993J      06 10 01  40.3  23.0 -3.8    -110.0    -6   1  5   1733  20 50 42
20 52 42  ---          06 12 01  40.4  22.9 -3.7    -110.6   114   F  1   3333

20 52 42  M81          06 12 01  40.4  22.9 -3.7    -110.6    -6   1  5   3333  20 52 42
20 53 52  ---          06 13 11  40.5  22.8 -3.7    -110.9    64   F  1   4267

20 53 52  SN1993J      06 13 11  40.5  22.9 -3.7    -110.9    -6   1  5   4267  20 53 52
20 55 52  ---          06 15 12  40.7  22.8 -3.7    -111.4   114   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

20 55 52  M81          06 15 12  40.7  22.8 -3.7    -111.4    -6   1  5   5867  20 55 52
20 57 02  ---          06 16 22  40.8  22.7 -3.7    -111.7    64   F  1   6800

20 57 02  SN1993J      06 16 22  40.8  22.8 -3.7    -111.7    -6   1  5   6800  20 57 02
20 59 02  ---          06 18 22  41.0  22.7 -3.6    -112.2   114   F  1   8400

20 59 02  M81          06 18 22  40.9  22.6 -3.6    -112.2    -6   1  5   8400  20 59 02
21 00 12  ---          06 19 32  41.0  22.6 -3.6    -112.5    64   F  1   9333

21 00 12  SN1993J      06 19 32  41.0  22.6 -3.6    -112.5    -6   1  5   9333  21 00 12
21 02 12  ---          06 21 33  41.2  22.5 -3.6    -113.1   114   F  1  10933

21 02 12  M81          06 21 33  41.2  22.5 -3.6    -113.1    -6   1  5  10933  21 02 12
21 03 22  ---          06 22 43  41.3  22.4 -3.6    -113.4    64   F  1  11867

21 03 22  SN1993J      06 22 43  41.3  22.5 -3.6    -113.4    -6   1  5  11867  21 03 22
21 05 22  ---          06 24 43  41.5  22.4 -3.5    -113.9   114   F  1  13467

21 05 22  M81          06 24 43  41.4  22.3 -3.5    -113.9    -6   1  5  13467  21 05 22
21 06 32  ---          06 25 53  41.5  22.3 -3.5    -114.2    64   F  1  14400

21 06 32  SN1993J      06 25 53  41.6  22.3 -3.5    -114.2    -6   1  5  14400  21 06 32
21 08 32  ---          06 27 54  41.7  22.2 -3.5    -114.7   114   F  1  16000

21 08 32  M81          06 27 54  41.7  22.2 -3.5    -114.7    -6   1  5  16000  21 08 32
21 10 32  ---          06 29 54  41.9  22.1 -3.4    -115.3   114   F  1  17600

21 11 12  M81          06 30 34  41.9  22.0 -3.4    -115.5    34   1  6  17600  21 11 12
21 13 22  ---          06 32 45  42.1  21.9 -3.4    -116.0   130   R  1  15867

21 13 22  SN1993J      06 32 45  42.1  22.0 -3.4    -116.0    -6   1  6  15867  21 13 22
21 15 22  ---          06 34 45  42.3  21.9 -3.4    -116.6   114   R  1  14267

21 15 22  M81          06 34 45  42.3  21.8 -3.4    -116.6    -6   1  6  14267  21 15 22
21 16 32  ---          06 35 55  42.3  21.8 -3.3    -116.9    64   R  1  13333

21 16 32  SN1993J      06 35 55  42.4  21.8 -3.3    -116.9    -6   1  6  13333  21 16 32
21 18 32  ---          06 37 55  42.5  21.7 -3.3    -117.4   114   R  1  11733

21 18 32  M81          06 37 55  42.5  21.6 -3.3    -117.4    -6   1  6  11733  21 18 32
21 19 42  ---          06 39 06  42.6  21.6 -3.3    -117.8    64   R  1  10800
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

21 19 42  SN1993J      06 39 06  42.6  21.6 -3.3    -117.8    -6   1  6  10800  21 19 42
21 21 42  ---          06 41 06  42.8  21.5 -3.2    -118.3   114   R  1   9200

21 21 42  M81          06 41 06  42.8  21.5 -3.2    -118.3    -6   1  6   9200  21 21 42
21 22 52  ---          06 42 16  42.9  21.4 -3.2    -118.6    64   R  1   8267

21 22 52  SN1993J      06 42 16  42.9  21.4 -3.2    -118.6    -6   1  6   8267  21 22 52
21 24 52  ---          06 44 17  43.0  21.3 -3.2    -119.2   114   R  1   6667

21 24 52  M81          06 44 17  43.0  21.3 -3.2    -119.2    -6   1  6   6667  21 24 52
21 26 02  ---          06 45 27  43.1  21.2 -3.2    -119.5    64   R  1   5733

21 26 02  SN1993J      06 45 27  43.1  21.2 -3.2    -119.5    -6   1  6   5733  21 26 02
21 28 02  ---          06 47 27  43.3  21.1 -3.1    -120.0   114   R  1   4133

21 28 02  M81          06 47 27  43.3  21.1 -3.1    -120.0    -6   1  6   4133  21 28 02
21 29 12  ---          06 48 37  43.3  21.0 -3.1    -120.4    64   R  1   3200

21 29 12  SN1993J      06 48 37  43.4  21.1 -3.1    -120.4    -6   1  6   3200  21 29 12
21 31 12  ---          06 50 38  43.5  20.9 -3.1    -120.9   114   R  1   1600

21 31 12  M81          06 50 38  43.5  20.9 -3.1    -120.9    -6   1  6   1600  21 31 12
21 33 12  ---          06 52 38  43.7  20.8 -3.1    -121.5   114   R  1      0

21 33 52  M81          06 53 18  43.7  20.7 -3.0    -121.7    34   1  7      0  21 33 52
21 36 02  ---          06 55 28  43.9  20.6 -3.0    -122.3   130   F  1   1733

21 36 02  SN1993J      06 55 28  43.9  20.6 -3.0    -122.3    -6   1  7   1733  21 36 02
21 38 02  ---          06 57 29  44.1  20.5 -3.0    -122.8   114   F  1   3333

21 38 02  M81          06 57 29  44.0  20.4 -3.0    -122.8    -6   1  7   3333  21 38 02
21 39 12  ---          06 58 39  44.1  20.4 -3.0    -123.2    64   F  1   4267

21 39 12  SN1993J      06 58 39  44.1  20.4 -3.0    -123.2    -6   1  7   4267  21 39 12
21 41 12  ---          07 00 39  44.3  20.3 -2.9    -123.7   114   F  1   5867

21 41 12  M81          07 00 39  44.3  20.2 -2.9    -123.7    -6   1  7   5867  21 41 12
21 42 22  ---          07 01 49  44.3  20.1 -2.9    -124.1    64   F  1   6800

21 42 22  SN1993J      07 01 49  44.4  20.2 -2.9    -124.1    -6   1  7   6800  21 42 22
21 44 22  ---          07 03 50  44.5  20.0 -2.9    -124.6   114   F  1   8400
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

21 44 22  M81          07 03 50  44.5  20.0 -2.9    -124.6    -6   1  7   8400  21 44 22
21 45 32  ---          07 05 00  44.6  19.9 -2.8    -125.0    64   F  1   9333

21 45 32  SN1993J      07 05 00  44.6  20.0 -2.8    -125.0    -6   1  7   9333  21 45 32
21 47 32  ---          07 07 00  44.8  19.8 -2.8    -125.5   114   F  1  10933

21 47 32  M81          07 07 00  44.7  19.8 -2.8    -125.5    -6   1  7  10933  21 47 32
21 48 42  ---          07 08 10  44.8  19.7 -2.8    -125.9    64   F  1  11867

21 48 42  SN1993J      07 08 10  44.8  19.7 -2.8    -125.9    -6   1  7  11867  21 48 42
21 50 42  ---          07 10 11  45.0  19.6 -2.8    -126.4   114   F  1  13467

21 50 42  M81          07 10 11  45.0  19.5 -2.8    -126.4    -6   1  7  13467  21 50 42
21 51 52  ---          07 11 21  45.0  19.4 -2.7    -126.8    64   F  1  14400

21 51 52  SN1993J      07 11 21  45.1  19.5 -2.7    -126.8    -6   1  7  14400  21 51 52
21 53 52  ---          07 13 21  45.2  19.3 -2.7    -127.4   114   F  1  16000

21 53 52  M81          07 13 21  45.2  19.3 -2.7    -127.3    -6   1  7  16000  21 53 52
21 55 52  ---          07 15 22  45.3  19.1 -2.7    -127.9   114   F  1  17600

22 05 52  0954+658     07 25 23  48.0  22.6 -2.6    -127.0   589   1  8  17600  22 05 52
22 08 52  ---          07 28 24  48.2  22.3 -2.5    -127.9   180   R  1  15200

22 08 52  M81          07 28 24  46.2  18.1 -2.5    -131.7   -10   1  8  15200  22 08 52
22 11 12  ---          07 30 44  46.4  17.9 -2.4    -132.4   130   R  1  13333

22 11 12  SN1993J      07 30 44  46.4  17.9 -2.4    -132.4    -6   1  8  13333  22 11 12
22 13 12  ---          07 32 44  46.5  17.7 -2.4    -133.0   114   R  1  11733

22 13 12  M81          07 32 44  46.5  17.7 -2.4    -133.0    -6   1  8  11733  22 13 12
22 14 22  ---          07 33 55  46.6  17.6 -2.4    -133.4    64   R  1  10800

22 14 22  SN1993J      07 33 55  46.6  17.6 -2.4    -133.4    -6   1  8  10800  22 14 22
22 16 22  ---          07 35 55  46.8  17.4 -2.3    -134.0   114   R  1   9200

22 16 22  M81          07 35 55  46.7  17.4 -2.3    -134.0    -6   1  8   9200  22 16 22
22 17 32  ---          07 37 05  46.8  17.3 -2.3    -134.3    64   R  1   8267

22 17 32  SN1993J      07 37 05  46.8  17.3 -2.3    -134.3    -6   1  8   8267  22 17 32
22 19 32  ---          07 39 05  47.0  17.1 -2.3    -134.9   114   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

22 19 32  M81          07 39 05  46.9  17.1 -2.3    -134.9    -6   1  8   6667  22 19 32
22 20 42  ---          07 40 16  47.0  17.0 -2.3    -135.3    64   R  1   5733

22 20 42  SN1993J      07 40 16  47.0  17.0 -2.3    -135.3    -6   1  8   5733  22 20 42
22 22 42  ---          07 42 16  47.2  16.8 -2.2    -135.9   114   R  1   4133

22 22 42  M81          07 42 16  47.1  16.8 -2.2    -135.9    -6   1  8   4133  22 22 42
22 23 52  ---          07 43 26  47.2  16.7 -2.2    -136.2    64   R  1   3200

22 23 52  SN1993J      07 43 26  47.2  16.7 -2.2    -136.2    -6   1  8   3200  22 23 52
22 25 52  ---          07 45 27  47.3  16.5 -2.2    -136.9   114   R  1   1600

22 25 52  M81          07 45 27  47.3  16.5 -2.2    -136.8    -6   1  8   1600  22 25 52
22 27 52  ---          07 47 27  47.4  16.3 -2.1    -137.5   114   R  1      0

22 28 32  M81          07 48 07  47.5  16.3 -2.1    -137.7    34   1  9      0  22 28 32
22 30 42  ---          07 50 17  47.6  16.0 -2.1    -138.3   130   F  1   1733

22 30 42  SN1993J      07 50 17  47.6  16.1 -2.1    -138.3    -6   1  9   1733  22 30 42
22 32 42  ---          07 52 18  47.8  15.9 -2.1    -139.0   114   F  1   3333

22 32 42  M81          07 52 18  47.7  15.8 -2.1    -138.9    -6   1  9   3333  22 32 42
22 33 52  ---          07 53 28  47.8  15.7 -2.0    -139.3    64   F  1   4267

22 33 52  SN1993J      07 53 28  47.8  15.8 -2.0    -139.3    -6   1  9   4267  22 33 52
22 35 52  ---          07 55 28  47.9  15.5 -2.0    -139.9   114   F  1   5867

22 35 52  M81          07 55 28  47.9  15.5 -2.0    -139.9    -6   1  9   5867  22 35 52
22 37 02  ---          07 56 38  48.0  15.4 -2.0    -140.3    64   F  1   6800

22 37 02  SN1993J      07 56 38  48.0  15.4 -2.0    -140.3    -6   1  9   6800  22 37 02
22 39 02  ---          07 58 39  48.1  15.2 -2.0    -140.9   114   F  1   8400

22 39 02  M81          07 58 39  48.1  15.2 -2.0    -140.9    -6   1  9   8400  22 39 02
22 40 12  ---          07 59 49  48.1  15.1 -1.9    -141.3    64   F  1   9333

22 40 12  SN1993J      07 59 49  48.2  15.1 -1.9    -141.3    -6   1  9   9333  22 40 12
22 42 12  ---          08 01 49  48.3  14.9 -1.9    -141.9   114   F  1  10933

22 42 12  M81          08 01 49  48.3  14.9 -1.9    -141.9    -6   1  9  10933  22 42 12
22 43 22  ---          08 02 59  48.3  14.7 -1.9    -142.3    64   F  1  11867
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

22 43 22  SN1993J      08 02 59  48.4  14.8 -1.9    -142.3    -6   1  9  11867  22 43 22
22 45 22  ---          08 05 00  48.5  14.5 -1.8    -142.9   114   F  1  13467

22 45 22  M81          08 05 00  48.4  14.5 -1.8    -142.9    -6   1  9  13467  22 45 22
22 46 32  ---          08 06 10  48.5  14.4 -1.8    -143.3    64   F  1  14400

22 46 32  SN1993J      08 06 10  48.5  14.4 -1.8    -143.3    -6   1  9  14400  22 46 32
22 48 32  ---          08 08 10  48.6  14.2 -1.8    -143.9   114   F  1  16000

22 48 32  M81          08 08 10  48.6  14.2 -1.8    -143.9    -6   1  9  16000  22 48 32
22 50 32  ---          08 10 11  48.7  14.0 -1.8    -144.5   114   F  1  17600

22 51 12  M81          08 10 51  48.7  13.9 -1.8    -144.7    34   1 10  17600  22 51 12
22 53 22  ---          08 13 01  48.9  13.6 -1.7    -145.4   130   R  1  15867

22 53 22  SN1993J      08 13 01  48.9  13.7 -1.7    -145.4    -6   1 10  15867  22 53 22
22 55 22  ---          08 15 01  49.0  13.4 -1.7    -146.1   114   R  1  14267

22 55 22  M81          08 15 01  49.0  13.4 -1.7    -146.1    -6   1 10  14267  22 55 22
22 56 32  ---          08 16 12  49.0  13.3 -1.7    -146.4    64   R  1  13333

22 56 32  SN1993J      08 16 12  49.1  13.3 -1.7    -146.5    -6   1 10  13333  22 56 32
22 58 32  ---          08 18 12  49.2  13.1 -1.6    -147.1   114   R  1  11733

22 58 32  M81          08 18 12  49.1  13.1 -1.6    -147.1    -6   1 10  11733  22 58 32
22 59 42  ---          08 19 22  49.2  12.9 -1.6    -147.4    64   R  1  10800

22 59 42  SN1993J      08 19 22  49.2  12.9 -1.6    -147.5    -6   1 10  10800  22 59 42
23 01 42  ---          08 21 22  49.3  12.7 -1.6    -148.1   114   R  1   9200

23 01 42  M81          08 21 22  49.3  12.7 -1.6    -148.1    -6   1 10   9200  23 01 42
23 02 52  ---          08 22 33  49.3  12.6 -1.6    -148.5    64   R  1   8267

23 02 52  SN1993J      08 22 33  49.4  12.6 -1.6    -148.5    -6   1 10   8267  23 02 52
23 04 52  ---          08 24 33  49.5  12.3 -1.5    -149.1   114   R  1   6667

23 04 52  M81          08 24 33  49.4  12.3 -1.5    -149.1    -6   1 10   6667  23 04 52
23 06 02  ---          08 25 43  49.5  12.2 -1.5    -149.5    64   R  1   5733

23 06 02  SN1993J      08 25 43  49.5  12.2 -1.5    -149.5    -6   1 10   5733  23 06 02
23 08 02  ---          08 27 43  49.6  12.0 -1.5    -150.2   114   R  1   4133
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

23 08 02  M81          08 27 43  49.6  11.9 -1.5    -150.1    -6   1 10   4133  23 08 02
23 09 12  ---          08 28 54  49.6  11.8 -1.5    -150.5    64   R  1   3200

23 09 12  SN1993J      08 28 54  49.7  11.8 -1.4    -150.5    -6   1 10   3200  23 09 12
23 11 12  ---          08 30 54  49.7  11.6 -1.4    -151.2   114   R  1   1600

23 11 12  M81          08 30 54  49.7  11.6 -1.4    -151.2    -6   1 10   1600  23 11 12
23 13 12  ---          08 32 54  49.8  11.3 -1.4    -151.8   114   R  1      0

23 13 52  M81          08 33 34  49.8  11.2 -1.4    -152.1    34   1 11      0  23 13 52
23 16 02  ---          08 35 45  49.9  11.0 -1.3    -152.8   130   F  1   1733

23 16 02  SN1993J      08 35 45  49.9  11.0 -1.3    -152.8    -6   1 11   1733  23 16 02
23 18 02  ---          08 37 45  50.0  10.7 -1.3    -153.4   114   F  1   3333

23 18 02  M81          08 37 45  50.0  10.7 -1.3    -153.4    -6   1 11   3333  23 18 02
23 19 12  ---          08 38 55  50.0  10.6 -1.3    -153.8    64   F  1   4267

23 19 12  SN1993J      08 38 55  50.1  10.6 -1.3    -153.8    -6   1 11   4267  23 19 12
23 21 12  ---          08 40 56  50.1  10.3 -1.2    -154.5   114   F  1   5867

23 21 12  M81          08 40 56  50.1  10.3 -1.2    -154.5    -6   1 11   5867  23 21 12
23 22 22  ---          08 42 06  50.1  10.2 -1.2    -154.9    64   F  1   6800

23 22 22  SN1993J      08 42 06  50.2  10.2 -1.2    -154.9    -6   1 11   6800  23 22 22
23 24 22  ---          08 44 06  50.3   9.9 -1.2    -155.5   114   F  1   8400

23 24 22  M81          08 44 06  50.2   9.9 -1.2    -155.5    -6   1 11   8400  23 24 22
23 25 32  ---          08 45 16  50.3   9.8 -1.2    -155.9    64   F  1   9333

23 25 32  SN1993J      08 45 16  50.3   9.8 -1.2    -155.9    -6   1 11   9333  23 25 32
23 27 32  ---          08 47 17  50.4   9.5 -1.1    -156.6   114   F  1  10933

23 27 32  M81          08 47 17  50.3   9.5 -1.1    -156.6    -6   1 11  10933  23 27 32
23 28 42  ---          08 48 27  50.4   9.4 -1.1    -157.0    64   F  1  11867

23 28 42  SN1993J      08 48 27  50.4   9.4 -1.1    -157.0    -6   1 11  11867  23 28 42
23 30 42  ---          08 50 27  50.5   9.1 -1.1    -157.7   114   F  1  13467

23 30 42  M81          08 50 27  50.4   9.1 -1.1    -157.6    -6   1 11  13467  23 30 42
23 31 52  ---          08 51 37  50.5   8.9 -1.1    -158.0    64   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

23 31 52  SN1993J      08 51 37  50.5   9.0 -1.1    -158.0    -6   1 11  14400  23 31 52
23 33 52  ---          08 53 38  50.6   8.7 -1.0    -158.7   114   F  1  16000

23 33 52  M81          08 53 38  50.6   8.7 -1.0    -158.7    -6   1 11  16000  23 33 52
23 35 52  ---          08 55 38  50.6   8.4 -1.0    -159.4   114   F  1  17600

23 36 32  M81          08 56 18  50.6   8.3 -1.0    -159.6    34   1 12  17600  23 36 32
23 38 42  ---          08 58 28  50.7   8.0 -1.0    -160.3   130   R  1  15867

23 38 42  SN1993J      08 58 28  50.8   8.1 -1.0    -160.3    -6   1 12  15867  23 38 42
23 40 42  ---          09 00 29  50.8   7.8 -0.9    -161.0   114   R  1  14267

23 40 42  M81          09 00 29  50.8   7.8 -0.9    -161.0    -6   1 12  14267  23 40 42
23 41 52  ---          09 01 39  50.8   7.6 -0.9    -161.4    64   R  1  13333

23 41 52  SN1993J      09 01 39  50.8   7.6 -0.9    -161.4    -6   1 12  13333  23 41 52
23 43 52  ---          09 03 39  50.9   7.4 -0.9    -162.1   114   R  1  11733

23 43 52  M81          09 03 39  50.9   7.4 -0.9    -162.1    -6   1 12  11733  23 43 52
23 45 02  ---          09 04 50  50.9   7.2 -0.9    -162.5    64   R  1  10800

23 45 02  SN1993J      09 04 50  50.9   7.2 -0.8    -162.5    -6   1 12  10800  23 45 02
23 47 02  ---          09 06 50  51.0   6.9 -0.8    -163.2   114   R  1   9200

23 47 02  M81          09 06 50  50.9   6.9 -0.8    -163.1    -6   1 12   9200  23 47 02
23 48 12  ---          09 08 00  51.0   6.8 -0.8    -163.5    64   R  1   8267

23 48 12  SN1993J      09 08 00  51.0   6.8 -0.8    -163.6    -6   1 12   8267  23 48 12
23 50 12  ---          09 10 00  51.1   6.5 -0.8    -164.2   114   R  1   6667

23 50 12  M81          09 10 00  51.0   6.5 -0.8    -164.2    -6   1 12   6667  23 50 12
23 51 22  ---          09 11 11  51.0   6.3 -0.7    -164.6    64   R  1   5733

23 51 22  SN1993J      09 11 11  51.1   6.3 -0.7    -164.6    -6   1 12   5733  23 51 22
23 53 22  ---          09 13 11  51.1   6.1 -0.7    -165.3   114   R  1   4133

23 53 22  M81          09 13 11  51.1   6.1 -0.7    -165.3    -6   1 12   4133  23 53 22
23 54 32  ---          09 14 21  51.1   5.9 -0.7    -165.7    64   R  1   3200

23 54 32  SN1993J      09 14 21  51.2   5.9 -0.7    -165.7    -6   1 12   3200  23 54 32
23 56 32  ---          09 16 21  51.2   5.6 -0.7    -166.4   114   R  1   1600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Tue  25 May 2004   Day 146 ---

23 56 32  M81          09 16 21  51.2   5.6 -0.7    -166.4    -6   1 12   1600  23 56 32
23 58 32  ---          09 18 22  51.2   5.3 -0.6    -167.1   114   R  1      0

 --- Wed  26 May 2004   Day 147 ---

00 08 32  0954+658     09 28 23  54.8   5.5 -0.5    -168.5   587   1 13      0  00 08 32
00 11 32  ---          09 31 24  54.8   5.0 -0.5    -169.6   180   F  1   2400

00 11 32  M81          09 31 24  51.4   3.5 -0.4    -171.5   -13   1 13   2400  00 11 32
00 13 52  ---          09 33 44  51.5   3.2 -0.4    -172.3   127   F  1   4267

00 13 52  SN1993J      09 33 44  51.5   3.2 -0.4    -172.4    -6   1 13   4267  00 13 52
00 15 52  ---          09 35 45  51.5   2.9 -0.3    -173.1   114   F  1   5867

00 15 52  M81          09 35 45  51.5   2.9 -0.3    -173.0    -6   1 13   5867  00 15 52
00 17 02  ---          09 36 55  51.5   2.7 -0.3    -173.4    64   F  1   6800

00 17 02  SN1993J      09 36 55  51.5   2.7 -0.3    -173.5    -6   1 13   6800  00 17 02
00 19 02  ---          09 38 55  51.6   2.4 -0.3    -174.2   114   F  1   8400

00 19 02  M81          09 38 55  51.5   2.4 -0.3    -174.1    -6   1 13   8400  00 19 02
00 20 12  ---          09 40 05  51.5   2.3 -0.3    -174.5    64   F  1   9333

00 20 12  SN1993J      09 40 05  51.6   2.3 -0.3    -174.6    -6   1 13   9333  00 20 12
00 22 12  ---          09 42 06  51.6   2.0 -0.2    -175.3   114   F  1  10933

00 22 12  M81          09 42 06  51.5   2.0 -0.2    -175.2    -6   1 13  10933  00 22 12
00 23 22  ---          09 43 16  51.5   1.8 -0.2    -175.6    64   F  1  11867

00 23 22  SN1993J      09 43 16  51.6   1.8 -0.2    -175.7    -6   1 13  11867  00 23 22
00 25 22  ---          09 45 16  51.6   1.5 -0.2    -176.4   114   F  1  13467

00 25 22  M81          09 45 16  51.6   1.5 -0.2    -176.3    -6   1 13  13467  00 25 22
00 26 32  ---          09 46 26  51.6   1.4 -0.2    -176.7    64   F  1  14400

00 26 32  SN1993J      09 46 26  51.6   1.3 -0.2    -176.8    -6   1 13  14400  00 26 32
00 28 32  ---          09 48 27  51.6   1.1 -0.1    -177.5   114   F  1  16000

00 28 32  M81          09 48 27  51.6   1.1 -0.1    -177.4    -6   1 13  16000  00 28 32
00 30 32  ---          09 50 27  51.6   0.8 -0.1    -178.1   114   F  1  17600

00 31 12  M81          09 51 07  51.6   0.7 -0.1    -178.3    34   1 14  17600  00 31 12
00 33 22  ---          09 53 17  51.6   0.4  0.0    -179.1   130   R  1  15867
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

00 33 22  SN1993J      09 53 17  51.6   0.4  0.0    -179.1    -6   1 14  15867  00 33 22
00 35 22  ---          09 55 18  51.6   0.1  0.0    -179.8   114   R  1  14267

00 35 22  M81          09 55 18  51.6   0.1  0.0    -179.8    -6   1 14  14267  00 35 22
00 36 32  ---          09 56 28  51.6  -0.1  0.0     179.8    64   R  1  13333

00 36 32  SN1993J      09 56 28  51.6  -0.1  0.0     179.8    -6   1 14  13333  00 36 32
00 38 32  ---          09 58 28  51.6  -0.4  0.0     179.1   114   R  1  11733

00 38 32  M81          09 58 28  51.6  -0.4  0.0     179.1    -6   1 14  11733  00 38 32
00 39 42  ---          09 59 39  51.6  -0.5  0.1     178.7    64   R  1  10800

00 39 42  SN1993J      09 59 39  51.6  -0.6  0.1     178.7    -6   1 14  10800  00 39 42
00 41 42  ---          10 01 39  51.6  -0.8  0.1     178.0   114   R  1   9200

00 41 42  M81          10 01 39  51.6  -0.8  0.1     178.0    -6   1 14   9200  00 41 42
00 42 52  ---          10 02 49  51.6  -1.0  0.1     177.6    64   R  1   8267

00 42 52  SN1993J      10 02 49  51.6  -1.0  0.1     177.6    -6   1 14   8267  00 42 52
00 44 52  ---          10 04 49  51.6  -1.3  0.2     176.9   114   R  1   6667

00 44 52  M81          10 04 49  51.6  -1.3  0.1     176.9    -6   1 14   6667  00 44 52
00 46 02  ---          10 06 00  51.6  -1.5  0.2     176.5    64   R  1   5733

00 46 02  SN1993J      10 06 00  51.6  -1.5  0.2     176.5    -6   1 14   5733  00 46 02
00 48 02  ---          10 08 00  51.6  -1.8  0.2     175.8   114   R  1   4133

00 48 02  M81          10 08 00  51.5  -1.7  0.2     175.8    -6   1 14   4133  00 48 02
00 49 12  ---          10 09 10  51.5  -1.9  0.2     175.4    64   R  1   3200

00 49 12  SN1993J      10 09 10  51.6  -1.9  0.2     175.4    -6   1 14   3200  00 49 12
00 51 12  ---          10 11 10  51.6  -2.2  0.3     174.7   114   R  1   1600

00 51 12  M81          10 11 10  51.5  -2.2  0.3     174.7    -6   1 14   1600  00 51 12
00 53 12  ---          10 13 11  51.5  -2.5  0.3     174.0   114   R  1      0

-----------  Tape Change ------------

01 08 12  M81          10 28 13  51.3  -4.6  0.5     168.8   893   2  1      0  01 08 12
01 10 22  ---          10 30 24  51.3  -4.9  0.6     168.1   130   F  1   1733

01 10 22  SN1993J      10 30 24  51.3  -4.9  0.6     168.0    -6   2  1   1733  01 10 22
01 12 22  ---          10 32 24  51.3  -5.2  0.6     167.4   114   F  1   3333
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

01 12 22  M81          10 32 24  51.2  -5.2  0.6     167.4    -6   2  1   3333  01 12 22
01 13 32  ---          10 33 34  51.2  -5.4  0.6     167.0    64   F  1   4267

01 13 32  SN1993J      10 33 34  51.2  -5.4  0.6     167.0    -6   2  1   4267  01 13 32
01 15 32  ---          10 35 34  51.2  -5.7  0.7     166.3   114   F  1   5867

01 15 32  M81          10 35 34  51.2  -5.6  0.7     166.3    -6   2  1   5867  01 15 32
01 16 42  ---          10 36 45  51.1  -5.8  0.7     165.9    64   F  1   6800

01 16 42  SN1993J      10 36 45  51.2  -5.8  0.7     165.9    -6   2  1   6800  01 16 42
01 18 42  ---          10 38 45  51.1  -6.1  0.7     165.2   114   F  1   8400

01 18 42  M81          10 38 45  51.1  -6.1  0.7     165.2    -6   2  1   8400  01 18 42
01 19 52  ---          10 39 55  51.1  -6.2  0.7     164.8    64   F  1   9333

01 19 52  SN1993J      10 39 55  51.1  -6.3  0.7     164.8    -6   2  1   9333  01 19 52
01 21 52  ---          10 41 55  51.1  -6.5  0.8     164.1   114   F  1  10933

01 21 52  M81          10 41 55  51.0  -6.5  0.8     164.2    -6   2  1  10933  01 21 52
01 23 02  ---          10 43 06  51.0  -6.7  0.8     163.8    64   F  1  11867

01 23 02  SN1993J      10 43 06  51.0  -6.7  0.8     163.7    -6   2  1  11867  01 23 02
01 25 02  ---          10 45 06  51.0  -7.0  0.8     163.0   114   F  1  13467

01 25 02  M81          10 45 06  50.9  -6.9  0.8     163.1    -6   2  1  13467  01 25 02
01 26 12  ---          10 46 16  50.9  -7.1  0.8     162.7    64   F  1  14400

01 26 12  SN1993J      10 46 16  50.9  -7.1  0.8     162.6    -6   2  1  14400  01 26 12
01 28 12  ---          10 48 16  50.9  -7.4  0.9     162.0   114   F  1  16000

01 28 12  M81          10 48 16  50.9  -7.4  0.9     162.0    -6   2  1  16000  01 28 12
01 30 12  ---          10 50 17  50.8  -7.6  0.9     161.3   114   F  1  17600

01 30 52  M81          10 50 57  50.8  -7.7  0.9     161.1    34   2  2  17600  01 30 52
01 33 02  ---          10 53 07  50.7  -8.0  1.0     160.4   130   R  1  15867

01 33 02  SN1993J      10 53 07  50.8  -8.1  1.0     160.3    -6   2  2  15867  01 33 02
01 35 02  ---          10 55 08  50.7  -8.3  1.0     159.6   114   R  1  14267

01 35 02  M81          10 55 08  50.7  -8.3  1.0     159.7    -6   2  2  14267  01 35 02
01 36 12  ---          10 56 18  50.6  -8.4  1.0     159.3    64   R  1  13333
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

01 36 12  SN1993J      10 56 18  50.7  -8.5  1.0     159.2    -6   2  2  13333  01 36 12
01 38 12  ---          10 58 18  50.6  -8.7  1.0     158.6   114   R  1  11733

01 38 12  M81          10 58 18  50.6  -8.7  1.0     158.6    -6   2  2  11733  01 38 12
01 39 22  ---          10 59 28  50.5  -8.9  1.1     158.3    64   R  1  10800

01 39 22  SN1993J      10 59 28  50.5  -8.9  1.1     158.2    -6   2  2  10800  01 39 22
01 41 22  ---          11 01 29  50.5  -9.2  1.1     157.5   114   R  1   9200

01 41 22  M81          11 01 29  50.4  -9.1  1.1     157.6    -6   2  2   9200  01 41 22
01 42 32  ---          11 02 39  50.4  -9.3  1.1     157.2    64   R  1   8267

01 42 32  SN1993J      11 02 39  50.4  -9.3  1.1     157.1    -6   2  2   8267  01 42 32
01 44 32  ---          11 04 39  50.4  -9.6  1.1     156.5   114   R  1   6667

01 44 32  M81          11 04 39  50.3  -9.5  1.1     156.5    -6   2  2   6667  01 44 32
01 45 42  ---          11 05 49  50.3  -9.7  1.2     156.1    64   R  1   5733

01 45 42  SN1993J      11 05 49  50.3  -9.7  1.2     156.1    -6   2  2   5733  01 45 42
01 47 42  ---          11 07 50  50.3 -10.0  1.2     155.4   114   R  1   4133

01 47 42  M81          11 07 50  50.2  -9.9  1.2     155.5    -6   2  2   4133  01 47 42
01 48 52  ---          11 09 00  50.2 -10.1  1.2     155.1    64   R  1   3200

01 48 52  SN1993J      11 09 00  50.2 -10.1  1.2     155.0    -6   2  2   3200  01 48 52
01 50 52  ---          11 11 00  50.1 -10.4  1.3     154.4   114   R  1   1600

01 50 52  M81          11 11 00  50.1 -10.3  1.3     154.4    -6   2  2   1600  01 50 52
01 52 52  ---          11 13 01  50.0 -10.6  1.3     153.8   114   R  1      0

01 53 32  M81          11 13 41  50.0 -10.7  1.3     153.5    34   2  3      0  01 53 32
01 55 42  ---          11 15 51  49.9 -10.9  1.3     152.8   130   F  1   1733

01 55 42  SN1993J      11 15 51  49.9 -11.0  1.3     152.8    -6   2  3   1733  01 55 42
01 57 42  ---          11 17 51  49.9 -11.2  1.4     152.1   114   F  1   3333

01 57 42  M81          11 17 51  49.8 -11.2  1.4     152.2    -6   2  3   3333  01 57 42
01 58 52  ---          11 19 02  49.8 -11.3  1.4     151.8    64   F  1   4267

01 58 52  SN1993J      11 19 02  49.8 -11.4  1.4     151.7    -6   2  3   4267  01 58 52
02 00 52  ---          11 21 02  49.7 -11.6  1.4     151.1   114   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

02 00 52  M81          11 21 02  49.7 -11.6  1.4     151.1    -6   2  3   5867  02 00 52
02 02 02  ---          11 22 12  49.6 -11.7  1.4     150.8    64   F  1   6800

02 02 02  SN1993J      11 22 12  49.7 -11.8  1.4     150.7    -6   2  3   6800  02 02 02
02 04 02  ---          11 24 12  49.6 -12.0  1.5     150.0   114   F  1   8400

02 04 02  M81          11 24 12  49.5 -12.0  1.5     150.1    -6   2  3   8400  02 04 02
02 05 12  ---          11 25 23  49.5 -12.1  1.5     149.7    64   F  1   9333

02 05 12  SN1993J      11 25 23  49.5 -12.1  1.5     149.7    -6   2  3   9333  02 05 12
02 07 12  ---          11 27 23  49.4 -12.4  1.5     149.0   114   F  1  10933

02 07 12  M81          11 27 23  49.4 -12.3  1.5     149.1    -6   2  3  10933  02 07 12
02 08 22  ---          11 28 33  49.4 -12.5  1.5     148.7    64   F  1  11867

02 08 22  SN1993J      11 28 33  49.4 -12.5  1.5     148.6    -6   2  3  11867  02 08 22
02 10 22  ---          11 30 33  49.3 -12.8  1.6     148.0   114   F  1  13467

02 10 22  M81          11 30 33  49.3 -12.7  1.6     148.1    -6   2  3  13467  02 10 22
02 11 32  ---          11 31 44  49.2 -12.8  1.6     147.7    64   F  1  14400

02 11 32  SN1993J      11 31 44  49.2 -12.9  1.6     147.6    -6   2  3  14400  02 11 32
02 13 32  ---          11 33 44  49.1 -13.1  1.6     147.0   114   F  1  16000

02 13 32  M81          11 33 44  49.1 -13.1  1.6     147.0    -6   2  3  16000  02 13 32
02 15 32  ---          11 35 44  49.0 -13.3  1.7     146.4   114   F  1  17600

02 20 32  OQ208        11 40 45  58.2  84.6 -2.4     -76.9   229   2  4  17600  02 20 32
02 22 42  ---          11 42 55  58.7  84.8 -2.4     -77.0   130   R  1  15867

02 22 42  M81          11 42 55  48.6 -14.1  1.8     144.1   -72   2  4  15867  02 22 42
02 25 52  ---          11 46 06  48.5 -14.4  1.8     143.1   118   R  1  13333

02 25 52  SN1993J      11 46 06  48.5 -14.5  1.8     143.0    -6   2  4  13333  02 25 52
02 27 52  ---          11 48 06  48.4 -14.7  1.9     142.4   114   R  1  11733

02 27 52  M81          11 48 06  48.4 -14.7  1.9     142.5    -6   2  4  11733  02 27 52
02 29 02  ---          11 49 16  48.3 -14.8  1.9     142.1    64   R  1  10800

02 29 02  SN1993J      11 49 16  48.3 -14.8  1.9     142.0    -6   2  4  10800  02 29 02
02 31 02  ---          11 51 17  48.2 -15.1  1.9     141.4   114   R  1   9200
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

02 31 02  M81          11 51 17  48.2 -15.0  1.9     141.5    -6   2  4   9200  02 31 02
02 32 12  ---          11 52 27  48.1 -15.1  1.9     141.1    64   R  1   8267

02 32 12  SN1993J      11 52 27  48.2 -15.2  1.9     141.1    -6   2  4   8267  02 32 12
02 34 12  ---          11 54 27  48.0 -15.4  2.0     140.4   114   R  1   6667

02 34 12  M81          11 54 27  48.0 -15.3  2.0     140.5    -6   2  4   6667  02 34 12
02 35 22  ---          11 55 38  47.9 -15.4  2.0     140.1    64   R  1   5733

02 35 22  SN1993J      11 55 38  48.0 -15.5  2.0     140.1    -6   2  4   5733  02 35 22
02 37 22  ---          11 57 38  47.9 -15.7  2.0     139.4   114   R  1   4133

02 37 22  M81          11 57 38  47.8 -15.6  2.0     139.5    -6   2  4   4133  02 37 22
02 38 32  ---          11 58 48  47.8 -15.8  2.0     139.2    64   R  1   3200

02 38 32  SN1993J      11 58 48  47.8 -15.8  2.1     139.1    -6   2  4   3200  02 38 32
02 40 32  ---          12 00 48  47.7 -16.0  2.1     138.5   114   R  1   1600

02 40 32  M81          12 00 48  47.6 -16.0  2.1     138.5    -6   2  4   1600  02 40 32
02 42 32  ---          12 02 49  47.5 -16.2  2.1     137.9   114   R  1      0

02 43 12  M81          12 03 29  47.5 -16.2  2.1     137.7    34   2  5      0  02 43 12
02 45 22  ---          12 05 39  47.4 -16.4  2.2     137.1   130   F  1   1733

02 45 22  SN1993J      12 05 39  47.4 -16.5  2.2     137.0    -6   2  5   1733  02 45 22
02 47 22  ---          12 07 39  47.3 -16.7  2.2     136.4   114   F  1   3333

02 47 22  M81          12 07 39  47.2 -16.6  2.2     136.5    -6   2  5   3333  02 47 22
02 48 32  ---          12 08 50  47.2 -16.7  2.2     136.1    64   F  1   4267

02 48 32  SN1993J      12 08 50  47.2 -16.8  2.2     136.0    -6   2  5   4267  02 48 32
02 50 32  ---          12 10 50  47.1 -17.0  2.3     135.4   114   F  1   5867

02 50 32  M81          12 10 50  47.0 -16.9  2.2     135.5    -6   2  5   5867  02 50 32
02 51 42  ---          12 12 00  47.0 -17.0  2.3     135.1    64   F  1   6800

02 51 42  SN1993J      12 12 00  47.0 -17.1  2.3     135.1    -6   2  5   6800  02 51 42
02 53 42  ---          12 14 01  46.9 -17.3  2.3     134.5   114   F  1   8400

02 53 42  M81          12 14 01  46.8 -17.2  2.3     134.5    -6   2  5   8400  02 53 42
02 54 52  ---          12 15 11  46.8 -17.3  2.3     134.2    64   F  1   9333
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

02 54 52  SN1993J      12 15 11  46.8 -17.4  2.3     134.1    -6   2  5   9333  02 54 52
02 56 52  ---          12 17 11  46.6 -17.6  2.4     133.5   114   F  1  10933

02 56 52  M81          12 17 11  46.6 -17.5  2.4     133.6    -6   2  5  10933  02 56 52
02 58 02  ---          12 18 21  46.6 -17.6  2.4     133.2    64   F  1  11867

02 58 02  SN1993J      12 18 21  46.6 -17.7  2.4     133.2    -6   2  5  11867  02 58 02
03 00 02  ---          12 20 22  46.4 -17.9  2.4     132.6   114   F  1  13467

03 00 02  M81          12 20 22  46.4 -17.8  2.4     132.6    -6   2  5  13467  03 00 02
03 01 12  ---          12 21 32  46.3 -17.9  2.4     132.3    64   F  1  14400

03 01 12  SN1993J      12 21 32  46.4 -18.0  2.4     132.2    -6   2  5  14400  03 01 12
03 03 12  ---          12 23 32  46.2 -18.1  2.5     131.6   114   F  1  16000

03 03 12  M81          12 23 32  46.2 -18.1  2.5     131.7    -6   2  5  16000  03 03 12
03 05 12  ---          12 25 32  46.1 -18.2  2.5     131.1   114   F  1  17600

03 05 52  M81          12 26 13  46.0 -18.3  2.5     130.9    34   2  6  17600  03 05 52
03 08 02  ---          12 28 23  45.9 -18.5  2.5     130.3   130   R  1  15867

03 08 02  SN1993J      12 28 23  45.9 -18.5  2.5     130.2    -6   2  6  15867  03 08 02
03 10 02  ---          12 30 23  45.8 -18.7  2.6     129.6   114   R  1  14267

03 10 02  M81          12 30 23  45.7 -18.6  2.6     129.7    -6   2  6  14267  03 10 02
03 11 12  ---          12 31 33  45.7 -18.7  2.6     129.3    64   R  1  13333

03 11 12  SN1993J      12 31 33  45.7 -18.8  2.6     129.3    -6   2  6  13333  03 11 12
03 13 12  ---          12 33 34  45.5 -19.0  2.6     128.7   114   R  1  11733

03 13 12  M81          12 33 34  45.5 -18.9  2.6     128.8    -6   2  6  11733  03 13 12
03 14 22  ---          12 34 44  45.4 -19.0  2.6     128.4    64   R  1  10800

03 14 22  SN1993J      12 34 44  45.5 -19.1  2.6     128.3    -6   2  6  10800  03 14 22
03 16 22  ---          12 36 44  45.3 -19.2  2.7     127.8   114   R  1   9200

03 16 22  M81          12 36 44  45.3 -19.2  2.7     127.8    -6   2  6   9200  03 16 22
03 17 32  ---          12 37 54  45.2 -19.2  2.7     127.5    64   R  1   8267

03 17 32  SN1993J      12 37 54  45.2 -19.3  2.7     127.4    -6   2  6   8267  03 17 32
03 19 32  ---          12 39 55  45.1 -19.5  2.7     126.8   114   R  1   6667
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

03 19 32  M81          12 39 55  45.1 -19.4  2.7     126.9    -6   2  6   6667  03 19 32
03 20 42  ---          12 41 05  45.0 -19.5  2.8     126.6    64   R  1   5733

03 20 42  SN1993J      12 41 05  45.0 -19.6  2.8     126.5    -6   2  6   5733  03 20 42
03 22 42  ---          12 43 05  44.9 -19.7  2.8     125.9   114   R  1   4133

03 22 42  M81          12 43 05  44.8 -19.6  2.8     126.0    -6   2  6   4133  03 22 42
03 23 52  ---          12 44 15  44.8 -19.7  2.8     125.7    64   R  1   3200

03 23 52  SN1993J      12 44 15  44.8 -19.8  2.8     125.6    -6   2  6   3200  03 23 52
03 25 52  ---          12 46 16  44.6 -19.9  2.8     125.0   114   R  1   1600

03 25 52  M81          12 46 16  44.6 -19.9  2.8     125.1    -6   2  6   1600  03 25 52
03 27 52  ---          12 48 16  44.5 -20.0  2.9     124.5   114   R  1      0

03 28 32  M81          12 48 56  44.4 -20.1  2.9     124.4    34   2  7      0  03 28 32
03 30 42  ---          12 51 07  44.3 -20.2  2.9     123.7   130   F  1   1733

03 30 42  SN1993J      12 51 07  44.3 -20.3  2.9     123.7    -6   2  7   1733  03 30 42
03 32 42  ---          12 53 07  44.1 -20.4  3.0     123.1   114   F  1   3333

03 32 42  M81          12 53 07  44.1 -20.4  3.0     123.2    -6   2  7   3333  03 32 42
03 33 52  ---          12 54 17  44.0 -20.4  3.0     122.8    64   F  1   4267

03 33 52  SN1993J      12 54 17  44.0 -20.5  3.0     122.8    -6   2  7   4267  03 33 52
03 35 52  ---          12 56 17  43.9 -20.6  3.0     122.2   114   F  1   5867

03 35 52  M81          12 56 17  43.9 -20.6  3.0     122.3    -6   2  7   5867  03 35 52
03 37 02  ---          12 57 28  43.8 -20.6  3.0     122.0    64   F  1   6800

03 37 02  SN1993J      12 57 28  43.8 -20.7  3.0     121.9    -6   2  7   6800  03 37 02
03 39 02  ---          12 59 28  43.6 -20.8  3.1     121.3   114   F  1   8400

03 39 02  M81          12 59 28  43.6 -20.8  3.1     121.4    -6   2  7   8400  03 39 02
03 40 12  ---          13 00 38  43.5 -20.8  3.1     121.1    64   F  1   9333

03 40 12  SN1993J      13 00 38  43.6 -20.9  3.1     121.0    -6   2  7   9333  03 40 12
03 42 12  ---          13 02 38  43.4 -21.0  3.1     120.4   114   F  1  10933

03 42 12  M81          13 02 38  43.4 -21.0  3.1     120.5    -6   2  7  10933  03 42 12
03 43 22  ---          13 03 49  43.3 -21.0  3.1     120.2    64   F  1  11867
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

03 43 22  SN1993J      13 03 49  43.3 -21.1  3.1     120.1    -6   2  7  11867  03 43 22
03 45 22  ---          13 05 49  43.2 -21.2  3.2     119.6   114   F  1  13467

03 45 22  M81          13 05 49  43.1 -21.2  3.2     119.6    -6   2  7  13467  03 45 22
03 46 32  ---          13 06 59  43.1 -21.2  3.2     119.3    64   F  1  14400

03 46 32  SN1993J      13 06 59  43.1 -21.3  3.2     119.2    -6   2  7  14400  03 46 32
03 48 32  ---          13 09 00  42.9 -21.4  3.2     118.7   114   F  1  16000

03 48 32  M81          13 09 00  42.9 -21.4  3.2     118.8    -6   2  7  16000  03 48 32
03 50 32  ---          13 11 00  42.7 -21.5  3.3     118.2   114   F  1  17600

03 51 12  M81          13 11 40  42.7 -21.5  3.3     118.0    34   2  8  17600  03 51 12
03 53 22  ---          13 13 50  42.5 -21.6  3.3     117.5   130   R  1  15867

03 53 22  SN1993J      13 13 50  42.5 -21.7  3.3     117.4    -6   2  8  15867  03 53 22
03 55 22  ---          13 15 51  42.4 -21.8  3.3     116.8   114   R  1  14267

03 55 22  M81          13 15 51  42.4 -21.7  3.3     116.9    -6   2  8  14267  03 55 22
03 56 32  ---          13 17 01  42.3 -21.8  3.4     116.6    64   R  1  13333

03 56 32  SN1993J      13 17 01  42.3 -21.9  3.4     116.5    -6   2  8  13333  03 56 32
03 58 32  ---          13 19 01  42.1 -22.0  3.4     116.0   114   R  1  11733

03 58 32  M81          13 19 01  42.1 -21.9  3.4     116.1    -6   2  8  11733  03 58 32
03 59 42  ---          13 20 11  42.0 -22.0  3.4     115.7    64   R  1  10800

03 59 42  SN1993J      13 20 11  42.0 -22.0  3.4     115.7    -6   2  8  10800  03 59 42
04 01 42  ---          13 22 12  41.8 -22.1  3.4     115.1   114   R  1   9200

04 01 42  M81          13 22 12  41.8 -22.1  3.4     115.2    -6   2  8   9200  04 01 42
04 02 52  ---          13 23 22  41.7 -22.1  3.5     114.9    64   R  1   8267

04 02 52  SN1993J      13 23 22  41.8 -22.2  3.5     114.8    -6   2  8   8267  04 02 52
04 04 52  ---          13 25 22  41.6 -22.3  3.5     114.3   114   R  1   6667

04 04 52  M81          13 25 22  41.6 -22.2  3.5     114.4    -6   2  8   6667  04 04 52
04 06 02  ---          13 26 32  41.5 -22.3  3.5     114.0    64   R  1   5733

04 06 02  SN1993J      13 26 32  41.5 -22.4  3.5     114.0    -6   2  8   5733  04 06 02
04 08 02  ---          13 28 33  41.3 -22.5  3.5     113.4   114   R  1   4133
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

04 08 02  M81          13 28 33  41.3 -22.4  3.5     113.5    -6   2  8   4133  04 08 02
04 09 12  ---          13 29 43  41.2 -22.5  3.6     113.2    64   R  1   3200

04 09 12  SN1993J      13 29 43  41.2 -22.5  3.6     113.1    -6   2  8   3200  04 09 12
04 11 12  ---          13 31 43  41.1 -22.6  3.6     112.6   114   R  1   1600

04 11 12  M81          13 31 43  41.1 -22.5  3.6     112.7    -6   2  8   1600  04 11 12
04 13 12  ---          13 33 44  40.9 -22.6  3.6     112.1   114   R  1      0

04 23 12  0954+658     13 43 45  41.5 -27.3  3.7     107.5   591   2  9      0  04 23 12
04 26 12  ---          13 46 46  41.2 -27.4  3.8     106.7   180   F  1   2400

04 26 12  M81          13 46 46  39.8 -23.2  3.8     108.8    -9   2  9   2400  04 26 12
04 28 32  ---          13 49 06  39.6 -23.3  3.9     108.2   131   F  1   4267

04 28 32  SN1993J      13 49 06  39.6 -23.3  3.9     108.1    -6   2  9   4267  04 28 32
04 30 32  ---          13 51 06  39.4 -23.4  3.9     107.6   114   F  1   5867

04 30 32  M81          13 51 06  39.4 -23.3  3.9     107.6    -6   2  9   5867  04 30 32
04 31 42  ---          13 52 17  39.3 -23.4  3.9     107.3    64   F  1   6800

04 31 42  SN1993J      13 52 17  39.3 -23.4  3.9     107.3    -6   2  9   6800  04 31 42
04 33 42  ---          13 54 17  39.2 -23.5  4.0     106.8   114   F  1   8400

04 33 42  M81          13 54 17  39.2 -23.4  4.0     106.8    -6   2  9   8400  04 33 42
04 34 52  ---          13 55 27  39.1 -23.5  4.0     106.5    64   F  1   9333

04 34 52  SN1993J      13 55 27  39.1 -23.5  4.0     106.5    -6   2  9   9333  04 34 52
04 36 52  ---          13 57 27  38.9 -23.6  4.0     106.0   114   F  1  10933

04 36 52  M81          13 57 27  38.9 -23.5  4.0     106.0    -6   2  9  10933  04 36 52
04 38 02  ---          13 58 38  38.8 -23.6  4.0     105.7    64   F  1  11867

04 38 02  SN1993J      13 58 38  38.8 -23.6  4.0     105.7    -6   2  9  11867  04 38 02
04 40 02  ---          14 00 38  38.6 -23.7  4.1     105.2   114   F  1  13467

04 40 02  M81          14 00 38  38.6 -23.6  4.1     105.2    -6   2  9  13467  04 40 02
04 41 12  ---          14 01 48  38.5 -23.7  4.1     104.9    64   F  1  14400

04 41 12  SN1993J      14 01 48  38.5 -23.7  4.1     104.9    -6   2  9  14400  04 41 12
04 43 12  ---          14 03 49  38.3 -23.8  4.1     104.4   114   F  1  16000
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

04 43 12  M81          14 03 49  38.3 -23.7  4.1     104.4    -6   2  9  16000  04 43 12
04 45 12  ---          14 05 49  38.2 -23.8  4.2     103.9   114   F  1  17600

04 45 52  M81          14 06 29  38.1 -23.8  4.2     103.8    34   2 10  17600  04 45 52
04 48 02  ---          14 08 39  37.9 -23.9  4.2     103.2   130   R  1  15867

04 48 02  SN1993J      14 08 39  37.9 -23.9  4.2     103.1    -6   2 10  15867  04 48 02
04 50 02  ---          14 10 40  37.7 -24.0  4.2     102.6   114   R  1  14267

04 50 02  M81          14 10 40  37.8 -23.9  4.2     102.7    -6   2 10  14267  04 50 02
04 51 12  ---          14 11 50  37.6 -23.9  4.3     102.4    64   R  1  13333

04 51 12  SN1993J      14 11 50  37.6 -24.0  4.3     102.4    -6   2 10  13333  04 51 12
04 53 12  ---          14 13 50  37.5 -24.0  4.3     101.9   114   R  1  11733

04 53 12  M81          14 13 50  37.5 -24.0  4.3     101.9    -6   2 10  11733  04 53 12
04 54 22  ---          14 15 00  37.4 -24.0  4.3     101.6    64   R  1  10800

04 54 22  SN1993J      14 15 00  37.4 -24.1  4.3     101.6    -6   2 10  10800  04 54 22
04 56 22  ---          14 17 01  37.2 -24.1  4.4     101.1   114   R  1   9200

04 56 22  M81          14 17 01  37.2 -24.1  4.4     101.1    -6   2 10   9200  04 56 22
04 57 32  ---          14 18 11  37.1 -24.1  4.4     100.8    64   R  1   8267

04 57 32  SN1993J      14 18 11  37.1 -24.1  4.4     100.8    -6   2 10   8267  04 57 32
04 59 32  ---          14 20 11  36.9 -24.2  4.4     100.3   114   R  1   6667

04 59 32  M81          14 20 11  36.9 -24.1  4.4     100.4    -6   2 10   6667  04 59 32
05 00 42  ---          14 21 21  36.8 -24.2  4.4     100.1    64   R  1   5733

05 00 42  SN1993J      14 21 21  36.8 -24.2  4.4     100.0    -6   2 10   5733  05 00 42
05 02 42  ---          14 23 22  36.6 -24.2  4.5      99.5   114   R  1   4133

05 02 42  M81          14 23 22  36.6 -24.2  4.5      99.6    -6   2 10   4133  05 02 42
05 03 52  ---          14 24 32  36.5 -24.2  4.5      99.3    64   R  1   3200

05 03 52  SN1993J      14 24 32  36.5 -24.3  4.5      99.2    -6   2 10   3200  05 03 52
05 05 52  ---          14 26 32  36.4 -24.3  4.5      98.7   114   R  1   1600

05 05 52  M81          14 26 32  36.4 -24.2  4.5      98.8    -6   2 10   1600  05 05 52
05 07 52  ---          14 28 33  36.2 -24.3  4.5      98.3   114   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

05 12 52  OQ208        14 33 33  83.9 250.6  0.4      67.4   111   2 11      0  05 12 52
05 15 02  ---          14 35 44  83.4 252.2  0.5      68.7   130   F  1   1733

05 15 02  M81          14 35 44  35.5 335.6  4.7      96.6  -102   2 11   1733  05 15 02
05 18 12  ---          14 38 54  35.3 335.6  4.7      95.8    88   F  1   4267

05 18 12  SN1993J      14 38 54  35.3 335.5  4.7      95.7    -6   2 11   4267  05 18 12
05 20 12  ---          14 40 55  35.1 335.5  4.8      95.3   114   F  1   5867

05 20 12  M81          14 40 55  35.1 335.6  4.8      95.3    -6   2 11   5867  05 20 12
05 21 22  ---          14 42 05  35.0 335.5  4.8      95.1    64   F  1   6800

05 21 22  SN1993J      14 42 05  35.0 335.5  4.8      95.0    -6   2 11   6800  05 21 22
05 23 22  ---          14 44 05  34.8 335.5  4.8      94.5   114   F  1   8400

05 23 22  M81          14 44 05  34.8 335.5  4.8      94.6    -6   2 11   8400  05 23 22
05 24 32  ---          14 45 15  34.7 335.5  4.8      94.3    64   F  1   9333

05 24 32  SN1993J      14 45 15  34.7 335.5  4.8      94.2    -6   2 11   9333  05 24 32
05 26 32  ---          14 47 16  34.5 335.5  4.9      93.8   114   F  1  10933

05 26 32  M81          14 47 16  34.5 335.5  4.9      93.8    -6   2 11  10933  05 26 32
05 27 42  ---          14 48 26  34.4 335.5  4.9      93.5    64   F  1  11867

05 27 42  SN1993J      14 48 26  34.4 335.4  4.9      93.5    -6   2 11  11867  05 27 42
05 29 42  ---          14 50 26  34.2 335.4  4.9      93.0   114   F  1  13467

05 29 42  M81          14 50 26  34.2 335.5  4.9      93.1    -6   2 11  13467  05 29 42
05 30 52  ---          14 51 36  34.1 335.5  4.9      92.8    64   F  1  14400

05 30 52  SN1993J      14 51 36  34.1 335.4  4.9      92.7    -6   2 11  14400  05 30 52
05 32 52  ---          14 53 37  33.9 335.4  5.0      92.3   114   F  1  16000

05 32 52  M81          14 53 37  34.0 335.5  5.0      92.3    -6   2 11  16000  05 32 52
05 34 52  ---          14 55 37  33.8 335.5  5.0      91.8   114   F  1  17600

05 35 32  M81          14 56 17  33.7 335.5  5.0      91.7    34   2 12  17600  05 35 32
05 37 42  ---          14 58 27  33.5 335.5  5.0      91.2   130   R  1  15867

05 37 42  SN1993J      14 58 27  33.5 335.4  5.0      91.1    -6   2 12  15867  05 37 42
05 39 42  ---          15 00 28  33.3 335.4  5.1      90.6   114   R  1  14267
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

05 39 42  M81          15 00 28  33.3 335.4  5.1      90.7    -6   2 12  14267  05 39 42
05 40 52  ---          15 01 38  33.2 335.4  5.1      90.4    64   R  1  13333

05 40 52  SN1993J      15 01 38  33.2 335.4  5.1      90.4    -6   2 12  13333  05 40 52
05 42 52  ---          15 03 38  33.0 335.4  5.1      89.9   114   R  1  11733

05 42 52  M81          15 03 38  33.1 335.4  5.1      90.0    -6   2 12  11733  05 42 52
05 44 02  ---          15 04 49  32.9 335.4  5.1      89.7    64   R  1  10800

05 44 02  SN1993J      15 04 49  32.9 335.4  5.2      89.6    -6   2 12  10800  05 44 02
05 46 02  ---          15 06 49  32.8 335.4  5.2      89.2   114   R  1   9200

05 46 02  M81          15 06 49  32.8 335.4  5.2      89.2    -6   2 12   9200  05 46 02
05 47 12  ---          15 07 59  32.7 335.5  5.2      89.0    64   R  1   8267

05 47 12  SN1993J      15 07 59  32.7 335.4  5.2      88.9    -6   2 12   8267  05 47 12
05 49 12  ---          15 09 59  32.5 335.4  5.2      88.4   114   R  1   6667

05 49 12  M81          15 09 59  32.5 335.5  5.2      88.5    -6   2 12   6667  05 49 12
05 50 22  ---          15 11 10  32.4 335.5  5.3      88.2    64   R  1   5733

05 50 22  SN1993J      15 11 10  32.4 335.4  5.3      88.2    -6   2 12   5733  05 50 22
05 52 22  ---          15 13 10  32.2 335.4  5.3      87.7   114   R  1   4133

05 52 22  M81          15 13 10  32.2 335.5  5.3      87.8    -6   2 12   4133  05 52 22
05 53 32  ---          15 14 20  32.1 335.5  5.3      87.5    64   R  1   3200

05 53 32  SN1993J      15 14 20  32.1 335.4  5.3      87.4    -6   2 12   3200  05 53 32
05 55 32  ---          15 16 20  31.9 335.4  5.3      87.0   114   R  1   1600

05 55 32  M81          15 16 20  31.9 335.5  5.3      87.0    -6   2 12   1600  05 55 32
05 57 32  ---          15 18 21  31.7 335.5  5.4      86.6   114   R  1      0

05 58 12  M81          15 19 01  31.7 335.5  5.4      86.4    34   2 13      0  05 58 12
06 00 22  ---          15 21 11  31.5 335.5  5.4      85.9   130   F  1   1733

06 00 22  SN1993J      15 21 11  31.5 335.5  5.4      85.8    -6   2 13   1733  06 00 22
06 02 22  ---          15 23 12  31.3 335.5  5.5      85.4   114   F  1   3333

06 02 22  M81          15 23 12  31.3 335.5  5.5      85.4    -6   2 13   3333  06 02 22
06 03 32  ---          15 24 22  31.2 335.5  5.5      85.2    64   F  1   4267
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

06 03 32  SN1993J      15 24 22  31.2 335.5  5.5      85.1    -6   2 13   4267  06 03 32
06 05 32  ---          15 26 22  31.0 335.5  5.5      84.7   114   F  1   5867

06 05 32  M81          15 26 22  31.0 335.6  5.5      84.7    -6   2 13   5867  06 05 32
06 06 42  ---          15 27 32  30.9 335.6  5.5      84.4    64   F  1   6800

06 06 42  SN1993J      15 27 32  30.9 335.5  5.5      84.4    -6   2 13   6800  06 06 42
06 08 42  ---          15 29 33  30.7 335.5  5.6      83.9   114   F  1   8400

06 08 42  M81          15 29 33  30.7 335.6  5.6      84.0    -6   2 13   8400  06 08 42
06 09 52  ---          15 30 43  30.6 335.6  5.6      83.7    64   F  1   9333

06 09 52  SN1993J      15 30 43  30.6 335.6  5.6      83.7    -6   2 13   9333  06 09 52
06 11 52  ---          15 32 43  30.4 335.6  5.6      83.2   114   F  1  10933

06 11 52  M81          15 32 43  30.5 335.6  5.6      83.3    -6   2 13  10933  06 11 52
06 13 02  ---          15 33 53  30.4 335.6  5.6      83.0    64   F  1  11867

06 13 02  SN1993J      15 33 53  30.3 335.6  5.6      82.9    -6   2 13  11867  06 13 02
06 15 02  ---          15 35 54  30.2 335.6  5.7      82.5   114   F  1  13467

06 15 02  M81          15 35 54  30.2 335.7  5.7      82.5    -6   2 13  13467  06 15 02
06 16 12  ---          15 37 04  30.1 335.7  5.7      82.3    64   F  1  14400

06 16 12  SN1993J      15 37 04  30.1 335.6  5.7      82.2    -6   2 13  14400  06 16 12
06 18 12  ---          15 39 04  29.9 335.7  5.7      81.8   114   F  1  16000

06 18 12  M81          15 39 04  29.9 335.7  5.7      81.8    -6   2 13  16000  06 18 12
06 20 12  ---          15 41 04  29.7 335.7  5.8      81.4   114   F  1  17600

06 20 52  M81          15 41 45  29.7 335.8  5.8      81.2    34   2 14  17600  06 20 52
06 23 02  ---          15 43 55  29.5 335.8  5.8      80.7   130   R  1  15867

06 23 02  SN1993J      15 43 55  29.5 335.7  5.8      80.7    -6   2 14  15867  06 23 02
06 25 02  ---          15 45 55  29.3 335.8  5.8      80.2   114   R  1  14267

06 25 02  M81          15 45 55  29.3 335.8  5.8      80.3    -6   2 14  14267  06 25 02
06 26 12  ---          15 47 05  29.2 335.8  5.9      80.0    64   R  1  13333

06 26 12  SN1993J      15 47 05  29.2 335.8  5.9      80.0    -6   2 14  13333  06 26 12
06 28 12  ---          15 49 06  29.0 335.8  5.9      79.5   114   R  1  11733
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  26 May 2004   Day 147 ---

06 28 12  M81          15 49 06  29.0 335.9  5.9      79.6    -6   2 14  11733  06 28 12
06 29 22  ---          15 50 16  28.9 335.9  5.9      79.3    64   R  1  10800

06 29 22  SN1993J      15 50 16  28.9 335.9  5.9      79.3    -6   2 14  10800  06 29 22
06 31 22  ---          15 52 16  28.7 335.9  5.9      78.8   114   R  1   9200

06 31 22  M81          15 52 16  28.7 335.9  5.9      78.9    -6   2 14   9200  06 31 22
06 32 32  ---          15 53 26  28.6 336.0  6.0      78.6    64   R  1   8267

06 32 32  SN1993J      15 53 26  28.6 335.9  6.0      78.5    -6   2 14   8267  06 32 32
06 34 32  ---          15 55 27  28.4 336.0  6.0      78.1   114   R  1   6667

06 34 32  M81          15 55 27  28.5 336.0  6.0      78.1    -6   2 14   6667  06 34 32
06 35 42  ---          15 56 37  28.4 336.0  6.0      77.9    64   R  1   5733

06 35 42  SN1993J      15 56 37  28.3 336.0  6.0      77.8    -6   2 14   5733  06 35 42
06 37 42  ---          15 58 37  28.2 336.0  6.0      77.4   114   R  1   4133

06 37 42  M81          15 58 37  28.2 336.1  6.0      77.4    -6   2 14   4133  06 37 42
06 38 52  ---          15 59 48  28.1 336.1  6.1      77.2    64   R  1   3200

06 38 52  SN1993J      15 59 48  28.1 336.1  6.1      77.1    -6   2 14   3200  06 38 52
06 40 52  ---          16 01 48  27.9 336.1  6.1      76.7   114   R  1   1600

06 40 52  M81          16 01 48  27.9 336.1  6.1      76.7    -6   2 14   1600  06 40 52
06 42 52  ---          16 03 48  27.7 336.2  6.1      76.3   114   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/sched.2002Jul02a/setups/v6cm-256-8-2-UL.set
   Matches group v6cm_2 in /usr/local/sched.2002Jul02a/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
   BBC SB=         L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4979.49   4979.49   4979.49   4979.49   4995.49   4995.49   4995.49   4995.49
   BBC fr=     879.49    879.49    879.49    879.49    895.49    895.49    895.49    895.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   510   490   510  6490  6510  6490  6510
    PCALFR2=   490   510   490   510  6490  6510  6490  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- 32rd epoch of obs. of SN1993J in M81: VLBA/MkIV 6 pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * SN1993J           09 51 19.038889   * 09 55 24.774900     09 55 45.611833 
                     69 15 26.46784    * 69 01 13.70300      69 00 22.82179 
                     From catalog imbedded in main SCHED input file.

 * M81               09 51 27.310854   * 09 55 33.173100     09 55 54.023981 
                     69 18 08.14534    * 69 03 55.06200      69 03 04.16045 
                     From catalog imbedded in main SCHED input file.

 * 0954+658          09 54 57.847119   * 09 58 47.244300     09 59 06.718912 
                     65 48 15.53178    * 65 33 54.81100      65 33 02.59761 
                     From catalog imbedded in main SCHED input file.

   J1407+2827        14 04 45.615151   * 14 07 00.394410     14 07 13.071224 
   1404+286          28 41 29.23495    * 28 27 14.68998      28 26 02.45770 
   J1407+28          /usr/local/sched.2002Jul02a/catalogs/sources.vlba
 * OQ208             ICRF - Ext.1 Source - 1998 IERS Annual Report



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1993J             68.8
   M81                 68.8
   0954+658            69.4
   OQ208              121.9

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

