  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1993J @ 6cm
 Exp. Code:  gm046   


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 30 Jan. 2001                       

PI:       J.M.Marcaide                                                    

Address:  Universitat de Valencia                                         
          C/ Dr. Moliner, 50                                              
          Burjassot, E 46100, Spain                                       
                                                                          

Phone:    34-96-398-3079/8 (work) or 34-96-337-1786 (home)                
EMAIL:    J.M.Marcaide@uv.es (internet)                                   
Fax:      34-96-398-3084                                                  
Phone during observation: 34-958-121311 (work) or 34-958-810928 (home)    

Observing mode: VLBA                                                      

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

 Next scan frequencies:  4966.49  4966.49  4982.49  4982.49  4998.49  4998.49
                         5014.49  5014.49
 Next BBC frequencies:    866.49   866.49   882.49   882.49   898.49   898.49
                          914.49   914.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

10 00 30  1803+784     06 54 48  19.4   2.8-11.1     -12.3     0   1  1      0  10 00 30
10 04 30  ---          06 58 48  19.4   3.1-11.0     -13.3   240   F  1   3200

10 06 43  2007+777     07 01 01  19.0  -3.5 10.9      14.6   126   1  1   3200  10 06 43
10 10 43  ---          07 05 02  18.9  -3.3 11.0      13.7   240   F  1   6400

10 13 00  1803+784     07 07 19  19.5   3.5-10.9     -15.2   131   1  1   6400  10 13 00
10 17 00  ---          07 11 20  19.6   3.7-10.8     -16.1   240   F  1   9600

10 26 03  3C286        07 20 25  12.9  62.0 -6.2     -61.9   503   1  1   9600  10 26 03
10 31 03  ---          07 25 26  13.9  62.5 -6.1     -62.4   300   F  1  13600

10 34 27  3C48         07 28 50  17.9 -61.5  5.9      64.6   119   1  1  13600  10 34 27
10 39 27  ---          07 33 51  16.9 -61.0  5.9      64.1   300   F  1  17600

10 50 48  M81          07 45 14  47.3  16.5 -2.2    -136.9   619   1  2  17600  10 50 48
10 54 48  ---          07 49 15  47.6  16.1 -2.1    -138.1   240   R  1  14400

10 55 03  SN1993J      07 49 30  47.6  16.1 -2.1    -138.2    13   1  2  14400  10 55 03
11 02 03  ---          07 56 31  48.0  15.4 -2.0    -140.3   420   R  1   8800

11 02 19  M81          07 56 47  48.0  15.4 -2.0    -140.4    13   1  2   8800  11 02 19
11 06 19  ---          08 00 47  48.2  14.9 -1.9    -141.6   240   R  1   5600

11 06 34  SN1993J      08 01 02  48.3  14.9 -1.9    -141.7    13   1  2   5600  11 06 34
11 13 34  ---          08 08 04  48.7  14.2 -1.8    -143.9   420   R  1      0

11 14 14  M81          08 08 44  48.6  14.1 -1.8    -144.1    38   1  3      0  11 14 14
11 19 14  ---          08 13 45  48.9  13.5 -1.7    -145.7   300   F  1   4000

11 19 29  SN1993J      08 14 00  49.0  13.5 -1.7    -145.8    13   1  3   4000  11 19 29
11 26 29  ---          08 21 01  49.3  12.7 -1.6    -148.1   420   F  1   9600

11 27 09  0917+624     08 21 41  56.9  12.8 -1.0    -155.9    23   1  3   9600  11 27 09
11 30 09  ---          08 24 42  57.1  12.2 -1.0    -157.1   180   F  1  12000
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

11 30 49  SN1993J      08 25 21  49.5  12.2 -1.5    -149.5    22   1  3  12000  11 30 49
11 37 49  ---          08 32 22  49.8  11.4 -1.4    -151.8   420   F  1  17600

11 38 29  M81          08 33 02  49.8  11.3 -1.4    -151.9    38   1  4  17600  11 38 29
11 42 29  ---          08 37 03  50.0  10.8 -1.3    -153.3   240   R  1  14400

11 42 44  SN1993J      08 37 18  50.0  10.8 -1.3    -153.4    13   1  4  14400  11 42 44
11 49 44  ---          08 44 19  50.3   9.9 -1.2    -155.7   420   R  1   8800

11 49 59  M81          08 44 35  50.2   9.8 -1.2    -155.7    13   1  4   8800  11 49 59
11 53 59  ---          08 48 35  50.4   9.3 -1.1    -157.1   240   R  1   5600

11 54 14  SN1993J      08 48 51  50.4   9.3 -1.1    -157.2    13   1  4   5600  11 54 14
12 01 14  ---          08 55 52  50.7   8.4 -1.0    -159.5   420   R  1      0

12 01 54  0954+658     08 56 32  53.8  10.9 -1.0    -157.0    32   1  5      0  12 01 54
12 04 54  ---          08 59 32  53.9  10.4 -1.0    -158.0   180   F  1   2400

12 05 22  SN1993J      09 00 00  50.8   7.8 -0.9    -160.9    20   1  5   2400  12 05 22
12 12 22  ---          09 07 02  51.0   6.9 -0.8    -163.3   420   F  1   8000

12 12 37  M81          09 07 17  51.0   6.8 -0.8    -163.4    13   1  5   8000  12 12 37
12 17 37  ---          09 12 18  51.1   6.1 -0.7    -165.1   300   F  1  12000

12 17 53  SN1993J      09 12 33  51.1   6.1 -0.7    -165.2    13   1  5  12000  12 17 53
12 24 53  ---          09 19 34  51.3   5.1 -0.6    -167.6   420   F  1  17600

12 25 33  M81          09 20 14  51.2   5.0 -0.6    -167.8    38   1  6  17600  12 25 33
12 30 33  ---          09 25 15  51.3   4.3 -0.5    -169.5   300   R  1  13600

12 30 48  SN1993J      09 25 30  51.4   4.3 -0.5    -169.6    13   1  6  13600  12 30 48
12 37 48  ---          09 32 31  51.5   3.3 -0.4    -172.0   420   R  1   8000

12 38 31  0917+624     09 33 15  58.3  -2.6  0.2     175.3    28   1  6   8000  12 38 31
12 41 31  ---          09 36 15  58.3  -3.2  0.2     174.0   180   R  1   5600

12 42 14  SN1993J      09 36 58  51.5   2.7 -0.3    -173.6    27   1  6   5600  12 42 14
12 49 14  ---          09 43 59  51.6   1.7 -0.2    -176.0   420   R  1      0

12 54 14  M81          09 49 00  51.6   1.0 -0.1    -177.7   298   1  7      0  12 54 14
12 58 14  ---          09 53 01  51.6   0.4  0.0    -179.1   240   F  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

12 58 29  SN1993J      09 53 16  51.6   0.3  0.0    -179.2    13   1  7   3200  12 58 29
13 05 29  ---          10 00 17  51.6  -0.7  0.1     178.4   420   F  1   8800

13 05 44  M81          10 00 33  51.6  -0.7  0.1     178.3    13   1  7   8800  13 05 44
13 09 44  ---          10 04 33  51.6  -1.3  0.1     176.9   240   F  1  12000

13 10 00  SN1993J      10 04 49  51.6  -1.3  0.2     176.8    13   1  7  12000  13 10 00
13 17 00  ---          10 11 50  51.6  -2.3  0.3     174.4   420   F  1  17600

13 17 40  0954+658     10 12 30  55.0  -2.5  0.2     174.9    31   1  8  17600  13 17 40
13 20 40  ---          10 15 30  55.0  -3.0  0.3     173.8   180   R  1  15200

13 21 05  SN1993J      10 15 56  51.5  -2.9  0.3     172.9    16   1  8  15200  13 21 05
13 28 05  ---          10 22 57  51.4  -3.9  0.5     170.5   420   R  1   9600

13 28 20  M81          10 23 12  51.4  -3.9  0.5     170.5    13   1  8   9600  13 28 20
13 33 20  ---          10 28 13  51.3  -4.6  0.5     168.8   300   R  1   5600

13 33 35  SN1993J      10 28 28  51.3  -4.7  0.5     168.6    13   1  8   5600  13 33 35
13 40 35  ---          10 35 29  51.2  -5.7  0.7     166.2   420   R  1      0

13 41 20  0917+624     10 36 14  56.2 -15.5  1.2     150.4    33   1  9      0  13 41 20
13 44 20  ---          10 39 15  56.0 -16.0  1.3     149.3   180   F  1   2400

13 45 05  SN1993J      10 40 00  51.1  -6.3  0.7     164.7    33   1  9   2400  13 45 05
13 52 05  ---          10 47 01  50.9  -7.3  0.9     162.3   420   F  1   8000

13 52 20  M81          10 47 16  50.9  -7.3  0.9     162.3    13   1  9   8000  13 52 20
13 57 20  ---          10 52 17  50.7  -7.9  0.9     160.6   300   F  1  12000

13 57 35  SN1993J      10 52 32  50.8  -8.0  0.9     160.4    13   1  9  12000  13 57 35
14 04 35  ---          10 59 33  50.5  -8.9  1.1     158.1   420   F  1  17600

14 05 15  M81          11 00 13  50.5  -9.0  1.1     157.9    38   1 10  17600  14 05 15
14 10 15  ---          11 05 14  50.3  -9.6  1.2     156.3   300   R  1  13600

14 10 31  SN1993J      11 05 29  50.3  -9.7  1.2     156.1    13   1 10  13600  14 10 31
14 17 31  ---          11 12 31  50.1 -10.6  1.3     153.8   420   R  1   8000

14 17 56  0954+658     11 12 56  53.3 -12.7  1.2     152.8    17   1 10   8000  14 17 56
14 20 56  ---          11 15 57  53.1 -13.2  1.3     151.8   180   R  1   5600
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

14 21 22  SN1993J      11 16 22  49.9 -11.1  1.3     152.5    17   1 10   5600  14 21 22
14 28 22  ---          11 23 23  49.6 -11.9  1.5     150.2   420   R  1      0

14 29 02  M81          11 24 03  49.5 -12.0  1.5     150.1    38   1 11      0  14 29 02
14 34 02  ---          11 29 04  49.3 -12.6  1.6     148.5   300   F  1   4000

14 34 17  SN1993J      11 29 19  49.3 -12.6  1.6     148.3    13   1 11   4000  14 34 17
14 41 17  ---          11 36 21  49.0 -13.4  1.7     146.1   420   F  1   9600

14 42 02  0917+624     11 37 06  51.6 -24.7  2.3     129.5    36   1 11   9600  14 42 02
14 45 02  ---          11 40 07  51.3 -25.0  2.3     128.6   180   F  1  12000

14 45 47  SN1993J      11 40 52  48.8 -13.9  1.8     144.6    36   1 11  12000  14 45 47
14 52 47  ---          11 47 53  48.4 -14.7  1.9     142.4   420   F  1  17600

14 53 27  M81          11 48 33  48.3 -14.7  1.9     142.3    38   1 12  17600  14 53 27
14 57 27  ---          11 52 34  48.1 -15.2  1.9     141.0   240   R  1  14400

14 57 43  SN1993J      11 52 49  48.1 -15.2  2.0     140.9    13   1 12  14400  14 57 43
15 04 43  ---          11 59 50  47.7 -15.9  2.1     138.7   420   R  1   8800

15 04 58  M81          12 00 06  47.7 -15.9  2.1     138.7    13   1 12   8800  15 04 58
15 08 58  ---          12 04 06  47.4 -16.3  2.1     137.5   240   R  1   5600

15 09 13  SN1993J      12 04 21  47.4 -16.4  2.1     137.3    13   1 12   5600  15 09 13
15 16 13  ---          12 11 23  47.0 -17.1  2.3     135.2   420   R  1      0

15 16 53  0954+658     12 12 03  49.6 -20.5  2.2     133.2    33   1 13      0  15 16 53
15 19 53  ---          12 15 03  49.4 -20.8  2.3     132.3   180   F  1   2400

15 20 20  SN1993J      12 15 30  46.7 -17.4  2.3     133.9    20   1 13   2400  15 20 20
15 27 20  ---          12 22 31  46.3 -18.1  2.4     131.9   420   F  1   8000

15 27 35  M81          12 22 47  46.2 -18.0  2.5     131.9    13   1 13   8000  15 27 35
15 32 35  ---          12 27 47  45.9 -18.5  2.5     130.4   300   F  1  12000

15 32 50  SN1993J      12 28 03  45.9 -18.5  2.5     130.2    13   1 13  12000  15 32 50
15 39 50  ---          12 35 04  45.4 -19.1  2.7     128.2   420   F  1  17600

15 40 30  0917+624     12 35 44  45.8 -30.0  3.2     112.5    31   1 14  17600  15 40 30
15 43 30  ---          12 38 44  45.4 -30.2  3.3     111.7   180   R  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

15 43 30  SN1993J      12 38 44  45.2 -19.4  2.7     127.1    -9   1 14  15200  15 43 30
15 50 30  ---          12 45 46  44.7 -19.9  2.8     125.1   411   R  1   9600

15 50 30  M81          12 45 46  44.6 -19.8  2.8     125.2    -2   1 14   9600  15 50 30
15 55 30  ---          12 50 46  44.3 -20.2  2.9     123.8   298   R  1   5600

15 55 30  SN1993J      12 50 46  44.3 -20.3  2.9     123.7    -2   1 14   5600  15 55 30
16 02 30  ---          12 57 47  43.8 -20.7  3.0     121.7   418   R  1      0

-----------  Tape Change ------------

16 17 30  0954+658     13 12 50  44.4 -25.7  3.2     115.6   895   2  1      0  16 17 30
16 27 30  ---          13 22 52  43.5 -26.3  3.4     112.9   600   F  1   8000

16 28 10  M81          13 23 32  41.7 -22.2  3.5     114.8    34   2  1   8000  16 28 10
16 33 10  ---          13 28 33  41.3 -22.4  3.5     113.5   300   F  1  12000

16 33 26  SN1993J      13 28 48  41.3 -22.5  3.6     113.3    13   2  1  12000  16 33 26
16 40 26  ---          13 35 49  40.7 -22.8  3.7     111.5   420   F  1  17600

16 41 06  M81          13 36 29  40.7 -22.8  3.7     111.4    38   2  2  17600  16 41 06
16 45 06  ---          13 40 30  40.3 -22.9  3.7     110.3   240   R  1  14400

16 45 21  SN1993J      13 40 45  40.3 -23.0  3.8     110.2    13   2  2  14400  16 45 21
16 52 21  ---          13 47 46  39.7 -23.3  3.9     108.4   420   R  1   8800

16 52 36  M81          13 48 01  39.7 -23.2  3.9     108.4    13   2  2   8800  16 52 36
16 56 36  ---          13 52 02  39.3 -23.4  3.9     107.3   240   R  1   5600

16 56 51  SN1993J      13 52 17  39.3 -23.4  3.9     107.2    13   2  2   5600  16 56 51
17 03 51  ---          13 59 18  38.7 -23.7  4.1     105.4   420   R  1      0

17 04 34  0917+624     14 00 01  36.2 -32.7  4.6      92.0    35   2  3      0  17 04 34
17 07 34  ---          14 03 02  35.9 -32.7  4.7      91.4   180   F  1   2400

17 08 16  SN1993J      14 03 44  38.3 -23.8  4.1     104.3    34   2  3   2400  17 08 16
17 15 16  ---          14 10 45  37.7 -24.0  4.3     102.6   420   F  1   8000

17 15 31  M81          14 11 01  37.7 -23.9  4.3     102.6    13   2  3   8000  17 15 31
17 20 31  ---          14 16 01  37.3 -24.0  4.3     101.3   300   F  1  12000

17 20 47  SN1993J      14 16 17  37.2 -24.1  4.3     101.2    13   2  3  12000  17 20 47
17 27 47  ---          14 23 18  36.6 -24.2  4.5      99.5   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

17 28 27  M81          14 23 58  36.6 -24.2  4.5      99.4    38   2  4  17600  17 28 27
17 33 27  ---          14 28 59  36.1 -24.3  4.6      98.2   300   R  1  13600

17 33 42  SN1993J      14 29 14  36.1 -24.3  4.6      98.0    13   2  4  13600  17 33 42
17 40 42  ---          14 36 15  35.5 -24.4  4.7      96.3   420   R  1   8000

17 41 11  0954+658     14 36 44  36.1 -28.7  4.6      94.5    24   2  4   8000  17 41 11
17 44 11  ---          14 39 44  35.8 -28.7  4.7      93.8   180   R  1   5600

17 44 39  SN1993J      14 40 13  35.1 -24.5  4.7      95.4    24   2  4   5600  17 44 39
17 51 39  ---          14 47 15  34.5 -24.5  4.9      93.7   420   R  1      0

17 52 19  M81          14 47 55  34.4 -24.5  4.9      93.6    38   2  5      0  17 52 19
17 56 19  ---          14 51 55  34.1 -24.5  4.9      92.7   240   F  1   3200

17 56 35  SN1993J      14 52 10  34.0 -24.6  4.9      92.5    13   2  5   3200  17 56 35
18 04 35  ---          15 00 12  33.3 -24.6  5.1      90.7   480   F  1   9600

18 05 14  0917+624     15 00 52  29.2 -32.1  5.7      78.9    29   2  5   9600  18 05 14
18 08 14  ---          15 03 52  28.8 -32.0  5.7      78.3   180   F  1  12000

18 08 54  SN1993J      15 04 32  32.9 -24.6  5.1      89.6    29   2  5  12000  18 08 54
18 15 54  ---          15 11 33  32.3 -24.6  5.3      88.0   420   F  1  17600

18 19 14  M81          15 14 54  32.0 -24.5  5.3      87.3   197   2  6  17600  18 19 14
18 23 14  ---          15 18 54  31.7 -24.5  5.4      86.4   240   R  1  14400

18 23 29  SN1993J      15 19 09  31.6 -24.5  5.4      86.3    13   2  6  14400  18 23 29
18 30 29  ---          15 26 11  31.0 -24.5  5.5      84.7   420   R  1   8800

18 30 44  M81          15 26 26  31.0 -24.4  5.5      84.7    13   2  6   8800  18 30 44
18 34 44  ---          15 30 26  30.6 -24.4  5.6      83.7   240   R  1   5600

18 34 59  SN1993J      15 30 42  30.6 -24.4  5.6      83.6    13   2  6   5600  18 34 59
18 41 59  ---          15 37 43  30.0 -24.4  5.7      82.0   420   R  1      0

18 42 39  0954+658     15 38 23  29.7 -28.3  5.7      80.7    35   2  7      0  18 42 39
18 45 39  ---          15 41 23  29.4 -28.3  5.7      80.0   180   F  1   2400

18 46 08  SN1993J      15 41 52  29.6 -24.3  5.8      81.1    24   2  7   2400  18 46 08
18 53 08  ---          15 48 53  29.0 -24.2  5.9      79.5   420   F  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

18 53 23  M81          15 49 09  29.0 -24.1  5.9      79.5    13   2  7   8000  18 53 23
18 57 23  ---          15 53 09  28.6 -24.0  6.0      78.6   240   F  1  11200

18 57 39  SN1993J      15 53 25  28.6 -24.1  6.0      78.5    13   2  7  11200  18 57 39
19 05 39  ---          16 01 26  27.9 -23.9  6.1      76.7   480   F  1  17600

19 06 19  0917+624     16 02 06  22.4 -29.7  6.7      66.4    27   2  8  17600  19 06 19
19 09 19  ---          16 05 06  22.1 -29.6  6.7      65.8   180   R  1  15200

19 09 55  SN1993J      16 05 42  27.5 -23.8  6.2      75.8    23   2  8  15200  19 09 55
19 16 55  ---          16 12 44  26.9 -23.6  6.3      74.2   420   R  1   9600

19 17 10  M81          16 12 59  26.9 -23.6  6.3      74.2    13   2  8   9600  19 17 10
19 21 10  ---          16 16 59  26.6 -23.5  6.4      73.3   240   R  1   6400

19 21 25  SN1993J      16 17 15  26.5 -23.5  6.4      73.2    13   2  8   6400  19 21 25
19 29 25  ---          16 25 16  25.8 -23.2  6.5      71.4   480   R  1      0

19 30 05  M81          16 25 56  25.8 -23.2  6.5      71.3    38   2  9      0  19 30 05
19 35 05  ---          16 30 57  25.4 -23.0  6.6      70.2   300   F  1   4000

19 35 20  SN1993J      16 31 12  25.3 -23.1  6.6      70.1    13   2  9   4000  19 35 20
19 42 20  ---          16 38 13  24.8 -22.8  6.7      68.6   420   F  1   9600

19 42 48  0954+658     16 38 42  23.7 -26.4  6.7      67.8    24   2  9   9600  19 42 48
19 45 48  ---          16 41 42  23.4 -26.3  6.7      67.1   180   F  1  12000

19 46 17  SN1993J      16 42 10  24.4 -22.7  6.8      67.7    24   2  9  12000  19 46 17
19 53 17  ---          16 49 12  23.8 -22.4  6.9      66.2   420   F  1  17600

19 53 57  M81          16 49 52  23.8 -22.3  6.9      66.1    38   2 10  17600  19 53 57
19 58 57  ---          16 54 53  23.4 -22.1  7.0      65.0   300   R  1  13600

19 59 12  SN1993J      16 55 08  23.4 -22.2  7.0      64.9    13   2 10  13600  19 59 12
20 06 12  ---          17 02 09  22.8 -21.9  7.1      63.4   420   R  1   8000

20 06 49  0917+624     17 02 46  16.3 -26.0  7.7      54.2    22   2 10   8000  20 06 49
20 09 49  ---          17 05 47  16.0 -25.8  7.7      53.5   180   R  1   5600

20 10 26  SN1993J      17 06 24  22.5 -21.7  7.2      62.5    22   2 10   5600  20 10 26
20 17 26  ---          17 13 25  21.9 -21.3  7.3      61.0   420   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

20 18 06  M81          17 14 05  21.9 -21.3  7.3      60.9    38   2 11      0  20 18 06
20 22 06  ---          17 18 06  21.6 -21.1  7.4      60.0   240   F  1   3200

20 22 21  SN1993J      17 18 21  21.5 -21.1  7.4      59.9    13   2 11   3200  20 22 21
20 29 21  ---          17 25 22  21.0 -20.8  7.5      58.4   420   F  1   8800

20 29 37  M81          17 25 38  21.0 -20.7  7.5      58.4    13   2 11   8800  20 29 37
20 33 37  ---          17 29 38  20.7 -20.5  7.6      57.5   240   F  1  12000

20 33 52  SN1993J      17 29 53  20.6 -20.5  7.6      57.4    13   2 11  12000  20 33 52
20 40 52  ---          17 36 55  20.1 -20.2  7.7      55.9   420   F  1  17600

20 42 30  3C286        17 38 34  37.5 -73.2  4.1      72.9    61   2 12  17600  20 42 30
20 46 30  ---          17 42 34  36.7 -72.9  4.2      72.6   240   R  1  14400

20 49 37  2007+777     17 45 41  40.3   9.1 -2.3    -139.8   130   2 12  14400  20 49 37
20 53 37  ---          17 49 42  40.4   8.8 -2.3    -140.9   240   R  1  11200

20 54 16  1803+784     17 50 21  42.2   0.7 -0.2    -177.0    31   2 12  11200  20 54 16
20 57 16  ---          17 53 21  42.2   0.5 -0.1    -177.9   180   R  1   8800


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gm046.6cm
   Matches group v6cm_2 in /usr/local/sched/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         U         L         U         L         U         L         U
   Pol.  =      LCP       LCP       LCP       LCP       LCP       LCP       LCP       LCP 
   BBC   =         1         1         2         2         3         3         4         4
   BBC SB=         L         U         L         U         L         U         L         U
   IF    =        C         C         C         C         C         C         C         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4966.49   4966.49   4982.49   4982.49   4998.49   4998.49   5014.49   5014.49
   BBC fr=     866.49    866.49    882.49    882.49    898.49    898.49    914.49    914.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   490   490   490  6490  6490  6490  6490
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- SN1993J @ 6cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * 0917+624          09 17 40.306287   * 09 21 36.230500     09 21 43.767309 
                     62 28 38.63575    * 62 15 52.17600      62 15 13.17277 
                     From catalog imbedded in main SCHED input file.

 * 0954+658          09 54 57.847920   * 09 58 47.245100     09 58 54.102631 
                     65 48 15.53881    * 65 33 54.81800      65 33 12.05452 
                     From catalog imbedded in main SCHED input file.

 * SN1993J           09 51 19.039486   * 09 55 24.775500     09 55 32.163700 
                     69 15 26.47487    * 69 01 13.71000      69 00 30.45083 
                     From catalog imbedded in main SCHED input file.

 * M81               09 51 27.310854   * 09 55 33.173100     09 55 40.562637 
                     69 18 08.14534    * 69 03 55.06200      69 03 11.78427 
                     From catalog imbedded in main SCHED input file.

 * 1803+784          18 03 39.193244   * 18 00 45.683600     18 00 34.644747 
                     78 27 54.30008    * 78 28 04.02100      78 28 15.28122 
                     From catalog imbedded in main SCHED input file.

 * 2007+777          20 07 20.430477   * 20 05 30.998800     20 05 24.625121 
                     77 43 58.12445    * 77 52 43.24900      77 53 17.52795 
                     From catalog imbedded in main SCHED input file.

 * 3C48              01 34 49.826399   * 01 37 41.299465     01 37 47.826915 
                     32 54 20.26003    * 33 09 35.13422      33 10 12.81964 
                     From catalog imbedded in main SCHED input file.

 * 3C286             13 28 49.657781   * 13 31 08.288074     13 31 11.216243 
                     30 45 58.64118    * 30 30 32.95982      30 30 02.81081 
                     From catalog imbedded in main SCHED input file.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0917+624           108.7
   0954+658           105.2
   SN1993J            106.3
   M81                106.3
   1803+784            99.9
   2007+777           104.3
   3C48               150.2
   3C286               58.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

