  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GLOBAL-6cm-2016+112
 Exp. Code:  GP030A  


Schedule Version:       1.00                                              
Processed by SCHED version: 16 Oct. 2001                                  

PI:       Richard Porcas                                                  

Address:  MPIfR                                                           
          Auf dem Huegel 69                                               
          D 53121 BONN                                                    
          Germany                                                         

Phone:    +49 228 525288                                                  
EMAIL:    porcas@mpifr-bonn.mpg.de                                        
Fax:      +49 228 525229                                                  
Phone during observation:                                                 

Observing mode: Continuum                                                 

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

 Next scan frequencies:  4982.49  4982.49  4990.49  4990.49
 Next BBC frequencies:    882.49   882.49   890.49   890.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00

17 58 00  2016+112     14 49 40  12.3  83.8 -5.5     -60.8     0   1  1      0  17 58 00
18 00 00  ---          14 51 40  12.7  84.1 -5.5     -60.8   120   F  1    800

18 00 00  2016+112     14 51 40  12.7  84.1 -5.5     -60.8    -2   1  1    800  18 00 00
18 04 30  ---          14 56 11  13.7  84.6 -5.4     -60.9   268   F  1   2600

18 04 30  2029+121     14 56 11  11.4  82.3 -5.6     -60.8    -7   1  1   2600  18 04 30
18 06 00  ---          14 57 41  11.7  82.5 -5.6     -60.8    83   F  1   3200

18 06 00  2016+112     14 57 41  14.0  84.8 -5.4     -61.0    -7   1  1   3200  18 06 00
18 10 30  ---          15 02 12  14.9  85.4 -5.3     -61.1   263   F  1   5000

18 10 30  2029+121     15 02 12  12.7  83.0 -5.5     -61.0    -7   1  1   5000  18 10 30
18 12 00  ---          15 03 42  13.0  83.2 -5.5     -61.0    83   F  1   5600

18 12 00  2016+112     15 03 42  15.3  85.5 -5.3     -61.1    -7   1  1   5600  18 12 00
18 16 30  ---          15 08 13  16.2  86.1 -5.2     -61.2   263   F  1   7400

18 16 30  2029+121     15 08 13  14.0  83.8 -5.4     -61.1    -7   1  1   7400  18 16 30
18 18 00  ---          15 09 43  14.3  83.9 -5.4     -61.1    83   F  1   8000

18 18 00  2016+112     15 09 43  16.6  86.3 -5.2     -61.2    -7   1  1   8000  18 18 00
18 22 30  ---          15 14 14  17.5  86.8 -5.1     -61.2   263   F  1   9800

18 22 30  2029+121     15 14 14  15.2  84.5 -5.3     -61.2    -7   1  1   9800  18 22 30
18 24 00  ---          15 15 44  15.6  84.7 -5.3     -61.3    83   F  1  10400

18 24 00  2016+112     15 15 44  17.9  87.0 -5.1     -61.3    -7   1  1  10400  18 24 00
18 28 30  ---          15 20 15  18.8  87.6 -5.0     -61.3   263   F  1  12200

18 28 30  2029+121     15 20 15  16.5  85.2 -5.2     -61.4    -7   1  1  12200  18 28 30
18 30 00  ---          15 21 45  16.9  85.4 -5.2     -61.4    83   F  1  12800

18 30 00  2016+112     15 21 45  19.1  87.8 -5.0     -61.3    -7   1  1  12800  18 30 00
18 34 30  ---          15 26 16  20.1  88.3 -4.9     -61.4   263   F  1  14600

18 34 30  2029+121     15 26 16  17.8  86.0 -5.1     -61.5    -7   1  1  14600  18 34 30
18 36 00  ---          15 27 46  18.1  86.1 -5.1     -61.5    83   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

18 36 00  2016+112     15 27 46  20.4  88.5 -4.9     -61.4    -7   1  1  15200  18 36 00
18 40 30  ---          15 32 17  21.4  89.1 -4.8     -61.4   263   F  1  17000

18 40 30  2029+121     15 32 17  19.1  86.7 -5.0     -61.6    -7   1  1  17000  18 40 30
18 42 00  ---          15 33 47  19.4  86.9 -5.0     -61.6    83   F  1  17600

18 46 00  2016+112     15 37 47  22.6  89.8 -4.7     -61.4   232   1  2  17600  18 46 00
18 48 00  ---          15 39 48  23.0  90.0 -4.7     -61.4   120   R  1  16800

18 48 00  2016+112     15 39 48  23.0  90.0 -4.7     -61.4    -2   1  2  16800  18 48 00
18 52 30  ---          15 44 19  24.0  90.6 -4.6     -61.4   268   R  1  15000

18 52 30  2029+121     15 44 19  21.7  88.2 -4.8     -61.7    -7   1  2  15000  18 52 30
18 54 00  ---          15 45 49  22.0  88.4 -4.8     -61.7    83   R  1  14400

18 54 00  2016+112     15 45 49  24.3  90.8 -4.6     -61.4    -7   1  2  14400  18 54 00
18 58 30  ---          15 50 20  25.3  91.4 -4.5     -61.4   263   R  1  12600

18 58 30  2029+121     15 50 20  23.0  88.9 -4.7     -61.7    -7   1  2  12600  18 58 30
19 00 00  ---          15 51 50  23.3  89.1 -4.7     -61.7    83   R  1  12000

19 00 00  2016+112     15 51 50  25.6  91.6 -4.5     -61.4    -7   1  2  12000  19 00 00
19 04 30  ---          15 56 21  26.6  92.2 -4.4     -61.3   263   R  1  10200

19 04 30  2029+121     15 56 21  24.3  89.7 -4.6     -61.7    -7   1  2  10200  19 04 30
19 06 00  ---          15 57 51  24.6  89.9 -4.6     -61.7    83   R  1   9600

19 06 00  2016+112     15 57 51  26.9  92.4 -4.4     -61.3    -7   1  2   9600  19 06 00
19 10 30  ---          16 02 21  27.9  93.0 -4.3     -61.3   263   R  1   7800

19 10 30  2029+121     16 02 21  25.6  90.5 -4.5     -61.7    -7   1  2   7800  19 10 30
19 12 00  ---          16 03 52  25.9  90.7 -4.5     -61.7    83   R  1   7200

19 12 00  2016+112     16 03 52  28.2  93.2 -4.3     -61.2    -7   1  2   7200  19 12 00
19 16 30  ---          16 08 22  29.2  93.8 -4.2     -61.2   263   R  1   5400

19 16 30  2029+121     16 08 22  26.9  91.2 -4.4     -61.7    -7   1  2   5400  19 16 30
19 18 00  ---          16 09 53  27.2  91.4 -4.4     -61.7    83   R  1   4800

19 18 00  2016+112     16 09 53  29.5  94.0 -4.2     -61.1    -7   1  2   4800  19 18 00
19 22 30  ---          16 14 23  30.5  94.6 -4.1     -61.1   263   R  1   3000
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

19 22 30  2029+121     16 14 23  28.2  92.0 -4.3     -61.7    -7   1  2   3000  19 22 30
19 30 00  ---          16 21 55  29.8  93.0 -4.2     -61.6   443   R  1      0

19 34 00  2029+121     16 25 55  30.6  93.6 -4.1     -61.5   236   1  3      0  19 34 00
19 36 00  ---          16 27 56  31.1  93.8 -4.1     -61.5   120   F  1    800

19 36 00  2016+112     16 27 56  33.4  96.5 -3.9     -60.7    -7   1  3    800  19 36 00
19 40 30  ---          16 32 26  34.3  97.2 -3.8     -60.6   263   F  1   2600

19 40 30  2029+121     16 32 26  32.0  94.5 -4.0     -61.4    -7   1  3   2600  19 40 30
19 43 00  ---          16 34 57  32.6  94.8 -4.0     -61.4   143   F  1   3600

19 43 00  2016+112     16 34 57  34.9  97.5 -3.7     -60.5    -7   1  3   3600  19 43 00
19 47 30  ---          16 39 28  35.8  98.2 -3.7     -60.3   263   F  1   5400

19 47 30  2029+121     16 39 28  33.6  95.4 -3.9     -61.3    -7   1  3   5400  19 47 30
19 50 00  ---          16 41 58  34.1  95.8 -3.8     -61.2   143   F  1   6400

19 50 00  2016+112     16 41 58  36.4  98.6 -3.6     -60.2    -7   1  3   6400  19 50 00
19 54 30  ---          16 46 29  37.3  99.3 -3.5     -60.1   263   F  1   8200

19 54 30  2029+121     16 46 29  35.1  96.4 -3.8     -61.1    -7   1  3   8200  19 54 30
19 57 00  ---          16 48 59  35.6  96.8 -3.7     -61.0   143   F  1   9200

19 57 00  2016+112     16 48 59  37.8  99.7 -3.5     -59.9    -7   1  3   9200  19 57 00
20 01 30  ---          16 53 30  38.8 100.4 -3.4     -59.7   263   F  1  11000

20 01 30  2029+121     16 53 30  36.6  97.5 -3.6     -60.8    -6   1  3  11000  20 01 30
20 04 00  ---          16 56 00  37.1  97.8 -3.6     -60.8   144   F  1  12000

20 04 00  2016+112     16 56 00  39.3 100.8 -3.4     -59.6    -6   1  3  12000  20 04 00
20 08 30  ---          17 00 31  40.3 101.5 -3.3     -59.4   264   F  1  13800

20 08 30  2029+121     17 00 31  38.0  98.5 -3.5     -60.6    -6   1  3  13800  20 08 30
20 11 00  ---          17 03 01  38.6  98.9 -3.5     -60.5   144   F  1  14800

20 11 00  2016+112     17 03 01  40.8 101.9 -3.3     -59.2    -6   1  3  14800  20 11 00
20 15 30  ---          17 07 32  41.8 102.7 -3.2     -58.9   264   F  1  16600

20 15 30  2029+121     17 07 32  39.5  99.6 -3.4     -60.3    -6   1  3  16600  20 15 30
20 18 00  ---          17 10 03  40.1 100.0 -3.4     -60.2   144   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

20 21 00  2029+121     17 13 03  40.7 100.5 -3.3     -60.0   177   1  4  17600  20 21 00
20 23 00  ---          17 15 03  41.1 100.8 -3.3     -59.9   120   R  1  16800

20 23 00  2016+112     17 15 03  43.3 104.0 -3.1     -58.4    -6   1  4  16800  20 23 00
20 27 30  ---          17 19 34  44.3 104.8 -3.0     -58.1   264   R  1  15000

20 27 30  2029+121     17 19 34  42.1 101.6 -3.2     -59.6    -6   1  4  15000  20 27 30
20 30 00  ---          17 22 05  42.6 102.0 -3.2     -59.5   144   R  1  14000

20 30 00  2016+112     17 22 05  44.8 105.2 -3.0     -57.9    -6   1  4  14000  20 30 00
20 34 30  ---          17 26 35  45.7 106.1 -2.9     -57.5   264   R  1  12200

20 34 30  2029+121     17 26 35  43.6 102.7 -3.1     -59.2    -6   1  4  12200  20 34 30
20 37 00  ---          17 29 06  44.1 103.2 -3.0     -59.0   144   R  1  11200

20 37 00  2016+112     17 29 06  46.2 106.5 -2.8     -57.3    -6   1  4  11200  20 37 00
20 41 30  ---          17 33 36  47.2 107.4 -2.8     -56.9   264   R  1   9400

20 41 30  2029+121     17 33 36  45.0 104.0 -3.0     -58.7    -6   1  4   9400  20 41 30
20 44 00  ---          17 36 07  45.5 104.4 -2.9     -58.5   144   R  1   8400

20 44 00  2016+112     17 36 07  47.7 107.9 -2.7     -56.7    -6   1  4   8400  20 44 00
20 48 30  ---          17 40 38  48.6 108.8 -2.6     -56.2   264   R  1   6600

20 48 30  2029+121     17 40 38  46.5 105.3 -2.9     -58.2    -6   1  4   6600  20 48 30
20 51 00  ---          17 43 08  47.0 105.7 -2.8     -58.0   144   R  1   5600

20 51 00  2016+112     17 43 08  49.1 109.3 -2.6     -55.9    -6   1  4   5600  20 51 00
20 55 30  ---          17 47 39  50.0 110.3 -2.5     -55.4   264   R  1   3800

20 55 30  2029+121     17 47 39  47.9 106.6 -2.7     -57.6    -6   1  4   3800  20 55 30
20 58 00  ---          17 50 09  48.5 107.1 -2.7     -57.3   144   R  1   2800

20 58 00  2016+112     17 50 09  50.5 110.9 -2.5     -55.1    -6   1  4   2800  20 58 00
21 02 30  ---          17 54 40  51.4 111.9 -2.4     -54.6   264   R  1   1000

21 02 30  2029+121     17 54 40  49.4 108.0 -2.6     -56.9    -6   1  4   1000  21 02 30
21 05 00  ---          17 57 10  49.9 108.5 -2.6     -56.6   144   R  1      0

21 08 00  2029+121     18 00 11  50.5 109.2 -2.5     -56.3   177   1  5      0  21 08 00
21 10 00  ---          18 02 11  50.9 109.6 -2.5     -56.1   120   F  1    800
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

21 10 00  2016+112     18 02 11  52.9 113.6 -2.3     -53.5    -6   1  5    800  21 10 00
21 14 30  ---          18 06 42  53.8 114.7 -2.2     -52.9   264   F  1   2600

21 14 30  2029+121     18 06 42  51.8 110.6 -2.4     -55.5    -6   1  5   2600  21 14 30
21 17 00  ---          18 09 12  52.3 111.1 -2.4     -55.2   144   F  1   3600

21 17 00  2016+112     18 09 12  54.3 115.4 -2.2     -52.5    -6   1  5   3600  21 17 00
21 21 30  ---          18 13 43  55.2 116.6 -2.1     -51.8   264   F  1   5400

21 21 30  2029+121     18 13 43  53.2 112.2 -2.3     -54.6    -6   1  5   5400  21 21 30
21 24 00  ---          18 16 13  53.7 112.8 -2.3     -54.3   144   F  1   6400

21 24 00  2016+112     18 16 13  55.7 117.2 -2.1     -51.3    -6   1  5   6400  21 24 00
21 28 30  ---          18 20 44  56.5 118.5 -2.0     -50.5   264   F  1   8200

21 28 30  2029+121     18 20 44  54.6 113.9 -2.2     -53.6    -6   1  5   8200  21 28 30
21 31 00  ---          18 23 15  55.1 114.5 -2.1     -53.3   144   F  1   9200

21 31 00  2016+112     18 23 15  57.0 119.2 -1.9     -50.0    -6   1  5   9200  21 31 00
21 35 30  ---          18 27 45  57.8 120.5 -1.9     -49.1   264   F  1  11000

21 35 30  2029+121     18 27 45  56.0 115.7 -2.1     -52.5    -6   1  5  11000  21 35 30
21 38 00  ---          18 30 16  56.5 116.4 -2.0     -52.1   144   F  1  12000

21 38 00  2016+112     18 30 16  58.3 121.3 -1.8     -48.6    -6   1  5  12000  21 38 00
21 42 30  ---          18 34 46  59.1 122.7 -1.7     -47.6   264   F  1  13800

21 42 30  2029+121     18 34 46  57.3 117.6 -2.0     -51.3    -6   1  5  13800  21 42 30
21 52 00  ---          18 44 18  59.1 120.5 -1.8     -49.4   564   F  1  17600

21 55 00  2029+121     18 47 19  59.7 121.4 -1.7     -48.7   177   1  6  17600  21 55 00
21 57 00  ---          18 49 19  60.1 122.0 -1.7     -48.3   120   R  1  16800

21 57 00  2016+112     18 49 19  61.7 127.7 -1.5     -44.0    -6   1  6  16800  21 57 00
22 01 30  ---          18 53 50  62.4 129.5 -1.4     -42.7   264   R  1  15000

22 01 30  2029+121     18 53 50  60.9 123.5 -1.6     -47.2    -6   1  6  15000  22 01 30
22 04 00  ---          18 56 20  61.3 124.4 -1.6     -46.6   144   R  1  14000

22 04 00  2016+112     18 56 20  62.8 130.4 -1.4     -41.9    -6   1  6  14000  22 04 00
22 08 30  ---          19 00 51  63.6 132.3 -1.3     -40.5   264   R  1  12200
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

22 08 30  2029+121     19 00 51  62.1 126.0 -1.5     -45.4    -6   1  6  12200  22 08 30
22 11 00  ---          19 03 21  62.5 127.0 -1.5     -44.7   144   R  1  11200

22 11 00  2016+112     19 03 21  64.0 133.3 -1.3     -39.7    -6   1  6  11200  22 11 00
22 15 00  ---          19 07 22  64.6 135.1 -1.2     -38.3   234   R  1   9600

22 15 00  2029+121     19 07 22  63.2 128.5 -1.4     -43.6    -6   1  6   9600  22 15 00
22 25 00  ---          19 17 23  64.9 132.7 -1.2     -40.4   594   R  1   5600

22 25 00  2016+112     19 17 23  66.0 139.8 -1.0     -34.5    -7   1  6   5600  22 25 00
22 29 30  ---          19 21 54  66.7 142.1 -1.0     -32.6   263   R  1   3800

22 29 30  2029+121     19 21 54  65.6 134.7 -1.2     -38.8    -7   1  6   3800  22 29 30
22 32 00  ---          19 24 25  65.9 135.9 -1.1     -37.8   143   R  1   2800

22 32 00  2016+112     19 24 25  67.0 143.5 -0.9     -31.5    -7   1  6   2800  22 32 00
22 36 30  ---          19 28 55  67.5 145.9 -0.8     -29.5   263   R  1   1000

22 36 30  2029+121     19 28 55  66.6 138.0 -1.1     -36.1    -7   1  6   1000  22 36 30
22 39 00  ---          19 31 26  67.0 139.3 -1.0     -35.0   143   R  1      0

22 42 00  2029+121     19 34 26  67.4 140.9 -1.0     -33.8   177   1  7      0  22 42 00
22 44 00  ---          19 36 27  67.6 141.9 -0.9     -32.9   120   F  1    800

22 44 00  2016+112     19 36 27  68.4 150.3 -0.7     -25.8    -8   1  7    800  22 44 00
22 48 30  ---          19 40 57  68.9 153.0 -0.6     -23.5   262   F  1   2600

22 48 30  2029+121     19 40 57  68.2 144.4 -0.9     -30.8    -8   1  7   2600  22 48 30
22 50 00  ---          19 42 28  68.4 145.3 -0.8     -30.1    82   F  1   3200

22 50 00  2016+112     19 42 28  69.0 154.0 -0.6     -22.6    -8   1  7   3200  22 50 00
22 54 30  ---          19 46 58  69.4 156.9 -0.5     -20.2   262   F  1   5000

22 54 30  2029+121     19 46 58  69.0 147.9 -0.8     -27.9    -8   1  7   5000  22 54 30
22 56 00  ---          19 48 29  69.1 148.9 -0.7     -27.1    82   F  1   5600

22 56 00  2016+112     19 48 29  69.5 157.9 -0.5     -19.3    -8   1  7   5600  22 56 00
23 00 30  ---          19 52 59  69.9 160.9 -0.4     -16.7   262   F  1   7400

23 00 30  2029+121     19 52 59  69.6 151.7 -0.6     -24.7    -8   1  7   7400  23 00 30
23 02 00  ---          19 54 30  69.8 152.6 -0.6     -23.9    82   F  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

23 02 00  2016+112     19 54 30  70.0 161.9 -0.4     -15.8    -8   1  7   8000  23 02 00
23 06 30  ---          19 59 00  70.3 165.1 -0.3     -13.1   262   F  1   9800

23 06 30  2029+121     19 59 00  70.2 155.6 -0.5     -21.3    -8   1  7   9800  23 06 30
23 08 00  ---          20 00 31  70.3 156.6 -0.5     -20.5    82   F  1  10400

23 08 00  2016+112     20 00 31  70.3 166.2 -0.3     -12.1    -8   1  7  10400  23 08 00
23 12 30  ---          20 05 01  70.5 169.4 -0.2      -9.3   262   F  1  12200

23 12 30  2029+121     20 05 01  70.7 159.7 -0.4     -17.8    -8   1  7  12200  23 12 30
23 14 00  ---          20 06 31  70.8 160.8 -0.4     -16.8    82   F  1  12800

23 14 00  2016+112     20 06 31  70.6 170.5 -0.2      -8.3    -8   1  7  12800  23 14 00
23 18 30  ---          20 11 02  70.7 173.8 -0.1      -5.4   262   F  1  14600

23 18 30  2029+121     20 11 02  71.1 164.0 -0.3     -14.0    -9   1  7  14600  23 18 30
23 20 00  ---          20 12 32  71.2 165.2 -0.3     -13.0    81   F  1  15200

23 20 00  2016+112     20 12 32  70.8 174.9 -0.1      -4.5    -9   1  7  15200  23 20 00
23 24 30  ---          20 17 03  70.8 178.3  0.0      -1.5   261   F  1  17000

23 24 30  2029+121     20 17 03  71.4 168.5 -0.2     -10.1    -9   1  7  17000  23 24 30
23 26 00  ---          20 18 33  71.4 169.7 -0.2      -9.1    81   F  1  17600

23 29 00  2029+121     20 21 34  71.5 171.9 -0.2      -7.1   176   1  8  17600  23 29 00
23 31 00  ---          20 23 34  71.6 173.5 -0.1      -5.7   120   R  1  16800

23 31 00  2016+112     20 23 34  70.8 183.1  0.1       2.8    -8   1  8  16800  23 31 00
23 35 30  ---          20 28 05  70.7 186.5  0.1       5.7   262   R  1  15000

23 35 30  2029+121     20 28 05  71.7 177.0 -0.1      -2.7    -8   1  8  15000  23 35 30
23 37 00  ---          20 29 35  71.7 178.1  0.0      -1.6    82   R  1  14400

23 37 00  2016+112     20 29 35  70.7 187.6  0.2       6.7    -8   1  8  14400  23 37 00
23 41 30  ---          20 34 06  70.5 190.9  0.2       9.5   262   R  1  12600

23 41 30  2029+121     20 34 06  71.7 181.6  0.0       1.5    -8   1  8  12600  23 41 30
23 43 00  ---          20 35 36  71.7 182.8  0.1       2.5    82   R  1  12000

23 43 00  2016+112     20 35 36  70.5 192.0  0.3      10.5    -8   1  8  12000  23 43 00
23 47 30  ---          20 40 07  70.2 195.2  0.3      13.3   262   R  1  10200
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sat  17 Nov 2001   Day 321 ---

23 47 30  2029+121     20 40 07  71.6 186.3  0.1       5.6    -8   1  8  10200  23 47 30
23 49 00  ---          20 41 37  71.6 187.5  0.2       6.6    82   R  1   9600

23 49 00  2016+112     20 41 37  70.1 196.2  0.4      14.2    -8   1  8   9600  23 49 00
23 53 30  ---          20 46 08  69.8 199.4  0.4      16.9   262   R  1   7800

23 53 30  2029+121     20 46 08  71.4 190.9  0.2       9.6    -8   1  8   7800  23 53 30
23 55 00  ---          20 47 38  71.3 192.0  0.3      10.6    82   R  1   7200

23 55 00  2016+112     20 47 38  69.7 200.4  0.5      17.8    -8   1  8   7200  23 55 00
23 59 30  ---          20 52 09  69.4 203.4  0.5      20.4   262   R  1   5400

 --- Start: Sat  17 Nov 2001   Day 321 -- Stop: Sun  18 Nov 2001   Day 322 ---

23 59 30  2029+121     20 52 09  71.1 195.4  0.3      13.5    -7   1  8   5400  23 59 30
00 01 00  ---          20 53 39  71.0 196.5  0.4      14.5    83   R  1   4800

00 01 00  2016+112     20 53 39  69.2 204.3  0.6      21.2    -7   1  8   4800  00 01 00
00 05 30  ---          20 58 10  68.8 207.2  0.6      23.7   263   R  1   3000

00 05 30  2029+121     20 58 10  70.7 199.7  0.4      17.3    -7   1  8   3000  00 05 30
00 07 00  ---          20 59 40  70.6 200.8  0.5      18.2    83   R  1   2400

00 07 00  2016+112     20 59 40  68.7 208.1  0.7      24.5    -7   1  8   2400  00 07 00
00 11 30  ---          21 04 11  68.2 210.8  0.7      26.8   263   R  1    600

00 11 30  2029+121     21 04 11  70.2 203.9  0.5      20.9    -7   1  8    600  00 11 30
00 13 00  ---          21 05 41  70.1 204.9  0.6      21.8    83   R  1      0

00 16 00  2029+121     21 08 42  69.8 206.9  0.6      23.5   177   1  9      0  00 16 00
00 24 00  ---          21 16 43  69.0 211.9  0.7      27.7   480   F  1   3200

00 24 00  2016+112     21 16 43  66.7 217.8  1.0      32.6    -7   1  9   3200  00 24 00
00 28 30  ---          21 21 14  66.1 220.1  1.0      34.4   263   F  1   5000

00 28 30  2029+121     21 21 14  68.4 214.6  0.8      30.0    -7   1  9   5000  00 28 30
00 30 00  ---          21 22 44  68.3 215.4  0.8      30.7    83   F  1   5600

00 30 00  2016+112     21 22 44  65.9 220.8  1.1      35.0    -7   1  9   5600  00 30 00
00 34 30  ---          21 27 15  65.2 223.0  1.1      36.8   263   F  1   7400

00 34 30  2029+121     21 27 15  67.7 217.9  0.9      32.8    -7   1  9   7400  00 34 30
00 36 00  ---          21 28 45  67.5 218.7  0.9      33.4    83   F  1   8000
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

00 36 00  2016+112     21 28 45  65.0 223.7  1.2      37.3    -7   1  9   8000  00 36 00
00 40 30  ---          21 33 16  64.3 225.7  1.2      39.0   263   F  1   9800

00 40 30  2029+121     21 33 16  66.9 221.1  1.0      35.3    -7   1  9   9800  00 40 30
00 42 00  ---          21 34 46  66.6 221.8  1.0      36.0    83   F  1  10400

00 42 00  2016+112     21 34 46  64.1 226.4  1.3      39.5    -7   1  9  10400  00 42 00
00 46 30  ---          21 39 17  63.4 228.3  1.3      41.0   263   F  1  12200

00 46 30  2029+121     21 39 17  66.0 224.0  1.1      37.7    -7   1  9  12200  00 46 30
00 48 00  ---          21 40 47  65.8 224.7  1.1      38.3    83   F  1  12800

00 48 00  2016+112     21 40 47  63.1 228.9  1.4      41.4    -7   1  9  12800  00 48 00
00 52 30  ---          21 45 18  62.4 230.7  1.4      42.8   263   F  1  14600

00 52 30  2029+121     21 45 18  65.1 226.8  1.2      39.9    -7   1  9  14600  00 52 30
00 54 00  ---          21 46 48  64.8 227.4  1.2      40.4    83   F  1  15200

00 54 00  2016+112     21 46 48  62.1 231.3  1.5      43.2    -7   1  9  15200  00 54 00
00 58 30  ---          21 51 19  61.3 233.0  1.5      44.5   263   F  1  17000

00 58 30  2029+121     21 51 19  64.1 229.4  1.3      41.9    -8   1  9  17000  00 58 30
01 00 00  ---          21 52 49  63.9 230.0  1.3      42.4    82   F  1  17600

01 03 00  2029+121     21 55 49  63.4 231.2  1.4      43.3   177   1 10  17600  01 03 00
01 05 00  ---          21 57 50  63.0 232.0  1.4      43.9   120   R  1  16800

01 05 00  2016+112     21 57 50  60.2 235.3  1.6      46.2    -8   1 10  16800  01 05 00
01 09 30  ---          22 02 20  59.4 236.8  1.7      47.3   262   R  1  15000

01 09 30  2029+121     22 02 20  62.2 233.7  1.5      45.2    -8   1 10  15000  01 09 30
01 11 00  ---          22 03 51  62.0 234.2  1.5      45.6    82   R  1  14400

01 11 00  2016+112     22 03 51  59.1 237.3  1.7      47.6    -8   1 10  14400  01 11 00
01 15 30  ---          22 08 21  58.3 238.7  1.8      48.6   262   R  1  12600

01 15 30  2029+121     22 08 21  61.2 235.8  1.6      46.8    -8   1 10  12600  01 15 30
01 17 00  ---          22 09 52  60.9 236.4  1.6      47.2    82   R  1  12000

01 17 00  2016+112     22 09 52  58.0 239.1  1.8      48.9    -8   1 10  12000  01 17 00
01 21 30  ---          22 14 22  57.2 240.5  1.9      49.8   262   R  1  10200
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

01 21 30  2029+121     22 14 22  60.1 237.9  1.7      48.2    -8   1 10  10200  01 21 30
01 23 00  ---          22 15 53  59.8 238.4  1.7      48.6    82   R  1   9600

01 23 00  2016+112     22 15 53  56.9 240.9  1.9      50.1    -8   1 10   9600  01 23 00
01 27 30  ---          22 20 23  56.1 242.2  2.0      50.9   262   R  1   7800

01 27 30  2029+121     22 20 23  59.0 239.8  1.8      49.6    -8   1 10   7800  01 27 30
01 29 00  ---          22 21 54  58.7 240.2  1.8      49.9    82   R  1   7200

01 29 00  2016+112     22 21 54  55.8 242.6  2.0      51.2    -8   1 10   7200  01 29 00
01 33 30  ---          22 26 24  54.9 243.8  2.1      52.0   262   R  1   5400

01 33 30  2029+121     22 26 24  57.9 241.6  1.9      50.8    -8   1 10   5400  01 33 30
01 35 00  ---          22 27 55  57.6 242.0  1.9      51.1    82   R  1   4800

01 35 00  2016+112     22 27 55  54.6 244.2  2.1      52.2    -8   1 10   4800  01 35 00
01 39 30  ---          22 32 25  53.7 245.4  2.2      52.9   262   R  1   3000

01 39 30  2029+121     22 32 25  56.7 243.3  2.0      51.9    -8   1 10   3000  01 39 30
01 41 00  ---          22 33 56  56.4 243.7  2.0      52.1    82   R  1   2400

01 41 00  2016+112     22 33 56  53.4 245.7  2.2      53.2    -8   1 10   2400  01 41 00
01 45 30  ---          22 38 26  52.6 246.8  2.3      53.8   262   R  1    600

01 45 30  2029+121     22 38 26  55.6 244.9  2.1      52.9    -8   1 10    600  01 45 30
01 47 00  ---          22 39 57  55.3 245.3  2.1      53.1    82   R  1      0

01 50 00  2029+121     22 42 57  54.7 246.0  2.2      53.6   177   1 11      0  01 50 00
01 52 00  ---          22 44 57  54.3 246.5  2.2      53.9   120   F  1    800

01 52 00  2016+112     22 44 57  51.3 248.3  2.4      54.7    -8   1 11    800  01 52 00
01 56 30  ---          22 49 28  50.4 249.3  2.5      55.2   262   F  1   2600

01 56 30  2029+121     22 49 28  53.4 247.6  2.3      54.5    -8   1 11   2600  01 56 30
01 58 00  ---          22 50 58  53.1 248.0  2.3      54.7    82   F  1   3200

01 58 00  2016+112     22 50 58  50.1 249.7  2.5      55.4    -8   1 11   3200  01 58 00
02 02 30  ---          22 55 29  49.1 250.6  2.6      55.9   262   F  1   5000

02 02 30  2029+121     22 55 29  52.2 249.0  2.4      55.3    -8   1 11   5000  02 02 30
02 04 00  ---          22 56 59  51.9 249.4  2.4      55.5    82   F  1   5600
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

02 04 00  2016+112     22 56 59  48.8 250.9  2.6      56.1    -8   1 11   5600  02 04 00
02 08 30  ---          23 01 30  47.9 251.9  2.7      56.5   262   F  1   7400

02 08 30  2029+121     23 01 30  51.0 250.4  2.5      56.0    -8   1 11   7400  02 08 30
02 10 00  ---          23 03 00  50.7 250.7  2.5      56.2    82   F  1   8000

02 10 00  2016+112     23 03 00  47.6 252.2  2.7      56.7    -8   1 11   8000  02 10 00
02 14 30  ---          23 07 31  46.7 253.1  2.8      57.1   262   F  1   9800

02 14 30  2029+121     23 07 31  49.7 251.6  2.6      56.7    -8   1 11   9800  02 14 30
02 16 00  ---          23 09 01  49.4 251.9  2.6      56.9    82   F  1  10400

02 16 00  2016+112     23 09 01  46.4 253.3  2.8      57.3    -8   1 11  10400  02 16 00
02 20 30  ---          23 13 32  45.4 254.2  2.9      57.6   262   F  1  12200

02 20 30  2029+121     23 13 32  48.5 252.9  2.7      57.3    -8   1 11  12200  02 20 30
02 22 00  ---          23 15 02  48.2 253.1  2.7      57.5    82   F  1  12800

02 22 00  2016+112     23 15 02  45.1 254.5  2.9      57.8    -8   1 11  12800  02 22 00
02 26 30  ---          23 19 33  44.2 255.3  3.0      58.1   262   F  1  14600

02 26 30  2029+121     23 19 33  47.3 254.0  2.8      57.9    -8   1 11  14600  02 26 30
02 28 00  ---          23 21 03  47.0 254.3  2.8      58.0    82   F  1  15200

02 28 00  2016+112     23 21 03  43.9 255.6  3.0      58.2    -8   1 11  15200  02 28 00
02 32 30  ---          23 25 34  42.9 256.4  3.1      58.6   262   F  1  17000

02 32 30  2029+121     23 25 34  46.0 255.2  2.9      58.4    -8   1 11  17000  02 32 30
02 34 00  ---          23 27 04  45.7 255.4  2.9      58.5    82   F  1  17600

02 37 00  2029+121     23 30 05  45.1 256.0  3.0      58.7   177   1 12  17600  02 37 00
02 39 00  ---          23 32 05  44.7 256.3  3.0      58.9   120   R  1  16800

02 39 00  2016+112     23 32 05  41.6 257.5  3.2      59.0    -8   1 12  16800  02 39 00
02 43 30  ---          23 36 36  40.6 258.2  3.3      59.3   262   R  1  15000

02 43 30  2029+121     23 36 36  43.7 257.1  3.1      59.2    -8   1 12  15000  02 43 30
02 45 00  ---          23 38 06  43.4 257.4  3.1      59.3    82   R  1  14400

02 45 00  2016+112     23 38 06  40.3 258.5  3.3      59.3    -8   1 12  14400  02 45 00
02 49 30  ---          23 42 37  39.4 259.2  3.4      59.6   262   R  1  12600
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

02 49 30  2029+121     23 42 37  42.5 258.2  3.2      59.5    -8   1 12  12600  02 49 30
02 51 00  ---          23 44 07  42.1 258.4  3.2      59.6    82   R  1  12000

02 51 00  2016+112     23 44 07  39.0 259.5  3.4      59.7    -8   1 12  12000  02 51 00
02 55 30  ---          23 48 38  38.1 260.2  3.5      59.9   262   R  1  10200

02 55 30  2029+121     23 48 38  41.2 259.1  3.3      59.9    -8   1 12  10200  02 55 30
02 57 00  ---          23 50 08  40.9 259.4  3.3      60.0    82   R  1   9600

02 57 00  2016+112     23 50 08  37.8 260.4  3.5      60.0    -8   1 12   9600  02 57 00
03 01 30  ---          23 54 39  36.8 261.1  3.6      60.2   262   R  1   7800

03 01 30  2029+121     23 54 39  39.9 260.1  3.4      60.2    -8   1 12   7800  03 01 30
03 03 00  ---          23 56 09  39.6 260.4  3.4      60.3    82   R  1   7200

03 03 00  2016+112     23 56 09  36.5 261.3  3.6      60.2    -8   1 12   7200  03 03 00
03 07 30  ---          00 00 40  35.5 262.0  3.7      60.4   262   R  1   5400

03 07 30  2029+121     00 00 40  38.6 261.1  3.5      60.5    -8   1 12   5400  03 07 30
03 09 00  ---          00 02 10  38.3 261.3  3.5      60.5    82   R  1   4800

03 09 00  2016+112     00 02 10  35.2 262.2  3.7      60.4    -8   1 12   4800  03 09 00
03 13 30  ---          00 06 41  34.2 262.9  3.8      60.6   262   R  1   3000

03 13 30  2029+121     00 06 41  37.4 262.0  3.6      60.7    -8   1 12   3000  03 13 30
03 15 00  ---          00 08 11  37.0 262.2  3.6      60.8    82   R  1   2400

03 15 00  2016+112     00 08 11  33.9 263.1  3.8      60.6    -8   1 12   2400  03 15 00
03 19 30  ---          00 12 42  33.0 263.8  3.9      60.8   262   R  1    600

03 19 30  2029+121     00 12 42  36.1 262.9  3.7      60.9    -8   1 12    600  03 19 30
03 21 00  ---          00 14 12  35.8 263.1  3.7      61.0    82   R  1      0

03 24 00  2029+121     00 17 13  35.1 263.5  3.8      61.1   177   1 13      0  03 24 00
03 26 00  ---          00 19 13  34.7 263.8  3.8      61.1   120   F  1    800

03 26 00  2016+112     00 19 13  31.6 264.7  4.0      60.9    -8   1 13    800  03 26 00
03 30 30  ---          00 23 44  30.6 265.3  4.1      61.0   262   F  1   2600

03 30 30  2029+121     00 23 44  33.7 264.5  3.9      61.2    -8   1 13   2600  03 30 30
03 32 00  ---          00 25 14  33.4 264.7  3.9      61.3    82   F  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GLOBAL-6cm-2016+112
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun  18 Nov 2001   Day 322 ---

03 32 00  2016+112     00 25 14  30.3 265.5  4.1      61.1    -8   1 13   3200  03 32 00
03 36 30  ---          00 29 45  29.3 266.1  4.2      61.2   262   F  1   5000

03 36 30  2029+121     00 29 45  32.4 265.3  4.0      61.4    -8   1 13   5000  03 36 30
03 38 00  ---          00 31 15  32.1 265.5  4.0      61.4    82   F  1   5600

03 38 00  2016+112     00 31 15  29.0 266.3  4.2      61.2    -8   1 13   5600  03 38 00
03 42 30  ---          00 35 46  28.0 266.9  4.3      61.2   262   F  1   7400

03 42 30  2029+121     00 35 46  31.1 266.1  4.1      61.5    -8   1 13   7400  03 42 30
03 44 00  ---          00 37 16  30.8 266.3  4.1      61.5    82   F  1   8000

03 44 00  2016+112     00 37 16  27.7 267.1  4.3      61.3    -8   1 13   8000  03 44 00
03 48 30  ---          00 41 47  26.7 267.7  4.4      61.3   262   F  1   9800

03 48 30  2029+121     00 41 47  29.8 266.9  4.2      61.6    -8   1 13   9800  03 48 30
03 50 00  ---          00 43 17  29.5 267.1  4.2      61.6    82   F  1  10400

03 50 00  2016+112     00 43 17  26.4 267.9  4.4      61.3    -8   1 13  10400  03 50 00
03 54 30  ---          00 47 48  25.4 268.5  4.5      61.4   262   F  1  12200

03 54 30  2029+121     00 47 48  28.6 267.7  4.3      61.7    -8   1 13  12200  03 54 30
04 00 00  ---          00 53 18  27.4 268.5  4.4      61.7   322   F  1  14400


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gp030a.6cm
   Matches group v6cm_2 in /aps3/sched/catalogs/freq.dat

   Setup group:    8         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   8  Setup file default.  Used pcal sets:   1
   LO sum=    4982.49   4982.49   4990.49   4990.49
   BBC fr=     882.49    882.49    890.49    890.49
   Bandwd=      8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=   510   510  6510  6510     0     0     0     0
    PCALFR2=   510   510  6510  6510     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- GLOBAL-6cm-2016+112
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * 2016+112          20 16 55.366162   * 20 19 18.080000     20 19 21.840030 
                     11 17 44.94038    * 11 27 12.96000      11 27 38.45993 
                     From catalog imbedded in main SCHED input file.

 * 2029+121          20 29 32.681203   * 20 31 54.994210     20 31 58.810987 
                     12 09 28.75325    * 12 19 41.34040      12 20 08.53060 
                     From catalog imbedded in main SCHED input file.

 * 2134+004          21 34 05.207365   * 21 36 38.586300     21 36 43.117799 
                     00 28 25.08052    * 00 41 54.21335      00 42 23.61247 
                     From catalog imbedded in main SCHED input file.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   2016+112            76.9
   2029+121            80.1
   2134+004            91.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

