  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Mkn 273 GLOBAL 21cm
 Exp. Code:  GB055B  


Schedule Version:       2.00                                              
Processed by SCHED version:   6.02  July 2005                             

PI:       M. Bondi                                                        

Address:  Istituto di Radioastronomia                                     
          Via Gobetti 101, I-40129 Bologna                                
          Italy                                                           
                                                                          

Phone:    39-051-639 9386                                                 
EMAIL:    bondi@ira.inaf.it                                               
Fax:      39-051-639 9431                                                 
Phone during observation: 39-051-639 9386                                 

Observing mode: 256Mbps                                                   

Notes:    Phase referencing                                               
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

 Next scan frequencies:  1400.49  1400.49  1408.49  1408.49  1416.49  1416.49
                         1424.49  1424.49
 Next BBC frequencies:    999.51   999.51   991.51   991.51   983.51   983.51
                          975.51   975.51
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

12 08 00  J1337+550    08 07 34  28.7  40.5 -5.5     -76.7     0   1  1      0  12 08 00
12 10 00  ---          08 09 35  29.0  40.5 -5.5     -77.1   120   F  1      0  12 08 10

12 10 00  MKN273       08 09 35  28.3  39.3 -5.6     -76.2    -7   1  1      0  12 10 00
12 16 30  ---          08 16 06  29.2  39.6 -5.5     -77.5   383   F  1      0  12 10 10

12 16 30  J1337+550    08 16 06  29.9  40.8 -5.4     -78.3    -8   1  1      0  12 16 30
12 20 00  ---          08 19 36  30.4  40.9 -5.3     -79.0   202   F  1      0  12 16 40

12 20 00  MKN273       08 19 36  29.6  39.7 -5.4     -78.1    -8   1  1      0  12 20 00
12 26 30  ---          08 26 07  30.5  39.9 -5.3     -79.4   382   F  1      0  12 20 10

12 26 30  J1337+550    08 26 07  31.3  41.1 -5.2     -80.2    -8   1  1      0  12 26 30
12 30 00  ---          08 29 38  31.8  41.2 -5.1     -80.9   202   F  1      0  12 26 40

12 32 00  J1337+550    08 31 38  32.1  41.2 -5.1     -81.2   114   1  1      0  12 32 00
12 34 00  ---          08 33 39  32.4  41.3 -5.1     -81.6   120   F  1      0  12 32 10

12 34 00  MKN273       08 33 39  31.6  40.1 -5.2     -80.8    -8   1  1      0  12 34 00
12 40 30  ---          08 40 10  32.5  40.2 -5.1     -82.1   382   F  1      0  12 34 10

12 40 30  J1337+550    08 40 10  33.3  41.4 -5.0     -82.9    -8   1  1      0  12 40 30
12 44 00  ---          08 43 40  33.8  41.5 -4.9     -83.6   202   F  1      0  12 40 40

12 44 00  MKN273       08 43 40  33.0  40.3 -5.0     -82.8    -8   1  1      0  12 44 00
12 50 30  ---          08 50 11  33.9  40.5 -4.9     -84.1   382   F  1      0  12 44 10

12 50 30  J1337+550    08 50 11  34.8  41.6 -4.8     -84.8    -8   1  1      0  12 50 30
12 54 00  ---          08 53 42  35.3  41.7 -4.7     -85.5   202   F  1      0  12 50 40

12 55 00  J1337+550    08 54 42  35.4  41.7 -4.7     -85.7    54   1  1      0  12 55 00
12 57 00  ---          08 56 42  35.7  41.7 -4.7     -86.1   120   F  1      0  12 55 10

12 57 00  MKN273       08 56 42  34.8  40.6 -4.8     -85.4    -8   1  1      0  12 57 00
13 03 30  ---          09 03 13  35.7  40.6 -4.7     -86.7   382   F  1      0  12 57 10
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

13 03 30  J1337+550    09 03 13  36.6  41.8 -4.6     -87.4    -8   1  1      0  13 03 30
13 07 00  ---          09 06 44  37.1  41.8 -4.5     -88.1   202   F  1      0  13 03 40

13 07 00  MKN273       09 06 44  36.2  40.7 -4.6     -87.4    -8   1  1      0  13 07 00
13 13 30  ---          09 13 15  37.1  40.7 -4.5     -88.7   382   F  1      0  13 07 10

13 13 30  J1337+550    09 13 15  38.1  41.8 -4.4     -89.4    -8   1  1      0  13 13 30
13 17 00  ---          09 16 46  38.6  41.8 -4.4     -90.1   202   F  1      0  13 13 40

13 18 00  J1337+550    09 17 46  38.7  41.8 -4.3     -90.3    54   1  1      0  13 18 00
13 20 00  ---          09 19 46  39.0  41.8 -4.3     -90.8   120   F  1      0  13 18 10

13 20 00  MKN273       09 19 46  38.0  40.7 -4.4     -90.0    -8   1  1      0  13 20 00
13 26 30  ---          09 26 17  38.9  40.7 -4.3     -91.4   382   F  1      0  13 20 10

13 26 30  J1337+550    09 26 17  39.9  41.8 -4.2     -92.1    -8   1  1      0  13 26 30
13 30 00  ---          09 29 48  40.4  41.8 -4.1     -92.9   202   F  1      0  13 26 40

13 30 00  MKN273       09 29 48  39.4  40.7 -4.3     -92.1    -8   1  1      0  13 30 00
13 36 30  ---          09 36 19  40.3  40.6 -4.1     -93.5   382   F  1      0  13 30 10

13 36 30  J1337+550    09 36 19  41.4  41.7 -4.0     -94.2    -8   1  1      0  13 36 30
13 40 00  ---          09 39 49  41.9  41.6 -4.0     -95.0   202   F  1      0  13 36 40

13 42 00  J1337+550    09 41 50  42.2  41.6 -3.9     -95.4   114   1  1      0  13 42 00
13 44 00  ---          09 43 50  42.5  41.6 -3.9     -95.9   120   F  1      0  13 42 10

13 44 00  MKN273       09 43 50  41.4  40.5 -4.0     -95.1    -8   1  1      0  13 44 00
13 50 30  ---          09 50 21  42.3  40.4 -3.9     -96.6   382   F  1      0  13 44 10

13 50 30  J1337+550    09 50 21  43.4  41.4 -3.8     -97.3    -8   1  1      0  13 50 30
13 54 00  ---          09 53 52  43.9  41.3 -3.7     -98.1   202   F  1      0  13 50 40

13 54 00  MKN273       09 53 52  42.8  40.3 -3.9     -97.4    -8   1  1      0  13 54 00
14 00 30  ---          10 00 23  43.7  40.1 -3.7     -98.8   382   F  1      0  13 54 10

14 00 30  J1337+550    10 00 23  44.8  41.1 -3.6     -99.6    -8   1  1      0  14 00 30
14 04 00  ---          10 03 53  45.3  41.0 -3.6    -100.4   202   F  1      0  14 00 40

14 05 00  J1337+550    10 04 53  45.4  41.0 -3.6    -100.6    54   1  1      0  14 05 00
14 07 00  ---          10 06 54  45.7  40.9 -3.5    -101.1   120   F  1      0  14 05 10

14 07 00  MKN273       10 06 54  44.6  39.9 -3.6    -100.3    -8   1  1      0  14 07 00
14 13 30  ---          10 13 25  45.5  39.7 -3.5    -101.8   382   F  1      0  14 07 10
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

14 13 30  J1337+550    10 13 25  46.6  40.6 -3.4    -102.6    -8   1  1      0  14 13 30
14 17 00  ---          10 16 55  47.1  40.4 -3.4    -103.4   202   F  1      0  14 13 40

14 17 00  MKN273       10 16 55  46.0  39.5 -3.5    -102.7    -8   1  1      0  14 17 00
14 23 30  ---          10 23 27  46.9  39.2 -3.4    -104.3   382   F  1      0  14 17 10

14 23 30  J1337+550    10 23 27  48.0  40.1 -3.2    -105.0    -8   1  1      0  14 23 30
14 27 00  ---          10 26 57  48.5  39.9 -3.2    -105.9   202   F  1      0  14 23 40

14 28 00  J1337+550    10 27 57  48.7  39.8 -3.2    -106.1    55   1  1      0  14 28 00
14 30 00  ---          10 29 58  48.9  39.7 -3.1    -106.6   120   F  1      0  14 28 10

14 30 00  MKN273       10 29 58  47.8  38.9 -3.2    -105.9    -8   1  1      0  14 30 00
14 36 30  ---          10 36 29  48.6  38.5 -3.1    -107.5   382   F  1      0  14 30 10

14 36 30  J1337+550    10 36 29  49.8  39.3 -3.0    -108.3    -8   1  1      0  14 36 30
14 40 00  ---          10 39 59  50.3  39.0 -3.0    -109.2   202   F  1      0  14 36 40

14 40 00  OQ208        10 39 59  45.3  79.1 -3.5     -73.9   -33   1  1      0  14 40 00
14 50 00  ---          10 50 01  47.4  80.0 -3.3     -74.5   567   F  1      0  14 40 10

14 54 00  J1337+550    10 54 02  52.2  37.9 -2.7    -113.0   206   1  1      0  14 54 00
14 56 00  ---          10 56 02  52.4  37.7 -2.7    -113.5   120   F  1      0  14 54 10

14 56 00  MKN273       10 56 02  51.2  37.0 -2.8    -112.7    -8   1  1      0  14 56 00
15 02 30  ---          11 02 33  52.0  36.4 -2.7    -114.5   382   F  1      0  14 56 10

15 02 30  J1337+550    11 02 33  53.3  37.0 -2.6    -115.4    -9   1  1      0  15 02 30
15 06 00  ---          11 06 04  53.7  36.7 -2.5    -116.4   201   F  1      0  15 02 40

15 06 00  MKN273       11 06 04  52.5  36.1 -2.6    -115.5    -9   1  1      0  15 06 00
15 12 30  ---          11 12 35  53.3  35.4 -2.5    -117.4   381   F  1      0  15 06 10

15 12 30  J1337+550    11 12 35  54.6  35.9 -2.4    -118.3    -9   1  1      0  15 12 30
15 16 00  ---          11 16 05  55.0  35.5 -2.4    -119.4   201   F  1      0  15 12 40

15 18 00  J1337+550    11 18 05  55.3  35.3 -2.3    -120.0   114   1  1      0  15 18 00
15 20 00  ---          11 20 06  55.5  35.0 -2.3    -120.6   120   F  1      0  15 18 10

15 20 00  MKN273       11 20 06  54.2  34.6 -2.4    -119.6    -9   1  1      0  15 20 00
15 26 30  ---          11 26 37  55.0  33.7 -2.3    -121.6   381   F  1      0  15 20 10

15 26 30  J1337+550    11 26 37  56.3  34.1 -2.2    -122.7    -9   1  1      0  15 26 30
15 30 00  ---          11 30 07  56.7  33.6 -2.1    -123.8   201   F  1      0  15 26 40
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

15 30 00  MKN273       11 30 07  55.4  33.3 -2.2    -122.7    -9   1  1      0  15 30 00
15 36 30  ---          11 36 39  56.2  32.4 -2.1    -124.8   381   F  1      0  15 30 10

15 36 30  J1337+550    11 36 39  57.5  32.7 -2.0    -126.0    -9   1  1      0  15 36 30
15 40 00  ---          11 40 09  57.9  32.1 -2.0    -127.2   201   F  1      0  15 36 40

15 41 00  J1337+550    11 41 09  58.0  31.9 -1.9    -127.5    55   1  1      0  15 41 00
15 43 00  ---          11 43 10  58.2  31.6 -1.9    -128.2   120   F  1      0  15 41 10

15 43 00  MKN273       11 43 10  56.9  31.4 -2.0    -127.0    -9   1  1      0  15 43 00
15 49 30  ---          11 49 41  57.7  30.4 -1.9    -129.2   381   F  1      0  15 43 10

15 49 30  J1337+550    11 49 41  59.0  30.5 -1.8    -130.5    -9   1  1      0  15 49 30
15 53 00  ---          11 53 11  59.3  29.8 -1.7    -131.8   201   F  1      0  15 49 40

15 53 00  MKN273       11 53 11  58.0  29.8 -1.9    -130.4    -9   1  1      0  15 53 00
15 59 30  ---          11 59 42  58.7  28.6 -1.8    -132.8   381   F  1      0  15 53 10

15 59 30  J1337+550    11 59 42  60.0  28.5 -1.6    -134.2    -9   1  1      0  15 59 30
16 03 00  ---          12 03 13  60.4  27.8 -1.6    -135.6   201   F  1      0  15 59 40

16 04 00  J1337+550    12 04 13  60.5  27.6 -1.6    -136.0    55   1  1      0  16 04 00
16 06 00  ---          12 06 13  60.7  27.2 -1.5    -136.7   120   F  1      0  16 04 10

16 06 00  MKN273       12 06 13  59.4  27.4 -1.6    -135.2    -9   1  1      0  16 06 00
16 12 30  ---          12 12 44  60.0  26.1 -1.5    -137.6   381   F  1      0  16 06 10

16 12 30  J1337+550    12 12 44  61.3  25.8 -1.4    -139.3    -9   1  1      0  16 12 30
16 16 00  ---          12 16 15  61.6  25.0 -1.4    -140.8   201   F  1      0  16 12 40

16 16 00  MKN273       12 16 15  60.3  25.3 -1.5    -139.0    -9   1  1      0  16 16 00
16 22 30  ---          12 22 46  60.9  23.9 -1.4    -141.6   381   F  1      0  16 16 10

16 22 30  J1337+550    12 22 46  62.2  23.4 -1.3    -143.5    -9   1  1      0  16 22 30
16 26 00  ---          12 26 17  62.5  22.5 -1.2    -145.0   201   F  1      0  16 22 40

16 30 00  J1337+550    12 30 17  62.8  21.5 -1.1    -146.7   234   1  1      0  16 30 00
16 32 00  ---          12 32 18  63.0  20.9 -1.1    -147.6   120   F  1      0  16 30 10

16 32 00  MKN273       12 32 18  61.7  21.7 -1.2    -145.6    -9   1  1      0  16 32 00
16 38 30  ---          12 38 49  62.2  20.0 -1.1    -148.3   381   F  1      0  16 32 10

16 38 30  J1337+550    12 38 49  63.5  19.2 -1.0    -150.5    -8   1  1      0  16 38 30
16 42 00  ---          12 42 19  63.7  18.2 -0.9    -152.1   202   F  1      0  16 38 40
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

16 42 00  MKN273       12 42 19  62.5  19.1 -1.0    -149.9    -8   1  1      0  16 42 00
16 48 30  ---          12 48 50  62.9  17.4 -0.9    -152.8   382   F  1      0  16 42 10

16 48 30  J1337+550    12 48 50  64.1  16.3 -0.8    -155.2    -8   1  1      0  16 48 30
16 52 00  ---          12 52 21  64.3  15.2 -0.8    -156.8   202   F  1      0  16 48 40

16 53 00  J1337+550    12 53 21  64.4  14.9 -0.7    -157.3    55   1  1      0  16 53 00
16 55 00  ---          12 55 21  64.5  14.3 -0.7    -158.3   120   F  1      0  16 53 10

16 55 00  MKN273       12 55 21  63.3  15.5 -0.8    -155.7    -8   1  1      0  16 55 00
17 01 30  ---          13 01 52  63.7  13.7 -0.7    -158.8   382   F  1      0  16 55 10

17 01 30  J1337+550    13 01 52  64.8  12.2 -0.6    -161.5    -8   1  1      0  17 01 30
17 05 00  ---          13 05 23  65.0  11.1 -0.5    -163.2   202   F  1      0  17 01 40

17 05 00  MKN273       13 05 23  63.8  12.6 -0.7    -160.4    -8   1  1      0  17 05 00
17 11 30  ---          13 11 54  64.1  10.6 -0.5    -163.6   382   F  1      0  17 05 10

17 11 30  J1337+550    13 11 54  65.2   9.0 -0.4    -166.5    -8   1  1      0  17 11 30
17 15 00  ---          13 15 25  65.3   7.8 -0.4    -168.3   202   F  1      0  17 11 40

17 16 00  J1337+550    13 16 25  65.3   7.4 -0.4    -168.8    55   1  1      0  17 16 00
17 18 00  ---          13 18 25  65.4   6.8 -0.3    -169.8   120   F  1      0  17 16 10

17 18 00  MKN273       13 18 25  64.3   8.6 -0.4    -166.8    -8   1  1      0  17 18 00
17 24 30  ---          13 24 56  64.5   6.5 -0.3    -170.0   382   F  1      0  17 18 10

17 24 30  J1337+550    13 24 56  65.5   4.5 -0.2    -173.2    -8   1  1      0  17 24 30
17 28 00  ---          13 28 27  65.6   3.3 -0.2    -175.0   202   F  1      0  17 24 40

17 28 00  MKN273       13 28 27  64.6   5.4 -0.3    -171.7    -8   1  1      0  17 28 00
17 34 30  ---          13 34 58  64.7   3.3 -0.2    -175.0   382   F  1      0  17 28 10

17 34 30  J1337+550    13 34 58  65.6   1.1 -0.1    -178.4    -8   1  1      0  17 34 30
17 38 00  ---          13 38 28  65.6  -0.2  0.0     179.8   202   F  1      0  17 34 40

17 40 00  J1337+550    13 40 29  65.6  -0.9  0.0     178.7   114   1  1      0  17 40 00
17 42 00  ---          13 42 29  65.6  -1.6  0.1     177.7   120   F  1      0  17 40 10

17 42 00  MKN273       13 42 29  64.8   0.8  0.0    -178.8    -8   1  1      0  17 42 00
17 48 30  ---          13 49 00  64.8  -1.4  0.1     177.9   382   F  1      0  17 42 10

17 48 30  J1337+550    13 49 00  65.6  -3.8  0.2     174.3    -8   1  1      0  17 48 30
17 52 00  ---          13 52 31  65.5  -5.0  0.2     172.5   202   F  1      0  17 48 40
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

17 52 00  MKN273       13 52 31  64.7  -2.5  0.1     176.2    -8   1  1      0  17 52 00
17 58 30  ---          13 59 02  64.7  -4.6  0.2     172.9   382   F  1      0  17 52 10

17 58 30  J1337+550    13 59 02  65.4  -7.2  0.4     169.1    -8   1  1      0  17 58 30
18 02 00  ---          14 02 32  65.3  -8.4  0.4     167.3   202   F  1      0  17 58 40

18 03 00  J1337+550    14 03 33  65.2  -8.8  0.4     166.8    55   1  1      0  18 03 00
18 05 00  ---          14 05 33  65.2  -9.4  0.5     165.8   120   F  1      0  18 03 10

18 05 00  MKN273       14 05 33  64.5  -6.7  0.3     169.6    -8   1  1      0  18 05 00
18 11 30  ---          14 12 04  64.3  -8.8  0.5     166.4   382   F  1      0  18 05 10

18 11 30  J1337+550    14 12 04  64.9 -11.5  0.6     162.5    -8   1  1      0  18 11 30
18 15 00  ---          14 15 35  64.7 -12.7  0.6     160.8   202   F  1      0  18 11 40

18 15 00  MKN273       14 15 35  64.2  -9.9  0.5     164.7    -8   1  1      0  18 15 00
18 21 30  ---          14 22 06  63.9 -11.9  0.6     161.5   382   F  1      0  18 15 10

18 21 30  J1337+550    14 22 06  64.4 -14.7  0.7     157.6    -8   1  1      0  18 21 30
18 25 00  ---          14 25 36  64.2 -15.8  0.8     155.9   202   F  1      0  18 21 40

18 27 00  J1337+550    14 27 37  64.1 -16.4  0.8     155.0   114   1  1      0  18 27 00
18 29 00  ---          14 29 37  64.0 -17.0  0.9     154.0   120   F  1      0  18 27 10

18 29 00  MKN273       14 29 37  63.6 -14.2  0.7     158.0    -8   1  1      0  18 29 00
18 35 30  ---          14 36 08  63.2 -16.0  0.9     155.0   382   F  1      0  18 29 10

18 35 30  J1337+550    14 36 08  63.5 -18.8  1.0     151.0    -8   1  1      0  18 35 30
18 39 00  ---          14 39 38  63.3 -19.8  1.0     149.4   202   F  1      0  18 35 40

18 39 00  MKN273       14 39 38  63.0 -17.0  0.9     153.4    -8   1  1      0  18 39 00
18 45 30  ---          14 46 10  62.6 -18.8  1.0     150.4   382   F  1      0  18 39 10

18 45 30  J1337+550    14 46 10  62.8 -21.6  1.1     146.5    -8   1  1      0  18 45 30
18 49 00  ---          14 49 40  62.5 -22.5  1.2     145.0   202   F  1      0  18 45 40

18 51 00  J1337+550    14 51 40  62.3 -23.0  1.2     144.2   114   1  1      0  18 51 00
18 53 00  ---          14 53 41  62.2 -23.5  1.3     143.3   120   F  1      0  18 51 10

18 53 00  MKN273       14 53 41  62.0 -20.7  1.1     147.2    -8   1  1      0  18 53 00
18 59 30  ---          15 00 12  61.5 -22.3  1.3     144.4   382   F  1      0  18 53 10

18 59 30  J1337+550    15 00 12  61.6 -25.0  1.4     140.6    -8   1  1      0  18 59 30
19 03 00  ---          15 03 42  61.3 -25.8  1.4     139.2   202   F  1      0  18 59 40
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

19 03 00  MKN273       15 03 42  61.2 -23.1  1.3     143.0    -8   1  1      0  19 03 00
19 09 30  ---          15 10 14  60.6 -24.6  1.4     140.3   382   F  1      0  19 03 10

19 09 30  J1337+550    15 10 14  60.6 -27.3  1.5     136.6    -8   1  1      0  19 09 30
19 13 00  ---          15 13 44  60.3 -28.0  1.6     135.2   202   F  1      0  19 09 40

19 14 00  J1337+550    15 14 44  60.2 -28.2  1.6     134.8    55   1  1      0  19 14 00
19 16 00  ---          15 16 45  60.0 -28.6  1.6     134.1   120   F  1      0  19 14 10

19 16 00  MKN273       15 16 45  60.0 -26.0  1.5     137.8    -8   1  1      0  19 16 00
19 22 30  ---          15 23 16  59.4 -27.3  1.6     135.3   382   F  1      0  19 16 10

19 22 30  J1337+550    15 23 16  59.3 -29.9  1.8     131.7    -8   1  1      0  19 22 30
19 26 00  ---          15 26 46  58.9 -30.5  1.8     130.4   202   F  1      0  19 22 40

19 26 00  OQ208        15 26 46  72.6 267.7  1.3      77.9  -205   1  1      0  19 26 00
19 36 00  ---          15 36 48  70.4 269.2  1.5      78.0   395   F  1      0  19 26 10

19 40 00  J1337+550    15 40 49  57.3 327.1  2.0     125.5   195   1  1      0  19 40 00
19 42 00  ---          15 42 49  57.1 326.8  2.1     124.9   120   F  1      0  19 40 10

19 42 00  MKN273       15 42 49  57.4 329.2  2.0     128.3    -8   1  1      0  19 42 00
19 48 30  ---          15 49 20  56.6 328.2  2.1     126.1   382   F  1      0  19 42 10

19 48 30  J1337+550    15 49 20  56.3 325.9  2.2     122.7    -7   1  1      0  19 48 30
19 52 00  ---          15 52 50  55.9 325.4  2.2     121.6   203   F  1      0  19 48 40

19 52 00  MKN273       15 52 50  56.2 327.7  2.1     124.9    -7   1  1      0  19 52 00
19 58 30  ---          15 59 22  55.5 326.7  2.2     122.8   383   F  1      0  19 52 10

19 58 30  J1337+550    15 59 22  55.1 324.6  2.4     119.6    -7   1  1      0  19 58 30
20 02 00  ---          16 02 52  54.7 324.1  2.4     118.5   203   F  1      0  19 58 40

20 03 00  J1337+550    16 03 52  54.5 324.0  2.4     118.2    55   1  1      0  20 03 00
20 05 00  ---          16 05 53  54.3 323.8  2.5     117.6   120   F  1      0  20 03 10

20 05 00  MKN273       16 05 53  54.7 325.9  2.3     120.8    -7   1  1      0  20 05 00
20 11 30  ---          16 12 24  53.9 325.1  2.5     118.8   383   F  1      0  20 05 10

20 11 30  J1337+550    16 12 24  53.4 323.1  2.6     115.7    -7   1  1      0  20 11 30
20 15 00  ---          16 15 54  53.0 322.7  2.6     114.7   203   F  1      0  20 11 40

20 15 00  MKN273       16 15 54  53.5 324.7  2.5     117.7    -7   1  1      0  20 15 00
20 21 30  ---          16 22 25  52.7 324.1  2.6     115.8   383   F  1      0  20 15 10
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

20 21 30  J1337+550    16 22 25  52.1 322.1  2.7     112.9    -7   1  1      0  20 21 30
20 25 00  ---          16 25 56  51.7 321.8  2.8     111.9   203   F  1      0  20 21 40

20 27 00  J1337+550    16 27 56  51.4 321.6  2.8     111.4   114   1  1      0  20 27 00
20 29 00  ---          16 29 57  51.1 321.4  2.9     110.8   120   F  1      0  20 27 10

20 29 00  MKN273       16 29 57  51.7 323.3  2.8     113.7    -7   1  1      0  20 29 00
20 35 30  ---          16 36 28  50.9 322.8  2.9     111.9   383   F  1      0  20 29 10

20 35 30  J1337+550    16 36 28  50.2 320.9  3.0     109.1    -7   1  1      0  20 35 30
20 39 00  ---          16 39 58  49.8 320.7  3.0     108.2   203   F  1      0  20 35 40

20 39 00  MKN273       16 39 58  50.4 322.5  2.9     111.0    -7   1  1      0  20 39 00
20 45 30  ---          16 46 29  49.5 322.0  3.0     109.3   383   F  1      0  20 39 10

20 45 30  J1337+550    16 46 29  48.9 320.3  3.1     106.5    -7   1  1      0  20 45 30
20 49 00  ---          16 50 00  48.4 320.1  3.2     105.7   203   F  1      0  20 45 40

20 51 00  J1337+550    16 52 00  48.1 319.9  3.2     105.2   114   1  1      0  20 51 00
20 53 00  ---          16 54 01  47.8 319.8  3.3     104.7   120   F  1      0  20 51 10

20 53 00  MKN273       16 54 01  48.5 321.5  3.2     107.3    -7   1  1      0  20 53 00
20 56 00  ---          16 57 01  48.1 321.3  3.2     106.6   173   F  1      0  20 53 10

20 56 00  J1337+550    16 57 01  47.4 319.7  3.3     103.9    -7   1  1      0  20 56 00
20 59 30  ---          17 00 32  46.9 319.5  3.4     103.1   203   F  1      0  20 56 10

20 59 30  MKN273       17 00 32  47.7 321.1  3.3     105.7    -7   1  1      0  20 59 30
21 06 00  ---          17 07 03  46.8 320.7  3.4     104.1   383   F  1      0  20 59 40

21 06 00  J1337+550    17 07 03  46.0 319.2  3.5     101.5    -7   1  1      0  21 06 00
21 09 30  ---          17 10 33  45.5 319.1  3.5     100.7   203   F  1      0  21 06 10

21 09 30  MKN273       17 10 33  46.3 320.6  3.4     103.2    -8   1  1      0  21 09 30
21 13 00  ---          17 14 04  45.8 320.4  3.5     102.4   202   F  1      0  21 09 40

21 14 00  J1337+550    17 15 04  44.9 318.9  3.6      99.7    52   1  1      0  21 14 00
21 16 00  ---          17 17 04  44.6 318.8  3.7      99.2   120   F  1      0  21 14 10

21 16 00  MKN273       17 17 04  45.4 320.3  3.5     101.7    -8   1  1      0  21 16 00
21 22 30  ---          17 23 35  44.5 320.1  3.6     100.2   382   F  1      0  21 16 10

21 22 30  J1337+550    17 23 35  43.7 318.6  3.8      97.8    -8   1  1      0  21 22 30
21 26 00  ---          17 27 06  43.2 318.6  3.8      97.0   202   F  1      0  21 22 40
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

21 26 00  3C345        17 27 06  77.2 318.7  0.7     132.3   -74   1  1      0  21 26 00
21 36 00  ---          17 37 08  75.7 313.5  0.9     125.7   526   F  1      0  21 26 10

21 40 00  J1337+550    17 41 08  41.2 318.3  4.1      93.9   165   1  1      0  21 40 00
21 42 00  ---          17 43 09  40.9 318.3  4.1      93.5   120   F  1      0  21 40 10

21 42 00  MKN273       17 43 09  41.8 319.5  4.0      95.8    -8   1  1      0  21 42 00
21 48 30  ---          17 49 40  40.9 319.4  4.1      94.3   382   F  1      0  21 42 10

21 48 30  J1337+550    17 49 40  40.0 318.2  4.2      92.1    -8   1  1      0  21 48 30
21 52 00  ---          17 53 10  39.5 318.2  4.3      91.4   202   F  1      0  21 48 40

21 52 00  MKN273       17 53 10  40.4 319.4  4.1      93.6    -8   1  1      0  21 52 00
21 58 30  ---          17 59 41  39.5 319.3  4.2      92.2   382   F  1      0  21 52 10

21 58 30  J1337+550    17 59 41  38.5 318.2  4.4      90.1    -8   1  1      0  21 58 30
22 02 00  ---          18 03 12  38.0 318.2  4.4      89.3   202   F  1      0  21 58 40

22 03 00  J1337+550    18 04 12  37.9 318.2  4.4      89.1    54   1  1      0  22 03 00
22 05 00  ---          18 06 12  37.6 318.2  4.5      88.7   120   F  1      0  22 03 10

22 05 00  MKN273       18 06 12  38.6 319.3  4.4      90.8    -8   1  1      0  22 05 00
22 11 30  ---          18 12 43  37.6 319.3  4.5      89.5   382   F  1      0  22 05 10

22 11 30  J1337+550    18 12 43  36.6 318.2  4.6      87.4    -8   1  1      0  22 11 30
22 15 00  ---          18 16 14  36.1 318.3  4.6      86.7   202   F  1      0  22 11 40

22 15 00  MKN273       18 16 14  37.2 319.3  4.5      88.8    -8   1  1      0  22 15 00
22 21 30  ---          18 22 45  36.2 319.3  4.6      87.4   382   F  1      0  22 15 10

22 21 30  J1337+550    18 22 45  35.2 318.3  4.7      85.4    -8   1  1      0  22 21 30
22 25 00  ---          18 26 16  34.7 318.4  4.8      84.7   202   F  1      0  22 21 40

22 27 00  J1337+550    18 28 16  34.4 318.4  4.8      84.4   114   1  1      0  22 27 00
22 29 00  ---          18 30 16  34.1 318.5  4.9      84.0   120   F  1      0  22 27 10

22 29 00  MKN273       18 30 16  35.2 319.4  4.8      85.9    -8   1  1      0  22 29 00
22 35 30  ---          18 36 47  34.3 319.5  4.9      84.6   382   F  1      0  22 29 10

22 35 30  J1337+550    18 36 47  33.2 318.6  5.0      82.7    -8   1  1      0  22 35 30
22 39 00  ---          18 40 18  32.7 318.7  5.0      82.0   202   F  1      0  22 35 40

22 39 00  MKN273       18 40 18  33.8 319.6  4.9      83.9    -8   1  1      0  22 39 00
22 45 30  ---          18 46 49  32.9 319.7  5.0      82.6   382   F  1      0  22 39 10
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Mkn 273 GLOBAL 21cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri   4 Nov 2005   Day 308 ---

22 45 30  J1337+550    18 46 49  31.8 318.8  5.1      80.8    -8   1  1      0  22 45 30
22 49 00  ---          18 50 20  31.3 318.9  5.2      80.1   202   F  1      0  22 45 40

22 50 00  J1337+550    18 51 20  31.1 319.0  5.2      79.9    54   1  1      0  22 50 00
22 52 00  ---          18 53 20  30.9 319.0  5.3      79.5   120   F  1      0  22 50 10

22 52 00  MKN273       18 53 20  32.0 319.8  5.1      81.4    -8   1  1      0  22 52 00
22 58 30  ---          18 59 51  31.1 320.0  5.2      80.1   382   F  1      0  22 52 10

22 58 30  J1337+550    18 59 51  29.9 319.2  5.4      78.3    -8   1  1      0  22 58 30
23 02 00  ---          19 03 22  29.5 319.4  5.4      77.7   202   F  1      0  22 58 40

23 02 00  MKN273       19 03 22  30.6 320.1  5.3      79.4    -8   1  1      0  23 02 00
23 08 30  ---          19 09 53  29.7 320.3  5.4      78.2   382   F  1      0  23 02 10

23 08 30  J1337+550    19 09 53  28.5 319.6  5.5      76.4    -8   1  1      0  23 08 30
23 12 00  ---          19 13 23  28.1 319.7  5.6      75.8   202   F  1      0  23 08 40


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: gb055b.21cm
   Matches group v20cm_2 in /irasoft/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:   11         Station: VLBA_FD           Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:  11  Setup file default.  Used pcal sets:   1
   LO sum=    1400.49   1400.49   1408.49   1408.49   1416.49   1416.49   1424.49   1424.49
   BBC fr=     999.51    999.51    991.51    991.51    983.51    983.51    975.51    975.51
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510  6510  6510  6510  6510
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_off 
 SOURCE LIST -- Mkn 273 GLOBAL 21cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * MKN273            13 42 51.721505   * 13 44 42.142000     13 44 53.354260       0.00
                     56 08 13.98754    * 55 53 13.15000      55 51 24.10327        0.00
                     From catalog imbedded in main SCHED input file.
                        9.208 scan hours,    581.056 baseline hours above horizon.

 * J1337+550         13 35 55.218449   * 13 37 49.642224     13 38 01.368505       0.00
                     55 16 15.76062    * 55 01 02.11786      54 59 11.51016        0.00
                     From catalog imbedded in main SCHED input file.
                        6.508 scan hours,    397.707 baseline hours above horizon.

   J1407+2827        14 04 45.615155   * 14 07 00.394413     14 07 14.666532       0.23
   1404+286          28 41 29.23518    * 28 27 14.69021      28 25 35.38265        0.40
   J1407+28          /irasoft/sched/catalogs/sources.vlba
 * OQ208             VLBA Calib Srcs - GSFC sols. - catalog 2004f_astro
                        0.475 scan hours,     21.078 baseline hours above horizon.

   J1642+3948        16 41 17.606231   * 16 42 58.809968     16 43 09.037734       0.26
   1641+399          39 54 10.81493    * 39 48 36.99399      39 48 00.83750        0.40
 * 3C345             /irasoft/sched/catalogs/sources.vlba
   J1642+39          VLBA Calib Srcs - GSFC sols. - catalog 2004f_astro
                        0.308 scan hours,      8.657 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   MKN273              72.3
   J1337+550           71.7
   OQ208               44.6
   3C345               62.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

