  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1993J @ 18cm
 Exp. Code:  GM057B  


Schedule Version:       1.00                                              
Processed by SCHED version:   6.01  Release: Late March 2005              

PI:       J.M.Marcaide                                                    

Address:  Universitat de Valencia                                         
          C/ Dr. Moliner, 50                                              
          Burjassot, E 46100, Spain                                       
                                                                          

Phone:    34-96-398-3079/8 (work) or 34-96-337-1786 (home)                
EMAIL:    J.M.Marcaide@uv.es (internet)                                   
Fax:      34-96-398-3084                                                  
Phone during observation: 34-958-121311 (work) or 34-958-810928 (home)    

Observing mode: VLBA                                                      

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

 Next scan frequencies:  1634.49  1634.49  1650.49  1650.49  1666.49  1666.49
                         1682.49  1682.49
 Next BBC frequencies:    765.51   765.51   749.51   749.51   733.51   733.51
                          717.51   717.51
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

08 35 00  1803+784     04 41 52  19.7  -4.1 10.7      17.9     0   1  1      0  08 35 00
08 39 00  ---          04 45 53  19.7  -3.9 10.8      17.0   240   F  1   3200

08 40 45  2007+777     04 47 38  22.4  -9.9  8.7      45.0    93   1  1   3200  08 40 45
08 47 45  ---          04 54 39  22.1  -9.6  8.8      43.4   420   F  1   8800

08 49 32  1803+784     04 56 27  19.5  -3.3 10.9      14.5    96   1  1   8800  08 49 32
08 56 32  ---          05 03 28  19.4  -3.0 11.1      13.0   420   F  1  14400

08 58 17  2007+777     05 05 13  21.8  -9.2  9.0      40.9    94   1  1  14400  08 58 17
09 02 17  ---          05 09 14  21.6  -9.0  9.1      40.0   240   F  1  17600

09 10 54  M81          05 17 52  35.7  24.4 -4.6     -97.0   483   1  2  17600  09 10 54
09 14 54  ---          05 21 53  36.0  24.3 -4.6     -97.9   240   R  1  14400

09 15 16  SN1993J      05 22 15  36.1  24.4 -4.6     -98.0    18   1  2  14400  09 15 16
09 22 16  ---          05 29 17  36.7  24.2 -4.4     -99.7   420   R  1   8800

09 22 39  M81          05 29 39  36.7  24.2 -4.4     -99.8    18   1  2   8800  09 22 39
09 26 39  ---          05 33 40  37.1  24.1 -4.4    -100.8   240   R  1   5600

09 27 02  SN1993J      05 34 03  37.1  24.2 -4.4    -100.9    18   1  2   5600  09 27 02
09 34 02  ---          05 41 04  37.8  24.0 -4.2    -102.6   420   R  1      0

09 34 42  M81          05 41 44  37.8  23.9 -4.2    -102.8    35   1  3      0  09 34 42
09 38 42  ---          05 45 45  38.1  23.8 -4.2    -103.8   240   F  1   3200

09 39 04  SN1993J      05 46 07  38.2  23.9 -4.2    -103.9    18   1  3   3200  09 39 04
09 46 04  ---          05 53 08  38.8  23.7 -4.0    -105.7   420   F  1   8800

09 46 27  M81          05 53 31  38.8  23.6 -4.0    -105.8    18   1  3   8800  09 46 27
09 50 27  ---          05 57 32  39.2  23.5 -4.0    -106.8   240   F  1  12000

09 50 50  SN1993J      05 57 54  39.2  23.5 -4.0    -106.9    18   1  3  12000  09 50 50
09 57 50  ---          06 04 56  39.8  23.2 -3.8    -108.7   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

09 58 30  M81          06 05 36  39.8  23.2 -3.8    -108.9    35   1  4  17600  09 58 30
10 02 30  ---          06 09 36  40.2  23.0 -3.8    -109.9   240   R  1  14400

10 02 52  SN1993J      06 09 59  40.2  23.1 -3.8    -110.0    18   1  4  14400  10 02 52
10 09 52  ---          06 17 00  40.8  22.8 -3.6    -111.8   420   R  1   8800

10 11 10  0917+624     06 18 18  46.9  29.3 -3.1    -115.3    59   1  4   8800  10 11 10
10 15 10  ---          06 22 18  47.3  29.0 -3.0    -116.4   240   R  1   5600

10 16 26  SN1993J      06 23 35  41.4  22.5 -3.5    -113.6    58   1  4   5600  10 16 26
10 23 26  ---          06 30 36  41.9  22.1 -3.4    -115.4   420   R  1      0

10 24 06  M81          06 31 16  42.0  22.0 -3.4    -115.6    35   1  5      0  10 24 06
10 28 06  ---          06 35 17  42.3  21.8 -3.3    -116.7   240   F  1   3200

10 28 28  SN1993J      06 35 39  42.4  21.8 -3.3    -116.8    18   1  5   3200  10 28 28
10 35 28  ---          06 42 40  42.9  21.4 -3.2    -118.7   420   F  1   8800

10 35 51  M81          06 43 03  42.9  21.4 -3.2    -118.8    18   1  5   8800  10 35 51
10 39 51  ---          06 47 04  43.2  21.1 -3.1    -119.9   240   F  1  12000

10 40 14  SN1993J      06 47 26  43.3  21.2 -3.1    -120.0    18   1  5  12000  10 40 14
10 47 14  ---          06 54 28  43.8  20.7 -3.0    -121.9   420   F  1  17600

10 49 14  M81          06 56 28  43.9  20.5 -3.0    -122.5   115   1  6  17600  10 49 14
10 53 14  ---          07 00 29  44.2  20.3 -2.9    -123.6   240   R  1  14400

10 53 36  SN1993J      07 00 51  44.3  20.3 -2.9    -123.7    18   1  6  14400  10 53 36
11 00 36  ---          07 07 53  44.8  19.8 -2.8    -125.7   420   R  1   8800

11 00 59  M81          07 08 15  44.8  19.7 -2.8    -125.8    18   1  6   8800  11 00 59
11 04 59  ---          07 12 16  45.1  19.4 -2.7    -127.0   240   R  1   5600

11 05 22  SN1993J      07 12 39  45.2  19.4 -2.7    -127.1    18   1  6   5600  11 05 22
11 12 22  ---          07 19 40  45.7  18.9 -2.6    -129.1   420   R  1      0

11 13 02  M81          07 20 20  45.7  18.8 -2.6    -129.3    35   1  7      0  11 13 02
11 17 02  ---          07 24 21  45.9  18.4 -2.5    -130.5   240   F  1   3200

11 17 24  SN1993J      07 24 43  46.0  18.4 -2.5    -130.6    18   1  7   3200  11 17 24
11 24 24  ---          07 31 45  46.5  17.8 -2.4    -132.7   420   F  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

11 24 47  M81          07 32 07  46.5  17.8 -2.4    -132.8    18   1  7   8800  11 24 47
11 28 47  ---          07 36 08  46.7  17.4 -2.3    -134.0   240   F  1  12000

11 29 10  SN1993J      07 36 31  46.8  17.4 -2.3    -134.1    18   1  7  12000  11 29 10
11 36 10  ---          07 43 32  47.2  16.8 -2.2    -136.2   420   F  1  17600

11 36 50  M81          07 44 12  47.2  16.7 -2.2    -136.4    35   1  8  17600  11 36 50
11 40 50  ---          07 48 13  47.5  16.3 -2.1    -137.6   240   R  1  14400

11 41 12  SN1993J      07 48 35  47.5  16.3 -2.1    -137.8    18   1  8  14400  11 41 12
11 48 12  ---          07 55 37  48.0  15.6 -2.0    -139.9   420   R  1   8800

11 48 56  0954+658     07 56 20  50.4  19.4 -2.0    -136.4    32   1  8   8800  11 48 56
11 52 56  ---          08 00 21  50.6  18.9 -2.0    -137.7   240   R  1   5600

11 53 39  SN1993J      08 01 04  48.3  15.0 -1.9    -141.6    32   1  8   5600  11 53 39
12 00 39  ---          08 08 05  48.6  14.2 -1.8    -143.8   420   R  1      0

12 01 19  M81          08 08 45  48.6  14.1 -1.8    -144.0    35   1  9      0  12 01 19
12 05 19  ---          08 12 46  48.8  13.7 -1.7    -145.3   240   F  1   3200

12 05 42  SN1993J      08 13 09  48.9  13.7 -1.7    -145.4    18   1  9   3200  12 05 42
12 12 42  ---          08 20 10  49.3  12.9 -1.6    -147.7   420   F  1   8800

12 13 04  M81          08 20 32  49.2  12.8 -1.6    -147.8    18   1  9   8800  12 13 04
12 17 04  ---          08 24 33  49.4  12.3 -1.5    -149.1   240   F  1  12000

12 17 27  SN1993J      08 24 56  49.5  12.3 -1.5    -149.2    18   1  9  12000  12 17 27
12 24 27  ---          08 31 57  49.8  11.5 -1.4    -151.5   420   F  1  17600

12 25 07  M81          08 32 37  49.8  11.4 -1.4    -151.7    35   1 10  17600  12 25 07
12 29 07  ---          08 36 38  49.9  10.9 -1.3    -153.0   240   R  1  14400

12 29 30  SN1993J      08 37 01  50.0  10.8 -1.3    -153.1    18   1 10  14400  12 29 30
12 36 30  ---          08 44 02  50.3  10.0 -1.2    -155.5   420   R  1   8800

12 36 52  M81          08 44 24  50.2   9.9 -1.2    -155.6    18   1 10   8800  12 36 52
12 40 52  ---          08 48 25  50.4   9.4 -1.1    -156.9   240   R  1   5600

12 41 15  SN1993J      08 48 48  50.4   9.4 -1.1    -157.0    18   1 10   5600  12 41 15
12 48 15  ---          08 55 49  50.7   8.4 -1.0    -159.4   420   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

12 48 55  4C39.25      08 56 29  79.5  35.0 -0.5    -140.6   -24   1 11      0  12 48 55
12 57 55  ---          09 05 31  80.5  26.7 -0.4    -150.2   516   F  1   7200

12 57 55  M81          09 05 31  50.9   7.1 -0.8    -162.6   -65   1 11   7200  12 57 55
13 02 55  ---          09 10 31  51.0   6.4 -0.8    -164.3   235   F  1  11200

13 02 55  SN1993J      09 10 31  51.1   6.4 -0.8    -164.4    -5   1 11  11200  13 02 55
13 10 55  ---          09 18 33  51.3   5.3 -0.6    -167.1   475   F  1  17600

13 11 35  M81          09 19 13  51.2   5.2 -0.6    -167.3    35   1 12  17600  13 11 35
13 15 35  ---          09 23 13  51.3   4.7 -0.5    -168.7   240   R  1  14400

13 15 58  SN1993J      09 23 36  51.4   4.6 -0.5    -168.8    18   1 12  14400  13 15 58
13 22 58  ---          09 30 38  51.5   3.6 -0.4    -171.3   420   R  1   8800

13 23 56  0917+624     09 31 36  58.4  -2.1  0.2     176.1    38   1 12   8800  13 23 56
13 27 56  ---          09 35 37  58.3  -3.0  0.2     174.4   240   R  1   5600

13 28 54  SN1993J      09 36 34  51.5   2.8 -0.3    -173.3    38   1 12   5600  13 28 54
13 35 54  ---          09 43 35  51.6   1.8 -0.2    -175.7   420   R  1      0

13 36 34  M81          09 44 16  51.6   1.7 -0.2    -175.9    35   1 13      0  13 36 34
13 40 34  ---          09 48 16  51.6   1.1 -0.1    -177.3   240   F  1   3200

13 40 57  SN1993J      09 48 39  51.6   1.0 -0.1    -177.5    18   1 13   3200  13 40 57
13 47 57  ---          09 55 40  51.6   0.0  0.0    -179.9   420   F  1   8800

13 48 19  M81          09 56 03  51.6   0.0  0.0     180.0    17   1 13   8800  13 48 19
13 52 19  ---          10 00 03  51.6  -0.6  0.1     178.6   240   F  1  12000

13 52 42  SN1993J      10 00 26  51.6  -0.7  0.1     178.4    18   1 13  12000  13 52 42
13 59 42  ---          10 07 28  51.6  -1.7  0.2     176.0   420   F  1  17600

14 00 22  M81          10 08 08  51.6  -1.7  0.2     175.8    35   1 14  17600  14 00 22
14 04 22  ---          10 12 08  51.5  -2.3  0.3     174.4   240   R  1  14400

14 04 22  SN1993J      10 12 08  51.6  -2.3  0.3     174.4    -5   1 14  14400  14 04 22
14 11 22  ---          10 19 10  51.5  -3.3  0.4     171.9   415   R  1   8800

14 11 22  M81          10 19 10  51.5  -3.3  0.4     172.0    -5   1 14   8800  14 11 22
14 15 22  ---          10 23 10  51.4  -3.9  0.5     170.6   235   R  1   5600
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

14 15 22  SN1993J      10 23 10  51.4  -3.9  0.5     170.6    -5   1 14   5600  14 15 22
14 22 22  ---          10 30 11  51.3  -4.9  0.6     168.2   415   R  1      0

-----------  Tape Change ------------

14 37 22  4C39.25      10 45 14  72.0 -57.0  1.3     111.8   853   2  1      0  14 37 22
14 46 22  ---          10 54 15  70.4 -58.8  1.4     108.6   540   F  1   7200

14 49 17  M81          10 57 10  50.6  -8.5  1.0     159.1   129   2  1   7200  14 49 17
14 54 17  ---          11 02 11  50.4  -9.2  1.1     157.4   300   F  1  11200

14 54 39  SN1993J      11 02 34  50.5  -9.3  1.1     157.2    18   2  1  11200  14 54 39
15 02 39  ---          11 10 35  50.2 -10.3  1.2     154.5   480   F  1  17600

15 03 19  M81          11 11 16  50.1 -10.4  1.3     154.4    35   2  2  17600  15 03 19
15 07 19  ---          11 15 16  49.9 -10.9  1.3     153.1   240   R  1  14400

15 07 42  SN1993J      11 15 39  50.0 -11.0  1.3     152.9    18   2  2  14400  15 07 42
15 14 42  ---          11 22 40  49.7 -11.8  1.4     150.6   420   R  1   8800

15 15 22  0954+658     11 23 21  52.8 -14.2  1.4     149.3    28   2  2   8800  15 15 22
15 19 22  ---          11 27 21  52.6 -14.8  1.5     147.9   240   R  1   5600

15 20 03  SN1993J      11 28 01  49.4 -12.5  1.5     148.8    28   2  2   5600  15 20 03
15 27 03  ---          11 35 03  49.1 -13.3  1.7     146.6   420   R  1      0

15 27 43  M81          11 35 43  49.0 -13.3  1.7     146.4    35   2  3      0  15 27 43
15 31 43  ---          11 39 43  48.8 -13.7  1.7     145.2   240   F  1   3200

15 32 05  SN1993J      11 40 06  48.8 -13.8  1.7     145.0    18   2  3   3200  15 32 05
15 39 05  ---          11 47 07  48.5 -14.6  1.9     142.7   420   F  1   8800

15 39 27  M81          11 47 30  48.4 -14.6  1.9     142.7    17   2  3   8800  15 39 27
15 43 27  ---          11 51 30  48.2 -15.0  1.9     141.4   240   F  1  12000

15 43 50  SN1993J      11 51 53  48.2 -15.1  1.9     141.3    18   2  3  12000  15 43 50
15 50 50  ---          11 58 54  47.8 -15.8  2.1     139.1   420   F  1  17600

15 51 30  M81          11 59 34  47.7 -15.8  2.1     139.0    35   2  4  17600  15 51 30
15 55 30  ---          12 03 35  47.5 -16.2  2.1     137.7   240   R  1  14400

15 55 53  SN1993J      12 03 58  47.5 -16.3  2.1     137.5    18   2  4  14400  15 55 53
16 02 53  ---          12 10 59  47.1 -17.0  2.3     135.4   420   R  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

16 03 15  M81          12 11 21  47.0 -17.0  2.3     135.4    17   2  4   8800  16 03 15
16 07 15  ---          12 15 22  46.8 -17.4  2.3     134.2   240   R  1   5600

16 07 38  SN1993J      12 15 45  46.8 -17.5  2.3     134.0    18   2  4   5600  16 07 38
16 14 38  ---          12 22 46  46.3 -18.1  2.4     131.9   420   R  1      0

16 15 18  M81          12 23 26  46.2 -18.1  2.5     131.8    35   2  5      0  16 15 18
16 19 18  ---          12 27 27  46.0 -18.4  2.5     130.6   240   F  1   3200

16 19 41  SN1993J      12 27 49  46.0 -18.5  2.5     130.4    18   2  5   3200  16 19 41
16 26 41  ---          12 34 51  45.5 -19.1  2.6     128.3   420   F  1   8800

16 27 03  M81          12 35 13  45.4 -19.0  2.7     128.3    17   2  5   8800  16 27 03
16 31 03  ---          12 39 14  45.1 -19.4  2.7     127.1   240   F  1  12000

16 31 26  SN1993J      12 39 36  45.1 -19.4  2.7     127.0    18   2  5  12000  16 31 26
16 38 26  ---          12 46 37  44.6 -20.0  2.8     125.0   420   F  1  17600

16 39 06  M81          12 47 18  44.6 -20.0  2.9     124.8    35   2  6  17600  16 39 06
16 43 06  ---          12 51 18  44.3 -20.2  2.9     123.7   240   R  1  14400

16 43 28  SN1993J      12 51 41  44.3 -20.3  2.9     123.5    18   2  6  14400  16 43 28
16 50 28  ---          12 58 42  43.7 -20.8  3.0     121.6   420   R  1   8800

16 51 31  0917+624     12 59 45  43.2 -31.3  3.6     106.4    50   2  6   8800  16 51 31
16 55 31  ---          13 03 45  42.7 -31.5  3.7     105.4   240   R  1   5600

16 56 33  SN1993J      13 04 48  43.3 -21.2  3.1     119.9    49   2  6   5600  16 56 33
17 03 33  ---          13 11 49  42.7 -21.6  3.3     118.0   420   R  1      0

17 05 33  M81          13 13 49  42.5 -21.6  3.3     117.5   114   2  7      0  17 05 33
17 09 33  ---          13 17 50  42.2 -21.9  3.4     116.4   240   F  1   3200

17 11 33  SN1993J      13 19 50  42.1 -22.0  3.4     115.8   114   2  7   3200  17 11 33
17 18 33  ---          13 26 51  41.5 -22.4  3.5     113.9   420   F  1   8800

17 20 33  M81          13 28 52  41.3 -22.4  3.5     113.5   114   2  7   8800  17 20 33
17 24 33  ---          13 32 52  41.0 -22.6  3.6     112.4   240   F  1  12000

17 26 33  SN1993J      13 34 53  40.8 -22.8  3.6     111.8   114   2  7  12000  17 26 33
17 33 33  ---          13 41 54  40.2 -23.1  3.8     110.0   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

17 34 13  M81          13 42 34  40.2 -23.0  3.8     109.9    35   2  8  17600  17 34 13
17 38 13  ---          13 46 34  39.8 -23.2  3.8     108.8   240   R  1  14400

17 38 35  SN1993J      13 46 57  39.8 -23.3  3.9     108.7    18   2  8  14400  17 38 35
17 45 35  ---          13 53 58  39.2 -23.5  4.0     106.9   420   R  1   8800

17 45 58  M81          13 54 21  39.2 -23.5  4.0     106.8    18   2  8   8800  17 45 58
17 49 58  ---          13 58 21  38.8 -23.6  4.0     105.8   240   R  1   5600

17 50 20  SN1993J      13 58 44  38.8 -23.7  4.0     105.7    18   2  8   5600  17 50 20
17 57 20  ---          14 05 45  38.2 -23.9  4.2     103.9   420   R  1      0

17 58 00  M81          14 06 25  38.1 -23.8  4.2     103.8    35   2  9      0  17 58 00
18 02 00  ---          14 10 26  37.8 -23.9  4.2     102.8   240   F  1   3200

18 02 22  SN1993J      14 10 48  37.8 -24.0  4.2     102.6    18   2  9   3200  18 02 22
18 09 22  ---          14 17 49  37.1 -24.2  4.4     100.9   420   F  1   8800

18 09 45  M81          14 18 12  37.1 -24.1  4.4     100.9    18   2  9   8800  18 09 45
18 13 45  ---          14 22 12  36.8 -24.2  4.4      99.9   240   F  1  12000

18 14 07  SN1993J      14 22 35  36.7 -24.2  4.4      99.7    18   2  9  12000  18 14 07
18 21 07  ---          14 29 36  36.1 -24.4  4.6      98.0   420   F  1  17600

18 21 47  M81          14 30 16  36.0 -24.3  4.6      97.9    35   2 10  17600  18 21 47
18 25 47  ---          14 34 17  35.7 -24.4  4.6      96.9   240   R  1  14400

18 26 09  SN1993J      14 34 39  35.6 -24.4  4.6      96.8    17   2 10  14400  18 26 09
18 33 09  ---          14 41 40  35.0 -24.5  4.8      95.1   420   R  1   8800

18 33 51  0954+658     14 42 22  35.5 -28.7  4.7      93.3    33   2 10   8800  18 33 51
18 37 51  ---          14 46 23  35.1 -28.7  4.8      92.4   240   R  1   5600

18 38 33  SN1993J      14 47 05  34.5 -24.6  4.9      93.8    33   2 10   5600  18 38 33
18 45 33  ---          14 54 06  33.9 -24.6  5.0      92.2   420   R  1      0

18 46 13  M81          14 54 46  33.9 -24.6  5.0      92.1    35   2 11      0  18 46 13
18 50 13  ---          14 58 47  33.5 -24.6  5.0      91.1   240   F  1   3200

18 50 53  SN1993J      14 59 27  33.4 -24.6  5.1      90.9    35   2 11   3200  18 50 53
18 57 53  ---          15 06 28  32.8 -24.6  5.2      89.3   420   F  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1993J @ 18cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Sun   6 Nov 2005   Day 310 ---

18 58 33  M81          15 07 08  32.8 -24.6  5.2      89.2    35   2 11   8800  18 58 33
19 02 33  ---          15 11 09  32.4 -24.6  5.3      88.2   240   F  1  12000

19 03 13  SN1993J      15 11 49  32.3 -24.6  5.3      88.0    35   2 11  12000  19 03 13
19 10 13  ---          15 18 50  31.7 -24.6  5.4      86.4   420   F  1  17600

19 10 53  M81          15 19 30  31.6 -24.5  5.4      86.3    35   2 12  17600  19 10 53
19 14 53  ---          15 23 31  31.3 -24.5  5.5      85.4   240   R  1  14400

19 15 33  SN1993J      15 24 11  31.2 -24.5  5.5      85.2    35   2 12  14400  19 15 33
19 22 33  ---          15 31 12  30.6 -24.5  5.6      83.6   420   R  1   8800

19 23 13  M81          15 31 52  30.5 -24.4  5.6      83.5    35   2 12   8800  19 23 13
19 27 13  ---          15 35 53  30.2 -24.4  5.7      82.6   240   R  1   5600

19 27 53  SN1993J      15 36 33  30.1 -24.4  5.7      82.4    35   2 12   5600  19 27 53
19 34 53  ---          15 43 34  29.5 -24.3  5.8      80.8   420   R  1      0

19 35 33  M81          15 44 14  29.5 -24.2  5.8      80.7    35   2 13      0  19 35 33
19 39 33  ---          15 48 15  29.1 -24.2  5.9      79.8   240   F  1   3200

19 40 13  SN1993J      15 48 55  29.0 -24.2  5.9      79.6    35   2 13   3200  19 40 13
19 47 13  ---          15 55 56  28.4 -24.1  6.0      78.0   420   F  1   8800

19 47 53  M81          15 56 36  28.4 -24.0  6.0      77.9    35   2 13   8800  19 47 53
19 51 53  ---          16 00 37  28.0 -23.9  6.1      77.0   240   F  1  12000

19 52 33  SN1993J      16 01 17  27.9 -23.9  6.1      76.8    35   2 13  12000  19 52 33
19 59 33  ---          16 08 18  27.3 -23.8  6.2      75.3   420   F  1  17600

20 00 13  M81          16 08 58  27.3 -23.7  6.2      75.2    35   2 14  17600  20 00 13
20 04 13  ---          16 12 59  26.9 -23.6  6.3      74.3   240   R  1  14400

20 04 53  SN1993J      16 13 39  26.9 -23.6  6.3      74.1    35   2 14  14400  20 04 53
20 11 53  ---          16 20 40  26.3 -23.4  6.4      72.5   420   R  1   8800

20 12 44  0917+624     16 21 31  20.4 -28.7  7.0      62.5    33   2 14   8800  20 12 44
20 16 44  ---          16 25 32  20.0 -28.5  7.1      61.7   240   R  1   5600

20 17 34  SN1993J      16 26 22  25.8 -23.2  6.5      71.3    33   2 14   5600  20 17 34
20 24 34  ---          16 33 23  25.2 -23.0  6.6      69.7   420   R  1      0


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: GM057B.18cm
   Matches group v20cm_2 in /instalables/SCHED/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    2         Station: VLBA_FD           Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         L         U         L         U         L         U         L         U
   Pol.  =      LCP       LCP       LCP       LCP       LCP       LCP       LCP       LCP 
   BBC   =         1         1         2         2         3         3         4         4
   BBC SB=         U         L         U         L         U         L         U         L
   IF    =        C         C         C         C         C         C         C         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   2  Setup file default.  Used pcal sets:   1
   LO sum=    1634.49   1634.49   1650.49   1650.49   1666.49   1666.49   1682.49   1682.49
   BBC fr=     765.51    765.51    749.51    749.51    733.51    733.51    717.51    717.51
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   490   490   490  6490  6490  6490  6490
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- SN1993J @ 18cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 0917+624          09 17 40.306287   * 09 21 36.230500     09 22 03.915409       0.00
                     62 28 38.63575    * 62 15 52.17600      62 14 14.08240        0.00
                     From catalog imbedded in main SCHED input file.
                        0.267 scan hours,     42.133 baseline hours above horizon.

 * 0954+658          09 54 57.847920   * 09 58 47.245100     09 59 13.867182       0.00
                     65 48 15.53881    * 65 33 54.81800      65 32 04.46385        0.00
                     From catalog imbedded in main SCHED input file.
                        0.200 scan hours,     33.067 baseline hours above horizon.

 * SN1993J           09 51 19.039486   * 09 55 24.775500     09 55 53.363784       0.00
                     69 15 26.47487    * 69 01 13.71000      68 59 23.49565        0.00
                     From catalog imbedded in main SCHED input file.
                        6.100 scan hours,   1003.194 baseline hours above horizon.

 * M81               09 51 27.310854   * 09 55 33.173100     09 56 01.774923       0.00
                     69 18 08.14534    * 69 03 55.06200      69 02 04.79926        0.00
                     From catalog imbedded in main SCHED input file.
                        3.033 scan hours,    496.414 baseline hours above horizon.

 * 1803+784          18 03 39.193244   * 18 00 45.683600     18 00 20.843911       0.00
                     78 27 54.30008    * 78 28 04.02100      78 28 09.87791        0.00
                     From catalog imbedded in main SCHED input file.
                        0.183 scan hours,     34.833 baseline hours above horizon.

 * 2007+777          20 07 20.430477   * 20 05 30.998800     20 05 14.942339       0.00
                     77 43 58.12445    * 77 52 43.24900      77 53 55.56398        0.00
                     From catalog imbedded in main SCHED input file.
                        0.183 scan hours,     31.350 baseline hours above horizon.

 * 4C39.25           09 23 55.319212   * 09 27 03.013933     09 27 24.787221       0.00
                     39 15 23.56648    * 39 02 20.85188      39 00 47.78966        0.00
                     From catalog imbedded in main SCHED input file.
                        0.300 scan hours,     37.616 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0917+624           100.3
   0954+658            97.5
   SN1993J             99.1
   M81                 99.1
   1803+784            98.3
   2007+777           103.6
   4C39.25             92.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

