  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 8GHz obs of SN/SNR in ARP 220
 Exp. Code:  GC028   


Schedule Version:       1.00                                              
Processed by SCHED version:   6.05  June 2006                             

PI:       John Conway                                                     

Address:  Onsala Space Observatory                                        
          S-439 92 Onsala                                                 
          Sweden                                                          
                                                                          

Phone:    +46(0)31 772 5505                                               
EMAIL:    jconway@oso.chalmers.se                                         
Fax:      +46(0)31 772 5590                                               
Phone during observation: +46(0)31 772 5505                               

Observing mode: 8GHz @ 256 Mbps                                           

Notes:                                                                    
                                                                          
                                                                          
                                                                          


COVER LETTER:


8GHz global network standard 256Mbit/s obs of Arp220.
The correlation position is midway between the two
nuclei. One correlation pass is sufficient.

A dual polarisation mode is used (forced by VLA use)
hence at Onsala and Noto which are single pol stations
will only get useful signal in RCP.

The expt starts at 0400. 30 mins later than block
schedule. Assume Bonn pointing done before recording
starts.

The source J1516+1932 (0.66Jy) is used for phasing
up WSRT and VLA27

The fringe finder is J1613+3412, schedule contains two
10 min scans and some shorter ones.

The schedule has three periods  where  Bonn is taken out of the
array to allow pointing updates. These are at

07:22 - 07:33
11:20 - 11:30
13:48 - 14:00

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

 Next scan frequencies:  8405.49  8405.49  8413.49  8413.49  8421.49  8421.49
                         8429.49  8429.49
 Next BBC frequencies:    805.49   805.49   813.49   813.49   821.49   821.49
                          829.49   829.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

11 30 58  J1516+1932   09 04 06   7.1  71.5 -6.2     -60.0     0   1  1      0  11 30 58
11 31 58  =1514+197    09 05 06   7.3  71.6 -6.2     -60.0    60   F  1      2  11 30 59

11 32 40  J1532+2344   09 05 49   6.4  66.2 -6.5  H  -59.3    33   1  1      2  11 32 40
11 33 40  ---          09 06 49   6.6  66.3 -6.4     -59.4     0   F  1      4  11 32 41

11 34 06  ARP220       09 07 15   6.1  66.3 -6.5  H  -59.2    19   1  1      4  11 34 06
11 36 06  ---          09 09 15   6.5  66.5 -6.4     -59.4     0   F  1      8  11 34 07

11 36 33  J1532+2344   09 09 42   7.2  66.6 -6.4     -59.6    20   1  1      8  11 36 33
11 37 33  ---          09 10 43   7.4  66.8 -6.4     -59.7    60   F  1     10  11 36 34

11 37 59  ARP220       09 11 09   6.9  66.8 -6.4     -59.5    19   1  1     10  11 37 59
11 39 59  ---          09 13 09   7.3  67.0 -6.4     -59.7   120   F  1     14  11 38 00

11 40 26  J1532+2344   09 13 36   7.9  67.1 -6.3     -60.0    20   1  1     14  11 40 26
11 41 26  ---          09 14 36   8.1  67.2 -6.3     -60.0    60   F  1     15  11 40 27

11 41 53  ARP220       09 15 03   7.7  67.2 -6.3     -59.9    19   1  1     15  11 41 53
11 43 53  ---          09 17 03   8.1  67.4 -6.3     -60.0   120   F  1     19  11 41 54

11 44 20  J1532+2344   09 17 30   8.7  67.5 -6.3     -60.3    20   1  1     19  11 44 20
11 45 20  ---          09 18 30   8.9  67.7 -6.2     -60.4    60   F  1     21  11 44 21

11 45 46  ARP220       09 18 56   8.5  67.7 -6.3     -60.2    19   1  1     21  11 45 46
11 47 46  ---          09 20 57   8.8  67.9 -6.2     -60.4   120   F  1     25  11 45 47

11 48 13  J1532+2344   09 21 24   9.5  68.0 -6.2     -60.6    20   1  1     25  11 48 13
11 49 13  ---          09 22 24   9.7  68.1 -6.2     -60.7    60   F  1     27  11 48 14

11 49 39  ARP220       09 22 50   9.2  68.1 -6.2     -60.5    19   1  1     27  11 49 39
11 51 39  ---          09 24 50   9.6  68.3 -6.2     -60.7   120   F  1     31  11 49 40

11 52 06  J1532+2344   09 25 18  10.3  68.4 -6.1     -60.9    20   1  1     31  11 52 06
11 53 06  ---          09 26 18  10.5  68.5 -6.1     -61.0    60   F  1     33  11 52 07
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

11 53 32  ARP220       09 26 44  10.0  68.5 -6.1     -60.8    19   1  1     33  11 53 32
11 55 32  ---          09 28 44  10.4  68.8 -6.1     -61.0   120   F  1     37  11 53 33

11 55 59  J1532+2344   09 29 11  11.0  68.9 -6.1     -61.2    20   1  1     37  11 55 59
11 56 59  ---          09 30 12  11.2  69.0 -6.0     -61.3    60   F  1     39  11 56 00

11 57 25  ARP220       09 30 38  10.8  69.0 -6.1     -61.1    19   1  1     39  11 57 25
11 59 25  ---          09 32 38  11.2  69.2 -6.0     -61.3   120   F  1     43  11 57 26

11 59 52  J1532+2344   09 33 05  11.8  69.3 -6.0     -61.5    20   1  1     43  11 59 52
12 00 52  ---          09 34 05  12.0  69.4 -6.0     -61.6    60   F  1     45  11 59 53

12 01 36  J1516+1932   09 34 49  13.4  75.1 -5.7     -61.9    34   1  1     45  12 01 36
12 11 36  =1514+197    09 44 51  15.5  76.2 -5.5     -62.4   600   F  1     64  12 01 37

12 12 19  J1532+2344   09 45 34  14.4  70.7 -5.8     -62.5    33   1  1     64  12 12 19
12 13 19  ---          09 46 34  14.6  70.8 -5.8     -62.6    60   F  1     66  12 12 20

12 13 46  ARP220       09 47 02  14.1  70.8 -5.8     -62.4    21   1  1     66  12 13 46
12 15 46  ---          09 49 02  14.5  71.0 -5.8     -62.5   120   F  1     70  12 13 47

12 16 14  J1532+2344   09 49 30  15.2  71.1 -5.7     -62.8    21   1  1     70  12 16 14
12 17 14  ---          09 50 30  15.4  71.2 -5.7     -62.8    60   F  1     72  12 16 15

12 17 42  ARP220       09 50 58  14.9  71.2 -5.7     -62.7    21   1  1     72  12 17 42
12 19 42  ---          09 52 58  15.3  71.5 -5.7     -62.8   120   F  1     75  12 17 43

12 20 10  J1532+2344   09 53 26  16.0  71.5 -5.7     -63.0    21   1  1     75  12 20 10
12 21 10  ---          09 54 26  16.2  71.6 -5.6     -63.1    60   F  1     77  12 20 11

12 21 38  ARP220       09 54 54  15.7  71.7 -5.7     -62.9    21   1  1     77  12 21 38
12 23 38  ---          09 56 54  16.1  71.9 -5.6     -63.1   120   F  1     81  12 21 39

12 24 06  J1532+2344   09 57 23  16.8  72.0 -5.6     -63.3    21   1  1     81  12 24 06
12 25 06  ---          09 58 23  17.0  72.1 -5.6     -63.4    60   F  1     83  12 24 07

12 25 33  ARP220       09 58 50  16.5  72.1 -5.6     -63.2    21   1  1     83  12 25 33
12 27 33  ---          10 00 51  16.9  72.3 -5.6     -63.3   120   F  1     87  12 25 34

12 28 01  J1532+2344   10 01 19  17.6  72.4 -5.5     -63.6    21   1  1     87  12 28 01
12 29 01  ---          10 02 19  17.8  72.5 -5.5     -63.7    60   F  1     89  12 28 02

12 30 17  J1613+3412   10 03 35  14.7  58.7 -6.2     -62.7    60   1  1     89  12 30 17
12 40 17  =1611+343    10 13 36  16.6  59.7 -6.0     -63.9   600   F  1    108  12 30 18
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

12 41 56  J1516+1932   10 15 16  21.9  79.6 -5.0     -63.9    80   1  1    108  12 41 56
12 44 56  =1514+197    10 18 16  22.6  80.0 -5.0     -64.0   180   F  1    114  12 41 57

12 45 40  J1532+2344   10 19 01  21.2  74.2 -5.2     -64.8    34   1  1    114  12 45 40
12 46 40  ---          10 20 01  21.4  74.4 -5.2     -64.8    60   F  1    116  12 45 41

12 47 08  ARP220       10 20 28  21.0  74.4 -5.2     -64.6    21   1  1    116  12 47 08
12 49 08  ---          10 22 29  21.4  74.6 -5.2     -64.8   120   F  1    120  12 47 09

12 49 36  J1532+2344   10 22 57  22.0  74.7 -5.2     -65.0    21   1  1    120  12 49 36
12 50 36  ---          10 23 57  22.2  74.8 -5.2     -65.1    60   F  1    122  12 49 37

12 51 03  ARP220       10 24 25  21.8  74.8 -5.2     -64.9    21   1  1    122  12 51 03
12 53 03  ---          10 26 25  22.2  75.0 -5.1     -65.0   120   F  1    126  12 51 04

12 53 31  J1532+2344   10 26 53  22.8  75.1 -5.1     -65.2    21   1  1    126  12 53 31
12 54 31  ---          10 27 53  23.1  75.2 -5.1     -65.3    60   F  1    128  12 53 32

12 54 59  ARP220       10 28 21  22.6  75.2 -5.1     -65.1    21   1  1    128  12 54 59
12 56 59  ---          10 30 21  23.0  75.4 -5.1     -65.2   120   F  1    132  12 55 00

12 57 27  J1532+2344   10 30 49  23.7  75.5 -5.0     -65.5    21   1  1    132  12 57 27
12 58 27  ---          10 31 50  23.9  75.6 -5.0     -65.5    60   F  1    134  12 57 28

12 58 54  ARP220       10 32 17  23.4  75.6 -5.0     -65.3    21   1  1    134  12 58 54
13 00 54  ---          10 34 17  23.8  75.8 -5.0     -65.5   120   F  1    137  12 58 55

13 01 23  J1532+2344   10 34 46  24.5  75.9 -5.0     -65.7    21   1  1    137  13 01 23
13 02 23  ---          10 35 46  24.7  76.0 -5.0     -65.8    60   F  1    139  13 01 24

13 03 08  J1516+1932   10 36 31  26.4  82.0 -4.7     -64.7    35   1  1    139  13 03 08
13 04 08  =1514+197    10 37 32  26.6  82.1 -4.7     -64.7    60   F  1    141  13 03 09

13 04 53  J1532+2344   10 38 17  25.2  76.3 -4.9     -65.9    35   1  1    141  13 04 53
13 05 53  ---          10 39 17  25.4  76.4 -4.9     -66.0    60   F  1    143  13 04 54

13 06 21  ARP220       10 39 44  25.0  76.4 -4.9     -65.8    21   1  1    143  13 06 21
13 08 21  ---          10 41 45  25.4  76.6 -4.9     -65.9   120   F  1    147  13 06 22

13 08 49  J1532+2344   10 42 13  26.0  76.7 -4.8     -66.1    21   1  1    147  13 08 49
13 09 49  ---          10 43 13  26.3  76.8 -4.8     -66.2    60   F  1    149  13 08 50

13 10 16  ARP220       10 43 41  25.8  76.8 -4.9     -66.0    21   1  1    149  13 10 16
13 12 16  ---          10 45 41  26.2  77.0 -4.8     -66.1   120   F  1    153  13 10 17
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

13 12 44  J1532+2344   10 46 09  26.9  77.1 -4.8     -66.3    21   1  1    153  13 12 44
13 13 44  ---          10 47 09  27.1  77.2 -4.8     -66.4    60   F  1    155  13 12 45

13 14 12  ARP220       10 47 37  26.6  77.2 -4.8     -66.2    21   1  1    155  13 14 12
13 16 12  ---          10 49 37  27.0  77.4 -4.8     -66.3   120   F  1    159  13 14 13

13 16 40  J1532+2344   10 50 05  27.7  77.5 -4.7     -66.5    21   1  1    159  13 16 40
13 17 40  ---          10 51 06  27.9  77.6 -4.7     -66.6    60   F  1    161  13 16 41

13 18 07  ARP220       10 51 33  27.5  77.6 -4.7     -66.4    21   1  1    161  13 18 07
13 20 07  ---          10 53 33  27.9  77.8 -4.7     -66.5   120   F  1    165  13 18 08

13 20 35  J1532+2344   10 54 02  28.5  77.9 -4.7     -66.7    21   1  1    165  13 20 35
13 21 35  ---          10 55 02  28.7  78.0 -4.6     -66.8    60   F  1    166  13 20 36

13 22 22  J1516+1932   10 55 48  30.6  84.2 -4.4     -65.3    36   1  1    166  13 22 22
13 23 22  =1514+197    10 56 49  30.8  84.3 -4.3     -65.3    60   F  1    168  13 22 23

13 24 08  J1532+2344   10 57 35  29.3  78.2 -4.6     -66.9    36   1  1    168  13 24 08
13 25 08  ---          10 58 35  29.5  78.3 -4.6     -67.0    60   F  1    170  13 24 09

13 25 35  ARP220       10 59 02  29.0  78.4 -4.6     -66.8    21   1  1    170  13 25 35
13 27 35  ---          11 01 03  29.4  78.6 -4.6     -66.9   120   F  1    174  13 25 36

13 28 03  J1532+2344   11 01 31  30.1  78.6 -4.5     -67.1    21   1  1    174  13 28 03
13 29 03  ---          11 02 31  30.3  78.7 -4.5     -67.2    60   F  1    176  13 28 04

13 29 31  ARP220       11 02 59  29.9  78.8 -4.5     -67.0    21   1  1    176  13 29 31
13 31 31  ---          11 04 59  30.3  79.0 -4.5     -67.1   120   F  1    180  13 29 32

13 31 59  J1532+2344   11 05 27  30.9  79.1 -4.5     -67.3    21   1  1    180  13 31 59
13 32 59  ---          11 06 27  31.1  79.2 -4.4     -67.4    60   F  1    182  13 32 00

13 33 27  ARP220       11 06 55  30.7  79.2 -4.5     -67.2    21   1  1    182  13 33 27
13 35 27  ---          11 08 55  31.1  79.4 -4.4     -67.2   120   F  1    186  13 33 28

13 35 55  J1532+2344   11 09 23  31.8  79.5 -4.4     -67.5    21   1  1    186  13 35 55
13 36 55  ---          11 10 24  32.0  79.6 -4.4     -67.5    60   F  1    188  13 35 56

13 37 22  ARP220       11 10 51  31.5  79.6 -4.4     -67.3    21   1  1    188  13 37 22
13 39 22  ---          11 12 52  31.9  79.8 -4.4     -67.4   120   F  1    192  13 37 23

13 39 50  J1532+2344   11 13 20  32.6  79.9 -4.3     -67.7    21   1  1    192  13 39 50
13 40 50  ---          11 14 20  32.8  80.0 -4.3     -67.7    60   F  1    194  13 39 51
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

13 41 38  J1516+1932   11 15 08  34.7  86.4 -4.0     -65.7    37   1  1    194  13 41 38
13 42 38  =1514+197    11 16 08  34.9  86.6 -4.0     -65.7    60   F  1    195  13 41 39

13 43 25  J1532+2344   11 16 55  33.4  80.2 -4.3     -67.8    37   1  1    195  13 43 25
13 44 25  ---          11 17 55  33.6  80.3 -4.3     -67.9    60   F  1    197  13 43 26

13 44 53  ARP220       11 18 23  33.1  80.4 -4.3     -67.7    21   1  1    197  13 44 53
13 46 53  ---          11 20 23  33.5  80.6 -4.2     -67.8   120   F  1    201  13 44 54

13 47 21  J1532+2344   11 20 51  34.2  80.6 -4.2     -68.0    21   1  1    201  13 47 21
13 48 21  ---          11 21 52  34.4  80.7 -4.2     -68.1    60   F  1    203  13 47 22

13 48 48  ARP220       11 22 19  34.0  80.8 -4.2     -67.8    21   1  1    203  13 48 48
13 50 48  ---          11 24 19  34.4  81.0 -4.2     -67.9   120   F  1    207  13 48 49

13 51 16  J1532+2344   11 24 48  35.0  81.0 -4.1     -68.2    21   1  1    207  13 51 16
13 52 16  ---          11 25 48  35.2  81.2 -4.1     -68.2    60   F  1    209  13 51 17

13 52 44  ARP220       11 26 15  34.8  81.2 -4.1     -68.0    21   1  1    209  13 52 44
13 54 44  ---          11 28 16  35.2  81.4 -4.1     -68.1   120   F  1    213  13 52 45

13 55 12  J1532+2344   11 28 44  35.9  81.5 -4.1     -68.3    21   1  1    213  13 55 12
13 56 12  ---          11 29 44  36.1  81.6 -4.1     -68.4    60   F  1    215  13 55 13

13 56 40  ARP220       11 30 12  35.6  81.6 -4.1     -68.1    21   1  1    215  13 56 40
13 58 40  ---          11 32 12  36.1  81.9 -4.1     -68.2   120   F  1    219  13 56 41

13 59 08  J1532+2344   11 32 40  36.7  81.9 -4.0     -68.5    21   1  1    219  13 59 08
14 00 08  ---          11 33 40  36.9  82.0 -4.0     -68.5    60   F  1    221  13 59 09

14 00 34  J1532+2344   11 34 07  37.0  82.0 -4.0     -68.5    21   1  1    221  14 00 34
14 01 34  ---          11 35 07  37.2  82.1 -4.0     -68.6    60   F  1    223  14 00 35

14 02 02  ARP220       11 35 35  36.8  82.2 -4.0     -68.3    21   1  1    223  14 02 02
14 04 02  ---          11 37 35  37.2  82.4 -4.0     -68.4   120   F  1    226  14 02 03

14 04 30  J1532+2344   11 38 03  37.8  82.4 -3.9     -68.7    21   1  1    226  14 04 30
14 05 30  ---          11 39 03  38.1  82.5 -3.9     -68.7    60   F  1    228  14 04 31

14 05 57  ARP220       11 39 31  37.6  82.6 -3.9     -68.5    21   1  1    228  14 05 57
14 07 57  ---          11 41 31  38.0  82.8 -3.9     -68.6   120   F  1    232  14 05 58

14 08 25  J1532+2344   11 41 59  38.7  82.9 -3.9     -68.8    21   1  1    232  14 08 25
14 09 25  ---          11 42 59  38.9  83.0 -3.8     -68.9    60   F  1    234  14 08 26
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

14 09 53  ARP220       11 43 27  38.5  83.1 -3.9     -68.6    21   1  1    234  14 09 53
14 11 53  ---          11 45 27  38.9  83.3 -3.8     -68.7   120   F  1    238  14 09 54

14 12 43  J1516+1932   11 46 18  41.4  90.3 -3.5     -65.9    40   1  1    238  14 12 43
14 15 43  =1514+197    11 49 19  42.0  90.7 -3.5     -65.9   180   F  1    244  14 12 44

14 17 24  J1532+2344   11 51 00  40.6  83.8 -3.7     -69.1    90   1  1    244  14 17 24
14 18 24  ---          11 52 00  40.8  83.9 -3.7     -69.1    60   F  1    246  14 17 25

14 18 52  ARP220       11 52 27  40.4  84.0 -3.7     -68.9    21   1  1    246  14 18 52
14 20 52  ---          11 54 28  40.8  84.2 -3.7     -69.0   120   F  1    250  14 18 53

14 21 20  J1532+2344   11 54 56  41.5  84.2 -3.6     -69.2    21   1  1    250  14 21 20
14 22 20  ---          11 55 56  41.7  84.3 -3.6     -69.3    60   F  1    252  14 21 21

14 22 47  ARP220       11 56 24  41.2  84.4 -3.6     -69.0    21   1  1    252  14 22 47
14 24 47  ---          11 58 24  41.6  84.7 -3.6     -69.1   120   F  1    255  14 22 48

14 25 15  J1532+2344   11 58 52  42.3  84.7 -3.6     -69.3    21   1  1    255  14 25 15
14 26 15  ---          11 59 52  42.5  84.8 -3.6     -69.4    60   F  1    257  14 25 16

14 26 43  ARP220       12 00 20  42.1  84.9 -3.6     -69.1    21   1  1    257  14 26 43
14 28 43  ---          12 02 20  42.5  85.1 -3.5     -69.2   120   F  1    261  14 26 44

14 29 11  J1532+2344   12 02 48  43.1  85.1 -3.5     -69.4    21   1  1    261  14 29 11
14 30 11  ---          12 03 49  43.4  85.2 -3.5     -69.5    60   F  1    263  14 29 12

14 30 38  ARP220       12 04 16  42.9  85.3 -3.5     -69.2    21   1  1    263  14 30 38
14 32 38  ---          12 06 16  43.3  85.5 -3.5     -69.3   120   F  1    267  14 30 39

14 33 07  J1532+2344   12 06 45  44.0  85.5 -3.4     -69.5    21   1  1    267  14 33 07
14 34 07  ---          12 07 45  44.2  85.6 -3.4     -69.6    60   F  1    269  14 33 08

14 36 15  J1516+1932   12 09 54  46.5  93.4 -3.1     -65.7   117   1  1    269  14 36 15
14 37 15  =1514+197    12 10 54  46.7  93.6 -3.1     -65.7    60   F  1    271  14 36 16

14 39 04  J1532+2344   12 12 43  45.3  86.2 -3.3     -69.7    98   1  1    271  14 39 04
14 40 04  ---          12 13 43  45.5  86.3 -3.3     -69.7    60   F  1    273  14 39 05

14 40 31  ARP220       12 14 11  45.0  86.4 -3.4     -69.4    21   1  1    273  14 40 31
14 42 31  ---          12 16 11  45.5  86.7 -3.3     -69.5   120   F  1    277  14 40 32

14 42 59  J1532+2344   12 16 39  46.1  86.6 -3.3     -69.7    21   1  1    277  14 42 59
14 43 59  ---          12 17 39  46.3  86.8 -3.3     -69.8    60   F  1    279  14 43 00
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

14 44 27  ARP220       12 18 07  45.9  86.9 -3.3     -69.5    21   1  1    279  14 44 27
14 46 27  ---          12 20 07  46.3  87.1 -3.3     -69.5   120   F  1    283  14 44 28

14 46 55  J1532+2344   12 20 35  47.0  87.1 -3.2     -69.8    21   1  1    283  14 46 55
14 47 55  ---          12 21 36  47.2  87.2 -3.2     -69.8    60   F  1    284  14 46 56

14 48 23  ARP220       12 22 03  46.7  87.3 -3.2     -69.6    21   1  1    284  14 48 23
14 50 23  ---          12 24 03  47.2  87.6 -3.2     -69.6   120   F  1    288  14 48 24

14 50 51  J1532+2344   12 24 32  47.8  87.6 -3.1     -69.9    21   1  1    288  14 50 51
14 51 51  ---          12 25 32  48.0  87.7 -3.1     -69.9    60   F  1    290  14 50 52

14 52 18  ARP220       12 25 59  47.6  87.8 -3.2     -69.6    21   1  1    290  14 52 18
14 54 18  ---          12 28 00  48.0  88.0 -3.1     -69.6   120   F  1    294  14 52 19

14 54 46  J1532+2344   12 28 28  48.7  88.0 -3.1     -69.9    21   1  1    294  14 54 46
14 55 46  ---          12 29 28  48.9  88.1 -3.1     -69.9    60   F  1    296  14 54 47

14 58 09  J1516+1932   12 31 51  51.2  96.7 -2.8     -65.0   131   1  1    296  14 58 09
14 59 09  =1514+197    12 32 51  51.4  96.9 -2.7     -65.0    60   F  1    298  14 58 10

15 01 13  J1532+2344   12 34 56  50.0  88.8 -3.0     -70.0   112   1  1    298  15 01 13
15 02 13  ---          12 35 56  50.3  88.9 -3.0     -70.0    60   F  1    300  15 01 14

15 02 40  ARP220       12 36 23  49.8  89.1 -3.0     -69.7    21   1  1    300  15 02 40
15 04 40  ---          12 38 24  50.2  89.3 -2.9     -69.7   120   F  1    304  15 02 41

15 05 08  J1532+2344   12 38 52  50.9  89.3 -2.9     -70.0    21   1  1    304  15 05 08
15 06 08  ---          12 39 52  51.1  89.4 -2.9     -70.0    60   F  1    306  15 05 09

15 06 36  ARP220       12 40 20  50.7  89.5 -2.9     -69.7    21   1  1    306  15 06 36
15 08 36  ---          12 42 20  51.1  89.8 -2.9     -69.7   120   F  1    310  15 06 37

15 09 04  J1532+2344   12 42 48  51.7  89.8 -2.8     -70.0    21   1  1    310  15 09 04
15 10 04  ---          12 43 48  51.9  89.9 -2.8     -70.0    60   F  1    312  15 09 05

15 10 31  ARP220       12 44 16  51.5  90.0 -2.8     -69.7    21   1  1    312  15 10 31
15 12 31  ---          12 46 16  51.9  90.3 -2.8     -69.7   120   F  1    315  15 10 32

15 13 00  J1532+2344   12 46 44  52.6  90.3 -2.8     -70.0    21   1  1    315  15 13 00
15 14 00  ---          12 47 44  52.8  90.4 -2.8     -70.0    60   F  1    317  15 13 01

15 14 27  ARP220       12 48 12  52.3  90.5 -2.8     -69.7    21   1  1    317  15 14 27
15 16 27  ---          12 50 12  52.8  90.8 -2.8     -69.7   120   F  1    321  15 14 28
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

15 16 56  J1532+2344   12 50 41  53.4  90.8 -2.7     -70.0    21   1  1    321  15 16 56
15 17 56  ---          12 51 41  53.6  90.9 -2.7     -70.0    60   F  1    323  15 16 57

15 18 23  ARP220       12 52 09  53.2  91.1 -2.7     -69.7    21   1  1    323  15 18 23
15 20 23  ---          12 54 09  53.6  91.3 -2.7     -69.7   120   F  1    327  15 18 24

15 20 52  J1532+2344   12 54 38  54.3  91.3 -2.6     -70.0    22   1  1    327  15 20 52
15 21 52  ---          12 55 38  54.5  91.5 -2.6     -70.0    60   F  1    329  15 20 53

15 22 19  ARP220       12 56 06  54.0  91.6 -2.7     -69.7    21   1  1    329  15 22 19
15 24 19  ---          12 58 06  54.5  91.9 -2.6     -69.7   120   F  1    333  15 22 20

15 35 03  J1516+1932   13 08 52  59.0 103.4 -2.1     -62.6   629   1  1    333  15 35 03
15 36 03  =1514+197    13 09 52  59.2 103.6 -2.1     -62.5    60   F  1    335  15 35 04

15 38 31  J1532+2344   13 12 19  58.1  93.8 -2.3     -69.7   135   1  1    335  15 38 31
15 39 31  ---          13 13 20  58.3  94.0 -2.3     -69.6    60   F  1    337  15 38 32

15 39 58  ARP220       13 13 47  57.8  94.1 -2.4     -69.3    21   1  1    337  15 39 58
15 41 58  ---          13 15 48  58.3  94.4 -2.3     -69.3   120   F  1    341  15 39 59

15 42 29  J1532+2344   13 16 19  58.9  94.4 -2.3     -69.5    23   1  1    341  15 42 29
15 43 29  ---          13 17 19  59.2  94.6 -2.3     -69.5    60   F  1    343  15 42 30

15 43 57  ARP220       13 17 47  58.7  94.7 -2.3     -69.2    21   1  1    343  15 43 57
15 45 57  ---          13 19 47  59.1  95.1 -2.3     -69.1   120   F  1    346  15 43 58

15 46 28  J1532+2344   13 20 18  59.8  95.1 -2.2     -69.4    24   1  1    346  15 46 28
15 47 28  ---          13 21 18  60.0  95.2 -2.2     -69.4    60   F  1    348  15 46 29

15 47 56  ARP220       13 21 47  59.6  95.4 -2.2     -69.1    22   1  1    348  15 47 56
15 49 56  ---          13 23 47  60.0  95.7 -2.2     -69.0   120   F  1    352  15 47 57

15 50 28  J1532+2344   13 24 19  60.7  95.7 -2.1     -69.2    24   1  1    352  15 50 28
15 51 28  ---          13 25 19  60.9  95.9 -2.1     -69.2    60   F  1    354  15 50 29

15 51 57  ARP220       13 25 48  60.4  96.0 -2.2     -68.9    22   1  1    354  15 51 57
15 53 57  ---          13 27 48  60.8  96.4 -2.1     -68.8   120   F  1    358  15 51 58

15 54 28  J1532+2344   13 28 20  61.5  96.4 -2.1     -69.1    25   1  1    358  15 54 28
15 55 28  ---          13 29 20  61.7  96.6 -2.1     -69.0    60   F  1    360  15 54 29

15 57 04  J1516+1932   13 30 56  63.6 108.6 -1.8     -59.9    82   1  1    360  15 57 04
15 58 04  =1514+197    13 31 56  63.8 108.9 -1.8     -59.7    60   F  1    362  15 57 05
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

15 59 31  J1532+2344   13 33 23  62.6  97.3 -2.0     -68.8    73   1  1    362  15 59 31
16 00 31  ---          13 34 23  62.8  97.5 -2.0     -68.7    60   F  1    364  15 59 32

16 01 00  ARP220       13 34 53  62.4  97.6 -2.0     -68.4    23   1  1    364  16 01 00
16 03 00  ---          13 36 53  62.8  98.0 -2.0     -68.3   120   F  1    368  16 01 01

16 03 33  J1532+2344   13 37 26  63.5  98.0 -1.9     -68.5    25   1  1    368  16 03 33
16 04 33  ---          13 38 26  63.7  98.2 -1.9     -68.5    60   F  1    370  16 03 34

16 05 02  ARP220       13 38 56  63.2  98.4 -1.9     -68.1    23   1  1    370  16 05 02
16 07 02  ---          13 40 56  63.6  98.8 -1.9     -68.0   120   F  1    374  16 05 03

16 07 35  J1532+2344   13 41 29  64.3  98.8 -1.9     -68.2    26   1  1    374  16 07 35
16 08 35  ---          13 42 29  64.5  99.0 -1.8     -68.2    60   F  1    375  16 07 36

16 09 05  ARP220       13 42 59  64.1  99.2 -1.9     -67.8    23   1  1    375  16 09 05
16 11 05  ---          13 45 00  64.5  99.6 -1.8     -67.7   120   F  1    379  16 09 06

16 11 39  J1532+2344   13 45 33  65.2  99.6 -1.8     -67.9    26   1  1    379  16 11 39
16 12 39  ---          13 46 33  65.4  99.8 -1.8     -67.8    60   F  1    381  16 11 40

16 13 09  ARP220       13 47 04  64.9 100.0 -1.8     -67.5    24   1  1    381  16 13 09
16 15 09  ---          13 49 04  65.4 100.4 -1.8     -67.3   120   F  1    385  16 13 10

16 15 43  J1532+2344   13 49 38  66.0 100.5 -1.7     -67.5    26   1  1    385  16 15 43
16 16 43  ---          13 50 38  66.3 100.7 -1.7     -67.4    60   F  1    387  16 15 44

16 18 02  J1516+1932   13 51 58  67.8 115.0 -1.4     -55.8    64   1  1    387  16 18 02
16 19 02  =1514+197    13 52 58  68.0 115.4 -1.4     -55.6    60   F  1    389  16 18 03

16 20 10  J1532+2344   13 54 06  67.0 101.5 -1.6     -67.1    53   1  1    389  16 20 10
16 21 10  ---          13 55 06  67.2 101.7 -1.6     -67.0    60   F  1    391  16 20 11

16 21 41  ARP220       13 55 37  66.8 101.9 -1.7     -66.6    24   1  1    391  16 21 41
16 23 41  ---          13 57 37  67.2 102.3 -1.6     -66.4   120   F  1    395  16 21 42

16 24 15  J1532+2344   13 58 11  67.8 102.4 -1.6     -66.6    27   1  1    395  16 24 15
16 25 15  ---          13 59 12  68.1 102.7 -1.6     -66.5    60   F  1    397  16 24 16

16 25 46  ARP220       13 59 43  67.6 102.8 -1.6     -66.2    24   1  1    397  16 25 46
16 27 46  ---          14 01 43  68.0 103.3 -1.6     -65.9   120   F  1    401  16 25 47

16 28 20  J1532+2344   14 02 17  68.7 103.4 -1.5     -66.1    27   1  1    401  16 28 20
16 29 20  ---          14 03 17  68.9 103.7 -1.5     -65.9    60   F  1    403  16 28 21
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

16 29 51  ARP220       14 03 48  68.5 103.9 -1.5     -65.6    24   1  1    403  16 29 51
16 31 51  ---          14 05 49  68.9 104.4 -1.5     -65.3   120   F  1    406  16 29 52

16 32 25  J1532+2344   14 06 23  69.6 104.5 -1.4     -65.5    27   1  1    406  16 32 25
16 33 25  ---          14 07 23  69.8 104.8 -1.4     -65.3    60   F  1    408  16 32 26

16 33 56  ARP220       14 07 54  69.3 104.9 -1.5     -65.0    24   1  1    408  16 33 56
16 35 56  ---          14 09 55  69.7 105.5 -1.4     -64.7   120   F  1    412  16 33 57

16 36 31  J1532+2344   14 10 29  70.4 105.7 -1.4     -64.8    27   1  1    412  16 36 31
16 37 31  ---          14 11 29  70.6 106.0 -1.4     -64.6    60   F  1    414  16 36 32

16 40 50  J1613+3412   14 14 49  64.7  74.0 -2.0     -89.8   172   1  1    414  16 40 50
16 50 50  =1611+343    14 24 50  66.8  74.0 -1.8     -91.2   600   F  1    434  16 40 51

16 53 07  J1516+1932   14 27 08  74.1 131.6 -0.8     -43.0    93   1  1    434  16 53 07
16 56 07  =1514+197    14 30 08  74.6 133.5 -0.8     -41.4   180   F  1    439  16 53 08

16 56 57  J1532+2344   14 30 59  74.6 112.9 -1.0     -59.9    31   1  1    439  16 56 57
16 57 57  ---          14 31 59  74.8 113.4 -1.0     -59.6    60   F  1    441  16 56 58

16 58 28  ARP220       14 32 30  74.3 113.4 -1.0     -59.4    24   1  1    441  16 58 28
17 00 28  ---          14 34 31  74.7 114.3 -1.0     -58.8   120   F  1    445  16 58 29

17 01 02  J1532+2344   14 35 04  75.4 114.8 -1.0     -58.6    26   1  1    445  17 01 02
17 02 02  ---          14 36 04  75.6 115.2 -0.9     -58.2    60   F  1    447  17 01 03

17 02 33  ARP220       14 36 36  75.1 115.2 -1.0     -58.1    24   1  1    447  17 02 33
17 04 33  ---          14 38 36  75.5 116.2 -0.9     -57.3   120   F  1    451  17 02 34

17 05 06  J1532+2344   14 39 09  76.2 116.8 -0.9     -57.0    26   1  1    451  17 05 06
17 06 06  ---          14 40 09  76.4 117.3 -0.9     -56.6    60   F  1    453  17 05 07

17 06 37  ARP220       14 40 40  75.9 117.2 -0.9     -56.5    24   1  1    453  17 06 37
17 08 37  ---          14 42 41  76.3 118.3 -0.9     -55.7   120   F  1    457  17 06 38

17 09 10  J1532+2344   14 43 14  76.9 119.0 -0.8     -55.3    26   1  1    457  17 09 10
17 10 10  ---          14 44 14  77.1 119.6 -0.8     -54.8    60   F  1    459  17 09 11

17 10 41  ARP220       14 44 45  76.7 119.5 -0.8     -54.8    24   1  1    459  17 10 41
17 12 41  ---          14 46 45  77.1 120.7 -0.8     -53.8   120   F  1    463  17 10 42

17 13 14  J1532+2344   14 47 18  77.7 121.5 -0.8     -53.2    26   1  1    463  17 13 14
17 14 14  ---          14 48 18  77.9 122.2 -0.7     -52.7    60   F  1    464  17 13 15
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

17 14 44  ARP220       14 48 49  77.4 121.9 -0.8     -52.8    24   1  1    464  17 14 44
17 16 44  ---          14 50 49  77.8 123.3 -0.7     -51.7   120   F  1    468  17 14 45

17 17 17  J1532+2344   14 51 22  78.4 124.3 -0.7     -50.9    25   1  1    468  17 17 17
17 18 17  ---          14 52 22  78.6 125.0 -0.7     -50.3    60   F  1    470  17 17 18

17 18 48  ARP220       14 52 53  78.2 124.7 -0.7     -50.5    24   1  1    470  17 18 48
17 20 48  ---          14 54 53  78.5 126.2 -0.7     -49.2   120   F  1    474  17 18 49

17 21 20  J1532+2344   14 55 26  79.1 127.4 -0.6     -48.3    25   1  1    474  17 21 20
17 22 20  ---          14 56 26  79.3 128.2 -0.6     -47.6    60   F  1    476  17 21 21

17 23 17  J1516+1932   14 57 23  78.0 156.9 -0.3     -21.0    32   1  1    476  17 23 17
17 24 17  =1514+197    14 58 23  78.1 158.0 -0.3     -20.0    60   F  1    478  17 23 18

17 25 13  J1532+2344   14 59 19  79.8 130.7 -0.6     -45.4    31   1  1    478  17 25 13
17 26 13  ---          15 00 19  80.0 131.6 -0.5     -44.6    60   F  1    480  17 25 14

17 26 43  ARP220       15 00 50  79.5 131.0 -0.6     -45.1    24   1  1    480  17 26 43
17 28 43  ---          15 02 50  79.8 132.9 -0.5     -43.4   120   F  1    484  17 26 44

17 29 15  J1532+2344   15 03 22  80.4 134.6 -0.5     -42.0    25   1  1    484  17 29 15
17 30 15  ---          15 04 22  80.6 135.7 -0.5     -41.1    60   F  1    486  17 29 16

17 30 45  ARP220       15 04 52  80.2 134.8 -0.5     -41.7    23   1  1    486  17 30 45
17 32 45  ---          15 06 53  80.5 136.9 -0.5     -39.9   120   F  1    490  17 30 46

17 33 17  J1532+2344   15 07 24  81.0 139.0 -0.4     -38.1    24   1  1    490  17 33 17
17 34 17  ---          15 08 25  81.2 140.2 -0.4     -37.0    60   F  1    492  17 33 18

17 34 47  ARP220       15 08 55  80.8 139.1 -0.4     -37.9    23   1  1    492  17 34 47
17 36 47  ---          15 10 55  81.0 141.5 -0.4     -35.8   120   F  1    495  17 34 48

17 37 18  J1532+2344   15 11 27  81.6 144.0 -0.4     -33.6    24   1  1    495  17 37 18
17 38 18  ---          15 12 27  81.7 145.3 -0.3     -32.4    60   F  1    497  17 37 19

17 38 48  ARP220       15 12 57  81.3 143.9 -0.4     -33.5    23   1  1    497  17 38 48
17 40 48  ---          15 14 57  81.5 146.6 -0.3     -31.1   120   F  1    501  17 38 49

17 41 19  J1532+2344   15 15 28  82.0 149.5 -0.3     -28.5    23   1  1    501  17 41 19
17 42 19  ---          15 16 28  82.2 151.0 -0.3     -27.1    60   F  1    503  17 41 20

17 43 19  J1516+1932   15 17 28  78.9 180.3  0.0       0.3    34   1  1    503  17 43 19
17 44 19  =1514+197    15 18 28  78.9 181.5  0.0       1.4    60   F  1    505  17 43 20
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

17 45 15  J1532+2344   15 19 25  82.4 155.5 -0.2     -22.9    33   1  1    505  17 45 15
17 46 15  ---          15 20 25  82.5 157.2 -0.2     -21.4    60   F  1    507  17 45 16

17 46 45  ARP220       15 20 55  82.2 155.1 -0.2     -23.2    22   1  1    507  17 46 45
17 48 45  ---          15 22 55  82.3 158.3 -0.2     -20.3   120   F  1    511  17 46 46

17 49 16  J1532+2344   15 23 26  82.8 162.3 -0.2     -16.6    22   1  1    511  17 49 16
17 50 16  ---          15 24 26  82.8 164.0 -0.1     -15.0    60   F  1    513  17 49 17

17 50 45  ARP220       15 24 55  82.5 161.6 -0.2     -17.2    22   1  1    513  17 50 45
17 52 45  ---          15 26 56  82.6 165.0 -0.1     -14.0   120   F  1    517  17 50 46

17 53 16  J1532+2344   15 27 27  83.0 169.5 -0.1      -9.9    22   1  1    517  17 53 16
17 54 16  ---          15 28 27  83.0 171.3 -0.1      -8.2    60   F  1    519  17 53 17

17 54 45  ARP220       15 28 56  82.7 168.5 -0.1     -10.7    21   1  1    519  17 54 45
17 56 45  ---          15 30 56  82.8 172.1 -0.1      -7.4   120   F  1    523  17 54 46

17 57 15  J1532+2344   15 31 27  83.1 177.0  0.0      -2.9    21   1  1    523  17 57 15
17 58 15  ---          15 32 27  83.1 178.9  0.0      -1.1    60   F  1    524  17 57 16

17 58 44  ARP220       15 32 56  82.8 175.8  0.0      -4.0    21   1  1    524  17 58 44
18 00 44  ---          15 34 56  82.8 179.5  0.0      -0.5   120   F  1    528  17 58 45

18 01 15  J1532+2344   15 35 27  83.1 184.5  0.0       4.3    21   1  1    528  18 01 15
18 02 15  ---          15 36 27  83.0 186.4  0.1       6.0    60   F  1    530  18 01 16

18 03 10  J1516+1932   15 37 22  78.0 203.4  0.3      21.3    38   1  1    530  18 03 10
18 04 10  =1514+197    15 38 23  77.9 204.5  0.4      22.2    60   F  1    532  18 03 11

18 05 01  J1532+2344   15 39 14  82.9 191.6  0.1      10.9    35   1  1    532  18 05 01
18 06 01  ---          15 40 14  82.9 193.4  0.1      12.6    60   F  1    534  18 05 02

18 06 30  ARP220       15 40 43  82.7 190.0  0.1       9.4    21   1  1    534  18 06 30
18 08 30  ---          15 42 44  82.7 193.6  0.1      12.7   120   F  1    538  18 06 31

18 09 01  J1532+2344   15 43 15  82.7 198.7  0.2      17.6    22   1  1    538  18 09 01
18 10 01  ---          15 44 15  82.6 200.4  0.2      19.2    60   F  1    540  18 09 02

18 10 31  ARP220       15 44 44  82.5 197.0  0.2      15.9    21   1  1    540  18 10 31
18 12 31  ---          15 46 45  82.4 200.4  0.2      19.1   120   F  1    544  18 10 32

18 13 02  J1532+2344   15 47 16  82.4 205.4  0.2      23.7    22   1  1    544  18 13 02
18 14 02  ---          15 48 16  82.3 206.9  0.3      25.2    60   F  1    546  18 13 03
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

18 14 31  ARP220       15 48 46  82.2 203.6  0.2      22.1    21   1  1    546  18 14 31
18 16 31  ---          15 50 46  82.1 206.7  0.3      24.9   120   F  1    550  18 14 32

18 17 03  J1532+2344   15 51 18  82.0 211.4  0.3      29.4    22   1  1    550  18 17 03
18 18 03  ---          15 52 18  81.9 212.9  0.3      30.7    60   F  1    552  18 17 04

18 18 32  ARP220       15 52 48  81.8 209.7  0.3      27.7    21   1  1    552  18 18 32
18 20 32  ---          15 54 48  81.6 212.5  0.3      30.2   120   F  1    555  18 18 33

18 21 04  J1532+2344   15 55 20  81.5 216.9  0.4      34.3    23   1  1    555  18 21 04
18 22 04  ---          15 56 20  81.4 218.2  0.4      35.5    60   F  1    557  18 21 05

18 22 49  J1516+1932   15 57 05  75.7 221.3  0.7      37.0    27   1  1    557  18 22 49
18 23 49  =1514+197    15 58 05  75.6 222.0  0.7      37.7    60   F  1    559  18 22 50

18 24 33  J1532+2344   15 58 49  81.0 221.1  0.4      38.2    27   1  1    559  18 24 33
18 25 33  ---          15 59 49  80.9 222.3  0.4      39.2    60   F  1    561  18 24 34

18 26 02  ARP220       16 00 19  80.9 219.4  0.4      36.6    22   1  1    561  18 26 02
18 28 02  ---          16 02 19  80.6 221.7  0.5      38.6   120   F  1    565  18 26 03

18 28 34  J1532+2344   16 02 51  80.4 225.5  0.5      42.1    23   1  1    565  18 28 34
18 29 34  ---          16 03 51  80.3 226.5  0.5      43.0    60   F  1    567  18 28 35

18 30 03  ARP220       16 04 21  80.4 223.9  0.5      40.6    22   1  1    567  18 30 03
18 32 03  ---          16 06 21  80.0 225.9  0.5      42.4   120   F  1    571  18 30 04

18 32 35  J1532+2344   16 06 52  79.8 229.4  0.6      45.5    23   1  1    571  18 32 35
18 33 35  ---          16 07 53  79.6 230.3  0.6      46.3    60   F  1    573  18 32 36

18 34 05  ARP220       16 08 22  79.7 227.8  0.6      44.1    22   1  1    573  18 34 05
18 36 05  ---          16 10 23  79.4 229.6  0.6      45.6   120   F  1    577  18 34 06

18 36 36  J1532+2344   16 10 54  79.1 232.8  0.6      48.5    23   1  1    577  18 36 36
18 37 36  ---          16 11 54  78.9 233.6  0.6      49.1    60   F  1    579  18 36 37

18 38 05  ARP220       16 12 24  79.1 231.3  0.6      47.1    22   1  1    579  18 38 05
18 40 05  ---          16 14 24  78.7 232.9  0.7      48.5   120   F  1    583  18 38 06

18 40 36  J1532+2344   16 14 55  78.4 235.9  0.7      51.1    23   1  1    583  18 40 36
18 41 36  ---          16 15 55  78.2 236.6  0.7      51.6    60   F  1    584  18 40 37

18 42 21  J1516+1932   16 16 40  72.6 233.8  1.0      47.4    27   1  1    584  18 42 21
18 43 21  =1514+197    16 17 40  72.4 234.3  1.0      47.9    60   F  1    586  18 42 22
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

18 44 05  J1532+2344   16 18 24  77.8 238.2  0.8      53.0    27   1  1    586  18 44 05
18 45 05  ---          16 19 24  77.6 238.9  0.8      53.6    60   F  1    588  18 44 06

18 45 34  ARP220       16 19 54  77.8 236.9  0.7      51.8    22   1  1    588  18 45 34
18 47 34  ---          16 21 54  77.4 238.2  0.8      52.9   120   F  1    592  18 45 35

18 48 05  J1532+2344   16 22 25  77.0 240.7  0.8      55.0    23   1  1    592  18 48 05
18 49 05  ---          16 23 25  76.8 241.3  0.8      55.5    60   F  1    594  18 48 06

18 49 34  ARP220       16 23 54  77.0 239.5  0.8      53.9    22   1  1    594  18 49 34
18 51 34  ---          16 25 55  76.7 240.6  0.8      54.8   120   F  1    598  18 49 35

18 52 05  J1532+2344   16 26 25  76.3 242.9  0.9      56.8    23   1  1    598  18 52 05
18 53 05  ---          16 27 25  76.1 243.5  0.9      57.2    60   F  1    600  18 52 06

18 53 34  ARP220       16 27 55  76.3 241.7  0.9      55.7    22   1  1    600  18 53 34
18 55 34  ---          16 29 55  75.9 242.8  0.9      56.6   120   F  1    604  18 53 35

18 56 04  J1532+2344   16 30 25  75.5 244.9  1.0      58.4    23   1  1    604  18 56 04
18 57 04  ---          16 31 26  75.3 245.4  1.0      58.7    60   F  1    606  18 56 05

18 57 33  ARP220       16 31 55  75.5 243.8  0.9      57.3    22   1  1    606  18 57 33
18 59 33  ---          16 33 55  75.1 244.8  1.0      58.1   120   F  1    610  18 57 34

19 00 03  J1532+2344   16 34 25  74.7 246.8  1.0      59.7    23   1  1    610  19 00 03
19 01 03  ---          16 35 25  74.5 247.2  1.0      60.0    60   F  1    612  19 00 04

19 01 48  J1516+1932   16 36 10  69.0 242.6  1.3      54.2    27   1  1    612  19 01 48
19 02 48  =1514+197    16 37 10  68.8 243.0  1.3      54.4    60   F  1    614  19 01 49

19 03 31  J1532+2344   16 37 54  74.0 248.2  1.1      60.8    27   1  1    614  19 03 31
19 04 31  ---          16 38 54  73.8 248.6  1.1      61.1    60   F  1    615  19 03 32

19 05 00  ARP220       16 39 23  74.0 247.2  1.1      59.9    22   1  1    615  19 05 00
19 07 00  ---          16 41 23  73.7 248.0  1.1      60.5   120   F  1    619  19 05 01

19 07 30  J1532+2344   16 41 53  73.2 249.8  1.1      61.9    23   1  1    619  19 07 30
19 08 30  ---          16 42 53  73.0 250.2  1.2      62.1    60   F  1    621  19 07 31

19 08 58  ARP220       16 43 22  73.3 248.8  1.1      61.0    22   1  1    621  19 08 58
19 10 58  ---          16 45 22  72.9 249.6  1.2      61.5   120   F  1    625  19 08 59

19 11 28  J1532+2344   16 45 52  72.4 251.2  1.2      62.8    22   1  1    625  19 11 28
19 12 28  ---          16 46 52  72.2 251.6  1.2      63.1    60   F  1    627  19 11 29
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

19 12 56  ARP220       16 47 20  72.5 250.3  1.2      62.0    22   1  1    627  19 12 56
19 14 56  ---          16 49 21  72.0 251.0  1.2      62.5   120   F  1    631  19 12 57

19 15 26  J1532+2344   16 49 50  71.6 252.6  1.3      63.7    22   1  1    631  19 15 26
19 16 26  ---          16 50 50  71.4 252.9  1.3      63.9    60   F  1    633  19 15 27

19 16 54  ARP220       16 51 19  71.6 251.7  1.3      62.9    22   1  1    633  19 16 54
19 18 54  ---          16 53 19  71.2 252.3  1.3      63.4   120   F  1    637  19 16 55

19 19 23  J1532+2344   16 53 48  70.8 253.8  1.3      64.5    22   1  1    637  19 19 23
19 20 23  ---          16 54 49  70.6 254.1  1.4      64.7    60   F  1    639  19 19 24

19 21 08  J1516+1932   16 55 33  65.2 249.1  1.6      58.5    28   1  1    639  19 21 08
19 22 08  =1514+197    16 56 33  65.0 249.4  1.7      58.7    60   F  1    641  19 21 09

19 22 51  J1532+2344   16 57 17  70.1 254.8  1.4      65.1    27   1  1    641  19 22 51
19 23 51  ---          16 58 17  69.9 255.1  1.4      65.2    60   F  1    643  19 22 52

19 24 19  ARP220       16 58 45  70.1 254.0  1.4      64.4    22   1  1    643  19 24 19
19 26 19  ---          17 00 46  69.7 254.6  1.4      64.7   120   F  1    646  19 24 20

19 26 48  J1532+2344   17 01 15  69.2 255.9  1.5      65.7    22   1  1    646  19 26 48
19 27 48  ---          17 02 15  69.0 256.1  1.5      65.8    60   F  1    648  19 26 49

19 28 17  ARP220       17 02 43  69.3 255.1  1.5      65.0    22   1  1    648  19 28 17
19 30 17  ---          17 04 44  68.9 255.6  1.5      65.3   120   F  1    652  19 28 18

19 30 45  J1532+2344   17 05 12  68.4 256.9  1.5      66.2    22   1  1    652  19 30 45
19 31 45  ---          17 06 13  68.2 257.2  1.6      66.4    60   F  1    654  19 30 46

19 32 13  ARP220       17 06 41  68.5 256.1  1.5      65.6    22   1  1    654  19 32 13
19 34 13  ---          17 08 41  68.0 256.7  1.6      65.9   120   F  1    658  19 32 14

19 34 42  J1532+2344   17 09 10  67.6 257.9  1.6      66.7    22   1  1    658  19 34 42
19 35 42  ---          17 10 10  67.4 258.1  1.6      66.9    60   F  1    660  19 34 43

19 36 10  ARP220       17 10 38  67.6 257.1  1.6      66.1    22   1  1    660  19 36 10
19 38 10  ---          17 12 38  67.2 257.6  1.6      66.4   120   F  1    664  19 36 11

19 38 39  J1532+2344   17 13 07  66.8 258.8  1.7      67.2    22   1  1    664  19 38 39
19 39 39  ---          17 14 07  66.5 259.0  1.7      67.3    60   F  1    666  19 38 40

19 40 23  J1516+1932   17 14 52  61.2 254.2  2.0      61.4    28   1  1    666  19 40 23
19 41 23  =1514+197    17 15 52  61.0 254.4  2.0      61.6    60   F  1    668  19 40 24
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

19 42 06  J1532+2344   17 16 35  66.0 259.5  1.7      67.5    27   1  1    668  19 42 06
19 43 06  ---          17 17 36  65.8 259.8  1.7      67.6    60   F  1    670  19 42 07

19 43 34  ARP220       17 18 04  66.1 258.9  1.7      67.0    22   1  1    670  19 43 34
19 45 34  ---          17 20 04  65.7 259.3  1.7      67.2   120   F  1    674  19 43 35

19 46 03  J1532+2344   17 20 32  65.2 260.4  1.8      67.9    22   1  1    674  19 46 03
19 47 03  ---          17 21 32  65.0 260.6  1.8      68.0    60   F  1    675  19 46 04

19 47 31  ARP220       17 22 00  65.2 259.7  1.8      67.4    22   1  1    675  19 47 31
19 49 31  ---          17 24 01  64.8 260.1  1.8      67.6   120   F  1    679  19 47 32

19 49 59  J1532+2344   17 24 29  64.3 261.2  1.9      68.2    22   1  1    679  19 49 59
19 50 59  ---          17 25 29  64.1 261.4  1.9      68.3    60   F  1    681  19 50 00

19 51 27  ARP220       17 25 57  64.4 260.5  1.8      67.7    22   1  1    681  19 51 27
19 53 27  ---          17 27 58  64.0 260.9  1.9      67.9   120   F  1    685  19 51 28

19 53 55  J1532+2344   17 28 26  63.5 261.9  1.9      68.5    21   1  1    685  19 53 55
19 54 55  ---          17 29 26  63.3 262.1  1.9      68.6    60   F  1    687  19 53 56

19 55 23  ARP220       17 29 54  63.6 261.3  1.9      68.0    22   1  1    687  19 55 23
19 57 23  ---          17 31 54  63.1 261.7  1.9      68.2   120   F  1    691  19 55 24

19 57 51  J1532+2344   17 32 22  62.7 262.6  2.0      68.8    21   1  1    691  19 57 51
19 58 51  ---          17 33 22  62.4 262.8  2.0      68.8    60   F  1    693  19 57 52

19 59 35  J1516+1932   17 34 07  57.2 258.3  2.3      63.4    28   1  1    693  19 59 35
20 00 35  =1514+197    17 35 07  57.0 258.5  2.3      63.4    60   F  1    695  19 59 36

20 01 19  J1532+2344   17 35 51  61.9 263.3  2.0      69.0    28   1  1    695  20 01 19
20 02 19  ---          17 36 51  61.7 263.4  2.1      69.0    60   F  1    697  20 01 20

20 02 46  ARP220       17 37 19  62.0 262.7  2.0      68.5    22   1  1    697  20 02 46
20 04 46  ---          17 39 19  61.6 263.0  2.1      68.6   120   F  1    701  20 02 47

20 05 14  J1532+2344   17 39 47  61.1 263.9  2.1      69.1    21   1  1    701  20 05 14
20 06 14  ---          17 40 47  60.9 264.1  2.1      69.2    60   F  1    703  20 05 15

20 06 42  ARP220       17 41 15  61.2 263.4  2.1      68.7    21   1  1    703  20 06 42
20 08 42  ---          17 43 15  60.7 263.7  2.1      68.8   120   F  1    706  20 06 43

20 09 10  J1532+2344   17 43 43  60.2 264.6  2.2      69.3    21   1  1    706  20 09 10
20 10 10  ---          17 44 43  60.0 264.8  2.2      69.4    60   F  1    708  20 09 11
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

20 10 37  ARP220       17 45 11  60.3 264.0  2.2      68.9    21   1  1    708  20 10 37
20 12 37  ---          17 47 11  59.9 264.4  2.2      69.0   120   F  1    712  20 10 38

20 13 05  J1532+2344   17 47 39  59.4 265.2  2.2      69.5    21   1  1    712  20 13 05
20 14 05  ---          17 48 39  59.2 265.4  2.3      69.5    60   F  1    714  20 13 06

20 14 33  ARP220       17 49 07  59.5 264.7  2.2      69.1    21   1  1    714  20 14 33
20 16 33  ---          17 51 07  59.0 265.0  2.3      69.2   120   F  1    718  20 14 34

20 17 01  J1532+2344   17 51 35  58.6 265.8  2.3      69.6    21   1  1    718  20 17 01
20 18 01  ---          17 52 35  58.3 266.0  2.3      69.6    60   F  1    720  20 17 02

20 18 45  J1516+1932   17 53 20  53.2 261.8  2.6      64.6    28   1  1    720  20 18 45
20 19 45  =1514+197    17 54 20  52.9 261.9  2.6      64.7    60   F  1    722  20 18 46

20 20 28  J1532+2344   17 55 04  57.8 266.4  2.4      69.7    28   1  1    722  20 20 28
20 21 28  ---          17 56 04  57.6 266.5  2.4      69.7    60   F  1    724  20 20 29

20 21 56  ARP220       17 56 31  57.9 265.8  2.4      69.3    21   1  1    724  20 21 56
20 23 56  ---          17 58 32  57.4 266.1  2.4      69.4   120   F  1    728  20 21 57

20 24 24  J1532+2344   17 58 59  57.0 266.9  2.4      69.8    21   1  1    728  20 24 24
20 25 24  ---          18 00 00  56.7 267.1  2.4      69.8    60   F  1    730  20 24 25

20 25 51  ARP220       18 00 27  57.0 266.4  2.4      69.4    21   1  1    730  20 25 51
20 27 51  ---          18 02 27  56.6 266.7  2.5      69.5   120   F  1    734  20 25 52

20 28 19  J1532+2344   18 02 55  56.1 267.5  2.5      69.9    21   1  1    734  20 28 19
20 29 19  ---          18 03 55  55.9 267.6  2.5      69.9    60   F  1    735  20 28 20

20 29 46  ARP220       18 04 23  56.2 267.0  2.5      69.5    21   1  1    735  20 29 46
20 31 46  ---          18 06 23  55.8 267.3  2.5      69.6   120   F  1    739  20 29 47

20 32 14  J1532+2344   18 06 51  55.3 268.0  2.6      69.9    21   1  1    739  20 32 14
20 33 14  ---          18 07 51  55.1 268.2  2.6      69.9    60   F  1    741  20 32 15

20 33 41  ARP220       18 08 19  55.3 267.6  2.6      69.6    21   1  1    741  20 33 41
20 35 41  ---          18 10 19  54.9 267.8  2.6      69.6   120   F  1    745  20 33 42

20 36 09  J1532+2344   18 10 47  54.4 268.6  2.6      70.0    21   1  1    745  20 36 09
20 37 09  ---          18 11 47  54.2 268.7  2.6      70.0    60   F  1    747  20 36 10

20 37 53  J1516+1932   18 12 31  49.1 264.8  2.9      65.4    28   1  1    747  20 37 53
20 38 53  =1514+197    18 13 31  48.8 265.0  2.9      65.4    60   F  1    749  20 37 54
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

20 39 37  J1532+2344   18 14 15  53.7 269.0  2.7      70.0    28   1  1    749  20 39 37
20 40 37  ---          18 15 15  53.5 269.2  2.7      70.0    60   F  1    751  20 39 38

20 41 04  ARP220       18 15 43  53.8 268.6  2.7      69.7    21   1  1    751  20 41 04
20 43 04  ---          18 17 43  53.3 268.9  2.7      69.7   120   F  1    755  20 41 05

20 43 32  J1532+2344   18 18 11  52.8 269.6  2.8      70.0    21   1  1    755  20 43 32
20 44 32  ---          18 19 11  52.6 269.7  2.8      70.0    60   F  1    757  20 43 33

20 44 59  ARP220       18 19 38  52.9 269.1  2.7      69.7    21   1  1    757  20 44 59
20 46 59  ---          18 21 38  52.5 269.4  2.8      69.7   120   F  1    761  20 45 00

20 47 26  J1532+2344   18 22 06  52.0 270.1  2.8      70.0    21   1  1    761  20 47 26
20 48 26  ---          18 23 06  51.8 270.2  2.8      70.0    60   F  1    763  20 47 27

20 48 54  ARP220       18 23 34  52.1 269.6  2.8      69.7    21   1  1    763  20 48 54
20 50 54  ---          18 25 34  51.6 269.9  2.8      69.7   120   F  1    766  20 48 55

20 51 21  J1532+2344   18 26 02  51.1 270.6  2.9      70.0    21   1  1    766  20 51 21
20 52 21  ---          18 27 02  50.9 270.7  2.9      70.0    60   F  1    768  20 51 22

20 52 49  ARP220       18 27 29  51.2 270.1  2.9      69.7    21   1  1    768  20 52 49
20 54 49  ---          18 29 29  50.8 270.4  2.9      69.7   120   F  1    772  20 52 50

20 55 16  J1532+2344   18 29 57  50.3 271.0  2.9      70.0    21   1  1    772  20 55 16
20 56 16  ---          18 30 57  50.1 271.2  3.0      70.0    60   F  1    774  20 55 17

20 57 00  J1516+1932   18 31 42  44.9 267.6  3.2      65.8    28   1  1    774  20 57 00
20 58 00  =1514+197    18 32 42  44.7 267.7  3.3      65.8    60   F  1    776  20 57 01

20 58 44  J1532+2344   18 33 25  49.6 271.5  3.0      70.0    28   1  1    776  20 58 44
20 59 44  ---          18 34 25  49.3 271.6  3.0      69.9    60   F  1    778  20 58 45

21 00 11  ARP220       18 34 53  49.6 271.0  3.0      69.7    21   1  1    778  21 00 11
21 02 11  ---          18 36 53  49.2 271.3  3.0      69.7   120   F  1    782  21 00 12

21 02 39  J1532+2344   18 37 21  48.7 271.9  3.1      69.9    21   1  1    782  21 02 39
21 03 39  ---          18 38 21  48.5 272.1  3.1      69.9    60   F  1    784  21 02 40

21 04 06  ARP220       18 38 48  48.8 271.5  3.1      69.7    21   1  1    784  21 04 06
21 06 06  ---          18 40 48  48.4 271.8  3.1      69.7   120   F  1    788  21 04 07

21 06 33  J1532+2344   18 41 16  47.9 272.4  3.1      69.9    21   1  1    788  21 06 33
21 07 33  ---          18 42 16  47.7 272.5  3.2      69.9    60   F  1    790  21 06 34
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

21 08 00  ARP220       18 42 43  47.9 272.0  3.1      69.6    21   1  1    790  21 08 00
21 10 00  ---          18 44 44  47.5 272.2  3.2      69.6   120   F  1    793  21 08 01

21 10 28  J1532+2344   18 45 11  47.0 272.9  3.2      69.8    21   1  1    793  21 10 28
21 11 28  ---          18 46 12  46.8 273.0  3.2      69.8    60   F  1    795  21 10 29

21 11 55  ARP220       18 46 39  47.1 272.5  3.2      69.6    21   1  1    795  21 11 55
21 13 55  ---          18 48 39  46.7 272.7  3.2      69.6   120   F  1    799  21 11 56

21 14 23  J1532+2344   18 49 07  46.2 273.3  3.3      69.7    21   1  1    799  21 14 23
21 15 23  ---          18 50 07  46.0 273.4  3.3      69.7    60   F  1    801  21 14 24

21 18 06  J1516+1932   18 52 50  40.4 270.3  3.6      65.9   146   1  1    801  21 18 06
21 19 06  =1514+197    18 53 50  40.2 270.5  3.6      65.9    60   F  1    803  21 18 07

21 20 24  J1532+2344   18 55 09  44.9 274.0  3.4      69.6    63   1  1    803  21 20 24
21 21 24  ---          18 56 09  44.7 274.1  3.4      69.6    60   F  1    805  21 20 25

21 21 51  ARP220       18 56 37  45.0 273.6  3.4      69.4    21   1  1    805  21 21 51
21 23 51  ---          18 58 37  44.5 273.8  3.4      69.4   120   F  1    809  21 21 52

21 24 19  J1532+2344   18 59 05  44.0 274.4  3.4      69.5    21   1  1    809  21 24 19
21 25 19  ---          19 00 05  43.8 274.5  3.5      69.5    60   F  1    811  21 24 20

21 25 46  ARP220       19 00 32  44.1 274.1  3.4      69.3    21   1  1    811  21 25 46
21 27 46  ---          19 02 32  43.7 274.3  3.5      69.3   120   F  1    815  21 25 47

21 28 14  J1532+2344   19 03 00  43.2 274.9  3.5      69.4    21   1  1    815  21 28 14
21 29 14  ---          19 04 00  43.0 275.0  3.5      69.4    60   F  1    817  21 28 15

21 29 41  ARP220       19 04 27  43.3 274.5  3.5      69.3    21   1  1    817  21 29 41
21 31 41  ---          19 06 28  42.9 274.7  3.5      69.2   120   F  1    821  21 29 42

21 32 08  J1532+2344   19 06 55  42.4 275.3  3.6      69.3    21   1  1    821  21 32 08
21 33 08  ---          19 07 55  42.2 275.4  3.6      69.3    60   F  1    823  21 32 09

21 33 35  ARP220       19 08 22  42.4 274.9  3.6      69.2    21   1  1    823  21 33 35
21 35 35  ---          19 10 23  42.0 275.1  3.6      69.1   120   F  1    826  21 33 36

21 36 03  J1532+2344   19 10 50  41.5 275.7  3.6      69.2    21   1  1    826  21 36 03
21 37 03  ---          19 11 51  41.3 275.8  3.6      69.2    60   F  1    828  21 36 04

21 37 47  J1516+1932   19 12 35  36.1 272.8  3.9      65.8    28   1  1    828  21 37 47
21 38 47  =1514+197    19 13 35  35.9 272.9  3.9      65.7    60   F  1    830  21 37 48
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

21 39 31  J1532+2344   19 14 19  40.8 276.1  3.7      69.1    28   1  1    830  21 39 31
21 40 31  ---          19 15 19  40.6 276.2  3.7      69.1    60   F  1    832  21 39 32

21 40 58  ARP220       19 15 46  40.9 275.7  3.7      69.0    21   1  1    832  21 40 58
21 42 58  ---          19 17 47  40.4 276.0  3.7      68.9   120   F  1    836  21 40 59

21 43 25  J1532+2344   19 18 14  39.9 276.5  3.8      69.0    21   1  1    836  21 43 25
21 44 25  ---          19 19 14  39.7 276.6  3.8      69.0    60   F  1    838  21 43 26

21 44 52  ARP220       19 19 42  40.0 276.2  3.7      68.9    21   1  1    838  21 44 52
21 46 52  ---          19 21 42  39.6 276.4  3.8      68.8   120   F  1    842  21 44 53

21 47 20  J1532+2344   19 22 09  39.1 276.9  3.8      68.9    21   1  1    842  21 47 20
21 48 20  ---          19 23 10  38.9 277.0  3.8      68.9    60   F  1    844  21 47 21

21 48 47  ARP220       19 23 37  39.2 276.6  3.8      68.7    21   1  1    844  21 48 47
21 50 47  ---          19 25 37  38.8 276.8  3.8      68.7   120   F  1    848  21 48 48

21 51 15  J1532+2344   19 26 05  38.3 277.4  3.9      68.8    21   1  1    848  21 51 15
21 52 15  ---          19 27 05  38.1 277.5  3.9      68.7    60   F  1    850  21 51 16

21 52 42  ARP220       19 27 32  38.3 277.0  3.9      68.6    21   1  1    850  21 52 42
21 54 42  ---          19 29 32  37.9 277.2  3.9      68.5   120   F  1    853  21 52 43

21 55 09  J1532+2344   19 30 00  37.4 277.8  3.9      68.6    21   1  1    853  21 55 09
21 56 09  ---          19 31 00  37.2 277.9  4.0      68.6    60   F  1    855  21 55 10

21 56 54  J1516+1932   19 31 45  32.0 275.0  4.2      65.4    28   1  1    855  21 56 54
21 57 54  =1514+197    19 32 45  31.8 275.1  4.3      65.4    60   F  1    857  21 56 55

21 58 37  J1532+2344   19 33 29  36.7 278.1  4.0      68.5    28   1  1    857  21 58 37
21 59 37  ---          19 34 29  36.5 278.2  4.0      68.4    60   F  1    859  21 58 38

22 00 04  ARP220       19 34 56  36.8 277.8  4.0      68.3    21   1  1    859  22 00 04
22 02 04  ---          19 36 56  36.3 278.0  4.0      68.3   120   F  1    863  22 00 05

22 02 32  J1532+2344   19 37 24  35.9 278.5  4.1      68.3    21   1  1    863  22 02 32
22 03 32  ---          19 38 24  35.6 278.6  4.1      68.3    60   F  1    865  22 02 33

22 03 59  ARP220       19 38 51  35.9 278.2  4.1      68.2    21   1  1    865  22 03 59
22 05 59  ---          19 40 51  35.5 278.4  4.1      68.1   120   F  1    869  22 04 00

22 06 26  J1532+2344   19 41 19  35.0 279.0  4.1      68.2    21   1  1    869  22 06 26
22 07 26  ---          19 42 19  34.8 279.1  4.2      68.1    60   F  1    871  22 06 27
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

22 07 53  ARP220       19 42 46  35.1 278.6  4.1      68.1    21   1  1    871  22 07 53
22 09 53  ---          19 44 47  34.7 278.8  4.2      68.0   120   F  1    875  22 07 54

22 10 21  J1532+2344   19 45 14  34.2 279.4  4.2      68.0    21   1  1    875  22 10 21
22 11 21  ---          19 46 14  34.0 279.5  4.2      68.0    60   F  1    877  22 10 22

22 11 48  ARP220       19 46 41  34.3 279.0  4.2      67.9    21   1  1    877  22 11 48
22 13 48  ---          19 48 42  33.8 279.2  4.2      67.8   120   F  1    881  22 11 49

22 14 15  J1532+2344   19 49 09  33.4 279.8  4.3      67.8    21   1  1    881  22 14 15
22 15 15  ---          19 50 09  33.2 279.9  4.3      67.8    60   F  1    883  22 14 16

22 15 42  ARP220       19 50 36  33.4 279.4  4.3      67.7    21   1  1    883  22 15 42
22 17 42  ---          19 52 37  33.0 279.6  4.3      67.6   120   F  1    886  22 15 43

22 18 10  J1532+2344   19 53 04  32.5 280.2  4.3      67.7    21   1  1    886  22 18 10
22 19 10  ---          19 54 05  32.3 280.3  4.4      67.6    60   F  1    888  22 18 11

22 19 37  ARP220       19 54 32  32.6 279.8  4.3      67.6    21   1  1    888  22 19 37
22 21 37  ---          19 56 32  32.2 280.0  4.4      67.5   120   F  1    892  22 19 38

22 22 04  J1532+2344   19 56 59  31.7 280.6  4.4      67.5    21   1  1    892  22 22 04
22 23 04  ---          19 58 00  31.5 280.7  4.4      67.4    60   F  1    894  22 22 05

22 23 31  ARP220       19 58 27  31.8 280.2  4.4      67.4    21   1  1    894  22 23 31
22 25 31  ---          20 00 27  31.3 280.5  4.4      67.3   120   F  1    898  22 23 32

22 25 59  J1532+2344   20 00 55  30.9 281.0  4.5      67.3    21   1  1    898  22 25 59
22 26 59  ---          20 01 55  30.7 281.1  4.5      67.3    60   F  1    900  22 26 00

22 27 41  J1516+1932   20 02 37  25.4 278.5  4.8      64.5    26   1  1    900  22 27 41
22 30 41  =1514+197    20 05 38  24.8 278.9  4.8      64.4   180   F  1    906  22 27 42

22 31 22  J1532+2344   20 06 19  29.7 281.5  4.6      67.0    25   1  1    906  22 31 22
22 32 22  ---          20 07 19  29.5 281.6  4.6      67.0    60   F  1    908  22 31 23

22 32 49  ARP220       20 07 46  29.8 281.2  4.5      67.0    21   1  1    908  22 32 49
22 34 49  ---          20 09 47  29.4 281.4  4.6      66.9   120   F  1    912  22 32 50

22 35 17  J1532+2344   20 10 14  28.9 281.9  4.6      66.8    21   1  1    912  22 35 17
22 36 17  ---          20 11 14  28.7 282.0  4.6      66.8    60   F  1    913  22 35 18

22 36 44  ARP220       20 11 41  29.0 281.6  4.6      66.8    21   1  1    913  22 36 44
22 38 44  ---          20 13 42  28.5 281.8  4.6      66.7   120   F  1    917  22 36 45
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

22 39 11  J1532+2344   20 14 09  28.1 282.3  4.7      66.6    21   1  1    917  22 39 11
22 40 11  ---          20 15 09  27.9 282.4  4.7      66.6    60   F  1    919  22 39 12

22 40 38  ARP220       20 15 36  28.1 282.0  4.7      66.6    21   1  1    919  22 40 38
22 42 38  ---          20 17 37  27.7 282.2  4.7      66.5   120   F  1    923  22 40 39

22 43 06  J1532+2344   20 18 04  27.3 282.7  4.8      66.4    21   1  1    923  22 43 06
22 44 06  ---          20 19 04  27.1 282.8  4.8      66.4    60   F  1    925  22 43 07

22 44 33  ARP220       20 19 31  27.3 282.4  4.7      66.4    21   1  1    925  22 44 33
22 46 33  ---          20 21 32  26.9 282.6  4.8      66.3   120   F  1    929  22 44 34

22 47 00  J1532+2344   20 21 59  26.4 283.1  4.8      66.2    21   1  1    929  22 47 00
22 48 00  ---          20 23 00  26.2 283.2  4.8      66.2    60   F  1    931  22 47 01

22 48 42  J1516+1932   20 23 42  21.0 280.9  5.1      63.7    26   1  1    931  22 48 42
22 49 42  =1514+197    20 24 42  20.8 281.0  5.1      63.7    60   F  1    933  22 48 43

22 50 24  J1532+2344   20 25 24  25.7 283.5  4.9      66.0    25   1  1    933  22 50 24
22 51 24  ---          20 26 24  25.5 283.6  4.9      66.0    60   F  1    935  22 50 25

22 51 51  ARP220       20 26 51  25.8 283.2  4.9      66.0    21   1  1    935  22 51 51
22 53 51  ---          20 28 51  25.4 283.4  4.9      65.9   120   F  1    939  22 51 52

22 54 18  J1532+2344   20 29 19  24.9 283.9  4.9      65.8    21   1  1    939  22 54 18
22 55 18  ---          20 30 19  24.7 284.0  5.0      65.8    60   F  1    941  22 54 19

22 55 45  ARP220       20 30 46  25.0 283.6  4.9      65.8    21   1  1    941  22 55 45
22 57 45  ---          20 32 46  24.5 283.8  5.0      65.6   120   F  1    944  22 55 46

22 58 13  J1532+2344   20 33 14  24.1 284.3  5.0      65.6    21   1  1    944  22 58 13
22 59 13  ---          20 34 14  23.9 284.4  5.0      65.5    60   F  1    946  22 58 14

22 59 40  ARP220       20 34 41  24.1 284.0  5.0      65.5    21   1  1    946  22 59 40
23 01 40  ---          20 36 41  23.7 284.2  5.0      65.4   120   F  1    950  22 59 41

23 02 07  J1532+2344   20 37 09  23.3 284.7  5.1      65.4    21   1  1    950  23 02 07
23 03 07  ---          20 38 09  23.1 284.8  5.1      65.3    60   F  1    952  23 02 08

23 03 34  ARP220       20 38 36  23.3 284.4  5.1      65.3    21   1  1    952  23 03 34
23 05 34  ---          20 40 36  22.9 284.6  5.1      65.2   120   F  1    956  23 03 35

23 06 01  J1532+2344   20 41 04  22.5 285.1  5.1      65.1    21   1  1    956  23 06 01
23 07 01  ---          20 42 04  22.3 285.2  5.2      65.1    60   F  1    958  23 06 02
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

23 07 44  J1516+1932   20 42 46  17.0 283.0  5.4      62.8    26   1  1    958  23 07 44
23 08 44  =1514+197    20 43 46  16.7 283.1  5.4      62.7    60   F  1    960  23 07 45

23 09 25  J1532+2344   20 44 28  21.8 285.5  5.2      64.9    25   1  1    960  23 09 25
23 10 25  ---          20 45 28  21.5 285.6  5.2      64.9    60   F  1    962  23 09 26

23 10 52  ARP220       20 45 55  21.8 285.2  5.2      64.9    21   1  1    962  23 10 52
23 12 52  ---          20 47 56  21.4 285.4  5.2      64.8   120   F  1    966  23 10 53

23 13 20  J1532+2344   20 48 23  20.9 285.9  5.3      64.7    21   1  1    966  23 13 20
23 14 20  ---          20 49 23  20.7 286.0  5.3      64.6    60   F  1    968  23 13 21

23 14 46  ARP220       20 49 50  21.0 285.6  5.2      64.6    21   1  1    968  23 14 46
23 16 46  ---          20 51 51  20.6 285.8  5.3      64.5   120   F  1    972  23 14 47

23 17 14  J1532+2344   20 52 18  20.1 286.3  5.3      64.4    21   1  1    972  23 17 14
23 18 14  ---          20 53 18  19.9 286.4  5.3      64.4    60   F  1    973  23 17 15

23 18 41  ARP220       20 53 45  20.2 286.0  5.3      64.4    21   1  1    973  23 18 41
23 20 41  ---          20 55 46  19.8 286.2  5.3      64.3   120   F  1    977  23 18 42

23 21 08  J1532+2344   20 56 13  19.3 286.7  5.4      64.2    21   1  1    977  23 21 08
23 22 08  ---          20 57 13  19.1 286.8  5.4      64.1    60   F  1    979  23 21 09

23 22 35  ARP220       20 57 40  19.4 286.4  5.4      64.1    21   1  1    979  23 22 35
23 24 35  ---          20 59 41  19.0 286.6  5.4      64.0   120   F  1    983  23 22 36

23 25 03  J1532+2344   21 00 08  18.5 287.1  5.5      63.9    21   1  1    983  23 25 03
23 26 03  ---          21 01 08  18.3 287.2  5.5      63.8    60   F  1    985  23 25 04

23 26 45  J1516+1932   21 01 51  13.0 285.2  5.7      61.8    26   1  1    985  23 26 45
23 27 45  =1514+197    21 02 51  12.8 285.3  5.8      61.7    60   F  1    987  23 26 46

23 28 27  J1532+2344   21 03 33  17.8 287.5  5.5      63.7    25   1  1    987  23 28 27
23 29 27  ---          21 04 33  17.6 287.6  5.5      63.6    60   F  1    989  23 28 28

23 29 54  ARP220       21 05 00  17.9 287.2  5.5      63.7    21   1  1    989  23 29 54
23 31 54  ---          21 07 00  17.5 287.4  5.5      63.5   120   F  1    993  23 29 55

23 32 21  J1532+2344   21 07 28  17.0 287.9  5.6      63.4    21   1  1    993  23 32 21
23 33 21  ---          21 08 28  16.8 288.0  5.6      63.3    60   F  1    995  23 32 22

23 33 48  ARP220       21 08 55  17.1 287.6  5.6      63.4    21   1  1    995  23 33 48
23 35 48  ---          21 10 55  16.7 287.8  5.6      63.3   120   F  1    999  23 33 49
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Tue  28 Nov 2006   Day 332 ---

23 36 15  J1532+2344   21 11 23  16.2 288.3  5.6      63.1    21   1  1    999  23 36 15
23 37 15  ---          21 12 23  16.0 288.4  5.7      63.1    60   F  1   1001  23 36 16

23 37 42  ARP220       21 12 50  16.3 288.0  5.6      63.1    21   1  1   1001  23 37 42
23 39 42  ---          21 14 50  15.9 288.3  5.7      63.0   120   F  1   1004  23 37 43

23 40 10  J1532+2344   21 15 18  15.4 288.7  5.7      62.9    21   1  1   1004  23 40 10
23 41 10  ---          21 16 18  15.2 288.9  5.7      62.8    60   F  1   1006  23 40 11

23 41 36  ARP220       21 16 45  15.5 288.5  5.7      62.9    21   1  1   1006  23 41 36
23 43 36  ---          21 18 45  15.1 288.7  5.7      62.7   120   F  1   1010  23 41 37

23 44 04  J1532+2344   21 19 13  14.6 289.2  5.8      62.6    21   1  1   1010  23 44 04
23 45 04  ---          21 20 13  14.4 289.3  5.8      62.5    60   F  1   1012  23 44 05

23 45 46  J1516+1932   21 20 55   9.0 287.4  6.1      60.6    26   1  1   1012  23 45 46
23 46 46  =1514+197    21 21 55   8.8 287.5  6.1      60.5    60   F  1   1014  23 45 47

23 47 28  J1532+2344   21 22 37  13.9 289.5  5.8      62.3    25   1  1   1014  23 47 28
23 48 28  ---          21 23 37  13.7 289.7  5.8      62.2    60   F  1   1016  23 47 29

23 48 55  ARP220       21 24 04  14.0 289.3  5.8      62.3    21   1  1   1016  23 48 55
23 50 55  ---          21 26 05  13.6 289.5  5.8      62.2   120   F  1   1020  23 48 56

23 51 22  J1532+2344   21 26 32  13.1 290.0  5.9      62.0    21   1  1   1020  23 51 22
23 52 22  ---          21 27 32  12.9 290.1  5.9      62.0    60   F  1   1022  23 51 23

23 52 49  ARP220       21 27 59  13.2 289.7  5.9      62.0    21   1  1   1022  23 52 49
23 54 49  ---          21 30 00  12.8 289.9  5.9      61.9   120   F  1   1026  23 52 50

23 55 17  J1532+2344   21 30 27  12.3 290.4  6.0      61.7    21   1  1   1026  23 55 17
23 56 17  ---          21 31 27  12.1 290.5  6.0      61.7    60   F  1   1028  23 55 18

23 56 44  ARP220       21 31 54  12.4 290.1  5.9      61.7    21   1  1   1028  23 56 44
23 58 44  ---          21 33 55  12.0 290.3  6.0      61.6   120   F  1   1032  23 56 45

 --- Start: Tue  28 Nov 2006   Day 332 -- Stop: Wed  29 Nov 2006   Day 333 ---

23 59 11  J1532+2344   21 34 22  11.6 290.8  6.0      61.4    21   1  1   1032  23 59 11
00 00 11  ---          21 35 22  11.4 291.0  6.0      61.4    60   F  1   1033  23 59 12

00 00 38  ARP220       21 35 49  11.6 290.6  6.0      61.4    21   1  1   1033  00 00 38
00 02 38  ---          21 37 50  11.2 290.8  6.0      61.3   120   F  1   1037  00 00 39
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Wed  29 Nov 2006   Day 333 ---

00 03 05  J1532+2344   21 38 17  10.8 291.3  6.1      61.1    21   1  1   1037  00 03 05
00 04 05  ---          21 39 17  10.6 291.4  6.1      61.0    60   F  1   1039  00 03 06

00 04 48  J1516+1932   21 40 00   5.2 289.7  6.4      59.3    26   1  1   1039  00 04 48
00 05 48  =1514+197    21 41 00   4.9 289.8  6.4      59.2    60   F  1   1041  00 04 49

00 06 30  J1532+2344   21 41 42  10.1 291.7  6.1      60.8    25   1  1   1041  00 06 30
00 07 30  ---          21 42 42   9.9 291.8  6.2      60.8    60   F  1   1043  00 06 31

00 07 56  ARP220       21 43 09  10.1 291.4  6.1      60.9    21   1  1   1043  00 07 56
00 09 56  ---          21 45 09   9.7 291.6  6.2      60.7   120   F  1   1047  00 07 57

00 10 24  J1532+2344   21 45 37   9.3 292.1  6.2      60.5    21   1  1   1047  00 10 24
00 11 24  ---          21 46 37   9.1 292.2  6.2      60.4    60   F  1   1049  00 10 25

00 11 51  ARP220       21 47 04   9.3 291.8  6.2      60.6    21   1  1   1049  00 11 51
00 13 51  ---          21 49 04   8.9 292.1  6.2      60.4   120   F  1   1053  00 11 52

00 14 18  J1532+2344   21 49 32   8.5 292.6  6.3      60.2    21   1  1   1053  00 14 18
00 15 18  ---          21 50 32   8.3 292.7  6.3      60.1    60   F  1   1055  00 14 19

00 15 45  ARP220       21 50 59   8.6 292.3  6.3      60.2    21   1  1   1055  00 15 45
00 17 45  ---          21 52 59   8.2 292.5  6.3      60.1   120   F  1   1059  00 15 46

00 18 12  J1532+2344   21 53 27   7.8 293.0  6.3      59.9    21   1  1   1059  00 18 12
00 19 12  ---          21 54 27   7.6 293.1  6.4      59.8    60   F  1   1061  00 18 13

00 19 39  ARP220       21 54 54   7.8 292.7  6.3      59.9    21   1  1   1061  00 19 39
00 21 39  ---          21 56 54   7.4 293.0  6.4      59.7   120   F  1   1064  00 19 40

00 22 07  J1532+2344   21 57 21   7.0 293.5  6.4      59.5    21   1  1   1064  00 22 07
00 23 07  ---          21 58 22   6.8 293.6  6.4      59.5    60   F  1   1066  00 22 08

00 24 41  J1532+2344   21 59 56   6.5 293.8  6.4      59.3    88   1  1   1066  00 24 41
00 25 41  ---          22 00 56   6.3 293.9  6.5      59.2    60   F  1   1068  00 24 42

00 25 48  ARP220       22 01 03   6.6 293.4  6.4      59.4     1   1  1   1068  00 25 41
00 27 48  ---          22 03 03   6.2 293.7  6.5      59.2   120   F  1   1072  00 25 42

00 27 54  J1532+2344   22 03 10   5.8 294.2  6.5      59.0     1   1  1   1072  00 27 48
00 28 54  ---          22 04 10   5.6 294.3  6.5      58.9    60   F  1   1075  00 27 49

00 29 01  ARP220       22 04 17   5.9 293.8  6.5      59.1     1   1  1   1075  00 28 54
00 31 01  ---          22 06 17   5.5 294.1  6.5      58.9   120   F  1   1079  00 28 55
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               8GHz obs of SN/SNR in ARP 220
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Wed  29 Nov 2006   Day 333 ---

00 31 08  J1532+2344   22 06 24   5.2 294.5  6.6      58.7     1   1  1   1079  00 31 01
00 32 08  ---          22 07 24   5.0 294.7  6.6      58.7    60   F  1   1081  00 31 02

00 32 15  ARP220       22 07 31   5.3 294.2  6.5      58.8     1   1  1   1081  00 32 08
00 34 15  ---          22 09 32   4.9 294.5  6.6      58.6   120   F  1   1085  00 32 09

00 34 21  J1532+2344   22 09 38   4.6 294.9  6.6      58.5     1   1  1   1085  00 34 15
00 35 21  ---          22 10 39   4.4 295.0  6.6      58.4    60   F  1   1087  00 34 16

00 35 28  ARP220       22 10 45   4.7 294.6  6.6      58.5     1   1  1   1087  00 35 21
00 37 28  ---          22 12 46   4.3 294.8  6.6      58.4   120   F  1   1091  00 35 22

00 37 35  J1532+2344   22 12 52   3.9 295.3  6.7      58.2     1   1  1   1091  00 37 28
00 38 35  ---          22 13 53   3.7 295.4  6.7      58.1    60   F  1   1093  00 37 29

00 40 09  J1532+2344   22 15 27   3.4 295.6  6.7      57.9    88   1  1   1093  00 40 09
00 41 09  ---          22 16 27   3.2 295.8  6.7      57.8    60   F  1   1095  00 40 10

00 41 16  ARP220       22 16 34   3.5 295.3  6.7      58.0     1   1  1   1095  00 41 09
00 43 16  ---          22 18 34   3.1 295.6  6.7      57.8   120   F  1   1099  00 41 10

00 43 23  J1532+2344   22 18 41   2.8 296.0  6.8      57.6     1   1  1   1099  00 43 16
00 44 23  ---          22 19 41   2.6 296.2  6.8      57.5    60   F  1   1101  00 43 17

00 44 29  ARP220       22 19 48   2.9 295.7  6.7      57.7     1   1  1   1101  00 44 23
00 46 29  ---          22 21 48   2.5 295.9  6.8      57.5   120   F  1   1106  00 44 24

00 47 43  ARP220       22 23 02   2.3 296.1  6.8      57.4    68   1  1   1106  00 47 36
00 49 43  ---          22 25 02   1.9 296.3  6.8  D   57.2     0   F  1   1110  00 47 37


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /home/rodrigo/ASTRO/SCHED_6.05/setups/v4cm-256-8-2.set
   Matches group v4cm_3 in /home/rodrigo/ASTRO/SCHED_6.05/catalogs/freq.dat

   Setup group:   10         Station: VLBA_FD           Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:  10  Setup file default.  Used pcal sets:   1
   LO sum=    8405.49   8405.49   8413.49   8413.49   8421.49   8421.49   8429.49   8429.49
   BBC fr=     805.49    805.49    813.49    813.49    821.49    821.49    829.49    829.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   510   510   510   510  6510  6510  6510  6510
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_off 
 SOURCE LIST -- 8GHz obs of SN/SNR in ARP 220
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * ARP220            15 32 46.905485   * 15 34 57.250000     15 35 14.038743       0.00
                     23 40 07.75728    * 23 30 11.33000      23 28 43.14854        0.00
                     From catalog imbedded in main SCHED input file.
                        8.800 scan hours,    432.388 baseline hours above horizon.

 * J1516+1932        15 14 40.985837   * 15 16 56.796160     15 17 14.400593       0.32
   1514+197          19 43 10.94235    * 19 32 12.99192      19 30 36.58254        0.23
   J1516+19          From catalog imbedded in main SCHED input file.
                     VLBA Calib Srcs - GSFC sols. - catalog 2004f_astro
                        1.300 scan hours,     73.118 baseline hours above horizon.

 * J1532+2344        15 30 36.092761   * 15 32 46.345216     15 33 03.125666       0.27
                     23 54 09.32935    * 23 44 05.26818      23 42 35.97157        0.48
                     From catalog imbedded in main SCHED input file.
                     VLBA Calib Srcs - GSFC sols. - catalog 2004f_astro
                        5.417 scan hours,    263.604 baseline hours above horizon.

 * J1613+3412        16 11 47.914253   * 16 13 41.064244     16 13 55.290649       0.24
   1611+343          34 20 19.83395    * 34 12 47.90897      34 11 39.77789        0.40
   J1613+34          From catalog imbedded in main SCHED input file.
                     VLBA Calib Srcs - GSFC sols. - catalog 2004f_astro
                        0.400 scan hours,     38.167 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   ARP220              46.0
   J1516+1932          43.4
   J1532+2344          46.3
   J1613+3412          55.5

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

