  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The true nature of the jet base in 3C84
 Exp. Code:  GP058A  


Schedule Version:      10.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Georgios Filippos Paraschos

Address:  Max-Planck-Institute for Radiostronomy
          Auf dem Huegel, 69
          Bonn, NRW, 53121
          Germany

Phone:    +49228525292
EMAIL:    gfparaschos@mpifr-bonn.mpg.de
Fax:
Phone during observation: +492257301155

Observing mode:

Notes:    PHASECAL should be ON
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   8 Nov 2021   Day 312 ---

 Next scan frequencies:  22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
 Next BBC frequencies:     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

22 36 01  0716+714     18 53 34  12.1  -2.5 11.5       6.8     0        0   22 36 01
22 41 01  ---          18 58 35  12.0  -2.1 11.6       5.7   300       77   22 36 02

22 42 01  0716+714     18 59 35  12.0  -2.0 11.6       5.4    54       77   22 42 01
22 47 01  ---          19 04 36  12.0  -1.6 11.7       4.3   300      155   22 42 02

23 00 01  0716+714     19 17 38  11.9  -0.6 11.9       1.5   774      155   23 00 01
23 06 01  ---          19 23 39  11.9  -0.1 12.0       0.2   360      247   23 00 02

23 07 41  0716+714     19 25 19  11.9   0.1-12.0      -0.2    94      247   23 07 41
23 13 41  ---          19 31 20  11.9   0.6-11.9      -1.5   360      340   23 07 42

23 15 21  0716+714     19 33 01  11.9   0.7-11.9      -1.9    94      340   23 15 21
23 21 21  ---          19 39 02  12.0   1.2-11.8      -3.2   360      433   23 15 22

23 23 01  0716+714     19 40 42  12.0   1.3-11.7      -3.6    94      433   23 23 01
23 29 01  ---          19 46 43  12.0   1.8-11.6      -4.9   360      526   23 23 02

23 30 41  0716+714     19 48 23  12.0   2.0-11.6      -5.3    94      526   23 30 41
23 36 41  ---          19 54 24  12.1   2.5-11.5      -6.6   360      618   23 30 42

23 38 21  0716+714     19 56 04  12.1   2.6-11.5      -7.0    94      618   23 38 21
23 44 21  ---          20 02 05  12.2   3.1-11.4      -8.3   360      711   23 38 22

23 46 01  0716+714     20 03 46  12.2   3.2-11.3      -8.7    94      711   23 46 01
23 52 01  ---          20 09 47  12.2   3.7-11.2     -10.0   360      804   23 46 02

23 53 41  0716+714     20 11 27  12.3   3.8-11.2     -10.4    94      804   23 53 41
23 59 41  ---          20 17 28  12.4   4.3-11.1     -11.7   360      897   23 53 42

 --- Tue   9 Nov 2021   Day 313 ---

00 01 21  0716+714     20 19 08  12.4   4.5-11.1     -12.0    94      897   00 01 21
00 07 21  ---          20 25 09  12.5   4.9-11.0     -13.4   360      989   00 01 22

00 09 01  0716+714     20 26 50  12.5   5.1-11.0     -13.7    94      989   00 09 01
00 15 01  ---          20 32 50  12.6   5.6-10.9     -15.0   360     1082   00 09 02

00 16 41  0716+714     20 34 31  12.7   5.7-10.8     -15.4    94     1082   00 16 41
00 22 41  ---          20 40 32  12.8   6.2-10.7     -16.7   360     1175   00 16 42
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   9 Nov 2021   Day 313 ---

00 24 21  0716+714     20 42 12  12.9   6.3-10.7     -17.1    94     1175   00 24 21
00 30 21  ---          20 48 13  13.0   6.8-10.6     -18.4   360     1268   00 24 22

00 32 01  0716+714     20 49 53  13.0   6.9-10.6     -18.8    94     1268   00 32 01
00 38 01  ---          20 55 54  13.2   7.4-10.5     -20.1   360     1360   00 32 02

00 40 00  3C84         20 57 54  15.8  50.7 -6.4     -62.8    80     1360   00 40 00
00 50 00  ---          21 07 55  17.5  51.5 -6.2     -64.2   600     1515   00 40 01

00 50 45  3C84         21 08 40  17.6  51.6 -6.2     -64.4    39     1515   00 50 45
01 00 45  ---          21 18 42  19.3  52.4 -6.0     -65.8   600     1669   00 50 46

01 10 45  J0102+58     21 28 44  44.4  36.2 -3.6    -103.5   545     1669   01 10 45
01 16 45  ---          21 34 45  45.2  35.9 -3.5    -105.0   360     1762   01 10 46

 ---------- POINTING ----------

01 26 45  3C84         21 44 46  23.8  54.4 -5.6     -69.3   547     1762   01 26 45
01 36 45  ---          21 54 48  25.6  55.1 -5.4     -70.7   600     1917   01 26 46

01 37 30  3C84         21 55 33  25.7  55.2 -5.4     -70.8    39     1917   01 37 30
01 47 30  ---          22 05 35  27.5  55.8 -5.3     -72.2   600     2071   01 37 31

01 50 00  NRAO150      22 08 05  24.4  43.6 -5.9     -70.8   133     2071   01 50 00
01 56 00  ---          22 14 06  25.3  44.0 -5.8     -71.8   360     2164   01 50 01

01 58 30  3C84         22 16 36  29.5  56.5 -5.1     -73.7   133     2164   01 58 30
02 08 30  ---          22 26 38  31.3  57.1 -4.9     -75.1   600     2319   01 58 31

02 09 15  3C84         22 27 23  31.4  57.2 -4.9     -75.2    39     2319   02 09 15
02 19 15  ---          22 37 25  33.2  57.7 -4.7     -76.5   600     2473   02 09 16

02 22 35  J0102+58     22 40 45  53.0  30.5 -2.4    -123.1   154     2473   02 22 35
02 28 35  ---          22 46 46  53.7  29.8 -2.3    -125.0   360     2566   02 22 36

 ---------- POINTING ----------

02 36 55  3C84         22 55 08  36.5  58.6 -4.4     -79.0   455     2566   02 36 55
02 46 55  ---          23 05 09  38.3  59.0 -4.3     -80.4   600     2721   02 36 56

02 47 40  3C84         23 05 55  38.5  59.0 -4.3     -80.5    39     2721   02 47 40
02 57 40  ---          23 15 56  40.3  59.4 -4.1     -81.9   600     2875   02 47 41

03 00 10  NRAO150      23 18 27  35.1  46.5 -4.7     -83.0   131     2875   03 00 10
03 06 10  ---          23 24 28  36.1  46.7 -4.6     -84.1   360     2968   03 00 11
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   9 Nov 2021   Day 313 ---

03 07 50  3C84         23 26 08  42.2  59.7 -3.9     -83.4    80     2968   03 07 50
03 17 50  ---          23 36 10  44.1  60.0 -3.8     -84.9   600     3123   03 07 51

03 18 35  3C84         23 36 55  44.2  60.0 -3.7     -85.0    39     3123   03 18 35
03 28 35  ---          23 46 56  46.1  60.2 -3.6     -86.5   600     3277   03 18 36

03 31 55  J0102+58     23 50 17  59.4  19.0 -1.2    -147.6   163     3277   03 31 55
03 37 55  ---          23 56 18  59.8  17.6 -1.1    -150.1   360     3370   03 31 56

 ---------- POINTING ----------

03 47 55  3C84         00 06 19  49.7  60.4 -3.2     -89.6   562     3370   03 47 55
03 57 55  ---          00 16 21  51.6  60.3 -3.1     -91.3   600     3524   03 47 56

03 58 40  3C84         00 17 06  51.7  60.3 -3.1     -91.4    39     3524   03 58 40
04 08 40  ---          00 27 08  53.6  60.2 -2.9     -93.2   600     3679   03 58 41

04 10 20  NRAO150      00 28 48  46.2  46.5 -3.5     -96.7    77     3679   04 10 20
04 16 20  ---          00 34 49  47.1  46.4 -3.4     -98.0   360     3772   04 10 21

 ---------- preempt no ----------

04 17 40  3C84         00 36 09  55.3  60.0 -2.8     -94.8    56     3772   04 17 40
04 27 40  ---          00 46 11  57.1  59.7 -2.6     -96.8   600     3926   04 17 41

04 28 25  3C84         00 46 56  57.3  59.6 -2.6     -96.9    39     3926   04 28 25
04 38 25  ---          00 56 58  59.1  59.1 -2.4     -99.0   600     4081   04 28 26

04 42 35  J0102+58     01 01 08  62.1   0.8 -0.0    -178.6   201     4081   04 42 35
04 48 35  ---          01 07 09  62.1  -0.9  0.1     178.6   360     4174   04 42 36

 ---------- POINTING ----------

04 56 55  3C84         01 15 31  62.5  57.8 -2.1    -103.3   450     4174   04 56 55
05 06 55  ---          01 25 32  64.4  56.7 -1.9    -105.9   600     4328   04 56 56

05 07 40  3C84         01 26 18  64.5  56.6 -1.9    -106.1    39     4328   05 07 40
05 17 40  ---          01 36 19  66.3  55.3 -1.7    -109.0   600     4483   05 07 41

05 19 20  NRAO150      01 37 59  56.6  42.0 -2.4    -113.8    73     4483   05 19 20
05 25 20  ---          01 44 00  57.5  41.2 -2.3    -115.6   360     4576   05 19 21

05 27 50  3C84         01 46 31  68.1  53.5 -1.6    -112.3   122     4576   05 27 50
05 37 50  ---          01 56 33  69.8  51.4 -1.4    -116.0   600     4730   05 27 51
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   9 Nov 2021   Day 313 ---

05 38 35  3C84         01 57 18  69.9  51.2 -1.4    -116.3    39     4730   05 38 35
05 48 35  ---          02 07 19  71.5  48.5 -1.2    -120.5   600     4885   05 38 36

05 51 55  J0102+58     02 10 40  59.9 -17.3  1.1     150.6   146     4885   05 51 55
05 57 55  ---          02 16 41  59.5 -18.7  1.2     148.1   360     4978   05 51 56

 ---------- POINTING ----------

06 02 55  3C84         02 21 42  73.8  43.5 -1.0    -127.7   247     4978   06 02 55
06 12 55  ---          02 31 43  75.2  38.9 -0.8    -133.8   600     5132   06 02 56

06 13 40  3C84         02 32 28  75.3  38.5 -0.8    -134.3    39     5132   06 13 40
06 23 40  ---          02 42 30  76.6  32.8 -0.6    -141.5   600     5287   06 13 41

06 25 20  NRAO150      02 44 10  65.1  29.5 -1.3    -137.6    69     5287   06 25 20
06 31 20  ---          02 50 11  65.7  27.8 -1.2    -140.4   360     5379   06 25 21

06 33 00  3C84         02 51 52  77.6  26.3 -0.5    -149.3    69     5379   06 33 00
06 43 00  ---          03 01 53  78.4  18.3 -0.3    -158.9   600     5534   06 33 01

06 43 45  3C84         03 02 38  78.4  17.6 -0.3    -159.6    39     5534   06 43 45
06 53 45  ---          03 12 40  78.9   8.4 -0.1    -170.3   600     5689   06 43 46

06 55 25  NRAO150      03 14 20  67.8  19.8 -0.8    -152.4    70     5689   06 55 25
07 01 25  ---          03 20 21  68.2  17.5 -0.7    -155.7   360     5781   06 55 26

 ---------- POINTING ----------

07 08 05  3C84         03 27 02  79.0  -5.7  0.1     173.5   371     5781   07 08 05
07 18 05  ---          03 37 04  78.6 -15.1  0.3     162.6   600     5936   07 08 06

07 18 50  3C84         03 37 49  78.5 -15.8  0.3     161.8    39     5936   07 18 50
07 28 50  ---          03 47 51  77.8 -24.2  0.4     151.9   600     6091   07 18 51

07 32 10  NRAO150      03 51 11  69.5   4.5 -0.2    -173.9   171     6091   07 32 10
07 38 10  ---          03 57 12  69.6   1.8 -0.1    -177.6   360     6183   07 32 11

07 39 50  3C84         03 58 53  76.7 -32.1  0.6     142.4    69     6183   07 39 50
07 49 50  ---          04 08 54  75.4 -37.9  0.8     135.0   600     6338   07 39 51

 ---------- Segment (D). VLBA (0800-0830) ----------

08 00 00  3C84         04 19 06  74.0 -42.7  1.0     128.7   604     6338   08 00 00
08 10 00  ---          04 29 08  72.5 -46.6  1.1     123.3   600     6492   08 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   9 Nov 2021   Day 313 ---

08 10 45  3C84         04 29 53  72.4 -46.8  1.1     123.0    39     6492   08 10 45
08 20 45  ---          04 39 54  70.8 -49.9  1.3     118.4   600     6647   08 10 46

 ---------- Segment (E). VLBA+KVN (0830-1530) ----------

08 30 00  NRAO150      04 49 11  67.7 -20.2  0.8     151.8   524     6647   08 30 00
08 36 00  ---          04 55 12  67.3 -22.4  0.9     148.6   360     6740   08 30 01

08 40 00  3C84         04 59 12  67.5 -54.1  1.6     111.2   210     6740   08 40 00
08 50 00  ---          05 09 14  65.7 -55.7  1.8     108.1   600     6894   08 40 01

08 51 10  3C84         05 10 24  65.5 -55.9  1.8     107.8    64     6894   08 51 10
09 01 10  ---          05 20 26  63.7 -57.1  2.0     105.0   600     7049   08 51 11

09 02 20  J0102+58     05 21 36  39.0 -37.3  4.3      93.8    13     7049   09 02 20
09 08 20  ---          05 27 37  38.2 -37.3  4.4      92.5   360     7142   09 02 21

09 09 30  3C84         05 28 47  62.2 -57.9  2.1     102.9    15     7142   09 09 30
09 19 30  ---          05 38 49  60.4 -58.7  2.3     100.5   600     7296   09 09 31

09 20 40  3C84         05 39 59  60.2 -58.8  2.3     100.3    64     7296   09 20 40
09 30 40  ---          05 50 01  58.3 -59.4  2.5      98.1   600     7451   09 20 41

09 31 50  NRAO150      05 51 11  61.2 -37.1  1.8     124.5    46     7451   09 31 50
09 37 50  ---          05 57 12  60.4 -38.1  1.9     122.4   360     7544   09 31 51

09 39 00  3C84         05 58 22  56.8 -59.7  2.6      96.4    47     7544   09 39 00
09 49 00  ---          06 08 24  54.9 -60.1  2.8      94.5   600     7698   09 39 01

09 50 10  3C84         06 09 34  54.7 -60.1  2.8      94.2    64     7698   09 50 10
10 00 10  ---          06 19 36  52.8 -60.3  3.0      92.4   600     7853   09 50 11

10 01 20  J0102+58     06 20 46  31.3 -36.9  5.3      81.4    20     7853   10 01 20
10 07 20  ---          06 26 47  30.5 -36.7  5.4      80.2   360     7946   10 01 21

10 08 30  3C84         06 27 57  51.2 -60.4  3.1      91.0    21     7946   10 08 30
10 18 30  ---          06 37 59  49.4 -60.4  3.3      89.3   600     8100   10 08 31

10 19 40  3C84         06 39 09  49.2 -60.4  3.3      89.1    64     8100   10 19 40
10 29 40  ---          06 49 10  47.3 -60.3  3.5      87.5   600     8255   10 19 41

10 30 50  NRAO150      06 50 21  52.8 -44.4  2.8     106.7    51     8255   10 30 50
10 36 50  ---          06 56 22  51.9 -44.9  2.9     105.2   360     8347   10 30 51
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   9 Nov 2021   Day 313 ---

10 38 00  3C84         06 57 32  45.7 -60.2  3.6      86.2    50     8347   10 38 00
10 48 00  ---          07 07 33  43.8 -59.9  3.8      84.7   600     8502   10 38 01

10 49 10  3C84         07 08 44  43.6 -59.9  3.8      84.5    64     8502   10 49 10
10 59 10  ---          07 18 45  41.8 -59.6  4.0      83.1   600     8657   10 49 11

11 00 20  J0102+58     07 19 55  23.8 -34.7  6.3      69.7    27     8657   11 00 20
11 06 20  ---          07 25 56  23.1 -34.4  6.4      68.6   360     8749   11 00 21

11 07 30  3C84         07 27 07  40.2 -59.4  4.1      81.8    28     8749   11 07 30
11 17 30  ---          07 37 08  38.4 -59.0  4.3      80.4   600     8904   11 07 31

11 18 40  3C84         07 38 19  38.1 -58.9  4.3      80.3    64     8904   11 18 40
11 28 40  ---          07 48 20  36.3 -58.5  4.5      78.9   600     9059   11 18 41

11 29 50  NRAO150      07 49 30  43.6 -46.9  3.8      93.4    47     9059   11 29 50
11 35 50  ---          07 55 31  42.7 -46.9  3.9      92.2   360     9151   11 29 51

11 37 00  3C84         07 56 42  34.8 -58.1  4.6      77.7    47     9151   11 37 00
11 47 00  ---          08 06 43  32.9 -57.6  4.8      76.3   600     9306   11 37 01

11 48 10  3C84         08 07 53  32.7 -57.6  4.8      76.1    64     9306   11 48 10
11 58 10  ---          08 17 55  30.9 -57.0  4.9      74.8   600     9460   11 48 11

11 59 20  J0102+58     08 19 05  16.9 -31.1  7.2      58.4    34     9460   11 59 20
12 05 20  ---          08 25 06  16.2 -30.7  7.3      57.2   360     9553   11 59 21

12 06 30  3C84         08 26 16  29.4 -56.5  5.1      73.6    36     9553   12 06 30
12 16 30  ---          08 36 18  27.6 -55.9  5.3      72.3   600     9708   12 06 31

12 17 40  3C84         08 37 28  27.4 -55.8  5.3      72.1    64     9708   12 17 40
12 27 40  ---          08 47 30  25.6 -55.1  5.4      70.7   600     9862   12 17 41

12 28 50  NRAO150      08 48 40  34.4 -46.4  4.8      82.2    45     9862   12 28 50
12 34 50  ---          08 54 41  33.4 -46.2  4.9      81.1   360     9955   12 28 51

12 36 00  3C84         08 55 51  24.2 -54.6  5.6      69.6    44     9955   12 36 00
12 46 00  ---          09 05 53  22.4 -53.8  5.7      68.2   600    10110   12 36 01

12 47 10  3C84         09 07 03  22.2 -53.7  5.8      68.1    64    10110   12 47 10
12 57 10  ---          09 17 05  20.5 -53.0  5.9      66.7   600    10264   12 47 11

12 58 20  J0102+58     09 18 15  10.7 -26.3  8.2      46.9    43    10264   12 58 20
13 04 20  ---          09 24 16  10.2 -25.7  8.3      45.7   360    10357   12 58 21
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue   9 Nov 2021   Day 313 ---

13 05 30  3C84         09 25 26  19.1 -52.3  6.1      65.5    43    10357   13 05 30
13 15 30  ---          09 35 28  17.4 -51.5  6.2      64.1   600    10512   13 05 31

13 16 40  3C84         09 36 38  17.2 -51.4  6.3      64.0    64    10512   13 16 40
13 26 40  ---          09 46 40  15.5 -50.5  6.4      62.5   600    10666   13 16 41

13 27 50  NRAO150      09 47 50  25.3 -44.0  5.8      71.8    42    10666   13 27 50
13 33 50  ---          09 53 51  24.4 -43.7  5.9      70.8   360    10759   13 27 51

13 35 00  3C84         09 55 01  14.1 -49.7  6.6      61.4    42    10759   13 35 00
13 45 00  ---          10 05 03  12.5 -48.8  6.7      59.9   600    10914   13 35 01

13 46 10  3C84         10 06 13  12.3 -48.7  6.7      59.7    64    10914   13 46 10
13 56 10  ---          10 16 14  10.7 -47.7  6.9      58.3   600    11068   13 46 11

14 26 50  NRAO150      10 46 59  16.8 -40.1  6.8      61.7  1811    11068   14 26 50
14 32 50  ---          10 53 00  15.9 -39.6  6.9      60.7   360    11161   14 26 51

14 34 30  0716+714     10 54 41  40.6 -19.6  3.5     115.9    43    11161   14 34 30
14 44 30  ---          11 04 42  39.8 -20.0  3.7     113.2   600    11315   14 34 31

14 45 40  0716+714     11 05 53  39.7 -20.1  3.7     112.9    64    11315   14 45 40
14 55 40  ---          11 15 54  39.0 -20.5  3.9     110.3   600    11470   14 45 41

14 56 50  0716+714     11 17 04  38.9 -20.5  3.9     110.0    64    11470   14 56 50
15 06 50  ---          11 27 06  38.2 -20.8  4.0     107.4   600    11625   14 56 51

15 08 00  0716+714     11 28 16  38.1 -20.9  4.1     107.1    64    11625   15 08 00
15 18 00  ---          11 38 18  37.3 -21.1  4.2     104.6   600    11779   15 08 01

15 19 10  0716+714     11 39 28  37.2 -21.2  4.3     104.3    64    11779   15 19 10
15 30 00  ---          11 50 20  36.3 -21.4  4.4     101.6   650    11947   15 19 11


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess321K2Gglob.setini
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    4         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         D         B         D         B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  17  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22140.00  22140.00  22204.00  22204.00  22268.00  22268.00  22332.00  22332.00
   BBC fr=     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     727.99    727.99    791.99    791.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  17  18  19  20  21  22  23  24  25  26

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J0102+5824        00 59 43.470972   * 01 02 45.762380     01 04 06.438676       0.19
   0059+581          58 08 04.84744    * 58 24 11.13659      58 31 19.64003        0.10
 * J0102+58          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
                     rfc_2012b Petrov, 2012, unpublished 288749 observations

   J0319+4130        03 16 29.567260   * 03 19 48.160090     03 21 15.535667       1.30
   0316+413          41 19 51.91699    * 41 30 42.10412      41 35 25.91632        2.72
 * 3C84              /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
   J0319+41          GSFC 2011B astro solution      9957 Observations

   J0359+5057        03 55 45.261370   * 03 59 29.747271     04 01 08.622013       0.16
   0355+508          50 49 20.28582    * 50 57 50.16177      51 01 29.66951        0.10
   J0359+50          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
 * NRAO150           rfc_2012b Petrov, 2012, unpublished 18568 observations

   J0721+7120        07 16 13.029741   * 07 21 53.448476     07 24 21.470878       0.31
 * 0716+714          71 26 15.17406    * 71 20 36.36340      71 17 52.44207        0.10
   J0721+71          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
                     rfc_2012b Petrov, 2012, unpublished 27599 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J0102+58   sess321K2Gglob.setini 1 2 3 4 6 9 10 13 14 15 17        1.867   217.500
  3C84       sess321K2Gglob.setini 1 2 3 4 6 9 10 13 14 15 17       14.250  1564.083
  NRAO150    sess321K2Gglob.setini 1 2 3 4 6 9 10 13 14 15 17        2.300   272.100
  0716+714   sess321K2Gglob.setini 17                                2.314    60.125


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J0102+58           133.4
   3C84               154.8
   NRAO150            143.6
   0716+714           113.4

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

