  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The true nature of the jet base in 3C84
 Exp. Code:  GP058B  


Schedule Version:      10.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Georgios Filippos Paraschos

Address:  Max-Planck-Institute for Radiostronomy
          Auf dem Huegel, 69
          Bonn, NRW, 53121
          Germany

Phone:    +49228525292
EMAIL:    gfparaschos@mpifr-bonn.mpg.de
Fax:
Phone during observation: +492257301155

Observing mode:

Notes:    PHASECAL should be ON
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed  10 Nov 2021   Day 314 ---

 Next scan frequencies:  43040.00  43040.00  43104.00  43104.00  43168.00  43168.00  43232.00  43232.00
 Next BBC frequencies:     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

22 32 01  0716+714     18 57 27  12.0  -2.2 11.6       5.9     0        0   22 32 01
22 38 01  ---          19 03 28  12.0  -1.7 11.7       4.6   360       93   22 32 02

22 39 01  0716+714     19 04 28  12.0  -1.6 11.7       4.4    54       93   22 39 01
22 45 01  ---          19 10 29  12.0  -1.1 11.8       3.1   360      185   22 39 02

22 46 01  0716+714     19 11 29  12.0  -1.1 11.8       2.8    54      185   22 46 01
22 52 01  ---          19 17 30  11.9  -0.6 11.9       1.5   360      278   22 46 02

23 00 01  0716+714     19 25 31  11.9   0.1-12.0      -0.3   474      278   23 00 01
23 06 01  ---          19 31 32  11.9   0.6-11.9      -1.6   360      371   23 00 02

23 07 41  0716+714     19 33 13  11.9   0.7-11.9      -1.9    94      371   23 07 41
23 13 41  ---          19 39 14  12.0   1.2-11.8      -3.3   360      464   23 07 42

23 15 21  0716+714     19 40 54  12.0   1.4-11.7      -3.6    94      464   23 15 21
23 21 21  ---          19 46 55  12.0   1.8-11.6      -5.0   360      556   23 15 22

23 23 01  0716+714     19 48 35  12.0   2.0-11.6      -5.3    94      556   23 23 01
23 29 01  ---          19 54 36  12.1   2.5-11.5      -6.6   360      649   23 23 02

23 30 41  0716+714     19 56 16  12.1   2.6-11.5      -7.0    94      649   23 30 41
23 36 41  ---          20 02 17  12.2   3.1-11.4      -8.3   360      742   23 30 42

23 38 21  0716+714     20 03 58  12.2   3.2-11.3      -8.7    94      742   23 38 21
23 44 21  ---          20 09 59  12.3   3.7-11.2     -10.0   360      835   23 38 22

23 46 01  0716+714     20 11 39  12.3   3.9-11.2     -10.4    94      835   23 46 01
23 52 01  ---          20 17 40  12.4   4.3-11.1     -11.7   360      927   23 46 02

23 53 41  0716+714     20 19 20  12.4   4.5-11.1     -12.1    94      927   23 53 41
23 59 41  ---          20 25 21  12.5   5.0-11.0     -13.4   360     1020   23 53 42

 --- Thu  11 Nov 2021   Day 315 ---

00 01 21  0716+714     20 27 01  12.5   5.1-11.0     -13.8    94     1020   00 01 21
00 07 21  ---          20 33 02  12.7   5.6-10.9     -15.1   360     1113   00 01 22

00 09 01  0716+714     20 34 43  12.7   5.7-10.8     -15.5    94     1113   00 09 01
00 15 01  ---          20 40 44  12.8   6.2-10.7     -16.8   360     1206   00 09 02
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

00 16 41  0716+714     20 42 24  12.9   6.3-10.7     -17.1    94     1206   00 16 41
00 22 41  ---          20 48 25  13.0   6.8-10.6     -18.5   360     1298   00 16 42

00 24 21  0716+714     20 50 05  13.1   6.9-10.6     -18.8    94     1298   00 24 21
00 30 21  ---          20 56 06  13.2   7.4-10.5     -20.1   360     1391   00 24 22

00 32 01  0716+714     20 57 46  13.3   7.5-10.4     -20.5    94     1391   00 32 01
00 38 01  ---          21 03 47  13.4   8.0-10.3     -21.8   360     1484   00 32 02

 ---------- POINTING ----------

00 40 00  3C84         21 05 47  17.1  51.3 -6.3     -63.9    80     1484   00 40 00
00 46 40  ---          21 12 28  18.3  51.9 -6.1     -64.9   400     1587   00 40 01

00 47 25  3C84         21 13 13  18.4  52.0 -6.1     -65.0    39     1587   00 47 25
00 54 05  ---          21 19 54  19.5  52.5 -6.0     -65.9   400     1690   00 47 26

00 54 50  3C84         21 20 39  19.7  52.6 -6.0     -66.0    39     1690   00 54 50
01 01 30  ---          21 27 20  20.8  53.1 -5.9     -67.0   400     1793   00 54 51

01 04 50  J0102+58     21 30 41  44.6  36.1 -3.6    -104.0   146     1793   01 04 50
01 10 50  ---          21 36 42  45.4  35.8 -3.5    -105.5   360     1886   01 04 51

 ---------- POINTING ----------

01 19 10  3C84         21 45 03  23.9  54.4 -5.6     -69.4   447     1886   01 19 10
01 25 50  ---          21 51 44  25.1  54.9 -5.5     -70.3   400     1989   01 19 11

01 26 35  3C84         21 52 29  25.2  55.0 -5.5     -70.4    39     1989   01 26 35
01 33 15  ---          21 59 10  26.4  55.4 -5.4     -71.3   400     2092   01 26 36

01 34 00  3C84         21 59 56  26.5  55.5 -5.4     -71.4    39     2092   01 34 00
01 40 40  ---          22 06 37  27.7  55.9 -5.2     -72.3   400     2195   01 34 01

01 43 10  NRAO150      22 09 07  24.5  43.7 -5.9     -70.9   133     2195   01 43 10
01 49 10  ---          22 15 08  25.4  44.0 -5.8     -72.0   360     2288   01 43 11

 ---------- POINTING ----------

01 56 40  3C84         22 22 39  30.6  56.9 -5.0     -74.5   433     2288   01 56 40
02 03 20  ---          22 29 20  31.8  57.3 -4.9     -75.4   400     2391   01 56 41

02 04 05  3C84         22 30 06  31.9  57.3 -4.9     -75.5    39     2391   02 04 05
02 10 45  ---          22 36 47  33.1  57.7 -4.7     -76.4   400     2494   02 04 06
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

02 11 30  3C84         22 37 32  33.3  57.7 -4.7     -76.5    39     2494   02 11 30
02 18 10  ---          22 44 13  34.5  58.1 -4.6     -77.5   400     2597   02 11 31

02 21 30  J0102+58     22 47 33  53.8  29.7 -2.3    -125.3   155     2597   02 21 30
02 27 30  ---          22 53 34  54.4  28.9 -2.2    -127.2   360     2690   02 21 31

 ---------- POINTING ----------

02 35 50  3C84         23 01 56  37.7  58.9 -4.3     -79.9   456     2690   02 35 50
02 42 30  ---          23 08 37  39.0  59.1 -4.2     -80.9   400     2793   02 35 51

02 43 15  3C84         23 09 22  39.1  59.1 -4.2     -81.0    39     2793   02 43 15
02 49 55  ---          23 16 03  40.3  59.4 -4.1     -81.9   400     2896   02 43 16

02 50 40  3C84         23 16 48  40.5  59.4 -4.1     -82.1    39     2896   02 50 40
02 57 20  ---          23 23 29  41.7  59.6 -4.0     -83.0   400     2999   02 50 41

02 59 50  NRAO150      23 26 00  36.3  46.7 -4.6     -84.4   131     2999   02 59 50
03 05 50  ---          23 32 01  37.2  46.8 -4.5     -85.5   360     3092   02 59 51

 ---------- POINTING ----------

03 12 30  3C84         23 38 42  44.5  60.0 -3.7     -85.3   380     3092   03 12 30
03 19 10  ---          23 45 23  45.8  60.2 -3.6     -86.3   400     3195   03 12 31

03 19 55  3C84         23 46 08  45.9  60.2 -3.6     -86.4    39     3195   03 19 55
03 26 35  ---          23 52 49  47.2  60.3 -3.5     -87.4   400     3298   03 19 56

03 27 20  3C84         23 53 34  47.3  60.3 -3.5     -87.6    39     3298   03 27 20
03 34 00  ---          00 00 15  48.6  60.3 -3.4     -88.6   400     3401   03 27 21

03 37 20  J0102+58     00 03 36  60.3  15.9 -1.0    -153.1   161     3401   03 37 20
03 43 20  ---          00 09 37  60.6  14.5 -0.9    -155.6   360     3494   03 37 21

 ---------- POINTING ----------

03 51 40  3C84         00 17 58  51.9  60.3 -3.1     -91.6   459     3494   03 51 40
03 58 20  ---          00 24 39  53.1  60.3 -2.9     -92.7   400     3597   03 51 41

03 59 05  3C84         00 25 24  53.3  60.2 -2.9     -92.9    39     3597   03 59 05
04 05 45  ---          00 32 06  54.5  60.1 -2.8     -94.1   400     3700   03 59 06

04 06 30  3C84         00 32 51  54.7  60.1 -2.8     -94.2    39     3700   04 06 30
04 13 10  ---          00 39 32  55.9  59.9 -2.7     -95.5   400     3803   04 06 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

04 14 50  NRAO150      00 41 12  48.1  46.1 -3.3     -99.4    76     3803   04 14 50
04 20 50  ---          00 47 13  49.0  45.9 -3.2    -100.8   360     3895   04 14 51

 ---------- POINTING & preempt no ----------

04 27 30  3C84         00 53 54  58.6  59.3 -2.5     -98.4   375     3895   04 27 30
04 34 10  ---          01 00 35  59.8  58.9 -2.3     -99.8   400     3999   04 27 31

04 34 55  3C84         01 01 20  59.9  58.9 -2.3    -100.0    39     3999   04 34 55
04 41 35  ---          01 08 01  61.2  58.4 -2.2    -101.5   400     4102   04 34 56

04 42 20  3C84         01 08 47  61.3  58.3 -2.2    -101.7    39     4102   04 42 20
04 49 00  ---          01 15 28  62.5  57.8 -2.1    -103.3   400     4205   04 42 21

04 53 10  J0102+58     01 19 38  62.0  -4.3  0.3     172.9   199     4205   04 53 10
04 59 10  ---          01 25 39  61.9  -6.0  0.4     170.1   360     4297   04 53 11

 ---------- POINTING ----------

05 07 30  3C84         01 34 01  65.9  55.6 -1.8    -108.3   448     4297   05 07 30
05 14 10  ---          01 40 42  67.0  54.6 -1.7    -110.4   400     4400   05 07 31

05 14 55  3C84         01 41 27  67.2  54.4 -1.7    -110.6    39     4400   05 14 55
05 21 35  ---          01 48 08  68.3  53.2 -1.6    -112.9   400     4504   05 14 56

05 22 20  3C84         01 48 53  68.5  53.1 -1.5    -113.1    39     4504   05 22 20
05 29 00  ---          01 55 34  69.6  51.6 -1.4    -115.6   400     4607   05 22 21

05 30 40  NRAO150      01 57 14  59.3  39.4 -2.1    -119.7    71     4607   05 30 40
05 36 40  ---          02 03 15  60.1  38.4 -2.0    -121.7   360     4699   05 30 41

 ---------- POINTING ----------

05 44 10  3C84         02 10 47  72.1  47.4 -1.2    -122.1   421     4699   05 44 10
05 50 50  ---          02 17 28  73.1  45.1 -1.1    -125.4   400     4802   05 44 11

05 51 35  3C84         02 18 13  73.3  44.8 -1.1    -125.8    39     4802   05 51 35
05 58 15  ---          02 24 54  74.2  42.1 -0.9    -129.5   400     4905   05 51 36

05 59 00  3C84         02 25 39  74.3  41.8 -0.9    -130.0    39     4905   05 59 00
06 05 40  ---          02 32 20  75.3  38.6 -0.8    -134.2   400     5008   05 59 01

06 09 00  J0102+58     02 35 41  58.0 -22.6  1.5     140.8   149     5008   06 09 00
06 15 00  ---          02 41 42  57.5 -23.7  1.6     138.5   360     5101   06 09 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

 ---------- POINTING ----------

06 22 30  3C84         02 49 13  77.3  28.3 -0.5    -147.0   402     5101   06 22 30
06 29 10  ---          02 55 54  77.9  23.2 -0.4    -153.0   400     5204   06 22 31

06 29 55  3C84         02 56 39  78.0  22.6 -0.4    -153.7    39     5204   06 29 55
06 36 35  ---          03 03 20  78.5  17.0 -0.3    -160.4   400     5307   06 29 56

06 37 20  3C84         03 04 05  78.5  16.3 -0.3    -161.1    39     5307   06 37 20
06 44 00  ---          03 10 46  78.8  10.2 -0.2    -168.3   400     5410   06 37 21

06 45 40  NRAO150      03 12 27  67.7  20.5 -0.8    -151.4    70     5410   06 45 40
06 51 40  ---          03 18 28  68.1  18.2 -0.7    -154.7   360     5503   06 45 41

 ---------- POINTING ----------

06 58 20  3C84         03 25 09  79.0  -3.8  0.1     175.6   371     5503   06 58 20
07 05 00  ---          03 31 50  78.8 -10.3  0.2     168.2   400     5606   06 58 21

07 05 45  3C84         03 32 35  78.8 -11.0  0.2     167.3    39     5606   07 05 45
07 12 25  ---          03 39 16  78.5 -17.1  0.3     160.3   400     5709   07 05 46

07 13 10  3C84         03 40 01  78.4 -17.7  0.3     159.5    39     5709   07 13 10
07 19 50  ---          03 46 42  77.9 -23.3  0.4     152.9   400     5812   07 13 11

07 21 30  NRAO150      03 48 23  69.5   5.7 -0.2    -172.1    71     5812   07 21 30
07 27 30  ---          03 54 24  69.6   3.0 -0.1    -175.8   360     5905   07 21 31

 ---------- POINTING ----------

07 34 10  3C84         04 01 05  76.4 -33.4  0.7     140.7   369     5905   07 34 10
07 40 50  ---          04 07 46  75.6 -37.3  0.8     135.8   400     6008   07 34 11

07 41 35  3C84         04 08 31  75.5 -37.7  0.8     135.3    39     6008   07 41 35
07 48 15  ---          04 15 12  74.6 -41.0  0.9     131.0   400     6111   07 41 36

07 49 00  3C84         04 15 57  74.5 -41.4  0.9     130.5    39     6111   07 49 00
07 55 40  ---          04 22 38  73.5 -44.2  1.0     126.7   400     6214   07 49 01

 ---------- Segment (D). VLBA (0800-0830) ----------

08 00 00  3C84         04 26 59  72.8 -45.8  1.1     124.4   254     6214   08 00 00
08 06 40  ---          04 33 40  71.8 -48.0  1.2     121.2   400     6317   08 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

08 07 25  3C84         04 34 25  71.7 -48.3  1.2     120.8    39     6317   08 07 25
08 14 05  ---          04 41 06  70.6 -50.2  1.3     117.9   400     6420   08 07 26

08 14 50  3C84         04 41 51  70.5 -50.4  1.3     117.6    39     6420   08 14 50
08 21 30  ---          04 48 33  69.3 -52.0  1.5     115.0   400     6523   08 14 51

08 22 15  3C84         04 49 18  69.2 -52.1  1.5     114.7    39     6523   08 22 15
08 28 55  ---          04 55 59  68.1 -53.5  1.6     112.3   400     6626   08 22 16

 ---------- Segment (E). VLBA+KVN (0830-1530) ----------

08 31 00  NRAO150      04 58 04  67.0 -23.3  0.9     147.2    95     6626   08 31 00
08 37 00  ---          05 04 05  66.5 -25.3  1.0     144.2   360     6719   08 31 01

08 40 00  3C84         05 07 06  66.1 -55.4  1.8     108.8   151     6719   08 40 00
08 46 40  ---          05 13 47  64.9 -56.3  1.9     106.8   400     6822   08 40 01

08 47 50  3C84         05 14 57  64.7 -56.5  1.9     106.5    64     6822   08 47 50
08 54 30  ---          05 21 38  63.5 -57.2  2.0     104.7   400     6925   08 47 51

08 55 40  3C84         05 22 48  63.3 -57.4  2.0     104.4    64     6925   08 55 40
09 02 20  ---          05 29 29  62.1 -58.0  2.1     102.7   400     7028   08 55 41

09 03 30  J0102+58     05 30 39  37.8 -37.3  4.4      91.8    14     7028   09 03 30
09 09 30  ---          05 36 40  37.0 -37.4  4.5      90.5   360     7121   09 03 31

09 10 40  3C84         05 37 51  60.6 -58.6  2.3     100.7    16     7121   09 10 40
09 17 20  ---          05 44 32  59.3 -59.1  2.4      99.3   400     7224   09 10 41

09 18 30  3C84         05 45 42  59.1 -59.2  2.4      99.0    64     7224   09 18 30
09 25 10  ---          05 52 23  57.9 -59.5  2.5      97.6   400     7327   09 18 31

09 26 20  3C84         05 53 33  57.7 -59.5  2.5      97.4    64     7327   09 26 20
09 33 00  ---          06 00 14  56.4 -59.8  2.6      96.0   400     7430   09 26 21

09 34 10  NRAO150      06 01 24  59.8 -38.8  2.0     120.9    47     7430   09 34 10
09 40 10  ---          06 07 25  59.0 -39.8  2.1     119.0   360     7523   09 34 11

09 41 20  3C84         06 08 36  54.9 -60.1  2.8      94.4    48     7523   09 41 20
09 48 00  ---          06 15 17  53.6 -60.2  2.9      93.2   400     7626   09 41 21

09 49 10  3C84         06 16 27  53.4 -60.2  2.9      93.0    64     7626   09 49 10
09 55 50  ---          06 23 08  52.1 -60.3  3.0      91.8   400     7729   09 49 11
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

09 57 00  3C84         06 24 18  51.9 -60.3  3.1      91.6    64     7729   09 57 00
10 03 40  ---          06 30 59  50.7 -60.4  3.2      90.5   400     7832   09 57 01

10 04 50  J0102+58     06 32 09  29.8 -36.6  5.5      79.1    21     7832   10 04 50
10 10 50  ---          06 38 10  29.0 -36.4  5.6      77.9   360     7925   10 04 51

10 12 00  3C84         06 39 21  49.1 -60.4  3.3      89.1    22     7925   10 12 00
10 18 40  ---          06 46 02  47.9 -60.3  3.4      88.0   400     8028   10 12 01

10 19 50  3C84         06 47 12  47.6 -60.3  3.4      87.8    64     8028   10 19 50
10 26 30  ---          06 53 53  46.4 -60.2  3.5      86.8   400     8131   10 19 51

10 27 40  3C84         06 55 03  46.2 -60.2  3.6      86.6    64     8131   10 27 40
10 34 20  ---          07 01 44  44.9 -60.1  3.7      85.6   400     8234   10 27 41

10 35 30  NRAO150      07 02 55  50.9 -45.3  3.0     103.6    50     8234   10 35 30
10 41 30  ---          07 08 56  50.0 -45.6  3.1     102.2   360     8327   10 35 31

10 42 40  3C84         07 10 06  43.4 -59.9  3.8      84.3    49     8327   10 42 40
10 49 20  ---          07 16 47  42.1 -59.7  3.9      83.3   400     8430   10 42 41

10 50 30  3C84         07 17 57  41.9 -59.7  3.9      83.2    64     8430   10 50 30
10 57 10  ---          07 24 38  40.7 -59.5  4.1      82.2   400     8533   10 50 31

10 58 20  3C84         07 25 48  40.5 -59.4  4.1      82.0    64     8533   10 58 20
11 05 00  ---          07 32 29  39.2 -59.2  4.2      81.1   400     8636   10 58 21

11 06 10  J0102+58     07 33 40  22.1 -34.0  6.5      67.1    28     8636   11 06 10
11 12 10  ---          07 39 41  21.4 -33.7  6.6      65.9   360     8729   11 06 11

11 13 20  3C84         07 40 51  37.7 -58.8  4.3      79.9    30     8729   11 13 20
11 20 00  ---          07 47 32  36.5 -58.6  4.4      79.0   400     8832   11 13 21

11 21 10  3C84         07 48 42  36.2 -58.5  4.5      78.8    64     8832   11 21 10
11 27 50  ---          07 55 23  35.0 -58.2  4.6      77.9   400     8935   11 21 11

11 29 00  3C84         07 56 33  34.8 -58.1  4.6      77.7    64     8935   11 29 00
11 35 40  ---          08 03 14  33.6 -57.8  4.7      76.8   400     9038   11 29 01

11 36 50  NRAO150      08 04 25  41.3 -47.0  4.1      90.4    47     9038   11 36 50
11 42 50  ---          08 10 26  40.4 -47.0  4.2      89.3   360     9131   11 36 51

11 44 00  3C84         08 11 36  32.1 -57.4  4.8      75.6    46     9131   11 44 00
11 50 40  ---          08 18 17  30.9 -57.0  5.0      74.7   400     9234   11 44 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

11 51 50  3C84         08 19 27  30.6 -56.9  5.0      74.6    64     9234   11 51 50
11 58 30  ---          08 26 08  29.4 -56.5  5.1      73.7   400     9337   11 51 51

11 59 40  3C84         08 27 18  29.2 -56.5  5.1      73.5    64     9337   11 59 40
12 06 20  ---          08 33 59  28.0 -56.0  5.2      72.6   400     9440   11 59 41

12 07 30  J0102+58     08 35 10  15.1 -29.9  7.5      55.3    37     9440   12 07 30
12 13 30  ---          08 41 11  14.5 -29.4  7.6      54.1   360     9533   12 07 31

12 14 40  3C84         08 42 21  26.6 -55.5  5.4      71.4    38     9533   12 14 40
12 21 20  ---          08 49 02  25.4 -55.0  5.5      70.5   400     9636   12 14 41

12 22 30  3C84         08 50 12  25.2 -55.0  5.5      70.4    64     9636   12 22 30
12 29 10  ---          08 56 53  24.0 -54.5  5.6      69.5   400     9739   12 22 31

12 30 20  3C84         08 58 03  23.8 -54.4  5.6      69.3    64     9739   12 30 20
12 37 00  ---          09 04 44  22.6 -53.9  5.7      68.4   400     9842   12 30 21

12 38 10  NRAO150      09 05 55  31.7 -45.9  5.1      79.1    44     9842   12 38 10
12 44 10  ---          09 11 56  30.8 -45.7  5.2      78.0   360     9935   12 38 11

12 45 20  3C84         09 13 06  21.2 -53.3  5.9      67.2    43     9935   12 45 20
12 52 00  ---          09 19 47  20.0 -52.8  6.0      66.3   400    10038   12 45 21

12 53 10  3C84         09 20 57  19.8 -52.7  6.0      66.2    64    10038   12 53 10
12 59 50  ---          09 27 38  18.7 -52.1  6.1      65.2   400    10141   12 53 11

13 01 00  3C84         09 28 48  18.5 -52.0  6.1      65.1    64    10141   13 01 00
13 07 40  ---          09 35 30  17.4 -51.5  6.2      64.1   400    10244   13 01 01

13 16 00  3C84         09 43 51  16.0 -50.7  6.4      62.9   494    10244   13 16 00
13 22 40  ---          09 50 32  14.8 -50.1  6.5      62.0   400    10347   13 16 01

13 23 50  3C84         09 51 42  14.7 -50.0  6.5      61.8    64    10347   13 23 50
13 30 30  ---          09 58 23  13.6 -49.4  6.6      60.9   400    10450   13 23 51

13 31 40  3C84         09 59 33  13.4 -49.3  6.6      60.7    64    10450   13 31 40
13 38 20  ---          10 06 15  12.3 -48.7  6.7      59.7   400    10553   13 31 41

13 39 30  NRAO150      10 07 25  22.4 -42.9  6.1      68.5    42    10553   13 39 30
13 45 30  ---          10 13 26  21.5 -42.5  6.2      67.5   360    10646   13 39 31

13 47 01  NRAO150      10 14 57  21.3 -42.4  6.2      67.2    85    10646   13 47 01
13 53 01  ---          10 20 58  20.5 -42.0  6.3      66.2   360    10738   13 47 02
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               The true nature of the jet base in 3C84
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Thu  11 Nov 2021   Day 315 ---

13 54 31  0716+714     10 22 28  42.8 -17.8  3.0     124.7    38    10738   13 54 31
14 00 31  ---          10 28 29  42.4 -18.2  3.1     123.0   360    10831   13 54 32

14 01 01  0716+714     10 28 59  42.4 -18.2  3.1     122.9    24    10831   14 01 01
14 07 01  ---          10 35 00  41.9 -18.6  3.2     121.2   360    10924   14 01 02

14 07 31  0716+714     10 35 30  41.9 -18.6  3.2     121.1    24    10924   14 07 31
14 13 31  ---          10 41 31  41.5 -18.9  3.3     119.4   360    11017   14 07 32

14 15 01  NRAO150      10 43 02  17.3 -40.4  6.7      62.4    35    11017   14 15 01
14 21 01  ---          10 49 03  16.5 -39.9  6.8      61.4   360    11109   14 15 02

14 22 31  0716+714     10 50 33  40.9 -19.4  3.4     117.0    34    11109   14 22 31
14 28 31  ---          10 56 34  40.4 -19.7  3.5     115.4   360    11202   14 22 32

14 29 01  0716+714     10 57 04  40.4 -19.7  3.5     115.3    24    11202   14 29 01
14 35 01  ---          11 03 05  40.0 -20.0  3.6     113.7   360    11295   14 29 02

14 35 31  0716+714     11 03 35  39.9 -20.0  3.7     113.5    24    11295   14 35 31
14 41 31  ---          11 09 36  39.5 -20.2  3.8     112.0   360    11388   14 35 32

14 43 01  NRAO150      11 11 06  13.5 -38.1  7.2      57.6    31    11388   14 43 01
14 49 01  ---          11 17 07  12.7 -37.6  7.3      56.5   360    11480   14 43 02

14 50 31  0716+714     11 18 37  38.8 -20.6  3.9     109.6    31    11480   14 50 31
14 56 31  ---          11 24 38  38.3 -20.7  4.0     108.1   360    11573   14 50 32

14 57 01  0716+714     11 25 08  38.3 -20.8  4.0     107.9    24    11573   14 57 01
15 03 01  ---          11 31 09  37.8 -20.9  4.1     106.4   360    11666   14 57 02

15 03 31  0716+714     11 31 40  37.8 -21.0  4.1     106.3    24    11666   15 03 31
15 09 31  ---          11 37 41  37.3 -21.1  4.2     104.8   360    11759   15 03 32

15 18 31  0716+714     11 46 42  36.6 -21.3  4.4     102.5   534    11759   15 18 31
15 24 31  ---          11 52 43  36.2 -21.5  4.5     101.0   360    11851   15 18 32

15 25 01  0716+714     11 53 13  36.1 -21.5  4.5     100.9    24    11851   15 25 01
15 30 00  ---          11 58 13  35.7 -21.6  4.6      99.6   299    11928   15 25 02


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess321Q2Gglob.setini
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v7mm_c8

   Setup group:    4         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   8  Setup file default.  Used with PCAL = 1MHz
   LO sum=   43040.00  43040.00  43104.00  43104.00  43168.00  43168.00  43232.00  43232.00
   BBC fr=     640.00    640.00    704.00    704.00    768.00    768.00    832.00    832.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     727.99    727.99    791.99    791.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   8   9  10  11  12  13  14  15  16  17

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

   J0102+5824        00 59 43.470972   * 01 02 45.762380     01 04 06.429509       0.19
   0059+581          58 08 04.84744    * 58 24 11.13659      58 31 20.25312        0.10
 * J0102+58          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
                     rfc_2012b Petrov, 2012, unpublished 288749 observations

   J0319+4130        03 16 29.567260   * 03 19 48.160090     03 21 15.580901       1.30
   0316+413          41 19 51.91699    * 41 30 42.10412      41 35 26.37875        2.72
 * 3C84              /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
   J0319+41          GSFC 2011B astro solution      9957 Observations

   J0359+5057        03 55 45.261370   * 03 59 29.747271     04 01 08.686030       0.16
   0355+508          50 49 20.28582    * 50 57 50.16177      51 01 30.19335        0.10
   J0359+50          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
 * NRAO150           rfc_2012b Petrov, 2012, unpublished 18568 observations

   J0721+7120        07 16 13.029741   * 07 21 53.448476     07 24 21.674661       0.31
 * 0716+714          71 26 15.17406    * 71 20 36.36340      71 17 52.60644        0.10
   J0721+71          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.vlba.2012jul
                     rfc_2012b Petrov, 2012, unpublished 27599 observations



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J0102+58   sess321Q2Gglob.setini 1 2 3 6 7 8                       1.700    87.200
  3C84       sess321Q2Gglob.setini 1 2 3 6 7 8                      13.667   679.778
  NRAO150    sess321Q2Gglob.setini 1 2 3 6 7 8                       2.600   125.200
  0716+714   sess321Q2Gglob.setini 8                                 2.683    72.737


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J0102+58           133.2
   3C84               155.6
   NRAO150            144.7
   0716+714           114.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

