  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Improving the K-band celestial reference frame for the next multi-waveba
 Exp. Code:  GC040A  


Schedule Version:       1.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       P. Charlot

Address:  Laboratoire d'Astrophysique de Bordeaux
          Universite de Bordeaux - Bat. B18N
          Allee Geoffroy Saint-Hilaire, CS 50023
          33615 Pessac Cedex - France

Phone:    +33 540003284
EMAIL:    patrick.charlot@u-bordeaux.fr
Fax:
Phone during observation:

Observing mode: vlbi

Notes:    Phase cal should be on
          System temperatures should be measured
          Pointing gaps of 8 min for Effelsberg every 2 hours
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   2 Nov 2024   Day 307 ---

 Next scan frequencies:  22012.00  22076.00  22140.00  22204.00  22268.00  22332.00  22396.00  22460.00
 Next BBC frequencies:     512.00    576.00    640.00    704.00    768.00    832.00    896.00    960.00
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

20 30 00  1904+013     16 24 38  41.5 118.9 -2.7     -48.9     0        0   20 30 00
20 34 37  ---          16 29 16  42.4 120.0 -2.7     -48.2   277       71   20 30 01

20 36 12  1803+784     16 30 51  41.2   5.7 -1.5    -154.5     6       71   20 36 12
20 38 01  ---          16 32 40  41.2   5.6 -1.4    -155.0   109       99   20 36 13

20 38 34  1849+670     16 33 13  48.3  19.1 -2.3    -133.7    11       99   20 38 34
20 39 51  ---          16 34 30  48.4  18.9 -2.2    -134.1    77      119   20 38 35

20 40 16  1749+701     16 34 56  49.2   9.4 -1.2    -155.5    10      119   20 40 16
20 42 27  ---          16 37 07  49.3   9.2 -1.2    -156.2   131      153   20 40 17

20 43 45  1215+303     16 38 25  34.9 -72.8  4.3      71.6    12      153   20 43 45
20 44 47  ---          16 39 27  34.6 -72.7  4.3      71.6    62      169   20 43 46

20 48 52  3C274        16 43 33  29.4 267.1  4.2      61.6    -5      169   20 48 57
20 50 06  ---          16 44 47  29.2 267.2  4.2      61.6    69      187   20 48 53

20 50 30  1208+186     16 45 11  27.6 275.8  4.5      64.3    10      187   20 50 30
20 52 16  ---          16 46 58  27.2 276.0  4.6      64.3   106      214   20 50 31

20 53 19  4C39.25      16 48 01   5.3 312.7  7.3      54.4    12      214   20 53 19
20 54 26  ---          16 49 08   5.2 312.8  7.3      54.2    67      231   20 53 20

20 55 26  1128+385     16 50 08  26.0 300.6  5.3      70.2    11      231   20 55 26
20 56 37  ---          16 51 19  25.8 300.7  5.3      70.1    71      250   20 55 27

20 57 37  3C309.1      16 52 19  46.3 347.5  1.9     143.8    12      250   20 57 37
20 58 43  ---          16 53 26  46.2 347.4  1.9     143.5    66      267   20 57 38

20 59 14  1352+757     16 53 57  40.2 346.5  3.0     127.0    11      267   20 59 14
21 00 15  ---          16 54 58  40.2 346.4  3.0     126.8    61      282   20 59 15

21 01 19  1637+574     16 56 02  63.2 354.8  0.3     171.7    11      282   21 01 19
21 03 05  ---          16 57 48  63.1 354.3  0.3     170.9   106      310   21 01 20

21 04 49  1509+022     16 59 33  51.9 226.3  1.8      38.5     5      310   21 04 49
21 05 55  ---          17 00 39  51.7 226.7  1.8      38.8    66      327   21 04 50

21 06 32  1510-089     17 01 16  42.6 217.2  1.8      31.8    11      327   21 06 32
21 10 32  ---          17 05 17  42.1 218.3  1.9      32.7   240      389   21 06 33
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   2 Nov 2024   Day 307 ---

21 12 09  1435+638     17 06 54  49.6 335.3  2.5     126.3     6      389   21 12 09
21 14 44  ---          17 09 29  49.3 335.0  2.5     125.6   155      428   21 12 10

21 15 39  1140+668     17 10 24  31.3 332.4  5.4      84.3    11      428   21 15 39
21 16 55  ---          17 11 41  31.1 332.5  5.4      84.0    76      448   21 15 40

21 17 23  1227+587     17 12 09  35.9 322.5  4.7      88.6    10      448   21 17 23
21 19 00  ---          17 13 46  35.7 322.5  4.7      88.3    97      473   21 17 24

21 20 33  1514-241     17 15 19  28.3 210.1  1.9      28.3     5      473   21 20 33
21 22 40  ---          17 17 27  28.0 210.6  2.0      28.8   127      506   21 20 34

21 23 50  1855+031     17 18 37  53.8 134.1 -1.7     -38.2     8      506   21 23 50
21 26 12  ---          17 20 59  54.1 134.9 -1.6     -37.6   142      542   21 23 51

21 27 00  1949-052     17 21 47  39.2 128.0 -2.5     -42.9    10      542   21 27 00
21 28 23  ---          17 23 10  39.4 128.3 -2.5     -42.7    83      564   21 27 01

21 29 03  1825-214     17 23 51  35.6 161.0 -1.1     -17.5     9      564   21 29 03
21 30 04  ---          17 24 52  35.7 161.3 -1.1     -17.2    61      579   21 29 04

21 31 32  1325+126     17 26 20  32.5 265.1  4.0      61.3     6      579   21 31 32
21 32 52  ---          17 27 40  32.2 265.3  4.0      61.4    80      600   21 31 33

21 33 23  1351-018     17 28 11  29.7 247.1  3.5      52.5    10      600   21 33 23
21 34 59  ---          17 29 48  29.4 247.4  3.6      52.6    96      625   21 33 24

21 36 35  0346+800     17 31 24  21.6 364.1-10.5     -21.3     5      625   21 36 35
21 37 50  ---          17 32 39  21.6 364.2-10.4     -21.6    75      644   21 36 36

21 41 24  2008+355     17 36 14  57.5 430.4 -2.6     -87.8   136      644   21 41 24
21 42 36  ---          17 37 26  57.7 430.4 -2.6     -88.0    72      663   21 41 25

21 43 01  1951+355     17 37 51  61.1 430.7 -2.3     -90.2    10      663   21 43 01
21 44 13  ---          17 39 03  61.4 430.7 -2.3     -90.4    72      681   21 43 02

21 45 55  1144+402     17 40 45  20.4 305.1  5.9      66.5     5      681   21 45 55
21 46 55  ---          17 41 46  20.2 305.1  5.9      66.4    60      697   21 45 56

21 50 32  1334-127     17 45 23  16.5 243.3  4.1      52.1   165      697   21 50 32
21 52 56  ---          17 47 47  16.0 243.7  4.1      52.4   144      734   21 50 33

21 53 31  1222+037     17 48 23   9.8 268.1  5.4      59.5    10      734   21 53 31
21 55 47  ---          17 50 39   9.3 268.4  5.4      59.5   136      769   21 53 32
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   2 Nov 2024   Day 307 ---

21 57 52  2227-088     17 52 44  12.9 108.0 -4.6     -55.8     3      769   21 57 52
21 58 53  ---          17 53 45  13.1 108.2 -4.6     -55.7    61      785   21 57 53

22 01 09  1147+245     17 56 02  11.1 -68.4  6.1      61.3     2      785   22 01 09
22 03 07  ---          17 58 00  10.8 -68.2  6.1      61.1   118      815   22 01 10

22 05 15  2021+222     18 00 09  56.9  95.4 -2.4     -68.0     4      815   22 05 15
22 08 19  ---          18 03 13  57.5  95.9 -2.4     -67.9   184      862   22 05 16

22 09 02  2029+024     18 03 56  45.1 121.0 -2.5     -47.6    10      862   22 09 02
22 10 02  ---          18 04 56  45.3 121.3 -2.5     -47.4    60      878   22 09 03

22 11 02  2128-123     18 05 56  24.5 122.4 -3.4     -48.0    11      878   22 11 02
22 12 11  ---          18 07 06  24.7 122.6 -3.4     -47.8    69      896   22 11 03

22 12 44  2134+00      18 07 39  32.0 110.5 -3.5     -53.7    11      896   22 12 44
22 15 05  ---          18 10 00  32.5 111.0 -3.5     -53.5   141      932   22 12 45

22 16 47  0901+697     18 11 42  15.1 -14.7  9.0      38.5     5      932   22 16 47
22 18 47  ---          18 13 43  15.0 -14.6  9.1      38.0   120      963   22 16 48

22 19 31  0219+628     18 14 27  14.2  23.0 -8.2     -48.3     9      963   22 19 31
22 21 50  ---          18 16 46  14.4  23.2 -8.1     -48.8   139      999   22 19 32

22 24 31  1557+032     18 19 28  47.2 236.7  2.3      46.1     1      999   22 24 31
22 25 37  ---          18 20 34  47.0 237.0  2.3      46.3    66     1016   22 24 32

22 26 00  1546+027     18 20 57  44.8 239.0  2.5      47.6    11     1016   22 26 00
22 27 08  ---          18 22 05  44.5 239.3  2.5      47.8    68     1033   22 26 01

22 27 34  1532+016     18 22 31  41.0 241.6  2.8      49.2    11     1033   22 27 34
22 30 07  ---          18 25 05  40.5 242.1  2.8      49.5   153     1073   22 27 35

22 30 36  1502+106     18 25 34  39.5 257.5  3.3      58.7    10     1073   22 30 36
22 32 04  ---          18 27 02  39.2 257.8  3.4      58.7    88     1095   22 30 37

22 34 10  VR422201     18 29 08  46.1 419.0 -3.6     -87.3     3     1095   22 34 10
22 35 15  ---          18 30 13  46.3 419.0 -3.6     -87.5    65     1112   22 34 11

22 35 57  2309+454     18 30 56  34.4 412.7 -4.7     -79.6    11     1112   22 35 57
22 37 28  ---          18 32 27  34.7 412.8 -4.7     -79.9    91     1135   22 35 58

22 38 09  0044+566     18 33 08  23.4 396.2 -6.3     -69.3    11     1135   22 38 09
22 39 14  ---          18 34 13  23.5 396.2 -6.2     -69.5    65     1152   22 38 10
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   2 Nov 2024   Day 307 ---

22 39 34  0039+568     18 34 33  24.2 396.3 -6.2     -70.5    11     1152   22 39 34
22 40 42  ---          18 35 41  24.4 396.4 -6.1     -70.7    68     1170   22 39 35

22 41 08  0041+677     18 36 07  27.3 384.7 -6.2     -75.3    10     1170   22 41 08
22 42 17  ---          18 37 17  27.4 384.7 -6.2     -75.6    69     1187   22 41 09

22 43 36  2100+468     18 38 36  57.8 408.8 -2.4    -107.8    11     1187   22 43 36
22 45 16  ---          18 40 16  58.1 408.7 -2.4    -108.2   100     1213   22 43 37

22 45 40  2118+443     18 40 40  55.7 414.4 -2.7    -100.2    11     1213   22 45 40
22 46 58  ---          18 41 58  55.9 414.3 -2.7    -100.5    78     1233   22 45 41

22 47 19  2112+463     18 42 19  56.5 410.4 -2.6    -104.9    10     1233   22 47 19
22 52 19  ---          18 47 20  57.4 410.0 -2.5    -106.2   300     1311   22 47 20

22 53 57  1839+548     18 48 59  65.7 357.4  0.1     176.1    53     1311   22 53 57
22 55 09  ---          18 50 11  65.7 356.9  0.1     175.4    72     1329   22 53 58

22 56 43  2356+385     18 51 45  27.9 419.1 -5.2     -71.7    12     1329   22 56 43
22 58 50  ---          18 53 52  28.3 419.2 -5.1     -72.0   127     1362   22 56 44

23 00 00  0954+658     18 55 03  12.5 342.0  8.9      39.7     7     1362   23 00 00
23 05 00  ---          19 00 03  12.2 342.5  9.0      38.6   300     1439   23 00 01

23 07 42  2233-234     19 02 46  15.6 129.6 -3.6     -46.1     3     1439   23 07 42
23 08 52  ---          19 03 56  15.8 129.8 -3.6     -45.9    70     1457   23 07 43

23 10 49  2052+239     19 05 53  64.9  98.1 -1.8     -69.1    12     1457   23 10 49
23 11 50  ---          19 06 54  65.1  98.3 -1.8     -69.0    61     1473   23 10 50

23 14 53  M81          19 09 58  14.2 -14.3  9.2      36.4    75     1473   23 14 53
23 17 08  ---          19 12 13  14.1 -14.2  9.2      35.9   135     1508   23 14 54

23 17 32  0954+658     19 12 37  11.4 -16.5  9.2      36.0    11     1508   23 17 32
23 19 14  ---          19 14 20  11.3 -16.3  9.2      35.6   102     1534   23 17 33

23 21 00  NRAO530      19 16 06  39.9 213.0  1.7      28.8   -65     1534   23 22 05
23 22 07  ---          19 17 13  39.8 213.3  1.7      29.0     2     1534   23 21 01

23 22 30  1721-146     19 17 36  37.3 214.6  1.9      30.4    10     1534   23 22 30
23 24 39  ---          19 19 46  37.0 215.2  1.9      30.8   129     1568   23 22 31

23 25 06  1706-174     19 20 13  32.7 217.3  2.2      33.1    11     1568   23 25 06
23 27 12  ---          19 22 19  32.4 217.8  2.2      33.5   126     1600   23 25 07
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   2 Nov 2024   Day 307 ---

23 29 24  0344+558     19 24 31   7.9 387.0 -8.4     -44.4     4     1600   23 29 24
23 32 49  ---          19 27 57   8.3 387.4 -8.4     -45.1   205     1653   23 29 25

23 34 14  1417+273     19 29 22  23.8 288.4  5.1      66.4     7     1653   23 34 14
23 35 14  ---          19 30 22  23.5 288.5  5.2      66.3    60     1668   23 34 15

23 36 39  1657+265     19 31 48  56.6 272.4  2.5      73.8    12     1668   23 36 39
23 39 27  ---          19 34 36  56.0 272.7  2.6      73.7   168     1712   23 36 40

23 41 34  0017+257     19 36 43  28.4 434.8 -4.7     -67.7     4     1712   23 41 34
23 42 35  ---          19 37 45  28.6 434.9 -4.7     -67.8    61     1727   23 41 35

23 46 13  2255-282     19 41 23  14.8 135.9 -3.3     -42.6    -3     1727   23 46 16
23 47 45  ---          19 42 55  15.1 136.2 -3.3     -42.4    89     1750   23 46 14

23 49 34  2201+315     19 44 45  60.3  78.4 -2.3     -83.1    12     1750   23 49 34
23 51 56  ---          19 47 07  60.8  78.5 -2.3     -83.3   142     1787   23 49 35

23 53 37  0013-005     19 48 48  19.4 102.2 -4.5     -57.2    12     1787   23 53 37
23 55 09  ---          19 50 21  19.8 102.4 -4.5     -57.2    92     1811   23 53 38

23 55 32  0003-066     19 50 44  18.5 109.3 -4.3     -54.8    10     1811   23 55 32
23 56 57  ---          19 52 09  18.8 109.6 -4.3     -54.6    85     1833   23 55 33

23 57 27  0009-148     19 52 39  13.0 115.7 -4.3     -53.2    10     1833   23 57 27
23 58 33  ---          19 53 45  13.2 115.8 -4.3     -53.1    66     1850   23 57 28

 --- Start: Sat   2 Nov 2024   Day 307 -- Stop: Sun   3 Nov 2024   Day 308 ---

23 59 32  2037-253     19 54 44  33.2 167.3 -0.8     -12.1    12     1850   23 59 32
00 00 34  ---          19 55 46  33.3 167.6 -0.8     -11.8    62     1866   23 59 33

00 01 16  1830-211     19 56 29  34.8 203.3  1.4      21.3     9     1866   00 01 16
00 02 42  ---          19 57 55  34.6 203.6  1.4      21.7    86     1888   00 01 17

00 03 17  1741-038     19 58 30  43.1 228.6  2.2      40.3     9     1888   00 03 17
00 04 31  ---          19 59 44  42.9 228.9  2.2      40.6    74     1907   00 03 18

00 06 32  2146+608     20 01 45  54.7 382.1 -1.8    -137.8     4     1907   00 06 32
00 09 26  ---          20 04 40  54.9 381.6 -1.7    -138.8   174     1952   00 06 33

00 11 09  1743+173     20 06 23  55.6 255.4  2.3      60.7     5     1952   00 11 09
00 13 08  ---          20 08 23  55.2 255.8  2.4      60.9   119     1982   00 11 10
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

00 14 34  2126-158     20 09 49  39.9 154.3 -1.3     -22.8     6     1982   00 14 34
00 15 34  ---          20 10 49  40.0 154.6 -1.3     -22.5    60     1998   00 14 35

00 15 58  2112-144     20 11 13  42.5 158.3 -1.1     -19.2    11     1998   00 15 58
00 17 13  ---          20 12 28  42.6 158.6 -1.1     -18.9    75     2017   00 15 59

00 18 35  1722+119     20 13 50  47.0 253.4  2.8      57.4     7     2017   00 18 35
00 21 28  ---          20 16 44  46.4 254.0  2.8      57.7   173     2062   00 18 36

00 22 08  1821+107     20 17 24  57.3 238.7  1.9      48.4    11     2062   00 22 08
00 23 15  ---          20 18 31  57.1 239.0  1.9      48.7    67     2079   00 22 09

00 23 48  1749+096     20 19 04  50.0 246.2  2.4      53.0    11     2079   00 23 48
00 25 31  ---          20 20 48  49.7 246.6  2.5      53.2   103     2105   00 23 49

00 26 32  2008-159     20 21 49  43.6 183.0  0.2       2.7     8     2105   00 26 32
00 28 22  ---          20 23 39  43.6 183.7  0.2       3.3   110     2134   00 26 33

00 30 08  0251+393     20 25 25  13.6  51.8 -6.5     -61.3     4     2134   00 30 08
00 32 30  ---          20 27 48  14.0  52.0 -6.5     -61.7   142     2170   00 30 09

00 34 24  1921-293     20 29 42  28.3 195.7  1.1      15.5     4     2170   00 34 24
00 35 24  ---          20 30 42  28.2 195.9  1.1      15.7    60     2186   00 34 25

00 36 21  1937-101     20 31 39  47.6 198.6  0.8      16.2    11     2186   00 36 21
00 37 37  ---          20 32 56  47.5 199.0  0.9      16.5    76     2205   00 36 22

00 38 15  2033-219     20 33 34  37.7 178.6 -0.1      -1.3    11     2205   00 38 15
00 39 30  ---          20 34 49  37.7 179.0 -0.1      -0.9    75     2225   00 38 16

00 40 11  2149-306     20 35 30  26.3 161.3 -1.3     -18.7    11     2225   00 40 11
00 41 17  ---          20 36 36  26.3 161.5 -1.3     -18.4    66     2242   00 40 12

00 42 04  2208-137     20 37 23  40.4 148.9 -1.6     -27.2    11     2242   00 42 04
00 47 04  ---          20 42 24  40.9 150.3 -1.5     -25.9   300     2319   00 42 05

00 49 35  2123-463     20 44 56  12.7 172.3 -0.7      -9.5    87     2319   00 49 35
00 51 35  ---          20 46 56  12.8 172.7 -0.7      -9.1   120     2350   00 49 36

00 52 51  1655+077     20 48 12  32.0 259.2  3.8      58.5     7     2350   00 52 51
00 54 48  ---          20 50 09  31.6 259.5  3.8      58.6   117     2380   00 52 52

00 56 34  0415+572     20 51 56  14.7 391.0 -7.5     -55.3     5     2380   00 56 34
00 59 49  ---          20 55 11  15.0 391.2 -7.4     -56.0   195     2430   00 56 35
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

01 00 59  1637+574     20 56 21  39.0 321.2  4.3      92.7    12     2430   01 00 59
01 02 26  ---          20 57 49  38.8 321.1  4.3      92.4    87     2453   01 01 00

01 02 54  1642+690     20 58 17  37.7 335.9  4.3     102.2    10     2453   01 02 54
01 04 53  ---          21 00 16  37.5 335.8  4.3     101.7   119     2483   01 02 55

01 06 34  1914-154     21 01 57  37.8 212.2  1.7      28.4     5     2483   01 06 34
01 07 56  ---          21 03 20  37.6 212.6  1.8      28.7    82     2505   01 06 35

01 08 37  1825-214     21 04 01  26.2 220.3  2.6      36.7    11     2505   01 08 37
01 13 22  ---          21 08 46  25.5 221.3  2.6      37.5   285     2578   01 08 38

01 15 23  1849+670     21 10 48  47.9 340.4  2.4     132.0    28     2578   01 15 23
01 16 38  ---          21 12 03  47.8 340.3  2.4     131.6    75     2597   01 15 24

01 17 09  1749+701     21 12 34  41.5 339.3  3.4     116.6    11     2597   01 17 09
01 18 40  ---          21 14 05  41.4 339.2  3.4     116.2    91     2621   01 17 10

01 19 32  1352+757     21 14 57  24.7 344.9  7.4      62.6    11     2621   01 19 32
01 20 35  ---          21 16 01  24.6 345.0  7.4      62.4    63     2637   01 19 33

01 23 07  2357-318     21 18 33  17.0 144.5 -2.7     -35.8     1     2637   01 23 07
01 24 09  ---          21 19 35  17.1 144.7 -2.7     -35.6    62     2653   01 23 08

01 26 21  1459+480     21 21 48  19.0 314.9  6.3      65.1     3     2653   01 26 21
01 28 18  ---          21 23 45  18.8 315.0  6.4      64.7   117     2683   01 26 22

01 31 42  0418+532     21 27 09  16.4 396.9 -7.0     -60.3   138     2683   01 31 42
01 35 58  ---          21 31 26  16.9 397.3 -6.9     -61.1   256     2749   01 31 43

01 36 37  0615+820     21 32 05  24.9 366.2 -9.0     -42.3     9     2749   01 36 37
01 38 02  ---          21 33 30  24.9 366.3 -9.0     -42.6    85     2771   01 36 38

01 38 29  0346+800     21 33 58  29.1 371.1 -6.4     -78.2    11     2771   01 38 29
01 40 40  ---          21 36 09  29.2 371.2 -6.4     -78.7   131     2805   01 38 30

01 41 18  0444+634     21 36 47  19.5 386.5 -7.2     -59.8    11     2805   01 41 18
01 44 52  ---          21 40 22  19.8 386.8 -7.2     -60.5   214     2860   01 41 19

01 46 26  2351-154     21 41 56  34.1 140.0 -2.2  W  -35.0   -89     2860   01 47 55
01 47 37  ---          21 43 07  34.3 140.3 -2.2  W  -34.7     0     2855   01 46 27

01 48 31  2345+061     21 44 01  51.9 122.8 -2.1     -46.7    11     2855   01 48 31
01 50 12  ---          21 45 42  52.3 123.2 -2.1     -46.4   101     2881   01 48 32
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

01 51 48  1904+013     21 47 19  42.4 240.0  2.6      48.2     5     2881   01 51 48
01 53 15  ---          21 48 46  42.2 240.3  2.7      48.4    87     2904   01 51 49

01 54 11  1725+044     21 49 42  23.7 260.7  4.3      58.4    12     2904   01 54 11
01 55 46  ---          21 51 17  23.3 260.9  4.4      58.5    95     2928   01 54 12

01 57 27  1951+355     21 52 59  64.8 289.5  2.0      93.0    11     2928   01 57 27
01 58 28  ---          21 54 00  64.6 289.5  2.0      92.9    61     2944   01 57 28

01 59 42  1726+455     21 55 14  37.0 306.3  4.5      81.7    12     2944   01 59 42
02 01 20  ---          21 56 52  36.7 306.3  4.5      81.5    98     2969   01 59 43

02 02 35  0219+628     21 58 08  37.4 391.4 -4.5     -95.3     7     2969   02 02 35
02 04 54  ---          22 00 27  37.7 391.4 -4.4     -95.8   139     3005   02 02 36

02 06 49  1855+031     22 02 22  38.9 246.8  3.1      52.4     4     3005   02 06 49
02 08 11  ---          22 03 44  38.6 247.1  3.1      52.6    82     3026   02 06 50

02 08 56  3C395        22 04 30  51.7 284.2  3.0      79.8    11     3026   02 08 56
02 10 00  ---          22 05 34  51.5 284.2  3.0      79.7    64     3042   02 08 57

02 11 35  2233-148     22 07 09  44.3 169.6 -0.5      -9.3     5     3042   02 11 35
02 12 54  ---          22 08 28  44.4 170.0 -0.5      -8.9    79     3063   02 11 36

02 13 50  0111+021     22 09 24  38.0 113.4 -3.1     -52.2     8     3063   02 13 50
02 16 13  ---          22 11 48  38.4 113.9 -3.1     -51.9   143     3100   02 13 51

02 16 46  0202+149     22 12 21  34.7  92.0 -3.9     -63.1    10     3100   02 16 46
02 18 28  ---          22 14 03  35.0  92.3 -3.9     -63.1   102     3126   02 16 47

02 19 09  0213-026     22 14 44  23.7 108.1 -4.0     -54.9    11     3126   02 19 09
02 21 31  ---          22 17 07  24.2 108.5 -4.0     -54.8   142     3163   02 19 10

02 22 04  0235+164     22 17 40  29.2  87.0 -4.4     -63.8    10     3163   02 22 04
02 24 35  ---          22 20 11  29.7  87.3 -4.3     -63.8   151     3201   02 22 05

02 26 11  2356+385     22 21 47  68.1  60.8 -1.7    -104.8    13     3201   02 26 11
02 27 53  ---          22 23 30  68.4  60.6 -1.6    -105.3   102     3228   02 26 12

02 29 08  2105+551     22 24 45  61.7 -23.3  1.3     143.1     7     3228   02 29 08
02 30 34  ---          22 26 11  61.5 -23.7  1.3     142.5    86     3250   02 29 09

02 32 57  0002-478     22 28 34   8.9 163.6 -1.6     -21.0     2     3250   02 32 57
02 35 01  ---          22 30 39   9.0 164.0 -1.6     -20.6   124     3282   02 32 58
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

02 36 53  2216-038     22 32 31  55.8 185.5  0.2       4.7    12     3282   02 36 53
02 37 53  ---          22 33 31  55.7 185.9  0.2       5.1    60     3297   02 36 54

02 38 25  2134+00      22 34 03  57.3 206.7  0.9      22.7     9     3297   02 38 25
02 40 23  ---          22 36 02  57.1 207.5  1.0      23.4   118     3328   02 38 26

02 41 18  2021+222     22 36 57  59.4 262.6  2.2      67.4     8     3328   02 41 18
02 42 32  ---          22 38 11  59.1 262.8  2.2      67.5    74     3347   02 41 19

02 44 54  2319+317     22 40 33  80.8 437.4 -0.7     -97.0    10     3347   02 44 54
02 47 01  ---          22 42 41  81.2 437.1 -0.7     -97.7   127     3379   02 44 55

02 48 09  0039+568     22 43 49  56.3 389.1 -2.0    -129.3    11     3379   02 48 09
02 49 16  ---          22 44 56  56.4 388.9 -2.0    -129.6    67     3397   02 48 10

02 49 50  0041+677     22 45 30  48.5 376.4 -2.0    -139.1    11     3397   02 49 50
02 51 17  ---          22 46 58  48.6 376.3 -2.0    -139.6    87     3419   02 49 51

02 51 51  0044+566     22 47 32  56.3 389.5 -2.0    -128.7    11     3419   02 51 51
02 54 04  ---          22 49 45  56.5 389.2 -2.0    -129.5   133     3453   02 51 52

02 56 06  2233-234     22 51 47  36.2 184.0  0.2       3.7   -32     3453   02 56 38
03 01 06  ---          22 56 48  36.1 185.4  0.3       5.1   268     3522   02 56 07

03 10 06  3C418        23 05 50  56.0 318.3  2.4     113.4   437     3522   03 10 06
03 15 06  ---          23 10 50  55.3 317.8  2.5     112.0   300     3600   03 10 07

03 17 36  0446+112     23 13 21  10.6 443.0 -5.6     -60.6    53     3600   03 17 36
03 18 42  ---          23 14 27  10.9 443.1 -5.6     -60.6    66     3617   03 17 37

03 19 48  0350+465     23 15 33  34.8 411.7 -4.7     -80.4    11     3617   03 19 48
03 21 12  ---          23 16 57  35.1 411.7 -4.7     -80.7    84     3638   03 19 49

03 22 26  0642+449     23 18 12   7.2 401.3 -7.5     -53.2    11     3638   03 22 26
03 23 32  ---          23 19 18   7.4 401.4 -7.5     -53.4    66     3655   03 22 27

03 26 04  2149-306     23 21 50  25.5 201.1  1.5      21.0     2     3655   03 26 04
03 27 34  ---          23 23 20  25.4 201.4  1.5      21.4    90     3679   03 26 05

03 28 05  2037-253     23 23 52  22.1 219.5  2.7      37.2    10     3679   03 28 05
03 33 03  ---          23 28 50  21.4 220.5  2.8      38.0   298     3755   03 28 06

03 34 42  1657+265     23 30 30   7.2 296.5  6.5      59.3    37     3755   03 34 42
03 35 42  ---          23 31 30   7.1 296.6  6.5      59.2    60     3771   03 34 43
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

03 38 16  3C120        23 34 04  15.6  92.9 -5.0     -59.7     1     3771   03 38 16
03 39 34  ---          23 35 22  15.8  93.1 -5.0     -59.7    78     3791   03 38 17

03 41 30  2118+443     23 37 19  60.0 -52.5  2.3     106.2     4     3791   03 41 30
03 42 35  ---          23 38 24  59.8 -52.6  2.3     105.9    65     3808   03 41 31

03 43 20  2008+355     23 39 09  46.6 -68.7  3.5      81.3    11     3808   03 43 20
03 44 35  ---          23 40 24  46.4 -68.7  3.5      81.2    75     3827   03 43 21

03 45 24  2146+608     23 41 13  54.3 -22.8  1.9     136.1     8     3827   03 45 24
03 48 46  ---          23 44 36  54.0 -23.3  1.9     134.9   202     3879   03 45 25

03 50 30  M81          23 46 20  11.6   9.6-10.2     -23.7    12     3879   03 50 30
03 54 09  ---          23 50 00  11.7  10.0-10.1     -24.5   219     3935   03 50 31

03 54 46  1435+638     23 50 37   9.7 -17.5  9.2      35.5    10     3935   03 54 46
03 57 26  ---          23 53 17   9.6 -17.3  9.3      34.9   160     3977   03 54 47

03 57 57  1140+668     23 53 48   7.1   0.9-11.9      -1.9    10     3977   03 57 57
04 00 08  ---          23 56 00   7.1   1.1-11.8      -2.4   131     4010   03 57 58

04 02 36  0109+224     23 58 28  71.6 110.4 -1.2     -61.1    13     4010   04 02 36
04 03 54  ---          23 59 46  71.8 110.9 -1.2     -60.8    78     4030   04 02 37

04 04 41  0109+351     00 00 34  74.0  67.5 -1.2    -102.5     8     4030   04 04 41
04 06 08  ---          00 02 01  74.3  67.2 -1.2    -102.9    87     4053   04 04 42

04 07 08  0250+320     00 03 01  53.5  75.7 -2.9     -81.0    11     4053   04 07 08
04 08 31  ---          00 04 24  53.8  75.8 -2.8     -81.1    83     4074   04 07 09

04 08 58  0251+393     00 04 51  54.2  63.5 -2.9     -91.0    10     4074   04 08 58
04 12 47  ---          00 08 41  54.9  63.5 -2.8     -91.6   229     4133   04 08 59

04 14 03  0148-177     00 09 57  36.0 149.4 -1.7     -27.3     7     4133   04 14 03
04 15 03  ---          00 10 57  36.1 149.6 -1.7     -27.1    60     4149   04 14 04

04 15 43  2357-318     00 11 37  27.9 182.6  0.2       2.6     9     4149   04 15 43
04 17 48  ---          00 13 43  27.9 183.1  0.2       3.1   125     4181   04 15 44

04 18 30  2208-137     00 14 25  37.2 218.2  2.0      33.1     9     4181   04 18 30
04 19 40  ---          00 15 35  37.0 218.5  2.0      33.4    70     4199   04 18 31

04 20 11  2227-088     00 16 06  43.5 217.2  1.8      31.7    10     4199   04 20 11
04 21 43  ---          00 17 38  43.3 217.6  1.8      32.1    92     4223   04 20 12
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

04 22 33  2112-144     00 18 29  27.4 231.1  3.0      43.7    11     4223   04 22 33
04 25 01  ---          00 20 57  27.0 231.6  3.1      44.1   148     4261   04 22 34

04 26 56  0901+697     00 22 52  16.1 375.9 -8.8     -42.1     4     4261   04 26 56
04 31 56  ---          00 27 53  16.4 376.3 -8.7     -43.2   300     4338   04 26 57

04 33 06  1839+548     00 29 03  26.3 320.2  5.8      73.5    22     4338   04 33 06
04 37 22  ---          00 33 20  25.7 320.4  5.9      72.7   256     4404   04 33 07

04 38 09  1637+574     00 34 07  11.8 331.1  7.9      50.3    12     4404   04 38 09
04 39 27  ---          00 35 25  11.7 331.2  7.9      50.1    78     4424   04 38 10

04 40 00  1642+690     00 35 58  19.1 340.4  7.9      53.2    10     4424   04 40 00
04 41 48  ---          00 37 47  19.0 340.5  7.9      52.8   108     4452   04 40 01

04 42 42  0633+595     00 38 41  25.9 394.3 -6.0     -73.0     8     4452   04 42 42
04 43 47  ---          00 39 46  26.0 394.3 -6.0     -73.2    65     4469   04 42 43

04 46 53  0322-294     00 42 52  18.7 143.0 -2.7     -36.3    -1     4469   04 46 54
04 47 53  ---          00 43 53  18.8 143.2 -2.7     -36.2    59     4484   04 46 54

04 48 23  0414-189     00 44 23  18.8 126.7 -3.6     -46.8    10     4484   04 48 23
04 49 31  ---          00 45 31  19.0 126.9 -3.5     -46.7    68     4501   04 48 24

04 50 08  0502+049     00 46 08  23.9  98.7 -4.3     -58.6     9     4501   04 50 08
04 51 15  ---          00 47 15  24.1  98.8 -4.3     -58.6    67     4519   04 50 09

04 51 44  0507+179     00 47 44  29.4  85.5 -4.4     -64.4    11     4519   04 51 44
04 52 44  ---          00 48 44  29.6  85.6 -4.4     -64.5    60     4534   04 51 45

04 54 29  2320-035     00 50 30  50.5 215.0  1.4      29.6     5     4534   04 54 29
04 55 29  ---          00 51 30  50.4 215.3  1.4      29.9    60     4550   04 54 30

04 56 12  2243-123     00 52 13  37.9 219.9  2.1      34.3    10     4550   04 56 12
04 58 56  ---          00 54 57  37.5 220.6  2.1      34.9   164     4592   04 56 13

04 59 45  2029+024     00 55 47  22.2 259.5  4.4      57.9    11     4592   04 59 45
05 01 07  ---          00 57 09  21.9 259.7  4.4      57.9    82     4613   04 59 46

05 02 33  2211+374     00 58 35  55.7 293.3  2.7      89.6    11     4613   05 02 33
05 04 58  ---          01 01 00  55.3 293.3  2.8      89.2   145     4650   05 02 34

05 06 22  1039+811     01 02 25  22.9 365.6 -9.7     -31.4    12     4650   05 06 22
05 08 01  ---          01 04 04  22.9 365.6 -9.7     -31.8    99     4676   05 06 23
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

05 08 37  0615+820     01 04 40  31.5 369.3 -5.4     -93.5    11     4676   05 08 37
05 11 06  ---          01 07 09  31.5 369.3 -5.4     -94.2   149     4714   05 08 38

05 12 18  NRAO140      01 08 22  58.2 436.9 -2.5     -83.0    12     4714   05 12 18
05 14 05  ---          01 10 09  58.6 437.0 -2.5     -83.2   107     4742   05 12 19

05 14 44  3C119        01 10 48  48.1 420.2 -3.4     -88.3    10     4742   05 14 44
05 16 35  ---          01 12 39  48.4 420.2 -3.4     -88.6   111     4770   05 14 45

05 17 06  0454+550     01 13 10  43.3 401.1 -3.8     -97.4    10     4770   05 17 06
05 18 32  ---          01 14 37  43.5 401.1 -3.8     -97.8    86     4793   05 17 07

05 20 56  2255-282     01 17 01  22.9 212.8  2.3      31.9     2     4793   05 20 56
05 22 11  ---          01 18 16  22.8 213.1  2.3      32.1    75     4812   05 20 57

05 23 21  2201+315     01 19 26  48.6 284.8  3.3      78.4    11     4812   05 23 21
05 24 29  ---          01 20 35  48.4 284.9  3.3      78.3    68     4829   05 23 22

05 26 01  0415+572     01 22 07  49.3 395.6 -3.0    -111.6     5     4829   05 26 01
05 27 26  ---          01 23 32  49.5 395.4 -3.0    -112.0    85     4851   05 26 02

05 27 56  0444+634     01 24 02  43.8 389.0 -3.5    -110.1    11     4851   05 27 56
05 30 04  ---          01 26 11  44.0 388.9 -3.4    -110.7   128     4884   05 27 57

05 31 17  0804+499     01 27 24  16.6 401.5 -6.7     -61.9    11     4884   05 31 17
05 32 52  ---          01 28 59  16.8 401.6 -6.7     -62.1    95     4909   05 31 18

05 33 35  0628+203     01 29 42  22.1 438.7 -5.0     -64.1     9     4909   05 33 35
05 35 29  ---          01 31 36  22.5 438.9 -5.0     -64.2   114     4938   05 33 36

05 35 58  0600+177     01 32 06  27.4 444.8 -4.5     -64.1    11     4938   05 35 58
05 37 24  ---          01 33 32  27.7 444.9 -4.5     -64.1    86     4960   05 35 59

05 40 35  0104-408     01 36 43  18.6 185.8  0.5       6.5    -1     4960   05 40 36
05 43 34  ---          01 39 43  18.5 186.4  0.5       7.2   178     5006   05 40 36

05 45 10  3C395        01 41 19   8.7 302.2  6.6      59.2     6     5006   05 45 10
05 46 30  ---          01 42 39   8.5 302.3  6.6      59.0    80     5027   05 45 11

05 47 10  1951+355     01 43 19  19.3 300.7  5.8      65.6    10     5027   05 47 10
05 48 40  ---          01 44 50  19.1 300.9  5.8      65.4    90     5050   05 47 11

05 49 47  2149-306     01 45 57   7.7 227.7  3.9      47.5     7     5050   05 49 47
05 50 47  ---          01 46 57   7.6 227.9  3.9      47.7    60     5065   05 49 48
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

05 52 04  2351-154     01 48 14  36.9 214.7  1.9      30.5    11     5065   05 52 04
05 53 04  ---          01 49 14  36.8 214.9  1.9      30.7    60     5081   05 52 05

05 54 10  0111+021     01 50 21  60.7 198.2  0.6      15.6    11     5081   05 54 10
05 55 10  ---          01 51 21  60.6 198.7  0.6      16.1    60     5096   05 54 11

05 57 17  0748+126     01 53 28   6.6  79.4 -6.0     -60.0    13     5096   05 57 17
05 59 21  ---          01 55 32   7.0  79.6 -5.9     -60.1   124     5128   05 57 18

06 00 10  0520-165     01 56 22  21.4 125.8 -3.5     -46.6     8     5128   06 00 10
06 01 57  ---          01 58 09  21.7 126.2 -3.4     -46.4   107     5156   06 00 11

06 03 36  0219+628     01 59 48  57.1   5.3 -0.4    -169.8     5     5156   06 03 36
06 05 29  ---          02 01 41  57.2   4.9 -0.4    -170.5   113     5185   06 03 37

06 06 59  1849+670     02 03 12  21.3 -23.3  7.2      61.2    11     5185   06 06 59
06 08 46  ---          02 04 59  21.2 -23.2  7.3      60.8   107     5213   06 07 00

06 09 29  2105+551     02 05 42  33.3 -40.9  5.0      83.1    11     5213   06 09 29
06 11 15  ---          02 07 28  33.1 -40.8  5.0      82.7   106     5240   06 09 30

06 12 13  2309+454     02 08 27  52.9 -53.1  2.9      98.6    11     5240   06 12 13
06 14 03  ---          02 10 17  52.6 -53.2  3.0      98.2   110     5268   06 12 14

06 15 31  1749+701     02 11 45  17.9 -16.9  8.4      47.1    12     5268   06 15 31
06 16 54  ---          02 13 08  17.8 -16.8  8.4      46.8    83     5290   06 15 32

06 20 10  2216-038     02 16 25  24.2 249.9  3.9      54.0    -2     5290   06 20 12
06 21 33  ---          02 17 48  24.0 250.1  4.0      54.2    81     5310   06 20 11

06 22 26  2126-158     02 18 41   6.9 247.4  4.8      55.5    11     5310   06 22 26
06 23 26  ---          02 19 41   6.7 247.5  4.8      55.6    60     5326   06 22 27

06 24 00  2233-234     02 20 15  14.4 231.6  3.7      47.1    11     5326   06 24 00
06 27 27  ---          02 23 43  13.8 232.2  3.8      47.6   207     5379   06 24 01

06 28 23  2052+239     02 24 39  18.3 287.8  5.5      63.9     9     5379   06 28 23
06 30 11  ---          02 26 27  18.0 288.0  5.5      63.8   108     5407   06 28 24

06 31 51  2356+385     02 28 08  58.9 295.7  2.5      94.1    11     5407   06 31 51
06 33 17  ---          02 29 34  58.6 295.7  2.5      93.9    86     5429   06 31 52

06 34 01  0044+566     02 30 18  58.2 333.7  1.7     135.4     9     5429   06 34 01
06 35 27  ---          02 31 44  58.1 333.4  1.7     134.9    86     5451   06 34 02
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

06 36 03  0041+677     02 32 20  49.4 345.3  1.8     143.9    11     5451   06 36 03
06 37 59  ---          02 34 17  49.3 345.0  1.8     143.3   116     5481   06 36 04

06 39 24  1352+757     02 35 42  16.3 362.7-11.3      -9.4    12     5481   06 39 24
06 40 46  ---          02 37 04  16.3 362.8-11.3      -9.7    82     5502   06 39 25

06 41 13  3C309.1      02 37 31  12.3 358.3 11.6       4.8    11     5502   06 41 13
06 42 23  ---          02 38 41  12.3 358.3 11.7       4.5    70     5520   06 41 14

06 43 54  2319+317     02 40 13  48.3 285.5  3.3      78.6    12     5520   06 43 54
06 45 59  ---          02 42 18  47.9 285.6  3.3      78.4   125     5553   06 43 55

06 47 44  0529+483     02 44 03  53.2 408.8 -2.9    -102.9     9     5553   06 47 44
06 50 27  ---          02 46 47  53.6 408.6 -2.8    -103.6   163     5595   06 47 45

06 51 17  0350+465     02 47 37  69.1 394.5 -1.1    -134.6    12     5595   06 51 17
06 53 00  ---          02 49 20  69.3 393.9 -1.1    -135.4   103     5621   06 51 18

06 55 13  4C39.25      02 51 34  12.3 411.8 -6.6     -60.4    13     5621   06 55 13
06 56 25  ---          02 52 46  12.5 411.9 -6.6     -60.5    72     5640   06 55 14

06 56 59  0859+470     02 53 20  20.0 406.7 -6.2     -66.1    11     5640   06 56 59
06 59 27  ---          02 55 48  20.4 406.9 -6.1     -66.5   148     5678   06 57 00

07 00 00  0954+658     02 56 21  21.4 385.4 -7.1     -62.6    10     5678   07 00 00
07 05 00  ---          03 01 22  21.8 385.6 -7.0     -63.6   300     5755   07 00 01

07 09 39  VR422201     03 06 02  30.1 304.2  5.0      74.5   213     5755   07 09 39
07 14 39  ---          03 11 03  29.2 304.5  5.1      73.8   300     5832   07 09 40

07 15 11  2118+443     03 11 35  22.6 309.7  5.8      68.6    11     5832   07 15 11
07 16 11  ---          03 12 35  22.5 309.8  5.9      68.5    60     5848   07 15 12

07 16 34  2100+468     03 12 58  20.4 313.5  6.2      66.5    11     5848   07 16 34
07 17 40  ---          03 14 04  20.2 313.6  6.2      66.3    66     5865   07 16 35

07 18 02  2112+463     03 14 26  21.9 312.3  6.0      68.0    11     5865   07 18 02
07 19 04  ---          03 15 28  21.8 312.4  6.0      67.9    62     5881   07 18 03

07 21 28  0524+034     03 17 53  48.9 124.7 -2.2     -45.1     3     5881   07 21 28
07 22 43  ---          03 19 08  49.1 125.1 -2.2     -44.9    75     5900   07 21 29

07 24 23  2233-148     03 20 48   8.5 247.6  4.7      55.2     5     5900   07 24 23
07 26 31  ---          03 22 57   8.1 247.9  4.8      55.4   128     5933   07 24 24
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

07 27 29  0229-479     03 23 55  10.8 188.8  0.9      11.3     8     5933   07 27 29
07 31 25  ---          03 27 52  10.7 189.5  0.9      12.2   236     5994   07 27 30

07 33 01  VR422201     03 29 28  26.0 305.7  5.4      71.2     5     5994   07 33 01
07 34 10  ---          03 30 37  25.8 305.7  5.4      71.0    69     6012   07 33 02

07 35 57  0928+144     03 32 24   7.1 437.8 -6.0     -60.1     5     6012   07 35 57
07 36 58  ---          03 33 25   7.4 437.9 -6.0     -60.2    61     6027   07 35 58

07 40 14  0401-248     03 36 42  34.3 172.3 -0.5      -7.3    -1     6027   07 40 15
07 42 32  ---          03 39 00  34.4 172.9 -0.4      -6.7   137     6063   07 40 15

07 43 41  0823+033     03 40 10  17.2  96.8 -4.8     -58.8     7     6063   07 43 41
07 44 41  ---          03 41 10  17.5  96.9 -4.8     -58.8    60     6078   07 43 42

07 46 38  0003-066     03 43 07  26.6 244.0  3.6      51.1     4     6078   07 46 38
07 48 16  ---          03 44 45  26.3 244.3  3.6      51.2    98     6103   07 46 39

07 50 30  0850+284     03 47 00  24.3  70.5 -5.1     -66.9     2     6103   07 50 30
07 52 15  ---          03 48 45  24.7  70.7 -5.1     -67.0   105     6131   07 50 31

07 53 07  0746+483     03 49 37  41.4  50.8 -4.0     -88.1    11     6131   07 53 07
07 55 37  ---          03 52 08  41.8  50.8 -4.0     -88.5   150     6169   07 53 08

07 56 42  0344+558     03 53 13  64.6  -1.1  0.1     178.4    12     6169   07 56 42
07 58 35  ---          03 55 06  64.6  -1.7  0.1     177.4   113     6198   07 56 43

08 00 43  0454-234     03 57 14  34.1 163.1 -1.0     -15.8     3     6198   08 00 43
08 01 56  ---          03 58 28  34.1 163.4 -1.0     -15.5    73     6217   08 00 44

08 02 36  0402-362     03 59 08  23.3 178.7 -0.1      -1.3    11     6217   08 02 36
08 03 40  ---          04 00 12  23.3 179.0 -0.1      -1.1    64     6234   08 02 37

08 05 42  0901+697     04 02 14  33.2  24.1 -5.1     -90.5     4     6234   08 05 42
08 09 34  ---          04 06 07  33.5  24.1 -5.0     -91.4   232     6293   08 05 43

08 10 19  1803+784     04 06 52  20.3  -5.8 10.1      25.6    11     6293   08 10 19
08 12 55  ---          04 09 28  20.3  -5.6 10.2      25.0   156     6334   08 10 20

08 13 33  1140+668     04 10 06  19.2  22.8 -7.6     -56.5    10     6334   08 13 33
08 17 18  ---          04 13 52  19.5  23.0 -7.5     -57.3   225     6391   08 13 34

08 17 58  M81          04 14 32  29.9  24.4 -5.7     -81.8    12     6391   08 17 58
08 21 08  ---          04 17 43  30.2  24.5 -5.7     -82.5   190     6440   08 17 59
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

08 22 08  1642+690     04 18 43   9.6  -2.1 11.6       5.1    12     6440   08 22 08
08 24 04  ---          04 20 39   9.6  -1.9 11.6       4.7   116     6470   08 22 09

08 26 56  0213-026     04 23 32  45.4 228.3  2.1      40.0     0     6470   08 26 56
08 28 09  ---          04 24 45  45.2 228.6  2.1      40.2    73     6489   08 26 57

08 28 59  0148-177     04 25 35  29.4 222.8  2.6      37.8    11     6489   08 28 59
08 30 59  ---          04 27 35  29.1 223.2  2.6      38.1   120     6520   08 29 00

08 31 57  0017+257     04 28 33  36.1 281.7  4.1      69.9     9     6520   08 31 57
08 35 00  ---          04 31 37  35.4 282.0  4.2      69.7   183     6567   08 31 58

08 36 11  2320-035     04 32 48   9.5 260.6  5.1      58.2    12     6567   08 36 11
08 37 29  ---          04 34 06   9.2 260.7  5.2      58.3    78     6587   08 36 12

08 38 08  2345+061     04 34 45  19.5 266.1  4.7      59.8    11     6587   08 38 08
08 40 36  ---          04 37 14  18.9 266.4  4.8      59.8   148     6625   08 38 09

08 42 01  0202+149     04 38 39  52.0 255.1  2.5      59.6    12     6625   08 42 01
08 43 25  ---          04 40 03  51.7 255.3  2.6      59.7    84     6647   08 42 02

08 44 20  0358+040     04 40 59  62.2 200.8  0.6      17.9     8     6647   08 44 20
08 45 25  ---          04 42 04  62.1 201.4  0.7      18.3    65     6664   08 44 21

08 46 22  0528+134     04 43 01  69.5 143.7 -0.8     -31.6     8     6664   08 46 22
08 47 33  ---          04 44 12  69.6 144.4 -0.8     -31.0    71     6682   08 46 23

08 48 04  0507+179     04 44 43  76.0 152.7 -0.4     -24.5    10     6682   08 48 04
08 49 20  ---          04 45 59  76.1 153.8 -0.4     -23.5    76     6702   08 48 05

08 51 14  1039+811     04 47 54  30.2  10.7 -6.0     -84.9     4     6702   08 51 14
08 52 19  ---          04 48 59  30.3  10.7 -6.0     -85.1    65     6718   08 51 15

08 54 24  0537-441     04 51 04  14.5 171.0 -0.8     -10.8     3     6718   08 54 24
08 55 27  ---          04 52 07  14.5 171.2 -0.8     -10.5    63     6735   08 54 25

08 57 24  0633+595     04 54 05  56.0  23.9 -1.8    -136.5     4     6735   08 57 24
09 00 02  ---          04 56 43  56.3  23.5 -1.7    -137.4   158     6775   08 57 25

09 02 50  0009-148     04 59 32   7.8 248.1  4.8      55.5     0     6775   09 02 50
09 07 39  ---          05 04 21   6.8 248.7  4.9      55.9   289     6850   09 02 51

09 09 12  0346+800     05 05 55  39.9 356.3  1.1     161.1     9     6850   09 09 12
09 11 04  ---          05 07 47  39.9 356.2  1.1     160.6   112     6879   09 09 13
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

09 12 14  0418+532     05 08 57  65.8 343.8  0.7     156.3    11     6879   09 12 14
09 13 27  ---          05 10 10  65.7 343.4  0.8     155.6    73     6897   09 12 15

09 13 53  0415+572     05 10 36  61.9 345.9  0.8     157.1    10     6897   09 13 53
09 18 06  ---          05 14 50  61.6 344.8  0.9     155.3   253     6963   09 13 54

09 19 54  2146+608     05 16 38  17.0 332.2  7.5      56.6    12     6963   09 19 54
09 24 54  ---          05 21 39  16.5 332.5  7.5      55.6   300     7040   09 19 55

09 26 24  0111+021     05 23 09  25.2 257.2  4.1      57.1    28     7040   09 26 24
09 27 45  ---          05 24 31  24.9 257.4  4.2      57.2    81     7061   09 26 25

09 28 53  0235+164     05 25 39  49.9 259.4  2.8      62.0    11     7061   09 28 53
09 30 18  ---          05 27 04  49.6 259.7  2.8      62.1    85     7083   09 28 54

09 31 39  0444+634     05 28 25  56.5 352.6  0.6     165.6     7     7083   09 31 39
09 34 45  ---          05 31 32  56.5 352.0  0.7     164.4   186     7131   09 31 40

09 35 36  0642+449     05 32 23  69.4 401.1 -1.3    -127.1     8     7131   09 35 36
09 37 28  ---          05 34 15  69.7 400.5 -1.2    -128.0   112     7160   09 35 37

09 38 58  0109+351     05 35 45  35.9 293.9  4.4      75.1     6     7160   09 38 58
09 43 58  ---          05 40 46  34.9 294.2  4.5      74.6   300     7237   09 38 59

09 45 34  2105+551     05 42 23   6.6 333.6  8.6      42.5    32     7237   09 45 34
09 47 05  ---          05 43 54   6.4 333.7  8.6      42.2    91     7260   09 45 35

09 47 37  1849+670     05 44 26   8.5 353.7 10.9      14.0    10     7260   09 47 37
09 49 16  ---          05 46 05   8.5 353.9 10.9      13.7    99     7286   09 47 38

09 50 01  2309+454     05 46 50  16.1 314.2  6.6      62.4     9     7286   09 50 01
09 53 30  ---          05 50 20  15.6 314.5  6.6      61.8   209     7340   09 50 02

09 54 46  0219+628     05 51 36  44.1 330.6  3.4     110.2    12     7340   09 54 46
09 58 08  ---          05 54 59  43.7 330.4  3.5     109.4   202     7392   09 54 47

09 59 30  1435+638     05 56 21  12.0 380.4 -8.7     -42.2    11     7392   09 59 30
10 03 04  ---          05 59 55  12.3 380.7 -8.6     -42.9   214     7447   09 59 31

10 05 17  3C119        06 02 09  69.2 308.2  1.5     115.1    13     7447   10 05 17
10 06 59  ---          06 03 51  68.9 307.8  1.5     114.4   102     7473   10 05 18

10 08 32  0041+677     06 05 24  32.0 334.5  5.3      86.8    12     7473   10 08 32
10 10 09  ---          06 07 02  31.9 334.5  5.3      86.4    97     7498   10 08 33
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

10 10 36  0044+566     06 07 29  30.7 321.6  5.3      80.1    10     7498   10 10 36
10 12 31  ---          06 09 24  30.5 321.6  5.3      79.7   115     7528   10 10 37

10 13 28  0251+393     06 10 21  49.8 296.6  3.2      87.4    11     7528   10 13 28
10 16 04  ---          06 12 58  49.3 296.6  3.3      87.0   156     7568   10 13 29

10 17 14  0109+224     06 14 08  23.6 283.5  5.0      65.2    12     7568   10 17 14
10 19 33  ---          06 16 27  23.2 283.8  5.0      65.1   139     7604   10 17 15

10 21 16  0743-247     06 18 10  30.6 156.7 -1.5     -22.0     5     7604   10 21 16
10 22 21  ---          06 19 16  30.7 157.0 -1.4     -21.7    65     7620   10 21 17

10 24 17  0628+203     06 21 12  79.4 165.5 -0.2     -13.3    12     7620   10 24 17
10 25 26  ---          06 22 21  79.4 166.9 -0.2     -12.0    69     7638   10 24 18

10 26 32  0821+248     06 23 27  62.3  95.1 -2.0     -70.5     7     7638   10 26 32
10 27 56  ---          06 24 52  62.6  95.3 -2.0     -70.4    84     7660   10 26 33

10 28 17  0827+243     06 25 13  61.1  95.2 -2.1     -69.8    10     7660   10 28 17
10 30 14  ---          06 27 10  61.6  95.6 -2.1     -69.7   117     7690   10 28 18

10 31 30  1005+066     06 28 26  32.9 103.5 -3.7     -57.3    11     7690   10 31 30
10 33 03  ---          06 29 59  33.2 103.7 -3.7     -57.2    93     7714   10 31 31

10 33 45  0951+268     06 30 41  45.1  81.9 -3.4     -72.2    11     7714   10 33 45
10 35 15  ---          06 32 12  45.4  82.0 -3.4     -72.3    90     7737   10 33 46

10 36 11  0748+126     06 33 08  64.2 130.5 -1.3     -42.0    11     7737   10 36 11
10 37 16  ---          06 34 13  64.4 131.0 -1.3     -41.7    65     7754   10 36 12

10 37 55  0725+219     06 34 52  74.9 122.3 -0.9     -51.6    10     7754   10 37 55
10 38 57  ---          06 35 54  75.1 122.9 -0.9     -51.1    62     7770   10 37 56

10 40 32  0446+112     06 37 30  58.6 238.0  1.8      48.1     5     7770   10 40 32
10 41 32  ---          06 38 30  58.5 238.3  1.8      48.3    60     7785   10 40 33

10 43 27  1115-122     06 40 25  10.3 111.5 -4.7     -55.1    12     7785   10 43 27
10 45 10  ---          06 42 08  10.6 111.8 -4.6     -55.0   103     7812   10 43 28

10 45 36  1133-032     06 42 34  12.0 101.6 -4.9     -57.6    11     7812   10 45 36
10 48 26  ---          06 45 25  12.6 102.0 -4.9     -57.5   170     7856   10 45 37

10 50 12  4C39.25      06 47 11  56.1  64.7 -2.7     -91.6    12     7856   10 50 12
10 51 55  ---          06 48 54  56.5  64.6 -2.7     -91.9   103     7882   10 50 13
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

10 53 01  1128+385     06 50 01  32.7  61.8 -4.7     -74.6    11     7882   10 53 01
10 54 20  ---          06 51 20  32.9  61.9 -4.7     -74.7    79     7903   10 53 02

10 54 43  1144+402     06 51 43  30.5  59.0 -4.9     -73.8    10     7903   10 54 43
10 56 02  ---          06 53 02  30.7  59.1 -4.9     -74.0    79     7923   10 54 44

10 57 26  0736+017     06 54 26  58.9 157.2 -0.8     -19.5     6     7923   10 57 26
10 58 35  ---          06 55 36  59.0 157.7 -0.7     -19.0    69     7941   10 57 27

11 00 00  1055+018     06 57 01  25.7 104.6 -4.0     -56.4    11     7941   11 00 00
11 05 00  ---          07 02 02  26.8 105.4 -4.0     -56.1   300     8018   11 00 01

11 06 59  3C120        07 04 01  46.8 241.9  2.5      49.7    14     8018   11 06 59
11 11 59  ---          07 09 02  45.8 243.1  2.6      50.4   300     8095   11 07 00

11 12 48  CTA26        07 09 51  30.8 246.9  3.5      52.4    11     8095   11 12 48
11 14 04  ---          07 11 07  30.5 247.1  3.5      52.5    76     8115   11 12 49

11 15 56  1055+018     07 12 59  29.0 107.2 -3.8     -55.3     4     8115   11 15 56
11 17 37  ---          07 14 41  29.4 107.4 -3.8     -55.2   101     8141   11 15 57

11 18 46  0928+144     07 15 50  54.6 110.1 -2.3     -56.4    11     8141   11 18 46
11 19 58  ---          07 17 02  54.8 110.3 -2.3     -56.3    72     8159   11 18 47

11 21 23  3C309.1      07 18 27  21.6  17.9 -7.7     -56.9    11     8159   11 21 23
11 22 27  ---          07 19 31  21.6  18.0 -7.7     -57.1    64     8176   11 21 24

11 22 57  1352+757     07 20 02  27.5  16.3 -6.6     -73.6    11     8176   11 22 57
11 26 50  ---          07 23 55  27.7  16.4 -6.5     -74.6   233     8236   11 22 58

11 27 24  1343+537     07 24 29  21.1  39.5 -6.4     -66.6    10     8236   11 27 24
11 28 57  ---          07 26 03  21.3  39.6 -6.3     -66.9    93     8260   11 27 25

11 30 40  0814-241     07 27 46  33.7 166.3 -0.8     -12.9     5     8260   11 30 40
11 31 58  ---          07 29 04  33.7 166.7 -0.8     -12.6    78     8280   11 30 41

11 33 07  0636+022     07 30 13  59.2 204.8  0.8      21.2    11     8280   11 33 07
11 34 57  ---          07 32 04  59.0 205.7  0.9      21.9   110     8308   11 33 08

11 35 51  3C120        07 32 58  41.1 248.2  3.0      53.4    11     8308   11 35 51
11 37 02  ---          07 34 09  40.9 248.4  3.0      53.5    71     8327   11 35 52

11 37 32  0502+049     07 34 39  46.8 241.2  2.5      49.2    10     8327   11 37 32
11 38 57  ---          07 36 04  46.6 241.5  2.5      49.4    85     8349   11 37 33
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

11 40 06  0414-189     07 37 13  21.2 230.9  3.3      44.9    11     8349   11 40 06
11 42 09  ---          07 39 17  20.8 231.3  3.4      45.2   123     8380   11 40 07

11 44 36  1308+328     07 41 44  21.5  64.1 -5.5     -66.5    20     8380   11 44 36
11 46 19  ---          07 43 27  21.9  64.3 -5.5     -66.7   103     8407   11 44 37

11 48 08  NRAO140      07 45 17  38.0 -70.9  4.1      74.3     5     8407   11 48 08
11 49 24  ---          07 46 33  37.8 -70.8  4.1      74.2    76     8426   11 48 09

11 51 57  1102-242     07 49 06  17.4 133.9 -3.3     -43.0    -1     8426   11 51 58
11 55 09  ---          07 52 19  17.8 134.4 -3.2     -42.5   191     8476   11 51 58

11 56 53  1803+784     07 54 03  20.4   5.9-10.1     -26.2     5     8476   11 56 53
11 58 50  ---          07 56 00  20.4   6.0-10.1     -26.6   117     8506   11 56 54

12 00 04  M81          07 57 15  48.0  15.6 -2.0    -139.9    12     8506   12 00 04
12 02 44  ---          07 59 55  48.1  15.3 -2.0    -140.7   160     8547   12 00 05

12 03 16  1140+668     08 00 27  41.2  26.2 -3.7    -108.2    10     8547   12 03 16
12 05 27  ---          08 02 39  41.4  26.1 -3.7    -108.8   131     8581   12 03 17

12 06 03  0901+697     08 03 15  50.1   8.9 -1.1    -157.7    11     8581   12 06 03
12 09 17  ---          08 06 29  50.2   8.5 -1.0    -158.8   194     8631   12 06 04

12 10 43  1642+690     08 07 55  16.4  17.1 -8.6     -44.6    11     8631   12 10 43
12 12 15  ---          08 09 28  16.5  17.2 -8.5     -44.9    92     8654   12 10 44

12 13 18  0344+558     08 10 31  38.7 -40.5  4.3      91.1    11     8654   12 13 18
12 16 29  ---          08 13 42  38.2 -40.5  4.4      90.5   191     8704   12 13 19

12 17 21  0529+483     08 14 34  55.0 -48.0  2.7     105.8    11     8704   12 17 21
12 19 33  ---          08 16 47  54.7 -48.1  2.7     105.2   132     8738   12 17 22

12 21 21  1325+126     08 18 35  16.8  85.4 -5.2     -61.4     5     8738   12 21 21
12 22 43  ---          08 19 57  17.0  85.6 -5.2     -61.4    82     8759   12 21 22

12 23 08  1354+195     08 20 22  14.2  75.9 -5.6     -62.1    10     8759   12 23 08
12 25 59  ---          08 23 14  14.8  76.2 -5.6     -62.2   171     8803   12 23 09

12 27 05  1039+811     08 24 20  38.0   6.8 -2.4    -140.6     9     8803   12 27 05
12 28 22  ---          08 25 37  38.0   6.7 -2.4    -140.9    77     8823   12 27 06

12 28 48  0615+820     08 26 03  37.5  -4.8  1.9     148.6    10     8823   12 28 48
12 30 07  ---          08 27 23  37.5  -4.9  1.9     148.3    79     8843   12 28 49
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

12 31 30  1125+221     08 28 46  48.9  91.3 -3.0     -67.8     7     8843   12 31 30
12 33 04  ---          08 30 20  49.2  91.5 -3.0     -67.8    94     8867   12 31 31

12 33 32  1156+295     08 30 48  44.9  78.0 -3.5     -74.4    10     8867   12 33 32
12 34 49  ---          08 32 05  45.1  78.1 -3.5     -74.5    77     8887   12 33 33

12 35 13  1147+245     08 32 29  45.7  85.7 -3.3     -70.1    11     8887   12 35 13
12 36 30  ---          08 33 47  46.0  85.9 -3.3     -70.2    77     8907   12 35 14

12 37 54  0804+499     08 35 11  70.3 -11.9  0.4     164.1     7     8907   12 37 54
12 39 08  ---          08 36 25  70.3 -12.5  0.4     163.3    74     8926   12 37 55

12 39 33  0746+483     08 36 50  70.5 -22.7  0.7     150.1    10     8926   12 39 33
12 41 16  ---          08 38 33  70.3 -23.5  0.8     149.0   103     8952   12 39 34

12 42 51  1208+186     08 40 09  40.6  91.7 -3.5     -64.9     5     8952   12 42 51
12 44 05  ---          08 41 23  40.8  91.8 -3.5     -64.9    74     8971   12 42 52

12 45 10  1417+273     08 42 28  17.6  68.6 -5.6     -64.0    11     8971   12 45 10
12 46 10  ---          08 43 28  17.8  68.7 -5.6     -64.1    60     8987   12 45 11

12 48 42  0507+179     08 46 01  40.0 268.4  3.6      64.8     2     8987   12 48 42
12 50 11  ---          08 47 30  39.7 268.6  3.6      64.8    89     9010   12 48 43

12 51 13  0358+040     08 48 32  18.1 264.1  4.8      59.1    12     9010   12 51 13
12 55 56  ---          08 53 16  17.1 264.8  4.8      59.2   283     9083   12 51 14

12 56 40  0607-157     08 54 00  29.3 226.1  2.7      40.1     9     9083   12 56 40
12 58 01  ---          08 55 21  29.1 226.4  2.7      40.4    81     9104   12 56 41

12 58 59  0600+177     08 56 19  49.0 261.8  2.9      63.4    11     9104   12 58 59
13 00 28  ---          08 57 49  48.7 262.0  2.9      63.4    89     9127   12 59 00

13 01 44  0520-165     08 59 05  20.1 235.5  3.6      47.7    12     9127   13 01 44
13 05 56  ---          09 03 17  19.3 236.2  3.7      48.2   252     9192   13 01 45

13 10 54  1222+037     09 08 16  36.0 110.3 -3.3     -54.0   200     9192   13 10 54
13 12 36  ---          09 09 59  36.4 110.6 -3.3     -53.8   102     9218   13 10 55

13 13 44  1227+587     09 11 07  46.4  35.6 -3.3    -107.1     7     9218   13 13 44
13 14 59  ---          09 12 22  46.5  35.6 -3.3    -107.4    75     9237   13 13 45

13 15 29  1308+471     09 12 52  41.9  52.7 -4.0     -87.4    10     9237   13 15 29
13 16 33  ---          09 13 56  42.1  52.7 -4.0     -87.6    64     9254   13 15 30
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

13 18 43  0721-071     09 16 07  43.7 219.6  1.8      33.5     3     9254   13 18 43
13 20 05  ---          09 17 29  43.5 220.0  1.9      33.9    82     9275   13 18 44

13 20 30  0727-115     09 17 54  40.5 215.2  1.8      30.5    11     9275   13 20 30
13 21 37  ---          09 19 01  40.4 215.5  1.8      30.7    67     9292   13 20 31

13 22 00  0744-158     09 19 24  38.4 208.6  1.5      25.4    10     9292   13 22 00
13 23 14  ---          09 20 38  38.3 209.0  1.6      25.7    74     9311   13 22 01

13 25 23  1849+670     09 22 48  12.0 374.3 -9.4     -33.1     3     9311   13 25 23
13 26 24  ---          09 23 49  12.0 374.4 -9.4     -33.3    61     9327   13 25 24

13 29 33  1215-002     09 26 58  38.5 119.2 -2.9     -48.7     0     9327   13 29 33
13 30 43  ---          09 28 09  38.8 119.5 -2.9     -48.5    70     9345   13 29 34

13 31 15  M84          09 28 41  45.4 103.6 -3.0     -59.0    11     9345   13 31 15
13 32 15  ---          09 29 41  45.6 103.8 -2.9     -59.0    60     9360   13 31 16

13 34 28  0547+234     09 31 54  41.1 275.6  3.7      69.0     3     9360   13 34 28
13 36 51  ---          09 34 18  40.5 275.9  3.7      68.9   143     9397   13 34 29

13 37 55  0743-247     09 35 22  28.6 208.3  1.8      26.7     8     9397   13 37 55
13 42 55  ---          09 40 23  28.1 209.4  1.9      27.8   300     9474   13 37 56

13 46 02  1005-333     09 43 30  25.4 174.2 -0.4      -6.0   154     9474   13 46 02
13 48 45  ---          09 46 14  25.5 174.8 -0.4      -5.3   163     9516   13 46 03

13 50 27  1459+480     09 47 56  29.6  49.2 -5.2     -75.7     5     9516   13 50 27
13 52 44  ---          09 50 13  29.9  49.3 -5.2     -76.1   137     9552   13 50 28

13 55 29  0628+203     09 52 59  44.0 269.4  3.3      66.6     0     9552   13 55 29
13 57 02  ---          09 54 32  43.6 269.6  3.4      66.6    93     9576   13 55 30

13 57 41  0731+050     09 55 11  48.2 239.0  2.3      47.8     9     9576   13 57 41
13 59 53  ---          09 57 23  47.8 239.6  2.4      48.1   132     9610   13 57 42

14 00 55  3C119        09 58 26  26.1 304.8  5.4      71.1     8     9610   14 00 55
14 02 03  ---          09 59 34  25.9 304.9  5.4      70.9    68     9627   14 00 56

14 04 20  1331-195     10 01 51  18.0 127.6 -3.6     -46.5     3     9627   14 04 20
14 08 17  ---          10 05 49  18.7 128.3 -3.5     -46.0   237     9688   14 04 21

14 10 10  0041+677     10 07 42  13.1 -14.1  9.4      34.3     4     9688   14 10 10
14 11 53  ---          10 09 25  13.0 -14.0  9.4      34.0   103     9715   14 10 11
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

14 16 48  0633+595     10 14 21  44.3 -34.7  3.6     104.8   225     9715   14 16 48
14 18 20  ---          10 15 53  44.1 -34.8  3.6     104.4    92     9738   14 16 49

14 19 56  0251+393     10 17 30   5.5 -46.5  7.4      54.2    12     9738   14 19 56
14 21 56  ---          10 19 30   5.1 -46.3  7.4      53.9   120     9769   14 19 57

14 23 51  0219+628     10 21 25  15.5 -24.1  7.9      51.3    86     9769   14 23 51
14 24 52  ---          10 22 26  15.4 -24.1  8.0      51.1    61     9785   14 23 52

14 28 12  OJ287        10 25 47  67.2 247.5  1.5      57.8    -1     9785   14 28 13
14 29 37  ---          10 27 12  66.9 248.0  1.5      58.1    84     9807   14 28 13

14 31 12  0346+800     10 28 47  28.9 348.9  6.5      77.0    12     9807   14 31 12
14 33 32  ---          10 31 08  28.8 348.9  6.5      76.4   140     9843   14 31 13

14 35 17  1144+402     10 32 53  72.1 413.9 -1.3    -115.1    12     9843   14 35 17
14 37 34  ---          10 35 11  72.5 413.3 -1.2    -116.1   137     9878   14 35 18

14 38 00  1128+385     10 35 37  76.2 413.5 -0.9    -118.5    11     9878   14 38 00
14 39 00  ---          10 36 37  76.3 413.1 -0.9    -119.0    60     9894   14 38 01

14 41 00  1637+574     10 38 37  25.4 396.7 -6.0     -72.2    12     9894   14 41 00
14 43 01  ---          10 40 38  25.6 396.8 -6.0     -72.6   121     9925   14 41 01

14 43 52  1657+265     10 41 30   9.4 424.7 -6.3     -60.4    11     9925   14 43 52
14 44 54  ---          10 42 32   9.6 424.9 -6.3     -60.5    62     9941   14 43 53

14 48 04  1124-186     10 45 42  39.2 167.0 -0.7     -11.8    -1     9941   14 48 05
14 50 35  ---          10 48 14  39.4 167.7 -0.7     -11.2   150     9979   14 48 05

14 52 06  0528+134     10 49 45  15.9 276.6  5.3      61.6     6     9979   14 52 06
14 57 06  ---          10 54 46  14.8 277.2  5.4      61.4   300    10057   14 52 07

15 07 12  1546+027     11 04 53  17.2  97.4 -4.8     -58.7   469    10057   15 07 12
15 12 12  ---          11 09 54  18.3  98.1 -4.7     -58.5   300    10134   15 07 13

15 14 18  0748+126     11 12 01  40.6 259.8  3.3      60.1     3    10134   15 14 18
15 15 53  ---          11 13 36  40.3 260.0  3.4      60.2    95    10158   15 14 19

15 16 51  0814-241     11 14 34  20.5 222.7  2.9      39.8    11    10158   15 16 51
15 18 32  ---          11 16 15  20.3 223.0  3.0      40.1   101    10184   15 16 52

15 20 13  1546+027     11 17 57  20.0  99.2 -4.5     -58.2     5    10184   15 20 13
15 23 55  ---          11 21 39  20.8  99.8 -4.5     -58.1   222    10242   15 20 14
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

15 25 07  3C309.1      11 22 51  40.0  19.5 -3.6    -114.5     7    10242   15 25 07
15 26 31  ---          11 24 16  40.1  19.5 -3.6    -114.9    84    10263   15 25 08

15 27 13  1803+784     11 24 58  28.3  13.0 -6.6     -75.0    11    10263   15 27 13
15 32 13  ---          11 29 59  28.5  13.0 -6.5     -76.2   300    10341   15 27 14

15 33 45  1749+701     11 31 31  27.2  22.5 -6.3     -74.8    77    10341   15 33 45
15 35 14  ---          11 33 00  27.4  22.5 -6.3     -75.2    89    10364   15 33 46

15 36 02  1352+757     11 33 48  42.1  11.2 -2.3    -138.4    11    10364   15 36 02
15 37 23  ---          11 35 09  42.2  11.1 -2.3    -138.7    81    10384   15 36 03

15 38 36  1308+328     11 36 23  69.6  78.7 -1.6     -88.6    11    10384   15 38 36
15 39 42  ---          11 37 29  69.8  78.7 -1.6     -88.8    66    10401   15 38 37

15 40 23  1215+303     11 38 10  81.1  91.6 -0.7     -83.2    11    10401   15 40 23
15 42 44  ---          11 40 31  81.7  92.1 -0.6     -83.1   141    10438   15 40 24

15 44 12  1435+638     11 41 59  47.1  27.0 -2.9    -118.8    12    10438   15 44 12
15 47 32  ---          11 45 20  47.5  26.7 -2.9    -119.8   200    10489   15 44 13

15 48 09  1140+668     11 45 57  54.2  -0.2  0.0     179.7    10    10489   15 48 09
15 50 38  ---          11 48 27  54.2  -0.6  0.1     178.7   149    10528   15 48 10

15 51 08  M81          11 48 57  48.5 -14.7  1.9     142.7    11    10528   15 51 08
15 53 22  ---          11 51 11  48.4 -14.9  1.9     142.0   134    10562   15 51 09

15 53 47  0901+697     11 51 36  44.9 -18.9  2.7     127.6    10    10562   15 53 47
15 56 48  ---          11 54 38  44.7 -19.1  2.8     126.7   181    10609   15 53 48

15 57 36  1642+690     11 55 26  35.0  24.6 -4.8     -94.9     9    10609   15 57 36
16 02 29  ---          12 00 19  35.4  24.6 -4.7     -96.0   293    10684   15 57 37

16 03 49  2146+608     12 01 40   5.7  15.3 -9.8     -28.2    14    10684   16 03 49
16 08 49  ---          12 06 41   6.0  15.9 -9.7     -29.3   300    10762   16 03 50

16 11 08  1343+537     12 09 00  61.2  30.7 -1.6    -132.5    23    10762   16 11 08
16 12 42  ---          12 10 34  61.3  30.4 -1.6    -133.1    94    10786   16 11 09

16 13 45  1039+811     12 11 37  39.2  -4.3  1.4     156.3    11    10786   16 13 45
16 15 28  ---          12 13 21  39.1  -4.4  1.4     155.8   103    10812   16 13 46

16 16 34  0454+550     12 14 27  15.3 -34.2  7.2      57.8    11    10812   16 16 34
16 17 45  ---          12 15 38  15.1 -34.1  7.2      57.6    71    10831   16 16 35
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

16 18 14  0418+532     12 16 07   9.8 -32.3  7.9      50.5    11    10831   16 18 14
16 19 38  ---          12 17 31   9.6 -32.2  7.9      50.3    84    10852   16 18 15

16 22 13  1244-255     12 20 07  33.0 172.5 -0.5      -7.2     1    10852   16 22 13
16 23 35  ---          12 21 29  33.1 172.9 -0.4      -6.8    82    10873   16 22 14

16 24 46  1655+077     12 22 40  21.8  94.0 -4.6     -60.0     7    10873   16 24 46
16 26 11  ---          12 24 05  22.1  94.2 -4.6     -60.0    85    10895   16 24 47

16 27 14  1600+335     12 25 09  44.3  71.6 -3.6     -77.9    11    10895   16 27 14
16 28 52  ---          12 26 47  44.6  71.7 -3.6     -78.0    98    10921   16 27 15

16 29 52  1417+273     12 27 47  65.0  91.2 -1.9     -74.9    12    10921   16 29 52
16 33 40  ---          12 31 36  65.8  91.8 -1.8     -74.8   228    10979   16 29 53

16 35 50  0415+572     12 33 46  10.2 -27.3  8.2      47.1    13    10979   16 35 50
16 36 59  ---          12 34 55  10.1 -27.2  8.2      46.9    69    10997   16 35 51

16 37 31  0444+634     12 35 27  16.8 -24.7  7.7      53.9    11    10997   16 37 31
16 40 31  ---          12 38 28  16.5 -24.5  7.8      53.3   180    11043   16 37 32

16 42 03  0529+483     12 40 00  12.8 -40.8  7.1      57.9    72    11043   16 42 03
16 43 29  ---          12 41 26  12.6 -40.7  7.1      57.7    86    11066   16 42 04

16 44 32  0827+243     12 42 29  34.8 -80.4  4.2      68.3    11    11066   16 44 32
16 47 00  ---          12 44 58  34.2 -80.2  4.2      68.2   148    11104   16 44 33

16 51 05  0823+033     12 49 03  22.6 259.7  4.4      58.0    -5    11104   16 51 10
16 52 18  ---          12 50 17  22.3 259.9  4.4      58.0    68    11121   16 51 06

16 53 32  1013+127     12 51 31  50.0 251.4  2.6      56.6    11    11121   16 53 32
16 55 24  ---          12 53 23  49.6 251.8  2.6      56.8   112    11150   16 53 33

16 57 13  1502+106     12 55 12  53.6 116.7 -2.2     -51.4     5    11150   16 57 13
16 58 14  ---          12 56 14  53.8 117.0 -2.2     -51.2    61    11166   16 57 14

16 59 09  1354+195     12 57 09  72.1 126.1 -1.0     -47.4    11    11166   16 59 09
17 02 50  ---          13 00 50  72.7 128.1 -1.0     -45.8   221    11223   16 59 10

17 05 16  0736+017     13 03 17   8.8 266.6  5.4      59.2    12    11223   17 05 16
17 06 16  ---          13 04 17   8.6 266.7  5.4      59.2    60    11238   17 05 17

17 08 26  1725+044     13 06 27  23.0  98.9 -4.4     -58.5     3    11238   17 08 26
17 09 37  ---          13 07 39  23.3  99.0 -4.4     -58.5    71    11256   17 08 27
Schedule for VLBA_FD   (Code Fd )                                   Page  27
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

17 10 05  1722+119     13 08 07  27.8  92.5 -4.3     -61.4    11    11256   17 10 05
17 12 12  ---          13 10 14  28.3  92.7 -4.3     -61.4   127    11289   17 10 06

17 13 05  1839+548     13 11 07  28.7  40.6 -5.5     -76.7     8    11289   17 13 05
17 15 28  ---          13 13 30  29.1  40.7 -5.5     -77.1   143    11326   17 13 06

17 15 56  1849+670     13 13 59  30.4  26.6 -5.6     -82.5    10    11326   17 15 56
17 18 45  ---          13 16 48  30.6  26.6 -5.5     -83.1   169    11370   17 15 57

17 20 05  1227+587     13 18 08  61.1 -12.8  0.8     158.8    12    11370   17 20 05
17 21 56  ---          13 20 00  61.0 -13.2  0.8     158.0   111    11398   17 20 06

17 22 59  0859+470     13 21 03  39.0 -52.4  4.3      84.5    12    11398   17 22 59
17 24 21  ---          13 22 25  38.7 -52.4  4.3      84.2    82    11419   17 23 00

17 24 57  0804+499     13 23 01  30.2 -47.0  5.2      77.0    11    11419   17 24 57
17 27 32  ---          13 25 36  29.8 -46.9  5.3      76.6   155    11459   17 24 58

17 30 50  1045-188     13 28 55  27.0 222.8  2.7      38.3    -2    11459   17 30 52
17 32 03  ---          13 30 08  26.9 223.1  2.7      38.5    71    11478   17 30 51

17 32 55  1005-333     13 31 00   9.9 220.8  3.4      42.4    11    11478   17 32 55
17 34 12  ---          13 32 18   9.7 221.0  3.4      42.7    77    11497   17 32 56

17 35 38  1055+018     13 33 44  43.3 238.8  2.6      47.4    12    11497   17 35 38
17 37 26  ---          13 35 32  43.0 239.2  2.6      47.7   108    11525   17 35 39

17 39 03  1557+032     13 37 09  46.3 122.1 -2.4     -46.9     6    11525   17 39 03
17 41 04  ---          13 39 11  46.7 122.6 -2.4     -46.6   121    11556   17 39 04

17 42 30  1115-122     13 40 37  35.0 223.4  2.4      37.3     6    11556   17 42 30
17 43 56  ---          13 42 03  34.8 223.8  2.4      37.6    86    11579   17 42 31

17 44 42  1331-195     13 42 49  39.4 182.4  0.1       2.2     9    11579   17 44 42
17 45 49  ---          13 43 56  39.3 182.7  0.1       2.5    67    11596   17 44 43

17 46 26  1514-241     13 44 34  30.4 155.0 -1.6     -23.6     9    11596   17 46 26
17 47 34  ---          13 45 42  30.5 155.2 -1.6     -23.3    68    11613   17 46 27

17 48 11  1706-174     13 46 19  21.2 127.2 -3.4     -46.0     9    11613   17 48 11
17 49 15  ---          13 47 23  21.4 127.4 -3.4     -45.8    64    11630   17 48 12

17 50 31  2100+468     13 48 39  10.8  41.0 -7.2     -56.1     7    11630   17 50 31
17 52 49  ---          13 50 58  11.1  41.2 -7.2     -56.5   138    11665   17 50 32
Schedule for VLBA_FD   (Code Fd )                                   Page  28
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

17 55 03  1459+480     13 53 12  68.4  32.6 -1.1    -136.4    13    11665   17 55 03
17 56 24  ---          13 54 33  68.6  32.1 -1.1    -137.1    81    11686   17 55 04

17 58 25  0633+595     13 56 35  17.3 -30.1  7.3      58.4    12    11686   17 58 25
17 59 28  ---          13 57 38  17.1 -30.0  7.3      58.2    63    11702   17 58 26

18 00 00  0642+449     13 58 10  10.1 -43.4  7.2      56.5    10    11702   18 00 00
18 05 00  ---          14 03 11   9.4 -42.9  7.2      55.7   300    11780   18 00 01

18 07 13  OJ287        14 05 24  20.6 -78.3  5.2      63.7   100    11780   18 07 13
18 12 13  ---          14 10 25  19.6 -77.8  5.2      63.5   300    11857   18 07 14

18 14 47  NRAO530      14 12 59  24.8 124.3 -3.4     -46.9     2    11857   18 14 47
18 17 19  ---          14 15 32  25.2 124.8 -3.3     -46.5   152    11896   18 14 48

18 18 31  2118+443     14 16 44  10.8  44.0 -7.1     -57.3     7    11896   18 18 31
18 20 08  ---          14 18 21  11.1  44.2 -7.1     -57.5    97    11921   18 18 32

18 20 59  0346+800     14 19 12  21.7  -4.4 10.3      23.0     9    11921   18 20 59
18 25 16  ---          14 23 30  21.6  -4.2 10.4      22.0   257    11987   18 21 00

18 25 57  0041+677     14 24 11  10.5   9.0-10.4     -21.2    11    11987   18 25 57
18 30 57  ---          14 29 12  10.7   9.4-10.3     -22.3   300    12065   18 25 58

18 35 15  1144+402     14 33 31  55.4 -63.1  2.8      92.3   161    12065   18 35 15
18 36 21  ---          14 34 37  55.1 -63.1  2.8      92.1    66    12082   18 35 16

18 36 46  1128+385     14 35 02  51.9 -66.0  3.0      87.2    11    12082   18 36 46
18 38 26  ---          14 36 42  51.6 -65.9  3.1      87.0   100    12107   18 36 47

18 40 04  1726+455     14 38 20  53.9  53.5 -2.8     -99.3     5    12107   18 40 04
18 41 05  ---          14 39 22  54.1  53.5 -2.8     -99.6    61    12123   18 40 05

18 42 20  1951+355     14 40 37  25.9  62.2 -5.2     -69.6    11    12123   18 42 20
18 44 23  ---          14 42 40  26.3  62.4 -5.2     -69.8   123    12155   18 42 21

18 45 06  1821+107     14 43 23  35.1  98.7 -3.7     -60.0     9    12155   18 45 06
18 46 12  ---          14 44 29  35.3  98.8 -3.7     -59.9    66    12172   18 45 07

18 47 21  1509+022     14 45 39  60.6 165.7 -0.5     -12.3    11    12172   18 47 21
18 48 25  ---          14 46 43  60.6 166.3 -0.4     -11.8    64    12188   18 47 22

18 48 50  1532+016     14 47 08  58.6 156.0 -0.8     -20.5    10    12188   18 48 50
18 50 24  ---          14 48 42  58.7 156.7 -0.8     -19.9    94    12213   18 48 51
Schedule for VLBA_FD   (Code Fd )                                   Page  29
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

18 51 45  M84          14 50 03  52.4 249.6  2.4      55.8     7    12213   18 51 45
18 56 45  ---          14 55 04  51.4 250.7  2.5      56.4   300    12290   18 51 46

18 59 18  2008+355     14 57 38  26.1 422.2 -5.2     -69.7    23    12290   18 59 18
19 00 48  ---          14 59 08  26.4 422.3 -5.2     -69.9    90    12313   18 59 19

19 01 54  1743+173     15 00 14  50.0  99.6 -2.8  W  -62.7  -171    12313   19 04 45
19 03 02  ---          15 01 22  50.2  99.8 -2.8  W  -62.6     0    12287   19 01 55

19 03 31  1749+096     15 01 51  45.1 108.6 -2.8     -55.8    11    12287   19 03 31
19 04 49  ---          15 03 09  45.4 108.8 -2.8     -55.7    78    12307   19 03 32

19 06 57  1147+245     15 05 18  46.8 273.7  3.2      70.2     3    12307   19 06 57
19 08 05  ---          15 06 26  46.6 273.8  3.2      70.2    68    12324   19 06 58

19 08 35  1125+221     15 06 56  40.8 273.3  3.6      67.6    11    12324   19 08 35
19 10 58  ---          15 09 19  40.3 273.6  3.7      67.6   143    12361   19 08 36

19 11 56  0922+364     15 10 18  20.6 300.6  5.7      66.5    11    12361   19 11 56
19 13 57  ---          15 12 19  20.2 300.8  5.7      66.2   121    12392   19 11 57

19 16 22  1937-101     15 14 44  14.3 111.1 -4.4     -54.6     2    12392   19 16 22
19 17 37  ---          15 16 00  14.6 111.2 -4.4     -54.5    75    12411   19 16 23

19 19 30  3C274        15 17 53  47.6 253.6  2.8      57.6     4    12411   19 19 30
19 20 57  ---          15 19 20  47.3 253.9  2.8      57.8    87    12434   19 19 31

19 21 57  1133-032     15 20 20  26.9 247.5  3.7      52.8    12    12434   19 21 57
19 23 16  ---          15 21 39  26.6 247.7  3.7      52.9    79    12454   19 21 58

19 24 13  1102-242     15 22 37   7.4 235.6  4.3      51.3    11    12454   19 24 13
19 25 23  ---          15 23 47   7.2 235.7  4.3      51.5    70    12472   19 24 14

19 25 56  1124-186     15 24 20  14.6 236.8  3.9      49.7    10    12472   19 25 56
19 27 35  ---          15 25 59  14.3 237.1  4.0      49.9    99    12498   19 25 57

19 29 54  2201+315     15 28 19   8.9  58.1 -6.6     -59.3     4    12498   19 29 54
19 31 00  ---          15 29 25   9.1  58.2 -6.6     -59.5    66    12515   19 29 55

19 33 15  1325+126     15 31 40  56.3 243.7  2.0      52.1    -5    12515   19 33 20
19 34 15  ---          15 32 40  56.1 244.0  2.1      52.3    55    12529   19 33 16

19 35 09  1222+037     15 33 34  38.1 247.8  3.1      52.9    11    12529   19 35 09
19 36 11  ---          15 34 37  37.9 248.0  3.1      53.1    62    12545   19 35 10
Schedule for VLBA_FD   (Code Fd )                                   Page  30
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

19 36 50  1334-127     15 35 16  38.1 217.0  1.9      32.1     9    12545   19 36 50
19 38 02  ---          15 36 28  38.0 217.3  2.0      32.4    72    12563   19 36 51

19 38 43  1405-287     15 37 09  26.8 201.2  1.4      20.9    11    12563   19 38 43
19 40 12  ---          15 38 38  26.6 201.6  1.5      21.2    89    12586   19 38 44

19 41 14  1825-214     15 39 40  23.9 136.5 -2.8     -39.5     8    12586   19 41 14
19 42 18  ---          15 40 45  24.0 136.7 -2.8     -39.3    64    12603   19 41 15

19 44 32  1308+471     15 42 59  56.8 309.9  2.5     105.5     3    12603   19 44 32
19 45 43  ---          15 44 10  56.7 309.8  2.5     105.2    71    12621   19 44 33

19 47 02  2105+551     15 45 29  30.0 400.2 -5.4     -78.6     7    12621   19 47 02
19 48 23  ---          15 46 51  30.2 400.3 -5.3     -78.8    81    12642   19 47 03

19 49 15  1352+757     15 47 43  43.1 350.5  1.9     145.7     9    12642   19 49 15
19 50 33  ---          15 49 01  43.1 350.4  1.9     145.4    78    12662   19 49 16

19 51 03  1803+784     15 49 31  40.1 368.1 -2.2    -142.9    10    12662   19 51 03
19 52 22  ---          15 50 50  40.2 368.0 -2.1    -143.2    79    12683   19 51 04

19 53 25  2052+239     15 51 53  23.6 434.8 -5.1     -65.6     8    12683   19 53 25
19 55 26  ---          15 53 55  24.0 435.0 -5.0     -65.7   121    12714   19 53 26

19 57 32  1005+066     15 56 01   6.0 273.7  5.8      59.7     3    12714   19 57 32
20 00 38  ---          15 59 08   5.4 274.1  5.8      59.7   186    12762   19 57 33

20 02 17  1351-018     16 00 47  45.6 228.0  2.1      39.8    12    12762   20 02 17
20 03 42  ---          16 02 12  45.4 228.4  2.1      40.1    85    12784   20 02 18

20 05 10  1511-476     16 03 40  10.7 188.0  0.8      10.3    12    12784   20 05 10
20 07 14  ---          16 05 45  10.7 188.4  0.8      10.8   124    12815   20 05 11

20 08 37  1156+295     16 07 08  37.3 285.1  4.1      72.0     6    12815   20 08 37
20 09 43  ---          16 08 14  37.0 285.1  4.1      71.9    66    12832   20 08 38

20 10 48  0615+820     16 09 19  24.0 354.9  9.6      33.2     7    12832   20 10 48
20 12 53  ---          16 11 25  24.0 355.0  9.7      32.7   125    12865   20 10 49

20 14 00  1749+701     16 12 32  48.3 372.0 -1.6    -148.3    11    12865   20 14 00
20 15 19  ---          16 13 51  48.4 371.8 -1.6    -148.8    79    12885   20 14 01

20 15 44  1642+690     16 14 16  51.5 364.0 -0.5    -170.4    11    12885   20 15 44
20 17 10  ---          16 15 42  51.5 363.8 -0.4    -170.9    86    12907   20 15 45
Schedule for VLBA_FD   (Code Fd )                                   Page  31
               Improving the K-band celestial reference frame for the next multi-waveba
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   3 Nov 2024   Day 308 ---

20 17 37  3C309.1      16 16 09  47.8 351.1  1.3     155.1    10    12907   20 17 37
20 18 51  ---          16 17 24  47.7 351.0  1.3     154.7    74    12926   20 17 38

20 19 21  1435+638     16 17 54  53.5 341.4  1.7     142.1    11    12926   20 19 21
20 21 46  ---          16 20 19  53.3 341.1  1.7     141.3   145    12964   20 19 22

20 22 18  1343+537     16 20 51  54.1 320.7  2.6     113.8    10    12964   20 22 18
20 25 22  ---          16 23 56  53.7 320.4  2.6     113.0   184    13011   20 22 19

20 26 43  VR422201     16 25 17  23.8 413.5 -5.6     -69.4     7    13011   20 26 43
20 27 55  ---          16 26 29  24.0 413.5 -5.6     -69.6    72    13030   20 26 44

20 28 33  2309+454     16 27 07  14.3 404.8 -6.8     -60.5    11    13030   20 28 33
20 30 00  ---          16 28 34  14.5 404.9 -6.7     -60.7    87    13052   20 28 34


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess324.K2048globgeo
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v1cm_b3

   Setup group:    9         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00  21500.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       RCP       RCP       RCP       RCP       RCP       RCP       RCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        B         B         B         B         B         B         B         B 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1      6.1     12.4

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  15  Setup file default.  Used with PCAL = 1MHz
   LO sum=   22012.00  22076.00  22140.00  22204.00  22268.00  22332.00  22396.00  22460.00
   BBC fr=     512.00    576.00    640.00    704.00    768.00    832.00    896.00    960.00
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   2  4  5  7
   CRD fr=     599.99    727.99    791.99    919.99
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  15  16  17  18  19  20  22  23  24  26

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 0002-478          00 02 02.949642   * 00 04 35.655494     00 05 53.111009       0.00
   0002-478         -47 53 01.89774    *-47 36 19.60398     -47 28 08.66928        0.00
                     From catalog imbedded in main SCHED input file.

 * 0003-066          00 03 40.288766   * 00 06 13.892887     00 07 31.016477       0.00
   0003-066         -06 40 17.30036    *-06 23 35.33579     -06 15 14.06246        0.00
                     From catalog imbedded in main SCHED input file.

 * 0009-148          00 09 07.482319   * 00 11 40.455843     00 12 57.366692       0.00
   0009-148         -14 50 45.84853    *-14 34 04.63495     -14 25 45.57114        0.00
                     From catalog imbedded in main SCHED input file.

 * 0013-005          00 13 37.349900   * 00 16 11.088549     00 17 28.280587       0.00
   0013-005         -00 31 52.48992    *-00 15 12.44530     -00 06 50.43224        0.00
                     From catalog imbedded in main SCHED input file.

 * 0017+257          00 17 03.415159   * 00 19 39.780584     00 20 58.247705       0.00
   0017+257          25 46 13.48168    * 26 02 52.27718      26 11 18.68797        0.00
                     From catalog imbedded in main SCHED input file.

 * 0039+568          00 39 27.423037   * 00 42 19.451676     00 43 46.340110       0.00
   0039+568          56 52 10.63306    * 57 08 36.58590      57 16 58.55477        0.00
                     From catalog imbedded in main SCHED input file.

 * 0041+677          00 41 46.066632   * 00 44 50.759608     00 46 24.740249       0.00
   0041+677          67 46 38.69753    * 68 03 02.68590      68 11 23.41394        0.00
                     From catalog imbedded in main SCHED input file.

 * 0044+566          00 44 06.482811   * 00 47 00.428843     00 48 28.301862       0.00
   0044+566          56 41 20.26684    * 56 57 42.39444      57 06 02.25887        0.00
                     From catalog imbedded in main SCHED input file.

 * 0104-408          01 04 27.574524   * 01 06 45.107979     01 07 55.140870       0.00
   0104-408         -40 50 21.55660    *-40 34 19.96069     -40 26 23.20577        0.00
                     From catalog imbedded in main SCHED input file.

 * 0109+224          01 09 23.608517   * 01 12 05.824710     01 13 27.401376       0.00
   0109+224          22 28 44.12485    * 22 44 38.78632      22 52 42.37993        0.00
                     From catalog imbedded in main SCHED input file.

 * 0109+351          01 09 24.829662   * 01 12 12.944390     01 13 37.545335       0.00
   0109+351          35 06 24.83554    * 35 22 19.33625      35 30 23.82524        0.00
                     From catalog imbedded in main SCHED input file.

 * 0111+021          01 11 08.570354   * 01 13 43.144946     01 15 00.946342       0.00
   0111+021          02 06 24.80041    * 02 22 17.31623      02 30 17.38514        0.00
                     From catalog imbedded in main SCHED input file.

 * 0148-177          01 48 42.143425   * 01 51 06.083347     01 52 18.881188       0.00
   0148-177         -17 47 33.94581    *-17 32 44.71826     -17 25 17.48405        0.00
                     From catalog imbedded in main SCHED input file.

 * 0159-668          01 59 52.068056   * 02 01 07.744008     02 01 49.720894       0.00
   0159-668         -66 52 39.75851    *-66 38 12.66620     -66 31 01.45270        0.00
                     From catalog imbedded in main SCHED input file.

 * 0202+149          02 02 07.396229   * 02 04 50.413897     02 06 12.505166       0.00
   0202+149          14 59 50.93912    * 15 14 11.04334      15 21 26.79624        0.00
                     From catalog imbedded in main SCHED input file.

 * 0213-026          02 13 09.874047   * 02 15 42.017287     02 16 58.769082       0.00
   0213-026         -02 36 51.41452    *-02 22 56.75261     -02 15 54.37396        0.00
                     From catalog imbedded in main SCHED input file.

 * 0219+628          02 19 39.890162   * 02 23 29.607025     02 25 26.304175       0.00
   0219+628          62 53 40.64823    * 63 07 17.30521      63 14 09.02105        0.00
                     From catalog imbedded in main SCHED input file.

 * 0229-479          02 29 23.107922   * 02 31 11.804068     02 32 08.093669       0.00
   0229-479         -47 59 26.10075    *-47 46 11.58246     -47 39 31.64901        0.00
                     From catalog imbedded in main SCHED input file.

 * 0235+164          02 35 52.630205   * 02 38 38.930097     02 40 02.698180       0.00
   0235+164          16 24 04.01613    * 16 36 59.27455      16 43 32.72282        0.00
                     From catalog imbedded in main SCHED input file.

 * 0235-618          02 35 37.736079   * 02 36 53.245751     02 37 34.346794       0.00
   0235-618         -61 49 13.55934    *-61 36 15.18349     -61 29 43.68108        0.00
                     From catalog imbedded in main SCHED input file.

 * 0250+320          02 50 31.214605   * 02 53 33.650138     02 55 05.566141       0.00
   0250+320          32 05 08.22927    * 32 17 20.89211      32 23 32.16808        0.00
                     From catalog imbedded in main SCHED input file.

 * 0251+393          02 51 31.227603   * 02 54 42.632053     02 56 19.131728       0.00
   0251+393          39 19 25.29311    * 39 31 34.71047      39 37 43.73687        0.00
                     From catalog imbedded in main SCHED input file.

 * 0302-623          03 02 48.121187   * 03 03 50.631402     03 04 25.349184       0.00
   0302-623         -62 23 04.08369    *-62 11 25.54994     -62 05 30.76682        0.00
                     From catalog imbedded in main SCHED input file.

 * 0308-611          03 08 51.270290   * 03 09 56.099182     03 10 31.779648       0.00
   0308-611         -61 09 58.29613    *-60 58 39.05599     -60 52 53.17395        0.00
                     From catalog imbedded in main SCHED input file.

 * 0322-294          03 22 39.763642   * 03 24 44.295382     03 25 47.712396       0.00
   0322-294         -29 28 53.05300    *-29 18 21.21736     -29 12 57.15235        0.00
                     From catalog imbedded in main SCHED input file.

   0333+321          03 33 22.404674   * 03 36 30.107593     03 38 04.635669       0.00
 * NRAO140           32 08 36.66046    * 32 18 29.34223      32 23 29.66915        0.00
                     From catalog imbedded in main SCHED input file.

   0336-019          03 36 58.953141   * 03 39 30.937781     03 40 47.605837       0.00
 * CTA26            -01 56 16.89656    *-01 46 35.80416     -01 41 37.52804        0.00
                     From catalog imbedded in main SCHED input file.

 * 0344+558          03 44 00.851013   * 03 47 56.812053     03 49 56.068911       0.00
   0344+558          55 48 18.57376    * 55 57 31.57848      56 02 07.69082        0.00
                     From catalog imbedded in main SCHED input file.

 * 0346+800          03 46 49.431783   * 03 54 46.125973     03 58 52.496758       0.00
   0346+800          80 00 33.53208    * 80 09 28.84736      80 13 46.87132        0.00
                     From catalog imbedded in main SCHED input file.

 * 0350+465          03 50 56.138348   * 03 54 30.011650     03 56 17.847845       0.00
   0350+465          46 34 30.51346    * 46 43 18.74983      46 47 43.95928        0.00
                     From catalog imbedded in main SCHED input file.

 * 0358+040          03 58 41.959781   * 04 01 19.912969     04 02 39.490549       0.00
   0358+040          04 05 13.38626    * 04 13 34.40719      04 17 52.58801        0.00
                     From catalog imbedded in main SCHED input file.

 * 0401-248          04 01 34.904683   * 04 03 41.736055     04 04 46.118194       0.00
   0401-248         -24 52 19.62099    *-24 44 08.45840     -24 39 52.18259        0.00
                     From catalog imbedded in main SCHED input file.

 * 0402-362          04 02 02.589857   * 04 03 53.749903     04 04 50.613733       0.00
   0402-362         -36 13 11.84946    *-36 05 01.91317     -36 00 45.51861        0.00
                     From catalog imbedded in main SCHED input file.

 * 0414-189          04 14 23.350984   * 04 16 36.544449     04 17 43.959465       0.00
   0414-189         -18 58 29.71005    *-18 51 08.34021     -18 47 16.70751        0.00
                     From catalog imbedded in main SCHED input file.

 * 0415+572          04 15 11.815257   * 04 19 19.412944     04 21 24.452723       0.00
   0415+572          57 15 45.79208    * 57 22 59.98413      57 26 34.73588        0.00
                     From catalog imbedded in main SCHED input file.

 * 0418+532          04 18 49.157457   * 04 22 44.398892     04 24 43.055566       0.00
   0418+532          53 17 25.97726    * 53 24 26.26272      53 27 54.85203        0.00
                     From catalog imbedded in main SCHED input file.

   0429+415          04 29 07.898986   * 04 32 36.503095     04 34 21.483407       0.00
 * 3C119             41 32 08.57548    * 41 38 28.45520      41 41 39.15386        0.00
                     From catalog imbedded in main SCHED input file.

   0430+052          04 30 31.602100   * 04 33 11.095569     04 34 31.366074       0.00
 * 3C120             05 14 59.61676    * 05 21 15.61954      05 24 31.74114        0.00
                     From catalog imbedded in main SCHED input file.

 * 0444+634          04 44 42.365059   * 04 49 23.310587     04 51 45.259614       0.00
   0444+634          63 26 55.93312    * 63 32 09.43416      63 34 40.55879        0.00
                     From catalog imbedded in main SCHED input file.

 * 0446+112          04 46 21.217277   * 04 49 07.671096     04 50 31.355519       0.00
   0446+112          11 16 17.84560    * 11 21 28.59639      11 24 11.14362        0.00
                     From catalog imbedded in main SCHED input file.

 * 0454+550          04 54 48.928132   * 04 58 54.840103     05 00 58.719671       0.00
   0454+550          55 04 09.57968    * 55 08 42.05910      55 10 54.68456        0.00
                     From catalog imbedded in main SCHED input file.

 * 0454-234          04 54 57.297213   * 04 57 03.179225     04 58 06.880744       0.00
   0454-234         -23 29 28.31971    *-23 24 52.02030     -23 22 20.07226        0.00
                     From catalog imbedded in main SCHED input file.

 * 0454-810          04 54 17.961981   * 04 50 05.440230     04 48 11.226489       0.00
   0454-810         -81 05 54.60914    *-81 01 02.23137     -80 58 12.26296        0.00
                     From catalog imbedded in main SCHED input file.

 * 0458-020          04 58 41.344685   * 05 01 12.809881     05 02 29.024908       0.00
   0458-020         -02 03 33.86898    *-01 59 14.25643     -01 56 54.28939        0.00
                     From catalog imbedded in main SCHED input file.

 * 0502+049          05 02 43.812113   * 05 05 23.184719     05 06 43.297909       0.00
   0502+049          04 55 40.51646    * 04 59 42.72453      05 01 52.59320        0.00
                     From catalog imbedded in main SCHED input file.

 * 0507+179          05 07 07.486537   * 05 10 02.369123     05 11 30.192815       0.00
   0507+179          17 56 58.64620    * 18 00 41.58165      18 02 38.79410        0.00
                     From catalog imbedded in main SCHED input file.

 * 0520-165          05 20 30.409421   * 05 22 44.654959     05 23 52.319242       0.00
   0520-165         -16 30 39.48478    *-16 27 52.40629     -16 26 15.00908        0.00
                     From catalog imbedded in main SCHED input file.

 * 0524+034          05 24 54.913882   * 05 27 32.705438     05 28 51.952905       0.00
   0524+034          03 29 04.36402    * 03 31 31.51652      03 32 54.59620        0.00
                     From catalog imbedded in main SCHED input file.

 * 0528+134          05 28 06.759205   * 05 30 56.416735     05 32 21.552474       0.00
   0528+134          13 29 42.28881    * 13 31 55.14948      13 33 08.54059        0.00
                     From catalog imbedded in main SCHED input file.

 * 0529+483          05 29 27.565374   * 05 33 15.865783     05 35 10.542619       0.00
   0529+483          48 20 47.97041    * 48 22 52.80774      48 23 52.30339        0.00
                     From catalog imbedded in main SCHED input file.

 * 0537-441          05 37 21.071425   * 05 38 50.361559     05 39 36.065938       0.00
   0537-441         -44 06 44.66655    *-44 05 08.93923     -44 04 01.52847        0.00
                     From catalog imbedded in main SCHED input file.

 * 0547+234          05 47 44.714952   * 05 50 47.390891     05 52 18.953763       0.00
   0547+234          23 26 01.27057    * 23 26 48.17718      23 27 15.78421        0.00
                     From catalog imbedded in main SCHED input file.

 * 0600+177          06 00 14.060250   * 06 03 09.130264     06 04 36.831094       0.00
   0600+177          17 42 24.20517    * 17 42 16.81034      17 42 18.98267        0.00
                     From catalog imbedded in main SCHED input file.

 * 0607-157          06 07 25.981293   * 06 09 40.949547     06 10 48.731272       0.00
   0607-157         -15 42 03.30596    *-15 42 40.67276     -15 42 43.84752        0.00
                     From catalog imbedded in main SCHED input file.

 * 0615+820          06 15 32.765132   * 06 26 03.006249     06 31 20.062125       0.00
   0615+820          82 03 56.43124    * 82 02 25.56778      82 01 17.82856        0.00
                     From catalog imbedded in main SCHED input file.

 * 0622-645          06 22 53.923140   * 06 23 07.696311     06 23 16.261572       0.00
   0622-645         -64 34 40.30440    *-64 36 20.72158     -64 36 45.20831        0.00
                     From catalog imbedded in main SCHED input file.

 * 0628+203          06 28 02.724026   * 06 31 01.062563     06 32 30.263668       0.00
   0628+203          20 23 07.96432    * 20 20 59.21081      20 19 59.86279        0.00
                     From catalog imbedded in main SCHED input file.

 * 0633+595          06 33 36.766662   * 06 38 02.871911     06 40 16.176408       0.00
   0633+595          59 35 58.24769    * 59 33 22.21383      59 31 55.82394        0.00
                     From catalog imbedded in main SCHED input file.

 * 0636+022          06 36 34.655127   * 06 39 10.946213     06 40 29.118049       0.00
   0636+022          02 14 15.53706    * 02 11 30.68489      02 10 19.30492        0.00
                     From catalog imbedded in main SCHED input file.

 * 0642+449          06 42 53.021434   * 06 46 32.025981     06 48 21.544382       0.00
   0642+449          44 54 30.82729    * 44 51 16.59003      44 49 36.02625        0.00
                     From catalog imbedded in main SCHED input file.

 * 0644-671          06 44 30.202665   * 06 44 28.044122     06 44 28.426071       0.00
   0644-671         -67 09 44.07088    *-67 12 57.35838     -67 14 06.52641        0.00
                     From catalog imbedded in main SCHED input file.

 * 0721-071          07 21 51.448486   * 07 24 17.292637     07 25 30.025397       0.00
   0721-071         -07 09 25.03069    *-07 15 20.35185     -07 18 03.22280        0.00
                     From catalog imbedded in main SCHED input file.

 * 0725+219          07 25 21.869712   * 07 28 20.608294     07 29 49.704790       0.00
   0725+219          21 59 17.09416    * 21 53 06.39026      21 50 05.50785        0.00
                     From catalog imbedded in main SCHED input file.

 * 0727-115          07 27 58.097816   * 07 30 19.112476     07 31 29.410495       0.00
   0727-115         -11 34 52.58106    *-11 41 12.60062     -11 44 06.28902        0.00
                     From catalog imbedded in main SCHED input file.

 * 0731+050          07 31 18.351470   * 07 33 57.459898     07 35 16.734505       0.00
   0731+050          05 02 48.56597    * 04 56 14.49649      04 53 08.14701        0.00
                     From catalog imbedded in main SCHED input file.

 * 0736+017          07 36 42.512344   * 07 39 18.033902     07 40 35.491929       0.00
   0736+017          01 44 00.18080    * 01 37 04.61772      01 33 48.74726        0.00
                     From catalog imbedded in main SCHED input file.

 * 0738-674          07 38 49.583222   * 07 38 56.496184     07 39 00.180884       0.00
   0738-674         -67 28 51.66893    *-67 35 50.82663     -67 38 50.84278        0.00
                     From catalog imbedded in main SCHED input file.

 * 0742-562          07 42 16.905746   * 07 43 20.485138     07 43 52.272218       0.00
   0742-562         -56 12 18.27456    *-56 19 32.95872     -56 22 42.67372        0.00
                     From catalog imbedded in main SCHED input file.

 * 0743-247          07 43 04.262457   * 07 45 10.263452     07 46 13.009701       0.00
   0743-247         -24 44 23.97577    *-24 51 43.76585     -24 55 03.09741        0.00
                     From catalog imbedded in main SCHED input file.

 * 0744-158          07 44 01.516034   * 07 46 18.236028     07 47 26.299365       0.00
   0744-158         -15 48 10.87431    *-15 55 34.74619     -15 58 58.78154        0.00
                     From catalog imbedded in main SCHED input file.

 * 0746+483          07 46 39.939662   * 07 50 20.436327     07 52 10.259623       0.00
   0746+483          48 22 30.38674    * 48 14 53.55671      48 10 59.88944        0.00
                     From catalog imbedded in main SCHED input file.

 * 0748+126          07 48 05.060491   * 07 50 52.045729     07 52 15.151321       0.00
   0748+126          12 38 45.47744    * 12 31 04.82811      12 27 22.50093        0.00
                     From catalog imbedded in main SCHED input file.

 * 0804+499          08 04 58.395749   * 08 08 39.666290     08 10 29.736344       0.00
   0804+499          49 59 23.07795    * 49 50 36.53026      49 46 07.39841        0.00
                     From catalog imbedded in main SCHED input file.

 * 0814-241          08 14 31.677667   * 08 16 40.412360     08 17 44.291080       0.00
   0814-241         -24 11 47.60748    *-24 21 06.57051     -24 25 25.26436        0.00
                     From catalog imbedded in main SCHED input file.

 * 0821+248          08 21 34.302495   * 08 24 33.009305     08 26 01.771109       0.00
   0821+248          24 48 28.74144    * 24 38 43.11583      24 33 53.77277        0.00
                     From catalog imbedded in main SCHED input file.

 * 0823+033          08 23 13.540330   * 08 25 50.338359     08 27 08.163358       0.00
   0823+033          03 19 15.40170    * 03 09 24.51996      03 04 40.68356        0.00
                     From catalog imbedded in main SCHED input file.

 * 0827+243          08 27 54.398587   * 08 30 52.086186     08 32 20.303653       0.00
   0827+243          24 21 07.66373    * 24 10 59.82033      24 05 59.55508        0.00
                     From catalog imbedded in main SCHED input file.

 * 0850+284          08 50 17.726552   * 08 53 17.828433     08 54 47.119424       0.00
   0850+284          28 25 12.68721    * 28 13 49.99744      28 08 10.82497        0.00
                     From catalog imbedded in main SCHED input file.

   0851+202          08 51 57.250612   * 08 54 48.874924     08 56 13.934732       0.00
 * OJ287             20 17 58.41741    * 20 06 30.64086      20 00 52.01025        0.00
                     From catalog imbedded in main SCHED input file.

 * 0859+470          08 59 39.983390   * 09 03 03.990088     09 04 45.078621       0.00
   0859+470          47 02 56.80551    * 46 51 04.13746      46 45 03.24006        0.00
                     From catalog imbedded in main SCHED input file.

 * 0859-140          08 59 54.946358   * 09 02 16.830922     09 03 26.974285       0.00
   0859-140         -14 03 38.85710    *-14 15 30.87569     -14 21 09.18198        0.00
                     From catalog imbedded in main SCHED input file.

 * 0901+697          09 01 52.295852   * 09 06 30.748723     09 08 48.277384       0.00
   0901+697          69 42 32.10007    * 69 30 30.82860      69 24 18.09859        0.00
                     From catalog imbedded in main SCHED input file.

 * 0922+364          09 22 47.257057   * 09 25 51.851374     09 27 23.178867       0.00
   0922+364          36 25 35.22075    * 36 12 35.67484      36 06 05.29222        0.00
                     From catalog imbedded in main SCHED input file.

   0923+392          09 23 55.319255   * 09 27 03.013976     09 28 35.868246       0.00
 * 4C39.25           39 15 23.56618    * 39 02 20.85158      38 55 47.88442        0.00
                     From catalog imbedded in main SCHED input file.

 * 0925-203          09 25 33.543222   * 09 27 51.824333     09 28 59.979004       0.00
   0925-203         -20 21 44.97481    *-20 34 51.23270     -20 41 04.88728        0.00
                     From catalog imbedded in main SCHED input file.

 * 0928+144          09 28 21.175086   * 09 31 05.342424     09 32 26.485493       0.00
   0928+144          14 27 30.73517    * 14 14 16.51857      14 07 46.91781        0.00
                     From catalog imbedded in main SCHED input file.

 * 0951+268          09 51 48.338627   * 09 54 39.796532     09 56 04.445967       0.00
   0951+268          26 53 37.10825    * 26 39 24.54333      26 32 21.27502        0.00
                     From catalog imbedded in main SCHED input file.

   0951+693          09 51 27.310784   * 09 55 33.173028     09 57 34.011941       0.00
 * M81               69 18 08.14400    * 69 03 55.06066      68 56 37.88915        0.00
                     From catalog imbedded in main SCHED input file.

 * 0954+658          09 54 57.847919   * 09 58 47.245099     10 00 40.121856       0.00
   0954+658          65 48 15.53881    * 65 33 54.81800      65 26 34.92000        0.00
                     From catalog imbedded in main SCHED input file.

 * 1005+066          10 05 23.466065   * 10 08 00.816158     10 09 18.357537       0.00
   1005+066          06 36 03.30794    * 06 21 21.21590      06 14 10.40452        0.00
                     From catalog imbedded in main SCHED input file.

 * 1005-333          10 05 18.612619   * 10 07 31.387436     10 08 36.407168       0.00
   1005-333         -33 18 25.03882    *-33 33 06.71624     -33 40 05.45730        0.00
                     From catalog imbedded in main SCHED input file.

 * 1013+127          10 13 03.644999   * 10 15 44.023389     10 17 03.047005       0.00
   1013+127          12 42 04.59776    * 12 27 07.07026      12 19 46.38766        0.00
                     From catalog imbedded in main SCHED input file.

 * 1022-665          10 22 13.388870   * 10 23 43.533218     10 24 25.718824       0.00
   1022-665         -66 31 34.81333    *-66 46 48.71706     -66 53 59.49951        0.00
                     From catalog imbedded in main SCHED input file.

 * 1039+811          10 39 27.760978   * 10 44 23.062556     10 46 44.569202       0.00
   1039+811          81 10 23.70042    * 80 54 39.44307      80 46 35.42155        0.00
                     From catalog imbedded in main SCHED input file.

 * 1045-188          10 45 40.093280   * 10 48 06.620620     10 49 18.417012       0.00
   1045-188         -18 53 44.08718    *-19 09 35.72681     -19 17 14.15400        0.00
                     From catalog imbedded in main SCHED input file.

 * 1055+018          10 55 55.313729   * 10 58 29.605206     10 59 45.364008       0.00
   1055+018          01 50 03.53735    * 01 33 58.82386      01 26 07.75514        0.00
                     From catalog imbedded in main SCHED input file.

 * 1102-242          11 02 19.807547   * 11 04 46.176443     11 05 57.744357       0.00
   1102-242         -24 15 13.81416    *-24 31 25.79949     -24 39 13.65824        0.00
                     From catalog imbedded in main SCHED input file.

 * 1115-122          11 15 46.125700   * 11 18 17.141380     11 19 31.088092       0.00
   1115-122         -12 16 29.65679    *-12 32 54.26177     -12 40 51.75435        0.00
                     From catalog imbedded in main SCHED input file.

 * 1124-186          11 24 34.018132   * 11 27 04.392457     11 28 17.915124       0.00
   1124-186         -18 40 46.35956    *-18 57 17.44164     -19 05 16.92741        0.00
                     From catalog imbedded in main SCHED input file.

 * 1125+221          11 25 12.775883   * 11 27 50.467256     11 29 07.840120       0.00
   1125+221          22 10 06.11988    * 21 53 34.80646      21 45 24.10331        0.00
                     From catalog imbedded in main SCHED input file.

 * 1128+385          11 28 12.513444   * 11 30 53.282613     11 32 12.120360       0.00
   1128+385          38 31 51.62101    * 38 15 18.54678      38 07 02.25913        0.00
                     From catalog imbedded in main SCHED input file.

 * 1133-032          11 33 51.244608   * 11 36 24.576932     11 37 39.669494       0.00
   1133-032         -03 13 53.26989    *-03 30 29.49654     -03 38 35.59608        0.00
                     From catalog imbedded in main SCHED input file.

 * 1140+668          11 40 55.894824   * 11 43 41.603326     11 45 02.164715       0.00
   1140+668          66 50 10.06445    * 66 33 31.22967      66 25 05.45516        0.00
                     From catalog imbedded in main SCHED input file.

 * 1143-696          11 43 31.954236   * 11 45 53.624206     11 47 00.186763       0.00
   1143-696         -69 37 21.59645    *-69 54 01.79753     -70 02 01.22361        0.00
                     From catalog imbedded in main SCHED input file.

 * 1144+402          11 44 21.020895   * 11 46 58.297907     11 48 15.323184       0.00
   1144+402          40 15 14.23954    * 39 58 34.30446      39 50 14.38907        0.00
                     From catalog imbedded in main SCHED input file.

 * 1147+245          11 47 44.000025   * 11 50 19.212177     11 51 35.265319       0.00
   1147+245          24 34 34.65386    * 24 17 53.83528      24 09 37.76163        0.00
                     From catalog imbedded in main SCHED input file.

 * 1156+295          11 56 57.786208   * 11 59 31.833908     12 00 47.265237       0.00
   1156+295          29 31 25.73880    * 29 14 43.82690      29 06 25.93537        0.00
                     From catalog imbedded in main SCHED input file.

 * 1208+186          12 08 33.885024   * 12 11 06.688276     12 12 21.473907       0.00
   1208+186          18 37 15.35602    * 18 20 34.28321      18 12 19.66573        0.00
                     From catalog imbedded in main SCHED input file.

 * 1215+303          12 15 21.141962   * 12 17 52.081964     12 19 05.904288       0.00
   1215+303          30 23 39.93993    * 30 07 00.63592      29 58 43.99292        0.00
                     From catalog imbedded in main SCHED input file.

 * 1215-002          12 15 24.936329   * 12 17 58.729045     12 19 13.921104       0.00
   1215-002         -00 13 06.85464    *-00 29 46.29968     -00 37 55.70725        0.00
                     From catalog imbedded in main SCHED input file.

 * 1222+037          12 22 19.097173   * 12 24 52.421939     12 26 07.382129       0.00
   1222+037          03 47 27.06586    * 03 30 50.29271      03 22 41.18977        0.00
                     From catalog imbedded in main SCHED input file.

   1222+131          12 22 31.582017   * 12 25 03.743334     12 26 18.158294       0.00
 * M84               13 09 49.76843    * 12 53 13.13904      12 45 01.98514        0.00
                     From catalog imbedded in main SCHED input file.

 * 1227+587          12 27 47.106409   * 12 30 07.057263     12 31 15.011076       0.00
   1227+587          58 46 41.60244    * 58 30 07.76265      58 21 47.66967        0.00
                     From catalog imbedded in main SCHED input file.

   1228+126          12 28 17.569276   * 12 30 49.423378     12 32 03.667453       0.00
 * 3C274             12 40 01.74890    * 12 23 28.04373      12 15 18.41207        0.00
                     From catalog imbedded in main SCHED input file.

 * 1244-255          12 44 06.713930   * 12 46 46.802044     12 48 04.762189       0.00
   1244-255         -25 31 26.67465    *-25 47 49.28899     -25 55 47.03631        0.00
                     From catalog imbedded in main SCHED input file.

 * 1307-556          13 07 40.422354   * 13 10 43.355594     13 12 11.601126       0.00
   1307-556         -55 36 14.46673    *-55 52 11.52940     -55 59 56.31914        0.00
                     From catalog imbedded in main SCHED input file.

 * 1308+328          13 08 38.495361   * 13 10 59.402728     13 12 08.082608       0.00
   1308+328          32 49 30.23282    * 32 33 34.44950      32 25 39.60581        0.00
                     From catalog imbedded in main SCHED input file.

 * 1308+471          13 08 41.327140   * 13 10 53.591577     13 11 57.849618       0.00
   1308+471          47 09 47.97624    * 46 53 52.22050      46 45 54.63464        0.00
                     From catalog imbedded in main SCHED input file.

 * 1312-533          13 12 01.988093   * 13 15 04.181113     13 16 32.184328       0.00
   1312-533         -53 18 44.65392    *-53 34 35.87450     -53 42 18.12717        0.00
                     From catalog imbedded in main SCHED input file.

 * 1325+126          13 25 26.389373   * 13 27 54.683000     13 29 07.021388       0.00
   1325+126          12 38 40.39063    * 12 23 09.17831      12 15 30.19066        0.00
                     From catalog imbedded in main SCHED input file.

 * 1331-195          13 31 02.012301   * 13 33 45.175689     13 35 04.650620       0.00
   1331-195         -19 35 20.46463    *-19 50 42.34341     -19 58 12.91028        0.00
                     From catalog imbedded in main SCHED input file.

 * 1334-127          13 34 59.803875   * 13 37 39.782780     13 38 57.752642       0.00
   1334-127         -12 42 09.74298    *-12 57 24.69325     -13 04 52.59459        0.00
                     From catalog imbedded in main SCHED input file.

 * 1343+537          13 43 51.697817   * 13 45 45.355236     13 46 40.181248       0.00
   1343+537          53 47 51.16049    * 53 32 52.28898      53 25 22.91530        0.00
                     From catalog imbedded in main SCHED input file.

 * 1351-018          13 51 32.032824   * 13 54 06.895328     13 55 22.393493       0.00
   1351-018         -01 51 20.07679    *-02 06 03.19029     -02 13 16.83246        0.00
                     From catalog imbedded in main SCHED input file.

 * 1352+757          13 52 53.318626   * 13 53 23.168061     13 53 35.594921       0.00
   1352+757          75 47 39.90464    * 75 32 57.73559      75 25 32.86324        0.00
                     From catalog imbedded in main SCHED input file.

 * 1354+195          13 54 42.085877   * 13 57 04.436646     13 58 13.781981       0.00
   1354+195          19 33 43.95868    * 19 19 07.37266      19 11 54.49780        0.00
                     From catalog imbedded in main SCHED input file.

 * 1405-287          14 05 56.389393   * 14 08 49.613749     14 10 13.897047       0.00
   1405-287         -28 46 12.19729    *-29 00 23.60812     -29 07 20.56589        0.00
                     From catalog imbedded in main SCHED input file.

 * 1417+273          14 17 45.094583   * 14 19 59.297069     14 21 04.552490       0.00
   1417+273          27 20 09.10596    * 27 06 25.55273      26 59 38.29236        0.00
                     From catalog imbedded in main SCHED input file.

 * 1435+638          14 35 37.240716   * 14 36 45.802264     14 37 17.872962       0.00
   1435+638          63 49 35.86059    * 63 36 37.86693      63 30 08.86345        0.00
                     From catalog imbedded in main SCHED input file.

   1458+718          14 58 56.613452   * 14 59 07.583957     14 59 10.699097       0.00
 * 3C309.1           71 52 11.18790    * 71 40 19.86642      71 34 23.19977        0.00
                     From catalog imbedded in main SCHED input file.

 * 1459+480          14 59 07.241803   * 15 00 48.654219     15 01 37.398949       0.00
   1459+480          48 03 04.02867    * 47 51 15.53805      47 45 24.25113        0.00
                     From catalog imbedded in main SCHED input file.

 * 1502+106          15 02 00.157712   * 15 04 24.979781     15 05 35.500956       0.00
   1502+106          10 41 17.74006    * 10 29 39.19864      10 23 55.42941        0.00
                     From catalog imbedded in main SCHED input file.

 * 1509+022          15 09 43.818072   * 15 12 15.741745     15 13 29.767279       0.00
   1509+022          02 14 30.75205    * 02 03 16.97914      01 57 45.53870        0.00
                     From catalog imbedded in main SCHED input file.

 * 1510-089          15 10 08.900183   * 15 12 50.532931     15 14 09.314922       0.00
   1510-089         -08 54 47.61945    *-09 05 59.82960     -09 11 30.64450        0.00
                     From catalog imbedded in main SCHED input file.

 * 1511-476          15 11 11.447387   * 15 14 40.024607     15 16 21.375315       0.00
   1511-476         -47 37 22.13997    *-47 48 29.85762     -47 54 00.42564        0.00
                     From catalog imbedded in main SCHED input file.

 * 1514-241          15 14 45.267394   * 15 17 41.813142     15 19 07.833423       0.00
   1514-241         -24 11 22.67803    *-24 22 19.47598     -24 27 43.45041        0.00
                     From catalog imbedded in main SCHED input file.

 * 1530-536          15 30 33.938967   * 15 34 20.660670     15 36 10.794906       0.00
   1530-536         -53 41 11.72354    *-53 51 13.42290     -53 56 13.04402        0.00
                     From catalog imbedded in main SCHED input file.

 * 1532+016          15 32 20.172139   * 15 34 52.453673     15 36 06.666931       0.00
   1532+016          01 41 01.64847    * 01 31 04.20662      01 26 10.32134        0.00
                     From catalog imbedded in main SCHED input file.

 * 1546+027          15 46 58.292176   * 15 49 29.436850     15 50 43.102680       0.00
   1546+027          02 46 06.07602    * 02 37 01.16337      02 32 33.21337        0.00
                     From catalog imbedded in main SCHED input file.

 * 1557+032          15 57 00.361035   * 15 59 30.972614     16 00 44.386539       0.00
   1557+032          03 13 15.85207    * 03 04 48.25686      03 00 38.74927        0.00
                     From catalog imbedded in main SCHED input file.

 * 1600+335          16 00 11.909360   * 16 02 07.263489     16 03 03.102657       0.00
   1600+335          33 35 09.59402    * 33 26 53.07371      33 22 49.95001        0.00
                     From catalog imbedded in main SCHED input file.

 * 1619-680          16 19 13.497235   * 16 24 18.437068     16 26 46.518672       0.00
   1619-680         -68 02 15.80516    *-68 09 12.49572     -68 12 44.44848        0.00
                     From catalog imbedded in main SCHED input file.

 * 1637+574          16 37 17.425184   * 16 38 13.456299     16 38 39.412912       0.00
   1637+574          57 26 15.76138    * 57 20 23.97909      57 17 32.91108        0.00
                     From catalog imbedded in main SCHED input file.

 * 1642+690          16 42 18.064912   * 16 42 07.848542     16 42 00.318209       0.00
   1642+690          69 02 13.21690    * 68 56 39.75619      68 53 55.95785        0.00
                     From catalog imbedded in main SCHED input file.

 * 1655+077          16 55 43.951806   * 16 58 09.011463     16 59 19.779214       0.00
   1655+077          07 45 59.75728    * 07 41 27.54063      07 39 15.02967        0.00
                     From catalog imbedded in main SCHED input file.

 * 1657+265          16 57 22.517644   * 16 59 24.149456     17 00 23.232366       0.00
   1657+265          26 34 03.01799    * 26 29 36.94315      26 27 29.42258        0.00
                     From catalog imbedded in main SCHED input file.

 * 1659-621          16 59 00.275387   * 17 03 36.541209     17 05 51.114898       0.00
   1659-621         -62 08 26.03822    *-62 12 40.00846     -62 14 53.87869        0.00
                     From catalog imbedded in main SCHED input file.

 * 1706-174          17 06 40.093173   * 17 09 34.345385     17 10 59.535879       0.00
   1706-174         -17 25 08.43141    *-17 28 53.36472     -17 30 46.55922        0.00
                     From catalog imbedded in main SCHED input file.

 * 1721-146          17 21 55.862150   * 17 24 46.966547     17 26 10.664426       0.00
   1721-146         -14 41 20.21290    *-14 43 59.76071     -14 45 20.38215        0.00
                     From catalog imbedded in main SCHED input file.

 * 1722+119          17 22 44.449755   * 17 25 04.340900     17 26 12.606564       0.00
   1722+119          11 54 52.59041    * 11 52 15.47161      11 51 00.77133        0.00
                     From catalog imbedded in main SCHED input file.

 * 1725+044          17 25 56.336678   * 17 28 24.952730     17 29 37.563760       0.00
   1725+044          04 29 27.90723    * 04 27 04.91391      04 25 56.04027        0.00
                     From catalog imbedded in main SCHED input file.

 * 1726+455          17 26 01.198760   * 17 27 27.650814     17 28 09.087648       0.00
   1726+455          45 33 04.55112    * 45 30 39.73127      45 29 34.13420        0.00
                     From catalog imbedded in main SCHED input file.

   1730-130          17 30 13.535193   * 17 33 02.705791     17 34 25.482240       0.00
 * NRAO530          -13 02 45.83958    *-13 04 49.54805     -13 05 52.23317        0.00
                     From catalog imbedded in main SCHED input file.

 * 1741-038          17 41 20.616010   * 17 43 58.856134     17 45 16.281801       0.00
   1741-038         -03 48 48.89993    *-03 50 04.61673     -03 50 41.74685        0.00
                     From catalog imbedded in main SCHED input file.

 * 1743+173          17 43 22.235909   * 17 45 35.208177     17 46 40.081869       0.00
   1743+173          17 21 09.18646    * 17 20 01.42378      17 19 32.12499        0.00
                     From catalog imbedded in main SCHED input file.

 * 1749+096          17 49 10.387933   * 17 51 32.818576     17 52 42.427110       0.00
   1749+096          09 39 42.82591    * 09 39 00.72846      09 38 42.92238        0.00
                     From catalog imbedded in main SCHED input file.

 * 1749+701          17 49 03.391243   * 17 48 32.840348     17 48 14.983834       0.00
   1749+701          70 06 39.62691    * 70 05 50.76884      70 05 31.29385        0.00
                     From catalog imbedded in main SCHED input file.

 * 1803+784          18 03 39.193558   * 18 00 45.683935     17 59 15.037963       0.00
   1803+784          78 27 54.29752    * 78 28 04.01846      78 28 10.03774        0.00
                     From catalog imbedded in main SCHED input file.

 * 1803-642          18 03 01.845012   * 18 07 54.032752     18 10 16.778352       0.00
   1803-642         -64 14 13.96902    *-64 13 50.11399     -64 13 50.10499        0.00
                     From catalog imbedded in main SCHED input file.

 * 1821+107          18 21 41.659106   * 18 24 02.855256     18 25 11.962485       0.00
   1821+107          10 42 43.89925    * 10 44 23.77414      10 45 16.90550        0.00
                     From catalog imbedded in main SCHED input file.

 * 1824-582          18 24 51.388720   * 18 29 12.402375     18 31 20.217418       0.00
   1824-582         -58 15 53.07866    *-58 13 55.16195     -58 13 09.04156        0.00
                     From catalog imbedded in main SCHED input file.

 * 1825-214          18 25 19.680580   * 18 28 19.487022     18 29 47.721440       0.00
   1825-214         -21 25 35.81986    *-21 23 38.76943     -21 22 45.04959        0.00
                     From catalog imbedded in main SCHED input file.

 * 1830-211          18 30 40.596669   * 18 33 39.886597     18 35 07.892760       0.00
   1830-211         -21 06 00.77989    *-21 03 40.55158     -21 02 35.34543        0.00
                     From catalog imbedded in main SCHED input file.

 * 1839+548          18 39 56.969500   * 18 40 57.376699     18 41 25.822899       0.00
   1839+548          54 49 19.91805    * 54 52 15.91045      54 53 52.66886        0.00
                     From catalog imbedded in main SCHED input file.

 * 1849+670          18 49 16.505884   * 18 49 16.072296     18 49 13.567439       0.00
   1849+670          67 02 07.88053    * 67 05 41.68027      67 07 36.50583        0.00
                     From catalog imbedded in main SCHED input file.

 * 1855+031          18 55 32.171131   * 18 58 02.352752     18 59 16.074619       0.00
   1855+031          03 09 10.49478    * 03 13 16.30095      03 15 20.29611        0.00
                     From catalog imbedded in main SCHED input file.

   1901+319          19 01 02.310070   * 19 02 55.938906     19 03 51.379983       0.00
 * 3C395             31 55 13.94308    * 31 59 41.70188      32 02 02.97469        0.00
                     From catalog imbedded in main SCHED input file.

 * 1903-802          19 03 56.022239   * 19 12 40.019094     19 16 54.641020       0.00
   1903-802         -80 15 00.26076    *-80 10 05.94649     -80 07 51.89822        0.00
                     From catalog imbedded in main SCHED input file.

 * 1904+013          19 04 39.788390   * 19 07 11.996148     19 08 26.767556       0.00
   1904+013          01 22 24.59959    * 01 27 08.96157      01 29 31.65901        0.00
                     From catalog imbedded in main SCHED input file.

 * 1914-154          19 14 01.353758   * 19 16 52.510995     19 18 16.726064       0.00
   1914-154         -15 24 24.09370    *-15 19 00.07148     -15 16 22.56983        0.00
                     From catalog imbedded in main SCHED input file.

 * 1921-293          19 21 42.234129   * 19 24 51.055956     19 26 24.027323       0.00
   1921-293         -29 20 26.35392    *-29 14 30.12101     -29 11 40.88426        0.00
                     From catalog imbedded in main SCHED input file.

 * 1937-101          19 37 12.649215   * 19 39 57.256596     19 41 18.351160       0.00
   1937-101         -10 09 39.45603    *-10 02 41.51998     -09 59 15.86182        0.00
                     From catalog imbedded in main SCHED input file.

 * 1949-052          19 49 08.265953   * 19 51 47.468456     19 53 05.942002       0.00
   1949-052         -05 17 28.53351    *-05 09 43.96252     -05 05 53.59428        0.00
                     From catalog imbedded in main SCHED input file.

 * 1951+355          19 51 39.207549   * 19 53 30.875713     19 54 25.540541       0.00
   1951+355          35 30 06.66614    * 35 37 59.35909      35 42 04.30999        0.00
                     From catalog imbedded in main SCHED input file.

 * 2008+355          20 08 04.366586   * 20 09 57.637624     20 10 53.185502       0.00
   2008+355          35 34 23.23414    * 35 43 18.00164      35 47 54.19198        0.00
                     From catalog imbedded in main SCHED input file.

 * 2008-159          20 08 25.916565   * 20 11 15.710927     20 12 39.557578       0.00
   2008-159         -15 55 38.19529    *-15 46 40.25367     -15 42 16.84829        0.00
                     From catalog imbedded in main SCHED input file.

 * 2021+222          20 21 11.678133   * 20 23 23.160238     20 24 27.938839       0.00
   2021+222          22 14 09.57701    * 22 23 52.52512      22 28 50.03514        0.00
                     From catalog imbedded in main SCHED input file.

 * 2029+024          20 29 15.845182   * 20 31 47.251109     20 33 02.055913       0.00
   2029+024          02 29 25.37984    * 02 39 37.28370      02 44 43.60155        0.00
                     From catalog imbedded in main SCHED input file.

 * 2033-219          20 33 56.507209   * 20 36 51.172714     20 38 17.599118       0.00
   2033-219         -21 57 05.44776    *-21 46 36.75050     -21 41 30.21406        0.00
                     From catalog imbedded in main SCHED input file.

   2037+511          20 37 07.456975   * 20 38 37.034730     20 39 20.732204       0.00
 * 3C418             51 08 35.76941    * 51 19 12.66244      51 24 42.35349        0.00
                     From catalog imbedded in main SCHED input file.

 * 2037-253          20 37 10.764884   * 20 40 08.772939     20 41 36.882247       0.00
   2037-253         -25 18 26.42638    *-25 07 46.66344     -25 02 35.74460        0.00
                     From catalog imbedded in main SCHED input file.

 * 2052+239          20 52 17.408380   * 20 54 29.533078     20 55 34.792759       0.00
   2052+239          23 56 05.92344    * 24 07 33.76528      24 13 24.31197        0.00
                     From catalog imbedded in main SCHED input file.

 * 2100+468          21 00 33.500109   * 21 02 17.056017     21 03 07.950241       0.00
   2100+468          46 50 23.37626    * 47 02 16.25323      47 08 23.76558        0.00
                     From catalog imbedded in main SCHED input file.

 * 2105+551          21 05 10.049437   * 21 06 37.538883     21 07 20.315183       0.00
   2105+551          55 08 35.24905    * 55 20 41.71604      55 26 56.84092        0.00
                     From catalog imbedded in main SCHED input file.

 * 2109-811          21 09 15.848370   * 21 16 30.845745     21 20 03.982931       0.00
   2109-811         -81 06 22.79281    *-80 53 55.22339     -80 48 01.51981        0.00
                     From catalog imbedded in main SCHED input file.

 * 2112+463          21 12 45.769652   * 21 14 32.875663     21 15 25.628872       0.00
   2112+463          46 22 09.87653    * 46 34 39.30172      46 41 05.12862        0.00
                     From catalog imbedded in main SCHED input file.

 * 2112-144          21 12 33.295355   * 21 15 18.435559     21 16 40.364510       0.00
   2112-144         -14 29 13.80392    *-14 16 43.37224     -14 10 33.46434        0.00
                     From catalog imbedded in main SCHED input file.

 * 2118+443          21 18 40.227957   * 21 20 31.774277     21 21 26.802292       0.00
   2118+443          44 21 47.83775    * 44 34 34.26272      44 41 08.35431        0.00
                     From catalog imbedded in main SCHED input file.

 * 2123-463          21 23 13.267464   * 21 26 30.704254     21 28 08.862649       0.00
   2123-463         -46 18 49.25142    *-46 05 47.89196     -45 59 32.90888        0.00
                     From catalog imbedded in main SCHED input file.

 * 2126-158          21 26 26.777518   * 21 29 12.175885     21 30 34.325840       0.00
   2126-158         -15 51 50.34789    *-15 38 41.04172     -15 32 12.10255        0.00
                     From catalog imbedded in main SCHED input file.

 * 2128-123          21 28 52.676078   * 21 31 35.261769     21 32 56.016280       0.00
   2128-123         -12 20 20.53541    *-12 07 04.79580     -12 00 31.40771        0.00
                     From catalog imbedded in main SCHED input file.

   2134+004          21 34 05.207441   * 21 36 38.586376     21 37 54.748604       0.00
 * 2134+00           00 28 25.07968    * 00 41 54.21251      00 48 38.65882        0.00
                     From catalog imbedded in main SCHED input file.

 * 2146+608          21 46 48.097291   * 21 48 16.042192     21 48 59.292518       0.00
   2146+608          60 53 06.64176    * 61 07 05.79336      61 14 17.84394        0.00
                     From catalog imbedded in main SCHED input file.

   2149-307          21 49 00.594066   * 21 51 55.523969     21 53 22.635981       0.00
 * 2149-306         -30 42 00.13432    *-30 27 53.69797     -30 21 01.01581        0.00
                     From catalog imbedded in main SCHED input file.

   2200+420          22 00 39.362501   * 22 02 43.291368     22 03 44.797044       0.00
 * VR422201          42 02 08.59076    * 42 16 39.97989      42 24 06.30402        0.00
                     From catalog imbedded in main SCHED input file.

 * 2201+315          22 01 01.441985   * 22 03 14.975776     22 04 21.309209       0.00
   2201+315          31 31 05.87489    * 31 45 38.26982      31 53 03.12363        0.00
                     From catalog imbedded in main SCHED input file.

 * 2204-540          22 04 26.258614   * 22 07 43.733303     22 09 22.418915       0.00
   2204-540         -54 01 14.91305    *-53 46 33.81987     -53 39 30.53914        0.00
                     From catalog imbedded in main SCHED input file.

 * 2208-137          22 08 42.863975   * 22 11 24.099450     22 12 44.437043       0.00
   2208-137         -13 42 58.83306    *-13 28 09.72394     -13 20 49.68062        0.00
                     From catalog imbedded in main SCHED input file.

 * 2211+374          22 11 55.008214   * 22 14 05.694861     22 15 10.660576       0.00
   2211+374          37 24 14.44252    * 37 39 09.19626      37 46 46.39486        0.00
                     From catalog imbedded in main SCHED input file.

 * 2216-038          22 16 16.381738   * 22 18 52.037727     22 20 09.595849       0.00
   2216-038         -03 50 40.62409    *-03 35 36.87918     -03 28 06.14327        0.00
                     From catalog imbedded in main SCHED input file.

 * 2227-088          22 27 02.336855   * 22 29 40.084333     22 30 58.770848       0.00
   2227-088         -08 48 17.57645    *-08 32 54.43563     -08 25 15.45412        0.00
                     From catalog imbedded in main SCHED input file.

 * 2233-148          22 33 53.979695   * 22 36 34.087156     22 37 54.025395       0.00
   2233-148         -14 48 56.65510    *-14 33 22.18973     -14 25 39.37511        0.00
                     From catalog imbedded in main SCHED input file.

 * 2233-234          22 33 42.046275   * 22 36 26.238709     22 37 48.273078       0.00
   2233-234         -23 25 00.84105    *-23 09 26.59721     -23 01 46.70415        0.00
                     From catalog imbedded in main SCHED input file.

 * 2243-123          22 43 39.792806   * 22 46 18.231968     22 47 37.382333       0.00
   2243-123         -12 22 40.29418    *-12 06 51.27808     -11 59 00.19302        0.00
                     From catalog imbedded in main SCHED input file.

 * 2255-282          22 55 22.460644   * 22 58 05.962877     22 59 27.848037       0.00
   2255-282         -28 14 25.61865    *-27 58 21.25664     -27 50 27.20313        0.00
                     From catalog imbedded in main SCHED input file.

 * 2309+454          23 09 28.211643   * 23 11 47.408970     23 12 57.017432       0.00
   2309+454          45 27 37.24971    * 45 43 56.01645      45 52 16.02576        0.00
                     From catalog imbedded in main SCHED input file.

 * 2319+317          23 19 28.286856   * 23 21 54.955984     23 23 08.307802       0.00
   2319+317          31 47 40.33722    * 32 04 07.62251      32 12 29.71984        0.00
                     From catalog imbedded in main SCHED input file.

 * 2320-035          23 20 57.525164   * 23 23 31.953751     23 24 49.257908       0.00
   2320-035         -03 33 33.63627    *-03 17 05.02388     -03 08 50.66644        0.00
                     From catalog imbedded in main SCHED input file.

 * 2344-514          23 44 40.998162   * 23 47 19.864109     23 48 40.379191       0.00
   2344-514         -51 27 16.60469    *-51 10 36.06529     -51 02 28.01799        0.00
                     From catalog imbedded in main SCHED input file.

 * 2345+061          23 45 58.408171   * 23 48 31.770666     23 49 48.618832       0.00
   2345+061          06 08 19.20781    * 06 24 59.78188      06 33 23.10331        0.00
                     From catalog imbedded in main SCHED input file.

 * 2351-154          23 51 55.881457   * 23 54 30.195174     23 55 47.696516       0.00
   2351-154         -15 29 53.02145    *-15 13 11.21294     -15 04 52.66773        0.00
                     From catalog imbedded in main SCHED input file.

 * 2356+385          23 56 59.812462   * 23 59 33.180790     00 00 50.116868       0.00
   2356+385          38 34 00.40168    * 38 50 42.31837      38 59 12.28855        0.00
                     From catalog imbedded in main SCHED input file.

 * 2357-318          23 57 01.415960   * 23 59 35.491545     00 00 53.140404       0.00
   2357-318         -31 50 26.12867    *-31 33 43.82451     -31 25 29.15053        0.00
                     From catalog imbedded in main SCHED input file.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  0002-478   sess324.K2048globgeo  1 4 5 6 13 15                     0.401     0.252
  0003-066   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 14 15 +     0.815     0.540
  0009-148   sess324.K2048globgeo  1 3 4 5 6 7 9 11 12 13 15 2 +     1.104     0.638
  0013-005   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 14 15 +     0.926     0.639
  0017+257   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 15 +     0.819     0.473
  0039+568   sess324.K2048globgeo  1 3 7 8 9 11 12 14 15 21 25 +     1.308     0.703
  0041+677   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.992     1.540
  0044+566   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.903     1.936
  0104-408   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.644     0.720
  0109+224   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.187     0.969
  0109+351   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.324     7.221
  0111+021   sess324.K2048globgeo  1 3 4 5 6 8 9 11 12 13 14 1 +     1.313     1.127
  0148-177   sess324.K2048globgeo  1 4 5 6 9 11 13 14 15 21          0.777     0.576
  0159-668   sess324.K2048globgeo  4 5 6                             0.186     0.119
  0202+149   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.438     1.151
  0213-026   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.087     0.596
  0219+628   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.979     2.209
  0229-479   sess324.K2048globgeo  4 5 6 15                          0.346     0.313
  0235+164   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.365     0.940
  0235-618   sess324.K2048globgeo  4 5 6                             0.246     0.246
  0250+320   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 14 15 2 +     0.918     0.832
  0251+393   sess324.K2048globgeo  1 3 4 5 7 8 9 11 12 13 14 1 +     2.595     1.785
  0302-623   sess324.K2048globgeo  4 5 6                             0.176     0.105
  0308-611   sess324.K2048globgeo  4 5 6                             0.089     0.056
  0322-294   sess324.K2048globgeo  1 3 4 5 6 7 9 11 13 14 15 2 +     0.636     0.901
  NRAO140    sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.199     0.744
  CTA26      sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.056     0.493
  0344+558   sess324.K2048globgeo  1 3 7 8 9 11 12 14 15 21 25       1.595     0.855
  0346+800   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 25 +     2.805     2.683
  0350+465   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.548     0.793
  0358+040   sess324.K2048globgeo  1 4 6 7 8 9 11 12 13 14 15  +     1.048     0.484
  0401-248   sess324.K2048globgeo  1 3 4 5 6 7 9 11 12 13 14 1 +     0.728     0.371
  0402-362   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.263     0.231
  0414-189   sess324.K2048globgeo  1 4 6 8 11 12 13 14 15 21 2 +     0.545     0.498
  0415+572   sess324.K2048globgeo  1 3 7 8 9 11 12 14 15 25 27       1.557     1.019
  0418+532   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.828     1.351
  3C119      sess324.K2048globgeo  1 3 4 5 6 8 9 11 12 13 14 1 +     1.479     0.507
  3C120      sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.103     6.593
  0444+634   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.616     7.194
  0446+112   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.842     0.646
  0454+550   sess324.K2048globgeo  1 3 7 8 9 11 12 14 15 21 25 +     0.936     1.017
  0454-234   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.791     0.476
  0454-810   sess324.K2048globgeo  4 5 6                             0.349     0.215
  0458-020   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.648     6.052
  0502+049   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.089     1.701
  0507+179   sess324.K2048globgeo  1 3 4 5 7 8 9 11 12 13 14 1 +     0.811     0.795
  0520-165   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 14 15 +     1.300     0.874
  0524+034   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     0.729     0.537
  0528+134   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.809     3.616
  0529+483   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.333     0.786
  0537-441   sess324.K2048globgeo  1 4 5 6 13 15                     0.285     0.251
  0547+234   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.227     0.436
  0600+177   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.459     0.730
  0607-157   sess324.K2048globgeo  1 4 5 6 7 9 11 12 14 15 21  +     0.624     0.520
  0615+820   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.214     2.114
  0622-645   sess324.K2048globgeo  4 5 6                             0.162     0.296
  0628+203   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     0.839     0.542
  0633+595   sess324.K2048globgeo  1 3 7 8 9 11 12 14 15 21 25       1.776     1.064
  0636+022   sess324.K2048globgeo  1 4 5 6 7 8 9 11 13 14 15 2 +     0.886     0.717
  0642+449   sess324.K2048globgeo  1 3 4 5 7 8 9 11 12 13 14 1 +     1.669    30.212
  0644-671   sess324.K2048globgeo  4 5 6                             0.253     0.160
  0721-071   sess324.K2048globgeo  1 5 7 8 9 11 12 13 14 15 25       0.584     0.944
  0725+219   sess324.K2048globgeo  1 3 5 6 7 8 9 11 12 14 15 2 +     1.139     0.459
  0727-115   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.814     0.514
  0731+050   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.929     0.427
  0736+017   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.841     0.500
  0738-674   sess324.K2048globgeo  4 5 6                             0.183     0.094
  0742-562   sess324.K2048globgeo  4 5 6                             0.185     0.103
  0743-247   sess324.K2048globgeo  1 4 6 11 13 14 15                 0.650     1.219
  0744-158   sess324.K2048globgeo  1 3 5 7 8 9 11 12 13 14 15  +     0.757     0.237
  0746+483   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.599     0.686
  0748+126   sess324.K2048globgeo  1 4 5 6 9 11 12 13 14 15 21 +     0.603     0.615
  0804+499   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 25 +     1.416     1.113
  0814-241   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.576     0.849
  0821+248   sess324.K2048globgeo  1 4 5 6 7 8 9 11 12 13 14 1 +     0.488     1.789
  0823+033   sess324.K2048globgeo  1 3 5 7 8 9 11 12 13 14 15  +     0.642     0.578
  0827+243   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.129     0.730
  0850+284   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.227     0.888
  OJ287      sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.819    14.382
  0859+470   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.380     1.283
  0859-140   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.620     0.442
  0901+697   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     3.341     3.497
  0922+364   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.842     0.926
  4C39.25    sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.251     1.285
  0925-203   sess324.K2048globgeo  1 3 4 5 6 11 13 14 15 21 25       0.416     0.455
  0928+144   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.249     1.151
  0951+268   sess324.K2048globgeo  1 3 5 7 8 9 11 12 14 15 25        0.932     0.246
  M81        sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.814     4.181
  0954+658   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     0.531    40.476
  1005+066   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.234     0.653
  1005-333   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.594     0.254
  1013+127   sess324.K2048globgeo  1 6 7 8 9 11 12 13 14 15 25       0.781     0.483
  1022-665   sess324.K2048globgeo  4 5 6                             0.217     0.195
  1039+811   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.116     1.869
  1045-188   sess324.K2048globgeo  1 3 4 5 6 9 11 15 21 25           0.405     0.249
  1055+018   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.928    12.012
  1102-242   sess324.K2048globgeo  1 4 6 11 13 14 15                 0.529     0.522
  1115-122   sess324.K2048globgeo  1 3 4 6 9 11 13 14 15 21 25       0.519     0.585
  1124-186   sess324.K2048globgeo  1 3 4 5 6 9 11 13 14 15 25        0.715     0.550
  1125+221   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.340     1.201
  1128+385   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.754     1.903
  1133-032   sess324.K2048globgeo  1 3 4 5 6 9 11 13 14 15 21  +     0.861     0.911
  1140+668   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.437     1.853
  1143-696   sess324.K2048globgeo  4 5 6                             0.426     0.476
  1144+402   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.238     1.791
  1147+245   sess324.K2048globgeo  1 4 6 7 8 9 11 12 13 14 15  +     0.969     0.418
  1156+295   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.090     0.544
  1208+186   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.492     0.880
  1215+303   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.010     0.605
  1215-002   sess324.K2048globgeo  1 4 5 6 8 9 11 12 13 14 15  +     1.014     0.404
  1222+037   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.881     1.014
  M84        sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.149     1.098
  1227+587   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.691     0.748
  3C274      sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.795     1.141
  1244-255   sess324.K2048globgeo  1 3 4 5 6 7 9 11 12 13 14 1 +     0.644     0.624
  1307-556   sess324.K2048globgeo  4 5 6                             0.224     0.136
  1308+328   sess324.K2048globgeo  1 3 5 7 8 9 11 12 13 14 15  +     0.998     0.498
  1308+471   sess324.K2048globgeo  9 15 25                           0.586     0.205
  1312-533   sess324.K2048globgeo  4 5 6                             0.074     0.041
  1325+126   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 15 +     1.016     0.831
  1331-195   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.833     1.285
  1334-127   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.744     0.921
  1343+537   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.036     0.545
  1351-018   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.792     1.450
  1352+757   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.296     1.354
  1354+195   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.444     0.625
  1405-287   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.676     0.671
  1417+273   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 14 15 +     0.901     0.354
  1435+638   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     3.148     3.238
  3C309.1    sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.534     1.425
  1459+480   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.165     0.533
  1502+106   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.121     0.786
  1509+022   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.579     3.042
  1510-089   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.766     0.380
  1511-476   sess324.K2048globgeo  4 5 6 13 15                       0.339     0.147
  1514-241   sess324.K2048globgeo  1 4 6 11 13 15                    0.374     0.534
  1530-536   sess324.K2048globgeo  4 5 6                             0.225     0.139
  1532+016   sess324.K2048globgeo  1 4 5 6 7 8 9 11 12 13 14 1 +     1.098     0.739
  1546+027   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.732     9.490
  1557+032   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.736     0.557
  1600+335   sess324.K2048globgeo  1 7 8 9 11 12 13 14 15 25         1.139     0.519
  1619-680   sess324.K2048globgeo  4 5 6                             0.329     0.195
  1637+574   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.186     1.034
  1642+690   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.486     1.846
  1655+077   sess324.K2048globgeo  1 4 5 6 7 8 9 11 12 13 14 1 +     1.109     0.784
  1657+265   sess324.K2048globgeo  1 3 4 6 11 12 13 14 15 21 2 +     0.891     0.723
  1659-621   sess324.K2048globgeo  4 5 6                             0.289     0.171
  1706-174   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.860     0.586
  1721-146   sess324.K2048globgeo  1 3 4 5 6 7 9 11 13 14 15 2 +     0.722     0.805
  1722+119   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.469     1.032
  1725+044   sess324.K2048globgeo  1 4 5 6 7 8 9 11 12 13 14 1 +     0.666     0.905
  1726+455   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.003     1.299
  NRAO530    sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.618     0.543
  1741-038   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.509     0.222
  1743+173   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.854     0.496
  1749+096   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.932     0.505
  1749+701   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.688     1.693
  1803+784   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.205     2.386
  1803-642   sess324.K2048globgeo  4 5 6                             0.233     0.129
  1821+107   sess324.K2048globgeo  1 3 4 6 9 11 12 15 21 25          0.684     0.812
  1824-582   sess324.K2048globgeo  4 5 6                             0.215     0.115
  1825-214   sess324.K2048globgeo  1 4 6 11 13 14 15                 0.708     0.409
  1830-211   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 14 15 +     0.534     0.229
  1839+548   sess324.K2048globgeo  1 3 7 8 9 11 12 14 15 21 25       1.319     1.150
  1849+670   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     2.033     1.987
  1855+031   sess324.K2048globgeo  1 3 4 6 8 9 11 12 15 25           0.749     0.614
  3C395      sess324.K2048globgeo  1 4 5 6 8 11 12 13 14 15 25       0.541     0.714
  1903-802   sess324.K2048globgeo  4 5 6                             0.440     0.264
  1904+013   sess324.K2048globgeo  1 3 5 6 7 8 9 11 12 13 14 1 +     0.850     0.364
  1914-154   sess324.K2048globgeo  1 4 5 6 9 11 12 13 14 15 25       0.799     0.727
  1921-293   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.322     0.954
  1937-101   sess324.K2048globgeo  1 3 5 6 7 8 9 11 12 13 14 1 +     1.032     0.374
  1949-052   sess324.K2048globgeo  1 4 5 6 7 8 9 11 12 13 14 1 +     0.980     0.660
  1951+355   sess324.K2048globgeo  1 4 6 8 11 12 13 15 25            0.863     0.634
  2008+355   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     0.773     0.886
  2008-159   sess324.K2048globgeo  1 4 5 6 8 9 11 12 14 15 25        0.486     0.352
  2021+222   sess324.K2048globgeo  1 3 5 7 8 9 11 12 14 15 21  +     1.349     0.371
  2029+024   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.665     0.633
  2033-219   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.630     0.691
  3C418      sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     0.554    14.842
  2037-253   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.489     0.482
  2052+239   sess324.K2048globgeo  1 3 5 6 7 8 9 11 12 13 14 1 +     1.776     0.886
  2100+468   sess324.K2048globgeo  1 7 8 9 11 13 14 15               0.470     0.950
  2105+551   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.840     1.467
  2109-811   sess324.K2048globgeo  4 5 6                             0.408     0.219
  2112+463   sess324.K2048globgeo  1 3 7 8 9 11 12 15 21 25          1.019     0.736
  2112-144   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.100     0.401
  2118+443   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     1.053     1.324
  2123-463   sess324.K2048globgeo  1 4 5 6 13 15                     0.294     0.191
  2126-158   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.568     0.541
  2128-123   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 14 15 2 +     0.801     0.411
  2134+00    sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.773     0.406
  2146+608   sess324.K2048globgeo  1 3 7 8 9 11 12 13 14 15 21 +     3.078     4.275
  2149-306   sess324.K2048globgeo  1 4 5 6 13 14 15                  0.371     0.508
  VR422201   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.306    15.013
  2201+315   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.546     0.826
  2204-540   sess324.K2048globgeo  4 5 6 15                          0.297     0.474
  2208-137   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 13 14 15 +     0.902     1.181
  2211+374   sess324.K2048globgeo  1 3 5 7 8 9 11 12 13 14 15  +     1.170     0.769
  2216-038   sess324.K2048globgeo  1 4 6 8 9 11 12 13 14 15 21 +     0.515     0.579
  2227-088   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     0.706     0.805
  2233-148   sess324.K2048globgeo  1 4 6 7 8 9 11 12 13 14 15  +     0.510     0.626
  2233-234   sess324.K2048globgeo  1 4 5 6 11 14 15                  0.657     1.166
  2243-123   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.400     0.817
  2255-282   sess324.K2048globgeo  1 4 5 6 9 11 13 14 15             0.534     0.350
  2309+454   sess324.K2048globgeo  1 3 4 6 7 8 9 11 12 13 14 1 +     1.718     2.162
  2319+317   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     2.258     1.872
  2320-035   sess324.K2048globgeo  1 4 5 6 7 8 9 11 12 13 14 1 +     0.596     0.502
  2344-514   sess324.K2048globgeo  4 5 6 15                          0.290     0.080
  2345+061   sess324.K2048globgeo  1 4 5 6 7 8 9 11 12 13 14 1 +     1.029     0.565
  2351-154   sess324.K2048globgeo  1 3 4 5 6 7 8 9 11 12 13 14 +     1.060     0.278
  2356+385   sess324.K2048globgeo  1 3 5 7 8 9 11 12 13 14 15  +     1.366     0.944
  2357-318   sess324.K2048globgeo  1 4 5 6 11 13 14 15               0.704     0.471


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0002-478           108.9
   0003-066           137.4
   0009-148           133.8
   0013-005           142.5
   0017+257           146.7
   0039+568           133.0
   0041+677           124.2
   0044+566           133.5
   0104-408           120.7
   0109+224           159.1
   0109+351           152.6
   0111+021           156.3
   0148-177           145.6
   0159-668            98.0
   0202+149           172.8
   0213-026           161.9
   0219+628           132.0
   0229-479           117.1
   0235+164           178.2
   0235-618           103.2
   0250+320           162.3
   0251+393           155.2
   0302-623           102.4
   0308-611           103.5
   0322-294           133.9
   NRAO140            157.8
   CTA26              156.7
   0344+558           136.8
   0346+800           114.4
   0350+465           144.3
   0358+040           156.0
   0401-248           134.6
   0402-362           124.6
   0414-189           137.7
   0415+572           133.4
   0418+532           136.2
   3C119              143.3
   3C120              149.3
   0444+634           126.3
   0446+112           147.1
   0454+550           131.3
   0454-234           128.0
   0454-810            82.4
   0458-020           139.9
   0502+049           141.6
   0507+179           142.7
   0520-165           127.8
   0524+034           135.9
   0528+134           137.3
   0529+483           130.6
   0537-441           107.4
   0547+234           133.2
   0600+177           130.1
   0607-157           118.6
   0615+820           109.3
   0622-645            89.3
   0628+203           123.7
   0633+595           117.6
   0636+022           118.4
   0642+449           119.7
   0644-671            86.1
   0721-071           104.8
   0725+219           110.7
   0727-115           102.0
   0731+050           105.9
   0736+017           103.8
   0738-674            81.2
   0742-562            84.3
   0743-247            94.4
   0744-158            97.0
   0746+483           108.6
   0748+126           103.6
   0804+499           105.7
   0814-241            87.8
   0821+248            98.5
   0823+033            92.9
   0827+243            97.0
   0850+284            93.1
   OJ287               90.6
   0859+470            96.2
   0859-140            79.8
   0901+697           101.4
   0922+364            88.9
   4C39.25             89.7
   0925-203            72.5
   0928+144            80.6
   0951+268            79.7
   M81                 97.2
   0954+658            95.4
   1005+066            69.4
   1005-333            62.5
   1013+127            69.7
   1022-665            65.5
   1039+811           100.1
   1045-188            54.0
   1055+018            56.0
   1102-242            49.9
   1115-122            47.6
   1124-186            44.9
   1125+221            58.9
   1128+385            68.6
   1133-032            45.4
   1140+668            87.6
   1143-696            60.6
   1144+402            67.5
   1147+245            56.2
   1156+295            58.1
   1208+186            48.7
   1215+303            56.0
   1215-002            36.8
   1222+037            37.1
   M84                 42.6
   1227+587            77.9
   3C274               41.2
   1244-255            27.3
   1307-556            43.8
   1308+328            51.7
   1308+471            64.8
   1312-533            41.5
   1325+126            32.1
   1331-195            15.2
   1334-127            14.0
   1343+537            69.5
   1351-018            16.4
   1352+757            90.9
   1354+195            35.7
   1405-287            15.1
   1417+273            42.4
   1435+638            78.8
   3C309.1             86.9
   1459+480            63.3
   1502+106            26.7
   1509+022            19.6
   1510-089            11.1
   1511-476            33.7
   1514-241            13.7
   1530-536            40.4
   1532+016            22.4
   1546+027            25.7
   1557+032            27.8
   1600+335            52.9
   1619-680            55.8
   1637+574            76.9
   1642+690            87.1
   1655+077            42.3
   1657+265            54.5
   1659-621            53.9
   1706-174            37.2
   1721-146            41.0
   1722+119            50.1
   1725+044            47.3
   1726+455            72.1
   NRAO530             43.2
   1741-038            47.9
   1743+173            57.2
   1749+096            54.7
   1749+701            91.6
   1803+784            97.8
   1803-642            60.9
   1821+107            62.4
   1824-582            60.9
   1825-214            55.5
   1830-211            56.8
   1839+548            87.1
   1849+670            94.2
   1855+031            67.7
   3C395               79.6
   1903-802            71.6
   1904+013            69.4
   1914-154            67.7
   1921-293            67.7
   1937-101            74.3
   1949-052            78.3
   1951+355            90.7
   2008+355            93.9
   2008-159            80.5
   2021+222            93.2
   2029+024            90.0
   2033-219            84.9
   3C418              102.4
   2037-253            84.8
   2052+239           100.6
   2100+468           105.7
   2105+551           106.9
   2109-811            76.7
   2112+463           107.7
   2112-144            95.8
   2118+443           108.7
   2123-463            87.8
   2126-158            98.6
   2128-123           100.2
   2134+00            105.1
   2146+608           112.1
   2149-306            98.2
   VR422201           116.3
   2201+315           116.6
   2204-540            90.8
   2208-137           108.9
   2211+374           118.8
   2216-038           114.0
   2227-088           114.9
   2233-148           114.1
   2233-234           110.3
   2243-123           117.3
   2255-282           112.2
   2309+454           127.9
   2319+317           133.2
   2320-035           129.3
   2344-514           104.3
   2345+061           138.4
   2351-154           130.1
   2356+385           138.6
   2357-318           120.3

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

