  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: SN1993J @ 6cm
 Exp. Code:  GM048C  


Schedule Version:       1.00                                              
Processed by SCHED version: Release of 18 Sept. 2003                      

PI:       J.M.Marcaide                                                    

Address:  Universitat de Valencia                                         
          C/ Dr. Moliner, 50                                              
          Burjassot, E 46100, Spain                                       
                                                                          

Phone:    34-96-398-3079/8 (work) or 34-96-337-1786 (home)                
EMAIL:    J.M.Marcaide@uv.es (internet)                                   
Fax:      34-96-398-3084                                                  
Phone during observation: 34-958-121311 (work) or 34-958-810928 (home)    

Observing mode: VLBA                                                      

Notes:                                                                    
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

 Next scan frequencies:  4966.49  4966.49  4982.49  4982.49  4998.49  4998.49
                         5014.49  5014.49
 Next BBC frequencies:    866.49   866.49   882.49   882.49   898.49   898.49
                          914.49   914.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00

11 07 00  1803+784     06 40 43  19.3   2.1-11.3      -9.2     0   1  1      0  11 07 00
11 11 00  ---          06 44 44  19.3   2.3-11.3     -10.1   240   F  1   3200

11 12 45  2007+777     06 46 28  19.2  -4.3 10.7      17.9    94   1  1   3200  11 12 45
11 16 45  ---          06 50 29  19.1  -4.1 10.8      17.0   240   F  1   6400

11 18 32  1803+784     06 52 17  19.4   2.7-11.1     -11.8    97   1  1   6400  11 18 32
11 22 32  ---          06 56 18  19.4   2.9-11.1     -12.7   240   F  1   9600

11 24 31  3C48         06 58 17  23.8 -64.3  5.3      67.8    68   1  1   9600  11 24 31
11 34 31  ---          07 08 19  21.8 -63.4  5.5      66.8   600   F  1  17600

11 47 49  M81          07 21 39  45.8  18.6 -2.6    -129.8   737   1  2  17600  11 47 49
11 51 49  ---          07 25 39  46.0  18.3 -2.5    -130.9   240   R  1  14400

11 52 04  SN1993J      07 25 55  46.1  18.3 -2.5    -131.0    10   1  2  14400  11 52 04
11 59 04  ---          07 32 56  46.6  17.7 -2.4    -133.1   420   R  1   8800

11 59 19  M81          07 33 11  46.5  17.6 -2.4    -133.2    10   1  2   8800  11 59 19
12 03 19  ---          07 37 12  46.8  17.3 -2.3    -134.4   240   R  1   5600

12 03 35  SN1993J      07 37 27  46.9  17.3 -2.3    -134.5    10   1  2   5600  12 03 35
12 10 35  ---          07 44 28  47.3  16.6 -2.2    -136.6   420   R  1      0

12 11 15  M81          07 45 08  47.3  16.5 -2.2    -136.8    35   1  3      0  12 11 15
12 16 15  ---          07 50 09  47.6  16.1 -2.1    -138.3   300   F  1   4000

12 16 30  SN1993J      07 50 24  47.7  16.1 -2.1    -138.4    10   1  3   4000  12 16 30
12 23 30  ---          07 57 25  48.1  15.3 -2.0    -140.6   420   F  1   9600

12 24 23  0917+624     07 58 19  55.6  17.1 -1.4    -147.1    32   1  3   9600  12 24 23
12 27 23  ---          08 01 19  55.8  16.6 -1.3    -148.2   180   F  1  12000

12 28 16  SN1993J      08 02 12  48.3  14.8 -1.9    -142.0    32   1  3  12000  12 28 16
12 35 16  ---          08 09 14  48.7  14.1 -1.8    -144.3   420   F  1  17600
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

12 35 56  M81          08 09 54  48.7  14.0 -1.8    -144.5    35   1  4  17600  12 35 56
12 39 56  ---          08 13 54  48.9  13.5 -1.7    -145.7   240   R  1  14400

12 40 11  SN1993J      08 14 10  49.0  13.5 -1.7    -145.8    10   1  4  14400  12 40 11
12 47 11  ---          08 21 11  49.3  12.7 -1.6    -148.1   420   R  1   8800

12 47 26  M81          08 21 26  49.3  12.7 -1.6    -148.1    10   1  4   8800  12 47 26
12 51 26  ---          08 25 27  49.5  12.2 -1.5    -149.4   240   R  1   5600

12 51 42  SN1993J      08 25 42  49.5  12.2 -1.5    -149.5    10   1  4   5600  12 51 42
12 58 42  ---          08 32 43  49.8  11.3 -1.4    -151.8   420   R  1      0

12 59 22  0954+658     08 33 24  52.7  14.4 -1.4    -148.8    29   1  5      0  12 59 22
13 02 22  ---          08 36 24  52.9  14.0 -1.4    -149.8   180   F  1   2400

13 03 03  SN1993J      08 37 05  50.0  10.8 -1.3    -153.2    29   1  5   2400  13 03 03
13 10 03  ---          08 44 06  50.3   9.9 -1.2    -155.6   420   F  1   8000

13 10 18  M81          08 44 22  50.2   9.9 -1.2    -155.6    10   1  5   8000  13 10 18
13 15 18  ---          08 49 22  50.4   9.2 -1.1    -157.3   300   F  1  12000

13 15 33  SN1993J      08 49 38  50.5   9.2 -1.1    -157.4    10   1  5  12000  13 15 33
13 22 33  ---          08 56 39  50.7   8.3 -1.0    -159.7   420   F  1  17600

13 23 13  M81          08 57 19  50.7   8.2 -1.0    -159.9    35   1  6  17600  13 23 13
13 28 13  ---          09 02 20  50.8   7.5 -0.9    -161.6   300   R  1  13600

13 28 29  SN1993J      09 02 35  50.9   7.5 -0.9    -161.7    10   1  6  13600  13 28 29
13 35 29  ---          09 09 36  51.1   6.5 -0.8    -164.1   420   R  1   8000

13 36 25  0917+624     09 10 33  58.3   2.5 -0.2    -175.4    36   1  6   8000  13 36 25
13 39 25  ---          09 13 33  58.4   1.8 -0.1    -176.6   180   R  1   5600

13 40 22  SN1993J      09 14 30  51.2   5.9 -0.7    -165.8    36   1  6   5600  13 40 22
13 47 22  ---          09 21 31  51.3   4.9 -0.6    -168.2   420   R  1      0

13 52 22  M81          09 26 32  51.4   4.2 -0.5    -169.9   294   1  7      0  13 52 22
13 56 22  ---          09 30 32  51.4   3.6 -0.4    -171.3   240   F  1   3200

13 56 37  SN1993J      09 30 47  51.5   3.6 -0.4    -171.4    10   1  7   3200  13 56 37
14 03 37  ---          09 37 49  51.5   2.6 -0.3    -173.8   420   F  1   8800
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

14 03 52  M81          09 38 04  51.5   2.6 -0.3    -173.9    10   1  7   8800  14 03 52
14 07 52  ---          09 42 04  51.5   2.0 -0.2    -175.2   240   F  1  12000

14 08 07  SN1993J      09 42 20  51.6   1.9 -0.2    -175.4    10   1  7  12000  14 08 07
14 15 07  ---          09 49 21  51.6   0.9 -0.1    -177.8   420   F  1  17600

14 15 47  0954+658     09 50 01  55.1   1.6 -0.2    -176.6    27   1  8  17600  14 15 47
14 18 47  ---          09 53 01  55.1   1.1 -0.1    -177.7   180   R  1  15200

14 19 24  SN1993J      09 53 38  51.6   0.3  0.0    -179.3    24   1  8  15200  14 19 24
14 26 24  ---          10 00 39  51.6  -0.7  0.1     178.3   420   R  1   9600

14 26 39  M81          10 00 54  51.6  -0.7  0.1     178.2    10   1  8   9600  14 26 39
14 31 39  ---          10 05 55  51.6  -1.5  0.2     176.5   300   R  1   5600

14 31 54  SN1993J      10 06 10  51.6  -1.5  0.2     176.4    10   1  8   5600  14 31 54
14 38 54  ---          10 13 12  51.6  -2.5  0.3     173.9   420   R  1      0

14 39 54  0917+624     10 14 12  57.3 -11.2  0.9     158.9    43   1  9      0  14 39 54
14 42 54  ---          10 17 13  57.1 -11.8  0.9     157.7   180   F  1   2400

14 43 54  SN1993J      10 18 13  51.5  -3.2  0.4     172.2    42   1  9   2400  14 43 54
14 50 54  ---          10 25 14  51.4  -4.2  0.5     169.8   420   F  1   8000

14 51 09  M81          10 25 29  51.4  -4.2  0.5     169.8    10   1  9   8000  14 51 09
14 56 09  ---          10 30 30  51.3  -4.9  0.6     168.0   300   F  1  12000

14 56 24  SN1993J      10 30 45  51.3  -5.0  0.6     167.9    10   1  9  12000  14 56 24
15 03 24  ---          10 37 46  51.2  -6.0  0.7     165.5   420   F  1  17600

15 04 04  M81          10 38 26  51.1  -6.0  0.7     165.3    35   1 10  17600  15 04 04
15 09 04  ---          10 43 27  51.0  -6.7  0.8     163.6   300   R  1  13600

15 09 19  SN1993J      10 43 42  51.0  -6.8  0.8     163.5    10   1 10  13600  15 09 19
15 16 19  ---          10 50 43  50.8  -7.8  0.9     161.1   420   R  1   8000

15 16 53  0954+658     10 51 17  54.2  -9.2  0.9     160.6    21   1 10   8000  15 16 53
15 19 53  ---          10 54 17  54.1  -9.7  0.9     159.5   180   R  1   5600

15 20 26  SN1993J      10 54 51  50.7  -8.3  1.0     159.7    21   1 10   5600  15 20 26
15 27 26  ---          11 01 52  50.5  -9.2  1.1     157.4   420   R  1      0
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

15 28 06  M81          11 02 32  50.4  -9.3  1.1     157.2    35   1 11      0  15 28 06
15 33 06  ---          11 07 33  50.2  -9.9  1.2     155.5   300   F  1   4000

15 33 21  SN1993J      11 07 48  50.3 -10.0  1.2     155.4    10   1 11   4000  15 33 21
15 40 21  ---          11 14 49  50.0 -10.9  1.3     153.1   420   F  1   9600

15 41 24  0917+624     11 15 52  53.4 -21.9  1.9     136.5    49   1 11   9600  15 41 24
15 44 24  ---          11 18 52  53.2 -22.3  1.9     135.5   180   F  1  12000

15 45 26  SN1993J      11 19 54  49.8 -11.5  1.4     151.4    49   1 11  12000  15 45 26
15 52 26  ---          11 26 56  49.5 -12.3  1.5     149.1   420   F  1  17600

15 53 06  M81          11 27 36  49.4 -12.4  1.5     149.0    35   1 12  17600  15 53 06
15 57 06  ---          11 31 36  49.2 -12.8  1.6     147.7   240   R  1  14400

15 57 21  SN1993J      11 31 52  49.2 -12.9  1.6     147.5    10   1 12  14400  15 57 21
16 04 21  ---          11 38 53  48.9 -13.7  1.7     145.3   420   R  1   8800

16 04 36  M81          11 39 08  48.8 -13.7  1.7     145.3    10   1 12   8800  16 04 36
16 08 36  ---          11 43 09  48.6 -14.1  1.8     144.0   240   R  1   5600

16 08 51  SN1993J      11 43 24  48.6 -14.2  1.8     143.9    10   1 12   5600  16 08 51
16 15 51  ---          11 50 25  48.3 -15.0  1.9     141.7   420   R  1      0

16 16 31  0954+658     11 51 05  51.1 -18.0  1.9     139.9    28   1 13      0  16 16 31
16 19 31  ---          11 54 05  50.9 -18.4  1.9     139.0   180   F  1   2400

16 20 04  SN1993J      11 54 39  48.0 -15.4  2.0     140.3    21   1 13   2400  16 20 04
16 27 04  ---          12 01 40  47.6 -16.1  2.1     138.2   420   F  1   8000

16 27 19  M81          12 01 55  47.6 -16.1  2.1     138.2    10   1 13   8000  16 27 19
16 32 19  ---          12 06 56  47.3 -16.6  2.2     136.6   300   F  1  12000

16 32 35  SN1993J      12 07 11  47.3 -16.7  2.2     136.5    10   1 13  12000  16 32 35
16 39 35  ---          12 14 12  46.8 -17.3  2.3     134.4   420   F  1  17600

16 40 15  0917+624     12 14 52  48.0 -28.5  2.9     118.3    27   1 14  17600  16 40 15
16 43 15  ---          12 17 53  47.7 -28.7  2.9     117.4   180   R  1  15200

16 43 15  SN1993J      12 17 53  46.6 -17.7  2.4     133.3   -13   1 14  15200  16 43 15
16 50 15  ---          12 24 54  46.1 -18.3  2.5     131.2   407   R  1   9600
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

16 50 15  M81          12 24 54  46.1 -18.2  2.5     131.3    -5   1 14   9600  16 50 15
16 55 15  ---          12 29 55  45.8 -18.6  2.6     129.8   295   R  1   5600

16 55 15  SN1993J      12 29 55  45.8 -18.7  2.6     129.7    -5   1 14   5600  16 55 15
17 02 15  ---          12 36 56  45.3 -19.2  2.7     127.7   415   R  1      0

-----------  Tape Change ------------

17 17 15  0954+658     12 51 58  46.3 -24.2  2.9     121.4   891   2  1      0  17 17 15
17 27 15  ---          13 02 00  45.4 -25.0  3.0     118.6   600   F  1   8000

17 27 55  M81          13 02 40  43.4 -21.0  3.1     120.5    30   2  1   8000  17 27 55
17 32 55  ---          13 07 41  43.0 -21.3  3.2     119.1   300   F  1  12000

17 33 10  SN1993J      13 07 56  43.0 -21.4  3.2     119.0    10   2  1  12000  17 33 10
17 40 10  ---          13 14 57  42.4 -21.8  3.3     117.1   420   F  1  17600

17 40 50  M81          13 15 37  42.4 -21.7  3.3     116.9    35   2  2  17600  17 40 50
17 44 50  ---          13 19 38  42.0 -22.0  3.4     115.9   240   R  1  14400

17 45 05  SN1993J      13 19 53  42.0 -22.0  3.4     115.7    10   2  2  14400  17 45 05
17 52 05  ---          13 26 54  41.5 -22.4  3.5     113.9   420   R  1   8800

17 52 20  M81          13 27 09  41.4 -22.3  3.5     113.9    10   2  2   8800  17 52 20
17 56 20  ---          13 31 10  41.1 -22.5  3.6     112.8   240   R  1   5600

17 56 35  SN1993J      13 31 25  41.1 -22.6  3.6     112.7    10   2  2   5600  17 56 35
18 03 35  ---          13 38 26  40.5 -22.9  3.7     110.8   420   R  1      0

18 22 53  0917+624     13 57 47  36.5 -32.7  4.6      92.6  1143   2  3      0  18 22 53
18 25 53  ---          14 00 48  36.1 -32.7  4.6      91.9   180   F  1   2400

18 26 51  SN1993J      14 01 46  38.5 -23.7  4.1     104.8    47   2  3   2400  18 26 51
18 33 51  ---          14 08 47  37.9 -23.9  4.2     103.1   420   F  1   8000

18 34 06  M81          14 09 03  37.9 -23.9  4.2     103.1    11   2  3   8000  18 34 06
18 39 06  ---          14 14 03  37.5 -24.0  4.3     101.8   300   F  1  12000

18 39 21  SN1993J      14 14 19  37.4 -24.1  4.3     101.7    10   2  3  12000  18 39 21
18 46 21  ---          14 21 20  36.8 -24.2  4.4     100.0   420   F  1  17600

18 47 01  M81          14 22 00  36.8 -24.2  4.4      99.9    35   2  4  17600  18 47 01
18 52 01  ---          14 27 01  36.3 -24.3  4.5      98.7   300   R  1  13600
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

18 52 16  SN1993J      14 27 16  36.3 -24.3  4.5      98.5    10   2  4  13600  18 52 16
18 59 16  ---          14 34 17  35.7 -24.4  4.6      96.8   420   R  1   8000

18 59 54  0954+658     14 34 55  36.3 -28.6  4.6      95.0    29   2  4   8000  18 59 54
19 02 54  ---          14 37 55  36.0 -28.7  4.6      94.3   180   R  1   5600

19 03 32  SN1993J      14 38 33  35.3 -24.5  4.7      95.8    29   2  4   5600  19 03 32
19 10 32  ---          14 45 34  34.7 -24.5  4.8      94.1   420   R  1      0

19 11 12  M81          14 46 14  34.6 -24.5  4.8      94.0    35   2  5      0  19 11 12
19 15 12  ---          14 50 15  34.2 -24.5  4.9      93.1   240   F  1   3200

19 15 27  SN1993J      14 50 30  34.2 -24.6  4.9      93.0    10   2  5   3200  19 15 27
19 23 27  ---          14 58 31  33.5 -24.6  5.0      91.1   480   F  1   9600

19 24 24  0917+624     14 59 29  29.3 -32.1  5.6      79.2    43   2  5   9600  19 24 24
19 27 24  ---          15 02 29  29.0 -32.0  5.7      78.6   180   F  1  12000

19 28 21  SN1993J      15 03 26  33.1 -24.6  5.1      89.9    43   2  5  12000  19 28 21
19 35 21  ---          15 10 28  32.4 -24.6  5.2      88.3   420   F  1  17600

19 38 41  M81          15 13 48  32.1 -24.5  5.3      87.6   194   2  6  17600  19 38 41
19 42 41  ---          15 17 49  31.8 -24.5  5.4      86.7   240   R  1  14400

19 42 56  SN1993J      15 18 04  31.7 -24.6  5.4      86.5    10   2  6  14400  19 42 56
19 49 56  ---          15 25 05  31.1 -24.5  5.5      84.9   420   R  1   8800

19 50 11  M81          15 25 20  31.1 -24.5  5.5      84.9    11   2  6   8800  19 50 11
19 54 11  ---          15 29 21  30.8 -24.4  5.6      84.0   240   R  1   5600

19 54 26  SN1993J      15 29 36  30.7 -24.5  5.6      83.9    10   2  6   5600  19 54 26
20 01 26  ---          15 36 37  30.1 -24.4  5.7      82.3   420   R  1      0

20 02 06  0954+658     15 37 17  29.8 -28.4  5.6      80.9    31   2  7      0  20 02 06
20 05 06  ---          15 40 18  29.5 -28.3  5.7      80.3   180   F  1   2400

20 05 45  SN1993J      15 40 56  29.7 -24.3  5.8      81.3    29   2  7   2400  20 05 45
20 12 45  ---          15 47 57  29.1 -24.2  5.9      79.8   420   F  1   8000

20 13 00  M81          15 48 12  29.1 -24.1  5.9      79.8    11   2  7   8000  20 13 00
20 17 00  ---          15 52 13  28.7 -24.1  5.9      78.9   240   F  1  11200
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

20 17 15  SN1993J      15 52 28  28.7 -24.1  5.9      78.7    10   2  7  11200  20 17 15
20 25 15  ---          16 00 29  28.0 -23.9  6.1      76.9   480   F  1  17600

20 26 07  0917+624     16 01 22  22.5 -29.8  6.7      66.5    35   2  8  17600  20 26 07
20 29 07  ---          16 04 23  22.2 -29.6  6.7      65.9   180   R  1  15200

20 30 00  SN1993J      16 05 15  27.6 -23.8  6.2      75.9    36   2  8  15200  20 30 00
20 37 00  ---          16 12 16  27.0 -23.6  6.3      74.3   420   R  1   9600

20 37 15  M81          16 12 31  27.0 -23.6  6.3      74.3    11   2  8   9600  20 37 15
20 41 15  ---          16 16 32  26.6 -23.5  6.3      73.4   240   R  1   6400

20 41 30  SN1993J      16 16 47  26.6 -23.5  6.4      73.3    10   2  8   6400  20 41 30
20 49 30  ---          16 24 49  25.9 -23.3  6.5      71.6   480   R  1      0

20 50 10  M81          16 25 29  25.9 -23.2  6.5      71.5    35   2  9      0  20 50 10
20 55 10  ---          16 30 29  25.4 -23.0  6.6      70.4   300   F  1   4000

20 55 25  SN1993J      16 30 45  25.4 -23.1  6.6      70.3    10   2  9   4000  20 55 25
21 02 25  ---          16 37 46  24.8 -22.8  6.7      68.7   420   F  1   9600

21 03 03  0954+658     16 38 24  23.8 -26.5  6.7      67.9    29   2  9   9600  21 03 03
21 06 03  ---          16 41 24  23.5 -26.3  6.7      67.2   180   F  1  12000

21 06 41  SN1993J      16 42 02  24.4 -22.7  6.8      67.8    29   2  9  12000  21 06 41
21 13 41  ---          16 49 03  23.9 -22.4  6.9      66.3   420   F  1  17600

21 14 21  M81          16 49 43  23.8 -22.3  6.9      66.2    35   2 10  17600  21 14 21
21 18 21  ---          16 53 44  23.5 -22.2  7.0      65.3   240   R  1  14400

21 18 36  SN1993J      16 53 59  23.5 -22.2  7.0      65.2    10   2 10  14400  21 18 36
21 25 36  ---          17 01 00  22.9 -21.9  7.1      63.7   420   R  1   8800

21 25 51  M81          17 01 15  22.9 -21.9  7.1      63.7    11   2 10   8800  21 25 51
21 29 51  ---          17 05 16  22.6 -21.7  7.2      62.8   240   R  1   5600

21 30 06  SN1993J      17 05 31  22.5 -21.7  7.2      62.7    10   2 10   5600  21 30 06
21 37 06  ---          17 12 32  22.0 -21.4  7.3      61.2   420   R  1      0

21 40 21  3C286        17 15 48  42.2 -75.0  3.7      74.7   149   2 11      0  21 40 21
21 44 21  ---          17 19 49  41.4 -74.7  3.8      74.4   240   F  1   3200
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               SN1993J @ 6cm
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  29 Oct 2003   Day 302 ---

21 49 28  1803+784     17 24 56  42.0   2.4 -0.6    -169.7   249   2 11   3200  21 49 28
21 52 28  ---          17 27 57  42.0   2.2 -0.5    -170.6   180   F  1   5600


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: GM048C.6cm
   Matches group v6cm_2 in /sched-2003/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  256
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  8    Passes/head pos:   1       Speedup factor:   1.00

   Tape speeds: Low density - 266.660 ips,  High density - 160.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:22:00

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         U         L         U         L         U         L         U
   Pol.  =      LCP       LCP       LCP       LCP       LCP       LCP       LCP       LCP 
   BBC   =         1         1         2         2         3         3         4         4
   BBC SB=         L         U         L         U         L         U         L         U
   IF    =        C         C         C         C         C         C         C         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    4966.49   4966.49   4982.49   4982.49   4998.49   4998.49   5014.49   5014.49
   BBC fr=     866.49    866.49    882.49    882.49    898.49    898.49    914.49    914.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S1    S3    S5    S7 
    PCALXB2=   S2    S4    S6    S8    S2    S4    S6    S8 
    PCALFR1=   490   490   490   490  6490  6490  6490  6490
    PCALFR2=   510   510   510   510  6510  6510  6510  6510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27
    barrel=roll_auto
 SOURCE LIST -- SN1993J @ 6cm
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * 0917+624          09 17 40.306287   * 09 21 36.230500     09 21 52.833260 
                     62 28 38.63575    * 62 15 52.17600      62 14 47.39267 
                     From catalog imbedded in main SCHED input file.

 * 0954+658          09 54 57.847920   * 09 58 47.245100     09 59 02.975320 
                     65 48 15.53881    * 65 33 54.81800      65 32 42.66264 
                     From catalog imbedded in main SCHED input file.

 * SN1993J           09 51 19.039486   * 09 55 24.775500     09 55 41.634887 
                     69 15 26.47487    * 69 01 13.71000      69 00 01.27338 
                     From catalog imbedded in main SCHED input file.

 * M81               09 51 27.310854   * 09 55 33.173100     09 55 50.038667 
                     69 18 08.14534    * 69 03 55.06200      69 02 42.59382 
                     From catalog imbedded in main SCHED input file.

 * 1803+784          18 03 39.193244   * 18 00 45.683600     18 00 29.313224 
                     78 27 54.30008    * 78 28 04.02100      78 28 14.62845 
                     From catalog imbedded in main SCHED input file.

 * 2007+777          20 07 20.430477   * 20 05 30.998800     20 05 21.315701 
                     77 43 58.12445    * 77 52 43.24900      77 53 35.46835 
                     From catalog imbedded in main SCHED input file.

 * 3C48              01 34 49.826399   * 01 37 41.299465     01 37 54.725002 
                     32 54 20.26003    * 33 09 35.13422      33 10 50.26611 
                     From catalog imbedded in main SCHED input file.

 * 3C286             13 28 49.657781   * 13 31 08.288074     13 31 16.838779 
                     30 45 58.64118    * 30 30 32.95982      30 29 28.30688 
                     From catalog imbedded in main SCHED input file.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0917+624            94.3
   0954+658            92.0
   SN1993J             93.9
   M81                 93.9
   1803+784            97.0
   2007+777           102.7
   3C48               158.6
   3C286               45.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

