  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Radio AGN feedback
 Exp. Code:  GM081D  


Schedule Version:       2.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Suma Murthy

Address:  JIVE
          Oude Hoogeveensedijk 4
          7991 PD Dwingeloo
          The Netherlands

Phone:    +31 521 596 508
EMAIL:    murthy@jive.eu
Fax:
Phone during observation: +31 521 596 508

Observing mode: vlbi

Notes:    # Please, make sure PHASE CAL is OFF #
          v2: fixed (mixed-BW) tunings, line at 1371.25 with DOPINCR 250kHz
            line centered in USB of 2nd DBBC per pol
            Mc,T6 low-end of 1350 falls in LSB of 1st DBBC BBC per pol (as for gm018a in sess.2)


COVER LETTER:


Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

 Next scan frequencies:  1343.25  1343.25  1359.25  1359.25  1375.25  1375.25  1391.25  1391.25
 Next BBC frequencies:    756.75   756.75   740.75   740.75   724.75   724.75   708.75   708.75
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

10 30 00  4C39.25      06 09 08  48.8  64.4 -3.3     -85.9     0        0   10 30 00
10 36 00  ---          06 15 09  49.9  64.5 -3.2     -86.7   360       23   10 30 01

10 38 00  J1103+1158   06 17 09  21.6  88.7 -4.8     -61.5    56       23   10 38 00
10 41 00  ---          06 20 09  22.2  89.1 -4.7     -61.5   180       35   10 38 01

10 41 00  J1100+1002   06 20 09  21.9  91.3 -4.7     -60.8    -9       35   10 41 09
10 46 00  ---          06 25 10  23.0  91.9 -4.6     -60.8   291       54   10 41 01

10 46 00  J1103+1158   06 25 10  23.3  89.7 -4.7     -61.5    -9       54   10 46 09
10 48 00  ---          06 27 11  23.8  90.0 -4.6     -61.5   111       61   10 46 01

10 48 00  J1100+1002   06 27 11  23.4  92.2 -4.6     -60.8    -9       61   10 48 09
10 53 00  ---          06 32 11  24.5  92.8 -4.5     -60.7   291       79   10 48 01

10 53 30  J1103+1158   06 32 42  24.9  90.7 -4.5     -61.5    21       79   10 53 30
10 55 00  ---          06 34 12  25.3  90.9 -4.5     -61.5    90       85   10 53 31

10 55 00  J1100+1002   06 34 12  24.9  93.1 -4.5     -60.7    -9       85   10 55 09
11 00 00  ---          06 39 13  26.0  93.8 -4.4     -60.6   291      104   10 55 01

11 00 00  J1103+1158   06 39 13  26.3  91.5 -4.4     -61.5    -9      104   11 00 09
11 02 00  ---          06 41 13  26.8  91.8 -4.4     -61.5   111      111   11 00 01

11 02 00  J1100+1002   06 41 13  26.4  94.1 -4.3     -60.6    -9      111   11 02 09
11 07 00  ---          06 46 14  27.5  94.7 -4.3     -60.5   291      130   11 02 01

11 07 30  J1103+1158   06 46 44  28.0  92.5 -4.3     -61.4    21      130   11 07 30
11 09 00  ---          06 48 14  28.3  92.7 -4.3     -61.4    90      136   11 07 31

11 09 00  J1100+1002   06 48 14  27.9  95.0 -4.2     -60.5    -9      136   11 09 09
11 14 00  ---          06 53 15  29.0  95.7 -4.1     -60.4   291      154   11 09 01

11 14 00  J1103+1158   06 53 15  29.4  93.4 -4.2     -61.4    -9      154   11 14 09
11 16 00  ---          06 55 15  29.8  93.7 -4.1     -61.3   111      162   11 14 01

11 16 00  J1100+1002   06 55 15  29.4  96.0 -4.1     -60.3   -10      162   11 16 10
11 21 00  ---          07 00 16  30.5  96.7 -4.0     -60.2   290      180   11 16 01

11 21 30  J1103+1158   07 00 46  31.0  94.4 -4.1     -61.2    20      180   11 21 30
11 23 00  ---          07 02 16  31.3  94.6 -4.0     -61.2    90      186   11 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

11 23 00  J1100+1002   07 02 16  30.9  97.0 -4.0     -60.1   -10      186   11 23 10
11 28 00  ---          07 07 17  32.0  97.7 -3.9     -60.0   290      205   11 23 01

11 28 00  J1103+1158   07 07 17  32.4  95.3 -3.9     -61.1   -10      205   11 28 10
11 30 00  ---          07 09 18  32.8  95.6 -3.9     -61.0   110      212   11 28 01

11 30 00  J1100+1002   07 09 18  32.4  98.0 -3.9     -59.9   -10      212   11 30 10
11 35 00  ---          07 14 18  33.5  98.7 -3.8     -59.7   290      230   11 30 01

11 35 30  J1103+1158   07 14 48  34.0  96.4 -3.8     -60.9    20      230   11 35 30
11 37 00  ---          07 16 19  34.3  96.6 -3.8     -60.8    90      236   11 35 31

11 37 00  J1100+1002   07 16 19  33.9  99.0 -3.8     -59.6   -10      236   11 37 10
11 42 00  ---          07 21 19  35.0  99.8 -3.7     -59.4   290      255   11 37 01

11 42 00  J1103+1158   07 21 19  35.4  97.3 -3.7     -60.7   -10      255   11 42 10
11 44 00  ---          07 23 20  35.8  97.6 -3.7     -60.6   110      262   11 42 01

11 44 00  J1100+1002   07 23 20  35.4 100.1 -3.6     -59.3   -10      262   11 44 10
11 49 00  ---          07 28 21  36.5 100.9 -3.6     -59.1   290      281   11 44 01

11 49 30  J1103+1158   07 28 51  37.0  98.5 -3.6     -60.4    20      281   11 49 30
11 51 00  ---          07 30 21  37.3  98.7 -3.6     -60.4    90      286   11 49 31

11 51 00  J1100+1002   07 30 21  36.9 101.2 -3.5     -59.0   -10      286   11 51 10
11 56 00  ---          07 35 22  38.0 102.0 -3.4     -58.7   290      305   11 51 01

11 56 00  J1103+1158   07 35 22  38.4  99.5 -3.5     -60.1   -10      305   11 56 10
11 58 00  ---          07 37 22  38.8  99.8 -3.4     -60.0   110      312   11 56 01

11 58 00  J1100+1002   07 37 22  38.4 102.3 -3.4     -58.6   -10      312   11 58 10
12 03 00  ---          07 42 23  39.4 103.2 -3.3     -58.3   290      331   11 58 01

12 03 30  J1103+1158   07 42 53  40.0 100.6 -3.4     -59.8    20      331   12 03 30
12 05 00  ---          07 44 23  40.3 100.9 -3.3     -59.7    90      337   12 03 31

12 05 00  J1100+1002   07 44 23  39.9 103.5 -3.3     -58.1   -10      337   12 05 10
12 10 00  ---          07 49 24  40.9 104.4 -3.2     -57.8   290      355   12 05 01

12 10 30  J1103+1158   07 49 54  41.4 101.8 -3.2     -59.4    20      355   12 10 30
12 12 00  ---          07 51 24  41.7 102.0 -3.2     -59.3    90      361   12 10 31

12 12 00  J1100+1002   07 51 24  41.3 104.7 -3.2     -57.7   -10      361   12 12 10
12 15 00  ---          07 54 25  41.9 105.2 -3.1     -57.4   170      372   12 12 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

12 15 00  J1103+1158   07 54 25  42.4 102.6 -3.2     -59.1   -10      372   12 15 10
12 17 00  ---          07 56 25  42.8 102.9 -3.1     -59.0   110      379   12 15 01

12 17 00  J1100+1002   07 56 25  42.4 105.6 -3.1     -57.3   -10      379   12 17 10
12 22 00  ---          08 01 26  43.4 106.5 -3.0     -56.9   290      398   12 17 01

12 22 30  J1103+1158   08 01 56  44.0 103.9 -3.0     -58.6    20      398   12 22 30
12 24 00  ---          08 03 26  44.3 104.1 -3.0     -58.5    90      404   12 22 31

12 24 00  4C39.25      08 03 26  70.7  58.7 -1.4    -109.0   -60      404   12 25 00
12 30 00  ---          08 09 27  71.8  57.5 -1.3    -111.2   300      423   12 24 01

12 31 00  J1103+1158   08 10 28  45.7 105.4 -2.9     -58.0     1      423   12 31 00
12 35 00  ---          08 14 28  46.6 106.2 -2.8     -57.6   240      439   12 31 01

12 35 00  J1100+1002   08 14 28  46.1 109.0 -2.8     -55.7   -10      439   12 35 10
12 42 00  ---          08 21 29  47.5 110.5 -2.7     -54.9   410      465   12 35 01

12 42 30  J1103+1158   08 21 59  48.1 107.6 -2.7     -56.9    20      465   12 42 30
12 44 00  ---          08 23 30  48.4 107.9 -2.7     -56.8    90      471   12 42 31

12 44 00  J1100+1002   08 23 30  47.9 110.9 -2.6     -54.7   -10      471   12 44 10
12 51 00  ---          08 30 31  49.3 112.4 -2.5     -53.9   410      497   12 44 01

12 51 30  J1103+1158   08 31 01  49.9 109.5 -2.6     -56.0    20      497   12 51 30
12 53 00  ---          08 32 31  50.3 109.8 -2.5     -55.8    90      503   12 51 31

12 53 00  J1100+1002   08 32 31  49.7 112.9 -2.5     -53.6   -10      503   12 53 10
13 00 00  ---          08 39 32  51.1 114.5 -2.4     -52.7   410      529   12 53 01

13 00 30  J1103+1158   08 40 02  51.8 111.5 -2.4     -54.9    20      529   13 00 30
13 02 00  ---          08 41 33  52.1 111.8 -2.4     -54.7    90      535   13 00 31

13 02 00  J1100+1002   08 41 33  51.5 115.0 -2.3     -52.4   -10      535   13 02 10
13 09 00  ---          08 48 34  52.8 116.7 -2.2     -51.3   410      562   13 02 01

13 09 30  J1103+1158   08 49 04  53.6 113.6 -2.3     -53.7    20      562   13 09 30
13 11 00  ---          08 50 34  53.9 114.0 -2.2     -53.5    90      567   13 09 31

13 11 00  J1100+1002   08 50 34  53.2 117.2 -2.2     -51.0   -10      567   13 11 10
13 18 00  ---          08 57 35  54.5 119.1 -2.1     -49.8   410      594   13 11 01

13 18 30  J1103+1158   08 58 05  55.3 115.9 -2.1     -52.3    20      594   13 18 30
13 20 00  ---          08 59 36  55.6 116.3 -2.1     -52.0    90      600   13 18 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

13 20 00  J1100+1002   08 59 36  54.9 119.6 -2.0     -49.4   -10      600   13 20 10
13 27 00  ---          09 06 37  56.2 121.7 -1.9     -48.0   410      626   13 20 01

13 27 30  J1103+1158   09 07 07  57.1 118.4 -2.0     -50.7    20      626   13 27 30
13 29 00  ---          09 08 37  57.3 118.8 -1.9     -50.4    90      632   13 27 31

13 29 00  J1100+1002   09 08 37  56.6 122.3 -1.9     -47.6   -10      632   13 29 10
13 36 00  ---          09 15 38  57.8 124.4 -1.8     -46.1   410      658   13 29 01

13 36 30  J1103+1158   09 16 08  58.7 121.0 -1.8     -48.9    20      658   13 36 30
13 38 00  ---          09 17 39  59.0 121.5 -1.8     -48.6    90      664   13 36 31

13 38 00  J1100+1002   09 17 39  58.2 125.1 -1.7     -45.6   -10      664   13 38 10
13 45 00  ---          09 24 40  59.4 127.5 -1.6     -43.9   410      690   13 38 01

13 45 30  J1103+1158   09 25 10  60.4 124.0 -1.7     -46.8    20      690   13 45 30
13 47 00  ---          09 26 40  60.6 124.5 -1.6     -46.4    90      696   13 45 31

13 47 00  J1100+1002   09 26 40  59.8 128.2 -1.6     -43.4   -11      696   13 47 11
13 54 00  ---          09 33 41  60.9 130.8 -1.5     -41.4   409      722   13 47 01

13 54 30  J1103+1158   09 34 11  62.0 127.2 -1.5     -44.5    19      722   13 54 30
13 56 00  ---          09 35 42  62.2 127.7 -1.5     -44.1    90      728   13 54 31

13 56 00  J1100+1002   09 35 42  61.3 131.5 -1.4     -40.8   -11      728   13 56 11
14 03 00  ---          09 42 43  62.4 134.3 -1.3     -38.7   409      755   13 56 01

14 03 30  J1103+1158   09 43 13  63.5 130.7 -1.4     -41.8    19      755   14 03 30
14 05 00  ---          09 44 43  63.7 131.3 -1.3     -41.3    90      760   14 03 31

14 05 00  J1100+1002   09 44 43  62.7 135.2 -1.3     -38.0   -11      760   14 05 11
14 12 00  ---          09 51 44  63.7 138.2 -1.2     -35.6   409      787   14 05 01

14 12 30  J1103+1158   09 52 14  64.9 134.5 -1.2     -38.8    19      787   14 12 30
14 14 00  ---          09 53 44  65.1 135.2 -1.2     -38.3    90      793   14 12 31

14 14 00  J1100+1002   09 53 44  64.0 139.2 -1.1     -34.8   -11      793   14 14 11
14 21 00  ---          10 00 46  64.9 142.5 -1.0     -32.1   409      819   14 14 01

14 21 30  J1103+1158   10 01 16  66.2 138.8 -1.0     -35.4    19      819   14 21 30
14 23 00  ---          10 02 46  66.4 139.5 -1.0     -34.8    90      825   14 21 31

14 23 00  J1100+1002   10 02 46  65.2 143.5 -1.0     -31.3   -11      825   14 23 11
14 30 00  ---          10 09 47  66.1 147.1 -0.9     -28.3   409      851   14 23 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

14 30 30  J1103+1158   10 10 17  67.4 143.5 -0.9     -31.5    19      851   14 30 30
14 32 00  ---          10 11 47  67.6 144.3 -0.9     -30.9    90      857   14 30 31

14 32 00  J1100+1002   10 11 47  66.3 148.2 -0.8     -27.4   -11      857   14 32 11
14 39 00  ---          10 18 49  67.0 152.1 -0.7     -24.1   409      883   14 32 01

14 39 30  J1103+1158   10 19 19  68.5 148.6 -0.7     -27.2    19      883   14 39 30
14 41 00  ---          10 20 49  68.7 149.5 -0.7     -26.5    90      889   14 39 31

14 41 00  J1100+1002   10 20 49  67.2 153.3 -0.7     -23.1   -11      889   14 41 11
14 48 00  ---          10 27 50  67.9 157.5 -0.6     -19.5   409      915   14 41 01

14 48 30  J1103+1158   10 28 20  69.5 154.2 -0.6     -22.5    19      915   14 48 30
14 50 00  ---          10 29 50  69.6 155.2 -0.6     -21.7    90      921   14 48 31

14 50 00  J1100+1002   10 29 50  68.0 158.8 -0.5     -18.4   -11      921   14 50 11
14 57 00  ---          10 36 52  68.5 163.2 -0.4     -14.6   409      947   14 50 01

14 57 30  J1103+1158   10 37 22  70.2 160.2 -0.4     -17.3    19      947   14 57 30
14 59 00  ---          10 38 52  70.3 161.3 -0.4     -16.4    90      953   14 57 31

14 59 00  J1100+1002   10 38 52  68.6 164.6 -0.4     -13.4   -11      953   14 59 11
15 06 00  ---          10 45 53  69.0 169.2 -0.3      -9.4   409      980   14 59 01

15 06 30  J1103+1158   10 46 23  70.8 166.6 -0.3     -11.7    18      980   15 06 30
15 08 00  ---          10 47 53  70.8 167.7 -0.3     -10.8    90      985   15 06 31

15 08 00  J1100+1002   10 47 53  69.1 170.6 -0.2      -8.2   -12      985   15 08 12
15 15 00  ---          10 54 54  69.2 175.4 -0.1      -4.0   408     1012   15 08 01

15 15 30  J1103+1158   10 55 25  71.1 173.3 -0.1      -5.9    18     1012   15 15 30
15 17 00  ---          10 56 55  71.1 174.5 -0.1      -4.9    90     1017   15 15 31

15 17 00  J1100+1002   10 56 55  69.3 176.8 -0.1      -2.8   -12     1017   15 17 12
15 24 00  ---          11 03 56  69.3 181.7  0.0       1.5   408     1044   15 17 01

15 24 30  J1103+1158   11 04 26  71.2 180.2  0.0       0.1    18     1044   15 24 30
15 26 00  ---          11 05 56  71.2 181.3  0.0       1.1    90     1050   15 24 31

15 26 00  J1100+1002   11 05 56  69.3 183.1  0.1       2.7   -12     1050   15 26 12
15 33 00  ---          11 12 57  69.1 188.0  0.2       6.9   408     1076   15 26 01

15 33 30  J1103+1158   11 13 28  71.1 187.0  0.2       6.1    18     1076   15 33 30
15 35 00  ---          11 14 58  71.1 188.1  0.2       7.1    90     1082   15 33 31
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

15 36 00  3C279        11 15 58  46.1 142.1 -1.7     -32.1     3     1082   15 36 00
15 41 00  ---          11 20 59  46.8 143.6 -1.6     -30.9   300     1101   15 36 01

15 43 00  J1103+1158   11 22 59  70.7 194.0  0.3      12.3    65     1101   15 43 00
15 46 00  ---          11 26 00  70.6 196.2  0.4      14.2   180     1113   15 43 01

15 46 00  J1100+1002   11 26 00  68.5 196.7  0.4      14.5   -12     1113   15 46 12
15 53 00  ---          11 33 01  68.0 201.2  0.5      18.4   408     1139   15 46 01

15 53 30  J1103+1158   11 33 31  70.0 201.4  0.5      18.7    18     1139   15 53 30
15 55 00  ---          11 35 01  69.9 202.4  0.5      19.6    90     1145   15 53 31

15 55 00  J1100+1002   11 35 01  67.9 202.4  0.6      19.5   -12     1145   15 55 12
16 02 00  ---          11 42 02  67.2 206.6  0.7      23.1   408     1171   15 55 01

16 02 30  J1103+1158   11 42 32  69.2 207.3  0.6      23.8    18     1171   16 02 30
16 04 00  ---          11 44 03  69.1 208.3  0.7      24.6    90     1177   16 02 31

16 04 00  J1100+1002   11 44 03  67.0 207.8  0.7      24.0   -12     1177   16 04 12
16 11 00  ---          11 51 04  66.3 211.7  0.8      27.4   408     1203   16 04 01

16 11 30  J1103+1158   11 51 34  68.3 212.8  0.8      28.4    18     1203   16 11 30
16 13 00  ---          11 53 04  68.1 213.7  0.8      29.2    90     1209   16 11 31

16 13 00  J1100+1002   11 53 04  66.1 212.8  0.9      28.3   -12     1209   16 13 12
16 20 00  ---          12 00 05  65.2 216.5  1.0      31.3   408     1235   16 13 01

16 20 30  J1103+1158   12 00 35  67.1 217.8  0.9      32.6    18     1235   16 20 30
16 22 00  ---          12 02 05  66.9 218.6  1.0      33.3    90     1241   16 20 31

16 22 00  J1100+1002   12 02 05  64.9 217.5  1.0      32.1   -12     1241   16 22 12
16 29 00  ---          12 09 07  64.0 220.8  1.1      34.8   408     1267   16 22 01

16 29 30  J1103+1158   12 09 37  65.9 222.4  1.1      36.3    18     1267   16 29 30
16 31 00  ---          12 11 07  65.7 223.1  1.1      36.9    90     1273   16 29 31

16 31 00  J1100+1002   12 11 07  63.7 221.7  1.2      35.5   -12     1273   16 31 12
16 38 00  ---          12 18 08  62.7 224.8  1.3      38.0   408     1299   16 31 01

16 38 30  J1103+1158   12 18 38  64.5 226.5  1.2      39.6    18     1299   16 38 30
16 40 00  ---          12 20 08  64.3 227.2  1.3      40.2    90     1305   16 38 31

16 40 00  J1100+1002   12 20 08  62.4 225.6  1.3      38.6   -12     1305   16 40 12
16 47 00  ---          12 27 10  61.3 228.4  1.4      40.8   408     1331   16 40 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

16 47 30  J1103+1158   12 27 40  63.1 230.3  1.4      42.6    18     1331   16 47 30
16 49 00  ---          12 29 10  62.8 230.9  1.4      43.0    90     1337   16 47 31

16 49 00  J1100+1002   12 29 10  60.9 229.2  1.5      41.4   -12     1337   16 49 12
16 56 00  ---          12 36 11  59.8 231.8  1.6      43.3   408     1363   16 49 01

16 56 30  J1103+1158   12 36 41  61.5 233.7  1.5      45.1    18     1363   16 56 30
16 58 00  ---          12 38 11  61.3 234.3  1.6      45.5    90     1369   16 56 31

16 58 00  J1100+1002   12 38 11  59.4 232.5  1.6      43.9   -12     1369   16 58 12
17 05 00  ---          12 45 13  58.2 234.9  1.7      45.6   408     1395   16 58 01

17 05 30  J1103+1158   12 45 43  59.9 236.8  1.7      47.4    18     1395   17 05 30
17 07 00  ---          12 47 13  59.7 237.3  1.7      47.7    90     1401   17 05 31

17 07 00  J1100+1002   12 47 13  57.9 235.5  1.8      46.1   -12     1401   17 07 12
17 14 00  ---          12 54 14  56.6 237.7  1.9      47.6   408     1428   17 07 01

17 14 30  J1103+1158   12 54 44  58.3 239.7  1.8      49.4    18     1428   17 14 30
17 16 00  ---          12 56 14  58.0 240.2  1.9      49.7    90     1433   17 14 31

17 16 00  J1100+1002   12 56 14  56.2 238.3  1.9      48.0   -12     1433   17 16 12
17 23 00  ---          13 03 16  54.9 240.3  2.0      49.4   408     1460   17 16 01

17 23 30  J1103+1158   13 03 46  56.6 242.3  2.0      51.1    19     1460   17 23 30
17 25 00  ---          13 05 16  56.3 242.7  2.0      51.4    90     1465   17 23 31

17 25 00  J1100+1002   13 05 16  54.6 240.9  2.1      49.7   -11     1465   17 25 11
17 32 00  ---          13 12 17  53.2 242.8  2.2      51.0   409     1492   17 25 01

17 32 30  J1103+1158   13 12 47  54.9 244.7  2.1      52.7    19     1492   17 32 30
17 34 00  ---          13 14 17  54.6 245.1  2.2      52.9    90     1498   17 32 31

17 34 00  J1100+1002   13 14 17  52.8 243.3  2.2      51.3   -11     1498   17 34 11
17 41 00  ---          13 21 18  51.5 245.0  2.3      52.4   409     1524   17 34 01

17 41 30  J1103+1158   13 21 49  53.1 247.0  2.3      54.0    19     1524   17 41 30
17 43 00  ---          13 23 19  52.8 247.3  2.3      54.2    90     1530   17 41 31

17 43 00  J1100+1002   13 23 19  51.1 245.5  2.4      52.6   -11     1530   17 43 11
17 50 00  ---          13 30 20  49.7 247.1  2.5      53.6   409     1556   17 43 01

17 50 30  J1103+1158   13 30 50  51.3 249.1  2.4      55.2    19     1556   17 50 30
17 52 00  ---          13 32 20  51.0 249.4  2.5      55.4    90     1562   17 50 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Radio AGN feedback
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun  30 Oct 2022   Day 303 ---

17 52 00  J1100+1002   13 32 20  49.3 247.6  2.5      53.8   -11     1562   17 52 11
17 59 00  ---          13 39 21  47.9 249.1  2.6      54.7   409     1588   17 52 01

17 59 30  J1103+1158   13 39 52  49.5 251.0  2.6      56.2    19     1588   17 59 30
18 01 00  ---          13 41 22  49.2 251.3  2.6      56.4    90     1594   17 59 31

18 01 00  J1100+1002   13 41 22  47.5 249.5  2.7      54.9   -11     1594   18 01 11
18 08 00  ---          13 48 23  46.1 251.0  2.8      55.7   409     1620   18 01 01

18 08 30  J1103+1158   13 48 53  47.6 252.9  2.7      57.2    19     1620   18 08 30
18 10 00  ---          13 50 23  47.3 253.1  2.8      57.3    90     1626   18 08 31

18 10 00  J1100+1002   13 50 23  45.7 251.4  2.8      55.9   -11     1626   18 10 11
18 17 00  ---          13 57 24  44.2 252.7  2.9      56.5   409     1652   18 10 01

18 17 30  J1103+1158   13 57 54  45.7 254.6  2.9      57.9    19     1652   18 17 30
18 19 00  ---          13 59 25  45.4 254.9  2.9      58.1    90     1658   18 17 31

18 19 00  J1100+1002   13 59 25  43.8 253.1  3.0      56.7   -11     1658   18 19 11
18 26 00  ---          14 06 26  42.4 254.4  3.1      57.3   409     1685   18 19 01

18 26 30  J1103+1158   14 06 56  43.9 256.2  3.0      58.6    19     1685   18 26 30
18 28 00  ---          14 08 26  43.6 256.5  3.1      58.7    90     1690   18 26 31

18 28 00  J1100+1002   14 08 26  42.0 254.7  3.1      57.4   -11     1690   18 28 11
18 35 00  ---          14 15 27  40.5 256.0  3.2      57.9   409     1717   18 28 01

18 35 30  J1103+1158   14 15 57  42.0 257.8  3.2      59.2    19     1717   18 35 30
18 37 00  ---          14 17 28  41.7 258.0  3.2      59.3    90     1723   18 35 31

18 37 00  J1100+1002   14 17 28  40.1 256.3  3.3      58.1   -11     1723   18 37 11
18 44 00  ---          14 24 29  38.6 257.5  3.4      58.5   409     1749   18 37 01

18 44 30  J1103+1158   14 24 59  40.1 259.3  3.3      59.7    19     1749   18 44 30
18 46 00  ---          14 26 29  39.8 259.5  3.4      59.8    90     1755   18 44 31

18 46 00  J1100+1002   14 26 29  38.2 257.8  3.4      58.6   -11     1755   18 46 11
18 52 30  ---          14 33 00  36.8 258.9  3.5      59.0   379     1779   18 46 01

18 52 30  J1103+1158   14 33 00  38.4 260.5  3.5      60.1   -11     1779   18 52 41
18 54 00  ---          14 34 30  38.1 260.8  3.5      60.2    79     1784   18 52 31

18 55 00  3C279        14 35 31  46.6 216.9  1.6      31.3    21     1784   18 55 00
19 00 00  ---          14 40 31  45.9 218.5  1.7      32.6   300     1803   18 55 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess322.H512globline
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v20cm_1         FD and KP filtered below 1330. SC filtered above 1440

   Setup group:    4         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00   2100.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  12.9      2.1     12.9

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  15  Setup file default.  Used with PCAL = off
   LO sum=   1343.25  1343.25  1359.25  1359.25  1375.25  1375.25  1391.25  1391.25
   BBC fr=    756.75   756.75   740.75   740.75   724.75   724.75   708.75   708.75
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     740.75    740.75    724.75    724.75
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  15  16  17  18  19  20  21  22  23  25

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * J1100+1002        10 57 41.079141   * 11 00 17.991000     11 01 28.050349       0.00
                     10 19 03.47115    * 10 02 56.72000      09 55 44.73020        0.00
                     From catalog imbedded in main SCHED input file.

 * J1103+1158        11 00 26.171571   * 11 03 03.529839     11 04 13.779978       0.00
                     12 14 26.46469    * 11 58 16.62439      11 51 02.65971        0.00
                     From catalog imbedded in main SCHED input file.

 * 4C39.25           09 23 55.319216   * 09 27 03.013937     09 28 27.391134       0.31
   J0927+3902        39 15 23.56644    * 39 02 20.85185      38 56 21.87603        0.16
   0923+392          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J0927+39          GSFC 2016a X/S astro solution, 250526 observations.

 * 3C279             12 53 35.831310   * 12 56 11.166577     12 57 20.091544       0.34
   J1256-0547       -05 31 07.99627    *-05 47 21.52513     -05 54 34.32431        0.56
   1253-055          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
   J1256-05          GSFC 2016a X/S astro solution,  13160 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  J1100+1002 sess322.H512globline  1 2 3 4 5 6 7 8 9 10 15 24       10.247   851.338
  J1103+1158 sess322.H512globline  1 2 3 4 5 6 7 8 9 10 15 24        3.303   273.638
  4C39.25    sess322.H512globline  1 2 3 4 5 6 7 8 9 10 15 24        0.500    49.341
  3C279      sess322.H512globline  15 24                             0.167     8.823


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   J1100+1002          54.4
   J1103+1158          54.6
   4C39.25             85.7
   3C279               21.6

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

