  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: 35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
 Exp. Code:  GB058   


Schedule Version:       2.00                                              
Processed by SCHED version:   6.04  March 2006                            

PI:       N. Bartel, M.P. Rupen                                           

Address:  York University                                                 
          Toronto, ON M3J 1P3                                             
          Canada                                                          
                                                                          

Phone:    +1-416-736-5424 (work)                                          
EMAIL:    bartel@yorku.ca                                                 
Fax:      +1-416-736-5516                                                 
Phone during observation: +1-416-483-9068 (home)                          

Observing mode: VLBA 512-16-2 6cm                                         

Notes:    Fringe finder  : 0954+658                                       
          Pol. Calibrator: 0954+658, OQ208                                
          Amplitude check: 0954+658, OQ208                                
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

 Next scan frequencies:  4958.49  4958.49  4958.49  4958.49  4974.49  4974.49
                         4974.49  4974.49  4990.49  4990.49  4990.49  4990.49
                         5006.49  5006.49  5006.49  5006.49
 Next BBC frequencies:    858.49   858.49   858.49   858.49   874.49   874.49
                          874.49   874.49   890.49   890.49   890.49   890.49
                          906.49   906.49   906.49   906.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00     8.00     8.00     8.00     8.00
                            8.00     8.00     8.00     8.00

17 40 00  0954+658     04 23 37  30.1  28.4 -5.6     -81.5     0   1  1      0  17 40 00
17 43 00  ---          04 26 38  30.4  28.5 -5.5     -82.2   180   F  1     12  17 40 18

17 43 00  M81          04 26 38  31.1  24.5 -5.5     -84.9    -9   1  1     12  17 43 00
17 45 20  ---          04 28 58  31.3  24.5 -5.5     -85.5   131   F  1     21  17 43 00

17 45 20  SN1993J      04 28 58  31.3  24.5 -5.4     -85.5    -5   1  1     21  17 45 20
17 47 20  ---          04 30 58  31.5  24.6 -5.4     -85.9   115   F  1     28  17 45 20

17 47 20  M81          04 30 58  31.5  24.5 -5.4     -85.9    -5   1  1     28  17 47 20
17 48 30  ---          04 32 09  31.6  24.5 -5.4     -86.2    65   F  1     33  17 47 20

17 48 30  SN1993J      04 32 09  31.6  24.6 -5.4     -86.2    -5   1  1     33  17 48 30
17 50 30  ---          04 34 09  31.8  24.6 -5.4     -86.7   115   F  1     41  17 48 30

17 50 30  M81          04 34 09  31.8  24.5 -5.4     -86.7    -5   1  1     41  17 50 30
17 51 40  ---          04 35 19  31.9  24.5 -5.3     -86.9    65   F  1     45  17 50 30

17 51 40  SN1993J      04 35 19  31.9  24.6 -5.3     -86.9    -5   1  1     45  17 51 40
17 53 40  ---          04 37 19  32.1  24.6 -5.3     -87.4   115   F  1     53  17 51 40

17 53 40  M81          04 37 19  32.1  24.5 -5.3     -87.4    -5   1  1     53  17 53 40
17 54 50  ---          04 38 30  32.2  24.5 -5.3     -87.7    65   F  1     57  17 53 40

17 54 50  SN1993J      04 38 30  32.2  24.6 -5.3     -87.7    -5   1  1     57  17 54 50
17 56 50  ---          04 40 30  32.4  24.6 -5.3     -88.1   115   F  1     65  17 54 50

17 56 50  M81          04 40 30  32.4  24.6 -5.3     -88.1    -5   1  1     65  17 56 50
17 58 00  ---          04 41 40  32.5  24.6 -5.2     -88.4    65   F  1     70  17 56 50

17 58 00  SN1993J      04 41 40  32.5  24.6 -5.2     -88.4    -5   1  1     70  17 58 00
18 00 00  ---          04 43 40  32.6  24.6 -5.2     -88.9   115   F  1     77  17 58 00
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

18 00 00  M81          04 43 40  32.6  24.6 -5.2     -88.9    -5   1  1     77  18 00 00
18 02 00  ---          04 45 41  32.8  24.6 -5.2     -89.3   115   F  1     85  18 00 00

18 02 40  M81          04 46 21  32.9  24.6 -5.2     -89.5    35   1  1     85  18 02 40
18 04 50  ---          04 48 31  33.1  24.6 -5.1     -90.0   130   F  1     94  18 02 58

18 04 50  SN1993J      04 48 31  33.1  24.6 -5.1     -90.0    -5   1  1     94  18 04 50
18 06 50  ---          04 50 32  33.3  24.6 -5.1     -90.5   115   F  1    101  18 04 50

18 06 50  M81          04 50 32  33.3  24.6 -5.1     -90.5    -5   1  1    101  18 06 50
18 08 00  ---          04 51 42  33.4  24.6 -5.1     -90.7    65   F  1    106  18 06 50

18 08 00  SN1993J      04 51 42  33.4  24.6 -5.1     -90.7    -5   1  1    106  18 08 00
18 10 00  ---          04 53 42  33.5  24.6 -5.0     -91.2   115   F  1    114  18 08 00

18 10 00  M81          04 53 42  33.5  24.6 -5.0     -91.2    -5   1  1    114  18 10 00
18 11 10  ---          04 54 52  33.6  24.6 -5.0     -91.5    65   F  1    118  18 10 00

18 11 10  SN1993J      04 54 52  33.7  24.6 -5.0     -91.5    -5   1  1    118  18 11 10
18 13 10  ---          04 56 53  33.8  24.6 -5.0     -92.0   115   F  1    126  18 11 10

18 13 10  M81          04 56 53  33.8  24.6 -5.0     -92.0    -5   1  1    126  18 13 10
18 14 20  ---          04 58 03  33.9  24.5 -5.0     -92.2    65   F  1    130  18 13 10

18 14 20  SN1993J      04 58 03  33.9  24.6 -5.0     -92.2    -5   1  1    130  18 14 20
18 16 20  ---          05 00 03  34.1  24.6 -4.9     -92.7   115   F  1    138  18 14 20

18 16 20  M81          05 00 03  34.1  24.5 -4.9     -92.7    -5   1  1    138  18 16 20
18 17 30  ---          05 01 13  34.2  24.5 -4.9     -93.0    65   F  1    143  18 16 20

18 17 30  SN1993J      05 01 13  34.2  24.6 -4.9     -93.0    -5   1  1    143  18 17 30
18 19 30  ---          05 03 14  34.4  24.6 -4.9     -93.5   115   F  1    150  18 17 30

18 19 30  M81          05 03 14  34.4  24.5 -4.9     -93.5    -5   1  1    150  18 19 30
18 20 40  ---          05 04 24  34.5  24.5 -4.9     -93.7    65   F  1    155  18 19 30

18 20 40  SN1993J      05 04 24  34.5  24.6 -4.9     -93.7    -5   1  1    155  18 20 40
18 22 40  ---          05 06 24  34.7  24.5 -4.8     -94.2   115   F  1    163  18 20 40

18 22 40  M81          05 06 24  34.7  24.5 -4.8     -94.2    -5   1  1    163  18 22 40
18 24 40  ---          05 08 25  34.8  24.5 -4.8     -94.7   115   F  1    170  18 22 40

18 34 40  0954+658     05 18 26  35.8  28.7 -4.7     -93.8   591   1  1    170  18 34 40
18 37 40  ---          05 21 27  36.1  28.7 -4.6     -94.5   180   F  1    182  18 34 58
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

18 37 40  M81          05 21 27  36.0  24.3 -4.6     -97.8    -9   1  1    182  18 37 40
18 40 00  ---          05 23 47  36.2  24.3 -4.5     -98.4   131   F  1    191  18 37 40

18 40 00  SN1993J      05 23 47  36.2  24.3 -4.5     -98.4    -5   1  1    191  18 40 00
18 42 00  ---          05 25 47  36.4  24.3 -4.5     -98.9   115   F  1    199  18 40 00

18 42 00  M81          05 25 47  36.4  24.3 -4.5     -98.9    -5   1  1    199  18 42 00
18 43 10  ---          05 26 58  36.5  24.2 -4.5     -99.2    65   F  1    203  18 42 00

18 43 10  SN1993J      05 26 58  36.5  24.3 -4.5     -99.2    -5   1  1    203  18 43 10
18 45 10  ---          05 28 58  36.7  24.2 -4.4     -99.7   115   F  1    211  18 43 10

18 45 10  M81          05 28 58  36.7  24.2 -4.5     -99.7    -5   1  1    211  18 45 10
18 46 20  ---          05 30 08  36.8  24.2 -4.4     -99.9    65   F  1    215  18 45 10

18 46 20  SN1993J      05 30 08  36.8  24.2 -4.4     -99.9    -5   1  1    215  18 46 20
18 48 20  ---          05 32 08  37.0  24.2 -4.4    -100.4   115   F  1    223  18 46 20

18 48 20  M81          05 32 08  37.0  24.1 -4.4    -100.4    -5   1  1    223  18 48 20
18 49 30  ---          05 33 19  37.1  24.1 -4.4    -100.7    65   F  1    228  18 48 20

18 49 30  SN1993J      05 33 19  37.1  24.2 -4.4    -100.7    -5   1  1    228  18 49 30
18 51 30  ---          05 35 19  37.3  24.1 -4.3    -101.2   115   F  1    235  18 49 30

18 51 30  M81          05 35 19  37.2  24.1 -4.3    -101.2    -5   1  1    235  18 51 30
18 52 40  ---          05 36 29  37.3  24.0 -4.3    -101.5    65   F  1    240  18 51 30

18 52 40  SN1993J      05 36 29  37.4  24.1 -4.3    -101.5    -5   1  1    240  18 52 40
18 54 40  ---          05 38 29  37.5  24.0 -4.3    -102.0   115   F  1    248  18 52 40

18 54 40  M81          05 38 29  37.5  24.0 -4.3    -102.0    -5   1  1    248  18 54 40
18 56 40  ---          05 40 30  37.7  23.9 -4.3    -102.5   115   F  1    255  18 54 40

18 57 20  M81          05 41 10  37.7  23.9 -4.2    -102.7    35   1  1    255  18 57 20
18 59 30  ---          05 43 20  37.9  23.9 -4.2    -103.2   130   F  1    264  18 57 38

18 59 30  SN1993J      05 43 20  38.0  23.9 -4.2    -103.2    -5   1  1    264  18 59 30
19 01 30  ---          05 45 21  38.1  23.9 -4.2    -103.7   115   F  1    272  18 59 30

19 01 30  M81          05 45 21  38.1  23.8 -4.2    -103.7    -5   1  1    272  19 01 30
19 02 40  ---          05 46 31  38.2  23.8 -4.2    -104.0    65   F  1    276  19 01 30

19 02 40  SN1993J      05 46 31  38.2  23.8 -4.2    -104.0    -5   1  1    276  19 02 40
19 04 40  ---          05 48 31  38.4  23.8 -4.1    -104.5   115   F  1    284  19 02 40
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

19 04 40  M81          05 48 31  38.4  23.7 -4.1    -104.5    -5   1  1    284  19 04 40
19 05 50  ---          05 49 41  38.5  23.7 -4.1    -104.8    65   F  1    288  19 04 40

19 05 50  SN1993J      05 49 41  38.5  23.8 -4.1    -104.8    -5   1  1    288  19 05 50
19 07 50  ---          05 51 42  38.7  23.7 -4.1    -105.3   115   F  1    296  19 05 50

19 07 50  M81          05 51 42  38.7  23.6 -4.1    -105.3    -5   1  1    296  19 07 50
19 09 00  ---          05 52 52  38.8  23.6 -4.1    -105.6    65   F  1    301  19 07 50

19 09 00  SN1993J      05 52 52  38.8  23.7 -4.1    -105.6    -5   1  1    301  19 09 00
19 11 00  ---          05 54 52  39.0  23.6 -4.0    -106.1   115   F  1    308  19 09 00

19 11 00  M81          05 54 52  38.9  23.5 -4.0    -106.1    -5   1  1    308  19 11 00
19 12 10  ---          05 56 02  39.0  23.5 -4.0    -106.4    65   F  1    313  19 11 00

19 12 10  SN1993J      05 56 02  39.1  23.6 -4.0    -106.4    -5   1  1    313  19 12 10
19 14 10  ---          05 58 03  39.2  23.5 -4.0    -106.9   115   F  1    321  19 12 10

19 14 10  M81          05 58 03  39.2  23.4 -4.0    -106.9    -5   1  1    321  19 14 10
19 15 20  ---          05 59 13  39.3  23.4 -3.9    -107.2    65   F  1    325  19 14 10

19 15 20  SN1993J      05 59 13  39.3  23.4 -3.9    -107.2    -5   1  1    325  19 15 20
19 17 20  ---          06 01 13  39.5  23.4 -3.9    -107.7   115   F  1    333  19 15 20

19 17 20  M81          06 01 13  39.5  23.3 -3.9    -107.7    -5   1  1    333  19 17 20
19 19 20  ---          06 03 14  39.6  23.3 -3.9    -108.2   115   F  1    341  19 17 20

19 20 00  M81          06 03 54  39.7  23.2 -3.9    -108.4    35   1  1    341  19 20 00
19 22 10  ---          06 06 04  39.9  23.2 -3.8    -109.0   130   F  1    349  19 20 18

19 22 10  SN1993J      06 06 04  39.9  23.2 -3.8    -109.0    -5   1  1    349  19 22 10
19 24 10  ---          06 08 04  40.1  23.1 -3.8    -109.5   115   F  1    357  19 22 10

19 24 10  M81          06 08 04  40.1  23.1 -3.8    -109.5    -5   1  1    357  19 24 10
19 25 20  ---          06 09 15  40.2  23.0 -3.8    -109.8    65   F  1    361  19 24 10

19 25 20  SN1993J      06 09 15  40.2  23.1 -3.8    -109.8    -5   1  1    361  19 25 20
19 27 20  ---          06 11 15  40.3  23.0 -3.7    -110.3   115   F  1    369  19 25 20

19 27 20  M81          06 11 15  40.3  22.9 -3.7    -110.3    -5   1  1    369  19 27 20
19 28 30  ---          06 12 25  40.4  22.9 -3.7    -110.6    65   F  1    374  19 27 20

19 28 30  SN1993J      06 12 25  40.4  22.9 -3.7    -110.6    -5   1  1    374  19 28 30
19 30 30  ---          06 14 25  40.6  22.9 -3.7    -111.1   115   F  1    381  19 28 30
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

19 30 30  M81          06 14 25  40.6  22.8 -3.7    -111.1    -5   1  1    381  19 30 30
19 31 40  ---          06 15 36  40.7  22.8 -3.7    -111.4    65   F  1    386  19 30 30

19 31 40  SN1993J      06 15 36  40.7  22.8 -3.7    -111.4    -5   1  1    386  19 31 40
19 33 40  ---          06 17 36  40.9  22.7 -3.6    -112.0   115   F  1    394  19 31 40

19 33 40  M81          06 17 36  40.8  22.7 -3.6    -112.0    -5   1  1    394  19 33 40
19 34 50  ---          06 18 46  40.9  22.6 -3.6    -112.3    65   F  1    398  19 33 40

19 34 50  SN1993J      06 18 46  41.0  22.7 -3.6    -112.3    -5   1  1    398  19 34 50
19 36 50  ---          06 20 46  41.1  22.6 -3.6    -112.8   115   F  1    406  19 34 50

19 36 50  M81          06 20 46  41.1  22.5 -3.6    -112.8    -5   1  1    406  19 36 50
19 38 00  ---          06 21 57  41.2  22.5 -3.6    -113.1    65   F  1    410  19 36 50

19 38 00  SN1993J      06 21 57  41.2  22.5 -3.6    -113.1    -5   1  1    410  19 38 00
19 40 00  ---          06 23 57  41.4  22.4 -3.5    -113.6   115   F  1    418  19 38 00

19 40 00  M81          06 23 57  41.4  22.4 -3.5    -113.6    -5   1  1    418  19 40 00
19 42 00  ---          06 25 57  41.5  22.3 -3.5    -114.2   115   F  1    426  19 40 00

19 42 40  M81          06 26 37  41.6  22.3 -3.5    -114.4    35   1  1    426  19 42 40
19 44 50  ---          06 28 48  41.8  22.1 -3.5    -114.9   130   F  1    434  19 42 58

19 44 50  SN1993J      06 28 48  41.8  22.2 -3.5    -114.9    -5   1  1    434  19 44 50
19 46 50  ---          06 30 48  42.0  22.1 -3.4    -115.5   115   F  1    442  19 44 50

19 46 50  M81          06 30 48  41.9  22.0 -3.4    -115.5    -5   1  1    442  19 46 50
19 48 00  ---          06 31 58  42.0  22.0 -3.4    -115.8    65   F  1    446  19 46 50

19 48 00  SN1993J      06 31 58  42.1  22.0 -3.4    -115.8    -5   1  1    446  19 48 00
19 50 00  ---          06 33 59  42.2  21.9 -3.4    -116.3   115   F  1    454  19 48 00

19 50 00  M81          06 33 59  42.2  21.9 -3.4    -116.3    -5   1  1    454  19 50 00
19 51 10  ---          06 35 09  42.3  21.8 -3.3    -116.6    65   F  1    459  19 50 00

19 51 10  SN1993J      06 35 09  42.3  21.9 -3.3    -116.6    -5   1  1    459  19 51 10
19 53 10  ---          06 37 09  42.5  21.8 -3.3    -117.2   115   F  1    466  19 51 10

19 53 10  M81          06 37 09  42.4  21.7 -3.3    -117.2    -5   1  1    466  19 53 10
19 54 20  ---          06 38 19  42.5  21.6 -3.3    -117.5    65   F  1    471  19 53 10

19 54 20  SN1993J      06 38 19  42.6  21.7 -3.3    -117.5    -5   1  1    471  19 54 20
19 56 20  ---          06 40 20  42.7  21.6 -3.3    -118.0   115   F  1    479  19 54 20
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

19 56 20  M81          06 40 20  42.7  21.5 -3.3    -118.0    -5   1  1    479  19 56 20
19 57 30  ---          06 41 30  42.8  21.5 -3.2    -118.4    65   F  1    483  19 56 20

19 57 30  SN1993J      06 41 30  42.8  21.5 -3.2    -118.4    -5   1  1    483  19 57 30
19 59 30  ---          06 43 30  43.0  21.4 -3.2    -118.9   115   F  1    491  19 57 30

19 59 30  M81          06 43 30  42.9  21.3 -3.2    -118.9    -5   1  1    491  19 59 30
20 00 40  ---          06 44 40  43.0  21.3 -3.2    -119.2    65   F  1    495  19 59 30

20 00 40  SN1993J      06 44 40  43.1  21.3 -3.2    -119.2    -5   1  1    495  20 00 40
20 02 40  ---          06 46 41  43.2  21.2 -3.2    -119.8   115   F  1    503  20 00 40

20 02 40  M81          06 46 41  43.2  21.2 -3.2    -119.8    -5   1  1    503  20 02 40
20 04 40  ---          06 48 41  43.3  21.0 -3.1    -120.3   115   F  1    511  20 02 40

20 05 20  M81          06 49 21  43.4  21.0 -3.1    -120.5    35   1  1    511  20 05 20
20 07 30  ---          06 51 31  43.6  20.8 -3.1    -121.1   130   F  1    519  20 05 38

20 07 30  SN1993J      06 51 31  43.6  20.9 -3.1    -121.1    -5   1  1    519  20 07 30
20 09 30  ---          06 53 32  43.7  20.8 -3.0    -121.7   115   F  1    527  20 07 30

20 09 30  M81          06 53 32  43.7  20.7 -3.0    -121.7    -5   1  1    527  20 09 30
20 10 40  ---          06 54 42  43.8  20.6 -3.0    -122.0    65   F  1    532  20 09 30

20 10 40  SN1993J      06 54 42  43.8  20.7 -3.0    -122.0    -5   1  1    532  20 10 40
20 12 40  ---          06 56 42  44.0  20.6 -3.0    -122.6   115   F  1    539  20 10 40

20 12 40  M81          06 56 42  44.0  20.5 -3.0    -122.6    -5   1  1    539  20 12 40
20 13 50  ---          06 57 52  44.0  20.4 -3.0    -122.9    65   F  1    544  20 12 40

20 13 50  SN1993J      06 57 52  44.1  20.5 -3.0    -122.9    -5   1  1    544  20 13 50
20 15 50  ---          06 59 53  44.2  20.3 -2.9    -123.5   115   F  1    552  20 13 50

20 15 50  M81          06 59 53  44.2  20.3 -2.9    -123.5    -5   1  1    552  20 15 50
20 17 00  ---          07 01 03  44.3  20.2 -2.9    -123.8    65   F  1    556  20 15 50

20 17 00  SN1993J      07 01 03  44.3  20.3 -2.9    -123.8    -5   1  1    556  20 17 00
20 19 00  ---          07 03 03  44.5  20.1 -2.9    -124.4   115   F  1    564  20 17 00

20 19 00  M81          07 03 03  44.4  20.1 -2.9    -124.3    -5   1  1    564  20 19 00
20 20 10  ---          07 04 14  44.5  20.0 -2.9    -124.7    65   F  1    568  20 19 00

20 20 10  SN1993J      07 04 14  44.6  20.0 -2.9    -124.7    -5   1  1    568  20 20 10
20 22 10  ---          07 06 14  44.7  19.9 -2.8    -125.3   115   F  1    576  20 20 10
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

20 22 10  M81          07 06 14  44.7  19.8 -2.8    -125.2    -5   1  1    576  20 22 10
20 23 20  ---          07 07 24  44.7  19.8 -2.8    -125.6    65   F  1    581  20 22 10

20 23 20  SN1993J      07 07 24  44.8  19.8 -2.8    -125.6    -5   1  1    581  20 23 20
20 25 20  ---          07 09 24  44.9  19.7 -2.8    -126.2   115   F  1    588  20 23 20

20 25 20  M81          07 09 24  44.9  19.6 -2.8    -126.2    -5   1  1    588  20 25 20
20 27 20  ---          07 11 25  45.0  19.5 -2.7    -126.7   115   F  1    596  20 25 20

20 37 20  0954+658     07 21 26  47.6  23.0 -2.6    -125.8   589   1  1    596  20 37 20
20 40 20  ---          07 24 27  47.9  22.7 -2.6    -126.6   180   F  1    608  20 37 38

20 40 20  M81          07 24 27  45.9  18.4 -2.5    -130.5   -10   1  1    608  20 40 20
20 42 40  ---          07 26 47  46.1  18.2 -2.5    -131.2   130   F  1    617  20 40 20

20 42 40  SN1993J      07 26 47  46.1  18.3 -2.5    -131.2    -5   1  1    617  20 42 40
20 44 40  ---          07 28 48  46.3  18.1 -2.5    -131.8   115   F  1    624  20 42 40

20 44 40  M81          07 28 48  46.2  18.1 -2.5    -131.8    -5   1  1    624  20 44 40
20 45 50  ---          07 29 58  46.3  18.0 -2.4    -132.1    65   F  1    629  20 44 40

20 45 50  SN1993J      07 29 58  46.4  18.0 -2.4    -132.1    -5   1  1    629  20 45 50
20 47 50  ---          07 31 58  46.5  17.8 -2.4    -132.7   115   F  1    637  20 45 50

20 47 50  M81          07 31 58  46.4  17.8 -2.4    -132.7    -5   1  1    637  20 47 50
20 49 00  ---          07 33 08  46.5  17.7 -2.4    -133.1    65   F  1    641  20 47 50

20 49 00  SN1993J      07 33 08  46.6  17.7 -2.4    -133.1    -5   1  1    641  20 49 00
20 51 00  ---          07 35 09  46.7  17.5 -2.3    -133.7   115   F  1    649  20 49 00

20 51 00  M81          07 35 09  46.7  17.5 -2.3    -133.7    -5   1  1    649  20 51 00
20 52 10  ---          07 36 19  46.7  17.4 -2.3    -134.0    65   F  1    654  20 51 00

20 52 10  SN1993J      07 36 19  46.8  17.4 -2.3    -134.0    -5   1  1    654  20 52 10
20 54 10  ---          07 38 19  46.9  17.2 -2.3    -134.6   115   F  1    661  20 52 10

20 54 10  M81          07 38 19  46.9  17.2 -2.3    -134.6    -5   1  1    661  20 54 10
20 55 20  ---          07 39 29  46.9  17.1 -2.3    -135.0    65   F  1    666  20 54 10

20 55 20  SN1993J      07 39 29  47.0  17.1 -2.3    -135.0    -5   1  1    666  20 55 20
20 57 20  ---          07 41 30  47.1  16.9 -2.2    -135.6   115   F  1    674  20 55 20

20 57 20  M81          07 41 30  47.1  16.9 -2.2    -135.6    -5   1  1    674  20 57 20
20 59 20  ---          07 43 30  47.2  16.7 -2.2    -136.2   115   F  1    681  20 57 20
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

21 00 00  M81          07 44 10  47.2  16.7 -2.2    -136.4    35   1  1    681  21 00 00
21 02 10  ---          07 46 20  47.4  16.5 -2.2    -137.1   130   F  1    690  21 00 18

21 02 10  SN1993J      07 46 20  47.4  16.5 -2.2    -137.1    -5   1  1    690  21 02 10
21 04 10  ---          07 48 21  47.5  16.3 -2.1    -137.7   115   F  1    697  21 02 10

21 04 10  M81          07 48 21  47.5  16.3 -2.1    -137.7    -5   1  1    697  21 04 10
21 05 20  ---          07 49 31  47.6  16.1 -2.1    -138.0    65   F  1    702  21 04 10

21 05 20  SN1993J      07 49 31  47.6  16.2 -2.1    -138.0    -5   1  1    702  21 05 20
21 07 20  ---          07 51 31  47.7  16.0 -2.1    -138.7   115   F  1    710  21 05 20

21 07 20  M81          07 51 31  47.7  15.9 -2.1    -138.6    -5   1  1    710  21 07 20
21 08 30  ---          07 52 41  47.7  15.8 -2.1    -139.0    65   F  1    714  21 07 20

21 08 30  SN1993J      07 52 41  47.8  15.9 -2.1    -139.0    -5   1  1    714  21 08 30
21 10 30  ---          07 54 42  47.9  15.7 -2.0    -139.6   115   F  1    722  21 08 30

21 10 30  M81          07 54 42  47.9  15.6 -2.0    -139.6    -5   1  1    722  21 10 30
21 11 40  ---          07 55 52  47.9  15.5 -2.0    -140.0    65   F  1    726  21 10 30

21 11 40  SN1993J      07 55 52  48.0  15.5 -2.0    -140.0    -5   1  1    726  21 11 40
21 13 40  ---          07 57 52  48.1  15.3 -2.0    -140.6   115   F  1    734  21 11 40

21 13 40  M81          07 57 52  48.0  15.3 -2.0    -140.6    -5   1  1    734  21 13 40
21 14 50  ---          07 59 02  48.1  15.2 -2.0    -141.0    65   F  1    739  21 13 40

21 14 50  SN1993J      07 59 02  48.1  15.2 -1.9    -141.0    -5   1  1    739  21 14 50
21 16 50  ---          08 01 03  48.3  15.0 -1.9    -141.6   115   F  1    746  21 14 50

21 16 50  M81          08 01 03  48.2  15.0 -1.9    -141.6    -5   1  1    746  21 16 50
21 18 00  ---          08 02 13  48.3  14.8 -1.9    -142.0    65   F  1    751  21 16 50

21 18 00  SN1993J      08 02 13  48.3  14.9 -1.9    -142.0    -5   1  1    751  21 18 00
21 20 00  ---          08 04 13  48.4  14.7 -1.9    -142.6   115   F  1    759  21 18 00

21 20 00  M81          08 04 13  48.4  14.6 -1.9    -142.6    -5   1  1    759  21 20 00
21 22 00  ---          08 06 14  48.5  14.4 -1.8    -143.2   115   F  1    766  21 20 00

21 22 40  M81          08 06 54  48.5  14.3 -1.8    -143.4    35   1  1    766  21 22 40
21 24 50  ---          08 09 04  48.7  14.1 -1.8    -144.1   130   F  1    775  21 22 58

21 24 50  SN1993J      08 09 04  48.7  14.1 -1.8    -144.1    -5   1  1    775  21 24 50
21 26 50  ---          08 11 04  48.8  13.9 -1.7    -144.8   115   F  1    783  21 24 50
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

21 26 50  M81          08 11 04  48.8  13.9 -1.7    -144.7    -5   1  1    783  21 26 50
21 28 00  ---          08 12 15  48.8  13.8 -1.7    -145.1    65   F  1    787  21 26 50

21 28 00  SN1993J      08 12 15  48.9  13.8 -1.7    -145.1    -5   1  1    787  21 28 00
21 30 00  ---          08 14 15  49.0  13.6 -1.7    -145.8   115   F  1    795  21 28 00

21 30 00  M81          08 14 15  48.9  13.5 -1.7    -145.8    -5   1  1    795  21 30 00
21 31 10  ---          08 15 25  49.0  13.4 -1.7    -146.1    65   F  1    799  21 30 00

21 31 10  SN1993J      08 15 25  49.0  13.4 -1.7    -146.1    -5   1  1    799  21 31 10
21 33 10  ---          08 17 26  49.1  13.2 -1.6    -146.8   115   F  1    807  21 31 10

21 33 10  M81          08 17 26  49.1  13.2 -1.6    -146.8    -5   1  1    807  21 33 10
21 34 20  ---          08 18 36  49.1  13.0 -1.6    -147.1    65   F  1    812  21 33 10

21 34 20  SN1993J      08 18 36  49.2  13.1 -1.6    -147.2    -5   1  1    812  21 34 20
21 36 20  ---          08 20 36  49.3  12.8 -1.6    -147.8   115   F  1    819  21 34 20

21 36 20  M81          08 20 36  49.2  12.8 -1.6    -147.8    -5   1  1    819  21 36 20
21 37 30  ---          08 21 46  49.3  12.7 -1.6    -148.2    65   F  1    824  21 36 20

21 37 30  SN1993J      08 21 46  49.3  12.7 -1.6    -148.2    -5   1  1    824  21 37 30
21 39 30  ---          08 23 47  49.4  12.5 -1.5    -148.8   115   F  1    832  21 37 30

21 39 30  M81          08 23 47  49.4  12.4 -1.5    -148.8    -5   1  1    832  21 39 30
21 40 40  ---          08 24 57  49.4  12.3 -1.5    -149.2    65   F  1    836  21 39 30

21 40 40  SN1993J      08 24 57  49.5  12.3 -1.5    -149.2    -5   1  1    836  21 40 40
21 42 40  ---          08 26 57  49.6  12.1 -1.5    -149.9   115   F  1    844  21 40 40

21 42 40  M81          08 26 57  49.5  12.1 -1.5    -149.8    -5   1  1    844  21 42 40
21 44 40  ---          08 28 57  49.6  11.8 -1.5    -150.5   115   F  1    852  21 42 40

21 45 20  M81          08 29 38  49.6  11.7 -1.4    -150.7    35   1  1    852  21 45 20
21 47 30  ---          08 31 48  49.7  11.5 -1.4    -151.4   130   F  1    860  21 45 38

21 47 30  SN1993J      08 31 48  49.8  11.5 -1.4    -151.4    -5   1  1    860  21 47 30
21 49 30  ---          08 33 48  49.9  11.2 -1.4    -152.1   115   F  1    868  21 47 30

21 49 30  M81          08 33 48  49.8  11.2 -1.4    -152.1    -5   1  1    868  21 49 30
21 50 40  ---          08 34 58  49.9  11.1 -1.4    -152.4    65   F  1    872  21 49 30

21 50 40  SN1993J      08 34 58  49.9  11.1 -1.3    -152.5    -5   1  1    872  21 50 40
21 52 40  ---          08 36 59  50.0  10.9 -1.3    -153.1   115   F  1    880  21 50 40
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

21 52 40  M81          08 36 59  50.0  10.8 -1.3    -153.1    -5   1  1    880  21 52 40
21 53 50  ---          08 38 09  50.0  10.7 -1.3    -153.5    65   F  1    884  21 52 40

21 53 50  SN1993J      08 38 09  50.0  10.7 -1.3    -153.5    -5   1  1    884  21 53 50
21 55 50  ---          08 40 09  50.1  10.5 -1.3    -154.2   115   F  1    892  21 53 50

21 55 50  M81          08 40 09  50.1  10.4 -1.3    -154.1    -5   1  1    892  21 55 50
21 57 00  ---          08 41 19  50.1  10.3 -1.2    -154.5    65   F  1    897  21 55 50

21 57 00  SN1993J      08 41 19  50.2  10.3 -1.2    -154.6    -5   1  1    897  21 57 00
21 59 00  ---          08 43 20  50.2  10.1 -1.2    -155.2   115   F  1    904  21 57 00

21 59 00  M81          08 43 20  50.2  10.0 -1.2    -155.2    -5   1  1    904  21 59 00
22 00 10  ---          08 44 30  50.2   9.9 -1.2    -155.6    65   F  1    909  21 59 00

22 00 10  SN1993J      08 44 30  50.3   9.9 -1.2    -155.6    -5   1  1    909  22 00 10
22 02 10  ---          08 46 30  50.4   9.6 -1.2    -156.3   115   F  1    917  22 00 10

22 02 10  M81          08 46 30  50.3   9.6 -1.2    -156.2    -5   1  1    917  22 02 10
22 03 20  ---          08 47 40  50.4   9.5 -1.1    -156.6    65   F  1    921  22 02 10

22 03 20  SN1993J      08 47 40  50.4   9.5 -1.1    -156.7    -5   1  1    921  22 03 20
22 05 20  ---          08 49 41  50.5   9.2 -1.1    -157.3   115   F  1    929  22 03 20

22 05 20  M81          08 49 41  50.4   9.2 -1.1    -157.3    -5   1  1    929  22 05 20
22 07 20  ---          08 51 41  50.5   9.0 -1.1    -158.0   115   F  1    937  22 05 20

22 08 00  M81          08 52 21  50.5   8.9 -1.1    -158.2    35   1  1    937  22 08 00
22 10 10  ---          08 54 32  50.6   8.6 -1.0    -158.9   130   F  1    945  22 08 18

22 10 10  SN1993J      08 54 32  50.6   8.6 -1.0    -159.0    -5   1  1    945  22 10 10
22 12 10  ---          08 56 32  50.7   8.3 -1.0    -159.6   115   F  1    953  22 10 10

22 12 10  M81          08 56 32  50.7   8.3 -1.0    -159.6    -5   1  1    953  22 12 10
22 13 20  ---          08 57 42  50.7   8.2 -1.0    -160.0    65   F  1    957  22 12 10

22 13 20  SN1993J      08 57 42  50.7   8.2 -1.0    -160.0    -5   1  1    957  22 13 20
22 15 20  ---          08 59 42  50.8   7.9 -0.9    -160.7   115   F  1    965  22 13 20

22 15 20  M81          08 59 42  50.7   7.9 -0.9    -160.7    -5   1  1    965  22 15 20
22 16 30  ---          09 00 53  50.8   7.8 -0.9    -161.1    65   F  1    970  22 15 20

22 16 30  SN1993J      09 00 53  50.8   7.8 -0.9    -161.1    -5   1  1    970  22 16 30
22 18 30  ---          09 02 53  50.9   7.5 -0.9    -161.8   115   F  1    977  22 16 30
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

22 18 30  M81          09 02 53  50.8   7.5 -0.9    -161.7    -5   1  1    977  22 18 30
22 19 40  ---          09 04 03  50.9   7.3 -0.9    -162.1    65   F  1    982  22 18 30

22 19 40  SN1993J      09 04 03  50.9   7.3 -0.9    -162.2    -5   1  1    982  22 19 40
22 21 40  ---          09 06 03  51.0   7.1 -0.8    -162.8   115   F  1    990  22 19 40

22 21 40  M81          09 06 03  50.9   7.1 -0.8    -162.8    -5   1  1    990  22 21 40
22 22 50  ---          09 07 14  51.0   6.9 -0.8    -163.2    65   F  1    994  22 21 40

22 22 50  SN1993J      09 07 14  51.0   6.9 -0.8    -163.2    -5   1  1    994  22 22 50
22 24 50  ---          09 09 14  51.1   6.6 -0.8    -163.9   115   F  1   1002  22 22 50

22 24 50  M81          09 09 14  51.0   6.6 -0.8    -163.9    -5   1  1   1002  22 24 50
22 26 00  ---          09 10 24  51.0   6.5 -0.8    -164.3    65   F  1   1006  22 24 50

22 26 00  SN1993J      09 10 24  51.1   6.5 -0.8    -164.3    -5   1  1   1006  22 26 00
22 28 00  ---          09 12 25  51.1   6.2 -0.7    -165.0   115   F  1   1014  22 26 00

22 28 00  M81          09 12 25  51.1   6.2 -0.7    -165.0    -5   1  1   1014  22 28 00
22 30 00  ---          09 14 25  51.1   5.9 -0.7    -165.7   115   F  1   1022  22 28 00

22 40 00  0954+658     09 24 26  54.7   6.2 -0.6    -167.0   587   1  1   1022  22 40 00
22 43 00  ---          09 27 27  54.8   5.7 -0.5    -168.1   180   F  1   1033  22 40 18

22 43 00  M81          09 27 27  51.4   4.1 -0.5    -170.1   -13   1  1   1033  22 43 00
22 45 20  ---          09 29 47  51.4   3.8 -0.4    -170.9   127   F  1   1043  22 43 00

22 45 20  SN1993J      09 29 47  51.5   3.8 -0.4    -171.0    -5   1  1   1043  22 45 20
22 47 20  ---          09 31 48  51.5   3.5 -0.4    -171.6   115   F  1   1050  22 45 20

22 47 20  M81          09 31 48  51.4   3.5 -0.4    -171.6    -5   1  1   1050  22 47 20
22 48 30  ---          09 32 58  51.5   3.3 -0.4    -172.0    65   F  1   1055  22 47 20

22 48 30  SN1993J      09 32 58  51.5   3.3 -0.4    -172.1    -5   1  1   1055  22 48 30
22 50 30  ---          09 34 58  51.5   3.0 -0.3    -172.7   115   F  1   1063  22 48 30

22 50 30  M81          09 34 58  51.5   3.0 -0.4    -172.7    -5   1  1   1063  22 50 30
22 51 40  ---          09 36 08  51.5   2.9 -0.3    -173.1    65   F  1   1067  22 50 30

22 51 40  SN1993J      09 36 08  51.5   2.8 -0.3    -173.1    -5   1  1   1067  22 51 40
22 53 40  ---          09 38 09  51.6   2.6 -0.3    -173.8   115   F  1   1075  22 51 40

22 53 40  M81          09 38 09  51.5   2.6 -0.3    -173.8    -5   1  1   1075  22 53 40
22 54 50  ---          09 39 19  51.5   2.4 -0.3    -174.2    65   F  1   1079  22 53 40
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

22 54 50  SN1993J      09 39 19  51.6   2.4 -0.3    -174.2    -5   1  1   1079  22 54 50
22 56 50  ---          09 41 19  51.6   2.1 -0.2    -174.9   115   F  1   1087  22 54 50

22 56 50  M81          09 41 19  51.5   2.1 -0.2    -174.9    -5   1  1   1087  22 56 50
22 58 00  ---          09 42 29  51.5   2.0 -0.2    -175.3    65   F  1   1092  22 56 50

22 58 00  SN1993J      09 42 29  51.6   1.9 -0.2    -175.3    -5   1  1   1092  22 58 00
23 00 00  ---          09 44 30  51.6   1.6 -0.2    -176.0   115   F  1   1099  22 58 00

23 00 00  M81          09 44 30  51.6   1.7 -0.2    -176.0    -5   1  1   1099  23 00 00
23 02 00  ---          09 46 30  51.6   1.4 -0.2    -176.7   115   F  1   1107  23 00 00

23 02 40  M81          09 47 10  51.6   1.3 -0.1    -176.9    35   1  1   1107  23 02 40
23 04 50  ---          09 49 21  51.6   1.0 -0.1    -177.7   130   F  1   1115  23 02 58

23 04 50  SN1993J      09 49 21  51.6   1.0 -0.1    -177.7    -5   1  1   1115  23 04 50
23 06 50  ---          09 51 21  51.6   0.7 -0.1    -178.4   115   F  1   1123  23 04 50

23 06 50  M81          09 51 21  51.6   0.7 -0.1    -178.4    -5   1  1   1123  23 06 50
23 08 00  ---          09 52 31  51.6   0.5 -0.1    -178.8    65   F  1   1128  23 06 50

23 08 00  SN1993J      09 52 31  51.6   0.5 -0.1    -178.8    -5   1  1   1128  23 08 00
23 10 00  ---          09 54 31  51.6   0.2  0.0    -179.5   115   F  1   1135  23 08 00

23 10 00  M81          09 54 31  51.6   0.2  0.0    -179.5    -5   1  1   1135  23 10 00
23 11 10  ---          09 55 42  51.6   0.1  0.0    -179.9    65   F  1   1140  23 10 00

23 11 10  SN1993J      09 55 42  51.6   0.0  0.0    -179.9    -5   1  1   1140  23 11 10
23 13 10  ---          09 57 42  51.6  -0.3  0.0     179.4   115   F  1   1148  23 11 10

23 13 10  M81          09 57 42  51.6  -0.2  0.0     179.4    -5   1  1   1148  23 13 10
23 14 20  ---          09 58 52  51.6  -0.4  0.0     179.0    65   F  1   1152  23 13 10

23 14 20  SN1993J      09 58 52  51.6  -0.4  0.0     179.0    -5   1  1   1152  23 14 20
23 16 20  ---          10 00 52  51.6  -0.7  0.1     178.3   115   F  1   1160  23 14 20

23 16 20  M81          10 00 52  51.6  -0.7  0.1     178.3    -5   1  1   1160  23 16 20
23 17 30  ---          10 02 03  51.6  -0.9  0.1     177.9    65   F  1   1164  23 16 20

23 17 30  SN1993J      10 02 03  51.6  -0.9  0.1     177.9    -5   1  1   1164  23 17 30
23 19 30  ---          10 04 03  51.6  -1.2  0.1     177.2   115   F  1   1172  23 17 30

23 19 30  M81          10 04 03  51.6  -1.1  0.1     177.2    -5   1  1   1172  23 19 30
23 20 40  ---          10 05 13  51.6  -1.3  0.2     176.8    65   F  1   1177  23 19 30
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Fri  16 Jun 2006   Day 167 ---

23 20 40  SN1993J      10 05 13  51.6  -1.3  0.2     176.8    -5   1  1   1177  23 20 40
23 22 40  ---          10 07 13  51.6  -1.6  0.2     176.1   115   F  1   1184  23 20 40

23 22 40  M81          10 07 13  51.6  -1.6  0.2     176.1    -5   1  1   1184  23 22 40
23 24 40  ---          10 09 14  51.5  -1.9  0.2     175.4   115   F  1   1192  23 22 40

23 54 40  M81          10 39 19  51.1  -6.1  0.7     165.1  1791   1  1   1192  23 54 40
23 56 50  ---          10 41 29  51.0  -6.4  0.8     164.4   130   F  1   1201  23 54 58

23 56 50  SN1993J      10 41 29  51.1  -6.5  0.8     164.3    -5   1  1   1201  23 56 50
23 58 50  ---          10 43 29  51.0  -6.7  0.8     163.6   115   F  1   1208  23 56 50

23 58 50  M81          10 43 29  51.0  -6.7  0.8     163.7    -5   1  1   1208  23 58 50
23 59 59  ---          10 44 40  51.0  -6.9  0.8     163.3    64   F  1   1213  23 58 50

 --- Sat  17 Jun 2006   Day 168 ---

00 00 00  SN1993J      10 44 40  51.0  -6.9  0.8     163.2    -5   1  1   1213  23 59 59
00 02 00  ---          10 46 40  50.9  -7.2  0.8     162.5   115   F  1   1221  23 59 59

00 02 00  M81          10 46 40  50.9  -7.1  0.8     162.6    -5   1  1   1221  00 02 00
00 03 10  ---          10 47 50  50.9  -7.3  0.9     162.2    65   F  1   1225  00 02 00

00 03 10  SN1993J      10 47 50  50.9  -7.3  0.9     162.2    -5   1  1   1225  00 03 10
00 05 10  ---          10 49 50  50.9  -7.6  0.9     161.5   115   F  1   1233  00 03 10

00 05 10  M81          10 49 50  50.8  -7.6  0.9     161.5    -5   1  1   1233  00 05 10
00 06 20  ---          10 51 01  50.8  -7.7  0.9     161.1    65   F  1   1237  00 05 10

00 06 20  SN1993J      10 51 01  50.8  -7.8  0.9     161.1    -5   1  1   1237  00 06 20
00 08 20  ---          10 53 01  50.8  -8.0  1.0     160.4   115   F  1   1245  00 06 20

00 08 20  M81          10 53 01  50.7  -8.0  0.9     160.5    -5   1  1   1245  00 08 20
00 09 30  ---          10 54 11  50.7  -8.1  1.0     160.1    65   F  1   1250  00 08 20

00 09 30  SN1993J      10 54 11  50.7  -8.2  1.0     160.0    -5   1  1   1250  00 09 30
00 11 30  ---          10 56 12  50.7  -8.5  1.0     159.3   115   F  1   1257  00 09 30

00 11 30  M81          10 56 12  50.6  -8.4  1.0     159.4    -5   1  1   1257  00 11 30
00 12 40  ---          10 57 22  50.6  -8.6  1.0     159.0    65   F  1   1262  00 11 30

00 12 40  SN1993J      10 57 22  50.6  -8.6  1.0     158.9    -5   1  1   1262  00 12 40
00 14 40  ---          10 59 22  50.6  -8.9  1.1     158.3   115   F  1   1270  00 12 40
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

00 14 40  M81          10 59 22  50.5  -8.8  1.1     158.3    -5   1  1   1270  00 14 40
00 16 40  ---          11 01 22  50.5  -9.1  1.1     157.7   115   F  1   1277  00 14 40

00 17 20  M81          11 02 02  50.4  -9.2  1.1     157.4    35   1  1   1277  00 17 20
00 19 30  ---          11 04 13  50.4  -9.5  1.1     156.7   130   F  1   1286  00 17 38

00 19 30  SN1993J      11 04 13  50.4  -9.5  1.1     156.7    -5   1  1   1286  00 19 30
00 21 30  ---          11 06 13  50.3  -9.8  1.2     156.0   115   F  1   1293  00 19 30

00 21 30  M81          11 06 13  50.3  -9.7  1.2     156.1    -5   1  1   1293  00 21 30
00 22 40  ---          11 07 23  50.3  -9.9  1.2     155.7    65   F  1   1298  00 21 30

00 22 40  SN1993J      11 07 23  50.3  -9.9  1.2     155.6    -5   1  1   1298  00 22 40
00 24 40  ---          11 09 24  50.2 -10.2  1.2     154.9   115   F  1   1306  00 22 40

00 24 40  M81          11 09 24  50.2 -10.1  1.2     155.0    -5   1  1   1306  00 24 40
00 25 50  ---          11 10 34  50.1 -10.3  1.2     154.6    65   F  1   1310  00 24 40

00 25 50  SN1993J      11 10 34  50.2 -10.3  1.2     154.5    -5   1  1   1310  00 25 50
00 27 50  ---          11 12 34  50.1 -10.6  1.3     153.9   115   F  1   1318  00 25 50

00 27 50  M81          11 12 34  50.1 -10.5  1.3     154.0    -5   1  1   1318  00 27 50
00 29 00  ---          11 13 44  50.0 -10.7  1.3     153.6    65   F  1   1322  00 27 50

00 29 00  SN1993J      11 13 44  50.0 -10.7  1.3     153.5    -5   1  1   1322  00 29 00
00 31 00  ---          11 15 45  50.0 -11.0  1.3     152.8   115   F  1   1330  00 29 00

00 31 00  M81          11 15 45  49.9 -10.9  1.3     152.9    -5   1  1   1330  00 31 00
00 32 10  ---          11 16 55  49.9 -11.1  1.3     152.5    65   F  1   1335  00 31 00

00 32 10  SN1993J      11 16 55  49.9 -11.1  1.3     152.5    -5   1  1   1335  00 32 10
00 34 10  ---          11 18 55  49.8 -11.4  1.4     151.8   115   F  1   1342  00 32 10

00 34 10  M81          11 18 55  49.8 -11.3  1.4     151.9    -5   1  1   1342  00 34 10
00 35 20  ---          11 20 05  49.7 -11.4  1.4     151.5    65   F  1   1347  00 34 10

00 35 20  SN1993J      11 20 05  49.8 -11.5  1.4     151.4    -5   1  1   1347  00 35 20
00 37 20  ---          11 22 06  49.7 -11.7  1.4     150.8   115   F  1   1355  00 35 20

00 37 20  M81          11 22 06  49.7 -11.7  1.4     150.8    -5   1  1   1355  00 37 20
00 39 20  ---          11 24 06  49.6 -11.9  1.5     150.2   115   F  1   1362  00 37 20

00 40 00  M81          11 24 46  49.5 -12.0  1.5     150.0    35   1  1   1362  00 40 00
00 42 10  ---          11 26 57  49.4 -12.3  1.5     149.3   130   F  1   1371  00 40 18
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

00 42 10  SN1993J      11 26 57  49.5 -12.3  1.5     149.2    -5   1  1   1371  00 42 10
00 44 10  ---          11 28 57  49.4 -12.6  1.6     148.5   115   F  1   1379  00 42 10

00 44 10  M81          11 28 57  49.4 -12.5  1.5     148.6    -5   1  1   1379  00 44 10
00 45 20  ---          11 30 07  49.3 -12.6  1.6     148.2    65   F  1   1383  00 44 10

00 45 20  SN1993J      11 30 07  49.3 -12.7  1.6     148.2    -5   1  1   1383  00 45 20
00 47 20  ---          11 32 07  49.2 -12.9  1.6     147.5   115   F  1   1391  00 45 20

00 47 20  M81          11 32 07  49.2 -12.9  1.6     147.6    -5   1  1   1391  00 47 20
00 48 30  ---          11 33 18  49.1 -13.0  1.6     147.2    65   F  1   1395  00 47 20

00 48 30  SN1993J      11 33 18  49.2 -13.1  1.6     147.1    -5   1  1   1395  00 48 30
00 50 30  ---          11 35 18  49.1 -13.3  1.7     146.5   115   F  1   1403  00 48 30

00 50 30  M81          11 35 18  49.0 -13.2  1.7     146.6    -5   1  1   1403  00 50 30
00 51 40  ---          11 36 28  49.0 -13.4  1.7     146.2    65   F  1   1408  00 50 30

00 51 40  SN1993J      11 36 28  49.0 -13.4  1.7     146.1    -5   1  1   1408  00 51 40
00 53 40  ---          11 38 28  48.9 -13.6  1.7     145.5   115   F  1   1415  00 51 40

00 53 40  M81          11 38 28  48.9 -13.6  1.7     145.6    -5   1  1   1415  00 53 40
00 54 50  ---          11 39 39  48.8 -13.7  1.7     145.2    65   F  1   1420  00 53 40

00 54 50  SN1993J      11 39 39  48.9 -13.8  1.7     145.1    -5   1  1   1420  00 54 50
00 56 50  ---          11 41 39  48.8 -14.0  1.8     144.5   115   F  1   1428  00 54 50

00 56 50  M81          11 41 39  48.7 -13.9  1.8     144.6    -5   1  1   1428  00 56 50
00 58 00  ---          11 42 49  48.7 -14.1  1.8     144.2    65   F  1   1432  00 56 50

00 58 00  SN1993J      11 42 49  48.7 -14.1  1.8     144.1    -5   1  1   1432  00 58 00
01 00 00  ---          11 44 49  48.6 -14.4  1.8     143.5   115   F  1   1440  00 58 00

01 00 00  M81          11 44 49  48.6 -14.3  1.8     143.6    -5   1  1   1440  01 00 00
01 02 00  ---          11 46 50  48.5 -14.5  1.8     142.9   115   F  1   1448  01 00 00

01 07 00  OQ208        11 51 51  60.6  85.6 -2.3     -77.3   227   1  1   1448  01 07 00
01 09 10  ---          11 54 01  61.0  85.8 -2.2     -77.4   130   F  1   1456  01 07 18

01 09 10  M81          11 54 01  48.1 -15.3  2.0     140.7   -73   1  1   1456  01 09 10
01 12 20  ---          11 57 12  47.9 -15.6  2.0     139.7   117   F  1   1468  01 09 10

01 12 20  SN1993J      11 57 12  47.9 -15.7  2.0     139.6    -5   1  1   1468  01 12 20
01 14 20  ---          11 59 12  47.8 -15.9  2.1     139.0   115   F  1   1476  01 12 20
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

01 14 20  M81          11 59 12  47.8 -15.8  2.1     139.1    -5   1  1   1476  01 14 20
01 15 30  ---          12 00 22  47.7 -15.9  2.1     138.7    65   F  1   1481  01 14 20

01 15 30  SN1993J      12 00 22  47.7 -16.0  2.1     138.6    -5   1  1   1481  01 15 30
01 17 30  ---          12 02 22  47.6 -16.2  2.1     138.0   115   F  1   1488  01 15 30

01 17 30  M81          12 02 22  47.6 -16.1  2.1     138.1    -5   1  1   1488  01 17 30
01 18 40  ---          12 03 33  47.5 -16.2  2.1     137.7    65   F  1   1493  01 17 30

01 18 40  SN1993J      12 03 33  47.5 -16.3  2.1     137.7    -5   1  1   1493  01 18 40
01 20 40  ---          12 05 33  47.4 -16.5  2.2     137.1   115   F  1   1501  01 18 40

01 20 40  M81          12 05 33  47.4 -16.4  2.2     137.1    -5   1  1   1501  01 20 40
01 21 50  ---          12 06 43  47.3 -16.5  2.2     136.8    65   F  1   1505  01 20 40

01 21 50  SN1993J      12 06 43  47.3 -16.6  2.2     136.7    -5   1  1   1505  01 21 50
01 23 50  ---          12 08 43  47.2 -16.8  2.2     136.1   115   F  1   1513  01 21 50

01 23 50  M81          12 08 43  47.2 -16.7  2.2     136.2    -5   1  1   1513  01 23 50
01 25 00  ---          12 09 54  47.1 -16.8  2.2     135.8    65   F  1   1517  01 23 50

01 25 00  SN1993J      12 09 54  47.1 -16.9  2.2     135.7    -5   1  1   1517  01 25 00
01 27 00  ---          12 11 54  47.0 -17.1  2.3     135.1   115   F  1   1525  01 25 00

01 27 00  M81          12 11 54  47.0 -17.0  2.3     135.2    -5   1  1   1525  01 27 00
01 29 00  ---          12 13 54  46.9 -17.2  2.3     134.6   115   F  1   1533  01 27 00

01 29 40  M81          12 14 34  46.8 -17.3  2.3     134.4    35   1  1   1533  01 29 40
01 31 50  ---          12 16 45  46.7 -17.5  2.3     133.8   130   F  1   1541  01 29 58

01 31 50  SN1993J      12 16 45  46.7 -17.5  2.3     133.7    -5   1  1   1541  01 31 50
01 33 50  ---          12 18 45  46.6 -17.7  2.4     133.1   115   F  1   1549  01 31 50

01 33 50  M81          12 18 45  46.5 -17.7  2.4     133.2    -5   1  1   1549  01 33 50
01 35 00  ---          12 19 55  46.5 -17.8  2.4     132.8    65   F  1   1553  01 33 50

01 35 00  SN1993J      12 19 55  46.5 -17.8  2.4     132.7    -5   1  1   1553  01 35 00
01 37 00  ---          12 21 56  46.4 -18.0  2.4     132.1   115   F  1   1561  01 35 00

01 37 00  M81          12 21 56  46.3 -17.9  2.4     132.2    -5   1  1   1561  01 37 00
01 38 10  ---          12 23 06  46.3 -18.0  2.5     131.9    65   F  1   1566  01 37 00

01 38 10  SN1993J      12 23 06  46.3 -18.1  2.5     131.8    -5   1  1   1566  01 38 10
01 40 10  ---          12 25 06  46.1 -18.3  2.5     131.2   115   F  1   1573  01 38 10
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

01 40 10  M81          12 25 06  46.1 -18.2  2.5     131.3    -5   1  1   1573  01 40 10
01 41 20  ---          12 26 16  46.0 -18.3  2.5     130.9    65   F  1   1578  01 40 10

01 41 20  SN1993J      12 26 16  46.1 -18.4  2.5     130.9    -5   1  1   1578  01 41 20
01 43 20  ---          12 28 17  45.9 -18.5  2.5     130.3   115   F  1   1586  01 41 20

01 43 20  M81          12 28 17  45.9 -18.5  2.5     130.3    -5   1  1   1586  01 43 20
01 44 30  ---          12 29 27  45.8 -18.6  2.6     130.0    65   F  1   1590  01 43 20

01 44 30  SN1993J      12 29 27  45.8 -18.6  2.6     129.9    -5   1  1   1590  01 44 30
01 46 30  ---          12 31 27  45.7 -18.8  2.6     129.3   115   F  1   1598  01 44 30

01 46 30  M81          12 31 27  45.7 -18.7  2.6     129.4    -5   1  1   1598  01 46 30
01 47 40  ---          12 32 37  45.6 -18.8  2.6     129.1    65   F  1   1602  01 46 30

01 47 40  SN1993J      12 32 37  45.6 -18.9  2.6     129.0    -5   1  1   1602  01 47 40
01 49 40  ---          12 34 38  45.5 -19.1  2.6     128.4   115   F  1   1610  01 47 40

01 49 40  M81          12 34 38  45.5 -19.0  2.6     128.5    -5   1  1   1610  01 49 40
01 51 40  ---          12 36 38  45.3 -19.1  2.7     127.9   115   F  1   1618  01 49 40

01 52 20  M81          12 37 18  45.3 -19.2  2.7     127.7    35   1  1   1618  01 52 20
01 54 30  ---          12 39 28  45.1 -19.4  2.7     127.1   130   F  1   1626  01 52 38

01 54 30  SN1993J      12 39 28  45.1 -19.4  2.7     127.0    -5   1  1   1626  01 54 30
01 56 30  ---          12 41 29  45.0 -19.6  2.8     126.4   115   F  1   1634  01 54 30

01 56 30  M81          12 41 29  45.0 -19.5  2.8     126.5    -5   1  1   1634  01 56 30
01 57 40  ---          12 42 39  44.9 -19.6  2.8     126.2    65   F  1   1639  01 56 30

01 57 40  SN1993J      12 42 39  44.9 -19.7  2.8     126.1    -5   1  1   1639  01 57 40
01 59 40  ---          12 44 39  44.8 -19.8  2.8     125.5   115   F  1   1646  01 57 40

01 59 40  M81          12 44 39  44.8 -19.8  2.8     125.6    -5   1  1   1646  01 59 40
02 00 50  ---          12 45 49  44.7 -19.8  2.8     125.3    65   F  1   1651  01 59 40

02 00 50  SN1993J      12 45 49  44.7 -19.9  2.8     125.2    -5   1  1   1651  02 00 50
02 02 50  ---          12 47 50  44.5 -20.0  2.9     124.6   115   F  1   1659  02 00 50

02 02 50  M81          12 47 50  44.5 -20.0  2.9     124.7    -5   1  1   1659  02 02 50
02 04 00  ---          12 49 00  44.4 -20.1  2.9     124.4    65   F  1   1663  02 02 50

02 04 00  SN1993J      12 49 00  44.4 -20.1  2.9     124.3    -5   1  1   1663  02 04 00
02 06 00  ---          12 51 00  44.3 -20.3  2.9     123.7   115   F  1   1671  02 04 00
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

02 06 00  M81          12 51 00  44.3 -20.2  2.9     123.8    -5   1  1   1671  02 06 00
02 07 10  ---          12 52 11  44.2 -20.3  2.9     123.5    65   F  1   1675  02 06 00

02 07 10  SN1993J      12 52 11  44.2 -20.4  2.9     123.4    -5   1  1   1675  02 07 10
02 09 10  ---          12 54 11  44.1 -20.5  3.0     122.8   115   F  1   1683  02 07 10

02 09 10  M81          12 54 11  44.0 -20.4  3.0     122.9    -5   1  1   1683  02 09 10
02 10 20  ---          12 55 21  44.0 -20.5  3.0     122.6    65   F  1   1688  02 09 10

02 10 20  SN1993J      12 55 21  44.0 -20.6  3.0     122.5    -5   1  1   1688  02 10 20
02 12 20  ---          12 57 21  43.8 -20.7  3.0     121.9   115   F  1   1695  02 10 20

02 12 20  M81          12 57 21  43.8 -20.6  3.0     122.0    -5   1  1   1695  02 12 20
02 14 20  ---          12 59 22  43.7 -20.8  3.1     121.5   115   F  1   1703  02 12 20

02 15 00  M81          13 00 02  43.6 -20.8  3.1     121.3    35   1  1   1703  02 15 00
02 17 10  ---          13 02 12  43.4 -20.9  3.1     120.7   130   F  1   1712  02 15 18

02 17 10  SN1993J      13 02 12  43.5 -21.0  3.1     120.6    -5   1  1   1712  02 17 10
02 19 10  ---          13 04 12  43.3 -21.1  3.1     120.1   115   F  1   1719  02 17 10

02 19 10  M81          13 04 12  43.3 -21.1  3.1     120.1    -5   1  1   1719  02 19 10
02 20 20  ---          13 05 23  43.2 -21.1  3.2     119.8    65   F  1   1724  02 19 10

02 20 20  SN1993J      13 05 23  43.2 -21.2  3.2     119.7    -5   1  1   1724  02 20 20
02 22 20  ---          13 07 23  43.0 -21.3  3.2     119.2   115   F  1   1732  02 20 20

02 22 20  M81          13 07 23  43.0 -21.3  3.2     119.3    -5   1  1   1732  02 22 20
02 23 30  ---          13 08 33  42.9 -21.3  3.2     118.9    65   F  1   1736  02 22 20

02 23 30  SN1993J      13 08 33  43.0 -21.4  3.2     118.9    -5   1  1   1736  02 23 30
02 25 30  ---          13 10 34  42.8 -21.5  3.2     118.3   115   F  1   1744  02 23 30

02 25 30  M81          13 10 34  42.8 -21.5  3.2     118.4    -5   1  1   1744  02 25 30
02 26 40  ---          13 11 44  42.7 -21.5  3.3     118.1    65   F  1   1748  02 25 30

02 26 40  SN1993J      13 11 44  42.7 -21.6  3.3     118.0    -5   1  1   1748  02 26 40
02 28 40  ---          13 13 44  42.5 -21.7  3.3     117.4   115   F  1   1756  02 26 40

02 28 40  M81          13 13 44  42.5 -21.6  3.3     117.5    -5   1  1   1756  02 28 40
02 29 50  ---          13 14 54  42.4 -21.7  3.3     117.2    65   F  1   1761  02 28 40

02 29 50  SN1993J      13 14 54  42.5 -21.8  3.3     117.1    -5   1  1   1761  02 29 50
02 31 50  ---          13 16 55  42.3 -21.9  3.3     116.6   115   F  1   1768  02 29 50
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

02 31 50  M81          13 16 55  42.3 -21.8  3.3     116.7    -5   1  1   1768  02 31 50
02 33 00  ---          13 18 05  42.2 -21.9  3.4     116.3    65   F  1   1773  02 31 50

02 33 00  SN1993J      13 18 05  42.2 -21.9  3.4     116.3    -5   1  1   1773  02 33 00
02 35 00  ---          13 20 05  42.0 -22.0  3.4     115.7   115   F  1   1781  02 33 00

02 35 00  M81          13 20 05  42.0 -22.0  3.4     115.8    -5   1  1   1781  02 35 00
02 37 00  ---          13 22 05  41.9 -22.1  3.4     115.3   115   F  1   1788  02 35 00

02 37 40  M81          13 22 46  41.8 -22.1  3.4     115.1    35   1  1   1788  02 37 40
02 39 50  ---          13 24 56  41.6 -22.2  3.5     114.5   130   F  1   1797  02 37 58

02 39 50  SN1993J      13 24 56  41.6 -22.3  3.5     114.4    -5   1  1   1797  02 39 50
02 41 50  ---          13 26 56  41.5 -22.4  3.5     113.9   115   F  1   1804  02 39 50

02 41 50  M81          13 26 56  41.5 -22.3  3.5     114.0    -5   1  1   1804  02 41 50
02 43 00  ---          13 28 06  41.4 -22.4  3.5     113.7    65   F  1   1809  02 41 50

02 43 00  SN1993J      13 28 06  41.4 -22.4  3.5     113.6    -5   1  1   1809  02 43 00
02 45 00  ---          13 30 07  41.2 -22.5  3.6     113.1   115   F  1   1817  02 43 00

02 45 00  M81          13 30 07  41.2 -22.5  3.6     113.1    -5   1  1   1817  02 45 00
02 46 10  ---          13 31 17  41.1 -22.5  3.6     112.8    65   F  1   1821  02 45 00

02 46 10  SN1993J      13 31 17  41.1 -22.6  3.6     112.8    -5   1  1   1821  02 46 10
02 48 10  ---          13 33 17  41.0 -22.7  3.6     112.2   115   F  1   1829  02 46 10

02 48 10  M81          13 33 17  41.0 -22.6  3.6     112.3    -5   1  1   1829  02 48 10
02 49 20  ---          13 34 27  40.9 -22.7  3.6     112.0    65   F  1   1833  02 48 10

02 49 20  SN1993J      13 34 27  40.9 -22.7  3.6     111.9    -5   1  1   1833  02 49 20
02 51 20  ---          13 36 28  40.7 -22.8  3.7     111.4   115   F  1   1841  02 49 20

02 51 20  M81          13 36 28  40.7 -22.8  3.7     111.5    -5   1  1   1841  02 51 20
02 52 30  ---          13 37 38  40.6 -22.8  3.7     111.2    65   F  1   1846  02 51 20

02 52 30  SN1993J      13 37 38  40.6 -22.9  3.7     111.1    -5   1  1   1846  02 52 30
02 54 30  ---          13 39 38  40.4 -23.0  3.7     110.6   115   F  1   1853  02 52 30

02 54 30  M81          13 39 38  40.4 -22.9  3.7     110.6    -5   1  1   1853  02 54 30
02 55 40  ---          13 40 48  40.3 -22.9  3.7     110.3    65   F  1   1858  02 54 30

02 55 40  SN1993J      13 40 48  40.3 -23.0  3.7     110.3    -5   1  1   1858  02 55 40
02 57 40  ---          13 42 49  40.2 -23.1  3.8     109.7   115   F  1   1866  02 55 40
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

02 57 40  M81          13 42 49  40.2 -23.0  3.8     109.8    -5   1  1   1866  02 57 40
02 59 40  ---          13 44 49  40.0 -23.1  3.8     109.3   115   F  1   1873  02 57 40

03 09 40  0954+658     13 54 51  40.4 -27.7  3.9     104.7   591   1  1   1873  03 09 40
03 12 40  ---          13 57 51  40.1 -27.8  4.0     104.0   180   F  1   1885  03 09 58

03 12 40  M81          13 57 51  38.9 -23.6  4.0     106.0    -9   1  1   1885  03 12 40
03 15 00  ---          14 00 12  38.7 -23.6  4.1     105.4   131   F  1   1894  03 12 40

03 15 00  SN1993J      14 00 12  38.7 -23.7  4.1     105.3    -5   1  1   1894  03 15 00
03 17 00  ---          14 02 12  38.5 -23.8  4.1     104.8   115   F  1   1902  03 15 00

03 17 00  M81          14 02 12  38.5 -23.7  4.1     104.9    -5   1  1   1902  03 17 00
03 18 10  ---          14 03 22  38.4 -23.7  4.1     104.6    65   F  1   1906  03 17 00

03 18 10  SN1993J      14 03 22  38.4 -23.8  4.1     104.5    -5   1  1   1906  03 18 10
03 20 10  ---          14 05 23  38.2 -23.8  4.2     104.0   115   F  1   1914  03 18 10

03 20 10  M81          14 05 23  38.2 -23.8  4.2     104.1    -5   1  1   1914  03 20 10
03 21 20  ---          14 06 33  38.1 -23.8  4.2     103.8    65   F  1   1919  03 20 10

03 21 20  SN1993J      14 06 33  38.1 -23.9  4.2     103.7    -5   1  1   1919  03 21 20
03 23 20  ---          14 08 33  38.0 -23.9  4.2     103.2   115   F  1   1926  03 21 20

03 23 20  M81          14 08 33  38.0 -23.9  4.2     103.3    -5   1  1   1926  03 23 20
03 24 30  ---          14 09 43  37.9 -23.9  4.2     103.0    65   F  1   1931  03 23 20

03 24 30  SN1993J      14 09 43  37.8 -24.0  4.2     102.9    -5   1  1   1931  03 24 30
03 26 30  ---          14 11 44  37.7 -24.0  4.3     102.4   115   F  1   1939  03 24 30

03 26 30  M81          14 11 44  37.7 -23.9  4.3     102.5    -5   1  1   1939  03 26 30
03 27 40  ---          14 12 54  37.6 -24.0  4.3     102.2    65   F  1   1943  03 26 30

03 27 40  SN1993J      14 12 54  37.6 -24.0  4.3     102.1    -5   1  1   1943  03 27 40
03 29 40  ---          14 14 54  37.4 -24.1  4.3     101.6   115   F  1   1951  03 27 40

03 29 40  M81          14 14 54  37.4 -24.0  4.3     101.7    -5   1  1   1951  03 29 40
03 31 40  ---          14 16 54  37.2 -24.1  4.3     101.2   115   F  1   1959  03 29 40

03 32 20  M81          14 17 35  37.2 -24.1  4.4     101.0    35   1  1   1959  03 32 20
03 34 30  ---          14 19 45  37.0 -24.1  4.4     100.5   130   F  1   1967  03 32 38

03 34 30  SN1993J      14 19 45  37.0 -24.2  4.4     100.4    -5   1  1   1967  03 34 30
03 36 30  ---          14 21 45  36.8 -24.2  4.4      99.9   115   F  1   1975  03 34 30
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

03 36 30  M81          14 21 45  36.8 -24.2  4.4     100.0    -5   1  1   1975  03 36 30
03 37 40  ---          14 22 55  36.7 -24.2  4.4      99.7    65   F  1   1979  03 36 30

03 37 40  SN1993J      14 22 55  36.7 -24.2  4.4      99.7    -5   1  1   1979  03 37 40
03 39 40  ---          14 24 56  36.5 -24.3  4.5      99.2   115   F  1   1987  03 37 40

03 39 40  M81          14 24 56  36.5 -24.2  4.5      99.2    -5   1  1   1987  03 39 40
03 40 50  ---          14 26 06  36.4 -24.2  4.5      98.9    65   F  1   1991  03 39 40

03 40 50  SN1993J      14 26 06  36.4 -24.3  4.5      98.9    -5   1  1   1991  03 40 50
03 42 50  ---          14 28 06  36.2 -24.3  4.5      98.4   115   F  1   1999  03 40 50

03 42 50  M81          14 28 06  36.2 -24.3  4.5      98.5    -5   1  1   1999  03 42 50
03 44 00  ---          14 29 16  36.1 -24.3  4.6      98.2    65   F  1   2004  03 42 50

03 44 00  SN1993J      14 29 16  36.1 -24.4  4.6      98.1    -5   1  1   2004  03 44 00
03 46 00  ---          14 31 17  35.9 -24.4  4.6      97.6   115   F  1   2011  03 44 00

03 46 00  M81          14 31 17  36.0 -24.3  4.6      97.7    -5   1  1   2011  03 46 00
03 47 10  ---          14 32 27  35.9 -24.3  4.6      97.4    65   F  1   2016  03 46 00

03 47 10  SN1993J      14 32 27  35.8 -24.4  4.6      97.3    -5   1  1   2016  03 47 10
03 49 10  ---          14 34 27  35.7 -24.4  4.6      96.9   115   F  1   2024  03 47 10

03 49 10  M81          14 34 27  35.7 -24.4  4.6      96.9    -5   1  1   2024  03 49 10
03 50 20  ---          14 35 37  35.6 -24.4  4.7      96.6    65   F  1   2028  03 49 10

03 50 20  SN1993J      14 35 37  35.6 -24.4  4.7      96.6    -5   1  1   2028  03 50 20
03 52 20  ---          14 37 38  35.4 -24.5  4.7      96.1   115   F  1   2036  03 50 20

03 52 20  M81          14 37 38  35.4 -24.4  4.7      96.2    -5   1  1   2036  03 52 20
03 54 20  ---          14 39 38  35.2 -24.4  4.7      95.7   115   F  1   2044  03 52 20

03 59 20  OQ208        14 44 39  81.6 257.1  0.6      72.5   106   1  1   2044  03 59 20
04 01 30  ---          14 46 49  81.1 258.0  0.7      73.2   130   F  1   2052  03 59 38

04 01 30  M81          14 46 49  34.6 335.5  4.8      94.0   -99   1  1   2052  04 01 30
04 04 40  ---          14 50 00  34.3 335.5  4.9      93.2    91   F  1   2064  04 01 30

04 04 40  SN1993J      14 50 00  34.3 335.4  4.9      93.1    -5   1  1   2064  04 04 40
04 06 40  ---          14 52 00  34.1 335.4  4.9      92.7   115   F  1   2072  04 04 40

04 06 40  M81          14 52 00  34.1 335.5  4.9      92.7    -5   1  1   2072  04 06 40
04 07 50  ---          14 53 10  34.0 335.5  5.0      92.5    65   F  1   2077  04 06 40
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

04 07 50  SN1993J      14 53 10  34.0 335.4  5.0      92.4    -5   1  1   2077  04 07 50
04 09 50  ---          14 55 11  33.8 335.4  5.0      91.9   115   F  1   2084  04 07 50

04 09 50  M81          14 55 11  33.8 335.5  5.0      92.0    -5   1  1   2084  04 09 50
04 11 00  ---          14 56 21  33.7 335.4  5.0      91.7    65   F  1   2089  04 09 50

04 11 00  SN1993J      14 56 21  33.7 335.4  5.0      91.6    -5   1  1   2089  04 11 00
04 13 00  ---          14 58 21  33.5 335.4  5.0      91.2   115   F  1   2097  04 11 00

04 13 00  M81          14 58 21  33.5 335.4  5.0      91.2    -5   1  1   2097  04 13 00
04 14 10  ---          14 59 31  33.4 335.4  5.1      91.0    65   F  1   2101  04 13 00

04 14 10  SN1993J      14 59 31  33.4 335.4  5.1      90.9    -5   1  1   2101  04 14 10
04 16 10  ---          15 01 32  33.2 335.4  5.1      90.4   115   F  1   2109  04 14 10

04 16 10  M81          15 01 32  33.3 335.4  5.1      90.5    -5   1  1   2109  04 16 10
04 17 20  ---          15 02 42  33.2 335.4  5.1      90.2    65   F  1   2113  04 16 10

04 17 20  SN1993J      15 02 42  33.1 335.4  5.1      90.2    -5   1  1   2113  04 17 20
04 19 20  ---          15 04 42  33.0 335.4  5.1      89.7   115   F  1   2121  04 17 20

04 19 20  M81          15 04 42  33.0 335.4  5.1      89.7    -5   1  1   2121  04 19 20
04 21 20  ---          15 06 43  32.8 335.4  5.2      89.3   115   F  1   2129  04 19 20

04 22 00  M81          15 07 23  32.7 335.4  5.2      89.1    35   1  1   2129  04 22 00
04 24 10  ---          15 09 33  32.5 335.4  5.2      88.6   130   F  1   2137  04 22 18

04 24 10  SN1993J      15 09 33  32.5 335.4  5.2      88.6    -5   1  1   2137  04 24 10
04 26 10  ---          15 11 33  32.3 335.4  5.3      88.1   115   F  1   2145  04 24 10

04 26 10  M81          15 11 33  32.4 335.4  5.3      88.2    -5   1  1   2145  04 26 10
04 27 20  ---          15 12 44  32.3 335.5  5.3      87.9    65   F  1   2150  04 26 10

04 27 20  SN1993J      15 12 44  32.2 335.4  5.3      87.8    -5   1  1   2150  04 27 20
04 29 20  ---          15 14 44  32.1 335.4  5.3      87.4   115   F  1   2157  04 27 20

04 29 20  M81          15 14 44  32.1 335.5  5.3      87.4    -5   1  1   2157  04 29 20
04 30 30  ---          15 15 54  32.0 335.5  5.3      87.2    65   F  1   2162  04 29 20

04 30 30  SN1993J      15 15 54  32.0 335.4  5.3      87.1    -5   1  1   2162  04 30 30
04 32 30  ---          15 17 54  31.8 335.4  5.4      86.6   115   F  1   2170  04 30 30

04 32 30  M81          15 17 54  31.8 335.5  5.4      86.7    -5   1  1   2170  04 32 30
04 33 40  ---          15 19 05  31.7 335.5  5.4      86.4    65   F  1   2174  04 32 30
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

04 33 40  SN1993J      15 19 05  31.7 335.4  5.4      86.4    -5   1  1   2174  04 33 40
04 35 40  ---          15 21 05  31.5 335.4  5.4      85.9   115   F  1   2182  04 33 40

04 35 40  M81          15 21 05  31.5 335.5  5.4      86.0    -5   1  1   2182  04 35 40
04 36 50  ---          15 22 15  31.4 335.5  5.4      85.7    65   F  1   2186  04 35 40

04 36 50  SN1993J      15 22 15  31.4 335.5  5.4      85.6    -5   1  1   2186  04 36 50
04 38 50  ---          15 24 15  31.2 335.5  5.5      85.2   115   F  1   2194  04 36 50

04 38 50  M81          15 24 15  31.2 335.5  5.5      85.2    -5   1  1   2194  04 38 50
04 40 00  ---          15 25 26  31.1 335.5  5.5      85.0    65   F  1   2199  04 38 50

04 40 00  SN1993J      15 25 26  31.1 335.5  5.5      84.9    -5   1  1   2199  04 40 00
04 42 00  ---          15 27 26  30.9 335.5  5.5      84.4   115   F  1   2206  04 40 00

04 42 00  M81          15 27 26  30.9 335.6  5.5      84.5    -5   1  1   2206  04 42 00
04 44 00  ---          15 29 26  30.8 335.6  5.6      84.0   115   F  1   2214  04 42 00

04 44 40  M81          15 30 06  30.7 335.6  5.6      83.9    35   1  1   2214  04 44 40
04 46 50  ---          15 32 17  30.5 335.6  5.6      83.4   130   F  1   2222  04 44 58

04 46 50  SN1993J      15 32 17  30.5 335.6  5.6      83.3    -5   1  1   2222  04 46 50
04 48 50  ---          15 34 17  30.3 335.6  5.6      82.9   115   F  1   2230  04 46 50

04 48 50  M81          15 34 17  30.3 335.6  5.6      82.9    -5   1  1   2230  04 48 50
04 50 00  ---          15 35 27  30.2 335.6  5.7      82.7    65   F  1   2235  04 48 50

04 50 00  SN1993J      15 35 27  30.2 335.6  5.7      82.6    -5   1  1   2235  04 50 00
04 52 00  ---          15 37 28  30.0 335.6  5.7      82.2   115   F  1   2242  04 50 00

04 52 00  M81          15 37 28  30.1 335.7  5.7      82.2    -5   1  1   2242  04 52 00
04 53 10  ---          15 38 38  30.0 335.7  5.7      82.0    65   F  1   2247  04 52 00

04 53 10  SN1993J      15 38 38  29.9 335.6  5.7      81.9    -5   1  1   2247  04 53 10
04 55 10  ---          15 40 38  29.8 335.7  5.7      81.4   115   F  1   2255  04 53 10

04 55 10  M81          15 40 38  29.8 335.7  5.7      81.5    -5   1  1   2255  04 55 10
04 56 20  ---          15 41 48  29.7 335.7  5.8      81.2    65   F  1   2259  04 55 10

04 56 20  SN1993J      15 41 48  29.7 335.7  5.8      81.2    -5   1  1   2259  04 56 20
04 58 20  ---          15 43 49  29.5 335.7  5.8      80.7   115   F  1   2267  04 56 20

04 58 20  M81          15 43 49  29.5 335.8  5.8      80.8    -5   1  1   2267  04 58 20
04 59 30  ---          15 44 59  29.4 335.8  5.8      80.5    65   F  1   2271  04 58 20
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

04 59 30  SN1993J      15 44 59  29.4 335.7  5.8      80.5    -5   1  1   2271  04 59 30
05 01 30  ---          15 46 59  29.2 335.8  5.9      80.0   115   F  1   2279  04 59 30

05 01 30  M81          15 46 59  29.2 335.8  5.8      80.1    -5   1  1   2279  05 01 30
05 02 40  ---          15 48 09  29.1 335.8  5.9      79.8    65   F  1   2284  05 01 30

05 02 40  SN1993J      15 48 09  29.1 335.8  5.9      79.8    -5   1  1   2284  05 02 40
05 04 40  ---          15 50 10  28.9 335.8  5.9      79.3   115   F  1   2291  05 02 40

05 04 40  M81          15 50 10  28.9 335.9  5.9      79.4    -5   1  1   2291  05 04 40
05 06 40  ---          15 52 10  28.8 335.9  5.9      78.9   115   F  1   2299  05 04 40

05 07 20  M81          15 52 50  28.7 335.9  5.9      78.8    35   1  1   2299  05 07 20
05 09 30  ---          15 55 00  28.5 336.0  6.0      78.3   130   F  1   2308  05 07 38

05 09 30  SN1993J      15 55 00  28.5 335.9  6.0      78.2    -5   1  1   2308  05 09 30
05 11 30  ---          15 57 01  28.3 336.0  6.0      77.8   115   F  1   2315  05 09 30

05 11 30  M81          15 57 01  28.3 336.0  6.0      77.8    -5   1  1   2315  05 11 30
05 12 40  ---          15 58 11  28.2 336.0  6.0      77.6    65   F  1   2320  05 11 30

05 12 40  SN1993J      15 58 11  28.2 336.0  6.0      77.5    -5   1  1   2320  05 12 40
05 14 40  ---          16 00 11  28.0 336.0  6.1      77.1   115   F  1   2328  05 12 40

05 14 40  M81          16 00 11  28.1 336.1  6.1      77.1    -5   1  1   2328  05 14 40
05 15 50  ---          16 01 22  28.0 336.1  6.1      76.9    65   F  1   2332  05 14 40

05 15 50  SN1993J      16 01 22  27.9 336.1  6.1      76.8    -5   1  1   2332  05 15 50
05 17 50  ---          16 03 22  27.8 336.1  6.1      76.4   115   F  1   2340  05 15 50

05 17 50  M81          16 03 22  27.8 336.2  6.1      76.4    -5   1  1   2340  05 17 50
05 19 00  ---          16 04 32  27.7 336.2  6.1      76.2    65   F  1   2344  05 17 50

05 19 00  SN1993J      16 04 32  27.7 336.1  6.1      76.1    -5   1  1   2344  05 19 00
05 21 00  ---          16 06 32  27.5 336.2  6.2      75.7   115   F  1   2352  05 19 00

05 21 00  M81          16 06 32  27.5 336.2  6.2      75.7    -5   1  1   2352  05 21 00
05 22 10  ---          16 07 43  27.4 336.3  6.2      75.4    65   F  1   2357  05 21 00

05 22 10  SN1993J      16 07 43  27.4 336.2  6.2      75.4    -5   1  1   2357  05 22 10
05 24 10  ---          16 09 43  27.2 336.3  6.2      75.0   115   F  1   2364  05 22 10

05 24 10  M81          16 09 43  27.2 336.3  6.2      75.0    -5   1  1   2364  05 24 10
05 25 20  ---          16 10 53  27.1 336.4  6.2      74.7    65   F  1   2369  05 24 10
Schedule for VLBA_FD   (Code Fd )                                   Page  26
               35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
         For disks, the footages are really the GBytes
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)   SYNC
----------------------------------------------------------------------------------------

 --- Sat  17 Jun 2006   Day 168 ---

05 25 20  SN1993J      16 10 53  27.1 336.3  6.2      74.7    -5   1  1   2369  05 25 20
05 27 20  ---          16 12 53  26.9 336.4  6.3      74.2   115   F  1   2377  05 25 20

05 27 20  M81          16 12 53  27.0 336.4  6.3      74.3    -5   1  1   2377  05 27 20
05 29 20  ---          16 14 54  26.8 336.5  6.3      73.9   115   F  1   2384  05 27 20


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: v6cm-512-16-2.set
   Matches group v6cm_2 in /usr/local/sched/catalogs/freq.dat

   Setup group:    4         Station: VLBA_FD           Total bit rate:  512
   Format: VLBA1:2           Bits per sample: 2         Sample rate: 16.000
   Number of channels: 16                               Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
             4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
                RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         1         2         3         4         3         4
                   5         6         5         6         7         8         7         8
   BBC SB=         L         L         U         U         L         L         U         U
                   L         L         U         U         L         L         U         U
   IF    =        A         C         A         C         A         C         A         C 
                  A         C         A         C         A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.4      4.1     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   4  Setup file default.  Used pcal sets:   1
   LO sum=    4958.49   4958.49   4958.49   4958.49   4974.49   4974.49   4974.49   4974.49
              4990.49   4990.49   4990.49   4990.49   5006.49   5006.49   5006.49   5006.49
   BBC fr=     858.49    858.49    858.49    858.49    874.49    874.49    874.49    874.49
               890.49    890.49    890.49    890.49    906.49    906.49    906.49    906.49
   Bandwd=      8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000
                8.000     8.000     8.000     8.000     8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S5    S7    S9    S11   S13   S15
    PCALXB2=   S2    S4    S6    S8    S10   S12   S14   S16
    PCALFR1=   490   510   490   510   490   510   490   510
    PCALFR2=   490   510   490   510   490   510   490   510

   Track assignments are: 
    track1=   2, 10, 18, 26,  3, 11, 19, 27, 66, 74, 82, 90, 67, 75, 83, 91
    barrel=roll_off 
 SOURCE LIST -- 35rd epoch of obs. of SN1993J in M81: VLBA/MkV 6 pol.
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).
     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * SN1993J           09 51 19.038889   * 09 55 24.774900     09 55 55.844469       0.00
                     69 15 26.46784    * 69 01 13.70300      68 59 43.89475        0.00
                     From catalog imbedded in main SCHED input file.
                        5.367 scan hours,    696.450 baseline hours above horizon.

 * M81               09 51 27.310854   * 09 55 33.173100     09 56 04.260179       0.00
                     69 18 08.14534    * 69 03 55.06200      69 02 25.21909        0.00
                     From catalog imbedded in main SCHED input file.
                        4.578 scan hours,    570.530 baseline hours above horizon.

 * 0954+658          09 54 57.847119   * 09 58 47.244300     09 59 16.341235       0.00
                     65 48 15.53178    * 65 33 54.81100      65 32 23.58742        0.00
                     From catalog imbedded in main SCHED input file.
                        0.250 scan hours,     35.700 baseline hours above horizon.

   J1407+2827        14 04 45.615156   * 14 07 00.394414     14 07 18.956301       0.23
   1404+286          28 41 29.23520    * 28 27 14.69023      28 25 27.27360        0.40
   J1407+28          /usr/local/sched/catalogs/sources.vlba
 * OQ208             VLBA Calib Survey - GSFC sols. - created L.Petrov 2005f_astro
                        0.072 scan hours,      6.978 baseline hours above horizon.



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   SN1993J             58.9
   M81                 59.0
   0954+658            58.4
   OQ208              107.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

