  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: High-resolution, multi-frequency mapping of the compact sources in M82
 Exp. Code:  GF019B  


Schedule Version:       1.00
Processed by SCHED version:  11.40  Release 11.4.  March 14, 2015

PI:       D. Fenech

Address:  Department of Physics and Astronomy
          University College London
          Gower street, London, WC1E 6BT
          United Kingdom

Phone:    +44 (0)20 7679 7682
EMAIL:    dmf@star.ucl.ac.uk
Fax:      +44 (0)20 7679 7145
Phone during observation: +44 (0)7791 563887

Observing mode: Phase-referencing of M82 at 18cm (512 Mb/s)

Notes:    Lovell telescope missing alternate phase reference scans to keep slewing rate down.
          Phase-cal is switched off for GF019 observation.
          Use of a single WSRT antenna required instead of the full array
          Effelsberg gaps included for pointing checks

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

 Next scan frequencies:  1626.25  1626.25  1642.25  1642.25  1658.25  1658.25  1674.25  1674.25
 Next BBC frequencies:    773.75   773.75   757.75   757.75   741.75   741.75   725.75   725.75
 Next scan bandwidths:     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00

00 00 00  J0958+65     04 04 48  28.1  28.1 -5.9     -77.2     0        0   00 00 00
00 02 00  ---          04 06 48  28.3  28.1 -5.9     -77.6   120        8   00 00 01

00 02 00  M82PTCEN     04 06 48  29.4  23.5 -5.8     -80.5   -11        8   00 02 11
00 06 35  ---          04 11 24  29.7  23.6 -5.8     -81.5   264       25   00 02 01

00 07 30  J0958+65     04 12 19  28.9  28.2 -5.8     -78.8    44       25   00 07 30
00 10 00  ---          04 14 49  29.1  28.3 -5.8     -79.4   150       34   00 07 31

00 10 00  M82PTCEN     04 14 49  30.0  23.7 -5.7     -82.3   -11       34   00 10 11
00 14 35  ---          04 19 25  30.4  23.7 -5.6     -83.4   264       51   00 10 01

00 15 30  J0958+65     04 20 20  29.7  28.4 -5.7     -80.6    44       51   00 15 30
00 18 00  ---          04 22 51  29.9  28.5 -5.6     -81.1   150       61   00 15 31

00 18 00  M82PTCEN     04 22 51  30.7  23.8 -5.6     -84.1   -11       61   00 18 11
00 22 35  ---          04 27 26  31.1  23.8 -5.5     -85.2   264       78   00 18 01

00 23 30  J0958+65     04 28 22  30.5  28.5 -5.5     -82.3    44       78   00 23 30
00 26 00  ---          04 30 52  30.8  28.6 -5.5     -82.9   150       88   00 23 31

00 26 00  M82PTCEN     04 30 52  31.4  23.8 -5.4     -86.0   -11       88   00 26 11
00 30 35  ---          04 35 28  31.8  23.9 -5.4     -87.1   264      105   00 26 01

00 31 30  J0958+65     04 36 23  31.3  28.7 -5.4     -84.1    44      105   00 31 30
00 34 00  ---          04 38 53  31.6  28.7 -5.4     -84.7   150      114   00 31 31

00 34 00  M82PTCEN     04 38 53  32.1  23.9 -5.3     -87.8   -11      114   00 34 11
00 38 35  ---          04 43 29  32.5  23.9 -5.2     -88.9   264      131   00 34 01

00 39 30  J0958+65     04 44 24  32.2  28.7 -5.3     -85.9    44      131   00 39 30
00 42 00  ---          04 46 55  32.4  28.8 -5.2     -86.4   150      141   00 39 31

00 42 00  M82PTCEN     04 46 55  32.8  23.9 -5.2     -89.7   -11      141   00 42 11
00 46 35  ---          04 51 30  33.2  23.9 -5.1     -90.8   264      158   00 42 01

00 47 30  J0958+65     04 52 26  33.0  28.8 -5.1     -87.7    44      158   00 47 30
00 50 00  ---          04 54 56  33.3  28.8 -5.1     -88.2   150      168   00 47 31

00 50 00  M82PTCEN     04 54 56  33.5  23.9 -5.0     -91.6   -11      168   00 50 11
00 54 35  ---          04 59 32  33.9  23.9 -5.0     -92.7   264      185   00 50 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

00 55 30  J0958+65     05 00 27  33.8  28.8 -5.0     -89.5    44      185   00 55 30
00 58 00  ---          05 02 57  34.1  28.8 -5.0     -90.1   150      194   00 55 31

00 58 00  M82PTCEN     05 02 57  34.2  23.8 -4.9     -93.5   -11      194   00 58 11
01 02 35  ---          05 07 33  34.6  23.8 -4.8     -94.6   264      211   00 58 01

01 03 30  J0958+65     05 08 28  34.7  28.8 -4.9     -91.3    44      211   01 03 30
01 06 00  ---          05 10 59  34.9  28.8 -4.8     -91.9   150      221   01 03 31

01 06 00  M82PTCEN     05 10 59  34.9  23.8 -4.8     -95.4   -11      221   01 06 11
01 10 35  ---          05 15 34  35.3  23.7 -4.7     -96.5   264      238   01 06 01

01 11 30  J0958+65     05 16 29  35.5  28.8 -4.7     -93.2    44      238   01 11 30
01 14 00  ---          05 19 00  35.7  28.8 -4.7     -93.7   150      248   01 11 31

01 14 00  M82PTCEN     05 19 00  35.6  23.7 -4.6     -97.4   -11      248   01 14 11
01 18 35  ---          05 23 36  36.0  23.6 -4.6     -98.5   264      265   01 14 01

01 19 30  J0958+65     05 24 31  36.3  28.7 -4.6     -95.0    43      265   01 19 30
01 22 00  ---          05 27 01  36.6  28.7 -4.6     -95.6   150      274   01 19 31

01 22 00  M82PTCEN     05 27 01  36.3  23.6 -4.5     -99.3   -12      274   01 22 12
01 26 35  ---          05 31 37  36.7  23.5 -4.4    -100.4   263      291   01 22 01

01 27 30  J0958+65     05 32 32  37.1  28.6 -4.5     -96.9    43      291   01 27 30
01 30 00  ---          05 35 03  37.4  28.6 -4.4     -97.5   150      301   01 27 31

01 30 00  M82PTCEN     05 35 03  37.0  23.4 -4.4    -101.3   -12      301   01 30 12
01 34 35  ---          05 39 38  37.4  23.3 -4.3    -102.4   263      318   01 30 01

01 35 30  J0958+65     05 40 33  38.0  28.5 -4.3     -98.8    43      318   01 35 30
01 38 00  ---          05 43 04  38.2  28.4 -4.3     -99.4   150      328   01 35 31

01 38 00  M82PTCEN     05 43 04  37.7  23.2 -4.2    -103.3   -12      328   01 38 12
01 42 35  ---          05 47 40  38.1  23.1 -4.2    -104.4   263      345   01 38 01

01 43 30  J0958+65     05 48 35  38.8  28.3 -4.2    -100.8    43      345   01 43 30
01 46 00  ---          05 51 05  39.0  28.2 -4.1    -101.4   150      354   01 43 31

01 46 00  M82PTCEN     05 51 05  38.4  23.0 -4.1    -105.3   -12      354   01 46 12
01 50 35  ---          05 55 41  38.7  22.9 -4.0    -106.5   263      371   01 46 01

01 51 30  J0958+65     05 56 36  39.6  28.1 -4.1    -102.7    43      371   01 51 30
01 54 00  ---          05 59 06  39.9  28.0 -4.0    -103.3   150      381   01 51 31
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

01 54 00  M82PTCEN     05 59 06  39.0  22.7 -4.0    -107.3   -12      381   01 54 12
01 58 35  ---          06 03 42  39.4  22.6 -3.9    -108.5   263      398   01 54 01

01 59 30  J0958+65     06 04 37  40.4  27.8 -3.9    -104.7    43      398   01 59 30
02 02 00  ---          06 07 08  40.7  27.7 -3.9    -105.3   150      407   01 59 31

02 02 00  M82PTCEN     06 07 08  39.7  22.5 -3.8    -109.4   -12      407   02 02 12
02 06 35  ---          06 11 44  40.1  22.3 -3.8    -110.6   263      424   02 02 01

02 07 30  J0958+65     06 12 39  41.2  27.5 -3.8    -106.7    43      424   02 07 30
02 10 00  ---          06 15 09  41.5  27.4 -3.7    -107.4   150      434   02 07 31

02 10 00  M82PTCEN     06 15 09  40.3  22.1 -3.7    -111.5   -12      434   02 10 12
02 14 35  ---          06 19 45  40.7  21.9 -3.6    -112.7   263      451   02 10 01

02 15 30  J0958+65     06 20 40  42.0  27.2 -3.7    -108.8    43      451   02 15 30
02 18 00  ---          06 23 10  42.3  27.0 -3.6    -109.4   150      461   02 15 31

02 18 00  M82PTCEN     06 23 10  41.0  21.8 -3.6    -113.6   -12      461   02 18 12
02 22 35  ---          06 27 46  41.4  21.6 -3.5    -114.8   263      478   02 18 01

02 23 30  J0958+65     06 28 41  42.8  26.8 -3.5    -110.9    43      478   02 23 30
02 26 00  ---          06 31 12  43.0  26.7 -3.5    -111.5   150      487   02 23 31

02 26 00  M82PTCEN     06 31 12  41.6  21.4 -3.4    -115.7   -12      487   02 26 12
02 30 35  ---          06 35 47  42.0  21.2 -3.4    -117.0   263      504   02 26 01

02 31 30  J0958+65     06 36 43  43.6  26.4 -3.4    -113.0    43      504   02 31 30
02 34 00  ---          06 39 13  43.8  26.2 -3.3    -113.7   150      514   02 31 31

02 34 00  M82PTCEN     06 39 13  42.3  21.0 -3.3    -117.9   -12      514   02 34 12
02 38 35  ---          06 43 49  42.6  20.7 -3.2    -119.1   263      531   02 34 01

02 39 30  J0958+65     06 44 44  44.3  25.9 -3.3    -115.1    43      531   02 39 30
02 42 00  ---          06 47 14  44.6  25.7 -3.2    -115.8   150      540   02 39 31

02 42 00  M82PTCEN     06 47 14  42.9  20.5 -3.2    -120.1   -12      540   02 42 12
02 46 35  ---          06 51 50  43.2  20.2 -3.1    -121.3   263      557   02 42 01

02 47 30  J0958+65     06 52 45  45.1  25.4 -3.1    -117.3    43      557   02 47 30
02 50 00  ---          06 55 16  45.3  25.2 -3.1    -118.0   150      567   02 47 31

02 50 00  M82PTCEN     06 55 16  43.5  20.0 -3.0    -122.3   -12      567   02 50 12
02 54 35  ---          06 59 51  43.8  19.7 -3.0    -123.6   263      584   02 50 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

02 55 30  J0958+65     07 00 47  45.8  24.8 -3.0    -119.6    43      584   02 55 30
02 58 00  ---          07 03 17  46.0  24.6 -2.9    -120.3   150      594   02 55 31

02 58 00  M82PTCEN     07 03 17  44.0  19.5 -2.9    -124.5   -12      594   02 58 12
03 02 35  ---          07 07 53  44.4  19.2 -2.8    -125.8   263      611   02 58 01

03 03 30  J0958+65     07 08 48  46.5  24.2 -2.9    -121.8    43      611   03 03 30
03 06 00  ---          07 11 18  46.7  24.0 -2.8    -122.5   150      620   03 03 31

03 06 00  M82PTCEN     07 11 18  44.6  18.9 -2.8    -126.8   -12      620   03 06 12
03 10 35  ---          07 15 54  44.9  18.6 -2.7    -128.1   263      637   03 06 01

03 11 30  J0958+65     07 16 49  47.2  23.5 -2.7    -124.1    43      637   03 11 30
03 14 00  ---          07 19 20  47.4  23.3 -2.7    -124.9   150      647   03 11 31

03 14 00  M82PTCEN     07 19 20  45.2  18.3 -2.6    -129.1   -12      647   03 14 12
03 18 35  ---          07 23 55  45.5  18.0 -2.6    -130.5   263      664   03 14 01

03 19 30  J0958+65     07 24 51  47.9  22.8 -2.6    -126.5    42      664   03 19 30
03 22 00  ---          07 27 21  48.1  22.6 -2.5    -127.2   150      673   03 19 31

03 22 00  M82PTCEN     07 27 21  45.7  17.7 -2.5    -131.5   -13      673   03 22 13
03 26 35  ---          07 31 57  46.0  17.3 -2.4    -132.8   262      690   03 22 01

03 27 30  J0958+65     07 32 52  48.5  22.0 -2.5    -128.9    42      690   03 27 30
03 30 00  ---          07 35 22  48.7  21.8 -2.4    -129.6   150      700   03 27 31

03 30 00  M82PTCEN     07 35 22  46.2  17.0 -2.4    -133.8   -13      700   03 30 13
03 34 35  ---          07 39 58  46.5  16.6 -2.3    -135.2   262      717   03 30 01

03 35 30  J0958+65     07 40 53  49.2  21.2 -2.3    -131.3    42      717   03 35 30
03 38 00  ---          07 43 24  49.4  21.0 -2.3    -132.1   150      726   03 35 31

03 38 00  M82PTCEN     07 43 24  46.7  16.3 -2.2    -136.2   -13      726   03 38 13
03 42 35  ---          07 47 59  47.0  15.8 -2.2    -137.6   262      743   03 38 01

03 43 30  J0958+65     07 48 54  49.8  20.4 -2.2    -133.8    42      743   03 43 30
03 46 00  ---          07 51 25  50.0  20.1 -2.1    -134.6   150      753   03 43 31

03 46 00  M82PTCEN     07 51 25  47.2  15.5 -2.1    -138.7   -14      753   03 46 14
03 50 35  ---          07 56 01  47.4  15.1 -2.0    -140.1   261      770   03 46 01

03 51 30  J0958+65     07 56 56  50.4  19.4 -2.1    -136.3    41      770   03 51 30
03 54 00  ---          07 59 26  50.6  19.2 -2.0    -137.1   150      779   03 51 31
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

03 54 00  M82PTCEN     07 59 26  47.6  14.7 -2.0    -141.1   -14      779   03 54 14
03 58 35  ---          08 04 02  47.9  14.3 -1.9    -142.5   261      796   03 54 01

03 59 30  J0958+65     08 04 57  50.9  18.5 -1.9    -138.9    41      796   03 59 30
04 02 00  ---          08 07 27  51.1  18.2 -1.9    -139.7   150      806   03 59 31

04 02 00  M82PTCEN     08 07 27  48.1  13.9 -1.8    -143.6   -14      806   04 02 14
04 06 50  ---          08 12 18  48.3  13.4 -1.7    -145.1   276      824   04 02 01

04 07 30  J0958+65     08 12 58  51.5  17.5 -1.8    -141.5    26      824   04 07 30
04 10 00  ---          08 15 29  51.6  17.1 -1.7    -142.4   150      833   04 07 31

04 10 00  M82PTCEN     08 15 29  48.5  13.0 -1.7    -146.1   -14      833   04 10 14
04 14 50  ---          08 20 20  48.7  12.5 -1.6    -147.7   276      851   04 10 01

04 15 30  J0958+65     08 21 00  52.0  16.4 -1.7    -144.2    26      851   04 15 30
04 18 00  ---          08 23 30  52.1  16.0 -1.6    -145.0   150      861   04 15 31

04 18 00  M82PTCEN     08 23 30  48.8  12.2 -1.6    -148.7   -15      861   04 18 15
04 22 50  ---          08 28 21  49.0  11.6 -1.5    -150.2   275      879   04 18 01

04 23 30  J0958+65     08 29 01  52.5  15.3 -1.5    -146.9    25      879   04 23 30
04 26 00  ---          08 31 31  52.6  14.9 -1.5    -147.8   150      888   04 23 31

04 26 00  M82PTCEN     08 31 31  49.2  11.2 -1.4    -151.3   -15      888   04 26 15
04 30 50  ---          08 36 22  49.4  10.7 -1.3    -152.8   275      906   04 26 01

04 31 30  J0958+65     08 37 02  52.9  14.1 -1.4    -149.7    25      906   04 31 30
04 34 00  ---          08 39 33  53.0  13.7 -1.3    -150.5   150      916   04 31 31

04 34 00  M82PTCEN     08 39 33  49.5  10.3 -1.3    -153.9   -15      916   04 34 15
04 38 50  ---          08 44 24  49.7   9.7 -1.2    -155.4   275      933   04 34 01

04 39 30  J0958+65     08 45 04  53.3  12.9 -1.2    -152.4    25      933   04 39 30
04 42 00  ---          08 47 34  53.4  12.5 -1.2    -153.3   150      943   04 39 31

04 42 00  M82PTCEN     08 47 34  49.8   9.3 -1.2    -156.5   -15      943   04 42 15
04 46 50  ---          08 52 25  50.0   8.7 -1.1    -158.1   275      961   04 42 01

04 47 30  J0958+65     08 53 05  53.7  11.6 -1.1    -155.3    25      961   04 47 30
04 50 00  ---          08 55 35  53.8  11.2 -1.1    -156.2   150      970   04 47 31

04 50 00  M82PTCEN     08 55 35  50.1   8.3 -1.0    -159.1   -15      970   04 50 15
04 54 50  ---          09 00 26  50.2   7.7 -0.9    -160.7   275      988   04 50 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

04 55 30  J0958+65     09 01 06  54.0  10.3 -1.0    -158.1    25      988   04 55 30
04 58 00  ---          09 03 37  54.1   9.9 -0.9    -159.1   150      998   04 55 31

04 58 00  M82PTCEN     09 03 37  50.3   7.3 -0.9    -161.8   -15      998   04 58 15
05 02 50  ---          09 08 27  50.4   6.6 -0.8    -163.4   275     1015   04 58 01

05 03 30  J0958+65     09 09 08  54.3   9.0 -0.8    -161.1    24     1015   05 03 30
05 06 00  ---          09 11 38  54.4   8.6 -0.8    -162.0   150     1025   05 03 31

05 06 00  M82PTCEN     09 11 38  50.5   6.2 -0.8    -164.5   -16     1025   05 06 16
05 10 50  ---          09 16 29  50.6   5.6 -0.7    -166.1   274     1043   05 06 01

05 11 30  J0958+65     09 17 09  54.5   7.6 -0.7    -164.0    24     1043   05 11 30
05 14 00  ---          09 19 39  54.6   7.2 -0.7    -164.9   150     1052   05 11 31

05 14 00  M82PTCEN     09 19 39  50.7   5.1 -0.6    -167.2   -16     1052   05 14 16
05 18 50  ---          09 24 30  50.8   4.5 -0.5    -168.8   274     1070   05 14 01

05 19 30  J0958+65     09 25 10  54.7   6.3 -0.6    -166.9    24     1070   05 19 30
05 22 00  ---          09 27 41  54.8   5.8 -0.5    -167.9   150     1080   05 19 31

05 22 00  M82PTCEN     09 27 41  50.8   4.1 -0.5    -169.9   -16     1080   05 22 16
05 26 50  ---          09 32 31  50.9   3.4 -0.4    -171.6   274     1097   05 22 01

05 27 30  J0958+65     09 33 12  54.9   4.8 -0.4    -169.9    24     1097   05 27 30
05 30 00  ---          09 35 42  54.9   4.4 -0.4    -170.9   150     1107   05 27 31

05 30 00  M82PTCEN     09 35 42  50.9   3.0 -0.4    -172.6   -16     1107   05 30 16
05 34 50  ---          09 40 33  51.0   2.3 -0.3    -174.3   274     1125   05 30 01

05 35 30  J0958+65     09 41 13  55.0   3.4 -0.3    -172.9    24     1125   05 35 30
05 38 00  ---          09 43 43  55.1   3.0 -0.3    -173.9   150     1134   05 35 31

05 38 00  M82PTCEN     09 43 43  51.0   1.9 -0.2    -175.4   -16     1134   05 38 16
05 42 50  ---          09 48 34  51.0   1.2 -0.1    -177.0   274     1152   05 38 01

05 43 30  J0958+65     09 49 14  55.1   2.0 -0.2    -175.9    24     1152   05 43 30
05 46 00  ---          09 51 45  55.1   1.5 -0.1    -176.9   150     1162   05 43 31

05 46 00  M82PTCEN     09 51 45  51.0   0.8 -0.1    -178.1   -16     1162   05 46 16
05 50 50  ---          09 56 35  51.0   0.1 -0.0    -179.8   274     1179   05 46 01

05 51 30  J0958+65     09 57 15  55.1   0.5 -0.0    -179.0    24     1179   05 51 30
05 54 00  ---          09 59 46  55.1   0.1 -0.0    -179.9   150     1189   05 51 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

05 54 00  M82PTCEN     09 59 46  51.0  -0.4  0.0     179.1   -16     1189   05 54 16
06 00 50  ---          10 06 37  51.0  -1.3  0.2     176.8   394     1214   05 54 01

06 01 30  J0958+65     10 07 17  55.1  -1.3  0.1     177.3    24     1214   06 01 30
06 04 00  ---          10 09 48  55.1  -1.8  0.2     176.3   150     1224   06 01 31

06 08 00  J0927+39     10 13 48  77.5 -45.3  0.8     128.2   187     1224   06 08 00
06 14 00  ---          10 19 49  76.5 -48.3  0.9     124.3   360     1247   06 08 01

06 18 00  J0958+65     10 23 50  55.0  -4.3  0.4     171.1   190     1247   06 18 00
06 20 00  ---          10 25 50  54.9  -4.7  0.4     170.3   120     1255   06 18 01

06 20 00  M82PTCEN     10 25 50  50.8  -3.9  0.5     170.2   -16     1255   06 20 16
06 24 50  ---          10 30 41  50.7  -4.6  0.6     168.6   274     1273   06 20 01

06 25 30  J0958+65     10 31 21  54.8  -5.6  0.5     168.3    24     1273   06 25 30
06 28 00  ---          10 33 51  54.8  -6.1  0.6     167.3   150     1282   06 25 31

06 28 00  M82PTCEN     10 33 51  50.7  -5.0  0.6     167.5   -16     1282   06 28 16
06 32 50  ---          10 38 42  50.6  -5.7  0.7     165.9   274     1300   06 28 01

06 33 30  J0958+65     10 39 22  54.6  -7.0  0.7     165.3    24     1300   06 33 30
06 36 00  ---          10 41 53  54.6  -7.5  0.7     164.4   150     1310   06 33 31

06 36 00  M82PTCEN     10 41 53  50.5  -6.1  0.7     164.8   -16     1310   06 36 16
06 40 50  ---          10 46 44  50.4  -6.7  0.8     163.2   274     1327   06 36 01

06 41 30  J0958+65     10 47 24  54.4  -8.4  0.8     162.4    24     1327   06 41 30
06 44 00  ---          10 49 54  54.3  -8.8  0.8     161.4   150     1337   06 41 31

06 44 00  M82PTCEN     10 49 54  50.3  -7.1  0.9     162.1   -16     1337   06 44 16
06 48 50  ---          10 54 45  50.2  -7.8  1.0     160.5   274     1354   06 44 01

06 49 30  J0958+65     10 55 25  54.1  -9.8  0.9     159.4    24     1354   06 49 30
06 52 00  ---          10 57 55  54.0 -10.2  1.0     158.5   150     1364   06 49 31

06 52 00  M82PTCEN     10 57 55  50.1  -8.2  1.0     159.4   -16     1364   06 52 16
06 56 50  ---          11 02 46  49.9  -8.8  1.1     157.8   274     1382   06 52 01

06 57 30  J0958+65     11 03 26  53.8 -11.1  1.1     156.5    24     1382   06 57 30
07 00 00  ---          11 05 57  53.7 -11.5  1.1     155.7   150     1391   06 57 31

07 00 00  M82PTCEN     11 05 57  49.8  -9.2  1.1     156.8   -16     1391   07 00 16
07 04 50  ---          11 10 48  49.7  -9.8  1.2     155.2   274     1409   07 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

07 05 30  J0958+65     11 11 28  53.5 -12.3  1.2     153.7    24     1409   07 05 30
07 08 00  ---          11 13 58  53.3 -12.7  1.2     152.8   150     1419   07 05 31

07 08 00  M82PTCEN     11 13 58  49.5 -10.2  1.3     154.2   -16     1419   07 08 16
07 12 50  ---          11 18 49  49.4 -10.7  1.4     152.6   274     1436   07 08 01

07 13 30  J0958+65     11 19 29  53.1 -13.6  1.3     150.9    25     1436   07 13 30
07 16 00  ---          11 21 59  52.9 -13.9  1.4     150.0   150     1446   07 13 31

07 16 00  M82PTCEN     11 21 59  49.2 -11.1  1.4     151.6   -15     1446   07 16 15
07 20 50  ---          11 26 50  49.0 -11.7  1.5     150.0   275     1464   07 16 01

07 21 30  J0958+65     11 27 30  52.7 -14.8  1.5     148.1    25     1464   07 21 30
07 24 00  ---          11 30 01  52.5 -15.1  1.5     147.3   150     1473   07 21 31

07 24 00  M82PTCEN     11 30 01  48.9 -12.0  1.5     149.0   -15     1473   07 24 15
07 28 50  ---          11 34 51  48.7 -12.6  1.6     147.4   275     1491   07 24 01

07 29 30  J0958+65     11 35 32  52.2 -15.9  1.6     145.4    25     1491   07 29 30
07 32 00  ---          11 38 02  52.0 -16.2  1.6     144.5   150     1501   07 29 31

07 32 00  M82PTCEN     11 38 02  48.5 -12.9  1.7     146.4   -15     1501   07 32 15
07 36 50  ---          11 42 53  48.3 -13.5  1.8     144.9   275     1519   07 32 01

07 37 30  J0958+65     11 43 33  51.7 -17.0  1.7     142.7    25     1519   07 37 30
07 40 00  ---          11 46 03  51.5 -17.3  1.8     141.9   150     1528   07 37 31

07 40 00  M82PTCEN     11 46 03  48.1 -13.8  1.8     143.9   -15     1528   07 40 15
07 44 50  ---          11 50 54  47.8 -14.3  1.9     142.4   275     1546   07 40 01

07 45 30  J0958+65     11 51 34  51.2 -18.0  1.9     140.1    25     1546   07 45 30
07 48 00  ---          11 54 05  51.0 -18.3  1.9     139.2   150     1556   07 45 31

07 48 00  M82PTCEN     11 54 05  47.7 -14.6  1.9     141.4   -15     1556   07 48 15
07 52 50  ---          11 58 55  47.4 -15.1  2.0     139.9   275     1573   07 48 01

07 53 30  J0958+65     11 59 36  50.6 -19.0  2.0     137.5    26     1573   07 53 30
07 56 00  ---          12 02 06  50.5 -19.3  2.0     136.7   150     1583   07 53 31

07 56 00  M82PTCEN     12 02 06  47.2 -15.4  2.1     138.9   -14     1583   07 56 14
08 00 50  ---          12 06 57  46.9 -15.9  2.2     137.5   276     1601   07 56 01

08 01 30  J0958+65     12 07 37  50.1 -20.0  2.1     134.9    26     1601   08 01 30
08 04 00  ---          12 10 07  49.9 -20.2  2.2     134.1   150     1610   08 01 31
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

08 04 00  M82PTCEN     12 10 07  46.8 -16.2  2.2     136.5   -14     1610   08 04 14
08 08 50  ---          12 14 58  46.5 -16.6  2.3     135.1   276     1628   08 04 01

08 09 30  J0958+65     12 15 38  49.5 -20.9  2.3     132.4    26     1628   08 09 30
08 12 00  ---          12 18 09  49.3 -21.1  2.3     131.6   150     1638   08 09 31

08 12 00  M82PTCEN     12 18 09  46.3 -16.9  2.3     134.1   -14     1638   08 12 14
08 16 50  ---          12 22 59  46.0 -17.3  2.4     132.7   276     1656   08 12 01

08 17 30  J0958+65     12 23 39  48.8 -21.7  2.4     130.0    26     1656   08 17 30
08 20 00  ---          12 26 10  48.6 -21.9  2.4     129.2   150     1665   08 17 31

08 20 00  M82PTCEN     12 26 10  45.8 -17.6  2.5     131.7   -14     1665   08 20 14
08 24 50  ---          12 31 01  45.4 -18.0  2.6     130.3   276     1683   08 20 01

08 25 30  J0958+65     12 31 41  48.2 -22.5  2.5     127.5    26     1683   08 25 30
08 28 00  ---          12 34 11  48.0 -22.7  2.6     126.8   150     1693   08 25 31

08 28 00  M82PTCEN     12 34 11  45.2 -18.2  2.6     129.4   -13     1693   08 28 13
08 32 40  ---          12 38 52  44.9 -18.6  2.7     128.0   267     1710   08 28 01

08 33 30  J0958+65     12 39 42  47.5 -23.2  2.7     125.2    37     1710   08 33 30
08 36 00  ---          12 42 13  47.3 -23.4  2.7     124.4   150     1720   08 33 31

08 36 00  M82PTCEN     12 42 13  44.7 -18.9  2.7     127.1   -13     1720   08 36 13
08 40 40  ---          12 46 53  44.3 -19.2  2.8     125.7   267     1737   08 36 01

08 41 30  J0958+65     12 47 43  46.8 -23.9  2.8     122.8    37     1737   08 41 30
08 44 00  ---          12 50 14  46.6 -24.1  2.8     122.1   150     1746   08 41 31

08 44 00  M82PTCEN     12 50 14  44.1 -19.4  2.9     124.8   -13     1746   08 44 13
08 48 40  ---          12 54 55  43.8 -19.7  3.0     123.5   267     1764   08 44 01

08 49 30  J0958+65     12 55 45  46.1 -24.5  2.9     120.6    37     1764   08 49 30
08 52 00  ---          12 58 15  45.9 -24.7  3.0     119.9   150     1773   08 49 31

08 52 00  M82PTCEN     12 58 15  43.5 -20.0  3.0     122.5   -13     1773   08 52 13
08 56 40  ---          13 02 56  43.2 -20.3  3.1     121.2   267     1790   08 52 01

08 57 30  J0958+65     13 03 46  45.4 -25.1  3.1     118.3    37     1790   08 57 30
09 00 00  ---          13 06 16  45.2 -25.3  3.1     117.6   150     1800   08 57 31

09 00 00  M82PTCEN     13 06 16  42.9 -20.5  3.2     120.3   -12     1800   09 00 12
09 04 40  ---          13 10 57  42.6 -20.7  3.2     119.0   268     1817   09 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

09 05 30  J0958+65     13 11 47  44.7 -25.7  3.2     116.1    38     1817   09 05 30
09 08 00  ---          13 14 18  44.4 -25.8  3.2     115.4   150     1827   09 05 31

09 08 00  M82PTCEN     13 14 18  42.3 -20.9  3.3     118.1   -12     1827   09 08 12
09 12 40  ---          13 18 59  42.0 -21.2  3.4     116.9   268     1844   09 08 01

09 13 30  J0958+65     13 19 49  43.9 -26.1  3.3     113.9    38     1844   09 13 30
09 16 00  ---          13 22 19  43.7 -26.3  3.4     113.3   150     1854   09 13 31

09 16 00  M82PTCEN     13 22 19  41.7 -21.4  3.4     116.0   -12     1854   09 16 12
09 20 40  ---          13 27 00  41.3 -21.6  3.5     114.7   268     1871   09 16 01

09 21 30  J0958+65     13 27 50  43.1 -26.6  3.5     111.8    38     1871   09 21 30
09 24 00  ---          13 30 20  42.9 -26.7  3.5     111.2   150     1881   09 21 31

09 24 00  M82PTCEN     13 30 20  41.1 -21.7  3.6     113.8   -12     1881   09 24 12
09 28 40  ---          13 35 01  40.7 -22.0  3.6     112.6   268     1898   09 24 01

09 29 30  J0958+65     13 35 51  42.4 -27.0  3.6     109.7    39     1898   09 29 30
09 32 00  ---          13 38 22  42.1 -27.1  3.6     109.1   150     1908   09 29 31

09 32 00  M82PTCEN     13 38 22  40.4 -22.1  3.7     111.7   -11     1908   09 32 11
09 36 40  ---          13 43 02  40.0 -22.3  3.8     110.5   269     1925   09 32 01

09 37 30  J0958+65     13 43 53  41.6 -27.4  3.7     107.6    39     1925   09 37 30
09 40 00  ---          13 46 23  41.3 -27.5  3.8     107.0   150     1935   09 37 31

09 40 00  M82PTCEN     13 46 23  39.8 -22.4  3.8     109.6   -11     1935   09 40 11
09 44 40  ---          13 51 04  39.4 -22.6  3.9     108.4   269     1952   09 40 01

09 45 30  J0958+65     13 51 54  40.8 -27.7  3.9     105.6    39     1952   09 45 30
09 48 00  ---          13 54 24  40.5 -27.8  3.9     105.0   150     1962   09 45 31

09 48 00  M82PTCEN     13 54 24  39.1 -22.7  4.0     107.6   -11     1962   09 48 11
09 52 40  ---          13 59 05  38.7 -22.9  4.0     106.4   269     1979   09 48 01

09 53 30  J0958+65     13 59 55  40.0 -27.9  4.0     103.6    39     1979   09 53 30
09 56 00  ---          14 02 26  39.7 -28.0  4.0     103.0   150     1989   09 53 31

09 56 00  M82PTCEN     14 02 26  38.4 -23.0  4.1     105.5   -11     1989   09 56 11
10 00 40  ---          14 07 06  38.0 -23.1  4.2     104.3   269     2006   09 56 01

10 01 30  J0958+65     14 07 57  39.2 -28.2  4.1     101.6    39     2006   10 01 30
10 04 00  ---          14 10 27  38.9 -28.2  4.2     101.0   150     2016   10 01 31
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

10 04 00  M82PTCEN     14 10 27  37.8 -23.2  4.2     103.5   -11     2016   10 04 11
10 08 40  ---          14 15 08  37.4 -23.3  4.3     102.3   269     2033   10 04 01

10 09 30  J0958+65     14 15 58  38.3 -28.4  4.3      99.7    39     2033   10 09 30
10 12 00  ---          14 18 28  38.1 -28.4  4.3      99.1   150     2043   10 09 31

10 12 00  M82PTCEN     14 18 28  37.1 -23.4  4.4     101.5   -11     2043   10 12 11
10 16 40  ---          14 23 09  36.7 -23.5  4.4     100.4   269     2060   10 12 01

10 17 30  J0958+65     14 23 59  37.5 -28.5  4.4      97.8    39     2060   10 17 30
10 20 00  ---          14 26 30  37.3 -28.6  4.4      97.2   150     2070   10 17 31

10 20 00  M82PTCEN     14 26 30  36.4 -23.5  4.5      99.5   -11     2070   10 20 11
10 24 40  ---          14 31 10  36.0 -23.6  4.6      98.4   269     2087   10 20 01

10 25 30  J0958+65     14 32 00  36.7 -28.7  4.5      95.9    39     2087   10 25 30
10 28 00  ---          14 34 31  36.4 -28.7  4.6      95.3   150     2097   10 25 31

10 28 00  M82PTCEN     14 34 31  35.7 -23.7  4.6      97.6   -11     2097   10 28 11
10 32 40  ---          14 39 12  35.3 -23.7  4.7      96.5   269     2114   10 28 01

10 33 30  J0958+65     14 40 02  35.9 -28.8  4.7      94.0    39     2114   10 33 30
10 36 00  ---          14 42 32  35.6 -28.8  4.7      93.4   150     2124   10 33 31

10 36 00  M82PTCEN     14 42 32  35.0 -23.8  4.8      95.6   -11     2124   10 36 11
10 40 40  ---          14 47 13  34.6 -23.8  4.8      94.5   269     2141   10 36 01

10 41 30  J0958+65     14 48 03  35.0 -28.8  4.8      92.1    39     2141   10 41 30
10 44 00  ---          14 50 34  34.8 -28.8  4.8      91.6   150     2151   10 41 31

10 44 00  M82PTCEN     14 50 34  34.3 -23.8  4.9      93.7   -11     2151   10 44 11
10 48 40  ---          14 55 14  33.9 -23.9  5.0      92.6   269     2168   10 44 01

10 49 30  J0958+65     14 56 04  34.2 -28.8  4.9      90.3    39     2168   10 49 30
10 52 00  ---          14 58 35  33.9 -28.8  5.0      89.7   150     2178   10 49 31

10 52 00  M82PTCEN     14 58 35  33.6 -23.9  5.0      91.8   -11     2178   10 52 11
10 56 40  ---          15 03 16  33.2 -23.9  5.1      90.7   269     2195   10 52 01

10 57 30  J0958+65     15 04 06  33.4 -28.8  5.1      88.5    39     2195   10 57 30
11 00 00  ---          15 06 36  33.1 -28.8  5.1      87.9   150     2205   10 57 31

11 00 00  M82PTCEN     15 06 36  32.9 -23.9  5.2      89.9   -11     2205   11 00 11
11 04 40  ---          15 11 17  32.5 -23.9  5.2      88.8   269     2222   11 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

11 05 30  J0958+65     15 12 07  32.5 -28.8  5.2      86.7    39     2222   11 05 30
11 08 00  ---          15 14 37  32.3 -28.8  5.2      86.1   150     2232   11 05 31

11 08 00  M82PTCEN     15 14 37  32.2 -23.9  5.3      88.1   -11     2232   11 08 11
11 12 40  ---          15 19 18  31.8 -23.9  5.4      87.0   269     2249   11 08 01

11 13 30  J0958+65     15 20 08  31.7 -28.7  5.3      84.9    39     2249   11 13 30
11 16 00  ---          15 22 39  31.4 -28.7  5.4      84.3   150     2259   11 13 31

11 16 00  M82PTCEN     15 22 39  31.5 -23.8  5.4      86.2   -11     2259   11 16 11
11 20 40  ---          15 27 20  31.1 -23.8  5.5      85.1   269     2276   11 16 01

11 21 30  J0958+65     15 28 10  30.9 -28.6  5.5      83.1    39     2276   11 21 30
11 24 00  ---          15 30 40  30.6 -28.6  5.5      82.6   150     2286   11 21 31

11 24 00  M82PTCEN     15 30 40  30.8 -23.8  5.6      84.4   -11     2286   11 24 11
11 28 40  ---          15 35 21  30.4 -23.7  5.6      83.3   269     2303   11 24 01

11 29 30  J0958+65     15 36 11  30.0 -28.5  5.6      81.4    39     2303   11 29 30
11 32 00  ---          15 38 41  29.8 -28.4  5.6      80.8   150     2313   11 29 31

11 32 00  M82PTCEN     15 38 41  30.1 -23.7  5.7      82.5   -11     2313   11 32 11
11 36 40  ---          15 43 22  29.7 -23.6  5.8      81.5   269     2330   11 32 01

11 37 30  J0958+65     15 44 12  29.2 -28.3  5.7      79.6    39     2330   11 37 30
11 40 00  ---          15 46 43  29.0 -28.3  5.8      79.1   150     2340   11 37 31

11 40 00  M82PTCEN     15 46 43  29.4 -23.6  5.8      80.7   -11     2340   11 40 11
11 46 40  ---          15 53 24  28.9 -23.4  5.9      79.2   389     2365   11 40 01

11 47 30  J0958+65     15 54 14  28.2 -28.1  5.9      77.4    39     2365   11 47 30
11 50 00  ---          15 56 44  28.0 -28.0  5.9      76.9   150     2374   11 47 31

12 10 00  J0958+65     16 16 48  25.9 -27.4  6.3      72.6  1194     2374   12 10 00
12 12 00  ---          16 18 48  25.8 -27.3  6.3      72.2   120     2382   12 10 01

12 12 00  M82PTCEN     16 18 48  26.7 -22.9  6.4      73.5   -11     2382   12 12 11
12 16 40  ---          16 23 29  26.3 -22.7  6.4      72.5   269     2399   12 12 01

12 17 30  J0958+65     16 24 19  25.2 -27.1  6.4      71.0    39     2399   12 17 30
12 20 00  ---          16 26 49  25.0 -27.0  6.4      70.5   150     2409   12 17 31

12 20 00  M82PTCEN     16 26 49  26.0 -22.6  6.5      71.7   -11     2409   12 20 11
12 24 40  ---          16 31 30  25.7 -22.5  6.6      70.7   269     2426   12 20 01
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

12 25 30  J0958+65     16 32 20  24.4 -26.8  6.5      69.3    39     2426   12 25 30
12 28 00  ---          16 34 51  24.2 -26.7  6.6      68.8   150     2436   12 25 31

12 28 00  M82PTCEN     16 34 51  25.4 -22.4  6.6      70.0   -11     2436   12 28 11
12 32 40  ---          16 39 31  25.0 -22.2  6.7      68.9   269     2453   12 28 01

12 33 30  J0958+65     16 40 22  23.7 -26.5  6.7      67.6    39     2453   12 33 30
12 36 00  ---          16 42 52  23.4 -26.4  6.7      67.1   150     2463   12 33 31

12 36 00  M82PTCEN     16 42 52  24.7 -22.1  6.8      68.2   -11     2463   12 36 11
12 40 40  ---          16 47 33  24.3 -21.9  6.8      67.2   269     2480   12 36 01

12 41 30  J0958+65     16 48 23  22.9 -26.1  6.8      66.0    39     2480   12 41 30
12 44 00  ---          16 50 53  22.6 -26.0  6.8      65.4   150     2490   12 41 31

12 44 00  M82PTCEN     16 50 53  24.1 -21.8  6.9      66.5   -11     2490   12 44 11
12 48 40  ---          16 55 34  23.7 -21.6  7.0      65.4   269     2507   12 44 01

12 49 30  J0958+65     16 56 24  22.1 -25.7  6.9      64.3    39     2507   12 49 30
12 52 00  ---          16 58 55  21.9 -25.6  7.0      63.8   150     2517   12 49 31

12 52 00  M82PTCEN     16 58 55  23.4 -21.5  7.0      64.7   -11     2517   12 52 11
12 56 40  ---          17 03 35  23.1 -21.3  7.1      63.7   269     2534   12 52 01

12 57 30  J0958+65     17 04 25  21.4 -25.3  7.1      62.6    39     2534   12 57 30
13 00 00  ---          17 06 56  21.2 -25.2  7.1      62.1   150     2544   12 57 31

13 00 00  M82PTCEN     17 06 56  22.8 -21.1  7.2      63.0   -11     2544   13 00 11
13 04 40  ---          17 11 37  22.5 -20.9  7.2      61.9   269     2561   13 00 01

13 05 30  J0958+65     17 12 27  20.7 -24.9  7.2      60.9    39     2561   13 05 30
13 08 00  ---          17 14 57  20.4 -24.8  7.2      60.4   150     2571   13 05 31

13 08 00  M82PTCEN     17 14 57  22.2 -20.8  7.3      61.2   -12     2571   13 08 12
13 12 40  ---          17 19 38  21.8 -20.6  7.4      60.2   268     2588   13 08 01

13 13 30  J0958+65     17 20 28  19.9 -24.5  7.3      59.3    38     2588   13 13 30
13 16 00  ---          17 22 59  19.7 -24.3  7.4      58.7   150     2598   13 13 31

13 16 00  M82PTCEN     17 22 59  21.6 -20.4  7.4      59.5   -12     2598   13 16 12
13 20 40  ---          17 27 39  21.2 -20.2  7.5      58.5   268     2615   13 16 01

13 21 30  J0958+65     17 28 29  19.2 -24.0  7.5      57.6    38     2615   13 21 30
13 24 00  ---          17 31 00  19.0 -23.9  7.5      57.1   150     2625   13 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

13 24 00  M82PTCEN     17 31 00  21.0 -20.0  7.6      57.7   -12     2625   13 24 12
13 28 40  ---          17 35 41  20.7 -19.8  7.6      56.7   268     2642   13 24 01

13 29 30  J0958+65     17 36 31  18.5 -23.5  7.6      55.9    38     2642   13 29 30
13 32 00  ---          17 39 01  18.3 -23.4  7.6      55.4   150     2652   13 29 31

13 32 00  M82PTCEN     17 39 01  20.4 -19.6  7.7      56.0   -12     2652   13 32 12
13 36 40  ---          17 43 42  20.1 -19.4  7.8      55.0   268     2669   13 32 01

13 37 30  J0958+65     17 44 32  17.8 -23.0  7.7      54.3    38     2669   13 37 30
13 40 00  ---          17 47 02  17.6 -22.9  7.8      53.7   150     2679   13 37 31

13 40 00  M82PTCEN     17 47 02  19.8 -19.2  7.8      54.3   -12     2679   13 40 12
13 44 40  ---          17 51 43  19.5 -18.9  7.9      53.3   268     2696   13 40 01

13 45 30  J0958+65     17 52 33  17.2 -22.5  7.9      52.6    37     2696   13 45 30
13 48 00  ---          17 55 04  17.0 -22.4  7.9      52.1   150     2706   13 45 31

13 48 00  M82PTCEN     17 55 04  19.3 -18.8  8.0      52.5   -13     2706   13 48 13
13 52 40  ---          17 59 45  19.0 -18.5  8.0      51.5   267     2723   13 48 01

13 53 30  J0958+65     18 00 35  16.5 -22.0  8.0      50.9    37     2723   13 53 30
13 56 00  ---          18 03 05  16.3 -21.8  8.1      50.4   150     2732   13 53 31

13 56 00  M82PTCEN     18 03 05  18.7 -18.3  8.1      50.8   -13     2732   13 56 13
14 00 40  ---          18 07 46  18.4 -18.0  8.2      49.8   267     2750   13 56 01

14 01 30  J0958+65     18 08 36  15.9 -21.4  8.1      49.2    37     2750   14 01 30
14 04 00  ---          18 11 06  15.7 -21.2  8.2      48.7   150     2759   14 01 31

14 04 00  M82PTCEN     18 11 06  18.2 -17.8  8.2      49.1   -13     2759   14 04 13
14 08 40  ---          18 15 47  17.9 -17.5  8.3      48.1   267     2777   14 04 01

14 09 30  J0958+65     18 16 37  15.3 -20.9  8.3      47.6    37     2777   14 09 30
14 12 00  ---          18 19 08  15.1 -20.7  8.3      47.1   150     2786   14 09 31

14 12 00  M82PTCEN     18 19 08  17.7 -17.3  8.4      47.3   -13     2786   14 12 13
14 16 40  ---          18 23 48  17.4 -17.0  8.4      46.3   267     2803   14 12 01

14 17 30  J0958+65     18 24 39  14.7 -20.3  8.4      45.9    37     2803   14 17 30
14 20 00  ---          18 27 09  14.5 -20.1  8.5      45.4   150     2813   14 17 31

14 20 00  M82PTCEN     18 27 09  17.2 -16.8  8.5      45.6   -13     2813   14 20 13
14 24 40  ---          18 31 50  16.9 -16.5  8.6      44.6   267     2830   14 20 01
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

14 25 30  J0958+65     18 32 40  14.1 -19.7  8.5      44.2    37     2830   14 25 30
14 28 00  ---          18 35 10  13.9 -19.5  8.6      43.7   150     2840   14 25 31

14 28 00  M82PTCEN     18 35 10  16.7 -16.3  8.6      43.9   -13     2840   14 28 13
14 32 40  ---          18 39 51  16.4 -16.0  8.7      42.9   267     2857   14 28 01

14 33 30  J0958+65     18 40 41  13.5 -19.0  8.7      42.6    36     2857   14 33 30
14 36 00  ---          18 43 12  13.3 -18.8  8.7      42.0   150     2867   14 33 31

14 36 00  M82PTCEN     18 43 12  16.2 -15.8  8.8      42.2   -14     2867   14 36 14
14 40 40  ---          18 47 52  15.9 -15.5  8.8      41.1   266     2884   14 36 01

14 41 30  J0958+65     18 48 43  12.9 -18.4  8.8      40.9    36     2884   14 41 30
14 44 00  ---          18 51 13  12.8 -18.2  8.9      40.3   150     2894   14 41 31

14 44 00  M82PTCEN     18 51 13  15.7 -15.2  8.9      40.4   -14     2894   14 44 14
14 48 40  ---          18 55 54  15.5 -14.9  9.0      39.4   266     2911   14 44 01

14 49 30  J0958+65     18 56 44  12.4 -17.7  8.9      39.2    36     2911   14 49 30
14 52 00  ---          18 59 14  12.2 -17.5  9.0      38.7   150     2920   14 49 31

14 52 00  M82PTCEN     18 59 14  15.3 -14.7  9.0      38.7   -14     2920   14 52 14
14 56 40  ---          19 03 55  15.0 -14.3  9.1      37.7   266     2937   14 52 01

14 57 30  J0958+65     19 04 45  11.9 -17.1  9.1      37.5    36     2937   14 57 30
15 00 00  ---          19 07 16  11.7 -16.9  9.1      37.0   150     2947   14 57 31

15 00 00  M82PTCEN     19 07 16  14.9 -14.1  9.2      37.0   -14     2947   15 00 14
15 04 40  ---          19 11 56  14.6 -13.8  9.2      36.0   266     2964   15 00 01

15 05 30  J0958+65     19 12 46  11.4 -16.4  9.2      35.8    36     2964   15 05 30
15 08 00  ---          19 15 17  11.2 -16.2  9.3      35.3   150     2974   15 05 31

15 08 00  M82PTCEN     19 15 17  14.4 -13.5  9.3      35.2   -14     2974   15 08 14
15 12 40  ---          19 19 58  14.2 -13.2  9.4      34.2   266     2991   15 08 01

15 13 30  J0958+65     19 20 48  10.9 -15.7  9.3      34.1    36     2991   15 13 30
15 16 00  ---          19 23 18  10.8 -15.5  9.4      33.6   150     3001   15 13 31

15 16 00  M82PTCEN     19 23 18  14.1 -12.9  9.4      33.5   -14     3001   15 16 14
15 20 40  ---          19 27 59  13.8 -12.6  9.5      32.5   266     3018   15 16 01

15 21 30  J0958+65     19 28 49  10.5 -15.0  9.5      32.4    35     3018   15 21 30
15 24 00  ---          19 31 20  10.3 -14.8  9.5      31.9   150     3028   15 21 31
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

15 24 00  M82PTCEN     19 31 20  13.7 -12.3  9.6      31.8   -15     3028   15 24 15
15 28 40  ---          19 36 00  13.5 -12.0  9.6      30.8   265     3045   15 24 01

15 29 30  J0958+65     19 36 50  10.0 -14.3  9.6      30.7    35     3045   15 29 30
15 32 00  ---          19 39 21   9.9 -14.0  9.7      30.2   150     3054   15 29 31

15 32 00  M82PTCEN     19 39 21  13.3 -11.7  9.7      30.0   -15     3054   15 32 15
15 36 40  ---          19 44 02  13.1 -11.3  9.8      29.0   265     3071   15 32 01

15 37 30  J0958+65     19 44 52   9.6 -13.5  9.7      29.0    35     3071   15 37 30
15 40 00  ---          19 47 22   9.5 -13.3  9.8      28.5   150     3081   15 37 31

15 40 00  M82PTCEN     19 47 22  13.0 -11.1  9.8      28.3   -15     3081   15 40 15
15 44 40  ---          19 52 03  12.8 -10.7  9.9      27.3   265     3098   15 40 01

15 45 30  J0958+65     19 52 53   9.2 -12.8  9.9      27.3    35     3098   15 45 30
15 48 00  ---          19 55 23   9.1 -12.6  9.9      26.8   150     3108   15 45 31

15 48 00  M82PTCEN     19 55 23  12.7 -10.4 10.0      26.6   -15     3108   15 48 15
15 52 40  ---          20 00 04  12.5 -10.1 10.0      25.5   265     3125   15 48 01

15 53 30  J0958+65     20 00 54   8.8 -12.0 10.0      25.6    35     3125   15 53 30
15 56 00  ---          20 03 25   8.7 -11.8 10.1      25.1   150     3134   15 53 31

15 56 00  M82PTCEN     20 03 25  12.4  -9.8 10.1      24.8   -15     3134   15 56 15
16 00 40  ---          20 08 06  12.2  -9.4 10.2      23.8   265     3151   15 56 01

16 01 30  J0958+65     20 08 56   8.5 -11.3 10.1      23.9    35     3151   16 01 30
16 04 00  ---          20 11 26   8.4 -11.0 10.2      23.4   150     3161   16 01 31

16 04 00  M82PTCEN     20 11 26  12.1  -9.1 10.2      23.1   -15     3161   16 04 15
16 08 40  ---          20 16 07  11.9  -8.7 10.3      22.1   265     3178   16 04 01

16 09 30  J0958+65     20 16 57   8.2 -10.5 10.3      22.2    35     3178   16 09 30
16 12 00  ---          20 19 27   8.1 -10.3 10.3      21.7   150     3188   16 09 31

16 12 00  M82PTCEN     20 19 27  11.8  -8.5 10.4      21.3   -15     3188   16 12 15
16 16 40  ---          20 24 08  11.7  -8.1 10.4      20.3   265     3205   16 12 01

16 17 30  J0958+65     20 24 58   7.9  -9.7 10.4      20.5    35     3205   16 17 30
16 20 00  ---          20 27 29   7.8  -9.5 10.5      20.0   150     3215   16 17 31

16 20 00  M82PTCEN     20 27 29  11.6  -7.8 10.5      19.6   -15     3215   16 20 15
16 24 40  ---          20 32 09  11.4  -7.4 10.6      18.6   265     3232   16 20 01
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

16 25 30  J0958+65     20 33 00   7.6  -8.9 10.5      18.8    34     3232   16 25 30
16 28 00  ---          20 35 30   7.5  -8.7 10.6      18.2   150     3241   16 25 31

16 28 00  M82PTCEN     20 35 30  11.3  -7.1 10.6      17.8   -16     3241   16 28 16
16 32 50  ---          20 40 21  11.2  -6.7 10.7      16.8   274     3259   16 28 01

16 33 30  J0958+65     20 41 01   7.3  -8.1 10.7      17.1    24     3259   16 33 30
16 36 00  ---          20 43 31   7.3  -7.9 10.7      16.5   150     3269   16 33 31

16 36 00  M82PTCEN     20 43 31  11.1  -6.4 10.8      16.1   -16     3269   16 36 16
16 40 50  ---          20 48 22  11.0  -6.0 10.9      15.0   274     3286   16 36 01

16 41 30  J0958+65     20 49 02   7.1  -7.3 10.8      15.3    24     3286   16 41 30
16 44 00  ---          20 51 33   7.0  -7.1 10.9      14.8   150     3296   16 41 31

16 44 00  M82PTCEN     20 51 33  10.9  -5.8 10.9      14.3   -16     3296   16 44 16
16 50 50  ---          20 58 24  10.8  -5.2 11.0      12.8   394     3321   16 44 01

16 51 30  J0958+65     20 59 04   6.8  -6.3 11.0      13.2    24     3321   16 51 30
16 54 00  ---          21 01 34   6.8  -6.1 11.0      12.6   150     3331   16 51 31

17 06 00  J0958+65     21 13 36   6.5  -4.8 11.2      10.0   714     3331   17 06 00
17 09 00  ---          21 16 37   6.5  -4.5 11.3       9.4   180     3343   17 06 01

17 21 40  3C84         21 29 19  21.2  53.3 -5.9     -67.3   712     3343   17 21 40
17 29 40  ---          21 37 20  22.6  53.9 -5.7     -68.4   480     3374   17 21 41

17 37 40  J0958+65     21 45 22   6.2  -1.5 11.8       3.2   432     3374   17 37 40
17 40 40  ---          21 48 22   6.1  -1.2 11.8       2.5   180     3385   17 37 41

17 40 40  M82PTCEN     21 48 22  10.2  -0.8 11.9       1.9   -16     3385   17 40 56
17 45 10  ---          21 52 53  10.2  -0.4 11.9       0.9   254     3401   17 40 41

17 46 10  J0958+65     21 53 53   6.1  -0.6 11.9       1.3    44     3401   17 46 10
17 48 40  ---          21 56 24   6.1  -0.4 11.9       0.8   150     3411   17 46 11

17 48 40  M82PTCEN     21 56 24  10.2  -0.1 12.0       0.2   -16     3411   17 48 56
17 53 10  ---          22 00 54  10.2   0.3-11.9      -0.8   254     3427   17 48 41

17 54 10  J0958+65     22 01 54   6.1   0.2-12.0      -0.4    44     3427   17 54 10
17 56 40  ---          22 04 25   6.1   0.5-11.9      -0.9   150     3437   17 54 11

17 56 40  M82PTCEN     22 04 25  10.2   0.6-11.9      -1.6   -16     3437   17 56 56
18 01 10  ---          22 08 56  10.3   1.0-11.8      -2.6   254     3454   17 56 41
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

18 02 10  J0958+65     22 09 56   6.1   1.0-11.8      -2.1    44     3454   18 02 10
18 04 40  ---          22 12 26   6.2   1.3-11.8      -2.7   150     3463   18 02 11

18 04 40  M82PTCEN     22 12 26  10.3   1.3-11.7      -3.3   -16     3463   18 04 56
18 09 10  ---          22 16 57  10.3   1.7-11.7      -4.3   254     3480   18 04 41

18 10 10  J0958+65     22 17 57   6.2   1.9-11.7      -3.9    44     3480   18 10 10
18 12 40  ---          22 20 27   6.2   2.1-11.7      -4.4   150     3489   18 10 11

18 12 40  M82PTCEN     22 20 27  10.3   2.1-11.6      -5.1   -16     3489   18 12 56
18 17 10  ---          22 24 58  10.4   2.5-11.5      -6.1   254     3506   18 12 41

18 18 10  J0958+65     22 25 58   6.3   2.7-11.6      -5.6    44     3506   18 18 10
18 20 40  ---          22 28 29   6.3   3.0-11.5      -6.1   150     3515   18 18 11

18 20 40  M82PTCEN     22 28 29  10.4   2.8-11.5      -6.8   -16     3515   18 20 56
18 25 10  ---          22 33 00  10.4   3.2-11.4      -7.8   254     3532   18 20 41

18 26 10  J0958+65     22 34 00   6.3   3.5-11.4      -7.3    44     3532   18 26 10
18 28 40  ---          22 36 30   6.4   3.8-11.4      -7.9   150     3541   18 26 11

18 28 40  M82PTCEN     22 36 30  10.5   3.5-11.3      -8.6   -16     3541   18 28 56
18 33 10  ---          22 41 01  10.6   3.9-11.3      -9.6   254     3558   18 28 41

18 34 10  J0958+65     22 42 01   6.5   4.4-11.3      -9.1    44     3558   18 34 10
18 36 40  ---          22 44 31   6.5   4.6-11.3      -9.6   150     3567   18 34 11

18 36 40  M82PTCEN     22 44 31  10.6   4.2-11.2     -10.3   -16     3567   18 36 56
18 41 10  ---          22 49 02  10.7   4.6-11.1     -11.3   254     3584   18 36 41

18 42 10  J0958+65     22 50 02   6.6   5.2-11.2     -10.8    44     3584   18 42 10
18 44 40  ---          22 52 33   6.7   5.4-11.1     -11.3   150     3593   18 42 11

18 44 40  M82PTCEN     22 52 33  10.7   4.9-11.1     -12.1   -16     3593   18 44 56
18 49 10  ---          22 57 03  10.8   5.3-11.0     -13.1   254     3610   18 44 41

18 50 10  J0958+65     22 58 04   6.8   6.0-11.0     -12.5    44     3610   18 50 10
18 52 40  ---          23 00 34   6.8   6.3-11.0     -13.1   150     3619   18 50 11

18 52 40  M82PTCEN     23 00 34  10.9   5.6-10.9     -13.8   -16     3619   18 52 56
18 57 10  ---          23 05 05  11.0   5.9-10.9     -14.8   254     3636   18 52 41

18 58 10  J0958+65     23 06 05   7.0   6.8-10.9     -14.3    44     3636   18 58 10
19 00 40  ---          23 08 35   7.0   7.1-10.9     -14.8   150     3645   18 58 11
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

19 00 40  M82PTCEN     23 08 35  11.1   6.2-10.8     -15.6   -16     3645   19 00 56
19 05 10  ---          23 13 06  11.2   6.6-10.7     -16.6   254     3662   19 00 41

19 06 10  J0958+65     23 14 06   7.2   7.6-10.8     -16.0    44     3662   19 06 10
19 08 40  ---          23 16 37   7.3   7.9-10.7     -16.5   150     3671   19 06 11

19 08 40  M82PTCEN     23 16 37  11.3   6.9-10.7     -17.3   -16     3671   19 08 56
19 13 10  ---          23 21 07  11.4   7.3-10.6     -18.3   254     3688   19 08 41

19 14 10  J0958+65     23 22 08   7.4   8.4-10.6     -17.7    44     3688   19 14 10
19 16 40  ---          23 24 38   7.5   8.7-10.6     -18.2   150     3697   19 14 11

19 16 40  M82PTCEN     23 24 38  11.5   7.6-10.5     -19.1   -16     3697   19 16 56
19 21 10  ---          23 29 09  11.6   8.0-10.5     -20.1   254     3714   19 16 41

19 22 10  J0958+65     23 30 09   7.7   9.2-10.5     -19.4    44     3714   19 22 10
19 24 40  ---          23 32 39   7.8   9.5-10.5     -20.0   150     3723   19 22 11

19 24 40  M82PTCEN     23 32 39  11.7   8.3-10.4     -20.8   -16     3723   19 24 56
19 29 10  ---          23 37 10  11.9   8.7-10.3     -21.8   254     3740   19 24 41

19 30 10  J0958+65     23 38 10   8.0  10.0-10.4     -21.1    44     3740   19 30 10
19 32 40  ---          23 40 41   8.1  10.3-10.3     -21.7   150     3749   19 30 11

19 32 40  M82PTCEN     23 40 41  12.0   8.9-10.3     -22.6   -16     3749   19 32 56
19 37 10  ---          23 45 11  12.1   9.3-10.2     -23.5   254     3766   19 32 41

19 38 10  J0958+65     23 46 12   8.3  10.8-10.2     -22.9    44     3766   19 38 10
19 40 40  ---          23 48 42   8.4  11.0-10.2     -23.4   150     3775   19 38 11

19 40 40  M82PTCEN     23 48 42  12.3   9.6-10.1     -24.3   -16     3775   19 40 56
19 45 10  ---          23 53 13  12.4  10.0-10.1     -25.3   254     3792   19 40 41

19 46 10  J0958+65     23 54 13   8.6  11.6-10.1     -24.6    44     3792   19 46 10
19 48 40  ---          23 56 43   8.7  11.8-10.1     -25.1   150     3801   19 46 11

19 48 40  M82PTCEN     23 56 43  12.6  10.2-10.0     -26.0   -16     3801   19 48 56
19 53 10  ---          00 01 14  12.7  10.6 -9.9     -27.0   254     3818   19 48 41

19 54 10  J0958+65     00 02 14   9.0  12.3-10.0     -26.3    45     3818   19 54 10
19 56 40  ---          00 04 45   9.1  12.6 -9.9     -26.8   150     3827   19 54 11

19 56 40  M82PTCEN     00 04 45  12.9  10.9 -9.9     -27.8   -15     3827   19 56 56
20 01 10  ---          00 09 15  13.1  11.2 -9.8     -28.8   255     3844   19 56 41
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

20 02 10  J0958+65     00 10 15   9.4  13.1 -9.8     -28.0    45     3844   20 02 10
20 04 40  ---          00 12 46   9.5  13.3 -9.8     -28.5   150     3854   20 02 11

20 04 40  M82PTCEN     00 12 46  13.2  11.5 -9.7     -29.5   -15     3854   20 04 56
20 09 10  ---          00 17 17  13.4  11.9 -9.7     -30.5   255     3870   20 04 41

20 10 10  J0958+65     00 18 17   9.8  13.8 -9.7     -29.7    45     3870   20 10 10
20 12 40  ---          00 20 47   9.9  14.0 -9.7     -30.2   150     3880   20 10 11

20 12 40  M82PTCEN     00 20 47  13.6  12.1 -9.6     -31.3   -15     3880   20 12 55
20 17 10  ---          00 25 18  13.8  12.5 -9.5     -32.2   255     3896   20 12 41

20 18 10  J0958+65     00 26 18  10.2  14.5 -9.6     -31.4    45     3896   20 18 10
20 20 40  ---          00 28 48  10.3  14.8 -9.5     -31.9   150     3906   20 18 11

20 20 40  M82PTCEN     00 28 48  13.9  12.7 -9.5     -33.0   -15     3906   20 20 55
20 25 10  ---          00 33 19  14.2  13.1 -9.4     -34.0   255     3922   20 20 41

20 26 10  J0958+65     00 34 19  10.6  15.3 -9.4     -33.1    45     3922   20 26 10
20 28 40  ---          00 36 50  10.8  15.5 -9.4     -33.6   150     3932   20 26 11

20 28 40  M82PTCEN     00 36 50  14.3  13.3 -9.3     -34.7   -15     3932   20 28 55
20 33 10  ---          00 41 21  14.6  13.7 -9.3     -35.7   255     3948   20 28 41

20 34 10  J0958+65     00 42 21  11.1  16.0 -9.3     -34.8    45     3948   20 34 10
20 36 40  ---          00 44 51  11.2  16.2 -9.3     -35.3   150     3958   20 34 11

20 36 40  M82PTCEN     00 44 51  14.7  13.9 -9.2     -36.5   -15     3958   20 36 55
20 41 10  ---          00 49 22  15.0  14.3 -9.1     -37.4   255     3974   20 36 41

20 42 10  J0958+65     00 50 22  11.6  16.7 -9.2     -36.5    45     3974   20 42 10
20 44 40  ---          00 52 52  11.7  16.9 -9.1     -37.0   150     3984   20 42 11

20 44 40  M82PTCEN     00 52 52  15.2  14.5 -9.1     -38.2   -15     3984   20 44 55
20 49 10  ---          00 57 23  15.4  14.8 -9.0     -39.2   255     4000   20 44 41

20 50 10  J0958+65     00 58 23  12.1  17.3 -9.0     -38.1    45     4000   20 50 10
20 52 40  ---          01 00 54  12.2  17.5 -9.0     -38.7   150     4010   20 50 11

20 52 40  M82PTCEN     01 00 54  15.6  15.1 -8.9     -39.9   -15     4010   20 52 55
20 57 00  ---          01 05 14  15.8  15.4 -8.9     -40.9   245     4026   20 52 41

20 58 00  J0958+65     01 06 15  12.6  18.0 -8.9     -39.8    45     4026   20 58 00
21 00 30  ---          01 08 45  12.8  18.2 -8.9     -40.3   150     4036   20 58 01
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

21 00 30  M82PTCEN     01 08 45  16.1  15.6 -8.8     -41.6   -15     4036   21 00 45
21 04 50  ---          01 13 06  16.3  15.9 -8.7     -42.6   245     4051   21 00 31

21 05 50  J0958+65     01 14 06  13.1  18.6 -8.8     -41.4    46     4051   21 05 50
21 08 20  ---          01 16 36  13.3  18.8 -8.7     -42.0   150     4061   21 05 51

21 08 20  M82PTCEN     01 16 36  16.5  16.1 -8.7     -43.3   -14     4061   21 08 35
21 12 40  ---          01 20 57  16.8  16.4 -8.6     -44.2   246     4077   21 08 21

21 13 40  J0958+65     01 21 57  13.7  19.2 -8.6     -43.1    46     4077   21 13 40
21 16 10  ---          01 24 28  13.9  19.4 -8.6     -43.6   150     4086   21 13 41

21 16 10  M82PTCEN     01 24 28  17.0  16.6 -8.5     -45.0   -14     4086   21 16 24
21 20 30  ---          01 28 48  17.3  16.9 -8.5     -45.9   246     4102   21 16 11

21 21 30  J0958+65     01 29 48  14.2  19.8 -8.5     -44.7    46     4102   21 21 30
21 24 00  ---          01 32 19  14.4  20.0 -8.5     -45.2   150     4112   21 21 31

21 24 00  M82PTCEN     01 32 19  17.5  17.1 -8.4     -46.7   -14     4112   21 24 14
21 28 20  ---          01 36 40  17.8  17.4 -8.3     -47.6   246     4128   21 24 01

21 29 20  J0958+65     01 37 40  14.8  20.4 -8.4     -46.4    46     4128   21 29 20
21 31 50  ---          01 40 10  15.0  20.6 -8.3     -46.9   150     4137   21 29 21

21 31 50  M82PTCEN     01 40 10  18.0  17.6 -8.3     -48.4   -14     4137   21 32 04
21 36 10  ---          01 44 31  18.3  17.9 -8.2     -49.3   246     4153   21 31 51

21 37 10  J0958+65     01 45 31  15.4  21.0 -8.2     -48.0    46     4153   21 37 10
21 39 40  ---          01 48 01  15.6  21.2 -8.2     -48.5   150     4163   21 37 11

21 39 40  M82PTCEN     01 48 01  18.5  18.1 -8.2     -50.1   -14     4163   21 39 54
21 44 00  ---          01 52 22  18.8  18.4 -8.1     -51.0   246     4179   21 39 41

21 45 00  J0958+65     01 53 22  16.0  21.6 -8.1     -49.6    46     4179   21 45 00
21 47 30  ---          01 55 53  16.2  21.7 -8.1     -50.2   150     4188   21 45 01

21 47 30  M82PTCEN     01 55 53  19.0  18.6 -8.0     -51.8   -14     4188   21 47 44
21 51 50  ---          02 00 13  19.3  18.8 -7.9     -52.7   246     4204   21 47 31

21 52 50  J0958+65     02 01 14  16.7  22.1 -8.0     -51.3    47     4204   21 52 50
21 55 20  ---          02 03 44  16.9  22.3 -7.9     -51.8   150     4214   21 52 51

21 55 20  M82PTCEN     02 03 44  19.6  19.0 -7.9     -53.5   -13     4214   21 55 34
21 59 40  ---          02 08 05  19.9  19.2 -7.8     -54.4   247     4230   21 55 21
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

22 00 40  J0958+65     02 09 05  17.3  22.6 -7.8     -52.9    47     4230   22 00 40
22 03 10  ---          02 11 35  17.5  22.8 -7.8     -53.4   150     4240   22 00 41

22 03 10  M82PTCEN     02 11 35  20.1  19.4 -7.8     -55.2   -13     4240   22 03 23
22 07 30  ---          02 15 56  20.4  19.6 -7.7     -56.1   247     4255   22 03 11

22 08 30  J0958+65     02 16 56  18.0  23.1 -7.7     -54.5    47     4255   22 08 30
22 11 00  ---          02 19 27  18.2  23.3 -7.7     -55.1   150     4265   22 08 31

22 11 00  M82PTCEN     02 19 27  20.7  19.8 -7.6     -56.9   -13     4265   22 11 13
22 15 20  ---          02 23 47  21.0  20.0 -7.6     -57.8   247     4281   22 11 01

22 16 20  J0958+65     02 24 47  18.6  23.6 -7.6     -56.2    47     4281   22 16 20
22 18 50  ---          02 27 18  18.8  23.8 -7.5     -56.7   150     4291   22 16 21

22 18 50  M82PTCEN     02 27 18  21.3  20.2 -7.5     -58.6   -13     4291   22 19 03
22 23 10  ---          02 31 39  21.6  20.4 -7.4     -59.5   247     4307   22 18 51

22 24 10  J0958+65     02 32 39  19.3  24.1 -7.5     -57.8    47     4307   22 24 10
22 26 40  ---          02 35 09  19.5  24.2 -7.4     -58.3   150     4316   22 24 11

22 26 40  M82PTCEN     02 35 09  21.9  20.6 -7.4     -60.3   -13     4316   22 26 53
22 30 50  ---          02 39 20  22.2  20.8 -7.3     -61.2   237     4332   22 26 41

22 31 40  J0958+65     02 40 10  20.0  24.5 -7.3     -59.4    37     4332   22 31 40
22 33 40  ---          02 42 10  20.2  24.6 -7.3     -59.8   120     4339   22 31 41

22 33 40  M82PTCEN     02 42 10  22.4  20.9 -7.3     -61.8   -12     4339   22 33 53
22 37 50  ---          02 46 21  22.7  21.1 -7.2     -62.7   238     4355   22 33 41

22 38 40  J0958+65     02 47 11  20.6  24.9 -7.2     -60.8    38     4355   22 38 40
22 40 40  ---          02 49 11  20.8  25.0 -7.2     -61.3   120     4362   22 38 41

22 40 40  M82PTCEN     02 49 11  22.9  21.2 -7.1     -63.3   -12     4362   22 40 53
22 47 10  ---          02 55 43  23.5  21.5 -7.0     -64.7   378     4387   22 40 41

22 48 10  J0958+65     02 56 43  21.5  25.4 -7.1     -62.8    48     4387   22 48 10
22 50 40  ---          02 59 13  21.7  25.5 -7.0     -63.3   150     4396   22 48 11

22 58 40  3C84         03 07 14  78.7  13.1 -0.2    -164.8   361     4396   22 58 40
23 06 40  ---          03 15 16  79.0   5.5 -0.1    -173.7   480     4427   22 58 41

23 14 40  J0958+65     03 23 17  24.0  26.6 -6.6     -68.4   363     4427   23 14 40
23 16 40  ---          03 25 17  24.2  26.7 -6.6     -68.8   120     4435   23 14 41
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               High-resolution, multi-frequency mapping of the compact sources in M82
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon   7 Mar 2016   Day  67 ---

23 32 03  J0927+39     03 40 43  20.9  56.2 -5.8     -66.9   895     4435   23 32 03
23 38 03  ---          03 46 44  22.0  56.7 -5.7     -67.7   360     4458   23 32 04

23 46 03  J0958+65     03 54 45  27.1  27.8 -6.1     -75.1   451     4458   23 46 03
23 49 03  ---          03 57 46  27.4  27.9 -6.0     -75.7   180     4470   23 46 04

23 49 03  M82PTCEN     03 57 46  28.6  23.4 -6.0     -78.5   -11     4470   23 49 14
23 56 53  ---          04 05 37  29.2  23.5 -5.9     -80.2   459     4499   23 49 04

23 57 43  J0958+65     04 06 27  28.3  28.1 -5.9     -77.6    39     4499   23 57 43
23 59 58  ---          04 08 43  28.5  28.1 -5.9     -78.1   135     4508   23 57 44


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess116.L512glob
   Matching groups in /home/guest/rmc/SCHED/sched11.4/catalogs/freq_RDBE.dat:
     v20cm_2         FD filtered above 1760.  SC filtered above 1740.

   Setup group:    2         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 32.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00   2400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         L         L         L         L         L         L         L         L
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         L         L         L         L         L         L         L         L
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  14.6      2.4     14.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  11  Setup file default.  Used with PCAL = off
   LO sum=   1626.25  1626.25  1642.25  1642.25  1658.25  1658.25  1674.25  1674.25
   BBC fr=    773.75   773.75   757.75   757.75   741.75   741.75   725.75   725.75
   Bandwd=     16.00    16.00    16.00    16.00    16.00    16.00    16.00    16.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     757.75    757.75    741.75    741.75
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  11  12  13  14  15  16  17  18  19  20

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * M82PTCEN          09 51 42.970082   * 09 55 51.700000     09 57 13.357469       0.00
                     69 55 00.43524    * 69 40 46.70000      69 36 06.47889        0.00
                     From catalog imbedded in main SCHED input file.

 * 3C84              03 16 29.567263   * 03 19 48.160094     03 20 52.097105       1.30
   J0319+4130        41 19 51.91701    * 41 30 42.10413      41 34 08.62570        2.69
   0316+413          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
   J0319+41          GSFC 2015a astro solution, unpublished  10208 observations.

   4C39.25           09 23 55.319215   * 09 27 03.013936     09 28 04.588754       0.30
   J0927+3902        39 15 23.56645    * 39 02 20.85186      38 57 59.32276        0.16
   0923+392          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
 * J0927+39          GSFC 2015a astro solution, unpublished 245753 observations.

   0954+658          09 54 57.847923   * 09 58 47.245104     10 00 02.566321       0.02
   J0958+6533        65 48 15.53888    * 65 33 54.81807      65 29 11.75369        0.01
 * J0958+65          /home/guest/rmc/SCHED/sched11.4/catalogs/sources.gsfc
                     GSFC 2015a astro solution, unpublished  13811 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  M82PTCEN   sess116.L512glob      1 2 3 4 5 6 7 10 11 21           12.608  1956.566
  3C84       sess116.L512glob      1 2 3 4 5 6 7 10 11 21            0.400    46.931
  J0927+39   sess116.L512glob      1 2 3 4 5 6 7 10 11 21            0.300    33.997
  J0958+65   sess116.L512glob      1 2 3 4 5 6 7 10 11 21            6.971  1109.658


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   M82PTCEN           114.2
   3C84                72.9
   J0927+39           138.5
   J0958+65           118.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

