  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: GM038 18cm global observation of M82
 Exp. Code:  GM038   


Schedule Version:       1.70                                              
Processed by SCHED version: Release of 1 Dec. 1998                        

PI:       Andrew McDonald                                                 

Address:  Jodrell Bank Observatory                                        
          Macclesfield                                                    
          Cheshire, England                                               
                                                                          

Phone:    (+44) 1477 571321                                               
EMAIL:    amd@jb.man.ac.uk                                                
Fax:                                                                      
Phone during observation: (+44) 1477 571321                               

Observing mode: 128-4-2-UL                                                

Notes:    WSRT - use single antenna ONLY                                  
                                                                          
                                                                          
                                                                          

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

 ---------- Forward pass 1 ----------

 Next scan frequencies:  1659.49  1659.49  1667.49  1667.49
 Next BBC frequencies:    740.51   740.51   732.51   732.51
 Next scan bandwidths:      8.00     8.00     8.00     8.00

14 00 00  J0958+65     17 18 20  20.1 335.5  7.3      59.5     0   1  1      0
14 02 10  ---          17 20 31  19.9 335.6  7.4      59.0   130   F  1    867

14 02 10  M82          17 20 31  21.7 339.6  7.4      59.8    -6   1  1    867
14 06 20  ---          17 24 41  21.4 339.8  7.5      58.8   244   F  1   2533

14 06 20  J0958+65     17 24 41  19.5 335.9  7.4      58.2    -6   1  1   2533
14 08 30  ---          17 26 52  19.3 336.0  7.5      57.7   124   F  1   3400

14 08 30  M82          17 26 52  21.2 339.9  7.5      58.4    -6   1  1   3400
14 12 40  ---          17 31 02  20.9 340.1  7.6      57.5   244   F  1   5067

14 12 40  J0958+65     17 31 02  18.9 336.3  7.5      56.8    -6   1  1   5067
14 14 50  ---          17 33 13  18.8 336.4  7.6      56.4   124   F  1   5933

14 14 50  M82          17 33 13  20.8 340.2  7.6      57.0    -6   1  1   5933
14 19 00  ---          17 37 23  20.5 340.4  7.7      56.1   244   F  1   7600

14 19 00  J0958+65     17 37 23  18.4 336.6  7.6      55.5    -6   1  1   7600
14 21 10  ---          17 39 34  18.2 336.8  7.7      55.1   124   F  1   8467

14 21 10  M82          17 39 34  20.3 340.5  7.7      55.6    -6   1  1   8467
14 25 20  ---          17 43 44  20.0 340.8  7.8      54.7   244   F  1  10133

14 25 20  J0958+65     17 43 44  17.9 337.0  7.7      54.2    -6   1  1  10133
14 27 30  ---          17 45 55  17.7 337.2  7.8      53.7   124   F  1  11000

14 27 30  M82          17 45 55  19.9 340.9  7.8      54.3    -6   1  1  11000
14 31 40  ---          17 50 05  19.6 341.1  7.9      53.4   244   F  1  12667

14 31 40  J0958+65     17 50 05  17.3 337.5  7.9      52.9    -6   1  1  12667
14 33 50  ---          17 52 16  17.2 337.6  7.9      52.4   124   F  1  13533

14 33 50  M82          17 52 16  19.4 341.2  7.9      52.9    -7   1  1  13533
14 38 00  ---          17 56 26  19.1 341.5  8.0      52.0   243   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

14 38 00  J0958+65     17 56 26  16.8 337.9  8.0      51.6    -7   1  1  15200
14 40 00  ---          17 58 27  16.6 338.0  8.0      51.1   113   F  1  16000

14 40 00  M82          17 58 27  19.0 341.6  8.0      51.5    -7   1  1  16000
14 44 00  ---          18 02 27  18.7 341.8  8.1      50.7   233   F  1  17600

 ---------- Reverse pass 1 ----------

14 44 40  J0958+65     18 03 08  16.3 338.3  8.1      50.2    33   1  2  17600
14 46 50  ---          18 05 18  16.1 338.5  8.1      49.7   130   R  1  16733

14 46 50  M82          18 05 18  18.5 342.0  8.2      50.1    -7   1  2  16733
14 51 00  ---          18 09 29  18.3 342.2  8.2      49.2   243   R  1  15067

14 51 00  J0958+65     18 09 29  15.8 338.8  8.2      48.8    -7   1  2  15067
14 53 10  ---          18 11 39  15.6 338.9  8.2      48.4   123   R  1  14200

14 53 10  M82          18 11 39  18.1 342.3  8.3      48.7    -7   1  2  14200
14 57 20  ---          18 15 50  17.9 342.6  8.3      47.8   243   R  1  12533

14 57 20  J0958+65     18 15 50  15.3 339.2  8.3      47.5    -7   1  2  12533
14 59 30  ---          18 18 00  15.1 339.4  8.3      47.1   123   R  1  11667

14 59 30  M82          18 18 00  17.7 342.7  8.4      47.3    -7   1  2  11667
15 03 40  ---          18 22 11  17.4 343.0  8.4      46.4   243   R  1  10000

15 03 40  J0958+65     18 22 11  14.8 339.7  8.4      46.2    -7   1  2  10000
15 05 50  ---          18 24 21  14.6 339.9  8.4      45.7   123   R  1   9133

15 05 50  M82          18 24 21  17.3 343.1  8.5      46.0    -7   1  2   9133
15 10 00  ---          18 28 32  17.1 343.4  8.5      45.1   243   R  1   7467

15 10 00  J0958+65     18 28 32  14.3 340.2  8.5      44.9    -7   1  2   7467
15 12 10  ---          18 30 42  14.2 340.3  8.5      44.4   123   R  1   6600

15 12 10  M82          18 30 42  16.9 343.5  8.6      44.6    -7   1  2   6600
15 16 20  ---          18 34 53  16.7 343.8  8.6      43.7   243   R  1   4933

15 16 20  J0958+65     18 34 53  13.9 340.7  8.6      43.5    -8   1  2   4933
15 18 30  ---          18 37 03  13.7 340.8  8.6      43.1   122   R  1   4067

15 18 30  M82          18 37 03  16.5 344.0  8.7      43.2    -8   1  2   4067
15 22 40  ---          18 41 14  16.3 344.2  8.8      42.3   242   R  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

15 22 40  J0958+65     18 41 14  13.4 341.2  8.7      42.2    -8   1  2   2400
15 24 40  ---          18 43 14  13.3 341.3  8.7      41.8   112   R  1   1600

15 24 40  M82          18 43 14  16.2 344.4  8.8      41.9    -8   1  2   1600
15 28 40  ---          18 47 15  15.9 344.6  8.9      41.0   232   R  1      0

 ---------- Forward pass 2 ----------

15 30 40  J0958+65     18 49 15  12.9 341.8  8.8      40.5   112   1  3      0
15 32 50  ---          18 51 25  12.7 342.0  8.9      40.1   130   F  1    867

15 32 50  M82          18 51 25  15.7 344.9  8.9      40.1    -8   1  3    867
15 37 00  ---          18 55 36  15.5 345.2  9.0      39.2   242   F  1   2533

15 37 00  J0958+65     18 55 36  12.5 342.3  8.9      39.2    -8   1  3   2533
15 39 10  ---          18 57 46  12.3 342.5  9.0      38.7   122   F  1   3400

15 39 10  M82          18 57 46  15.4 345.4  9.0      38.8    -8   1  3   3400
15 43 20  ---          19 01 57  15.1 345.7  9.1      37.9   242   F  1   5067

15 43 20  J0958+65     19 01 57  12.1 342.8  9.1      37.9    -8   1  3   5067
15 45 30  ---          19 04 08  11.9 343.0  9.1      37.4   122   F  1   5933

15 45 30  M82          19 04 08  15.0 345.8  9.1      37.4    -8   1  3   5933
15 49 40  ---          19 08 18  14.8 346.1  9.2      36.5   242   F  1   7600

15 49 40  J0958+65     19 08 18  11.7 343.4  9.2      36.5    -8   1  3   7600
15 51 50  ---          19 10 29  11.5 343.6  9.2      36.1   122   F  1   8467

15 51 50  M82          19 10 29  14.7 346.3  9.2      36.0    -8   1  3   8467
15 56 00  ---          19 14 39  14.5 346.6  9.3      35.1   242   F  1  10133

15 56 00  J0958+65     19 14 39  11.3 343.9  9.3      35.2    -8   1  3  10133
15 58 10  ---          19 16 50  11.1 344.1  9.3      34.7   122   F  1  11000

15 58 10  M82          19 16 50  14.4 346.7  9.3      34.6    -8   1  3  11000
16 02 20  ---          19 21 00  14.2 347.0  9.4      33.7   242   F  1  12667

16 02 20  J0958+65     19 21 00  10.9 344.5  9.4      33.9    -9   1  3  12667
16 04 30  ---          19 23 11  10.8 344.7  9.4      33.4   121   F  1  13533

16 04 30  M82          19 23 11  14.1 347.2  9.5      33.3    -9   1  3  13533
16 08 40  ---          19 27 21  13.9 347.5  9.5      32.4   241   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

16 08 40  J0958+65     19 27 21  10.5 345.0  9.5      32.5    -9   1  3  15200
16 10 40  ---          19 29 22  10.4 345.2  9.5      32.1   111   F  1  16000

16 10 40  M82          19 29 22  13.8 347.7  9.6      31.9    -9   1  3  16000
16 14 40  ---          19 33 22  13.6 348.0  9.6      31.1   231   F  1  17600

 ---------- Reverse pass 2 ----------

16 15 20  J0958+65     19 34 02  10.2 345.6  9.6      31.1    31   1  4  17600
16 17 30  ---          19 36 13  10.1 345.8  9.6      30.6   130   R  1  16733

16 17 30  M82          19 36 13  13.5 348.2  9.7      30.4    -9   1  4  16733
16 21 40  ---          19 40 23  13.3 348.5  9.7      29.5   241   R  1  15067

16 21 40  J0958+65     19 40 23   9.8 346.2  9.7      29.8    -9   1  4  15067
16 23 50  ---          19 42 34   9.7 346.4  9.7      29.3   121   R  1  14200

16 23 50  M82          19 42 34  13.2 348.7  9.8      29.1    -9   1  4  14200
16 28 00  ---          19 46 45  13.0 349.0  9.8      28.2   241   R  1  12533

16 28 00  J0958+65     19 46 45   9.5 346.8  9.8      28.4    -9   1  4  12533
16 30 10  ---          19 48 55   9.4 347.0  9.8      27.9   121   R  1  11667

16 30 10  M82          19 48 55  12.9 349.2  9.9      27.7    -9   1  4  11667
16 34 20  ---          19 53 06  12.8 349.5 10.0      26.8   241   R  1  10000

16 34 20  J0958+65     19 53 06   9.2 347.4  9.9      27.1    -9   1  4  10000
16 36 30  ---          19 55 16   9.1 347.6  9.9      26.6   121   R  1   9133

16 36 30  M82          19 55 16  12.7 349.7 10.0      26.3    -9   1  4   9133
16 40 40  ---          19 59 27  12.5 350.0 10.1      25.4   241   R  1   7467

16 40 40  J0958+65     19 59 27   8.9 348.0 10.0      25.7    -9   1  4   7467
16 42 50  ---          20 01 37   8.8 348.2 10.0      25.2   121   R  1   6600

16 42 50  M82          20 01 37  12.4 350.2 10.1      24.9    -9   1  4   6600
16 47 00  ---          20 05 48  12.3 350.5 10.2      24.0   241   R  1   4933

16 47 00  J0958+65     20 05 48   8.7 348.6 10.1      24.3    -9   1  4   4933
16 49 10  ---          20 07 58   8.6 348.8 10.2      23.9   121   R  1   4067

16 49 10  M82          20 07 58  12.2 350.7 10.2      23.6    -9   1  4   4067
16 53 20  ---          20 12 09  12.1 351.1 10.3      22.7   241   R  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

16 53 20  J0958+65     20 12 09   8.4 349.2 10.2      23.0    -9   1  4   2400
16 55 20  ---          20 14 09   8.3 349.4 10.3      22.6   111   R  1   1600

16 55 20  M82          20 14 09  12.0 351.2 10.3      22.2    -9   1  4   1600
16 59 20  ---          20 18 10  11.9 351.6 10.4      21.3   231   R  1      0

 ---------- Forward pass 3 ----------

17 01 20  J0958+65     20 20 10   8.1 350.0 10.4      21.3   110   1  5      0
17 03 30  ---          20 22 20   8.0 350.2 10.4      20.8   130   F  1    867

17 03 30  M82          20 22 20  11.7 351.9 10.4      20.4   -10   1  5    867
17 07 40  ---          20 26 31  11.6 352.2 10.5      19.5   240   F  1   2533

17 07 40  J0958+65     20 26 31   7.8 350.6 10.5      19.9   -10   1  5   2533
17 09 50  ---          20 28 41   7.8 350.8 10.5      19.5   120   F  1   3400

17 09 50  M82          20 28 41  11.6 352.4 10.5      19.1   -10   1  5   3400
17 14 00  ---          20 32 52  11.4 352.8 10.6      18.1   240   F  1   5067

17 14 00  J0958+65     20 32 52   7.6 351.2 10.6      18.6   -10   1  5   5067
17 16 10  ---          20 35 02   7.6 351.4 10.6      18.1   120   F  1   5933

17 16 10  M82          20 35 02  11.4 353.0 10.7      17.7   -10   1  5   5933
17 20 20  ---          20 39 13  11.3 353.3 10.7      16.8   240   F  1   7600

17 20 20  J0958+65     20 39 13   7.4 351.8 10.7      17.2   -10   1  5   7600
17 22 30  ---          20 41 23   7.4 352.0 10.7      16.7   120   F  1   8467

17 22 30  M82          20 41 23  11.2 353.5 10.8      16.3   -10   1  5   8467
17 26 40  ---          20 45 34  11.1 353.9 10.8      15.4   240   F  1  10133

17 26 40  J0958+65     20 45 34   7.2 352.5 10.8      15.8   -10   1  5  10133
17 28 50  ---          20 47 45   7.2 352.7 10.8      15.4   120   F  1  11000

17 28 50  M82          20 47 45  11.1 354.0 10.9      14.9   -10   1  5  11000
17 33 00  ---          20 51 55  11.0 354.4 10.9      14.0   240   F  1  12667

17 33 00  J0958+65     20 51 55   7.1 353.1 10.9      14.5   -10   1  5  12667
17 35 10  ---          20 54 06   7.0 353.3 10.9      14.0   120   F  1  13533

17 35 10  M82          20 54 06  10.9 354.6 11.0      13.5   -10   1  5  13533
17 39 20  ---          20 58 16  10.9 354.9 11.0      12.6   240   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

17 39 20  J0958+65     20 58 16   6.9 353.7 11.0      13.1   -10   1  5  15200
17 41 20  ---          21 00 17   6.9 353.9 11.0      12.7   110   F  1  16000

17 41 20  M82          21 00 17  10.8 355.1 11.1      12.2   -10   1  5  16000
17 45 20  ---          21 04 17  10.8 355.5 11.1      11.3   230   F  1  17600

 ---------- Reverse pass 3 ----------

17 46 00  J0958+65     21 04 57   6.8 354.4 11.1      11.7    30   1  6  17600
17 48 10  ---          21 07 08   6.7 354.6 11.1      11.2   130   R  1  16733

17 48 10  M82          21 07 08  10.7 355.7 11.2      10.7   -10   1  6  16733
17 52 20  ---          21 11 18  10.6 356.1 11.3       9.8   240   R  1  15067

17 52 20  J0958+65     21 11 18   6.6 355.1 11.2      10.3   -10   1  6  15067
17 54 30  ---          21 13 29   6.6 355.3 11.2       9.8   120   R  1  14200

17 54 30  M82          21 13 29  10.6 356.3 11.3       9.3   -10   1  6  14200
17 58 40  ---          21 17 39  10.6 356.6 11.4       8.4   240   R  1  12533

17 58 40  J0958+65     21 17 39   6.5 355.7 11.3       8.9   -10   1  6  12533
18 00 50  ---          21 19 50   6.5 355.9 11.3       8.4   120   R  1  11667

18 00 50  M82          21 19 50  10.5 356.8 11.4       7.9   -10   1  6  11667
18 05 00  ---          21 24 00  10.5 357.2 11.5       7.0   240   R  1  10000

18 05 00  J0958+65     21 24 00   6.4 356.4 11.4       7.5   -10   1  6  10000
18 07 10  ---          21 26 11   6.4 356.6 11.5       7.1   120   R  1   9133

18 07 10  M82          21 26 11  10.5 357.4 11.5       6.5   -10   1  6   9133
18 11 20  ---          21 30 21  10.4 357.7 11.6       5.6   240   R  1   7467

18 11 20  J0958+65     21 30 21   6.4 357.0 11.5       6.2   -10   1  6   7467
18 13 30  ---          21 32 32   6.3 357.3 11.6       5.7   120   R  1   6600

18 13 30  M82          21 32 32  10.4 357.9 11.6       5.1   -10   1  6   6600
18 17 40  ---          21 36 43  10.4 358.3 11.7       4.2   240   R  1   4933

18 17 40  J0958+65     21 36 43   6.3 357.7 11.6       4.8   -10   1  6   4933
18 19 50  ---          21 38 53   6.3 357.9 11.7       4.3   120   R  1   4067

18 19 50  M82          21 38 53  10.4 358.5 11.7       3.7   -10   1  6   4067
18 24 00  ---          21 43 04  10.3 358.9 11.8       2.8   240   R  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

18 24 00  J0958+65     21 43 04   6.2 358.4 11.7       3.4   -10   1  6   2400
18 26 00  ---          21 45 04   6.2 358.6 11.8       3.0   110   R  1   1600

18 26 00  M82          21 45 04  10.3 359.0 11.8       2.4   -10   1  6   1600
18 30 00  ---          21 49 05  10.3 359.4 11.9       1.5   230   R  1      0

 ---------- Forward pass 4 ----------

18 32 00  J0958+65     21 51 05   6.2 359.2 11.9       1.7   110   1  7      0
18 34 10  ---          21 53 15   6.2 359.4 11.9       1.2   130   F  1    867

18 34 10  M82          21 53 15  10.3 359.8 12.0       0.6   -10   1  7    867
18 38 20  ---          21 57 26  10.3 360.1-12.0      -0.3   240   F  1   2533

18 38 20  J0958+65     21 57 26   6.2 359.8 12.0       0.3   -10   1  7   2533
18 40 30  ---          21 59 36   6.2 360.1-12.0      -0.2   120   F  1   3400

18 40 30  M82          21 59 36  10.3 360.3-11.9      -0.8   -10   1  7   3400
18 44 40  ---          22 03 47  10.3 360.7-11.9      -1.7   240   F  1   5067

18 44 40  J0958+65     22 03 47   6.2 360.5-11.9      -1.1   -10   1  7   5067
18 46 50  ---          22 05 57   6.2 360.7-11.9      -1.5   120   F  1   5933

18 46 50  M82          22 05 57  10.3 360.9-11.8      -2.2   -10   1  7   5933
18 51 00  ---          22 10 08  10.3 361.2-11.8      -3.1   240   F  1   7600

18 51 00  J0958+65     22 10 08   6.2 361.2-11.8      -2.4   -10   1  7   7600
18 53 10  ---          22 12 18   6.2 361.4-11.8      -2.9   120   F  1   8467

18 53 10  M82          22 12 18  10.4 361.4-11.7      -3.6   -10   1  7   8467
18 57 20  ---          22 16 29  10.4 361.8-11.7      -4.5   240   F  1  10133

18 57 20  J0958+65     22 16 29   6.3 361.8-11.7      -3.8   -10   1  7  10133
18 59 30  ---          22 18 39   6.3 362.1-11.7      -4.3   120   F  1  11000

18 59 30  M82          22 18 39  10.4 362.0-11.6      -5.0   -10   1  7  11000
19 03 40  ---          22 22 50  10.4 362.4-11.6      -5.9   240   F  1  12667

19 03 40  J0958+65     22 22 50   6.3 362.5-11.6      -5.2   -10   1  7  12667
19 05 50  ---          22 25 00   6.3 362.7-11.6      -5.6   120   F  1  13533

19 05 50  M82          22 25 00  10.4 362.6-11.5      -6.3   -10   1  7  13533
19 10 00  ---          22 29 11  10.5 362.9-11.4      -7.3   240   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

19 10 00  J0958+65     22 29 11   6.4 363.1-11.5      -6.6   -10   1  7  15200
19 12 00  ---          22 31 11   6.4 363.4-11.5      -7.0   110   F  1  16000

19 12 00  M82          22 31 11  10.5 363.1-11.4      -7.7   -10   1  7  16000
19 16 00  ---          22 35 12  10.6 363.5-11.3      -8.6   230   F  1  17600

 ---------- Reverse pass 4 ----------

19 16 40  J0958+65     22 35 52   6.5 363.8-11.4      -8.0    30   1  8  17600
19 18 50  ---          22 38 03   6.5 364.1-11.3      -8.5   130   R  1  16733

19 18 50  M82          22 38 03  10.6 363.7-11.3      -9.2   -10   1  8  16733
19 23 00  ---          22 42 13  10.7 364.1-11.2     -10.1   240   R  1  15067

19 23 00  J0958+65     22 42 13   6.6 364.5-11.3      -9.4   -10   1  8  15067
19 25 10  ---          22 44 24   6.6 364.7-11.2      -9.8   120   R  1  14200

19 25 10  M82          22 44 24  10.7 364.3-11.2     -10.6   -10   1  8  14200
19 29 20  ---          22 48 34  10.8 364.6-11.1     -11.5   240   R  1  12533

19 29 20  J0958+65     22 48 34   6.7 365.1-11.2     -10.7   -10   1  8  12533
19 31 30  ---          22 50 45   6.7 365.4-11.1     -11.2   120   R  1  11667

19 31 30  M82          22 50 45  10.8 364.8-11.1     -12.0   -10   1  8  11667
19 35 40  ---          22 54 55  10.9 365.2-11.0     -12.9   240   R  1  10000

19 35 40  J0958+65     22 54 55   6.8 365.8-11.1     -12.1   -10   1  8  10000
19 37 50  ---          22 57 06   6.9 366.0-11.0     -12.6   120   R  1   9133

19 37 50  M82          22 57 06  10.9 365.3-11.0     -13.4   -10   1  8   9133
19 42 00  ---          23 01 16  11.0 365.7-10.9     -14.3   240   R  1   7467

19 42 00  J0958+65     23 01 16   7.0 366.4-11.0     -13.5   -10   1  8   7467
19 44 10  ---          23 03 27   7.0 366.7-10.9     -13.9   120   R  1   6600

19 44 10  M82          23 03 27  11.1 365.9-10.9     -14.7   -10   1  8   6600
19 48 20  ---          23 07 37  11.2 366.3-10.8     -15.6   240   R  1   4933

19 48 20  J0958+65     23 07 37   7.1 367.1-10.9     -14.8   -10   1  8   4933
19 50 30  ---          23 09 48   7.2 367.3-10.8     -15.3   120   R  1   4067

19 50 30  M82          23 09 48  11.2 366.4-10.8     -16.1   -10   1  8   4067
19 54 40  ---          23 13 58  11.3 366.8-10.7     -17.0   240   R  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

19 54 40  J0958+65     23 13 58   7.3 367.7-10.7     -16.2   -10   1  8   2400
19 56 40  ---          23 15 59   7.3 367.9-10.7     -16.6   110   R  1   1600

19 56 40  M82          23 15 59  11.4 367.0-10.7     -17.5   -10   1  8   1600
20 00 40  ---          23 19 59  11.5 367.3-10.6     -18.3   230   R  1      0

 ---------- Forward pass 5 ----------

20 02 40  J0958+65     23 22 00   7.5 368.5-10.6     -17.9   110   1  9      0
20 04 50  ---          23 24 10   7.6 368.7-10.6     -18.4   130   F  1    867

20 04 50  M82          23 24 10  11.6 367.6-10.5     -19.3   -10   1  9    867
20 09 00  ---          23 28 21  11.7 368.0-10.5     -20.2   240   F  1   2533

20 09 00  J0958+65     23 28 21   7.7 369.1-10.5     -19.3   -10   1  9   2533
20 11 10  ---          23 30 31   7.8 369.4-10.5     -19.8   120   F  1   3400

20 11 10  M82          23 30 31  11.8 368.2-10.4     -20.6   -10   1  9   3400
20 15 20  ---          23 34 42  11.9 368.5-10.4     -21.5   240   F  1   5067

20 15 20  J0958+65     23 34 42   8.0 369.8-10.4     -20.7   -10   1  9   5067
20 17 30  ---          23 36 52   8.0 370.0-10.4     -21.1   120   F  1   5933

20 17 30  M82          23 36 52  12.0 368.7-10.3     -22.0   -10   1  9   5933
20 21 40  ---          23 41 03  12.1 369.0-10.2     -22.9   240   F  1   7600

20 21 40  J0958+65     23 41 03   8.2 370.4-10.3     -22.0   -10   1  9   7600
20 23 50  ---          23 43 13   8.3 370.6-10.3     -22.5   120   F  1   8467

20 23 50  M82          23 43 13  12.2 369.2-10.2     -23.4   -10   1  9   8467
20 28 00  ---          23 47 24  12.3 369.6-10.1     -24.3   240   F  1  10133

20 28 00  J0958+65     23 47 24   8.5 371.0-10.2     -23.4   -10   1  9  10133
20 30 10  ---          23 49 34   8.5 371.2-10.2     -23.8   120   F  1  11000

20 30 10  M82          23 49 34  12.4 369.7-10.1     -24.8   -10   1  9  11000
20 34 20  ---          23 53 45  12.6 370.1-10.0     -25.7   240   F  1  12667

20 34 20  J0958+65     23 53 45   8.7 371.6-10.1     -24.7   -10   1  9  12667
20 36 30  ---          23 55 55   8.8 371.8-10.0     -25.2   120   F  1  13533

20 36 30  M82          23 55 55  12.6 370.2-10.0     -26.2   -10   1  9  13533
20 40 40  ---          00 00 06  12.8 370.6 -9.9     -27.1   240   F  1  15200
Schedule for VLBA_FD   (Code Fd )                                   Page  11
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

20 40 40  J0958+65     00 00 06   9.0 372.2-10.0     -26.1   -10   1  9  15200
20 42 40  ---          00 02 06   9.1 372.4 -9.9     -26.5   110   F  1  16000

20 42 40  M82          00 02 06  12.9 370.7 -9.9     -27.5   -10   1  9  16000
20 46 40  ---          00 06 07  13.1 371.1 -9.8     -28.4   230   F  1  17600

 ---------- Reverse pass 5 ----------

20 47 20  J0958+65     00 06 47   9.3 372.8 -9.9     -27.5    31   1 10  17600
20 49 30  ---          00 08 57   9.4 373.0 -9.8     -28.0   130   R  1  16733

20 49 30  M82          00 08 57  13.2 371.3 -9.8     -29.0    -9   1 10  16733
20 53 40  ---          00 13 08  13.4 371.6 -9.7     -29.9   241   R  1  15067

20 53 40  J0958+65     00 13 08   9.6 373.4 -9.8     -28.8    -9   1 10  15067
20 55 50  ---          00 15 19   9.7 373.6 -9.7     -29.3   121   R  1  14200

20 55 50  M82          00 15 19  13.4 371.8 -9.7     -30.4    -9   1 10  14200
21 00 00  ---          00 19 29  13.6 372.1 -9.6     -31.3   241   R  1  12533

21 00 00  J0958+65     00 19 29  10.0 374.0 -9.7     -30.2    -9   1 10  12533
21 02 10  ---          00 21 40  10.1 374.2 -9.6     -30.7   121   R  1  11667

21 02 10  M82          00 21 40  13.7 372.3 -9.6     -31.7    -9   1 10  11667
21 06 20  ---          00 25 50  13.9 372.6 -9.5     -32.6   241   R  1  10000

21 06 20  J0958+65     00 25 50  10.3 374.6 -9.6     -31.5    -9   1 10  10000
21 08 30  ---          00 28 01  10.4 374.8 -9.5     -32.0   121   R  1   9133

21 08 30  M82          00 28 01  14.0 372.7 -9.5     -33.1    -9   1 10   9133
21 12 40  ---          00 32 11  14.2 373.0 -9.4     -34.0   241   R  1   7467

21 12 40  J0958+65     00 32 11  10.6 375.1 -9.4     -32.9    -9   1 10   7467
21 14 50  ---          00 34 22  10.8 375.3 -9.4     -33.3   121   R  1   6600

21 14 50  M82          00 34 22  14.3 373.2 -9.4     -34.5    -9   1 10   6600
21 19 00  ---          00 38 32  14.5 373.5 -9.3     -35.4   241   R  1   4933

21 19 00  J0958+65     00 38 32  11.0 375.7 -9.3     -34.2    -9   1 10   4933
21 21 10  ---          00 40 43  11.1 375.9 -9.3     -34.7   121   R  1   4067

21 21 10  M82          00 40 43  14.6 373.7 -9.3     -35.8    -9   1 10   4067
21 25 20  ---          00 44 53  14.9 374.0 -9.2     -36.7   241   R  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page  12
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

21 25 20  J0958+65     00 44 53  11.4 376.2 -9.2     -35.6    -9   1 10   2400
21 27 20  ---          00 46 54  11.5 376.4 -9.2     -36.0   111   R  1   1600

21 27 20  M82          00 46 54  15.0 374.1 -9.2     -37.2    -9   1 10   1600
21 31 20  ---          00 50 54  15.2 374.4 -9.1     -38.0   231   R  1      0

 ---------- Forward pass 6 ----------

21 33 20  J0958+65     00 52 55  11.9 376.9 -9.1     -37.2   111   1 11      0
21 35 20  ---          00 54 55  12.0 377.1 -9.1     -37.7   120   F  1    800

21 35 20  M82          00 54 55  15.4 374.7 -9.0     -38.9    -9   1 11    800
21 39 20  ---          00 58 56  15.6 375.0 -9.0     -39.8   231   F  1   2400

21 39 20  J0958+65     00 58 56  12.3 377.4 -9.0     -38.5    -9   1 11   2400
21 41 20  ---          01 00 56  12.4 377.6 -9.0     -38.9   111   F  1   3200

21 41 20  M82          01 00 56  15.7 375.1 -8.9     -40.2    -9   1 11   3200
21 45 20  ---          01 04 57  16.0 375.4 -8.9     -41.1   231   F  1   4800

21 45 20  J0958+65     01 04 57  12.6 377.9 -8.9     -39.8    -9   1 11   4800
21 47 20  ---          01 06 57  12.8 378.1 -8.9     -40.2   111   F  1   5600

21 47 20  M82          01 06 57  16.1 375.5 -8.8     -41.5    -9   1 11   5600
21 51 20  ---          01 10 58  16.3 375.8 -8.8     -42.4   231   F  1   7200

21 51 20  J0958+65     01 10 58  13.0 378.4 -8.8     -41.0    -9   1 11   7200
21 53 20  ---          01 12 58  13.2 378.6 -8.8     -41.5   111   F  1   8000

21 53 20  M82          01 12 58  16.4 375.9 -8.7     -42.8    -8   1 11   8000
21 57 20  ---          01 16 59  16.7 376.2 -8.6     -43.7   232   F  1   9600

21 57 20  J0958+65     01 16 59  13.5 378.9 -8.7     -42.3    -8   1 11   9600
21 59 20  ---          01 18 59  13.6 379.0 -8.7     -42.7   112   F  1  10400

21 59 20  M82          01 18 59  16.8 376.3 -8.6     -44.1    -8   1 11  10400
22 03 20  ---          01 23 00  17.0 376.6 -8.5     -45.0   232   F  1  12000

22 03 20  J0958+65     01 23 00  13.9 379.3 -8.6     -43.6    -8   1 11  12000
22 05 20  ---          01 25 00  14.0 379.5 -8.6     -44.0   112   F  1  12800

22 05 20  M82          01 25 00  17.2 376.7 -8.5     -45.4    -8   1 11  12800
22 09 20  ---          01 29 01  17.4 377.0 -8.4     -46.3   232   F  1  14400
Schedule for VLBA_FD   (Code Fd )                                   Page  13
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

22 09 20  J0958+65     01 29 01  14.3 379.8 -8.5     -44.8    -8   1 11  14400
22 11 20  ---          01 31 01  14.5 380.0 -8.5     -45.2   112   F  1  15200

22 22 20  3C84         01 42 03  67.6 414.3 -1.6    -111.1   552   1 11  15200
22 28 20  ---          01 48 04  68.6 413.1 -1.5    -113.2   360   F  1  17600

 ---------- Reverse pass 6 ----------

22 39 20  J0958+65     01 59 06  16.6 382.0 -8.0     -51.1   554   1 12  17600
22 41 30  ---          02 01 16  16.8 382.1 -8.0     -51.5   130   R  1  16733

22 41 30  M82          02 01 16  19.5 378.9 -7.9     -53.2    -7   1 12  16733
22 45 40  ---          02 05 27  19.8 379.1 -7.8     -54.1   243   R  1  15067

22 45 40  J0958+65     02 05 27  17.1 382.4 -7.9     -52.4    -7   1 12  15067
22 47 50  ---          02 07 37  17.3 382.5 -7.9     -52.9   123   R  1  14200

22 47 50  M82          02 07 37  20.0 379.2 -7.8     -54.6    -7   1 12  14200
22 52 00  ---          02 11 48  20.3 379.4 -7.7     -55.5   243   R  1  12533

22 52 00  J0958+65     02 11 48  17.7 382.8 -7.8     -53.7    -7   1 12  12533
22 54 10  ---          02 13 58  17.9 382.9 -7.7     -54.2   123   R  1  11667

22 54 10  M82          02 13 58  20.4 379.5 -7.7     -56.0    -7   1 12  11667
22 58 20  ---          02 18 09  20.7 379.8 -7.6     -56.9   243   R  1  10000

22 58 20  J0958+65     02 18 09  18.2 383.2 -7.7     -55.0    -7   1 12  10000
23 00 30  ---          02 20 19  18.4 383.3 -7.6     -55.5   123   R  1   9133

23 00 30  M82          02 20 19  20.9 379.9 -7.6     -57.3    -7   1 12   9133
23 04 40  ---          02 24 30  21.2 380.1 -7.5     -58.3   243   R  1   7467

23 04 40  J0958+65     02 24 30  18.7 383.6 -7.6     -56.4    -7   1 12   7467
23 06 50  ---          02 26 40  18.9 383.7 -7.5     -56.8   123   R  1   6600

23 06 50  M82          02 26 40  21.4 380.2 -7.5     -58.7    -7   1 12   6600
23 11 00  ---          02 30 51  21.7 380.4 -7.4     -59.6   243   R  1   4933

23 11 00  J0958+65     02 30 51  19.3 384.0 -7.5     -57.7    -7   1 12   4933
23 13 10  ---          02 33 01  19.5 384.1 -7.4     -58.1   123   R  1   4067

23 13 10  M82          02 33 01  21.8 380.5 -7.4     -60.1    -7   1 12   4067
23 17 20  ---          02 37 12  22.2 380.7 -7.3     -61.0   243   R  1   2400
Schedule for VLBA_FD   (Code Fd )                                   Page  14
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Fri  23 Feb 2001   Day  54 ---

23 17 20  J0958+65     02 37 12  19.9 384.3 -7.4     -59.0    -7   1 12   2400
23 19 20  ---          02 39 12  20.0 384.5 -7.3     -59.4   113   R  1   1600

23 19 20  M82          02 39 12  22.3 380.8 -7.3     -61.4    -7   1 12   1600
23 23 20  ---          02 43 13  22.6 380.9 -7.2     -62.3   233   R  1      0

 ---------- Forward pass 7 ----------

23 25 20  J0958+65     02 45 13  20.6 384.8 -7.2     -60.7   114   1 13      0
23 27 30  ---          02 47 23  20.8 384.9 -7.2     -61.1   130   F  1    867

23 27 30  M82          02 47 23  22.9 381.1 -7.1     -63.2    -6   1 13    867
23 31 40  ---          02 51 34  23.3 381.3 -7.1     -64.1   244   F  1   2533

23 31 40  J0958+65     02 51 34  21.2 385.1 -7.1     -62.0    -6   1 13   2533
23 33 50  ---          02 53 44  21.3 385.2 -7.1     -62.5   124   F  1   3400

23 33 50  M82          02 53 44  23.4 381.4 -7.0     -64.6    -6   1 13   3400
23 38 00  ---          02 57 55  23.8 381.6 -7.0     -65.5   244   F  1   5067

23 38 00  J0958+65     02 57 55  21.7 385.5 -7.0     -63.3    -6   1 13   5067
23 40 10  ---          03 00 06  21.9 385.6 -7.0     -63.8   124   F  1   5933

23 40 10  M82          03 00 06  23.9 381.6 -6.9     -66.0    -6   1 13   5933
23 44 20  ---          03 04 16  24.3 381.8 -6.9     -66.9   244   F  1   7600

23 44 20  J0958+65     03 04 16  22.3 385.8 -6.9     -64.7    -6   1 13   7600
23 46 30  ---          03 06 27  22.5 385.9 -6.9     -65.1   124   F  1   8467

23 46 30  M82          03 06 27  24.4 381.9 -6.8     -67.4    -6   1 13   8467
23 50 40  ---          03 10 37  24.8 382.0 -6.8     -68.3   244   F  1  10133

23 50 40  J0958+65     03 10 37  22.9 386.1 -6.8     -66.0    -6   1 13  10133
23 52 50  ---          03 12 48  23.1 386.2 -6.8     -66.5   124   F  1  11000

23 52 50  M82          03 12 48  25.0 382.1 -6.7     -68.8    -6   1 13  11000
23 57 00  ---          03 16 58  25.3 382.2 -6.7     -69.7   244   F  1  12667

23 57 00  J0958+65     03 16 58  23.5 386.3 -6.7     -67.3    -6   1 13  12667
23 59 10  ---          03 19 09  23.7 386.4 -6.7     -67.8   124   F  1  13533

23 59 10  M82          03 19 09  25.5 382.3 -6.6     -70.2    -5   1 13  13533
23 59 59  ---          03 19 59  25.5 382.3 -6.6     -70.4    44   F  1  13867
Schedule for VLBA_FD   (Code Fd )                                   Page  15
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

00 00 00  M82          03 19 59  25.5 382.3 -6.6     -70.4    -2   1 13  13867
00 03 20  ---          03 23 19  25.8 382.5 -6.5     -71.1   198   F  1  15200

00 03 20  J0958+65     03 23 19  24.1 386.6 -6.6     -68.7    -5   1 13  15200
00 05 20  ---          03 25 20  24.3 386.7 -6.6     -69.1   115   F  1  16000

00 05 20  M82          03 25 20  26.0 382.5 -6.5     -71.5    -5   1 13  16000
00 09 20  ---          03 29 20  26.3 382.6 -6.4     -72.4   235   F  1  17600

 ---------- Reverse pass 7 ----------

00 10 00  J0958+65     03 30 00  24.8 386.9 -6.5     -70.1    35   1 14  17600
00 12 00  ---          03 32 01  25.0 387.0 -6.4     -70.5   120   R  1  16800

00 12 00  M82          03 32 01  26.5 382.7 -6.4     -73.0    -5   1 14  16800
00 16 00  ---          03 36 01  26.9 382.8 -6.3     -73.9   235   R  1  15200

00 16 00  J0958+65     03 36 01  25.4 387.1 -6.4     -71.4    -5   1 14  15200
00 18 00  ---          03 38 02  25.6 387.2 -6.3     -71.8   115   R  1  14400

00 18 00  M82          03 38 02  27.0 382.9 -6.3     -74.4    -5   1 14  14400
00 22 00  ---          03 42 02  27.4 383.0 -6.2     -75.3   235   R  1  12800

00 22 00  J0958+65     03 42 02  26.0 387.3 -6.3     -72.6    -5   1 14  12800
00 24 00  ---          03 44 03  26.2 387.4 -6.2     -73.1   115   R  1  12000

00 24 00  M82          03 44 03  27.5 383.0 -6.2     -75.7    -5   1 14  12000
00 28 00  ---          03 48 03  27.9 383.1 -6.1     -76.6   235   R  1  10400

00 28 00  J0958+65     03 48 03  26.6 387.5 -6.2     -73.9    -5   1 14  10400
00 30 00  ---          03 50 04  26.8 387.6 -6.1     -74.3   115   R  1   9600

00 30 00  M82          03 50 04  28.0 383.2 -6.1     -77.0    -5   1 14   9600
00 34 00  ---          03 54 04  28.4 383.3 -6.0     -77.9   235   R  1   8000

00 34 00  J0958+65     03 54 04  27.2 387.7 -6.1     -75.2    -5   1 14   8000
00 36 00  ---          03 56 05  27.4 387.8 -6.0     -75.6   115   R  1   7200

00 36 00  M82          03 56 05  28.6 383.3 -6.0     -78.4    -5   1 14   7200
00 40 00  ---          04 00 05  28.9 383.4 -5.9     -79.3   235   R  1   5600

00 40 00  J0958+65     04 00 05  27.8 387.9 -6.0     -76.5    -5   1 14   5600
00 42 00  ---          04 02 06  28.0 387.9 -5.9     -76.9   115   R  1   4800
Schedule for VLBA_FD   (Code Fd )                                   Page  16
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

00 42 00  M82          04 02 06  29.1 383.4 -5.9     -79.8    -5   1 14   4800
00 46 00  ---          04 06 06  29.4 383.5 -5.8     -80.7   235   R  1   3200

00 46 00  J0958+65     04 06 06  28.4 388.0 -5.9     -77.8    -5   1 14   3200
00 48 00  ---          04 08 07  28.6 388.1 -5.8     -78.2   115   R  1   2400

00 48 00  M82          04 08 07  29.6 383.5 -5.8     -81.1    -5   1 14   2400
00 52 00  ---          04 12 07  29.9 383.6 -5.7     -82.0   235   R  1    800

00 52 00  J0958+65     04 12 07  29.0 388.2 -5.8     -79.1    -5   1 14    800
00 54 00  ---          04 14 08  29.2 388.2 -5.7     -79.5   115   R  1      0

 ---------- Forward pass 1 ----------

-----------  Tape Change ------------

01 09 00  J0958+65     04 29 10  30.7 388.5 -5.5     -82.8   895   2  1      0
01 11 10  ---          04 31 20  30.9 388.5 -5.5     -83.3   130   F  1    867

01 11 10  M82          04 31 20  31.6 383.8 -5.4     -86.4    -5   2  1    867
01 15 20  ---          04 35 31  31.9 383.8 -5.3     -87.4   245   F  1   2533

01 15 20  J0958+65     04 35 31  31.4 388.6 -5.4     -84.2    -5   2  1   2533
01 17 30  ---          04 37 41  31.6 388.6 -5.4     -84.7   125   F  1   3400

01 17 30  M82          04 37 41  32.1 383.8 -5.3     -87.9    -5   2  1   3400
01 21 40  ---          04 41 52  32.5 383.8 -5.2     -88.9   245   F  1   5067

01 21 40  J0958+65     04 41 52  32.0 388.6 -5.3     -85.6    -5   2  1   5067
01 23 50  ---          04 44 03  32.2 388.7 -5.2     -86.1   125   F  1   5933

01 23 50  M82          04 44 03  32.7 383.8 -5.2     -89.4    -5   2  1   5933
01 28 00  ---          04 48 13  33.1 383.8 -5.1     -90.4   245   F  1   7600

01 28 00  J0958+65     04 48 13  32.7 388.7 -5.2     -87.0    -5   2  1   7600
01 30 00  ---          04 50 14  32.9 388.7 -5.1     -87.5   115   F  1   8400

01 30 00  M82          04 50 14  33.2 383.8 -5.1     -90.8    -5   2  1   8400
01 34 20  ---          04 54 34  33.6 383.8 -5.0     -91.9   255   F  1  10133

01 34 20  J0958+65     04 54 34  33.3 388.7 -5.1     -88.5    -5   2  1  10133
01 36 30  ---          04 56 45  33.6 388.7 -5.0     -89.0   125   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  17
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

01 36 30  M82          04 56 45  33.8 383.8 -5.0     -92.4    -5   2  1  11000
01 40 40  ---          05 00 55  34.2 383.8 -4.9     -93.4   245   F  1  12667

01 40 40  J0958+65     05 00 55  34.0 388.7 -5.0     -89.9    -5   2  1  12667
01 42 50  ---          05 03 06  34.2 388.7 -4.9     -90.4   125   F  1  13533

01 42 50  M82          05 03 06  34.3 383.8 -4.9     -93.9    -5   2  1  13533
01 47 00  ---          05 07 16  34.7 383.7 -4.8     -94.9   245   F  1  15200

01 47 00  J0958+65     05 07 16  34.6 388.7 -4.9     -91.4    -5   2  1  15200
01 49 00  ---          05 09 17  34.9 388.7 -4.8     -91.8   115   F  1  16000

01 49 00  M82          05 09 17  34.9 383.7 -4.8     -95.4    -5   2  1  16000
01 53 00  ---          05 13 17  35.2 383.7 -4.7     -96.3   235   F  1  17600

 ---------- Reverse pass 1 ----------

01 53 40  J0958+65     05 13 57  35.3 388.7 -4.7     -92.9    35   2  2  17600
01 55 50  ---          05 16 08  35.6 388.7 -4.7     -93.4   130   R  1  16733

01 55 50  M82          05 16 08  35.5 383.6 -4.7     -97.0    -5   2  2  16733
02 00 00  ---          05 20 18  35.8 383.6 -4.6     -98.0   245   R  1  15067

02 00 00  J0958+65     05 20 18  36.0 388.6 -4.6     -94.4    -5   2  2  15067
02 02 10  ---          05 22 29  36.2 388.6 -4.6     -94.9   125   R  1  14200

02 02 10  M82          05 22 29  36.0 383.5 -4.6     -98.6    -5   2  2  14200
02 06 20  ---          05 26 40  36.4 383.5 -4.5     -99.6   245   R  1  12533

02 06 20  J0958+65     05 26 40  36.6 388.6 -4.5     -95.9    -5   2  2  12533
02 08 30  ---          05 28 50  36.9 388.5 -4.5     -96.4   125   R  1  11667

02 08 30  M82          05 28 50  36.6 383.4 -4.5    -100.1    -5   2  2  11667
02 12 40  ---          05 33 01  36.9 383.3 -4.4    -101.1   245   R  1  10000

02 12 40  J0958+65     05 33 01  37.3 388.5 -4.4     -97.4    -5   2  2  10000
02 14 50  ---          05 35 11  37.5 388.4 -4.4     -97.9   125   R  1   9133

02 14 50  M82          05 35 11  37.1 383.3 -4.3    -101.7    -5   2  2   9133
02 19 00  ---          05 39 22  37.5 383.2 -4.3    -102.7   245   R  1   7467

02 19 00  J0958+65     05 39 22  38.0 388.4 -4.3     -98.9    -5   2  2   7467
02 21 10  ---          05 41 32  38.2 388.3 -4.3     -99.4   125   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page  18
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

02 21 10  M82          05 41 32  37.6 383.1 -4.2    -103.3    -5   2  2   6600
02 25 20  ---          05 45 43  38.0 383.0 -4.2    -104.3   245   R  1   4933

02 25 20  J0958+65     05 45 43  38.6 388.2 -4.2    -100.4    -5   2  2   4933
02 27 30  ---          05 47 53  38.8 388.2 -4.2    -100.9   125   R  1   4067

02 27 30  M82          05 47 53  38.2 383.0 -4.1    -104.9    -5   2  2   4067
02 31 40  ---          05 52 04  38.5 382.8 -4.1    -105.9   245   R  1   2400

02 31 40  J0958+65     05 52 04  39.2 388.1 -4.1    -102.0    -5   2  2   2400
02 33 40  ---          05 54 04  39.4 388.0 -4.1    -102.4   115   R  1   1600

02 33 40  M82          05 54 04  38.7 382.8 -4.0    -106.4    -5   2  2   1600
02 37 40  ---          05 58 05  39.0 382.7 -4.0    -107.4   235   R  1      0

 ---------- Forward pass 2 ----------

02 39 40  J0958+65     06 00 05  40.1 387.8 -4.0    -103.9   115   2  3      0
02 41 50  ---          06 02 15  40.3 387.7 -3.9    -104.5   130   F  1    867

02 41 50  M82          06 02 15  39.4 382.5 -3.9    -108.5    -5   2  3    867
02 46 00  ---          06 06 26  39.7 382.4 -3.8    -109.6   245   F  1   2533

02 46 00  J0958+65     06 06 26  40.7 387.6 -3.9    -105.5    -5   2  3   2533
02 48 10  ---          06 08 36  40.9 387.5 -3.8    -106.1   125   F  1   3400

02 48 10  M82          06 08 36  39.9 382.3 -3.8    -110.2    -5   2  3   3400
02 52 20  ---          06 12 47  40.2 382.1 -3.7    -111.2   245   F  1   5067

02 52 20  J0958+65     06 12 47  41.3 387.4 -3.8    -107.1    -6   2  3   5067
02 54 30  ---          06 14 57  41.5 387.3 -3.7    -107.7   124   F  1   5933

02 54 30  M82          06 14 57  40.4 382.0 -3.7    -111.8    -6   2  3   5933
02 58 40  ---          06 19 08  40.7 381.8 -3.6    -112.9   244   F  1   7600

02 58 40  J0958+65     06 19 08  41.9 387.1 -3.7    -108.8    -6   2  3   7600
03 00 50  ---          06 21 18  42.2 387.0 -3.6    -109.3   124   F  1   8467

03 00 50  M82          06 21 18  40.9 381.7 -3.6    -113.5    -6   2  3   8467
03 05 00  ---          06 25 29  41.2 381.5 -3.5    -114.6   244   F  1  10133

03 05 00  J0958+65     06 25 29  42.6 386.8 -3.6    -110.4    -6   2  3  10133
03 07 10  ---          06 27 40  42.8 386.7 -3.5    -111.0   124   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  19
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

03 07 10  M82          06 27 40  41.4 381.4 -3.5    -115.2    -5   2  3  11000
03 11 20  ---          06 31 50  41.7 381.2 -3.4    -116.3   245   F  1  12667

03 11 20  J0958+65     06 31 50  43.2 386.5 -3.5    -112.1    -5   2  3  12667
03 13 30  ---          06 34 01  43.4 386.3 -3.4    -112.6   125   F  1  13533

03 13 30  M82          06 34 01  41.9 381.1 -3.4    -116.9    -5   2  3  13533
03 17 40  ---          06 38 11  42.2 380.9 -3.3    -118.0   245   F  1  15200

03 17 40  J0958+65     06 38 11  43.8 386.1 -3.3    -113.8    -5   2  3  15200
03 19 40  ---          06 40 12  44.0 386.0 -3.3    -114.3   115   F  1  16000

03 19 40  M82          06 40 12  42.4 380.8 -3.3    -118.5    -5   2  3  16000
03 23 40  ---          06 44 12  42.7 380.5 -3.2    -119.6   235   F  1  17600

 ---------- Reverse pass 2 ----------

03 24 20  J0958+65     06 44 52  44.4 385.7 -3.2    -115.6    35   2  4  17600
03 26 20  ---          06 46 53  44.6 385.6 -3.2    -116.1   120   R  1  16800

03 26 20  M82          06 46 53  42.9 380.4 -3.2    -120.4    -5   2  4  16800
03 30 20  ---          06 50 53  43.2 380.1 -3.1    -121.5   235   R  1  15200

03 30 20  J0958+65     06 50 53  45.0 385.3 -3.1    -117.2    -6   2  4  15200
03 32 20  ---          06 52 54  45.1 385.2 -3.1    -117.7   114   R  1  14400

03 32 20  M82          06 52 54  43.3 380.0 -3.1    -122.0    -6   2  4  14400
03 36 20  ---          06 56 54  43.6 379.8 -3.0    -123.2   234   R  1  12800

03 36 20  J0958+65     06 56 54  45.5 384.9 -3.0    -118.9    -6   2  4  12800
03 38 20  ---          06 58 55  45.7 384.8 -3.0    -119.4   114   R  1  12000

03 38 20  M82          06 58 55  43.8 379.6 -3.0    -123.7    -6   2  4  12000
03 42 20  ---          07 02 55  44.1 379.3 -2.9    -124.8   234   R  1  10400

03 42 20  J0958+65     07 02 55  46.1 384.5 -2.9    -120.5    -6   2  4  10400
03 44 20  ---          07 04 56  46.2 384.3 -2.9    -121.1   114   R  1   9600

03 44 20  M82          07 04 56  44.2 379.2 -2.9    -125.4    -6   2  4   9600
03 48 20  ---          07 08 56  44.5 378.9 -2.8    -126.6   234   R  1   8000

03 48 20  J0958+65     07 08 56  46.6 384.0 -2.8    -122.3    -6   2  4   8000
03 50 20  ---          07 10 57  46.8 383.8 -2.8    -122.8   114   R  1   7200
Schedule for VLBA_FD   (Code Fd )                                   Page  20
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

03 50 20  M82          07 10 57  44.6 378.8 -2.8    -127.1    -6   2  4   7200
03 54 20  ---          07 14 57  44.9 378.5 -2.7    -128.3   234   R  1   5600

03 54 20  J0958+65     07 14 57  47.1 383.5 -2.7    -124.0    -6   2  4   5600
03 56 20  ---          07 16 58  47.3 383.3 -2.7    -124.6   114   R  1   4800

03 56 20  M82          07 16 58  45.0 378.3 -2.7    -128.9    -6   2  4   4800
04 00 20  ---          07 20 58  45.3 378.0 -2.6    -130.0   234   R  1   3200

04 00 20  J0958+65     07 20 58  47.6 383.0 -2.6    -125.7    -7   2  4   3200
04 02 20  ---          07 22 59  47.8 382.8 -2.6    -126.3   113   R  1   2400

04 06 20  J0927+39     07 26 59  64.1 422.9 -2.0     -99.7   205   2  4   2400
04 12 20  ---          07 33 00  65.2 422.4 -1.9    -101.1   360   R  1      0

 ---------- Forward pass 3 ----------

04 16 20  J0958+65     07 37 01  48.9 381.4 -2.4    -130.5   205   2  5      0
04 18 30  ---          07 39 11  49.1 381.2 -2.3    -131.2   130   F  1    867

04 18 30  M82          07 39 11  46.5 376.5 -2.3    -135.4    -7   2  5    867
04 22 40  ---          07 43 22  46.7 376.1 -2.2    -136.7   243   F  1   2533

04 22 40  J0958+65     07 43 22  49.4 380.8 -2.3    -132.5    -7   2  5   2533
04 24 50  ---          07 45 32  49.6 380.5 -2.2    -133.2   123   F  1   3400

04 24 50  M82          07 45 32  46.9 375.9 -2.2    -137.3    -7   2  5   3400
04 29 00  ---          07 49 43  47.1 375.5 -2.1    -138.6   243   F  1   5067

04 29 00  J0958+65     07 49 43  49.9 380.1 -2.2    -134.5    -8   2  5   5067
04 31 10  ---          07 51 53  50.1 379.8 -2.1    -135.2   122   F  1   5933

04 31 10  M82          07 51 53  47.2 375.3 -2.1    -139.2    -8   2  5   5933
04 35 20  ---          07 56 04  47.5 374.9 -2.0    -140.5   242   F  1   7600

04 35 20  J0958+65     07 56 04  50.4 379.3 -2.0    -136.5    -8   2  5   7600
04 37 30  ---          07 58 14  50.5 379.1 -2.0    -137.2   122   F  1   8467

04 37 30  M82          07 58 14  47.6 374.7 -2.0    -141.2    -8   2  5   8467
04 41 40  ---          08 02 25  47.8 374.2 -1.9    -142.5   242   F  1  10133

04 41 40  J0958+65     08 02 25  50.8 378.6 -1.9    -138.5    -8   2  5  10133
04 43 50  ---          08 04 35  50.9 378.3 -1.9    -139.2   122   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  21
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

04 43 50  M82          08 04 35  47.9 374.0 -1.9    -143.2    -8   2  5  11000
04 48 00  ---          08 08 46  48.1 373.6 -1.8    -144.5   242   F  1  12667

04 48 00  J0958+65     08 08 46  51.2 377.8 -1.8    -140.6    -8   2  5  12667
04 50 10  ---          08 10 56  51.4 377.5 -1.8    -141.3   122   F  1  13533

04 50 10  M82          08 10 56  48.2 373.3 -1.8    -145.1    -8   2  5  13533
04 54 20  ---          08 15 07  48.4 372.9 -1.7    -146.5   242   F  1  15200

04 54 20  J0958+65     08 15 07  51.6 377.0 -1.7    -142.7    -8   2  5  15200
04 56 20  ---          08 17 07  51.8 376.7 -1.7    -143.3   112   F  1  16000

04 56 20  M82          08 17 07  48.5 372.7 -1.6    -147.1    -8   2  5  16000
05 00 20  ---          08 21 08  48.7 372.2 -1.6    -148.4   232   F  1  17600

 ---------- Reverse pass 3 ----------

05 01 00  J0958+65     08 21 48  52.0 376.1 -1.6    -144.9    31   2  6  17600
05 03 10  ---          08 23 59  52.2 375.8 -1.6    -145.6   130   R  1  16733

05 03 10  M82          08 23 59  48.8 371.9 -1.5    -149.3    -9   2  6  16733
05 07 20  ---          08 28 09  49.0 371.4 -1.5    -150.6   241   R  1  15067

05 07 20  J0958+65     08 28 09  52.4 375.2 -1.5    -147.0    -9   2  6  15067
05 09 30  ---          08 30 20  52.5 374.9 -1.5    -147.8   121   R  1  14200

05 09 30  M82          08 30 20  49.1 371.2 -1.4    -151.3    -9   2  6  14200
05 13 40  ---          08 34 30  49.3 370.7 -1.4    -152.7   241   R  1  12533

05 13 40  J0958+65     08 34 30  52.8 374.2 -1.4    -149.2    -9   2  6  12533
05 15 50  ---          08 36 41  52.9 373.9 -1.4    -150.0   121   R  1  11667

05 15 50  M82          08 36 41  49.4 370.4 -1.3    -153.4    -9   2  6  11667
05 20 00  ---          08 40 51  49.5 369.9 -1.3    -154.7   241   R  1  10000

05 20 00  J0958+65     08 40 51  53.1 373.3 -1.3    -151.4    -9   2  6  10000
05 22 10  ---          08 43 02  53.2 373.0 -1.3    -152.2   121   R  1   9133

05 22 10  M82          08 43 02  49.6 369.7 -1.2    -155.4    -9   2  6   9133
05 26 20  ---          08 47 12  49.8 369.1 -1.1    -156.8   241   R  1   7467

05 26 20  J0958+65     08 47 12  53.4 372.3 -1.2    -153.6    -9   2  6   7467
05 28 30  ---          08 49 23  53.5 372.0 -1.2    -154.4   121   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page  22
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

05 28 30  M82          08 49 23  49.8 368.9 -1.1    -157.5    -9   2  6   6600
05 32 40  ---          08 53 33  50.0 368.4 -1.0    -158.9   241   R  1   4933

05 32 40  J0958+65     08 53 33  53.7 371.3 -1.1    -155.9    -9   2  6   4933
05 34 50  ---          08 55 44  53.8 371.0 -1.1    -156.7   121   R  1   4067

05 34 50  M82          08 55 44  50.0 368.1 -1.0    -159.6    -9   2  6   4067
05 39 00  ---          08 59 54  50.2 367.5 -0.9    -161.0   241   R  1   2400

05 39 00  J0958+65     08 59 54  53.9 370.3 -1.0    -158.2   -10   2  6   2400
05 41 00  ---          09 01 55  54.0 370.0 -0.9    -158.9   110   R  1   1600

05 41 00  M82          09 01 55  50.2 367.3 -0.9    -161.7   -10   2  6   1600
05 45 00  ---          09 05 55  50.3 366.8 -0.8    -163.0   230   R  1      0

 ---------- Forward pass 4 ----------

05 47 00  J0958+65     09 07 56  54.2 369.0 -0.8    -161.1   110   2  7      0
05 49 10  ---          09 10 06  54.3 368.6 -0.8    -161.9   130   F  1    867

05 49 10  M82          09 10 06  50.4 366.2 -0.8    -164.4   -10   2  7    867
05 53 20  ---          09 14 17  50.5 365.7 -0.7    -165.8   240   F  1   2533

05 53 20  J0958+65     09 14 17  54.4 367.9 -0.7    -163.4   -10   2  7   2533
05 55 30  ---          09 16 27  54.5 367.5 -0.7    -164.2   120   F  1   3400

05 55 30  M82          09 16 27  50.6 365.4 -0.7    -166.6   -10   2  7   3400
05 59 40  ---          09 20 38  50.6 364.8 -0.6    -168.0   240   F  1   5067

05 59 40  J0958+65     09 20 38  54.6 366.8 -0.6    -165.7   -10   2  7   5067
06 01 50  ---          09 22 48  54.6 366.4 -0.6    -166.5   120   F  1   5933

06 01 50  M82          09 22 48  50.7 364.5 -0.6    -168.7   -10   2  7   5933
06 06 00  ---          09 26 59  50.7 364.0 -0.5    -170.1   240   F  1   7600

06 06 00  J0958+65     09 26 59  54.7 365.7 -0.5    -168.1   -10   2  7   7600
06 08 10  ---          09 29 09  54.8 365.3 -0.5    -168.9   120   F  1   8467

06 08 10  M82          09 29 09  50.8 363.7 -0.4    -170.9   -10   2  7   8467
06 12 20  ---          09 33 20  50.8 363.1 -0.4    -172.3   240   F  1  10133

06 12 20  J0958+65     09 33 20  54.9 364.6 -0.4    -170.4   -10   2  7  10133
06 14 30  ---          09 35 30  54.9 364.2 -0.4    -171.2   120   F  1  11000
Schedule for VLBA_FD   (Code Fd )                                   Page  23
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

06 14 30  M82          09 35 30  50.9 362.8 -0.3    -173.0   -10   2  7  11000
06 18 40  ---          09 39 41  50.9 362.2 -0.3    -174.4   240   F  1  12667

06 18 40  J0958+65     09 39 41  54.9 363.5 -0.3    -172.8   -10   2  7  12667
06 20 50  ---          09 41 51  55.0 363.1 -0.3    -173.6   120   F  1  13533

06 20 50  M82          09 41 51  50.9 361.9 -0.2    -175.2   -10   2  7  13533
06 25 00  ---          09 46 02  50.9 361.4 -0.2    -176.6   240   F  1  15200

06 25 00  J0958+65     09 46 02  55.0 362.3 -0.2    -175.2   -10   2  7  15200
06 27 00  ---          09 48 02  55.0 362.0 -0.2    -175.9   110   F  1  16000

06 27 00  M82          09 48 02  50.9 361.1 -0.1    -177.3   -10   2  7  16000
06 31 00  ---          09 52 03  51.0 360.5 -0.1    -178.7   230   F  1  17600

 ---------- Reverse pass 4 ----------

06 31 40  J0958+65     09 52 43  55.1 361.1 -0.1    -177.7    30   2  8  17600
06 33 50  ---          09 54 53  55.1 360.7 -0.1    -178.5   130   R  1  16733

06 33 50  M82          09 54 53  51.0 360.1  0.0    -179.6   -10   2  8  16733
06 38 00  ---          09 59 04  51.0 359.6  0.1     178.9   240   R  1  15067

06 38 00  J0958+65     09 59 04  55.1 360.0  0.0     179.9   -10   2  8  15067
06 40 10  ---          10 01 15  55.1 359.6  0.0     179.1   120   R  1  14200

06 40 10  M82          10 01 15  51.0 359.3  0.1     178.2   -10   2  8  14200
06 44 20  ---          10 05 25  50.9 358.7  0.2     176.8   240   R  1  12533

06 44 20  J0958+65     10 05 25  55.1 358.8  0.1     177.6   -10   2  8  12533
06 46 30  ---          10 07 36  55.0 358.4  0.1     176.7   120   R  1  11667

06 46 30  M82          10 07 36  50.9 358.4  0.2     176.0   -10   2  8  11667
06 50 40  ---          10 11 46  50.9 357.8  0.3     174.6   240   R  1  10000

06 50 40  J0958+65     10 11 46  55.0 357.7  0.2     175.2   -10   2  8  10000
06 52 50  ---          10 13 57  55.0 357.3  0.3     174.4   120   R  1   9133

06 52 50  M82          10 13 57  50.9 357.5  0.3     173.9   -10   2  8   9133
06 57 00  ---          10 18 07  50.8 357.0  0.4     172.4   240   R  1   7467

06 57 00  J0958+65     10 18 07  54.9 356.5  0.3     172.8   -10   2  8   7467
06 59 10  ---          10 20 18  54.9 356.2  0.4     172.0   120   R  1   6600
Schedule for VLBA_FD   (Code Fd )                                   Page  24
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

06 59 10  M82          10 20 18  50.8 356.7  0.4     171.7   -10   2  8   6600
07 03 20  ---          10 24 28  50.8 356.1  0.5     170.3   240   R  1   4933

07 03 20  J0958+65     10 24 28  54.9 355.4  0.4     170.4   -10   2  8   4933
07 05 30  ---          10 26 39  54.8 355.0  0.5     169.6   120   R  1   4067

07 05 30  M82          10 26 39  50.7 355.8  0.5     169.6   -10   2  8   4067
07 09 40  ---          10 30 49  50.6 355.2  0.6     168.1   240   R  1   2400

07 09 40  J0958+65     10 30 49  54.7 354.3  0.5     168.1   -10   2  8   2400
07 11 40  ---          10 32 50  54.7 353.9  0.6     167.3   110   R  1   1600

07 11 40  M82          10 32 50  50.6 355.0  0.6     167.5   -10   2  8   1600
07 15 40  ---          10 36 50  50.5 354.4  0.7     166.1   230   R  1      0

 ---------- Forward pass 5 ----------

07 17 40  J0958+65     10 38 51  54.5 352.9  0.7     165.1   110   2  9      0
07 19 40  ---          10 40 51  54.5 352.6  0.7     164.4   120   F  1    800

07 19 40  M82          10 40 51  50.4 353.9  0.7     164.8   -10   2  9    800
07 23 40  ---          10 44 52  50.3 353.4  0.8     163.4   230   F  1   2400

07 23 40  J0958+65     10 44 52  54.4 351.9  0.8     162.9   -10   2  9   2400
07 26 00  ---          10 47 12  54.3 351.5  0.8     162.0   130   F  1   3333

07 26 00  M82          10 47 12  50.3 353.1  0.9     162.6   -10   2  9   3333
07 30 20  ---          10 51 33  50.2 352.5  0.9     161.2   250   F  1   5067

07 30 20  J0958+65     10 51 33  54.1 350.7  0.9     160.5   -10   2  9   5067
07 32 40  ---          10 53 53  54.1 350.4  0.9     159.6   130   F  1   6000

07 32 40  M82          10 53 53  50.1 352.2  1.0     160.4   -10   2  9   6000
07 37 00  ---          10 58 14  50.0 351.7  1.0     159.0   250   F  1   7733

07 37 00  J0958+65     10 58 14  53.9 349.6  1.0     158.0   -10   2  9   7733
07 39 20  ---          11 00 34  53.8 349.3  1.0     157.2   130   F  1   8667

07 39 20  M82          11 00 34  49.9 351.4  1.1     158.2   -10   2  9   8667
07 43 40  ---          11 04 55  49.8 350.8  1.1     156.8   250   F  1  10400

07 43 40  J0958+65     11 04 55  53.6 348.6  1.1     155.7   -10   2  9  10400
07 46 00  ---          11 07 15  53.5 348.2  1.1     154.8   130   F  1  11333
Schedule for VLBA_FD   (Code Fd )                                   Page  25
               GM038 18cm global observation of M82
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
     Automatic tape allocation specified.  Tape positions are just estimates.
-------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
-------------------------------------------------------------------------------

 --- Sat  24 Feb 2001   Day  55 ---

07 46 00  M82          11 07 15  49.7 350.5  1.2     156.0   -10   2  9  11333
07 50 20  ---          11 11 36  49.5 350.0  1.3     154.6   250   F  1  13067

07 50 20  J0958+65     11 11 36  53.3 347.5  1.2     153.3   -10   2  9  13067
07 52 40  ---          11 13 56  53.2 347.2  1.3     152.5   130   F  1  14000

07 52 40  M82          11 13 56  49.4 349.7  1.3     153.8   -10   2  9  14000
07 57 00  ---          11 18 17  49.3 349.2  1.4     152.4   250   F  1  15733

07 57 00  J0958+65     11 18 17  53.0 346.5  1.3     151.0   -10   2  9  15733
08 00 00  ---          11 21 18  52.9 346.1  1.4     149.9   170   F  1  16933


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /usr/local/sched/setups/v18cm-128-4-2.set
   Matches group v20cm_2 in /usr/local/sched/catalogs/freq.dat
    FD filtered above 1760.  SC filtered above 1740.

   Setup group:    8         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   LO sum=  1659.49  1659.49  1667.49  1667.49
   1st LO=  2400.00  2400.00  2400.00  2400.00
   Net SB=        U        U        U        U
   Pol.  =     RCP      LCP      RCP      LCP 
   BBC fr=   740.51   740.51   732.51   732.51
   Bandwd=     8.00     8.00     8.00     8.00
   BBC   =        1        2        3        4
   BBC SB=        L        L        L        L
   IF    =       A        C        A        C 

   VLBA FE=     20cm     omit     20cm     omit
   VLBA Synth=  15.4      2.4     15.4

   Pulse cal detection.  PCAL = 1MHz
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=   510   510  6510  6510     0     0     0     0
    PCALFR2=   510   510  6510  6510     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- GM038 18cm global observation of M82
     Catalog positions marked with *. 
     Position of date is for stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

 * M82               09 51 41.957031   * 09 55 50.694000     09 55 58.296778 
                     69 54 57.38676    * 69 40 43.69000      69 40 26.97874 
                     From catalog imbedded in main SCHED input file.

   J0319+4130        03 16 29.567269   * 03 19 48.160100     03 19 51.184433 
   0316+413          41 19 51.91887    * 41 30 42.10600      41 30 58.70156 
 * 3C84              /usr/local/sched/catalogs/sources.vlba
   J0319+41          VLA Calibrator Source List

   J0927+3902        09 23 55.319194   * 09 27 03.013915     09 27 07.717867 
   0923+392          39 15 23.56652    * 39 02 20.85193      39 02 03.16609 
   4C39.25           /usr/local/sched/catalogs/sources.vlba
 * J0927+39          USNO - Ref Frame 1998-6, Eubanks June 1998

   J0958+6533        09 54 57.847929   * 09 58 47.245110     09 58 53.982373 
   0954+658          65 48 15.53887    * 65 33 54.81806      65 33 37.26533 
 * J0958+65          /usr/local/sched/catalogs/sources.vlba
                     USNO - Ref Frame 1998-6, Eubanks June 1998



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   M82                119.6
   3C84                83.7
   J0927+39           147.4
   J0958+65           123.7

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

