  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Third epoch observations of CSOs
 Exp. Code:  gp032   


Schedule Version:       1.00                                              
Processed by SCHED version: 16 Oct. 2001                                  

PI:       Antonis Polatidis                                               

Address:  Max Planck Institut fur Radioastronomie                         
          Bonn                                                            
          D-53121                                                         
          Germany                                                         

Phone:    +49 228 525 424                                                 
EMAIL:    apolatid@mpifr-bonn.mpg.de                                      
Fax:      +49 228 525 229                                                 
Phone during observation: +49 228 525 424                                 

Observing mode: 4 cm Continuum RCP VLBA/Mark IV                           

Notes:     Using VLBA + 7 antennae of the EVN                             
           X band RCP only                                                
           Tape change for the EVN is at 0620 UT                          
          Some sources not up in Sh, Ur, Wb and MK                        


COVER LETTER:


This is an Xband RCP experiment using 10 VLBA and 7 EVN stations
It uses 2 thin tapes
The data will be correlated at Socorro

Some sources are not up at Sh, Ur, Wb, Mk. Some set during the observation
in the EVN telescopes.

Tape change for the EVN telescopes is at 0610 UT

Please add TSYS in your POSTOB procedure

Thank you for your efforts

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Third epoch observations of CSOs
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  27 Feb 2002   Day  58 ---

 Next scan frequencies:  8405.49  8413.49  8421.49  8429.49
 Next BBC frequencies:    805.49   813.49   821.49   829.49
 Next scan bandwidths:      8.00     8.00     8.00     8.00

18 00 00  0108+388     21 33 49  45.2  63.6 -3.6     -83.5     0   1  1      0  18 00 00
18 14 40  ---          21 48 31  48.0  64.0 -3.4     -85.5   880   F  1   5867

18 17 54  1943+546     21 51 45  56.9 -33.8  2.1     123.8   126   1  1   5867  18 17 54
18 25 14  ---          21 59 06  56.0 -34.9  2.2     121.5   440   F  1   8800

18 25 54  2002+475     21 59 46  61.9 -44.9  2.0     116.1    26   1  1   8800  18 25 54
18 33 14  ---          22 07 08  60.8 -46.0  2.1     113.8   440   F  1  11733

18 34 24  2021+614     22 08 19  54.5 -21.5  1.8     138.5    52   1  1  11733  18 34 24
18 41 44  ---          22 15 40  53.9 -22.6  1.9     136.0   440   F  1  14667

18 44 35  2352+495     22 18 31  63.6  36.4 -1.6    -127.6   129   1  1  14667  18 44 35
18 51 55  ---          22 25 52  64.5  34.7 -1.5    -130.5   440   F  1  17600

18 54 01  1943+546     22 27 58  52.3 -38.1  2.7     112.9    76   1  2  17600  18 54 01
19 01 21  ---          22 35 20  51.3 -38.7  2.8     110.9   440   R  1  14667

19 04 55  0108+388     22 38 54  57.8  64.2 -2.5     -93.4   143   1  2  14667  19 04 55
19 19 35  ---          22 53 36  60.6  63.7 -2.3     -96.1   880   R  1   8800

19 22 36  2021+614     22 56 38  50.2 -27.6  2.6     123.0   119   1  2   8800  19 22 36
19 29 56  ---          23 04 00  49.4 -28.3  2.7     120.9   440   R  1   5867

19 31 54  2352+495     23 05 58  68.7  22.2 -0.8    -149.7    77   1  2   5867  19 31 54
19 39 14  ---          23 13 19  69.2  19.3 -0.7    -153.8   440   R  1   2933

19 42 48  0108+388     23 16 53  65.1  62.2 -1.9    -101.1   183   1  2   2933  19 42 48
19 50 08  ---          23 24 14  66.5  61.5 -1.8    -102.9   440   R  1      0

19 51 30  2352+495     23 25 37  70.0  14.1 -0.5    -161.1    48   1  3      0  19 51 30
20 06 10  ---          23 40 19  70.6   7.2 -0.2    -170.3   880   F  1   5867

20 07 45  0108+388     23 41 54  69.8  59.1 -1.5    -107.9    58   1  3   5867  20 07 45
20 22 25  ---          23 56 37  72.5  56.0 -1.3    -113.2   880   F  1  11733

20 24 14  2352+495     23 58 26  70.8  -1.6  0.1     177.9    69   1  3  11733  20 24 14
20 31 34  ---          00 05 47  70.7  -5.2  0.2     173.1   440   F  1  14667
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Third epoch observations of CSOs
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  27 Feb 2002   Day  58 ---

20 33 32  2021+614     00 07 45  42.4 -32.4  3.8     103.8    59   1  3  14667  20 33 32
20 40 52  ---          00 15 07  41.6 -32.7  3.9     102.0   440   F  1  17600

20 43 44  0108+388     00 18 00  76.1  48.7 -0.9    -123.6   102   1  4  17600  20 43 44
20 58 24  ---          00 32 42  78.4  40.6 -0.7    -133.8   880   R  1  11733

20 59 36  2352+495     00 33 54  69.5 -18.0  0.6     155.7    31   1  4  11733  20 59 36
21 14 16  ---          00 48 36  68.3 -23.8  0.9     147.5   880   R  1   5867

21 15 26  0108+388     00 49 47  80.4  26.4 -0.4    -150.5    35   1  4   5867  21 15 26
21 22 46  ---          00 57 08  81.0  18.4 -0.2    -159.5   440   R  1   2933

21 24 06  2352+495     00 58 28  67.4 -27.2  1.1     142.4    48   1  4   2933  21 24 06
21 31 26  ---          01 05 49  66.7 -29.6  1.2     138.8   440   R  1      0

21 33 12  0108+388     01 07 36  81.5   5.4 -0.1    -174.0    74   1  5      0  21 33 12
21 47 52  ---          01 22 18  81.2 -13.6  0.2     164.9   880   F  1   5867

21 51 40  0615+820     01 26 07  32.4   9.1 -5.0    -100.1   128   1  5   5867  21 51 40
21 59 00  ---          01 33 28  32.6   9.1 -4.9    -102.0   440   F  1   8800

22 02 00  0108+388     01 36 28  80.1 -29.2  0.4     147.3    83   1  5   8800  22 02 00
22 09 20  ---          01 43 50  79.3 -35.6  0.5     139.8   440   F  1  11733

22 13 34  0710+439     01 48 04  26.4  52.8 -5.4     -71.9   146   1  5  11733  22 13 34
22 28 14  ---          02 02 46  29.0  53.7 -5.2     -74.0   880   F  1  17600

22 30 36  0646+600     02 05 09  35.4  35.5 -4.8     -88.8   127   1  6  17600  22 30 36
22 45 16  ---          02 19 51  37.2  35.5 -4.5     -92.0   880   R  1  11733

22 47 25  0710+439     02 22 01  32.3  54.7 -4.9     -76.8   115   1  6  11733  22 47 25
23 02 05  ---          02 36 43  34.9  55.4 -4.6     -79.0   880   R  1   5867

23 06 08  0615+820     02 40 47  34.8   8.1 -3.8    -119.2   209   1  6   5867  23 06 08
23 13 28  ---          02 48 08  35.0   7.9 -3.6    -121.1   440   R  1   2933

23 17 01  DA193        02 51 42  51.8  63.2 -3.1     -89.2   174   1  6   2933  23 17 01
23 24 21  ---          02 59 03  53.2  63.2 -2.9     -90.4   440   R  1      0

23 25 52  0646+600     03 00 34  42.2  34.7 -3.8    -101.3    67   1  7      0  23 25 52
23 40 32  ---          03 15 17  44.0  34.1 -3.6    -104.9   880   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Third epoch observations of CSOs
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Wed  27 Feb 2002   Day  58 ---

23 42 16  0710+439     03 17 01  42.1  56.7 -3.9     -85.2    87   1  7   5867  23 42 16
23 56 56  ---          03 31 43  44.8  56.9 -3.7     -87.5   880   F  1  11733

 --- Start: Wed  27 Feb 2002   Day  58 -- Stop: Thu  28 Feb 2002   Day  59 ---

23 58 35  0646+600     03 33 23  46.2  33.2 -3.3    -109.5    82   1  7  11733  23 58 35
00 05 55  ---          03 40 44  47.0  32.7 -3.2    -111.4   440   F  1  14667

00 07 31  0710+439     03 42 20  46.7  57.0 -3.5     -89.3    78   1  7  14667  00 07 31
00 14 51  ---          03 49 41  48.0  57.0 -3.4     -90.6   440   F  1  17600

00 18 16  0615+820     03 53 06  36.7   6.2 -2.6    -138.2   169   1  8  17600  00 18 16
00 25 36  ---          04 00 28  36.9   5.9 -2.4    -140.2   440   R  1  14667

00 25 36  0646+600     04 00 28  49.3  31.2 -2.8    -116.8   -27   1  8  14667  00 25 36
00 40 16  ---          04 15 10  50.9  29.8 -2.6    -121.1   853   R  1   8800

00 40 16  0710+439     04 15 10  52.6  56.6 -3.0     -95.3   -20   1  8   8800  00 40 16
00 54 56  ---          04 29 52  55.2  56.1 -2.7     -98.3   860   R  1   2933

00 54 56  0646+600     04 29 52  52.4  28.2 -2.3    -125.5   -21   1  8   2933  00 54 56
01 02 16  ---          04 37 14  53.2  27.3 -2.2    -127.9   419   R  1      0

01 02 56  0710+439     04 37 54  56.7  55.7 -2.6    -100.0    19   1  9      0  01 02 56
01 17 36  ---          04 52 36  59.3  54.7 -2.4    -103.4   880   F  1   5867

01 18 56  0646+600     04 53 56  54.8  25.0 -1.9    -133.3    58   1  9   5867  01 18 56
01 33 36  ---          05 08 39  56.0  22.7 -1.7    -138.4   880   F  1  11733

01 34 52  0710+439     05 09 55  62.3  52.9 -2.1    -107.9    54   1  9  11733  01 34 52
01 49 32  ---          05 24 38  64.8  50.9 -1.8    -112.3   880   F  1  17600

01 50 47  0646+600     05 25 53  57.4  19.6 -1.4    -144.7    52   1 10  17600  01 50 47
02 12 47  ---          05 47 56  58.8  15.1 -1.0    -153.3  1320   R  1   8800

02 13 57  0710+439     05 49 07  68.7  45.9 -1.4    -121.2    48   1 10   8800  02 13 57
02 28 37  ---          06 03 49  70.9  41.5 -1.2    -127.8   880   R  1   2933

02 31 08  0615+820     06 06 21  38.6   0.9 -0.3    -174.4    84   1 10   2933  02 31 08
02 38 28  ---          06 13 42  38.6   0.6 -0.2    -176.5   440   R  1      0

02 40 03  0646+600     06 15 17  60.0   8.9 -0.6    -164.6    50   1 11      0  02 40 03
02 54 43  ---          06 29 59  60.4   5.2 -0.3    -170.9   880   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Third epoch observations of CSOs
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu  28 Feb 2002   Day  59 ---

02 55 47  0710+439     06 31 04  74.3  29.7 -0.7    -143.8    35   1 11   5867  02 55 47
03 10 27  ---          06 45 46  75.7  20.9 -0.5    -154.9   880   F  1  11733

03 15 09  1242+410     06 50 29  20.4  53.9 -5.9     -66.6   169   1 11  11733  03 15 09
03 29 49  ---          07 05 11  23.0  55.0 -5.7     -68.6   880   F  1  17600

03 34 06  1245+676     07 09 29  30.1  26.3 -5.6     -82.0   235   1 12  17600  03 34 06
03 48 46  ---          07 24 11  31.5  26.5 -5.4     -85.3   880   R  1  11733

03 52 10  0710+439     07 27 36  76.5 -10.8  0.2     167.1   112   1 12  11733  03 52 10
04 06 50  ---          07 42 18  75.7 -21.2  0.5     154.5   880   R  1   5867

04 10 37  1242+410     07 46 05  30.3  57.8 -5.0     -74.0   134   1 12   5867  04 10 37
04 25 17  ---          08 00 48  33.0  58.6 -4.7     -76.0   880   R  1      0

04 28 56  0646+600     08 04 28  58.1 -17.4  1.2     149.0   166   1 13      0  04 28 56
04 43 36  ---          08 19 10  57.1 -20.3  1.5     143.4   880   F  1   5867

04 47 07  1242+410     08 22 42  37.0  59.7 -4.4     -78.9   156   1 13   5867  04 47 07
05 01 47  ---          08 37 24  39.8  60.3 -4.1     -80.9   880   F  1  11733

05 06 03  0615+820     08 41 41  37.1  -5.5  2.3     143.1   210   1 13  11733  05 06 03
05 13 23  ---          08 49 02  37.0  -5.8  2.4     141.1   440   F  1  14667

05 16 07  1245+676     08 51 46  39.9  25.4 -3.9    -106.1   141   1 13  14667  05 16 07
05 23 27  ---          08 59 08  40.5  25.2 -3.8    -108.0   440   F  1  17600

05 26 00  0646+600     09 01 41  53.4 -27.0  2.2     128.7   117   1 14  17600  05 26 00
05 40 40  ---          09 16 24  51.9 -28.8  2.4     124.1   880   R  1  11733

05 40 40  1242+410     09 16 24  47.1  61.4 -3.5     -86.6   -62   1 14  11733  05 40 40
05 55 20  ---          09 31 06  49.9  61.6 -3.2     -88.8   818   R  1   5867

05 55 20  1245+676     09 31 06  43.4  23.6 -3.3    -116.4   -27   1 14   5867  05 55 20
06 10 00  ---          09 45 49  44.6  22.7 -3.0    -120.5   853   R  1      0

-----------  Tape Change ------------

06 25 00  0646+600     10 00 51  47.0 -32.7  3.2     111.4   861   2  1      0  06 25 00
06 32 20  ---          10 08 12  46.2 -33.2  3.3     109.5   440   F  1   2933

06 33 13  DA193        10 09 05  38.5 -61.3  4.2      79.4    32   2  1   2933  06 33 13
06 40 33  ---          10 16 26  37.1 -61.0  4.3      78.4   440   F  1   5867
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Third epoch observations of CSOs
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu  28 Feb 2002   Day  59 ---

06 43 02  0615+820     10 18 56  34.6  -8.2  3.9     117.5   113   2  1   5867  06 43 02
06 50 22  ---          10 26 18  34.4  -8.3  4.0     115.6   440   F  1   8800

06 53 59  1242+410     10 29 55  61.0  60.2 -2.3     -99.7   161   2  1   8800  06 53 59
07 15 59  ---          10 51 58  65.1  58.2 -1.9    -105.0  1320   F  1  17600

07 23 38  2021+614     10 59 39   7.6  17.7 -9.4     -33.4   342   2  2  17600  07 23 38
07 38 18  ---          11 14 21   8.6  19.2 -9.1     -36.5   880   R  1  11733

07 40 30  1943+546     11 16 34   6.8  27.6 -8.5     -43.8   124   2  2  11733  07 40 30
07 55 10  ---          11 31 16   8.3  29.1 -8.2     -46.6   880   R  1   5867

07 59 50  1245+676     11 35 56  51.7  11.0 -1.2    -154.7   191   2  2   5867  07 59 50
08 07 10  ---          11 43 18  52.0  10.0 -1.1    -157.2   440   R  1   2933

08 09 55  1242+410     11 46 03  74.4  45.5 -1.0    -125.8   119   2  2   2933  08 09 55
08 17 15  ---          11 53 24  75.5  42.2 -0.9    -130.2   440   R  1      0

08 22 49  1843+356     11 59 00   9.0  53.6 -6.8     -58.6   199   2  3      0  08 22 49
08 30 09  ---          12 06 21  10.3  54.4 -6.7     -59.5   440   F  1   2933

08 39 00  2021+614     12 15 13  13.5  24.6 -8.1     -48.8   509   2  3   2933  08 39 00
08 46 20  ---          12 22 34  14.2  25.2 -8.0     -50.3   440   F  1   5867

08 47 54  1943+546     12 24 08  14.2  33.9 -7.3     -56.5    86   2  3   5867  08 47 54
08 55 14  ---          12 31 29  15.1  34.5 -7.2     -57.8   440   F  1   8800

09 01 03  1843+356     12 37 19  15.8  57.5 -6.1     -63.3   332   2  3   8800  09 01 03
09 08 23  ---          12 44 41  17.1  58.2 -6.0     -64.2   440   F  1  11733

09 12 35  1242+410     12 48 54  79.8  -4.2  0.1     175.2   125   2  3  11733  09 12 35
09 27 15  ---          13 03 36  79.2 -19.1  0.3     158.1   880   F  1  17600

09 33 15  2021+614     13 09 37  18.7  28.5 -7.2     -59.7   237   2  4  17600  09 33 15
09 40 35  ---          13 16 58  19.5  28.9 -7.1     -61.2   440   R  1  14667

09 59 22  1943+546     13 35 48  23.4  38.9 -6.1     -69.6  1116   2  4  14667  09 59 22
10 14 02  ---          13 50 30  25.4  39.6 -5.9     -72.2   880   R  1   8800

10 17 39  1843+356     13 54 08  30.2  63.9 -4.9     -72.1   199   2  4   8800  10 17 39
10 32 19  ---          14 08 50  33.1  64.9 -4.6     -73.7   880   R  1   2933
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Third epoch observations of CSOs
  UP:  D => Below limits;  H => Below horizon mask.  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Tapes: Drive, Index, Start footage / Direction, Head Group, End footage.
  TPStart:  Tape motion start time.  Frequencies are LO sum (band edge).
     Automatic tape allocation specified.  Tape positions are just estimates.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Tapes      TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell  (see above)
----------------------------------------------------------------------------------------

 --- Thu  28 Feb 2002   Day  59 ---

10 57 29  2002+475     14 34 05  27.1  48.8 -5.5     -73.2  1496   2  4   2933  10 57 29
11 04 49  ---          14 41 26  28.3  49.2 -5.3     -74.4   440   R  1      0

11 07 17  2021+614     14 43 55  29.2  32.8 -5.6     -78.8   135   2  5      0  11 07 17
11 14 37  ---          14 51 16  30.0  33.0 -5.5     -80.3   440   F  1   2933

11 15 55  1943+546     14 52 34  34.2  41.8 -4.9     -83.9    68   2  5   2933  11 15 55
11 23 15  ---          14 59 55  35.2  41.9 -4.7     -85.3   440   F  1   5867

11 24 45  1843+356     15 01 25  43.4  68.1 -3.7     -79.4    70   2  5   5867  11 24 45
11 39 25  ---          15 16 08  46.4  68.8 -3.5     -81.0   880   F  1  11733

11 41 40  2021+614     15 18 23  33.2  33.4 -5.1     -86.0   107   2  5  11733  11 41 40
11 56 20  ---          15 33 05  35.0  33.5 -4.8     -89.2   880   F  1  17600

12 03 26  2352+495     15 40 13   4.7  32.5 -8.3     -45.9   364   2  6  17600  12 03 26
12 10 46  ---          15 47 34   5.5  33.4 -8.1     -47.2   440   R  1  14667

12 18 38  1943+546     15 55 27  43.2  41.7 -3.8     -96.8   395   2  6  14667  12 18 38
12 25 58  ---          16 02 49  44.3  41.5 -3.7     -98.4   440   R  1  11733

12 29 29  1843+356     16 06 20  56.5  70.5 -2.7     -87.0   184   2  6  11733  12 29 29
12 44 09  ---          16 21 02  59.5  70.7 -2.4     -89.0   880   R  1   5867

12 52 17  2352+495     16 29 12  10.7  37.6 -7.4     -54.6   389   2  6   5867  12 52 17
13 06 37  ---          16 43 34  12.6  39.0 -7.2     -57.0   860   R  1    133

13 11 02  1943+546     16 48 00  50.6  39.2 -2.9    -109.4   187   2  7    133  13 11 02
13 20 42  ---          16 57 42  51.9  38.4 -2.8    -112.0   580   F  1   4000

13 21 33  2002+475     16 58 33  51.3  51.0 -3.1     -98.8    40   2  7   4000  13 21 33
13 26 53  ---          17 03 53  52.2  50.7 -3.0    -100.0   320   F  1   6133

13 28 08  2021+614     17 05 09  45.7  31.0 -3.3    -111.1    60   2  7   6133  13 28 08
13 35 28  ---          17 12 30  46.5  30.5 -3.2    -113.1   440   F  1   9067

13 51 39  0108+388     17 28 43   1.8  44.4 -7.7  D  -50.8   880   2  7   9067  13 51 39
13 59 59  ---          17 37 04   3.1  45.4 -7.6     -52.1     0   F  1  12400


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 Setup file: /homes/antonios/sched/setups/v4cm-128-4-2-R.set
   Matches group v4cm_3 in /homes/antonios/sched/catalogs/freq.dat

   Setup group:    1         Station: VLBA              Total bit rate:  128
   Format: VLBA1:4           Bits per sample: 2         Sample rate: 16.000
   Number of channels:  4    Passes/head pos:   1       Speedup factor:   2.00

   Tape speeds: Low density - 133.330 ips,  High density -  80.00 ips
   Time per pass for  17600 ft, High density tapes is: 00:44:00

   1st LO=   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U
   Pol.  =      RCP       RCP       RCP       RCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        B         B         B         B 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.4     15.4

  The following frequency sets based on this setup were used.

   Frequency Set:   1  Setup file default.  Used pcal sets:   1
   LO sum=    8405.49   8413.49   8421.49   8429.49
   BBC fr=     805.49    813.49    821.49    829.49
   Bandwd=      8.000     8.000     8.000     8.000

  The following pulse cal sets were used with this setup:

   Pulse cal detection set:   1  PCAL = 1MHZ
    PCALXB1=   S1    S3    S1    S3    S1    S2    S3    S4 
    PCALXB2=   S2    S4    S2    S4    M1    M2    M3    M4 
    PCALFR1=   510   510  6510  6510     0     0     0     0
    PCALFR2=   510   510  6510  6510     0     0     0     0

   Track assignments are: 
    track1=   2, 18,  3, 19
    barrel=roll_auto
 SOURCE LIST -- Third epoch observations of CSOs
     Catalog positions marked with *. 
     Precession of date coordinates is based on stop time of first scan.
     Names used in schedule marked with *. 
     Short names used in VLA and SNAP files marked with +. 
     Observation date used in B1950/J2000 coordinate conversion (PRECDATE):  1979.900
     No adjustments are made for rates (DRA, DDEC).

   Source                         Source position (RA/Dec) 
                        (B1950)           (J2000)           (Date) 

   J0111+3906        01 08 47.254786   * 01 11 37.316982     01 11 42.275721 
 * 0108+388          38 50 32.81467    * 39 06 28.10430      39 07 05.88123 
   0108+388          From catalog imbedded in main SCHED input file.
   J0111+39          ICRF - Ext.1 Source - 1998 IERS Annual Report

   J0650+6001        06 46 04.111958   * 06 50 31.254326     06 50 42.644967 
 * 0646+600          60 05 14.15445    * 60 01 44.55569      60 01 47.71495 
   0646+600          From catalog imbedded in main SCHED input file.
   J0650+60          VLBA Calib. Survey - ICRF Frame - reduced by GSFC group - Aug 2001

   J0713+4349        07 10 03.347941   * 07 13 38.164127     07 13 47.293989 
 * 0710+439          43 54 26.19428    * 43 49 17.20698      43 49 11.50012 
   0710+439          From catalog imbedded in main SCHED input file.
   J0713+43          ICRF - Ext.1 Source - 1998 IERS Annual Report

   J1244+4048        12 42 26.387662   * 12 44 49.187214     12 44 55.923961 
 * 1242+410          41 04 29.93437    * 40 48 06.15357      40 47 16.64666 
   1242+410          From catalog imbedded in main SCHED input file.
   J1244+40          VLBA Calib. Survey - ICRF Frame - reduced by GSFC group - Aug 2001

   J1845+3541        18 43 48.344987   * 18 45 35.108871     18 45 38.120854 
 * 1843+356          35 38 02.50175    * 35 41 16.72651      35 41 06.99866 
   1843+356          From catalog imbedded in main SCHED input file.
   J1845+35          VLBA Calib. Survey - ICRF Frame - reduced by GSFC group - Aug 2001

   J1944+5448        19 43 22.654850   * 19 44 31.512621     19 44 32.278877 
 * 1943+546          54 40 47.99945    * 54 48 07.06308      54 48 07.27265 
   1943+546          From catalog imbedded in main SCHED input file.
                     VLBA Calib. Survey - ICRF Frame - reduced by GSFC group - Aug 2001

   J2022+6136        20 21 13.300161   * 20 22 06.681679     20 22 06.205184 
 * 2021+614          61 27 18.15569    * 61 36 58.80470      61 37 06.59483 
   2021+614          From catalog imbedded in main SCHED input file.
   J2022+61          ICRF - Ext.1 Source - 1998 IERS Annual Report

   J2355+4950        23 52 37.783457   * 23 55 09.458169     23 55 13.093467 
 * 2352+495          49 33 26.79934    * 49 50 08.34000      49 50 45.90725 
   2352+495          From catalog imbedded in main SCHED input file.
   J2355+49          ICRF - Ext.1 Source - 1998 IERS Annual Report

   J0626+8202        06 15 32.765073   * 06 26 03.006188     06 26 30.911948 
 * 0615+820          82 03 56.43109    * 82 02 25.56764      82 02 38.40794 
   0615+820          From catalog imbedded in main SCHED input file.
   J0626+82          ICRF - Ext.1 Source - 1998 IERS Annual Report

 * 2002+475          20 00 39.216117   * 20 02 10.418300     20 02 12.179438 
                     47 17 02.42779    * 47 25 28.77700      47 25 32.64999 
                     From catalog imbedded in main SCHED input file.

 * DA193             05 52 01.407166   * 05 55 30.805609     05 55 39.159443 
                     39 48 21.94585    * 39 48 49.16500      39 48 57.06031 
                     From catalog imbedded in main SCHED input file.
                     ICRF - Ext.1 Source - 1998 IERS Annual Report

   J1247+6723        12 45 32.137494   * 12 47 33.331818     12 47 40.753691 
 * 1245+676          67 39 37.58900    * 67 23 16.38040      67 22 26.65660 
   1245+676          /homes/antonios/sched/catalogs/sources.vlba
                     VLBA Calib. Survey - ICRF Frame - reduced by GSFC group - Aug 2001



  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   0108+388            58.3
   0646+600           112.4
   0710+439           122.1
   1242+410           137.6
   1843+356            71.0
   1943+546            73.1
   2021+614            74.9
   2352+495            59.9
   0615+820           101.4
   2002+475            66.0
   DA193              108.9
   1245+676           117.1

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

