  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: The nuclear structure in nearby AGN
 Exp. Code:  gs032c  


Schedule Version:       1.00
Processed by SCHED version:  11.10  Version 11.1 Beta of about April 26, 201

PI:       Tuomas Savolainen

Address:  MPIfR Bonn
          Auf dem Huegel 69
          53121 Bonn, Germany
 

Phone:    +49 228 525 473
EMAIL:    tsavolainen@mpifr-bonn.mpg.de
Fax:      +49 228 525 229
Phone during observation: +7 903 661 4865

Observing mode: C/K-band, dual-pol

Notes:    C/K-band, Radioastron-compatible frequency setup
          P-CAL is ON, Tsys is ON
          auto-level (AGC) is ON
          Please, send Mk5 disk packs to MPIfR-Bonn

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               The nuclear structure in nearby AGN
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Feb 2014   Day  36 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00
 Next scan bandwidths:      16.00     16.00     16.00     16.00

04 21 15  1228+126     06 26 27   5.2  78.7 -6.1     -59.7     0        0   04 21 15
04 25 00  ---          06 30 13   6.0  79.2 -6.0     -59.9   225        7   04 21 16

04 25 40  1228+126     06 30 53   6.1  79.3 -6.0     -59.9    34        7   04 25 40
04 34 00  ---          06 39 14   7.9  80.3 -5.9     -60.2   500       23   04 25 41

04 34 40  1228+126     06 39 54   8.0  80.4 -5.9     -60.3    34       23   04 34 40
04 43 00  ---          06 48 16   9.8  81.4 -5.7     -60.6   500       39   04 34 41

 ---------- Space segment 06: K-band VLBI scans ----------

04 45 00  1228+126     06 50 16  10.2  81.7 -5.7     -60.6   114       39   04 45 00
04 54 30  ---          06 59 47  12.2  82.8 -5.5     -60.9   570       58   04 45 01

04 55 00  1228+126     07 00 18  12.3  82.9 -5.5     -60.9    24       58   04 55 00
05 04 30  ---          07 09 49  14.4  84.0 -5.4     -61.2   570       76   04 55 01

05 05 00  1228+126     07 10 19  14.5  84.1 -5.4     -61.2    24       76   05 05 00
05 15 00  ---          07 20 21  16.6  85.3 -5.2     -61.4   600       95   05 05 01

 ---------- K-band GRT-only VLBI scans - segment 07Ka ----------

05 17 00  1236+077     07 22 21  12.8  88.9 -5.3     -60.2   104       95   05 17 00
05 19 00  ---          07 24 22  13.3  89.2 -5.3     -60.2   120       99   05 17 01

05 20 00  1228+126     07 25 22  17.7  85.9 -5.1     -61.5    44       99   05 20 00
05 28 00  ---          07 33 23  19.4  86.9 -5.0     -61.6   480      114   05 20 01

05 28 40  1228+126     07 34 03  19.6  87.0 -5.0     -61.6    34      114   05 28 40
05 33 00  ---          07 38 24  20.5  87.5 -4.9     -61.6   260      123   05 28 41

05 34 00  1236+077     07 39 24  16.5  91.1 -5.0     -60.2    44      123   05 34 00
05 36 00  ---          07 41 24  16.9  91.3 -5.0     -60.2   120      126   05 34 01

05 37 00  1228+126     07 42 24  21.4  88.0 -4.8     -61.7    44      126   05 37 00
05 41 00  ---          07 46 25  22.2  88.5 -4.8     -61.7   240      134   05 37 01

05 41 40  1228+126     07 47 05  22.4  88.6 -4.7     -61.7    34      134   05 41 40
05 52 00  ---          07 57 27  24.6  89.9 -4.6     -61.7   620      154   05 41 41

05 54 00  1236+077     07 59 27  20.8  93.7 -4.7     -60.0   104      154   05 54 00
05 56 00  ---          08 01 28  21.2  94.0 -4.6     -60.0   120      158   05 54 01
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               The nuclear structure in nearby AGN
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Feb 2014   Day  36 ---

05 57 00  1228+126     08 02 28  25.7  90.6 -4.5     -61.7    44      158   05 57 00
06 06 00  ---          08 11 29  27.6  91.7 -4.3     -61.7   540      175   05 57 01

06 06 40  1228+126     08 12 09  27.8  91.8 -4.3     -61.7    34      175   06 06 40
06 11 00  ---          08 16 30  28.7  92.4 -4.3     -61.6   260      183   06 06 41

06 12 00  1236+077     08 17 30  24.7  96.1 -4.4     -59.6    44      183   06 12 00
06 14 00  ---          08 19 31  25.1  96.4 -4.3     -59.6   120      187   06 12 01

06 15 00  1228+126     08 20 31  29.6  92.9 -4.2     -61.6    44      187   06 15 00
06 19 00  ---          08 24 31  30.4  93.5 -4.1     -61.5   240      195   06 15 01

06 19 40  1228+126     08 25 11  30.6  93.6 -4.1     -61.5    34      195   06 19 40
06 29 30  ---          08 35 03  32.7  94.9 -3.9     -61.3   590      214   06 19 41

 ---------- Space segment 07: K-band VLBI scans ----------

06 30 00  1228+126     08 35 33  32.8  95.0 -3.9     -61.3    24      214   06 30 00
06 39 30  ---          08 45 05  34.8  96.3 -3.8     -61.1   570      232   06 30 01

06 40 00  1228+126     08 45 35  34.9  96.4 -3.8     -61.1    24      232   06 40 00
06 49 30  ---          08 55 06  37.0  97.8 -3.6     -60.8   570      250   06 40 01

06 50 00  1228+126     08 55 36  37.1  97.9 -3.6     -60.7    24      250   06 50 00
07 00 00  ---          09 05 38  39.2  99.4 -3.4     -60.3   600      270   06 50 01

 ---------- K-band GRT-only VLBI scans - segment 08Ka ----------

07 02 00  1236+077     09 07 38  35.3 103.6 -3.5     -57.5   104      270   07 02 00
07 04 00  ---          09 09 39  35.7 103.9 -3.5     -57.4   120      274   07 02 01

07 05 00  1226+023     09 10 39  34.9 111.4 -3.3     -53.3    47      274   07 05 00
07 15 00  ---          09 20 41  36.9 113.3 -3.2     -52.3   600      293   07 05 01

07 16 00  1228+126     09 21 41  42.6 102.0 -3.2     -59.5    41      293   07 16 00
07 25 10  ---          09 30 52  44.5 103.6 -3.0     -58.9   550      310   07 16 01

07 25 50  1228+126     09 31 32  44.7 103.7 -3.0     -58.8    34      310   07 25 50
07 35 00  ---          09 40 44  46.6 105.4 -2.8     -58.1   550      328   07 25 51

07 37 00  1236+077     09 42 44  42.5 109.8 -3.0     -54.7   103      328   07 37 00
07 39 00  ---          09 44 45  42.9 110.2 -2.9     -54.5   120      332   07 37 01

07 40 00  1226+023     09 45 45  41.8 118.4 -2.7     -49.2    46      332   07 40 00
07 50 00  ---          09 55 46  43.7 120.6 -2.6     -47.8   600      351   07 40 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               The nuclear structure in nearby AGN
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Feb 2014   Day  36 ---

07 51 00  1228+126     09 56 46  49.9 108.6 -2.6     -56.6    40      351   07 51 00
08 02 00  ---          10 07 48  52.1 111.0 -2.4     -55.3   660      372   07 51 01

 ---------- U-band GRT-only VLBI scans - segment 08Ua ----------

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

08 03 00  1228+126     10 08 48  52.3 111.2 -2.4     -55.2    45      372   08 03 00
08 08 00  ---          10 13 49  53.3 112.4 -2.3     -54.5   300      382   08 03 01

 ---------- Q-band GRT-only VLBI scans - segment 08Qa ----------

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

08 09 00  1228+126     10 14 49  53.5 112.6 -2.3     -54.4    45      382   08 09 00
08 14 00  ---          10 19 50  54.5 113.8 -2.2     -53.7   300      392   08 09 01

 ---------- Space segment 08: K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

08 15 00  1228+126     10 20 50  54.7 114.1 -2.2     -53.5    54      392   08 15 00
08 24 30  ---          10 30 22  56.6 116.6 -2.0     -52.0   570      410   08 15 01

08 25 00  1228+126     10 30 52  56.7 116.7 -2.0     -51.9    24      410   08 25 00
08 34 30  ---          10 40 24  58.5 119.4 -1.9     -50.1   570      428   08 25 01

08 35 00  1228+126     10 40 54  58.6 119.6 -1.8     -50.0    24      428   08 35 00
08 45 00  ---          10 50 55  60.4 122.8 -1.7     -47.8   600      447   08 35 01

 ---------- U-band GRT-only VLBI scans - segment 09Ua ----------

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

08 46 00  1236+077     10 51 56  55.7 126.9 -1.8     -43.9    42      447   08 46 00
08 48 00  ---          10 53 56  56.0 127.6 -1.8     -43.5   120      451   08 46 01

08 49 00  1228+126     10 54 56  61.1 124.1 -1.6     -46.8    42      451   08 49 00
08 54 00  ---          10 59 57  62.0 125.9 -1.5     -45.5   300      461   08 49 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               The nuclear structure in nearby AGN
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Feb 2014   Day  36 ---

 ---------- Q-band GRT-only VLBI scans - segment 09Qa ----------

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

08 55 00  1236+077     11 00 57  57.2 129.9 -1.7     -41.7    42      461   08 55 00
08 57 00  ---          11 02 57  57.5 130.6 -1.6     -41.2   120      465   08 55 01

08 58 00  1228+126     11 03 57  62.7 127.4 -1.5     -44.4    42      465   08 58 00
09 03 00  ---          11 08 58  63.5 129.3 -1.4     -42.9   300      474   08 58 01

 ---------- K-band GRT-only VLBI scans - segment 09Ka ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

09 04 00  1236+077     11 09 58  58.6 133.1 -1.5     -39.3    42      474   09 04 00
09 06 00  ---          11 11 59  58.9 133.8 -1.5     -38.8   120      478   09 04 01

09 07 00  1228+126     11 12 59  64.2 131.0 -1.3     -41.7    42      478   09 07 00
09 17 00  ---          11 23 01  65.8 135.4 -1.1     -38.2   600      497   09 07 01

09 18 00  1236+077     11 24 01  60.7 138.6 -1.3     -35.0    42      497   09 18 00
09 20 00  ---          11 26 01  61.0 139.4 -1.2     -34.4   120      501   09 18 01

09 21 00  1228+126     11 27 01  66.4 137.4 -1.1     -36.6    42      501   09 21 00
09 31 00  ---          11 37 03  67.8 142.5 -0.9     -32.4   600      520   09 21 01

09 32 00  1236+077     11 38 03  62.6 144.8 -1.0     -30.0    42      520   09 32 00
09 34 00  ---          11 40 03  62.9 145.7 -1.0     -29.3   120      524   09 32 01

09 35 00  1228+126     11 41 04  68.3 144.8 -0.8     -30.5    42      524   09 35 00
09 45 00  ---          11 51 05  69.4 150.8 -0.7     -25.5   600      543   09 35 01

09 46 00  1236+077     11 52 05  64.2 151.7 -0.8     -24.3    42      543   09 46 00
09 48 00  ---          11 54 06  64.4 152.7 -0.8     -23.4   120      547   09 46 01

09 49 00  1228+126     11 55 06  69.8 153.3 -0.6     -23.3    41      547   09 49 00
09 59 00  ---          12 05 08  70.7 160.1 -0.4     -17.4   600      567   09 49 01

 ---------- U-band GRT-only VLBI scans - segment 09Ub ----------

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

10 00 00  1236+077     12 06 08  65.5 159.3 -0.6     -17.8    42      567   10 00 00
10 02 00  ---          12 08 08  65.6 160.5 -0.5     -16.9   120      570   10 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               The nuclear structure in nearby AGN
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Feb 2014   Day  36 ---

10 03 00  1228+126     12 09 08  71.0 163.0 -0.4     -14.9    42      570   10 03 00
10 09 00  ---          12 15 09  71.3 167.4 -0.3     -11.1   360      582   10 03 01

 ---------- Q-band GRT-only VLBI scans - segment 09Qb ----------

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

10 10 00  1236+077     12 16 09  66.1 165.2 -0.4     -12.8    42      582   10 10 00
10 12 00  ---          12 18 10  66.2 166.4 -0.4     -11.8   120      586   10 10 01

10 13 00  1228+126     12 19 10  71.5 170.4 -0.2      -8.4    42      586   10 13 00
10 19 00  ---          12 25 11  71.6 175.1 -0.1      -4.4   360      597   10 13 01

 ---------- Space segment 09: K-band VLBI scans ----------

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

10 20 00  1228+126     12 26 11  71.6 175.8 -0.1      -3.7    54      597   10 20 00
10 29 30  ---          12 35 43  71.6 183.2  0.1       2.8   570      616   10 20 01

10 30 00  1228+126     12 36 13  71.6 183.6  0.1       3.2    24      616   10 30 00
10 39 30  ---          12 45 44  71.4 190.9  0.2       9.6   570      634   10 30 01

10 40 00  1228+126     12 46 14  71.4 191.3  0.2       9.9    24      634   10 40 00
10 49 30  ---          12 55 46  70.8 198.3  0.4      16.0   570      652   10 40 01

10 50 00  1228+126     12 56 16  70.8 198.6  0.4      16.4    24      652   10 50 00
10 59 30  ---          13 05 47  70.0 205.2  0.6      22.0   570      670   10 50 01

11 00 00  1228+126     13 06 18  70.0 205.5  0.6      22.3    24      670   11 00 00
11 09 30  ---          13 15 49  69.0 211.6  0.7      27.5   570      689   11 00 01

11 10 00  1228+126     13 16 19  69.0 211.9  0.7      27.7    24      689   11 10 00
11 20 00  ---          13 26 21  67.7 217.6  0.9      32.5   600      708   11 10 01

 ---------- C/U/K/Q-band VLBA + GBT scans - segment 10 ----------

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

11 21 00  1228+126     13 27 21  67.6 218.2  0.9      33.0    54      708   11 21 00
11 26 00  ---          13 32 22  66.9 220.8  1.0      35.1   300      717   11 21 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               The nuclear structure in nearby AGN
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Feb 2014   Day  36 ---

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

11 26 30  1228+126     13 32 52  66.8 221.0  1.0      35.3    24      717   11 26 30
11 31 30  ---          13 37 53  66.1 223.5  1.1      37.3   300      727   11 26 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

11 32 00  1228+126     13 38 23  66.0 223.7  1.1      37.5    24      727   11 32 00
11 37 00  ---          13 43 24  65.3 226.1  1.2      39.4   300      737   11 32 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

11 37 30  1228+126     13 43 54  65.2 226.3  1.2      39.5    24      737   11 37 30
11 42 30  ---          13 48 55  64.4 228.5  1.3      41.3   300      746   11 37 31

 Next scan frequencies:  4836.00  4836.00  4836.00  4836.00
 Next BBC frequencies:    736.00   736.00   736.00   736.00

11 43 00  1226+023     13 49 25  55.7 217.1  1.3      31.3     5      746   11 43 00
11 46 00  ---          13 52 25  55.3 218.2  1.4      32.2   180      752   11 43 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

11 46 30  1226+023     13 52 55  55.2 218.4  1.4      32.4    24      752   11 46 30
11 49 30  ---          13 55 56  54.8 219.5  1.4      33.2   180      758   11 46 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

11 50 00  1226+023     13 56 26  54.8 219.7  1.4      33.4    24      758   11 50 00
11 53 00  ---          13 59 26  54.4 220.8  1.5      34.2   180      764   11 50 01

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

11 53 30  1226+023     13 59 56  54.3 221.0  1.5      34.4    24      764   11 53 30
11 56 30  ---          14 02 57  53.9 222.0  1.6      35.2   180      769   11 53 31

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

11 57 00  1228+126     14 03 27  62.0 234.2  1.5      45.6     6      769   11 57 00
12 02 00  ---          14 08 28  61.1 236.0  1.6      46.9   300      779   11 57 01

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

12 02 30  1228+126     14 08 58  61.0 236.2  1.6      47.0    24      779   12 02 30
12 07 30  ---          14 13 59  60.1 237.8  1.7      48.2   300      789   12 02 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               The nuclear structure in nearby AGN
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Wed   5 Feb 2014   Day  36 ---

 Next scan frequencies:  22236.00  22236.00  22236.00  22236.00
 Next BBC frequencies:     736.00    736.00    736.00    736.00

12 08 00  1228+126     14 14 29  60.0 238.0  1.7      48.3    24      789   12 08 00
12 13 00  ---          14 19 30  59.1 239.6  1.8      49.4   300      798   12 08 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

12 13 30  1228+126     14 20 00  59.0 239.7  1.8      49.5    24      798   12 13 30
12 18 30  ---          14 25 00  58.0 241.2  1.9      50.5   300      808   12 13 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

12 19 00  1228+126     14 25 31  57.9 241.4  1.9      50.6    24      808   12 19 00
12 24 00  ---          14 30 31  57.0 242.8  2.0      51.6   300      817   12 19 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

12 24 30  1228+126     14 31 01  56.9 243.0  2.0      51.7    24      817   12 24 30
12 29 30  ---          14 36 02  55.9 244.3  2.1      52.5   300      827   12 24 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

12 30 00  1228+126     14 36 32  55.8 244.5  2.1      52.6    24      827   12 30 00
12 35 00  ---          14 41 33  54.9 245.8  2.2      53.4   300      837   12 30 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

12 35 30  1228+126     14 42 03  54.8 245.9  2.2      53.5    24      837   12 35 30
12 40 30  ---          14 47 04  53.8 247.1  2.3      54.2   300      846   12 35 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

12 41 00  1228+126     14 47 34  53.7 247.2  2.3      54.3    24      846   12 41 00
12 46 00  ---          14 52 35  52.7 248.4  2.4      55.0   300      856   12 41 01

 Next scan frequencies:  15369.00  15369.00  15369.00  15369.00
 Next BBC frequencies:     769.00    769.00    769.00    769.00

12 46 30  1228+126     14 53 05  52.6 248.5  2.4      55.0    24      856   12 46 30
12 52 30  ---          14 59 06  51.4 249.9  2.5      55.8   360      867   12 46 31

 Next scan frequencies:  43120.00  43120.00  43136.00  43136.00
 Next BBC frequencies:     720.00    720.00    736.00    736.00

12 53 00  1228+126     14 59 36  51.3 250.0  2.5      55.8    24      867   12 53 00
12 59 00  ---          15 05 37  50.0 251.3  2.6      56.5   360      879   12 53 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: ra1cm2.set
   Matching groups in ./gs032c_freq_sess313rdbe.dat:
     v1cm_b3

   Setup group:   34         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  21500.00  21500.00  21500.00  21500.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     1cm      omit     1cm 
   VLBA Synth=   9.1     15.1     12.4

  The following frequency sets based on these setups were used.

   Frequency Set:  28  Setup file default.
   LO sum=   22236.00  22236.00  22236.00  22236.00
   BBC fr=     736.00    736.00    736.00    736.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  28  33  34  36  37  67  68  69  70  71

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra2cm2.set
   Matching groups in ./gs032c_freq_sess313rdbe.dat:
     v2cm_d3         Fourth 2cm filter

   Setup group:   57         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  14600.00  14600.00  14600.00  14600.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        B         D         B         D 

   VLBA FE=     omit     2cm      omit     2cm 
   VLBA Synth=  14.6     11.4     11.4

  The following frequency sets based on these setups were used.

   Frequency Set:  39  Setup file default.
   LO sum=   15369.00  15369.00  15369.00  15369.00
   BBC fr=     769.00    769.00    769.00    769.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  39  40  41  42  43  44  45  46  47  48

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra7mm2.set
   Matching groups in ./gs032c_freq_sess313rdbe.dat:
     v7mm_c8

   Setup group:   67         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=  15.1      7.6     11.6

  The following frequency sets based on these setups were used.

   Frequency Set:  49  Setup file default.
   LO sum=   43120.00  43120.00  43136.00  43136.00
   BBC fr=     720.00    720.00    736.00    736.00
   Bandwd=      16.00     16.00     16.00     16.00
    Matching frequency sets:  49  50  51  52  53  54  55  56  57  58

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 


 ======== Setup file: ra6cm2.set
   Matching groups in ./gs032c_freq_sess313rdbe.dat:
     vc_d

   Setup group:    7         Station: VLBA_FD           Total bit rate:   256
   Format: MARK5B            Bits per sample: 2         Sample rate: 32.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   4100.00   4100.00   4100.00   4100.00
   Net SB=         L         L         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4
   BBC SB=         L         L         U         U
   IF    =        A         C         A         C 

   VLBA FE=     6cm      omit     6cm      omit
   VLBA Synth=  15.1      4.1     15.1

  The following frequency sets based on these setups were used.

   Frequency Set:  27  Setup file default.
   LO sum=   4836.00  4836.00  4836.00  4836.00
   BBC fr=    736.00   736.00   736.00   736.00
   Bandwd=     16.00    16.00    16.00    16.00
    Matching frequency sets:  27  29  32  35  59  61  63  64  65  66

   Track assignments are: 
    track1=   2,  4,  6,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * FAKERA            11 57 21.769299   * 12 00 00.000000     12 00 48.003338       0.00
                     85 16 41.77889    * 85 00 00.00000      84 54 58.14016        0.00
                     From catalog imbedded in main SCHED input file.
                     fake circumpolar target for a TS to look at

   J1239+0730        12 36 52.308755   * 12 39 24.588327     12 40 08.812805       0.10
 * 1236+077          07 46 45.39997    * 07 30 17.18902      07 25 28.10329        0.11
   J1239+07          From catalog imbedded in main SCHED input file.
                     rfc_2012b Petrov, 2012, unpublished 1855 observations

 * 1226+023          12 26 33.245835   * 12 29 06.699731     12 29 51.363058       0.00
   J1229+0203        02 19 43.30547    * 02 03 08.59797      01 58 18.79035        0.00
   3C273B            ./gs032c_sources.radioastron
   3C273             AGN, rfc_2013d Petrov, 2013, unpublished 32011 observations

 * 1228+126          12 28 17.569280   * 12 30 49.423382     12 31 33.520344       0.00
   J1230+1223        12 40 01.74883    * 12 23 28.04365      12 18 35.78136        0.00
   3C274             ./gs032c_sources.radioastron
   M87               AGN, rfc_2013d Petrov, 2013, unpublished 55201 observations
   VIR-A



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  FAKERA     ra6cm2.set            11                                4.825     0.000
  1236+077   ra6cm2.set            1 2 3 4 11 13 16 17 18 19 2 +     1.333    27.967
             ra1cm2.set            5 8 9 10 14 15 21 25 26 28  +     1.200    31.800
             ra2cm2.set            39                                0.067     3.000
             ra7mm2.set            49                                0.067     3.000
  1226+023   ra6cm2.set            1 2 3 4 11 13 16 17 18 19 2 +     1.550    39.583
             ra1cm2.set            5 8 9 10 14 15 21 25 26 28  +     1.550    47.583
             ra2cm2.set            39                                0.050     2.250
             ra7mm2.set            49                                0.050     2.250
  1228+126   ra6cm2.set            1 2 3 4 11 13 16 17 18 19 2 +    15.742   317.813
             ra1cm2.set            5 8 9 10 14 15 21 25 26 28  +    14.357   328.818
             ra2cm2.set            39                                0.783    35.250
             ra7mm2.set            49                                0.783    35.250


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   FAKERA             109.8
   1236+077           129.1
   1226+023           130.0
   1228+126           132.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

