  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: Global VLBI observations
 Exp. Code:  GA043A  


Schedule Version:       4.00
Processed by SCHED version:  11.50  Development version 11.5. Started Apr. 2

PI:       Javier Alcolea

Address:  Observatorio Astronomico Nacional
          Calle Alfonso XII, 3
          28014 MADRID
          Spain

Phone:    +34 91 792 94 22
EMAIL:    j.alcolea@oan.es, desmurs@oan.es
Fax:      +34 91 527 19 35
Phone during observation: +34 91 792 94 34

Observing mode:

Notes:    This is a global line vlbi experiment at 7mm
          ** SWITCH PHAS CAL OFF ** please, thank you
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  24 Feb 2020   Day  55 ---

 ---------- 17:00 Start EVN+VLBA ----------

 Next scan frequencies:  42970.75  42970.75  43062.75  43062.75  43126.75  43126.75  43190.75  43190.75
 Next BBC frequencies:     570.75    570.75    662.75    662.75    726.75    726.75    790.75    790.75
 Next scan bandwidths:      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00

17 00 00  0221+067     20 20 24   2.5  83.3 -6.1  H  -59.4     0        0   17 00 00
17 03 00  ---          20 23 25   3.1  83.6 -6.0  H  -59.5     0       46   17 00 01

17 07 41  OCETI        20 28 06   0.2  93.5 -5.9  D  -59.3   266       46   17 07 41
17 18 41  ---          20 39 08   2.6  94.9 -5.7  H  -59.1     0      216   17 07 42

17 18 57  OCETI        20 39 24   2.6  94.9 -5.7  H  -59.1    10      216   17 18 57
17 29 57  ---          20 50 26   5.0  96.3 -5.5  H  -58.9     0      386   17 18 58

17 30 30  J0215-02     20 50 59   6.2  96.4 -5.4     -58.8    23      386   17 30 30
17 33 30  ---          20 53 59   6.8  96.8 -5.4     -58.8   180      433   17 30 31

17 34 02  OCETI        20 54 32   5.9  96.9 -5.4     -58.8    22      433   17 34 02
17 45 02  ---          21 05 33   8.2  98.3 -5.2     -58.5   660      603   17 34 03

17 45 18  OCETI        21 05 49   8.3  98.4 -5.2     -58.5    10      603   17 45 18
17 56 18  ---          21 16 51  10.6  99.8 -5.1     -58.1   660      773   17 45 19

17 56 51  J0215-02     21 17 24  11.8  99.9 -5.0     -58.0    23      773   17 56 51
17 59 51  ---          21 20 25  12.4 100.3 -4.9     -57.9   180      819   17 56 52

18 00 23  OCETI        21 20 57  11.5 100.4 -5.0     -57.9    22      819   18 00 23
18 12 23  ---          21 32 59  14.0 102.0 -4.8     -57.4   720     1005   18 00 24

 ---------- Start Block I EVN+VLBA+GBT (33min) ----------

18 20 00  J0215-02     21 40 37  16.7 103.1 -4.6     -57.0   447     1005   18 20 00
18 23 00  ---          21 43 38  17.3 103.5 -4.6     -56.9   180     1051   18 20 01

18 23 00  OCETI        21 43 38  16.2 103.5 -4.6     -56.9   -10     1051   18 23 10
18 28 00  ---          21 48 38  17.3 104.2 -4.5     -56.6   290     1126   18 23 01

18 28 00  OCETI        21 48 38  17.3 104.2 -4.5     -56.6    -6     1126   18 28 06
18 33 00  ---          21 53 39  18.3 105.0 -4.4     -56.3   294     1202   18 28 01

18 33 00  OCETI        21 53 39  18.3 105.0 -4.4     -56.3    -6     1202   18 33 06
18 38 00  ---          21 58 40  19.4 105.7 -4.4     -56.0   294     1277   18 33 01

18 38 30  J0215-02     21 59 10  20.6 105.8 -4.3     -56.0    20     1277   18 38 30
18 43 00  ---          22 03 41  21.5 106.5 -4.2     -55.7   270     1347   18 38 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  24 Feb 2020   Day  55 ---

18 43 00  OCETI        22 03 41  20.4 106.4 -4.3     -55.7   -10     1347   18 43 10
18 48 00  ---          22 08 42  21.4 107.2 -4.2     -55.4   290     1422   18 43 01

18 48 00  OCETI        22 08 42  21.4 107.2 -4.2     -55.4    -6     1422   18 48 06
18 53 00  ---          22 13 43  22.5 108.0 -4.1     -55.0   294     1497   18 48 01

 ---------- Eff: Gap of ~10min for pointing at Eff (P_Eff-3). Observe: VLBA+Yb+On60 ----------

18 53 15  OCETI        22 13 58  22.5 108.0 -4.1     -55.0     9     1497   18 53 15
19 01 15  ---          22 21 59  24.2 109.3 -4.0     -54.4   480     1621   18 53 16

 ---------- Start Block II EVN+VLBA+GBT (33min) ----------

19 07 00  J0215-02     22 27 45  26.4 110.2 -3.8     -53.9   335     1621   19 07 00
19 10 00  ---          22 30 45  27.0 110.7 -3.8     -53.6   180     1667   19 07 01

19 10 00  OCETI        22 30 45  25.9 110.7 -3.8     -53.7   -10     1667   19 10 10
19 15 00  ---          22 35 46  26.9 111.5 -3.7     -53.3   290     1742   19 10 01

19 15 00  OCETI        22 35 46  26.9 111.5 -3.7     -53.3    -6     1742   19 15 06
19 20 00  ---          22 40 47  27.9 112.4 -3.7     -52.8   294     1818   19 15 01

19 20 00  OCETI        22 40 47  27.9 112.4 -3.7     -52.8    -6     1818   19 20 06
19 25 00  ---          22 45 48  28.9 113.2 -3.6     -52.3   294     1894   19 20 01

19 25 30  J0215-02     22 46 18  30.1 113.4 -3.5     -52.2    20     1894   19 25 30
19 30 00  ---          22 50 49  31.0 114.2 -3.4     -51.8   270     1963   19 25 31

19 30 00  OCETI        22 50 49  29.9 114.1 -3.5     -51.8   -10     1963   19 30 10
19 35 00  ---          22 55 49  30.9 115.0 -3.4     -51.3   290     2038   19 30 01

19 35 00  OCETI        22 55 49  30.9 115.0 -3.4     -51.3    -6     2038   19 35 06
19 40 00  ---          23 00 50  31.9 115.9 -3.3     -50.8   294     2114   19 35 01

 ---------- Observe : VLBA+EVN ----------

19 40 16  OCETI        23 01 06  31.9 116.0 -3.3     -50.8    10     2114   19 40 16
19 51 16  ---          23 12 08  34.0 118.1 -3.1     -49.5   660     2284   19 40 17

 ---------- Start Block III EVN+VLBA+GBT (33min) ----------

19 52 00  J0215-02     23 12 52  35.3 118.4 -3.1     -49.2    34     2284   19 52 00
19 55 00  ---          23 15 53  35.8 119.0 -3.0     -48.9   180     2330   19 52 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  24 Feb 2020   Day  55 ---

 ---------- End EVN at 20h00 ----------

19 55 00  OCETI        23 15 53  34.8 118.8 -3.1     -49.0   -10     2330   19 55 10
20 00 00  ---          23 20 54  35.7 119.8 -3.0     -48.4   290     2405   19 55 01

20 00 00  OCETI        23 20 54  35.7 119.8 -3.0     -48.4    -6     2405   20 00 06
20 05 00  ---          23 25 54  36.6 120.9 -2.9     -47.7   294     2481   20 00 01

20 05 00  OCETI        23 25 54  36.6 120.9 -2.9     -47.7    -6     2481   20 05 06
20 10 00  ---          23 30 55  37.5 121.9 -2.8     -47.0   294     2556   20 05 01

20 10 00  J0215-02     23 30 55  38.6 122.2 -2.8     -46.8   -10     2556   20 10 10
20 15 00  ---          23 35 56  39.5 123.3 -2.7     -46.0   290     2631   20 10 01

20 15 00  OCETI        23 35 56  38.5 123.0 -2.7     -46.2   -10     2631   20 15 10
20 20 00  ---          23 40 57  39.4 124.2 -2.7     -45.5   290     2706   20 15 01

20 20 00  OCETI        23 40 57  39.4 124.2 -2.7     -45.5    -6     2706   20 20 06
20 25 00  ---          23 45 58  40.2 125.3 -2.6     -44.7   294     2781   20 20 01

 ---------- Observe : VLBA ----------

20 25 06  OCETI        23 46 04  40.3 125.3 -2.6     -44.7     0     2781   20 25 06
20 34 06  ---          23 55 05  41.8 127.5 -2.4     -43.1   540     2921   20 25 01

 ---------- Start Block IV VLBA+GBT (33min) ----------

20 35 00  J0215-02     23 55 59  43.0 128.1 -2.3     -42.7    44     2921   20 35 00
20 38 00  ---          23 59 00  43.5 128.8 -2.3     -42.1   180     2967   20 35 01

20 38 00  OCETI        23 59 00  42.5 128.4 -2.4     -42.4   -10     2967   20 38 10
20 43 00  ---          00 04 01  43.3 129.7 -2.3     -41.5   290     3042   20 38 01

20 43 00  OCETI        00 04 01  43.3 129.7 -2.3     -41.5    -6     3042   20 43 06
20 48 00  ---          00 09 01  44.1 131.0 -2.2     -40.5   294     3117   20 43 01

20 48 00  OCETI        00 09 01  44.1 131.0 -2.2     -40.5    -6     3117   20 48 06
20 53 00  ---          00 14 02  44.9 132.4 -2.1     -39.5   294     3193   20 48 01

20 53 00  J0215-02     00 14 02  46.0 132.8 -2.0     -39.2   -10     3193   20 53 10
20 58 00  ---          00 19 03  46.8 134.2 -2.0     -38.1   290     3268   20 53 01

20 58 00  OCETI        00 19 03  45.7 133.7 -2.0     -38.5   -10     3268   20 58 10
21 03 00  ---          00 24 04  46.5 135.2 -1.9     -37.4   290     3343   20 58 01
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  24 Feb 2020   Day  55 ---

21 03 00  OCETI        00 24 04  46.5 135.2 -1.9     -37.4    -6     3343   21 03 06
21 08 00  ---          00 29 05  47.3 136.6 -1.9     -36.3   294     3418   21 03 01

 ---------- Observe : VLBA ----------

21 08 06  OCETI        00 29 11  47.3 136.7 -1.9     -36.2     0     3418   21 08 06
21 17 06  ---          00 38 12  48.6 139.4 -1.7     -34.1   540     3557   21 08 01

 ---------- Start Block V VLBA+GBT (33min) ----------

21 18 00  0420-014     00 39 06  27.8 110.0 -3.8     -54.0     5     3557   21 18 00
21 21 00  ---          00 42 07  28.4 110.5 -3.7     -53.7   180     3604   21 18 01

21 25 00  J0215-02     00 46 08  50.6 142.7 -1.5     -31.5   189     3604   21 25 00
21 28 00  ---          00 49 08  51.0 143.7 -1.5     -30.7   180     3650   21 25 01

21 28 00  OCETI        00 49 08  50.0 142.9 -1.5     -31.3   -10     3650   21 28 10
21 33 00  ---          00 54 09  50.7 144.6 -1.4     -29.9   290     3725   21 28 01

21 33 00  OCETI        00 54 09  50.7 144.6 -1.4     -29.9    -6     3725   21 33 06
21 38 00  ---          00 59 10  51.3 146.4 -1.4     -28.5   294     3801   21 33 01

21 38 00  J0215-02     00 59 10  52.2 147.2 -1.3     -27.8   -10     3801   21 38 10
21 43 00  ---          01 04 11  52.8 149.0 -1.2     -26.3   290     3875   21 38 01

21 43 00  OCETI        01 04 11  51.9 148.1 -1.3     -27.0   -10     3875   21 43 10
21 48 00  ---          01 09 11  52.4 150.0 -1.2     -25.5   290     3950   21 43 01

21 48 00  OCETI        01 09 11  52.4 150.0 -1.2     -25.5    -6     3950   21 48 06
21 53 00  ---          01 14 12  53.0 151.9 -1.1     -24.0   294     4026   21 48 01

 ---------- Observe : VLBA ----------

21 53 06  OCETI        01 14 18  53.0 151.9 -1.1     -23.9     0     4026   21 53 06
22 02 06  ---          01 23 20  53.8 155.4 -1.0     -21.0   540     4165   21 53 01

 ---------- Start Block VI VLBA+GBT (33min) ----------

22 05 00  J0215-02     01 26 14  54.9 157.7 -0.8     -19.1   164     4165   22 05 00
22 08 00  ---          01 29 15  55.2 158.9 -0.8     -18.0   180     4211   22 05 01

22 08 00  OCETI        01 29 15  54.3 157.7 -0.9     -19.0   -10     4211   22 08 10
22 13 00  ---          01 34 15  54.7 159.8 -0.8     -17.3   290     4286   22 08 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  24 Feb 2020   Day  55 ---

22 13 00  OCETI        01 34 15  54.7 159.8 -0.8     -17.3    -6     4286   22 13 06
22 18 00  ---          01 39 16  55.1 161.9 -0.7     -15.5   294     4362   22 13 01

22 18 00  OCETI        01 39 16  55.1 161.9 -0.7     -15.5    -6     4362   22 18 06
22 23 00  ---          01 44 17  55.4 164.0 -0.6     -13.7   294     4438   22 18 01

22 23 00  J0215-02     01 44 17  56.2 165.3 -0.5     -12.6   -10     4438   22 23 10
22 28 00  ---          01 49 18  56.4 167.6 -0.5     -10.7   290     4512   22 23 01

22 28 00  OCETI        01 49 18  55.7 166.2 -0.5     -11.9    -9     4512   22 28 09
22 33 00  ---          01 54 19  55.9 168.4 -0.4     -10.0   291     4587   22 28 01

22 33 00  OCETI        01 54 19  55.9 168.4 -0.4     -10.0    -6     4587   22 33 06
22 38 00  ---          01 59 20  56.1 170.6 -0.4      -8.1   294     4663   22 33 01

 ---------- Observe : VLBA ----------

22 38 06  OCETI        01 59 26  56.1 170.6 -0.3      -8.1     0     4663   22 38 06
22 47 06  ---          02 08 27  56.4 174.6 -0.2      -4.6   540     4802   22 38 01

 ---------- Start Block VII VLBA+GBT (33min) ----------

22 48 00  0420-014     02 09 21  44.7 128.6 -2.2     -42.3    13     4802   22 48 00
22 51 00  ---          02 12 22  45.2 129.4 -2.2     -41.7   180     4848   22 48 01

22 55 00  J0215-02     02 16 22  57.1 179.9 -0.0      -0.1   197     4848   22 55 00
22 58 00  ---          02 19 23  57.1 181.2  0.0       1.1   180     4895   22 55 01

22 58 00  OCETI        02 19 23  56.5 179.6 -0.0      -0.4    -9     4895   22 58 09
23 03 00  ---          02 24 24  56.5 181.8  0.1       1.6   291     4970   22 58 01

23 03 00  OCETI        02 24 24  56.5 181.8  0.1       1.6    -6     4970   23 03 06
23 08 00  ---          02 29 24  56.4 184.1  0.2       3.5   294     5046   23 03 01

23 08 00  J0215-02     02 29 24  56.9 185.8  0.2       5.0    -9     5046   23 08 09
23 13 00  ---          02 34 25  56.8 188.1  0.3       7.0   291     5121   23 08 01

23 13 00  OCETI        02 34 25  56.3 186.3  0.2       5.5    -9     5121   23 13 09
23 18 00  ---          02 39 26  56.2 188.6  0.3       7.4   291     5196   23 13 01

23 18 00  OCETI        02 39 26  56.2 188.6  0.3       7.4    -6     5196   23 18 06
23 23 00  ---          02 44 27  56.0 190.8  0.4       9.3   294     5271   23 18 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Mon  24 Feb 2020   Day  55 ---

 ---------- Observe : VLBA ----------

23 23 06  OCETI        02 44 33  56.0 190.8  0.4       9.3     0     5271   23 23 06
23 32 06  ---          02 53 34  55.6 194.8  0.6      12.7   540     5410   23 23 01

 ---------- Start Block VIII VLBA+GBT (33min) ----------

23 33 00  J0215-02     02 54 29  55.9 197.0  0.6      14.6    45     5410   23 33 00
23 36 00  ---          02 57 29  55.7 198.3  0.7      15.7   180     5457   23 33 01

23 36 00  OCETI        02 57 29  55.3 196.5  0.6      14.1    -9     5457   23 36 09
23 41 00  ---          03 02 30  55.0 198.6  0.7      15.9   291     5532   23 36 01

23 41 00  OCETI        03 02 30  55.0 198.6  0.7      15.9    -6     5532   23 41 06
23 46 00  ---          03 07 31  54.6 200.7  0.8      17.7   294     5607   23 41 01

23 46 00  OCETI        03 07 31  54.6 200.7  0.8      17.7    -6     5607   23 46 06
23 51 00  ---          03 12 32  54.2 202.7  0.9      19.4   294     5683   23 46 01

23 51 00  J0215-02     03 12 32  54.5 204.5  0.9      20.9    -9     5683   23 51 09
23 56 00  ---          03 17 32  54.0 206.5  1.0      22.6   291     5758   23 51 01

 --- Start: Mon  24 Feb 2020   Day  55 -- Stop: Tue  25 Feb 2020   Day  56 ---

23 56 00  OCETI        03 17 32  53.8 204.7  1.0      21.1    -9     5758   23 56 09
00 01 00  ---          03 22 33  53.3 206.6  1.0      22.7   291     5833   23 56 01

00 01 00  OCETI        03 22 33  53.3 206.6  1.0      22.7    -6     5833   00 01 06
00 06 00  ---          03 27 34  52.8 208.6  1.1      24.3   294     5909   00 01 01

 ---------- Observe : VLBA ----------

00 06 06  OCETI        03 27 40  52.8 208.6  1.1      24.4     0     5909   00 06 06
00 15 06  ---          03 36 42  51.9 211.9  1.3      27.1   540     6048   00 06 01

 ---------- Start Block IX VLBA+GBT (33min) ----------

00 16 00  0420-014     03 37 36  56.2 158.7 -0.8     -18.2     8     6048   00 16 00
00 19 00  ---          03 40 36  56.4 160.0 -0.7     -17.1   180     6094   00 16 01

00 23 00  J0215-02     03 44 37  51.0 216.4  1.5      30.8   193     6094   00 23 00
00 26 00  ---          03 47 37  50.6 217.5  1.5      31.6   180     6141   00 23 01

00 26 00  OCETI        03 47 37  50.5 215.7  1.5      30.2    -9     6141   00 26 09
00 31 00  ---          03 52 38  49.9 217.4  1.5      31.6   291     6216   00 26 01
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Feb 2020   Day  56 ---

00 31 00  OCETI        03 52 38  49.9 217.4  1.5      31.6    -6     6216   00 31 06
00 36 00  ---          03 57 39  49.2 219.1  1.6      32.9   294     6292   00 31 01

00 36 00  J0215-02     03 57 39  49.2 220.7  1.7      34.2    -9     6292   00 36 09
00 41 00  ---          04 02 40  48.5 222.3  1.8      35.4   291     6367   00 36 01

00 41 00  OCETI        04 02 40  48.5 220.6  1.7      34.1    -9     6367   00 41 09
00 46 00  ---          04 07 41  47.8 222.2  1.8      35.3   291     6441   00 41 01

00 46 00  OCETI        04 07 41  47.8 222.2  1.8      35.3    -6     6441   00 46 06
00 51 00  ---          04 12 41  47.1 223.7  1.9      36.5   294     6517   00 46 01

 ---------- Observe : VLBA ----------

00 51 06  OCETI        04 12 47  47.1 223.7  1.9      36.5     0     6517   00 51 06
01 00 06  ---          04 21 49  45.7 226.3  2.0      38.5   540     6656   00 51 01

 ---------- Start Block X VLBA+GBT (33min) ----------

01 01 00  J0215-02     04 22 43  45.4 228.1  2.1      39.9    45     6656   01 01 00
01 04 00  ---          04 25 44  45.0 228.9  2.2      40.5   180     6703   01 01 01

01 04 00  OCETI        04 25 44  45.1 227.4  2.1      39.3    -9     6703   01 04 09
01 09 00  ---          04 30 44  44.3 228.7  2.2      40.4   291     6778   01 04 01

01 09 00  OCETI        04 30 44  44.3 228.7  2.2      40.4    -6     6778   01 09 06
01 14 00  ---          04 35 45  43.5 230.0  2.3      41.3   294     6853   01 09 01

01 14 00  OCETI        04 35 45  43.5 230.0  2.3      41.3    -6     6853   01 14 06
01 19 00  ---          04 40 46  42.6 231.3  2.3      42.3   294     6929   01 14 01

01 19 00  J0215-02     04 40 46  42.5 232.8  2.4      43.3    -9     6929   01 19 09
01 24 00  ---          04 45 47  41.6 234.0  2.5      44.2   291     7004   01 19 01

01 24 00  OCETI        04 45 47  41.8 232.6  2.4      43.2    -9     7004   01 24 09
01 29 00  ---          04 50 48  40.9 233.8  2.5      44.0   291     7079   01 24 01

01 29 00  OCETI        04 50 48  40.9 233.8  2.5      44.0    -6     7079   01 29 06
01 34 00  ---          04 55 48  40.0 235.0  2.6      44.9   294     7155   01 29 01

 ---------- Observe : VLBA ----------

01 34 06  OCETI        04 55 54  40.0 235.0  2.6      44.9     0     7155   01 34 06
01 43 06  ---          05 04 56  38.4 237.0  2.7      46.3   540     7294   01 34 01
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Feb 2020   Day  56 ---

01 43 16  J0215-02     05 05 06  38.1 238.4  2.8      47.2     1     7294   01 43 15
01 46 16  ---          05 08 06  37.6 239.0  2.9      47.6   180     7341   01 43 07

 ----------  AUTOPHASING VLA continuously, is it possible ?? ----------

01 47 27  0420-014     05 09 18  56.3 200.6  0.8      17.6    26     7341   01 47 27
01 50 27  ---          05 12 18  56.1 201.9  0.8      18.7   180     7387   01 47 28

 ----------  VLBA+GBT: 2 last scans ----------

01 52 20  OCETI        05 14 11  36.7 239.0  2.9      47.6    67     7387   01 52 20
01 56 20  ---          05 18 12  36.0 239.8  3.0      48.1   240     7449   01 52 21

 ---------- GBT : Last scans. Start last hour with VLBA ----------

01 56 49  J0215-02     05 18 41  35.6 241.2  3.0      49.0    21     7449   01 56 49
01 59 49  ---          05 21 42  35.0 241.8  3.1      49.4   180     7495   01 56 50

01 59 59  OCETI        05 21 51  35.3 240.6  3.0      48.6     1     7495   01 59 58
02 10 29  ---          05 32 23  33.3 242.7  3.2      49.9   630     7658   01 59 50

02 10 38  J0215-02     05 32 33  33.0 243.9  3.3      50.7     1     7658   02 10 37
02 13 38  ---          05 35 33  32.4 244.5  3.3      51.0   180     7704   02 10 30

02 13 47  OCETI        05 35 42  32.7 243.3  3.3      50.3     1     7704   02 13 47
02 24 17  ---          05 46 14  30.6 245.2  3.4      51.5   630     7867   02 13 39

02 24 27  J0215-02     05 46 24  30.3 246.5  3.5      52.1     1     7867   02 24 26
02 27 27  ---          05 49 24  29.7 247.0  3.5      52.4   180     7914   02 24 18

02 27 37  OCETI        05 49 34  30.0 245.8  3.5      51.8     1     7914   02 27 36
02 38 07  ---          06 00 06  27.9 247.7  3.7      52.8   630     8076   02 27 28

02 38 16  J0215-02     06 00 15  27.5 248.9  3.7      53.4     1     8076   02 38 15
02 41 16  ---          06 03 16  26.9 249.4  3.8      53.7   180     8123   02 38 08

02 41 26  OCETI        06 03 26  27.2 248.2  3.7      53.1     1     8123   02 41 25
02 51 56  ---          06 13 57  25.1 250.0  3.9      54.0   630     8285   02 41 17

02 52 06  J0215-02     06 14 07  24.7 251.1  4.0      54.6     1     8285   02 52 05
02 55 06  ---          06 17 08  24.1 251.6  4.0      54.8   180     8332   02 51 57
Schedule for VLBA_FD   (Code Fd )                                   Page  10
               Global VLBI observations
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Tue  25 Feb 2020   Day  56 ---

 ---------- 03:00 : Last scan VLBA, End Project ----------

02 56 03  0420-014     06 18 05  48.1 225.5  1.9      37.9     2     8332   02 56 03
02 59 03  ---          06 21 06  47.7 226.4  1.9      38.6   180     8378   02 56 04


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess120.Q2048globGA43A
   Matching groups in /home/guest/rmc/SCHED/sched11.5/catalogs/freq_RDBE.dat:
     v7mm_c8

   Setup group:    4         Station: VLBA_FD           Total bit rate:  2048
   Format: VDIF              Bits per sample: 2         Sample rate:128.000
   Number of channels:  8    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00  42400.00
   Net SB=         U         U         U         U         U         U         U         U
   IF SB =         U         U         U         U         U         U         U         U
   Pol.  =      RCP       LCP       RCP       LCP       RCP       LCP       RCP       LCP 
   BBC   =         1         2         3         4         5         6         7         8
   BBC SB=         U         U         U         U         U         U         U         U
   IF    =        A         C         A         C         A         C         A         C 

   VLBA FE=     7mm      omit     7mm      omit
   VLBA Synth=   3.9      7.6     11.6

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:   4  Setup file default.  Used with PCAL = off
   LO sum=   42970.75  42970.75  43062.75  43062.75  43126.75  43126.75  43190.75  43190.75
   BBC fr=     570.75    570.75    662.75    662.75    726.75    726.75    790.75    790.75
   Bandwd=      64.00     64.00     64.00     64.00     64.00     64.00     64.00     64.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   3  4  5  6
   CRD fr=     686.75    686.75    750.75    750.75
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:   4   5   6   7   8   9  10  14  15  16

   Track assignments are: 
    track1=   1,  2,  3,  4,  5,  6,  7,  8
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * OCETI             02 16 49.081086   * 02 19 20.792102     02 20 20.395861       0.00
                    -03 12 25.22156    *-02 58 39.49561     -02 53 22.26368        0.00
                     From catalog imbedded in main SCHED input file.

 * 0420-014          04 20 43.539847   * 04 23 15.800724     04 24 16.299585       0.00
   J0423-0120       -01 27 28.70032    *-01 20 33.06561     -01 17 59.21821        0.00
   J0423-01          From catalog imbedded in main SCHED input file.
                     GSFC 2016a X/S astro solution,  73969 observations.

   0213-026          02 13 09.874050   * 02 15 42.017290     02 16 41.775763       0.04
   J0215-0222       -02 36 51.41463    *-02 22 56.75272     -02 17 35.75526        0.09
 * J0215-02          From catalog imbedded in main SCHED input file.
                     GSFC 2016a X/S astro solution,    281 observations.

 * 0215+015          02 15 14.130233   * 02 17 48.954753     02 18 49.801318       0.01
   J0217+0144        01 31 00.16091    * 01 44 49.69901      01 50 09.84309        0.01
   J0217+01          From catalog imbedded in main SCHED input file.
                     GSFC 2016a X/S astro solution,  16209 observations.

 * 3C48              01 34 49.826446   * 01 37 41.299512     01 38 48.554668       0.55
   J0137+3309        32 54 20.25968    * 33 09 35.13386      33 15 38.61842        0.56
   0134+329          From catalog imbedded in main SCHED input file.
   J0137+33          GSFC 2016a X/S astro solution,     90 observations.

 * 0221+067          02 21 49.960395   * 02 24 28.428193     02 25 30.768296       0.02
   J0224+0659        06 45 50.43663    * 06 59 23.34146      07 04 38.41782        0.02
   J0224+06          /home/guest/rmc/SCHED/sched11.5/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,   2444 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  OCETI      ess120.Q2048globGA43A 1 2 3 4 11 13                    13.017   347.270
  0420-014   ess120.Q2048globGA43A 1 2 3 4 11 13                     0.725    15.175
             ps/vla_x_pointing.set 12                                0.300     0.000
  J0215-02   ess120.Q2048globGA43A 1 2 3 4 11 13                     5.750    89.936
             ps/vla_x_pointing.set 12                                0.700     0.000
  0215+015   ps/vla_x_pointing.set 12                                0.200     0.000
  3C48       ess120.Q2048globGA43A 11                                0.067     0.000
             ps/vla_x_pointing.set 12                                0.050     0.000
  0221+067   ess120.Q2048globGA43A 1 2 3 4                           0.050     0.696

 POSITIONS OF ADDITIONAL SOURCES USED ONLY IN NON-RECORDING SCANS

     An unused dummy source of a scan that becomes a geodetic segment will show up here.

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 0202+149          02 02 07.396227   * 02 04 50.413895     02 05 54.473095       0.20
   J0204+1514        14 59 50.93938    * 15 14 11.04360      15 19 47.50987        0.33
   J0204+15          /home/guest/rmc/SCHED/sched11.5/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  35637 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   OCETI               57.6
   0420-014            88.4
   J0215-02            56.8
   0215+015            58.1
   3C48                62.0
   0202+149            59.0
   0221+067            61.0

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

