  COVER INFORMATION 

 Station:    VLBA_FD   (Code Fd ) 
 Experiment: JUNO tracking
 Exp. Code:  gd023d  


Schedule Version:       1.00
Processed by SCHED version:  11.60  Release 11.6; April 2020

PI:       Dominic Dirkx

Address:  DELFT
 
 
 

Phone:    +31 521 596545
EMAIL:    D.Dirkx@tudelft.nl
Fax:
Phone during observation:

Observing mode:

Notes:    JUNO freq. 8403.5
 
 
 

Schedule for VLBA_FD   (Code Fd )                                   Page   2
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   3 Feb 2024   Day  34 ---

 Next scan frequencies:  8400.00  8432.00  8464.00  8496.00
 Next BBC frequencies:    800.00   832.00   864.00   896.00
 Next scan bandwidths:     32.00    32.00    32.00    32.00

19 30 00  J0238+1636   21 28 08  18.6  81.2 -5.2     -62.6     0        0   19 30 00
19 33 00  =0235+164    21 31 09  19.2  81.5 -5.1     -62.7   180       12   19 30 01

19 34 00  J0213+1213   21 32 09  22.9  88.9 -4.7     -61.7    45       12   19 34 00
19 36 00  =0210+119    21 34 09  23.3  89.1 -4.7     -61.7   120       19   19 34 01

19 37 00  J0225+1134   21 35 10  20.5  88.3 -4.9     -61.4    46       19   19 37 00
19 38 30  =0223+113    21 36 40  20.8  88.5 -4.8     -61.4    90       25   19 37 01

19 39 00  031940       21 37 10  22.6  87.8 -4.8     -62.0    19       25   19 39 00
19 42 00  ---          21 40 10  23.3  88.2 -4.7     -62.0   180       37   19 39 01

19 43 00  J0225+1134   21 41 11  21.8  89.0 -4.8     -61.5    49       37   19 43 00
19 44 30  =0223+113    21 42 41  22.1  89.2 -4.7     -61.5    90       43   19 43 01

19 45 30  J0213+1213   21 43 41  25.4  90.3 -4.5     -61.7    46       43   19 45 30
19 47 30  =0210+119    21 45 41  25.8  90.6 -4.5     -61.7   120       50   19 45 31

19 48 00  031940       21 46 11  24.6  89.0 -4.6     -62.0    19       50   19 48 00
19 51 00  ---          21 49 12  25.2  89.3 -4.5     -62.0   180       62   19 48 01

19 52 00  J0213+1213   21 50 12  26.8  91.2 -4.4     -61.7    49       62   19 52 00
19 54 00  =0210+119    21 52 12  27.2  91.4 -4.4     -61.7   120       70   19 52 01

19 54 30  032000       21 52 42  26.0  89.8 -4.5     -62.0    19       70   19 54 30
19 57 30  ---          21 55 43  26.6  90.2 -4.4     -62.0   180       81   19 54 31

19 58 30  J0213+1213   21 56 43  28.2  92.0 -4.3     -61.7    49       81   19 58 30
20 00 30  =0210+119    21 58 43  28.6  92.3 -4.3     -61.6   120       89   19 58 31

20 01 00  032000       21 59 13  27.4  90.6 -4.4     -62.0    19       89   20 01 00
20 04 00  ---          22 02 14  28.0  91.0 -4.3     -62.0   180      100   20 01 01

20 05 00  J0213+1213   22 03 14  29.6  92.9 -4.2     -61.6    49      100   20 05 00
20 07 00  =0210+119    22 05 14  30.0  93.2 -4.2     -61.6   120      108   20 05 01

20 07 30  032000       22 05 45  28.8  91.4 -4.3     -62.0    19      108   20 07 30
20 10 30  ---          22 08 45  29.4  91.8 -4.2     -62.0   180      120   20 07 31

20 11 30  J0213+1213   22 09 45  31.0  93.8 -4.1     -61.5    49      120   20 11 30
20 13 30  =0210+119    22 11 46  31.4  94.0 -4.0     -61.5   120      128   20 11 31
Schedule for VLBA_FD   (Code Fd )                                   Page   3
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   3 Feb 2024   Day  34 ---

20 14 00  032020       22 12 16  30.2  92.3 -4.2     -62.0    19      128   20 14 00
20 17 00  ---          22 15 16  30.8  92.7 -4.1     -61.9   180      139   20 14 01

20 18 00  J0213+1213   22 16 16  32.4  94.7 -4.0     -61.4    49      139   20 18 00
20 20 00  =0210+119    22 18 17  32.8  94.9 -3.9     -61.3   120      147   20 18 01

20 20 30  032020       22 18 47  31.6  93.2 -4.1     -61.9    19      147   20 20 30
20 23 30  ---          22 21 47  32.2  93.6 -4.0     -61.8   180      158   20 20 31

20 24 30  J0213+1213   22 22 47  33.7  95.6 -3.9     -61.2    49      158   20 24 30
20 26 30  =0210+119    22 24 48  34.2  95.9 -3.8     -61.2   120      166   20 24 31

20 27 00  032020       22 25 18  33.0  94.1 -3.9     -61.8    19      166   20 27 00
20 30 00  ---          22 28 18  33.6  94.5 -3.9     -61.7   180      178   20 27 01

20 31 00  J0213+1213   22 29 18  35.1  96.5 -3.8     -61.1    49      178   20 31 00
20 33 00  =0210+119    22 31 19  35.6  96.8 -3.7     -61.0   120      185   20 31 01

20 33 30  032040       22 31 49  34.4  95.0 -3.8     -61.6    19      185   20 33 30
20 36 30  ---          22 34 49  35.0  95.4 -3.8     -61.6   180      197   20 33 31

20 37 30  J0213+1213   22 35 49  36.5  97.5 -3.6     -60.8    49      197   20 37 30
20 39 30  =0210+119    22 37 50  37.0  97.8 -3.6     -60.8   120      205   20 37 31

20 40 00  032040       22 38 20  35.8  95.9 -3.7     -61.5    19      205   20 40 00
20 43 00  ---          22 41 20  36.4  96.3 -3.7     -61.4   180      216   20 40 01

20 44 00  J0213+1213   22 42 21  37.9  98.4 -3.5     -60.6    49      216   20 44 00
20 46 00  =0210+119    22 44 21  38.3  98.7 -3.5     -60.5   120      224   20 44 01

20 46 30  032040       22 44 51  37.1  96.8 -3.6     -61.3    19      224   20 46 30
20 49 30  ---          22 47 51  37.8  97.3 -3.6     -61.2   180      236   20 46 31

20 50 30  J0213+1213   22 48 52  39.3  99.4 -3.4     -60.3    49      236   20 50 30
20 52 30  =0210+119    22 50 52  39.7  99.8 -3.4     -60.2   120      243   20 50 31

20 53 30  J0225+1134   22 51 52  36.9  98.7 -3.6     -60.3    46      243   20 53 30
20 55 30  =0223+113    22 53 52  37.4  99.0 -3.6     -60.2   120      251   20 53 31

20 56 00  032100       22 54 23  39.2  98.2 -3.5     -61.0    19      251   20 56 00
20 59 00  ---          22 57 23  39.8  98.7 -3.4     -60.8   180      263   20 56 01

21 00 00  J0225+1134   22 58 23  38.3  99.7 -3.5     -60.0    49      263   21 00 00
21 02 00  =0223+113    23 00 24  38.8 100.0 -3.4     -59.9   120      271   21 00 01
Schedule for VLBA_FD   (Code Fd )                                   Page   4
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   3 Feb 2024   Day  34 ---

21 03 00  J0213+1213   23 01 24  42.0 101.5 -3.2     -59.7    46      271   21 03 00
21 05 00  =0210+119    23 03 24  42.4 101.8 -3.2     -59.6   120      278   21 03 01

21 05 30  032100       23 03 54  41.2  99.7 -3.3     -60.5    19      278   21 05 30
21 08 30  ---          23 06 55  41.8 100.2 -3.3     -60.4   180      290   21 05 31

21 09 30  J0213+1213   23 07 55  43.3 102.6 -3.1     -59.3    49      290   21 09 30
21 11 30  =0210+119    23 09 55  43.8 102.9 -3.1     -59.1   120      298   21 09 31

21 12 00  032120       23 10 25  42.6 100.8 -3.2     -60.2    19      298   21 12 00
21 15 00  ---          23 13 26  43.2 101.3 -3.1     -60.0   180      309   21 12 01

21 16 00  J0213+1213   23 14 26  44.7 103.7 -3.0     -58.8    49      309   21 16 00
21 18 00  =0210+119    23 16 26  45.1 104.1 -3.0     -58.7   120      317   21 16 01

21 18 30  032120       23 16 56  44.0 101.9 -3.1     -59.8    20      317   21 18 30
21 21 30  ---          23 19 57  44.6 102.4 -3.0     -59.6   180      328   21 18 31

21 22 30  J0213+1213   23 20 57  46.1 104.9 -2.9     -58.3    49      328   21 22 30
21 24 30  =0210+119    23 22 57  46.5 105.3 -2.9     -58.2   120      336   21 22 31

21 25 00  032120       23 23 27  45.3 103.0 -3.0     -59.4    20      336   21 25 00
21 28 00  ---          23 26 28  46.0 103.5 -2.9     -59.2   180      348   21 25 01

21 29 00  J0213+1213   23 27 28  47.4 106.1 -2.8     -57.8    49      348   21 29 00
21 31 00  =0210+119    23 29 28  47.8 106.5 -2.7     -57.6   120      356   21 29 01

21 31 30  032140       23 29 58  46.7 104.2 -2.9     -58.9    20      356   21 31 30
21 34 30  ---          23 32 59  47.3 104.7 -2.8     -58.7   180      367   21 31 31

21 35 30  J0213+1213   23 33 59  48.7 107.4 -2.7     -57.2    50      367   21 35 30
21 37 30  =0210+119    23 35 59  49.2 107.8 -2.6     -57.0   120      375   21 35 31

21 38 00  032140       23 36 29  48.0 105.4 -2.8     -58.4    20      375   21 38 00
21 41 00  ---          23 39 30  48.7 106.0 -2.7     -58.1   180      386   21 38 01

21 42 00  J0213+1213   23 40 30  50.1 108.7 -2.6     -56.5    50      386   21 42 00
21 44 00  =0210+119    23 42 30  50.5 109.1 -2.5     -56.3   120      394   21 42 01

21 44 30  032140       23 43 00  49.4 106.6 -2.7     -57.8    20      394   21 44 30
21 47 30  ---          23 46 01  50.0 107.3 -2.6     -57.5   180      406   21 44 31

21 48 30  J0213+1213   23 47 01  51.4 110.1 -2.5     -55.8    50      406   21 48 30
21 50 30  =0210+119    23 49 01  51.8 110.6 -2.4     -55.5   120      414   21 48 31
Schedule for VLBA_FD   (Code Fd )                                   Page   5
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   3 Feb 2024   Day  34 ---

21 51 00  032200       23 49 32  50.7 108.0 -2.5     -57.2    20      414   21 51 00
21 54 00  ---          23 52 32  51.3 108.6 -2.5     -56.8   180      425   21 51 01

21 55 00  J0213+1213   23 53 32  52.7 111.6 -2.3     -55.0    50      425   21 55 00
21 57 00  =0210+119    23 55 33  53.1 112.1 -2.3     -54.7   120      433   21 55 01

21 57 30  032200       23 56 03  52.0 109.4 -2.4     -56.5    20      433   21 57 30
22 00 30  ---          23 59 03  52.7 110.0 -2.4     -56.1   180      444   21 57 31

22 01 30  J0213+1213   00 00 03  54.0 113.1 -2.2     -54.1    50      444   22 01 30
22 03 30  =0210+119    00 02 04  54.4 113.6 -2.2     -53.8   120      452   22 01 31

22 04 00  032200       00 02 34  53.4 110.8 -2.3     -55.7    20      452   22 04 00
22 07 00  ---          00 05 34  54.0 111.5 -2.3     -55.3   180      464   22 04 01

22 08 00  J0213+1213   00 06 34  55.3 114.8 -2.1     -53.1    50      464   22 08 00
22 10 00  =0210+119    00 08 35  55.7 115.3 -2.1     -52.8   120      471   22 08 01

22 10 30  032220       00 09 05  54.7 112.4 -2.2     -54.8    20      471   22 10 30
22 13 30  ---          00 12 05  55.3 113.1 -2.2     -54.3   180      483   22 10 31

22 14 30  J0213+1213   00 13 05  56.6 116.5 -2.0     -52.0    50      483   22 14 30
22 16 30  =0210+119    00 15 06  56.9 117.1 -2.0     -51.7   120      491   22 14 31

22 17 00  032220       00 15 36  56.0 114.0 -2.1     -53.8    20      491   22 17 00
22 20 00  ---          00 18 36  56.5 114.8 -2.1     -53.3   180      502   22 17 01

22 21 00  J0213+1213   00 19 36  57.8 118.3 -1.9     -50.8    50      502   22 21 00
22 23 00  =0210+119    00 21 37  58.2 118.9 -1.9     -50.4   120      510   22 21 01

22 24 00  J0238+1636   00 22 37  55.8 106.0 -2.3     -59.7    43      510   22 24 00
22 26 00  =0235+164    00 24 37  56.2 106.5 -2.3     -59.5   120      518   22 24 01

22 27 00  J0213+1213   00 25 37  58.9 120.1 -1.8     -49.6    43      518   22 27 00
22 29 00  =0210+119    00 27 38  59.3 120.7 -1.8     -49.2   120      526   22 27 01

22 29 30  032240       00 28 08  58.4 117.4 -1.9     -51.7    20      526   22 29 30
22 32 30  ---          00 31 08  59.0 118.3 -1.9     -51.1   180      537   22 29 31

22 33 30  J0213+1213   00 32 09  60.1 122.2 -1.7     -48.2    50      537   22 33 30
22 35 30  =0210+119    00 34 09  60.5 122.9 -1.7     -47.7   120      545   22 33 31

22 36 00  032240       00 34 39  59.6 119.3 -1.8     -50.4    20      545   22 36 00
22 39 00  ---          00 37 39  60.2 120.3 -1.7     -49.7   180      556   22 36 01
Schedule for VLBA_FD   (Code Fd )                                   Page   6
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   3 Feb 2024   Day  34 ---

22 40 00  J0213+1213   00 38 40  61.3 124.4 -1.6     -46.6    49      556   22 40 00
22 42 00  =0210+119    00 40 40  61.7 125.1 -1.6     -46.1   120      564   22 40 01

22 42 30  032240       00 41 10  60.8 121.4 -1.7     -48.9    19      564   22 42 30
22 45 30  ---          00 44 11  61.4 122.4 -1.6     -48.2   180      576   22 42 31

22 46 30  J0213+1213   00 45 11  62.4 126.8 -1.5     -44.9    49      576   22 46 30
22 48 30  =0210+119    00 47 11  62.8 127.5 -1.5     -44.3   120      584   22 46 31

22 49 00  032240       00 47 41  62.0 123.6 -1.6     -47.4    19      584   22 49 00
22 52 00  ---          00 50 42  62.5 124.7 -1.5     -46.6   180      595   22 49 01

22 53 00  J0213+1213   00 51 42  63.5 129.3 -1.4     -43.0    49      595   22 53 00
22 55 00  =0210+119    00 53 42  63.9 130.1 -1.3     -42.4   120      603   22 53 01

22 56 00  J0225+1134   00 54 42  61.4 126.6 -1.5     -44.9    47      603   22 56 00
22 58 00  =0223+113    00 56 43  61.8 127.3 -1.5     -44.3   120      611   22 56 01

22 58 30  032300       00 57 13  63.7 127.1 -1.4     -44.8    18      611   22 58 30
23 01 30  ---          01 00 13  64.2 128.3 -1.4     -43.9   180      622   22 58 31

23 02 30  J0225+1134   01 01 13  62.6 129.0 -1.4     -43.0    48      622   23 02 30
23 04 30  =0223+113    01 03 14  62.9 129.8 -1.4     -42.4   120      630   23 02 31

23 05 30  J0213+1213   01 04 14  65.6 134.7 -1.2     -38.8    47      630   23 05 30
23 07 30  =0210+119    01 06 14  65.9 135.6 -1.1     -38.0   120      638   23 05 31

23 08 30  J0213+1213   01 07 14  66.0 136.1 -1.1     -37.7    54      638   23 08 30
23 11 30  =0210+119    01 10 15  66.5 137.5 -1.1     -36.5   180      649   23 08 31

23 12 00  032300       01 10 45  65.9 132.8 -1.2     -40.4    19      649   23 12 00
23 15 00  ---          01 13 45  66.4 134.2 -1.1     -39.3   180      661   23 12 01

23 16 00  J0213+1213   01 14 46  67.1 139.8 -1.0     -34.6    48      661   23 16 00
23 18 00  =0210+119    01 16 46  67.4 140.8 -1.0     -33.8   120      669   23 16 01

23 18 30  032320       01 17 16  66.9 135.9 -1.1     -37.9    18      669   23 18 30
23 21 30  ---          01 20 16  67.3 137.4 -1.0     -36.7   180      680   23 18 31

23 22 30  J0213+1213   01 21 17  68.0 143.3 -0.9     -31.8    48      680   23 22 30
23 24 30  =0210+119    01 23 17  68.2 144.4 -0.9     -30.8   120      688   23 22 31

23 25 00  032320       01 23 47  67.8 139.2 -1.0     -35.2    18      688   23 25 00
23 28 00  ---          01 26 47  68.3 140.8 -0.9     -33.9   180      699   23 25 01
Schedule for VLBA_FD   (Code Fd )                                   Page   7
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sat   3 Feb 2024   Day  34 ---

23 29 00  J0213+1213   01 27 48  68.8 147.0 -0.8     -28.7    48      699   23 29 00
23 31 00  =0210+119    01 29 48  69.0 148.2 -0.7     -27.6   120      707   23 29 01

23 31 30  032320       01 30 18  68.7 142.8 -0.9     -32.3    18      707   23 31 30
23 34 30  ---          01 33 19  69.1 144.5 -0.8     -30.8   180      719   23 31 31

23 35 30  J0213+1213   01 34 19  69.5 151.0 -0.7     -25.3    48      719   23 35 30
23 37 30  =0210+119    01 36 19  69.7 152.3 -0.6     -24.2   120      727   23 35 31

23 38 00  032340       01 36 49  69.5 146.6 -0.8     -29.1    18      727   23 38 00
23 41 00  ---          01 39 50  69.9 148.5 -0.7     -27.5   180      738   23 38 01

23 42 00  J0213+1213   01 40 50  70.1 155.2 -0.6     -21.7    48      738   23 42 00
23 44 00  =0210+119    01 42 50  70.3 156.6 -0.5     -20.5   120      746   23 42 01

23 44 30  032340       01 43 20  70.3 150.7 -0.7     -25.6    18      746   23 44 30
23 47 30  ---          01 46 21  70.6 152.7 -0.6     -23.9   180      757   23 44 31

23 48 30  J0213+1213   01 47 21  70.7 159.7 -0.5     -17.8    48      757   23 48 30
23 50 30  =0210+119    01 49 21  70.8 161.1 -0.4     -16.6   120      765   23 48 31

23 51 00  040000       01 49 51  70.9 155.1 -0.5     -21.8    18      765   23 51 00
23 54 00  ---          01 52 52  71.2 157.2 -0.5     -20.0   180      777   23 51 01

23 55 00  J0213+1213   01 53 52  71.1 164.4 -0.3     -13.7    47      777   23 55 00
23 57 00  =0210+119    01 55 52  71.2 165.8 -0.3     -12.4   120      785   23 55 01

 --- Start: Sat   3 Feb 2024   Day  34 -- Stop: Sun   4 Feb 2024   Day  35 ---

23 57 30  040000       01 56 22  71.4 159.7 -0.4     -17.8    18      785   23 57 30
00 00 30  ---          01 59 23  71.7 161.9 -0.4     -15.9   180      796   23 57 31

00 01 30  J0213+1213   02 00 23  71.4 169.2 -0.2      -9.5    47      796   00 01 30
00 03 30  =0210+119    02 02 23  71.5 170.7 -0.2      -8.1   120      804   00 01 31

00 04 00  040000       02 02 53  71.9 164.6 -0.3     -13.6    18      804   00 04 00
00 07 00  ---          02 05 54  72.0 166.9 -0.3     -11.6   180      815   00 04 01

00 08 00  J0213+1213   02 06 54  71.6 174.2 -0.1      -5.1    47      815   00 08 00
00 10 00  =0210+119    02 08 54  71.7 175.8 -0.1      -3.7   120      823   00 08 01

00 10 30  040020       02 09 24  72.2 169.6 -0.2      -9.2    18      823   00 10 30
00 13 30  ---          02 12 25  72.3 172.0 -0.2      -7.1   180      835   00 10 31
Schedule for VLBA_FD   (Code Fd )                                   Page   8
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Feb 2024   Day  35 ---

00 14 30  J0213+1213   02 13 25  71.7 179.3 -0.0      -0.7    47      835   00 14 30
00 16 30  =0210+119    02 15 25  71.7 180.8  0.0       0.7   120      842   00 14 31

00 17 00  040020       02 15 56  72.4 174.8 -0.1      -4.6    18      842   00 17 00
00 20 00  ---          02 18 56  72.4 177.2 -0.1      -2.5   180      854   00 17 01

00 21 00  J0213+1213   02 19 56  71.7 184.3  0.1       3.8    48      854   00 21 00
00 23 00  =0210+119    02 21 57  71.6 185.9  0.1       5.2   120      862   00 21 01

00 24 00  J0225+1134   02 22 57  71.0 177.0 -0.1      -2.7    45      862   00 24 00
00 26 00  =0223+113    02 24 57  71.0 178.5 -0.0      -1.4   120      870   00 24 01

00 26 30  040020       02 25 27  72.4 182.5  0.1       2.2    19      870   00 26 30
00 29 30  ---          02 28 28  72.4 184.9  0.1       4.3   180      881   00 26 31

00 30 30  J0225+1134   02 29 28  71.0 181.9  0.0       1.6    49      881   00 30 30
00 32 30  =0223+113    02 31 28  71.0 183.4  0.1       3.0   120      889   00 30 31

00 33 30  J0213+1213   02 32 28  71.2 193.9  0.3      12.2    45      889   00 33 30
00 35 30  =0210+119    02 34 29  71.1 195.3  0.3      13.5   120      897   00 33 31

00 36 00  040040       02 34 59  72.2 190.1  0.2       8.9    18      897   00 36 00
00 39 00  ---          02 37 59  72.1 192.4  0.3      10.9   180      908   00 36 01

00 40 00  J0213+1213   02 38 59  70.8 198.6  0.4      16.3    48      908   00 40 00
00 42 00  =0210+119    02 41 00  70.7 200.0  0.4      17.6   120      916   00 40 01

00 42 30  040040       02 41 30  71.9 195.1  0.3      13.3    18      916   00 42 30
00 45 30  ---          02 44 30  71.7 197.4  0.4      15.3   180      927   00 42 31

00 46 30  J0213+1213   02 45 30  70.3 203.1  0.5      20.3    48      927   00 46 30
00 48 30  =0210+119    02 47 31  70.2 204.5  0.6      21.4   120      935   00 46 31

00 49 00  040040       02 48 01  71.5 200.0  0.4      17.6    19      935   00 49 00
00 52 00  ---          02 51 01  71.2 202.2  0.5      19.5   180      947   00 49 01

00 53 00  J0213+1213   02 52 01  69.7 207.5  0.6      24.0    49      947   00 53 00
00 55 00  =0210+119    02 54 02  69.5 208.7  0.7      25.1   120      955   00 53 01

00 55 30  040100       02 54 32  70.9 204.6  0.5      21.6    19      955   00 55 30
00 58 30  ---          02 57 32  70.7 206.7  0.6      23.4   180      966   00 55 31

00 59 30  J0213+1213   02 58 33  69.0 211.5  0.7      27.4    49      966   00 59 30
01 01 30  =0210+119    03 00 33  68.8 212.7  0.8      28.5   120      974   00 59 31
Schedule for VLBA_FD   (Code Fd )                                   Page   9
               JUNO tracking
  UP:  D => Below limits;  H => Below horizon mask;  W => still slewing at end;  blank => Up.
  Early: Seconds between end of slew and start.   Dwell: On source seconds. 
  Disk: GBytes recorded to this point.
  TPStart:  Recording start time.  Frequencies are LO sum (band edge).
  SYNC: Time correlator is expected to sync up.
----------------------------------------------------------------------------------------
Start UT  Source               Start / Stop                 Early    Disk   TPStart
Stop UT                  LST      EL    AZ   HA  UP   ParA  Dwell   GBytes    SYNC
----------------------------------------------------------------------------------------

 --- Sun   4 Feb 2024   Day  35 ---

01 02 00  040100       03 01 03  70.3 209.0  0.6      25.4    19      974   01 02 00
01 05 00  ---          03 04 03  70.0 210.9  0.7      27.0   180      985   01 02 01

01 06 00  J0213+1213   03 05 04  68.3 215.4  0.8      30.6    49      985   01 06 00
01 08 00  =0210+119    03 07 04  68.0 216.5  0.9      31.6   120      993   01 06 01

01 08 30  040100       03 07 34  69.6 213.1  0.8      28.9    19      993   01 08 30
01 11 30  ---          03 10 35  69.2 214.9  0.8      30.4   180     1005   01 08 31

01 12 30  J0213+1213   03 11 35  67.4 218.9  1.0      33.6    49     1005   01 12 30
01 14 30  =0210+119    03 13 35  67.1 220.0  1.0      34.5   120     1013   01 12 31

01 15 00  040120       03 14 05  68.8 217.0  0.9      32.1    19     1013   01 15 00
01 18 00  ---          03 17 06  68.4 218.7  0.9      33.5   180     1024   01 15 01

01 19 00  J0213+1213   03 18 06  66.5 222.3  1.1      36.3    49     1024   01 19 00
01 21 00  =0210+119    03 20 06  66.2 223.3  1.1      37.1   120     1032   01 19 01

01 21 30  040120       03 20 36  67.9 220.5  1.0      35.0    19     1032   01 21 30
01 24 30  ---          03 23 37  67.5 222.1  1.0      36.3   180     1043   01 21 31

01 25 30  J0213+1213   03 24 37  65.5 225.4  1.2      38.8    48     1043   01 25 30
01 27 30  =0210+119    03 26 37  65.2 226.3  1.2      39.5   120     1051   01 25 31

01 28 00  J0238+1636   03 27 07  72.4 220.4  0.8      35.6     8     1051   01 28 00
01 30 00  =0235+164    03 29 08  72.1 221.6  0.8      36.6   120     1059   01 28 01


SETUP FILE INFORMATION:
   NOTE: If DOPPLER, FREQ, or BW were used, see the individual scans for the final BBC settings.


 ======== Setup file: sess323.X512Rglob
   Matching groups in /home/guest/rmc/SCHED/sched11.6/catalogs/freq_RDBE.dat:
     v4cm_3

   Setup group:    2         Station: VLBA_FD           Total bit rate:   512
   Format: VDIF              Bits per sample: 2         Sample rate: 64.000
   Number of channels:  4    DBE type: RDBE_DDC         Speedup factor:   1.00

   Disk used to record data.

   1st LO=   7600.00   7600.00   7600.00   7600.00
   Net SB=         U         U         U         U
   IF SB =         U         U         U         U
   Pol.  =      RCP       RCP       RCP       RCP 
   BBC   =         1         2         3         4
   BBC SB=         U         U         U         U
   IF    =        B         B         B         B 

   VLBA FE=     omit     4cm      omit     4cm 
   VLBA Synth=   7.6     15.1     15.1

  The following frequency sets based on these setups were used.
     See the crd files for VLBA legacy system setups and pcal detection details.

   Frequency Set:  10  Setup file default.  Used with PCAL = off
   LO sum=   8400.00  8432.00  8464.00  8496.00
   BBC fr=    800.00   832.00   864.00   896.00
   Bandwd=     32.00    32.00    32.00    32.00
   VLBA legacy crd files using  4 channels based on RDBE channels:   1  2  3  4
   CRD fr=     808.00    840.00    872.00    904.00
   CRD bw=      16.00     16.00     16.00     16.00
    Matching frequency sets:  10  11  12  13  14  15  16  17  18

   Track assignments are: 
    track1=   1,  2,  3,  4
    barrel=roll_off 

 POSITIONS OF SOURCES USED IN RECORDING SCANS

   Source                         Source position (RA/Dec)                        Error
                        (B1950)             (J2000)             (Date)            (mas)

 * 031940            02 18 09.922314   * 02 20 52.390000     02 22 10.237998       0.00
                     12 43 51.53835    * 12 57 33.60000      13 04 09.67925        0.00
                     From catalog imbedded in main SCHED input file.

 * 032000            02 18 10.720027   * 02 20 53.190000     02 22 11.039171       0.00
                     12 43 59.57166    * 12 57 41.60000      13 04 17.66427        0.00
                     From catalog imbedded in main SCHED input file.

 * 032020            02 18 11.557684   * 02 20 54.030000     02 22 11.880376       0.00
                     12 44 07.70663    * 12 57 49.70000      13 04 25.74851        0.00
                     From catalog imbedded in main SCHED input file.

 * 032040            02 18 12.425314   * 02 20 54.900000     02 22 12.751596       0.00
                     12 44 15.84286    * 12 57 57.80000      13 04 33.83215        0.00
                     From catalog imbedded in main SCHED input file.

 * 032100            02 18 13.362859   * 02 20 55.840000     02 22 13.692864       0.00
                     12 44 24.08200    * 12 58 06.00000      13 04 42.01442        0.00
                     From catalog imbedded in main SCHED input file.

 * 032120            02 18 14.380371   * 02 20 56.860000     02 22 14.714158       0.00
                     12 44 32.12449    * 12 58 14.00000      13 04 49.99509        0.00
                     From catalog imbedded in main SCHED input file.

 * 032140            02 18 15.497869   * 02 20 57.980000     02 22 15.835469       0.00
                     12 44 39.77115    * 12 58 21.60000      13 04 57.57375        0.00
                     From catalog imbedded in main SCHED input file.

 * 032200            02 18 16.775493   * 02 20 59.260000     02 22 17.116737       0.00
                     12 44 46.02448    * 12 58 27.80000      13 05 03.74911        0.00
                     From catalog imbedded in main SCHED input file.

 * 032220            02 18 18.223704   * 02 21 00.710000     02 22 18.567747       0.00
                     12 44 48.48492    * 12 58 30.20000      13 05 06.12073        0.00
                     From catalog imbedded in main SCHED input file.

 * 032240            02 18 19.673376   * 02 21 02.160000     02 22 20.018064       0.00
                     12 44 43.44539    * 12 58 25.10000      13 05 00.99160        0.00
                     From catalog imbedded in main SCHED input file.

 * 032300            02 18 20.774401   * 02 21 03.260000     02 22 21.117700       0.00
                     12 44 33.09128    * 12 58 14.70000      13 04 50.56886        0.00
                     From catalog imbedded in main SCHED input file.

 * 032320            02 18 21.585828   * 02 21 04.070000     02 22 21.927114       0.00
                     12 44 22.02509    * 12 58 03.60000      13 04 39.45176        0.00
                     From catalog imbedded in main SCHED input file.

 * 032340            02 18 22.227234   * 02 21 04.710000     02 22 22.566519       0.00
                     12 44 11.85181    * 12 57 53.40000      13 04 29.23811        0.00
                     From catalog imbedded in main SCHED input file.

 * 040000            02 18 22.768575   * 02 21 05.250000     02 22 23.105943       0.00
                     12 44 02.47436    * 12 57 44.00000      13 04 19.82652        0.00
                     From catalog imbedded in main SCHED input file.

 * 040020            02 18 23.259826   * 02 21 05.740000     02 22 23.595405       0.00
                     12 43 53.79482    * 12 57 35.30000      13 04 11.11598        0.00
                     From catalog imbedded in main SCHED input file.

 * 040040            02 18 23.710977   * 02 21 06.190000     02 22 24.044910       0.00
                     12 43 45.81361    * 12 57 27.30000      13 04 03.10630        0.00
                     From catalog imbedded in main SCHED input file.

 * 040100            02 18 24.132057   * 02 21 06.610000     02 22 24.464444       0.00
                     12 43 38.33115    * 12 57 19.80000      13 03 55.59726        0.00
                     From catalog imbedded in main SCHED input file.

 * 040120            02 18 24.533078   * 02 21 07.010000     02 22 24.864005       0.00
                     12 43 31.24785    * 12 57 12.70000      13 03 48.48865        0.00
                     From catalog imbedded in main SCHED input file.

   0210+119          02 10 23.637337   * 02 13 05.183047     02 14 22.542298       0.18
 * J0213+1213        11 59 09.87174    * 12 13 10.91092      12 19 55.70606        0.38
                     /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,     59 observations.

   0223+113          02 23 00.175714   * 02 25 41.909882     02 26 59.441975       0.10
 * J0225+1134        11 20 55.65804    * 11 34 25.46498      11 40 55.25109        0.11
                     /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,    222 observations.

   0235+164          02 35 52.630214   * 02 38 38.930106     02 39 58.718043       0.12
 * J0238+1636        16 24 04.01612    * 16 36 59.27454      16 43 14.44663        0.16
   J0238+16          /home/guest/rmc/SCHED/sched11.6/catalogs/sources.gsfc
                     GSFC 2016a X/S astro solution,  64441 observations.



SOURCE SCAN SUMMARY FOR SOURCES LISTED ABOVE

     Scan hours are for recording scans only. 
     Baseline hours are only counted for scans above horizon at both ends.
  Source       Setup file             Frequency sets                  Observing hours
                                   (duplicates not shown)              Scan  Baseline
  031940     sess323.X512Rglob     1 3 4 5 6 7 8 10                  0.100    13.536
  032000     sess323.X512Rglob     1 3 4 5 6 7 8 10                  0.150    20.327
  032020     sess323.X512Rglob     1 3 4 5 6 7 8 10                  0.150    19.527
  032040     sess323.X512Rglob     1 3 4 5 6 8 10                    0.150    17.931
  032100     sess323.X512Rglob     1 3 4 5 6 8 10                    0.100    11.944
  032120     sess323.X512Rglob     1 3 4 5 6 8 10                    0.150    17.928
  032140     sess323.X512Rglob     1 3 4 5 6 8 10                    0.150    17.927
  032200     sess323.X512Rglob     1 3 4 5 6 8 10                    0.150    20.322
  032220     sess323.X512Rglob     1 3 4 5 6 8 10                    0.100    13.548
  032240     sess323.X512Rglob     1 3 4 8 10                        0.200    18.200
  032300     sess323.X512Rglob     1 10                              0.100     4.500
  032320     sess323.X512Rglob     1 10                              0.150     6.750
  032340     sess323.X512Rglob     1 10                              0.100     4.500
  040000     sess323.X512Rglob     10                                0.150     5.400
  040020     sess323.X512Rglob     10                                0.150     5.400
  040040     sess323.X512Rglob     10                                0.150     5.400
  040100     sess323.X512Rglob     10                                0.150     5.400
  040120     sess323.X512Rglob     10                                0.100     3.600
  J0213+1213 sess323.X512Rglob     1 3 4 5 6 7 8 10                  1.750   151.650
  J0225+1134 sess323.X512Rglob     1 3 4 5 6 7 8 10                  0.250    19.800
  J0238+1636 sess323.X512Rglob     1 3 4 5 6 7 8 10                  0.117    11.733


EFFECT OF SOLAR CORONA

  The solar corona can cause unstable phases for sources too close to the Sun.
  SCHED provides warnings at individual scans for distances less than 10 degrees.
  The distance from the Sun to each source in this schedule is:
    Source         Sun distance (deg) 
   031940              83.0
   032000              83.0
   032020              83.0
   032040              83.0
   032100              83.0
   032120              83.0
   032140              83.0
   032200              83.0
   032220              83.0
   032240              83.0
   032300              83.0
   032320              83.0
   032340              83.0
   040000              83.0
   040020              83.0
   040040              83.0
   040100              83.0
   040120              83.0
   J0213+1213          80.9
   J0225+1134          83.6
   J0238+1636          88.2

  Barry Clark estimates from predictions by Ketan Desai of IPM scattering sizes 
  that the Sun will cause amplitude reductions on the  longest VLBA baselines 
  at a solar distance of 60deg F^(-0.6) where F is in GHz. 
  For common VLBI bands, this is: 
       327 MHz        117. deg 
       610 MHz         81. deg 
       1.6 GHz         45. deg 
       2.3 GHz         36. deg 
       5.0 GHz         23. deg 
       8.4 GHz         17. deg 
      15.0 GHz         12. deg 
      22.0 GHz          9. deg 
      43.0 GHz          6. deg 

